{"text_format":"1","workbook":"xlsx","n_sheets":35,"sheets":["Instructions","CONTENTS","Business & other details","2.1 Expenditure summary","2.2 Repex","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","5.4 MD & utilisation-Spatial","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","Additional Info 7.3","7.4 Shared Assets","7.7 TSS-LRMC","7.8 Export Services","AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":1,"defined_names":726,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[13,2,13,4],[16,2,16,4],[10,1,11,1],[10,2,10,3],[11,2,11,4],[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List)),\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by Energex to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nBusinesses must use the macro at the top of  \neach worksheet to identify confidential\ninformation in the confidential workbook and\nwhere confidential information has been \nremoved in the public workbook. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the NON-CONFIDENTIAL macro."]
[]
[null,"PROTECTED (SOCI) INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify information in the \nconfidential workbook that is protected \ninformation under the SOCI Act. All \ninformation marked Protected (SOCI) is also \ndeemed to be confidential information."]
[null,null,"-Do this by selecting the cell or cells that contain protected information and then run the PROTECTED (SOCI) macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as protected..\n\n-To reverse this, select the cell or cells and run the NON-PROTECTED macro."]
[]
[null,"RESPONSES","\nPlease return two (2) files to the AER: \n\n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information redacted or aggregated.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential or public. "]
[]
[]
[null,"ORDER OF MAGNITUDE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. \n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," PLEASE DO NOT ENTER TEXT into cells that are to contain numbers \n(including 'numbers stored as text')"]

{"sheet":"CONTENTS","index":1,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[[6,3,6,4],[8,3,8,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"DRAFT RIN ONLY - DO NOT USE FOR SUBMISSION"]
[]
[null,null,null,"TEMPLATE","OCTOBER 2023 - FINAL RIN"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 FORECAST price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[null,null,null,null,"7.8 Export Services"]

{"sheet":"Business & other details","index":2,"n_rows":77,"n_cols":79,"rows_kept":77,"cut":false,"hidden":false,"merged":[[10,16,10,93],[11,16,11,93],[18,37,18,58],[27,37,27,51],[0,7,2,15],[6,21,6,75],[27,21,27,35],[45,37,45,44],[45,46,45,53],[45,55,45,62],[45,64,45,71],[3,21,3,57],[8,16,8,93],[25,68,25,89],[26,68,26,89],[28,68,28,71],[28,80,28,82],[27,68,27,82],[28,37,28,40],[25,37,25,58],[26,37,26,58],[28,49,28,51],[27,60,27,66],[28,60,28,66],[18,21,18,35],[46,73,46,80],[44,73,44,80],[54,55,54,62],[28,21,28,35],[26,21,26,35],[48,73,48,80],[48,64,48,71],[49,73,49,80],[48,55,48,62],[45,73,45,80],[35,21,35,35],[36,21,36,35],[36,60,36,66],[35,60,35,66],[34,21,34,35],[34,68,34,89],[35,68,35,89],[36,68,36,89],[34,37,34,58],[44,46,44,53],[44,25,44,34],[44,55,44,62],[44,64,44,71],[46,64,46,71],[19,21,19,35],[19,37,19,48],[48,25,48,34],[52,25,52,34],[25,21,25,35],[25,60,25,66],[26,60,26,66],[34,60,34,66],[56,25,56,34],[48,46,48,53],[48,37,48,44],[52,37,52,44],[50,73,50,80],[54,73,54,80],[52,73,52,80],[56,37,56,44],[52,46,52,53],[53,46,53,53],[49,46,49,53],[49,37,49,44],[54,64,54,71],[50,46,50,53],[53,55,53,62],[50,37,50,44],[53,37,53,44],[52,64,52,71],[50,64,50,71],[52,55,52,62],[50,55,50,62],[49,64,49,71],[49,55,49,62],[76,25,76,34],[76,37,76,52],[58,25,58,34],[66,25,66,34],[68,25,68,34],[58,37,58,44],[64,25,64,34],[64,37,64,52],[35,37,35,58],[36,37,36,58],[46,37,46,44],[46,46,46,53],[46,55,46,62],[44,37,44,44],[66,37,66,52],[68,37,68,52],[70,37,70,52],[72,37,74,81],[70,25,70,34],[72,25,74,34],[54,46,54,53],[54,37,54,44],[53,73,53,80],[53,64,53,71]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRAFT TEMPLATE ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DO NOT USE FOR SUBMISSIONS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energex"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":40078849055}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"26 Reddacliff Street"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"26 Reddacliff Street"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NEWSTEAD"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NEWSTEAD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Qld"},null,null,null,null,null,null,null,null,null,"Post code",null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"QLD"},null,null,null,null,null,null,null,null,null,"Post code"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2025-26",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2029-30"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2034-35"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2035-36"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2036-37"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2037-38"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2038-39"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2039-40"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2024-25"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2029-30"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2034-35"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2015-16"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2019-20"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2024-25"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2029-30"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2022-23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2028-29"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Regulatory proposal"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Public"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"31/01/24",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"2.1 Expenditure summary","index":3,"n_rows":113,"n_cols":37,"rows_kept":113,"cut":false,"hidden":false,"merged":[[8,1,9,1],[24,1,25,1],[38,1,39,1],[91,1,92,1],[104,1,105,1],[51,1,52,1],[63,1,64,1],[77,1,78,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX (including dual function assets)"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure",{"$f":"SUM('2.2 Repex'!D12:D119,'2.2 Repex'!D129:D177 )","v":166122500.12621698},{"$f":"SUM('2.2 Repex'!E12:E119,'2.2 Repex'!E129:E177 )","v":161456323.65061399},{"$f":"SUM('2.2 Repex'!F12:F119,'2.2 Repex'!F129:F177 )","v":162287450.05325323},{"$f":"SUM('2.2 Repex'!G12:G119,'2.2 Repex'!G129:G177 )","v":183870743.52228856},{"$f":"SUM('2.2 Repex'!H12:H119,'2.2 Repex'!H129:H177 )","v":189515465.30029389},{"$f":"SUM('2.2 Repex'!I12:I119,'2.2 Repex'!I129:I177 )","v":198119984.13785279},{"$f":"SUM('2.2 Repex'!J12:J119,'2.2 Repex'!J129:J177 )","v":180279268.13898793}]
[null,"Connections",{"$f":"SUM('2.5 Connections'!E124:E137, '2.5 Connections'!E142:E155)","v":71178790.407074824},{"$f":"SUM('2.5 Connections'!F124:F137, '2.5 Connections'!F142:F155)","v":70166631.009547472},{"$f":"SUM('2.5 Connections'!G124:G137, '2.5 Connections'!G142:G155)","v":71179521.002218887},{"$f":"SUM('2.5 Connections'!H124:H137, '2.5 Connections'!H142:H155)","v":73690167.166764095},{"$f":"SUM('2.5 Connections'!I124:I137, '2.5 Connections'!I142:I155)","v":76321788.105436206},{"$f":"SUM('2.5 Connections'!J124:J137, '2.5 Connections'!J142:J155)","v":79155677.287858278},{"$f":"SUM('2.5 Connections'!K124:K137, '2.5 Connections'!K142:K155)","v":81245665.711651966},null,null,null,null,null,null,null,"ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO",{"$f":"B12","v":"Connections"}]
[null,"Augmentation Expenditure",{"$f":"SUM('2.3 Augex (b)'!D48:D56)","v":68233106.418702453},{"$f":"SUM('2.3 Augex (b)'!E48:E56)","v":98685048.298931003},{"$f":"SUM('2.3 Augex (b)'!F48:F56)","v":127881687.1931989},{"$f":"SUM('2.3 Augex (b)'!G48:G56)","v":120638454.08555226},{"$f":"SUM('2.3 Augex (b)'!H48:H56)","v":115550878.19765413},{"$f":"SUM('2.3 Augex (b)'!I48:I56)","v":109480069.96358067},{"$f":"SUM('2.3 Augex (b)'!J48:J56)","v":136770878.30833453},null,null,null,null,null,null,null,"ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Augmentation Expenditure"]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E33:E51)","v":136452158.51844984},{"$f":"SUM('2.6 Non-network'!F33:F51)","v":187717142.87418687},{"$f":"SUM('2.6 Non-network'!G33:G51)","v":157437075.19640133},{"$f":"SUM('2.6 Non-network'!H33:H51)","v":155290478.66719109},{"$f":"SUM('2.6 Non-network'!I33:I51)","v":117129893.27701458},{"$f":"SUM('2.6 Non-network'!J33:J51)","v":106822374.35686339},{"$f":"SUM('2.6 Non-network'!K33:K51)","v":105063891.18371511}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C24:C26)","v":11861810},{"$f":"SUM('7.8 Export Services'!D24:D26)","v":5022684},{"$f":"SUM('7.8 Export Services'!E24:E26)","v":11168222.385660999},{"$f":"SUM('7.8 Export Services'!F24:F26)","v":13771974.70307558},{"$f":"SUM('7.8 Export Services'!G24:G26)","v":12283830.602465529},{"$f":"SUM('7.8 Export Services'!H24:H26)","v":9610703.1673105285},{"$f":"SUM('7.8 Export Services'!I24:I26)","v":9058434.6992856916}]
[null,"Public lighting"]
[null,"Metering"]
[null,"Capitalised network overheads",{"$f":"'2.10 Overheads'!D16","v":124925433.7509841},{"$f":"'2.10 Overheads'!E16","v":143839843.74642706},{"$f":"'2.10 Overheads'!F16","v":151848673.66928712},{"$f":"'2.10 Overheads'!G16","v":158082945.6066497},{"$f":"'2.10 Overheads'!H16","v":156009478.47745401},{"$f":"'2.10 Overheads'!I16","v":153860326.68528903},{"$f":"'2.10 Overheads'!J16","v":152433829.83911717}]
[null,"Capitalised corporate overheads",{"$f":"'2.10 Overheads'!D31","v":11227736.322429609},{"$f":"'2.10 Overheads'!E31","v":10944192.447418854},{"$f":"'2.10 Overheads'!F31","v":12941019.709513061},{"$f":"'2.10 Overheads'!G31","v":13694967.624126861},{"$f":"'2.10 Overheads'!H31","v":13538313.559348769},{"$f":"'2.10 Overheads'!I31","v":13136684.849546567},{"$f":"'2.10 Overheads'!J31","v":12564596.175871866}]
[null,"capcons (included in the above)",3423158.4205738516,3747087.6298883785,4096725.9896561662,3941337.8655054364,3881697.2936015874,3835513.8136860118,3698235.8445723904]
[null,"Total",{"$f":"SUM(C11:C19)","v":590001535.54385793},677831866.02712524,694743649.20953357,719039731.37564826,680349647.51966715,670185820.4483012,677416564.05696416]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"}]
[null,"Vegetation management",43658931.93064516,43435282.046609178]
[null,"Maintenance",93575013.240864232,93095660.221114919]
[null,"Emergency response",55416167.13890963,55132288.931031711,null," "]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E13:E31)","v":158212771.17563835},{"$f":"SUM('2.6 Non-network'!F13:F31)","v":157402387.01910481}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C14:C15)","v":4762225.8882167945},{"$f":"SUM('7.8 Export Services'!D14:D15)","v":4751684.9857648825}]
[null,"Metering"]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D13","v":219926232.7747044},{"$f":"'2.10 Overheads'!E13","v":218799625.35941824}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D28","v":82224275.293777838},{"$f":"'2.10 Overheads'!E28","v":81803068.250426188}]
[null,"Total",{"$f":"SUM(C27:C29,C32:C34)","v":494800620.37890124},{"$f":"SUM(D27:D29,D32:D34)","v":492265924.80860019}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Connections",15082923.91202743,14555911.587884475,15078417.034636859,16386553.308929412,17721346.613755565,19142900.107434791,20114504.258902352]
[null,"Metering"]
[null,"Public lighting",{"$f":"SUM('4.1 Public lighting'!D15,'4.1 Public lighting'!D19,'4.1 Public lighting'!D23)","v":31547732.188522197},{"$f":"SUM('4.1 Public lighting'!E15,'4.1 Public lighting'!E19,'4.1 Public lighting'!E23)","v":28802146.98689083},{"$f":"SUM('4.1 Public lighting'!F15,'4.1 Public lighting'!F19,'4.1 Public lighting'!F23)","v":39402441.758679822},{"$f":"SUM('4.1 Public lighting'!G15,'4.1 Public lighting'!G19,'4.1 Public lighting'!G23)","v":39259397.912789792},{"$f":"SUM('4.1 Public lighting'!H15,'4.1 Public lighting'!H19,'4.1 Public lighting'!H23)","v":39110810.770283565},{"$f":"SUM('4.1 Public lighting'!I15,'4.1 Public lighting'!I19,'4.1 Public lighting'!I23)","v":39034465.316761278},{"$f":"SUM('4.1 Public lighting'!J15,'4.1 Public lighting'!J19,'4.1 Public lighting'!J23)","v":38996234.836608812}]
[null,"Fee and quoted",20063383.241224661,19362348.727373071,20057388.169656597,21797477.793920394,23573026.737795439,25463984.53271243,26756417.390118405]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D17","v":6807726.9438940184},{"$f":"'2.10 Overheads'!E17","v":6848886.5442624297},{"$f":"'2.10 Overheads'!F17","v":7524260.9000188028},{"$f":"'2.10 Overheads'!G17","v":7604997.7154228166},{"$f":"'2.10 Overheads'!H17","v":7546238.7872547712},{"$f":"'2.10 Overheads'!I17","v":7477119.5410701381},{"$f":"'2.10 Overheads'!J17","v":7411978.7694842694}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D32","v":402455.78665359615},{"$f":"'2.10 Overheads'!E32","v":404889.03926215949},{"$f":"'2.10 Overheads'!F32","v":444815.4816520657},{"$f":"'2.10 Overheads'!G32","v":449588.44020682562},{"$f":"'2.10 Overheads'!H32","v":446114.75936538068},{"$f":"'2.10 Overheads'!I32","v":442028.60244025756},{"$f":"'2.10 Overheads'!J32","v":438177.64298082638}]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C41:C46)","v":73904222.072321892},69974182.885672972,82507323.344644129,85498015.171269238,88397537.668454722,91560498.100418881,93717312.898094669]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Connections",27120701.821792118,26714035.055720098,26415682.858946074,26158776.658254057,25904369.003456406,25652435.5948999,25402952.369258042]
[null,"Metering",{"$f":"'3.2 Operating expenditure'!K72","v":0},{"$f":"'3.2 Operating expenditure'!L72","v":0},{"$f":"'3.2 Operating expenditure'!M72","v":0},{"$f":"'3.2 Operating expenditure'!N72","v":0},{"$f":"'3.2 Operating expenditure'!O72","v":0},{"$f":"'3.2 Operating expenditure'!P72","v":0},{"$f":"'3.2 Operating expenditure'!Q72","v":0}]
[null,"Public lighting",{"$f":"'3.2 Operating expenditure'!K74","v":24130471.039790615},{"$f":"'3.2 Operating expenditure'!L74","v":22711458.590764008},{"$f":"'3.2 Operating expenditure'!M74","v":17994836.054987252},{"$f":"'3.2 Operating expenditure'!N74","v":17385971.941928718},{"$f":"'3.2 Operating expenditure'!O74","v":16782254.676833037},{"$f":"'3.2 Operating expenditure'!P74","v":16236621.278856363},{"$f":"'3.2 Operating expenditure'!Q74","v":15728168.917003969}]
[null,"Fee and quoted",51032980.500466019,50267756.308278441,49706347.464942172,49222927.485012688,48744209.014828205,48270146.329770796,47800694.149918132]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D14","v":45860303.100718513},{"$f":"'2.10 Overheads'!E14","v":46137575.054184981},{"$f":"'2.10 Overheads'!F14","v":50687239.4159761},{"$f":"'2.10 Overheads'!G14","v":51231123.572366327},{"$f":"'2.10 Overheads'!H14","v":50835293.616513461},{"$f":"'2.10 Overheads'!I14","v":50369671.301422887},{"$f":"'2.10 Overheads'!J14","v":49930850.010004602}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D29","v":15420207.377946917},{"$f":"'2.10 Overheads'!E29","v":15513438.140359266},{"$f":"'2.10 Overheads'!F29","v":17043231.081430655},{"$f":"'2.10 Overheads'!G29","v":17226108.339409042},{"$f":"'2.10 Overheads'!H29","v":17093013.27476785},{"$f":"'2.10 Overheads'!I29","v":16936451.015623428},{"$f":"'2.10 Overheads'!J29","v":16788900.413948003}]
[null,"Total",{"$f":"SUM(C54:C59)","v":163564663.84071416},161344263.14930677,161847336.87628224,161224907.99697083,159359139.58639896,157465325.52057338,155651565.86013275]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C66:C72)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Export services"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total",{"$f":"SUM(C80:C87)","v":0},{"$f":"SUM(D80:D87)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure"]
[null,"Connections",3423158.4205738516,3747087.6298883785,4096725.9896561662,3941337.8655054364,3881697.2936015874,3835513.8136860118,3698235.8445723904]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total",{"$f":"SUM(C94:C100)","v":3423158.4205738516},3747087.6298883785,4096725.9896561662,3941337.8655054364,3881697.2936015874,3835513.8136860118,3698235.8445723904]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure",89790471.186634958,102126403.19731057,95390247.707262307,99436850.696020722,98146047.533677951,96668129.204347894,95508397.282620877]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",46314910.997628517,52601974.364205554,63463247.839514986,66150671.591001503,65291467.594017565,64312903.176270522,63551016.840319164]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Export services",47787.889150275914,55658.63232979022,5936197.8320231177,6190390.9437545817,6110276.9091074876,6015979.1542174099,5939011.8920492567]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C107:C111)","v":136153170.07341373},154784036.1938459,164789693.37880042,171777913.23077682,169547792.03680298,166997011.53483585,164998426.01498929]

{"sheet":"2.2 Repex","index":4,"n_rows":521,"n_cols":10,"rows_kept":521,"cut":false,"hidden":false,"merged":[[472,1,479,1],[374,1,380,1],[381,1,386,1],[387,1,395,1],[396,1,403,1],[404,1,419,1],[420,1,448,1],[300,1,307,1],[355,1,373,1],[449,1,462,1],[463,1,471,1],[308,1,348,1],[224,1,231,1],[232,1,247,1],[248,1,276,1],[277,1,290,1],[291,1,299,1],[480,1,520,1],[11,1,29,1],[30,1,36,1],[37,1,42,1],[43,1,51,1],[52,1,59,1],[60,1,75,1],[76,1,104,1],[105,1,118,1],[119,1,127,1],[128,1,135,1],[183,1,201,1],[202,1,208,1],[209,1,214,1],[215,1,223,1],[136,1,176,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.2 REPEX"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",9703086.7097322941,9951234.8349684216,10155748.697482526,10189931.864146866,10218257.619594617,10237323.394425893,10305221.212107787]
[null,null,"> 1 kV & < = 11 kV; Wood",11451353.644905007,11744212.198415497,11930980.20306888,11971138.609593013,12004415.725594109,12026814.210318776,12106580.610879185]
[null,null,"˃ 11 kV & < = 22 kV; Wood"]
[null,null,"> 22 kV & < = 66 kV; Wood",4511921.6582282595,4627310.1870743046,4704286.0085948724,4720120.1334298411,4733241.0227906397,4742072.5585496947,4773523.7851652401]
[null,null,"> 66 kV & < = 132 kV; Wood",865654.46538569604,887792.83630969131,894649.54618070298,897660.84110875195,900156.13958564703,901835.69934125734,907817.01628648897]
[null,null,"> 132 kV; Wood"]
[null,null,"˂ = 1 kV; Concrete"]
[null,null,"> 1 kV & < = 11 kV; Concrete",886273.5986538016,908939.28623666405,931586.36693345685,934721.98725960823,937320.30752079759,939069.210180455,945297.47391374968]
[null,null,"˃ 11 kV & < = 22 kV; Concrete"]
[null,null,"> 22 kV & < = 66 kV; Concrete"]
[null,null,"> 66 kV & < = 132 kV; Concrete"]
[null,null,"> 132 kV; Concrete"]
[null,null,"˂ = 1 kV; Steel"]
[null,null,"> 1 kV & < = 11 kV; Steel"]
[null,null,"˃ 11 kV & < = 22 kV; Steel"]
[null,null,"> 22 kV & < = 66 kV; Steel"]
[null,null,"> 66 kV & < = 132 kV; Steel"]
[null,null,"> 132 kV; Steel"]
[null,null,"Other"]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",19895710.9439069,20404526.69694129,20898490.712597266,20968832.802810557,21027121.517388429,21066355.052020755,21206075.121362604]
[null,null,"> 1 kV & < = 11 kV",7254345.3969420288,7439869.0621341495,7453131.7667142497,7478218.2131144069,7499006.0047418382,7512998.0536084296,7562827.1107197916]
[null,null,"˃ 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 66 kV",871116.35278923542,893394.40680171433,896987.80771397788,900006.9729808938,902508.79318517074,904192.74264844507,910189.69240027794]
[null,null,"> 66 kV & < = 132 kV"]
[null,null,"> 132 kV"]
[null,null,"Other"]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",673094.84788269363,690308.67164875939,685854.39709933219,688162.90983058244,690075.85042252683,691363.43107183708,695948.81598020124]
[null,null,"> 1 kV & < = 11 kV",849327.2086690258,871048.0239980137,865427.51363218506,868340.45031618618,870754.24459557573,872378.94471362734,878164.89327220665]
[null,null,"˃ 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 66 kV",90904.51833581664,93229.323470032366,92627.753448028976,92939.528584276894,93197.87990528722,93371.773523864525,93991.05059572203]
[null,null,"> 66 kV & < = 132 kV"]
[null,null,"> 132 kV"]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",11654258.563731311,11952306.236613212,12816171.846916467,12859309.714078398,12895055.749188749,12919116.037987823,13004800.523234829]
[null,null,"> 1 kV & < = 11 kV",4345372.663871102,4456501.8449501898,4527736.4584392766,4542976.3363233553,4555604.8051319048,4564104.8976788344,4594375.7751615522]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",197.22055150795657,202.26429805776812,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase"]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase"]
[null,null,"> 22 kV & < = 66 kV",4126312.2412867434,4780596.0493820794,1308272.3934281575,1312828.5498230252,1316324.8472233634,1318780.9169444719,1327527.5729610056]
[null,null,"> 66 kV & < = 132 kV",1938.734642714129,1988.3161193423139,0,0,0,0,0]
[null,null,"> 132 kV"]
[null,null,"Other"]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",985865.46270349203,1011078.1268405177,1004554.0605020324,1007935.2823002825,1010737.1193188453,1012623.0070159407,1019339.1074712898]
[null,null,"> 1 kV & < = 11 kV",4433198.8848528219,4066664.42805618,2000361.2418674403,2007094.244401915,3827070.5106619471,3818411.568436373,2910696.3783796579]
[null,null,"> 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 33 kV",513956.51377343107,527100.51105605369,523699.35083916207,525462.06698397745,3308504.0360173662,3290455.3223178778,1881871.0857494315]
[null,null,"> 33 kV & < = 66 kV"]
[null,null,"> 66 kV & < = 132 kV",3647.1220900887092,0,0,0,0,0,0]
[null,null,">  132 kV"]
[null,null,"Other"]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",7505566.2363754893,7184016.6142010475,6626881.2352663791,6649186.6105250288,6667669.8777703065,6680110.7749634907,6724415.8072476406]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",652657.93359786877,669349.10079936893,576250.54219707649,578190.14004565473,579797.38067567884,580879.19782291225,584731.80932588188]
[null,null,"˂ = 11 kV ; Residential ; Complex Type"]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type"]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type"]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  "]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  "]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  "]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  "]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  "]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  "]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  "]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  "]
[null,null,"> 132 kV ; Commercial & Industrial  "]
[null,null,"> 132 kV ; Subdivision  "]
[null,null,"Other"]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",1187391.9750746021,1217758.5070194986,1287422.2230236444,1291755.5488795608,1295346.3434269296,1297763.2703269655,1306370.5293269982]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",19004.635679389161,19490.662946352146,19364.897810436869,19430.077990550635,19484.089307292365,19520.443769408583,19649.910767867048]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase"]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",3570207.1763262297,3661512.1645235745,3915930.6330439644,3929111.2377893841,3940033.2974785394,3947384.8235873939,3973565.3792605833]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",11311730.417304276,11601018.226452172,12259249.739872085,12300513.066636134,12334705.770733925,12357720.528395141,12439681.625360938]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",2156631.674873576,2211785.6813206123,2197513.9488714701,2204910.5463847681,2211039.7097348012,2215165.1865840028,2229857.00359311]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",312455.44919949252,320446.22947984369,318378.5233317769,319450.15147555852,320338.15219912387,320935.85635839106,323064.42487410968]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",309478.11388304585,317392.75136481371,315344.74804015562,316406.16481995961,317285.7039342873,317877.71267135354,319985.99841641937]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",1558812.6228035334,517769.86187297059,291016.44010676746,291995.97039749805,292807.65457355324,293353.99084914959,295299.62595507747]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",5225885.3059660485,2556843.4113675272,2396541.1114226445,5672906.1768461652,6584679.4611355197,7162482.4101967551,7784431.7284171619]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",117087.17902726293,214940.33887331351,495626.58251033333,873063.43047064834,2716939.5167232943,5344364.1506190272,622055.81937299517]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA"]
[null,null,"Other"]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",17258184.155798435,17716070.482572824,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",6991125.4815394515,8592226.4611354023,18245188.378852569,18306773.021470983,18357623.299333207,18395254.682345074,18512827.544580903]
[null,null,"˂ = 11 kV ;  Circuit Breaker",1320335.6359804964,1354102.0880954079,7110367.0255618412,12614317.017709084,11832425.991925208,11585671.75099887,10670697.551696155]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,2368743.8062937721,2376716.7452397435,2383323.4918001508,2387770.4249991747,2403607.0255183186]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",10371.596516664815,45249.282175115484,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",1536361.7383826773,2575102.742496381,52935.916557721917,6605.6866497682786,17362.20118828175,36619.619515730526,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,3081907.8822091003,2362999.8233631956,2782010.6659708964,3653294.4825134519,2220154.1695649652]
[null,null,"> 33 kV & < = 66 kV ; Switch"]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker"]
[null,null,"> 66 kV & < = 132 kV ; Switch",40549.285292179004,154165.63768122598,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,346640.82903937501,237519.937751102,407793.36655589135,540161.65817523794,362406.12272619025]
[null,null,"> 132 kV ; Switch"]
[null,null,"> 132 kV ; Circuit Breaker"]
[null,null,"Other"]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",7363474.1569255479,6401055.4561297968,9764517.5832963418,15771812.53635223,14762919.188117698,14073065.673843095,10700375.001225593]
[null,null,"Local Network Wiring Assets"]
[null,null,"Communications Network Assets",5934973.1520282477,4081054.5662443582,2061961.9555942069,5584381.4733278966,6100455.2136661448,5376002.0995463608,5907331.6918704053]
[null,null,"Master Station Assets"]
[null,null,"Communications Site Infrastructure",0,0,746784.77343026607,1905095.072337043,2163682.7571796305,1965219.9801068329,2120577.7011661427]
[null,null,"Communications Linear Assets"]
[null,null,"AFLC",55483.396472465582,189326.95928404736,256099.11521117526,949337.06811506522,1209554.8916879713,938990.8880015061,612345.48313012684]
[null,null,"Other"]
[null,"OTHER: ","CURRENT TRANSFORMERS",679479.84967294743,263111.60711771785,1143382.8339970466,1160103.3397994069,578527.09344448405,723394.17048691271,533554.60500048671]
[null,null,"VOLTAGE TRANSFORMERS",152514.07709563361,277677.9213900278,133655.11266935754,570485.09738942678,180100.4126792211,335409.60699178715,235907.94526394317]
[null,null,"OTHER",7735202.1274674423,4006553.5907564876,4585178.0895857066,5611997.073436806,4670207.5961850388,10660303.933400387,4252126.4096848732]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",1806,1806,1862,1862,1862,1862,1862]
[null,null,"> 1 kV & < = 11 kV; Wood"]
[null,null,"˃ 11 kV & < = 22 kV; Wood",193,193,199,199,199,199,199]
[null,null,"> 22 kV & < = 66 kV; Wood",23,23,24,24,24,24,24]
[null,null,"> 66 kV & < = 132 kV; Wood"]
[null,null,"> 132 kV; Wood"]
[null,null,"˂ = 1 kV; Concrete",41,41,42,42,42,42,42]
[null,null,"> 1 kV & < = 11 kV; Concrete"]
[null,null,"˃ 11 kV & < = 22 kV; Concrete"]
[null,null,"> 22 kV & < = 66 kV; Concrete"]
[null,null,"> 66 kV & < = 132 kV; Concrete"]
[null,null,"> 132 kV; Concrete"]
[null,null,"˂ = 1 kV; Steel"]
[null,null,"> 1 kV & < = 11 kV; Steel"]
[null,null,"˃ 11 kV & < = 22 kV; Steel"]
[null,null,"> 22 kV & < = 66 kV; Steel"]
[null,null,"> 66 kV & < = 132 kV; Steel"]
[null,null,"> 132 kV; Steel"]
[null,null,"Other"]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",5936.2404736956723,5936.2404736956723,6090.47075568322,6090.47075568322,6090.47075568322,6090.47075568322,6090.47075568322]
[null,null,"> 1 kV & < = 11 kV",5446.0584196188483,5446.0584196188483,5586.5214782289231,5586.5214782289231,5586.5214782289231,5586.5214782289231,5586.5214782289231]
[null,null,"˃ 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 66 kV",190.3062362191277,190.3062362191277,192.09875265355609,192.09875265355609,192.09875265355609,192.09875265355609,192.09875265355609]
[null,null,"> 66 kV & < = 132 kV"]
[null,null,"> 132 kV"]
[null,null,"Other"]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",584.92743590820714,584.92743590820714,584.92743590820714,584.92743590820714,584.92743590820714,584.92743590820714,584.92743590820714]
[null,null,"> 1 kV & < = 11 kV",738.0754554526452,738.0754554526452,738.0754554526452,738.0754554526452,738.0754554526452,738.0754554526452,738.0754554526452]
[null,null,"˃ 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 66 kV",78.997108639147825,78.997108639147825,78.997108639147825,78.997108639147825,78.997108639147825,78.997108639147825,78.997108639147825]
[null,null,"> 66 kV & < = 132 kV"]
[null,null,"> 132 kV"]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",104.37899999999999,104.37899999999999,111.13112068567203,111.13112068567203,111.13112068567203,111.13112068567203,111.13112068567203]
[null,null,"> 1 kV & < = 11 kV",169.40833880891404,169.40833880891404,180.97078722662422,180.97078722662422,180.97078722662422,180.97078722662422,180.97078722662422]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",2.9666666666666664E-2,2.9666666666666664E-2,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase"]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase"]
[null,null,"> 22 kV & < = 66 kV",7.692080093674333,11.792080093674333,7.898092087703767,7.898092087703767,7.898092087703767,7.898092087703767,7.898092087703767]
[null,null,"> 66 kV & < = 132 kV",2.0900000733333336E-3,2.0900000733333336E-3,0,0,0,0,0]
[null,null,"> 132 kV"]
[null,null,"Other"]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",3.1323466682433332,3.1323466682433332,3.1323466682433332,3.1323466682433332,3.1323466682433332,3.1323466682433332,3.1323466682433332]
[null,null,"> 1 kV & < = 11 kV",1.4085633370083332,1.4085633370083332,1.4085633370083332,1.4085633370083332,1.4085633370083332,1.4085633370083332,11.408563337008333]
[null,null,"> 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 33 kV",0.4482933464053333,0.4482933464053333,0.4482933464053333,0.4482933464053333,0.4482933464053333,0.4482933464053333,5.4482933464053334]
[null,null,"> 33 kV & < = 66 kV"]
[null,null,"> 66 kV & < = 132 kV",0.01,0,0,0,0,0,0]
[null,null,">  132 kV"]
[null,null,"Other"]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",8269.264297792959,8569.264297792959,7361.27445659162,7361.27445659162,7361.27445659162,7361.27445659162,7361.27445659162]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",719.06646067764859,719.06646067764859,640.11082231231489,640.11082231231489,640.11082231231489,640.11082231231489,640.11082231231489]
[null,null,"˂ = 11 kV ; Residential ; Complex Type"]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type"]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type"]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  "]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  "]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  "]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  "]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  "]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  "]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  "]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  "]
[null,null,"> 132 kV ; Commercial & Industrial  "]
[null,null,"> 132 kV ; Subdivision  "]
[null,null,"Other"]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",84.699137829777044,84.699137829777044,90.126025763363259,90.126025763363259,90.126025763363259,90.126025763363259,90.126025763363259]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",1.1253916618436546,1.1253916618436546,1.1253916618436546,1.1253916618436546,1.1253916618436546,1.1253916618436546,1.1253916618436546]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase"]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",136.38116962104675,136.38116962104675,146.80482213083303,146.80482213083303,146.80482213083303,146.80482213083303,146.80482213083303]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",341.55999978968703,341.55999978968703,363.28393209211924,363.28393209211924,363.28393209211924,363.28393209211924,363.28393209211924]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",30.573140146752618,30.573140146752618,30.573140146752618,30.573140146752618,30.573140146752618,30.573140146752618,30.573140146752618]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",3.3761749855309637,3.3761749855309637,3.3761749855309637,3.3761749855309637,3.3761749855309637,3.3761749855309637,3.3761749855309637]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",1.8756527697394243,1.8756527697394243,1.8756527697394243,1.8756527697394243,1.8756527697394243,1.8756527697394243,1.8756527697394243]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",4.8766972013225027,4.8766972013225027,4.8766972013225027,4.8766972013225027,4.8766972013225027,4.8766972013225027,4.8766972013225027]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0,0,1,2,2,4,8]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",1,0,0,0,0,2,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA"]
[null,null,"Other"]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse"]
[null,null,"˂ = 11 kV  ; Switch",2110.5733771381874,2110.5733771381874,2221.2730820178281,2224.2730820178281,2224.2730820178281,2222.2730820178281,2226.2730820178281]
[null,null,"˂ = 11 kV ;  Circuit Breaker",29.281379950962918,29.281379950962918,50.59296751987565,73.592967519875657,88.592967519875657,63.59296751987565,157.59296751987566]
[null,null,"> 11 kV & < = 22 kV  ; Switch",59.666666666666664,59.666666666666664,105.05333934194232,105.05333934194232,105.05333934194232,105.05333934194232,105.05333934194232]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker"]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,8,0,0,4,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,11,12,22,6,39]
[null,null,"> 33 kV & < = 66 kV ; Switch"]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker"]
[null,null,"> 66 kV & < = 132 kV ; Switch"]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,4,0,5]
[null,null,"> 132 kV ; Switch"]
[null,null,"> 132 kV ; Circuit Breaker"]
[null,null,"Other"]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",44,8,28,86,186,65,406]
[null,null,"Local Network Wiring Assets"]
[null,null,"Communications Network Assets",7,5,1,0,0,0,9]
[null,null,"Master Station Assets"]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,3]
[null,null,"Communications Linear Assets"]
[null,null,"AFLC",0,0,0,0,2,1,3]
[null,null,"Other"]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"CURRENT TRANSFORMERS",0,0,0,0,23,0,21]
[null,null,"VOLTAGE TRANSFORMERS",0,0,1,0,23,0,20]
[null,null,"OTHER",1,2,0,2,1,2,5]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C177),\"\",C177)","v":""}]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",4,2,2,2,2,2,2]
[null,null,"> 1 kV & < = 11 kV; Wood",8,5,5,5,5,5,5]
[null,null,"˃ 11 kV & < = 22 kV; Wood"]
[null,null,"> 22 kV & < = 66 kV; Wood"]
[null,null,"> 66 kV & < = 132 kV; Wood"]
[null,null,"> 132 kV; Wood"]
[null,null,"˂ = 1 kV; Concrete"]
[null,null,"> 1 kV & < = 11 kV; Concrete"]
[null,null,"˃ 11 kV & < = 22 kV; Concrete"]
[null,null,"> 22 kV & < = 66 kV; Concrete"]
[null,null,"> 66 kV & < = 132 kV; Concrete"]
[null,null,"> 132 kV; Concrete"]
[null,null,"˂ = 1 kV; Steel"]
[null,null,"> 1 kV & < = 11 kV; Steel"]
[null,null,"˃ 11 kV & < = 22 kV; Steel"]
[null,null,"> 22 kV & < = 66 kV; Steel"]
[null,null,"> 66 kV & < = 132 kV; Steel"]
[null,null,"> 132 kV; Steel"]
[null,null,"Other"]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",107,110,113,114,116,118,120]
[null,null,"> 1 kV & < = 11 kV",66,68,69,71,72,73,74]
[null,null,"˃ 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 66 kV",8,8,8,9,9,9,9]
[null,null,"> 66 kV & < = 132 kV"]
[null,null,"> 132 kV"]
[null,null,"Other"]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv"]
[null,null,"> 1 kV & < = 11 kV"]
[null,null,"˃ 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 66 kV"]
[null,null,"> 66 kV & < = 132 kV"]
[null,null,"> 132 kV"]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",154,120,120,124,127,130,133]
[null,null,"> 1 kV & < = 11 kV",64,50,50,51,53,54,56]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER"]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase"]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase"]
[null,null,"> 22 kV & < = 66 kV",25,20,20,20,21,22,22]
[null,null,"> 66 kV & < = 132 kV",1,1,1,1,1,1,1]
[null,null,"> 132 kV"]
[null,null,"Other"]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",77,77,77,77,77,77,77]
[null,null,"> 1 kV & < = 11 kV",43,43,43,43,43,43,43]
[null,null,"> 11 kV & < = 22 kV"]
[null,null,"> 22 kV & < = 33 kV",6,6,6,6,6,6,6]
[null,null,"> 33 kV & < = 66 kV"]
[null,null,"> 66 kV & < = 132 kV",1,1,1,1,1,1,1]
[null,null,">  132 kV"]
[null,null,"Other"]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",1626.625412248809,1701.5826972120587,1777.4796829661896,1854.0096072702656,1930.9336332978419,2008.0382759701647,2085.1260877800632]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type"]
[null,null,"˂ = 11 kV ; Residential ; Complex Type"]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type"]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type"]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  "]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  "]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  "]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  "]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  "]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  "]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  "]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  "]
[null,null,"> 132 kV ; Commercial & Industrial  "]
[null,null,"> 132 kV ; Subdivision  "]
[null,null,"Other"]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",5,5,5,5,5,5,5]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",1,1,0,1,1,0,1]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase"]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",3,3,3,3,3,3,3]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",20,20,20,20,20,20,20]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase"]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",1,1,0,1,1,0,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",1,0,0,1,0,0,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",1,1,0,1,1,0,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",1,1,0,1,1,0,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",1,1,1,1,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA"]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA"]
[null,null,"Other"]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse"]
[null,null,"˂ = 11 kV  ; Switch",38,40,42,43,45,47,46]
[null,null,"˂ = 11 kV ;  Circuit Breaker",18,18,18,18,18,18,18]
[null,null,"> 11 kV & < = 22 kV  ; Switch"]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker"]
[null,null,"> 22 kV & < = 33 kV ; Switch",1,0,0,1,0,0,1]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",5,5,5,5,5,5,5]
[null,null,"> 33 kV & < = 66 kV ; Switch"]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker"]
[null,null,"> 66 kV & < = 132 kV ; Switch"]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",1,1,0,1,1,0,1]
[null,null,"> 132 kV ; Switch"]
[null,null,"> 132 kV ; Circuit Breaker"]
[null,null,"Other"]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",93,93,93,93,93,93,93]
[null,null,"Local Network Wiring Assets",11,11,11,11,11,11,11]
[null,null,"Communications Network Assets",41,41,41,41,41,41,41]
[null,null,"Master Station Assets",4,4,4,4,4,4,4]
[null,null,"Communications Site Infrastructure",31,31,31,31,31,31,31]
[null,null,"Communications Linear Assets",65,65,65,65,65,65,65]
[null,null,"AFLC",20,20,20,20,20,20,20]
[null,null,"Other"]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"CURRENT TRANSFORMERS"]
[null,null,"VOLTAGE TRANSFORMERS"]
[null,null,"OTHER"]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C177),\"\",C177)","v":""}]

{"sheet":"2.3 Augex (b)","index":5,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[68,1,69,2],[60,1,61,2],[45,1,46,2],[6,1,6,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.3 AUGEX PROJECT DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,null,null,"VOLUMES"]
[null,"PROJECT TYPE","UNITS",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",19.829999999999998,21.434072604572137,33.6427576424013,28.0382185162326,33.6427576424013,44.853335527002926,49.853335527002926]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",9.5,9.5,9.5,9.5,9.5,9.5,9.5]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",2.5,2.5,2.5,2.5,2.5,2.5,2.5]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",52,52,52,52,52,52,52]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",3,3,3,3,3,3,3]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",54,55,66,64,66,79,84]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",4.8,4.8,4.8,4.8,4.8,4.8,4.8]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",20.94,20.94,20.94,20.94,20.94,20.94,20.94]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.9,0.9,0.9,0.9,0.9,0.9,0.9]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",306,306,306,306,306,306,306]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",12,12,12,12,12,12,12]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,"PROJECT TYPE",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,3945557.4879901204,4853376.3891024711,5283294.478994837,5170100.3342505405,5297753.2300057439,5729586.0185436262,6338896.0715290047]
[null,"HV Feeder Augmentations - Underground Cables",null,2721134.0989815448,3347229.8978733635,3643731.6666946462,3565665.0188238891,3653703.4388774685,3951525.7186251413,4371748.8092980292]
[null,"HV Feeder Non-Material Projects",null,22300532.891828958,27431580.994841851,29861504.40455519,29221724.156588636,29943226.151982516,32383971.555863291,35827829.342572212]
[null,"LV Feeder Augmentations - Overhead Lines",null,2226222.5499654766,1856702.0801150554,1096987.8874389373,989617.67426185426,1242604.0909993234,1249063.9035079179,1001111.6056554457]
[null,"LV Feeder Augmentations - Underground Cables",null,335269.62750565779,279619.75984782295,165206.62788433908,149036.6491112636,187136.46159626325,188109.31084421757,150767.63781990137]
[null,"LV Feeder Non-Material Projects",null,2603470.5220673257,2171332.391685456,1282879.6600126401,1157314.8619384512,1453171.4816953819,1460725.9516851271,1170756.5151848185]
[null,"Distribution Substation Augmentations - Pole Mounted",null,11001068.712722123,13087898.108619936,11374138.066113021,11528361.135667462,11438628.303329328,11498464.12226733,11515639.028181031]
[null,"Distribution Substation Augmentations - Ground Mounted",null,1663110.8712984691,1978591.9164126844,1719510.4551548243,1742825.4684757025,1729259.9092676803,1738305.7214126175,1740902.1757648729]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,15409460.224697838,16520060.20823703,17480439.303438388,17650856.389039956,14279498.365178337,14649543.074615749,27396565.355664458]
[null,"Subtransmission Lines",null,2305866.6303460076,20590271.683191698,37191859.312805437,28509761.060445204,30665764.904609241,23130029.040102419,33919065.916313663]
[null,"HV Feeders",null,28967224.478800625,35632187.281817682,38788530.550244667,37957489.509663068,38894682.820865728,42065083.293032058,46538474.223399244]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,12664179.58402059,15349005.036146851,13093648.521267848,13271186.604143165,13167888.212597011,13236769.843679946,13256541.203945905]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,5164962.69953846,4307654.2316483343,2545074.1753359162,2295969.1853115689,2882912.0342909684,2897899.1660372629,2322635.7586601656]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,3721412.8012989326,6285869.8578893915,18782135.330106642,20953191.336949293,15660131.860112838,13500745.546113245,13337595.850351095]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,3569647.7063113777,26579230.157342967,48972584.717602268,30376198.559365671,6134781.2061935673,14690137.254633062,27356512.319525078]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,64663457.593361013,72105818.141588017,78909102.475596622,90262255.526186571,109416096.99146055,94789932.708947673,109414365.98880945]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,1389915.9064265578,8940573.8122273684,11160941.795139501,7120746.4280158347,3368256.8434993876,5390898.9546244275,10980338.650325948]
[null,"Subtransmission Lines",null,1965081.6915666792,15858821.388248637,35527778.55662743,21811041.639949981,2321165.73064778,7406476.1874290397,11093409.045126924]
[null,"HV Feeders",null,187354.72706040621,1585655.2979657257,1837028.3288001192,1177295.5799639039,442412.94969775382,1892762.1125795946,5282764.6240722071]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,3978.1518682865512,27.412792645096594,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,23317.229389447781,194152.24610859019,446836.03703521669,267114.91143594915,2945.6823486452186,0,0]

{"sheet":"2.5 Connections","index":6,"n_rows":212,"n_cols":17,"rows_kept":212,"cut":false,"hidden":false,"merged":[[11,16,11,93],[12,16,12,93],[139,1,140,1],[139,2,140,3],[103,1,104,1],[103,2,104,2],[103,3,104,3],[121,1,122,1],[121,2,122,3],[6,1,6,2],[10,1,11,1],[10,2,11,2],[10,3,11,3],[55,1,56,1],[55,2,56,2],[55,3,56,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.5 CONNECTIONS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,null,null,null,null,"DRAFT TEMPLATE ONLY"]
[null,"RESIDENTIAL","Underground connections","0's",22380.621919999998,22482.863870720001,22993.349692651522,23515.083287733942,24051.068620337683,24598.309718263088,25158.810673755295,null,null,null,null,null,"DO NOT USE FOR SUBMISSIONS"]
[null,null,"Overhead connections","0's",17569.218399999998,17679.341894399997,18063.283364710398,18456.055898545765,18857.672792922494,19268.147557609256,19688.493918531003]
[null,null,"Distribution substations installed","MVA added",7.7148530144690906,7.7735673757942392,8.0065677434651406,8.206462860900583,8.4201103352158206,8.6425405400527282,8.777019100873293]
[null,null,"Distribution substations installed","0's",90.879190439328596,91.57083208361972,94.315522714314085,96.670241127125948,99.186959134424526,101.80713568307952,103.39126213576736]
[null,null,"Distribution substations installed ","total spend $0s",3023247.3797790948,3189730.0873807548,3241099.9910819842,3328614.2515795222,3422008.5055615306,3522947.1922824001,3587593.961973717]
[null,null,"Augmentation HV ","net circuit KM added",3.249918875493381,3.2746525821207491,3.3728051057618842,3.4570118837852641,3.5470119081767022,3.640711699970995,3.6973614394203751]
[null,null,"Augmentation HV","total spend $0s",1414107.3904865761,1491978.7644212241,1516006.7553022748,1556941.0709557885,1600625.7213315009,1647839.2387673189,1678077.4109403994]
[null,null,"Augmentation LV","net circuit KM added",56.216681825023805,56.644522324769554,58.342352148604512,59.7989502450515,61.355759177609791,62.976566214391916,63.95648617550566]
[null,null,"Augmentation LV","total spend $0s",19562979.015697248,20640263.573048193,20972670.492464416,21538962.107612595,22143302.276087407,22796461.333926957,23214780.855962317]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",15.252000000000001,15.007968,14.767840511999999,14.531555063808,14.299050182787072,14.070265379862478,13.845141133784679]
[null,null,"Volume of GSL breaches for residential customers","0's",203.68799999999999,200.42899199999999,197.22212812799998,194.06657407795197,190.96150889270473,187.90612475042144,184.8996267544147]
[null,null,"Volume of customer complaints relating to connection services","0's",553.99199999999996,545.12812799999995,536.40607795199992,527.82358070476789,519.37840341349158,511.06834895887573,502.89125537553372]
[null,null,"GSL payments","$",55566.0864,53434.369267199996,51356.6421645312,49331.723130615384,47358.454205390772,45435.7009646519,43562.352063340106]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1748.73216,1598.75187456,1633.81990455296,1669.9370230258073,1707.1040153942201,1745.3216796405277,1784.5908265147762]
[null,null,"Overhead connections","0's",1392.9780000000001,1308.3216480000001,1334.7827943679999,1362.363319077888,1391.0651321831342,1418.8901742980643,1448.8404170868334]
[null,null,"Distribution substations installed","MVA added",102.59270341304726,94.815231068941387,97.720924629439921,100.22561643208992,102.90128109597256,105.68742947289429,107.40041307370815]
[null,null,"Distribution substations installed","0's",186.21278359217484,172.09613858403748,177.37017141644921,181.916358592492,186.77287322214201,191.82992335833555,194.93910592145662]
[null,null,"Distribution substations installed ","total spend $0s",39768793.34155301,38585873.561483882,39207960.815393887,40295722.515103206,41456012.047537237,42711050.09562888,43526797.131276384]
[null,null,"Augmentation HV ","net circuit KM added",24.12568139621888,22.296732420321838,22.980034787288396,23.569037654121615,24.198246467774386,24.853436611205751,25.256261521899429]
[null,null,"Augmentation HV","total spend $0s",33133415.063763801,32147864.11371237,32666156.811523262,33572426.699507907,34539123.233197004,35584759.599658921,36264400.163228713]
[null,null,"Augmentation LV","net circuit KM added",26.386000090136474,24.385698127662664,25.133018629010063,25.77720477414368,26.46536373392993,27.181938196624532,27.622503499436597]
[null,null,"Augmentation LV","total spend $0s",5112199.9818840828,4960137.9762229482,5040106.0662993994,5179935.6883296408,5329088.6202716772,5490421.2871095743,5595283.9603378763]
[null,"SUBDIVISION","Underground connections","0's",13497,13466,13964,13956,14113,14335,14461]
[null,null,"Overhead connections","0's",96,96,100,100,101,102,103]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",8.4921631935472899,8.2642834236273632,8.2695570296551963,8.3760738653341686,8.4240355585629789,8.4069705421193976,8.4109525519717483]
[null,null,"Augmentation HV","total spend $0s",4287123.380468593,4381828.4321587794,4320492.4326297995,4384476.1741209663,4417342.7641033884,4420066.3838018915,4433346.3815279007]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Cost per lot","$",385.09793486074096,386.85718731668914,395.64099307973811,404.61833654820367,413.84090620865163,423.25715109386073,432.90155513317086]
[null,"EMBEDDED GENERATION","Underground connections","0's",22176.232,22531.051712,22891.548539391999,23257.813316022271,23629.938329078628,24008.017342343886,24392.145619821389]
[null,null,"Overhead connections","0's",16137.128000000001,16395.322048000002,16657.647200768002,16924.16955598029,17194.956268875976,17470.075569177992,17749.596778284838]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",23232.006694515498,23303.423218766675,23669.815755571159,23922.447646601646,24199.463563841979,24485.309158270982,24509.614846847704]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Underground connections","0's",21428,21515,22010,22516,23036,23567,24111]
[null,null,"Overhead connections","0's",14374,14433,14765,15105,15453,15809,16174]
[null,null,"Distribution substations installed","MVA added",4.6928160503514018,4.726275686940185,4.911039451996877,5.0777610188084603,5.2549603124149691,5.4397054748865328,5.5708502946554264]
[null,null,"Distribution substations installed","0's",55.280291502218823,55.674438309666712,57.850912878836454,59.81485451093193,61.902221349830619,64.078476784834962,65.623332536273921]
[null,null,"Distribution substations installed ","total spend $0s",1797594.5878712614,1941856.3676521087,1964884.5423179786,2044522.1635524943,2125994.5134709533,2214141.2390839281,2281544.1937000188]
[null,null,"Augmentation HV ","net circuit KM added",1.9768712939380424,1.9909663265087334,2.0687989496888255,2.1390312102278917,2.213677263488508,2.2915020502402932,2.3467474352645779]
[null,null,"Augmentation HV","total spend $0s",840815.01527445694,908292.67202107387,919063.9744960973,956314.03530876164,994422.28040659404,1035652.4281511058,1067179.7907152006]
[null,null,"Augmentation LV","net circuit KM added",34.195667275992093,34.43948135003405,35.785820129723724,37.000688806708013,38.291906706726756,39.638109932879985,40.593737550427704]
[null,null,"Augmentation LV","total spend $0s",11631964.170866489,12565460.44692249,12714472.301119862,13229795.368458372,13756990.68911745,14327374.890887618,14763529.270965811]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",15.252000000000001,15.007968,14.767840511999999,14.531555063808,14.299050182787072,14.070265379862478,13.845141133784679]
[null,null,"Volume of GSL breaches for residential customers","0's",203.68799999999999,200.42899199999999,197.22212812799998,194.06657407795197,190.96150889270473,187.90612475042144,184.8996267544147]
[null,null,"Volume of customer complaints relating to connection services","0's",553.99199999999996,545.12812799999995,536.40607795199992,527.82358070476789,519.37840341349158,511.06834895887573,502.89125537553372]
[null,null,"GSL payments","$",55566.0864,53434.369267199996,51356.6421645312,49331.723130615384,47358.454205390772,45435.7009646519,43562.352063340106]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1560,1407,1439,1472,1506,1541,1577]
[null,null,"Overhead connections","0's",934,842,861,881,902,922,944]
[null,null,"Distribution substations installed","MVA added",68.179461827817107,60.367149360960141,62.727075556651812,64.856554747469815,67.119862462116913,69.479551053168208,71.154620271999633]
[null,null,"Distribution substations installed","0's",123.75039304364064,109.57051082640028,113.85393851036119,117.71908909643497,121.82714761959579,126.11014403486011,129.15050939780758]
[null,null,"Distribution substations installed ","total spend $0s",25859003.303210866,24558323.333518993,24849556.695906647,25856719.987882901,26887086.777810998,28001863.248643279,28854296.817196999]
[null,null,"Augmentation HV ","net circuit KM added",16.033069790559733,14.195927817760039,14.750887630902147,15.251655568468935,15.783894597255813,16.338798535334085,16.732707506885774]
[null,null,"Augmentation HV","total spend $0s",21544457.791865859,20460794.806901839,20703436.211521052,21542555.445122946,22401006.699235659,23329783.974275842,24039989.964148425]
[null,null,"Augmentation LV","net circuit KM added",17.535197202976253,15.52593464728804,16.132888268166276,16.680572813475973,17.262676955154042,17.869569466071688,18.300383501462928]
[null,null,"Augmentation LV","total spend $0s",3324123.8949054978,3156924.0490266411,3194361.5236096717,3323830.3792215297,3456281.9987505688,3599584.3163504079,3709162.9710581531]
[null,"SUBDIVISION","Underground connections","0's",9355,9334,9679,9674,9782,9936,10024]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",5.5836168855401986,5.3382111950657425,5.3057325087178855,5.3840311035853379,5.4028979232272905,5.3577181826490632,5.362594929544894]
[null,null,"Augmentation HV","total spend $0s",2757673.2225065515,2827891.7036159257,2737019.7635914022,2795091.9217116558,2818307.853042393,2811763.376780082,2831726.8592949882]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Cost per lot","$",0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL SERVICE CLASSIFICATIONS (including capcons)"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,18751728.788330942,19794295.950473312,20113152.137303531,20659421.135852017,21242332.312635437,21872443.001376025,22277309.677514713]
[null,null,"Complex connection LV",null,1065224.6711842045,1121863.3060570091,1139915.7737451617,1170048.5761849706,1202218.3663530617,1236964.1844199721,1258951.7571934378]
[null,null,"Complex connection HV",null,4183380.3264477747,4405813.1683198502,4476709.327799987,4595047.7181109227,4721385.8239919432,4857840.5791806821,4944190.794168286]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,5915127.3096886165,6026723.9180961568,6124095.2792690778,6303009.8987544961,6493685.7154156882,6700239.5849470282,6838096.6841468643]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,61908889.313723996,59820513.062035754,60784770.097385794,62463407.807229534,64254115.111600339,66190786.339919731,67446487.308675379]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,2734942.7554362826,2642684.7685220549,2685282.6542609688,2759439.6629624888,2838547.5588314924,2924103.6882382571,2979576.6632110327]
[null,null,"Complex connection HV (customer connected at HV)",null,7455449.0083519965,7203953.9027652219,7320075.6623007022,7522227.5339942286,7737875.5151583888,7971101.369292343,8122320.5988096856]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,1390126.6502911947,1394399.9795364107,1416323.7004003492,1431440.3594583827,1448016.0782145916,1465120.1357292568,1466574.5079618611]
[null,null,"Complex connection HV (with upstream asset works)",null,2896996.7301773983,2987428.4526223685,2904168.7322294507,2953035.8146625832,2969326.6858887966,2954946.2480726345,2966771.8735660398]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,23232.006694515498,23303.423218766675,23669.815755571159,23922.447646601646,24199.463563841979,24485.309158270982,24509.614846847704]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES (excluding capcons)"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,11263459.501844227,12167382.291325785,12311673.398175176,12810670.851577846,13321164.441188255,13873478.673140662,14295815.530820025]
[null,null,"Complex connection LV",null,610264.87386540801,659240.26433196117,667058.09278039914,694094.24609635666,721753.27092986228,751678.17766400694,774560.78749966261]
[null,null,"Complex connection HV",null,2396649.3983025737,2588986.9309379281,2619689.3269783626,2725866.4696454275,2834489.7708768812,2952011.7073179842,3041876.9370613433]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,4088436.5254446827,4166551.4205437764,4215961.9101479193,4386836.6717476118,4561648.1258502817,4750780.4792709854,4895403.8824138669]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,40047249.248896696,37789262.972487688,38237400.004001059,39787178.381777376,41372661.277084269,43088030.060193561,44399717.175440803]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,1769163.288544754,1669412.4566852916,1689209.7611009681,1757674.164094086,1827715.8819548921,1903495.5555732059,1961441.8248894815]
[null,null,"Complex connection HV (customer connected at HV)",null,4822735.9270960931,4550815.3397307163,4604782.7557874201,4791416.5946083078,4982350.1909077726,5188925.4442317756,5346886.8696594201]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,2757673.2225065515,2827891.7036159257,2737019.7635914022,2795091.9217116558,2818307.853042393,2811763.376780082,2831726.8592949882]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,569053.89423881832,686428.20097905619,751870.16845403006,723900.0656451073,713813.68216803018,706476.41534867336,681767.24250041659]
[null,null,"Complex connection LV",null,30831.877447014453,37191.328243294469,40737.035849388325,39221.589262139089,38675.099479014389,38277.559432876827,36938.793110763181]
[null,null,"Complex connection HV",null,121083.81736587184,146058.83162140436,159983.63438266548,154032.1298687557,151885.93980277923,150324.70933846958,145067.06853729012]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,206556.49587691802,235057.8232369289,257467.51794508484,247889.54391575276,244435.6016956151,241923.05637098147,233461.74260879616]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,2023272.0803857716,2131897.8213597946,2335146.4461779534,2248277.3444182905,2216951.214563034,2194163.2476283833,2117421.8904293822]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,89381.886508839132,94180.634905459854,103159.52889242698,99321.921350723278,97938.030073505724,96931.328357969876,93541.133165641833]
[null,null,"Complex connection HV (customer connected at HV)",null,243654.86107977168,256736.24053599712,281212.68931656878,270751.37809374026,266978.89297320513,264234.62591610523,254992.95994904923]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,139323.50767084662,159536.74900644278,167148.96863804839,157943.89295092737,151018.83284640373,143182.87129255265,135045.01427105142]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,39436,39645,40528,41431,42357,43302,44270]
[null,null,"Complex connection LV",null,77,77,79,80,82,84,86]
[null,null,"Complex connection HV",null,438,440,450,460,470,480,491]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1292,1195,1220,1247,1274,1301,1329]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1369,1267,1294,1322,1350,1379,1409]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,374,346,353,361,369,377,385]
[null,null,"Complex connection HV (customer connected at HV)",null,107,99,101,103,105,107,110]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,13593,13562,14064,14056,14214,14437,14564]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,38303,38916,39539,40171,40814,41467,42131]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,10,10,10,11,11,11,11]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,35341,35485,36302,37137,37994,38869,39767]
[null,null,"Complex connection LV",null,69,69,70,72,74,75,77]
[null,null,"Complex connection HV",null,392,394,403,412,422,431,441]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1025,925,946,967,990,1013,1036]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1087,980,1003,1026,1050,1074,1099]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,297,268,274,280,287,293,300]
[null,null,"Complex connection HV (customer connected at HV)",null,85,76,78,80,82,84,86]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,13593,13562,14064,14056,14214,14437,14564]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,1442592,1463411,1482989,1502496,1523060,1543233,1579852]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,123625,124673,126170,127996,130195,132452,134444]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,775,781,781,781,781,781,781]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,573186,626311,678186,730479,787030,842682,895030]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,15,15,15,15,15,15,15]

{"sheet":"2.6 Non-network","index":7,"n_rows":112,"n_cols":11,"rows_kept":112,"cut":false,"hidden":false,"merged":[[85,1,89,1],[63,4,63,10],[65,1,69,1],[70,1,74,1],[75,1,79,1],[80,1,84,1],[56,1,57,3],[56,4,56,10],[6,1,6,2],[13,1,17,1],[20,1,30,1],[33,1,37,1],[40,1,50,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.6 NON-NETWORK EXPENDITURE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,90124850.686742231,89662888.583503053,85116470.341885671,85584991.710963488,85990002.200818613,86471451.739988506,86983802.317210823]
[null,"MOTOR VEHICLES","Car",null,784509.93350423651,780501.14634972962,713884.28480179526,718474.41539244715,722480.71629435418,727061.57841171382,731866.5475763838]
[null,null,"Light commercial vehicle",null,6609103.5257708309,6575331.500477829,6014117.7851006193,6052787.3378683189,6086538.4177275887,6125129.8882468697,6165609.3484693691]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,7796115.8544508545,7756278.2848323686,7094269.1141291074,7139883.8200027952,7179696.6823327141,7225219.282181358,7272968.959636054]
[null,null,"Heavy commercial vehicle",null,6301037.2170931334,6268839.3876238195,5733785.2015990252,5770652.2729359353,5802830.1332888696,5839622.7619799115,5878215.3766053673]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,31359076.589560568,31198336.184815764,23254582.900692139,23382587.139756601,23493239.637142304,23624775.968197342,23764754.739924803]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","Office furniture and equipment",null,0,0,0,0,0,0,0]
[null,null,"Plant and equipment",null,3496341.9270951767,3478475.8810369764,3181583.1125271432,3202040.0441089435,3219895.0096328706,3240310.6342147356,3261725.0413896632]
[null,null,"Crane borer plant HCV",null,3466054.7123309541,3448343.4316776353,3154022.5097518326,3174302.2322696582,3192002.5283743157,3212241.3017158993,3233470.205652677]
[null,null,"Other fleet assets",null,7681970.5907304501,7642716.2948825136,6990399.7984270481,7035346.6457505692,7074576.596056737,7119432.6859070733,7166483.2460542032]
[null,null,"EWP Hired",null,0,0,0,0,0,0,0]
[null,null,"Car Hired",null,0,0,0,0,0,0,0]
[null,null,"LCV Hired",null,593710.13835987239,590676.32390512584,540261.27573606267,543735.04573141877,546766.97861231666,550233.73430954118,553870.09222642367]
[null,null,"Other Hire",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,84870001.238267586,75028479.115014002,74885470,62816850,47127460,36949710,44254990]
[null,"MOTOR VEHICLES","Car",null,325818.03564490593,300912.71469487849,536110.46370974404,213006.76751269892,313687.9437833812,331242.01133783587,259931.26651480925]
[null,null,"Light commercial vehicle",null,6019850.1392814014,17532124.672280654,15955464.771829352,13812845.001868526,7557570.6906523192,3537464.2838433469,12622255.684534075]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,12391641.196131194,16983757.930397756,20145771.400991455,22188843.307405382,13329448.658571279,11553052.601488238,10273525.644236766]
[null,null,"Heavy commercial vehicle",null,10509904.305622796,9788624.8374779522,4542203.0278134821,6606572.9385855393,6691793.9675419331,7631726.4427988669,8581787.6190684717]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,14253036.763619995,53173711.842390344,29968460.877744682,41182046.705272868,28798837.228904452,23593441.074238788,14494223.686782664]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","Plant and equipment",null,71548.867634592578,1303451.0142924858,1111397.2092657308,0,3298327.2612045771,0,1226248.0497455299]
[null,null,"Tools and Equipment",null,4054756.7552197552,4965476.7905532708,5347950.6464334438,5045359.3612993835,5143900.7673979178,4931706.7723527821,4778761.1715793656]
[null,null,"Crane borer plant HCV",null,1334931.0273244691,3801946.1798548247,2427512.660051683,2060799.2261458188,1328840.5406985707,4749906.5654702792,5227990.5180497635]
[null,null,"Refurbishment/ Rebuild EWP (HCV)",null,0,0,0,0,0,0,0]
[null,null,"Other fleet assets",null,2620670.1897031413,4838657.7772307536,2516734.1385617591,1364155.359100864,3540026.2182601616,1621278.789516178,1378938.9846303181]
[null,null,"Property leases",null,0,0,0,0,0,11922845.815817075,1965238.5585733433]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Employee numbers",null,null,2676,2756,2839,2867,2896,2896,2896]
[null,"User numbers",null,null,3329,3441,3555,3595,3626,3626,3626]
[null,"Number of devices",null,null,9190,9465,9750,9847,9946,9946,9946]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  or PER CENT"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","UNITS",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"CAR","Average kilometres travelled ","0's",14633.459000000001,14869.094302476104,14875.513688403418,14878.393412931562,14881.333131720705,14882.383031288256,14882.383031288256]
[null,null,"Number purchased","0's",7,8,11.221882174058791,5.6172159480561055,7.757804704529728,7.7444411595400773,6.0879619946616703]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",68.37,69.470928060159338,69.500920518938258,69.514375079885824,69.52810994418644,69.533015252865241,69.533015252865241]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",22577.97393987342,24495.711908971873,24816.034559199619,24959.730701357861,25105.04348616799,25157.432704663184,26077.747008460654]
[null,null,"Number purchased","0's",144.91,224.77624637265134,207.21906337160752,190.37518730688936,101.91,45.000641205636747,146.63]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",801.73500000000001,869.83312318632557,881.20765487212941,886.31024852557414,891.47024852557411,893.33056912839265,926.0105691283926]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",14729.384833333332,15134.164232087973,15308.929110767514,15387.328308679829,15467.36082321532,15495.943864120854,15495.943864120854]
[null,null,"Number purchased","0's",43.43,44.773245041753654,39.435645615866392,38.808981210855947,22.946043319415448,18.883586899791229,20.21]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",212.20499999999998,218.03662252087682,220.55444532881003,221.68393593423798,222.8369575939457,223.24875104384134,223.24875104384134]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",10805.405913461538,11312.128652509986,11510.792011884987,11593.179720131333,11677.283838966147,11707.321024264291,11707.321024264291]
[null,null,"Number purchased","0's",62.78,44.669560281837164,18.973749999999999,22.687123173277662,27.495604906054279,31.903430323590818,36.549999999999997]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",247.035,258.61978014091858,263.16165514091858,265.04521672755743,266.96801918058458,267.65473434237992,267.65473434237992]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[]
[]
[null,"Table 2.6.4 intentionally omitted"]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RECURRENT"]
[null,"Recurrent",null,null,29216899.364904299,12026095.934703214,46517336.993117161,37435870.908077262,25794283.246424556,19693315.157084044,25899927.397028863]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NON-RECURRENT"]
[null,"Maintain",null,null,45117785.614436671,54865323.244392216,17861514.860308945,15682014.610239785,12408912.184679588,10320117.605030762,11701947.642383531]
[null,"Comply",null,null,744130.14468254929,1076963.8150480478,4660890.0493100649,4833166.4314059718,5396652.6318660676,4624636.3890793007,4397872.3482585885]
[null,"New / Expanded",null,null,9752021.3697870951,7060096.1208705362,5845728.0972638233,4865798.0502769882,3527611.9370297859,2311640.8488058965,2255242.6123290192]

{"sheet":"2.10 Overheads","index":8,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[6,1,6,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.10 OVERHEADS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",219926232.7747044,218799625.35941824,220692534.09858042,221907330.33961108,222957453.67042604,224205770.45815489,225534208.38303462]
[null,"Alternative Control Services","Total  ",45860303.100718513,46137575.054184981,50687239.4159761,51231123.572366327,50835293.616513461,50369671.301422887,49930850.010004602]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",124925433.7509841,143839843.74642706,151848673.66928712,158082945.6066497,156009478.47745401,153860326.68528903,152433829.83911717]
[null,"Alternative Control Services","Total  ",6807726.9438940184,6848886.5442624297,7524260.9000188028,7604997.7154228166,7546238.7872547712,7477119.5410701381,7411978.7694842694]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  "]
[null,"Unregulated Distribution Services","Total  ",206125.27506625105,214159.08563723692,220087.55791885121,224158.8598071126,223788.56820120258,223395.5306510886,223313.94571889617]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",82224275.293777838,81803068.250426188,82510773.953885004,82964952.335827619,83357564.11640498,83824274.894437581,84320940.727648601]
[null,"Alternative Control Services","Total  ",15420207.377946917,15513438.140359266,17043231.081430655,17226108.339409042,17093013.27476785,16936451.015623428,16788900.413948003]
[null,"CAPEX"]
[null,"Standard Control Services","Total",11227736.322429609,10944192.447418854,12941019.709513061,13694967.624126861,13538313.559348769,13136684.849546567,12564596.175871866]
[null,"Alternative Control Services","Total",402455.78665359615,404889.03926215949,444815.4816520657,449588.44020682562,446114.75936538068,442028.60244025756,438177.64298082638]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total"]
[null,"Unregulated Distribution Services","Total",26839.039754338271,27885.101481723283,28657.03254741912,29187.146252280589,29138.93153854147,29087.755134148236,29077.132170817978]

{"sheet":"2.11 Labour","index":9,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.11 LABOUR"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"In-house labour expenditure",283836736.9235611,282382737.69611883,268064327.36982358,269539880.39916986,270815413.37304264,272331682.15582579,273945270.12897575]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",91580172.820240483,91111038.69062455,86491191.004923567,86967279.487681717,87378831.323611394,87868056.780027956,88388682.358814582]
[null,"Controllable non-labour expenditure",119383710.63509968,118772148.42185675,96822690.194688737,97773294.765038729,98619285.226211905,99510153.805588663,100414003.26662594]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C13:C17)","v":494800620.37890124},492265924.80860013,451378208.56943589,454280454.65189028,456813529.92286593,459709892.74144238,462747955.75441629]
[null,"CAPEX"]
[null,"In-house labour expenditure",207496707.05187434,215845429.81114399,226905231.79101995,234680945.05727339,233106040.65862614,226734222.17336208,232801146.33250323]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",173188563.27611256,190301665.51388088,186376005.45101991,192611949.71559924,184822091.47990465,183804343.51603603,186317766.15180728]
[null,"Controllable non-labour expenditure",197454452.09785557,266662093.54592732,281462408.79145777,291746835.90008014,262421518.64460111,259647253.78703162,258297655.41179314]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C20:C24)","v":578139722.42584252},672809188.87095213,694743646.03349757,719039730.67295277,680349650.78313184,670185819.4764297,677416567.89610362]

{"sheet":"2.14 Forecast price changes","index":10,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[6,1,6,2],[12,4,12,8],[8,1,8,2],[9,1,9,2],[12,2,12,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There is ONE table on this worksheet."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. FORECAST price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"Energex must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. FORECAST price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"FORECAST"]
[null,"DESCRIPTION",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"Labour - internal",0,0,1.6020560115463097E-2,1.1417206065738138E-2,1.0105273511247521E-2,1.1599457880484405E-2,1.2399187195934525E-2]
[null,"Contractors",0,0,0,0,0,0,0]
[null,"CPI",3.5999999999999997E-2,3.1E-2,2.7997811278454687E-2,2.7997811278454687E-2,2.7997811278454687E-2,2.7997811278454687E-2,2.7997811278454687E-2]
[null,"CAPEX"]
[null,"Labour - internal",1.3334878719465749E-2,1.3142428831592359E-2,1.6020560115463097E-2,1.1417206065738138E-2,1.0105273511247521E-2,1.1599457880484405E-2,1.2399187195934525E-2]
[null,"Contractors",0,0,0,0,0,0,0]
[null,"Materials",0,0,0,0,0,0,0]
[null,"Other",0,0,0,0,0,0,0]
[null,"CPI",4.1000000000000002E-2,3.3000000000000002E-2,2.7997811278454687E-2,2.7997811278454687E-2,2.7997811278454687E-2,2.7997811278454687E-2,2.7997811278454687E-2]

{"sheet":"2.16 Opex Summary","index":11,"n_rows":62,"n_cols":12,"rows_kept":62,"cut":false,"hidden":false,"merged":[[9,1,9,7],[9,9,9,10],[6,9,6,11],[7,1,7,7],[7,9,7,10],[7,11,8,11],[8,1,8,7],[8,9,8,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.16 OPEX SUMMARY"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nEnergex's total forecast opex must reconcile to Table 2.16.1 (and if Energex owns any dual function assets Table 2.16.3). If Energex did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if Energex owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has Energex used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If Energex does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2023-24"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Base year total opex, excluding category specific",null,null,null,488295128.54909217,488326920.17151284,485792224.60121167,485792224.60121167,485792224.60121167,485792224.60121167,485792224.60121167]
[null,"Increment from base year to final year",null,null,null,null,-2534695.5703011532,-48119471.35213013,-48119471.35213013,-48119471.35213013,-48119471.35213013,-48119471.35213013]
[null,"Price growth",null,null,null,null,null,4103296.1408487195,7040203.1856046645,9654995.9319083877,12684446.529864775,15950729.047013588]
[null,"Output growth",null,null,null,null,null,4009624.8660447164,7853862.8006709777,11730098.108282495,15643391.580254531,19532631.842291392]
[null,"Productivity growth",null,null,null,null,null,-4326467.6335961157,-8677612.0379081685,-13068040.656637484,-17513731.79736257,-22011932.457520265]
[null,"Step changes",null,null,null,null,null,2105606.978048,2541965.4756439999,2938655.2131159995,3335344.9505879995,3724141.3108199998]
[null,"Category specific",null,null,null,6505491.8298090771,6473700.2073884336,7813394.969009039,7849281.9787972504,7885068.0771149658,7887688.2290160777,7879632.7627300117]
[null,"Total opex",{"$f":"SUM(C16:C22)","v":0},0,0,494800620.37890124,492265924.80860013,451378208.56943589,454280454.65189028,456813529.92286587,459709892.74144238,462747955.75441629]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C29:C35)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Base year total opex, excluding category specific"]
[null,"Increment from base year to final year"]
[null,"Price growth"]
[null,"Output growth"]
[null,"Productivity growth"]
[null,"Step changes"]
[null,"Category specific"]
[null,"Total opex",{"$f":"SUM(C42:C48)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C55:C61)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":12,"n_rows":133,"n_cols":11,"rows_kept":133,"cut":false,"hidden":false,"merged":[[55,1,55,3],[29,1,29,3],[30,1,30,3],[132,1,132,2],[106,1,106,3],[80,1,80,3],[81,1,81,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.17 STEP CHANGES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Smart meter data","The acquisition, processing, and use of smart meter data.",null,0,0,2105606.978048,2541965.4756439999,2938655.2131159995,3335344.9505879995,3724141.3108199998]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E10:E29)","v":0},0,2105606.978048,2541965.4756439999,2938655.2131159995,3335344.9505879995,3724141.3108199998]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$30,0)-ROUND('2.16 Opex Summary'!H$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$30,0)-ROUND('2.16 Opex Summary'!I$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$30,0)-ROUND('2.16 Opex Summary'!J$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$30,0)-ROUND('2.16 Opex Summary'!K$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$30,0)-ROUND('2.16 Opex Summary'!L$21,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E36:E55)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E61:E80)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$30,0)-ROUND('2.16 Opex Summary'!H$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$30,0)-ROUND('2.16 Opex Summary'!I$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$30,0)-ROUND('2.16 Opex Summary'!J$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$30,0)-ROUND('2.16 Opex Summary'!K$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$30,0)-ROUND('2.16 Opex Summary'!L$47,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E87:E106)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE \n($, real June 2024)"]
[null,"CATEGORY","DESCRIPTION",{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D113:D132)","v":0},{"$f":"SUM(E113:E132)","v":0},{"$f":"SUM(F113:F132)","v":0},0,0,0,0,0]

{"sheet":"3.1 Revenue","index":13,"n_rows":51,"n_cols":17,"rows_kept":51,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[29,2,29,8],[29,10,29,16],[42,2,42,8],[42,10,42,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.1 REVENUE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DREV0101","Revenue from Fixed Customer Charges ",350272955.70278478,350677894.03650779,345188534.39279485,346143081.0023827,346160490.40546858,344488210.19815141,340973118.2934339,null,1583545.3921258668,1587380.5767018499,1689208.8621426055,1662586.4439503744,1632211.1567468029,1607120.1190059285,1584923.333065134]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",497165062.12316221,497900983.8022756,318689779.45583397,279107863.74033183,234622844.59940261,187768246.71632382,139378759.77443501]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",19851184.417674541,21946711.758714091,6651576.20070526,4082974.4079562849,4810961.956205314,-7478738.5670870282,-7076715.3403768269]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",662805.43225349183,509364.28798532212,115381208.34909734,144994398.93558952,169379907.88360277,198360847.97782105,211101015.02248171]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",13639433.028925426,14871887.196491856,3309876.3812192488,1709351.5497292206,2397418.7770857019,3106646.4461812475,3833739.9491793243]
["DREV0106","Revenue from controlled load customer charges",36405112.611192122,34560040.651922964,28816228.813911341,29084052.286626551,29435590.94334998,29550736.827060953,29500953.823617879]
["DREV0107","Revenue from unmetered supplies",3276338.8790948796,3290295.3243846814,3413256.1053251619,3266179.7299245857,3119490.0554793845,2930969.1134580127,2736039.7144065583]
["DREV0108","Revenue from Contracted Maximum Demand charges",5697281.3794592293,5760975.2628297228,5963187.6059894888,6274463.369550677,6601314.7076470591,6944833.9434618261,7307562.6465648422]
["DREV0109","Revenue from Measured Maximum Demand charges",407286920.26291782,481102593.19530803,632535385.30220187,721914121.79297197,820632380.9411602,936344771.63753211,1063513887.4236455]
["DREV0110","Revenue from metering charges",60523776.177986011,57526924.31371177,61307233.481387913,66340939.1469943,71787943.395640656,77682180.614851847,84060371.416698262]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,78681414.909759849,78923286.102804273,80164172.591312349,81019778.174548537,81957966.795428127,82926059.483723789,83008377.209984794]
["DREV0112","Revenue from public lighting charges",8562587.2942468785,8599061.9342402592,8920415.2677704282,8536036.7435205895,8152668.8475388754,7659976.5216163518,7150535.936503781,null,55105103.825357854,54955336.516051903,47514913.861131646,49563250.175077945,51709401.430951171,53958038.62091165,56314055.792691112]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,30369958.985650219,30443511.912427161,31157596.326486561,31571688.517120015,31908363.996720776,32342482.204538707,32833169.577000026]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":1403343457.3096974},1476746731.7643723,1530176681.3562369,1611453462.7055783,1697101012.5125811,1787358681.4293718,1882479268.6605899,null,{"$f":"SUM(K13:K25)","v":165740023.11289379},165909515.10798517,160525891.64107317,163817303.31069687,167207943.37984687,170833700.42818007,173740525.91274107]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DREV0201","Revenue from residential Customers ",778479912.97617233,814577002.03753865,893620510.17549801,940553832.02386069,985785498.55291224,1038812184.1519322,1089755843.1544476]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",103395025.78221396,93091174.230489671,77544590.518532127,63501114.353577279,50042051.851090148,36731748.991998754,24252515.569777187]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",351740552.51444566,389941749.05808526,391308729.41375184,432180078.15350407,478090403.38825756,520395410.95899343,568364784.98246574]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",157355433.95353329,166765523.72202361,155369179.87535945,163416221.70119122,171910899.81730285,180828391.69137308,190219549.3029891]
["DREV0205","Revenue from unmetered supplies",3424010.5313560748,3423664.7778702853,3413256.1053251643,3266179.7299245857,3119490.055479378,2930969.1134580197,2736039.7144065597]
["DREV0206","Revenue from Other Customers",8948521.5519758817,8947617.9383651968,8920415.2677704319,8536036.7435205895,8152668.8475388596,7659976.5216163695,7150535.9365037847,null,165740023.11289379,165909515.10798517,160525891.64107317,163817303.31069687,167207943.37984687,170833700.42818007,173740525.91274107]
["DREV02","Total revenue by customer class",{"$f":"SUM(C33:C38)","v":1403343457.3096972},1476746731.7643726,1530176681.3562372,1611453462.7055783,1697101012.5125811,1787358681.4293718,1882479268.6605899,null,{"$f":"SUM(K33:K38)","v":165740023.11289379},165909515.10798517,160525891.64107317,163817303.31069687,167207943.37984687,170833700.42818007,173740525.91274107]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DREV0301","EBSS",37703978.313470125,0,-68837391.60355179,-32085590.4708784,-23985317.072260216,3065125.6782006156,0]
["DREV0302","STPIS",4221141.9128736025,23094478.066143256]
["DREV0303","F-Factor"]
["DREV0304","S-Factor True  up"]
["DREV0305","Other",23188318.58326887,23986644.510215536,-8204626.2752294838,-8175646.0922449213,-8145454.6297411444,-8114518.351918499,-8101284.9017772134]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C46:C50)","v":65113438.809612602},47081122.576358795,-77042017.878781274,-40261236.563123323,-32130771.702001359,-5049392.6737178834,-8101284.9017772134,null,{"$f":"SUM(K46:K50)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":14,"n_rows":76,"n_cols":17,"rows_kept":76,"cut":false,"hidden":false,"merged":[[10,2,10,8],[10,10,10,16],[67,2,67,8],[67,10,67,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.2 OPERATING EXPENDITURE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOPEX0101","Inspection",0,0,0,0,0,0,0]
["DOPEX0102","Preventative maintenance",146630138.38300827,145878541.38606998,133198072.63554314,134058811.56760925,134808722.5037623,135677684.45494992,136592403.3370983]
["DOPEX0103","Corrective repair",96855814.209735662,96359350.522946388,87983329.474768013,88551886.328131407,89047236.295790613,89621224.823849648,90225437.86681959]
["DOPEX0104","Vegetation",54106759.599187784,53829419.084630072,49150305.487276517,49467919.553446963,49744637.908832058,50065286.282435432,50402819.038000062]
["DOPEX0105","Emergency response / storms",2607939.8468791102,2594572.0646569445,2369039.3051827406,2384348.2681520856,2397686.0623707301,2413141.2786237798,2429410.3202256933]
["DOPEX0106","Other network maintenane costs",0,0,0,0,0,0,0,null,15596469.869681049,14679306.467878766,11760739.430011271,11357074.941023558,10957260.825390078,10595878.00108696,10259254.234212227]
["DOPEX0107","Network operating costs",54942103.199691072,54660480.879575051,58030777.26598537,58405777.806628041,58732493.603967682,59111076.69037585,59509594.827017263]
["DOPEX0108","Network billing and other energy market services (incl meter reading)",4093985.8271278604,4073000.8680525315,3718955.9225966907,3742988.1783634508,3763926.0617895671,3788187.908308343,3813727.3109210581,null,165811.48697004531,156060.80436570983,88617.681540254329,85576.052113201513,82563.43541632159,79840.400165962259,77303.925486856358]
["DOPEX0109","Customer services (incl call centre)",19400112.451708492,19300671.324394796,17622963.573359195,17736844.882193733,17836062.932797585,17951032.200065553,18072055.404238131,null,1395237.5477197049,1313189.4415597017,741913.21646183555,716448.48941992281,691226.65891498537,668429.22384312167,647193.68647697382]
["DOPEX0110","DSM initiatives",5355369.2642201958,5327918.7039133525,4864790.2273849184,4896226.9761470594,4923615.9564935593,4955353.034399135,4988761.2916706624]
["DOPEX0111","Levies",13589571.549868528,13519914.102366978,0,0,0,0,0]
["DOPEX0112","Debt raising costs",6505491.8298090771,6473700.2073884336,7813394.969009039,7849281.9787972504,7885068.0771149658,7887688.2290160777,7879632.7627300117,null,112699.91530246491,106072.50290944807,56990.079841370301,63807.61436871464,69899.287529192952,75458.225628819811,80434.914535231932]
["DOPEX0113","Other operating costs (incl self insurance)",28568472.36175923,28422036.040611364,30174502.975052297,30369493.555264656,30539377.31804169,30736230.729374915,30943449.851127863,null,82016125.165626228,80617100.038731664,79034560.160686046,78194267.062573597,77362127.55940336,76546635.540422454,75744335.753748283]
["DOPEX0114","Corporate allocations",62144861.85590592,61826319.623994224,56452076.733277977,56816875.557156377,57134703.201905198,57502987.110043749,57890663.744567662,null,2997809.3767492492,2821520.6993172481,2434045.8103347123,2350501.9256964568,2267754.928463697,2192961.8123797458,2123292.9217205686]
["DOPEX0115"]
["DOPEX0116"]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C14:C62)","v":494800620.37890124},492265924.80860025,451378208.56943589,454280454.65189028,456813529.92286593,459709892.74144244,462747955.75441635,null,{"$f":"SUM(K14:K62)","v":102284153.36204875},99693249.954762533,94116866.378875494,92767676.085195452,91430832.695117638,90159203.203527063,88931815.436180145]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOPEX0201","Opex for network services",494211524.6117596,491679846.77904803,450825765.24858981,453724441.38844216,456254406.37951881,459147165.15025502,462181434.33703536]
["DOPEX0202","Opex for metering",529434.72308074473,526722.60876219615,496494.27631964529,499702.67074097926,502497.95508843567,505737.00071850786,509146.60477990319]
["DOPEX0203","Opex for connection services",59661.044060892578,59355.420789877106,55949.044526438702,56310.592707151307,56625.588258719778,56990.590468862894,57374.812601014361,null,78153682.32225813,76981791.363998532,76122030.323888242,75381704.143266737,74648578.018284604,73922581.924670696,73203646.51917617]
["DOPEX0204","Opex for public lighting",null,null,null,null,null,null,null,null,24130471.039790615,22711458.590764008,17994836.054987252,17385971.941928718,16782254.676833037,16236621.278856363,15728168.917003969]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP"]
["DOPEX0207","Opex for transmission connection point planning"]

{"sheet":"3.3 Assets (RAB)","index":15,"n_rows":138,"n_cols":25,"rows_kept":138,"cut":false,"hidden":false,"merged":[[98,2,98,8],[98,10,98,16],[98,18,98,24],[115,2,115,8],[115,10,115,16],[115,18,115,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[22,2,22,8],[22,10,22,16],[22,18,22,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.3 ASSETS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - BENCHMARKING ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",12564641263.00462,12713544338.302479,12998340765.557322,13099874608.599329,13203950590.19001,13244276270.087605,13265936377.981079,null,15195421027.396111,15327043140.761669,15590723145.889391,15662331510.289351,15733738517.557762,15738966726.684935,15722892978.311127,null,157455595.76250428,159971124.5528008,166925372.15835845,186894101.65210626,204736765.01054168,221019034.02417248,235595880.55836824]
["DRAB0102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0103","Straight line depreciation",-372981824.51662815,-387325002.82747614,-530396473.84307468,-550420768.02669442,-567221362.09025121,-578076158.90825307,-569646871.81427681,null,-460169354.66037953,-475879364.41944498,-628486435.85216987,-653928571.93698645,-675911733.60155773,-692360718.3927083,-690338971.74279237,null,-13363546.844199652,-13363546.844199652,-19634553.80700611,-21799592.642012667,-23587100.526278373,-25580569.003273834,-27588439.78014731]
["DRAB0105","Actual additions (recognised in RAB)",523054676.47020227,618292826.17372954,633289104.07371843,655612273.6159029,613850261.67665505,600957271.59057891,606511446.51144135,null,592961244.68165255,686437244.21587694,701453587.44076514,726451103.20392585,687443162.41754007,677507974.80775034,685357145.60539246,null,15879075.63449618,15797308.427220142,39603283.300753929,39642256.000448078,39869369.539909199,40157415.537469588,40469905.768682815]
["DRAB0106","Disposals ",-1169776.6557147796,-1093332.8693129893,-1358787.1886375004,-1115523.9985272875,-6303219.688808674,-1221004.7888511936,-4221653.1074916981,null,-1169776.6557147796,-1093332.8693129893,-1358787.1886375004,-1115523.9985272875,-6303219.688808674,-1221004.7888511936,-4221653.1074916981,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C14+C15+C16+C17+C18)","v":12713544338.302479},12943418828.779419,13099874608.599329,13203950590.19001,13244276270.087605,13265936377.981079,13298579299.570751,null,{"$f":"SUM(K14+K15+K16+K17+K18)","v":15327043140.761669},15536507687.688789,15662331510.289351,15733738517.557762,15738966726.684935,15722892978.311127,15713689499.066235,null,{"$f":"SUM(S14+S15+S16+S17+S18)","v":159971124.5528008},162404886.13582128,186894101.65210626,204736765.01054168,221019034.02417248,235595880.55836824,248477346.54690373]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",2679805559.999979,2772468785.5543447,2868820431.759913,2947185266.7303104,3037712350.8599772,3127300304.2903881,3216552022.00068,null,3512085945.4510832,3612539299.2176743,3713581478.8342819,3792793550.7629733,3883704755.7430801,3973231680.8163691,4061975062.7252765,null,null,{"$f":"S32","v":0},0,0,0,0,0]
["DRAB0202","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-73216887.910954416,-75474372.572978258,-102735629.14490141,-105883968.05540125,-109417518.05061859,-112940382.84909761,-116463144.11293571,null,-102273230.10035175,-104911715.36097634,-135525383.08727676,-140481525.01320702,-145822459.26527151,-151256935.1737715,-156801095.64676231]
["DRAB0205","Actual additions (recognised in RAB)",165880113.46532029,174921888.35002193,181100464.11529893,196411052.18506798,199005471.48102966,202192100.5593898,195341795.78225413,null,202726583.86694282,211191592.0035564,214737455.01596823,231392729.99331361,235349384.3385604,240000317.08267885,234288356.86931363]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C27+C28+C29+C30+C31)","v":2772468785.5543447},2871916301.331388,2947185266.7303104,3037712350.8599772,3127300304.2903881,3216552022.00068,3295430673.6699986,null,{"$f":"SUM(K27+K28+K29+K30+K31)","v":3612539299.2176743},3718819175.8602543,3792793550.7629733,3883704755.7430801,3973231680.8163691,4061975062.7252765,4139462323.9478278,null,{"$f":"SUM(S27+S28+S29+S30+S31)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",2119039241.6225367,2082878601.3351541,2048187745.9003952,2007781302.9457643,1967927839.9814246,1928087489.8158817,1888290339.2191694,null,2747718239.3472614,2706203138.3971372,2666705408.3840303,2616754611.3667331,2566881534.181232,2516507911.2539263,2465638048.1225858,null,null,{"$f":"S39","v":0},0,0,0,0,0]
["DRAB0302","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-45188562.191523425,-45646229.290855795,-53825166.957958512,-53415213.495571904,-52970227.544597395,-52476235.210978411,-51928625.675243989,null,-59912247.599838212,-60689084.793668166,-70162326.35341157,-70499185.175680146,-70842953.642183125,-71184109.154097736,-71522679.921143696]
["DRAB0305","Actual additions (recognised in RAB)",9027921.9041406941,10955373.856097022,13418724.003327707,13561750.531232039,13129877.379054567,12679084.614266152,13771407.277697984,null,18397146.649713885,20455822.613772586,20211529.336114276,20626107.99017895,20469330.714877561,20314246.022756968,21636451.110754158]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C34+C35+C36+C37+C38)","v":2082878601.3351541},2048187745.9003952,2007781302.9457643,1967927839.9814246,1928087489.8158817,1888290339.2191694,1850133120.8216233,null,{"$f":"SUM(K34+K35+K36+K37+K38)","v":2706203138.3971372},2665969876.2172413,2616754611.3667331,2566881534.181232,2516507911.2539263,2465638048.1225858,2415751819.3121963,null,{"$f":"SUM(S34+S35+S36+S37+S38)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",1564330624.250895,1558583937.2780745,1565967336.7788582,1566038934.1716805,1567521489.4385235,1567333347.9936607,1565612793.0228004,null,2261241871.7268176,2263597258.061615,2278090107.747611,2271556022.150774,2264912180.5118332,2254963492.859014,2241753036.9412179,null,null,{"$f":"S46","v":0},0,0,0,0,0]
["DRAB0402","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-53732418.579469487,-54944736.591113508,-68320344.984639615,-68237707.332656264,-68084548.794858217,-67734643.166668937,-67165860.324175104,null,-78716733.537065759,-80590141.62805298,-99828438.69780463,-102262024.5117113,-104751516.20886558,-107215030.52086078,-109652631.91862905]
["DRAB0405","Actual additions (recognised in RAB)",47985731.606648929,57049277.584121205,68391942.37746188,69720262.599499553,67896407.3499953,66014088.195808738,70614190.672708943,null,81072119.871863306,90455808.958279461,93294353.100967303,95618182.872770339,94802828.556046486,94004574.603064448,99447425.587272912]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C41+C42+C43+C44+C45)","v":1558583937.2780745},1560688478.2710822,1566038934.1716805,1567521489.4385235,1567333347.9936607,1565612793.0228004,1569061123.3713343,null,{"$f":"SUM(K41+K42+K43+K44+K45)","v":2263597258.061615},2273462925.3918414,2271556022.150774,2264912180.5118332,2254963492.859014,2241753036.9412179,2231547830.6098619,null,{"$f":"SUM(S41+S42+S43+S44+S45)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",615604076.06263733,630601855.28503776,655086114.86760855,673602909.41538167,692811461.93176532,710698130.95851707,727312580.72219026,null,757495335.67179704,768757619.06408262,791386265.52684689,807186869.26543593,823927266.01712263,839425128.05088341,853718115.83542359,null,null,{"$f":"S53","v":0},0,0,0,0,0]
["DRAB0502","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-15545764.867533693,-15799391.584464336,-20692383.14078436,-21683758.822981544,-22540184.238151245,-23371805.527573105,-24179932.811865646,null,-19103183.607653446,-19361137.106215425,-25016499.78601421,-25824119.562915739,-26666314.187264819,-27500587.5592677,-28327528.108215224]
["DRAB0505","Actual additions (recognised in RAB)",30543544.08993407,34570736.756344803,39209177.688557543,40892311.339365236,40426853.264902942,39986255.291246243,41136259.7795173,null,30365466.999939065,34117894.794692025,40817103.524603307,42564516.314602412,42164176.221025534,41793575.343807764,42997995.330772333]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C48+C49+C50+C51+C52)","v":630601855.28503776},649373200.45691824,673602909.41538167,692811461.93176532,710698130.95851707,727312580.72219026,744268907.68984187,null,{"$f":"SUM(K48+K49+K50+K51+K52)","v":768757619.06408262},783514376.75255919,807186869.26543593,823927266.01712263,839425128.05088341,853718115.83542359,868388583.05798066,null,{"$f":"SUM(S48+S49+S50+S51+S52)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",689805908.20517468,673558336.39252603,659612584.61702597,642390800.41857946,625195040.36148298,607683997.21129978,589889826.67509675,null,920730485.18731701,896261130.56372917,874432589.62681508,848210107.13685572,821665523.92737436,794419860.52588856,766455996.45999312,null,null,{"$f":"S60","v":0},0,0,0,0,0]
["DRAB0602","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-22735688.44985652,-22917920.698963214,-27846646.645559214,-27733299.237400535,-27580366.554748509,-27367592.92920782,-27085551.399299853,null,-30481212.290843718,-30663444.538228311,-36922290.632820018,-37160064.147105806,-37395963.723497458,-37621525.952875502,-37836140.661475055]
["DRAB0605","Actual additions (recognised in RAB)",6488116.6372078964,8268661.4657692006,10624862.447112722,10537539.180304082,10069323.40456536,9573422.3930047639,10761987.261693904,null,6011857.6672558645,7720330.6452403078,10699808.142860616,10615480.93762446,10150300.322011754,9657661.8869800903,10848763.0712863]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C55+C56+C57+C58+C59)","v":673558336.39252603},658909077.15933204,642390800.41857946,625195040.36148298,607683997.21129978,589889826.67509675,573566262.53749084,null,{"$f":"SUM(K55+K56+K57+K58+K59)","v":896261130.56372917},873318016.6707412,848210107.13685572,821665523.92737436,794419860.52588856,766455996.45999312,739468618.86980438,null,{"$f":"SUM(S55+S56+S57+S58+S59)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",3359181049.1045413,3332530747.191165,3322059766.5553889,3301040270.7130852,3280269154.4562597,3255875974.5693212,3227858149.9943027,null,3432559913.9576578,3400077978.2833929,3383839663.0437698,3361426670.6664791,3339333726.9065223,3313688445.9354014,3284478420.4576669,null,null,{"$f":"S67","v":0},0,0,0,0,0]
["DRAB0702","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-83115384.888220355,-84221200.682791278,-101206457.70275357,-102827976.56522405,-104487280.66137731,-106098921.70155071,-107661523.2352626,null,-85015216.19659695,-86122275.950901359,-103308531.72481169,-104886707.95574841,-106504981.69232546,-108087568.72912437,-109633731.84450334]
["DRAB0705","Actual additions (recognised in RAB)",57634859.630559124,67950454.175628483,80728535.86780791,82598293.86722587,80635457.82521002,78622731.276327178,83565519.637238577,null,53703057.178047173,63407165.486234158,81437113.354878902,83335197.75461854,81401057.771975905,79419177.401184797,84385945.473384857]
["DRAB0706","Disposals ",-1169776.6557147796,-1093332.8693129893,-541574.00735801843,-541433.55882707529,-541357.05077131186,-541634.14979488926,-541917.0419022002,null,-1169776.6557147796,-1093332.8693129893,-541574.00735801843,-541433.55882707529,-541357.05077131186,-541634.14979488926,-541917.0419022002]
["DRAB0707","Closing value",{"$f":"SUM(C62+C63+C64+C65+C66)","v":3332530747.191165},3315166667.8146896,3301040270.7130852,3280269154.4562597,3255875974.5693212,3227858149.9943027,3203220229.3543768,null,{"$f":"SUM(K62+K63+K64+K65+K66)","v":3400077978.2833929},3376269534.9494128,3361426670.6664791,3339333726.9065223,3313688445.9354014,3284478420.4576669,3258688717.0446463,null,{"$f":"SUM(S62+S63+S64+S65+S66)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",212144657.43679392,214462345.49518487,217506043.20135614,221524741.35112351,225468984.17605558,229210052.81861091,232734851.6509836,null,212158293.33271572,214261951.56693476,219576518.47071451,223595216.62048188,227539459.44541395,231280528.08796927,234805326.92034197,null,null,{"$f":"S73","v":0},0,0,0,0,0]
["DRAB0802","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",2317688.0583909531,3043697.7061712863,4018698.1497673672,3944242.824932083,3741068.6425553206,3524798.8323727059,4041208.0686803032,null,2103658.2342190542,2802560.5918484032,4018698.1497673672,3944242.824932083,3741068.6425553206,3524798.8323727059,4041208.0686803032]
["DRAB0804","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",{"$f":"SUM(C69+C70+C71+C72)","v":214462345.49518487},217506043.20135614,221524741.35112351,225468984.17605558,229210052.81861091,232734851.6509836,236776059.71966392,null,{"$f":"SUM(K69+K70+K71+K72)","v":214261951.56693476},217064512.15878317,223595216.62048188,227539459.44541395,231280528.08796927,234805326.92034197,238846534.98902228,null,{"$f":"SUM(S69+S70+S71+S72)","v":0},0,0,0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",45857134.29660055,45665155.163089335,43257346.295226812,42831202.484784737,41972629.601491943,42552366.106671609,43902873.886925839,null,71287559.655559838,65501544.636547886,55317838.668554932,52854921.639597893,49851698.303938821,48794985.734949343,48962868.375166163,null,null,{"$f":"S80","v":0},0,0,0,0,0]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0903","Straight line depreciation",-4283712.6229777178,-4776912.0662301145,-7274673.4618252041,-7623364.8713994315,-5865974.1065742932,-4756537.3732593078,-5157072.7282647416,null,-9504126.5049555507,-9997325.9482079484,-9311446.680340169,-9768015.3237657119,-7502423.1807434438,-5939162.5132967122,-6346298.856864281]
["DRAB0905","Actual additions (recognised in RAB)",4091733.4894665005,5274248.2658364326,6848529.6513831355,6764791.9881066373,6445710.6117539657,6107045.1535135349,6917464.6452009659,null,3718111.485943601,4853261.8865951803,6848529.6513831355,6764791.9881066373,6445710.6117539657,6107045.1535135349,6917464.6452009659]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C75+C76+C77+C78+C79)","v":45665155.163089335},46162491.362695649,42831202.484784737,41972629.601491943,42552366.106671609,43902873.886925839,45663265.803862065,null,{"$f":"SUM(K75+K76+K77+K78+K79)","v":65501544.636547886},60357480.574935116,52854921.639597893,49851698.303938821,48794985.734949343,48962868.375166163,49534034.16350285,null,{"$f":"SUM(S75+S76+S77+S78+S79)","v":0},0,0,0,0,0,0]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",986838735.73746538,1037447397.2393879,1143547813.3153625,1202769195.6114161,1273605416.183778,1323912344.5789919,1371295270.8496673,null,988081669.09036255,1034468605.7287071,1136650682.7683043,1196528051.2662632,1268190146.9662986,1319476832.7342327,1367975664.8186345,null,157455595.76250428,159971124.5528008,166925372.15835845,186894101.65210626,204736765.01054168,221019034.02417248,235595880.55836824]
["DRAB1002","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1003","Straight line depreciation",-21544992.268448308,-22194446.057947747,-38530318.252995878,-41982030.14437516,-45626244.892228059,-48830276.069077179,-52029339.462789595,null,-21544992.27122033,-22194446.061546735,-38283126.755170055,-41581291.874812692,-45088179.796488322,-48173858.404307239,-51268689.335555606,null,-13363546.844199652,-13363546.844199652,-19634553.80700611,-21799592.642012667,-23587100.526278373,-25580569.003273834,-27588439.78014731]
["DRAB1005","Actual additions (recognised in RAB)",72153653.770370871,115056871.46086794,97751700.549049541,112818250.71673693,101016012.85117841,96213202.339752704,87330718.292572364,null,67931928.909564883,110231190.68278714,98160495.253128976,113243387.57484804,101457705.12815873,96672690.488709033,87804040.89034906,null,15879075.63449618,15797308.427220142,39603283.300753929,39642256.000448078,39869369.539909199,40157415.537469588,40469905.768682815]
["DRAB1006","Disposals ",0,0,0,0,-5082839.5637363475,0,-3000010.5955244754,null,0,0,0,0,-5082839.5637363475,0,-3000010.5955244754,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"SUM(C82+C83+C84+C85+C86)","v":1037447397.2393879},1130309822.642308,1202769195.6114161,1273605416.183778,1323912344.5789919,1371295270.8496673,1403596639.0839255,null,{"$f":"SUM(K82+K83+K84+K85+K86)","v":1034468605.7287071},1122505350.3499475,1196528051.2662632,1268190146.9662986,1319476832.7342327,1367975664.8186345,1401511005.7779036,null,{"$f":"SUM(S82+S83+S84+S85+S86)","v":159971124.5528008},162404886.13582128,186894101.65210626,204736765.01054168,221019034.02417248,235595880.55836824,248477346.54690373]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",292034276.28799695,365347177.36851561,470707687.89436835,491122090.38538355,487878328.8274315,448034367.37244231,398899775.58744305,null,292061713.97553861,365374615.24184763,471142592.81846213,491425489.41375488,487732225.55494571,447177860.68630117,397130437.65482032,null,null,{"$f":"S94","v":0},0,0,0,0,0]
["DRAB1102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1103","Straight line depreciation",-53618412.737644203,-61349793.282131851,-109964853.55165702,-121033449.50168431,-130649017.24709752,-134499764.08083999,-117975822.06443956,null,-53618412.551853888,-61349793.031647682,-110128392.13452086,-121465638.37203974,-131336941.90491799,-135381940.3851068,-118950175.44964379]
["DRAB1105","Actual additions (recognised in RAB)",126931313.81816289,141201616.55287141,131196469.22395173,118363778.38343248,91484078.866409376,86044542.93489708,93030895.093876958,null,126931313.81816289,141201616.55287141,131228501.91109309,118346464.95293075,91461600.110574439,86013887.992682248,92989494.558378056]
["DRAB1106","Disposals ",0,0,-817213.18127948174,-574090.43970021221,-679023.07430101512,-679370.63905630424,-679725.47006502224,null,0,0,-817213.18127948174,-574090.43970021221,-679023.07430101512,-679370.63905630424,-679725.47006502224]
["DRAB1107","Closing value",{"$f":"SUM(C89+C90+C91+C92+C93)","v":365347177.36851561},445199000.63925517,491122090.38538355,487878328.8274315,448034367.37244231,398899775.58744305,373275123.14681542,null,{"$f":"SUM(K89+K90+K91+K92+K93)","v":365374615.24184763},445226438.76307136,491425489.41375488,487732225.55494571,447177860.68630117,397130437.65482032,370490031.29348958,null,{"$f":"SUM(S89+S90+S91+S92+S93)","v":0},0,0,0,0,0,0]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED BENCHMARKING ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",{"$f":"IFERROR(AVERAGE(C27,C32),\"\")","v":2726137172.7771616},{"$f":"IFERROR(AVERAGE(D27,D32),\"\")","v":2822192543.4428663},2908002849.2451115,2992448808.7951441,3082506327.5751829,3171926163.145534,3255991347.8353395,null,{"$f":"IFERROR(AVERAGE(K27,K32),\"\")","v":3562312622.3343787},{"$f":"IFERROR(AVERAGE(L27,L32),\"\")","v":3665679237.5389643},3753187514.7986279,3838249153.253027,3928468218.2797246,4017603371.7708225,4100718693.3365521,null,{"$f":"IFERROR(AVERAGE(S27,S32),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T27,T32),\"\")","v":0},0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",{"$f":"IFERROR(AVERAGE(C34,C39),\"\")","v":2100958921.4788454},{"$f":"IFERROR(AVERAGE(D34,D39),\"\")","v":2065533173.6177745},2027984524.4230797,1987854571.4635944,1948007664.898653,1908188914.5175257,1869211730.0203962,null,{"$f":"IFERROR(AVERAGE(K34,K39),\"\")","v":2726960688.8721991},{"$f":"IFERROR(AVERAGE(L34,L39),\"\")","v":2686086507.307189},2641730009.8753815,2591818072.7739825,2541694722.7175789,2491072979.6882563,2440694933.717391,null,{"$f":"IFERROR(AVERAGE(S34,S39),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T34,T39),\"\")","v":0},0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",{"$f":"IFERROR(AVERAGE(C41,C46),\"\")","v":1561457280.7644849},{"$f":"IFERROR(AVERAGE(D41,D46),\"\")","v":1559636207.7745783},1566003135.4752693,1566780211.8051019,1567427418.7160921,1566473070.5082307,1567336958.1970673,null,{"$f":"IFERROR(AVERAGE(K41,K46),\"\")","v":2262419564.8942165},{"$f":"IFERROR(AVERAGE(L41,L46),\"\")","v":2268530091.7267284},2274823064.9491925,2268234101.3313036,2259937836.6854239,2248358264.900116,2236650433.7755399,null,{"$f":"IFERROR(AVERAGE(S41,S46),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T41,T46),\"\")","v":0},0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",{"$f":"IFERROR(AVERAGE(C48,C53),\"\")","v":623102965.67383754},{"$f":"IFERROR(AVERAGE(D48,D53),\"\")","v":639987527.870978},664344512.14149511,683207185.67357349,701754796.4451412,719005355.84035373,735790744.20601606,null,{"$f":"IFERROR(AVERAGE(K48,K53),\"\")","v":763126477.36793983},{"$f":"IFERROR(AVERAGE(L48,L53),\"\")","v":776135997.9083209},799286567.39614141,815557067.64127922,831676197.03400302,846571621.9431535,861053349.44670212,null,{"$f":"IFERROR(AVERAGE(S48,S53),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T48,T53),\"\")","v":0},0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",{"$f":"IFERROR(AVERAGE(C55,C60),\"\")","v":681682122.2988503},{"$f":"IFERROR(AVERAGE(D55,D60),\"\")","v":666233706.77592897},651001692.51780272,633792920.39003122,616439518.78639138,598786911.9431982,581728044.6062938,null,{"$f":"IFERROR(AVERAGE(K55,K60),\"\")","v":908495807.87552309},{"$f":"IFERROR(AVERAGE(L55,L60),\"\")","v":884789573.61723518},861321348.38183546,834937815.53211498,808042692.2266314,780437928.4929409,752962307.66489875,null,{"$f":"IFERROR(AVERAGE(S55,S60),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T55,T60),\"\")","v":0},0,0,0,0,0]
["DRAB1206","Zone substations and transformers",{"$f":"IFERROR(AVERAGE(C62,C67),\"\")","v":3345855898.1478529},{"$f":"IFERROR(AVERAGE(D62,D67),\"\")","v":3323848707.5029273},3311550018.6342373,3290654712.5846725,3268072564.5127907,3241867062.2818117,3215539189.6743398,null,{"$f":"IFERROR(AVERAGE(K62,K67),\"\")","v":3416318946.1205254},{"$f":"IFERROR(AVERAGE(L62,L67),\"\")","v":3388173756.6164026},3372633166.8551245,3350380198.7865009,3326511086.4209619,3299083433.1965342,3271583568.7511568,null,{"$f":"IFERROR(AVERAGE(S62,S67),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T62,T67),\"\")","v":0},0,0,0,0,0]
["DRAB1207","Easements ",{"$f":"IFERROR(AVERAGE(C69,C73),\"\")","v":213303501.46598941},{"$f":"IFERROR(AVERAGE(D69,D73),\"\")","v":215984194.34827051},219515392.27623981,223496862.76358956,227339518.49733323,230972452.23479724,234755455.68532377,null,{"$f":"IFERROR(AVERAGE(K69,K73),\"\")","v":213210122.44982523},{"$f":"IFERROR(AVERAGE(L69,L73),\"\")","v":215663231.86285895},221585867.54559821,225567338.0329479,229409993.76669163,233042927.50415564,236825930.95468211,null,{"$f":"IFERROR(AVERAGE(S69,S73),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T69,T73),\"\")","v":0},0,0,0,0,0]
["DRAB1208","Meters",{"$f":"IFERROR(AVERAGE(C75,C80),\"\")","v":45761144.729844943},{"$f":"IFERROR(AVERAGE(D75,D80),\"\")","v":45913823.262892492},43044274.390005775,42401916.04313834,42262497.85408178,43227619.996798724,44783069.845393956,null,{"$f":"IFERROR(AVERAGE(K75,K80),\"\")","v":68394552.146053866},{"$f":"IFERROR(AVERAGE(L75,L80),\"\")","v":62929512.605741501},54086380.154076412,51353309.971768357,49323342.019444078,48878927.055057749,49248451.26933451,null,{"$f":"IFERROR(AVERAGE(S75,S80),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T75,T80),\"\")","v":0},0,0,0,0,0]
["DRAB1209","“Other” assets with long lives",{"$f":"IFERROR(AVERAGE(C82,C87),\"\")","v":1012143066.4884267},{"$f":"IFERROR(AVERAGE(D82,D87),\"\")","v":1083878609.9408479},1173158504.4633894,1238187305.8975971,1298758880.3813848,1347603807.7143297,1387445954.9667964,null,{"$f":"IFERROR(AVERAGE(K82,K87),\"\")","v":1011275137.4095348},{"$f":"IFERROR(AVERAGE(L82,L87),\"\")","v":1078486978.0393271},1166589367.0172839,1232359099.116281,1293833489.8502655,1343726248.7764335,1384743335.298269,null,{"$f":"IFERROR(AVERAGE(S82,S87),\"\")","v":158713360.15765256},{"$f":"IFERROR(AVERAGE(T82,T87),\"\")","v":161188005.34431106},176909736.90523237,195815433.33132398,212877899.51735708,228307457.29127038,242036613.55263597]
["DRAB1210","“Other” assets with short lives",{"$f":"IFERROR(AVERAGE(C89,C94),\"\")","v":328690726.82825625},{"$f":"IFERROR(AVERAGE(D89,D94),\"\")","v":405273089.00388539},480914889.13987595,489500209.60640752,467956348.0999369,423467071.47994268,386087449.36712921,null,{"$f":"IFERROR(AVERAGE(K89,K94),\"\")","v":328718164.60869312},{"$f":"IFERROR(AVERAGE(L89,L94),\"\")","v":405300527.00245953},481284041.11610854,489578857.48435032,467455043.12062347,422154149.17056072,383810234.47415495,null,{"$f":"IFERROR(AVERAGE(S89,S94),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T89,T94),\"\")","v":0},0,0,0,0,0]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)"]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"FORECAST\n( years )",null,null,null,null,null,null,null,"FORECAST\n( years )",null,null,null,null,null,null,null,"FORECAST\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",43.503772402839935,43.372334560783003,43.273311372528234,43.167011712019622,43.064095714430849,42.962699122891799,42.878921783671487,null,43.484538340253877,43.487728690369103,43.506121880203253,43.5245490611116,43.541954768313211,43.558542759104213,43.575401280034697]
["DRAB1402","Underground network assets less than 33kV (cables)",60,60,60,60,60,60,60,null,60,60,60,60,60,60,60]
["DRAB1403","Distribution substations including transformers",38.841269174067058,38.81005840920966,39.095527164064279,39.399659173041293,39.718624138926643,40.048244670018875,40.382958382230846,null,39.36871261060481,39.350503624024341,39.543221184190649,39.750145023786565,39.969835144439287,40.200054277673701,40.437639837242543]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",50.54,50.54,50.54,50.54,50.54,50.54,50.54,null,50.54,50.54,50.54,50.54,50.54,50.54,50.54]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",45,45,45,45,45,45,45,null,45,45,45,45,45,45,45]
["DRAB1406","Zone substations and transformers",50.86664362663074,50.912163814487123,51.450191196944182,51.985111141166456,52.516497576823696,53.043854582752786,53.575630602989413,null,54.353181816373521,54.32834882129228,54.802255230183022,55.27176983800485,55.740284939318812,56.206946777259546,56.673860765410133]
["DRAB1407","Meters",15,15,15,15,15,15,15,null,15,15,15,15,15,15,15]
["DRAB1408","“Other” assets with long lives",33.917313112323036,33.965431738209602,34.365763234695024,34.86270758352611,35.326124081048036,35.837899781044833,36.382716617726103,null,33.917313112323036,33.965431738209602,34.365763234695024,34.86270758352611,35.326124081048036,35.837899781044833,36.382716617726103,null,20,20,20,20,20,20,20]
["DRAB1409","“Other” assets with short lives",6.4386431713780308,6.4175370577173467,6.0397393019407719,6.0113338979577922,5.9376534357405255,5.8453530092947759,5.806469014720312,null,6.4386431713780308,6.4175370577173467,6.0397393019407719,6.0113338979577922,5.9376534357405255,5.8453530092947759,5.806469014720312]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",31.499672136406506,31.424806259989335,31.357448120451135,31.342573373485727,31.316988705782002,31.285899044782791,31.213145618162084,null,30.054646573643751,29.984382409340306,29.923410355924332,29.918227558971576,29.913623259799646,29.913326866772941,29.88332174886164]
["DRAB1502","Underground network assets less than 33kV (cables)",39.040800137521728,38.174749916541167,37.347321828951294,36.533271907646366,35.725483440394804,34.923736710779835,34.151794674927622,null,39.41794339931387,38.605926070660047,37.802020661102709,37.014808384736646,36.239438192169644,35.476462475012752,34.743320934098357]
["DRAB1503","Distribution substations including transformers",24.875448490867846,24.47533241493603,24.19819974275428,23.961369569147223,23.733012563319001,23.515119371794967,23.366023941852635,null,25.185082532660545,24.862163729632364,24.571365535867251,24.340330960277633,24.145522300122046,23.98711197498238,23.913365211733513]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",34.681386101807924,34.679163431319829,34.76899965184915,34.870360836259067,34.930433035839684,34.957034613466512,34.991333379068678,null,33.62026021292926,33.494325294871558,33.516978933210417,33.564853413919764,33.58819685952286,33.592120379679073,33.613411991098438]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",25.514983161137348,24.808072584107087,24.206123620120337,23.630327835627515,23.067745395911036,22.518220305329901,22.056390680898442,null,25.047256919377936,24.259401911965348,23.571850290291234,22.907991876846637,22.258026709309508,21.62210195708051,21.060964909690945]
["DRAB1506","Zone substations and transformers",32.881025414858641,32.428302831723549,32.101130142093666,31.808331709544547,31.522719687521175,31.244814284857178,31.037762033529059,null,32.835868134873188,32.338962944191479,32.021001734531879,31.754774037098326,31.512012095903472,31.29259144504784,31.165003403604118]
["DRAB1507","Meters",10.814364544646002,10.484930567704019,10.365357779557446,10.257278299251572,10.153365886638388,10.072875235267421,10.15143554450594,null,8.2248524969174532,7.9686363583681628,8.0998299369726094,8.3830967925067501,8.8423930425611257,9.5629213082311271,10.801717359996832]
["DRAB1508","“Other” assets with long lives",26.160911766277945,26.388625510956803,26.265537203669663,26.353700005202725,26.222467164220884,26.142169191703406,25.962161714503083,null,26.160911766277945,26.388625510956803,26.265537203669663,26.353700005202725,26.222467164220884,26.142169191703406,25.962161714503083,null,12.154290941284666,12.345430077861284,13.634583960274089,14.556533801881798,15.255762356243173,15.812908399600666,16.278388465340189]
["DRAB1509","“Other” assets with short lives",5.2188648054578932,5.2725148179003698,5.1790288347694613,5.0999253713419384,4.929031921635576,4.8688892366345096,5.0786521877964015,null,5.2188648054578932,5.2725148179003698,5.1790288347694613,5.0999253713419384,4.929031921635576,4.8688892366345096,5.0786521877964015]

{"sheet":"3.4 Operational data","index":16,"n_rows":110,"n_cols":10,"rows_kept":110,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.4 OPERATIONAL DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped for ease of navigation. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOPED01","TOTAL ENERGY DELIVERED"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",16440.851254020788,16867.723826998306,8353.6929972059261,7632.8607782068148,6950.0639324152926,6285.5101981260068,5640.0460671655028]
["DOPED0202","Energy Delivery at On-peak times","GWh",1838.0269496905914,1701.7141347788258,2830.2162033343443,3064.5366885931157,3310.4376111286942,3552.4462845039748,3826.3336404168281]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",17.134122660030378,12.291247760062692,7080.182889417677,7526.7941682552628,7998.1756397343543,8404.6872131274922,8884.0293149948156]
["DOPED0204","Energy Delivery at Off-peak times","GWh",1538.3100988326805,1431.3800097338421,1818.4044605349513,1937.2482922501245,2062.00034497158,2180.4207254810713,2315.6858518562158]
["DOPED0205","Controlled load energy deliveries","GWh",1239.551461,1213.134753,1184.9208060000001,1156.7719320000001,1129.560403,1097.4977690000001,1070.097362]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",225.73882200000006,215.31213700000001,203.613091,188.43239800000001,173.69789499999999,157.89330000000001,143.98435900000001]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",8465,8269,8064,7877,7724,7552,7469]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",0,0,0,0,0,0,0]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",10666,10504,10328,10140,9995,9772,9664]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",-1.8,-1.8,-1.8,-1.8,-1.8,-1.8,-1.8]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",126,126,126,126,126,126,126]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh"]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",157,157,157,157,157,157,157]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh"]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",3070,3481,3889,4305,4746,5184,5589]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh"]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh"]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh"]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",8228.7942369324974,8350.3521667881087,8365.6442406506831,8387.3786375908658,8456.8819121561919,8558.5464056388337,8742.8668504569287]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",1004.4916098037842,886.44445849395095,695.30866735578797,544.30142491774325,412.83731533922065,292.52061031121173,188.61969753500199]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",6308.0894567981368,6464.8985626889789,6681.9156641864274,6861.9830124967075,7055.9699194545101,7144.9463899884986,7280.1569041414314]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",5532.498582669672,5524.5487842999992,5524.5487842999992,5524.5487842999992,5524.5487842999992,5524.5487842999992,5524.5487842999992]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",225.73882200000006,215.31213700000001,203.613091,188.43239800000001,173.69789499999999,157.89330000000001,143.98435900000001]
[]
[]
[]
[null,"3.4.2 - CUSTOMER NUMBERS (Benchmarking)"]
[null,null,null,"FORECAST"]
[null,null,"Units","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30"]
[null,"3.4.2.1 - Distribution customer numbers by customer type or class"]
["DOPCN0101","Residential customer numbers","number",1458606.3606371135,1477831.8979431984,1497354.2199389427,1518545.6812313071,1539456.7483479551,1558267.7564102791,1576530.9064634026]
["DOPCN0102","Non residential customers not on demand tariff customer numbers","number",90848.577999999994,92120.458092000001,93373.296322051203,94512.450537180222,95618.246208465236,96784.788812208513,97936.527799073796]
["DOPCN0103","Low voltage demand tariff customer numbers","number",40839.0524,41410.799133599998,41973.986001816957,42486.068631039125,42983.155634022281,43507.550132757351,44025.289979337162]
["DOPCN0104","High voltage demand tariff customer numbers","number",783.71019999999999,794.68214279999995,805.48981994207998,815.31679574537338,824.85600225559426,834.91924548311249,844.85478450436153]
["DOPCN0105","Unmetered Customer Numbers","number",32600.7232,33057.133324800001,33506.710338017278,33915.49220414109,34312.303462929543,34730.913565177281,35144.211436602891]
["DOPCN0106","Other Customer Numbers","number",0,0,0,0,0,0,0]
[null,"Total customer numbers",null,{"$f":"SUM(D48:D53)","v":1623678.4244371133},{"$f":"SUM(E48:E53)","v":1645214.9706363985},1667013.7024207702,1690275.0093994131,1713195.3096556277,1734125.9281659052,1754481.7904629209]
[]
[]
[null,"Table 3.4.2.2 Distribution customer numbers by location on the network"]
["DOPCN0201",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},"number",4065.5510857801255,4122.468800981047,4178.534376674389,4229.5124960698167,4278.9977922738335,4331.2015653395747,4382.7428639671152]
["DOPCN0202",{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},"number",1051394.1630535026,1064918.7295934169,1078825.4324996043,1094910.8425852088,1110865.3820896975,1124447.5754836707,1137548.2653837674]
["DOPCN0203",{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},"number",535617.98709783063,543116.63891720027,550503.02520647424,557219.1621139932,563738.62631072686,570616.23755171779,577406.57077858318]
["DOPCN0204",{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},"number",0,0,0,0,0,0,0]
["DOPCN0205",{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},"number"]
[null,"Total customer numbers",null,{"$f":"SUM(D58:D62)","v":1591077.7012371132},{"$f":"SUM(E58:E62)","v":1612157.8373115982},1633506.9920827528,1656359.5171952718,1678883.0061926981,1699395.0146007279,1719337.5790263177]
[]
[]
[null," 3.4.2.4 - Unmetered Supply"]
["DOPCN0301","Number of unmetered connections reported in customer numbers in the economic benchmarking RIN",null,{"$f":"D52","v":32600.7232},{"$f":"E52","v":33057.133324800001},33506.710338017278,33915.49220414109,34312.303462929543,34730.913565177281,35144.211436602891]
["DOPCN0302","Unmetered connections not reported in customer numbers in the economic benchmarking RIN"]
["DOPCN0303","Total unmetered connections",null,{"$f":"SUM(D67:D68)","v":32600.7232},{"$f":"SUM(E67:E68)","v":33057.133324800001},33506.710338017278,33915.49220414109,34312.303462929543,34730.913565177281,35144.211436602891]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5852.8058204352801,5860.9196110963803,5862.4684228002998,5835.6720570325797,5841.2000680267802,5873.5889724195004,5907.2385393083096]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5493.0098959803499,5508.63552123308,5512.1707423031303,5489.0798836648401,5494.8623912036401,5525.1318645477204,5556.9189122915204]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5414.8371868108397,5418.7385578543399,5413.7517185056704,5386.8577851007703,5393.3042058076599,5423.9844763480796,5455.1143996445298]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5076.8059240675002,5085.5802248720402,5082.7074326863803,5059.3572203254398,5065.9973158796402,5094.6694035269202,5123.63952018084]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",6019.9951629638599,6080.1179351806604,6108.6841964721598,6125.7815208435004,6145.9663543701099,6177.31247711181,6210.4193763732901]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5665.2410545349103,5729.5109272003101,5760.1406269073404,5780.7383613586398,5801.3298072814896,5830.62232017517,5861.4285945892298]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5641.66525840759,5689.2163219451904,5720.0033760070801,5739.9763183593705,5762.8231048583903,5793.9236698150598,5825.5860500335602]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5294.6066594123804,5346.49873971939,5379.4077191352799,5402.9795041084199,5426.0223603248596,5455.0864415168699,5484.5473351478504]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5888.9435266256296,5897.87250974774,5900.2257741391604,5873.4499544799301,5878.8633228838398,5910.2320550978102,5943.8098788261404]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5527.4415174126598,5545.0321345031198,5548.9656793475096,5525.9517027735701,5531.6219318210997,5562.0491327047303,5592.59835919737]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5462.9480805222902,5467.1697545737397,5461.7340719247304,5435.0962808678796,5442.5428205009503,5473.4775628202397,5504.9089722661101]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5121.9264358824503,5132.1228036586499,5129.1054465016696,5105.5430819725698,5112.1120906879296,5141.3353832401199,5170.5766857242697]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",6084.4613113403302,6145.37233543396,6173.9427757263102,6190.7052497863697,6211.1996898651096,6242.8649520873996,6276.2712917327799]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5724.9453954696601,5790.0737943649201,5820.7194643020603,5841.0336484909003,5861.9236478805497,5891.4934244155802,5922.5599431991504]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5677.0317134857096,5720.7439746856599,5748.9915161132803,5769.7354507446198,5793.6228141784604,5824.9075622558503,5856.7540588378897]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5326.80412340164,5375.4415631294196,5410.6841759681702,5435.1770482063203,5458.7029080390903,5485.42647409439,5515.0314774513199]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.99,0.99,0.99,0.99,0.99,0.99,0.99]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.96,0.96,0.96,0.96,0.96,0.96,0.96]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.99,0.99,0.99,0.99,0.99,0.99,0.99]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",1,1,1,1,1,1,1]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0.99,0.99,0.99,0.99,0.99,0.99,0.99]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0.97,0.97,0.97,0.97,0.97,0.97,0.97]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0.99,0.99,0.99,0.99,0.99,0.99,0.99]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]

{"sheet":"3.5 Physical assets","index":17,"n_rows":96,"n_cols":10,"rows_kept":96,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",14153.4,14150.4,14150.4,14147.4,14145.4,14143.4,14143.4]
["DPA0102","Overhead 2.2 kV","km"]
["DPA0103","Overhead 7.6 kV","km"]
["DPA0104","Overhead 11 kV","km",17534.203999300898,17535.808071905471,17542.412217817131,17548.0167569433,17553.621963505586,17559.227334827901,17564.227334827901]
["DPA0105","Overhead SWER","km",41,41,41,41,41,41,41]
["DPA0106","Overhead 22 kV","km"]
["DPA0107","Overhead 33 kV","km",2183,2186,2188,2191,2191,2191,2215.6055360899118]
["DPA0108","Overhead 44 kV","km"]
["DPA0109","Overhead 66 kV","km"]
["DPA0110","Overhead 132 kV","km",822,822,822,822,822,822,826]
["DPA0111","Overhead 6.6kv","km"]
["DPA0112","Overhead 110kV","km",366,366,366,375,375,375,375]
["DPA0113","Overhead 220kV","km"]
["DPA0114","Other ","km"]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D14:D27)","v":35099.603999300896},35101.208071905472,35109.812217817132,35124.416756943298,35128.021963505584,35131.627334827899,35165.232870917811]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",13784.920889186007,14077.731063919982,14377.500768806276,14687.569662550051,15001.744421657999,15323.307439600336,15648.551462768673]
["DPA0202","Underground 5 kV","km"]
["DPA0203","Underground 6.6 Kv","km"]
["DPA0204","Underground 7.6 kV","km"]
["DPA0205","Underground 11 kV","km",6838.0635556298266,6978.7660993133204,7121.2085255348939,7266.2257489708372,7412.2694387478241,7560.1601932334088,7708.9711990254928]
["DPA0206","Underground SWER","km"]
["DPA0207","Underground 22 kV","km"]
["DPA0208","Underground 33 kV","km",815,815,815,815,815,819,829]
["DPA0209","Underground 66 kV","km"]
["DPA0210","Underground 110 kV","km",165,165,165,165,165,170,170]
["DPA0211","Underground 132 kV","km"]
["DPA0212","Other ","km"]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D30:D41)","v":21602.984444815833},22036.497163233304,22478.70929434117,22933.795411520889,23394.013860405823,23872.467632833745,24356.522661794166]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001]
["DPA0302","Overhead 6.6 kV","MVA"]
["DPA0303","Overhead 7.6 kV","MVA"]
["DPA0304","Overhead 11 kV","MVA",1.01383333333333,1.02433333333333,1.0348333333333299,1.0453333333333299,1.0558333333333301,1.06633333333333,1.07683333333333]
["DPA0305","Overhead SWER","MVA",0.09,0.09,0.09,0.09,0.09,0.09,0.09]
["DPA0306","Overhead 22 kV","MVA"]
["DPA0307","Overhead 33 kV","MVA",24.817,24.817,24.817,24.817,24.817,24.817,24.817]
["DPA0308","Overhead 44 kV","MVA"]
["DPA0309","Overhead 66 kV","MVA"]
["DPA0310","Overhead 110 kV","MVA",150.73500000000001,150.73500000000001,150.73500000000001,150.73500000000001,150.73500000000001,150.73500000000001,150.73500000000001]
["DPA0311","Overhead 132 kV","MVA",184.20599999999999,184.20599999999999,184.20599999999999,183,183,183,183]
["DPA0312","Overhead 220 kV","MVA"]
["DPA0313","Other ","MVA"]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.15,0.15,0.15,0.15,0.15,0.15,0.15]
["DPA0402","Underground 5 kV","MVA"]
["DPA0403","Underground 6.6 kV","MVA"]
["DPA0404","Underground 7.6 kV","MVA"]
["DPA0405","Underground 11 kV","MVA",2.8620000000000001,2.8620000000000001,2.8620000000000001,2.8620000000000001,2.8620000000000001,2.8620000000000001,2.8620000000000001]
["DPA0406","Underground SWER","MVA"]
["DPA0407","Underground 12.7 kV","MVA"]
["DPA0408","Underground 22 kV","MVA"]
["DPA0409","Underground 33 kV","MVA",34.811999999999998,34.811999999999998,34.811999999999998,34.811999999999998,34.811999999999998,34.811999999999998,34.811999999999998]
["DPA0410","Underground 66 kV","MVA"]
["DPA0411","Underground 110 kV","MVA",167.28800000000001,167.28800000000001,167.28800000000001,167.28800000000001,167.28800000000001,167.28800000000001,167.28800000000001]
["DPA0412","Underground 132 kV","MVA",0,0,0,180,180,180,180]
["DPA0413","Other","MVA"]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",16880.400000000001,17159,17437.599999999999,17716.2,17994.8,18273.400000000001,18552]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",2456,2456,2456,2456,2456,2456,2456]
["DPA0503","Cold spare capacity included in DPA0501","MVA",133,133,133,133,133,133,133]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",8324,8324,8324,8324,8324,8354,8369]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",8610,8610,8610,8610,8610,8640,8655]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",3915,3967.0093998842476,4058.0187997684952,4093.0281996527428,4128.0375995369905,4196.0469994212381,4280.0563993054857]
["DPA0604","Total zone substation transformer  capacity ","MVA",21430,21482.009399884249,21573.018799768495,21608.028199652741,21643.03759953699,21771.04699942124,21885.056399305486]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",581,581,581,581,581,581,581]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DPA0701","Public lighting luminaires","0's",352045,355732.4,359419.8,363107.2,366794.6,370482,374169.4]
["DPA0702","Public lighting poles","0's",188986.4,191853,194719.6,197586.2,200452.8,203319.4,206186]

{"sheet":"3.6 Quality of service","index":18,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DQS0201","Energy Not Supplied (planned)","GWh",2.0259999999999998,2.0529999999999999,2.08,2.109,2.1379999999999999,2.1640000000000001,2.1890000000000001]
["DQS0202","Energy Not Supplied (unplanned)","GWh",3.613,3.661,3.7090000000000001,3.7610000000000001,3.8119999999999998,3.859,3.9039999999999999]
["DQS02","Total",null,{"$f":"SUM(D10:D11)","v":5.6389999999999993},5.7140000000000004,5.7889999999999997,5.87,5.9499999999999993,6.0229999999999997,6.093]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DQS03","System losses","%",{"$f":"(('3.4 Operational data'!D22+'3.4 Operational data'!D24+'3.4 Operational data'!D25+'3.4 Operational data'!D27+'3.4 Operational data'!D29+'3.4 Operational data'!D31)-SUM('3.4 Operational data'!D15:D20))/('3.4 Operational data'!D22+'3.4 Operational data'!D24+'3.4 Operational data'!D25+'3.4 Operational data'!D27+'3.4 Operational data'!D29+'3.4 Operational data'!D31)","v":5.2601048464825932E-2},{"$f":"(('3.4 Operational data'!E22+'3.4 Operational data'!E24+'3.4 Operational data'!E25+'3.4 Operational data'!E27+'3.4 Operational data'!E29+'3.4 Operational data'!E31)-SUM('3.4 Operational data'!E15:E20))/('3.4 Operational data'!E22+'3.4 Operational data'!E24+'3.4 Operational data'!E25+'3.4 Operational data'!E27+'3.4 Operational data'!E29+'3.4 Operational data'!E31)","v":4.8530471916333688E-2},{"$f":"(('3.4 Operational data'!F22+'3.4 Operational data'!F24+'3.4 Operational data'!F25+'3.4 Operational data'!F27+'3.4 Operational data'!F29+'3.4 Operational data'!F31)-SUM('3.4 Operational data'!F15:F20))/('3.4 Operational data'!F22+'3.4 Operational data'!F24+'3.4 Operational data'!F25+'3.4 Operational data'!F27+'3.4 Operational data'!F29+'3.4 Operational data'!F31)","v":4.8362728479806973E-2},{"$f":"(('3.4 Operational data'!G22+'3.4 Operational data'!G24+'3.4 Operational data'!G25+'3.4 Operational data'!G27+'3.4 Operational data'!G29+'3.4 Operational data'!G31)-SUM('3.4 Operational data'!G15:G20))/('3.4 Operational data'!G22+'3.4 Operational data'!G24+'3.4 Operational data'!G25+'3.4 Operational data'!G27+'3.4 Operational data'!G29+'3.4 Operational data'!G31)","v":4.8513296466636734E-2},{"$f":"(('3.4 Operational data'!H22+'3.4 Operational data'!H24+'3.4 Operational data'!H25+'3.4 Operational data'!H27+'3.4 Operational data'!H29+'3.4 Operational data'!H31)-SUM('3.4 Operational data'!H15:H20))/('3.4 Operational data'!H22+'3.4 Operational data'!H24+'3.4 Operational data'!H25+'3.4 Operational data'!H27+'3.4 Operational data'!H29+'3.4 Operational data'!H31)","v":4.9338534513460625E-2},{"$f":"(('3.4 Operational data'!I22+'3.4 Operational data'!I24+'3.4 Operational data'!I25+'3.4 Operational data'!I27+'3.4 Operational data'!I29+'3.4 Operational data'!I31)-SUM('3.4 Operational data'!I15:I20))/('3.4 Operational data'!I22+'3.4 Operational data'!I24+'3.4 Operational data'!I25+'3.4 Operational data'!I27+'3.4 Operational data'!I29+'3.4 Operational data'!I31)","v":4.8739951808815338E-2},{"$f":"(('3.4 Operational data'!J22+'3.4 Operational data'!J24+'3.4 Operational data'!J25+'3.4 Operational data'!J27+'3.4 Operational data'!J29+'3.4 Operational data'!J31)-SUM('3.4 Operational data'!J15:J20))/('3.4 Operational data'!J22+'3.4 Operational data'!J24+'3.4 Operational data'!J25+'3.4 Operational data'!J27+'3.4 Operational data'!J29+'3.4 Operational data'!J31)","v":4.8820312155119297E-2}]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DQS04","Overall utilisation","%",{"$f":"'3.4 Operational data'!D88/('3.5 Physical assets'!D87-'3.5 Physical assets'!D88)","v":0.26511782423198521},{"$f":"'3.4 Operational data'!E88/('3.5 Physical assets'!E87-'3.5 Physical assets'!E88)","v":0.26529972923383444},{"$f":"'3.4 Operational data'!F88/('3.5 Physical assets'!F87-'3.5 Physical assets'!F88)","v":0.26433692406033404},{"$f":"'3.4 Operational data'!G88/('3.5 Physical assets'!G87-'3.5 Physical assets'!G88)","v":0.26280231568172008},{"$f":"'3.4 Operational data'!H88/('3.5 Physical assets'!H87-'3.5 Physical assets'!H88)","v":0.26263470026008795},{"$f":"'3.4 Operational data'!I88/('3.5 Physical assets'!I87-'3.5 Physical assets'!I88)","v":0.26248403945761167},{"$f":"'3.4 Operational data'!J88/('3.5 Physical assets'!J87-'3.5 Physical assets'!J88)","v":0.26251330987744143}]

{"sheet":"3.7 Operating Environment","index":19,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOEF0101","Customer density","Customer / km",34.402882117914935]
["DOEF0102","Energy density","MWh/customer",13.11812264524492]
["DOEF0103","Demand density","kVA / customer",3.4409522944402404]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOEF0201","Rural proportion","%",0.37180000000000002]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",87609]
["DOEF0203","Rural vegetation maintenance spans","0's",41247]
["DOEF0204","Total vegetation maintenance spans","0's",128853]
["DOEF0205","Total number of spans","0's",287860.36922547099]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",1.38]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1.77]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",2.52]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",3.05]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",2.52]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",3.05]
["DOEF0212","Tropical proportion","Spans",92981]
["DOEF0213","Standard vehicle access","km",5206,5211,5216,5221,5226,5231,5236]
["DOEF0214","Bushfire risk","Spans",11270]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOEF0301","Route Line length","km",47196,47509,47824,48141,48460,48781,49104]

{"sheet":"4.1 Public lighting","index":20,"n_rows":159,"n_cols":10,"rows_kept":159,"cut":false,"hidden":false,"merged":[[213,1,213,2],[214,1,214,2],[215,1,215,2],[216,1,216,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2],[212,1,212,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[206,1,206,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[151,1,151,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[96,1,96,2],[94,1,94,2],[97,1,97,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[6,1,6,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[55,1,55,2],[56,1,56,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"4.1 PUBLIC LIGHTING"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. There are no further instructions."]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","number",591,603,615,627,639,652,665]
[null,"Number of poles installed ","number",402,412,422,433,444,455,466]
[null,"Total expenditure","$",4760051.3127704933,4893428.5948977992,5008562.3510174863,5141419.3705026982,5271049.7559998967,5425198.7034218982,5587962.1383584421]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","number",41228,34139,48246,48246,48246,48246,48246]
[null,"Number of poles replaced","number",421,432,443,454,465,477,489]
[null,"Total expenditure","$",17443564.457193442,14479078.202232381,25204067.079700459,25243588.634772137,25277784.855122477,25329674.087763324,25391717.140810546]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","number",46534,44207,41997,39897,37902,36007,34207]
[null,"Number of poles maintained","number",43136,44214,45234,46277,47344,48436,49553]
[null,"Total expenditure","$",9344116.4185582623,9429640.1897606477,9189812.3279618751,8874389.9075149521,8561976.1591611877,8279592.5255760578,8016555.5574398283]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","number of days",14,14,14,14,14,14,14]
[null,"GSO breaches","number",0,0,0,0,0,0,0]
[null,"GSL payments ","$",0,0,0,0,0,0,0]
[null,"Customer complaints ","number",41,41,41,41,41,41,41]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"LIGHT INSTALLATION"]
[null,"Minor LED",0,4857.3942265972419,5324.4401384528601,5359.8890553847177,5371.466838670407,5403.8999124013044,5431.2393592662256,5472.6102200219739]
[null,"Major LED",0,10228.826971167269,11212.422587156705,11272.399711971244,11291.988523514805,11346.863049442256,11393.119509692646,11463.116155401236]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"LED Major",0,722.31550166826412,722.96440995552746,723.25274448740925,723.84259496706693,724.35296600230436,725.12740133782609,726.05338020006866]
[null,"LED Minor",0,298.08980458150904,298.73871286877244,299.02704740065423,299.61689788031191,300.12726891554939,300.90170425107107,301.8276831133137]
[null,"Nostalgia LED",0,980.84872642490473,982.96849349663182,983.9103863007789,985.8372312009941,987.50444324943646,990.03426534547395,993.05912962879984]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"Major Road",0,29.889024562500005,30.162589443719686,29.395452078239241,28.386510403071636,27.387192567127002,26.483932057282431,25.642555724914093]
[null,"Minor Road",0,21.655281750000007,21.853485761888376,21.29767719892595,20.566675884400482,19.842647261454641,19.188214367753787,18.578617975702979]

{"sheet":"5.4 MD & utilisation-Spatial","index":21,"n_rows":11580,"n_cols":12,"rows_kept":11580,"cut":false,"hidden":false,"merged":[[11566,1,11566,2],[11567,1,11567,2],[11568,1,11568,2],[11569,1,11569,2],[11570,1,11570,2],[11571,1,11571,2],[11572,1,11572,2],[11579,1,11579,2],[11573,1,11573,2],[11574,1,11574,2],[11575,1,11575,2],[11576,1,11576,2],[11577,1,11577,2],[11578,1,11578,2],[11531,1,11531,2],[11532,1,11532,2],[11533,1,11533,2],[11534,1,11534,2],[11535,1,11535,2],[11536,1,11536,2],[11537,1,11537,2],[11538,1,11538,2],[11539,1,11539,2],[11540,1,11540,2],[11541,1,11541,2],[11542,1,11542,2],[11543,1,11543,2],[11544,1,11544,2],[11545,1,11545,2],[11546,1,11546,2],[11547,1,11547,2],[11548,1,11548,2],[11549,1,11549,2],[11550,1,11550,2],[11551,1,11551,2],[11552,1,11552,2],[11553,1,11553,2],[11554,1,11554,2],[11555,1,11555,2],[11556,1,11556,2],[11557,1,11557,2],[11558,1,11558,2],[11559,1,11559,2],[11560,1,11560,2],[11561,1,11561,2],[11562,1,11562,2],[11563,1,11563,2],[11500,1,11500,2],[11501,1,11501,2],[11502,1,11502,2],[11503,1,11503,2],[11504,1,11504,2],[11505,1,11505,2],[11506,1,11506,2],[11507,1,11507,2],[11508,1,11508,2],[11509,1,11509,2],[11510,1,11510,2],[11511,1,11511,2],[11512,1,11512,2],[11513,1,11513,2],[11514,1,11514,2],[11515,1,11515,2],[11516,1,11516,2],[11517,1,11517,2],[11518,1,11518,2],[11519,1,11519,2],[11520,1,11520,2],[11521,1,11521,2],[11522,1,11522,2],[11523,1,11523,2],[11524,1,11524,2],[11525,1,11525,2],[11526,1,11526,2],[11527,1,11527,2],[11528,1,11528,2],[11529,1,11529,2],[11530,1,11530,2],[11564,1,11564,2],[11565,1,11565,2],[11467,1,11467,2],[11468,1,11468,2],[11469,1,11469,2],[11470,1,11470,2],[11471,1,11471,2],[11472,1,11472,2],[11473,1,11473,2],[11474,1,11474,2],[11475,1,11475,2],[11476,1,11476,2],[11477,1,11477,2],[11478,1,11478,2],[11479,1,11479,2],[11480,1,11480,2],[11481,1,11481,2],[11482,1,11482,2],[11483,1,11483,2],[11484,1,11484,2],[11485,1,11485,2],[11486,1,11486,2],[11487,1,11487,2],[11488,1,11488,2],[11489,1,11489,2],[11490,1,11490,2],[11491,1,11491,2],[11492,1,11492,2],[11493,1,11493,2],[11494,1,11494,2],[11495,1,11495,2],[11496,1,11496,2],[11497,1,11497,2],[11498,1,11498,2],[11499,1,11499,2],[11434,1,11434,2],[11435,1,11435,2],[11436,1,11436,2],[11437,1,11437,2],[11438,1,11438,2],[11439,1,11439,2],[11440,1,11440,2],[11441,1,11441,2],[11442,1,11442,2],[11443,1,11443,2],[11444,1,11444,2],[11445,1,11445,2],[11446,1,11446,2],[11447,1,11447,2],[11448,1,11448,2],[11449,1,11449,2],[11450,1,11450,2],[11451,1,11451,2],[11452,1,11452,2],[11453,1,11453,2],[11454,1,11454,2],[11455,1,11455,2],[11456,1,11456,2],[11457,1,11457,2],[11458,1,11458,2],[11459,1,11459,2],[11460,1,11460,2],[11461,1,11461,2],[11462,1,11462,2],[11463,1,11463,2],[11464,1,11464,2],[11465,1,11465,2],[11466,1,11466,2],[11401,1,11401,2],[11402,1,11402,2],[11403,1,11403,2],[11404,1,11404,2],[11405,1,11405,2],[11406,1,11406,2],[11407,1,11407,2],[11408,1,11408,2],[11409,1,11409,2],[11410,1,11410,2],[11411,1,11411,2],[11412,1,11412,2],[11413,1,11413,2],[11414,1,11414,2],[11415,1,11415,2],[11416,1,11416,2],[11417,1,11417,2],[11418,1,11418,2],[11419,1,11419,2],[11420,1,11420,2],[11421,1,11421,2],[11422,1,11422,2],[11423,1,11423,2],[11424,1,11424,2],[11425,1,11425,2],[11426,1,11426,2],[11427,1,11427,2],[11428,1,11428,2],[11429,1,11429,2],[11430,1,11430,2],[11431,1,11431,2],[11432,1,11432,2],[11433,1,11433,2],[11368,1,11368,2],[11369,1,11369,2],[11370,1,11370,2],[11371,1,11371,2],[11372,1,11372,2],[11373,1,11373,2],[11374,1,11374,2],[11375,1,11375,2],[11376,1,11376,2],[11377,1,11377,2],[11378,1,11378,2],[11379,1,11379,2],[11380,1,11380,2],[11381,1,11381,2],[11382,1,11382,2],[11383,1,11383,2],[11384,1,11384,2],[11385,1,11385,2],[11386,1,11386,2],[11387,1,11387,2],[11388,1,11388,2],[11389,1,11389,2],[11390,1,11390,2],[11391,1,11391,2],[11392,1,11392,2],[11393,1,11393,2],[11394,1,11394,2],[11395,1,11395,2],[11396,1,11396,2],[11397,1,11397,2],[11398,1,11398,2],[11399,1,11399,2],[11400,1,11400,2],[11335,1,11335,2],[11336,1,11336,2],[11337,1,11337,2],[11338,1,11338,2],[11339,1,11339,2],[11340,1,11340,2],[11341,1,11341,2],[11342,1,11342,2],[11343,1,11343,2],[11344,1,11344,2],[11345,1,11345,2],[11346,1,11346,2],[11347,1,11347,2],[11348,1,11348,2],[11349,1,11349,2],[11350,1,11350,2],[11351,1,11351,2],[11352,1,11352,2],[11353,1,11353,2],[11354,1,11354,2],[11355,1,11355,2],[11356,1,11356,2],[11357,1,11357,2],[11358,1,11358,2],[11359,1,11359,2],[11360,1,11360,2],[11361,1,11361,2],[11362,1,11362,2],[11363,1,11363,2],[11364,1,11364,2],[11365,1,11365,2],[11366,1,11366,2],[11367,1,11367,2],[11302,1,11302,2],[11303,1,11303,2],[11304,1,11304,2],[11305,1,11305,2],[11306,1,11306,2],[11307,1,11307,2],[11308,1,11308,2],[11309,1,11309,2],[11310,1,11310,2],[11311,1,11311,2],[11312,1,11312,2],[11313,1,11313,2],[11314,1,11314,2],[11315,1,11315,2],[11316,1,11316,2],[11317,1,11317,2],[11318,1,11318,2],[11319,1,11319,2],[11320,1,11320,2],[11321,1,11321,2],[11322,1,11322,2],[11323,1,11323,2],[11324,1,11324,2],[11325,1,11325,2],[11326,1,11326,2],[11327,1,11327,2],[11328,1,11328,2],[11329,1,11329,2],[11330,1,11330,2],[11331,1,11331,2],[11332,1,11332,2],[11333,1,11333,2],[11334,1,11334,2],[11269,1,11269,2],[11270,1,11270,2],[11271,1,11271,2],[11272,1,11272,2],[11273,1,11273,2],[11274,1,11274,2],[11275,1,11275,2],[11276,1,11276,2],[11277,1,11277,2],[11278,1,11278,2],[11279,1,11279,2],[11280,1,11280,2],[11281,1,11281,2],[11282,1,11282,2],[11283,1,11283,2],[11284,1,11284,2],[11285,1,11285,2],[11286,1,11286,2],[11287,1,11287,2],[11288,1,11288,2],[11289,1,11289,2],[11290,1,11290,2],[11291,1,11291,2],[11292,1,11292,2],[11293,1,11293,2],[11294,1,11294,2],[11295,1,11295,2],[11296,1,11296,2],[11297,1,11297,2],[11298,1,11298,2],[11299,1,11299,2],[11300,1,11300,2],[11301,1,11301,2],[11236,1,11236,2],[11237,1,11237,2],[11238,1,11238,2],[11239,1,11239,2],[11240,1,11240,2],[11241,1,11241,2],[11242,1,11242,2],[11243,1,11243,2],[11244,1,11244,2],[11245,1,11245,2],[11246,1,11246,2],[11247,1,11247,2],[11248,1,11248,2],[11249,1,11249,2],[11250,1,11250,2],[11251,1,11251,2],[11252,1,11252,2],[11253,1,11253,2],[11254,1,11254,2],[11255,1,11255,2],[11256,1,11256,2],[11257,1,11257,2],[11258,1,11258,2],[11259,1,11259,2],[11260,1,11260,2],[11261,1,11261,2],[11262,1,11262,2],[11263,1,11263,2],[11264,1,11264,2],[11265,1,11265,2],[11266,1,11266,2],[11267,1,11267,2],[11268,1,11268,2],[11203,1,11203,2],[11204,1,11204,2],[11205,1,11205,2],[11206,1,11206,2],[11207,1,11207,2],[11208,1,11208,2],[11209,1,11209,2],[11210,1,11210,2],[11211,1,11211,2],[11212,1,11212,2],[11213,1,11213,2],[11214,1,11214,2],[11215,1,11215,2],[11216,1,11216,2],[11217,1,11217,2],[11218,1,11218,2],[11219,1,11219,2],[11220,1,11220,2],[11221,1,11221,2],[11222,1,11222,2],[11223,1,11223,2],[11224,1,11224,2],[11225,1,11225,2],[11226,1,11226,2],[11227,1,11227,2],[11228,1,11228,2],[11229,1,11229,2],[11230,1,11230,2],[11231,1,11231,2],[11232,1,11232,2],[11233,1,11233,2],[11234,1,11234,2],[11235,1,11235,2],[11170,1,11170,2],[11171,1,11171,2],[11172,1,11172,2],[11173,1,11173,2],[11174,1,11174,2],[11175,1,11175,2],[11176,1,11176,2],[11177,1,11177,2],[11178,1,11178,2],[11179,1,11179,2],[11180,1,11180,2],[11181,1,11181,2],[11182,1,11182,2],[11183,1,11183,2],[11184,1,11184,2],[11185,1,11185,2],[11186,1,11186,2],[11187,1,11187,2],[11188,1,11188,2],[11189,1,11189,2],[11190,1,11190,2],[11191,1,11191,2],[11192,1,11192,2],[11193,1,11193,2],[11194,1,11194,2],[11195,1,11195,2],[11196,1,11196,2],[11197,1,11197,2],[11198,1,11198,2],[11199,1,11199,2],[11200,1,11200,2],[11201,1,11201,2],[11202,1,11202,2],[11137,1,11137,2],[11138,1,11138,2],[11139,1,11139,2],[11140,1,11140,2],[11141,1,11141,2],[11142,1,11142,2],[11143,1,11143,2],[11144,1,11144,2],[11145,1,11145,2],[11146,1,11146,2],[11147,1,11147,2],[11148,1,11148,2],[11149,1,11149,2],[11150,1,11150,2],[11151,1,11151,2],[11152,1,11152,2],[11153,1,11153,2],[11154,1,11154,2],[11155,1,11155,2],[11156,1,11156,2],[11157,1,11157,2],[11158,1,11158,2],[11159,1,11159,2],[11160,1,11160,2],[11161,1,11161,2],[11162,1,11162,2],[11163,1,11163,2],[11164,1,11164,2],[11165,1,11165,2],[11166,1,11166,2],[11167,1,11167,2],[11168,1,11168,2],[11169,1,11169,2],[11104,1,11104,2],[11105,1,11105,2],[11106,1,11106,2],[11107,1,11107,2],[11108,1,11108,2],[11109,1,11109,2],[11110,1,11110,2],[11111,1,11111,2],[11112,1,11112,2],[11113,1,11113,2],[11114,1,11114,2],[11115,1,11115,2],[11116,1,11116,2],[11117,1,11117,2],[11118,1,11118,2],[11119,1,11119,2],[11120,1,11120,2],[11121,1,11121,2],[11122,1,11122,2],[11123,1,11123,2],[11124,1,11124,2],[11125,1,11125,2],[11126,1,11126,2],[11127,1,11127,2],[11128,1,11128,2],[11129,1,11129,2],[11130,1,11130,2],[11131,1,11131,2],[11132,1,11132,2],[11133,1,11133,2],[11134,1,11134,2],[11135,1,11135,2],[11136,1,11136,2],[11067,1,11067,2],[11068,1,11068,2],[11069,1,11069,2],[11070,1,11070,2],[11071,1,11071,2],[11072,1,11072,2],[11073,1,11073,2],[11077,5,11077,11],[11079,1,11079,2],[11080,1,11080,2],[11081,1,11081,2],[11082,1,11082,2],[11083,1,11083,2],[11084,1,11084,2],[11085,1,11085,2],[11086,1,11086,2],[11087,1,11087,2],[11088,1,11088,2],[11089,1,11089,2],[11090,1,11090,2],[11091,1,11091,2],[11092,1,11092,2],[11093,1,11093,2],[11094,1,11094,2],[11095,1,11095,2],[11096,1,11096,2],[11097,1,11097,2],[11098,1,11098,2],[11099,1,11099,2],[11100,1,11100,2],[11101,1,11101,2],[11102,1,11102,2],[11103,1,11103,2],[11034,1,11034,2],[11035,1,11035,2],[11036,1,11036,2],[11037,1,11037,2],[11038,1,11038,2],[11039,1,11039,2],[11040,1,11040,2],[11041,1,11041,2],[11042,1,11042,2],[11043,1,11043,2],[11044,1,11044,2],[11045,1,11045,2],[11046,1,11046,2],[11047,1,11047,2],[11048,1,11048,2],[11049,1,11049,2],[11050,1,11050,2],[11051,1,11051,2],[11052,1,11052,2],[11053,1,11053,2],[11054,1,11054,2],[11055,1,11055,2],[11056,1,11056,2],[11057,1,11057,2],[11058,1,11058,2],[11059,1,11059,2],[11060,1,11060,2],[11061,1,11061,2],[11062,1,11062,2],[11063,1,11063,2],[11064,1,11064,2],[11065,1,11065,2],[11066,1,11066,2],[10995,2,10996,2],[10995,3,10996,3],[10997,2,10998,2],[10997,3,10998,3],[10999,2,11000,2],[10999,3,11000,3],[11001,2,11002,2],[11001,3,11002,3],[11003,2,11004,2],[11003,3,11004,3],[11005,2,11006,2],[11005,3,11006,3],[11007,2,11008,2],[11007,3,11008,3],[11009,2,11010,2],[11009,3,11010,3],[11011,2,11012,2],[11011,3,11012,3],[11013,2,11014,2],[11013,3,11014,3],[11015,2,11016,2],[11015,3,11016,3],[11022,5,11022,11],[11024,1,11024,2],[11025,1,11025,2],[11026,1,11026,2],[11027,1,11027,2],[11028,1,11028,2],[11029,1,11029,2],[11030,1,11030,2],[11031,1,11031,2],[11032,1,11032,2],[11033,1,11033,2],[10961,2,10962,2],[10961,3,10962,3],[10963,2,10964,2],[10963,3,10964,3],[10965,2,10966,2],[10965,3,10966,3],[10967,2,10968,2],[10967,3,10968,3],[10969,2,10970,2],[10969,3,10970,3],[10971,2,10972,2],[10971,3,10972,3],[10973,2,10974,2],[10973,3,10974,3],[10975,2,10976,2],[10975,3,10976,3],[10977,2,10978,2],[10977,3,10978,3],[10979,2,10980,2],[10979,3,10980,3],[10981,2,10982,2],[10981,3,10982,3],[10983,2,10984,2],[10983,3,10984,3],[10985,2,10986,2],[10985,3,10986,3],[10987,2,10988,2],[10987,3,10988,3],[10989,2,10990,2],[10989,3,10990,3],[10991,2,10992,2],[10991,3,10992,3],[10993,2,10994,2],[10993,3,10994,3],[10927,2,10928,2],[10927,3,10928,3],[10929,2,10930,2],[10929,3,10930,3],[10931,2,10932,2],[10931,3,10932,3],[10933,2,10934,2],[10933,3,10934,3],[10935,2,10936,2],[10935,3,10936,3],[10937,2,10938,2],[10937,3,10938,3],[10939,2,10940,2],[10939,3,10940,3],[10941,2,10942,2],[10941,3,10942,3],[10943,2,10944,2],[10943,3,10944,3],[10945,2,10946,2],[10945,3,10946,3],[10947,2,10948,2],[10947,3,10948,3],[10949,2,10950,2],[10949,3,10950,3],[10951,2,10952,2],[10951,3,10952,3],[10953,2,10954,2],[10953,3,10954,3],[10955,2,10956,2],[10955,3,10956,3],[10957,2,10958,2],[10957,3,10958,3],[10959,2,10960,2],[10959,3,10960,3],[10893,2,10894,2],[10893,3,10894,3],[10895,2,10896,2],[10895,3,10896,3],[10897,2,10898,2],[10897,3,10898,3],[10899,2,10900,2],[10899,3,10900,3],[10901,2,10902,2],[10901,3,10902,3],[10903,2,10904,2],[10903,3,10904,3],[10905,2,10906,2],[10905,3,10906,3],[10907,2,10908,2],[10907,3,10908,3],[10909,2,10910,2],[10909,3,10910,3],[10911,2,10912,2],[10911,3,10912,3],[10913,2,10914,2],[10913,3,10914,3],[10915,2,10916,2],[10915,3,10916,3],[10917,2,10918,2],[10917,3,10918,3],[10919,2,10920,2],[10919,3,10920,3],[10921,2,10922,2],[10921,3,10922,3],[10923,2,10924,2],[10923,3,10924,3],[10925,2,10926,2],[10925,3,10926,3],[10859,2,10860,2],[10859,3,10860,3],[10861,2,10862,2],[10861,3,10862,3],[10863,2,10864,2],[10863,3,10864,3],[10865,2,10866,2],[10865,3,10866,3],[10867,2,10868,2],[10867,3,10868,3],[10869,2,10870,2],[10869,3,10870,3],[10871,2,10872,2],[10871,3,10872,3],[10873,2,10874,2],[10873,3,10874,3],[10875,2,10876,2],[10875,3,10876,3],[10877,2,10878,2],[10877,3,10878,3],[10879,2,10880,2],[10879,3,10880,3],[10881,2,10882,2],[10881,3,10882,3],[10883,2,10884,2],[10883,3,10884,3],[10885,2,10886,2],[10885,3,10886,3],[10887,2,10888,2],[10887,3,10888,3],[10889,2,10890,2],[10889,3,10890,3],[10891,2,10892,2],[10891,3,10892,3],[10825,2,10826,2],[10825,3,10826,3],[10827,2,10828,2],[10827,3,10828,3],[10829,2,10830,2],[10829,3,10830,3],[10831,2,10832,2],[10831,3,10832,3],[10833,2,10834,2],[10833,3,10834,3],[10835,2,10836,2],[10835,3,10836,3],[10837,2,10838,2],[10837,3,10838,3],[10839,2,10840,2],[10839,3,10840,3],[10841,2,10842,2],[10841,3,10842,3],[10843,2,10844,2],[10843,3,10844,3],[10845,2,10846,2],[10845,3,10846,3],[10847,2,10848,2],[10847,3,10848,3],[10849,2,10850,2],[10849,3,10850,3],[10851,2,10852,2],[10851,3,10852,3],[10853,2,10854,2],[10853,3,10854,3],[10855,2,10856,2],[10855,3,10856,3],[10857,2,10858,2],[10857,3,10858,3],[10791,2,10792,2],[10791,3,10792,3],[10793,2,10794,2],[10793,3,10794,3],[10795,2,10796,2],[10795,3,10796,3],[10797,2,10798,2],[10797,3,10798,3],[10799,2,10800,2],[10799,3,10800,3],[10801,2,10802,2],[10801,3,10802,3],[10803,2,10804,2],[10803,3,10804,3],[10805,2,10806,2],[10805,3,10806,3],[10807,2,10808,2],[10807,3,10808,3],[10809,2,10810,2],[10809,3,10810,3],[10811,2,10812,2],[10811,3,10812,3],[10813,2,10814,2],[10813,3,10814,3],[10815,2,10816,2],[10815,3,10816,3],[10817,2,10818,2],[10817,3,10818,3],[10819,2,10820,2],[10819,3,10820,3],[10821,2,10822,2],[10821,3,10822,3],[10823,2,10824,2],[10823,3,10824,3],[10757,2,10758,2],[10757,3,10758,3],[10759,2,10760,2],[10759,3,10760,3],[10761,2,10762,2],[10761,3,10762,3],[10763,2,10764,2],[10763,3,10764,3],[10765,2,10766,2],[10765,3,10766,3],[10767,2,10768,2],[10767,3,10768,3],[10769,2,10770,2],[10769,3,10770,3],[10771,2,10772,2],[10771,3,10772,3],[10773,2,10774,2],[10773,3,10774,3],[10775,2,10776,2],[10775,3,10776,3],[10777,2,10778,2],[10777,3,10778,3],[10779,2,10780,2],[10779,3,10780,3],[10781,2,10782,2],[10781,3,10782,3],[10783,2,10784,2],[10783,3,10784,3],[10785,2,10786,2],[10785,3,10786,3],[10787,2,10788,2],[10787,3,10788,3],[10789,2,10790,2],[10789,3,10790,3],[10723,2,10724,2],[10723,3,10724,3],[10725,2,10726,2],[10725,3,10726,3],[10727,2,10728,2],[10727,3,10728,3],[10729,2,10730,2],[10729,3,10730,3],[10731,2,10732,2],[10731,3,10732,3],[10733,2,10734,2],[10733,3,10734,3],[10735,2,10736,2],[10735,3,10736,3],[10737,2,10738,2],[10737,3,10738,3],[10739,2,10740,2],[10739,3,10740,3],[10741,2,10742,2],[10741,3,10742,3],[10743,2,10744,2],[10743,3,10744,3],[10745,2,10746,2],[10745,3,10746,3],[10747,2,10748,2],[10747,3,10748,3],[10749,2,10750,2],[10749,3,10750,3],[10751,2,10752,2],[10751,3,10752,3],[10753,2,10754,2],[10753,3,10754,3],[10755,2,10756,2],[10755,3,10756,3],[10689,2,10690,2],[10689,3,10690,3],[10691,2,10692,2],[10691,3,10692,3],[10693,2,10694,2],[10693,3,10694,3],[10695,2,10696,2],[10695,3,10696,3],[10697,2,10698,2],[10697,3,10698,3],[10699,2,10700,2],[10699,3,10700,3],[10701,2,10702,2],[10701,3,10702,3],[10703,2,10704,2],[10703,3,10704,3],[10705,2,10706,2],[10705,3,10706,3],[10707,2,10708,2],[10707,3,10708,3],[10709,2,10710,2],[10709,3,10710,3],[10711,2,10712,2],[10711,3,10712,3],[10713,2,10714,2],[10713,3,10714,3],[10715,2,10716,2],[10715,3,10716,3],[10717,2,10718,2],[10717,3,10718,3],[10719,2,10720,2],[10719,3,10720,3],[10721,2,10722,2],[10721,3,10722,3],[10655,2,10656,2],[10655,3,10656,3],[10657,2,10658,2],[10657,3,10658,3],[10659,2,10660,2],[10659,3,10660,3],[10661,2,10662,2],[10661,3,10662,3],[10663,2,10664,2],[10663,3,10664,3],[10665,2,10666,2],[10665,3,10666,3],[10667,2,10668,2],[10667,3,10668,3],[10669,2,10670,2],[10669,3,10670,3],[10671,2,10672,2],[10671,3,10672,3],[10673,2,10674,2],[10673,3,10674,3],[10675,2,10676,2],[10675,3,10676,3],[10677,2,10678,2],[10677,3,10678,3],[10679,2,10680,2],[10679,3,10680,3],[10681,2,10682,2],[10681,3,10682,3],[10683,2,10684,2],[10683,3,10684,3],[10685,2,10686,2],[10685,3,10686,3],[10687,2,10688,2],[10687,3,10688,3],[10621,2,10622,2],[10621,3,10622,3],[10623,2,10624,2],[10623,3,10624,3],[10625,2,10626,2],[10625,3,10626,3],[10627,2,10628,2],[10627,3,10628,3],[10629,2,10630,2],[10629,3,10630,3],[10631,2,10632,2],[10631,3,10632,3],[10633,2,10634,2],[10633,3,10634,3],[10635,2,10636,2],[10635,3,10636,3],[10637,2,10638,2],[10637,3,10638,3],[10639,2,10640,2],[10639,3,10640,3],[10641,2,10642,2],[10641,3,10642,3],[10643,2,10644,2],[10643,3,10644,3],[10645,2,10646,2],[10645,3,10646,3],[10647,2,10648,2],[10647,3,10648,3],[10649,2,10650,2],[10649,3,10650,3],[10651,2,10652,2],[10651,3,10652,3],[10653,2,10654,2],[10653,3,10654,3],[10587,2,10588,2],[10587,3,10588,3],[10589,2,10590,2],[10589,3,10590,3],[10591,2,10592,2],[10591,3,10592,3],[10593,2,10594,2],[10593,3,10594,3],[10595,2,10596,2],[10595,3,10596,3],[10597,2,10598,2],[10597,3,10598,3],[10599,2,10600,2],[10599,3,10600,3],[10601,2,10602,2],[10601,3,10602,3],[10603,2,10604,2],[10603,3,10604,3],[10605,2,10606,2],[10605,3,10606,3],[10607,2,10608,2],[10607,3,10608,3],[10609,2,10610,2],[10609,3,10610,3],[10611,2,10612,2],[10611,3,10612,3],[10613,2,10614,2],[10613,3,10614,3],[10615,2,10616,2],[10615,3,10616,3],[10617,2,10618,2],[10617,3,10618,3],[10619,2,10620,2],[10619,3,10620,3],[10553,2,10554,2],[10553,3,10554,3],[10555,2,10556,2],[10555,3,10556,3],[10557,2,10558,2],[10557,3,10558,3],[10559,2,10560,2],[10559,3,10560,3],[10561,2,10562,2],[10561,3,10562,3],[10563,2,10564,2],[10563,3,10564,3],[10565,2,10566,2],[10565,3,10566,3],[10567,2,10568,2],[10567,3,10568,3],[10569,2,10570,2]],"merged_total":11555,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"DEMAND"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Abermain BS","Substation Rating","MVA","Non-Coincident",264,264,264,264,264,264,264]
[null,null,null,null,"Coincident",264,264,264,264,264,264,264]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",110.18,109.8,109.93,109.63,110.15,111.23,112.2]
[null,null,null,null,"Coincident",110.14,109.75,109.9,109.6,110.14,111.23,112.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",112.57,112.19,112.32,112.01,112.55,113.65,114.64]
[null,null,null,null,"Coincident",110.34,109.77,109.91,109.61,110.16,111.25,112.22]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",101.3,100.82,100.97,100.72,101.24,102.25,103.15]
[null,null,null,null,"Coincident",101.3,100.82,100.97,100.72,101.24,102.25,103.15]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",103.5,103.01,103.17,102.91,103.44,104.47,105.39]
[null,null,null,null,"Coincident",101.4,103.49,103.65,103.41,103.94,104.98,105.9]
[null,"Algester BS","Substation Rating","MVA","Non-Coincident",202,202,202,202,202,202,202]
[null,null,null,null,"Coincident",202,202,202,202,202,202,202]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",77.22,76.14,75.66,74.900000000000006,74.98,75.56,76.2]
[null,null,null,null,"Coincident",76.89,75.81,75.34,74.58,74.66,75.239999999999995,75.88]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",78.709999999999994,77.61,77.12,76.349999999999994,76.430000000000007,77.03,77.680000000000007]
[null,null,null,null,"Coincident",78.3,77.209999999999994,76.72,75.95,76.03,76.61,77.25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",73.05,72.03,71.58,70.86,70.92,71.47,72.06]
[null,null,null,null,"Coincident",72.739999999999995,71.73,71.28,70.56,70.63,71.17,71.760000000000005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",74.459999999999994,73.430000000000007,72.97,72.23,72.3,72.849999999999994,73.459999999999994]
[null,null,null,null,"Coincident",74.09,73.06,72.599999999999994,71.86,71.930000000000007,72.47,73.069999999999993]
[null,"Archerfield BS","Substation Rating","MVA","Non-Coincident",176,176,176,176,176,176,176]
[null,null,null,null,"Coincident",176,176,176,176,176,176,176]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63.99,63.1,62.14,60.92,60.5,60.38,60.44]
[null,null,null,null,"Coincident",47.11,46.71,46.08,45.28,45.05,45.06,45.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.38,66.44,65.430000000000007,64.150000000000006,63.71,63.59,63.65]
[null,null,null,null,"Coincident",48.11,47.73,47.08,46.26,46.03,46.03,46.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.88,60.07,59.15,57.99,57.59,57.47,57.52]
[null,null,null,null,"Coincident",44.71,44.37,43.77,43,42.79,42.79,42.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64.11,63.25,62.29,61.07,60.64,60.52,60.57]
[null,null,null,null,"Coincident",45.67,45.34,44.73,43.94,43.72,43.72,43.83]
[null,"Ashgrove West BS","Substation Rating","MVA","Non-Coincident",168,168,168,168,168,168,168]
[null,null,null,null,"Coincident",168,168,168,168,168,168,168]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",83.32,81.819999999999993,84.37,83.42,83.36,83.98,84.88]
[null,null,null,null,"Coincident",76.62,75.12,77.77,76.819999999999993,76.75,77.38,78.27]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",83.76,82.25,84.81,83.86,83.79,84.43,85.32]
[null,null,null,null,"Coincident",76.95,75.44,77.81,76.87,76.8,77.430000000000007,78.319999999999993]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",77.989999999999995,76.599999999999994,79.209999999999994,78.319999999999993,78.260000000000005,78.849999999999994,79.680000000000007]
[null,null,null,null,"Coincident",71.36,69.97,72.680000000000007,71.8,71.739999999999995,72.319999999999993,73.150000000000006]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",78.400000000000006,77,79.62,78.739999999999995,78.67,79.260000000000005,80.099999999999994]
[null,null,null,null,"Coincident",71.67,70.27,72.72,71.83,71.77,72.36,73.19]
[null,"Beaudesert BS","Substation Rating","MVA","Non-Coincident",145,145,145,145,145,145,145]
[null,null,null,null,"Coincident",145,145,145,145,145,145,145]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.6,39.590000000000003,39.86,39.869999999999997,40.24,40.81,41.33]
[null,null,null,null,"Coincident",37.479999999999997,37.479999999999997,37.74,37.75,38.1,38.64,39.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.06,41.05,41.33,41.34,41.72,42.32,42.86]
[null,null,null,null,"Coincident",38.49,38.49,38.76,38.770000000000003,39.130000000000003,39.69,40.200000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.630000000000003,37.619999999999997,37.880000000000003,37.89,38.24,38.79,39.28]
[null,null,null,null,"Coincident",35.61,35.61,35.86,35.869999999999997,36.200000000000003,36.72,37.19]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.020000000000003,39.01,39.28,39.29,39.65,40.22,40.729999999999997]
[null,null,null,null,"Coincident",36.78,36.78,37.03,37.04,37.39,37.71,38.19]
[null,"Beenleigh BS","Substation Rating","MVA","Non-Coincident",260,260,260,260,260,260,260]
[null,null,null,null,"Coincident",260,260,260,260,260,260,260]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",137.86000000000001,162.41,161.07,159.31,158.83000000000001,159.15,159.34]
[null,null,null,null,"Coincident",136.74,158.46,157.13,155.38999999999999,154.91999999999999,155.25,155.44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",139.11000000000001,162.41999999999999,161.07,159.32,158.84,159.16,159.35]
[null,null,null,null,"Coincident",137.37,158.46,157.13,155.4,154.91999999999999,155.25,155.44999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",127.2,151.81,150.57,148.96,148.52000000000001,148.81,148.99]
[null,null,null,null,"Coincident",125.98,147.88999999999999,146.68,145.08000000000001,144.65,144.94999999999999,145.13]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",128.35,151.81,150.57,148.96,148.52000000000001,148.81,148.99]
[null,null,null,null,"Coincident",126.58,147.88999999999999,146.68,146.44,146,146.30000000000001,146.47999999999999]
[null,"Beerwah BS","Substation Rating","MVA","Non-Coincident",144,144,144,144,144,144,144]
[null,null,null,null,"Coincident",144,144,144,144,144,144,144]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",59.99,59.32,59.05,58.36,58.21,58.38,58.47]
[null,null,null,null,"Coincident",55.06,54.45,54.2,53.58,53.44,53.61,53.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",61.11,60.42,60.15,59.44,59.3,59.47,59.56]
[null,null,null,null,"Coincident",55.94,55.31,55.07,54.43,54.29,54.45,54.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",55.61,54.98,54.73,54.09,53.96,54.12,54.2]
[null,null,null,null,"Coincident",51.06,50.5,50.27,49.69,49.57,49.72,49.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.64,56,55.75,55.1,54.96,55.13,55.21]
[null,null,null,null,"Coincident",51.86,51.29,51.06,50.46,50.34,50.49,50.57]
[null,"Belmont BS","Substation Rating","MVA","Non-Coincident",299,299,299,299,299,299,299]
[null,null,null,null,"Coincident",299,299,299,299,299,299,299]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",142.83000000000001,140.1,138.56,137.62,138.11000000000001,138.58000000000001,139.07]
[null,null,null,null,"Coincident",141.19999999999999,138.5,136.97999999999999,136.32,137.06,137.53,138.03]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",142.86000000000001,140.13,138.58000000000001,137.63999999999999,138.13,138.6,139.09]
[null,null,null,null,"Coincident",141.24,138.54,137.01,136.35,137.11000000000001,137.58000000000001,138.08000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",133.55000000000001,131.02000000000001,129.6,128.80000000000001,129.32,129.77000000000001,130.24]
[null,null,null,null,"Coincident",132.05000000000001,129.55000000000001,128.15,127.61,128.38999999999999,128.85,129.32]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",133.56,131.03,129.6,128.80000000000001,129.33000000000001,129.78,130.24]
[null,null,null,null,"Coincident",132.07,129.56,128.15,127.62,128.41,128.87,129.34]
[null,"Brendale BS","Substation Rating","MVA","Non-Coincident",273,273,273,273,273,273,273]
[null,null,null,null,"Coincident",273,273,273,273,273,273,273]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",196.9,194.82,193.24,190.76,190.35,191.19,191.96]
[null,null,null,null,"Coincident",196.54,194.6,193.06,190.62,190.24,191.12,191.92]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",197.56,195.46,193.85,191.34,190.92,191.78,192.55]
[null,null,null,null,"Coincident",196.65,194.73,193.18,190.73,190.35,191.23,192.04]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",184.04,182.25,180.74,178.39,178.01,178.8,179.52]
[null,null,null,null,"Coincident",183.68,181.95,180.52,178.25,177.9,178.71,179.46]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",184.54,182.72,181.2,178.82,178.44,179.23,179.96]
[null,null,null,null,"Coincident",183.74,182.03,180.59,178.31,177.95,178.77,179.52]
[null,"Browns Plains BS","Substation Rating","MVA","Non-Coincident",196,196,196,196,196,196,196]
[null,null,null,null,"Coincident",196,196,196,196,196,196,196]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Summer","Summer","Summer","Summer","Summer","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",125.15,103.15,101.52,99.75,98.99,98.75,97.77]
[null,null,null,null,"Coincident",105.3,103.15,101.52,99.75,98.99,98.75,98.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",127.07,108.04,106.33,104.47,103.68,103.43,99.27]
[null,null,null,null,"Coincident",107.01,104.85,103.21,101.42,100.66,100.42,100.04]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",118.59,96.94,95.41,93.75,93.05,92.82,93.74]
[null,null,null,null,"Coincident",98.92,96.94,95.41,93.75,93.05,92.82,92.45]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",120.41,101.54,99.93,98.19,97.45,97.21,95.18]
[null,null,null,null,"Coincident",100.58,98.58,97.04,95.36,94.66,94.43,94.07]
[null,"Burleigh Heads BS","Substation Rating","MVA","Non-Coincident",165,165,165,165,165,165,165]
[null,null,null,null,"Coincident",165,165,165,165,165,165,165]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",113.57,114.45,115.4,115.91,116.39,117.65,119.43]
[null,null,null,null,"Coincident",90.62,90.2,90.39,90.13,90.78,92.05,93.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",114.1,114.98,115.94,116.45,116.93,118.19,119.99]
[null,null,null,null,"Coincident",91.3,90.88,91.06,90.8,91.45,92.73,94.05]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",109.27,110.1,111.01,111.49,111.94,113.13,114.83]
[null,null,null,null,"Coincident",85.51,85.11,85.28,85.02,85.62,86.81,88.03]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",109.77,110.61,111.52,112,112.46,113.66,115.36]
[null,null,null,null,"Coincident",86.15,85.75,85.92,85.66,86.26,87.46,88.69]
[null,"Caboolture BS","Substation Rating","MVA","Non-Coincident",283,283,283,283,283,283,310]
[null,null,null,null,"Coincident",283,283,283,283,283,283,310]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",165.68,162.66999999999999,161.35,159.65,159.27000000000001,159.68,160.08000000000001]
[null,null,null,null,"Coincident",165.68,162.66,161.33000000000001,159.63999999999999,159.26,159.66999999999999,160.06]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",165.71,162.69999999999999,161.37,159.68,159.29,159.71,160.1]
[null,null,null,null,"Coincident",165.68,162.66,161.33000000000001,159.63999999999999,159.26,159.66999999999999,160.06]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",155.68,152.85,151.6,150.02000000000001,149.66999999999999,150.05000000000001,150.41999999999999]
[null,null,null,null,"Coincident",155.68,152.85,151.6,150.02000000000001,149.66999999999999,150.05000000000001,150.41999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",155.69999999999999,152.86000000000001,151.61000000000001,150.03,149.66999999999999,150.06,150.43]
[null,null,null,null,"Coincident",155.68,152.85,151.6,150.02000000000001,149.66999999999999,150.05000000000001,150.41999999999999]
[null,"Cleveland BS","Substation Rating","MVA","Non-Coincident",287,287,287,287,287,287,287]
[null,null,null,null,"Coincident",287,287,287,287,287,287,287]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",180.79,178.08,176.78,174.41,173.72,174.33,175]
[null,null,null,null,"Coincident",179.23,176.55,175.27,172.92,172.25,172.86,173.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",180.96,178.23,176.93,174.54,173.86,174.46,175.14]
[null,null,null,null,"Coincident",179.9,177.2,175.92,173.56,172.88,173.49,174.17]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",169.59,167.04,165.83,163.6,162.96,163.53,164.16]
[null,null,null,null,"Coincident",168.12,165.61,164.41,162.21,161.58000000000001,162.15,162.79]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",169.7,167.14,165.92,163.68,163.04,163.61000000000001,164.24]
[null,null,null,null,"Coincident",168.75,166.22,165.02,162.80000000000001,162.16999999999999,162.74,163.38]
[null,"Coomera BS","Substation Rating","MVA","Non-Coincident",190,190,190,190,190,190,190]
[null,null,null,null,"Coincident",190,190,190,190,190,190,190]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",128.07,126.62,126.7,129.29,132.99,134.94999999999999,137.03]
[null,null,null,null,"Coincident",121.86,120.47,120.56,123.25,126.98,128.84,130.84]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",130.97999999999999,129.5,129.58000000000001,132.22999999999999,136.02000000000001,138.01,140.13999999999999]
[null,null,null,null,"Coincident",123.91,122.46,122.54,125.8,130.18,132.05000000000001,134.06]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",119.07,117.71,117.78,120.39,124.03,125.85,127.79]
[null,null,null,null,"Coincident",113.28,111.98,112.06,114.77,118.43,120.17,122.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",121.78,120.39,120.46,123.13,126.85,128.71,130.69]
[null,null,null,null,"Coincident",115.16,113.81,113.88,117.16,121.48,123.23,125.09]
[null,"Coorparoo BS","Substation Rating","MVA","Non-Coincident",191,191,191,191,191,191,191]
[null,null,null,null,"Coincident",191,191,191,191,191,191,191]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",85.06,83.73,83.3,82.46,82.46,83.12,83.93]
[null,null,null,null,"Coincident",84.26,82.93,82.5,81.66,81.67,82.32,83.12]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",86.34,84.99,84.55,83.7,83.7,84.37,85.2]
[null,null,null,null,"Coincident",84.28,82.95,82.52,81.69,81.69,82.35,83.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",80.72,79.459999999999994,79.05,78.25,78.260000000000005,78.89,79.66]
[null,null,null,null,"Coincident",79.95,78.69,78.290000000000006,77.489999999999995,77.5,78.12,78.88]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",81.94,80.66,80.239999999999995,79.430000000000007,79.430000000000007,80.08,80.86]
[null,null,null,null,"Coincident",79.97,78.72,78.31,77.52,77.52,78.14,78.900000000000006]
[null,"Doboy BS","Substation Rating","MVA","Non-Coincident",263,263,263,263,263,263,263]
[null,null,null,null,"Coincident",263,263,263,263,263,263,263]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",141.46,144.49,167.41,189.61,188.98,189.2,189.6]
[null,null,null,null,"Coincident",130.43,132.58000000000001,155.53,177.79,177.21,177.49,177.94]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",141.51,144.55000000000001,167.63,190.06,189.43,189.65,190.05]
[null,null,null,null,"Coincident",131.44,133.66999999999999,157.19999999999999,177.85,177.27,177.55,178]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",135.47,138.6,161.57,183.86,183.26,183.46,183.82]
[null,null,null,null,"Coincident",124.52,126.77,149.77000000000001,172.11,171.56,171.82,172.24]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",135.5,138.63999999999999,161.75,184.25,183.64,183.85,184.21]
[null,null,null,null,"Coincident",125.5,127.83,151.41999999999999,172.16,171.61,171.86,172.28]
[null,"Gatton BS","Substation Rating","MVA","Non-Coincident",143,143,143,143,143,143,143]
[null,null,null,null,"Coincident",143,143,143,143,143,143,143]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.15,33.6,33.32,32.85,32.700000000000003,32.69,32.619999999999997]
[null,null,null,null,"Coincident",32.18,31.67,31.41,30.97,30.83,30.83,30.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.32,34.75,34.46,33.979999999999997,33.82,33.81,33.74]
[null,null,null,null,"Coincident",32.979999999999997,32.46,32.19,31.75,31.61,31.61,31.55]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.96,31.44,31.18,30.74,30.6,30.59,30.52]
[null,null,null,null,"Coincident",30.06,29.58,29.33,28.93,28.8,28.79,28.73]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.06,32.520000000000003,32.25,31.8,31.65,31.64,31.57]
[null,null,null,null,"Coincident",30.8,30.31,30.07,29.65,29.52,29.52,29.46]
[null,"Goodna BS","Substation Rating","MVA","Non-Coincident",218,218,218,218,218,218,218]
[null,null,null,null,"Coincident",218,218,218,218,218,218,218]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",145.28,156.13,156.36000000000001,156.44,157.91,160.47,163.38]
[null,null,null,null,"Coincident",145.19999999999999,155.77000000000001,155.99,156.08000000000001,157.55000000000001,160.13,163.06]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",146.09,157,157.22999999999999,157.31,158.78,161.35,164.29]
[null,null,null,null,"Coincident",145.22999999999999,155.77000000000001,155.99,156.16,157.62,160.19,163.12]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",134.58000000000001,145.49,145.68,145.74,147.08000000000001,149.44,152.12]
[null,null,null,null,"Coincident",134.58000000000001,145.19999999999999,145.38999999999999,145.46,146.80000000000001,149.16999999999999,151.87]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",135.33000000000001,146.30000000000001,146.49,146.55000000000001,147.88999999999999,150.26,152.96]
[null,null,null,null,"Coincident",134.6,145.28,145.46,145.52000000000001,146.86000000000001,149.22999999999999,151.93]
[null,"Griffin BS","Substation Rating","MVA","Non-Coincident",191,191,191,191,191,191,191]
[null,null,null,null,"Coincident",191,191,191,191,191,191,191]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",78.010000000000005,76.27,76.17,76.459999999999994,76.400000000000006,76.39,76.709999999999994]
[null,null,null,null,"Coincident",77.83,76.069999999999993,75.98,76.27,76.209999999999994,76.19,76.52]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",78.88,77.12,77.02,77.31,77.25,77.239999999999995,77.56]
[null,null,null,null,"Coincident",77.83,76.08,75.98,76.27,76.209999999999994,76.2,76.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",72.83,71.209999999999994,71.17,71.56,71.56,71.55,71.849999999999994]
[null,null,null,null,"Coincident",72.63,70.98,70.95,71.34,71.34,71.33,71.63]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",73.64,72,71.959999999999994,72.349999999999994,72.349999999999994,72.34,72.64]
[null,null,null,null,"Coincident",72.63,70.989999999999995,70.95,71.34,71.34,71.33,71.63]
[null,"Gympie BS","Substation Rating","MVA","Non-Coincident",145,145,145,145,145,145,145]
[null,null,null,null,"Coincident",145,145,145,145,145,145,230]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.7,53.78,53.73,53.49,53.21,53.24,53.43]
[null,null,null,null,"Coincident",40.68,40.880000000000003,40.549999999999997,40.020000000000003,39.83,39.82,39.74]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.03,54.12,54.07,53.83,53.55,53.58,53.77]
[null,null,null,null,"Coincident",40.869999999999997,41.09,40.76,40.229999999999997,40.03,40.020000000000003,39.950000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.37,51.39,51.35,51.15,50.9,50.92,51.09]
[null,null,null,null,"Coincident",36.78,37.04,36.74,36.26,36.08,36.07,36.01]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",50.69,51.72,51.67,51.47,51.22,51.25,51.41]
[null,null,null,null,"Coincident",36.96,37.24,36.94,36.46,36.28,36.270000000000003,36.21]
[null,"Hays Inlet BS","Substation Rating","MVA","Non-Coincident",268,268,268,268,268,268,268]
[null,null,null,null,"Coincident",268,268,268,268,268,268,268]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",175.09,173.53,173.41,176.08,180.41,182.34,184.08]
[null,null,null,null,"Coincident",171.7,170.16,170.05,172.64,176.86,178.77,180.49]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",175.13,173.57,173.45,176.13,180.47,182.41,184.15]
[null,null,null,null,"Coincident",172.63,171.07,170.96,173.75,176.87,178.78,180.5]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",164.91,163.44999999999999,163.34,166.05,170.33,172.15,173.79]
[null,null,null,null,"Coincident",161.68,160.22999999999999,160.13,162.76,166.94,168.73,170.35]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",164.93,163.46,163.36000000000001,166.08,170.36,172.19,173.83]
[null,null,null,null,"Coincident",162.55000000000001,161.09,160.97999999999999,163.82,166.94,168.74,170.35]
[null,"Ibis BS","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2999999999999998,2.29,2.2999999999999998,2.29,2.2799999999999998,2.29,2.2999999999999998]
[null,null,null,null,"Coincident",1.1299999999999999,1.1200000000000001,1.1100000000000001,1.1000000000000001,1.1000000000000001,1.1100000000000001,1.1100000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.42,2.42,2.42,2.42,2.41,2.41,2.42]
[null,null,null,null,"Coincident",1.1499999999999999,1.1399999999999999,1.1299999999999999,1.1200000000000001,1.1200000000000001,1.1200000000000001,1.1299999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.19,2.19,2.2000000000000002,2.19,2.1800000000000002,2.19,2.2000000000000002]
[null,null,null,null,"Coincident",1.06,1.05,1.04,1.03,1.03,1.04,1.04]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.31,2.31,2.3199999999999998,2.31,2.2999999999999998,2.31,2.3199999999999998]
[null,null,null,null,"Coincident",1.0900000000000001,1.07,1.07,1.05,1.05,1.06,1.06]
[null,"Jimboomba BS","Substation Rating","MVA","Non-Coincident",88,88,88,88,197,197,197]
[null,null,null,null,"Coincident",88,88,88,88,197,197,197]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",102.18,101.93,104.48,106.22,109.13,110.56,111.76]
[null,null,null,null,"Coincident",94.49,94.27,96.61,98.2,100.86,102.19,103.31]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",104.45,104.2,106.8,108.58,111.55,113.02,114.25]
[null,null,null,null,"Coincident",160.31,159.36000000000001,158.28,158.59,159.81,162.76,165.27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",91.62,91.4,93.91,95.64,98.46,99.74,100.82]
[null,null,null,null,"Coincident",84.74,84.55,86.85,88.43,91.01,92.2,93.2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",93.65,93.43,96,97.77,100.65,101.96,103.06]
[null,null,null,null,"Coincident",142.66,141.83000000000001,140.77000000000001,140.96,141.96,144.58000000000001,146.81]
[null,"Lockrose BS","Substation Rating","MVA","Non-Coincident",144,144,144,144,144,144,144]
[null,null,null,null,"Coincident",144,144,144,144,144,144,144]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.010000000000005,68.55,70.86,70.12,69.989999999999995,70.22,70.31]
[null,null,null,null,"Coincident",59.39,59.02,61.06,60.42,60.3,60.49,60.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",69.010000000000005,68.56,70.87,70.13,70,70.23,70.319999999999993]
[null,null,null,null,"Coincident",60.56,60.21,62.14,61.49,61.37,61.57,61.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.84,63.45,65.78,65.099999999999994,64.98,65.19,65.28]
[null,null,null,null,"Coincident",55,54.68,56.74,56.15,56.04,56.22,56.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64.94,64.540000000000006,65.78,65.099999999999994,64.98,65.19,65.28]
[null,null,null,null,"Coincident",56.07,55.78,57.74,57.13,57.02,57.21,57.28]
[null,"Loganlea BS","Substation Rating","MVA","Non-Coincident",256,256,256,256,256,256,256]
[null,null,null,null,"Coincident",256,256,256,256,256,256,256]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",104.26,102.11,101.42,100.34,100.23,100.62,100.98]
[null,null,null,null,"Coincident",103.23,101.13,100.44,99.37,99.26,99.65,100]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",105.39,103.22,102.52,101.43,101.31,101.71,102.07]
[null,null,null,null,"Coincident",103.39,101.28,100.59,99.52,99.41,99.8,100.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",98.43,96.37,95.72,94.71,94.61,94.98,95.33]
[null,null,null,null,"Coincident",97.47,95.45,94.81,93.81,93.71,94.08,94.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",99.49,97.41,96.76,95.74,95.63,96.01,96.36]
[null,null,null,null,"Coincident",97.62,95.6,94.95,93.95,93.85,94.22,94.56]
[null,"Lytton BS","Substation Rating","MVA","Non-Coincident",239,239,239,239,239,239,239]
[null,null,null,null,"Coincident",239,239,239,239,239,239,239]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",116.45,129.21,135.49,137.68,138.25,138.34,138.94]
[null,null,null,null,"Coincident",103.78,114.33,119.72,119.66,119.19,119.31,119.29]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",116.94,129.75,136.06,138.26,138.83000000000001,138.91999999999999,139.53]
[null,null,null,null,"Coincident",103.88,114.52,119.74,119.69,119.21,119.33,119.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",111.51,124.26,130.53,132.72999999999999,133.33000000000001,133.41,133.97]
[null,null,null,null,"Coincident",100.65,111.24,116.64,116.62,116.17,116.27,116.24]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",111.98,124.78,131.08000000000001,133.29,133.88999999999999,133.97,134.54]
[null,null,null,null,"Coincident",100.74,111.42,116.66,116.64,116.18,116.29,116.26]
[null,"Meeandah BS","Substation Rating","MVA","Non-Coincident",168,168,168,168,168,168,168]
[null,null,null,null,"Coincident",168,168,168,168,168,168,168]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.45,50.42,50.53,50.36,50.62,51.06,51.85]
[null,null,null,null,"Coincident",33.380000000000003,37.08,37.130000000000003,36.97,37.14,37.44,38.020000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",49.28,54.68,54.79,54.61,54.89,55.36,56.22]
[null,null,null,null,"Coincident",33.700000000000003,37.67,37.71,37.54,37.71,38.01,38.61]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.21,49.19,49.29,49.14,49.39,49.81,50.59]
[null,null,null,null,"Coincident",32.450000000000003,36.159999999999997,36.21,36.06,36.22,36.51,37.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.94,53.34,53.45,53.28,53.56,54.02,54.86]
[null,null,null,null,"Coincident",32.74,36.72,36.76,36.6,36.76,37.049999999999997,37.64]
[null,"Molendinar BS","Substation Rating","MVA","Non-Coincident",316,316,316,316,316,316,316]
[null,null,null,null,"Coincident",316,316,316,316,316,316,316]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",146.4,147.78,147.63,145.84,145.55000000000001,146.26,146.97]
[null,null,null,null,"Coincident",146.34,147.69999999999999,147.56,145.79,145.5,146.22,146.93]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",147.9,149.29,149.13999999999999,147.33000000000001,147.04,147.76,148.47999999999999]
[null,null,null,null,"Coincident",146.71,148.13,148,146.22,145.93,146.65,147.36000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",135.88999999999999,137.41999999999999,137.34,135.68,135.4,136.07,136.72]
[null,null,null,null,"Coincident",135.82,137.34,137.27000000000001,135.62,135.35,136.01,136.66999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",137.28,138.83000000000001,138.75,137.07,136.79,137.46,138.12]
[null,null,null,null,"Coincident",136.16999999999999,137.74,137.68,136.02000000000001,135.75,136.41999999999999,137.08000000000001]
[null,"Mudgeeraba BS","Substation Rating","MVA","Non-Coincident",98,98,98,98,98,98,98]
[null,null,null,null,"Coincident",98,98,98,98,98,98,98]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.91,24.64,24.55,24.3,24.27,24.49,24.73]
[null,null,null,null,"Coincident",24.67,24.39,24.3,24.04,24.01,24.23,24.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.35,25.07,24.98,24.72,24.69,24.91,25.16]
[null,null,null,null,"Coincident",24.98,24.7,24.62,24.35,24.33,24.55,24.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.23,22.98,22.9,22.66,22.63,22.83,23.06]
[null,null,null,null,"Coincident",22.96,22.71,22.62,22.38,22.36,22.56,22.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.64,23.38,23.29,23.05,23.03,23.23,23.47]
[null,null,null,null,"Coincident",23.27,23.01,22.92,22.68,22.66,22.86,23.1]
[null,"Myrtletown BS","Substation Rating","MVA","Non-Coincident",240,240,240,240,240,240,240]
[null,null,null,null,"Coincident",240,240,240,240,240,240,240]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.78,43.68,43.71,60.16,76.739999999999995,76.89,77]
[null,null,null,null,"Coincident",34.31,34.21,34.24,52.58,71.05,71.180000000000007,71.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.09,43.99,44.02,60.58,77.28,77.430000000000007,77.540000000000006]
[null,null,null,null,"Coincident",34.409999999999997,34.32,34.340000000000003,53.23,72.41,72.55,72.66]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.7,42.61,42.63,59.09,75.66,75.81,75.91]
[null,null,null,null,"Coincident",33.36,33.270000000000003,33.299999999999997,51.65,70.099999999999994,70.239999999999995,70.33]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43,42.91,42.93,59.5,76.19,76.34,76.44]
[null,null,null,null,"Coincident",33.450000000000003,33.36,33.380000000000003,52.26,71.430000000000007,71.569999999999993,71.67]
[null,"Nambour BS","Substation Rating","MVA","Non-Coincident",144,144,144,144,144,144,144]
[null,null,null,null,"Coincident",144,144,144,144,144,144,144]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Winter","Summer","Summer","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",86.47,86.07,85.75,84.76,84.85,85.36,86.06]
[null,null,null,null,"Coincident",80.73,80.33,80.03,79.209999999999994,79.19,79.67,80.150000000000006]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",87.01,86.61,86.29,84.86,85.38,85.89,86.17]
[null,null,null,null,"Coincident",80.83,80.44,80.14,79.31,79.290000000000006,79.77,80.25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",80.11,79.77,79.47,78.67,78.63,79.09,79.87]
[null,null,null,null,"Coincident",74.819999999999993,74.48,74.19,73.42,73.41,73.84,74.290000000000006]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",80.61,80.27,79.97,78.73,79.12,79.59,79.94]
[null,null,null,null,"Coincident",74.92,74.59,74.3,73.53,73.510000000000005,73.95,74.400000000000006]
[null,"Nudgee BS","Substation Rating","MVA","Non-Coincident",250,250,250,250,250,250,250]
[null,null,null,null,"Coincident",250,250,250,250,250,250,250]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",180.3,183.25,181.88,181.99,181.68,182.29,183.34]
[null,null,null,null,"Coincident",154.74,157.9,156.74,157.13999999999999,156.94,157.58000000000001,158.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",180.3,183.26,181.88,182,181.69,182.29,183.34]
[null,null,null,null,"Coincident",154.82,158.01,156.84,157.25,157.05000000000001,157.68,158.69999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",170.78,173.79,172.5,172.72,172.42,172.99,173.98]
[null,null,null,null,"Coincident",146.07,149.27000000000001,148.16999999999999,148.66999999999999,148.47999999999999,149.08000000000001,150.04]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",170.94,173.96,172.66,172.88,172.58,173.16,174.15]
[null,null,null,null,"Coincident",146.15,149.37,148.27000000000001,148.77000000000001,148.58000000000001,149.18,150.13999999999999]
[null,"Postmans Ridge BS","Substation Rating","MVA","Non-Coincident",127,127,127,127,139,139,139]
[null,null,null,null,"Coincident",127,127,127,127,139,139,139]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.119999999999997,32.950000000000003,32.86,32.72,32.68,32.71,32.72]
[null,null,null,null,"Coincident",18.91,18.77,18.7,18.579999999999998,18.54,18.57,18.579999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.4,33.229999999999997,33.15,33,32.96,32.99,33]
[null,null,null,null,"Coincident",18.91,18.78,18.7,18.579999999999998,18.55,18.57,18.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.59,30.44,30.36,30.23,30.19,30.22,30.23]
[null,null,null,null,"Coincident",17.399999999999999,17.27,17.21,17.100000000000001,17.07,17.09,17.100000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.85,30.7,30.62,30.49,30.45,30.48,30.49]
[null,null,null,null,"Coincident",17.41,17.28,17.21,17.11,17.07,17.09,17.11]
[null,"Raceview BS","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,264,264]
[null,null,null,null,"Coincident",132,132,132,132,132,264,264]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",113.3,113.75,115.1,115.02,115.98,117.48,118.77]
[null,null,null,null,"Coincident",113.3,113.75,115.1,115.02,115.98,117.48,118.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",114.65,115.1,116.47,116.39,117.36,118.89,120.18]
[null,null,null,null,"Coincident",113.3,113.76,115.11,115.04,116,117.48,118.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",105.48,105.93,107.23,107.16,108.04,109.43,110.62]
[null,null,null,null,"Coincident",105.48,105.93,107.23,107.16,108.04,109.43,110.62]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",106.74,107.2,108.51,108.43,109.33,110.74,111.94]
[null,null,null,null,"Coincident",105.52,105.98,107.28,107.2,108.09,109.48,110.67]
[null,"Richlands BS","Substation Rating","MVA","Non-Coincident",259,259,259,259,259,259,259]
[null,null,null,null,"Coincident",259,259,259,259,259,259,259]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",136.99,148.43,147.91999999999999,145.88,145.19999999999999,145.13,145.04]
[null,null,null,null,"Coincident",127.83,138.75,138.27000000000001,136.41,135.82,135.82,135.81]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",136.99,148.46,147.94999999999999,145.9,145.22,145.15,145.06]
[null,null,null,null,"Coincident",129.13999999999999,140.1,139.66,137.77000000000001,137.16999999999999,137.16,137.13]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",128.03,139.63,139.22,137.32,136.68,136.61000000000001,136.52000000000001]
[null,null,null,null,"Coincident",119.51,130.57,130.19,128.44999999999999,127.9,127.9,127.88]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",128.08000000000001,139.63999999999999,139.22999999999999,137.32,136.68,136.61000000000001,136.52000000000001]
[null,null,null,null,"Coincident",120.77,131.88,131.53,129.77000000000001,129.21,129.19,129.16]
[null,"Runcorn BS","Substation Rating","MVA","Non-Coincident",187,187,187,187,187,187,187]
[null,null,null,null,"Coincident",187,187,187,187,187,187,187]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",71.459999999999994,70.31,69.86,70.06,71.91,73.27,73.7]
[null,null,null,null,"Coincident",70.78,69.650000000000006,69.209999999999994,69.5,71.400000000000006,72.72,73.150000000000006]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",72.040000000000006,70.88,70.42,70.63,72.5,73.86,74.3]
[null,null,null,null,"Coincident",71.16,70.02,69.569999999999993,69.89,71.86,73.22,73.66]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",67.37,66.290000000000006,65.86,66.11,67.97,69.3,69.7]
[null,null,null,null,"Coincident",66.73,65.66,65.25,65.58,67.48,68.78,69.180000000000007]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.92,66.83,66.400000000000006,66.650000000000006,68.52,69.86,70.260000000000005]
[null,null,null,null,"Coincident",67.06,65.98,66.39,66.78,67.89,69.23,69.64]
[null,"Sandgate BS","Substation Rating","MVA","Non-Coincident",191,191,191,191,191,191,191]
[null,null,null,null,"Coincident",191,191,191,191,191,191,191]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",93.27,91.73,90.87,89.55,89.23,89.49,89.85]
[null,null,null,null,"Coincident",93.18,91.63,90.77,89.44,89.1,89.34,89.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",93.57,92.03,91.16,89.84,89.52,89.78,90.14]
[null,null,null,null,"Coincident",93.19,91.64,90.77,89.44,89.11,89.35,89.7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",85.91,84.49,83.7,82.49,82.19,82.43,82.76]
[null,null,null,null,"Coincident",85.86,84.44,83.64,82.41,82.1,82.32,82.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",86.19,84.77,83.97,82.75,82.46,82.69,83.02]
[null,null,null,null,"Coincident",85.87,84.44,83.64,82.42,82.11,82.33,82.65]
[null,"Stafford BS","Substation Rating","MVA","Non-Coincident",262,262,262,262,262,262,262]
[null,null,null,null,"Coincident",262,262,262,262,262,262,262]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",175.23,172.93,171.65,169.59,168.94,169.34,169.8]
[null,null,null,null,"Coincident",156.66,154.33000000000001,153.04,150.94999999999999,150.29,150.69999999999999,151.15]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",175.36,173.04,171.75,169.68,169.03,169.44,169.89]
[null,null,null,null,"Coincident",157.1,154.76,153.46,151.37,150.71,151.11000000000001,151.57]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",164.56,162.41,161.21,159.29,158.68,159.06,159.47999999999999]
[null,null,null,null,"Coincident",146.32,144.13999999999999,142.93,140.99,140.37,140.75,141.16]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",164.63,162.47,161.27000000000001,159.34,158.72999999999999,159.11000000000001,159.53]
[null,null,null,null,"Coincident",146.72,144.54,143.33000000000001,141.38,140.76,141.13,141.55000000000001]
[null,"Stradbroke Is BS","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",72,72,72,72,72,72,72]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8,4.74,4.71,4.6500000000000004,4.63,4.6399999999999997,4.6500000000000004]
[null,null,null,null,"Coincident",3.52,3.47,3.45,3.41,3.4,3.4,3.41]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9400000000000004,4.87,4.84,4.78,4.7699999999999996,4.78,4.78]
[null,null,null,null,"Coincident",3.57,3.52,3.5,3.45,3.44,3.45,3.45]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.67,4.6100000000000003,4.57,4.5199999999999996,4.5,4.51,4.5199999999999996]
[null,null,null,null,"Coincident",3.42,3.38,3.35,3.31,3.3,3.31,3.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.8,4.74,4.7,4.6500000000000004,4.63,4.6399999999999997,4.6500000000000004]
[null,null,null,null,"Coincident",3.47,3.42,3.4,3.35,3.34,3.35,3.35]
[null,"Sunrise Hills BS","Substation Rating","MVA","Non-Coincident",143,143,143,143,143,143,143]
[null,null,null,null,"Coincident",143,143,143,143,143,143,143]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",88.92,88,87.68,86.61,86.45,86.92,87.66]
[null,null,null,null,"Coincident",75.31,74.52,74.239999999999995,73.34,73.2,73.59,74.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",90.83,89.89,89.56,88.47,88.31,88.79,89.54]
[null,null,null,null,"Coincident",76.040000000000006,75.239999999999995,74.95,74.03,73.89,74.28,74.900000000000006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",81.38,80.540000000000006,80.239999999999995,79.260000000000005,79.12,79.55,80.22]
[null,null,null,null,"Coincident",68.97,68.25,67.989999999999995,67.16,67.03,67.39,67.959999999999994]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",83.13,82.26,81.96,80.959999999999994,80.819999999999993,81.25,81.94]
[null,null,null,null,"Coincident",69.680000000000007,68.94,68.680000000000007,67.84,67.709999999999994,68.06,68.63]
[null,"Tennyson BS","Substation Rating","MVA","Non-Coincident",258,258,258,258,258,258,258]
[null,null,null,null,"Coincident",258,258,258,258,258,258,258]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",197.77,206.65,205.4,203.16,202.92,204.29,206.14]
[null,null,null,null,"Coincident",193.87,203.58,202.34,200.13,199.9,201.26,203.13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",199.13,206.65,205.4,204.56,204.31,204.29,206.14]
[null,null,null,null,"Coincident",193.94,203.73,202.49,200.28,200.32,201.68,203.55]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",183.73,192.79,191.63,189.55,189.33,190.59,192.29]
[null,null,null,null,"Coincident",179.94,189.83,188.68,186.64,186.42,187.68,189.39]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",185,194.12,192.95,190.86,190.63,191.9,193.61]
[null,null,null,null,"Coincident",180.01,190.24,189.09,187.05,186.83,188.08,189.8]
[null,"Victoria Park BS","Substation Rating","MVA","Non-Coincident",251,251,251,251,251,251,251]
[null,null,null,null,"Coincident",251,251,251,251,251,251,251]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",65.709999999999994,64.98,64.599999999999994,63.93,63.75,63.85,64.09]
[null,null,null,null,"Coincident",46.78,46.08,45.72,45.08,44.92,45.01,45.24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",66.5,65.760000000000005,65.38,64.7,64.52,64.62,64.86]
[null,null,null,null,"Coincident",47.1,46.4,46.04,45.4,45.23,45.32,45.56]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.2,62.5,62.15,61.51,61.34,61.43,61.66]
[null,null,null,null,"Coincident",44.55,43.89,43.55,42.94,42.79,42.87,43.09]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",63.96,63.26,62.89,62.25,62.08,62.17,62.4]
[null,null,null,null,"Coincident",44.86,44.19,43.85,43.24,43.08,43.17,43.39]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Acacia Ridge","Substation Rating","MVA","Non-Coincident",42,42,42,42,42,42,42]
[null,null,null,null,"Coincident",42,42,42,42,42,42,42]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.010000000000002,17.77,17.649999999999999,17.420000000000002,17.37,17.420000000000002,17.48]
[null,null,null,null,"Coincident",17.75,17.52,17.399999999999999,17.170000000000002,17.12,17.170000000000002,17.23]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.02,17.78,17.66,17.43,17.38,17.43,17.489999999999998]
[null,null,null,null,"Coincident",18.309999999999999,18.07,17.95,17.71,17.66,17.71,17.78]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.149999999999999,16.93,16.82,16.59,16.55,16.600000000000001,16.649999999999999]
[null,null,null,null,"Coincident",16.91,16.690000000000001,16.579999999999998,16.36,16.309999999999999,16.36,16.420000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.16,16.93,16.82,16.600000000000001,16.55,16.600000000000001,16.66]
[null,null,null,null,"Coincident",17.440000000000001,17.21,17.100000000000001,16.87,16.829999999999998,16.87,16.93]
[null,"Albany Creek","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.68,28.09,27.84,27.43,27.29,27.36,27.44]
[null,null,null,null,"Coincident",28.15,27.56,27.32,26.91,26.78,26.85,26.92]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.74,28.15,27.9,27.48,27.35,27.42,27.5]
[null,null,null,null,"Coincident",28.18,27.59,27.35,26.95,26.81,26.88,26.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.05,26.48,26.25,25.86,25.73,25.8,25.87]
[null,null,null,null,"Coincident",26.54,25.99,25.76,25.38,25.25,25.31,25.39]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.1,26.54,26.3,25.92,25.79,25.85,25.93]
[null,null,null,null,"Coincident",26.57,26.02,25.79,25.41,25.28,25.35,25.42]
[null,"Alexandra Headland","Substation Rating","MVA","Non-Coincident",144,144,144,144,144,144,144]
[null,null,null,null,"Coincident",144,144,144,144,144,144,144]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",73.150000000000006,71.58,70.52,70.040000000000006,69.38,70.349999999999994,70.94]
[null,null,null,null,"Coincident",64.84,63.45,62.52,62.2,61.61,62.57,63.1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.61,72.010000000000005,70.930000000000007,70.44,69.760000000000005,70.75,71.36]
[null,null,null,null,"Coincident",64.849999999999994,63.46,62.52,62.2,61.62,62.58,63.11]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",70.34,68.84,67.819999999999993,67.39,66.760000000000005,67.72,68.290000000000006]
[null,null,null,null,"Coincident",62.35,61.02,60.12,59.85,59.28,60.24,60.75]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",70.739999999999995,69.2,68.16,67.73,67.08,68.069999999999993,68.650000000000006]
[null,null,null,null,"Coincident",62.36,61.02,60.12,59.85,59.29,60.25,60.76]
[null,"Algester","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.16,21.78,21.63,21.56,21.77,22.11,22.46]
[null,null,null,null,"Coincident",21.14,20.78,20.63,20.56,20.76,21.09,21.42]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.53,22.14,21.99,21.91,22.12,22.47,22.83]
[null,null,null,null,"Coincident",21.18,20.82,20.67,20.6,20.8,21.13,21.47]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.16,19.82,19.68,19.61,19.8,20.11,20.43]
[null,null,null,null,"Coincident",19.23,18.899999999999999,18.77,18.7,18.88,19.18,19.489999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.49,20.14,20,19.93,20.13,20.440000000000001,20.77]
[null,null,null,null,"Coincident",19.27,18.940000000000001,18.809999999999999,18.739999999999998,18.920000000000002,19.22,19.53]
[null,"Amamoor","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.83,5.8,5.78,5.74,5.7,5.7,5.72]
[null,null,null,null,"Coincident",4.3899999999999997,4.32,4.29,4.22,4.2,4.1900000000000004,4.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.86,5.83,5.81,5.78,5.73,5.73,5.75]
[null,null,null,null,"Coincident",4.4400000000000004,4.37,4.33,4.2699999999999996,4.24,4.24,4.22]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.43,5.41,5.39,5.36,5.31,5.31,5.33]
[null,null,null,null,"Coincident",4.1100000000000003,4.04,4.01,3.95,3.93,3.92,3.91]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.46,5.44,5.42,5.39,5.34,5.34,5.36]
[null,null,null,null,"Coincident",4.1500000000000004,4.09,4.05,3.99,3.97,3.96,3.95]
[null,"Amberley","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,52,52]
[null,null,null,null,"Coincident",26,26,26,26,26,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.08,2.06,2.0499999999999998,2.0299999999999998,2.02,2.04,2.04]
[null,null,null,null,"Coincident",2.0099999999999998,1.99,1.97,1.95,1.95,1.96,1.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.12,2.1,2.09,2.0699999999999998,2.06,2.08,2.08]
[null,null,null,null,"Coincident",2.0099999999999998,1.99,1.97,1.95,1.95,1.96,1.97]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.88,1.85,1.84,1.83,1.82,1.83,1.84]
[null,null,null,null,"Coincident",1.81,1.79,1.78,1.76,1.76,1.77,1.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.91,1.89,1.88,1.86,1.86,1.87,1.88]
[null,null,null,null,"Coincident",1.81,1.79,1.78,1.76,1.76,1.77,1.78]
[null,"Ann St","Substation Rating","MVA","Non-Coincident",188,188,188,188,188,188,188]
[null,null,null,null,"Coincident",188,188,188,188,188,188,188]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.4,43.68,43.33,51.37,51.12,51.07,50.89]
[null,null,null,null,"Coincident",34.04,36.090000000000003,35.81,42.95,42.75,42.71,42.56]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.4,43.69,43.34,51.41,51.17,51.11,50.93]
[null,null,null,null,"Coincident",34.08,36.19,35.9,42.97,42.77,42.72,42.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.03,42.33,42,50.05,49.82,49.76,49.59]
[null,null,null,null,"Coincident",32.909999999999997,34.99,34.71,41.87,41.68,41.63,41.49]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.21,42.34,42,50.09,49.85,49.79,49.62]
[null,null,null,null,"Coincident",32.950000000000003,35.07,34.79,41.88,41.69,41.64,41.5]
[null,"Annerley","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.66,17.510000000000002,17.510000000000002,17.38,17.43,17.62,17.850000000000001]
[null,null,null,null,"Coincident",17.2,17.05,17.059999999999999,16.93,16.98,17.16,17.39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.73,17.579999999999998,17.59,17.45,17.5,17.690000000000001,17.920000000000002]
[null,null,null,null,"Coincident",17.21,17.059999999999999,17.07,16.940000000000001,16.989999999999998,17.170000000000002,17.399999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.84,16.690000000000001,16.7,16.57,16.62,16.8,17.02]
[null,null,null,null,"Coincident",16.399999999999999,16.260000000000002,16.27,16.14,16.190000000000001,16.37,16.579999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.91,16.760000000000002,16.77,16.64,16.690000000000001,16.87,17.09]
[null,null,null,null,"Coincident",16.41,16.27,16.28,16.149999999999999,16.2,16.37,16.59]
[null,"Arana Hills","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.25,34.75,34.5,34.090000000000003,34.020000000000003,34.19,34.35]
[null,null,null,null,"Coincident",34.53,34.04,33.799999999999997,33.4,33.32,33.49,33.65]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.36,34.86,34.61,34.200000000000003,34.130000000000003,34.299999999999997,34.46]
[null,null,null,null,"Coincident",34.6,34.11,33.869999999999997,33.46,33.39,33.56,33.72]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.369999999999997,32.9,32.659999999999997,32.270000000000003,32.200000000000003,32.36,32.520000000000003]
[null,null,null,null,"Coincident",32.69,32.22,31.99,31.61,31.54,31.7,31.85]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.47,33,32.76,32.369999999999997,32.31,32.46,32.619999999999997]
[null,null,null,null,"Coincident",32.75,32.29,32.06,31.68,31.61,31.76,31.92]
[null,"Archerfield","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.68,20.09,19.62,19.04,18.670000000000002,18.41,18.27]
[null,null,null,null,"Coincident",8.92,8.67,8.4700000000000006,8.2200000000000006,8.06,7.95,7.88]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.68,20.09,20.34,19.739999999999998,19.37,19.100000000000001,18.95]
[null,null,null,null,"Coincident",9.1199999999999992,8.86,8.65,8.4,8.24,8.1199999999999992,8.06]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.97,19.399999999999999,18.940000000000001,18.38,18.03,17.78,17.64]
[null,null,null,null,"Coincident",8.6199999999999992,8.3699999999999992,8.18,7.93,7.78,7.67,7.61]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.97,20.12,19.649999999999999,19.07,18.7,18.440000000000001,18.3]
[null,null,null,null,"Coincident",8.81,8.56,8.36,8.11,7.96,7.84,7.78]
[null,"Arundel","Substation Rating","MVA","Non-Coincident",53,53,53,53,53,53,53]
[null,null,null,null,"Coincident",53,53,53,53,53,53,53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.99,22.23,21.96,21.57,21.54,21.74,21.94]
[null,null,null,null,"Coincident",21.25,20.56,20.309999999999999,19.95,19.920000000000002,20.100000000000001,20.29]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.19,22.44,22.16,21.77,21.73,21.94,22.14]
[null,null,null,null,"Coincident",21.32,20.62,20.37,20.010000000000002,19.98,20.170000000000002,20.350000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.74,21.03,20.77,20.399999999999999,20.37,20.56,20.75]
[null,null,null,null,"Coincident",20.100000000000001,19.440000000000001,19.21,18.86,18.829999999999998,19.010000000000002,19.190000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.93,21.22,20.96,20.59,20.55,20.75,20.94]
[null,null,null,null,"Coincident",20.16,19.5,19.27,18.920000000000002,18.89,19.07,19.25]
[null,"Ashgrove","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.1,25.67,25.44,25.09,25.12,25.44,25.88]
[null,null,null,null,"Coincident",25.82,25.39,25.17,24.82,24.85,25.17,25.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.14,25.71,25.48,25.13,25.16,25.48,25.92]
[null,null,null,null,"Coincident",25.86,25.43,25.2,24.86,24.89,25.2,25.64]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.48,24.08,23.86,23.54,23.57,23.86,24.28]
[null,null,null,null,"Coincident",24.22,23.82,23.61,23.28,23.31,23.61,24.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.52,24.12,23.9,23.58,23.6,23.9,24.32]
[null,null,null,null,"Coincident",24.25,23.85,23.64,23.32,23.34,23.64,24.05]
[null,"Astor Terrace","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.47,25.18,25.03,24.72,24.65,24.69,24.7]
[null,null,null,null,"Coincident",22.64,22.38,22.25,21.97,21.91,21.95,21.96]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.48,25.18,25.04,24.72,24.65,24.69,24.7]
[null,null,null,null,"Coincident",22.99,22.72,22.59,22.31,22.25,22.28,22.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.39,24.11,23.97,23.67,23.6,23.64,23.65]
[null,null,null,null,"Coincident",21.68,21.43,21.31,21.03,20.98,21.01,21.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.39,24.11,24.57,24.26,24.19,24.23,24.24]
[null,null,null,null,"Coincident",22.01,21.76,21.64,21.36,21.3,21.34,21.35]
[null,"Bald Hills Bus 1","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.119999999999999,9.94,9.82,9.66,9.59,9.59,9.57]
[null,null,null,null,"Coincident",10.119999999999999,9.94,9.82,9.66,9.59,9.59,9.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.130000000000001,9.94,9.83,9.66,9.6,9.59,9.57]
[null,null,null,null,"Coincident",10.119999999999999,9.94,9.83,9.66,9.59,9.59,9.57]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.36,9.19,9.08,8.93,8.86,8.86,8.84]
[null,null,null,null,"Coincident",9.36,9.19,9.08,8.93,8.86,8.86,8.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.36,9.19,9.08,8.93,8.8699999999999992,8.86,8.85]
[null,null,null,null,"Coincident",9.36,9.19,9.08,8.93,8.8699999999999992,8.86,8.84]
[null,"Bald Hills Bus 2","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.22,11.83,11.52,11.19,11.08,11.03,10.97]
[null,null,null,null,"Coincident",12.18,11.8,11.49,11.16,11.05,11,10.94]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.31,11.92,11.61,11.28,11.17,11.12,11.06]
[null,null,null,null,"Coincident",12.21,11.83,11.52,11.19,11.07,11.03,10.97]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.9,10.55,10.28,9.98,9.8800000000000008,9.84,9.7899999999999991]
[null,null,null,null,"Coincident",10.87,10.52,10.25,9.9499999999999993,9.85,9.81,9.76]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.98,10.64,10.36,10.06,9.9600000000000009,9.92,9.8699999999999992]
[null,null,null,null,"Coincident",10.89,10.55,10.27,9.98,9.8800000000000008,9.83,9.7799999999999994]
[null,"Beaudesert","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.149999999999999,18.29,18.53,18.64,18.91,19.25,19.559999999999999]
[null,null,null,null,"Coincident",17.55,17.68,17.91,18.02,18.28,18.61,18.91]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.61,18.75,18.989999999999998,19.100000000000001,19.38,19.73,20.05]
[null,null,null,null,"Coincident",17.75,17.88,18.11,18.22,18.489999999999998,18.82,19.12]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.29,17.420000000000002,17.649999999999999,17.760000000000002,18.010000000000002,18.34,18.63]
[null,null,null,null,"Coincident",16.72,16.84,17.059999999999999,17.170000000000002,17.41,17.73,18.010000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.73,17.86,18.09,18.2,18.46,18.8,19.100000000000001]
[null,null,null,null,"Coincident",16.91,17.04,17.260000000000002,17.36,17.61,17.93,18.22]
[null,"Beenleigh","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.6,34.79,34.270000000000003,33.799999999999997,33.67,33.71,33.71]
[null,null,null,null,"Coincident",35.6,34.79,34.270000000000003,33.799999999999997,33.67,33.71,33.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.950000000000003,35.130000000000003,34.61,34.130000000000003,34.01,34.04,34.049999999999997]
[null,null,null,null,"Coincident",35.83,35.020000000000003,34.5,34.020000000000003,33.89,33.93,33.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.549999999999997,31.81,31.34,30.9,30.79,30.82,30.82]
[null,null,null,null,"Coincident",32.549999999999997,31.81,31.34,30.9,30.79,30.82,30.82]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.869999999999997,32.119999999999997,31.65,31.21,31.09,31.12,31.13]
[null,null,null,null,"Coincident",32.76,32.020000000000003,31.54,31.11,30.99,31.02,31.03]
[null,"Beenleigh North","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.89,19.7,19.64,19.53,19.559999999999999,19.73,19.89]
[null,null,null,null,"Coincident",19.89,19.7,19.64,19.53,19.559999999999999,19.73,19.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.059999999999999,19.88,19.809999999999999,19.7,19.73,19.91,20.059999999999999]
[null,null,null,null,"Coincident",19.989999999999998,19.809999999999999,19.739999999999998,19.63,19.66,19.84,19.989999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.78,18.61,18.55,18.45,18.47,18.64,18.78]
[null,null,null,null,"Coincident",18.78,18.61,18.55,18.45,18.47,18.64,18.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.95,18.78,18.71,18.61,18.64,18.809999999999999,18.95]
[null,null,null,null,"Coincident",18.88,18.71,18.649999999999999,18.55,18.57,18.739999999999998,18.88]
[null,"Beerwah","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.12,18.93,18.87,18.59,18.48,18.47,18.45]
[null,null,null,null,"Coincident",18.43,18.25,18.18,17.91,17.809999999999999,17.809999999999999,17.78]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.25,19.059999999999999,18.989999999999998,18.71,18.600000000000001,18.600000000000001,18.57]
[null,null,null,null,"Coincident",18.5,18.309999999999999,18.25,17.98,17.88,17.87,17.850000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.309999999999999,17.13,17.07,16.82,16.73,16.72,16.7]
[null,null,null,null,"Coincident",16.68,16.510000000000002,16.46,16.21,16.12,16.11,16.100000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.420000000000002,17.25,17.190000000000001,16.93,16.84,16.829999999999998,16.809999999999999]
[null,null,null,null,"Coincident",16.739999999999998,16.57,16.52,16.27,16.18,16.170000000000002,16.149999999999999]
[null,"Belmont","Substation Rating","MVA","Non-Coincident",41,41,41,41,58,58,58]
[null,null,null,null,"Coincident",41,41,41,41,58,58,58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.05,20.39,20.03,19.73,19.61,19.64,19.68]
[null,null,null,null,"Coincident",21.05,20.39,20.03,19.73,19.61,19.64,19.68]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.13,20.46,20.11,19.8,19.68,19.71,19.75]
[null,null,null,null,"Coincident",21.13,20.47,20.11,19.8,19.690000000000001,19.72,19.760000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.809999999999999,18.22,17.91,17.63,17.53,17.55,17.59]
[null,null,null,null,"Coincident",18.809999999999999,18.22,17.91,17.63,17.53,17.55,17.59]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.88,18.29,17.97,17.7,17.59,17.62,17.649999999999999]
[null,null,null,null,"Coincident",18.88,18.29,17.98,17.7,17.59,17.62,17.66]
[null,"Bethania","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",48,48,48,48,48,48,48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.51,24.33,24.31,24.14,24.17,24.33,24.43]
[null,null,null,null,"Coincident",23.23,23.06,23.03,22.87,22.9,23.05,23.15]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.54,24.36,24.34,24.17,24.2,24.36,24.46]
[null,null,null,null,"Coincident",23.23,23.06,23.04,22.88,22.91,23.06,23.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.4,22.24,22.21,22.06,22.09,22.23,22.33]
[null,null,null,null,"Coincident",21.23,21.07,21.05,20.91,20.93,21.07,21.16]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.43,22.27,22.24,22.09,22.12,22.26,22.36]
[null,null,null,null,"Coincident",21.23,21.07,21.05,20.91,20.94,21.07,21.16]
[null,"Birkdale","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.65,33.25,33.08,32.67,32.57,32.69,32.79]
[null,null,null,null,"Coincident",32.590000000000003,32.21,32.049999999999997,31.65,31.55,31.67,31.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.79,33.39,33.22,32.81,32.71,32.83,32.93]
[null,null,null,null,"Coincident",32.69,32.31,32.14,31.75,31.65,31.77,31.86]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.3,30.93,30.77,30.39,30.3,30.41,30.5]
[null,null,null,null,"Coincident",30.32,29.96,29.81,29.44,29.35,29.46,29.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.43,31.06,30.9,30.52,30.42,30.54,30.63]
[null,null,null,null,"Coincident",30.41,30.05,29.9,29.53,29.44,29.55,29.64]
[null,"Birtinya","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.67,21.47,21.43,21.27,21.34,21.53,21.67]
[null,null,null,null,"Coincident",20.13,19.940000000000001,19.899999999999999,19.760000000000002,19.82,19.989999999999998,20.12]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.67,21.47,21.43,21.28,21.34,21.53,21.67]
[null,null,null,null,"Coincident",20.13,19.95,19.91,19.760000000000002,19.82,20,20.13]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.52,20.329999999999998,20.29,20.14,20.2,20.38,20.51]
[null,null,null,null,"Coincident",19.05,18.88,18.84,18.71,18.760000000000002,18.93,19.05]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.52,20.329999999999998,20.29,20.149999999999999,20.21,20.39,20.52]
[null,null,null,null,"Coincident",19.059999999999999,18.89,18.850000000000001,18.71,18.77,18.940000000000001,19.059999999999999]
[null,"Black Mountain","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.83,6.74,6.69,6.6,6.58,6.62,6.66]
[null,null,null,null,"Coincident",5.95,5.87,5.83,5.75,5.73,5.76,5.8]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.87,6.78,6.73,6.64,6.61,6.65,6.7]
[null,null,null,null,"Coincident",5.95,5.87,5.83,5.75,5.73,5.76,5.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.29,6.21,6.17,6.09,6.06,6.1,6.14]
[null,null,null,null,"Coincident",5.48,5.41,5.37,5.3,5.28,5.31,5.35]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.33,6.25,6.21,6.12,6.1,6.13,6.18]
[null,null,null,null,"Coincident",5.48,5.41,5.38,5.3,5.28,5.31,5.35]
[null,"Boonah","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.1199999999999992,8.02,7.96,7.86,7.84,7.86,7.86]
[null,null,null,null,"Coincident",7.72,7.62,7.58,7.48,7.46,7.47,7.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.16,8.06,8.01,7.91,7.88,7.9,7.9]
[null,null,null,null,"Coincident",7.74,7.64,7.59,7.49,7.47,7.49,7.49]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.47,7.37,7.32,7.23,7.21,7.22,7.23]
[null,null,null,null,"Coincident",7.1,7.01,6.97,6.88,6.86,6.87,6.88]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.51,7.41,7.36,7.27,7.25,7.26,7.27]
[null,null,null,null,"Coincident",7.11,7.02,6.98,6.89,6.87,6.88,6.89]
[null,"Booval","Substation Rating","MVA","Non-Coincident",37,37,37,37,37,37,37]
[null,null,null,null,"Coincident",37,37,37,37,37,37,37]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.01,29.02,29.25,29.41,29.87,30.48,31.03]
[null,null,null,null,"Coincident",28,28.01,28.24,28.39,28.83,29.43,29.96]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.32,29.33,29.57,29.73,30.19,30.81,31.37]
[null,null,null,null,"Coincident",28.17,28.18,28.41,28.56,29.01,29.6,30.14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.88,26.9,27.11,27.26,27.68,28.25,28.76]
[null,null,null,null,"Coincident",25.95,25.96,26.17,26.32,26.72,27.27,27.77]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.17,27.19,27.4,27.56,27.98,28.56,29.08]
[null,null,null,null,"Coincident",26.11,26.12,26.33,26.48,26.88,27.44,27.93]
[null,"Brendale","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.67,38.18,37.96,37.46,37.33,37.42,37.46]
[null,null,null,null,"Coincident",37.909999999999997,37.43,37.22,36.729999999999997,36.6,36.68,36.729999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.9,38.409999999999997,38.19,37.69,37.549999999999997,37.64,37.68]
[null,null,null,null,"Coincident",38.090000000000003,37.61,37.39,36.9,36.770000000000003,36.85,36.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.46,35.99,35.79,35.32,35.19,35.270000000000003,35.32]
[null,null,null,null,"Coincident",35.74,35.29,35.090000000000003,34.630000000000003,34.5,34.58,34.630000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.67,36.21,36,35.53,35.4,35.479999999999997,35.53]
[null,null,null,null,"Coincident",35.909999999999997,35.450000000000003,35.25,34.79,34.659999999999997,34.74,34.79]
[null,"Bribie Island","Substation Rating","MVA","Non-Coincident",42,42,42,42,42,42,42]
[null,null,null,null,"Coincident",42,42,42,42,42,42,42]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.24,22.95,22.82,22.55,22.5,22.6,22.74]
[null,null,null,null,"Coincident",21.89,21.62,21.5,21.24,21.2,21.3,21.43]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.28,22.98,22.86,22.58,22.53,22.64,22.78]
[null,null,null,null,"Coincident",26.75,26.42,26.28,25.96,25.91,26.03,26.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.74,21.47,21.36,21.1,21.06,21.15,21.28]
[null,null,null,null,"Coincident",20.48,20.23,20.12,19.88,19.84,19.93,20.05]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.76,21.49,21.37,21.11,21.07,21.16,21.29]
[null,null,null,null,"Coincident",25.03,24.72,24.59,24.29,24.24,24.35,24.5]
[null,"Brighton","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.34,11.21,11.16,11.03,11.01,11.07,11.12]
[null,null,null,null,"Coincident",10.93,10.81,10.76,10.64,10.62,10.67,10.72]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.34,11.21,11.16,11.03,11.02,11.07,11.12]
[null,null,null,null,"Coincident",10.93,10.81,10.76,10.64,10.62,10.67,10.72]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.62,10.5,10.45,10.33,10.31,10.37,10.41]
[null,null,null,null,"Coincident",10.24,10.119999999999999,10.08,9.9600000000000009,9.9499999999999993,10,10.039999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.62,10.5,10.45,10.33,10.32,10.37,10.42]
[null,null,null,null,"Coincident",10.24,10.119999999999999,10.08,9.9600000000000009,9.9499999999999993,10,10.039999999999999]
[null,"Broadbeach","Substation Rating","MVA","Non-Coincident",127,127,127,127,127,127,127]
[null,null,null,null,"Coincident",127,127,127,127,127,127,127]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",61.99,60.9,60.23,59.22,58.78,58.7,58.57]
[null,null,null,null,"Coincident",61.12,60.05,59.39,58.39,57.96,57.88,57.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.11,61.01,60.34,59.32,58.88,58.8,58.67]
[null,null,null,null,"Coincident",61.15,60.07,59.41,58.41,57.98,57.9,57.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",57.08,56.08,55.46,54.53,54.13,54.05,53.94]
[null,null,null,null,"Coincident",56.28,55.29,54.69,53.77,53.37,53.3,53.18]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",57.17,56.16,55.54,54.6,54.2,54.12,54]
[null,null,null,null,"Coincident",56.3,55.31,54.7,53.78,53.38,53.31,53.19]
[null,"Bromelton","Substation Rating","MVA","Non-Coincident",31,31,31,31,31,31,31]
[null,null,null,null,"Coincident",31,31,31,31,31,31,31]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.4700000000000006,8.48,8.4700000000000006,8.5299999999999994,8.57,8.68,8.83]
[null,null,null,null,"Coincident",6.84,6.85,6.9,6.91,6.98,7.08,7.16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.58,8.59,8.4700000000000006,8.5299999999999994,8.57,8.69,8.83]
[null,null,null,null,"Coincident",6.85,6.86,6.92,6.92,6.99,7.09,7.18]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.08,8.09,8.16,8.2200000000000006,8.27,8.3699999999999992,8.51]
[null,null,null,null,"Coincident",6.52,6.53,6.58,6.58,6.65,6.75,6.83]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.18,8.19,8.17,8.2200000000000006,8.27,8.3699999999999992,8.52]
[null,null,null,null,"Coincident",6.53,6.54,6.59,6.6,6.67,6.76,6.84]
[null,"Browns Plains","Substation Rating","MVA","Non-Coincident",80,80,80,80,80,80,80]
[null,null,null,null,"Coincident",80,80,80,80,80,80,80]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.98,52.18,51.21,50.4,49.98,49.75,49.46]
[null,null,null,null,"Coincident",53.98,52.18,51.21,50.4,49.98,49.75,49.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54,52.2,51.23,50.42,49.99,49.77,49.47]
[null,null,null,null,"Coincident",54,52.19,51.23,50.42,49.99,49.76,49.47]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.98,49.29,48.38,47.62,47.22,47.01,46.74]
[null,null,null,null,"Coincident",50.98,49.29,48.38,47.62,47.22,47.01,46.74]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",50.99,49.3,48.39,47.63,47.23,47.02,46.74]
[null,null,null,null,"Coincident",50.99,49.3,48.39,47.63,47.23,47.01,46.74]
[null,"Bulimba","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.12,26.62,26.32,26.02,25.99,26.22,26.66]
[null,null,null,null,"Coincident",26.22,25.74,25.45,25.16,25.13,25.35,25.78]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.32,26.82,26.52,26.22,26.19,26.41,26.86]
[null,null,null,null,"Coincident",26.31,25.83,25.55,25.25,25.22,25.44,25.87]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.36,24.89,24.62,24.33,24.31,24.51,24.93]
[null,null,null,null,"Coincident",24.52,24.07,23.8,23.53,23.5,23.7,24.11]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.55,25.08,24.8,24.52,24.49,24.7,25.12]
[null,null,null,null,"Coincident",24.61,24.16,23.89,23.61,23.59,23.79,24.2]
[null,"Bundall","Substation Rating","MVA","Non-Coincident",31,31,31,31,31,31,55]
[null,null,null,null,"Coincident",31,31,31,31,31,31,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.2,15.79,15.56,15.23,15.02,14.87,14.74]
[null,null,null,null,"Coincident",12.8,14.26,14.06,13.76,13.58,13.44,13.32]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.72,16.37,16.13,15.79,15.58,15.42,15.28]
[null,null,null,null,"Coincident",12.99,14.53,14.32,14.03,13.84,13.7,13.57]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.15,14.76,14.55,14.25,14.05,13.91,13.79]
[null,null,null,null,"Coincident",11.85,13.34,13.15,12.87,12.7,12.57,12.46]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.63,15.3,15.08,14.77,14.57,14.42,14.29]
[null,null,null,null,"Coincident",12.03,13.59,13.4,13.12,12.95,12.82,12.7]
[null,"Bundamba","Substation Rating","MVA","Non-Coincident",122,122,122,122,122,122,122]
[null,null,null,null,"Coincident",122,122,122,122,122,122,122]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.79,37.22,36.93,36.299999999999997,36,35.94,35.880000000000003]
[null,null,null,null,"Coincident",36.5,35.950000000000003,35.67,35.06,34.78,34.71,34.659999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.909999999999997,37.340000000000003,37.04,36.4,36.1,36.03,35.979999999999997]
[null,null,null,null,"Coincident",36.630000000000003,36.07,35.79,35.17,34.880000000000003,34.81,34.76]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.42,34.89,34.619999999999997,34.020000000000003,33.75,33.68,33.630000000000003]
[null,null,null,null,"Coincident",34.22,33.700000000000003,33.44,32.86,32.6,32.54,32.479999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.51,34.97,34.700000000000003,34.090000000000003,33.82,33.75,33.700000000000003]
[null,null,null,null,"Coincident",34.31,33.79,33.520000000000003,32.94,32.67,32.61,32.549999999999997]
[null,"Buranda","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.399999999999999,28.66,28.8,28.83,29.09,29.48,29.89]
[null,null,null,null,"Coincident",18.2,26.51,26.63,26.66,26.89,27.24,27.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.63,28.98,29.12,29.15,29.41,29.8,30.22]
[null,null,null,null,"Coincident",18.32,26.95,27.07,27.1,27.33,27.68,28.05]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.34,27.6,27.73,27.76,28.01,28.37,28.76]
[null,null,null,null,"Coincident",17.25,25.57,25.68,25.71,25.92,26.25,26.6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.55,27.91,28.04,28.07,28.32,28.69,29.08]
[null,null,null,null,"Coincident",17.37,26,26.11,26.14,26.36,26.69,27.04]
[null,"Burleigh Heads","Substation Rating","MVA","Non-Coincident",130,130,130,130,130,130,130]
[null,null,null,null,"Coincident",130,130,130,130,130,130,130]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",60.04,58.72,58.3,57.54,57.44,57.9,58.38]
[null,null,null,null,"Coincident",60.04,58.72,58.3,57.54,57.44,57.9,58.38]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",60.09,58.76,58.34,57.58,57.48,57.94,58.43]
[null,null,null,null,"Coincident",60.05,58.73,58.31,57.55,57.45,57.9,58.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",54.76,53.55,53.17,52.47,52.39,52.8,53.24]
[null,null,null,null,"Coincident",54.76,53.55,53.17,52.47,52.39,52.8,53.24]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.79,53.57,53.19,52.5,52.41,52.82,53.27]
[null,null,null,null,"Coincident",54.76,53.55,53.17,52.48,52.39,52.8,53.25]
[null,"Burpengary","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.91,26.63,26.53,26.32,26.36,26.55,26.69]
[null,null,null,null,"Coincident",26.02,25.74,25.65,25.45,25.48,25.66,25.8]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.98,26.7,26.6,26.39,26.42,26.61,26.76]
[null,null,null,null,"Coincident",26.05,25.78,25.69,25.48,25.52,25.7,25.84]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.32,25.06,24.97,24.77,24.8,24.98,25.11]
[null,null,null,null,"Coincident",24.48,24.22,24.14,23.94,23.98,24.15,24.28]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.39,25.12,25.03,24.83,24.86,25.04,25.17]
[null,null,null,null,"Coincident",24.51,24.25,24.17,23.98,24.01,24.18,24.31]
[null,"Caboolture","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.73,28.22,27.9,27.51,27.36,27.36,27.34]
[null,null,null,null,"Coincident",26.68,26.2,25.91,25.55,25.41,25.41,25.39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.83,28.31,28,27.6,27.46,27.46,27.44]
[null,null,null,null,"Coincident",26.74,26.27,25.97,25.61,25.47,25.47,25.45]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.34,25.87,25.58,25.23,25.09,25.1,25.08]
[null,null,null,null,"Coincident",24.46,24.03,23.76,23.43,23.3,23.31,23.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.43,25.96,25.67,25.31,25.18,25.18,25.16]
[null,null,null,null,"Coincident",24.52,24.08,23.82,23.49,23.36,23.36,23.34]
[null,"Caboolture West","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.84,29.39,29.1,28.84,28.77,28.79,28.85]
[null,null,null,null,"Coincident",28.31,27.88,27.61,27.36,27.29,27.31,27.37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.12,29.67,29.37,29.11,29.04,29.06,29.12]
[null,null,null,null,"Coincident",28.44,28.01,27.73,27.48,27.41,27.43,27.49]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.4,27.97,27.69,27.45,27.37,27.4,27.46]
[null,null,null,null,"Coincident",26.94,26.53,26.27,26.04,25.97,25.99,26.05]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.66,28.23,27.95,27.7,27.63,27.65,27.71]
[null,null,null,null,"Coincident",27.06,26.65,26.39,26.15,26.08,26.11,26.16]
[null,"Cades County","Substation Rating","MVA","Non-Coincident",134,134,134,134,134,134,134]
[null,null,null,null,"Coincident",134,134,134,134,134,134,134]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",65.34,63.4,61.9,60.03,59.2,59.11,59.02]
[null,null,null,null,"Coincident",65.34,63.4,61.9,60.03,59.2,59.11,59.02]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",65.37,63.43,61.93,60.05,59.22,59.12,59.04]
[null,null,null,null,"Coincident",65.34,63.4,61.9,60.03,59.2,59.11,59.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",62.47,60.62,59.19,57.4,56.6,56.52,56.44]
[null,null,null,null,"Coincident",62.47,60.62,59.19,57.4,56.6,56.52,56.44]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.5,60.64,59.21,57.41,56.62,56.53,56.45]
[null,null,null,null,"Coincident",62.47,60.62,59.19,57.4,56.6,56.52,56.44]
[null,"Calamvale","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.46,37.97,37.75,37.29,37.22,37.42,37.67]
[null,null,null,null,"Coincident",37.9,37.42,37.200000000000003,36.75,36.68,36.880000000000003,37.119999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.61,38.119999999999997,37.9,37.44,37.36,37.57,37.81]
[null,null,null,null,"Coincident",38.03,37.549999999999997,37.340000000000003,36.880000000000003,36.81,37.01,37.25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.049999999999997,36.58,36.369999999999997,35.93,35.85,36.049999999999997,36.28]
[null,null,null,null,"Coincident",36.51,36.04,35.840000000000003,35.4,35.33,35.53,35.76]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.19,36.72,36.51,36.07,35.99,36.19,36.43]
[null,null,null,null,"Coincident",36.64,36.17,35.97,35.53,35.46,35.659999999999997,35.880000000000003]
[null,"Caloundra","Substation Rating","MVA","Non-Coincident",122,122,122,122,122,122,122]
[null,null,null,null,"Coincident",122,122,122,122,122,122,122]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",59.41,59.26,63.19,63.07,63.51,64.28,65.02]
[null,null,null,null,"Coincident",54.24,54.11,57.69,57.59,57.98,58.69,59.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",59.52,59.37,63.3,63.18,63.62,64.39,65.13]
[null,null,null,null,"Coincident",54.28,54.14,57.77,57.67,58.06,58.77,59.44]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",57.08,56.94,60.85,60.74,61.16,61.9,62.61]
[null,null,null,null,"Coincident",52.11,51.98,55.56,55.46,55.84,56.52,57.16]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",57.18,57.04,60.96,60.85,61.27,62.01,62.72]
[null,null,null,null,"Coincident",52.15,52.02,55.64,55.54,55.92,56.6,57.25]
[null,"Camp Hill","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.700000000000003,37.36,37.29,36.950000000000003,36.99,37.340000000000003,37.78]
[null,null,null,null,"Coincident",36.9,36.56,36.49,36.17,36.200000000000003,36.549999999999997,36.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.770000000000003,37.43,37.36,37.020000000000003,37.06,37.409999999999997,37.85]
[null,null,null,null,"Coincident",36.94,36.6,36.53,36.21,36.24,36.590000000000003,37.01]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.14,35.81,35.74,35.42,35.46,35.799999999999997,36.21]
[null,null,null,null,"Coincident",35.369999999999997,35.049999999999997,34.979999999999997,34.67,34.700000000000003,35.03,35.44]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.200000000000003,35.869999999999997,35.81,35.49,35.520000000000003,35.86,36.28]
[null,null,null,null,"Coincident",35.409999999999997,35.08,35.020000000000003,34.71,34.74,35.07,35.479999999999997]
[null,"Capalaba","Substation Rating","MVA","Non-Coincident",29,29,29,29,53,53,53]
[null,null,null,null,"Coincident",29,29,29,29,53,53,53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.29,16.920000000000002,16.68,16.32,16.13,16.02,15.94]
[null,null,null,null,"Coincident",17.03,16.670000000000002,16.43,16.079999999999998,15.89,15.78,15.7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.73,17.36,17.100000000000001,16.739999999999998,16.54,16.43,16.350000000000001]
[null,null,null,null,"Coincident",17.29,16.93,16.68,16.329999999999998,16.13,16.02,15.94]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.260000000000002,15.92,15.69,15.36,15.17,15.07,15]
[null,null,null,null,"Coincident",16.02,15.69,15.46,15.13,14.95,14.85,14.77]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.68,16.329999999999998,16.09,15.75,15.56,15.46,15.38]
[null,null,null,null,"Coincident",16.260000000000002,15.92,15.69,15.36,15.17,15.07,15]
[null,"Capalaba South","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.309999999999999,16.829999999999998,16.61,16.350000000000001,16.239999999999998,16.28,16.329999999999998]
[null,null,null,null,"Coincident",17.309999999999999,16.829999999999998,16.61,16.350000000000001,16.239999999999998,16.28,16.329999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.420000000000002,16.940000000000001,16.72,16.45,16.34,16.38,16.43]
[null,null,null,null,"Coincident",17.37,16.89,16.670000000000002,16.399999999999999,16.3,16.34,16.38]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.21,15.77,15.56,15.31,15.21,15.25,15.29]
[null,null,null,null,"Coincident",16.21,15.77,15.56,15.31,15.21,15.25,15.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.32,15.87,15.66,15.41,15.31,15.35,15.39]
[null,null,null,null,"Coincident",16.27,15.82,15.61,15.36,15.27,15.3,15.35]
[null,"Carole Park","Substation Rating","MVA","Non-Coincident",47,47,47,47,47,47,47]
[null,null,null,null,"Coincident",47,47,47,47,47,47,47]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.02,23.56,23.28,22.89,22.72,22.69,22.62]
[null,null,null,null,"Coincident",24.02,23.56,23.28,22.89,22.72,22.69,22.62]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.1,23.63,23.35,22.95,22.78,22.74,22.67]
[null,null,null,null,"Coincident",24.03,23.57,23.29,22.89,22.73,22.69,22.62]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.39,22.94,22.67,22.29,22.13,22.09,22.02]
[null,null,null,null,"Coincident",23.39,22.94,22.67,22.29,22.13,22.09,22.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.46,23,22.72,22.33,22.17,22.13,22.06]
[null,null,null,null,"Coincident",23.4,22.95,22.68,22.29,22.13,22.09,22.03]
[null,"Carole Park Central","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.08,29.82,29.78,29.59,29.36,29.33,29.41]
[null,null,null,null,"Coincident",26.28,29.82,29.62,29.25,29.12,29.13,29.1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.14,29.82,29.78,29.59,29.37,29.33,29.41]
[null,null,null,null,"Coincident",26.61,29.82,29.62,29.74,29.61,29.62,29.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.92,29.07,29.03,28.85,28.63,28.6,28.67]
[null,null,null,null,"Coincident",23.32,26.91,26.73,26.41,26.29,26.3,26.27]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.94,29.08,29.03,28.86,28.63,28.6,28.67]
[null,null,null,null,"Coincident",23.62,27.37,27.19,26.86,26.75,26.75,26.73]
[null,"Carpendale","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.91,1.89,1.87,1.85,1.84,1.85,1.84]
[null,null,null,null,"Coincident",1.32,1.3,1.3,1.28,1.27,1.28,1.27]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.93,1.91,1.89,1.87,1.86,1.87,1.86]
[null,null,null,null,"Coincident",1.33,1.32,1.31,1.29,1.29,1.29,1.29]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.75,1.73,1.72,1.69,1.69,1.69,1.69]
[null,null,null,null,"Coincident",1.21,1.19,1.19,1.17,1.17,1.17,1.17]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.77,1.75,1.74,1.71,1.71,1.71,1.71]
[null,null,null,null,"Coincident",1.22,1.21,1.2,1.18,1.18,1.18,1.18]
[null,"Charlotte St","Substation Rating","MVA","Non-Coincident",187,187,187,187,187,187,187]
[null,null,null,null,"Coincident",187,187,187,187,187,187,187]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",89.08,87.83,94.35,99.98,99.55,99.48,99.23]
[null,null,null,null,"Coincident",80.44,79.31,85.5,90.66,90.28,90.22,89.98]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",89.09,87.84,94.38,100.03,99.6,99.53,99.28]
[null,null,null,null,"Coincident",80.489999999999995,79.349999999999994,85.63,90.67,90.28,90.22,89.99]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",87.19,85.96,92.5,98.15,97.74,97.67,97.42]
[null,null,null,null,"Coincident",78.73,77.62,83.83,89.01,88.64,88.58,88.35]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",87.19,85.97,92.52,98.2,97.78,97.71,97.46]
[null,null,null,null,"Coincident",78.77,77.66,83.95,89.02,88.64,88.58,88.36]
[null,"Chermside","Substation Rating","MVA","Non-Coincident",70,70,70,70,70,70,70]
[null,null,null,null,"Coincident",70,70,70,70,70,70,70]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.56,42.86,42.47,41.83,41.6,41.6,41.53]
[null,null,null,null,"Coincident",41.94,41.26,40.89,40.270000000000003,40.049999999999997,40.049999999999997,39.979999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.63,42.92,42.53,41.89,41.65,41.65,41.58]
[null,null,null,null,"Coincident",41.99,41.31,40.93,40.32,40.090000000000003,40.090000000000003,40.03]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.22,40.56,40.19,39.58,39.36,39.36,39.299999999999997]
[null,null,null,null,"Coincident",39.68,39.04,38.69,38.11,37.89,37.89,37.83]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.27,40.6,40.229999999999997,39.619999999999997,39.39,39.39,39.33]
[null,null,null,null,"Coincident",39.72,39.08,38.729999999999997,38.14,37.93,37.93,37.869999999999997]
[null,"Clayfield","Substation Rating","MVA","Non-Coincident",51,51,51,51,51,51,51]
[null,null,null,null,"Coincident",51,51,51,51,51,51,51]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.32,19.18,19.170000000000002,19.079999999999998,19.190000000000001,19.440000000000001,19.71]
[null,null,null,null,"Coincident",17.34,17.21,17.2,17.12,17.22,17.440000000000001,17.690000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.52,19.38,19.37,19.28,19.39,19.63,19.91]
[null,null,null,null,"Coincident",17.399999999999999,17.28,17.27,17.190000000000001,17.28,17.5,17.75]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.53,18.39,18.39,18.3,18.399999999999999,18.64,18.899999999999999]
[null,null,null,null,"Coincident",16.62,16.5,16.5,16.420000000000002,16.510000000000002,16.72,16.96]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.71,18.579999999999998,18.57,18.48,18.59,18.829999999999998,19.09]
[null,null,null,null,"Coincident",16.690000000000001,16.57,16.559999999999999,16.48,16.57,16.79,17.02]
[null,"Cleveland","Substation Rating","MVA","Non-Coincident",65,65,65,65,65,65,65]
[null,null,null,null,"Coincident",65,65,65,65,65,65,65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.15,28.72,28.48,28,27.77,27.78,27.86]
[null,null,null,null,"Coincident",28.72,28.29,28.06,27.58,27.35,27.37,27.44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.24,28.8,28.57,28.08,27.85,27.86,27.94]
[null,null,null,null,"Coincident",28.81,28.38,28.15,27.67,27.44,27.46,27.53]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.16,26.76,26.54,26.09,25.87,25.89,25.96]
[null,null,null,null,"Coincident",26.76,26.36,26.14,25.7,25.49,25.5,25.57]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.24,26.84,26.62,26.16,25.95,25.96,26.03]
[null,null,null,null,"Coincident",26.84,26.45,26.23,25.78,25.57,25.58,25.65]
[null,"Coolum","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.91,25.92,26.02,25.98,25.8,25.86,26.07]
[null,null,null,null,"Coincident",22.53,22.32,22.27,21.99,21.94,22.06,22.26]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.92,25.93,26.02,25.98,25.8,25.86,26.08]
[null,null,null,null,"Coincident",22.54,22.33,22.28,22,21.95,22.06,22.26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.62,24.63,24.71,24.68,24.51,24.56,24.77]
[null,null,null,null,"Coincident",20.56,20.37,20.32,20.07,20.02,20.12,20.309999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.62,24.63,24.72,24.68,24.51,24.57,24.77]
[null,null,null,null,"Coincident",20.56,20.37,20.32,20.07,20.02,20.12,20.309999999999999]
[null,"Coomera","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.39,42.14,41.73,43.75,46.08,45.89,45.78]
[null,null,null,null,"Coincident",47.39,42.14,41.73,43.75,46.08,45.89,45.78]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.5,42.24,41.83,43.85,46.19,46,45.89]
[null,null,null,null,"Coincident",47.5,42.22,41.81,43.89,46.29,46.1,45.98]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.26,39.1,38.71,40.799999999999997,43.17,42.99,42.89]
[null,null,null,null,"Coincident",44.26,39.1,38.71,40.799999999999997,43.17,42.99,42.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.36,39.19,38.799999999999997,40.89,43.27,43.09,42.99]
[null,null,null,null,"Coincident",44.36,39.17,38.78,40.92,43.36,43.19,43.08]
[null,"Coominya","Substation Rating","MVA","Non-Coincident",13,13,13,13,16,16,16]
[null,null,null,null,"Coincident",13,13,13,13,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.83,5.74,5.71,5.64,5.62,5.62,5.61]
[null,null,null,null,"Coincident",5.58,5.5,5.47,5.4,5.38,5.39,5.38]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.94,5.86,5.82,5.75,5.73,5.74,5.73]
[null,null,null,null,"Coincident",5.63,5.55,5.51,5.44,5.42,5.43,5.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.49,5.41,5.38,5.31,5.29,5.3,5.29]
[null,null,null,null,"Coincident",5.26,5.19,5.15,5.09,5.07,5.08,5.07]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.6,5.52,5.49,5.42,5.4,5.41,5.4]
[null,null,null,null,"Coincident",5.3,5.23,5.19,5.13,5.1100000000000003,5.12,5.1100000000000003]
[null,"Cooneana","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident",26,26,26,26,26,26,26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7200000000000006,14.47,14.94,15.28,15.69,16.149999999999999,16.59]
[null,null,null,null,"Coincident",8.3800000000000008,13.91,14.36,14.69,15.08,15.52,15.94]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.73,14.48,14.95,15.29,15.69,16.149999999999999,16.600000000000001]
[null,null,null,null,"Coincident",8.41,13.94,14.38,14.71,15.1,15.54,15.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.81,13.51,13.94,14.24,14.61,15.02,15.41]
[null,null,null,null,"Coincident",7.51,12.99,13.39,13.69,14.04,14.43,14.81]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.82,13.52,13.94,14.25,14.61,15.02,15.42]
[null,null,null,null,"Coincident",7.54,13.02,13.42,13.72,14.06,14.45,14.83]
[null,"Coopers Plains","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.15,21.3,20.88,20.420000000000002,20.309999999999999,20.27,20.25]
[null,null,null,null,"Coincident",15.54,15.82,15.51,15.17,15.09,15.06,15.05]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.21,21.37,20.94,20.47,20.36,20.32,20.3]
[null,null,null,null,"Coincident",15.92,16.23,15.91,15.57,15.49,15.46,15.44]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.98,20.170000000000002,19.77,19.34,19.239999999999998,19.2,19.18]
[null,null,null,null,"Coincident",14.68,14.99,14.69,14.38,14.3,14.27,14.26]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.02,20.21,19.809999999999999,19.37,19.27,19.23,19.21]
[null,null,null,null,"Coincident",15.04,15.38,15.08,14.76,14.68,14.65,14.64]
[null,"Cooran","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.68,6.68,6.68,6.66,6.62,6.64,6.7]
[null,null,null,null,"Coincident",6.03,5.96,5.95,5.9,5.9,5.94,5.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.68,6.68,6.69,6.66,6.62,6.64,6.7]
[null,null,null,null,"Coincident",6.03,5.96,5.95,5.9,5.9,5.94,5.99]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.34,6.34,6.35,6.33,6.29,6.3,6.36]
[null,null,null,null,"Coincident",5.41,5.35,5.34,5.29,5.29,5.33,5.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.35,6.34,6.35,6.33,6.29,6.3,6.36]
[null,null,null,null,"Coincident",5.41,5.35,5.34,5.29,5.29,5.33,5.37]
[null,"Cooroy","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.82,7.83,7.86,7.84,7.8,7.83,7.91]
[null,null,null,null,"Coincident",6.58,6.52,6.49,6.43,6.44,6.5,6.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.82,7.83,7.86,7.84,7.8,7.83,7.91]
[null,null,null,null,"Coincident",6.58,6.52,6.5,6.43,6.44,6.51,6.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.36,7.37,7.4,7.38,7.35,7.37,7.45]
[null,null,null,null,"Coincident",6.02,5.96,5.94,5.88,5.89,5.95,6.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.36,7.37,7.4,7.38,7.35,7.37,7.45]
[null,null,null,null,"Coincident",6.03,5.96,5.95,5.88,5.9,5.95,6.02]
[null,"Coorparoo","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.88,21.44,21.27,21.05,21.05,21.2,21.39]
[null,null,null,null,"Coincident",21.15,20.72,20.56,20.350000000000001,20.350000000000001,20.5,20.68]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.99,21.54,21.38,21.15,21.16,21.31,21.5]
[null,null,null,null,"Coincident",21.19,20.77,20.61,20.39,20.39,20.54,20.72]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.29,19.88,19.73,19.52,19.52,19.66,19.84]
[null,null,null,null,"Coincident",19.61,19.22,19.07,18.87,18.87,19.010000000000002,19.18]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.39,19.98,19.829999999999998,19.62,19.62,19.760000000000002,19.940000000000001]
[null,null,null,null,"Coincident",19.649999999999999,19.260000000000002,19.11,18.91,18.91,19.05,19.22]
[null,"Cornubia","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.22,12.99,12.86,12.66,12.59,12.6,12.6]
[null,null,null,null,"Coincident",13.22,12.99,12.86,12.66,12.58,12.6,12.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.23,13,12.87,12.68,12.6,12.61,12.61]
[null,null,null,null,"Coincident",13.22,12.99,12.86,12.66,12.59,12.6,12.6]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.15,11.94,11.82,11.64,11.57,11.58,11.58]
[null,null,null,null,"Coincident",12.15,11.94,11.82,11.63,11.56,11.57,11.58]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.16,11.95,11.83,11.65,11.58,11.59,11.59]
[null,null,null,null,"Coincident",12.15,11.94,11.82,11.64,11.57,11.58,11.58]
[null,"Crestmead","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.81,30.79,30.3,29.69,29.55,29.62,29.65]
[null,null,null,null,"Coincident",30.81,30.79,30.3,29.69,29.55,29.62,29.65]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.11,31.09,30.58,29.96,29.81,29.88,29.91]
[null,null,null,null,"Coincident",37.89,37.520000000000003,36.92,36.18,36.01,36.1,36.130000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.69,28.72,28.26,27.69,27.56,27.63,27.65]
[null,null,null,null,"Coincident",28.69,28.72,28.26,27.69,27.56,27.63,27.65]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.93,28.95,28.48,27.89,27.76,27.83,27.86]
[null,null,null,null,"Coincident",35.33,35.020000000000003,34.46,33.770000000000003,33.61,33.69,33.72]
[null,"Currimundi","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",72,72,72,72,72,72,72]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.2,21.8,22.52,23.35,24.36,25.53,26.65]
[null,null,null,null,"Coincident",17.7,18.190000000000001,18.8,19.489999999999998,20.329999999999998,21.31,22.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.21,21.8,22.53,23.35,24.37,25.53,26.66]
[null,null,null,null,"Coincident",17.72,18.21,18.82,19.510000000000002,20.36,21.33,22.27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.28,19.82,20.48,21.23,22.15,23.21,24.24]
[null,null,null,null,"Coincident",16.09,16.54,17.100000000000001,17.72,18.489999999999998,19.38,20.23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.29,19.829999999999998,20.49,21.24,22.16,23.22,24.25]
[null,null,null,null,"Coincident",16.11,16.559999999999999,17.12,17.739999999999998,18.510000000000002,19.399999999999999,20.25]
[null,"Currumbin","Substation Rating","MVA","Non-Coincident",38,38,38,38,38,38,38]
[null,null,null,null,"Coincident",38,38,38,38,38,38,38]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.93,21.91,22.07,22.11,22.12,22.33,22.66]
[null,null,null,null,"Coincident",21.93,21.65,21.53,21.29,21.29,21.45,21.61]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22,21.93,22.09,22.14,22.15,22.36,22.69]
[null,null,null,null,"Coincident",21.98,21.7,21.58,21.34,21.34,21.5,21.66]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.02,21.05,21.2,21.25,21.26,21.46,21.78]
[null,null,null,null,"Coincident",21.02,20.75,20.64,20.41,20.41,20.56,20.71]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.09,21.08,21.23,21.27,21.28,21.48,21.8]
[null,null,null,null,"Coincident",21.07,20.8,20.69,20.46,20.46,20.61,20.76]
[null,"Darra","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.91,29.43,30.21,29.91,29.9,29.98,30.05]
[null,null,null,null,"Coincident",20.45,22.72,23.4,23.18,23.17,23.23,23.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.92,29.45,30.24,29.94,29.93,30,30.08]
[null,null,null,null,"Coincident",20.46,22.72,23.41,23.19,23.17,23.23,23.29]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.6,27.16,27.96,27.7,27.68,27.75,27.82]
[null,null,null,null,"Coincident",18.68,20.98,21.69,21.49,21.47,21.53,21.58]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.6,27.16,27.98,27.71,27.69,27.76,27.83]
[null,null,null,null,"Coincident",18.690000000000001,20.98,21.7,21.5,21.48,21.54,21.59]
[null,"Deception Bay","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.83,29.21,29.03,28.66,28.56,28.62,28.64]
[null,null,null,null,"Coincident",29.83,29.21,29.03,28.66,28.56,28.62,28.64]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.94,29.31,29.13,28.76,28.66,28.73,28.74]
[null,null,null,null,"Coincident",29.93,29.3,29.12,28.75,28.65,28.71,28.73]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.82,27.24,27.07,26.73,26.64,26.7,26.71]
[null,null,null,null,"Coincident",27.82,27.24,27.07,26.73,26.64,26.7,26.71]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.92,27.34,27.17,26.83,26.73,26.79,26.81]
[null,null,null,null,"Coincident",27.91,27.33,27.16,26.81,26.72,26.78,26.8]
[null,"Doboy","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.32,14.82,14.5,14.12,13.88,13.7,13.54]
[null,null,null,null,"Coincident",10.07,11.47,11.23,10.95,10.76,10.63,10.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.82,15.37,15.04,14.65,14.4,14.22,14.05]
[null,null,null,null,"Coincident",10.26,11.73,11.49,11.2,11.01,10.87,10.75]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.99,14.49,14.18,13.81,13.58,13.41,13.25]
[null,null,null,null,"Coincident",9.82,11.23,11,10.72,10.54,10.41,10.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.48,15.04,14.72,14.33,14.09,13.91,13.75]
[null,null,null,null,"Coincident",10.01,11.48,11.25,10.96,10.78,10.65,10.53]
[null,"Duffield Road","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.93,24.7,24.62,24.43,24.46,24.62,24.74]
[null,null,null,null,"Coincident",23.38,23.16,23.09,22.91,22.94,23.09,23.21]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25,24.77,24.7,24.5,24.53,24.69,24.82]
[null,null,null,null,"Coincident",23.4,23.18,23.11,22.93,22.95,23.11,23.23]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.64,23.42,23.35,23.16,23.19,23.35,23.47]
[null,null,null,null,"Coincident",22.17,21.97,21.9,21.72,21.75,21.9,22.01]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.71,23.49,23.42,23.23,23.26,23.42,23.53]
[null,null,null,null,"Coincident",22.19,21.98,21.92,21.74,21.77,21.92,22.03]
[null,"Eight Mile Plains Bus 1","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident",26,26,26,26,26,26,26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.13,17.559999999999999,17.309999999999999,18.079999999999998,19,19.059999999999999,19.18]
[null,null,null,null,"Coincident",17.57,17.02,16.78,17.63,18.62,18.68,18.79]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.329999999999998,17.760000000000002,17.510000000000002,18.29,19.21,19.28,19.39]
[null,null,null,null,"Coincident",17.760000000000002,17.21,16.98,17.86,18.89,18.95,19.059999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.2,16.670000000000002,16.440000000000001,17.22,18.14,18.2,18.3]
[null,null,null,null,"Coincident",16.670000000000002,16.16,15.94,16.79,17.78,17.84,17.940000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.39,16.86,16.63,17.420000000000002,18.34,18.399999999999999,18.510000000000002]
[null,null,null,null,"Coincident",16.86,16.350000000000001,16.13,17.02,18.05,18.11,18.21]
[null,"Eight Mile Plains Bus 2","Substation Rating","MVA","Non-Coincident",28,28,28,28,28,28,28]
[null,null,null,null,"Coincident",28,28,28,28,28,28,28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.98,17.72,17.57,18.309999999999999,19.2,19.239999999999998,19.3]
[null,null,null,null,"Coincident",17.47,17.23,17.079999999999998,18.059999999999999,19.2,19.239999999999998,19.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.190000000000001,17.93,17.77,18.53,19.37,19.41,19.47]
[null,null,null,null,"Coincident",17.7,17.45,17.29,18.329999999999998,19.510000000000002,19.55,19.61]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.04,16.8,16.66,17.420000000000002,18.329999999999998,18.37,18.420000000000002]
[null,null,null,null,"Coincident",16.57,16.34,16.2,17.2,18.329999999999998,18.37,18.420000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.239999999999998,17,16.850000000000001,17.62,18.5,18.53,18.59]
[null,null,null,null,"Coincident",16.78,16.55,16.41,17.45,18.64,18.68,18.73]
[null,"Enoggera","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.84,20.64,20.58,20.41,20.440000000000001,20.66,20.94]
[null,null,null,null,"Coincident",20.05,19.86,19.8,19.63,19.670000000000002,19.87,20.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21,20.79,20.73,20.56,20.59,20.81,21.09]
[null,null,null,null,"Coincident",20.100000000000001,19.899999999999999,19.850000000000001,19.68,19.71,19.920000000000002,20.190000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.010000000000002,18.82,18.77,18.61,18.649999999999999,18.84,19.09]
[null,null,null,null,"Coincident",18.29,18.11,18.059999999999999,17.91,17.940000000000001,18.12,18.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.149999999999999,18.96,18.91,18.75,18.78,18.98,19.23]
[null,null,null,null,"Coincident",18.329999999999998,18.149999999999999,18.100000000000001,17.95,17.98,18.16,18.41]
[null,"Esk","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.54,3.49,3.47,3.43,3.42,3.43,3.44]
[null,null,null,null,"Coincident",3.12,3.08,3.06,3.03,3.02,3.03,3.04]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.58,3.54,3.52,3.47,3.47,3.48,3.48]
[null,null,null,null,"Coincident",3.15,3.11,3.09,3.05,3.04,3.05,3.06]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.16,3.12,3.1,3.07,3.06,3.07,3.08]
[null,null,null,null,"Coincident",2.79,2.76,2.74,2.71,2.7,2.71,2.72]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2,3.16,3.14,3.11,3.1,3.11,3.11]
[null,null,null,null,"Coincident",2.81,2.78,2.76,2.73,2.72,2.73,2.74]
[null,"Eumundi","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.4400000000000004,4.46,4.49,4.49,4.49,4.53,4.6100000000000003]
[null,null,null,null,"Coincident",3.7,3.67,3.67,3.65,3.67,3.72,3.78]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.4400000000000004,4.47,4.49,4.49,4.49,4.54,4.6100000000000003]
[null,null,null,null,"Coincident",3.7,3.67,3.67,3.65,3.67,3.72,3.78]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.13,4.1500000000000004,4.17,4.18,4.18,4.22,4.29]
[null,null,null,null,"Coincident",3.39,3.36,3.36,3.35,3.36,3.41,3.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.13,4.16,4.18,4.18,4.18,4.22,4.29]
[null,null,null,null,"Coincident",3.39,3.36,3.36,3.35,3.36,3.41,3.47]
[null,"Fisherman Is A","Substation Rating","MVA","Non-Coincident",38,38,38,38,58,58,58]
[null,null,null,null,"Coincident",38,38,38,38,58,58,58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.81,18.71,21.96,23.48,23.41,23.4,23.35]
[null,null,null,null,"Coincident",7.6,14.49,17.010000000000002,18.190000000000001,18.14,18.12,18.079999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.99,19.07,22.38,23.92,23.86,23.84,23.79]
[null,null,null,null,"Coincident",7.62,14.78,17.420000000000002,18.66,18.61,18.600000000000001,18.559999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.5399999999999991,18.45,21.7,23.22,23.16,23.14,23.09]
[null,null,null,null,"Coincident",7.39,14.29,16.809999999999999,17.989999999999998,17.940000000000001,17.93,17.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7200000000000006,18.8,22.11,23.66,23.6,23.58,23.53]
[null,null,null,null,"Coincident",7.42,14.58,17.22,18.46,18.41,18.399999999999999,18.36]
[null,"Fisherman Is B","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident",26,26,26,26,26,26,26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.95,4.47,4.4400000000000004,4.38,4.3600000000000003,4.3499999999999996,4.33]
[null,null,null,null,"Coincident",2.86,3.09,3.07,3.02,3.01,3,2.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.25,4.8099999999999996,4.7699999999999996,4.71,4.68,4.68,4.66]
[null,null,null,null,"Coincident",3.07,3.32,3.29,3.24,3.23,3.22,3.21]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.86,4.38,4.34,4.29,4.26,4.26,4.24]
[null,null,null,null,"Coincident",2.79,3.02,3,2.96,2.94,2.94,2.92]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.1500000000000004,4.71,4.67,4.6100000000000003,4.59,4.58,4.5599999999999996]
[null,null,null,null,"Coincident",3,3.24,3.22,3.17,3.16,3.15,3.14]
[null,"Flinders","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.36,5.29,6.12,6.06,6.05,6.07,6.07]
[null,null,null,null,"Coincident",4.9400000000000004,4.88,5.64,5.58,5.57,5.59,5.59]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6,5.53,6.39,6.33,6.32,6.33,6.34]
[null,null,null,null,"Coincident",5.13,5.0599999999999996,5.86,5.81,5.8,5.81,5.82]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.9800000000000004,4.92,5.75,5.69,5.68,5.7,5.71]
[null,null,null,null,"Coincident",4.59,4.53,5.29,5.24,5.23,5.25,5.26]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2,5.14,6,5.94,5.93,5.95,5.96]
[null,null,null,null,"Coincident",4.7699999999999996,4.71,5.51,5.46,5.45,5.46,5.47]
[null,"Gatton A","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.34,18.09,17.96,17.73,17.68,17.7,17.690000000000001]
[null,null,null,null,"Coincident",18.059999999999999,17.809999999999999,17.68,17.46,17.399999999999999,17.420000000000002,17.41]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.71,18.45,18.32,18.09,18.03,18.05,18.04]
[null,null,null,null,"Coincident",18.45,18.2,18.07,17.84,17.79,17.809999999999999,17.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.8,16.57,16.46,16.239999999999998,16.190000000000001,16.21,16.21]
[null,null,null,null,"Coincident",16.54,16.32,16.2,15.99,15.94,15.96,15.95]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.14,16.91,16.79,16.57,16.52,16.54,16.53]
[null,null,null,null,"Coincident",16.91,16.68,16.559999999999999,16.350000000000001,16.29,16.32,16.309999999999999]
[null,"Gaven","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.91,30.43,30.19,29.7,29.48,29.45,29.44]
[null,null,null,null,"Coincident",30.68,30.21,29.97,29.48,29.26,29.24,29.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.02,30.55,30.3,29.81,29.59,29.56,29.55]
[null,null,null,null,"Coincident",30.75,30.28,30.03,29.54,29.33,29.3,29.29]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.88,28.44,28.21,27.75,27.54,27.52,27.5]
[null,null,null,null,"Coincident",28.66,28.23,28,27.54,27.34,27.32,27.3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.98,28.54,28.31,27.85,27.65,27.62,27.61]
[null,null,null,null,"Coincident",28.73,28.29,28.06,27.6,27.4,27.38,27.36]
[null,"Geebung","Substation Rating","MVA","Non-Coincident",79,79,79,79,79,79,79]
[null,null,null,null,"Coincident",79,79,79,79,79,79,79]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.18,36.75,36.07,35.47,35.25,35.200000000000003,35.31]
[null,null,null,null,"Coincident",27.84,28.33,27.81,27.34,27.17,27.14,27.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.33,36.92,36.229999999999997,35.619999999999997,35.39,35.340000000000003,35.450000000000003]
[null,null,null,null,"Coincident",28.07,28.6,28.07,27.6,27.43,27.39,27.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.43,35.049999999999997,34.409999999999997,33.83,33.619999999999997,33.57,33.68]
[null,null,null,null,"Coincident",26.5,27.02,26.53,26.08,25.92,25.89,25.97]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.56,35.19,34.53,33.950000000000003,33.729999999999997,33.69,33.79]
[null,null,null,null,"Coincident",26.72,27.28,26.78,26.33,26.17,26.13,26.21]
[null,"Gibson Island","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.7,20.58,20.43,20.170000000000002,20.05,20.02,19.91]
[null,null,null,null,"Coincident",0.8,0.91,0.91,0.9,0.89,0.89,0.88]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.77,20.75,20.6,20.329999999999998,20.2,20.16,20.059999999999999]
[null,null,null,null,"Coincident",0.86,0.98,0.97,0.96,0.96,0.95,0.95]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.53,20.41,20.260000000000002,20.010000000000002,19.88,19.850000000000001,19.75]
[null,null,null,null,"Coincident",0.79,0.91,0.9,0.89,0.88,0.88,0.88]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.59,20.57,20.420000000000002,20.149999999999999,20.03,19.989999999999998,19.89]
[null,null,null,null,"Coincident",0.85,0.97,0.97,0.95,0.95,0.95,0.94]
[null,"Glenore Grove","Substation Rating","MVA","Non-Coincident",19,19,19,19,19,19,19]
[null,null,null,null,"Coincident",19,19,19,19,19,19,19]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.73,10,9.98,9.9,9.91,9.9700000000000006,10.01]
[null,null,null,null,"Coincident",9,9.25,9.23,9.16,9.17,9.2200000000000006,9.26]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.73,10,9.98,9.91,9.91,9.9700000000000006,10.01]
[null,null,null,null,"Coincident",9.14,9.41,9.39,9.32,9.33,9.3800000000000008,9.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.33,9.6,9.58,9.51,9.52,9.57,9.61]
[null,null,null,null,"Coincident",8.6300000000000008,8.8800000000000008,8.86,8.7899999999999991,8.8000000000000007,8.85,8.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.33,9.6,9.59,9.51,9.52,9.57,9.61]
[null,null,null,null,"Coincident",8.77,9.0299999999999994,9.02,8.9499999999999993,8.9499999999999993,9.01,9.0399999999999991]
[null,"Goodna","Substation Rating","MVA","Non-Coincident",28,28,28,28,28,54,54]
[null,null,null,null,"Coincident",28,28,28,28,28,54,54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.760000000000002,15.97,16.21,16.440000000000001,16.93,17.61,18.350000000000001]
[null,null,null,null,"Coincident",16.63,15.84,16.079999999999998,16.309999999999999,16.79,17.47,18.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.77,15.98,16.22,16.46,16.940000000000001,17.62,18.36]
[null,null,null,null,"Coincident",16.63,15.84,16.079999999999998,16.32,16.8,17.47,18.2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.6,14.79,15.02,15.24,15.69,16.309999999999999,17]
[null,null,null,null,"Coincident",15.47,14.68,14.9,15.12,15.56,16.18,16.87]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.61,14.81,15.03,15.25,15.7,16.329999999999998,17.02]
[null,null,null,null,"Coincident",15.47,14.68,14.9,15.12,15.56,16.190000000000001,16.87]
[null,"Goomboorian","Substation Rating","MVA","Non-Coincident",9,9,9,9,9,9,9]
[null,null,null,null,"Coincident",9,9,9,9,9,9,9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.04,3,2.98,2.94,2.92,2.92,2.92]
[null,null,null,null,"Coincident",2.31,2.2799999999999998,2.27,2.23,2.2200000000000002,2.23,2.2200000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.04,3,2.98,2.94,2.93,2.93,2.92]
[null,null,null,null,"Coincident",2.31,2.2799999999999998,2.27,2.23,2.2200000000000002,2.23,2.2200000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.75,2.71,2.7,2.66,2.65,2.65,2.64]
[null,null,null,null,"Coincident",2.1,2.0699999999999998,2.0499999999999998,2.02,2.0099999999999998,2.02,2.0099999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.76,2.72,2.7,2.66,2.65,2.65,2.65]
[null,null,null,null,"Coincident",2.1,2.0699999999999998,2.0499999999999998,2.02,2.0099999999999998,2.02,2.0099999999999998]
[null,"Grantham","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.47,6.38,6.32,6.24,6.19,6.18,6.15]
[null,null,null,null,"Coincident",5.35,5.27,5.23,5.16,5.12,5.1100000000000003,5.09]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.71,6.61,6.55,6.46,6.42,6.41,6.38]
[null,null,null,null,"Coincident",5.43,5.35,5.3,5.23,5.19,5.18,5.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.39,6.29,6.24,6.15,6.11,6.1,6.07]
[null,null,null,null,"Coincident",5.28,5.2,5.16,5.09,5.05,5.04,5.0199999999999996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.62,6.52,6.46,6.37,6.33,6.32,6.29]
[null,null,null,null,"Coincident",5.36,5.28,5.23,5.16,5.12,5.1100000000000003,5.09]
[null,"Grovely","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.61,26.05,25.67,25.2,24.96,24.89,24.81]
[null,null,null,null,"Coincident",25.98,25.43,25.05,24.6,24.36,24.29,24.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.69,26.13,25.74,25.28,25.04,24.96,24.89]
[null,null,null,null,"Coincident",25.99,25.44,25.07,24.62,24.38,24.31,24.24]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.65,24.13,23.77,23.34,23.12,23.05,22.98]
[null,null,null,null,"Coincident",24.06,23.55,23.2,22.78,22.57,22.5,22.43]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.72,24.2,23.84,23.41,23.19,23.12,23.05]
[null,null,null,null,"Coincident",24.08,23.57,23.22,22.8,22.58,22.51,22.45]
[null,"Gympie","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.57,26.91,26.75,26.45,26.38,26.44,26.45]
[null,null,null,null,"Coincident",25.96,25.35,25.2,24.91,24.84,24.9,24.91]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.86,27.2,27.03,26.73,26.66,26.71,26.73]
[null,null,null,null,"Coincident",26.14,25.52,25.37,25.09,25.02,25.07,25.08]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.98,25.37,25.22,24.94,24.87,24.92,24.93]
[null,null,null,null,"Coincident",24.47,23.89,23.75,23.48,23.42,23.47,23.48]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.26,25.64,25.48,25.2,25.13,25.18,25.2]
[null,null,null,null,"Coincident",24.64,24.06,23.92,23.65,23.59,23.64,23.65]
[null,"Gympie North","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.59,18.309999999999999,18.16,17.91,17.829999999999998,17.84,17.809999999999999]
[null,null,null,null,"Coincident",15.56,15.32,15.19,14.98,14.92,14.92,14.9]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.68,18.39,18.239999999999998,17.989999999999998,17.91,17.920000000000002,17.89]
[null,null,null,null,"Coincident",15.59,15.35,15.23,15.02,14.95,14.96,14.94]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.69,15.44,15.32,15.11,15.04,15.05,15.03]
[null,null,null,null,"Coincident",13.12,12.92,12.82,12.64,12.58,12.59,12.57]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.76,15.52,15.39,15.18,15.11,15.12,15.1]
[null,null,null,null,"Coincident",13.16,12.95,12.85,12.67,12.61,12.62,12.6]
[null,"Gympie South","Substation Rating","MVA","Non-Coincident",16,16,16,16,16,16,16]
[null,null,null,null,"Coincident",16,16,16,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.42,8.58,8.49,8.44,8.39,8.39,8.42]
[null,null,null,null,"Coincident",5.07,5.74,5.67,5.57,5.53,5.5,5.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.67,8.8699999999999992,8.68,8.6300000000000008,8.58,8.58,8.61]
[null,null,null,null,"Coincident",5.15,5.86,5.79,5.69,5.64,5.62,5.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.16,8.33,8.2899999999999991,8.25,8.19,8.19,8.2200000000000006]
[null,null,null,null,"Coincident",4.8899999999999997,5.57,5.5,5.41,5.36,5.34,5.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.41,8.61,8.48,8.43,8.3800000000000008,8.3800000000000008,8.41]
[null,null,null,null,"Coincident",4.97,5.68,5.61,5.52,5.47,5.45,5.42]
[null,"Hamilton","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.79,22.41,22.28,22.11,22.17,22.36,22.67]
[null,null,null,null,"Coincident",22.28,21.9,21.77,21.6,21.66,21.85,22.16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.05,22.66,22.52,22.35,22.41,22.61,22.92]
[null,null,null,null,"Coincident",22.42,22.04,21.91,21.74,21.8,21.99,22.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.57,21.2,21.08,20.92,20.97,21.16,21.45]
[null,null,null,null,"Coincident",21.08,20.72,20.6,20.440000000000001,20.49,20.68,20.96]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.81,21.44,21.31,21.15,21.21,21.39,21.69]
[null,null,null,null,"Coincident",21.21,20.85,20.73,20.57,20.63,20.81,21.1]
[null,"Hamilton Lands","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.14,14.05,14.42,14.71,15.15,15.65,16.16]
[null,null,null,null,"Coincident",8.56,9.1300000000000008,9.3800000000000008,9.56,9.85,10.18,10.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.91,14.87,15.27,15.58,16.05,15.65,16.16]
[null,null,null,null,"Coincident",8.68,9.27,9.52,9.7100000000000009,10,10.33,10.67]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.81,13.7,14.07,14.35,14.78,15.27,15.76]
[null,null,null,null,"Coincident",8.34,8.91,9.15,9.33,9.61,9.93,10.25]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.56,14.51,14.9,15.2,15.65,16.170000000000002,15.76]
[null,null,null,null,"Coincident",8.4600000000000009,9.0399999999999991,9.2899999999999991,9.4700000000000006,9.76,10.08,10.4]
[null,"Heathwood","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.83,31.27,30.92,30.37,30.1,29.99,29.82]
[null,null,null,null,"Coincident",31.83,31.27,30.92,30.37,30.1,29.99,29.82]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.87,31.3,30.95,30.4,30.13,30.01,29.84]
[null,null,null,null,"Coincident",34.450000000000003,33.85,33.47,32.880000000000003,32.590000000000003,32.46,32.28]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.88,29.35,29.03,28.51,28.26,28.16,27.99]
[null,null,null,null,"Coincident",29.88,29.35,29.03,28.51,28.26,28.16,27.99]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.9,29.37,29.04,28.53,28.27,28.17,28]
[null,null,null,null,"Coincident",32.35,31.78,31.42,30.87,30.59,30.48,30.3]
[null,"Helidon","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.98,2.92,2.87,2.82,2.8,2.81,2.82]
[null,null,null,null,"Coincident",2.63,2.57,2.5299999999999998,2.48,2.46,2.4700000000000002,2.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.06,3,2.95,2.9,2.88,2.88,2.9]
[null,null,null,null,"Coincident",2.67,2.61,2.57,2.52,2.5,2.5099999999999998,2.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.81,2.74,2.7,2.65,2.63,2.64,2.66]
[null,null,null,null,"Coincident",2.4700000000000002,2.41,2.38,2.34,2.3199999999999998,2.3199999999999998,2.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.88,2.82,2.78,2.73,2.71,2.71,2.73]
[null,null,null,null,"Coincident",2.5099999999999998,2.4500000000000002,2.42,2.37,2.35,2.36,2.37]
[null,"Hemmant","Substation Rating","MVA","Non-Coincident",38,38,38,38,38,38,38]
[null,null,null,null,"Coincident",38,38,38,38,38,38,38]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.5,10.42,10.39,10.29,10.27,10.29,10.3]
[null,null,null,null,"Coincident",9.64,9.56,9.5399999999999991,9.44,9.43,9.4499999999999993,9.4499999999999993]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.69,10.6,10.57,10.47,10.45,10.47,10.48]
[null,null,null,null,"Coincident",9.73,9.65,9.6199999999999992,9.5299999999999994,9.52,9.5299999999999994,9.5399999999999991]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.09,10.01,9.98,9.8800000000000008,9.8699999999999992,9.89,9.89]
[null,null,null,null,"Coincident",9.26,9.19,9.16,9.07,9.06,9.07,9.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.27,10.18,10.15,10.06,10.039999999999999,10.06,10.07]
[null,null,null,null,"Coincident",9.35,9.27,9.24,9.15,9.14,9.16,9.16]
[null,"Hendra","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.28,17.77,17.600000000000001,19.32,19.28,19.41,19.57]
[null,null,null,null,"Coincident",17.32,16.84,16.68,18.329999999999998,18.29,18.41,18.559999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.52,18.010000000000002,17.829999999999998,19.579999999999998,19.54,19.670000000000002,19.829999999999998]
[null,null,null,null,"Coincident",17.399999999999999,16.920000000000002,16.75,18.46,18.420000000000002,18.54,18.690000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.899999999999999,16.440000000000001,16.28,18.02,17.98,18.100000000000001,18.25]
[null,null,null,null,"Coincident",16.02,15.58,15.42,17.09,17.059999999999999,17.170000000000002,17.309999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.13,16.66,16.5,18.260000000000002,18.23,18.34,18.489999999999998]
[null,null,null,null,"Coincident",16.09,15.65,15.49,17.22,17.18,17.3,17.440000000000001]
[null,"Holland Park","Substation Rating","MVA","Non-Coincident",48,49,49,49,49,49,49]
[null,null,null,null,"Coincident",48,49,49,49,49,49,49]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.93,25.37,25.17,24.87,24.84,25,25.19]
[null,null,null,null,"Coincident",25.7,25.14,24.95,24.66,24.62,24.78,24.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.09,25.53,25.33,25.04,25,25.16,25.35]
[null,null,null,null,"Coincident",25.83,25.27,25.07,24.78,24.75,24.9,25.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.7,24.16,23.97,23.7,23.66,23.81,24]
[null,null,null,null,"Coincident",24.48,23.95,23.76,23.49,23.45,23.6,23.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.86,24.32,24.13,23.85,23.82,23.97,24.15]
[null,null,null,null,"Coincident",24.61,24.08,23.89,23.61,23.58,23.72,23.91]
[null,"Holland Park East","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.58,20.3,20.170000000000002,19.93,19.91,20.03,20.190000000000001]
[null,null,null,null,"Coincident",20.329999999999998,20.05,19.920000000000002,19.690000000000001,19.66,19.79,19.95]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.78,20.49,20.36,20.12,20.100000000000001,20.22,20.39]
[null,null,null,null,"Coincident",20.41,20.13,20,19.760000000000002,19.739999999999998,19.86,20.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.57,19.3,19.170000000000002,18.95,18.920000000000002,19.05,19.2]
[null,null,null,null,"Coincident",19.329999999999998,19.059999999999999,18.940000000000001,18.72,18.690000000000001,18.809999999999999,18.96]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.75,19.48,19.36,19.13,19.100000000000001,19.23,19.38]
[null,null,null,null,"Coincident",19.399999999999999,19.13,19.010000000000002,18.79,18.760000000000002,18.88,19.03]
[null,"Hollywell","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.5,40.14,40.08,39.78,39.869999999999997,40.25,40.64]
[null,null,null,null,"Coincident",39.82,39.46,39.409999999999997,39.11,39.200000000000003,39.57,39.950000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.68,40.32,40.26,39.96,40.049999999999997,40.43,40.82]
[null,null,null,null,"Coincident",39.96,39.6,39.54,39.25,39.340000000000003,39.71,40.090000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.99,36.65,36.6,36.33,36.409999999999997,36.75,37.11]
[null,null,null,null,"Coincident",36.36,36.04,35.99,35.72,35.799999999999997,36.14,36.49]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.15,36.82,36.770000000000003,36.49,36.57,36.92,37.28]
[null,null,null,null,"Coincident",36.49,36.159999999999997,36.11,35.840000000000003,35.92,36.26,36.61]
[null,"Hope Island","Substation Rating","MVA","Non-Coincident",58,58,58,58,58,58,58]
[null,null,null,null,"Coincident",58,58,58,58,58,58,58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.93,38.56,38.479999999999997,38.340000000000003,38.61,39.159999999999997,39.729999999999997]
[null,null,null,null,"Coincident",29.8,29.51,29.46,29.35,29.55,29.98,30.42]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39,38.619999999999997,38.549999999999997,38.4,38.67,39.22,39.799999999999997]
[null,null,null,null,"Coincident",29.81,29.52,29.47,29.35,29.56,29.98,30.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.270000000000003,35.92,35.85,35.71,35.96,36.479999999999997,37.020000000000003]
[null,null,null,null,"Coincident",27.76,27.49,27.44,27.34,27.53,27.92,28.33]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.32,35.97,35.9,35.76,36.01,36.53,37.07]
[null,null,null,null,"Coincident",27.77,27.5,27.45,27.34,27.53,27.93,28.34]
[null,"Ibis","Substation Rating","MVA","Non-Coincident",9,9,9,9,9,9,9]
[null,null,null,null,"Coincident",9,9,9,9,9,9,9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.48,0.48,0.49,0.49,0.49,0.49,0.5]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.38,0.39,0.4,0.4]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.52,0.52,0.52,0.52,0.52,0.52,0.53]
[null,null,null,null,"Coincident",0.42,0.41,0.41,0.41,0.41,0.42,0.43]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.45,0.45,0.45,0.45,0.45,0.45,0.46]
[null,null,null,null,"Coincident",0.36,0.35,0.35,0.35,0.35,0.36,0.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.48,0.48,0.48,0.48,0.48,0.49,0.49]
[null,null,null,null,"Coincident",0.38,0.38,0.37,0.37,0.38,0.38,0.39]
[null,"Imbil","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4900000000000002,2.48,2.4700000000000002,2.4500000000000002,2.4300000000000002,2.42,2.4300000000000002]
[null,null,null,null,"Coincident",1.68,1.65,1.63,1.6,1.59,1.59,1.58]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.75,2.74,2.73,2.71,2.68,2.68,2.68]
[null,null,null,null,"Coincident",1.71,1.68,1.66,1.64,1.62,1.62,1.61]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.38,2.37,2.37,2.35,2.3199999999999998,2.3199999999999998,2.33]
[null,null,null,null,"Coincident",1.59,1.56,1.55,1.52,1.51,1.5,1.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.63,2.62,2.61,2.59,2.57,2.56,2.57]
[null,null,null,null,"Coincident",1.62,1.59,1.58,1.55,1.54,1.53,1.53]
[null,"Inala","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.82,32.46,32.340000000000003,32.119999999999997,32.22,32.49,32.72]
[null,null,null,null,"Coincident",32.82,32.46,32.340000000000003,32.119999999999997,32.22,32.49,32.72]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.94,32.590000000000003,32.46,32.24,32.340000000000003,32.61,32.85]
[null,null,null,null,"Coincident",32.880000000000003,32.53,32.4,32.19,32.28,32.56,32.79]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.94,30.61,30.49,30.29,30.38,30.64,30.86]
[null,null,null,null,"Coincident",30.94,30.61,30.49,30.29,30.38,30.64,30.86]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.06,30.73,30.61,30.4,30.49,30.75,30.97]
[null,null,null,null,"Coincident",31.01,30.67,30.55,30.35,30.44,30.7,30.92]
[null,"Indooroopilly","Substation Rating","MVA","Non-Coincident",54,54,54,54,54,54,54]
[null,null,null,null,"Coincident",54,54,54,54,54,54,54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.44,23.02,22.76,22.4,22.26,22.29,22.33]
[null,null,null,null,"Coincident",20.350000000000001,19.98,19.760000000000002,19.440000000000001,19.329999999999998,19.350000000000001,19.39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.76,23.33,23.07,22.7,22.56,22.59,22.64]
[null,null,null,null,"Coincident",20.56,20.190000000000001,19.97,19.649999999999999,19.53,19.55,19.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.31,21.91,21.67,21.32,21.19,21.21,21.26]
[null,null,null,null,"Coincident",19.37,19.02,18.809999999999999,18.510000000000002,18.399999999999999,18.420000000000002,18.46]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.61,22.2,21.96,21.6,21.48,21.5,21.55]
[null,null,null,null,"Coincident",19.57,19.22,19.010000000000002,18.7,18.59,18.61,18.649999999999999]
[null,"Innisplain","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.45,4.43,4.4400000000000004,4.42,4.4400000000000004,4.49,4.5199999999999996]
[null,null,null,null,"Coincident",4.2,4.18,4.1900000000000004,4.17,4.1900000000000004,4.24,4.2699999999999996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.5,4.4800000000000004,4.49,4.47,4.49,4.54,4.58]
[null,null,null,null,"Coincident",4.2,4.18,4.1900000000000004,4.17,4.1900000000000004,4.24,4.2699999999999996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.24,4.2300000000000004,4.2300000000000004,4.22,4.24,4.28,4.32]
[null,null,null,null,"Coincident",4.01,3.99,4,3.98,4,4.04,4.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.29,4.28,4.28,4.26,4.29,4.33,4.37]
[null,null,null,null,"Coincident",4.1100000000000003,4.09,4.0999999999999996,4.08,4.0999999999999996,4.04,4.08]
[null,"Ipswich South","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.53,24.68,24.99,25.1,25.45,25.94,26.38]
[null,null,null,null,"Coincident",22.44,22.57,22.86,22.96,23.28,23.73,24.13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.56,24.71,25.02,25.13,25.48,25.98,26.41]
[null,null,null,null,"Coincident",22.44,22.58,22.87,22.97,23.29,23.74,24.14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.38,22.51,22.8,22.9,23.22,23.67,24.07]
[null,null,null,null,"Coincident",20.47,20.6,20.86,20.95,21.24,21.65,22.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.41,22.55,22.83,22.93,23.25,23.7,24.1]
[null,null,null,null,"Coincident",20.48,20.6,20.86,20.96,21.25,21.66,22.02]
[null,"Jimboomba","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",48,48,48,48,48,48,48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.67,37.49,39.700000000000003,41.06,43.15,43.46,43.68]
[null,null,null,null,"Coincident",33.97,33.81,35.81,37.03,38.92,39.19,39.39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.869999999999997,37.700000000000003,39.92,41.28,43.39,43.69,43.92]
[null,null,null,null,"Coincident",34.08,33.93,35.97,37.229999999999997,39.17,39.450000000000003,39.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.68,33.520000000000003,35.72,37.11,39.200000000000003,39.47,39.67]
[null,null,null,null,"Coincident",30.37,30.23,32.22,33.47,35.35,35.6,35.770000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.86,33.71,35.92,37.32,39.409999999999997,39.69,39.89]
[null,null,null,null,"Coincident",30.47,30.33,32.36,33.659999999999997,35.6,35.840000000000003,36.020000000000003]
[null,"Jindalee","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.7,14.4,14.21,13.95,13.83,13.8,13.77]
[null,null,null,null,"Coincident",14.7,14.4,14.21,13.95,13.83,13.8,13.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.77,14.47,14.28,14.01,13.9,13.86,13.83]
[null,null,null,null,"Coincident",14.73,14.43,14.24,13.98,13.86,13.83,13.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.77,13.49,13.32,13.07,12.96,12.93,12.9]
[null,null,null,null,"Coincident",13.77,13.49,13.32,13.07,12.96,12.93,12.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.84,13.56,13.38,13.13,13.02,12.99,12.96]
[null,null,null,null,"Coincident",13.8,13.52,13.34,13.09,12.98,12.96,12.93]
[null,"Kalbar","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.91,8.7899999999999991,8.73,8.6199999999999992,8.59,8.59,8.58]
[null,null,null,null,"Coincident",7.8,7.7,7.64,7.54,7.51,7.52,7.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.91,8.8000000000000007,8.74,8.6199999999999992,8.59,8.59,8.58]
[null,null,null,null,"Coincident",7.8,7.7,7.65,7.55,7.52,7.52,7.51]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.06,7.96,7.91,7.8,7.77,7.78,7.77]
[null,null,null,null,"Coincident",7.06,6.97,6.92,6.83,6.8,6.81,6.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.06,8.09,8.0399999999999991,7.93,7.9,7.9,7.89]
[null,null,null,null,"Coincident",7.2,7.11,7.06,6.96,6.93,6.94,6.93]
[null,"Kallangur","Substation Rating","MVA","Non-Coincident",45,45,45,45,45,45,88]
[null,null,null,null,"Coincident",45,45,45,45,45,45,88]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.43,39.67,40.36,41.8,42.63,42.72,42.77]
[null,null,null,null,"Coincident",40.43,39.67,40.36,41.8,42.63,42.72,42.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.56,39.799999999999997,40.5,41.94,42.78,42.87,42.92]
[null,null,null,null,"Coincident",40.5,39.74,40.450000000000003,41.94,42.79,42.88,42.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.18,36.479999999999997,37.200000000000003,38.68,39.520000000000003,39.6,39.64]
[null,null,null,null,"Coincident",37.18,36.479999999999997,37.200000000000003,38.68,39.520000000000003,39.6,39.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.299999999999997,36.6,37.32,38.81,39.65,39.729999999999997,39.78]
[null,null,null,null,"Coincident",37.25,36.54,37.28,38.799999999999997,39.67,39.75,39.79]
[null,"Karrabin","Substation Rating","MVA","Non-Coincident",35,35,35,35,35,35,35]
[null,null,null,null,"Coincident",35,35,35,35,35,35,35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.41,21.36,21.52,21.55,21.77,22.11,22.39]
[null,null,null,null,"Coincident",19.809999999999999,19.760000000000002,19.91,19.940000000000001,20.14,20.45,20.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.63,21.59,21.75,21.78,22,22.34,22.62]
[null,null,null,null,"Coincident",19.989999999999998,19.95,20.100000000000001,20.12,20.329999999999998,20.64,20.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.73,19.68,19.829999999999998,19.86,20.059999999999999,20.37,20.63]
[null,null,null,null,"Coincident",18.25,18.21,18.34,18.37,18.55,18.84,19.079999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.93,19.89,20.04,20.07,20.27,20.58,20.84]
[null,null,null,null,"Coincident",18.420000000000002,18.38,18.510000000000002,18.54,18.73,19.02,19.260000000000002]
[null,"Kawana","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.61,27.18,26.91,26.48,26.49,26.67,26.96]
[null,null,null,null,"Coincident",25.29,24.89,24.65,24.26,24.26,24.43,24.7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.85,27.42,27.14,26.71,26.72,26.9,27.2]
[null,null,null,null,"Coincident",25.4,25,24.75,24.36,24.36,24.53,24.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.46,25.06,24.81,24.42,24.42,24.59,24.86]
[null,null,null,null,"Coincident",23.32,22.95,22.73,22.37,22.37,22.52,22.77]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.68,25.28,25.03,24.63,24.64,24.8,25.08]
[null,null,null,null,"Coincident",23.41,23.05,22.82,22.46,22.46,22.62,22.87]
[null,"Kedron","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.9,31.45,31.23,30.82,30.74,31.01,31.33]
[null,null,null,null,"Coincident",30.52,30.09,29.87,29.48,29.4,29.66,29.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.020000000000003,31.57,31.34,30.93,30.85,31.12,31.44]
[null,null,null,null,"Coincident",30.53,30.11,29.89,29.49,29.42,29.68,29.98]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.01,29.59,29.38,28.99,28.92,29.17,29.47]
[null,null,null,null,"Coincident",28.71,28.3,28.1,27.73,27.66,27.9,28.19]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.12,29.7,29.49,29.1,29.02,29.28,29.58]
[null,null,null,null,"Coincident",28.73,28.32,28.12,27.75,27.67,27.92,28.21]
[null,"Kelvin Grove","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.27,18.829999999999998,18.63,18.39,18.350000000000001,18.440000000000001,18.59]
[null,null,null,null,"Coincident",18.16,17.739999999999998,17.559999999999999,17.32,17.29,17.38,17.510000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.38,18.93,18.739999999999998,18.489999999999998,18.45,18.54,18.690000000000001]
[null,null,null,null,"Coincident",18.190000000000001,17.77,17.59,17.36,17.32,17.41,17.55]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.98,17.57,17.39,17.16,17.12,17.21,17.34]
[null,null,null,null,"Coincident",16.940000000000001,16.55,16.38,16.16,16.13,16.21,16.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.079999999999998,17.66,17.48,17.25,17.21,17.3,17.440000000000001]
[null,null,null,null,"Coincident",16.97,16.579999999999998,16.41,16.2,16.16,16.25,16.37]
[null,"Kenilworth","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.79,4.79,4.79,4.7699999999999996,4.74,4.74,4.78]
[null,null,null,null,"Coincident",4.29,4.2300000000000004,4.21,4.1500000000000004,4.13,4.1399999999999997,4.16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.79,4.8,4.8,4.78,4.74,4.75,4.79]
[null,null,null,null,"Coincident",4.34,4.28,4.26,4.2,4.18,4.1900000000000004,4.21]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.62,4.62,4.62,4.5999999999999996,4.57,4.58,4.6100000000000003]
[null,null,null,null,"Coincident",4.0199999999999996,3.97,3.94,3.89,3.87,3.89,3.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.63,4.63,4.63,4.6100000000000003,4.58,4.59,4.62]
[null,null,null,null,"Coincident",4.07,4.0199999999999996,3.99,3.93,3.92,3.93,3.94]
[null,"Kenmore","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.04,33.44,33.119999999999997,32.64,32.57,32.979999999999997,33.56]
[null,null,null,null,"Coincident",34.020000000000003,33.43,33.1,32.619999999999997,32.549999999999997,32.96,33.549999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.1,33.51,33.18,32.700000000000003,32.630000000000003,33.04,33.630000000000003]
[null,null,null,null,"Coincident",34.03,33.44,33.119999999999997,32.64,32.57,32.979999999999997,33.56]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.59,30.06,29.77,29.34,29.28,29.64,30.17]
[null,null,null,null,"Coincident",30.58,30.05,29.75,29.32,29.26,29.63,30.15]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.65,30.12,29.83,29.4,29.33,29.7,30.23]
[null,null,null,null,"Coincident",30.59,30.06,29.77,29.34,29.27,29.64,30.17]
[null,"Kilcoy","Substation Rating","MVA","Non-Coincident",28,28,28,28,28,28,28]
[null,null,null,null,"Coincident",28,28,28,28,28,28,28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.26,13.08,13,12.84,12.8,12.83,12.81]
[null,null,null,null,"Coincident",9.8699999999999992,9.74,9.67,9.56,9.5299999999999994,9.5399999999999991,9.5299999999999994]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.3,13.13,13.04,12.88,12.84,12.86,12.85]
[null,null,null,null,"Coincident",9.89,9.76,9.6999999999999993,9.58,9.5500000000000007,9.57,9.56]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.15,11.99,11.91,11.77,11.73,11.75,11.74]
[null,null,null,null,"Coincident",9.0399999999999991,8.92,8.86,8.76,8.73,8.74,8.73]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.18,12.02,11.94,11.79,11.76,11.78,11.76]
[null,null,null,null,"Coincident",9.06,8.94,8.8800000000000008,8.7799999999999994,8.75,8.76,8.75]
[null,"Kingston","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.81,37.020000000000003,37.130000000000003,37.14,37.450000000000003,37.909999999999997,38.28]
[null,null,null,null,"Coincident",35.36,34.61,34.72,34.729999999999997,35.020000000000003,35.450000000000003,35.79]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.03,37.229999999999997,37.340000000000003,37.36,37.659999999999997,38.130000000000003,38.5]
[null,null,null,null,"Coincident",35.47,34.71,34.82,34.83,35.119999999999997,35.549999999999997,35.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.270000000000003,35.479999999999997,35.58,35.6,35.89,36.33,36.69]
[null,null,null,null,"Coincident",33.92,33.18,33.28,33.29,33.56,33.979999999999997,34.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.479999999999997,35.68,35.79,35.81,36.1,36.549999999999997,36.9]
[null,null,null,null,"Coincident",34.020000000000003,33.270000000000003,33.369999999999997,33.39,33.659999999999997,34.08,34.409999999999997]
[null,"Kirra","Substation Rating","MVA","Non-Coincident",24,24,28,28,28,28,28]
[null,null,null,null,"Coincident",24,24,28,28,28,28,28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.309999999999999,19.23,19.27,19.18,19.28,19.48,19.64]
[null,null,null,null,"Coincident",18.63,18.55,18.59,18.510000000000002,18.600000000000001,18.79,18.95]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.510000000000002,19.420000000000002,19.46,19.38,19.47,19.670000000000002,19.84]
[null,null,null,null,"Coincident",18.690000000000001,18.61,18.64,18.559999999999999,18.649999999999999,18.850000000000001,19.010000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.39,18.3,18.34,18.260000000000002,18.350000000000001,18.54,18.7]
[null,null,null,null,"Coincident",17.739999999999998,17.66,17.690000000000001,17.62,17.7,17.89,18.04]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.57,18.489999999999998,18.53,18.45,18.54,18.73,18.89]
[null,null,null,null,"Coincident",17.79,17.71,17.75,17.670000000000002,17.760000000000002,17.940000000000001,18.09]
[null,"Labrador","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.27,24,23.91,23.86,24.05,24.41,24.77]
[null,null,null,null,"Coincident",24.27,24,23.91,23.86,24.05,24.41,24.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.52,24.24,24.15,24.1,24.3,24.65,25.02]
[null,null,null,null,"Coincident",24.45,24.18,24.08,24.03,24.23,24.58,24.95]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.48,22.23,22.14,22.09,22.28,22.6,22.94]
[null,null,null,null,"Coincident",22.48,22.23,22.14,22.09,22.28,22.6,22.94]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.7,22.45,22.36,22.32,22.5,22.83,23.17]
[null,null,null,null,"Coincident",22.64,22.39,22.3,22.26,22.44,22.77,23.11]
[null,"Laidley","Substation Rating","MVA","Non-Coincident",19,19,19,19,19,19,28]
[null,null,null,null,"Coincident",19,19,19,19,19,19,28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.16,12.99,15.54,15.38,15.34,15.38,15.38]
[null,null,null,null,"Coincident",11.36,11.22,13.41,13.28,13.25,13.28,13.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.17,13,15.56,15.4,15.37,15.4,15.41]
[null,null,null,null,"Coincident",11.49,11.35,13.43,13.3,13.26,13.29,13.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.34,12.18,14.73,14.58,14.55,14.58,14.59]
[null,null,null,null,"Coincident",10.65,10.52,12.72,12.59,12.56,12.59,12.59]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.34,12.18,14.75,14.6,14.56,14.6,14.6]
[null,null,null,null,"Coincident",10.77,10.64,12.73,12.6,12.57,12.6,12.6]
[null,"Landsborough","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.38,13.7,13.74,13.71,13.71,13.86,14.07]
[null,null,null,null,"Coincident",13.04,12.93,12.91,12.86,12.91,13.05,13.16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.39,13.71,13.75,13.72,13.72,13.87,14.08]
[null,null,null,null,"Coincident",13.04,12.93,12.92,12.86,12.91,13.05,13.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.61,12.57,12.61,12.58,12.58,12.71,12.91]
[null,null,null,null,"Coincident",12.28,12.19,12.17,12.11,12.17,12.29,12.4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.62,12.58,12.62,12.59,12.59,12.72,12.92]
[null,null,null,null,"Coincident",12.29,12.19,12.17,12.12,12.17,12.3,12.41]
[null,"Lawnton","Substation Rating","MVA","Non-Coincident",49,49,49,49,49,49,49]
[null,null,null,null,"Coincident",49,49,49,49,49,49,49]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.08,37.85,37.9,37.840000000000003,38.15,38.700000000000003,39.200000000000003]
[null,null,null,null,"Coincident",38.08,37.85,37.9,37.840000000000003,38.15,38.700000000000003,39.200000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.26,38.020000000000003,38.08,38.020000000000003,38.32,38.880000000000003,39.380000000000003]
[null,null,null,null,"Coincident",38.18,37.950000000000003,38.01,37.950000000000003,38.25,38.81,39.31]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.49,35.28,35.33,35.270000000000003,35.549999999999997,36.07,36.54]
[null,null,null,null,"Coincident",35.49,35.28,35.33,35.270000000000003,35.549999999999997,36.07,36.54]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.659999999999997,35.44,35.49,35.43,35.72,36.24,36.700000000000003]
[null,null,null,null,"Coincident",35.590000000000003,35.369999999999997,35.42,35.369999999999997,35.65,36.17,36.64]
[null,"Lockrose","Substation Rating","MVA","Non-Coincident",18,18,18,18,39,39,39]
[null,null,null,null,"Coincident",18,18,18,18,39,39,39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.82,10.69,10.64,10.53,10.5,10.54,10.55]
[null,null,null,null,"Coincident",8.86,8.76,8.7100000000000009,8.6199999999999992,8.6,8.6300000000000008,8.64]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.93,10.8,10.75,10.63,10.6,10.64,10.65]
[null,null,null,null,"Coincident",8.89,8.7799999999999994,8.74,8.64,8.6199999999999992,8.65,8.66]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.85,9.73,9.69,9.58,9.56,9.59,9.6]
[null,null,null,null,"Coincident",8.07,7.97,7.93,7.85,7.83,7.85,7.86]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.9499999999999993,9.83,9.7799999999999994,9.68,9.65,9.69,9.69]
[null,null,null,null,"Coincident",8.09,7.99,7.95,7.87,7.85,7.88,7.88]
[null,"Logan Village","Substation Rating","MVA","Non-Coincident",30,30,30,58,58,58,58]
[null,null,null,null,"Coincident",30,30,30,58,58,58,58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.15,25.37,25.75,25.76,25.96,26.31,26.63]
[null,null,null,null,"Coincident",23.7,23.91,24.27,24.28,24.46,24.8,25.1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.15,25.37,25.75,25.76,25.96,26.31,26.63]
[null,null,null,null,"Coincident",23.7,23.91,24.27,24.28,24.46,24.8,25.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.97,23.17,23.52,23.53,23.71,24.04,24.32]
[null,null,null,null,"Coincident",21.65,21.84,22.17,22.17,22.35,22.65,22.92]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.97,23.18,23.52,23.53,23.71,24.04,24.33]
[null,null,null,null,"Coincident",21.65,21.84,22.17,22.17,22.35,22.65,22.92]
[null,"Loganholme","Substation Rating","MVA","Non-Coincident",43,43,43,43,43,43,43]
[null,null,null,null,"Coincident",43,43,43,43,43,43,43]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.65,25.94,25.45,24.88,24.61,24.52,24.43]
[null,null,null,null,"Coincident",26.65,25.94,25.45,24.88,24.61,24.52,24.43]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.9,26.19,25.69,25.11,24.84,24.75,24.66]
[null,null,null,null,"Coincident",26.88,26.16,25.67,25.09,24.82,24.73,24.64]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.3,23.65,23.2,22.68,22.44,22.35,22.27]
[null,null,null,null,"Coincident",24.3,23.65,23.2,22.68,22.44,22.35,22.27]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.53,23.87,23.42,22.89,22.65,22.56,22.48]
[null,null,null,null,"Coincident",24.5,23.85,23.4,22.87,22.63,22.54,22.46]
[null,"Loganlea","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.75,17.34,17.059999999999999,16.73,16.59,16.53,16.510000000000002]
[null,null,null,null,"Coincident",16.63,16.25,15.99,15.68,15.54,15.49,15.47]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.059999999999999,17.649999999999999,17.37,17.03,16.88,16.829999999999998,16.8]
[null,null,null,null,"Coincident",16.75,16.37,16.11,15.79,15.65,15.61,15.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.09,16.690000000000001,16.420000000000002,16.11,15.96,15.91,15.89]
[null,null,null,null,"Coincident",16.010000000000002,15.64,15.39,15.09,14.95,14.91,14.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.39,16.989999999999998,16.71,16.39,16.239999999999998,16.190000000000001,16.170000000000002]
[null,null,null,null,"Coincident",16.13,15.75,15.5,15.2,15.07,15.02,15]
[null,"Lota","Substation Rating","MVA","Non-Coincident",41,41,41,41,41,41,41]
[null,null,null,null,"Coincident",41,41,41,41,41,41,41]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.08,27.75,27.62,27.29,27.23,27.38,27.53]
[null,null,null,null,"Coincident",26.94,26.63,26.5,26.18,26.13,26.26,26.41]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.21,27.88,27.75,27.42,27.36,27.5,27.66]
[null,null,null,null,"Coincident",27.03,26.71,26.58,26.26,26.21,26.35,26.5]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.81,26.5,26.37,26.06,26,26.14,26.29]
[null,null,null,null,"Coincident",25.72,25.42,25.3,25,24.94,25.08,25.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.94,26.62,26.49,26.18,26.12,26.26,26.41]
[null,null,null,null,"Coincident",25.8,25.5,25.38,25.08,25.02,25.15,25.3]
[null,"Lowood","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.11,3.03,2.98,2.93,2.9,2.9,2.89]
[null,null,null,null,"Coincident",2.81,2.74,2.69,2.64,2.62,2.61,2.61]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.16,3.08,3.03,2.97,2.95,2.95,2.94]
[null,null,null,null,"Coincident",2.83,2.76,2.71,2.66,2.64,2.63,2.63]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.83,2.76,2.71,2.66,2.64,2.64,2.63]
[null,null,null,null,"Coincident",2.5499999999999998,2.4900000000000002,2.4500000000000002,2.4,2.38,2.38,2.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.88,2.8,2.76,2.7,2.68,2.68,2.67]
[null,null,null,null,"Coincident",2.57,2.5099999999999998,2.4700000000000002,2.42,2.4,2.4,2.39]
[null,"Lytton","Substation Rating","MVA","Non-Coincident",65,65,65,65,65,65,65]
[null,null,null,null,"Coincident",65,65,65,65,65,65,65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.37,29.85,32.46,32.04,31.84,31.79,31.63]
[null,null,null,null,"Coincident",26.16,27.22,29.26,28.88,28.7,28.65,28.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.39,29.9,32.64,32.200000000000003,31.99,31.94,31.77]
[null,null,null,null,"Coincident",26.66,27.74,29.27,28.88,28.7,28.65,28.5]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.16,29.64,32.25,31.84,31.64,31.59,31.43]
[null,null,null,null,"Coincident",25.96,27.02,29.07,28.69,28.51,28.46,28.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.17,29.69,32.42,31.99,31.78,31.72,31.55]
[null,null,null,null,"Coincident",26.44,27.53,29.08,28.69,28.51,28.46,28.31]
[null,"Lytton B","Substation Rating","MVA","Non-Coincident",53,53,53,53,53,53,53]
[null,null,null,null,"Coincident",53,53,53,53,53,53,53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.89,24.73,26.13,25.73,25.5,25.34,25.16]
[null,null,null,null,"Coincident",13.16,15.76,16.7,16.45,16.309999999999999,16.2,16.09]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.44,26.56,28.07,27.65,27.4,27.23,27.03]
[null,null,null,null,"Coincident",13.47,16.2,17.190000000000001,16.940000000000001,16.79,16.690000000000001,16.57]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.260000000000002,24.1,25.51,25.13,24.91,24.75,24.58]
[null,null,null,null,"Coincident",12.76,15.36,16.309999999999999,16.07,15.93,15.83,15.72]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.76,25.9,27.41,27,26.76,26.59,26.41]
[null,null,null,null,"Coincident",13.06,15.8,16.8,16.55,16.41,16.309999999999999,16.2]
[null,"Makerston St","Substation Rating","MVA","Non-Coincident",157,157,157,157,157,157,157]
[null,null,null,null,"Coincident",157,157,157,157,157,157,157]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",61.11,60.28,59.83,61.41,61.22,61.26,61.18]
[null,null,null,null,"Coincident",54.53,53.79,53.79,55.25,55.08,55.12,55.04]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",61.15,60.31,59.86,61.45,61.26,61.3,61.22]
[null,null,null,null,"Coincident",54.54,53.8,53.88,55.25,55.08,55.12,55.04]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.27,59.45,59.01,60.6,60.41,60.45,60.37]
[null,null,null,null,"Coincident",53.78,53.05,53.05,54.52,54.35,54.39,54.32]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",60.3,59.48,59.03,60.63,60.44,60.48,60.4]
[null,null,null,null,"Coincident",53.79,53.06,53.14,54.52,54.47,54.51,54.44]
[null,"Maleny","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.87,10.9,10.94,10.92,10.89,10.95,11.08]
[null,null,null,null,"Coincident",7.7,7.62,7.59,7.52,7.53,7.6,7.68]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.88,10.91,10.95,10.93,10.9,10.96,11.09]
[null,null,null,null,"Coincident",7.71,7.62,7.6,7.52,7.53,7.6,7.68]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.68,9.6999999999999993,9.73,9.7200000000000006,9.69,9.74,9.86]
[null,null,null,null,"Coincident",7.33,7.25,7.22,7.15,7.16,7.23,7.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.69,9.7100000000000009,9.75,9.73,9.6999999999999993,9.76,9.8699999999999992]
[null,null,null,null,"Coincident",7.33,7.25,7.23,7.16,7.17,7.23,7.31]
[null,"Mango Hill Bus 1","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.93,22.72,22.65,22.54,22.69,22.97,23.23]
[null,null,null,null,"Coincident",21.89,21.69,21.63,21.51,21.66,21.93,22.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.93,22.73,22.66,22.54,22.69,22.97,23.24]
[null,null,null,null,"Coincident",21.89,21.69,21.63,21.51,21.66,21.93,22.18]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.37,21.18,21.11,21,21.14,21.41,21.65]
[null,null,null,null,"Coincident",20.399999999999999,20.22,20.16,20.05,20.190000000000001,20.440000000000001,20.67]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.37,21.18,21.12,21.01,21.15,21.41,21.66]
[null,null,null,null,"Coincident",20.399999999999999,20.22,20.16,20.05,20.190000000000001,20.440000000000001,20.67]
[null,"Mango Hill Bus 2","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.1,36.08,35.26,34.07,33.15,33.04,33.33]
[null,null,null,null,"Coincident",35.909999999999997,34.92,34.130000000000003,32.979999999999997,32.090000000000003,31.99,32.26]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.1,36.08,35.26,34.479999999999997,33.549999999999997,33.44,33.729999999999997]
[null,null,null,null,"Coincident",36.119999999999997,35.130000000000003,34.33,33.17,32.28,32.18,32.450000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.14,34.17,33.39,32.270000000000003,31.4,31.3,31.56]
[null,null,null,null,"Coincident",34.01,33.08,32.32,31.23,30.39,30.29,30.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.14,34.58,33.79,32.65,31.77,31.67,31.94]
[null,null,null,null,"Coincident",34.21,33.270000000000003,32.51,31.42,30.57,30.47,30.73]
[null,"Marburg","Substation Rating","MVA","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.27,5.45,5.65,5.87,6.13,6.43,6.71]
[null,null,null,null,"Coincident",4.91,5.08,5.27,5.47,5.72,5.99,6.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.28,5.46,5.66,5.88,6.15,6.44,6.72]
[null,null,null,null,"Coincident",4.93,5.09,5.28,5.48,5.73,6.01,6.27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.88,5.04,5.23,5.43,5.68,5.95,6.21]
[null,null,null,null,"Coincident",4.55,4.7,4.87,5.0599999999999996,5.29,5.55,5.79]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.8899999999999997,5.05,5.24,5.44,5.69,5.96,6.22]
[null,null,null,null,"Coincident",4.5599999999999996,4.71,4.8899999999999997,5.07,5.3,5.56,5.8]
[null,"McLachlan St","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.56,51.75,51.25,50.45,50.25,50.3,50.43]
[null,null,null,null,"Coincident",48.54,47.79,47.33,46.59,46.4,46.46,46.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.73,51.91,51.4,50.59,50.39,50.45,50.57]
[null,null,null,null,"Coincident",48.56,47.8,47.34,46.6,46.41,46.47,46.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.01,50.22,49.73,48.96,48.76,48.82,48.94]
[null,null,null,null,"Coincident",47.11,46.38,45.93,45.21,45.03,45.09,45.2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.16,50.36,49.87,49.09,48.89,48.95,49.07]
[null,null,null,null,"Coincident",47.12,46.39,45.94,45.22,45.04,45.09,45.21]
[null,"Meeandah","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.37,25.7,25.5,25.19,25.07,25.04,25.39]
[null,null,null,null,"Coincident",15.88,18.95,18.809999999999999,18.57,18.489999999999998,18.46,18.73]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.82,25.71,25.52,25.2,25.08,25.05,25.4]
[null,null,null,null,"Coincident",15.89,19.100000000000001,18.95,18.71,18.62,18.59,18.87]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.85,25.18,24.99,24.68,24.57,24.54,24.88]
[null,null,null,null,"Coincident",15.49,18.57,18.43,18.2,18.12,18.09,18.350000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.26,25.19,25,24.69,24.58,24.54,24.89]
[null,null,null,null,"Coincident",15.5,18.71,18.559999999999999,18.32,18.239999999999998,18.21,18.48]
[null,"Merrimac","Substation Rating","MVA","Non-Coincident",67,67,67,67,67,67,67]
[null,null,null,null,"Coincident",67,67,67,67,67,67,67]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.75,29.28,29.02,28.69,28.67,28.85,29.04]
[null,null,null,null,"Coincident",29.75,29.28,29.02,28.69,28.67,28.85,29.04]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.87,29.4,29.14,28.81,28.79,28.98,29.17]
[null,null,null,null,"Coincident",29.84,29.37,29.12,28.79,28.77,28.95,29.14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.77,27.33,27.1,26.79,26.77,26.94,27.12]
[null,null,null,null,"Coincident",27.77,27.33,27.1,26.79,26.77,26.94,27.12]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.89,27.45,27.21,26.9,26.88,27.05,27.23]
[null,null,null,null,"Coincident",27.86,27.42,27.18,26.88,26.86,27.03,27.2]
[null,"Miami","Substation Rating","MVA","Non-Coincident",45,45,45,45,51,51,51]
[null,null,null,null,"Coincident",45,45,45,45,51,51,51]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.36,27.51,27.84,28.11,28.67,29.43,30.22]
[null,null,null,null,"Coincident",24.35,24.48,24.78,25.02,25.51,26.19,26.9]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.45,27.6,27.94,28.21,28.76,29.53,30.33]
[null,null,null,null,"Coincident",24.38,24.52,24.81,25.05,25.55,26.23,26.94]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.17,25.31,25.62,25.87,26.38,27.08,27.81]
[null,null,null,null,"Coincident",22.4,22.53,22.8,23.02,23.47,24.1,24.75]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.26,25.4,25.71,25.96,26.47,27.17,27.91]
[null,null,null,null,"Coincident",22.43,22.56,22.83,23.05,23.51,24.13,24.78]
[null,"Milton","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.159999999999997,41.23,40.67,39.86,39.409999999999997,39.18,38.97]
[null,null,null,null,"Coincident",36.11,37.03,36.520000000000003,35.79,35.380000000000003,35.18,34.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.159999999999997,41.25,40.68,39.869999999999997,39.409999999999997,39.19,38.97]
[null,null,null,null,"Coincident",36.14,37.08,36.57,35.840000000000003,35.43,35.229999999999997,35.03]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.01,40.11,39.56,38.78,38.33,38.119999999999997,37.909999999999997]
[null,null,null,null,"Coincident",35.08,36.020000000000003,35.520000000000003,34.82,34.42,34.22,34.03]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.01,40.119999999999997,39.57,38.78,38.340000000000003,38.119999999999997,37.909999999999997]
[null,null,null,null,"Coincident",35.11,36.07,35.57,34.86,34.46,34.26,34.07]
[null,"Moggill","Substation Rating","MVA","Non-Coincident",34,34,34,34,34,34,34]
[null,null,null,null,"Coincident",34,34,34,34,34,34,34]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.65,20.23,19.98,19.64,19.5,19.52,19.59]
[null,null,null,null,"Coincident",19.760000000000002,19.36,19.11,18.78,18.649999999999999,18.68,18.739999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.72,20.3,20.04,19.7,19.559999999999999,19.579999999999998,19.649999999999999]
[null,null,null,null,"Coincident",19.78,19.38,19.14,18.809999999999999,18.670000000000002,18.7,18.760000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.45,18.079999999999998,17.850000000000001,17.55,17.420000000000002,17.45,17.5]
[null,null,null,null,"Coincident",17.649999999999999,17.3,17.079999999999998,16.78,16.66,16.690000000000001,16.739999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.510000000000002,18.14,17.91,17.600000000000001,17.47,17.5,17.559999999999999]
[null,null,null,null,"Coincident",17.68,17.32,17.100000000000001,16.809999999999999,16.690000000000001,16.71,16.77]
[null,"Molendinar","Substation Rating","MVA","Non-Coincident",65,65,65,65,65,65,65]
[null,null,null,null,"Coincident",65,65,65,65,65,65,65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.31,42.23,41.52,40.94,40.799999999999997,40.9,41.05]
[null,null,null,null,"Coincident",41.89,40.85,40.159999999999997,39.61,39.47,39.56,39.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.45,42.36,41.64,41.06,40.909999999999997,41.01,41.16]
[null,null,null,null,"Coincident",41.9,40.85,40.520000000000003,39.96,39.82,39.92,40.07]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.270000000000003,39.26,38.6,38.07,37.94,38.03,38.17]
[null,null,null,null,"Coincident",38.950000000000003,37.979999999999997,37.340000000000003,36.83,36.700000000000003,36.78,36.92]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.369999999999997,39.36,38.69,38.15,38.01,38.1,38.25]
[null,null,null,null,"Coincident",39.299999999999997,38.32,37.68,37.159999999999997,37.03,37.11,37.25]
[null,"Mooloolaba","Substation Rating","MVA","Non-Coincident",70,70,70,70,70,70,70]
[null,null,null,null,"Coincident",70,70,70,70,70,70,70]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.06,45.98,46.21,46.23,46.64,47.33,48]
[null,null,null,null,"Coincident",41.72,41.65,41.85,41.87,42.24,42.86,43.47]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.07,45.99,46.22,46.24,46.65,47.34,48.01]
[null,null,null,null,"Coincident",41.72,41.65,41.85,41.87,42.24,42.87,43.47]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.950000000000003,40.880000000000003,41.07,41.09,41.46,42.07,42.67]
[null,null,null,null,"Coincident",37.090000000000003,37.020000000000003,37.200000000000003,37.22,37.549999999999997,38.1,38.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.96,40.89,41.08,41.1,41.47,42.08,42.68]
[null,null,null,null,"Coincident",37.090000000000003,37.020000000000003,37.200000000000003,37.22,37.549999999999997,38.1,38.64]
[null,"Moorooka","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.53,19.36,19.329999999999998,19.18,19.23,19.440000000000001,19.71]
[null,null,null,null,"Coincident",17.350000000000001,17.2,17.170000000000002,17.03,17.079999999999998,17.27,17.510000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.73,19.559999999999999,19.52,19.37,19.43,19.64,19.91]
[null,null,null,null,"Coincident",17.37,17.22,17.2,17.059999999999999,17.11,17.3,17.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.64,17.489999999999998,17.46,17.329999999999998,17.37,17.559999999999999,17.8]
[null,null,null,null,"Coincident",15.67,15.53,15.51,15.39,15.43,15.6,15.81]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.82,17.670000000000002,17.64,17.5,17.55,17.739999999999998,17.989999999999998]
[null,null,null,null,"Coincident",15.7,15.56,15.54,15.42,15.46,15.63,15.84]
[null,"Morayfield","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",48,48,48,48,48,48,48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.520000000000003,35.1,34.869999999999997,34.61,34.57,34.68,34.75]
[null,null,null,null,"Coincident",35.520000000000003,35.1,34.869999999999997,34.61,34.57,34.68,34.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.67,35.25,35.020000000000003,34.75,34.72,34.82,34.9]
[null,null,null,null,"Coincident",35.65,35.229999999999997,35,34.729999999999997,34.700000000000003,34.81,34.880000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.68,33.270000000000003,33.06,32.799999999999997,32.78,32.880000000000003,32.94]
[null,null,null,null,"Coincident",33.68,33.270000000000003,33.06,32.799999999999997,32.78,32.880000000000003,32.94]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.82,33.409999999999997,33.19,32.94,32.909999999999997,33.01,33.08]
[null,null,null,null,"Coincident",33.799999999999997,33.4,33.18,32.93,32.9,33,33.06]
[null,"Morayfield North","Substation Rating","MVA","Non-Coincident",54,54,54,54,54,54,54]
[null,null,null,null,"Coincident",54,54,54,54,54,54,54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.25,30.11,29.8,29.43,29.33,29.39,29.45]
[null,null,null,null,"Coincident",31.25,30.11,29.8,29.43,29.33,29.39,29.45]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.44,30.29,29.98,29.61,29.51,29.57,29.62]
[null,null,null,null,"Coincident",31.35,30.21,29.9,29.53,29.42,29.48,29.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.49,28.42,28.12,27.78,27.68,27.73,27.79]
[null,null,null,null,"Coincident",29.49,28.42,28.12,27.78,27.68,27.73,27.79]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.66,28.59,28.29,27.94,27.84,27.9,27.96]
[null,null,null,null,"Coincident",29.58,28.5,28.21,27.86,27.77,27.82,27.88]
[null,"Mt Cotton","Substation Rating","MVA","Non-Coincident",16,16,16,16,16,16,16]
[null,null,null,null,"Coincident",16,16,16,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.4700000000000006,9.26,9.1199999999999992,8.94,8.84,8.8000000000000007,8.74]
[null,null,null,null,"Coincident",7.77,7.6,7.49,7.34,7.26,7.22,7.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.52,9.31,9.17,8.99,8.89,8.85,8.7899999999999991]
[null,null,null,null,"Coincident",7.77,7.6,7.49,7.34,7.26,7.23,7.18]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.89,8.69,8.57,8.4,8.31,8.27,8.2100000000000009]
[null,null,null,null,"Coincident",7.3,7.14,7.03,6.89,6.82,6.79,6.74]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.94,8.74,8.61,8.44,8.35,8.31,8.26]
[null,null,null,null,"Coincident",7.3,7.14,7.03,6.89,6.82,6.79,6.74]
[null,"Mt Crosby West","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.52,16.25,16.100000000000001,15.88,15.79,15.81,15.79]
[null,null,null,null,"Coincident",14.1,13.87,13.75,13.56,13.48,13.49,13.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.89,16.61,16.46,16.23,16.149999999999999,16.16,16.14]
[null,null,null,null,"Coincident",14.29,14.05,13.93,13.74,13.66,13.68,13.66]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.45,14.22,14.09,13.89,13.82,13.83,13.82]
[null,null,null,null,"Coincident",12.34,12.14,12.03,11.86,11.8,11.81,11.79]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.78,14.53,14.4,14.2,14.13,14.14,14.12]
[null,null,null,null,"Coincident",12.5,12.3,12.19,12.02,11.96,11.97,11.95]
[null,"Mt Gravatt","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.22,28.77,28.54,28.33,28.46,28.76,29.05]
[null,null,null,null,"Coincident",29.22,28.77,28.54,28.33,28.46,28.76,29.05]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.43,28.98,28.75,28.54,28.66,28.97,29.26]
[null,null,null,null,"Coincident",29.28,28.83,28.6,28.39,28.52,28.82,29.11]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.81,27.38,27.16,26.96,27.08,27.37,27.65]
[null,null,null,null,"Coincident",27.81,27.38,27.16,26.96,27.08,27.37,27.65]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.01,27.58,27.36,27.16,27.28,27.57,27.85]
[null,null,null,null,"Coincident",27.87,27.44,27.22,27.02,27.14,27.43,27.71]
[null,"Mt Sylvia","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.19,1.17,1.1599999999999999,1.1399999999999999,1.1299999999999999,1.1299999999999999,1.1299999999999999]
[null,null,null,null,"Coincident",1.02,1,0.99,0.98,0.97,0.97,0.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3,1.27,1.26,1.24,1.23,1.23,1.23]
[null,null,null,null,"Coincident",1.08,1.06,1.05,1.04,1.03,1.03,1.03]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1299999999999999,1.1100000000000001,1.1000000000000001,1.08,1.07,1.07,1.07]
[null,null,null,null,"Coincident",0.97,0.95,0.94,0.93,0.92,0.92,0.92]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.23,1.21,1.2,1.18,1.17,1.17,1.17]
[null,null,null,null,"Coincident",1.03,1.01,1,0.99,0.98,0.98,0.98]
[null,"Mt Tamborine Bus 1","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.199999999999999,10.199999999999999,10.210000000000001,10.16,10.1,10.130000000000001,10.220000000000001]
[null,null,null,null,"Coincident",8.68,8.5500000000000007,8.5,8.41,8.4,8.4499999999999993,8.52]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.210000000000001,10.220000000000001,10.220000000000001,10.18,10.119999999999999,10.15,10.24]
[null,null,null,null,"Coincident",8.7200000000000006,8.58,8.5399999999999991,8.44,8.43,8.49,8.5500000000000007]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.44,9.44,9.4499999999999993,9.41,9.35,9.3800000000000008,9.4600000000000009]
[null,null,null,null,"Coincident",7.88,7.76,7.72,7.64,7.63,7.68,7.74]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.4499999999999993,9.4499999999999993,9.4600000000000009,9.42,9.36,9.39,9.48]
[null,null,null,null,"Coincident",7.92,7.8,7.76,7.67,7.66,7.71,7.77]
[null,"Mt Tamborine Bus 2","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.19,10.19,10.199999999999999,10.16,10.11,10.14,10.23]
[null,null,null,null,"Coincident",8.1300000000000008,8,7.96,7.87,7.86,7.92,7.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.220000000000001,10.220000000000001,10.220000000000001,10.18,10.130000000000001,10.16,10.25]
[null,null,null,null,"Coincident",8.18,8.0500000000000007,8.01,7.92,7.91,7.97,8.0399999999999991]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.75,9.75,9.76,9.7200000000000006,9.67,9.6999999999999993,9.7899999999999991]
[null,null,null,null,"Coincident",7.63,7.51,7.48,7.4,7.39,7.44,7.51]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7799999999999994,9.77,9.7799999999999994,9.74,9.69,9.7200000000000006,9.81]
[null,null,null,null,"Coincident",7.68,7.56,7.53,7.44,7.44,7.49,7.55]
[null,"Mudgeeraba West Pkg","Substation Rating","MVA","Non-Coincident",45,45,45,45,45,45,45]
[null,null,null,null,"Coincident",45,45,45,45,45,45,45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.26,23.98,23.9,23.64,23.61,23.83,24.08]
[null,null,null,null,"Coincident",24.26,23.98,23.9,23.64,23.61,23.83,24.08]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.3,24.02,23.94,23.68,23.65,23.87,24.12]
[null,null,null,null,"Coincident",24.28,24,23.91,23.65,23.63,23.85,24.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.56,22.31,22.22,21.98,21.96,22.16,22.39]
[null,null,null,null,"Coincident",22.56,22.31,22.22,21.98,21.96,22.16,22.39]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.6,22.34,22.26,22.02,21.99,22.2,22.43]
[null,null,null,null,"Coincident",22.58,22.32,22.24,22,21.97,22.18,22.41]
[null,"Murarrie","Substation Rating","MVA","Non-Coincident",51,51,51,51,51,51,51]
[null,null,null,null,"Coincident",51,51,51,51,51,51,51]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.69,22.41,22.27,21.92,21.79,21.77,21.74]
[null,null,null,null,"Coincident",19.12,18.89,18.760000000000002,18.47,18.36,18.350000000000001,18.32]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.71,22.43,22.28,21.93,21.8,21.78,21.75]
[null,null,null,null,"Coincident",19.489999999999998,19.25,19.13,18.829999999999998,18.71,18.7,18.670000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.52,21.26,21.12,20.79,20.66,20.65,20.62]
[null,null,null,null,"Coincident",18.13,17.91,17.79,17.510000000000002,17.41,17.399999999999999,17.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.53,21.26,21.12,20.79,20.67,20.65,20.62]
[null,null,null,null,"Coincident",18.48,18.25,18.14,17.850000000000001,17.75,17.73,17.7]
[null,"Murrumba","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.78,1.77,1.77,1.7,1.7,1.73,1.75]
[null,null,null,null,"Coincident",0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.88,1.87,1.87,1.8,1.81,1.83,1.86]
[null,null,null,null,"Coincident",0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.65,1.65,1.65,1.65,1.66,1.68,1.71]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.75,1.74,1.74,1.76,1.76,1.79,1.82]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,"Myrtletown","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.36,17.25,17.28,17.2,17.27,17.440000000000001,17.559999999999999]
[null,null,null,null,"Coincident",13.38,13.29,13.31,13.25,13.31,13.44,13.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.37,17.260000000000002,17.29,17.21,17.28,17.45,17.579999999999998]
[null,null,null,null,"Coincident",13.4,13.31,13.33,13.27,13.33,13.46,13.56]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.68,16.57,16.600000000000001,16.52,16.59,16.75,16.87]
[null,null,null,null,"Coincident",12.85,12.76,12.79,12.73,12.78,12.91,13]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.68,16.57,16.600000000000001,16.53,16.600000000000001,16.760000000000002,16.88]
[null,null,null,null,"Coincident",12.86,12.77,12.8,12.74,12.79,12.92,13.01]
[null,"Nambour","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.799999999999997,36.29,36.03,35.549999999999997,35.479999999999997,35.61,35.28]
[null,null,null,null,"Coincident",33.86,33.39,33.159999999999997,32.72,32.65,32.770000000000003,32.9]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.1,36.590000000000003,36.33,35.85,35.770000000000003,35.9,35.380000000000003]
[null,null,null,null,"Coincident",34.08,33.61,33.369999999999997,32.93,32.86,32.979999999999997,33.11]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.880000000000003,34.4,34.15,33.700000000000003,33.630000000000003,33.75,33.89]
[null,null,null,null,"Coincident",32.1,31.65,31.43,31.01,30.95,31.06,31.18]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.17,34.68,34.44,33.979999999999997,33.909999999999997,34.03,33.99]
[null,null,null,null,"Coincident",32.299999999999997,31.86,31.63,31.21,31.15,31.26,31.39]
[null,"Narangba","Substation Rating","MVA","Non-Coincident",47,47,47,47,47,47,47]
[null,null,null,null,"Coincident",47,47,47,47,47,47,47]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.68,28.68,28.92,29.19,29.73,30.43,31.08]
[null,null,null,null,"Coincident",28.59,28.6,28.84,29.1,29.64,30.34,30.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.73,28.74,28.98,29.25,29.79,30.49,31.14]
[null,null,null,null,"Coincident",28.65,28.66,28.9,29.17,29.7,30.4,31.06]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.04,27.05,27.27,27.53,28.03,28.69,29.31]
[null,null,null,null,"Coincident",26.96,26.97,27.19,27.44,27.95,28.6,29.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.09,27.1,27.33,27.58,28.09,28.75,29.37]
[null,null,null,null,"Coincident",27.02,27.03,27.25,27.5,28.01,28.67,29.28]
[null,"Nerang","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.57,53.57,53.23,52.59,52.48,52.71,52.97]
[null,null,null,null,"Coincident",54.57,53.57,53.23,52.59,52.48,52.71,52.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.57,53.57,53.23,52.59,52.48,52.71,52.97]
[null,null,null,null,"Coincident",54.78,53.78,53.43,52.79,52.68,52.91,53.17]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.51,49.59,49.27,48.68,48.58,48.79,49.03]
[null,null,null,null,"Coincident",50.51,49.59,49.27,48.68,48.58,48.79,49.03]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",50.79,49.87,49.55,48.95,48.85,49.06,49.3]
[null,null,null,null,"Coincident",50.7,49.78,49.46,48.86,48.76,48.97,49.22]
[null,"Newmarket","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.37,23.91,23.67,23.3,23.18,23.25,23.48]
[null,null,null,null,"Coincident",23.27,22.83,22.6,22.25,22.14,22.2,22.42]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.55,24.08,23.84,23.47,23.35,23.41,23.65]
[null,null,null,null,"Coincident",23.34,22.9,22.66,22.31,22.2,22.26,22.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.05,22.62,22.39,22.04,21.93,21.99,22.21]
[null,null,null,null,"Coincident",22.01,21.6,21.38,21.05,20.94,21,21.21]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.22,22.78,22.55,22.2,22.09,22.15,22.37]
[null,null,null,null,"Coincident",22.08,21.66,21.44,21.11,21,21.06,21.27]
[null,"Newstead","Substation Rating","MVA","Non-Coincident",131,131,131,131,131,131,131]
[null,null,null,null,"Coincident",131,131,131,131,131,131,131]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.05,51.13,53.5,52.93,52.85,52.98,53.13]
[null,null,null,null,"Coincident",44.9,45.05,47.21,46.7,46.64,46.75,46.88]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.17,51.26,53.65,53.07,52.99,53.12,53.28]
[null,null,null,null,"Coincident",44.91,45.06,47.24,46.73,46.66,46.78,46.91]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.07,49.17,51.55,51,50.93,51.05,51.2]
[null,null,null,null,"Coincident",43.17,43.33,45.5,45.02,44.96,45.06,45.19]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.17,49.28,51.68,51.13,51.05,51.18,51.32]
[null,null,null,null,"Coincident",43.18,43.34,45.53,45.04,44.98,45.09,45.21]
[null,"Ningi","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.37,11.24,11.19,11.07,11.04,11.08,11.1]
[null,null,null,null,"Coincident",10.37,10.25,10.199999999999999,10.09,10.07,10.11,10.119999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.44,11.31,11.26,11.14,11.11,11.15,11.17]
[null,null,null,null,"Coincident",10.41,10.29,10.25,10.130000000000001,10.11,10.15,10.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.69,10.57,10.52,10.4,10.38,10.42,10.43]
[null,null,null,null,"Coincident",9.75,9.64,9.59,9.49,9.4700000000000006,9.5,9.51]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.76,10.63,10.58,10.47,10.45,10.48,10.5]
[null,null,null,null,"Coincident",9.7899999999999991,9.68,9.6300000000000008,9.5299999999999994,9.51,9.5399999999999991,9.5500000000000007]
[null,"Noosaville","Substation Rating","MVA","Non-Coincident",115,115,115,115,115,115,115]
[null,null,null,null,"Coincident",115,115,115,115,115,115,115]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.64,37.33,37.29,37.01,37.130000000000003,37.549999999999997,38.090000000000003]
[null,null,null,null,"Coincident",36.619999999999997,36.32,36.28,36.01,36.119999999999997,36.54,37.06]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.64,37.33,37.29,37.01,37.130000000000003,37.549999999999997,38.090000000000003]
[null,null,null,null,"Coincident",36.65,36.35,36.31,36.04,36.159999999999997,36.57,37.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.94,35.65,35.6,35.33,35.450000000000003,35.86,36.369999999999997]
[null,null,null,null,"Coincident",34.97,34.68,34.64,34.380000000000003,34.49,34.89,35.39]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.04,35.74,35.700000000000003,35.43,35.549999999999997,35.950000000000003,36.47]
[null,null,null,null,"Coincident",35,34.71,34.67,34.409999999999997,34.520000000000003,34.92,35.42]
[null,"North Maclean","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.96,38.67,38.619999999999997,38.99,39.590000000000003,40.36,41.02]
[null,null,null,null,"Coincident",35.43,35.17,35.119999999999997,35.450000000000003,36,36.700000000000003,37.31]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.06,38.76,38.71,39.090000000000003,39.700000000000003,40.49,41.17]
[null,null,null,null,"Coincident",47,46.65,46.58,47.03,47.75,48.69,49.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.61,34.35,34.299999999999997,34.630000000000003,35.159999999999997,35.85,36.44]
[null,null,null,null,"Coincident",31.47,31.23,31.19,31.49,31.98,32.6,33.130000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.630000000000003,34.369999999999997,34.32,34.65,35.19,35.89,36.49]
[null,null,null,null,"Coincident",41.72,41.41,41.35,41.74,42.39,43.22,43.92]
[null,"North Springwood","Substation Rating","MVA","Non-Coincident",135,135,135,135,135,135,135]
[null,null,null,null,"Coincident",135,135,135,135,135,135,135]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.05,49.98,49.3,48.37,47.98,47.93,47.94]
[null,null,null,null,"Coincident",49.72,48.67,48.02,47.11,46.73,46.68,46.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.05,49.98,49.37,48.43,48.04,47.99,48.01]
[null,null,null,null,"Coincident",49.73,48.68,48.02,47.11,46.73,46.68,46.7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.7,44.73,44.13,43.29,42.95,42.9,42.92]
[null,null,null,null,"Coincident",44.51,43.57,42.98,42.17,41.83,41.78,41.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.75,44.78,44.17,43.33,42.98,42.93,42.95]
[null,null,null,null,"Coincident",44.51,43.65,43.05,42.24,41.9,41.85,41.87]
[null,"Nth Ipswich","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.75,23.49,23.41,23.13,23.08,23.14,23.18]
[null,null,null,null,"Coincident",23.01,22.76,22.68,22.41,22.36,22.42,22.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.02,23.77,23.68,23.4,23.34,23.41,23.45]
[null,null,null,null,"Coincident",23.17,22.93,22.85,22.57,22.52,22.58,22.62]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.23,22,21.92,21.66,21.61,21.67,21.7]
[null,null,null,null,"Coincident",21.54,21.31,21.24,20.98,20.94,21,21.03]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.49,22.25,22.18,21.91,21.86,21.92,21.95]
[null,null,null,null,"Coincident",21.7,21.47,21.39,21.13,21.09,21.15,21.18]
[null,"Nth Pine Dam","Substation Rating","MVA","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.4,0.39,0.39,0.38,0.38,0.38,0.38]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.4,0.4,0.4,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.39,0.38,0.38,0.38,0.37,0.37,0.37]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.39,0.39,0.39,0.38,0.38,0.38,0.39]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Nudgee","Substation Rating","MVA","Non-Coincident",53,53,53,53,53,53,53]
[null,null,null,null,"Coincident",53,53,53,53,53,53,53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.74,24.2,23.84,23.34,23.11,23.07,23.15]
[null,null,null,null,"Coincident",15.29,14.96,14.73,14.43,14.28,14.26,14.31]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.75,24.2,23.84,23.34,23.11,23.07,23.15]
[null,null,null,null,"Coincident",15.41,15.07,14.85,14.54,14.39,14.37,14.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.24,22.74,22.4,21.93,21.71,21.67,21.75]
[null,null,null,null,"Coincident",14.37,14.05,13.84,13.55,13.42,13.39,13.44]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.24,22.74,22.55,22.07,21.85,21.81,21.89]
[null,null,null,null,"Coincident",14.48,14.16,13.95,13.66,13.52,13.5,13.55]
[null,"Nundah","Substation Rating","MVA","Non-Coincident",44,44,44,44,44,44,44]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.52,24.25,24.14,23.9,23.9,24.06,24.24]
[null,null,null,null,"Coincident",23.66,23.4,23.3,23.06,23.06,23.22,23.39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.64,24.37,24.26,24.02,24.02,24.18,24.36]
[null,null,null,null,"Coincident",23.7,23.44,23.34,23.1,23.1,23.26,23.43]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.68,22.42,22.33,22.1,22.1,22.25,22.42]
[null,null,null,null,"Coincident",21.88,21.64,21.55,21.33,21.33,21.47,21.63]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.79,22.54,22.44,22.21,22.21,22.36,22.53]
[null,null,null,null,"Coincident",21.92,21.68,21.58,21.37,21.36,21.51,21.67]
[null,"Oxley","Substation Rating","MVA","Non-Coincident",31,31,31,31,31,31,31]
[null,null,null,null,"Coincident",31,31,31,31,31,31,31]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.190000000000001,23.95,23.66,23.3,23.22,23.24,23.28]
[null,null,null,null,"Coincident",17.829999999999998,21.32,21.07,20.75,20.67,20.69,20.72]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.51,24.33,24.04,23.67,23.59,23.61,23.65]
[null,null,null,null,"Coincident",17.96,21.59,21.33,21.02,20.94,20.96,20.99]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.64,22.43,22.17,21.84,21.76,21.78,21.81]
[null,null,null,null,"Coincident",16.46,19.98,19.75,19.46,19.39,19.41,19.440000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.940000000000001,22.79,22.52,22.19,22.11,22.13,22.16]
[null,null,null,null,"Coincident",16.579999999999998,20.239999999999998,20.010000000000002,19.72,19.64,19.66,19.690000000000001]
[null,"Palm Beach","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.2,21.13,21.24,21.24,21.2,21.35,21.65]
[null,null,null,null,"Coincident",20.83,20.65,20.61,20.440000000000001,20.48,20.68,20.9]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.25,21.14,21.25,21.25,21.21,21.36,21.66]
[null,null,null,null,"Coincident",20.85,20.67,20.64,20.47,20.51,20.7,20.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.04,20.100000000000001,20.2,20.21,20.170000000000002,20.309999999999999,20.59]
[null,null,null,null,"Coincident",19.690000000000001,19.52,19.48,19.32,19.36,19.55,19.760000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.079999999999998,20.12,20.22,20.22,20.18,20.32,20.61]
[null,null,null,null,"Coincident",19.71,19.54,19.510000000000002,19.34,19.38,19.57,19.78]
[null,"Palmwoods Central","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.2,26,25.97,25.8,25.87,26.1,26.32]
[null,null,null,null,"Coincident",24.27,24.08,24.06,23.9,23.96,24.17,24.38]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.44,26.23,26.21,26.04,26.1,26.34,26.56]
[null,null,null,null,"Coincident",24.37,24.18,24.16,24,24.06,24.28,24.49]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.65,23.46,23.44,23.29,23.35,23.56,23.76]
[null,null,null,null,"Coincident",21.9,21.73,21.71,21.57,21.62,21.82,22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.86,23.68,23.65,23.5,23.56,23.77,23.97]
[null,null,null,null,"Coincident",22,21.83,21.81,21.66,21.72,21.91,22.1]
[null,"Parkwood","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.62,19.3,20.149999999999999,19.86,19.71,19.68,19.579999999999998]
[null,null,null,null,"Coincident",16.47,18.149999999999999,18.86,18.579999999999998,18.45,18.41,18.329999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.829999999999998,19.52,20.39,20.09,19.940000000000001,19.91,19.809999999999999]
[null,null,null,null,"Coincident",16.600000000000001,18.36,19.100000000000001,18.82,18.690000000000001,18.649999999999999,18.559999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.47,18.170000000000002,19.03,18.760000000000002,18.62,18.59,18.5]
[null,null,null,null,"Coincident",15.39,17.09,17.809999999999999,17.55,17.43,17.399999999999999,17.309999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.66,18.38,19.25,18.98,18.84,18.809999999999999,18.72]
[null,null,null,null,"Coincident",15.52,17.29,18.04,17.79,17.66,17.63,17.54]
[null,"Peregian","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.27,14.16,14.16,13.98,13.98,14.07,14.17]
[null,null,null,null,"Coincident",10.86,10.79,10.78,10.65,10.64,10.72,10.79]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.27,14.17,14.16,13.99,13.98,14.08,14.18]
[null,null,null,null,"Coincident",10.88,10.8,10.8,10.66,10.66,10.73,10.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.71,12.62,12.61,12.46,12.45,12.54,12.63]
[null,null,null,null,"Coincident",9.68,9.61,9.61,9.49,9.48,9.5500000000000007,9.6199999999999992]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.72,12.62,12.62,12.46,12.46,12.54,12.63]
[null,null,null,null,"Coincident",9.69,9.6199999999999992,9.6199999999999992,9.5,9.5,9.56,9.6300000000000008]
[null,"Pimpama East","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.42,48.56,49.13,49.9,51.08,52.71,54.37]
[null,null,null,null,"Coincident",44.42,48.56,49.13,49.9,51.08,52.71,54.37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.43,48.58,49.14,49.91,51.09,52.72,54.39]
[null,null,null,null,"Coincident",44.42,48.57,49.13,49.91,51.09,52.72,54.38]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.02,45.15,45.68,46.4,47.49,49.01,50.55]
[null,null,null,null,"Coincident",41.02,45.15,45.68,46.4,47.49,49.01,50.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.03,45.17,45.69,46.41,47.5,49.02,50.57]
[null,null,null,null,"Coincident",41.02,45.16,45.68,46.41,47.5,49.02,50.56]
[null,"Postmans Ridge","Substation Rating","MVA","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.7,6.62,6.58,6.5,6.49,6.51,6.51]
[null,null,null,null,"Coincident",4.8499999999999996,4.79,4.76,4.71,4.6900000000000004,4.71,4.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.72,6.63,6.59,6.52,6.5,6.52,6.53]
[null,null,null,null,"Coincident",4.8499999999999996,4.79,4.76,4.71,4.6900000000000004,4.71,4.71]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.9,5.82,5.79,5.72,5.71,5.72,5.73]
[null,null,null,null,"Coincident",4.26,4.21,4.1900000000000004,4.1399999999999997,4.13,4.1399999999999997,4.1399999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.91,5.83,5.8,5.73,5.72,5.74,5.74]
[null,null,null,null,"Coincident",4.2699999999999996,4.21,4.1900000000000004,4.1399999999999997,4.13,4.1399999999999997,4.1399999999999997]
[null,"Queensport","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.17,28.71,28.42,27.93,27.85,27.99,28.16]
[null,null,null,null,"Coincident",27.69,27.25,26.98,26.52,26.44,26.58,26.73]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.61,29.14,28.85,28.35,28.27,28.41,28.58]
[null,null,null,null,"Coincident",28.24,27.79,27.51,27.04,26.96,27.1,27.25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.9,27.46,27.19,26.72,26.64,26.78,26.93]
[null,null,null,null,"Coincident",26.49,26.07,25.81,25.37,25.29,25.42,25.57]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.32,27.87,27.6,27.12,27.04,27.18,27.34]
[null,null,null,null,"Coincident",27.01,26.58,26.32,25.87,25.79,25.92,26.07]
[null,"Raby Bay","Substation Rating","MVA","Non-Coincident",51,51,51,51,51,51,58]
[null,null,null,null,"Coincident",51,51,51,51,51,51,58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.77,30.52,30.49,30.22,30.28,30.57,30.88]
[null,null,null,null,"Coincident",30.63,30.38,30.35,30.08,30.14,30.44,30.74]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.84,30.59,30.56,30.29,30.35,30.65,30.95]
[null,null,null,null,"Coincident",30.71,30.46,30.43,30.16,30.22,30.52,30.82]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.88,28.65,28.62,28.37,28.43,28.7,28.99]
[null,null,null,null,"Coincident",28.75,28.52,28.49,28.24,28.3,28.57,28.86]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.95,28.72,28.69,28.44,28.5,28.77,29.06]
[null,null,null,null,"Coincident",28.83,28.6,28.57,28.31,28.37,28.65,28.93]
[null,"Redbank","Substation Rating","MVA","Non-Coincident",43,43,43,43,43,43,43]
[null,null,null,null,"Coincident",43,43,43,43,43,43,43]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.88,18.78,18.829999999999998,18.77,18.95,19.37,19.829999999999998]
[null,null,null,null,"Coincident",16.98,17.89,17.95,17.89,18.059999999999999,18.46,18.899999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.16,19.07,19.12,19.059999999999999,19.239999999999998,19.670000000000002,20.14]
[null,null,null,null,"Coincident",17.12,18.059999999999999,18.11,18.05,18.22,18.63,19.07]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.93,17.829999999999998,17.89,17.829999999999998,17.989999999999998,18.39,18.829999999999998]
[null,null,null,null,"Coincident",16.079999999999998,17,17.05,16.989999999999998,17.149999999999999,17.53,17.940000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.190000000000001,18.11,18.16,18.100000000000001,18.27,18.68,19.12]
[null,null,null,null,"Coincident",16.21,17.149999999999999,17.21,17.149999999999999,17.309999999999999,17.690000000000001,18.11]
[null,"Redbank Plains","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.75,37.950000000000003,38.14,38.39,39.24,40.49,41.75]
[null,null,null,null,"Coincident",27.2,28.1,28.24,28.42,29.05,29.97,30.91]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.81,38.020000000000003,38.21,38.450000000000003,39.31,40.56,41.83]
[null,null,null,null,"Coincident",27.26,28.16,28.3,28.48,29.11,30.03,30.97]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.200000000000003,35.409999999999997,35.58,35.81,36.61,37.770000000000003,38.950000000000003]
[null,null,null,null,"Coincident",25.32,26.21,26.34,26.51,27.1,27.96,28.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.26,35.47,35.65,35.869999999999997,36.67,37.840000000000003,39.020000000000003]
[null,null,null,null,"Coincident",25.37,26.27,26.4,26.57,27.16,28.02,28.9]
[null,"Redcliffe","Substation Rating","MVA","Non-Coincident",31,31,31,31,31,31,31]
[null,null,null,null,"Coincident",31,31,31,31,31,31,31]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.100000000000001,19.920000000000002,19.89,23.36,27.04,27.23,27.41]
[null,null,null,null,"Coincident",18.61,18.440000000000001,18.41,21.54,24.85,25.02,25.19]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.329999999999998,20.149999999999999,20.12,23.64,27.36,27.55,27.73]
[null,null,null,null,"Coincident",18.809999999999999,18.64,18.61,21.86,25.31,25.48,25.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.059999999999999,18.89,18.86,22.35,26.02,26.2,26.37]
[null,null,null,null,"Coincident",17.649999999999999,17.489999999999998,17.47,20.59,23.9,24.06,24.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.29,19.11,19.079999999999998,22.61,26.33,26.51,26.68]
[null,null,null,null,"Coincident",17.84,17.68,17.649999999999999,20.91,24.36,24.52,24.68]
[null,"Redland Bay","Substation Rating","MVA","Non-Coincident",32,32,32,32,32,32,32]
[null,null,null,null,"Coincident",32,32,32,32,32,32,32]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.91,19.670000000000002,19.600000000000001,19.510000000000002,19.59,19.82,20.059999999999999]
[null,null,null,null,"Coincident",19.38,19.149999999999999,19.09,18.989999999999998,19.07,19.3,19.54]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.93,19.7,19.63,19.53,19.61,19.850000000000001,20.09]
[null,null,null,null,"Coincident",19.39,19.16,19.100000000000001,19,19.079999999999998,19.309999999999999,19.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.829999999999998,18.600000000000001,18.54,18.45,18.52,18.739999999999998,18.97]
[null,null,null,null,"Coincident",18.329999999999998,18.11,18.05,17.96,18.04,18.25,18.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.850000000000001,18.62,18.559999999999999,18.47,18.55,18.77,18.989999999999998]
[null,null,null,null,"Coincident",18.34,18.12,18.059999999999999,17.97,18.04,18.260000000000002,18.48]
[null,"Robina","Substation Rating","MVA","Non-Coincident",131,131,131,131,131,131,131]
[null,null,null,null,"Coincident",131,131,131,131,131,131,131]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.38,49.37,48.72,47.8,47.35,47.21,47.09]
[null,null,null,null,"Coincident",48.71,47.73,47.11,46.21,45.78,45.64,45.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.43,49.41,48.76,47.83,47.38,47.24,47.12]
[null,null,null,null,"Coincident",48.72,47.73,47.11,46.22,45.79,45.65,45.53]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.3,45.36,44.77,43.92,43.51,43.38,43.28]
[null,null,null,null,"Coincident",44.76,43.86,43.29,42.47,42.07,41.94,41.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.32,45.39,44.79,43.94,43.53,43.4,43.29]
[null,null,null,null,"Coincident",44.76,43.86,43.29,42.47,42.07,42.29,42.19]
[null,"Rocklea","Substation Rating","MVA","Non-Coincident",32,32,32,32,32,32,32]
[null,null,null,null,"Coincident",32,32,32,32,32,32,32]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.72,16.309999999999999,16.21,16.010000000000002,15.98,16.05,16.14]
[null,null,null,null,"Coincident",13.46,13.14,13.05,12.89,12.87,12.92,13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.21,16.79,16.68,16.47,16.440000000000001,16.510000000000002,16.61]
[null,null,null,null,"Coincident",13.56,13.23,13.14,12.98,12.96,13.01,13.09]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.93,15.54,15.44,15.24,15.22,15.28,15.38]
[null,null,null,null,"Coincident",12.82,12.51,12.43,12.27,12.25,12.31,12.38]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.39,15.99,15.88,15.69,15.66,15.73,15.82]
[null,null,null,null,"Coincident",12.91,12.6,12.52,12.36,12.34,12.39,12.47]
[null,"Roderick St","Substation Rating","MVA","Non-Coincident",49,49,49,49,49,49,49]
[null,null,null,null,"Coincident",49,49,49,49,49,49,49]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.93,26.74,26.71,26.54,26.65,26.86,27.04]
[null,null,null,null,"Coincident",23.3,23.13,23.11,22.96,23.05,23.24,23.39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.94,26.74,26.72,26.55,26.66,26.87,27.05]
[null,null,null,null,"Coincident",23.3,23.22,23.19,23.04,23.14,23.24,23.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.08,25.89,25.86,25.69,25.8,26.01,26.18]
[null,null,null,null,"Coincident",22.56,22.39,22.37,22.23,22.32,22.5,22.65]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.08,25.89,25.86,25.7,25.8,26.01,26.19]
[null,null,null,null,"Coincident",22.64,22.47,22.45,22.3,22.4,22.58,22.73]
[null,"Rosewood","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.32,7.56,7.82,8.1,8.4700000000000006,8.86,9.23]
[null,null,null,null,"Coincident",7.28,7.51,7.77,8.0500000000000007,8.41,8.81,9.17]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.55,7.79,8.06,8.36,8.73,8.86,9.24]
[null,null,null,null,"Coincident",7.43,7.66,7.93,8.2200000000000006,8.58,8.99,9.36]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.92,7.14,7.39,7.66,8,8.3800000000000008,8.73]
[null,null,null,null,"Coincident",6.88,7.1,7.34,7.61,7.95,8.32,8.67]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.14,7.36,7.62,7.9,8.25,8.64,8.73]
[null,null,null,null,"Coincident",7.02,7.24,7.5,7.77,8.11,8.49,8.85]
[null,"Runcorn","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.71,23.54,23.55,23.42,23.53,23.85,24.21]
[null,null,null,null,"Coincident",23.09,22.93,22.93,22.81,22.92,23.23,23.58]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.75,23.58,23.59,23.46,23.57,23.89,24.25]
[null,null,null,null,"Coincident",23.12,22.96,22.96,22.83,22.94,23.25,23.61]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.1,21.94,21.95,21.83,21.93,22.23,22.57]
[null,null,null,null,"Coincident",21.52,21.37,21.38,21.26,21.36,21.65,21.98]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.14,21.98,21.99,21.87,21.97,22.27,22.61]
[null,null,null,null,"Coincident",21.55,21.4,21.4,21.28,21.39,21.67,22.01]
[null,"Russell Island","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.89,6.99,7.08,7.15,7.28,7.46,7.68]
[null,null,null,null,"Coincident",6.72,6.76,6.87,6.96,7.11,7.3,7.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.94,7.04,7.13,7.2,7.33,7.51,7.74]
[null,null,null,null,"Coincident",6.72,6.76,6.87,6.96,7.11,7.3,7.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.64,6.73,6.82,6.89,7.02,7.19,7.4]
[null,null,null,null,"Coincident",6.2,6.24,6.34,6.43,6.56,6.74,6.91]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.68,6.78,6.87,6.94,7.06,7.24,7.45]
[null,null,null,null,"Coincident",6.2,6.24,6.34,6.43,6.56,6.74,6.91]
[null,"Salisbury","Substation Rating","MVA","Non-Coincident",16,16,16,16,16,16,16]
[null,null,null,null,"Coincident",16,16,16,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.32,10.220000000000001,10.18,10.11,10.16,10.26,10.39]
[null,null,null,null,"Coincident",9.18,9.08,9.0500000000000007,8.99,9.0299999999999994,9.1300000000000008,9.24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.58,10.47,10.43,10.36,10.41,10.52,10.65]
[null,null,null,null,"Coincident",9.2100000000000009,9.1199999999999992,9.08,9.02,9.06,9.16,9.27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.65,9.5500000000000007,9.52,9.4499999999999993,9.49,9.6,9.7200000000000006]
[null,null,null,null,"Coincident",8.58,8.49,8.4600000000000009,8.41,8.44,8.5299999999999994,8.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.89,9.7899999999999991,9.75,9.69,9.73,9.83,9.9600000000000009]
[null,null,null,null,"Coincident",8.61,8.52,8.49,8.44,8.4700000000000006,8.56,8.67]
[null,"Samford","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.47,17.21,17.09,16.91,16.899999999999999,17.04,17.21]
[null,null,null,null,"Coincident",16.45,16.2,16.100000000000001,15.92,15.91,16.04,16.21]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.55,17.28,17.170000000000002,16.989999999999998,16.98,17.11,17.29]
[null,null,null,null,"Coincident",16.5,16.25,16.149999999999999,15.97,15.96,16.09,16.260000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.79,15.55,15.45,15.28,15.27,15.39,15.55]
[null,null,null,null,"Coincident",14.87,14.64,14.55,14.39,14.38,14.5,14.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.86,15.62,15.52,15.35,15.34,15.46,15.62]
[null,null,null,null,"Coincident",14.91,14.69,14.59,14.43,14.42,14.54,14.69]
[null,"Sandgate","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.08,36.35,35.92,35.299999999999997,35.03,35,35.1]
[null,null,null,null,"Coincident",37.08,36.35,35.92,35.299999999999997,35.03,35,35.1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.14,36.42,35.979999999999997,35.36,35.090000000000003,35.06,35.159999999999997]
[null,null,null,null,"Coincident",37.119999999999997,36.39,35.96,35.33,35.07,35.04,35.14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.299999999999997,33.630000000000003,33.24,32.659999999999997,32.409999999999997,32.380000000000003,32.47]
[null,null,null,null,"Coincident",34.299999999999997,33.630000000000003,33.24,32.659999999999997,32.409999999999997,32.380000000000003,32.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.36,33.69,33.29,32.71,32.47,32.43,32.53]
[null,null,null,null,"Coincident",34.340000000000003,33.67,33.270000000000003,32.69,32.450000000000003,32.409999999999997,32.51]
[null,"Scarborough","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.91,20.86,20.95,20.99,21.21,21.58,21.94]
[null,null,null,null,"Coincident",19.84,19.79,19.88,19.920000000000002,20.13,20.47,20.82]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.92,20.87,20.96,21,21.22,21.58,21.95]
[null,null,null,null,"Coincident",19.84,19.79,19.88,19.920000000000002,20.13,20.47,20.82]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.829999999999998,19.78,19.87,19.899999999999999,20.12,20.46,20.8]
[null,null,null,null,"Coincident",18.82,18.77,18.850000000000001,18.89,19.09,19.420000000000002,19.739999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.84,19.79,19.87,19.91,20.12,20.47,20.81]
[null,null,null,null,"Coincident",18.82,18.77,18.850000000000001,18.89,19.09,19.420000000000002,19.739999999999998]
[null,"Scrub Road","Substation Rating","MVA","Non-Coincident",47,47,47,47,47,47,47]
[null,null,null,null,"Coincident",47,47,47,47,47,47,47]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.96,31.21,30.72,30.08,29.75,29.66,29.59]
[null,null,null,null,"Coincident",29.91,29.21,28.75,28.15,27.85,27.76,27.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.200000000000003,31.44,30.95,30.3,29.97,29.88,29.81]
[null,null,null,null,"Coincident",30.03,29.32,28.86,28.25,27.95,27.87,27.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.02,28.34,27.9,27.31,27.01,26.93,26.87]
[null,null,null,null,"Coincident",27.16,26.52,26.11,25.56,25.28,25.21,25.14]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.23,28.55,28.1,27.51,27.21,27.13,27.06]
[null,null,null,null,"Coincident",27.26,26.62,26.21,25.65,25.38,25.3,25.24]
[null,"Sherwood","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.18,31.92,31.64,31.19,31.04,31.12,31.4]
[null,null,null,null,"Coincident",28.92,30.59,30.32,29.89,29.75,29.82,30.09]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.31,32.06,31.78,31.33,31.17,31.25,31.53]
[null,null,null,null,"Coincident",29.1,30.84,30.57,30.13,29.99,30.06,30.33]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.66,29.44,29.19,28.78,28.64,28.71,28.96]
[null,null,null,null,"Coincident",26.51,28.22,27.97,27.58,27.44,27.51,27.75]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.78,29.57,29.31,28.9,28.76,28.83,29.09]
[null,null,null,null,"Coincident",26.67,28.45,28.2,27.8,27.67,27.74,27.98]
[null,"Somerset Dam","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.44,0.44,0.43,0.43,0.43,0.43,0.43]
[null,null,null,null,"Coincident",0.39,0.39,0.38,0.38,0.38,0.38,0.38]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.44,0.44,0.44,0.43,0.43,0.43,0.43]
[null,null,null,null,"Coincident",0.39,0.39,0.38,0.38,0.38,0.38,0.38]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.42,0.41,0.41,0.41,0.41,0.41,0.41]
[null,null,null,null,"Coincident",0.37,0.37,0.36,0.36,0.36,0.36,0.36]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.42,0.42,0.41,0.41,0.41,0.41,0.41]
[null,null,null,null,"Coincident",0.37,0.37,0.37,0.36,0.36,0.36,0.36]
[null,"Southport","Substation Rating","MVA","Non-Coincident",183,183,183,183,183,183,183]
[null,null,null,null,"Coincident",183,183,183,183,183,183,183]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",74.819999999999993,73.91,73.47,72.86,73,73.510000000000005,74.02]
[null,null,null,null,"Coincident",72.760000000000005,71.88,71.45,70.849999999999994,70.989999999999995,71.48,71.989999999999995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",74.88,73.959999999999994,73.52,72.900000000000006,73.040000000000006,73.56,74.08]
[null,null,null,null,"Coincident",72.849999999999994,71.959999999999994,71.53,70.930000000000007,71.069999999999993,71.569999999999993,72.069999999999993]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",71.45,70.58,70.16,69.569999999999993,69.7,70.19,70.680000000000007]
[null,null,null,null,"Coincident",69.48,68.63,68.22,67.650000000000006,67.78,68.260000000000005,68.739999999999995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",71.48,70.61,70.19,69.59,69.73,70.22,70.709999999999994]
[null,null,null,null,"Coincident",69.55,68.7,68.290000000000006,67.72,67.849999999999994,68.319999999999993,68.81]
[null,"Spring Creek","Substation Rating","MVA","Non-Coincident",17,17,17,17,17,17,17]
[null,null,null,null,"Coincident",17,17,17,17,17,17,17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.68,3.55,3.5,3.44,3.41,3.39,3.37]
[null,null,null,null,"Coincident",3,2.89,2.86,2.8,2.78,2.76,2.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.0599999999999996,3.92,3.87,3.8,3.76,3.75,3.72]
[null,null,null,null,"Coincident",3.02,2.92,2.88,2.82,2.8,2.79,2.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.43,3.31,3.26,3.2,3.17,3.16,3.14]
[null,null,null,null,"Coincident",2.79,2.7,2.66,2.61,2.59,2.57,2.56]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.78,3.65,3.61,3.54,3.5,3.49,3.47]
[null,null,null,null,"Coincident",2.81,2.72,2.68,2.63,2.61,2.6,2.58]
[null,"Springfield","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31,30.24,29.91,29.49,29.27,29.17,29.35]
[null,null,null,null,"Coincident",31,30.24,29.91,29.49,29.27,29.17,29.35]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.28,30.52,30.18,29.76,29.54,29.44,29.62]
[null,null,null,null,"Coincident",31.24,30.47,30.14,29.72,29.49,29.39,29.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.65,27.95,27.64,27.26,27.05,26.96,27.13]
[null,null,null,null,"Coincident",28.65,27.95,27.64,27.26,27.05,26.96,27.13]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.92,28.2,27.9,27.51,27.3,27.21,27.38]
[null,null,null,null,"Coincident",28.87,28.16,27.85,27.47,27.26,27.17,27.34]
[null,"Springfield Central","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.42,25.05,25.34,26.1,27.05,28.25,29.51]
[null,null,null,null,"Coincident",22.42,25.05,25.34,26.1,27.05,28.25,29.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.44,25.08,25.37,26.13,27.09,28.29,29.55]
[null,null,null,null,"Coincident",22.46,25.06,25.35,26.11,27.06,28.26,29.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.62,23.24,23.51,24.21,25.09,26.19,27.35]
[null,null,null,null,"Coincident",20.62,23.24,23.51,24.21,25.09,26.19,27.35]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.65,23.27,23.54,24.24,25.12,26.22,27.38]
[null,null,null,null,"Coincident",20.66,23.25,23.52,24.22,25.1,26.2,27.36]
[null,"St Lucia","Substation Rating","MVA","Non-Coincident",49,49,49,49,49,49,49]
[null,null,null,null,"Coincident",49,49,49,49,49,49,49]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.52,27.07,26.82,26.41,26.23,26.21,26.14]
[null,null,null,null,"Coincident",26.4,25.97,25.72,25.33,25.16,25.14,25.07]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.56,27.11,26.85,26.43,26.25,26.23,26.16]
[null,null,null,null,"Coincident",26.4,25.97,25.72,25.33,25.73,25.71,25.64]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.32,25.89,25.65,25.25,25.08,25.07,25]
[null,null,null,null,"Coincident",25.25,24.84,24.6,24.22,24.06,24.05,23.98]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.35,25.91,25.67,25.27,25.1,25.08,25.02]
[null,null,null,null,"Coincident",25.25,25.4,25.16,24.77,24.61,24.59,24.53]
[null,"Stafford","Substation Rating","MVA","Non-Coincident",51,51,51,51,51,51,51]
[null,null,null,null,"Coincident",51,51,51,51,51,51,51]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.57,32.04,31.74,31.25,31.07,31.1,31.12]
[null,null,null,null,"Coincident",32.39,31.87,31.57,31.08,30.91,30.93,30.95]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.700000000000003,32.159999999999997,31.86,31.37,31.2,31.22,31.24]
[null,null,null,null,"Coincident",32.43,31.91,31.61,31.12,30.95,30.97,30.99]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.06,29.57,29.29,28.84,28.68,28.7,28.72]
[null,null,null,null,"Coincident",29.89,29.41,29.13,28.68,28.52,28.54,28.56]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.17,29.68,29.4,28.95,28.79,28.81,28.83]
[null,null,null,null,"Coincident",29.93,29.44,29.17,28.72,28.56,28.58,28.6]
[null,"Stapylton","Substation Rating","MVA","Non-Coincident",54,54,54,54,54,54,54]
[null,null,null,null,"Coincident",54,54,54,54,54,54,54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.53,11.36,11.26,11.1,11.04,11.03,10.99]
[null,null,null,null,"Coincident",8.67,8.5399999999999991,8.4700000000000006,8.34,8.3000000000000007,8.2899999999999991,8.26]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.94,11.76,11.66,11.49,11.44,11.42,11.38]
[null,null,null,null,"Coincident",8.89,8.76,8.68,8.5500000000000007,8.51,8.5,8.4700000000000006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.29,11.13,11.03,10.87,10.82,10.8,10.77]
[null,null,null,null,"Coincident",8.49,8.3699999999999992,8.2899999999999991,8.17,8.1300000000000008,8.1199999999999992,8.09]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.69,11.52,11.42,11.26,11.2,11.19,11.15]
[null,null,null,null,"Coincident",8.6999999999999993,8.58,8.5,8.3800000000000008,8.34,8.33,8.3000000000000007]
[null,"Stradbroke Is","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.03,4.97,4.93,4.87,4.8600000000000003,4.87,4.87]
[null,null,null,null,"Coincident",3.64,3.59,3.57,3.52,3.51,3.52,3.52]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.09,5.0199999999999996,4.99,4.93,4.91,4.92,4.93]
[null,null,null,null,"Coincident",3.65,3.61,3.58,3.54,3.53,3.54,3.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8899999999999997,4.83,4.79,4.7300000000000004,4.72,4.7300000000000004,4.7300000000000004]
[null,null,null,null,"Coincident",3.54,3.49,3.47,3.42,3.41,3.42,3.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.95,4.88,4.8499999999999996,4.79,4.7699999999999996,4.78,4.79]
[null,null,null,null,"Coincident",3.55,3.51,3.48,3.44,3.43,3.44,3.44]
[null,"Strathpine","Substation Rating","MVA","Non-Coincident",53,53,53,53,53,53,53]
[null,null,null,null,"Coincident",53,53,53,53,53,53,53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.81,30.46,29.98,29.39,29.23,29.19,29.12]
[null,null,null,null,"Coincident",23.29,23.94,23.57,23.11,22.98,22.95,22.9]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.05,30.71,30.23,29.64,29.47,29.43,29.37]
[null,null,null,null,"Coincident",23.29,23.94,23.57,23.11,22.98,22.95,22.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.12,28.81,28.36,27.81,27.65,27.61,27.55]
[null,null,null,null,"Coincident",21.97,22.66,22.31,21.87,21.75,21.72,21.67]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.35,29.05,28.6,28.04,27.88,27.84,27.78]
[null,null,null,null,"Coincident",21.97,22.66,22.31,21.87,21.75,21.72,21.67]
[null,"Sumner","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.19,34.39,33.86,33.159999999999997,32.840000000000003,32.75,32.729999999999997]
[null,null,null,null,"Coincident",35.130000000000003,34.33,33.81,33.11,32.79,32.700000000000003,32.68]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.24,34.43,33.9,33.200000000000003,32.880000000000003,32.79,32.76]
[null,null,null,null,"Coincident",35.18,34.380000000000003,33.86,33.159999999999997,32.840000000000003,32.75,32.729999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.64,31.89,31.41,30.76,30.46,30.38,30.36]
[null,null,null,null,"Coincident",32.590000000000003,31.85,31.36,30.71,30.42,30.33,30.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.67,31.93,31.44,30.79,30.49,30.4,30.38]
[null,null,null,null,"Coincident",32.64,31.89,31.4,30.76,30.46,30.38,30.35]
[null,"Sunnybank","Substation Rating","MVA","Non-Coincident",42,42,42,42,42,42,44]
[null,null,null,null,"Coincident",42,42,42,42,42,42,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.21,30.78,30.56,30.11,30.95,31.96,31.93]
[null,null,null,null,"Coincident",29.89,29.48,29.27,28.84,29.63,30.58,30.55]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.3,30.86,30.64,30.18,31.04,32.06,32.03]
[null,null,null,null,"Coincident",29.9,29.48,29.27,28.84,29.64,30.59,30.56]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.56,29.15,28.94,28.52,29.37,30.38,30.35]
[null,null,null,null,"Coincident",28.31,27.92,27.72,27.32,28.11,29.06,29.03]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.62,29.21,28.99,28.56,29.43,30.45,30.42]
[null,null,null,null,"Coincident",28.31,27.92,28.34,27.92,28.12,29.07,29.04]
[null,"Surfers Paradise","Substation Rating","MVA","Non-Coincident",185,185,185,185,185,185,185]
[null,null,null,null,"Coincident",185,185,185,185,185,185,185]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Summer","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.22,55.25,59.81,60.03,60.13,60.75,61.64]
[null,null,null,null,"Coincident",49.08,55.25,54.96,54.33,54.34,54.74,55.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.22,55.25,59.82,60.04,60.13,60.76,61.65]
[null,null,null,null,"Coincident",49.19,55.51,55.21,54.58,54.58,55,55.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.94,53.25,57.49,57.7,57.79,58.39,59.23]
[null,null,null,null,"Coincident",47.05,53.25,52.97,52.37,52.37,52.76,53.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.22,53.49,57.49,57.7,57.8,58.39,59.24]
[null,null,null,null,"Coincident",47.14,53.48,53.2,52.59,52.6,52.99,53.45]
[null,"Tamborine Village","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0199999999999996,4.96,4.93,4.87,4.8499999999999996,4.8600000000000003,4.8600000000000003]
[null,null,null,null,"Coincident",4.8899999999999997,4.83,4.8,4.74,4.7300000000000004,4.74,4.7300000000000004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.03,4.97,4.9400000000000004,4.88,4.8600000000000003,4.87,4.87]
[null,null,null,null,"Coincident",4.9000000000000004,4.84,4.8099999999999996,4.75,4.7300000000000004,4.74,4.74]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4800000000000004,4.42,4.4000000000000004,4.34,4.33,4.33,4.33]
[null,null,null,null,"Coincident",4.3600000000000003,4.3099999999999996,4.28,4.2300000000000004,4.22,4.22,4.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.49,4.43,4.41,4.3499999999999996,4.34,4.3499999999999996,4.34]
[null,null,null,null,"Coincident",4.37,4.3099999999999996,4.29,4.24,4.22,4.2300000000000004,4.2300000000000004]
[null,"Tanah Merah","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.579999999999998,18.170000000000002,17.989999999999998,17.72,17.63,17.64,17.649999999999999]
[null,null,null,null,"Coincident",18.579999999999998,18.170000000000002,17.989999999999998,17.72,17.63,17.64,17.649999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.63,18.22,18.04,17.77,17.670000000000002,17.690000000000001,17.7]
[null,null,null,null,"Coincident",18.59,18.190000000000001,18.010000000000002,17.739999999999998,17.64,17.66,17.670000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.52,17.13,16.97,16.71,16.62,16.64,16.649999999999999]
[null,null,null,null,"Coincident",17.52,17.13,16.97,16.71,16.62,16.64,16.649999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.57,17.18,17.010000000000002,16.760000000000002,16.670000000000002,16.690000000000001,16.690000000000001]
[null,null,null,null,"Coincident",17.53,17.149999999999999,16.98,16.73,16.64,16.66,16.66]
[null,"Tarampa","Substation Rating","MVA","Non-Coincident",13,13,13,16,16,16,16]
[null,null,null,null,"Coincident",13,13,13,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.18,8.08,8.0299999999999994,7.93,7.9,7.91,7.9]
[null,null,null,null,"Coincident",6.4,6.31,6.27,6.2,6.17,6.18,6.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.31,8.1999999999999993,8.15,8.0500000000000007,8.02,8.0299999999999994,8.02]
[null,null,null,null,"Coincident",6.43,6.35,6.31,6.23,6.21,6.22,6.21]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.51,7.42,7.37,7.28,7.25,7.26,7.25]
[null,null,null,null,"Coincident",5.87,5.8,5.76,5.69,5.67,5.68,5.67]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.63,7.53,7.48,7.39,7.36,7.37,7.36]
[null,null,null,null,"Coincident",5.91,5.83,5.79,5.72,5.7,5.71,5.7]
[null,"Taringa","Substation Rating","MVA","Non-Coincident",35,35,35,35,35,35,35]
[null,null,null,null,"Coincident",35,35,35,35,35,35,35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.97,15.56,15.4,15.24,15.24,15.38,15.59]
[null,null,null,null,"Coincident",15.73,15.33,15.18,15.01,15.01,15.16,15.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.03,15.63,15.46,15.3,15.3,15.45,15.65]
[null,null,null,null,"Coincident",15.76,15.36,15.2,15.04,15.04,15.18,15.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.39,14.02,13.88,13.73,13.73,13.86,14.05]
[null,null,null,null,"Coincident",14.18,13.82,13.67,13.53,13.53,13.66,13.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.45,14.08,13.93,13.79,13.79,13.92,14.1]
[null,null,null,null,"Coincident",14.2,13.84,13.7,13.55,13.55,13.68,13.86]
[null,"Tennyson","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.34,11.16,11.05,10.88,10.8,10.78,10.72]
[null,null,null,null,"Coincident",8.51,8.3699999999999992,8.2899999999999991,8.17,8.11,8.09,8.0500000000000007]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.57,11.38,11.27,11.09,11.02,10.99,10.93]
[null,null,null,null,"Coincident",8.67,8.5299999999999994,8.44,8.31,8.25,8.24,8.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.65,10.47,10.37,10.210000000000001,10.14,10.119999999999999,10.07]
[null,null,null,null,"Coincident",7.99,7.86,7.78,7.66,7.61,7.59,7.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.85,10.68,10.58,10.41,10.34,10.32,10.26]
[null,null,null,null,"Coincident",8.1300000000000008,8,7.93,7.8,7.75,7.73,7.69]
[null,"Tenthill","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.13,3.09,3.06,3.02,3.01,3,3]
[null,null,null,null,"Coincident",2.33,2.29,2.2799999999999998,2.2400000000000002,2.23,2.23,2.23]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.18,3.14,3.11,3.07,3.05,3.05,3.04]
[null,null,null,null,"Coincident",2.42,2.39,2.37,2.34,2.33,2.33,2.3199999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.96,2.92,2.9,2.86,2.85,2.85,2.84]
[null,null,null,null,"Coincident",2.2000000000000002,2.17,2.16,2.13,2.12,2.12,2.11]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.01,2.97,2.95,2.9,2.89,2.89,2.88]
[null,null,null,null,"Coincident",2.2999999999999998,2.2599999999999998,2.2400000000000002,2.21,2.2000000000000002,2.2000000000000002,2.2000000000000002]
[null,"Tewantin","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.75,26.41,26.23,25.89,25.79,25.84,26.02]
[null,null,null,null,"Coincident",23.52,23.21,23.06,22.75,22.67,22.71,22.87]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.91,26.57,26.39,26.04,25.94,26,26.17]
[null,null,null,null,"Coincident",23.63,23.32,23.17,22.87,22.78,22.83,22.98]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.86,24.54,24.37,24.06,23.96,24.01,24.17]
[null,null,null,null,"Coincident",21.85,21.57,21.42,21.14,21.06,21.11,21.25]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.01,24.68,24.52,24.2,24.1,24.16,24.32]
[null,null,null,null,"Coincident",21.96,21.67,21.53,21.25,21.16,21.21,21.35]
[null,"The Gap","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.64,18.32,18.14,17.87,17.79,17.899999999999999,18.079999999999998]
[null,null,null,null,"Coincident",18.46,18.14,17.96,17.690000000000001,17.62,17.72,17.899999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.66,18.34,18.16,17.89,17.809999999999999,17.920000000000002,18.100000000000001]
[null,null,null,null,"Coincident",18.46,18.14,17.96,17.7,17.62,17.72,17.899999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.45,17.14,16.98,16.73,16.66,16.75,16.920000000000002]
[null,null,null,null,"Coincident",17.27,16.98,16.809999999999999,16.559999999999999,16.489999999999998,16.59,16.75]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.47,17.16,16.989999999999998,16.739999999999998,16.670000000000002,16.77,16.940000000000001]
[null,null,null,null,"Coincident",17.28,16.98,16.809999999999999,16.559999999999999,16.5,16.59,16.760000000000002]
[null,"Tin Can Bay","Substation Rating","MVA","Non-Coincident",17,17,17,17,17,17,17]
[null,null,null,null,"Coincident",17,17,17,17,17,17,17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9600000000000009,8.83,8.76,8.64,8.61,8.6199999999999992,8.6300000000000008]
[null,null,null,null,"Coincident",7.5,7.39,7.34,7.24,7.21,7.22,7.23]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9,8.8699999999999992,8.8000000000000007,8.68,8.65,8.66,8.67]
[null,null,null,null,"Coincident",7.52,7.41,7.35,7.25,7.22,7.23,7.24]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.23,8.11,8.0500000000000007,7.94,7.91,7.92,7.92]
[null,null,null,null,"Coincident",6.89,6.79,6.74,6.65,6.62,6.63,6.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.27,8.15,8.08,7.98,7.94,7.96,7.96]
[null,null,null,null,"Coincident",6.91,6.8,6.75,6.66,6.63,6.64,6.65]
[null,"Tingalpa","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.29,23.79,23.59,23.27,23.19,23.26,23.34]
[null,null,null,null,"Coincident",24.29,23.79,23.59,23.27,23.19,23.26,23.34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.42,23.91,23.72,23.39,23.31,23.38,23.47]
[null,null,null,null,"Coincident",24.36,23.85,23.66,23.33,23.25,23.32,23.41]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23,22.52,22.34,22.03,21.95,22.02,22.1]
[null,null,null,null,"Coincident",23,22.52,22.34,22.03,21.95,22.02,22.1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.12,22.64,22.45,22.14,22.07,22.14,22.22]
[null,null,null,null,"Coincident",23.06,22.58,22.4,22.09,22.01,22.08,22.16]
[null,"Toogoolawah","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.07,5.0199999999999996,5,4.96,4.96,4.9800000000000004,4.99]
[null,null,null,null,"Coincident",3.86,3.82,3.81,3.78,3.78,3.79,3.8]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.07,5.0199999999999996,5.12,5.07,5.07,5.09,5.0999999999999996]
[null,null,null,null,"Coincident",3.9,3.87,3.85,3.82,3.82,3.84,3.84]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.5,4.46,4.45,4.41,4.41,4.43,4.43]
[null,null,null,null,"Coincident",3.43,3.4,3.39,3.36,3.36,3.37,3.38]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.5999999999999996,4.5599999999999996,4.55,4.51,4.51,4.53,4.53]
[null,null,null,null,"Coincident",3.47,3.43,3.42,3.39,3.39,3.41,3.42]
[null,"Toorbul Point","Substation Rating","MVA","Non-Coincident",12,12,12,10,10,10,10]
[null,null,null,null,"Coincident",12,12,12,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.01,6.93,6.91,6.85,6.85,6.88,6.9]
[null,null,null,null,"Coincident",5.92,5.85,5.84,5.79,5.78,5.81,5.83]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.02,6.94,6.92,6.86,6.86,6.89,6.91]
[null,null,null,null,"Coincident",5.95,5.88,5.86,5.81,5.81,5.83,5.85]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.54,6.46,6.45,6.39,6.38,6.41,6.44]
[null,null,null,null,"Coincident",5.52,5.46,5.44,5.39,5.39,5.42,5.44]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.55,6.47,6.46,6.4,6.39,6.42,6.45]
[null,null,null,null,"Coincident",5.54,5.48,5.47,5.42,5.41,5.44,5.46]
[null,"Toowong","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",48,48,48,48,48,48,48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.78,31.02,33.99,33.65,33.630000000000003,33.840000000000003,34.119999999999997]
[null,null,null,null,"Coincident",31.34,30.59,33.64,33.299999999999997,33.28,33.49,33.770000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.79,31.03,34.01,33.67,33.65,33.86,34.14]
[null,null,null,null,"Coincident",31.72,30.96,33.64,33.31,33.29,33.49,33.770000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.29,28.6,31.6,31.29,31.27,31.46,31.72]
[null,null,null,null,"Coincident",28.89,28.2,31.29,30.98,30.96,31.15,31.4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.3,28.6,31.61,31.3,31.28,31.47,31.73]
[null,null,null,null,"Coincident",29.24,28.54,31.29,30.98,30.96,31.15,31.4]
[null,"Upper Mt Gravatt","Substation Rating","MVA","Non-Coincident",82,82,82,82,82,82,82]
[null,null,null,null,"Coincident",82,82,82,82,82,82,82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.3,25.88,25.65,25.33,25.26,25.34,25.36]
[null,null,null,null,"Coincident",25.52,25.12,24.89,24.58,24.52,24.59,24.62]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.82,26.39,26.16,25.83,25.76,25.84,25.87]
[null,null,null,null,"Coincident",25.88,25.47,25.24,24.93,24.86,24.93,24.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.28,24.88,24.66,24.35,24.28,24.35,24.38]
[null,null,null,null,"Coincident",24.53,24.14,23.93,23.63,23.57,23.63,23.66]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.78,25.37,25.14,24.83,24.77,24.84,24.86]
[null,null,null,null,"Coincident",24.88,24.48,24.26,23.96,23.9,23.97,23.99]
[null,"Varsity Lakes","Substation Rating","MVA","Non-Coincident",68,68,68,68,68,68,68]
[null,null,null,null,"Coincident",68,68,68,68,68,68,68]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.630000000000003,35.979999999999997,35.64,35.15,35,35.090000000000003,35.19]
[null,null,null,null,"Coincident",36.28,35.64,35.299999999999997,34.81,34.67,34.76,34.86]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.86,36.21,35.869999999999997,35.369999999999997,35.229999999999997,35.32,35.42]
[null,null,null,null,"Coincident",36.369999999999997,35.729999999999997,35.39,34.9,34.76,34.85,34.950000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.26,32.67,32.36,31.91,31.78,31.87,31.96]
[null,null,null,null,"Coincident",32.94,32.36,32.049999999999997,31.61,31.48,31.57,31.66]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.47,32.880000000000003,32.57,32.119999999999997,31.99,32.07,32.17]
[null,null,null,null,"Coincident",33.03,32.450000000000003,32.14,31.69,31.57,31.65,31.74]
[null,"Victoria Park","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.86,46.22,45.87,45.23,45.01,45.02,44.98]
[null,null,null,null,"Coincident",42.16,41.58,41.26,40.68,40.49,40.5,40.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.9,46.25,45.9,45.25,45.04,45.05,45]
[null,null,null,null,"Coincident",42.16,41.58,41.26,40.68,40.49,40.5,40.46]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.27,44.65,44.31,43.69,43.49,43.5,43.45]
[null,null,null,null,"Coincident",40.72,40.159999999999997,39.86,39.299999999999997,39.11,39.119999999999997,39.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.3,44.67,44.34,43.71,43.51,43.51,43.47]
[null,null,null,null,"Coincident",40.72,40.159999999999997,39.86,39.299999999999997,39.11,39.119999999999997,39.08]
[null,"Victoria Point","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.3,24.92,24.72,24.37,24.26,24.31,24.36]
[null,null,null,null,"Coincident",24.78,24.41,24.21,23.87,23.77,23.82,23.86]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.33,24.95,24.75,24.4,24.3,24.35,24.39]
[null,null,null,null,"Coincident",24.79,24.42,24.22,23.88,23.78,23.83,23.87]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.97,23.61,23.42,23.09,22.99,23.04,23.08]
[null,null,null,null,"Coincident",23.48,23.12,22.94,22.61,22.52,22.56,22.61]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24,23.64,23.45,23.12,23.02,23.07,23.11]
[null,null,null,null,"Coincident",23.49,23.13,22.95,22.62,22.53,22.57,22.62]
[null,"Wacol","Substation Rating","MVA","Non-Coincident",77,77,77,77,77,77,77]
[null,null,null,null,"Coincident",77,77,77,77,77,77,77]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.87,31.26,30.82,30.21,29.79,29.43,29.05]
[null,null,null,null,"Coincident",19.440000000000001,24.16,23.84,23.38,23.06,22.79,22.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.98,31.5,31.05,30.43,29.99,29.62,29.23]
[null,null,null,null,"Coincident",19.96,24.17,23.84,23.38,23.07,22.79,22.51]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.64,30.05,29.63,29.05,28.65,28.31,27.95]
[null,null,null,null,"Coincident",18.510000000000002,23.25,22.94,22.51,22.21,21.95,21.68]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.71,30.26,29.83,29.24,28.83,28.47,28.1]
[null,null,null,null,"Coincident",19.010000000000002,23.26,22.95,22.51,22.21,21.95,21.68]
[null,"Wacol South","Substation Rating","MVA","Non-Coincident",53,53,53,53,53,53,53]
[null,null,null,null,"Coincident",53,53,53,53,53,53,53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.61,24.58,24.3,23.9,23.74,23.68,23.66]
[null,null,null,null,"Coincident",22.44,23.52,23.25,22.87,22.71,22.66,22.64]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.83,24.81,24.53,24.13,23.96,23.9,23.88]
[null,null,null,null,"Coincident",22.59,23.71,23.44,23.06,22.9,22.85,22.83]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.09,23.09,22.83,22.45,22.3,22.25,22.23]
[null,null,null,null,"Coincident",20.99,22.1,21.85,21.49,21.34,21.3,21.28]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.29,23.3,23.04,22.66,22.5,22.45,22.43]
[null,null,null,null,"Coincident",21.13,22.28,22.03,21.67,21.52,21.47,21.46]
[null,"Wamuran","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.5599999999999996,4.5,4.46,4.45,4.49,4.55,4.6100000000000003]
[null,null,null,null,"Coincident",4.28,4.21,4.18,4.17,4.2,4.26,4.3099999999999996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.57,4.5,4.47,4.46,4.49,4.5599999999999996,4.6100000000000003]
[null,null,null,null,"Coincident",4.28,4.21,4.18,4.17,4.21,4.26,4.32]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.28,4.21,4.18,4.17,4.2,4.26,4.3099999999999996]
[null,null,null,null,"Coincident",4,3.94,3.91,3.91,3.94,3.99,4.04]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.28,4.22,4.18,4.18,4.21,4.2699999999999996,4.32]
[null,null,null,null,"Coincident",4.01,3.95,3.92,3.91,3.94,3.99,4.05]
[null,"Wellington Rd","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",60.24,64.81,64.44,63.71,63.55,63.69,63.8]
[null,null,null,null,"Coincident",56.52,61.22,60.87,60.18,60.04,60.17,60.27]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",60.26,64.849999999999994,64.48,63.74,63.59,63.73,63.84]
[null,null,null,null,"Coincident",56.62,61.42,61.07,60.37,60.23,60.36,60.46]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.54,63.14,62.78,62.06,61.91,62.05,62.16]
[null,null,null,null,"Coincident",54.93,59.64,59.3,58.64,58.5,58.62,58.72]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",58.55,63.17,62.8,62.09,61.94,62.07,62.18]
[null,null,null,null,"Coincident",55.01,59.83,59.49,58.82,58.67,58.8,58.9]
[null,"West End","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",73.77,72.64,71.98,70.959999999999994,70.739999999999995,70.900000000000006,71.099999999999994]
[null,null,null,null,"Coincident",68.849999999999994,67.8,67.180000000000007,66.23,66.03,66.17,66.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.87,72.739999999999995,72.069999999999993,71.040000000000006,70.819999999999993,70.98,71.180000000000007]
[null,null,null,null,"Coincident",68.89,67.84,67.22,66.260000000000005,66.05,66.2,66.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",71.569999999999993,70.48,69.83,68.84,68.63,68.790000000000006,68.98]
[null,null,null,null,"Coincident",66.8,65.78,65.180000000000007,64.260000000000005,64.06,64.2,64.38]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",71.650000000000006,70.56,69.900000000000006,68.91,68.69,68.849999999999994,69.040000000000006]
[null,null,null,null,"Coincident",66.83,65.81,65.2,64.27,64.08,64.22,64.400000000000006]
[null,"West Maroochydore","Substation Rating","MVA","Non-Coincident",91,91,91,91,91,91,91]
[null,null,null,null,"Coincident",91,91,91,91,91,91,91]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.49,35.28,35.31,35,35.049999999999997,35.29,35.53]
[null,null,null,null,"Coincident",33.11,32.909999999999997,32.93,32.65,32.69,32.92,33.15]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.6,35.4,35.42,35.11,35.159999999999997,35.4,35.65]
[null,null,null,null,"Coincident",33.159999999999997,32.97,32.99,32.71,32.75,32.979999999999997,33.200000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.36,33.159999999999997,33.18,32.9,32.94,33.17,33.4]
[null,null,null,null,"Coincident",31.12,30.94,30.96,30.69,30.73,30.94,31.16]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.46,33.270000000000003,33.29,33,33.04,33.270000000000003,33.5]
[null,null,null,null,"Coincident",31.17,30.99,31.01,30.74,30.78,30.99,31.21]
[null,"Whinstanes","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.41,9.27,9.19,9.0500000000000007,8.98,8.9700000000000006,8.92]
[null,null,null,null,"Coincident",6.72,6.62,6.56,6.46,6.42,6.4,6.37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9600000000000009,9.81,9.73,9.58,9.51,9.5,9.44]
[null,null,null,null,"Coincident",6.97,6.86,6.8,6.7,6.65,6.64,6.6]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.0299999999999994,8.89,8.81,8.68,8.6199999999999992,8.6,8.5500000000000007]
[null,null,null,null,"Coincident",6.45,6.35,6.3,6.2,6.16,6.14,6.11]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.56,9.41,9.33,9.19,9.1300000000000008,9.11,9.06]
[null,null,null,null,"Coincident",6.68,6.58,6.53,6.43,6.38,6.37,6.33]
[null,"Whiteside","Substation Rating","MVA","Non-Coincident",17,17,17,17,17,17,17]
[null,null,null,null,"Coincident",17,17,17,17,17,17,17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.17,8.92,8.75,8.5500000000000007,8.44,8.39,8.36]
[null,null,null,null,"Coincident",7.52,7.32,7.18,7.01,6.92,6.88,6.86]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.6,9.34,9.16,8.9499999999999993,8.83,8.7899999999999991,8.75]
[null,null,null,null,"Coincident",7.56,7.35,7.21,7.05,6.95,6.92,6.89]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.42,8.19,8.0299999999999994,7.85,7.74,7.7,7.67]
[null,null,null,null,"Coincident",6.9,6.71,6.59,6.43,6.35,6.31,6.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.81,8.57,8.41,8.2100000000000009,8.1,8.06,8.0299999999999994]
[null,null,null,null,"Coincident",6.94,6.75,6.62,6.46,6.38,6.35,6.32]
[null,"Wivenhoe","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,15,15]
[null,null,null,null,"Coincident",12,12,12,12,12,15,15]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.01,6.96,6.94,6.89,6.89,6.93,6.96]
[null,null,null,null,"Coincident",6.09,6.04,6.03,5.98,5.98,6.02,6.05]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.05,7,6.98,6.93,6.93,6.97,7]
[null,null,null,null,"Coincident",6.11,6.06,6.05,6,6.01,6.04,6.07]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.44,6.39,6.38,6.33,6.33,6.37,6.4]
[null,null,null,null,"Coincident",5.59,5.55,5.54,5.49,5.49,5.53,5.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.48,6.42,6.41,6.36,6.36,6.4,6.43]
[null,null,null,null,"Coincident",5.62,5.57,5.56,5.51,5.52,5.55,5.58]
[null,"Woodford","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.03,10.86,10.77,10.62,10.57,10.58,10.57]
[null,null,null,null,"Coincident",10.44,10.28,10.199999999999999,10.06,10.01,10.01,10.01]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.06,10.89,10.8,10.64,10.59,10.6,10.6]
[null,null,null,null,"Coincident",10.45,10.29,10.210000000000001,10.06,10.01,10.02,10.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.58,10.42,10.33,10.19,10.14,10.15,10.14]
[null,null,null,null,"Coincident",10.02,9.86,9.7799999999999994,9.64,9.6,9.6,9.6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.6,10.44,10.36,10.210000000000001,10.16,10.17,10.16]
[null,null,null,null,"Coincident",10.029999999999999,9.8699999999999992,9.7899999999999991,9.65,9.61,9.61,9.61]
[null,"Woodridge","Substation Rating","MVA","Non-Coincident",90,90,90,90,90,90,90]
[null,null,null,null,"Coincident",90,90,90,90,90,90,90]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.11,35.47,35.090000000000003,34.54,34.36,34.35,34.380000000000003]
[null,null,null,null,"Coincident",33.35,32.76,32.409999999999997,31.9,31.73,31.72,31.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.11,35.479999999999997,35.090000000000003,34.54,34.36,34.35,34.380000000000003]
[null,null,null,null,"Coincident",33.72,33.130000000000003,32.770000000000003,32.26,32.090000000000003,32.08,32.11]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.21,32.630000000000003,32.270000000000003,31.77,31.6,31.59,31.62]
[null,null,null,null,"Coincident",30.67,30.14,29.81,29.34,29.19,29.18,29.2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.21,32.630000000000003,32.270000000000003,32.22,32.049999999999997,32.04,32.06]
[null,null,null,null,"Coincident",31.02,30.47,30.14,29.67,29.52,29.51,29.53]
[null,"Wynnum","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.36,23.16,23.12,22.88,22.88,23.03,23.18]
[null,null,null,null,"Coincident",22.89,22.7,22.66,22.43,22.42,22.57,22.72]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.54,23.34,23.29,23.06,23.05,23.2,23.35]
[null,null,null,null,"Coincident",22.99,22.8,22.76,22.52,22.52,22.67,22.82]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.42,22.23,22.19,21.97,21.96,22.11,22.25]
[null,null,null,null,"Coincident",21.98,21.79,21.75,21.53,21.53,21.67,21.81]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.6,22.4,22.36,22.14,22.13,22.27,22.42]
[null,null,null,null,"Coincident",22.07,21.89,21.85,21.62,21.62,21.76,21.9]
[null,"Yamanto","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.93,15.73,15.94,16.010000000000002,16.2,16.440000000000001,16.66]
[null,null,null,null,"Coincident",13.67,14.4,14.6,14.66,14.83,15.06,15.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15,15.8,16.010000000000002,16.079999999999998,16.27,16.52,16.73]
[null,null,null,null,"Coincident",13.69,14.44,14.63,14.7,14.86,15.09,15.29]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.49,14.28,14.47,14.53,14.7,14.92,15.11]
[null,null,null,null,"Coincident",12.35,13.07,13.25,13.31,13.46,13.66,13.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.55,14.34,14.53,14.6,14.76,14.99,15.18]
[null,null,null,null,"Coincident",12.37,13.1,13.28,13.34,13.49,13.7,13.87]
[null,"Yandina","Substation Rating","MVA","Non-Coincident",17,17,17,17,17,17,17]
[null,null,null,null,"Coincident",17,17,17,17,17,17,17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.07,11.53,11.55,11.45,11.44,11.51,11.57]
[null,null,null,null,"Coincident",9.8000000000000007,10.199999999999999,10.220000000000001,10.130000000000001,10.130000000000001,10.19,10.24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.09,11.54,11.57,11.46,11.46,11.53,11.58]
[null,null,null,null,"Coincident",9.81,10.220000000000001,10.24,10.15,10.15,10.210000000000001,10.26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.85,10.31,10.34,10.24,10.24,10.3,10.35]
[null,null,null,null,"Coincident",8.7200000000000006,9.1300000000000008,9.15,9.07,9.06,9.11,9.16]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.8699999999999992,10.33,10.35,10.26,10.26,10.31,10.36]
[null,null,null,null,"Coincident",8.73,9.15,9.17,9.09,9.08,9.1300000000000008,9.18]
[null,"Yatala","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",62.87,61.07,59.67,58.61,58.21,58.08,57.92]
[null,null,null,null,"Coincident",60.18,58.46,57.12,56.1,55.72,55.59,55.44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.96,61.15,59.73,58.66,58.26,58.12,57.97]
[null,null,null,null,"Coincident",60.3,58.56,57.21,56.18,55.8,55.67,55.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.39,56.73,55.43,54.45,54.08,53.96,53.81]
[null,null,null,null,"Coincident",55.89,54.3,53.05,52.11,51.76,51.64,51.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",58.45,56.77,55.46,54.47,54.11,53.98,53.83]
[null,null,null,null,"Coincident",55.98,54.37,53.12,52.17,51.82,51.7,51.56]
[null,"Zillmere","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.619999999999997,39.04,38.729999999999997,38.270000000000003,38.29,38.56,38.81]
[null,null,null,null,"Coincident",33.24,32.76,32.5,32.11,32.130000000000003,32.36,32.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.65,39.06,38.76,38.29,38.32,38.58,38.840000000000003]
[null,null,null,null,"Coincident",33.380000000000003,32.89,32.630000000000003,32.24,32.26,32.479999999999997,32.700000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.11,35.58,35.31,34.880000000000003,34.909999999999997,35.15,35.380000000000003]
[null,null,null,null,"Coincident",30.3,29.86,29.63,29.27,29.29,29.49,29.69]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.119999999999997,35.590000000000003,35.31,34.89,34.909999999999997,35.15,35.39]
[null,null,null,null,"Coincident",30.42,29.98,29.74,29.39,29.41,29.61,29.8]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",2,2,8,8,8,8,8]
[null,null,null,null,"Coincident",2,2,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.64,0.64,0.64,0.64,0.64,0.64,0.64]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.7,0.7,0.7,0.7,0.7,0.7,0.7]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.63,0.63,0.63,0.63,0.63,0.63,0.63]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.69,0.69,0.69,0.69,0.69,0.69,0.69]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",25,0,0,0,0,0,0]
[null,null,null,null,"Coincident",25,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer",0,0,0,0,0,0]
[null,null,null,null,"Coincident","Summer",0,0,0,0,0,0]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.85,0,0,0,0,0,0]
[null,null,null,null,"Coincident",9.74,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.83,0,0,0,0,0,0]
[null,null,null,null,"Coincident",11.23,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.15,0,0,0,0,0,0]
[null,null,null,null,"Coincident",9.2100000000000009,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.08,0,0,0,0,0,0]
[null,null,null,null,"Coincident",10.62,0,0,0,0,0,0]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.66,2.66,2.66,2.66,2.66,2.66,2.66]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.13,3.13,3.13,3.13,3.13,3.13,3.13]
[null,null,null,null,"Coincident",2.34,2.34,2.34,2.34,2.34,2.34,2.34]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.59,2.59,2.59,2.59,2.59,2.59,2.59]
[null,null,null,null,"Coincident",1.96,1.96,1.96,1.96,1.96,1.96,1.96]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.05,3.05,3.05,3.05,3.05,3.05,3.05]
[null,null,null,null,"Coincident",2.2799999999999998,2.2799999999999998,2.2799999999999998,2.2799999999999998,2.2799999999999998,2.2799999999999998,2.2799999999999998]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.31,15.31,15.31,15.31,15.31,15.31,15.31]
[null,null,null,null,"Coincident",13.3,13.3,13.3,13.3,13.3,13.3,13.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.12,16.12,16.12,16.12,16.12,16.12,16.12]
[null,null,null,null,"Coincident",13.65,13.65,13.65,13.65,13.65,13.65,13.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15,15,15,15,15,15,15]
[null,null,null,null,"Coincident",12.55,12.55,12.55,12.55,12.55,12.55,12.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.79,15.79,15.79,15.79,15.79,15.79,15.79]
[null,null,null,null,"Coincident",12.88,12.88,12.88,12.88,12.88,12.88,12.88]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.100000000000001,18.100000000000001,18.100000000000001,18.100000000000001,18.100000000000001,18.100000000000001,18.100000000000001]
[null,null,null,null,"Coincident",3.53,3.53,3.53,3.53,3.53,3.53,3.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.309999999999999,18.309999999999999,18.309999999999999,18.309999999999999,18.309999999999999,18.309999999999999,18.309999999999999]
[null,null,null,null,"Coincident",3.65,3.65,3.65,3.65,3.65,3.65,3.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.920000000000002,17.920000000000002,17.920000000000002,17.920000000000002,17.920000000000002,17.920000000000002,17.920000000000002]
[null,null,null,null,"Coincident",3.5,3.5,3.5,3.5,3.5,3.5,3.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.12,18.12,18.12,18.12,18.12,18.12,18.12]
[null,null,null,null,"Coincident",3.61,3.61,3.61,3.61,3.61,3.61,3.61]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",25,25,25,25,25,25,25]
[null,null,null,null,"Coincident",25,25,25,25,25,25,25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.83,17.43,17.309999999999999,17.11,17.010000000000002,16.98,16.91]
[null,null,null,null,"Coincident",11.7,14.2,14.11,13.93,13.85,13.83,13.76]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.43,20.69,20.55,20.309999999999999,20.2,20.170000000000002,20.07]
[null,null,null,null,"Coincident",12.42,15.05,14.94,14.76,14.68,14.65,14.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.7,17.29,17.18,16.98,16.88,16.850000000000001,16.78]
[null,null,null,null,"Coincident",11.59,14.09,13.99,13.82,13.74,13.72,13.65]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.260000000000002,20.53,20.39,20.149999999999999,20.04,20.010000000000002,19.920000000000002]
[null,null,null,null,"Coincident",12.3,14.93,14.82,14.64,14.56,14.53,14.46]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",15,15,15,15,15,15,15]
[null,null,null,null,"Coincident",15,15,15,15,15,15,15]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.56,8.56,8.56,8.56,8.56,8.56,8.56]
[null,null,null,null,"Coincident",1.75,1.75,1.75,1.75,1.75,1.75,1.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.67,9.67,9.67,9.67,9.67,9.67,9.67]
[null,null,null,null,"Coincident",2.1800000000000002,2.1800000000000002,2.1800000000000002,2.1800000000000002,2.1800000000000002,2.1800000000000002,2.1800000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.2100000000000009,8.2100000000000009,8.2100000000000009,8.2100000000000009,8.2100000000000009,8.2100000000000009,8.2100000000000009]
[null,null,null,null,"Coincident",1.68,1.68,1.68,1.68,1.68,1.68,1.68]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.2799999999999994,9.2799999999999994,9.2799999999999994,9.2799999999999994,9.2799999999999994,9.2799999999999994,9.2799999999999994]
[null,null,null,null,"Coincident",2.09,2.09,2.09,2.09,2.09,2.09,2.09]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.51,1.51,1.51,1.51,1.5,1.5,1.51]
[null,null,null,null,"Coincident",0.53,0.53,0.52,0.51,0.51,0.51,0.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.75,1.74,1.75,1.74,1.73,1.73,1.74]
[null,null,null,null,"Coincident",0.6,0.59,0.59,0.57999999999999996,0.56999999999999995,0.56999999999999995,0.56999999999999995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.43,1.43,1.43,1.42,1.41,1.42,1.42]
[null,null,null,null,"Coincident",0.51,0.5,0.5,0.49,0.49,0.49,0.48]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.65,1.65,1.65,1.64,1.63,1.63,1.64]
[null,null,null,null,"Coincident",0.56999999999999995,0.56999999999999995,0.56000000000000005,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.54]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.6300000000000008,8.6300000000000008,8.6300000000000008,8.6300000000000008,8.6300000000000008,8.6300000000000008,8.6300000000000008]
[null,null,null,null,"Coincident",7.56,7.56,7.56,7.56,7.56,7.56,7.56]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.77,8.77,8.77,8.77,8.77,8.77,8.77]
[null,null,null,null,"Coincident",7.64,7.64,7.64,7.64,7.64,7.64,7.64]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.33,8.33,8.33,8.33,8.33,8.33,8.33]
[null,null,null,null,"Coincident",7.3,7.3,7.3,7.3,7.3,7.3,7.3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.4700000000000006,8.4700000000000006,8.4700000000000006,8.4700000000000006,8.4700000000000006,8.4700000000000006,8.4700000000000006]
[null,null,null,null,"Coincident",7.38,7.38,7.38,7.38,7.38,7.38,7.38]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.2 Reliability & Cust serv","index":22,"n_rows":76,"n_cols":9,"rows_kept":76,"cut":false,"hidden":false,"merged":[[6,1,6,7],[17,1,17,3],[29,1,29,3],[71,4,71,8],[41,1,41,3],[53,1,53,3],[56,1,56,8],[68,1,68,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. There are no further instructions."]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,4.4356,4.4356,4.4356,4.4356,4.4356]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,54.035200000000003,54.035200000000003,54.035200000000003,54.035200000000003,54.035200000000003]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,132.38499999999999,132.38499999999999,132.38499999999999,132.38499999999999,132.38499999999999]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E13:E17)","v":190.85579999999999},{"$f":"SUM(F13:F17)","v":190.85579999999999},{"$f":"SUM(G13:G17)","v":190.85579999999999},{"$f":"SUM(H13:H17)","v":190.85579999999999},{"$f":"SUM(I13:I17)","v":190.85579999999999}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,5.2200000000000003E-2,5.2200000000000003E-2,5.2200000000000003E-2,5.2200000000000003E-2,5.2200000000000003E-2]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.56510000000000005,0.56510000000000005,0.56510000000000005,0.56510000000000005,0.56510000000000005]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1.1786000000000001,1.1786000000000001,1.1786000000000001,1.1786000000000001,1.1786000000000001]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E25:E29)","v":1.7959000000000001},{"$f":"SUM(F25:F29)","v":1.7959000000000001},{"$f":"SUM(G25:G29)","v":1.7959000000000001},{"$f":"SUM(H25:H29)","v":1.7959000000000001},{"$f":"SUM(I25:I29)","v":1.7959000000000001}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E37:E41)","v":0},{"$f":"SUM(F37:F41)","v":0},{"$f":"SUM(G37:G41)","v":0},{"$f":"SUM(H37:H41)","v":0},{"$f":"SUM(I37:I41)","v":0}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E49:E53)","v":0},{"$f":"SUM(F49:F53)","v":0},{"$f":"SUM(G49:G53)","v":0},{"$f":"SUM(H49:H53)","v":0},{"$f":"SUM(I49:I53)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS (STPIS)"]
[null,null,"FORECAST"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},4114,4169,4224,4283,4341,4394,4446]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1050509,1064443,1078547,1093597,1108426,1121968,1135138]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},534138,541223,548394,556046,563586,570471,577167]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C62:C66)","v":1588761},1609835,1631165,1653926,1676353,1696833,1716751]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Number of calls received"]
[null,"Number of calls answered within 30 seconds"]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E75/E74),\"\")","v":""},{"$f":"IFERROR((F75/F74),\"\")","v":""},{"$f":"IFERROR((G75/G74),\"\")","v":""},{"$f":"IFERROR((H75/H74),\"\")","v":""},{"$f":"IFERROR((I75/I74),\"\")","v":""}]

{"sheet":"7.1  Policies and Procedures","index":23,"n_rows":386,"n_cols":5,"rows_kept":386,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Governance framework"]
[null,"EQL Statement of Corporate Intent (public version)","It outlines the critical business objectives, key priorities, major initiatives, and financial and non-financial\nperformance measures for Energy Queensland","All","No"]
[null,"EQL Risk Appetite Statement Q015","EQL’s Risk Appetite establishes the amount of risk EQL is willing to pursue or accept in order to achieve its objectives","All","No"]
[null,"EQL Risk Evaluation Matrix R056","This matrix is a tool used for ranking risks.","All","No"]
[null,"EQL Risk management standard","This Standard is a key element of the Enterprise Risk Management Framework (Framework). It provides details regarding risk management at EQL","All","No"]
[null,"Risk management policy P043","The purpose of this Policy is to ensure the implementation of effective risk management practices that will protect and create value and are consistent with strategy formation, business planning and the achievement of the EQL Group’s strategic objectives. This policy\n defines the whole of business, enterprise-wide approach to risk management \nthrough the utilisation of an integrated framework.","All","No"]
[null,"Risk Management Procedure","This procedure provides the information necessary to support the effective application of the Enterprise Risk Management Framework in our day-to-day operations. It is designed to provide the ‘how’ and ensure a consistent and effective approach to the management of risk at EQL.","All","No"]
[null,"EQL Governance and delegations policy P013","This Policy sets out the overarching decision making governance and delegation of authority framework for Energy Queensland Limited (EQL) and its subsidiaries.","All","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Capitalisation Policy","This manual is designed to interpret the Accounting standard guidelines AASB 116 Property Plant and Equipment and AASB 138 Intangible Assets and provide guidance for employees on the application of those standards in practice.","Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Policy","The purpose of this policy is to set out Energy Queensland's principles by which it intends to apply asset management to achieve its organisational objectives.","ALL","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset Management Strategies"]
[null,"Strategic Asset Management Plan (SAMP)","The Strategic Asset Management Plan (SAMP) sets out how we will apply the principles stated in our Asset Management Policy to fulfil Energy Queensland’s (EQL’s)Strategic Objectives. It provides direction for asset management activities and form the basis for developing the more specific asset management strategies and plans.\nIt also describes the asset management system, which conceptualises the integration and\ninterrelationship between asset management activities that is necessary to optimise the value\nfrom assets and contribute to the achievement of the asset management objectives.","All CAPEX /' All OPEX","No"]
[null,"Network Risk Framework","This framework has been developed to undertake and risk based prioritisation of our program of work","Network Capex and Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset Management Plans"]
[null,"Distribution Annual Planning Report (DAPR) Energex","The DAPR covers a five year period and outlines our strategies and plans. In particular, it includes:\n•Planning for subtransmission and distribution network growth\n•Asset repair and replacement planning\n•Planning for future demand on the network\n•Capacity and load forecasts by region\n•Current and future limitations on our subtransmission and distribution networks\n•Possible solutions for network limitations.","All Capex","No"]
[null,"Asset Management Plan - Poles","This document outlines our processes, practises and procedures in managing this asset category","Poles capex","No"]
[null,"Asset Management Plan - Pole Top Structures","This document outlines our processes, practises and procedures in managing this asset category","Pole Top Structures capex","No"]
[null,"Asset Management Plan - Overhead Conductor","This document outlines our processes, practises and procedures in managing this asset category","Overhead Conductor capex","No"]
[null,"Asset Management Plan - Distribution Transformers","This document outlines our processes, practises and procedures in managing this asset category","Distribution Transformers capex","No"]
[null,"Asset Management Plan - Service Lines","This document outlines our processes, practises and procedures in managing this asset category","Service Lines capex","No"]
[null,"Asset Management Plan - Switches","This document outlines our processes, practises and procedures in managing this asset category","Switches capex","No"]
[null,"Asset Management Plan - DC Systems","This document outlines our processes, practises and procedures in managing this asset category","DC Systems capex","No"]
[null,"Asset Management Plan - Control Systems","This document outlines our processes, practises and procedures in managing this asset category","Control Systems capex","No"]
[null,"Asset Management Plan - Instrument Transformers","This document outlines our processes, practises and procedures in managing this asset category","Instrument Transformers capex","No"]
[null,"Asset Management Plan - Protection Relays","This document outlines our processes, practises and procedures in managing this asset category","Protection Relays capex","No"]
[null,"Asset Management Plan - Underground Cables","This document outlines our processes, practises and procedures in managing this asset category","Underground Cables capex","No"]
[null,"Asset Management Plan -Circuit Breakers and Reclosers","This document outlines our processes, practises and procedures in managing this asset category","Circuit Breakers and Reclosers capex","No"]
[null,"Asset Management Plan - Substation Transformers","This document outlines our processes, practises and procedures in managing this asset category","Substation Transformers capex","No"]
[null,"Asset Management Plan - Communications Linear Assets","This document outlines our processes, practises and procedures in managing this asset category","Fibre Optic and Metallic Pilot Cables capex","No"]
[null,"Asset Management Plan - Telecommunications","This document outlines our processes, practises and procedures in managing this asset category","Microwave, Multiplexers, Switches, Routers capex","No"]
[null,"Asset Management Plan - Telecommunications","This document outlines our processes, practises and procedures in managing this asset category","Microwave, Multiplexers, Switches, Routers capex","No"]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Property Plan 2025-30","Outlines the strategy, drivers and proposed expenditure for the 2025-30  period","Non-network capex","No"]
[null,"Fleet Plan 2025-30","Outlines the strategy, drivers and proposed expenditure for the 2025-30  period","Non-network capex","No"]
[null,"Tools and Equipment Plan 2025-30","Outlines the strategy, drivers and proposed expenditure for the 2025-30  period","Non-network capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Safety Net Application Guidelines","This document outlines the application of the Safety Net requirements under our Distribution Authority.","All Capex","No"]
[null,"Cost Benefit Analysis Framework and Principles","This document outlines how to approach quantifying the benefits to customers and the community in assessing investment options for projects and programs.","All Capex","No"]
[null,"Joint Supply and Planning Manual","This document outlines the calculation  is to specify the connection and technical requirements that Small \nand Major Customers connecting to the LV network and requiring a negotiated connection must \ncomply with in order to establish a new Connection, or to alter an existing Connection, to either the \nEnergex distribution networks.","Augmentation and Connections","No"]
[null,"Standard for Sub-transmission and Distribution Planning","This Standard establishes a set of parameters for electrical network planning, network development and network connection activities within Energy Queensland on the Energex and Ergon Energy Networks. ","All Capex","No"]
[null,"Standard for Voltage and Reactive Power Management","This standard describes a set of parameters for the management of voltages on the Energex and Ergon Energy networks","All Capex / All Opex","No"]
[null,"Standard for Network Performance","This Standard is a reference document to be used to assess network performance on a routine or case specific basis and to provide advice on network reliability, quality of supply, power quality, check customer connection requirements related to power quality, and determine if network augmentations are required to mitigate reliability and power quality risks.","All Capex / All Opex","No"]
[null,"Power Quality Planning Guideline","This guideline has been developed to assist with making appropriate assessments of power quality phenomena such as harmonics and flicker, and to assist in planning large customer connections to the ENERGEX, and Ergon Energy electrical distributions systems in Queensland","All Capex","No"]
[null,"Substation Design Manual","This document is a reference for the Designers of Ergon Energy substations and it covers all aspects of substation design for both Greenfield and Brownfield substation projects to meet the performance expected by Ergon Energy","Network Capex","No"]
[null,"Maintenance Standard for Overhead Pole Lines","This standard defines and communicates requirements for inspection and maintenance of overhead pole lines","Network Capex and Opex","No"]
[null,"Lines Defect Classification Manual\nSubstation Defect Classification Manual","This manual outlines the ways our asset inspectors determine asset defects","Network Capex and Opex","No"]
[null,"Maintenance Acceptance Criteria","This document sets out the Maintenance Acceptance Criteria which is used to evaluate the degree of deterioration in condition and performance of network plant and equipment as well as set setting safety criteria to determine if plant is fit to remain in service.\nNote: This document does not identify any safety / environmental hazards or provide warnings / cautions associated with carrying out the inspection or maintenance activities prescribed within it.  ","All Capex and All Opex","No"]
[null,"EQL Standard for Conductor Clearance Prioritisation and Remediation","This document sets out how we assess the criticality of a clearance to structure or clearance to ground issue and the timeframes for remediation.","Augex","No"]
[null,"CBRM/CNAIM Models","This model is utilised to predict asset condition by using condition and other data from our asset inspections and maintenance. This is utilised for the majority of our major asset classes","Repex","No"]
[null,"Maintenance Activity Frequency","This document sets out the frequency of our maintenance and inspection activities","Opex and Capex","No"]
[null,"EQL Maintenance Driven Relay Replacement Priorities & Spares Strategy","This document sets out our approach to prioritising replacements in our relay assets and the strategy for storing spares","Capex","No"]
[null,"Distribution Lines Refurbishment Guidelines - REPEX","This document outlines our approach for identifying and prioritising the bundling of REPEX lines work.","Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"EQL Procurement Policy P011","The Energy Queensland Limited Procurement Policy provides direction in procurement and purchasing activities that support Energy Queensland’s business strategies. \nAccording to the Policy, procurement activities will be undertaken in accordance with established probity and governance standards. \n","All Capex / All Opex","No"]
[null,"EQL Procurement Business Rules R052","The Business Rules have been developed to provide early process guidance and standards to all EQL business operations about the minimum requirements expected when purchasing on behalf of EQL and its subsidiaries, and in doing so seeks to identify the purchasing needs of both the regulated (and unregulated) businesses.  In respect to the unregulated business, the Strategic Procurement Group has identified that there is a particular need to tailor solutions as opportunities and challenges emerge, while ensuring that we continue to work together within important ring fencing parameters at all times.  \nTHe Procurement Business Rules align and support EQL's Sustainable Procurement Policy.","All Capex / All Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Information technology policies or strategies"]
[null,"Non-network ICT Plan 2025-30","Outlines the strategy, governance and expenditure for non-network ICT for the next regulatory control period (2025-30)","Non-Network Capex / Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Demand Management Plan","The purpose of the Demand Management Plan (DM Plan) is to engage and inform our end use customers and industry partners on our planned DM programs for the next five years.","All CAPEX /' All OPEX","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Self insurance guidelines or policy"]
[null,"Insurance Policy P042","The objective of this risk management plan is to ensure the current EQL Insurance Strategy and Program provides the appropriate balance of risk retention (self-insurance) and risk transfer (commercial insurance), to align to EQL’s risk appetite, ensuring adequate cover for existing and emerging risks that have the potential to impact the ongoing financial stability of EQL.\n\n","All CAPEX / All OPEX","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Land and easement acquisition polices"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"Natural Hazard Strategy","This strategy has been developed on behalf of both Ergon Energy Network and Energex. \nIt details planning and preparation activities critical to providing Queensland with a reliable network where\ndisruptions are minimised during natural hazard events","All Opex / All Capex","No"]
[null,"Bushfire Risk Management Plan","This Bushfire Risk Management Plan is a subset of the Summer Preparedness Plan and targets issues and initiatives relating specifically to bushfires.","All Opex / All Capex","No"]
[null,"Emergency Management Plan (EMP) - Distribution Network","This Emergency Management Plan (EMP) provides the direction for emergency response arrangements in response to emergency events on the Distribution Network. It details the higher level framework and processes to be applied by Energex and Ergon Energy Network when responding to a Level 2 or Level 3 event which disrupts or has the potential to disrupt the supply and distribution of electricity, or the provision of related services to customers and communities. This plan is supported by other detailed processes as referenced throughout the document.","All Opex / All Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"Manage Level 2 Emergency - Severe Weather ","The procedure for extreme weather events that have potential to affect the Energex network (covers Thunderstorms, Winds, Rain and Hot Weather that is likely to result in possible overloads).","Emergency response (Opex)","No"]

{"sheet":"7.2 Contingent projects","index":24,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.2 CONTINGENT PROJECTS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($, nominal)\")","v":"Proposed annual revenue requirement for 2025-26 \n($, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2025-26"}]
[null,null,null,null,null,{"$f":"+E9*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$9","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":25,"n_rows":296,"n_cols":5,"rows_kept":296,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"Electricity - National Scheme (Qld) Act 1997","This legislation provides that the National Electricity Law (NEL) and the National Electricity Rules (NER) apply as a law of Queensland","All","No"]
[null,"National Electricity Law","Electricity distribution entities have a large number of obligations under the NEL. The most significant obligations are to: register with AEMO as a \"Registered Participant\"; comply with the distribution determination that applies to the electricity distribution network services provided; provide the AER with the necessary information or prepare, maintain or keep the information as is requested by the AER in either a \"relevant notice\" or a \"regulatory information instrument\"; provide information to the AER for the purpose of the preparation of a NSP's performance or financial report; comply with the guidelines established by AEMO in relation to the shedding and restoration of loads in order to ensure the safety and security of the National Electricity System; comply with a wide range of obligations relating to the determination and resolution of access disputes, as well as to the restrictions on, variation of and compliance with access determinations; and comply with the general obligation not to prevent or hinder the access of another person to a regulated network service.","All","No"]
[null,"National Electricity Rules and subordinate Regulations","These Rules and Regulations are made under the NEL and set out the rights and obligations of participants in the NEM, AEMO as market operator, and the market institutions. This includes connections, planning and expansion, economic regulation, metering and transitional requirements. It also includes all procedures established under the Rules.","All","No"]
[null,"National Energy Retail Law (NERL)","The NERL establishes the NECF which is focussed on the sale and supply of energy to residential and small business customers. ","ACS, Connection Policy","No"]
[null,"National Energy Retail Rules (NERR)","The NERR are made under the NERL and provide the detailed content of the consumer protection measures and model contracts that govern the relationships between customers, retailers and distributors. ","Connection Policy, ACS\n","No"]
[null,"National Energy Retail Law (Qld) Act 2014","This legislation proivdes that the National Energy Retail Law (South Australia) Act applies as an Act in Queensland and provides the Queensland derogations from the national law as a schedule.","Connection Policy, ACS\n","No"]
[null,"National Energy Retail Law (Qld) Regulation 2014","This legislation provides the Queensland derogations to the NERR, including protections specific to consumers in regional and remote Queensland.","Connection Policy, ACS\n","No"]
[null,"Electricity Act 1994 (Qld)","The key obligations of an electricity distribution entity under this Act are to:  comply with the provisions of the National Electricity (Queensland) Law and the National Electricity Rules; operate, maintain and protect its supply network to ensure the adequate, economic, reliable and safe connection and supply of electricity; properly take into account the environmental effects of its activities; consider both demand and supply side options to provide for the efficient supply of electricity; pay the amounts required under the authority or regulations for administering the authority and its conditions; and pay any amount that, under the Energy and Water Ombudsman Act 2006, it is required to pay the Energy Ombudsman.","All Capex and All Opex;\nConnection Policy","No"]
[null,"Electricity Regulation 2006 (Qld)","The Regulation sets out a number of provisions which impose specific obligations on electricity distribution entities including: prescribing standards and procedures for the design, building and maintenance of electric lines and works; prescribing standards and procedures for the measurement of energy efficiency and the performance of electrical equipment; specifying caps on fees for certain services; and providing for GOEindustry  employee leave, award and allowance entitlements.","All Capex and All Opex","No"]
[null,"Electrical Safety Act 2002 (Qld) ","Electrical distribution entities are required to comply with all relevant provisions under this Act, with the most specific obligation being the responsibility to ensure that all electricity inspection, testing and maintenance works are operated in a way that is electrically safe. ","All Capex and All Opex","No"]
[null,"Electrical Safety Regulation 2013 (Qld) ","This Regulation identifies specific ways for an electricity entity to meet its obligations under the Electrical Safety Act 2002. The provisions of the Regulation include: safety and technical requirements for electrical work and equipment and the works of electrical entities; safety and technical requirements for work in contact with or near exposed parts; requirements for the development of safety management plans; notification and reporting requirements for electrical incidents and dangerous electrical events; all matters concerning electrical licences and electrical licensing provisions; approvals of electrical equipment; and administrative matters.  ","All Capex and All Opex","No"]
[null,"Work Health and Safety Act 2011 (Qld)","This Act details Energex's obligations in relation to having appropriate health and safety standards at its place of business to ensure the safety of its employees and other persons.  Energex must provide and maintain a safe and healthy work environment, provide and maintain safe plant, ensure a safe system of work and provide information, instruction, training and supervision to ensure health and safety.  The Work Health and Safety Act does not apply to circumstances where the Electrical Safety Act applies.","All Capex and All Opex","No"]
[null,"Work Health and Safety Regulation 2011 (Qld)","This instrument provides a framework for health and safety of workers and workplaces.","All","No"]
[null,"Workers Compensation and Rehabilitation Act 2003 (Qld)","Under this Act, Energex, as a registered Queensland business, is legally liable for compensation for injury sustained by a worker. Given the inherently dangerous nature of electricity distribution field operations, Energex is likely to have significantly higher compliance costs under this legislation than a typical Queensland business.","All","No"]
[null,"Workers Compensation and Rehabilitation Regulation 2014 (Qld) ","This Regulation sets out the legal requirements for the workers compensation scheme defined under the Workers Compensation and Rehabilitation Act 2003.  All organisations operating in Queensland, including an electricity distribution entity are obliged to comply with all provisions under this Regulation. ","Opex","No"]
[null,"Energy and Water Ombudsman Act 2006 (Qld) and subordinate Regulation","Establishes an independent dispute resolution mechanism for small customers who have a complaint about their energy supply.","Opex","No"]
[null,"National Greenhouse and Energy Reporting Act 2007 (Cth)","Establishes the framework for the reporting and dissemination of information related to greenhouse gas emissions, greenhouse gas projects, energy consumption and energy production of corporations.","All","No"]
[null,"Environment Protection and Biodiversity Conservation Act 1999 (Cth) and associated Regulation","The objects of this Act include, among other things, protection of the environment; promotion of ecologically sustainable development and biodiversity conservation; and provision for the protection and conservation of heritage.","All","No"]
[null,"Environmental Protection Act 1994 (Qld) and subordinate legislation","This legislation is relevant to Energex in terms of the environmental considerations that must be taken into account in constructing, operating and maintaining distribution network infrastructure.  This entails regular monitoring of environmental exposures and review of incident trends, as well as ensuring compliance with environmental regulations as part of an ongoing internal Environmental Management System.  Distribution entities are also required to comply with the framework established under the Act for the environmental evaluation of individual projects.  If the administering authority believes that an event or activity is causing or likely to cause environmental harm, it can require the responsible entity to either undertake or commission an environmental investigation into the activity and submit an accompanying report.  Electricity distribution entities are also required under the Act to obtain approvals prior to engaging in certain activities.","All","No"]
[null,"Nature Conservation Act 1992 and subordinate legislation (Qld)","The operation of an electricity supply network is classified as a \"service facility\" under the Nature Conservation Act and as such may be granted permission to operate on land situated in a national park.  This legislation provides the framework under which an electricity distribution entity must operate in order to obtain permission to construct distribution network infrastructure on land lying inside national park boundaries. The Act also regulates the taking of protected plants, protected animals and tampering with animal breeding places.","All","No"]
[null,"Native Title Act 1993 (Cth)","This Act provides for the recognition and protection of native title; establishes ways in which future dealings affecting native title may proceed and to set standards for those dealings; establishes a mechanism for determining claims to native title; and provides for, or permits, the validation of past acts, and intermediate period acts, invalidated because of the existence of native title.\n","All","No"]
[null,"Aboriginal Cultural Heritage Act 2003 (Qld) and Torres Strait Islander Cultural Heritage Act 2003 (Qld)","The main purpose of these Acts is to provide effective recognition, protection and conservation of Aboriginal and Torres Strait Islander cultural heritage.\n","All","No"]
[null,"Queensland Heritage Act 1992 (Qld) \nQueensland Heritage Regulation 2015 (Qld)","The obligations of an electricity distribution entity in relation to this legislation relate to the planning of expansions to its distribution network.  Distribution entities must take the provisions of this Act into account when planning an expansion project that has the potential to impact on an area that is registered as a heritage location under this Act.  Distribution entities must also follow the requirements outlined in the Act when applying to enter an area classified as a protected area.","All","No"]
[null,"Vegetation Management Act 1999 (Qld)\nVegetation Management Regulation 2012","Deals with various aspects of clearing, conservation and management of native vegetation.","Opex - Vegetation Management","No"]
[null,"Coastal Protection and Management Act 1995 (Qld) and associated regulation","The main objects of this Act are to: provide for the protection, conservation, rehabilitation and management of the coast, including its resources and biological diversity; and have regard to the goal, core objectives and guiding principles of the National Strategy for Ecologically Sustainable Development in the use of the coastal zone; and provide, in conjunction with other legislation, a coordinated and integrated management and administrative framework for the ecologically sustainable development of the coastal zone; and encourage the enhancement of knowledge of coastal resources and the effect of human activities on the coastal zone. ","All","No"]
[null,"Planning Act 2016 (Qld) and associated Regulation","In order to ensure compliance with the provisions of this Act, a distribution entity must consider and attempt to minimise, where practicable, any adverse environmental impacts of its network expansion programs. Under the Act, construction of new electricity infrastructure often requires a full impact assessment involving public consultation and negotiation. To accommodate the longer project delivery times due to such assessments, demand forecasting and project planning must often be initiated earlier than would otherwise be required.  There may also be implications for cost and timing of construction of infrastructure due to design requirements imposed under planning approvals.","All","No"]
[null,"State Development and Public Works Organisation Act 1971 (Qld)","Energex is obligated under this Act to cooperate with the Coordinator-General and provide information upon request to assist in the planning process for the Queensland Government's program of works.  ","All","No"]
[null,"Acquisition of Land Act 1967 (Qld)\nAcquisition of Land Regulation 2014 (Qld)","Electricity distribution entities are required to comply with all obligations under the Act relating to the acquiring of land for the purpose of constructing an easement and the payment of compensation to the holder of the land over which an easement is to be constructed.","All","No"]
[null,"Land Act 1994 (Qld)","There are a large number of specific obligations that a DNSP is required to comply with under this Act relating to the registration and administration of easements. ","All","No"]
[null,"Land Title Act 1994 (Qld)","The obligations upon a DNSP under this legislation relate to the registration and administration of easements and are broadly similar to its obligations under the Land Act 1994. ","All","No"]
[null,"Fire and Emergency Services Act 1990 (Qld)","This Act provide for the prevention of, and responses to, fires and other emergency incidents; provides for rescue services and operations; and establishes a framework for the management of the Queensland Fire and Emergency Service, the State Emergency Service, emergency service units established for an emergency service area, and the conduct of authorised rescue officers.","All","No"]
[null,"Building Fire Safety Regulation 2008 (Qld)","This instrument provdes a framework for safe evacuation of buildings and fire safety installations in buildings.","All","No"]
[null,"Government Owned Corporations Act 1993 (Qld)","This Act makes provision for a structural reform process (corporatisation) for nominated government entities.","All","No"]
[null,"Queensland Competition Authority Act 1997 (Qld)","The key ongoing obligation of Energex under this Act is to report to the QCA in accordance with the Electricity Distribution Network Code.  Part 3 (pricing practices relating to monopoly business activities) and Part 5 (access to services) of the Act are potentially applicable to Energex but do not impose ongoing obligations. ","All","No"]
[null,"Corporations Act 2001 (Cth)","This Act is the principal legislation regulating companies in Australia. It regulates matters such as the formation and operation of companies (in conjunction with a constitution that may be adopted by a company), duties of officers, takeovers and fundraising.","All","No"]
[null,"Financial Accountability Act 2009 (Qld)","The Financial Accountability Act 2009 sets out the principles to be observed by all Queensland public sector agencies in relation to their financial management.","All","No"]
[null,"Income Tax Assessment Act 1936 (Cth)\nIncome Tax Assessment Act 1997 (Cth)\nFringe Benefits Tax Assessment Act 1986 (Cth)\nA New Tax System (Goods and Service Tax) Act 1999 (Cth)","These instruments provide a framework for the treatment of income tax, fringe benefits tax, and goods and services tax.","All","No"]
[null,"Tax Administration Act 1953","The TAA and regulations made under it, contain provisions dealing with the administration of tax laws (including GST) by, and the powers of, the ATO.  The TAA has become increasingly important because it contains the PAYG withholding regimes and the generic provisions for tax administration including dealing with penalties for breaches of various tax laws.","All","No"]
[null,"Payroll Tax Act 1971 (Qld), Payroll Tax Act 2007 Act 21 of 2007 (NSW Consolidated Acts), Payroll Tax Act 2007 (Victorian Current Acts), Payroll Tax Act 2009 (South Australia)","Payroll Tax is a state impost controlled by eight separate legislatures. Accordingly, the requirements, liabilities and rates of tax vary from state to state.The legislation in each state broadly provides for payroll tax to be levied on \"wages\", in cash or in kind, provided by employers to employees.","All","No"]
[null,"Competition and Consumer Act 2010 (Cth)","The object of this Act is to enhance the welfare of Australians through the promotion of competition and fair trading and provision for consumer protection.\n","All","No"]
[null,"Fair Trading Act 1989 (Qld)","The principal objective of this Act is to improve consumer wellbeing through consumer empowerment and protection, fostering effective competition and enabling the confident participation of consumers in markets in which both consumers and suppliers trade fairly.","All","No"]
[null,"Privacy Act 1988 (Cth)","Energex is an organisation which is subject to the provisions of the Privacy Act 1988 and the Australian Privacy Principles for the protection of privacy of individuals and the responsible and transparent handling of personal information.  The Act also sets out a procedure for individuals to complain about privacy breaches.\n\n","Non Network Opex and Capex; Overheads","No"]
[null,"Public Records Act 2002 (Qld)","The main purposes of this Act are to ensure—\n(a) the public records of Queensland are made, managed, kept and, if appropriate, preserved in a useable form for the benefit of present and future generations; and\n(b) public access to records under this Act is consistent with the principles of the Right to Information Act 2009 and the Information Privacy Act 2009.","Non Network Opex and Capex; Overheads","No"]
[null,"Right to Information Act 2009 (Qld)","The public has a right of access to certain information in Energex's possession or control,  unless, on balance, it is contrary to the public interest to give the access.  The Act sets out the procedural steps for releasing information to the public, including when access to information may be refused.","Non Network Opex and Capex; Overheads","No"]
[null,"Information Privacy Act 2009 (Qld)","Contains a set of rules or ‘privacy principles’ that govern how Energex collects, stores, uses and discloses personal information. The Act also allows an individual to make a complaint about an agency's breach of the privacy principles.","Non Network Opex and Capex; Overheads","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"Distribution Authority","The Queensland Regulator (the Department of Energy and Public Works) has issued Energex a Distribution Authority in accordance with the Electricity Act 1994 (Qld)","All","No"]
[null,"Electrical Worker's Licence","Issued to Qualified Technical Person for Energex in accordance with the Electrical Safety Act 2002 (Qld)","All","No"]
[null,"Electrical Contractor's Licence","Issued to Energex Responsible Person in accordance with the Electrical Safety Act 2002 (Qld)","All","No"]
[]
[null,"RULES"]
[null,"National Electricity Rules","These Rules are made under the NEL and set out the rights and obligations of Registered Participants in the NEM, AEMO as market operator, and the market institutions. This includes connections, planning and expansation, economic regulation and transitional requirements. It also includes all procedures established under the Rules.","All","No"]
[null,"National Energy Retail Rules (NERR)","The NERR are made under the National Energy Retail Law and provide the detailed content of the consumer protection measures and model contracts that govern the relationships between customers, retailers and distributors. ","ACS, Connection Policy","No"]
[null,"Market Settlement and Transfer Solution (MSATS) Procedures","Energex is required to comply with various MSATS Procedures including Consumer Administration and Transfer Solution (CATS) Procedures Principles and Obligations; Wholesale, Interconnector, Generator and Sample (WIGS) NMI; and Meter Data Management (MDM) Procedures","All","No"]
[null,"See Tab Additional info 7.3"]
[null,"ORDERS"]
[null,"Regulatory Information Notice","The AER issued a RIN for Energex on 11 October 20223 in accordance with Division 4 of Part 3 of the National Electricity (QLD) Law (NEL).","Reset RIN","No"]
[]
[]
[null,"CODES"]
[null,"Electricity Distribution Network Code (EDNC)","The EDNC has been made under the Electricity Act 1994 and contains a wide range of obligations that impact on Energex's operations.","All","No"]
[null,"Traffic Management for Construction or Maintenance Work Code of Practice 2008","This Code provides advice about how to manage risks associated with working on, or adjacent to, a roadway.","All","No"]
[null,"Managing electrical risks in the workplace Code of Practice 2021","This Code gives practical advice on ways to manage electrical risk when working near exposed live parts.  It applies to Energex as an electricity entity and an employer. It also provides benchmarks for ensuring that electrical work (live and de-energised) is performed in ways that are electrically safe.  It also provides guidance on electrical risk.  As such, it applies to Energex's operations.","All","No"]
[null,"Electrical safety code of practice 2020 Works","This Code gives advice on ways for an electricity entity to manage electrical safety risks associated with earthing systems, underground cable systems and supporting structures for overhead lines forming part of the works of an electricity entity.  As such, this Code applies to Energex's operations.","All","No"]
[null,"How to manage and control asbestos in the workplace Code of Practice 2021","This is a national code of practice that has been developed to assist persons in control of premises to control the risks of asbestos-containing materials in workplaces.  This Code applies to parts of Energex's operations in terms of asset management.","All","No"]
[null,"How to safely remove asbestos Code of Practice 2021","The purpose of this Code is to provide advice for the safe removal of asbestos and asbestos-containing material from buildings and structures, plant and equipment and vehicles.  This Code applies to Energex in terms of asset management.","All","No"]
[null,"Electrical Safety Code of Practice 2020 - Working near overhead and underground electric lines","A person conducting a business or undertaking at a workplace is required to comply with the requirements of this Code to ensure that no person, plant or thing comes within an unsafe distance (exclusion zone) of an overhead electric line.","All","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"Framework and Approach","The AER issued its Framework and Approach for Energex in accordance with clause 6.8.1 of the NER on 3 July 2023","All","No"]
[null,"Distribution Annual Planning Report","Clause 5.13.2(b) of the NER requires each DNSP to publish a DAPR by the DAPR date each year, setting out the results of the distribution annual planning review for the forward planning period.","All Capex / All Opex","No"]
[null,"Cost Allocation Guideline (Distribution)","This guideline oulines the required content of Energex's cost allocation method and the basis on which the AER will assess that method for approval.","Overheads","No"]
[null,"Regulatory Investment Test for Distribution (RIT-D)","The RIT-D is required for all investment decisions (subject to a number of exclusions) to identify the credible option that maximises the present value of the net economic benefit to all those who produce, consume and transport electricity in the NEM, in accordance with clause 5.17 of the NER.","All Capex / All Opex","No"]
[null,"Ring-fencing Guideline","This guideline details Energex's obligations and related compliance reporting requirements","All","No"]
[null,"Expenditure Forecast Assessment Guideline","This guideline describes the process, techniques and associated data requirements for the AER's approach to setting efficient expenditure allowances for network businesses, in accordance with clause 6.2.8 of the NER.","All Capex / All Opex","No"]
[null,"Rate of Return Instrument","The Rate of Return Instrument sets out how the AER will determine the return that electricity and gas network businesses can earn on their investments, in accordance with clause 6.2.8 of the NER.","Rate of return","No"]
[null,"Expenditure Incentives Guideline","This guideline gives electricity network businesses incentives to spend efficiently and share the benefits of efficiencies with consumers, in accordance with clause 6.2.8 of the NER.","Expenditure incentives","No"]
[null,"Better Resets Handbook","The Handbook sets out the way the AER will undertake its revenue determinations, placing greater emphasis on high quality consumer engagement and providing more clarity on what the AER consider what would be in a proposal that is capable of acceptance.","All","No"]
[null,"Shared Asset Guideline","This guideline outlines how consumers will benefit from the other services electricity network businesses may provide using the assets consumers pay for, in accordance with clause 6.2.8 of the NER.","All","No"]
[null,"Confidentiality Guideline","The confidentiality guideline sets out how energy network businesses must make confidentiality claims over information they submit to the AER. The guideline balances protecting genuinely confidential information with ensuring that stakeholders can access sufficient information on issues affecting their interests, in accordance with clause 6.2.8 of the NER.","All","No"]
[null,"Post Tax Revenue Model (PTRM)","The PTRM will be used by the AER to determine the maximum allowed revenue to be earned by a network service provider over a regulatory control period. The AER has issued a PTRM and an associated PTRM Handbook.","Revenue","No"]
[null,"Roll Forward Model (RFM)","The RFM will be used by the AER to determine the closing regulated asset base for a regulatory control period. The AER has issued a RFM and associated RFM handbook.","Capex, RAB","No"]
[null,"Service Target Performance Incentive Scheme (STPIS)","The STPIS is designed to ensure DNSPs improve efficiency without a deterioration in service performance for customers, and improving service performance where customers are willing to pay for these improvements, in accordance with clause 6.6.2 of the NER.","STPIS - reliability targets","No"]
[null,"Efficiency Benefit Sharing Scheme (EBSS)","The EBSS should provide for a fair sharing between DNSPs and network users of efficiency gains and efficiency losses in accordance with clause 6.5.8 of the NER.","EBSS","No"]
[null,"Capital Expenditure Sharing Scheme (CESS)","The CESS provides financial rewards for DNSPs whose capex becomes more efficient and imposes financial penalties for those that become less efficient. Consumers benefit from improved efficiency through lower regulated prices, in accordance with clause 6.5.8A of the NER.","CESS","No"]
[null,"Demand Management Incentive Scheme (DMIS) and Demand Management Innovation Allowance Mechansim (DMIAM)","The DMIS provides DNSPs with an incentive to undertake efficient expenditure on non-network options relating to demand management. The separate DMIA provides DNSPs with funding for research and development in demand management projects that have the potential to reduce long term network costs.","DMIS and DMIA","No"]
[null,"Cost Allocation Method","The AER has approved the Cost Allocation Method that Energex submitted to it in accordance with the Cost Allocation Guidelines and clause 6.15 of the NER. This document will be used by Energex for the purposes of attributing costs to, or allocating costs between, its Distribution Services, and other unregulated activities within the Energex Group.","Overheads","No"]
[null,"Connection Charge Guideline","This guideline sets out how DNSPs should charge electricity customers for connection services. ","Connection Policy","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[null,"Standard Coordination Agreement (Annexure A, ENDC)","This is a deemed agreement that applies between Energex and any retailer with whom we have a common customer. The agreement defines the way in which the parties will discharge their respective obligations to customers and establishes common protocols for communicating customer information, in circumstances where a Negotiated Coordination Agreement has not been entered into.","All","No"]
[]
[]
[null,"OTHER"]
[null,"Negotiated Coordination Agreement ","Energex can negotiate with any retailer with whom it has a common customer. The agreement defines the terms and conditions under which the parties will discharge their respective obligations to customers and establish common protocols for communicating customer information.","All","No"]

{"sheet":"Additional Info 7.3","index":26,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":false,"merged":[[1,0,2,0]]}
["7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
["RULES"]
["Business to Business (B2B) Procedures","Comply with B2B procudures including Customer and Site Details Notification Process; Service Order Process; and Meter Data Process","All","No"]
["Queensland B2B Process Specification: Network Billing","This document describes the automation of the network billing process, its associated transactions and the associated business rules. ","All","No"]
["Retailer Handbook: Operating Procedures","This document defines the standard protocols for communication and transactions between Energex and retailers operating within its distribution area. In the Standard Coordination Agreement it is known as the Operational Procedures.","Connection Policy, ACS\n","No"]

{"sheet":"7.4 Shared Assets","index":27,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8],[30,2,30,8],[31,2,31,8],[32,2,32,8],[39,2,39,8],[40,2,40,8],[7,1,8,1],[7,2,8,2],[27,2,27,8],[28,2,28,8],[29,2,29,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.4 SHARED ASSETS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service",{"$f":"CONCATENATE(\"Shared asset unregulated revenue  \n($, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", FRCP_y5)","v":"Total 2025-26 to 2029-30"}]
[null,"License fee for use of Energex electricty distribution network assets","Energex owned electricity distribution network assets comprising of aerial transmission towers, distribution wood poles, public lighting columns and underground conduit and pit networks (used to support telephone or fibre optic cable for communication services for example)",9654421.9506021608,9341509.6242097877,9073850.8832816854,8826721.9868854787,8586323.7159116641,8352472.7598723266,8124990.8007925553,{"$f":"SUM(F10:J10)","v":42964360.146743707}]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]

{"sheet":"7.7 TSS-LRMC","index":28,"n_rows":155,"n_cols":22,"rows_kept":155,"cut":false,"hidden":false,"merged":[[69,1,70,1],[89,1,90,1],[6,3,7,4],[11,1,12,1],[23,1,24,1],[35,1,36,1],[49,1,50,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is Energex using the 'Average Incremental Cost' approach?"}]
[null,null,null,null,null,"YES"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C13,4)+1)&\"-\"&MID(C13,3,2)+2),VALUE(LEFT(C13,4)+1))","v":"2024-25"},"2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42","2042-43"]
[null,"Replacement expenditure"]
[null,"Connections",3169320.1261320636,3053738.7832702571,3173740.049626823,3282126.1093403823,3397328.2189847874,3517454.5403771866,3517454.5403771866,3517454.5403771866,3517454.5403771866,3517454.5403771866]
[null,"Augmentation Expenditure",12431958.689999999,21021448.120000001,21606322.968734007,16459116.874808572,20266875.42347436,18707367.626390036,29201722.051391348,21409225.387645256,21409225.387645256,21409225.387645256]
[null,"Non-network"]
[null,"Export services",9000000,9000000,11656697.77,23714797.879999999,15311197.92,17409208.84,18009955.049999997,16500000,12000000,12500000]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C14:C20)","v":24601278.816132061},{"$f":"SUM(D14:D20)","v":33075186.903270259},36436760.788360834,43456040.864148952,38975401.562459148,39634031.006767228,50729131.64176853,41426679.928022444,36926679.928022444,37426679.928022444,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C25,4)+1)&\"-\"&MID(C25,3,2)+2),VALUE(LEFT(C25,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D25,4)+1)&\"-\"&MID(D25,3,2)+2),VALUE(LEFT(D25,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E25,4)+1)&\"-\"&MID(E25,3,2)+2),VALUE(LEFT(E25,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F25,4)+1)&\"-\"&MID(F25,3,2)+2),VALUE(LEFT(F25,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G25,4)+1)&\"-\"&MID(G25,3,2)+2),VALUE(LEFT(G25,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H25,4)+1)&\"-\"&MID(H25,3,2)+2),VALUE(LEFT(H25,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I25,4)+1)&\"-\"&MID(I25,3,2)+2),VALUE(LEFT(I25,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J25,4)+1)&\"-\"&MID(J25,3,2)+2),VALUE(LEFT(J25,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K25,4)+1)&\"-\"&MID(K25,3,2)+2),VALUE(LEFT(K25,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L25,4)+1)&\"-\"&MID(L25,3,2)+2),VALUE(LEFT(L25,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M25,4)+1)&\"-\"&MID(M25,3,2)+2),VALUE(LEFT(M25,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N25,4)+1)&\"-\"&MID(N25,3,2)+2),VALUE(LEFT(N25,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O25,4)+1)&\"-\"&MID(O25,3,2)+2),VALUE(LEFT(O25,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P25,4)+1)&\"-\"&MID(P25,3,2)+2),VALUE(LEFT(P25,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q25,4)+1)&\"-\"&MID(Q25,3,2)+2),VALUE(LEFT(Q25,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R25,4)+1)&\"-\"&MID(R25,3,2)+2),VALUE(LEFT(R25,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S25,4)+1)&\"-\"&MID(S25,3,2)+2),VALUE(LEFT(S25,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T25,4)+1)&\"-\"&MID(T25,3,2)+2),VALUE(LEFT(T25,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U25,4)+1)&\"-\"&MID(U25,3,2)+2),VALUE(LEFT(U25,4)+1))","v":"2042-43"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C26:C32)","v":0},{"$f":"SUM(D26:D32)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C37,4)+1)&\"-\"&MID(C37,3,2)+2),VALUE(LEFT(C37,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D37,4)+1)&\"-\"&MID(D37,3,2)+2),VALUE(LEFT(D37,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E37,4)+1)&\"-\"&MID(E37,3,2)+2),VALUE(LEFT(E37,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F37,4)+1)&\"-\"&MID(F37,3,2)+2),VALUE(LEFT(F37,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G37,4)+1)&\"-\"&MID(G37,3,2)+2),VALUE(LEFT(G37,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H37,4)+1)&\"-\"&MID(H37,3,2)+2),VALUE(LEFT(H37,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I37,4)+1)&\"-\"&MID(I37,3,2)+2),VALUE(LEFT(I37,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J37,4)+1)&\"-\"&MID(J37,3,2)+2),VALUE(LEFT(J37,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K37,4)+1)&\"-\"&MID(K37,3,2)+2),VALUE(LEFT(K37,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L37,4)+1)&\"-\"&MID(L37,3,2)+2),VALUE(LEFT(L37,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M37,4)+1)&\"-\"&MID(M37,3,2)+2),VALUE(LEFT(M37,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N37,4)+1)&\"-\"&MID(N37,3,2)+2),VALUE(LEFT(N37,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O37,4)+1)&\"-\"&MID(O37,3,2)+2),VALUE(LEFT(O37,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P37,4)+1)&\"-\"&MID(P37,3,2)+2),VALUE(LEFT(P37,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q37,4)+1)&\"-\"&MID(Q37,3,2)+2),VALUE(LEFT(Q37,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R37,4)+1)&\"-\"&MID(R37,3,2)+2),VALUE(LEFT(R37,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S37,4)+1)&\"-\"&MID(S37,3,2)+2),VALUE(LEFT(S37,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T37,4)+1)&\"-\"&MID(T37,3,2)+2),VALUE(LEFT(T37,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U37,4)+1)&\"-\"&MID(U37,3,2)+2),VALUE(LEFT(U37,4)+1))","v":"2042-43"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C37:C43)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C51,4)+1)&\"-\"&MID(C51,3,2)+2),VALUE(LEFT(C51,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D51,4)+1)&\"-\"&MID(D51,3,2)+2),VALUE(LEFT(D51,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E51,4)+1)&\"-\"&MID(E51,3,2)+2),VALUE(LEFT(E51,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F51,4)+1)&\"-\"&MID(F51,3,2)+2),VALUE(LEFT(F51,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G51,4)+1)&\"-\"&MID(G51,3,2)+2),VALUE(LEFT(G51,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H51,4)+1)&\"-\"&MID(H51,3,2)+2),VALUE(LEFT(H51,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I51,4)+1)&\"-\"&MID(I51,3,2)+2),VALUE(LEFT(I51,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J51,4)+1)&\"-\"&MID(J51,3,2)+2),VALUE(LEFT(J51,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K51,4)+1)&\"-\"&MID(K51,3,2)+2),VALUE(LEFT(K51,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L51,4)+1)&\"-\"&MID(L51,3,2)+2),VALUE(LEFT(L51,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M51,4)+1)&\"-\"&MID(M51,3,2)+2),VALUE(LEFT(M51,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N51,4)+1)&\"-\"&MID(N51,3,2)+2),VALUE(LEFT(N51,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O51,4)+1)&\"-\"&MID(O51,3,2)+2),VALUE(LEFT(O51,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P51,4)+1)&\"-\"&MID(P51,3,2)+2),VALUE(LEFT(P51,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q51,4)+1)&\"-\"&MID(Q51,3,2)+2),VALUE(LEFT(Q51,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R51,4)+1)&\"-\"&MID(R51,3,2)+2),VALUE(LEFT(R51,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S51,4)+1)&\"-\"&MID(S51,3,2)+2),VALUE(LEFT(S51,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T51,4)+1)&\"-\"&MID(T51,3,2)+2),VALUE(LEFT(T51,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U51,4)+1)&\"-\"&MID(U51,3,2)+2),VALUE(LEFT(U51,4)+1))","v":"2042-43"}]
[null,"Opex for import",149772.2766348678,231121.79427139446,237888.60497626394,189515.93264782993,227176.35496760777,213358.29280096531,314104.0952809779,239296.12730901552,239296.12730901552,239296.12730901552]
[null,"Opex for export",90000,90000,116566.97769999999,237147.97879999998,153111.9792,174092.08840000001,180099.55049999998,165000,120000.00000000001,125000]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C52:C66)","v":239772.2766348678},{"$f":"SUM(D52:D66)","v":321121.79427139449},354455.58267626393,426663.91144782992,380288.33416760777,387450.38120096532,494203.64578097791,404296.12730901549,359296.12730901554,364296.12730901549,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C71,4)+1)&\"-\"&MID(C71,3,2)+2),VALUE(LEFT(C71,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D71,4)+1)&\"-\"&MID(D71,3,2)+2),VALUE(LEFT(D71,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E71,4)+1)&\"-\"&MID(E71,3,2)+2),VALUE(LEFT(E71,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F71,4)+1)&\"-\"&MID(F71,3,2)+2),VALUE(LEFT(F71,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G71,4)+1)&\"-\"&MID(G71,3,2)+2),VALUE(LEFT(G71,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H71,4)+1)&\"-\"&MID(H71,3,2)+2),VALUE(LEFT(H71,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I71,4)+1)&\"-\"&MID(I71,3,2)+2),VALUE(LEFT(I71,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J71,4)+1)&\"-\"&MID(J71,3,2)+2),VALUE(LEFT(J71,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K71,4)+1)&\"-\"&MID(K71,3,2)+2),VALUE(LEFT(K71,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L71,4)+1)&\"-\"&MID(L71,3,2)+2),VALUE(LEFT(L71,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M71,4)+1)&\"-\"&MID(M71,3,2)+2),VALUE(LEFT(M71,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N71,4)+1)&\"-\"&MID(N71,3,2)+2),VALUE(LEFT(N71,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O71,4)+1)&\"-\"&MID(O71,3,2)+2),VALUE(LEFT(O71,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P71,4)+1)&\"-\"&MID(P71,3,2)+2),VALUE(LEFT(P71,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q71,4)+1)&\"-\"&MID(Q71,3,2)+2),VALUE(LEFT(Q71,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R71,4)+1)&\"-\"&MID(R71,3,2)+2),VALUE(LEFT(R71,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S71,4)+1)&\"-\"&MID(S71,3,2)+2),VALUE(LEFT(S71,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T71,4)+1)&\"-\"&MID(T71,3,2)+2),VALUE(LEFT(T71,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U71,4)+1)&\"-\"&MID(U71,3,2)+2),VALUE(LEFT(U71,4)+1))","v":"2042-43"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C72:C86)","v":0},{"$f":"SUM(D72:D86)","v":0},{"$f":"SUM(E72:E86)","v":0},{"$f":"SUM(F72:F86)","v":0},{"$f":"SUM(G72:G86)","v":0},{"$f":"SUM(H72:H86)","v":0},{"$f":"SUM(I72:I86)","v":0},{"$f":"SUM(J72:J86)","v":0},{"$f":"SUM(K72:K86)","v":0},{"$f":"SUM(L72:L86)","v":0},{"$f":"SUM(M72:M86)","v":0},{"$f":"SUM(N72:N86)","v":0},{"$f":"SUM(O72:O86)","v":0},{"$f":"SUM(P72:P86)","v":0},{"$f":"SUM(Q72:Q86)","v":0},{"$f":"SUM(R72:R86)","v":0},{"$f":"SUM(S72:S86)","v":0},{"$f":"SUM(T72:T86)","v":0},{"$f":"SUM(U72:U86)","v":0},{"$f":"SUM(V72:V86)","v":0}]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C91,4)+1)&\"-\"&MID(C91,3,2)+2),VALUE(LEFT(C91,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D91,4)+1)&\"-\"&MID(D91,3,2)+2),VALUE(LEFT(D91,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E91,4)+1)&\"-\"&MID(E91,3,2)+2),VALUE(LEFT(E91,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F91,4)+1)&\"-\"&MID(F91,3,2)+2),VALUE(LEFT(F91,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G91,4)+1)&\"-\"&MID(G91,3,2)+2),VALUE(LEFT(G91,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H91,4)+1)&\"-\"&MID(H91,3,2)+2),VALUE(LEFT(H91,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I91,4)+1)&\"-\"&MID(I91,3,2)+2),VALUE(LEFT(I91,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J91,4)+1)&\"-\"&MID(J91,3,2)+2),VALUE(LEFT(J91,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K91,4)+1)&\"-\"&MID(K91,3,2)+2),VALUE(LEFT(K91,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L91,4)+1)&\"-\"&MID(L91,3,2)+2),VALUE(LEFT(L91,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M91,4)+1)&\"-\"&MID(M91,3,2)+2),VALUE(LEFT(M91,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N91,4)+1)&\"-\"&MID(N91,3,2)+2),VALUE(LEFT(N91,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O91,4)+1)&\"-\"&MID(O91,3,2)+2),VALUE(LEFT(O91,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P91,4)+1)&\"-\"&MID(P91,3,2)+2),VALUE(LEFT(P91,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q91,4)+1)&\"-\"&MID(Q91,3,2)+2),VALUE(LEFT(Q91,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R91,4)+1)&\"-\"&MID(R91,3,2)+2),VALUE(LEFT(R91,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S91,4)+1)&\"-\"&MID(S91,3,2)+2),VALUE(LEFT(S91,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T91,4)+1)&\"-\"&MID(T91,3,2)+2),VALUE(LEFT(T91,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U91,4)+1)&\"-\"&MID(U91,3,2)+2),VALUE(LEFT(U91,4)+1))","v":"2042-43"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C92:C106)","v":0},{"$f":"SUM(D92:D106)","v":0},{"$f":"SUM(E92:E106)","v":0},{"$f":"SUM(F92:F106)","v":0},{"$f":"SUM(G92:G106)","v":0},{"$f":"SUM(H92:H106)","v":0},{"$f":"SUM(I92:I106)","v":0},{"$f":"SUM(J92:J106)","v":0},{"$f":"SUM(K92:K106)","v":0},{"$f":"SUM(L92:L106)","v":0},{"$f":"SUM(M92:M106)","v":0},{"$f":"SUM(N92:N106)","v":0},{"$f":"SUM(O92:O106)","v":0},{"$f":"SUM(P92:P106)","v":0},{"$f":"SUM(Q92:Q106)","v":0},{"$f":"SUM(R92:R106)","v":0},{"$f":"SUM(S92:S106)","v":0},{"$f":"SUM(T92:T106)","v":0},{"$f":"SUM(U92:U106)","v":0},{"$f":"SUM(V92:V106)","v":0}]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C114,4)+1)&\"-\"&MID(C114,3,2)+2),VALUE(LEFT(C114,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D114,4)+1)&\"-\"&MID(D114,3,2)+2),VALUE(LEFT(D114,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E114,4)+1)&\"-\"&MID(E114,3,2)+2),VALUE(LEFT(E114,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F114,4)+1)&\"-\"&MID(F114,3,2)+2),VALUE(LEFT(F114,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G114,4)+1)&\"-\"&MID(G114,3,2)+2),VALUE(LEFT(G114,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H114,4)+1)&\"-\"&MID(H114,3,2)+2),VALUE(LEFT(H114,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I114,4)+1)&\"-\"&MID(I114,3,2)+2),VALUE(LEFT(I114,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J114,4)+1)&\"-\"&MID(J114,3,2)+2),VALUE(LEFT(J114,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K114,4)+1)&\"-\"&MID(K114,3,2)+2),VALUE(LEFT(K114,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L114,4)+1)&\"-\"&MID(L114,3,2)+2),VALUE(LEFT(L114,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M114,4)+1)&\"-\"&MID(M114,3,2)+2),VALUE(LEFT(M114,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N114,4)+1)&\"-\"&MID(N114,3,2)+2),VALUE(LEFT(N114,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O114,4)+1)&\"-\"&MID(O114,3,2)+2),VALUE(LEFT(O114,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P114,4)+1)&\"-\"&MID(P114,3,2)+2),VALUE(LEFT(P114,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q114,4)+1)&\"-\"&MID(Q114,3,2)+2),VALUE(LEFT(Q114,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R114,4)+1)&\"-\"&MID(R114,3,2)+2),VALUE(LEFT(R114,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S114,4)+1)&\"-\"&MID(S114,3,2)+2),VALUE(LEFT(S114,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T114,4)+1)&\"-\"&MID(T114,3,2)+2),VALUE(LEFT(T114,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U114,4)+1)&\"-\"&MID(U114,3,2)+2),VALUE(LEFT(U114,4)+1))","v":"2042-43"}]
[null,"Aggregated demand - all voltage levels (MW)",5536.6892681096579,5573.2885352990515,5601.7879543320169,5623.48753349246,5647.1870597785546,5677.28645339174,5705.4858894394229,5766.6846836065552,5833.4833196644577,5842.1831490499344]
[null,"Export capacity (MW)",910.38042199999859,1242.0694619999995,1559.0369539999995,1864.4008119999978,2166.6108089999993,2448.559444999999,2695.5200910000012,2892.1334270000011,3076.2752129999976,3254.6287619999989]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C115:C124)","v":-6447.0696901096562},{"$f":"-SUM(D115:D124)","v":-6815.357997299051},-7160.8249083320161,-7487.888345492458,-7813.7978687785544,-8125.845898391739,-8401.0059804394241,-8658.8181106065567,-8909.7585326644548,-9096.8119110499338,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C129,4)+1)&\"-\"&MID(C129,3,2)+2),VALUE(LEFT(C129,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D129,4)+1)&\"-\"&MID(D129,3,2)+2),VALUE(LEFT(D129,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E129,4)+1)&\"-\"&MID(E129,3,2)+2),VALUE(LEFT(E129,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F129,4)+1)&\"-\"&MID(F129,3,2)+2),VALUE(LEFT(F129,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G129,4)+1)&\"-\"&MID(G129,3,2)+2),VALUE(LEFT(G129,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H129,4)+1)&\"-\"&MID(H129,3,2)+2),VALUE(LEFT(H129,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I129,4)+1)&\"-\"&MID(I129,3,2)+2),VALUE(LEFT(I129,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J129,4)+1)&\"-\"&MID(J129,3,2)+2),VALUE(LEFT(J129,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K129,4)+1)&\"-\"&MID(K129,3,2)+2),VALUE(LEFT(K129,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L129,4)+1)&\"-\"&MID(L129,3,2)+2),VALUE(LEFT(L129,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M129,4)+1)&\"-\"&MID(M129,3,2)+2),VALUE(LEFT(M129,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N129,4)+1)&\"-\"&MID(N129,3,2)+2),VALUE(LEFT(N129,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O129,4)+1)&\"-\"&MID(O129,3,2)+2),VALUE(LEFT(O129,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P129,4)+1)&\"-\"&MID(P129,3,2)+2),VALUE(LEFT(P129,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q129,4)+1)&\"-\"&MID(Q129,3,2)+2),VALUE(LEFT(Q129,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R129,4)+1)&\"-\"&MID(R129,3,2)+2),VALUE(LEFT(R129,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S129,4)+1)&\"-\"&MID(S129,3,2)+2),VALUE(LEFT(S129,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T129,4)+1)&\"-\"&MID(T129,3,2)+2),VALUE(LEFT(T129,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U129,4)+1)&\"-\"&MID(U129,3,2)+2),VALUE(LEFT(U129,4)+1))","v":"2042-43"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C130:C139)","v":0},{"$f":"-SUM(D130:D139)","v":0},{"$f":"-SUM(E130:E139)","v":0},{"$f":"-SUM(F130:F139)","v":0},{"$f":"-SUM(G130:G139)","v":0},{"$f":"-SUM(H130:H139)","v":0},{"$f":"-SUM(I130:I139)","v":0},{"$f":"-SUM(J130:J139)","v":0},{"$f":"-SUM(K130:K139)","v":0},{"$f":"-SUM(L130:L139)","v":0},{"$f":"-SUM(M130:M139)","v":0},{"$f":"-SUM(N130:N139)","v":0},{"$f":"-SUM(O130:O139)","v":0},{"$f":"-SUM(P130:P139)","v":0},{"$f":"-SUM(Q130:Q139)","v":0},{"$f":"-SUM(R130:R139)","v":0},{"$f":"-SUM(S130:S139)","v":0},{"$f":"-SUM(T130:T139)","v":0},{"$f":"-SUM(U130:U139)","v":0},{"$f":"-SUM(V130:V139)","v":0}]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C144,4)+1)&\"-\"&MID(C144,3,2)+2),VALUE(LEFT(C144,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D144,4)+1)&\"-\"&MID(D144,3,2)+2),VALUE(LEFT(D144,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E144,4)+1)&\"-\"&MID(E144,3,2)+2),VALUE(LEFT(E144,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F144,4)+1)&\"-\"&MID(F144,3,2)+2),VALUE(LEFT(F144,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G144,4)+1)&\"-\"&MID(G144,3,2)+2),VALUE(LEFT(G144,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H144,4)+1)&\"-\"&MID(H144,3,2)+2),VALUE(LEFT(H144,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I144,4)+1)&\"-\"&MID(I144,3,2)+2),VALUE(LEFT(I144,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J144,4)+1)&\"-\"&MID(J144,3,2)+2),VALUE(LEFT(J144,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K144,4)+1)&\"-\"&MID(K144,3,2)+2),VALUE(LEFT(K144,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L144,4)+1)&\"-\"&MID(L144,3,2)+2),VALUE(LEFT(L144,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M144,4)+1)&\"-\"&MID(M144,3,2)+2),VALUE(LEFT(M144,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N144,4)+1)&\"-\"&MID(N144,3,2)+2),VALUE(LEFT(N144,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O144,4)+1)&\"-\"&MID(O144,3,2)+2),VALUE(LEFT(O144,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P144,4)+1)&\"-\"&MID(P144,3,2)+2),VALUE(LEFT(P144,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q144,4)+1)&\"-\"&MID(Q144,3,2)+2),VALUE(LEFT(Q144,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R144,4)+1)&\"-\"&MID(R144,3,2)+2),VALUE(LEFT(R144,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S144,4)+1)&\"-\"&MID(S144,3,2)+2),VALUE(LEFT(S144,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T144,4)+1)&\"-\"&MID(T144,3,2)+2),VALUE(LEFT(T144,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U144,4)+1)&\"-\"&MID(U144,3,2)+2),VALUE(LEFT(U144,4)+1))","v":"2042-43"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C145:C154)","v":0},{"$f":"-SUM(D145:D154)","v":0},{"$f":"-SUM(E145:E154)","v":0},{"$f":"-SUM(F145:F154)","v":0},{"$f":"-SUM(G145:G154)","v":0},{"$f":"-SUM(H145:H154)","v":0},{"$f":"-SUM(I145:I154)","v":0},{"$f":"-SUM(J145:J154)","v":0},{"$f":"-SUM(K145:K154)","v":0},{"$f":"-SUM(L145:L154)","v":0},{"$f":"-SUM(M145:M154)","v":0},{"$f":"-SUM(N145:N154)","v":0},{"$f":"-SUM(O145:O154)","v":0},{"$f":"-SUM(P145:P154)","v":0},{"$f":"-SUM(Q145:Q154)","v":0},{"$f":"-SUM(R145:R154)","v":0},{"$f":"-SUM(S145:S154)","v":0},{"$f":"-SUM(T145:T154)","v":0},{"$f":"-SUM(U145:U154)","v":0},{"$f":"-SUM(V145:V154)","v":0}]

{"sheet":"7.8 Export Services","index":29,"n_rows":57,"n_cols":9,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.8 EXPORT SERVICES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"Expenditure must only be related to DER integration, and must exclude amounts relating to DMIA"]
[]
[null,"Export service related overvoltage complaint management\nexamples include but not limited to: complaint processing, analysis, transformer tapping "]
[]
[null,"7.8.1 - OPEX FOR PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Export service related overvoltage complaint management",3985492.2826676057,3976670.6336403317,3775030.8226180822,3795810.380349033,3813773.1445067283,3835126.0841035112,3857849.5266197664]
[null,"Other opex",776733.6055491888,775014.35212455096,735716.71802331565,739766.45131931792,743267.21899876185,747428.69883256091,751857.27632922272]
[]
[]
[null,"ICT capex\nexamples include but not limited to: establishing systems for network visibility, hosting capacity assessments, generation of dynamic operating envelopes"]
[null,"Network monitoring capex\nexamples include but not limited to: implementing transformer monitors"]
[]
[null,"7.8.2 - CAPEX FOR THE PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"ICT capex",1176826.696173084,498307.47732777789,2858282.7705215774,2007177.5144827368,679778.54128265276,0,0]
[null,"Network monitoring capex",5754200.4717064397,2436519.438604428,5303498.7199086156,5336480.7689819187,5442148.4794661431,5493074.402969365,5538743.9503440317]
[null,"Other capex",4930782.8321204763,2087857.084067794,3006440.895230806,6428316.419610926,6161903.5817167321,4117628.7643411625,3519690.7489416604]
[]
[]
[]
[]
[null,"7.8.3 - EXPORT VOLUMES - NET METERED VOLUME OF ENERGY EXPORTED"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"VOLUMES\nMWh"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},548.77981421774473,568.80666982289972,693.10530966382453,820.59182565465608,948.713458486479,1066.0847474143277,1165.7047260765535]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1172640.0701039382,1215433.7238651756,1481036.7252158278,1753451.6230959429,2027223.6471633725,2278024.192137375,2490893.4991630772]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},595923.10655988427,617670.38242108212,752646.97900154896,891085.30833778158,1030213.3146466478,1157667.4616591851,1265845.3603751676]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},{"$f":"SUM(C35:C38)","v":1769111.9564780402},{"$f":"SUM(D35:D38)","v":1833672.9129560806},2234376.8095270405,2645357.523259379,3058385.6752685066,3436757.7385439742,3757904.5642643217]
[]
[]
[null,"7.8.4 EXPORT SERVICES - CUSTOMER NUMBERS"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"CUSTOMER NUMBERS"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},19,{"$f":"C53","v":19},{"$f":"D53","v":19},19,19,19,19]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},288858.13278190617,{"$f":"C54","v":304620},{"$f":"D54","v":320382},336144,351906,367667,383429]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},398381.70660659601,{"$f":"C55","v":420120},441858,463596,485334,507072,528811]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,{"$f":"C56","v":0},0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C57,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},19,19,19,19,19,19,19]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},304620,320382,336144,351906,367667,383429,399191]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},420120,441858,463596,485334,507072,528811,550549]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]

{"sheet":"AER Sheet Heading","index":30,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"dms_Header_Span","v":"2022-23 to 2029-30"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2025)"}]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C15:C35)","v":0},{"$f":"SUM(D15:D35)","v":0},0,0,0,0,0]
[null,null,{"$f":"SUM(C15:C36)","v":0},{"$f":"SUM(D15:D36)","v":0},0,0,0,0,0]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C46:C66)","v":0},{"$f":"SUM(D46:D66)","v":0},{"$f":"SUM(E46:E66)","v":0},{"$f":"SUM(F46:F66)","v":0},{"$f":"SUM(G46:G66)","v":0},{"$f":"SUM(H46:H66)","v":0},{"$f":"SUM(I46:I66)","v":0}]
[null,null,{"$f":"SUM(C46:C67)","v":0},{"$f":"SUM(D46:D67)","v":0},{"$f":"SUM(E46:E67)","v":0},{"$f":"SUM(F46:F67)","v":0},{"$f":"SUM(G46:G67)","v":0},{"$f":"SUM(H46:H67)","v":0},{"$f":"SUM(I46:I67)","v":0}]

{"sheet":"AER CF","index":31,"n_rows":77,"n_cols":25,"rows_kept":77,"cut":false,"hidden":true,"merged":[[3,1,3,22],[39,38,39,59],[40,38,40,59],[41,38,41,59],[39,69,39,90],[40,69,40,90],[41,69,41,90]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[null,"CELLS FLAGED \"Y\" and greyed out will be greyed out in the worksheets."]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":true},"=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",null,null,"=INDEX(dms_CF_F10, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6.1","dms_CF_3.6.6.2","dms_CF_3.6.6.3","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.8 (set from dms_MAIFI_flag)","dms_CF_7.12","dms_CF_8.1_A  (and 8.4)","dms_CF_8.1_B  (and 8.4)","dms_CF_8.1_Neg  (and 8.4)","dms_CF_4.4.1","dms_CF_MAIFI_flag (set from dms_MAIFI_flag)","9.5 TUOS (set from Jurisdiction)","dms_CF_F10"]
[null,"Amadeus","NT","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"APA GasNet","Vic","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C7=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ausgrid (Tx Assets)","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C8=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C9=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","Y","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C10=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co.","NSW","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C13=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co. (Vic)","Vic","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C14=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C15=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C16=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C17=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C18=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Energex","Qld","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C19=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C20=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C21=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C22=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution (Tx Assets)","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C23=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C25=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"JGN","Vic","Gas","Distribution","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C26=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Power and Water","NT","Electricity","Distribution",null,"N","N",null,null,"N","Y","N","N","N","Y",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","Y","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C27=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C28=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C29=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Roma to Brisbane Pipeline","Qld","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","N","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C31=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C32=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C33=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C34=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"United Energy","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C35=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE","dms_H2"]
[null,"TOP HEADER","dms_H1"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,5.1109999999999998,"dms_NUM"]
[null,5.45E-2,"dms_NUM%"]
[null,5.5555000000000003,"dms_NUM3d"]
[null,"Text description","dms_Row_Locked"]
[null,"Text description - not locked","dms_Row1"]
[null,"Text description","dms_Row2"]
[null,"Total","dms_T1"]
[null,"Total","dms_T2"]
[null,"EXPENSES","dms_BH"]
[null,2019,"dms_BY1"]
[null,2019,"dms_BY2"]
[null,"VOLUMES","dms_GH"]
[null,2019,"dms_GY1"]
[null,2019,"dms_GY2"]

{"sheet":"AER NRs","index":32,"n_rows":232,"n_cols":16,"rows_kept":232,"cut":false,"hidden":true,"merged":[[4,1,28,1],[176,1,177,1],[179,1,184,1],[65,1,78,1],[135,1,150,1],[84,1,97,1],[152,1,158,1],[118,1,132,1],[208,1,213,1],[199,1,200,1],[32,1,55,1],[100,1,107,1],[110,1,115,1],[191,1,192,1],[195,1,196,1],[160,1,174,1],[33,67,33,88],[34,67,34,88],[35,67,35,88],[36,10,40,10],[44,10,45,10],[33,10,35,10],[33,36,33,57],[34,36,34,57],[35,36,35,57]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Tariff cap"]
[null,null,"Final decision","Weighted average price cap"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Reallocated"]
[null,null,"Recast"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[null,null,null,null,null,null,null,null,null,null,null,null,"GAS ARR & RESET"]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140201_UOM","dms_E050201_UOM","dms_E050202_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number per km","per metre per connection","metres per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","per service per connection","number per connection"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number per connection","number per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","dms_E020202_UOM","Spare"]
[null,null,"number","number","Length of mains replaced"]
[null,null,"number","number","Number of services replaced"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)",""]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":{"$error":"#NAME?"}}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]
[]
[]
[]
[null,"PTRM input sheet","DMS_50_01_01a","DMS_50_01_01aa","DMS_50_01_01b","DMS_50_01_01bb","DMS_50_01_01c","DMS_50_01_01d","DMS_50_01_01dd"]

{"sheet":"AER lookups","index":33,"n_rows":101,"n_cols":37,"rows_kept":101,"cut":false,"hidden":true,"merged":[[17,60,17,81],[22,1,22,4],[4,24,4,35],[5,24,5,27],[5,29,7,33],[5,34,7,34],[5,35,7,35],[5,36,7,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Template number",5]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_MAIFI_flag_List","dms_Public_Lighting_List","Name"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Australian Distribution Co."]
[null,"Australian Transmission Co.","Australian Transmission Co.",11222333444,"NSW","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Australian Transmission Co."]
[null,"Directlink","Directlink",16779340889,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"Level 25","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO",{"$f":"B12","v":"Directlink"}]
[null,"ElectraNet","ElectraNet",41094482416,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"52-55 East Terrace","Rymill Park","ADELAIDE","SA",5000,"PO Box 7096","Hutt Street Post Office","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","ElectraNet"]
[null,"Energex","Energex",40078849055,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"26 Reddacliff Street",null,"NEWSTEAD","Qld",4006,"26 Reddacliff Street",null,"NEWSTEAD","QLD",4006,"YES","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Energex"]
[null,"Ergon Energy","Ergon Energy",50087646062,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"22 Walker Street",null,"TOWNSVILLE","Qld",4810,"Po Box 264",null,"FORTITUDE VALLEY","QLD",4006,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Ergon Energy"]
[null,"Murraylink","Murraylink",79181207909,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Murraylink"]
[null,"Powerlink","Queensland Electricity Transmission Corporation Limited trading as Powerlink Queensland",82078849233,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"33 Harold St",null,"VIRGINIA","Qld",4014,"PO Box 1193",null,"VIRGINIA","QLD",4014,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Powerlink"]
[null,"SA Power Networks","SA Power Networks",13332330749,"SA","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"1 Anzac Highway",null,"KESWICK","SA",5035,"GPO Box 77",null,"ADELAIDE","SA",5000,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","SA Power Networks"]
[]
[]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"EBSS","Efficiency Benefit Sharing Scheme","EFFICIENCY BENEFIT SHARING SCHEME",5]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"Profitability","Profitability","PROFITABILITY",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88",1988,"PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2015-16"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2020-21"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2025-26"}]
[null,"1988-89",1989,"PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2016-17"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2021-22"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2026-27"}]
[null,"1989-90",1990,"PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2017-18"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2022-23"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2027-28"}]
[null,"1990-91",1991,"PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2018-19"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2023-24"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2028-29"}]
[null,"1991-92",1992,"PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2019-20"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2024-25"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2029-30"}]
[null,"1992-93",1993,"PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2020-21"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2025-26"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2030-31"}]
[null,"1993-94",1994,"PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2021-22"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2026-27"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2031-32"}]
[null,"1994-95",1995,"PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2022-23"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2027-28"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2032-33"}]
[null,"1995-96",1996,"PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2023-24"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2028-29"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2033-34"}]
[null,"1996-97",1997,"PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2024-25"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2029-30"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2034-35"}]
[null,"1997-98",1998,"PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2025-26"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2030-31"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2035-36"}]
[null,"1998-99",1999,"PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2026-27"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2031-32"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2036-37"}]
[null,"1999-00",2000,"PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2027-28"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2032-33"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2037-38"}]
[null,"2000-01",2001,"PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2028-29"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2033-34"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2038-39"}]
[null,"2001-02",2002,"PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2029-30"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2034-35"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2039-40"}]
[null,"2002-03",2003,"PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2030-31"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2035-36"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2040-41"}]
[null,"2003-04",2004,"PRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+16)","v":"2031-32"},"CRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+16)","v":"2036-37"},"FRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+16)","v":"2041-42"}]
[null,"2004-05",2005,"PRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+17)","v":"2032-33"},"CRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+17)","v":"2037-38"},"FRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+17)","v":"2042-43"}]
[null,"2005-06",2006,"PRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+18)","v":"2033-34"},"CRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+18)","v":"2038-39"},"FRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+18)","v":"2043-44"}]
[null,"2006-07",2007,"PRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+19)","v":"2034-35"},"CRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+19)","v":"2039-40"},"FRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+19)","v":"2044-45"}]
[null,"2007-08",2008,"PRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+20)","v":"2035-36"},"CRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+20)","v":"2040-41"},"FRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+20)","v":"2045-46"}]
[null,"2008-09",2009,"PRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+21)","v":"2036-37"},"CRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+21)","v":"2041-42"},"FRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+21)","v":"2046-47"}]
[null,"2009-10",2010,"PRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+22)","v":"2037-38"},"CRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+22)","v":"2042-43"},"FRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+22)","v":"2047-48"}]
[null,"2010-11",2011,"PRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+23)","v":"2038-39"},"CRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+23)","v":"2043-44"},"FRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+23)","v":{"$error":"#REF!"}}]
[null,"2011-12",2012,"PRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+24)","v":"2039-40"},"CRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+24)","v":"2044-45"},"FRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+24)","v":{"$error":"#REF!"}}]
[null,"2012-13",2013]
[null,"2013-14",2014]
[null,"2014-15",2015]
[null,"2015-16",2016]
[null,"2016-17",2017]
[null,"2017-18",2018]
[null,"2018-19",2019]
[null,"2019-20",2020]
[null,"2020-21",2021]
[null,"2021-22",2022,null,"CRY - FRY"]
[null,"2022-23",2023,"dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2022-23"}]
[null,"2023-24",2024,"dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2023-24"}]
[null,"2024-25",2025,"dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2024-25"}]
[null,"2025-26",2026,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2025-26"}]
[null,"2026-27",2027,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2026-27"}]
[null,"2027-28",2028,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2027-28"}]
[null,"2028-29",2029,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2028-29"}]
[null,"2029-30",2030,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2029-30"}]
[null,"2030-31",2031,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2030-31"}]
[null,"2031-32",2032,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2031-32"}]
[null,"2032-33",2033,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2032-33"}]
[null,"2033-34",2034,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2033-34"}]
[null,"2034-35",2035,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2034-35"}]
[null,"2035-36",2036,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2035-36"}]
[null,"2036-37",2037,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2036-37"}]
[null,"2037-38",2038,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2037-38"}]
[null,"2038-39",2039,"dms_y17",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+16),0)","v":"2038-39"}]
[null,"2039-40",2040,"dms_y18",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+17),0)","v":"2039-40"}]
[null,"2040-41",2041,"dms_y19",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+18),0)","v":"2040-41"}]
[null,"2041-42",2042,"dms_y20",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+19),0)","v":"2041-42"}]
[null,"2042-43",2043,"dms_y21",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+20),0)","v":"2042-43"}]
[null,"2043-44",2044,"dms_y22",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+21),0)","v":"2043-44"}]
[null,"2044-45",2045,"dms_y23",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+22),0)","v":"2044-45"}]
[null,"2045-46",2046,"dms_y24",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+23),0)","v":"2045-46"}]
[null,"2046-47",2047,"dms_y25",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+24),0)","v":"2046-47"}]
[null,"2047-48",2048,"dms_y26",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+25),0)","v":"2047-48"}]

{"sheet":"AER ETL","index":34,"n_rows":145,"n_cols":10,"rows_kept":145,"cut":false,"hidden":true,"merged":[[12,4,12,8],[71,1,73,1],[11,0,15,0],[18,0,25,0],[26,0,31,0],[34,0,59,0],[14,2,14,4],[32,37,32,58],[33,37,33,58],[34,37,34,58],[32,68,32,89],[33,68,33,89],[34,68,34,89]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"Energex"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Regulatory proposal","dms_Source",{"$f":"IF(dms_Model=\"Reset\", \"Make sure you have set Reg Proposal as source\",\"\")","v":"Make sure you have set Reg Proposal as source"}]
[null,"Data quality","Consolidated","For DB purposes this is always Consoldiated"]
[null,"Data status","Public","For DB purposes this is always Public"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"31/01/24"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality","Consolidated","dms_DataQuality","Always Consolidated"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)","v":"2030"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)"]
[null,"Reporting Period Type","Financial","dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM",{"$f":"IF(dms_SingleYearModel=\"yes\",\"This is set to an historical template (EB, CA or ARR), apply UOM Named Range to cell !\",\"This is not an historical template, make sure UOM Named Range is not applied\")","v":"This is not an historical template, make sure UOM Named Range is not applied"},null,null,null,null,{"$f":"IFERROR(dms_dollar_nom_UOM, \"NR not applied\")","v":"NR not applied"}]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"Qld"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"2022-23"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"2022"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))","v":"June 2025"},"dms_DollarReal","=IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year","v":"June 2020"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2025-26"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2022-23"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":36},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":39},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":34},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":29},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":43},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2020-21"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2015-16"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2029-30"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2024-25"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2019-20"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2029-30"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2028-29"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2025"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2020"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":"2023"},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2030"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2030"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2025-26 to 2029-30"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_y1&\" to \"&FRCP_final_year,CRY))","v":"2022-23 to 2029-30"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"2022-23"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2029-30"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C50,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"2022-23"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(dms_SingleYearModel=\"yes\",(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(PRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(PRCP_y4,4))))","v":"1-Jul-2018"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060101_StartDateTxt)","v":43282},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"Does the NSP report MAIFI or MAIFIe",{"$f":"INDEX(dms_MAIFI_flag_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_MAIFI_Flag"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes","Must be present for ARRs","=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","0","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2017"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]