{"text_format":"1","workbook":"xlsx","n_sheets":34,"sheets":["Instructions","CONTENTS","Business & other details","2.1 Expenditure summary","2.2 Repex","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","5.4 MD & utilisation-Spatial","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.7 TSS-LRMC","7.8 Export Services","AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":726,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4],[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[13,2,13,4],[16,2,16,4],[10,1,11,1],[10,2,10,3],[11,2,11,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List)),\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by SA Power Networks to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nBusinesses must use the macro at the top of  \neach worksheet to identify confidential\ninformation in the confidential workbook and\nwhere confidential information has been \nremoved in the public workbook. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the NON-CONFIDENTIAL macro."]
[]
[null,"PROTECTED (SOCI) INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify information in the \nconfidential workbook that is protected \ninformation under the SOCI Act. All \ninformation marked Protected (SOCI) is also \ndeemed to be confidential information."]
[null,null,"-Do this by selecting the cell or cells that contain protected information and then run the PROTECTED (SOCI) macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as protected..\n\n-To reverse this, select the cell or cells and run the NON-PROTECTED macro."]
[]
[null,"RESPONSES","\nPlease return two (2) files to the AER: \n\n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information redacted or aggregated.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential or public. "]
[]
[]
[null,"ORDER OF MAGNITUDE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. \n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," PLEASE DO NOT ENTER TEXT into cells that are to contain numbers \n(including 'numbers stored as text')"]

{"sheet":"CONTENTS","index":1,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[[6,3,6,4],[8,3,8,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"DRAFT RIN ONLY - DO NOT USE FOR SUBMISSION"]
[]
[null,null,null,"TEMPLATE","OCTOBER 2023 - FINAL RIN"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 FORECAST price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[null,null,null,null,"7.8 Export Services"]

{"sheet":"Business & other details","index":2,"n_rows":77,"n_cols":79,"rows_kept":77,"cut":false,"hidden":false,"merged":[[76,25,76,34],[76,37,76,52],[58,25,58,34],[66,25,66,34],[68,25,68,34],[58,37,58,44],[64,25,64,34],[64,37,64,52],[35,37,35,58],[36,37,36,58],[46,37,46,44],[46,46,46,53],[46,55,46,62],[44,37,44,44],[66,37,66,52],[68,37,68,52],[70,37,70,52],[72,37,74,81],[70,25,70,34],[72,25,74,34],[54,46,54,53],[54,37,54,44],[53,73,53,80],[53,64,53,71],[56,25,56,34],[48,46,48,53],[48,37,48,44],[52,37,52,44],[50,73,50,80],[54,73,54,80],[52,73,52,80],[56,37,56,44],[52,46,52,53],[53,46,53,53],[49,46,49,53],[49,37,49,44],[54,64,54,71],[50,46,50,53],[53,55,53,62],[50,37,50,44],[53,37,53,44],[52,64,52,71],[50,64,50,71],[52,55,52,62],[50,55,50,62],[49,64,49,71],[49,55,49,62],[46,64,46,71],[19,21,19,35],[19,37,19,48],[48,25,48,34],[52,25,52,34],[25,21,25,35],[25,60,25,66],[26,60,26,66],[34,60,34,66],[18,21,18,35],[46,73,46,80],[44,73,44,80],[54,55,54,62],[28,21,28,35],[26,21,26,35],[48,73,48,80],[48,64,48,71],[49,73,49,80],[48,55,48,62],[45,73,45,80],[35,21,35,35],[36,21,36,35],[36,60,36,66],[35,60,35,66],[34,21,34,35],[34,68,34,89],[35,68,35,89],[36,68,36,89],[34,37,34,58],[44,46,44,53],[44,25,44,34],[44,55,44,62],[44,64,44,71],[10,16,10,93],[11,16,11,93],[18,37,18,58],[27,37,27,51],[0,7,2,15],[6,21,6,75],[27,21,27,35],[45,37,45,44],[45,46,45,53],[45,55,45,62],[45,64,45,71],[3,21,3,57],[8,16,8,93],[25,68,25,89],[26,68,26,89],[28,68,28,71],[28,80,28,82],[27,68,27,82],[28,37,28,40],[25,37,25,58],[26,37,26,58],[28,49,28,51],[27,60,27,66],[28,60,28,66]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRAFT TEMPLATE ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DO NOT USE FOR SUBMISSIONS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SA Power Networks"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":13332330749}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"1 Anzac Highway"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 77"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"KESWICK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"ADELAIDE"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA"},null,null,null,null,null,null,null,null,null,"Post code",null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA"},null,null,null,null,null,null,null,null,null,"Post code"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2025-26",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2029-30"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2034-35"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2035-36"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2036-37"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2037-38"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2038-39"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2039-40"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2024-25"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2029-30"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2034-35"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2015-16"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2019-20"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2024-25"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2029-30"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2022-23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2028-29"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Regulatory proposal"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Public"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"31/01/2024",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"2.1 Expenditure summary","index":3,"n_rows":113,"n_cols":37,"rows_kept":113,"cut":false,"hidden":false,"merged":[[8,1,9,1],[24,1,25,1],[38,1,39,1],[91,1,92,1],[104,1,105,1],[51,1,52,1],[63,1,64,1],[77,1,78,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX (including dual function assets)"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure",{"$f":"SUM('2.2 Repex'!D12:D119,'2.2 Repex'!D129:D177 )","v":155744159.98000005},{"$f":"SUM('2.2 Repex'!E12:E119,'2.2 Repex'!E129:E177 )","v":152067367.01999998},{"$f":"SUM('2.2 Repex'!F12:F119,'2.2 Repex'!F129:F177 )","v":170753632.01999998},{"$f":"SUM('2.2 Repex'!G12:G119,'2.2 Repex'!G129:G177 )","v":176501368.97},{"$f":"SUM('2.2 Repex'!H12:H119,'2.2 Repex'!H129:H177 )","v":194770883.99999997},{"$f":"SUM('2.2 Repex'!I12:I119,'2.2 Repex'!I129:I177 )","v":181454398.03},{"$f":"SUM('2.2 Repex'!J12:J119,'2.2 Repex'!J129:J177 )","v":185897117.96999994}]
[null,"Connections",{"$f":"SUM('2.5 Connections'!E124:E137, '2.5 Connections'!E142:E155)","v":159611458},{"$f":"SUM('2.5 Connections'!F124:F137, '2.5 Connections'!F142:F155)","v":148241170},{"$f":"SUM('2.5 Connections'!G124:G137, '2.5 Connections'!G142:G155)","v":150339865},{"$f":"SUM('2.5 Connections'!H124:H137, '2.5 Connections'!H142:H155)","v":146448986},{"$f":"SUM('2.5 Connections'!I124:I137, '2.5 Connections'!I142:I155)","v":150225068},{"$f":"SUM('2.5 Connections'!J124:J137, '2.5 Connections'!J142:J155)","v":152369957},{"$f":"SUM('2.5 Connections'!K124:K137, '2.5 Connections'!K142:K155)","v":145852754},null,null,null,null,null,null,null,"ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO",{"$f":"B12","v":"Connections"}]
[null,"Augmentation Expenditure",{"$f":"SUM('2.3 Augex (b)'!D48:D56)","v":77256190.099999994},{"$f":"SUM('2.3 Augex (b)'!E48:E56)","v":76802135.510000005},{"$f":"SUM('2.3 Augex (b)'!F48:F56)","v":96521072.12000002},{"$f":"SUM('2.3 Augex (b)'!G48:G56)","v":95209153.429999992},{"$f":"SUM('2.3 Augex (b)'!H48:H56)","v":97088166.229999989},{"$f":"SUM('2.3 Augex (b)'!I48:I56)","v":104786085.21000001},{"$f":"SUM('2.3 Augex (b)'!J48:J56)","v":111916404.8},null,null,null,null,null,null,null,"ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Augmentation Expenditure"]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E33:E51)","v":103086609.83757876},{"$f":"SUM('2.6 Non-network'!F33:F51)","v":102953519.2300339},{"$f":"SUM('2.6 Non-network'!G33:G51)","v":120308810.40620001},{"$f":"SUM('2.6 Non-network'!H33:H51)","v":147827794.26740003},{"$f":"SUM('2.6 Non-network'!I33:I51)","v":135880292.9068},{"$f":"SUM('2.6 Non-network'!J33:J51)","v":127616590.85600001},{"$f":"SUM('2.6 Non-network'!K33:K51)","v":122896764.49060002}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C24:C26)","v":9224375},{"$f":"SUM('7.8 Export Services'!D24:D26)","v":6261121},{"$f":"SUM('7.8 Export Services'!E24:E26)","v":35115037},{"$f":"SUM('7.8 Export Services'!F24:F26)","v":17411699},{"$f":"SUM('7.8 Export Services'!G24:G26)","v":16517535},{"$f":"SUM('7.8 Export Services'!H24:H26)","v":10592116},{"$f":"SUM('7.8 Export Services'!I24:I26)","v":11068750}]
[null,"Public lighting"]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",{"$f":"'2.10 Overheads'!D16","v":6551264},{"$f":"'2.10 Overheads'!E16","v":6364032},{"$f":"'2.10 Overheads'!F16","v":8372654},{"$f":"'2.10 Overheads'!G16","v":8431900},{"$f":"'2.10 Overheads'!H16","v":8863296},{"$f":"'2.10 Overheads'!I16","v":8454242},{"$f":"'2.10 Overheads'!J16","v":8607092}]
[null,"Capitalised corporate overheads",{"$f":"'2.10 Overheads'!D31","v":-5877666},{"$f":"'2.10 Overheads'!E31","v":-5854775},{"$f":"'2.10 Overheads'!F31","v":-6528751},{"$f":"'2.10 Overheads'!G31","v":-6528751},{"$f":"'2.10 Overheads'!H31","v":-6528751},{"$f":"'2.10 Overheads'!I31","v":-6528751},{"$f":"'2.10 Overheads'!J31","v":-6528751}]
[null,"capcons (included in the above)",103492235,97076548,107158241,102000248,103670847,104141384,97573262]
[null,"Total",{"$f":"SUM(C11:C19)","v":505596390.91757882},486834569.76003385,{"$f":"SUM(E11:E19)","v":574882319.54620004},585302150.66740012,596816491.13680005,578744638.09599996,579710132.26059997]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"}]
[null,"Vegetation management",47133744,48316759]
[null,"Maintenance",39277337,40263163]
[null,"Emergency response",43483727,44575129,null," "]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E13:E31)","v":61315895},{"$f":"SUM('2.6 Non-network'!F13:F31)","v":67095334}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C14:C15)","v":0},{"$f":"SUM('7.8 Export Services'!D14:D15)","v":0}]
[null,"Metering",0,0]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D13","v":98397895},{"$f":"'2.10 Overheads'!E13","v":102817373}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D28","v":62364547},{"$f":"'2.10 Overheads'!E28","v":62914460}]
[null,"Total",{"$f":"SUM(C27:C34)","v":351973145},{"$f":"SUM(D27:D34)","v":365982218}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Public lighting",{"$f":"SUM('4.1 Public lighting'!D15,'4.1 Public lighting'!D19,'4.1 Public lighting'!D23)","v":19099414.10023864},{"$f":"SUM('4.1 Public lighting'!E15,'4.1 Public lighting'!E19,'4.1 Public lighting'!E23)","v":18479681.232840944},{"$f":"SUM('4.1 Public lighting'!F15,'4.1 Public lighting'!F19,'4.1 Public lighting'!F23)","v":14987166.538364811},{"$f":"SUM('4.1 Public lighting'!G15,'4.1 Public lighting'!G19,'4.1 Public lighting'!G23)","v":14375284.560519481},{"$f":"SUM('4.1 Public lighting'!H15,'4.1 Public lighting'!H19,'4.1 Public lighting'!H23)","v":14920208.040155631},{"$f":"SUM('4.1 Public lighting'!I15,'4.1 Public lighting'!I19,'4.1 Public lighting'!I23)","v":14329574.932453413},{"$f":"SUM('4.1 Public lighting'!J15,'4.1 Public lighting'!J19,'4.1 Public lighting'!J23)","v":13793102.734408591}]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D17","v":233196},{"$f":"'2.10 Overheads'!E17","v":220410},{"$f":"'2.10 Overheads'!F17","v":198324},{"$f":"'2.10 Overheads'!G17","v":184712},{"$f":"'2.10 Overheads'!H17","v":180390},{"$f":"'2.10 Overheads'!I17","v":162656},{"$f":"'2.10 Overheads'!J17","v":145326}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D32","v":-52991},{"$f":"'2.10 Overheads'!E32","v":-54270},{"$f":"'2.10 Overheads'!F32","v":-68412},{"$f":"'2.10 Overheads'!G32","v":-71736},{"$f":"'2.10 Overheads'!H32","v":-72922},{"$f":"'2.10 Overheads'!I32","v":-73390},{"$f":"'2.10 Overheads'!J32","v":-74801}]
[null,"capcons (included in the above)",2567126.393994316,2704992.0423829285,604125.0422909878,606322.56717493944,608202.0775865264,610588.22736841964,613246.43897005916]
[null,"Total",{"$f":"SUM(C41:C46)","v":19279619.10023864},18645821.232840944,15117078.538364811,14488260.560519481,15027676.040155631,14418840.932453413,13863627.734408591]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Connections",{"$f":"SUM('3.2 Operating expenditure'!K73)","v":61567126},{"$f":"SUM('3.2 Operating expenditure'!L73)","v":60468110},{"$f":"SUM('3.2 Operating expenditure'!M73)","v":61017618},{"$f":"SUM('3.2 Operating expenditure'!N73)","v":61017618},{"$f":"SUM('3.2 Operating expenditure'!O73)","v":61017618},{"$f":"SUM('3.2 Operating expenditure'!P73)","v":61017618},{"$f":"SUM('3.2 Operating expenditure'!Q73)","v":61017618}]
[null,"Metering",{"$f":"'3.2 Operating expenditure'!K72","v":8033123},{"$f":"'3.2 Operating expenditure'!L72","v":7256367},{"$f":"'3.2 Operating expenditure'!M72","v":0},{"$f":"'3.2 Operating expenditure'!N72","v":0},{"$f":"'3.2 Operating expenditure'!O72","v":0},{"$f":"'3.2 Operating expenditure'!P72","v":0},{"$f":"'3.2 Operating expenditure'!Q72","v":0}]
[null,"Public lighting",{"$f":"'3.2 Operating expenditure'!K74","v":7488430},{"$f":"'3.2 Operating expenditure'!L74","v":6787048},{"$f":"'3.2 Operating expenditure'!M74","v":6252233},{"$f":"'3.2 Operating expenditure'!N74","v":5982168},{"$f":"'3.2 Operating expenditure'!O74","v":6662238},{"$f":"'3.2 Operating expenditure'!P74","v":6536717},{"$f":"'3.2 Operating expenditure'!Q74","v":6417080}]
[null,"Fee and quoted",52450764,51631783,51682655,51682655,51682655,51682686,51682655]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D14","v":3627912},{"$f":"'2.10 Overheads'!E14","v":3647457},{"$f":"'2.10 Overheads'!F14","v":2446142},{"$f":"'2.10 Overheads'!G14","v":2446982},{"$f":"'2.10 Overheads'!H14","v":2454902},{"$f":"'2.10 Overheads'!I14","v":2458372},{"$f":"'2.10 Overheads'!J14","v":2471018}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D29","v":10629459},{"$f":"'2.10 Overheads'!E29","v":10885983},{"$f":"'2.10 Overheads'!F29","v":11817481},{"$f":"'2.10 Overheads'!G29","v":12382788},{"$f":"'2.10 Overheads'!H29","v":12568516},{"$f":"'2.10 Overheads'!I29","v":12578084},{"$f":"'2.10 Overheads'!J29","v":12780597}]
[null,"Total",{"$f":"SUM(C54:C59)","v":143796814},140676748,133216129,133512211,134385929,134273477,134368968]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C66:C72)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Export services"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total",{"$f":"SUM(C80:C87)","v":0},{"$f":"SUM(D80:D87)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure",3157000,2796350,0,0,0,0,0]
[null,"Connections",96466207,89702614,102195099,97124398,98760549,99217077,92760756]
[null,"Augmentation Expenditure",2515418,3331602,3044120,3047405,3050222,3053816,3057873]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Export services",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",1353610,1245982,1919022,1828445,1860076,1870491,1754634]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C94:C100)","v":103492235},97076548,107158241,102000248,103670847,104141384,97573263]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Replacement expenditure",1037143,952124,1187092,1345808,1552086,1385915,1425962]
[null,"Connections",260559,276495,1028572,1034253,1094793,1062176,1022343]
[null,"Augmentation Expenditure",514470,480873,671234,728932,777814,803150,866343]
[null,"Non-network",-1200003,-1239437,-1286932,-1336664,-1221403,-1405902,-1320784]
[null,"Export services",61428,39202,243937,130821,131257,80153,84478]
[null,"capcons (included in the above)",1353610,1245982,1919022,1828445,1860076,1870491,1754634]
[null,"Total",{"$f":"SUM(C107:C111)","v":673597},509257,1843903,1903150,2334547,1925492,2078342]

{"sheet":"2.2 Repex","index":4,"n_rows":521,"n_cols":10,"rows_kept":521,"cut":false,"hidden":false,"merged":[[480,1,520,1],[11,1,29,1],[30,1,36,1],[37,1,42,1],[43,1,51,1],[52,1,59,1],[60,1,75,1],[76,1,104,1],[105,1,118,1],[119,1,127,1],[128,1,135,1],[183,1,201,1],[202,1,208,1],[209,1,214,1],[215,1,223,1],[136,1,176,1],[224,1,231,1],[232,1,247,1],[248,1,276,1],[277,1,290,1],[291,1,299,1],[300,1,307,1],[355,1,373,1],[449,1,462,1],[463,1,471,1],[308,1,348,1],[472,1,479,1],[374,1,380,1],[381,1,386,1],[387,1,395,1],[396,1,403,1],[404,1,419,1],[420,1,448,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.2 REPEX"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",5452909.1100000003,6182630.4199999999,6952451.9199999999,6800803.2400000002,6771657.3799999999,6793772.7000000002,6814925.6699999999]
[null,null,"> 1 kV & < = 11 kV",11370768.220000001,12892431.119999999,14497713.84,14181486.49,14120708.869999999,14166826.08,14210933.869999999]
[null,null,"˃ 11 kV & < = 22 kV",5144686.0999999996,5833160.2199999997,6559467.4500000002,6416391.5199999996,6388892.29,6409758.0499999998,6429715.3099999996]
[null,null,"> 22 kV & < = 66 kV",3119235.06,3536658.95,3977020.85,3890273.32,3873600.07,3886251.65,3898351.15]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",290108.01,217241.12,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",6556112.1299999999,4909415.71,4850449.9800000004,6820767.79,8857953.8000000007,10958342.470000001,13068609.17]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",779886.02,584002.31999999995,3530396.32,4964490.37,6447255.7400000002,7976021.46,9511977.2599999998]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",1938558.04,1451650.8,77591.98,109111.42,141700,175298.98,209056.95]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",2633564.0499999998,1789083.99,374248.95,468778.92,568970.13,673298.97,778109.99]
[null,null,"> 1 kV & < = 11 kV",11500877.220000001,7812998.3200000003,11463806,14359408.67,17428425.739999998,20624180.850000001,23834707.109999999]
[null,null,"> 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",27100,18410.009999999998,447652.31,560722.56999999995,680565.32,805357.41,930725.57]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",7060850.1399999997,9291015.1300000008,8801223.8200000003,8614910.6500000004,8583452.0999999996,8617253.5199999996,8650038.1500000004]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",783401.02,1030838.57,1087791.6100000001,1064764.44,1060875.8999999999,1065053.45,1069106.32]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",1949684.04,2747039.52,4689692.78,4804648.8099999996,5000269.46,5233643.6399999997,5467719.21]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",176345,248464.14,79541.17,81490.880000000005,84809.64,88767.72,92737.36]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",339347.01,478128.26,1169978.75,1198657.8999999999,1247460.78,1305682.6299999999,1364079.99]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",1665628.03,2346814.2999999998,969770.53,993542.02,1033993.95,1082253.3799999999,1130657.1299999999]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",34714,48911.03,19697.68,20180.88,21003.09,21982.560000000001,22966.46]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",231430,326076.18,9935.81,10180.18,10594.1,11088.73,11584.57]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",57857,81519.05,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",28929,40760.019999999997,3526.64,3613.6,3760.81,3936.48,4112.46]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",1203434.02,1695598.94,1050373.27,1076121.3400000001,1119935.3999999999,1172204.94,1224631.8]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",231430,326076.18,164473.69,168505.47,175366.07,183551.12,191760.68]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",79300,193019.11,723790.58,651763.06000000006,578799.72,562576.67000000004,547570.96]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",852426.02,707949.39,1123052.01,1120363.49,1124941.78,1131497.06,1136408.3899999999]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",914340.02,548478.30000000005,1158670.25,1188225.5,1213950.8899999999,1230581.6499999999,1252177.8500000001]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",244042,656970.36,1416961.63,1357980.46,1374576.43,1380739.23,1381240.17]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",2734152.05,1555362.86,828638.45,798129.03,730865.34,614657.9,578680.30000000005]
[null,null,"˂ = 11 kV ;  Circuit Breaker",7515979.1399999997,8617724.7599999998,11294761,11232941.460000001,11150844.24,11361749.130000001,11735787.16]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",689573.01,390027.22,502856.9,491979.71,489949.68,491649.52,493292.48]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",2682688.0499999998,1249738.69,648459.9,1055469.97,1079218.17,999625.8,920952.57]
[null,null,"> 33 kV & < = 66 kV ; Switch",425160.01,457074.25,632645.68999999994,336181.51,272194.7,273138.94,274051.38]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",11583058.220000001,12519369.92,13782248.83,4312429.4800000004,2462578.1800000002,2528386.48,2328819.9700000002]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",5656192.1100000003,5308449.93,7697883.4000000004,7289206.21,7220658.46,7229635.0999999996,7259175.54]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",10107461.189999999,7380039.0800000001,7794688,7362367.8600000003,5564793.3200000003,5526711.04,5277000.88]
[null,null,"Master Station Assets",0,0,1044355.72,1022028.86,1018034.84,1021851.5,1025586.24]
[null,null,"Communications Site Infrastructure",77471,326559.18,207388.72,202903.09,202065.81,202766.57,203443.7]
[null,null,"Communications Linear Assets",454570.01,433692.24,518742.67,507446.9,707402.92,709742.33,711984.41]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"OTHER: ","< = 1 kV; stobie pole",4833380.09,4953825.74,9637050.7300000004,9425593.6699999999,9384133.9600000009,9413424.8300000001,9441205.5099999998]
[null,null,"> 1 kV & < = 11 kV; stobie pole",12185755.23,12489419.9,9364022.6199999992,9158556.6400000006,9118271.2300000004,9146731.8800000008,9173725.7699999996]
[null,null,"> 11 kV & < = 22 kV; stobie pole",2130628.04,2183723.21,1705488.85,1668067.39,1660729.8,1665913.39,1670830.29]
[null,null,"> 22 kV & < = 66 kV; stobie pole",1032654.02,1058387.58,2781185.73,2720161.43,2708195.57,2716648.84,2724666.17]
[null,null,"> 66 kV & < = 132 kV; stobie pole",0,0,0,0,0,0,0]
[null,null,"> 132 kV; stobie pole",0,0,0,0,0,0,0]
[null,null,"Pole REFURBISHED; STOBIE Pole",6257989.1200000001,6785487.75,7384404.3300000001,7221303.46,7188628.4100000001,7209904.4299999997,7229873.9100000001]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ;  < = 60kVA; DISTRIBUTION TRANSFORMER",72845,102636.06,135654.26,138979.67000000001,144638.47,151388.69,158159.35]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ; > 60 KVA AND < = 600 KVA; DISTRIBUTION TRANSFORMER",156304,220227.12,53635.1,54950.05,57187.29,59856.75,62533.32]
[null,null,"Kiosk Mounted; > = 22 kV & < = 33 kV ; DISTRIBUTION TRANSFORMER",57857,81519.05,68435.45,70113.600000000006,72968.05,76373.58,79789.05]
[null,null,"Voltage regulator; DISTRIBUTION TRANSFORMER",1413689.03,2053714.13,1302642.1299999999,1273995.47,1268337.58,1272227.3400000001,1275904.8400000001]
[null,null,"Recloser ;SWITCHGEAR",4228756.08,3855051.13,3344042.17,3800738.42,4311689.88,4854759.92,5400537.7800000003]
[null,null,"Sectionalizer ;SWITCHGEAR",158988,144938.07999999999,149060.06,217054.84,287186.84999999998,359505.22,432290.83]
[null,null,">= 11 kV & < = 22 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",3484748.07,4018782.22,4150908.51,4061359.24,4044796.57,4059080.67,4072927.52]
[null,null,"> 22 kV & < = 33 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",0,0,0,0,0,0,0]
[null,null,"OTHER - Distribution",854650.02,1178130.6499999999,1115009.73,1090636.8700000001,1085917.45,1089407.55,1092735.83]
[null,null,"OTHER - Non Category Substation asset replacement/refurbishment",3234913.06,4541160.51,4125516.33,4042215.39,4026267.26,4041169.67,4055726.8]
[null,null,"Pipework Bus Substation Replacements",2588310.0499999998,1830610.01,2516532.88,2462101.65,2451939.7400000002,2460445.46,2468666.7599999998]
[null,null,"> = 11 kV ;  Circuit Breaker REFURBISHED",570147.01,127406.07,229724.42,224813.66,223934.63,224774.22,225595.58]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker REFURBISHED",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker REFURBISHED",1368353.03,101925.06,122519.83,119900.81,119432.06,119879.45,120318.16]
[null,null,"Ground Outdoor / Indoor Chamber Mounted;  22 kV ;  >  600 kVA ; Multiple Phase REFURBISHED",242609,101673.06,109169.7,106835.57,106418.17,106817.66,107207.7]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > = 22 kV & < = 33 kV ;  < = 15 MVA REFURBISHED",889568.02,372801.21,400289.21,391732.05,390200.91,391663.78,393094.58]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > 33 kV & < = 66 kV ;  < = 15 MVA REFURBISHED",1698266.03,711712.39,764187.87,747850.95,744928.13,747720.72,750453.91]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > 33 kV & < = 66 kV ;  > 15 MVA AND < = 40 MVA REFURBISHED",1617396.03,677821.37,727798.3,712239.74,709455.41,712114.83,714717.69]
[null,null,"Mobile Plant Renewal",73088,243035.13,414404.71,608319.31000000006,6665355.8600000003,2736958.4,203478.44]
[null,null,"Hindley St Substation 66kV Yard Renewal",0,0,0,10645582.02,19188145.600000001,1317795.04,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",5190,5884,6657,6657,6657,6657,6657]
[null,null,"> 1 kV & < = 11 kV",6723,7623,8624,8624,8624,8624,8624]
[null,null,"˃ 11 kV & < = 22 kV",2803,3178,3596,3596,3596,3596,3596]
[null,null,"> 22 kV & < = 66 kV",1149,1302,1473,1473,1473,1473,1473]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",145,109,108,155,203,250,297]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",16,12,72,103,135,166,198]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",25,19,1,1,2,2,3]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",1,1,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",4,2,4,5,6,7,8]
[null,null,"> 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",7828,10300,9816,9821,9826,9831,9836]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",868,1143,1213,1214,1214,1215,1216]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",110,155,267,278,290,301,313]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",3,5,2,2,2,2,2]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",15,22,54,56,58,61,63]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",68,96,40,42,43,45,47]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,1,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",3,4,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",1,1,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",13,19,12,12,13,13,14]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",3,4,2,2,2,2,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",0.4,1,4.2,3.7,3.1,3.1,3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0.3,0.7,1.5,1.5,1.5,1.5,1.5]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",1.4,1.1000000000000001,0.9,0.9,0.9,0.9,0.9]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",0.1,0.3,0.7,0.6,0.7,0.7,0.7]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",27.7,19.5,13.2,5.5,5,4.4000000000000004,4.3]
[null,null,"˂ = 11 kV ;  Circuit Breaker",11.7,15.4,21.4,25.1,25.8,23.8,21.9]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",8.3000000000000007,6.6,9.6999999999999993,9.6999999999999993,9.6999999999999993,9.6999999999999993,9.8000000000000007]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",2.5,2.8,1.4,2.4,2.5,2.2999999999999998,2.1]
[null,null,"> 33 kV & < = 66 kV ; Switch",11.8,10.6,11,6.4,5.4,5.4,5.4]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",16.899999999999999,11.9,9.5,5.4,4.9000000000000004,5.0999999999999996,4.7]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",121.2,146.30000000000001,129.4,108.7,107.6,106.6,106.6]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",400,500,400,350,300,250,300]
[null,null,"Master Station Assets",6,6,6,6,6,6,6]
[null,null,"Communications Site Infrastructure",0,0,0,0,1,0,0]
[null,null,"Communications Linear Assets",3,3,3.5,3.5,5,5,5]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"< = 1 kV; stobie pole",311,319,624,624,624,624,624]
[null,null,"> 1 kV & < = 11 kV; stobie pole",649,665,501,501,501,501,501]
[null,null,"> 11 kV & < = 22 kV; stobie pole",126,129,101,101,101,101,101]
[null,null,"> 22 kV & < = 66 kV; stobie pole",41,41,109,109,109,109,109]
[null,null,"> 66 kV & < = 132 kV; stobie pole",0,0,0,0,0,0,0]
[null,null,"> 132 kV; stobie pole",0,0,0,0,0,0,0]
[null,null,"Pole REFURBISHED; STOBIE Pole",3757,4066,4460,4460,4460,4460,4460]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ;  < = 60kVA; DISTRIBUTION TRANSFORMER",4,5,7,7,7,8,8]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ; > 60 KVA AND < = 600 KVA; DISTRIBUTION TRANSFORMER",3,5,1,1,1,1,1]
[null,null,"Kiosk Mounted; > = 22 kV & < = 33 kV ; DISTRIBUTION TRANSFORMER",1,1,1,1,1,1,1]
[null,null,"Voltage regulator; DISTRIBUTION TRANSFORMER",23,33,21,21,21,21,21]
[null,null,"Recloser ;SWITCHGEAR",130,118,103,120,136,153,169]
[null,null,"Sectionalizer ;SWITCHGEAR",18,17,17,26,34,43,51]
[null,null,">= 11 kV & < = 22 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",27,31,32,33,33,33,33]
[null,null,"> 22 kV & < = 33 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",0,0,0,0,0,0,0]
[null,null,"OTHER - Distribution",0,0,0,0,0,0,0]
[null,null,"OTHER - Non Category Substation asset replacement/refurbishment",81.599999999999994,87.1,60.2,63.9,72.2,77.900000000000006,82.6]
[null,null,"Pipework Bus Substation Replacements",2.6,1.3,2,2,1.9,2,2.1]
[null,null,"> = 11 kV ;  Circuit Breaker REFURBISHED",2,3.2,4.9000000000000004,4.9000000000000004,4.9000000000000004,4.9000000000000004,5]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker REFURBISHED",0,0,0,0,0,0,0]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":"> 33 kV & < = 66 kV ; Circuit Breaker REFURBISHED"},2,1.6,2,2,2,2,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted;  22 kV ;  >  600 kVA ; Multiple Phase REFURBISHED",1,0.6,0.7,0.6,0.5,0.6,0.7]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > = 22 kV & < = 33 kV ;  < = 15 MVA REFURBISHED",3.8,2.2999999999999998,2.5,2.1,1.9,2.1,2.5]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > 33 kV & < = 66 kV ;  < = 15 MVA REFURBISHED",7.2,4.4000000000000004,4.8,4.0999999999999996,3.5,4.0999999999999996,4.8]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > 33 kV & < = 66 kV ;  > 15 MVA AND < = 40 MVA REFURBISHED",6.9,4.2,4.5,3.9,3.4,3.9,4.5999999999999996]
[null,null,"Mobile Plant Renewal",0,0,0.1,0.2,1.8,0.9,0]
[null,null,"Hindley St Substation 66kV Yard Renewal",0,0,0,0.3,0.6,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C177),\"\",C177)","v":""}]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",2428,2428,2428,2428,2428,2428,2428]
[null,null,"> 1 kV & < = 11 kV",977,977,977,977,977,977,977]
[null,null,"˃ 11 kV & < = 22 kV",343,343,343,343,343,343,343]
[null,null,"> 22 kV & < = 66 kV",96,96,96,96,96,96,96]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",1121,1121,1141,1163,1185,1207,1230]
[null,null,"> 1 kV & < = 11 kV",145,145,129,129,130,131,133]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",102,102,108,113,118,123,128]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",6,6,9,10,10,10,11]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",549,549,558,563,567,571,575]
[null,null,"> 1 kV & < = 11 kV",116,116,106,106,106,107,107]
[null,null,"> 11 kV & < = 22 kV",6,6,6,6,6,6,6]
[null,null,"> 22 kV & < = 33 kV",6,6,10,10,10,10,10]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",4399,4399,4295,4300,4307,4315,4325]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",503,503,531,531,532,533,535]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",81,81,96,99,102,104,107]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",1,1,1,1,1,1,1]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",8,8,21,22,23,24,24]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",38,38,32,32,34,35,36]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",1,1,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",4,4,10,10,11,11,11]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",2,2,1,1,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",0.2,0,0.1,0.1,0.1,0.1,0.1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0.5,0.7,1.5,1.5,1.5,1.5,1.5]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0.3,0.4,0.9,0.9,0.9,0.9,0.9]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",0.1,0.3,0.7,0.6,0.7,0.7,0.7]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",24.2,16.3,7.8,0.1,0.1,0.1,0.1]
[null,null,"˂ = 11 kV ;  Circuit Breaker",0.2,0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",0.4,0.1,0.1,0.1,0.1,0.1,0.1]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0.2,0.4,0.4,0.4,0.4,0.4,0.3]
[null,null,"> 33 kV & < = 66 kV ; Switch",0.2,0.2,0.3,0.3,0.3,0.3,0.3]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",0.4,0.8,0.9,0.9,0.9,0.8,0.8]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",20,20,21,21,22,22,23]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",78,78,80,80,82,82,84]
[null,null,"Master Station Assets",0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",1,1,1,1,2,2,2]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"< = 1 kV; stobie pole",109,109,114,114,114,114,114]
[null,null,"> 1 kV & < = 11 kV; stobie pole",77,77,80,80,80,80,80]
[null,null,"> 11 kV & < = 22 kV; stobie pole",24,24,23,23,23,23,23]
[null,null,"> 22 kV & < = 66 kV; stobie pole",4,4,3,3,3,3,3]
[null,null,"> 66 kV & < = 132 kV; stobie pole",0,0,0,0,0,0,0]
[null,null,"> 132 kV; stobie pole",0,0,0,0,0,0,0]
[null,null,"Pole REFURBISHED; STOBIE Pole",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ;  < = 60kVA; DISTRIBUTION TRANSFORMER",4,4,4,4,4,4,4]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ; > 60 KVA AND < = 600 KVA; DISTRIBUTION TRANSFORMER",3,3,2,2,2,2,2]
[null,null,"Kiosk Mounted; > = 22 kV & < = 33 kV ; DISTRIBUTION TRANSFORMER",1,1,0,0,0,0,0]
[null,null,"Voltage regulator; DISTRIBUTION TRANSFORMER",30,30,30,30,30,30,30]
[null,null,"Recloser ;SWITCHGEAR",59,59,46,46,46,46,46]
[null,null,"Sectionalizer ;SWITCHGEAR",13,13,9,9,9,9,9]
[null,null,">= 11 kV & < = 22 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",6,6,7,7,7,7,7]
[null,null,"> 22 kV & < = 33 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",0,0,0,0,0,0,0]
[null,null,"OTHER - Distribution",0,0,0,0,0,0,0]
[null,null,"OTHER - Non Category Substation asset replacement/refurbishment",2.2999999999999998,3.7,3.4,3.6,3.8,3.8,3.8]
[null,null,"Pipework Bus Substation Replacements",0,0,0,0,0,0,0]
[null,null,"> = 11 kV ;  Circuit Breaker REFURBISHED",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker REFURBISHED",0,0,0,0,0,0,0]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":"> 33 kV & < = 66 kV ; Circuit Breaker REFURBISHED"},0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted;  22 kV ;  >  600 kVA ; Multiple Phase REFURBISHED",0,0,0,0,0,0,0]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > = 22 kV & < = 33 kV ;  < = 15 MVA REFURBISHED",0,0,0,0,0,0,0]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > 33 kV & < = 66 kV ;  < = 15 MVA REFURBISHED",0,0,0,0,0,0,0]
[null,null,"GROUND OUTDOOR / INDOOR CHAMBER MOUNTED ; > 33 kV & < = 66 kV ;  > 15 MVA AND < = 40 MVA REFURBISHED",0,0,0,0,0,0,0]
[null,null,"Mobile Plant Renewal",0,0,0,0,0,0,0]
[null,null,"Hindley St Substation 66kV Yard Renewal",0,0,0,0,0,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C177),\"\",C177)","v":""}]

{"sheet":"2.3 Augex (b)","index":5,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[68,1,69,2],[60,1,61,2],[45,1,46,2],[6,1,6,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.3 AUGEX PROJECT DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,null,null,"VOLUMES"]
[null,"PROJECT TYPE","UNITS",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,1.4]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.22,0,0,0.2,0,0,3.4]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0.25779999999999997,0.23799999999999999,0.218,0.21859999999999999,0.21909999999999999,0.21970000000000001,0.2205]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",1.7767999999999999,1.6400999999999999,1.5023,1.5063,1.5098,1.5141,1.5193000000000001]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",90,83,76,76,76,77,77]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",4.4000000000000004,0,0,1.8,0,0,0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",5.3644999999999996,4.9516999999999998,4.5357000000000003,4.5477999999999996,4.5583,4.5715000000000003,4.5869999999999997]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.1056,9.7500000000000003E-2,8.9300000000000004E-2,8.9499999999999996E-2,8.9700000000000002E-2,0.09,9.0300000000000005E-2]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",106,98,89,90,90,90,90]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,"PROJECT TYPE",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,760814.79,0,0,545604.23,0,0,424358.85]
[null,"HV Feeder Augmentations - Underground Cables",null,230063.12,0,0,209148.29,0,0,3555520.92]
[null,"HV Feeder Non-Material Projects",null,46824298.490000002,46744909.109999999,50635444.149999999,44898277.280000001,47736501.759999998,47721640.490000002,46586278.020000003]
[null,"LV Feeder Augmentations - Overhead Lines",null,814992.83,728460.28,885594.85,887965.06,890012.06,892597.73,895614.36]
[null,"LV Feeder Augmentations - Underground Cables",null,282541.71000000002,252542.61,307018.03000000003,307839.73,308549.38,309445.78000000003,310491.59000000003]
[null,"LV Feeder Non-Material Projects",null,808035.09,722241.29,878034.38,880384.35,882413.87,884977.47,887968.34]
[null,"Distribution Substation Augmentations - Pole Mounted",null,404988.4,361988.42,440072.15,441249.96,442267.16,443552.04,445051.07]
[null,"Distribution Substation Augmentations - Ground Mounted",null,0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,21140010.510000002,19453628.780000001,33088936.879999999,37826957.57,30248414.32,33901698.609999999,52777102.969999999]
[null,"Subtransmission Lines",null,5990445.1600000001,8538365.0199999996,10285971.68,9211726.9600000009,16580007.68,20632173.079999998,6034018.6799999997]
[null,"HV Feeders",null,47815176.399999999,46744909.109999999,50635444.149999999,45653029.799999997,47736501.759999998,47721640.490000002,50566157.789999999]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,404988.4,361988.42,440072.15,441249.96,442267.16,443552.04,445051.07]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,1905569.63,1703244.18,2070647.26,2076189.14,2080975.31,2087020.99,2094074.29]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,2950558,2302800,377375,1957505,7043269,15521838,15440004]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,74305632,74499336,96143697,93251648,90044897,89264248,96476401]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,2327564,2302800,377375,1957505,1580130,215355,8754015]
[null,"Subtransmission Lines",null,0,0,0,0,5463139,13462923,4842429]
[null,"HV Feeders",null,622994,0,0,0,0,1843560,1843560]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,0,0,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]

{"sheet":"2.5 Connections","index":6,"n_rows":212,"n_cols":17,"rows_kept":212,"cut":false,"hidden":false,"merged":[[6,1,6,2],[10,1,11,1],[10,2,11,2],[10,3,11,3],[55,1,56,1],[55,2,56,2],[55,3,56,3],[11,16,11,93],[12,16,12,93],[139,1,140,1],[139,2,140,3],[103,1,104,1],[103,2,104,2],[103,3,104,3],[121,1,122,1],[121,2,122,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.5 CONNECTIONS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,null,null,null,null,"DRAFT TEMPLATE ONLY"]
[null,"RESIDENTIAL","Underground connections","0's",6124,5628,6067,6552,6762,6836,6823,null,null,null,null,null,"DO NOT USE FOR SUBMISSIONS"]
[null,null,"Overhead connections","0's",106,97,105,113,117,118,118]
[null,null,"Distribution substations installed","MVA added",3,2,3,3,3,3,3]
[null,null,"Distribution substations installed","0's",60,55,59,64,66,67,67]
[null,null,"Distribution substations installed ","total spend $0s",1340370.72,1231800.6950000001,1323324.8289999999,1434177.8219999999,1484485.5330000001,1506508.365,1509908.2390000001]
[null,null,"Augmentation HV ","net circuit KM added",2,2,2,3,3,3,3]
[null,null,"Augmentation HV","total spend $0s",465035.42,427367.55099999998,459121.42599999998,497581.359,515035.38699999999,522676.10600000003,523855.67700000003]
[null,null,"Augmentation LV","net circuit KM added",3,3,3,3,3,3,3]
[null,null,"Augmentation LV","total spend $0s",607654.89,558434.84699999995,599927.16500000004,650182.18999999994,672989.10900000005,682973.12399999995,684514.451]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",11,11,11,11,11,11,11]
[null,null,"Volume of GSL breaches for residential customers","0's",205,205,205,205,205,205,205]
[null,null,"Volume of customer complaints relating to connection services","0's",220,220,220,220,220,220,220]
[null,null,"GSL payments","$",72318,72318,72318,72318,72318,72318,72318]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",646,719,663,651,678,702,681]
[null,null,"Overhead connections","0's",105,117,108,106,110,114,111]
[null,null,"Distribution substations installed","MVA added",95,105,97,95,99,103,100]
[null,null,"Distribution substations installed","0's",211,235,216,212,221,229,222]
[null,null,"Distribution substations installed ","total spend $0s",11393274.68,12686411.351,11667945.481000001,11479926.205,11976533.716,12420791.693,12062846.751]
[null,null,"Augmentation HV ","net circuit KM added",21,24,22,22,22,23,23]
[null,null,"Augmentation HV","total spend $0s",5126020.08,5707823.3609999996,5249598.9570000004,5165006.0180000002,5388437.8360000001,5588316.7450000001,5427271.4780000001]
[null,null,"Augmentation LV","net circuit KM added",8,8,8,8,8,8,8]
[null,null,"Augmentation LV","total spend $0s",3154638.66,3512690.145,3230691.1680000001,3178631.2560000001,3316134.9410000001,3439143.7710000002,3340033.8149999999]
[null,"SUBDIVISION","Underground connections","0's",184,168,175,179,165,143,142]
[null,null,"Overhead connections","0's",35,32,33,34,31,27,27]
[null,null,"Distribution substations installed","MVA added",22,20,21,21,19,17,17]
[null,null,"Distribution substations installed","0's",68,62,65,66,61,53,53]
[null,null,"Distribution substations installed ","total spend $0s",3890039.42,3559386.0669999998,3690139.236,3790768.3280000002,3486519.7030000002,3037096.7889999999,3027076.1710000001]
[null,null,"Augmentation HV ","net circuit KM added",14,13,13,14,13,11,11]
[null,null,"Augmentation HV","total spend $0s",3188999.4670000002,2917934.5120000001,3025124.1159999999,3107618.4270000001,2858199.6940000001,2489769.125,2481554.3640000001]
[null,null,"Augmentation LV","net circuit KM added",36,33,34,35,32,28,28]
[null,null,"Augmentation LV","total spend $0s",12764998.848999999,11679973.947000001,12109034.905999999,12439244.99,11440866.072000001,9966103.9000000004,9933221.6679999996]
[null,null,"Cost per lot","$",3258,2981,3097,3175,2914,2533,2517]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Underground connections","0's",6124,5628,6067,6552,6762,6836,6823]
[null,null,"Overhead connections","0's",106,97,105,113,117,118,118]
[null,null,"Distribution substations installed","MVA added",3,2,3,3,3,3,3]
[null,null,"Distribution substations installed","0's",60,55,59,64,66,67,67]
[null,null,"Distribution substations installed ","total spend $0s",1340370.72,1231800.69,1323324.83,1434177.82,1484485.53,1506508.36,1509908.24]
[null,null,"Augmentation HV ","net circuit KM added",2,2,2,3,3,3,3]
[null,null,"Augmentation HV","total spend $0s",465035.42,427367.55,459121.43,497581.36,515035.39,522676.11,523855.68]
[null,null,"Augmentation LV","net circuit KM added",3,3,3,3,3,3,3]
[null,null,"Augmentation LV","total spend $0s",607654.89,558434.85,599927.16,650182.18999999994,672989.11,682973.12,684514.45]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",11,11,11,11,11,11,11]
[null,null,"Volume of GSL breaches for residential customers","0's",205,205,205,205,205,205,205]
[null,null,"Volume of customer complaints relating to connection services","0's",220,220,220,220,220,220,220]
[null,null,"GSL payments","$",72318,72318,72318,72318,72318,72318,72318]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",646,719,663,651,678,702,681]
[null,null,"Overhead connections","0's",105,117,108,106,110,114,111]
[null,null,"Distribution substations installed","MVA added",95,105,97,95,99,103,100]
[null,null,"Distribution substations installed","0's",211,235,216,212,221,229,222]
[null,null,"Distribution substations installed ","total spend $0s",11393274.68,12686411.35,11667945.48,11479926.199999999,11976533.720000001,12420791.689999999,12062846.75]
[null,null,"Augmentation HV ","net circuit KM added",21,24,22,22,22,23,23]
[null,null,"Augmentation HV","total spend $0s",5126020.08,5707823.3600000003,5249598.96,5165006.0199999996,5388437.8399999999,5588316.75,5427271.4800000004]
[null,null,"Augmentation LV","net circuit KM added",8,8,8,8,8,8,8]
[null,null,"Augmentation LV","total spend $0s",3154638.66,3512690.14,3230691.17,3178631.26,3316134.94,3439143.77,3340033.81]
[null,"SUBDIVISION","Underground connections","0's",184,168,175,179,165,143,142]
[null,null,"Overhead connections","0's",35,32,33,34,31,27,27]
[null,null,"Distribution substations installed","MVA added",22,20,21,21,19,17,17]
[null,null,"Distribution substations installed","0's",68,62,65,66,61,53,53]
[null,null,"Distribution substations installed ","total spend $0s",3890039.42,3559386.07,3690139.24,3790768.33,3486519.7,3037096.79,3027076.17]
[null,null,"Augmentation HV ","net circuit KM added",14,13,13,14,13,11,11]
[null,null,"Augmentation HV","total spend $0s",3188999.47,2917934.51,3025124.12,3107618.43,2858199.69,2489769.13,2481554.36]
[null,null,"Augmentation LV","net circuit KM added",36,33,34,35,32,28,28]
[null,null,"Augmentation LV","total spend $0s",12764998.85,11679973.949999999,12109034.91,12439244.99,11440866.07,9966103.9000000004,9933221.6699999999]
[null,null,"Cost per lot","$",3258,2981,3097,3175,2914,2533,2517]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL SERVICE CLASSIFICATIONS (including capcons)"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,16661417,14034517,15967440,16447012,16849273,17119137,16854025]
[null,null,"Complex connection LV",null,4109776,3461814,3938597,4056890,4156113,4222679,4157285]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,3227615,3294139,3201995,3000414,3103583,3229706,3088887]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,34704221,35419510,34428749,32261291,33370593,34726705,33212581]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,28301865,28885194,28077213,26309615,27214269,28320201,27085407]
[null,null,"Complex connection HV (customer connected at HV)",null,11971315,12218056,11876291,11128620,11511277,11979071,11456770]
[null,null,"Complex connection sub-transmission",null,4585345,4679853,4548948,4262569,4409137,4588315,4388260]
[null,"SUBDIVISION","Complex connection LV",null,2183105,1902542,1852883,1903272,1749542,1523336,1518867]
[null,null,"Complex connection HV (no upstream asset works)",null,50385251,41311429,32377612,32528602,32067952,31390130,31376740]
[null,null,"Complex connection HV (with upstream asset works)",null,3481548,3034114,2954920,3035279,2790114,2429368,2422242]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,847393,877904,991329,978986,784610]
[null,null,"Complex connection HV (large capacity)",null,0,0,10267822,10637520,12011885,11862323,9507079]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES (excluding capcons)"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,14127555,12036637,13261822,13775739,14141347,14358445,14194676]
[null,null,"Complex connection LV",null,1931279,1744129,1612431,1760254,1827964,1849164,1870901]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1719234,1853113,1534709,1502901,1570812,1629201,1591163]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,13331136,15000799,10804046,11042202,11651913,12048249,11990491]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,18212631,19246476,16925096,16293076,16961896,17614763,17067452]
[null,null,"Complex connection HV (customer connected at HV)",null,2138625,2824426,1007743,1366776,1519595,1545845,1693545]
[null,null,"Complex connection sub-transmission",null,-4411150,-3914920,-5395312,-4669104,-4732828,-4957644,-4544677]
[null,"SUBDIVISION","Complex connection LV",null,-724128,-555174,-1138235,-1169190,-1074752,-935793,-933048]
[null,null,"Complex connection HV (no upstream asset works)",null,17068024,10421803,11082002,11018617,11211995,11496539,11502160]
[null,null,"Complex connection HV (with upstream asset works)",null,-247955,-118733,-882195,-906186,-832992,-725291,-723163]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,-50876,-52642,-59498,-58748,-47077]
[null,null,"Complex connection HV (large capacity)",null,0,0,-616465,-637855,-720934,-711850,-570425]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,2533862,1997880,2705618,2671272,2707926,2760692,2659349]
[null,null,"Complex connection LV",null,2178497,1717684,2326165,2296636,2328149,2373515,2286385]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1508381,1441027,1667286,1497512,1532771,1600506,1497724]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,21373086,20418711,23624703,21219089,21718680,22678456,21222090]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,10089233,9638718,11152117,10016539,10252373,10705438,10017955]
[null,null,"Complex connection HV (customer connected at HV)",null,9832691,9393631,10868548,9761844,9991682,10433226,9763225]
[null,null,"Complex connection sub-transmission",null,8996495,8594774,9944260,8931674,9141965,9545960,8932937]
[null,"SUBDIVISION","Complex connection LV",null,2907233,2457716,2991119,3072462,2824294,2459128,2451915]
[null,null,"Complex connection HV (no upstream asset works)",null,33317226,30889626,21295611,21509985,20855957,19893590,19874580]
[null,null,"Complex connection HV (with upstream asset works)",null,3729503,3152847,3837115,3941465,3623107,3154659,3145405]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,898270,930546,1050827,1037734,831687]
[null,null,"Complex connection HV (large capacity)",null,0,0,10884287,11275374,12732819,12574173,10077504]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,6079,5587,6022,6504,6712,6786,6772]
[null,null,"Complex connection LV",null,151,139,150,162,167,169,168]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,396,440,406,399,415,430,417]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,300,334,308,302,315,326,316]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,55,62,57,56,58,60,58]
[null,null,"Complex connection HV (customer connected at HV)",null,3,4,3,3,3,4,3]
[null,null,"Complex connection sub-transmission",null,0,1,0,0,0,0,1]
[null,"SUBDIVISION","Complex connection LV",null,73,67,69,71,65,57,56]
[null,null,"Complex connection HV (no upstream asset works)",null,108,99,103,106,97,84,84]
[null,null,"Complex connection HV (with upstream asset works)",null,38,34,36,37,34,29,29]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,110,157,199,197,213,212,227]
[null,null,"Complex connection HV (large capacity)",null,14,19,24,24,26,26,28]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,6079,5587,6022,6504,6712,6786,6772]
[null,null,"Complex connection LV",null,151,139,150,162,167,169,168]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,396,440,406,399,415,430,417]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,300,334,308,302,315,326,316]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,55,62,57,56,58,60,58]
[null,null,"Complex connection HV (customer connected at HV)",null,3,4,3,3,3,4,3]
[null,null,"Complex connection sub-transmission",null,0,1,0,0,0,0,1]
[null,"SUBDIVISION","Complex connection LV",null,73,67,69,71,65,57,56]
[null,null,"Complex connection HV (no upstream asset works)",null,108,99,103,106,97,84,84]
[null,null,"Complex connection HV (with upstream asset works)",null,38,34,36,37,34,29,29]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,110,157,199,197,213,212,227]
[null,null,"Complex connection HV (large capacity)",null,14,19,24,24,26,26,28]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RESIDENTIAL","Simple connection LV",null,831552,837139,843161,849665,856377,863163,869935]
[null,null,"Complex connection LV",null,11988,12127,12277,12439,12606,12775,12943]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,54169,54609,55015,55414,55829,56259,56676]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,23817,24151,24459,24761,25076,25402,25718]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,4366,4428,4485,4541,4599,4659,4717]
[null,null,"Complex connection HV (customer connected at HV)",null,238,242,245,248,251,255,258]
[null,null,"Complex connection sub-transmission",null,0,1,1,1,1,1,2]
[null,"SUBDIVISION","Complex connection LV",null,5796,5863,5932,6003,6068,6125,6181]
[null,null,"Complex connection HV (no upstream asset works)",null,8574,8673,8776,8882,8979,9063,9147]
[null,null,"Complex connection HV (with upstream asset works)",null,3017,3051,3087,3124,3158,3187,3216]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,1556,1713,1912,2109,2322,2534,2761]
[null,null,"Complex connection HV (large capacity)",null,198,217,241,265,291,317,345]

{"sheet":"2.6 Non-network","index":7,"n_rows":112,"n_cols":11,"rows_kept":112,"cut":false,"hidden":false,"merged":[[56,1,57,3],[56,4,56,10],[6,1,6,2],[13,1,17,1],[20,1,30,1],[33,1,37,1],[40,1,50,1],[85,1,89,1],[63,4,63,10],[65,1,69,1],[70,1,74,1],[75,1,79,1],[80,1,84,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.6 NON-NETWORK EXPENDITURE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,39924280,41928893,69727456,76714621,78807581,79441956,81467905]
[null,"MOTOR VEHICLES","Car",null,439206,556791,566648,576504,579774,595902,611588]
[null,null,"Light commercial vehicle",null,3211691,4071536,4143611,4215685,4239597,4357536,4472234]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,5311643,6733695,6852894,6972094,7011642,7206694,7396387]
[null,null,"Heavy commercial vehicle",null,947037,1200581,1221834,1243087,1250138,1284914,1318736]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,6409143,6477861,6481789,6502494,6519817,6578712,6662580]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","TEC Vehicles",null,1345067,1705173,1735358,1765543,1775558,1825568,1873604]
[null,null,"Cranes",null,988213,1252780,1274957,1297134,1304492,1341234,1376525]
[null,null,"Trailers",null,1180365,1496377,1522865,1549354,1558143,1602029,1644183]
[null,null,"Other Commercial Vehicles",null,301954,382794,389570,396346,398595,409821,420605]
[null,null,"Network Telephony",null,1257296,1288853,1274964,1279037,1282444,1294029,1310526]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,47905299,59715199,55046668,62743518,63044261,60503760,59479099]
[null,"MOTOR VEHICLES","Car",null,1068558.7173443981,311937.49918155745,963085.58380000002,2255639.2384000001,2547393.6260000002,1093483.0907999999,1943051.0436]
[null,null,"Light commercial vehicle",null,6433346.8031435758,7546928.7785495352,10735379.184,10120883.156599998,7980045.5200000005,8592915.4240000006,8035922.6277999999]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,10030554.866347492,9848004.2719544992,9446182.8054000009,6728875.8717999989,12662994.015799999,18746006.8638,8758916.1926000006]
[null,null,"Heavy commercial vehicle",null,1388796.0227595516,1782637.6948497766,4993802.8332000002,715317.00040000002,2488528.7776000001,3459763.4774000002,767508.62540000002]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,18878329,10606684,23942086,34512600,17726826,17754768,21855815]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","TEC Vehicles",null,1524959.1287330135,1179164.9965701753,1089774,1150317.0004,423800.99959999998,968687.99979999999,1089774.0001999999]
[null,null,"Cranes",null,2051682.6549173864,2786173.7920053289,659645.00040000002,1319289.9998000001,3433225.0002000001,3882125,5817160.0004000003]
[null,null,"Trailers",null,1140055.9677109122,955971.59730894817,767924.99939999997,2702279.0002000001,2438690.9671999998,1685192.0004,3101482.0002000001]
[null,null,"Other Commercial Vehicles",null,526001.67662243312,136978.59961408388,0,105811.99980000001,238404.00039999999,752927.99979999999,249642.00039999999]
[null,null,"ADMS Hardware Upgrade",null,0,0,577333,4161821,405041,0,0]
[null,null,"ADMS Software Upgrade",null,0,0,1674265,9132885,11398998,0,0]
[null,null,"Additional ADMS Functions",null,0,0,1004559,1005773,1006815,1008144,1009644]
[null,null,"ADMS/OMS Replacement",null,6635759,1107228,0,0,0,0,0]
[null,null,"Other Network Strategic",null,445224,2032207,3796558,3797557,4157462,3799506,3800740]
[null,null,"Non-Network Telecommuniations",null,1310257,1081704,741342,2505022,1057602,499106,2117805]
[null,null,"Non-Network Plant and Tools",null,3747786,3862700,4870205,4870205,4870205,4870205,4870205]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Employee numbers",null,null,1989,2001,2208,2206,2300,2334,2414]
[null,"User numbers",null,null,2984,3002,3312,3309,3450,3502,3621]
[null,"Number of devices",null,null,6266,6304,6956,6949,7244,7353,7605]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  or PER CENT"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","UNITS",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"CAR","Average kilometres travelled ","0's",11393,11393,11393,11393,11393,11393,11393]
[null,null,"Number purchased","0's",21,6,13,38,43,9,23]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",136,136,149,149,149,149,150]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%","87%","87%","87%","87%","87%","87%","87%"]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",18734,18734,18734,18734,18734,18734,18734]
[null,null,"Number purchased","0's",89,105,132,134,108,122,111]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",517,517,595,597,611,620,634]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%","87%","87%","87%","87%","87%","87%","87%"]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",14988,14988,14988,14988,14988,14988,14988]
[null,null,"Number purchased","0's",19,18,15,13,21,38,17]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",176,176,175,176,186,193,197]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%","87%","87%","87%","87%","87%","87%","87%"]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",8486,8486,8486,8486,8486,8486,8486]
[null,null,"Number purchased","0's",6,7,20,3,10,14,3]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",72,72,87,87,90,93,96]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%","87%","87%","87%","87%","87%","87%","87%"]
[]
[]
[null,"Table 2.6.4 intentionally omitted"]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"RECURRENT"]
[null,"ICT001 - IT Applications Refresh",null,null,13119175,17185263,13516577,14573126,13992379,14629332,15960375]
[null,"ICT002 - Client Device Refresh",null,null,5685439,6308059,7253090,7131630,7909855,7777813,7145804]
[null,"ICT003 - Cyber Security Refresh",null,null,3723676,3954821,0,0,0,0,0]
[null,"ICT015 - Data Mgmt & Analytics",null,null,2674172,2444882,1942977,3421770,3091126,2557524,2791679]
[null,"ICT004 - IT Infrastructure Refresh",null,null,5077270,6716247,10895392,5940466,4926352,9821277,7916020]
[null,"ICT040-045 Network Uplift - IT Costs",null,null,0,0,1140331,13853,444833,178336,372146]
[]
[]
[]
[]
[null,"NON-RECURRENT"]
[null,"COMPLIANCE",null,null,2560211,2612508,68950,1188446,965855,1046563,2091260]
[null,"MAJOR UPGRADES",null,null,8833043,10480599,14971101,21803792,22670914,17307792,17057984]
[null,"NEW OR EXPANDED CAPABILITY",null,null,6232312,10012820,5258249,8670436,9042946,7185124,6143829]

{"sheet":"2.10 Overheads","index":8,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[6,1,6,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.10 OVERHEADS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",98397895,102817373,113038531,107544596,108690569,110080648,111832160]
[null,"Alternative Control Services","Total  ",3627912,3647457,2446142,2446982,2454902,2458372,2471018]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",6551264,6364032,8372654,8431900,8863296,8454242,8607092]
[null,"Alternative Control Services","Total  ",233196,220410,198324,184712,180390,162656,145326]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total  ",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",62364547,62914460,66025967,65937171,66312251,66664515,67529422]
[null,"Alternative Control Services","Total  ",10629459,10885983,11817481,12382788,12568516,12578084,12780597]
[null,"CAPEX"]
[null,"Standard Control Services","Total",-5877666,-5854775,-6528751,-6528751,-6528751,-6528751,-6528751]
[null,"Alternative Control Services","Total",-52991,-54270,-68412,-71736,-72922,-73390,-74801]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",898594,920280,1160092,1216454,1236568,1244514,1268440]

{"sheet":"2.11 Labour","index":9,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.11 LABOUR"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"In-house labour expenditure",129271293,133220931,152383007,153300665,154929472,156435334,158810805]
[null,"Labour expenditure outsourced to related parties",8801804,9070726,10375431,10437912,10548814,10651345,10813086]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Controllable non-labour expenditure",192285159,198251108,228013465,229415162,231921215,234198172,237798447]
[null,"Uncontrollable non-labour expenditure",7889713,8039726,7949588,7968872,7985004,8039855,8117965]
[null,"Total",{"$f":"SUM(C13:C17)","v":338247969},348582491,398721491,401122611,405384505,409324706,415540303]
[null,"CAPEX"]
[null,"In-house labour expenditure",163845569,158750062,192323628,196354175,205476100,194363718,199443449]
[null,"Labour expenditure outsourced to related parties",6286583,6037721,7051151,7168916,7213012,7084738,7008906]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Controllable non-labour expenditure",335464237,322046786,375507539,381779062,384127380,377296184,373257776]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C20:C24)","v":505596389},486834569,574882318,585302153,596816492,578744640,579710131]

{"sheet":"2.14 Forecast price changes","index":10,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[[6,1,6,2],[12,4,12,8],[8,1,8,2],[9,1,9,2],[12,2,12,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There is ONE table on this worksheet."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. FORECAST price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"SA Power Networks must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. FORECAST price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"FORECAST"]
[null,"DESCRIPTION",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"OPEX"]
[null,"Real labour escalations",null,null,"1.16%","0.61%","0.52%","0.66%","0.74%"]
[null,"Real non-labour escalations",null,null,"0.00%","0.00%","0.00%","0.00%","0.00%"]
[null,"CPI",3.5999999999999997E-2,3.1E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2]
[null,"CAPEX"]
[null,"Real labour escalations","0.60%","1.03%","1.16%","0.61%","0.52%","0.66%","0.74%"]
[null,"Real contracts esclations","0.11%","0.96%","0.91%","0.78%","0.39%","0.68%","0.89%"]
[null,"CPI",4.1000000000000002E-2,3.3000000000000002E-2,2.8000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2]

{"sheet":"2.16 Opex Summary","index":11,"n_rows":62,"n_cols":12,"rows_kept":62,"cut":false,"hidden":false,"merged":[[9,1,9,7],[9,9,9,10],[6,9,6,11],[7,1,7,7],[7,9,7,10],[7,11,8,11],[8,1,8,7],[8,9,8,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.16 OPEX SUMMARY"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nSA Power Networks's total forecast opex must reconcile to Table 2.16.1 (and if SA Power Networks owns any dual function assets Table 2.16.3). If SA Power Networks did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if SA Power Networks owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has SA Power Networks used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If SA Power Networks does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2023-24"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Base year total opex, excluding category specific",null,null,null,355188433.80000001,355188433.80000001,358176386.80000001,358176386.80000001,358176386.80000001,358176386.80000001,358176386.80000001]
[null,"Increment from base year to final year",null,null,null,null,2987952.96]
[null,"Price growth",null,null,null,null,null,1632453.3049999999,3254038.8429999999,4858907.983,8467792.8000000007,13297783.74]
[null,"Output growth",null,null,null,null,null,2452581.639,3734627.0860000001,4807695.1840000004,6200023.4139999999,7754904.7000000002]
[null,"Productivity growth",null,null,null,null,null,-1783677.4509999999,-3535797.3339999998,-5250366.72,-6976185.1289999997,-8696804.6060000006]
[null,"Step changes",null,null,null,null,null,16916747.260000002,24814078.120000001,28018968.649999999,28590552.280000001,30465139.809999999]
[null,"Category specific",null,null,null,null,null,9489329.9800000004,2629713.3739999998,2629713.3739999998,2629713.3739999998,2629713.3739999998]
[null,"Total opex",{"$f":"SUM(C16:C22)","v":0},0,0,355188433.80000001,358176386.75999999,386883821.53300005,389073046.88900006,393241305.27099997,397088283.53899997,403627123.81800002]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C29:C35)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Base year total opex, excluding category specific"]
[null,"Increment from base year to final year"]
[null,"Price growth"]
[null,"Output growth"]
[null,"Productivity growth"]
[null,"Step changes"]
[null,"Category specific"]
[null,"Total opex",{"$f":"SUM(C42:C48)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y1","v":"2020-21"},{"$f":"CRCP_y2","v":"2021-22"},{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C55:C61)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":12,"n_rows":133,"n_cols":11,"rows_kept":133,"cut":false,"hidden":false,"merged":[[55,1,55,3],[29,1,29,3],[30,1,30,3],[132,1,132,2],[106,1,106,3],[80,1,80,3],[81,1,81,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"2.17 STEP CHANGES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Cyber Security Uplift","To implement a comprehensive cyber security uplift program.",null,null,null,4611828.6666478869,10873557.999561686,11346313.905276995,10447467.247194095,10369287.734141586]
[null,"Smart Meter Rollout - IT upgrades","To store and secure greater volumes of data from the increasing number of smart meters.",null,null,null,360624.01313131314,601040.02188552194,841456.03063973051,1202080.0437710439,1803120.0656565658]
[null,"IT Infrastructure Refresh","To ensure our existing services continue to function with sufficient capacity for growth and efficiently managed storage.",null,null,null,799189.1733604538,1280078.3343307127,1996643.6943198279,2665187.6551176356,3191566.331314811]
[null,"Operationalising Cyber Security ","To maintain our existing cyber security and IT resilience capabilities.",null,null,null,3473247.7564878934,3473247.7564878934,3473247.7564878934,3473247.7564878934,3473247.7564878934]
[null,"CER Compliance","To execute the second phase of the long-term CER compliance program.",null,null,null,314832.48499286285,520945.83847739897,520945.83847739897,588895.29567010328,588895.29567010328]
[null,"CER Integration","To continue the scaling and maintenance of IT systems to enable our flexible exports program.",null,null,null,606740.41295641928,742182.41930308216,874821.45733753312,1004315.8935302894,1130782.9648249494]
[null,"Network Visability","To build on the foundations established in the current RCP to significantly enhance our Network visibility capability.",null,null,null,1046295.3044742364,1203917.6348299044,1360716.0827715516,1516287.2892257452,1623698.7826665114]
[null,"Increases to Insurance Premiums","To reflect the significant market driven increases that are expected to apply to our insurance premiums.",null,null,null,2233861.5272937086,3315633.2136974111,4141274.8675422701,4639723.7877915036,5068555.1339645386]
[null,"Network Program Uplift","To support the proposed uplift in our total network capital program.",null,null,null,3538194.5131724388,3020118.5437933011,3871516.7218441218,3607138.979733103,3969953.0212938539]
[null,"Reliability Improvements","Resulting from a reduction in network interruptions achieved by proposed augex on our reliability programs.",null,null,null,-36062.401313131311,-84145.603063973089,-132228.80481481482,-180312.00656565657,-228395.20831649835]
[null,"Transitioning to Electric Vehicles","Resulting from reductions in fuel and maintenance that is expected to occur as a result of proposed EV program.",null,null,null,-32004.194337763685,-132498.04405291358,-275738.89728799375,-373479.66149588593,-525572.06402126886]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E10:E29)","v":0},0,16916747.256866321,24814078.115250025,28018968.65259451,28590552.28045987,30465139.813683048]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$30,0)-ROUND('2.16 Opex Summary'!H$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$30,0)-ROUND('2.16 Opex Summary'!I$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$30,0)-ROUND('2.16 Opex Summary'!J$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$30,0)-ROUND('2.16 Opex Summary'!K$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$30,0)-ROUND('2.16 Opex Summary'!L$21,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E36:E55)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E61:E80)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$30,0)-ROUND('2.16 Opex Summary'!H$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$30,0)-ROUND('2.16 Opex Summary'!I$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$30,0)-ROUND('2.16 Opex Summary'!J$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$30,0)-ROUND('2.16 Opex Summary'!K$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$30,0)-ROUND('2.16 Opex Summary'!L$47,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E87:E106)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE \n($, real June 2024)"]
[null,"CATEGORY","DESCRIPTION",{"$f":"CRCP_y3","v":"2022-23"},{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Enactment of the Small Compensation Claims Regime","To meet an expected new regulatory obligation relating to claims and damages that will apply to us from 1 July 2025",null,null,null,8379166.2556425305,2322061.2637874912,2322061.2637874912,2322061.2637874912,2322061.2637874912]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D113:D132)","v":0},{"$f":"SUM(E113:E132)","v":0},{"$f":"SUM(F113:F132)","v":0},8379166.2556425305,2322061.2637874912,2322061.2637874912,2322061.2637874912,2322061.2637874912]

{"sheet":"3.1 Revenue","index":13,"n_rows":51,"n_cols":17,"rows_kept":51,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[29,2,29,8],[29,10,29,16],[42,2,42,8],[42,10,42,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.1 REVENUE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DREV0101","Revenue from Fixed Customer Charges ",204125589.46000001,228010064.22999999,231688392.16999999,231784738.50999999,229987447.74000001,236682420.56999999,232084431.44,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",219670242.44,183393509.40000001,152234167.78,124671126.04000001,95170000.180000007,68748743.290000007,37135505.740000002,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",197666717.18000001,228807901.93000001,236085398.06999999,256766914.06,278433816.87,319114810.41000003,340734455.18000001,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",36640165.719999999,53064658.509999998,59012903.520000003,63393969.670000002,68839067.349999994,78561402.329999998,84186189.700000003,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",83514881.950000003,109669480.98,129684196.54000001,136751744.69,144144420.19,161883585.52000001,170123371.90000001,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",19462294.23,22521101.699999999,24630014.379999999,24838127.359999999,24484711.09,25099549.34,24451879.039999999,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",6931127.8600000003,7225050.71,6729009.7300000004,6306125.5499999998,6245817.8700000001,6595189.6100000003,6576723.1600000001,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",11454366.279999999,10578120.51,8383980.4800000004,8012813.9100000001,7833523.2800000003,8110205.0099999998,7895447.0199999996,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",101398265.23999999,117614751.73999999,99897675.790000007,100294369.66,102187730.28,109731637.56999999,111163705.95,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,12695067.68,12534900.189999999,12377114.970000001,12581701.029999999,12583508.82,null,15874962.84,15716213.210000001,0,0,0,0,0]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,65496943,64327777,64912360,64912360,64912360,64912360,64912360]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,18958704,18905758,18287637,18462187,18622958,18727201,18773887]
["DREV0113","Revenue from other Sources",3457015.77,2941491.55,3702746.66,3867948.9,4046635.2,4163295.69,4301898.55,null,62673368,62484958,60455164,58890087,56935369,55110966,53547192]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":884320666.13},963826131.25999999,964743552.79999983,969222778.53999996,973750285.01999998,1031272540.3700001,1031237116.5,null,{"$f":"SUM(K13:K25)","v":163003977.84},161434706.21000001,143655161,142264634,140470687,138750527,137233439]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DREV0201","Revenue from residential Customers ",476075282.00999999,480325751.97000003,501367437.87,510476267.31,510954180.56,539082526.91999996,537310615.72000003,null,14086828.99,13945960.699999999,0,0,0,0,0]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",113694655.68000001,130476849.38,124198996.61,119863372.22,117354658.94,120858423.64,117381658.73999999,null,1735152.97,1717801.44,0,0,0,0,0]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",234979877.83000001,288318862.94999999,279144201.33999997,280096989.92000002,286541302.02999997,308988795.45999998,314311366.36000001,null,52331.14,51807.83,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",49182706.990000002,54538124.719999999,53303907.270000003,52480023.530000001,52654325.619999997,55747604.740000002,55656752.530000001,null,649.74,643.24,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",6931127.8600000003,7225050.71,6729009.7300000004,6306125.5499999998,6245817.8700000001,6595189.6100000003,6576723.1600000001,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",3457015.77,2941491.55,0,0,0,0,0,null,147129015,145718493,143655161,142264634,140470687,138750527,137233439]
["DREV02","Total revenue by customer class",{"$f":"SUM(C33:C38)","v":884320666.1400001},963826131.27999997,964743552.81999993,969222778.52999997,973750285.01999998,1031272540.37,1031237116.51,null,{"$f":"SUM(K33:K38)","v":163003977.84},161434706.21000001,143655161,142264634,140470687,138750527,137233439]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DREV0301","EBSS",2237060.23,0,5167583.47,-26689913.129999999,-26063498.850000001,27182149.77,0,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",16927023.23,11954909,8000000,9756097.5600000005,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",16427267.85,15780276.51,-2321713.2000000002,-2321713.2000000002,-2321713.2000000002,-2321713.2000000002,-2321713.2000000002,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C46:C50)","v":35591351.310000002},27735185.509999998,10845870.27,-19255528.77,-28385212.050000001,24860436.57,-2321713.2000000002,null,{"$f":"SUM(K46:K50)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":14,"n_rows":76,"n_cols":17,"rows_kept":76,"cut":false,"hidden":false,"merged":[[10,2,10,8],[10,10,10,16],[67,2,67,8],[67,10,67,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.2 OPERATING EXPENDITURE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOPEX0101","Distribution licence fee",3286144,3368623,3306711,3317274,3326111,3356156,3398942,null,0,0,0,0,0,0,0]
["DOPEX0102","Network operating costs",33599934,34443263,35418514,35685935,35934593,36402479,36954635,null,0,0,0,0,0,0,0]
["DOPEX0103","Inspections",17560453,18001204,17781719,17838521,17886043,18047612,18277691,null,0,0,0,0,0,0,0]
["DOPEX0104","Maintenance & repair",22431732,22994749,22695361,22767859,22828512,23034728,23328385,null,451992,451992,0,0,0,0,0]
["DOPEX0105","Substation property maintenance",8013897,8215039,8122518,8148464,8170172,8243975,8349073,null,0,0,0,0,0,0,0]
["DOPEX0106","Vegetation management",47991578,49196124,48563966,48719099,48848885,49290149,49918523,null,0,0,0,0,0,0,0]
["DOPEX0107","Emergency response",44275131,45386397,44839604,44934872,45006717,45366386,45898953,null,0,0,0,0,0,0,0]
["DOPEX0108","Guaranteed service level payments",5469239,5606512,5542302,5560006,5574818,5625177,5696889,null,0,0,0,0,0,0,0]
["DOPEX0109","Network insurance",7481108,8603274,9785585,10891480,11737303,12304369,12830913,null,0,0,0,0,0,0,0]
["DOPEX0110","Call centre",3291158,3373763,3381294,3380250,3401134,3423119,3471149,null,0,0,0,0,0,0,0]
["DOPEX0111","Customer billing (previously full retail contestability)",16786581,17207909,17009164,17063498,17108954,17263504,17483587,null,939910,939910,0,0,0,0,0]
["DOPEX0112","Meter reading",0,0,0,0,0,0,0,null,4642245,3829111,0,0,0,0,0]
["DOPEX0113","Other customer services",19363044,20864421,29417464,22588695,22677985,22842325,23117043,null,1648631,1690010,1438563,1442131,1443787,1448630,1462600]
["DOPEX0114","Corporate costs and other operating",108697970,111321214,142235212,149154287,151639649,152685183,155659907,null,10629459,10885983,11817481,12382788,12568516,12578084,12780597]
["DOPEX0115","Public lighting",0,0,0,0,0,0,0,null,6881315,6234788,5722175,5473705,6104185,5989542,5880378]
["DOPEX0116","Fee-based and quoted services",0,0,0,0,0,0,0,null,53405368,52571481,52623279,52623279,52623279,52623311,52623279]
["DOPEX0117","Cost of Deriving Contributed Assets",0,0,0,0,0,0,0,null,61567126,60468110,61017618,61017618,61017618,61017618,61017618]
["DOPEX0118","Export Services",0,0,921573,1263128,1395767,1593211,1719678,null,0,0,0,0,0,0,0]
["DOPEX0119","Legacy Metering Services",0,0,9700504,9809242,9847862,9846333,9434934,null,0,0,0,0,0,0,0]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C14:C62)","v":338247969},348582492,398721491,401122610,405384505,409324706,415540302,null,{"$f":"SUM(K14:K62)","v":140166046},137071385,132619116,132939521,133757385,133657185,133764472]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOPEX0201","Opex for network services",334044031,344273038,382631689,384807331,388964226,392772568,399256390,null,63077367,62559859,65349265,65939735,66077529,66102850,66329774]
["DOPEX0202","Opex for metering",0,0,11837669,12049564,12143200,12236424,11913179,null,8033123,7256367,0,0,0,0,0]
["DOPEX0203","Opex for connection services",4203938,4309453,4252133,4265716,4277080,4315716,4370734,null,61567126,60468110,61017618,61017618,61017618,61017618,61017618]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,7488430,6787048,6252233,5982168,6662238,6536717,6417080]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]

{"sheet":"3.3 Assets (RAB)","index":15,"n_rows":138,"n_cols":25,"rows_kept":138,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[9,18,9,24],[22,2,22,8],[22,10,22,16],[22,18,22,24],[98,2,98,8],[98,10,98,16],[98,18,98,24],[115,2,115,8],[115,10,115,16],[115,18,115,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.3 ASSETS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - BENCHMARKING ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",{"$f":"SUM(C27,C34,C41,C48,C55,C62,C69,C75,C82,C89)","v":4978209236.5799999},{"$f":"C19","v":4975780203.4200001},{"$f":"SUM(E27,E34,E41,E48,E55,E62,E69,E75,E82,E89)","v":4949818772.5},{"$f":"E19","v":5011052381.6900005},{"$f":"F19","v":5088288829.5500011},5181406618.7200022,5310483806.1000023,null,{"$f":"SUM(K27,K34,K41,K48,K55,K62,K69,K75,K82,K89)","v":5240257438.54},{"$f":"K19","v":5245003057.7199993},{"$f":"SUM(M27,M34,M41,M48,M55,M62,M69,M75,M82,M89)","v":5223701455.5},5295824278.9000006,5383597823.5700006,5487481305.250001,5628399080.6800013,null,{"$f":"SUM(S27,S34,S41,S48,S55,S62,S69,S75,S82,S89)","v":73954421.070000008},{"$f":"S19","v":65549464.220000014},{"$f":"SUM(U27,U34,U41,U48,U55,U62,U69,U75,U82,U89)","v":58028425.210000008},57523160.480000004,57033445.010000005,56669112.580000006,56302892.990000002]
["DRAB0102","Inflation addition",{"$f":"SUM(C28,C35,C42,C49,C56,C63,C70,C76,C83,C90)","v":0},{"$f":"SUM(D28,D35,D42,D49,D56,D63,D70,D76,D83,D90)","v":0},{"$f":"SUM(E28,E35,E42,E49,E56,E63,E70,E76,E83,E90)","v":0},{"$f":"SUM(F28,F35,F42,F49,F56,F63,F70,F76,F83,F90)","v":0},{"$f":"SUM(G28,G35,G42,G49,G56,G63,G70,G76,G83,G90)","v":0},{"$f":"SUM(H28,H35,H42,H49,H56,H63,H70,H76,H83,H90)","v":0},{"$f":"SUM(I28,I35,I42,I49,I56,I63,I70,I76,I83,I90)","v":0}]
["DRAB0103","Straight line depreciation",{"$f":"SUM(C29,C36,C43,C50,C57,C64,C77,C84,C91)","v":-393901637.49000001},-384505862.32999998,-385092125.86000001,-383791300.54999995,-374765916.37000006,-319776707.75,-318275591.74000001,null,{"$f":"SUM(K29,K36,K43,K50,K57,K64,K77,K84,K91)","v":-414375569.88},-403798190.13999999,-400838329.47999996,-400026775.78999996,-391489152.05000001,-336998207.72000003,-336023664.25999999,null,{"$f":"SUM(S29,S36,S43,S50,S57,S64,S77,S84,S91)","v":-11863611.300000001},-11918314.66,-4168731.14,-4167276.87,-4054528.53,-4072762.82,-4145456.53]
["DRAB0105","Actual additions (recognised in RAB)",{"$f":"SUM(C30,C37,C44,C51,C58,C65,C71,C78,C85,C92)","v":396166146.41999996},362417457.79000002,449106383.00999999,464910172.84999996,474377021.98000002,454178121.32999992,460611305.15999997,null,{"$f":"SUM(K30,K37,K44,K51,K58,K65,K71,K78,K85,K92)","v":423814731.14999998},386369614.29999995,475741800.84000003,491682744.89999998,501865950.17000008,483240209.3499999,491152213.49000001,null,{"$f":"SUM(S30,S37,S44,S51,S58,S65,S71,S78,S85,S92)","v":3458654.45},5201088.8499999996,3663466.41,3677561.4,3690196.1,3706543.23,3724503.32]
["DRAB0106","Disposals ",-4693542.09,-4676839.58,-2780647.96,-3882424.44,-6493316.4400000004,-5324226.2,-3730934.76,null,-4693542.09,-4676839.58,-2780647.96,-3882424.44,-6493316.4400000004,-5324226.2,-3730934.76,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C14+C15+C16+C17+C18)","v":4975780203.4200001},4949014959.3000002,5011052381.6900005,5088288829.5500011,5181406618.7200022,5310483806.1000023,5449088584.7600021,null,{"$f":"SUM(K14+K15+K16+K17+K18)","v":5245003057.7199993},5222897642.2999992,5295824278.9000006,5383597823.5700006,5487481305.250001,5628399080.6800013,5779796695.1500006,null,{"$f":"SUM(S14+S15+S16+S17+S18)","v":65549464.220000014},58832238.410000019,57523160.480000004,57033445.010000005,56669112.580000006,56302892.990000002,55881939.780000001]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",660659806.29999995,{"$f":"C32","v":678748098.40999985},690496171.91999984,717949389.36999977,744514869.59999967,771656671.26999974,801508433.47999978,null,765277846.83000004,{"$f":"K32","v":786230490.10000014},799838916.56000006,831639457.38000011,862411684.36000013,893851495.51000011,928430399.94000006,null,null,{"$f":"S32","v":0},0,0,0,0,0]
["DRAB0202","Inflation addition"]
["DRAB0203","Straight line depreciation",-51617618.82,-48638630.030000001,-39698359.439999998,-40931881.460000001,-42161593.049999997,-43417786.289999999,-44745348.609999999,null,-59791468.789999999,-56340745.590000004,-45984748.5,-47413603.5,-48838044.689999998,-50293161.009999998,-51830947.969999999]
["DRAB0205","Actual additions (recognised in RAB)",69705910.930000007,60386703.539999999,67151576.890000001,67497361.689999998,69303394.719999999,73269548.5,76997859.299999997,null,80744112.060000002,69949172.049999997,77785289.319999993,78185830.480000004,80277855.840000004,84872065.439999998,89190768.700000003]
["DRAB0206","Disposals "]
["DRAB0207","Closing value",{"$f":"SUM(C27+C28+C29+C30+C31)","v":678748098.40999985},690496171.91999984,717949389.36999977,744514869.59999967,771656671.26999974,801508433.47999978,833760944.16999972,null,{"$f":"SUM(K27+K28+K29+K30+K31)","v":786230490.10000014},799838916.56000006,831639457.38000011,862411684.36000013,893851495.51000011,928430399.94000006,965790220.67000008,null,{"$f":"SUM(S27+S28+S29+S30+S31)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",1155398434.6400001,{"$f":"C39","v":1187032241.0200002},1207580398.8700001,1255592104.99,1302051287.1400001,1349518372.1200001,1401724786.0500002,null,1312828596.0699999,{"$f":"K39","v":1348772703.6300001},1372120337.23,1426673934.3700001,1479463466.5800002,1533398234.5900002,1592718094.3500001,null,null,{"$f":"S39","v":0},0,0,0,0,0]
["DRAB0302","Inflation addition"]
["DRAB0303","Straight line depreciation",-90271748.659999996,-85061928.189999998,-69426688.170000002,-71583939.739999995,-73734527.430000007,-75931427.709999993,-78253142.170000002,null,-102571831.08,-96652140.439999998,-78886502.549999997,-81337692.939999998,-83781311.469999999,-86277552.959999993,-88915615.329999998]
["DRAB0305","Actual additions (recognised in RAB)",121905555.04000001,105610086.04000001,117438394.29000001,118043121.89,121201612.41,128137841.64,134658117.91999999,null,138515938.63999999,119999774.04000001,133440099.69,134127225.15000001,137716079.47999999,145597412.72,153006116.84999999]
["DRAB0306","Disposals "]
["DRAB0307","Closing value",{"$f":"SUM(C34+C35+C36+C37+C38)","v":1187032241.0200002},1207580398.8700001,1255592104.99,1302051287.1400001,1349518372.1200001,1401724786.0500002,1458129761.8000002,null,{"$f":"SUM(K34+K35+K36+K37+K38)","v":1348772703.6300001},1372120337.23,1426673934.3700001,1479463466.5800002,1533398234.5900002,1592718094.3500001,1656808595.8700001,null,{"$f":"SUM(S34+S35+S36+S37+S38)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",1397299159.28,{"$f":"C46","v":1367942616.6499999},1331671898.1199999,1323488993.01,1306574435.55,1294571934.02,1306606940.73,null,1397299159.28,{"$f":"K46","v":1367942616.6499999},1331671898.1199999,1323488993.01,1306574435.55,1294571934.02,1306606940.73,null,null,{"$f":"S46","v":0},0,0,0,0,0]
["DRAB0402","Inflation addition"]
["DRAB0403","Straight line depreciation",-83721128.209999993,-84695684.099999994,-84773235.549999997,-86588639.019999996,-88221249.430000007,-46115472.329999998,-38909447.710000001,null,-83721128.209999993,-84695684.099999994,-84773235.549999997,-86588639.019999996,-88221249.430000007,-46115472.329999998,-38909447.710000001]
["DRAB0405","Actual additions (recognised in RAB)",54364585.579999998,48424965.57,76590330.439999998,69674081.560000002,76218747.900000006,58150479.039999999,68812587.870000005,null,54364585.579999998,48424965.57,76590330.439999998,69674081.560000002,76218747.900000006,58150479.039999999,68812587.870000005]
["DRAB0406","Disposals "]
["DRAB0407","Closing value",{"$f":"SUM(C41+C42+C43+C44+C45)","v":1367942616.6499999},1331671898.1199999,1323488993.01,1306574435.55,1294571934.02,1306606940.73,1336510080.8899999,null,{"$f":"SUM(K41+K42+K43+K44+K45)","v":1367942616.6499999},1331671898.1199999,1323488993.01,1306574435.55,1294571934.02,1306606940.73,1336510080.8899999,null,{"$f":"SUM(S41+S42+S43+S44+S45)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",211129346.75,{"$f":"C53","v":215387282.51999998},222894190.09999996,239603801.37999997,255036883.21999997,276897186.86999995,302022921.1099999,null,211129346.75,{"$f":"K53","v":215387282.51999998},222894190.09999996,239603801.37999997,255036883.21999997,276897186.86999995,302022921.1099999,null,null,{"$f":"S53","v":0},0,0,0,0,0]
["DRAB0502","Inflation addition"]
["DRAB0503","Straight line depreciation",-5532468.7999999998,-5717727.3600000003,-5070840.51,-5466848.7300000004,-5846847.46,-6350613.8499999996,-6922911.0899999999,null,-5532468.7999999998,-5717727.3600000003,-5070840.51,-5466848.7300000004,-5846847.46,-6350613.8499999996,-6922911.0899999999]
["DRAB0505","Actual additions (recognised in RAB)",9790404.5700000003,13224634.939999999,21780451.789999999,20899930.57,27707151.109999999,31476348.09,18155409.420000002,null,9790404.5700000003,13224634.939999999,21780451.789999999,20899930.57,27707151.109999999,31476348.09,18155409.420000002]
["DRAB0506","Disposals "]
["DRAB0507","Closing value",{"$f":"SUM(C48+C49+C50+C51+C52)","v":215387282.51999998},222894190.09999996,239603801.37999997,255036883.21999997,276897186.86999995,302022921.1099999,313255419.43999994,null,{"$f":"SUM(K48+K49+K50+K51+K52)","v":215387282.51999998},222894190.09999996,239603801.37999997,255036883.21999997,276897186.86999995,302022921.1099999,313255419.43999994,null,{"$f":"SUM(S48+S49+S50+S51+S52)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",27630939.949999999,{"$f":"C60","v":28188184.93},29170629.649999999,31357451.489999998,33377211.239999998,36238114.979999997,39526372.459999993,null,27630939.949999999,{"$f":"K60","v":28188184.93},29170629.649999999,31357451.489999998,33377211.239999998,36238114.979999997,39526372.459999993,null,null,{"$f":"S60","v":0},0,0,0,0,0]
["DRAB0602","Inflation addition"]
["DRAB0603","Straight line depreciation",-724045.78,-748290.96,-663631.52,-715457.95,-765189.18,-831118.14,-906015.88,null,-724045.78,-748290.96,-663631.52,-715457.95,-765189.18,-831118.14,-906015.88]
["DRAB0605","Actual additions (recognised in RAB)",1281290.76,1730735.68,2850453.36,2735217.7,3626092.92,4119375.62,2376036.4700000002,null,1281290.76,1730735.68,2850453.36,2735217.7,3626092.92,4119375.62,2376036.4700000002]
["DRAB0606","Disposals "]
["DRAB0607","Closing value",{"$f":"SUM(C55+C56+C57+C58+C59)","v":28188184.93},29170629.649999999,31357451.489999998,33377211.239999998,36238114.979999997,39526372.459999993,40996393.04999999,null,{"$f":"SUM(K55+K56+K57+K58+K59)","v":28188184.93},29170629.649999999,31357451.489999998,33377211.239999998,36238114.979999997,39526372.459999993,40996393.04999999,null,{"$f":"SUM(S55+S56+S57+S58+S59)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",524648665.08999997,{"$f":"C67","v":513626064.23999995},500007374.25999993,496934911.05999994,490583944.66999996,486077324.61999995,490596149.5,null,524648665.08999997,{"$f":"K67","v":513626064.23999995},500007374.25999993,496934911.05999994,490583944.66999996,486077324.61999995,490596149.5,null,null,{"$f":"S67","v":0},0,0,0,0,0]
["DRAB0702","Inflation addition"]
["DRAB0703","Straight line depreciation",-31435056.600000001,-31800976.41,-31830094.920000002,-32511730.629999999,-33124732.41,-17315133.149999999,-14609462.59,null,-31435056.600000001,-31800976.41,-31830094.920000002,-32511730.629999999,-33124732.41,-17315133.149999999,-14609462.59]
["DRAB0705","Actual additions (recognised in RAB)",20412455.75,18182286.43,28757631.719999999,26160764.239999998,28618112.359999999,21833958.030000001,25837296.280000001,null,20412455.75,18182286.43,28757631.719999999,26160764.239999998,28618112.359999999,21833958.030000001,25837296.280000001]
["DRAB0706","Disposals "]
["DRAB0707","Closing value",{"$f":"SUM(C62+C63+C64+C65+C66)","v":513626064.23999995},500007374.25999993,496934911.05999994,490583944.66999996,486077324.61999995,490596149.5,501823983.19000006,null,{"$f":"SUM(K62+K63+K64+K65+K66)","v":513626064.23999995},500007374.25999993,496934911.05999994,490583944.66999996,486077324.61999995,490596149.5,501823983.19000006,null,{"$f":"SUM(S62+S63+S64+S65+S66)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",10910927.640000001,{"$f":"C73","v":10910927.640000001},10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,null,10910927.640000001,{"$f":"K73","v":10910927.640000001},10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,null,null,{"$f":"S73","v":0},0,0,0,0,0]
["DRAB0802","Inflation addition"]
["DRAB0803","Actual additions (recognised in RAB)"]
["DRAB0804","Disposals "]
["DRAB0805","Closing value",{"$f":"SUM(C69+C70+C71+C72)","v":10910927.640000001},10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,null,{"$f":"SUM(K69+K70+K71+K72)","v":10910927.640000001},10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,null,{"$f":"SUM(S69+S70+S71+S72)","v":0},0,0,0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",null,null,{"$f":"T80","v":836156.37999999896},{"$f":"E80","v":7311.2299999989518},-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,null,null,{"$f":"K80","v":0},{"$f":"T80","v":836156.37999999896},7311.2299999989518,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,null,17646621.620000001,{"$f":"S80","v":9273810.3399999999}]
["DRAB0902","Inflation addition"]
["DRAB0903","Straight line depreciation",null,null,-836156.38,-7311.23,null,null,null,null,null,null,-836156.38,-7311.23,null,null,null,null,-8372811.2800000003,-8437653.9600000009]
["DRAB0905","Actual additions (recognised in RAB)",null,null,7311.23,null,null,null,null,null,null,null,7311.23]
["DRAB0906","Disposals "]
["DRAB0907","Closing value",{"$f":"SUM(C75+C76+C77+C78+C79)","v":0},0,7311.2299999989518,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,null,{"$f":"SUM(K75+K76+K77+K78+K79)","v":0},0,7311.2299999989518,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,null,{"$f":"SUM(S75+S76+S77+S78+S79)","v":9273810.3399999999},836156.37999999896,0,0,0,0,0]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",679332189.34000003,{"$f":"C87","v":687040850.92999995},680054972.08999991,694786546.76999986,708706409.8599999,712294960.83999979,719124510.61999989,null,679332189.34000003,{"$f":"K87","v":687040850.92999995},680054972.08999991,694786546.76999986,708706409.8599999,712294960.83999979,719124510.61999989,null,56990384.450000003,{"$f":"S87","v":56634372.050000004},58028425.210000008,57523160.480000004,57033445.010000005,56669112.580000006,56302892.990000002]
["DRAB1002","Inflation addition"]
["DRAB1003","Straight line depreciation",-43089618.969999999,-46302570.960000001,-45554120.719999999,-48653499.170000002,-50865465.479999997,-52267859.159999996,-54688400.039999999,null,-43089618.969999999,-46302570.960000001,-45554120.719999999,-48653499.170000002,-50865465.479999997,-52267859.159999996,-54688400.039999999,null,-3814666.85,-3807035.69,-4168731.14,-4167276.87,-4054528.53,-4072762.82,-4145456.53]
["DRAB1005","Actual additions (recognised in RAB)",52434165.259999998,40946755.340000004,61016098.759999998,63803649.380000003,55520465.280000001,60731235.450000003,57646405.950000003,null,52434165.259999998,40946755.340000004,61016098.759999998,63803649.380000003,55520465.280000001,60731235.450000003,57646405.950000003,null,3458654.45,5201088.8499999996,3663466.41,3677561.4,3690196.1,3706543.23,3724503.32]
["DRAB1006","Disposals ",-1635884.7,-1630063.22,-730403.36,-1230287.1200000001,-1066448.82,-1633826.51,-1048450.45,null,-1635884.7,-1630063.22,-730403.36,-1230287.1200000001,-1066448.82,-1633826.51,-1048450.45]
["DRAB1007","Closing value",{"$f":"SUM(C82+C83+C84+C85+C86)","v":687040850.92999995},680054972.08999991,694786546.76999986,708706409.8599999,712294960.83999979,719124510.61999989,721034066.07999992,null,{"$f":"SUM(K82+K83+K84+K85+K86)","v":687040850.92999995},680054972.08999991,694786546.76999986,708706409.8599999,712294960.83999979,719124510.61999989,721034066.07999992,null,{"$f":"SUM(S82+S83+S84+S85+S86)","v":56634372.050000004},58028425.210000008,57523160.480000004,57033445.010000005,56669112.580000006,56302892.990000002,55881939.780000001]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",311199767.58999997,{"$f":"C94","v":286903937.07999998},{"$f":"D94+T94","v":276196053.46999997},240420944.75,236532860.63,243241126.35999998,238462764.50999999,null,311199767.58999997,{"$f":"K94","v":286903937.07999998},{"$f":"L94+T94","v":276196053.46999997},240420944.56999999,236532860.44999999,243241126.17999998,238462764.32999998,null,-682585,{"$f":"S94","v":-358718.17},null,0,0,0,0]
["DRAB1102","Inflation addition"]
["DRAB1103","Straight line depreciation",-87509951.650000006,-81540054.319999993,-107238998.64999999,-97331992.620000005,-80046311.930000007,-77547297.120000005,-79240863.650000006,null,-87509951.650000006,-81540054.319999993,-107238998.83,-97331992.620000005,-80046311.930000007,-77547297.120000005,-79240863.650000006,null,323866.83,326374.99]
["DRAB1105","Actual additions (recognised in RAB)",66271778.530000001,73911290.25,73514134.530000001,96096045.819999993,92181445.280000001,76459334.959999993,76127591.950000003,null,66271778.530000001,73911290.25,73514134.530000001,96096045.819999993,92181445.280000001,76459334.959999993,76127591.950000003]
["DRAB1106","Disposals ",-3057657.39,-3046776.36,-2050244.6,-2652137.3199999998,-5426867.6200000001,-3690399.69,-2682484.31,null,-3057657.39,-3046776.36,-2050244.6,-2652137.3199999998,-5426867.6200000001,-3690399.69,-2682484.31]
["DRAB1107","Closing value",{"$f":"SUM(C89+C90+C91+C92+C93)","v":286903937.07999998},276228396.64999998,240420944.75,236532860.63,243241126.35999998,238462764.50999999,232667008.5,null,{"$f":"SUM(K89+K90+K91+K92+K93)","v":286903937.07999998},276228396.64999998,240420944.56999999,236532860.44999999,243241126.17999998,238462764.32999998,232667008.31999999,null,{"$f":"SUM(S89+S90+S91+S92+S93)","v":-358718.17},-32343.179999999993,0,0,0,0,0]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED BENCHMARKING ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",{"$f":"IFERROR(AVERAGE(C27,C32),\"\")","v":669703952.3549999},{"$f":"IFERROR(AVERAGE(D27,D32),\"\")","v":684622135.16499984},704222780.64499974,731232129.48499966,758085770.4349997,786582552.37499976,817634688.82499981,null,{"$f":"IFERROR(AVERAGE(K27,K32),\"\")","v":775754168.46500015},{"$f":"IFERROR(AVERAGE(L27,L32),\"\")","v":793034703.33000016},815739186.97000003,847025570.87000012,878131589.93500018,911140947.72500014,947110310.30500007,null,{"$f":"IFERROR(AVERAGE(S27,S32),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T27,T32),\"\")","v":0},0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",{"$f":"IFERROR(AVERAGE(C34,C39),\"\")","v":1171215337.8300002},{"$f":"IFERROR(AVERAGE(D34,D39),\"\")","v":1197306319.9450002},1231586251.9300001,1278821696.0650001,1325784829.6300001,1375621579.085,1429927273.9250002,null,{"$f":"IFERROR(AVERAGE(K34,K39),\"\")","v":1330800649.8499999},{"$f":"IFERROR(AVERAGE(L34,L39),\"\")","v":1360446520.4300001},1399397135.8000002,1453068700.4750001,1506430850.585,1563058164.4700003,1624763345.1100001,null,{"$f":"IFERROR(AVERAGE(S34,S39),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T34,T39),\"\")","v":0},0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",{"$f":"IFERROR(AVERAGE(C41,C46),\"\")","v":1382620887.9649999},{"$f":"IFERROR(AVERAGE(D41,D46),\"\")","v":1349807257.3849998},1327580445.5650001,1315031714.28,1300573184.7849998,1300589437.375,1321558510.8099999,null,{"$f":"IFERROR(AVERAGE(K41,K46),\"\")","v":1382620887.9649999},{"$f":"IFERROR(AVERAGE(L41,L46),\"\")","v":1349807257.3849998},1327580445.5650001,1315031714.28,1300573184.7849998,1300589437.375,1321558510.8099999,null,{"$f":"IFERROR(AVERAGE(S41,S46),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T41,T46),\"\")","v":0},0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",{"$f":"IFERROR(AVERAGE(C48,C53),\"\")","v":213258314.63499999},{"$f":"IFERROR(AVERAGE(D48,D53),\"\")","v":219140736.30999997},231248995.73999995,247320342.29999995,265967035.04499996,289460053.98999989,307639170.27499992,null,{"$f":"IFERROR(AVERAGE(K48,K53),\"\")","v":213258314.63499999},{"$f":"IFERROR(AVERAGE(L48,L53),\"\")","v":219140736.30999997},231248995.73999995,247320342.29999995,265967035.04499996,289460053.98999989,307639170.27499992,null,{"$f":"IFERROR(AVERAGE(S48,S53),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T48,T53),\"\")","v":0},0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",{"$f":"IFERROR(AVERAGE(C55,C60),\"\")","v":27909562.439999998},{"$f":"IFERROR(AVERAGE(D55,D60),\"\")","v":28679407.289999999},30264040.57,32367331.364999998,34807663.109999999,37882243.719999999,40261382.754999995,null,{"$f":"IFERROR(AVERAGE(K55,K60),\"\")","v":27909562.439999998},{"$f":"IFERROR(AVERAGE(L55,L60),\"\")","v":28679407.289999999},30264040.57,32367331.364999998,34807663.109999999,37882243.719999999,40261382.754999995,null,{"$f":"IFERROR(AVERAGE(S55,S60),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T55,T60),\"\")","v":0},0,0,0,0,0]
["DRAB1206","Zone substations and transformers",{"$f":"IFERROR(AVERAGE(C62,C67),\"\")","v":519137364.66499996},{"$f":"IFERROR(AVERAGE(D62,D67),\"\")","v":506816719.24999994},498471142.65999997,493759427.86499995,488330634.64499998,488336737.05999994,496210066.34500003,null,{"$f":"IFERROR(AVERAGE(K62,K67),\"\")","v":519137364.66499996},{"$f":"IFERROR(AVERAGE(L62,L67),\"\")","v":506816719.24999994},498471142.65999997,493759427.86499995,488330634.64499998,488336737.05999994,496210066.34500003,null,{"$f":"IFERROR(AVERAGE(S62,S67),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T62,T67),\"\")","v":0},0,0,0,0,0]
["DRAB1207","Easements ",{"$f":"IFERROR(AVERAGE(C69,C73),\"\")","v":10910927.640000001},{"$f":"IFERROR(AVERAGE(D69,D73),\"\")","v":10910927.640000001},10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,null,{"$f":"IFERROR(AVERAGE(K69,K73),\"\")","v":10910927.640000001},{"$f":"IFERROR(AVERAGE(L69,L73),\"\")","v":10910927.640000001},10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,10910927.640000001,null,{"$f":"IFERROR(AVERAGE(S69,S73),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T69,T73),\"\")","v":0},0,0,0,0,0]
["DRAB1208","Meters",{"$f":"IFERROR(AVERAGE(C75,C80),\"\")","v":0},{"$f":"IFERROR(AVERAGE(D75,D80),\"\")","v":0},421733.80499999895,3655.614999998952,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,null,{"$f":"IFERROR(AVERAGE(K75,K80),\"\")","v":0},{"$f":"IFERROR(AVERAGE(L75,L80),\"\")","v":0},421733.80499999895,3655.614999998952,-1.0477378964424133E-9,-1.0477378964424133E-9,-1.0477378964424133E-9,null,{"$f":"IFERROR(AVERAGE(S75,S80),\"\")","v":13460215.98},{"$f":"IFERROR(AVERAGE(T75,T80),\"\")","v":5054983.3599999994},0,0,0,0,0]
["DRAB1209","“Other” assets with long lives",{"$f":"IFERROR(AVERAGE(C82,C87),\"\")","v":683186520.13499999},{"$f":"IFERROR(AVERAGE(D82,D87),\"\")","v":683547911.50999999},687420759.42999983,701746478.31499982,710500685.3499999,715709735.72999978,720079288.3499999,null,{"$f":"IFERROR(AVERAGE(K82,K87),\"\")","v":683186520.13499999},{"$f":"IFERROR(AVERAGE(L82,L87),\"\")","v":683547911.50999999},687420759.42999983,701746478.31499982,710500685.3499999,715709735.72999978,720079288.3499999,null,{"$f":"IFERROR(AVERAGE(S82,S87),\"\")","v":56812378.25},{"$f":"IFERROR(AVERAGE(T82,T87),\"\")","v":57331398.63000001},57775792.845000006,57278302.745000005,56851278.795000002,56486002.785000004,56092416.385000005]
["DRAB1210","“Other” assets with short lives",{"$f":"IFERROR(AVERAGE(C89,C94),\"\")","v":299051852.33499998},{"$f":"IFERROR(AVERAGE(D89,D94),\"\")","v":281566166.86500001},258308499.10999998,238476902.69,239886993.495,240851945.435,235564886.505,null,{"$f":"IFERROR(AVERAGE(K89,K94),\"\")","v":299051852.33499998},{"$f":"IFERROR(AVERAGE(L89,L94),\"\")","v":281566166.86500001},258308499.01999998,238476902.50999999,239886993.315,240851945.255,235564886.32499999,null,{"$f":"IFERROR(AVERAGE(S89,S94),\"\")","v":-520651.58499999996},{"$f":"IFERROR(AVERAGE(T89,T94),\"\")","v":-195530.67499999999},0,0,0,0,0]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",-92756550.129999995,-89433743.920000002,-107158240.8,-102000247.7,-103670847.09999999,-104141383.7,-97573261.799999997,null,-92756550.129999995,-89433743.920000002,-107158240.8,-102000247.7,-103670847.09999999,-104141383.7,-97573261.799999997,null,-2567126.39,-2704992.04,-604125.04,-606322.56999999995,-608202.07999999996,-610588.23,-613246.43999999994]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"FORECAST\n( years )",null,null,null,null,null,null,null,"FORECAST\n( years )",null,null,null,null,null,null,null,"FORECAST\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",53,53,53,54,54,54,54,null,53,53,53,54,54,54,54]
["DRAB1402","Underground network assets less than 33kV (cables)",53,53,53,54,54,54,54,null,53,53,53,54,54,54,54]
["DRAB1403","Distribution substations including transformers",42,43,44,43,43,43,43,null,42,43,44,43,43,43,43]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",55,55,55,55,55,55,55,null,55,55,55,55,55,55,55]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",55,55,55,55,55,55,55,null,55,55,55,55,55,55,55]
["DRAB1406","Zone substations and transformers",42,43,44,43,43,43,43,null,42,43,44,43,43,43,43]
["DRAB1407","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1408","“Other” assets with long lives",20,18,21,24,20,19,21,null,20,18,21,24,20,19,21,null,28,28,27,27,27,27,27]
["DRAB1409","“Other” assets with short lives",5,5,5,5,5,5,5,null,5,5,5,5,5,5,5]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",14,17,18,18,18,18,19,null,14,17,18,18,18,18,19]
["DRAB1502","Underground network assets less than 33kV (cables)",14,17,18,18,18,18,19,null,14,17,18,18,18,18,19]
["DRAB1503","Distribution substations including transformers",16,16,15,15,28,34,34,null,16,16,15,15,28,34,34]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",38,44,44,44,44,44,45,null,38,44,44,44,44,44,45]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",38,44,44,44,44,44,45,null,38,44,44,44,44,44,45]
["DRAB1506","Zone substations and transformers",16,16,15,15,28,34,34,null,16,16,15,15,28,34,34]
["DRAB1507","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1508","“Other” assets with long lives",15,15,14,14,14,13,13,null,14,15,14,14,14,13,13,null,15,14,14,14,14,14,13]
["DRAB1509","“Other” assets with short lives",4,3,2,3,3,3,3,null,4,3,2,3,3,3,3,null,1,0,0,0,0,0,0]

{"sheet":"3.4 Operational data","index":16,"n_rows":110,"n_cols":10,"rows_kept":110,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.4 OPERATIONAL DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped for ease of navigation. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOPED01","TOTAL ENERGY DELIVERED"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",3676.84,3063.75,2796.66,2520.25,2229.0300000000002,1928.88,1610.2]
["DOPED0202","Energy Delivery at On-peak times","GWh",2837.85,3138.71,3337.01,3651.94,3911.74,4211.5600000000004,4482.45]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",354.76,515.33000000000004,619.80999999999995,713.02,786.42,857.92,926.89]
["DOPED0204","Energy Delivery at Off-peak times","GWh",2586.6799999999998,3144.18,3661.01,4008.82,4248.17,4536.04,4797.28]
["DOPED0205","Controlled load energy deliveries","GWh",450.5,458.08,451.84,445.68,439.61,433.62,427.71]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",99.47,98.23,98.23,98.23,98.23,98.23,98.23]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",3497.14,3631.73,3823.99,3953.14,4000.88,4077.74,4125.49]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",0,0,0,0,0,0,0]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",5128.62,5325.99,5607.94,5797.35,5867.36,5980.08,6050.1]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",0,0,0,0,0,0,0]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",343.06,371.9,401.41,437.42,474.57,515.82000000000005,558.66]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",348.43,377.73,407.7,444.27,482,523.91,567.41999999999996]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",955.09,990.13,1025.18,1104.31,1174.1199999999999,1246.0999999999999,1308.97]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",441.97,458.19,474.4,511.02,543.33000000000004,576.64,605.73]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",0,0,0,0,0,0,0]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",3889.54,3550.48,3588.9,3663.29,3737.85,3922.93,4064.4]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",967.77,1062.1500000000001,1118.18,1148.08,1139.32,1122.99,1099.82]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",3108.11,3615.16,3989.47,4297.68,4476.51,4635.17,4772.7700000000004]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",1941.21,2092.2600000000002,2169.77,2230.66,2261.29,2286.9299999999998,2307.5300000000002]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.4.2 - CUSTOMER NUMBERS (Benchmarking)"]
[null,null,null,"FORECAST"]
[null,null,"Units","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30"]
[null,"3.4.2.1 - Distribution customer numbers by customer type or class"]
["DOPCN0101","Residential customer numbers","number",828334,836404,844551,852779,861086,869474,877944]
["DOPCN0102","Non residential customers not on demand tariff customer numbers","number",90525,91050,91579,92109,92644,93181,93722]
["DOPCN0103","Low voltage demand tariff customer numbers","number",16991,17089,17188,17287,17387,17488,17589]
["DOPCN0104","High voltage demand tariff customer numbers","number",245,245,245,245,245,245,245]
["DOPCN0105","Unmetered Customer Numbers","number",9176,9176,9176,9176,9176,9176,9176]
["DOPCN0106","Other Customer Numbers","number",0,0,0,0,0,0,0]
[null,"Total customer numbers",null,{"$f":"SUM(D48:D53)","v":945271},{"$f":"SUM(E48:E53)","v":953964},962739,971596,980538,989564,998676]
[]
[]
[null,"Table 3.4.2.2 Distribution customer numbers by location on the network"]
["DOPCN0201",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},"number",6876,6907,6938,6969,7000,7031,7062]
["DOPCN0202",{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},"number",648222,654631,661094,667609,674179,680803,687482]
["DOPCN0203",{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},"number",142301,144475,146679,148915,151182,153482,155814]
["DOPCN0204",{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},"number",138696,138775,138853,138928,139002,139073,139143]
["DOPCN0205",{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},"number"]
[null,"Total customer numbers",null,{"$f":"SUM(D58:D62)","v":936095},{"$f":"SUM(E58:E62)","v":944788},953564,962421,971363,980389,989501]
[]
[]
[null," 3.4.2.4 - Unmetered Supply"]
["DOPCN0301","Number of unmetered connections reported in customer numbers in the economic benchmarking RIN",null,{"$f":"D52","v":9176},{"$f":"E52","v":9176},9176,9176,9176,9176,9176]
["DOPCN0302","Unmetered connections not reported in customer numbers in the economic benchmarking RIN",null,0,0,0,0,0,0,0]
["DOPCN0303","Total unmetered connections",null,{"$f":"SUM(D67:D68)","v":9176},{"$f":"SUM(E67:E68)","v":9176},9176,9176,9176,9176,9176]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",3323,3391,3480,3603,3656,3710,3768]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2986,3049,3125,3229,3280,3331,3386]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",3146,3221,3303,3397,3448,3498,3555]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2833,2902,2971,3050,3098,3146,3200]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",3411,3578,3680,3793,3850,3906,3975]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",3078,3236,3323,3424,3479,3533,3599]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",3283,3452,3540,3622,3676,3730,3796]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2985,3141,3224,3302,3355,3408,3472]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",3393,3462,3553,3678,3733,3788,3848]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",3050,3114,3191,3297,3350,3402,3458]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",3210,3286,3370,3465,3517,3568,3626]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2890,2961,3031,3112,3161,3210,3265]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",3444,3612,3715,3830,3887,3944,4013]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",3108,3267,3355,3457,3512,3567,3633]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",3314,3485,3573,3656,3711,3766,3832]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",3014,3172,3255,3334,3387,3441,3505]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.99033126176541997,0.99047718091529002,0.99049246899315002,0.99050182229497996,0.99047943710757003,0.99045723687328002,0.99045600281241997]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.97843390212935,0.97849401515825996,0.97854212650750005,0.97858174746111004,0.97859754881510996,0.97861942464477003,0.97865289119620003]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0.94830848458582995,0.94831766892338998,0.94832081826201997,0.94831802658685005,0.94832735877705998,0.94833774401454995,0.94834765318531999]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor"]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0.98481908029482002,0.98486648118554998,0.98489171498599004,0.98486772213205998,0.98488819065269995,0.98490830411039998,0.98492768511898998]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.97964586651912999,0.97967969628966001,0.97969553268461995,0.97969419746413,0.97969270554733001,0.97969787309631995,0.97971327748172998]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.96843957355888999,0.96959422506845006,0.96967426804572998,0.96884322135457002,0.96889043117871998,0.96893399812513004,0.96897124033679005]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0.97824975192359998,0.97892159854833005,0.97880918393378002,0.97869617915270002,0.97862179893566004,0.97854758502739003,0.97847304249121003]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.99286881974142005,0.99284276561813001,0.99286435379090998,0.99287563525876998,0.99286227869204002,0.99284910691994999,0.99285001546676999]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]

{"sheet":"3.5 Physical assets","index":17,"n_rows":96,"n_cols":10,"rows_kept":96,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",18366.02,18299.28,18232.79,18166.53,18100.52,18034.75,17969.21]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",184.59,174.73,165.4,156.56,148.19999999999999,140.29,132.80000000000001]
["DPA0104","Overhead 11 kV","km",17699.05,17713.11,17727.18,17741.259999999998,17755.36,17769.46,17783.580000000002]
["DPA0105","Overhead SWER","km",29101.74,29097.48,29093.22,29088.959999999999,29084.7,29080.44,29076.19]
["DPA0106","Overhead 22 kV","km",0,0,0,0,0,0,0]
["DPA0107","Overhead 33 kV","km",3997.46,4001.92,4006.39,4010.86,4015.33,4019.82,4024.3]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",1453.88,1455.75,1457.63,1459.52,1461.4,1463.29,1465.18]
["DPA0110","Overhead 132 kV","km",0,0,0,0,0,0,0]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0112","Overhead 110kV","km",0,0,0,0,0,0,0]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D14:D27)","v":70802.74000000002},70742.26999999999,70682.610000000015,70623.69,70565.509999999995,70508.05,70451.259999999995]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",15054.73,15294.2,15537.48,15784.64,16035.72,16290.8,16549.939999999999]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",0,0,0,0,0,0,0]
["DPA0204","Underground 7.6 kV","km",37,37,37,37,37,37,37]
["DPA0205","Underground 11 kV","km",4399.43,4469.97,4541.6499999999996,4614.47,4688.46,4763.6400000000003,4840.03]
["DPA0206","Underground SWER","km",68.400000000000006,69.83,71.290000000000006,72.77,74.290000000000006,75.849999999999994,77.430000000000007]
["DPA0207","Underground 22 kV","km",0,0,0,0,0,0,0]
["DPA0208","Underground 33 kV","km",143.58000000000001,147.26,151.03,154.9,158.86000000000001,162.93,167.1]
["DPA0209","Underground 66 kV","km",54.15,54.29,54.44,54.58,54.73,54.88,55.03]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",0,0,0,0,0,0,0]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D30:D41)","v":19757.290000000005},20072.550000000003,20392.889999999996,20718.360000000004,21049.06,21385.1,21726.529999999995]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.17199999999999999,0.17199999999999999,0.17199999999999999,0.17199999999999999,0.17199999999999999,0.17199999999999999,0.17199999999999999]
["DPA0302","Overhead 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0303","Overhead 7.6 kV","MVA",1.82,1.883,1.883,1.883,1.883,1.883,1.883]
["DPA0304","Overhead 11 kV","MVA",4.0259999999999998,4.024,4.0259999999999998,4.0270000000000001,4.0270000000000001,4.0270000000000001,4.03]
["DPA0305","Overhead SWER","MVA",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
["DPA0306","Overhead 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0307","Overhead 33 kV","MVA",10.452,10.452,10.465999999999999,10.509,10.512,10.512,10.561]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",59.802999999999997,59.802999999999997,61.152999999999999,61.296999999999997,61.296999999999997,61.658000000000001,61.646999999999998]
["DPA0310","Overhead 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0311","Overhead 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.14099999999999999,0.14099999999999999,0.14099999999999999,0.14099999999999999,0.14099999999999999,0.14099999999999999,0.14099999999999999]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0404","Underground 7.6 kV","MVA",2.8140000000000001,2.8130000000000002,2.8130000000000002,2.8130000000000002,2.8130000000000002,2.8130000000000002,2.8130000000000002]
["DPA0405","Underground 11 kV","MVA",5.5019999999999998,5.5019999999999998,5.5019999999999998,5.5019999999999998,5.5019999999999998,5.5019999999999998,5.5019999999999998]
["DPA0406","Underground SWER","MVA",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0409","Underground 33 kV","MVA",17.298999999999999,17.456,17.456,17.530999999999999,17.530999999999999,17.530999999999999,17.530999999999999]
["DPA0410","Underground 66 kV","MVA",126.315,126.315,126.315,126.315,126.315,126.892,126.892]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0413","Other","MVA",137.178,137.178,137.178,137.178,137.178,137.178,137.178]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",9862.09,9888.9,9894.24,9904.65,9920.06,9940.59,9956.1200000000008]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",552.30999999999995,593.6,618.48,638.04,647.87,656.1,662.72]
["DPA0503","Cold spare capacity included in DPA0501","MVA",140,150,140,135,135,140,140]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",245.5,238,238,238,238,238,238]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",113.6,109.3,109.3,109.3,109.3,114.2,114.2]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",4956.6000000000004,4985.6000000000004,4991.8,5025.8,5074.5,5087,5118.5]
["DPA0604","Total zone substation transformer  capacity ","MVA",5828.8,5833.5,5839.7,5873.7,5921.5,5959,5990.5]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",513.20000000000005,500.7,500.7,500.7,499.7,519.79999999999995,519.79999999999995]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DPA0701","Public lighting luminaires","0's",240200,242002,243817,245645,247488,249344,251214]
["DPA0702","Public lighting poles","0's",118754,120733,122711,124690,126669,128647,130626]

{"sheet":"3.6 Quality of service","index":18,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DQS0201","Energy Not Supplied (planned)","GWh",1.24,1.39,1.46,1.52,1.56,1.61,1.65]
["DQS0202","Energy Not Supplied (unplanned)","GWh",4.0199999999999996,4.4800000000000004,4.7,4.8899999999999997,4.97,5.12,5.22]
["DQS02","Total",null,{"$f":"SUM(D10:D11)","v":5.26},5.87,6.16,6.41,6.5299999999999994,6.73,6.8699999999999992]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DQS03","System losses","%","6.61%","6.61%","6.61%","6.61%","6.61%","6.61%","6.61%"]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DQS04","Overall utilisation","%","58.21%","59.35%","60.84%","62.63%","63.05%","63.56%","64.23%"]

{"sheet":"3.7 Operating Environment","index":19,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOEF0101","Customer density","Customer / km",11.361000000000001]
["DOEF0102","Energy density","MWh/customer",10.585000000000001]
["DOEF0103","Demand density","kVA / customer",3.589]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOEF0201","Rural proportion","%",0.80110000000000003]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",23365]
["DOEF0203","Rural vegetation maintenance spans","0's",73904]
["DOEF0204","Total vegetation maintenance spans","0's",97269]
["DOEF0205","Total number of spans","0's",621003]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",2.7909999999999999]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1.3839999999999999]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",3.4830000000000001]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",8.7460000000000004]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",1.893]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",1.1719999999999999]
["DOEF0212","Tropical proportion","Spans",0]
["DOEF0213","Standard vehicle access","km",5825,5838,5851,5865,5878,5892,5905]
["DOEF0214","Bushfire risk","Spans",374959]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
["DOEF0301","Route Line length","km",83206.100000000006,83396.100000000006,83586.5,83777.3,83968.6,84160.3,84352.4]

{"sheet":"4.1 Public lighting","index":20,"n_rows":200,"n_cols":10,"rows_kept":200,"cut":false,"hidden":false,"merged":[[6,1,6,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[55,1,55,2],[56,1,56,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[96,1,96,2],[94,1,94,2],[97,1,97,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[206,1,206,2],[213,1,213,2],[214,1,214,2],[215,1,215,2],[216,1,216,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2],[212,1,212,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"4.1 PUBLIC LIGHTING"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. There are no further instructions."]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","number",745,745,745,745,745,745,745]
[null,"Number of poles installed ","number",56,56,56,56,56,56,56]
[null,"Total expenditure","$",1497089.75,1506229.86,1516585.3,1522099.39,1526815.13,1532802.7,1539473.24]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","number",10118,10082,10121,10131,10212,10227,10323]
[null,"Number of poles replaced","number",195,195,195,195,195,195,195]
[null,"Total expenditure","$",10797697.35023864,10808423.372840945,7815361.2383648101,7443707.1705194805,7359698.9101556297,6876347.2324534124,6441045.4944085917]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","number",33833,30424,28027,27243,44292,44783,45293]
[null,"Number of poles maintained","number",9357,9357,9357,9357,9357,9357,9357]
[null,"Total expenditure","$",6804627,6165028,5655220,5409478,6033694,5920425,5812584]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","number of days",5.03,5.04,5.12,5.01,5.13,5.13,5.0999999999999996]
[null,"GSO breaches","number",1822,1898,1690,1761,1795,1802,1775]
[null,"GSL payments ","$",194956.43,192653.78,0,0,0,0,0]
[null,"Customer complaints ","number",150,156,180,180,150,140,130]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"LIGHT INSTALLATION"]
[null,"LED16",null,479.12,482.05,485.36,487.13,488.64,490.55,492.69]
[null,"LED24",null,484.76,487.72,491.08,492.86,494.39,496.33,498.49]
[null,"LED58",null,2096.4299999999998,2109.23,2123.73,2131.4499999999998,2138.0500000000002,2146.44,2155.7800000000002]
[null,"LED78",null,2099.0300000000002,2111.85,2126.37,2134.1,2140.71,2149.1,2158.46]
[null,"LED151",null,2099.0300000000002,2111.85,2126.37,2134.1,2140.71,2149.1,2158.46]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"cf-42",null,342.9,328.63,314.82,302.11,296.51,269.52999999999997,242.23]
[null,"cf-42 PT",null,1020.12,927.27,834.73,751.07,713.3,561.39,408.73]
[null,"F-40",null,159.6,166.71,174.2,302.06,296.36,269.73,242.47]
[null,"MV-80",null,159.6,166.71,174.2,179.9,296.52,269.54000000000002,242.33]
[null,"MV-80 PT",null,1019.47,926.11,833.56,753.39,717.51,565.44000000000005,409.76]
[null,"MV-80+",null,342.95,328.61,314.89999999999998,302.05,296.52999999999997,269.31,242.58]
[null,"S-HP Other",null,342.9,329.26,315.32,299.83999999999997,296.99,267,243.99]
[null,"S-HP100",null,716.74,649.14,583.07000000000005,513.19000000000005,439.17,369.66,299.54000000000002]
[null,"S-HP150",null,747.56,675.8,605.57000000000005,531.70000000000005,453.3,379.8,305.19]
[null,"S-HP250",null,751.05,678.49,608.15,534.05999999999995,454.39,380.43,306.17]
[null,"S-HP360f",null,1469.04,1351.86,1231.8900000000001,1101.99,963.51,826.32,686.29]
[null,"S-HP50",null,342.9,328.61,314.81,302.02999999999997,296.5,269.55,242.29]
[null,"S-HP50 PT",null,1020,925.45,832.59,753.33,718.86,569.73,409.15]
[null,"S-LP18",null,342.7,328.47,314.54000000000002,302.04000000000002,296.32,269.86,241.84]
[null,"S-LP90",null,747.6,675.6,605.55999999999995,531.69000000000005,453.69,379.13,304.98]
[null,"LED16",null,409.7,417.69,426.91,433.53,436.75,444.91,453.15]
[null,"LED17",null,508.68,517.02,526.91999999999996,533.91,537.44000000000005,545.99,554.66999999999996]
[null,"LED17 PT",null,1820.9,1833.88,1852.84,1864.64,1872.3,1886.09,1900.6]
[null,"LED18 PT",null,1136.6400000000001,1147.21,1161.44,1170.73,1176.24,1187.3,1198.77]
[null,"LED20",null,1401.86,1413.36,1429.43,1439.69,1446.04,1458.15,1470.8]
[null,"LED22",null,646.09,654.91999999999996,665.77,673.26,677.23,686.32,695.61]
[null,"LED23 PT",null,1309.8800000000001,1321.05,1336.48,1346.41,1352.46,1364.21,1376.45]
[null,"LED24",null,504.96,513.29,523.16999999999996,530.14,533.66,542.20000000000005,550.86]
[null,"LED28",null,1401.86,1413.36,1429.43,1439.69,1446.04,1458.15,1470.8]
[null,"LED29",null,543.96,552.42999999999995,562.57000000000005,569.69000000000005,573.33000000000004,582.02,590.86]
[null,"LED32 PT",null,1243.98,1254.93,1269.9000000000001,1279.5899999999999,1285.44,1296.92,1308.8599999999999]
[null,"LED35",null,1401.86,1413.36,1429.43,1439.69,1446.04,1458.15,1470.8]
[null,"LED43",null,516.1,524.48,534.42999999999995,541.44000000000005,545,553.58000000000004,562.29]
[null,"LED58",null,815.88,825.31,837.33,845.45,849.95,859.72,869.77]
[null,"LED72",null,1030.48,1040.6600000000001,1054.1600000000001,1063.07,1068.24,1078.8699999999999,1089.8699999999999]
[null,"LED78",null,860.86,870.45,882.78,891.06,895.7,905.66,915.9]
[null,"LED79",null,1401.86,1413.36,1429.43,1439.69,1446.04,1458.15,1470.8]
[null,"LED80",null,863.35,872.95,885.3,893.59,898.24,908.2,918.45]
[null,"LED81 TM",null,1578.39,1590.52,1607.8,1618.71,1625.61,1638.43,1651.86]
[null,"LED100",null,856.36,865.93,878.23,886.49,891.12,901.06,911.28]
[null,"LED105",null,1910.66,1923.96,1943.53,1955.67,1963.61,1977.75,1992.66]
[null,"LED117",null,1401.86,1413.36,1429.43,1439.69,1446.04,1458.15,1470.8]
[null,"LED120",null,856.36,865.93,878.23,886.49,891.12,901.06,911.28]
[null,"LED151",null,865.77,875.38,887.74,896.04,900.7,910.67,920.94]
[null,"LED155 TM",null,1647.68,1660.05,1677.81,1688.98,1696.1,1709.19,1722.93]
[null,"LED175",null,1123.32,1133.8399999999999,1147.98,1157.22,1162.69,1173.69,1185.0999999999999]
[null,"LED198",null,1910.66,1923.96,1943.53,1955.67,1963.61,1977.75,1992.66]
[null,"LED180 F",null,null,1831.18,1850.11,1861.91,1869.56,1883.33,1897.83]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"cf-42",null,218.33,222.13,224.42,225.79,215.31,214.85,212.99]
[null,"cf-42 PT",null,220.87,224.78,227.3,229.07,219.22,219.7,219.68]
[null,"F-40",null,284.41000000000003,288.48,291.61,225.27,213.98,213.28,210.92]
[null,"MV-80",null,282.66000000000003,286.5,289.04000000000002,290.27,211.92,209.75,204.9]
[null,"MV-80 PT",null,219.44,223.29,225.68,227.21,216.96,216.8,215.68]
[null,"MV-80+",null,216.22,219.91,222.04,223.16,212.27,211.32,208.37]
[null,"S-HP Other",null,184.09,187.75,189.53,190.31,179.25,178.41,176.68]
[null,"S-HP100",null,211.18,215.19,217.58,218.94,208.19,206.73,202.83]
[null,"S-HP150",null,201.56,205.64,207.96,209.14,198.03,195.98,191.45]
[null,"S-HP250",null,178.66,182.96,185.52,187.17,176.87,176.33,175.13]
[null,"S-HP360f",null,220.5,224.29,226.67,228.22,218.02,217.79,216.74]
[null,"S-HP50",null,219.49,223.33,225.73,227.26,217.02,216.89,215.8]
[null,"S-HP50 PT",null,221.44,225.37,227.93,229.74,219.93,220.39,220.86]
[null,"S-LP18",null,215.16,218.8,220.86,221.85,210.82,209.71,206.39]
[null,"S-LP90",null,219.02,222.98,225.51,227.2,217.15,217.05,216]
[null,"LED16",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED17",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED17 PT",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED18 PT",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED20",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED22",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED23 PT",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED24",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED28",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED29",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED32 PT",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED35",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED43",null,175.73,176.35,176.32,177.52,119.95,120.14,120.4]
[null,"LED58",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED72",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED78",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED79",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED80",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED81 TM",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED100",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED105",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED117",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED120",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED151",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED155 TM",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED175",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED198",null,187.09,183.12,178.09,179.42,124.15,124.39,124.69]
[null,"LED180 F",null,null,183.12,178.09,179.42,124.15,124.39,124.69]

{"sheet":"5.4 MD & utilisation-Spatial","index":21,"n_rows":11580,"n_cols":12,"rows_kept":11580,"cut":false,"hidden":false,"merged":[[6,1,6,2],[12,2,13,2],[12,3,13,3],[14,2,15,2],[14,3,15,3],[16,2,17,2],[16,3,17,3],[18,2,19,2],[18,3,19,3],[20,2,21,2],[20,3,21,3],[22,2,23,2],[22,3,23,3],[24,2,25,2],[24,3,25,3],[26,2,27,2],[26,3,27,3],[28,2,29,2],[28,3,29,3],[30,2,31,2],[30,3,31,3],[32,2,33,2],[32,3,33,3],[34,2,35,2],[34,3,35,3],[36,2,37,2],[36,3,37,3],[38,2,39,2],[38,3,39,3],[40,2,41,2],[40,3,41,3],[42,2,43,2],[42,3,43,3],[44,2,45,2],[44,3,45,3],[46,2,47,2],[46,3,47,3],[48,2,49,2],[48,3,49,3],[50,2,51,2],[50,3,51,3],[52,2,53,2],[52,3,53,3],[54,2,55,2],[54,3,55,3],[56,2,57,2],[56,3,57,3],[58,2,59,2],[58,3,59,3],[60,2,61,2],[60,3,61,3],[62,2,63,2],[62,3,63,3],[64,2,65,2],[64,3,65,3],[66,2,67,2],[66,3,67,3],[68,2,69,2],[68,3,69,3],[70,2,71,2],[70,3,71,3],[72,2,73,2],[72,3,73,3],[74,2,75,2],[74,3,75,3],[76,2,77,2],[76,3,77,3],[78,2,79,2],[78,3,79,3],[80,2,81,2],[80,3,81,3],[82,2,83,2],[82,3,83,3],[84,2,85,2],[84,3,85,3],[86,2,87,2],[86,3,87,3],[88,2,89,2],[88,3,89,3],[90,2,91,2],[90,3,91,3],[92,2,93,2],[92,3,93,3],[94,2,95,2],[94,3,95,3],[96,2,97,2],[96,3,97,3],[98,2,99,2],[98,3,99,3],[100,2,101,2],[100,3,101,3],[102,2,103,2],[102,3,103,3],[104,2,105,2],[104,3,105,3],[106,2,107,2],[106,3,107,3],[108,2,109,2],[108,3,109,3],[110,2,111,2],[110,3,111,3],[112,2,113,2],[112,3,113,3],[114,2,115,2],[114,3,115,3],[116,2,117,2],[116,3,117,3],[118,2,119,2],[118,3,119,3],[120,2,121,2],[120,3,121,3],[122,2,123,2],[122,3,123,3],[124,2,125,2],[124,3,125,3],[126,2,127,2],[126,3,127,3],[128,2,129,2],[128,3,129,3],[130,2,131,2],[130,3,131,3],[132,2,133,2],[132,3,133,3],[134,2,135,2],[134,3,135,3],[136,2,137,2],[136,3,137,3],[138,2,139,2],[138,3,139,3],[140,2,141,2],[140,3,141,3],[142,2,143,2],[142,3,143,3],[144,2,145,2],[144,3,145,3],[146,2,147,2],[146,3,147,3],[148,2,149,2],[148,3,149,3],[150,2,151,2],[150,3,151,3],[152,2,153,2],[152,3,153,3],[154,2,155,2],[154,3,155,3],[156,2,157,2],[156,3,157,3],[158,2,159,2],[158,3,159,3],[160,2,161,2],[160,3,161,3],[162,2,163,2],[162,3,163,3],[164,2,165,2],[164,3,165,3],[166,2,167,2],[166,3,167,3],[168,2,169,2],[168,3,169,3],[170,2,171,2],[170,3,171,3],[172,2,173,2],[172,3,173,3],[174,2,175,2],[174,3,175,3],[176,2,177,2],[176,3,177,3],[178,2,179,2],[178,3,179,3],[180,2,181,2],[180,3,181,3],[182,2,183,2],[182,3,183,3],[184,2,185,2],[184,3,185,3],[186,2,187,2],[186,3,187,3],[188,2,189,2],[188,3,189,3],[190,2,191,2],[190,3,191,3],[192,2,193,2],[192,3,193,3],[194,2,195,2],[194,3,195,3],[196,2,197,2],[196,3,197,3],[198,2,199,2],[198,3,199,3],[200,2,201,2],[200,3,201,3],[202,2,203,2],[202,3,203,3],[204,2,205,2],[204,3,205,3],[206,2,207,2],[206,3,207,3],[208,2,209,2],[208,3,209,3],[210,2,211,2],[210,3,211,3],[212,2,213,2],[212,3,213,3],[214,2,215,2],[214,3,215,3],[216,2,217,2],[216,3,217,3],[218,2,219,2],[218,3,219,3],[220,2,221,2],[220,3,221,3],[222,2,223,2],[222,3,223,3],[224,2,225,2],[224,3,225,3],[226,2,227,2],[226,3,227,3],[228,2,229,2],[228,3,229,3],[230,2,231,2],[230,3,231,3],[232,2,233,2],[232,3,233,3],[234,2,235,2],[234,3,235,3],[236,2,237,2],[236,3,237,3],[238,2,239,2],[238,3,239,3],[240,2,241,2],[240,3,241,3],[242,2,243,2],[242,3,243,3],[244,2,245,2],[244,3,245,3],[246,2,247,2],[246,3,247,3],[248,2,249,2],[248,3,249,3],[250,2,251,2],[250,3,251,3],[252,2,253,2],[252,3,253,3],[254,2,255,2],[254,3,255,3],[256,2,257,2],[256,3,257,3],[258,2,259,2],[258,3,259,3],[260,2,261,2],[260,3,261,3],[262,2,263,2],[262,3,263,3],[264,2,265,2],[264,3,265,3],[266,2,267,2],[266,3,267,3],[268,2,269,2],[268,3,269,3],[270,2,271,2],[270,3,271,3],[272,2,273,2],[272,3,273,3],[274,2,275,2],[274,3,275,3],[276,2,277,2],[276,3,277,3],[278,2,279,2],[278,3,279,3],[280,2,281,2],[280,3,281,3],[282,2,283,2],[282,3,283,3],[284,2,285,2],[284,3,285,3],[286,2,287,2],[286,3,287,3],[288,2,289,2],[288,3,289,3],[290,2,291,2],[290,3,291,3],[292,2,293,2],[292,3,293,3],[294,2,295,2],[294,3,295,3],[296,2,297,2],[296,3,297,3],[298,2,299,2],[298,3,299,3],[300,2,301,2],[300,3,301,3],[302,2,303,2],[302,3,303,3],[304,2,305,2],[304,3,305,3],[306,2,307,2],[306,3,307,3],[308,2,309,2],[308,3,309,3],[310,2,311,2],[310,3,311,3],[312,2,313,2],[312,3,313,3],[314,2,315,2],[314,3,315,3],[316,2,317,2],[316,3,317,3],[318,2,319,2],[318,3,319,3],[320,2,321,2],[320,3,321,3],[322,2,323,2],[322,3,323,3],[324,2,325,2],[324,3,325,3],[326,2,327,2],[326,3,327,3],[328,2,329,2],[328,3,329,3],[330,2,331,2],[330,3,331,3],[332,2,333,2],[332,3,333,3],[334,2,335,2],[334,3,335,3],[336,2,337,2],[336,3,337,3],[338,2,339,2],[338,3,339,3],[340,2,341,2],[340,3,341,3],[342,2,343,2],[342,3,343,3],[344,2,345,2],[344,3,345,3],[346,2,347,2],[346,3,347,3],[348,2,349,2],[348,3,349,3],[350,2,351,2],[350,3,351,3],[352,2,353,2],[352,3,353,3],[354,2,355,2],[354,3,355,3],[356,2,357,2],[356,3,357,3],[358,2,359,2],[358,3,359,3],[360,2,361,2],[360,3,361,3],[362,2,363,2],[362,3,363,3],[364,2,365,2],[364,3,365,3],[366,2,367,2],[366,3,367,3],[368,2,369,2],[368,3,369,3],[370,2,371,2],[370,3,371,3],[372,2,373,2],[372,3,373,3],[374,2,375,2],[374,3,375,3],[376,2,377,2],[376,3,377,3],[378,2,379,2],[378,3,379,3],[380,2,381,2],[380,3,381,3],[382,2,383,2],[382,3,383,3],[384,2,385,2],[384,3,385,3],[386,2,387,2],[386,3,387,3],[388,2,389,2],[388,3,389,3],[390,2,391,2],[390,3,391,3],[392,2,393,2],[392,3,393,3],[394,2,395,2],[394,3,395,3],[396,2,397,2],[396,3,397,3],[398,2,399,2],[398,3,399,3],[400,2,401,2],[400,3,401,3],[402,2,403,2],[402,3,403,3],[404,2,405,2],[404,3,405,3],[406,2,407,2],[406,3,407,3],[408,2,409,2],[408,3,409,3],[410,2,411,2],[410,3,411,3],[412,2,413,2],[412,3,413,3],[414,2,415,2],[414,3,415,3],[416,2,417,2],[416,3,417,3],[418,2,419,2],[418,3,419,3],[420,2,421,2],[420,3,421,3],[422,2,423,2],[422,3,423,3],[424,2,425,2],[424,3,425,3],[426,2,427,2],[426,3,427,3],[428,2,429,2],[428,3,429,3],[430,2,431,2],[430,3,431,3],[432,2,433,2],[432,3,433,3],[434,2,435,2],[434,3,435,3],[436,2,437,2],[436,3,437,3],[438,2,439,2],[438,3,439,3],[440,2,441,2],[440,3,441,3],[442,2,443,2],[442,3,443,3],[444,2,445,2],[444,3,445,3],[446,2,447,2],[446,3,447,3],[448,2,449,2],[448,3,449,3],[450,2,451,2],[450,3,451,3],[452,2,453,2],[452,3,453,3],[454,2,455,2],[454,3,455,3],[456,2,457,2],[456,3,457,3],[458,2,459,2],[458,3,459,3],[460,2,461,2],[460,3,461,3],[462,2,463,2],[462,3,463,3],[464,2,465,2],[464,3,465,3],[466,2,467,2],[466,3,467,3],[468,2,469,2],[468,3,469,3],[470,2,471,2],[470,3,471,3],[472,2,473,2],[472,3,473,3],[474,2,475,2],[474,3,475,3],[476,2,477,2],[476,3,477,3],[478,2,479,2],[478,3,479,3],[480,2,481,2],[480,3,481,3],[482,2,483,2],[482,3,483,3],[484,2,485,2],[484,3,485,3],[486,2,487,2],[486,3,487,3],[488,2,489,2],[488,3,489,3],[490,2,491,2],[490,3,491,3],[492,2,493,2],[492,3,493,3],[494,2,495,2],[494,3,495,3],[496,2,497,2],[496,3,497,3],[498,2,499,2],[498,3,499,3],[500,2,501,2],[500,3,501,3],[502,2,503,2],[502,3,503,3],[504,2,505,2],[504,3,505,3],[506,2,507,2],[506,3,507,3],[508,2,509,2],[508,3,509,3],[510,2,511,2],[510,3,511,3],[512,2,513,2],[512,3,513,3],[514,2,515,2],[514,3,515,3],[516,2,517,2],[516,3,517,3],[518,2,519,2],[518,3,519,3],[520,2,521,2],[520,3,521,3],[522,2,523,2],[522,3,523,3],[524,2,525,2],[524,3,525,3],[526,2,527,2],[526,3,527,3],[528,2,529,2],[528,3,529,3],[530,2,531,2],[530,3,531,3],[532,2,533,2],[532,3,533,3],[534,2,535,2],[534,3,535,3],[536,2,537,2],[536,3,537,3],[538,2,539,2],[538,3,539,3],[540,2,541,2],[540,3,541,3],[542,2,543,2],[542,3,543,3],[544,2,545,2],[544,3,545,3],[546,2,547,2],[546,3,547,3],[548,2,549,2],[548,3,549,3],[550,2,551,2],[550,3,551,3],[552,2,553,2],[552,3,553,3],[554,2,555,2],[554,3,555,3],[556,2,557,2],[556,3,557,3],[558,2,559,2],[558,3,559,3],[560,2,561,2],[560,3,561,3],[562,2,563,2],[562,3,563,3],[564,2,565,2],[564,3,565,3],[566,2,567,2],[566,3,567,3],[568,2,569,2],[568,3,569,3],[570,2,571,2],[570,3,571,3],[572,2,573,2],[572,3,573,3],[574,2,575,2],[574,3,575,3],[576,2,577,2],[576,3,577,3],[578,2,579,2],[578,3,579,3],[580,2,581,2],[580,3,581,3],[582,2,583,2],[582,3,583,3],[584,2,585,2],[584,3,585,3],[586,2,587,2],[586,3,587,3],[588,2,589,2],[588,3,589,3],[590,2,591,2],[590,3,591,3],[592,2,593,2],[592,3,593,3],[594,2,595,2],[594,3,595,3],[596,2,597,2],[596,3,597,3],[598,2,599,2],[598,3,599,3],[600,2,601,2],[600,3,601,3],[602,2,603,2],[602,3,603,3],[604,2,605,2],[604,3,605,3],[606,2,607,2],[606,3,607,3],[608,2,609,2],[608,3,609,3],[610,2,611,2],[610,3,611,3],[612,2,613,2],[612,3,613,3],[614,2,615,2],[614,3,615,3],[616,2,617,2],[616,3,617,3],[618,2,619,2],[618,3,619,3],[620,2,621,2],[620,3,621,3],[622,2,623,2],[622,3,623,3],[624,2,625,2],[624,3,625,3],[626,2,627,2],[626,3,627,3],[628,2,629,2],[628,3,629,3],[630,2,631,2],[630,3,631,3],[632,2,633,2],[632,3,633,3],[634,2,635,2],[634,3,635,3],[636,2,637,2],[636,3,637,3],[638,2,639,2],[638,3,639,3],[640,2,641,2],[640,3,641,3],[642,2,643,2],[642,3,643,3],[644,2,645,2],[644,3,645,3],[646,2,647,2],[646,3,647,3],[648,2,649,2],[648,3,649,3],[650,2,651,2],[650,3,651,3],[652,2,653,2],[652,3,653,3],[654,2,655,2],[654,3,655,3],[656,2,657,2],[656,3,657,3],[658,2,659,2],[658,3,659,3],[660,2,661,2],[660,3,661,3],[662,2,663,2],[662,3,663,3],[664,2,665,2],[664,3,665,3],[666,2,667,2],[666,3,667,3],[668,2,669,2],[668,3,669,3],[670,2,671,2],[670,3,671,3],[672,2,673,2],[672,3,673,3],[674,2,675,2],[674,3,675,3],[676,2,677,2],[676,3,677,3],[678,2,679,2],[678,3,679,3],[680,2,681,2],[680,3,681,3],[682,2,683,2],[682,3,683,3],[684,2,685,2],[684,3,685,3],[686,2,687,2],[686,3,687,3],[688,2,689,2],[688,3,689,3],[690,2,691,2],[690,3,691,3],[692,2,693,2],[692,3,693,3],[694,2,695,2],[694,3,695,3],[696,2,697,2],[696,3,697,3],[698,2,699,2],[698,3,699,3],[700,2,701,2],[700,3,701,3],[702,2,703,2],[702,3,703,3],[704,2,705,2],[704,3,705,3],[706,2,707,2],[706,3,707,3],[708,2,709,2],[708,3,709,3],[710,2,711,2],[710,3,711,3],[712,2,713,2],[712,3,713,3],[714,2,715,2],[714,3,715,3],[716,2,717,2],[716,3,717,3],[718,2,719,2],[718,3,719,3],[720,2,721,2],[720,3,721,3],[722,2,723,2],[722,3,723,3],[724,2,725,2],[724,3,725,3],[726,2,727,2],[726,3,727,3],[728,2,729,2],[728,3,729,3],[730,2,731,2],[730,3,731,3],[732,2,733,2],[732,3,733,3],[734,2,735,2],[734,3,735,3],[736,2,737,2],[736,3,737,3],[738,2,739,2],[738,3,739,3],[740,2,741,2],[740,3,741,3],[742,2,743,2],[742,3,743,3],[744,2,745,2],[744,3,745,3],[746,2,747,2],[746,3,747,3],[748,2,749,2],[748,3,749,3],[750,2,751,2],[750,3,751,3],[752,2,753,2],[752,3,753,3],[754,2,755,2],[754,3,755,3],[756,2,757,2],[756,3,757,3],[758,2,759,2],[758,3,759,3],[760,2,761,2],[760,3,761,3],[762,2,763,2],[762,3,763,3],[764,2,765,2],[764,3,765,3],[766,2,767,2],[766,3,767,3],[768,2,769,2],[768,3,769,3],[770,2,771,2],[770,3,771,3],[772,2,773,2],[772,3,773,3],[774,2,775,2],[774,3,775,3],[776,2,777,2],[776,3,777,3],[778,2,779,2],[778,3,779,3],[780,2,781,2],[780,3,781,3],[782,2,783,2],[782,3,783,3],[784,2,785,2],[784,3,785,3],[786,2,787,2],[786,3,787,3],[788,2,789,2],[788,3,789,3],[790,2,791,2],[790,3,791,3],[792,2,793,2],[792,3,793,3],[794,2,795,2],[794,3,795,3],[796,2,797,2],[796,3,797,3],[798,2,799,2],[798,3,799,3],[800,2,801,2],[800,3,801,3],[802,2,803,2],[802,3,803,3],[804,2,805,2],[804,3,805,3],[806,2,807,2],[806,3,807,3],[808,2,809,2],[808,3,809,3],[810,2,811,2],[810,3,811,3],[812,2,813,2],[812,3,813,3],[814,2,815,2],[814,3,815,3],[816,2,817,2],[816,3,817,3],[818,2,819,2],[818,3,819,3],[820,2,821,2],[820,3,821,3],[822,2,823,2],[822,3,823,3],[824,2,825,2],[824,3,825,3],[826,2,827,2],[826,3,827,3],[828,2,829,2],[828,3,829,3],[830,2,831,2],[830,3,831,3],[832,2,833,2],[832,3,833,3],[834,2,835,2],[834,3,835,3],[836,2,837,2],[836,3,837,3],[838,2,839,2],[838,3,839,3],[840,2,841,2],[840,3,841,3],[842,2,843,2],[842,3,843,3],[844,2,845,2],[844,3,845,3],[846,2,847,2],[846,3,847,3],[848,2,849,2],[848,3,849,3],[850,2,851,2],[850,3,851,3],[852,2,853,2],[852,3,853,3],[854,2,855,2],[854,3,855,3],[856,2,857,2],[856,3,857,3],[858,2,859,2],[858,3,859,3],[860,2,861,2],[860,3,861,3],[862,2,863,2],[862,3,863,3],[864,2,865,2],[864,3,865,3],[866,2,867,2],[866,3,867,3],[868,2,869,2],[868,3,869,3],[870,2,871,2],[870,3,871,3],[872,2,873,2],[872,3,873,3],[874,2,875,2],[874,3,875,3],[876,2,877,2],[876,3,877,3],[878,2,879,2],[878,3,879,3],[880,2,881,2],[880,3,881,3],[882,2,883,2],[882,3,883,3],[884,2,885,2],[884,3,885,3],[886,2,887,2],[886,3,887,3],[888,2,889,2],[888,3,889,3],[890,2,891,2],[890,3,891,3],[892,2,893,2],[892,3,893,3],[894,2,895,2],[894,3,895,3],[896,2,897,2],[896,3,897,3],[898,2,899,2],[898,3,899,3],[900,2,901,2],[900,3,901,3],[902,2,903,2],[902,3,903,3],[904,2,905,2],[904,3,905,3],[906,2,907,2],[906,3,907,3],[908,2,909,2],[908,3,909,3],[910,2,911,2],[910,3,911,3],[912,2,913,2],[912,3,913,3],[914,2,915,2],[914,3,915,3],[916,2,917,2],[916,3,917,3],[918,2,919,2],[918,3,919,3],[920,2,921,2],[920,3,921,3],[922,2,923,2],[922,3,923,3],[924,2,925,2],[924,3,925,3],[926,2,927,2],[926,3,927,3],[928,2,929,2],[928,3,929,3],[930,2,931,2],[930,3,931,3],[932,2,933,2],[932,3,933,3],[934,2,935,2],[934,3,935,3],[936,2,937,2],[936,3,937,3],[938,2,939,2],[938,3,939,3],[940,2,941,2],[940,3,941,3],[942,2,943,2],[942,3,943,3],[944,2,945,2],[944,3,945,3],[946,2,947,2],[946,3,947,3],[948,2,949,2],[948,3,949,3],[950,2,951,2],[950,3,951,3],[952,2,953,2],[952,3,953,3],[954,2,955,2],[954,3,955,3],[956,2,957,2],[956,3,957,3],[958,2,959,2],[958,3,959,3],[960,2,961,2],[960,3,961,3],[962,2,963,2],[962,3,963,3],[964,2,965,2],[964,3,965,3],[966,2,967,2],[966,3,967,3],[968,2,969,2],[968,3,969,3],[970,2,971,2],[970,3,971,3],[972,2,973,2],[972,3,973,3],[974,2,975,2],[974,3,975,3],[976,2,977,2],[976,3,977,3],[978,2,979,2],[978,3,979,3],[980,2,981,2],[980,3,981,3],[982,2,983,2],[982,3,983,3],[984,2,985,2],[984,3,985,3],[986,2,987,2],[986,3,987,3],[988,2,989,2],[988,3,989,3],[990,2,991,2],[990,3,991,3],[992,2,993,2],[992,3,993,3],[994,2,995,2],[994,3,995,3],[996,2,997,2],[996,3,997,3],[998,2,999,2],[998,3,999,3],[1000,2,1001,2],[1000,3,1001,3],[1002,2,1003,2],[1002,3,1003,3],[1004,2,1005,2],[1004,3,1005,3],[1006,2,1007,2],[1006,3,1007,3],[1008,2,1009,2],[1008,3,1009,3],[1010,2,1011,2]],"merged_total":11555,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"DEMAND"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"ACR 66kV","Substation Rating","MVA","Non-Coincident",525,525,525,525,525,525,525]
[null,null,null,null,"Coincident",525,525,525,525,525,525,525]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",202.53089477278999,201.923761735,200.90620791463999,199.13881869286999,197.40935767265,195.69448577295,194.04695217912999]
[null,null,null,null,"Coincident",130.46593006277999,130.07482836673,129.41934266558999,128.28082955695999,127.16674895823,126.06206634877999,125.00076158898]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",206.43109549702001,205.81227070860999,204.77512153638,202.97369714812001,201.21093135664,199.46303563294001,197.78377496990001]
[null,null,null,null,"Coincident",132.97835324389001,132.57971998027,131.91161138616999,130.75117357486999,129.61563877793,128.48968295029999,127.40794031311999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",189.96794359721,189.36916240004999,188.38933112647999,186.65486551295999,184.93372040080001,183.22716440916,181.58794672338999]
[null,null,null,null,"Coincident",122.37315433444,121.9874327097,121.35624704020999,120.23894259299,119.13021891859,118.03089323347,116.97494539800999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",193.62621564518,193.01590353141,192.01720334084999,190.24933658104999,188.49504683966001,186.75562716605,185.08484255311001]
[null,null,null,null,"Coincident",124.72973240464999,124.33658281805999,123.6932422089,122.55442148082,121.42434676819001,120.30385102485,119.22756847198001]
[null,"Angas Creek 33kV","Substation Rating","MVA","Non-Coincident",53.9,53.9,53.9,53.9,53.9,53.9,53.9]
[null,null,null,null,"Coincident",53.9,53.9,53.9,53.9,53.9,53.9,53.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.218969911399,20.756492764891998,21.414054601351999,22.195269550877999,22.755733719578998,23.318936447978999,23.880935713903]
[null,null,null,null,"Coincident",19.593711605871999,20.165453027114999,20.706147627880998,21.242251893393998,21.780021941504,22.320477889605002,22.856616729831]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.632073754438,21.180579005030999,21.851575814827999,22.648752156023001,23.220667447259,23.795377251068999,24.368859003865001]
[null,null,null,null,"Coincident",19.994040485100999,20.577463440041001,21.129205241453999,21.676262920189,22.225020415953999,22.776518688669999,23.323611648532001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.268329866058,18.744415702470999,19.356252277145,20.096692409077999,20.659125869035002,21.205388010181998,21.745845655444999]
[null,null,null,null,"Coincident",17.948417805329999,18.455614162297,18.985436795428999,19.513479515583999,20.061167714540002,20.592935123726999,21.115811023498999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.641579210938001,19.127392194159,19.751729506577998,20.507297939575999,21.081222757637001,21.638645852621,22.190145857175001]
[null,null,null,null,"Coincident",18.315130867585999,18.832690005899,19.373337709091999,19.912169133022001,20.471047422312999,21.013679636249002,21.547238673915]
[null,"Ardrossan West 33kV","Substation Rating","MVA","Non-Coincident",62,62,62,62,62,62,62]
[null,null,null,null,"Coincident",62,62,62,62,62,62,62]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12,12,12,13,13,13,13]
[null,null,null,null,"Coincident",10,10,10,11,11,11,11]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12,12,12,13,13,13,13]
[null,null,null,null,"Coincident",10,10,10,11,11,11,11]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10,10,11,11,11,12,12]
[null,null,null,null,"Coincident",9,9,9,9,10,10,10]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10,10,11,11,11,12,12]
[null,null,null,null,"Coincident",9,9,9,9,10,10,10]
[null,"Baroota 33kV","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.2632242077041003,7.3512409031950998,7.4789799454630996,7.6461426727698996,7.7341075996731004,7.8210020248141001,7.9058001211960001]
[null,null,null,null,"Coincident",6.1532722125446,6.2435796683206002,6.3221058235968002,6.3973707487378002,6.4713765619716002,6.5444950008238996,6.6149326761499996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2966346069375003,7.3850561739911997,7.5133828082537999,7.6813144741609998,7.7696840344945004,7.8569781688214002,7.9421663314017001]
[null,null,null,null,"Coincident",6.1815768986363002,6.272299763336,6.3511871342547002,6.4267982735734996,6.5011445091451003,6.5745992884661,6.6453609729079997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4882858322091002,6.5520071372027999,6.6604102029124999,6.8090963458455001,6.8939311786294004,6.9709872417733001,7.0464718306598]
[null,null,null,null,"Coincident",5.5728363702291999,5.6396213863879998,5.7110937455044999,5.7798770840428002,5.8523488064041,5.9181409961047002,5.9816662475831999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5181315610197004,6.5821459802254001,6.6910476935879002,6.8404177839324003,6.9256428518998998,7.0030533683499003,7.0788851818543002]
[null,null,null,null,"Coincident",5.5984710859789999,5.6655633092387996,5.7373644369549996,5.8064641747583998,5.8792692627307996,5.9453640925898004,6.0091815564455997]
[null,"Berri 66kV","Substation Rating","MVA","Non-Coincident",190,190,190,190,190,190,190]
[null,null,null,null,"Coincident",190,190,190,190,190,190,190]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",100.27809840092,105.94872778471,108.07691572072,110.78260319261,112.3474849358,113.90009716893,115.41611849907]
[null,null,null,null,"Coincident",96.346772817906,102.05238385014999,103.61120863089,105.11993747661,106.61154113725,108.09167371155,109.52177359311]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",101.73916334504,107.49241453694999,109.65161044815,112.39672013863,113.98440241247999,115.55963640791001,117.09774636612001]
[null,null,null,null,"Coincident",97.750557836653996,103.53930036417999,105.12083742484,106.6515486462,108.16488516629001,109.66658346481999,111.11752008777999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",92.331704798556999,97.808209045040996,99.841247627244002,102.49123757213,104.19218659493001,105.78281857816,107.31186286477001]
[null,null,null,null,"Coincident",89.939729497095001,95.478436503240999,97.091836523783002,98.666623354131005,100.31198314922,101.84988887367,103.31243471074001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",93.676989753732002,99.233287379813007,101.29594759874,103.984548242,105.71028031343,107.32408801166,108.87541067252]
[null,null,null,null,"Coincident",91.250163060831994,96.869569748876998,98.506477217691,100.10420889709999,101.77354179853,103.33385500954,104.81771032979]
[null,"Blanche 33kV","Substation Rating","MVA","Non-Coincident",126.3,126.3,126.3,126.3,126.3,126.3,126.3]
[null,null,null,null,"Coincident",126.3,126.3,126.3,126.3,126.3,126.3,126.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37,38,39,40,41,42,43]
[null,null,null,null,"Coincident",34,35,36,37,38,38,39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39,40,41,43,43,44,45]
[null,null,null,null,"Coincident",36,37,38,39,40,41,41]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34,35,36,37,38,39,39]
[null,null,null,null,"Coincident",32,33,34,34,35,36,36]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36,37,38,39,40,41,41]
[null,null,null,null,"Coincident",34,35,35,36,37,38,38]
[null,"Brinkworth 33kV","Substation Rating","MVA","Non-Coincident",25,25,25,25,25,25,25]
[null,null,null,null,"Coincident",25,25,25,25,25,25,25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.2099415845524,5.3131799410902003,5.4462377888561004,5.6094318563924999,5.7157368647819,5.8220121002207996,5.9272084425068003]
[null,null,null,null,"Coincident",4.8741624641312002,4.9833110563170999,5.084010759621,5.1828479584705001,5.2814011808089001,5.3799385494544003,5.4767165979690997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.3205338905530004,5.4259637050432996,5.5618459941156999,5.7285042095628,5.8370657722389998,5.9455969299694003,6.0530262927005003]
[null,null,null,null,"Coincident",4.9776271302856001,5.0890926379897996,5.1919299108272003,5.2928651435149003,5.3935103716743003,5.4941394096118001,5.5929717820342999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.6998365654947003,4.7913226791544998,4.9167226413521004,5.0735732753661003,5.1844028253637999,5.2904277680670004,5.3942329618971003]
[null,null,null,null,"Coincident",4.4577893555991999,4.5542983375099002,4.6556946723305996,4.7559089312756999,4.8601812664923996,4.9598926680469999,5.0567400119597004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7996007864881998,4.8930288912647999,5.0210907395444,5.1812708683390998,5.2944530158290997,5.4027285678179,5.5087372519509001]
[null,null,null,null,"Coincident",4.5524155997709999,4.6509731940675998,4.7545218859359002,4.8568634098054,4.9633491514137997,5.0651771436543997,5.1640802824199996]
[null,"Clare North 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.280221744031,12.412670910779999,12.611883987885999,12.876749340936,13.00754006951,13.135991580413,13.259681156593]
[null,null,null,null,"Coincident",11.676066292648001,11.831829689459999,11.965008877240001,12.091467981413,12.215051429019001,12.336451877950999,12.451633956065001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.537067494461001,12.672286888518,12.875666586827,13.146071704693,13.279597973679,13.410736099317999,13.537012692465]
[null,null,null,null,"Coincident",11.920275890122999,12.079297140691001,12.215261824461001,12.344365871388,12.470534116239,12.594473704126999,12.712064861482]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.06616915843,11.166790405347999,11.343483811840001,11.588242272369,11.723859156481,11.845839266169,11.960186306601001]
[null,null,null,null,"Coincident",10.66736825289,10.787420727827,10.916374663778999,11.039778384443,11.169854529292,11.286791981106999,11.394678282783]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.297622513356,11.400348293905999,11.58073731368,11.830614995325,11.969068360822,12.093599733301,12.210338387827999]
[null,null,null,null,"Coincident",10.890480527336999,11.013043947813999,11.144695006924,11.270679765773,11.403476505227999,11.522859750627999,11.633002537463]
[null,"Dalrymple 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.2649128842542998,7.3854726394914003,7.5468124278759001,7.7491374695355999,7.8722197646582002,7.9948727886400999,8.1159699247071]
[null,null,null,null,"Coincident",5.6235927481917001,5.7313650370106997,5.8289418408136999,5.9240574545311997,6.0185302144617996,6.1126858065979999,6.2047859096747002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2682464867672998,7.3888615624616998,7.5502753837676,7.7526932649806,7.8758320380617004,7.9985413430253001,8.1196940461340006]
[null,null,null,null,"Coincident",5.6261732089923999,5.7339949505685004,5.8316165287938997,5.9267757875838001,6.0212918976048,6.1154906942945999,6.2076330587364001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3830968706769999,6.4741229386582999,6.6100492641806996,6.7870678267075002,6.9014495668892,7.0087372574506999,7.1127889183314998]
[null,null,null,null,"Coincident",5.0093863353210999,5.0917058081890003,5.1788076587619001,5.2640267375162999,5.3531615696507,5.4367275915158002,5.5169259121463003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.3860258401097001,6.4770936766206004,6.6130823737568001,6.7901821636203001,6.9046163893942998,7.0119533103486997,7.1160527167268004]
[null,null,null,null,"Coincident",5.0116849592883996,5.0940422055483001,5.1811840239710998,5.2664422066404004,5.3556179394854997,5.4392223067382002,5.5194574274415]
[null,"Davenport West 33kV","Substation Rating","MVA","Non-Coincident",120,120,120,120,120,120,120]
[null,null,null,null,"Coincident",120,120,120,120,120,120,120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34,35,36,36,37,37,37]
[null,null,null,null,"Coincident",32,33,33,34,34,34,34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35,36,37,37,37,38,38]
[null,null,null,null,"Coincident",33,34,34,34,35,35,35]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31,32,32,33,33,34,34]
[null,null,null,null,"Coincident",29,31,31,31,31,31,32]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32,33,33,34,34,34,34]
[null,null,null,null,"Coincident",30,31,31,32,32,32,32]
[null,"Dorrien 33kV","Substation Rating","MVA","Non-Coincident",216,216,216,216,216,216,216]
[null,null,null,null,"Coincident",216,216,216,216,216,216,216]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63,64,65,66,67,68,69]
[null,null,null,null,"Coincident",60,61,62,62,63,64,65]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",65,66,67,69,70,71,72]
[null,null,null,null,"Coincident",62,63,64,65,66,66,67]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",57,57,58,60,61,61,62]
[null,null,null,null,"Coincident",55,55,56,57,58,58,59]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59,59,60,62,63,64,64]
[null,null,null,null,"Coincident",57,57,58,59,60,61,61]
[null,"Florieton SWER 19kV","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Hummocks 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14,15,15,16,16,16,17]
[null,null,null,null,"Coincident",12,12,12,13,13,13,14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14,15,15,16,16,17,17]
[null,null,null,null,"Coincident",12,12,13,13,13,14,14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13,13,13,14,14,14,15]
[null,null,null,null,"Coincident",11,11,11,11,12,12,12]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13,13,13,14,14,14,15]
[null,null,null,null,"Coincident",11,11,11,11,12,12,12]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kadina East 33kV","Substation Rating","MVA","Non-Coincident",120,120,120,120,120,120,120]
[null,null,null,null,"Coincident",120,120,120,120,120,120,120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41,41,42,43,43,44,44]
[null,null,null,null,"Coincident",32,33,33,34,34,34,35]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42,42,43,44,44,45,45]
[null,null,null,null,"Coincident",33,34,34,35,35,35,36]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37,38,38,39,40,40,41]
[null,null,null,null,"Coincident",30,31,31,31,32,32,32]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38,39,39,40,41,41,42]
[null,null,null,null,"Coincident",31,31,32,32,33,33,33]
[null,"Kanmantoo 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",1,1,2,2,2,2,2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",1,2,2,2,2,2,2]
[null,"Keith 33kV","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25,25,25,26,26,27,27]
[null,null,null,null,"Coincident",23,23,24,24,24,25,25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25,25,26,26,27,27,27]
[null,null,null,null,"Coincident",23,24,24,24,25,25,25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22,22,23,23,24,24,24]
[null,null,null,null,"Coincident",21,21,21,22,22,22,23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22,23,23,24,24,24,25]
[null,null,null,null,"Coincident",21,21,22,22,22,23,23]
[null,"Kincraig 33kV","Substation Rating","MVA","Non-Coincident",52,52,52,52,52,52,52]
[null,null,null,null,"Coincident",52,52,52,52,52,52,52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23,24,24,25,25,25,25]
[null,null,null,null,"Coincident",22,22,23,23,23,24,24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24,24,24,25,25,26,26]
[null,null,null,null,"Coincident",22,23,23,23,24,24,24]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21,21,21,22,22,22,23]
[null,null,null,null,"Coincident",20,20,20,21,21,21,22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21,21,22,22,23,23,23]
[null,null,null,null,"Coincident",20,21,21,21,21,22,22]
[null,"Leigh Creek South 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,"Mannum 33kV","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident",40,40,40,40,40,40,40]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14,15,15,15,16,16,16]
[null,null,null,null,"Coincident",11,11,11,11,11,12,12]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15,15,15,16,16,16,17]
[null,null,null,null,"Coincident",11,11,11,11,12,12,12]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13,13,13,14,14,14,14]
[null,null,null,null,"Coincident",10,10,10,10,10,10,11]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13,13,14,14,14,14,15]
[null,null,null,null,"Coincident",10,10,10,10,10,11,11]
[null,"Metro East 66kV","Substation Rating","MVA","Non-Coincident",1650,1650,1650,1650,1650,1650,1650]
[null,null,null,null,"Coincident",1650,1650,1650,1650,1650,1650,1650]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",789,803,822,845,860,875,891]
[null,null,null,null,"Coincident",779,795,810,824,839,853,869]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",797,811,830,854,869,884,900]
[null,null,null,null,"Coincident",787,803,818,833,847,862,877]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",699,711,724,745,759,774,790]
[null,null,null,null,"Coincident",699,711,724,737,751,766,782]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",706,718,732,753,767,782,798]
[null,null,null,null,"Coincident",706,718,732,745,759,774,790]
[null,"Metro North 66kV","Substation Rating","MVA","Non-Coincident",870,870,870,870,870,870,870]
[null,null,null,null,"Coincident",870,870,870,870,870,870,870]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",421,516,527,541,549,558,566]
[null,null,null,null,"Coincident",417,512,521,529,537,546,554]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",424,520,531,545,554,562,571]
[null,null,null,null,"Coincident",420,516,525,533,542,550,559]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",389,484,492,504,513,522,531]
[null,null,null,null,"Coincident",389,484,492,500,509,518,527]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",392,487,496,508,517,526,535]
[null,null,null,null,"Coincident",392,487,496,504,513,522,531]
[null,"Metro South 66kV","Substation Rating","MVA","Non-Coincident",1527,1527,1527,1527,1527,1527,1527]
[null,null,null,null,"Coincident",1527,1527,1527,1527,1527,1527,1527]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",782,803,840,875,883,890,908]
[null,null,null,null,"Coincident",782,803,840,875,883,890,908]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",785,806,844,879,886,893,912]
[null,null,null,null,"Coincident",785,806,844,879,886,893,912]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",702,720,756,790,797,802,820]
[null,null,null,null,"Coincident",702,720,756,790,797,802,820]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",704,722,759,793,800,805,823]
[null,null,null,null,"Coincident",704,722,759,793,800,805,823]
[null,"Metro West 66kV","Substation Rating","MVA","Non-Coincident",885,885,885,885,885,885,885]
[null,null,null,null,"Coincident",885,885,885,885,885,885,885]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",463,472,484,498,508,517,527]
[null,null,null,null,"Coincident",459,470,479,489,498,507,517]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",466,475,487,501,511,521,530]
[null,null,null,null,"Coincident",462,473,482,492,501,510,520]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",418,426,435,446,455,464,472]
[null,null,null,null,"Coincident",418,426,435,443,452,461,470]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",421,429,438,448,457,466,475]
[null,null,null,null,"Coincident",421,429,438,446,455,464,473]
[null,"Mobilong 33kV","Substation Rating","MVA","Non-Coincident",114,114,114,114,114,114,114]
[null,null,null,null,"Coincident",114,114,114,114,114,114,114]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42,43,43,45,45,46,47]
[null,null,null,null,"Coincident",39,40,41,42,42,43,44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44,45,46,47,48,48,49]
[null,null,null,null,"Coincident",41,42,43,44,44,45,46]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38,39,39,40,41,42,42]
[null,null,null,null,"Coincident",36,37,38,38,39,39,40]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40,40,41,42,43,44,44]
[null,null,null,null,"Coincident",38,39,39,40,41,41,42]
[null,"Mount Barker 66kV","Substation Rating","MVA","Non-Coincident",362,362,362,362,362,362,362]
[null,null,null,null,"Coincident",362,362,362,362,362,362,362]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",103,106,109,114,116,119,123]
[null,null,null,null,"Coincident",103,106,109,112,115,118,121]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",104,107,111,115,118,121,124]
[null,null,null,null,"Coincident",104,107,110,113,116,119,122]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",89,91,94,97,99,102,105]
[null,null,null,null,"Coincident",89,91,94,96,99,102,104]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",90,92,95,98,100,103,106]
[null,null,null,null,"Coincident",90,92,95,97,100,103,106]
[null,"Mount Gambier 33kV","Substation Rating","MVA","Non-Coincident",63,63,63,63,63,63,63]
[null,null,null,null,"Coincident",63,63,63,63,63,63,63]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24,24,24,25,25,25,26]
[null,null,null,null,"Coincident",22,22,22,22,23,23,23]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25,25,26,27,27,27,28]
[null,null,null,null,"Coincident",23,23,24,24,24,25,25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22,22,22,23,23,24,24]
[null,null,null,null,"Coincident",20,21,21,21,21,22,22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23,24,24,25,25,25,26]
[null,null,null,null,"Coincident",22,22,22,23,23,23,24]
[null,"Mount Gunson 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,2,2,2,2,3,3]
[null,null,null,null,"Coincident",0,1,2,2,2,2,2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,4,4,4,4,4,4]
[null,null,null,null,"Coincident",0,2,2,2,2,2,3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,2,2,2,2,2,2]
[null,null,null,null,"Coincident",0,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,4,4,4,4,4,4]
[null,null,null,null,"Coincident",0,2,2,2,2,2,2]
[null,"Neuroodla 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4,5,5,5,5,5,5]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5,5,5,5,5,5,5]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,"North West Bend 66kV","Substation Rating","MVA","Non-Coincident",74,74,74,74,74,74,74]
[null,null,null,null,"Coincident",74,74,74,74,74,74,74]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25,25,26,26,27,27,28]
[null,null,null,null,"Coincident",18,18,19,19,19,20,20]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26,26,27,28,28,29,29]
[null,null,null,null,"Coincident",19,19,20,20,20,21,21]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23,23,24,24,25,25,26]
[null,null,null,null,"Coincident",17,17,17,18,18,18,19]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24,24,25,25,26,26,27]
[null,null,null,null,"Coincident",17,18,18,19,19,19,20]
[null,"Penola West 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8,8,8,8,9,9,9]
[null,null,null,null,"Coincident",6,7,7,7,7,7,7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8,8,8,9,9,9,9]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7,7,7,7,8,8,8]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7,7,8,8,8,8,8]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,"Port Lincoln Terminal 33kV","Substation Rating","MVA","Non-Coincident",101,101,101,101,101,101,101]
[null,null,null,null,"Coincident",101,101,101,101,101,101,101]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31,35,39,40,40,41,41]
[null,null,null,null,"Coincident",29,33,36,37,37,38,38]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32,36,40,41,41,42,42]
[null,null,null,null,"Coincident",30,34,37,38,38,39,39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28,32,36,37,37,38,38]
[null,null,null,null,"Coincident",27,31,34,34,35,35,36]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29,33,37,38,38,39,39]
[null,null,null,null,"Coincident",27,32,35,35,36,36,37]
[null,"Port Pirie Bungama 33kV","Substation Rating","MVA","Non-Coincident",192,192,192,192,192,192,192]
[null,null,null,null,"Coincident",192,192,192,192,192,192,192]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",67,68,69,70,71,72,72]
[null,null,null,null,"Coincident",59,59,60,61,61,62,62]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",68,69,70,71,72,73,73]
[null,null,null,null,"Coincident",60,60,61,61,62,63,63]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63,64,65,66,67,67,68]
[null,null,null,null,"Coincident",56,56,57,58,58,59,59]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64,65,66,67,68,68,69]
[null,null,null,null,"Coincident",57,57,58,59,59,60,60]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Snuggery Rural 33kV","Substation Rating","MVA","Non-Coincident",29,29,29,29,29,29,29]
[null,null,null,null,"Coincident",29,29,29,29,29,29,29]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15,16,16,16,17,17,17]
[null,null,null,null,"Coincident",14,15,15,15,16,16,16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15,16,16,17,17,17,18]
[null,null,null,null,"Coincident",14,15,15,15,16,16,16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14,14,14,15,15,15,15]
[null,null,null,null,"Coincident",13,13,13,14,14,14,15]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14,14,14,15,15,15,16]
[null,null,null,null,"Coincident",13,13,13,14,14,14,15]
[null,"Stony Point 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Tailem Bend 33kV","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30,31,32,33,33,34,34]
[null,null,null,null,"Coincident",30,30,31,31,32,33,33]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31,32,33,33,34,35,35]
[null,null,null,null,"Coincident",30,31,32,32,33,33,34]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28,29,29,30,31,31,32]
[null,null,null,null,"Coincident",28,28,29,30,30,31,31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29,29,30,31,32,32,33]
[null,null,null,null,"Coincident",29,29,30,30,31,31,32]
[null,"Templers 33kV","Substation Rating","MVA","Non-Coincident",148,148,148,148,148,148,148]
[null,null,null,null,"Coincident",148,148,148,148,148,148,148]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35,35,36,38,38,39,40]
[null,null,null,null,"Coincident",34,35,36,37,37,38,39]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35,36,37,38,39,40,41]
[null,null,null,null,"Coincident",35,36,37,37,38,39,40]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31,32,33,34,34,35,36]
[null,null,null,null,"Coincident",31,32,33,33,34,35,36]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32,32,33,34,35,36,37]
[null,null,null,null,"Coincident",32,32,33,34,35,36,36]
[null,"Waterloo 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10,10,10,10,11,11,11]
[null,null,null,null,"Coincident",9,9,10,10,10,10,10]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10,10,10,10,11,11,11]
[null,null,null,null,"Coincident",9,9,10,10,10,10,10]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9,9,9,9,9,10,10]
[null,null,null,null,"Coincident",8,9,9,9,9,9,9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9,9,9,9,10,10,10]
[null,null,null,null,"Coincident",8,9,9,9,9,9,9]
[null,"Whyalla Central 33kV","Substation Rating","MVA","Non-Coincident",240,240,240,240,240,240,240]
[null,null,null,null,"Coincident",240,240,240,240,240,240,240]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",83,85,87,90,91,93,95]
[null,null,null,null,"Coincident",63,65,66,67,69,70,72]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",89,91,93,96,98,100,102]
[null,null,null,null,"Coincident",68,69,71,72,74,75,77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",79,80,82,85,87,89,91]
[null,null,null,null,"Coincident",61,62,63,65,66,68,69]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",85,86,88,91,93,95,97]
[null,null,null,null,"Coincident",65,67,68,70,71,73,74]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Wudinna 66kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15,15,15,16,16,16,16]
[null,null,null,null,"Coincident",12,12,12,13,13,13,13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15,15,16,16,16,16,16]
[null,null,null,null,"Coincident",12,12,13,13,13,13,13]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13,14,14,14,14,15,15]
[null,null,null,null,"Coincident",11,11,11,11,12,12,12]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14,14,14,14,14,15,15]
[null,null,null,null,"Coincident",11,11,11,12,12,12,12]
[null,"Yadnarie 66kV","Substation Rating","MVA","Non-Coincident",46,46,46,46,46,46,46]
[null,null,null,null,"Coincident",46,46,46,46,46,46,46]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,7,7,7,7,7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Aldgate 11kV","Substation Rating","MVA","Non-Coincident",13,13,13,13,13,13,13]
[null,null,null,null,"Coincident",13,13,13,13,13,13,13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7,7,7,7,7,7,8]
[null,null,null,null,"Coincident",7,7,7,7,7,7,8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,"Aldinga 11kV","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23,23,24,25,26,26,26]
[null,null,null,null,"Coincident",23,23,24,25,26,26,26]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23,24,25,25,26,26,27]
[null,null,null,null,"Coincident",23,24,25,25,26,26,27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20,21,22,23,23,24,24]
[null,null,null,null,"Coincident",20,21,22,23,23,24,24]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21,21,22,23,24,24,25]
[null,null,null,null,"Coincident",21,21,22,23,24,24,25]
[null,"Allendale East 11kV","Substation Rating","MVA","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",7,7,7,7,7,7,7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3,3,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,"Alma 11kV","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"American River 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Angaston 11kV","Substation Rating","MVA","Non-Coincident",29,29,29,29,29,29,29]
[null,null,null,null,"Coincident",29,29,29,29,29,29,29]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15,15,16,16,16,16,16]
[null,null,null,null,"Coincident",15,15,15,16,16,16,16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16,16,16,17,17,17,17]
[null,null,null,null,"Coincident",16,16,16,16,16,16,17]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14,14,15,15,15,15,15]
[null,null,null,null,"Coincident",14,14,14,15,15,15,15]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15,15,15,16,16,16,16]
[null,null,null,null,"Coincident",15,15,15,15,15,15,16]
[null,"Angle Vale 11kV","Substation Rating","MVA","Non-Coincident",29,29,29,29,29,29,29]
[null,null,null,null,"Coincident",29,29,29,29,29,29,29]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21,22,22,24,24,25,25]
[null,null,null,null,"Coincident",21,22,22,23,24,25,25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21,22,23,25,25,26,26]
[null,null,null,null,"Coincident",21,22,23,24,25,25,26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19,20,20,21,22,23,23]
[null,null,null,null,"Coincident",19,20,20,21,22,22,23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19,21,21,22,23,23,24]
[null,null,null,null,"Coincident",19,21,21,22,23,23,24]
[null,"Ardrossan 11kV","Substation Rating","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2,2,2,2,3,3,3]
[null,null,null,null,"Coincident",2,2,2,2,2,3,3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2,2,2,3,3,3,3]
[null,null,null,null,"Coincident",2,2,2,2,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,"Arno Bay 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,"Ascot Park 11kV","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",24,24,24,24,24,24,24]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22,23,23,24,24,24,25]
[null,null,null,null,"Coincident",22,23,23,24,24,24,25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22,23,23,24,24,25,25]
[null,null,null,null,"Coincident",22,23,23,24,24,25,25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20,20,21,22,22,22,23]
[null,null,null,null,"Coincident",20,20,21,22,22,22,23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20,20,21,22,22,22,23]
[null,null,null,null,"Coincident",20,20,21,22,22,22,23]
[null,"Athol Park 11kV","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident",26,26,26,26,26,26,26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18,18,19,19,20,20,20]
[null,null,null,null,"Coincident",18,18,18,19,19,19,19]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19,19,19,20,21,21,21]
[null,null,null,null,"Coincident",18,19,19,19,20,20,20]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16,17,17,17,18,18,18]
[null,null,null,null,"Coincident",16,16,17,17,17,17,17]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17,17,18,18,18,19,19]
[null,null,null,null,"Coincident",17,17,17,18,18,18,18]
[null,"Auburn 11kV","Substation Rating","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3,3,3,3,3,3,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,4]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3,3,3,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,4,4,4,4]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,"Balaklava 7.6kV","Substation Rating","MVA","Non-Coincident",5,5,5,5,5,5,5]
[null,null,null,null,"Coincident",5,5,5,5,5,5,5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,"Balhannah 33kV","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21,22,23,23,24,25,25]
[null,null,null,null,"Coincident",21,22,23,23,24,25,25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22,22,23,24,25,25,26]
[null,null,null,null,"Coincident",22,22,23,24,25,25,26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19,19,20,20,21,22,22]
[null,null,null,null,"Coincident",19,19,20,20,21,22,22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19,20,20,21,22,22,23]
[null,null,null,null,"Coincident",19,20,20,21,22,22,23]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Baroota Town 11kV","Substation Rating","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Barossa South TF1 11kV","Substation Rating","MVA","Non-Coincident",9,9,9,9,9,9,9]
[null,null,null,null,"Coincident",9,9,9,9,9,9,9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2,2,2,3,3,3,3]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2,2,2,3,3,3,3]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,"Barossa South TF2 11kV","Substation Rating","MVA","Non-Coincident",9,9,9,9,9,9,9]
[null,null,null,null,"Coincident",9,9,9,9,9,9,9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,4,4,4]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,"Beachport 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,"Belvedere Road 7.6kV","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Berri 11kV","Substation Rating","MVA","Non-Coincident",28,28,28,28,28,28,28]
[null,null,null,null,"Coincident",28,28,28,28,28,28,28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13,13,13,14,14,15,15]
[null,null,null,null,"Coincident",12,12,12,13,13,13,13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14,14,14,15,15,16,16]
[null,null,null,null,"Coincident",12,13,13,14,14,14,15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11,12,12,12,13,13,13]
[null,null,null,null,"Coincident",10,11,11,11,12,12,12]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12,13,13,13,14,14,14]
[null,null,null,null,"Coincident",11,12,12,12,13,13,13]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Binnies 11kV","Substation Rating","MVA","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,"Birdwood 11kV","Substation Rating","MVA","Non-Coincident",4,4,4,4,4,4,4]
[null,null,null,null,"Coincident",4,4,4,4,4,4,4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",2,2,3,3,3,3,3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",2,2,3,3,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2,3,3,3,3,3,3]
[null,null,null,null,"Coincident",2,2,2,2,3,3,3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",2,2,2,2,3,3,3]
[null,"Black Point 11kV","Substation Rating","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,1,1,1]
[null,null,null,null,"Coincident",0,0,0,0,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,1,1,1]
[null,null,null,null,"Coincident",0,0,0,0,1,1,1]
[null,"Blackpool 11kV","Substation Rating","MVA","Non-Coincident",35,35,35,35,35,35,35]
[null,null,null,null,"Coincident",35,35,35,35,35,35,35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16,16,17,18,18,18,19]
[null,null,null,null,"Coincident",15,15,15,16,16,16,17]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16,17,17,18,18,18,19]
[null,null,null,null,"Coincident",15,15,16,16,16,16,17]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14,14,15,15,15,16,16]
[null,null,null,null,"Coincident",13,13,13,14,14,14,14]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14,15,15,15,16,16,16]
[null,null,null,null,"Coincident",13,13,14,14,14,14,15]
[null,"Blackwood 11kV","Substation Rating","MVA","Non-Coincident",58,58,58,58,58,58,58]
[null,null,null,null,"Coincident",58,58,58,58,58,58,58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32,32,34,35,35,36,37]
[null,null,null,null,"Coincident",32,32,34,35,35,36,37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32,33,34,35,36,36,37]
[null,null,null,null,"Coincident",32,33,34,35,36,36,37]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28,29,30,31,32,32,33]
[null,null,null,null,"Coincident",28,29,30,31,32,32,33]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28,29,30,31,32,33,33]
[null,null,null,null,"Coincident",28,29,30,31,32,33,33]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Booleroo Centre 11kV","Substation Rating","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",0,0,0,0,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",0,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,1,1,1,1,1]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Boothby 33kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,null,null,"Coincident","                              -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  ","                         -  "]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,"Booyoolie 11kV","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1128157885500001E-2,2.1537288597784001E-2,2.2029243444825E-2,2.2806101529832E-2,2.3112887034194E-2,2.3414397150523E-2,2.3705216600368999E-2]
[null,null,null,null,"Coincident",2.1128157885500001E-2,2.1537288597784001E-2,2.1956057112446001E-2,2.2486482712864998E-2,2.277945655096E-2,2.3066913286863E-2,2.3343416290623E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1420927246218E-2,2.1835727214559002E-2,2.2334498997883E-2,2.3122121875832999E-2,2.3433158455772998E-2,2.3738846547506999E-2,2.4033695833976E-2]
[null,null,null,null,"Coincident",2.1420927246218E-2,2.1835727214559002E-2,2.2260298534700001E-2,2.2798074154215E-2,2.3095107681932001E-2,2.3386547657890999E-2,2.3666882117668001E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0391588896827E-2,2.0649699148926001E-2,2.1045293355266999E-2,2.1564863500469999E-2,2.1889239572474999E-2,2.2191257677620001E-2,2.2476087598227001E-2]
[null,null,null,null,"Coincident",2.0391588896827E-2,2.0649699148926001E-2,2.1045293355266999E-2,2.1564863500469999E-2,2.1889239572474999E-2,2.2191257677620001E-2,2.2476087598227001E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0674151743890999E-2,2.0935838586712999E-2,2.1336914476007E-2,2.1863684218074001E-2,2.2192555115219E-2,2.2498758234886E-2,2.2787534996207E-2]
[null,null,null,null,"Coincident",2.0674151743890999E-2,2.0935838586712999E-2,2.1336914476007E-2,2.1863684218074001E-2,2.2192555115219E-2,2.2498758234886E-2,2.2787534996207E-2]
[null,"Bordertown 11kV","Substation Rating","MVA","Non-Coincident",14.182050408719,14.182050408719,14.182050408719,14.182050408719,14.182050408719,14.182050408719,14.182050408719]
[null,null,null,null,"Coincident",14.182050408719,14.182050408719,14.182050408719,14.182050408719,14.182050408719,14.182050408719,14.182050408719]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.411581699156001,12.689281583007,13.052159160904999,13.55421761541,13.872103548328999,14.189313419786,14.502168978704001]
[null,null,null,null,"Coincident",11.326563642442,11.608333696659001,11.954124254571999,12.364900623405999,12.648658848890999,12.931618810371001,13.210399537866]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.461549557932001,12.740367435356999,13.104705924200999,13.608785618752,13.927951330492,14.246438259011001,14.560553344939001]
[null,null,null,null,"Coincident",11.372163320727999,11.655067754640999,12.002250432767999,12.414680548568001,12.699581157940001,12.98368028957,13.263583362014]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.340805429592001,11.558275818094,11.846958713547,12.260455323401001,12.545729035622999,12.820289153534,13.086701154347001]
[null,null,null,null,"Coincident",10.127860274432001,10.338314806489,10.619408028699,10.965864966172999,11.215621079338,11.455650062143,11.688235808424]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.386462443972,11.604808347772,11.894653453368999,12.309814761624001,12.596236958940001,12.871902430022001,13.139386980455001]
[null,null,null,null,"Coincident",10.168634085874,10.379935888052,10.662160765096999,11.010012505565999,11.260774113316,11.501769430195001,11.735291544780999]
[null,"Brinkworth Town 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.80927136931554999,0.81232874698648005,0.82594170240029996,0.85362381050726999,0.86287631009601995,0.87245845382667997,0.88230817065488998]
[null,null,null,null,"Coincident",0.78627538790675,0.79439341830823995,0.80701185058138003,0.82414484209754002,0.83304336330510997,0.84227145728689001,0.85176957026323996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.81725222128731001,0.82033975012821003,0.83408695344227002,0.86204205626454999,0.87138580192030002,0.88106244259424005,0.89100929511134996]
[null,null,null,null,"Coincident",0.79402945868924002,0.80222754727811996,0.81497041968828998,0.83227237290791001,0.84125864932741001,0.85057774869360003,0.86016952992086004]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.73810054950012005,0.74172317935111998,0.75527544081902998,0.78240926978191006,0.79403987563217004,0.80544504445218001,0.81695968333492996]
[null,null,null,null,"Coincident",0.70738143809183995,0.71474407610948998,0.72723990700829999,0.74449095805040999,0.75552282815958005,0.76635096658845003,0.77729449983155996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74537953087667996,0.74903788628734003,0.76272379710547,0.79012521377821998,0.80187051804381004,0.81338816206994002,0.8250163557279]
[null,null,null,null,"Coincident",0.71435747451055998,0.72179272120605997,0.73441178317474998,0.75183296019678003,0.76297362412424996,0.77390854721548996,0.78496000311863001]
[null,"Brukunga 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.55784041005027996,0.57245202459902,0.59024317050272002,0.61083229549796003,0.62521851802244,0.63962880529515997,0.65419776945746]
[null,null,null,null,"Coincident",0.55784041005027996,0.57245202459902,0.59024317050272002,0.61083229549796003,0.62521851802244,0.63962880529515997,0.65419776945746]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.56043241438281,0.57511192176888004,0.59298573419588996,0.61367052651860998,0.62812359459683997,0.64260083924012001,0.65723749806482001]
[null,null,null,null,"Coincident",0.56043241438281,0.57511192176888004,0.59298573419588996,0.61367052651860998,0.62812359459683997,0.64260083924012001,0.65723749806482001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.47501403934511999,0.48534981927004001,0.49605033133741,0.50873283901063004,0.52061023387288996,0.53188121158138002,0.54267365566065995]
[null,null,null,null,"Coincident",0.47501403934511999,0.48534981927004001,0.49605033133741,0.50873283901063004,0.52061023387288996,0.53188121158138002,0.54267365566065995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.47722119111436001,0.48760499621970999,0.49835522819466999,0.51109666511403995,0.52302924826742003,0.53435259655094003,0.54519518769971997]
[null,null,null,null,"Coincident",0.47722119111436001,0.48760499621970999,0.49835522819466999,0.51109666511403995,0.52302924826742003,0.53435259655094003,0.54519518769971997]
[null,"Bungama Napperby 11kV","Substation Rating","MVA","Non-Coincident",1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311]
[null,null,null,null,"Coincident",1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311,1.2961077844311]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.88371937051825,0.88667067695985002,0.90249983494366004,0.93427554986765005,0.94167922599889997,0.94853070697936004,0.95466461774615996]
[null,null,null,null,"Coincident",0.77284120414548996,0.78111151815803004,0.79324318737315003,0.80900712255582996,0.81571768274233003,0.82195235228902996,0.82756598452232]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.95023572444896998,0.95340917170854,0.97042976886410004,1.0045971985911999,1.0125581393456,1.0199253219719,1.0265209238515001]
[null,null,null,null,"Coincident",0.83101190944194003,0.83990471873106998,0.85294952217205999,0.86989998729505003,0.87711564221107996,0.88381958684674,0.88985574953586999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.8023208097458,0.81175766216536005,0.83220705024376995,0.86741452951671005,0.88407191173623001,0.89980712049712996,0.91517151081291004]
[null,null,null,null,"Coincident",0.69654580853708004,0.70906149530214002,0.72606774423627995,0.74743143485115004,0.76207254004476999,0.77592612774799996,0.78946541110782997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.86271040482250005,0.87285755627643002,0.89484614195586998,0.93270364026250996,0.95061480096448003,0.96753437746702997,0.98405522452492]
[null,null,null,null,"Coincident",0.74897386327399995,0.76243158874312,0.78071787488236,0.80368958140545999,0.81943270265473001,0.83432903104421996,0.84888739783028]
[null,"Burnside 11kV","Substation Rating","MVA","Non-Coincident",30.5,30.5,30.5,30.5,30.5,30.5,30.5]
[null,null,null,null,"Coincident",30.5,30.5,30.5,30.5,30.5,30.5,30.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.812080144399999,14.019810976624999,14.298377058791001,14.652241781678001,14.851504286677001,15.071406638871,15.312504240120999]
[null,null,null,null,"Coincident",13.812080144399999,14.019810976624999,14.298377058791001,14.652241781678001,14.851504286677001,15.071406638871,15.312504240120999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.041333096381001,14.252511845646,14.535701568567999,14.895439739297,15.098009604013001,15.321561896177,15.566661236211001]
[null,null,null,null,"Coincident",14.041333096381001,14.252511845646,14.535701568567999,14.895439739297,15.098009604013001,15.321561896177,15.566661236211001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.756517848214999,11.903912939786,12.074508432428001,12.380892996152999,12.578807600596001,12.801721904439001,13.019890632967]
[null,null,null,null,"Coincident",11.756517848214999,11.903912939786,12.074508432428001,12.380892996152999,12.578807600596001,12.801721904439001,13.019890632967]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.951652570395,12.101494126185001,12.274921163379,12.586391099107001,12.787590690809999,13.014204927007,13.235994820813]
[null,null,null,null,"Coincident",11.951652570395,12.101494126185001,12.274921163379,12.586391099107001,12.787590690809999,13.014204927007,13.235994820813]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Burra TF2 11kV","Substation Rating","MVA","Non-Coincident",3.7,3.7,3.7,3.7,3.7,3.7,3.7]
[null,null,null,null,"Coincident",3.7,3.7,3.7,3.7,3.7,3.7,3.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8147851158951001,1.8013600265819001,1.8020731391333,1.8231483708364,1.8139409373277999,1.8040559045430999,1.7933029271162]
[null,null,null,null,"Coincident",1.685929956861,1.6791802915259999,1.6807341277876999,1.6900947460369999,1.6810474035584,1.6713777722956,1.6609007012579]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8169835922413999,1.8035422394373,1.8042562158711,1.8253569786402,1.816138391015,1.8062413832527999,1.7954753793985001]
[null,null,null,null,"Coincident",1.6879723348258999,1.6812144927765,1.6827702113945,1.6921421693322001,1.6830838666753001,1.6734025213779999,1.6629127581528]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6335825332799001,1.6216399914538999,1.6226313845607001,1.6429495457993999,1.6400094868234001,1.6351373488231999,1.6289964444041001]
[null,null,null,null,"Coincident",1.5163122723167,1.5094821394864,1.5123295644778001,1.5234843996781,1.5203384259670001,1.5154027991279999,1.5092838306942]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6355614962589,1.6236044869371999,1.6245970810426,1.644939856213,1.6419962355755999,1.6371181953448,1.6309698516797]
[null,null,null,null,"Coincident",1.5181491711513,1.5113107641262,1.5141616385598,1.5253299870082,1.5221802021852999,1.5172385962038,1.5111122150977001]
[null,"Cadell 11kV","Substation Rating","MVA","Non-Coincident",2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002]
[null,null,null,null,"Coincident",2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002,2.6212765957447002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1762282253981999,1.2061244002169,1.2502139861651,1.3140340143485001,1.3518479704973001,1.389902625026,1.4277139284053999]
[null,null,null,null,"Coincident",0.85822866241856,0.88416311482064003,0.91527362242002996,0.95166711723175001,0.97856216291275999,1.0056113414062,1.0324662620600999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2426803977386001,1.2742655864054999,1.3208460569461,1.3882716604931999,1.4282219533466001,1.468426543072,1.5083740332850999]
[null,null,null,null,"Coincident",0.90671513617509003,0.93411478101462997,0.96698290738896997,1.0054324885427,1.0338469963248,1.0624243448043,1.0907964606563001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0490267688206001,1.0717871627011,1.1071185977972,1.1603312929536,1.1932364164759,1.2253706223992,1.2568639315873]
[null,null,null,null,"Coincident",0.76852225647545003,0.78837227485871997,0.81383879484979005,0.84455669645025999,0.86805221332487004,0.89097010667495002,0.91340575091215004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1082925695607,1.1323388343156,1.1696663536437999,1.2258853524347999,1.2606494833266,1.2945991428701,1.3278716975861]
[null,null,null,null,"Coincident",0.81194067845508,0.83291214318190998,0.85981741930790001,0.89227075902065001,0.91709367826738997,0.94130634057956997,0.96500950864014001]
[null,"Caloote 11kV","Substation Rating","MVA","Non-Coincident",3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001]
[null,null,null,null,"Coincident",3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001,3.9224681647940001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.7832892117276,1.8154974312573999,1.8576120956511,1.9095852098155,1.9417681289027999,1.9737030886772999,2.0049454683091001]
[null,null,null,null,"Coincident",1.7832892117276,1.8154974312573999,1.8576120956511,1.9095852098155,1.9417681289027999,1.9737030886772999,2.0049454683091001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8789477223024,1.9128836426942999,1.9572574056361001,2.0120184415005999,2.0459277042934998,2.0795757068359002,2.1124939781193999]
[null,null,null,null,"Coincident",1.8789477223024,1.9128836426942999,1.9572574056361001,2.0120184415005999,2.0459277042934998,2.0795757068359002,2.1124939781193999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5775668722756,1.5907727873466,1.6235985773593,1.6832487027245999,1.7104081686781001,1.7366492607885,1.7617202173412001]
[null,null,null,null,"Coincident",1.5616088670666,1.5825639415065,1.6142537870735001,1.6556690156456999,1.6823164402997,1.7080494551637999,1.7325643764122001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6621901046384,1.6761044063007999,1.7106910246528,1.7735408789856,1.8021572225133999,1.8298059291433999,1.8562217322565]
[null,null,null,null,"Coincident",1.6453760862824001,1.6674552247253001,1.7008449647387001,1.7444817729930999,1.7725586085,1.7996719838005,1.8255019249783]
[null,"Caltowie 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3480419603358003E-2,8.7213232056924994E-2,9.1303521544895003E-2,9.6270337314033005E-2,9.9064185414100003E-2,0.10158722085027,0.10380364147092]
[null,null,null,null,"Coincident",6.4737291817929005E-2,6.7611208304379999E-2,7.0411940651670002E-2,7.3445803394927997E-2,7.5545717685144995E-2,7.7437192335141999E-2,7.9092825851312998E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.9763860946164994E-2,9.3777636387306004E-2,9.8175795603230004E-2,0.10351645587020999,0.10652059257137,0.10923353296063,0.11161678011411]
[null,null,null,null,"Coincident",6.9609967084330995E-2,7.2700198794790005E-2,7.5711737909759005E-2,7.8973954783002995E-2,8.1231926355756004E-2,8.3265769360766004E-2,8.5046019836618997E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8447052143782003E-2,8.2669666895140007E-2,8.7330289586363005E-2,9.2812440107643002E-2,9.5969650915605997E-2,9.8659156784199994E-2,0.10088340125127999]
[null,null,null,null,"Coincident",6.2793573135596997E-2,6.5683459800561006E-2,6.8818048943493998E-2,7.2149689729716998E-2,7.4579437910797006E-2,7.6643929115108006E-2,7.8345053275213003E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.4351639746523002E-2,8.8892084142597999E-2,9.3903504654920006E-2,9.9798288119310005E-2,0.10319313727424,0.10608507806646,0.10847673795510999]
[null,null,null,null,"Coincident",6.7519947719930001E-2,7.0627351659399998E-2,7.3997876451757996E-2,7.7580284658112994E-2,8.0192916205689996E-2,8.2412798451955996E-2,8.4241963581760004E-2]
[null,"Cambrai 11kV","Substation Rating","MVA","Non-Coincident",1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001]
[null,null,null,null,"Coincident",1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001,1.2960921843687001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.79426894644558999,0.79866700527172996,0.80702668573486003,0.81917383476917005,0.82239143557700001,0.82517604697060998,0.82737356356781999]
[null,null,null,null,"Coincident",0.79426894644558999,0.79866700527172996,0.80702668573486003,0.81917383476917005,0.82239143557700001,0.82517604697060998,0.82737356356781999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.80265922113417998,0.80710373893596998,0.81555172703809997,0.82782719270563998,0.83107878269905,0.83389280938655996,0.83611353949093004]
[null,null,null,null,"Coincident",0.80265922113417998,0.80710373893596998,0.81555172703809997,0.82782719270563998,0.83107878269905,0.83389280938655996,0.83611353949093004]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.69948472520453997,0.69714387221514995,0.70314454730929998,0.72027297533393997,0.72303750211099005,0.72512655643195001,0.72647454990124005]
[null,null,null,null,"Coincident",0.68976417537621004,0.69089720891174999,0.69642712163521003,0.70576523878696995,0.70844585146407002,0.71046067944309998,0.71172260164259005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.70687374502106004,0.70450816438788,0.71057222772423001,0.72788159221474003,0.73067532212147002,0.73278644420632999,0.73414867722954003]
[null,null,null,null,"Coincident",0.69705051198504997,0.69819551434128002,0.70378384239993996,0.71322060292473999,0.71592953230337997,0.71796564395498996,0.71924089649293999]
[null,"Campbell Park 11kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.5016062819039,1.5196430358566999,1.5567565052089001,1.619470732758,1.6453567268833,1.6715566383894001,1.6976855432861]
[null,null,null,null,"Coincident",1.3074089632495001,1.3292668466326001,1.3584396611416001,1.3950551677489,1.4175272703671,1.4402583338273001,1.4629119336212]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5600378420039001,1.5787764548162999,1.6173341095991001,1.6824887172933001,1.7093820054341999,1.7366014263298,1.7637470775569]
[null,null,null,null,"Coincident",1.3582837806579,1.3809922133775001,1.4113002209692,1.4493405359306,1.4726870888162,1.4963026794101,1.5198377920171999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2890903976124,1.3125921138054,1.3526087374882001,1.4154722255376999,1.4403119610174999,1.4643736235194,1.4879782350032]
[null,null,null,null,"Coincident",1.2557866904677,1.2737625793676,1.3006711095076999,1.3357845129096999,1.3594209732994,1.3823119410961,1.4047564788456]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3392523901068001,1.3636686216149001,1.4052424003121999,1.4705520766364999,1.4963583933793001,1.5213563602211,1.5458794909539999]
[null,null,null,null,"Coincident",1.3046527456787,1.3233281250144999,1.3512837388109999,1.3877634996702,1.4123197186362,1.4361014358766999,1.45941935127]
[null,"Campbelltown 11kV","Substation Rating","MVA","Non-Coincident",73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995]
[null,null,null,null,"Coincident",73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995,73.859002770082995]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.459696876171002,53.502679933976999,54.870737122990001,56.594565426382999,57.803086265315997,59.092606997045003,60.497547858544003]
[null,null,null,null,"Coincident",52.459696876171002,53.502679933976999,54.870737122990001,56.594565426382999,57.803086265315997,59.092606997045003,60.497547858544003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.499235453867001,54.562886208762002,55.958052746649997,57.716040340497003,58.948509164431997,60.263582970752999,61.69636406603]
[null,null,null,null,"Coincident",53.499235453867001,54.562886208762002,55.958052746649997,57.716040340497003,58.948509164431997,60.263582970752999,61.69636406603]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.274789896359003,47.311499176151997,48.503465897334998,50.165100278465999,51.480055621527001,53.002798701945999,54.627292615138003]
[null,null,null,null,"Coincident",46.274789896359003,47.311499176151997,48.503465897334998,50.165100278465999,51.480055621527001,53.002798701945999,54.627292615138003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.191768684581,48.249021340611002,49.464608011274997,51.159169251386999,52.500181679952,54.053099356685998,55.709784155310999]
[null,null,null,null,"Coincident",47.191768684581,48.249021340611002,49.464608011274997,51.159169251386999,52.500181679952,54.053099356685998,55.709784155310999]
[null,"Cape Jervis 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.46788031940824998,0.47704300068229,0.49196921371690999,0.51246684434611001,0.5226326435609,0.53243532043820996,0.54203075700245995]
[null,null,null,null,"Coincident",0.42422239529530997,0.43554679419817,0.45266939992962002,0.46887665245539001,0.47527240394807002,0.48143518440534,0.49130128123622002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.47293268371232,0.48219430739080998,0.49728169981853998,0.51800067230166003,0.52827624600138001,0.53818477621914995,0.54788382825763005]
[null,null,null,null,"Coincident",0.42880332336188998,0.44025000778607998,0.45755751046318999,0.47393977557387001,0.48040459102415001,0.48663391972185999,0.49660655472796]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.42953014000064998,0.43889771557813001,0.45438432648449001,0.47576089035512997,0.48828569828511997,0.50025214578780997,0.51183342441131996]
[null,null,null,null,"Coincident",0.39838759158429998,0.40994406669112998,0.42879413344891998,0.44692078594134999,0.45514317360854001,0.46288906118188,0.47457562455650998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.43416838327962998,0.44363711379460002,0.45929095550098997,0.48089835230853001,0.49355840827071001,0.50565407439983001,0.51736041243764996]
[null,null,null,null,"Coincident",0.40268954480483998,0.41437081148740001,0.43342442902616002,0.45174682057450999,0.46005799696867999,0.46788752782484,0.47970028752186999]
[null,"Cape Jervis 33kV","Substation Rating","MVA","Non-Coincident",54.4,54.4,54.4,54.4,54.4,54.4,54.4]
[null,null,null,null,"Coincident",54.4,54.4,54.4,54.4,54.4,54.4,54.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.179708600071001,14.176568372043,14.173344063404,14.170262326234999,14.167293485027001,14.164448291776001,14.162173814487]
[null,null,null,null,"Coincident",7.1139397934256001,7.1123643454553998,7.1107467143614,7.1092006111729997,7.1077111477286996,7.1062837182900003,7.1051426162437998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.279693071526999,14.27653070101,14.273283657008999,14.270180189785,14.267190414577,14.264325159197,14.262034644031001]
[null,null,null,null,"Coincident",7.1641018616508996,7.1625153048253001,7.1608862674328,7.1593292623059002,7.1578292963034,7.1563918017228998,7.1552426534968996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.95,12.95,12.95,12.95,12.95,12.95,12.95]
[null,null,null,null,"Coincident",6.4969967242060997,6.4969967242060997,6.4969967242060997,6.4969967242060997,6.4969967242060997,6.4969967242060997,6.4969967242060997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.041313505931001,13.041313505931001,13.041313505931001,13.041313505931001,13.041313505931001,13.041313505931001,13.041313505931001]
[null,null,null,null,"Coincident",6.5428085812647003,6.5428085812647003,6.5428085812647003,6.5428085812647003,6.5428085812647003,6.5428085812647003,6.5428085812647003]
[null,"Caralue 11kV","Substation Rating","MVA","Non-Coincident",3.2,3.2,3.2,3.2,3.2,3.2,3.2]
[null,null,null,null,"Coincident",3.2,3.2,3.2,3.2,3.2,3.2,3.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.179624279934,2.1494646328522999,2.1235878751068,2.1090012212795002,2.0776341459603,2.0456026008418,2.0127699902998999]
[null,null,null,null,"Coincident",1.9391998239693,1.9135981334965,1.8973874277339999,1.8897689525470001,1.8614588873713001,1.8325598091818001,1.8029489439613]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3977446141730998,2.3645668174210002,2.3361005092193001,2.3200541332567002,2.2855480779694002,2.2503110577643,2.2141928075589998]
[null,null,null,null,"Coincident",2.1332602946910999,2.1050965804169999,2.0872636296686,2.0788827550307998,2.0477396323711998,2.0159485527243,1.9833744557769999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9749744565278999,1.9461307291809,1.9218169724448999,1.9092410799427,1.8855079589243,1.8594441182771,1.8320438543655999]
[null,null,null,null,"Coincident",1.7592316279039,1.7337260711716,1.7192759968266,1.7140264193071999,1.6925115275781999,1.6689108084149999,1.6441168025631001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1726149822540002,2.1408847925439001,2.1141378986867001,2.1003035058544,2.0741953533515001,2.0455232404045001,2.0153809650474002]
[null,null,null,null,"Coincident",1.9352822409454,1.9072242807504001,1.8913281521129,1.8855532365279,1.8618852969465001,1.8359227960764,1.8086475933991999]
[null,"Cavan 11kV","Substation Rating","MVA","Non-Coincident",56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001]
[null,null,null,null,"Coincident",56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001,56.652712516019001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.308482377221999,40.105354313183,43.097819075532001,46.287142039606998,48.870582138743998,50.001849424979,51.201924170961]
[null,null,null,null,"Coincident",36.942512264116999,38.758587581878999,41.423275996488996,43.820782217944,46.211219676151003,47.244162220219998,48.339743822825]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.272035838066003,42.161008893403,45.306856514480003,48.659652572638997,51.375510414082001,52.564762346462999,53.826348558691997]
[null,null,null,null,"Coincident",38.836051065633001,40.745211798271001,43.546482448299997,46.066876117817998,48.579838704997002,49.665726126582001,50.817463256994998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.678769021599003,36.380777703056999,39.108326486461998,41.915397879586997,44.472546694169999,45.730705842254999,46.969695644406002]
[null,null,null,null,"Coincident",33.713400766150002,35.463999381020997,37.886513103744001,40.053720562987003,42.444940700654001,43.610498354065001,44.757531880773001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.456276578793997,38.245524034264001,41.11287704694,44.063828709048998,46.752047670324004,48.074695479829003,49.377191392455003]
[null,null,null,null,"Coincident",35.441427058064001,37.281754990190997,39.828437954527999,42.106728584987998,44.620513968929998,45.845813867977,47.051640160969001]
[null,"CBD 33kV","Substation Rating","MVA","Non-Coincident",82.2,82.2,82.2,82.2,82.2,82.2,82.2]
[null,null,null,null,"Coincident",82.2,82.2,82.2,82.2,82.2,82.2,82.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.987322777563001,22.808689519603998,22.629777337537,22.465567053272,22.335810907426001,22.222980114342999,22.127240879311]
[null,null,null,null,"Coincident",22.951716554278001,22.770879910411999,22.604270923017001,22.456303107743,22.327393914222998,22.215492034267001,22.120746190392001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.373508620734,23.191874333207998,23.009956435662001,22.842987427046999,22.711051384608002,22.596325039991999,22.498977390722999]
[null,null,null,null,"Coincident",23.337304214724998,23.153429524520998,22.984021514687001,22.833567847708998,22.702492986351,22.588711160553999,22.492373591364]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.121453863896001,21.958667112320001,21.788717207845,21.623042313532,21.496576016641001,21.384263221775999,21.284465270264999]
[null,null,null,null,"Coincident",22.034263797282001,21.864691923721999,21.710351956204999,21.571332480873,21.445907856656,21.334676180751998,21.235974290973001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.493093153745999,22.327571593097002,22.154766538945999,21.986308314910001,21.857717390720001,21.743517746664001,21.642043194688]
[null,null,null,null,"Coincident",22.404438298487001,22.232017626150999,22.075084755100001,21.933729759715,21.806198008247001,21.693097645895001,21.592737569432]
[null,"Ceduna 11kV","Substation Rating","MVA","Non-Coincident",12.79043348281,12.79043348281,12.79043348281,12.79043348281,12.79043348281,12.79043348281,12.79043348281]
[null,null,null,null,"Coincident",12.79043348281,12.79043348281,12.79043348281,12.79043348281,12.79043348281,12.79043348281,12.79043348281]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.7865174399203001,6.8775896804716004,7.0053884022341997,7.1695986973746999,7.2589290550754999,7.3474165792935002,7.4337973050911996]
[null,null,null,null,"Coincident",6.7865174399203001,6.8775896804716004,7.0053884022341997,7.1695986973746999,7.2589290550754999,7.3474165792935002,7.4337973050911996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.9450054132433996,7.0382044964587998,7.1689877475598003,7.3370329045578,7.4284494261083003,7.5190034311835996,7.6074014370203002]
[null,null,null,null,"Coincident",6.9450054132433996,7.0382044964587998,7.1689877475598003,7.3370329045578,7.4284494261083003,7.5190034311835996,7.6074014370203002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.0546225341242002,6.1242851155449998,6.2352229144263998,6.3835626971902002,6.4748223457157001,6.5602577715940003,6.6418739800141999]
[null,null,null,null,"Coincident",6.0546225341242002,6.1242851155449998,6.2352229144263998,6.3835626971902002,6.4748223457157001,6.5602577715940003,6.6418739800141999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.1960183034809004,6.2673077401250996,6.3808363091717997,6.5326403240313002,6.6260311918264003,6.7134618218159998,6.7969840427937998]
[null,null,null,null,"Coincident",6.1960183034809004,6.2673077401250996,6.3808363091717997,6.5326403240313002,6.6260311918264003,6.7134618218159998,6.7969840427937998]
[null,"Chain of Ponds 11kV","Substation Rating","MVA","Non-Coincident",0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005]
[null,null,null,null,"Coincident",0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005,0.61750000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.44026294354290002,0.43623487432445002,0.43577799753466001,0.44047816626431002,0.43762225437972002,0.43465165651520998,0.43171781133907]
[null,null,null,null,"Coincident",0.38447643370492002,0.38267514397497998,0.38272090808523002,0.38457899122297001,0.38227278950702998,0.37985743537327998,0.37746360960226]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.45387925419240999,0.44972660614533,0.44925559921720998,0.45410113325290002,0.45115689464453002,0.44809442308515002,0.44506984088945001]
[null,null,null,null,"Coincident",0.39636739712923003,0.39451039769014001,0.39455757717807,0.39647312651319,0.39409559933268001,0.39160554390349001,0.38913768265931997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.41053661485546,0.40780700440313,0.40874761434426998,0.41506126934602,0.41487113260200997,0.4142445964243,0.41354877798848999]
[null,null,null,null,"Coincident",0.35843467443093002,0.35761274685973998,0.35904292154624001,0.36248973344063001,0.36255743575923999,0.36223558428239,0.36184302717255001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.42323355917671002,0.42041952821064998,0.42138922903338,0.42789815072539999,0.42770213349336,0.42705622000635002,0.42633888152186]
[null,null,null,null,"Coincident",0.36952022670416002,0.36867287882152999,0.37014728549053,0.37370069927407001,0.37377049546821001,0.37343868987244999,0.37303399188261999]
[null,"Cheltenham 11kV","Substation Rating","MVA","Non-Coincident",30.7,30.7,30.7,30.7,30.7,30.7,30.7]
[null,null,null,null,"Coincident",30.7,30.7,30.7,30.7,30.7,30.7,30.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.574311576018999,11.678236325915,11.955398266566,12.478433654095999,12.744084954838,13.099127199667,13.51272420467]
[null,null,null,null,"Coincident",10.954880358597,11.077042839106999,11.278054472826,11.594734922314,11.8274077037,12.147458789056,12.521085068879]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.650105012644,11.7547103053,12.033687218346,12.560147660508999,12.827538557157,13.184905767207001,13.601211178510001]
[null,null,null,null,"Coincident",11.026617500347999,11.149579951911001,11.351907893941,11.670662099559999,11.904858519703,12.227005433524001,12.603078374608]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.525658828062999,10.664148454756999,10.913638973773001,11.355665006937,11.630224072419001,11.975654922319,12.355556977491]
[null,null,null,null,"Coincident",10.043131980766001,10.202882969038001,10.376860503093001,10.650324339511,10.894392161032,11.208910697081,11.555578768873]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.594585247582,10.733981762316001,10.985106049675,11.430026654314,11.706383647473,12.054076523158001,12.436466335995]
[null,null,null,null,"Coincident",10.108898612527,10.269695717134001,10.444812528901,10.720067120977999,10.965733200748,11.282311335813,11.631249535237]
[null,"Cheltenham 33kV","Substation Rating","MVA","Non-Coincident",33.1,33.1,33.1,33.1,33.1,33.1,33.1]
[null,null,null,null,"Coincident",33.1,33.1,33.1,33.1,33.1,33.1,33.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Clare 11kV","Substation Rating","MVA","Non-Coincident",13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999]
[null,null,null,null,"Coincident",13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999,13.154856361148999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.6670642002998992,9.7673072323040007,9.9472694828110999,10.24602178804,10.380181586808,10.513021959448,10.642714749759]
[null,null,null,null,"Coincident",9.6106834798410006,9.7435452964160998,9.9283217171503004,10.164585321483999,10.294544177540001,10.423115612071999,10.548429045563999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9933208138049991,10.096946977592999,10.282982827405,10.591817812685999,10.730505410247,10.867829051976001,11.001898882688]
[null,null,null,null,"Coincident",9.9350372837087999,10.072383093091,10.263395587988001,10.507632922695,10.641977798685,10.774888428648,10.904431102330999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6721254088652007,8.7452585004084007,8.8902297454534995,9.1458591932274,9.2765769935876996,9.3987597455138996,9.5152738313539]
[null,null,null,null,"Coincident",8.6142698253371002,8.7114718310126005,8.8671674015362996,9.0757734877490002,9.2029490594954009,9.3215846408124001,9.4344682354211002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.9648035383535998,9.0404048202685008,9.1902687428095007,9.4545255045449998,9.5896549386740002,9.7159612724907998,9.8364076267304004]
[null,null,null,null,"Coincident",8.9049953695976001,9.0054778745580997,9.1664280610152993,9.3820744558300007,9.5135421136222007,9.6361815623181997,9.7528748988023999]
[null,"Clarence Gardens 11kV","Substation Rating","MVA","Non-Coincident",37,37,37,37,37,37,37]
[null,null,null,null,"Coincident",37,37,37,37,37,37,37]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.611170325526,22.249166732595,23.186891737562998,24.082951940882001,24.478686824461999,24.864702743795998,25.446944613002]
[null,null,null,null,"Coincident",21.611170325526,22.249166732595,23.186891737562998,24.082951940882001,24.478686824461999,24.864702743795998,25.446944613002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.827268639850001,22.471644615727001,23.418746289788999,24.323766539998001,24.723458527241,25.113334366617,25.701398293794998]
[null,null,null,null,"Coincident",21.827268639850001,22.471644615727001,23.418746289788999,24.323766539998001,24.723458527241,25.113334366617,25.701398293794998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.036503915240001,19.509420204201,20.323719821648002,21.097837071977001,21.400500377048999,21.678931515024999,22.141748147438999]
[null,null,null,null,"Coincident",19.036503915240001,19.509420204201,20.323719821648002,21.097837071977001,21.400500377048999,21.678931515024999,22.141748147438999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.226857160563998,19.704502319425,20.526944428557002,21.308802371793998,21.614492122405998,21.895707399262999,22.363151911269]
[null,null,null,null,"Coincident",19.226857160563998,19.704502319425,20.526944428557002,21.308802371793998,21.614492122405998,21.895707399262999,22.363151911269]
[null,"Clarendon 11kV","Substation Rating","MVA","Non-Coincident",8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993]
[null,null,null,null,"Coincident",8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2272632871840998,3.3098694334042,3.4362110761592999,3.5555065158537,3.6003665993471001,3.6435264449693001,3.7153357997043002]
[null,null,null,null,"Coincident",3.2272632871840998,3.3098694334042,3.4362110761592999,3.5555065158537,3.6003665993471001,3.6435264449693001,3.7153357997043002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2932711793939999,3.3775668864309001,3.5064926212772001,3.6282280355952001,3.6740056517756998,3.7180482547635001,3.7913263412768998]
[null,null,null,null,"Coincident",3.2932711793939999,3.3775668864309001,3.5064926212772001,3.6282280355952001,3.6740056517756998,3.7180482547635001,3.7913263412768998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9169828155541002,2.9894973369371001,3.1142829426699001,3.2329886645536998,3.2795159514221002,3.3224025481549999,3.3938781399261]
[null,null,null,null,"Coincident",2.9169828155541002,2.9894973369371001,3.1142829426699001,3.2329886645536998,3.2795159514221002,3.3224025481549999,3.3938781399261]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9766444762658,3.0506421523483001,3.1779800242211,3.2991136591064998,3.3465925783219999,3.3903563436036999,3.4632938406293001]
[null,null,null,null,"Coincident",2.9766444762658,3.0506421523483001,3.1779800242211,3.2991136591064998,3.3465925783219999,3.3903563436036999,3.4632938406293001]
[null,"Clearview 11kV","Substation Rating","MVA","Non-Coincident",26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002]
[null,null,null,null,"Coincident",26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002,26.597262247839002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.906435083902,25.097501042428998,25.797367224045999,27.114642098752,27.55177244835,27.986430673569998,28.431711211511999]
[null,null,null,null,"Coincident",24.558508908791001,25.009636474188,25.594527353703,26.319099646942998,26.770988411438001,27.221830065353,27.683942753894001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.123745318516001,25.316478339717001,26.022450898405001,27.351219080408001,27.792163420186,28.230614066143001,28.679779705179001]
[null,null,null,null,"Coincident",24.772783465337,25.227847147514002,25.817841237256999,26.548735469968001,27.004566992754,27.459342268854002,27.925486920076001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.335620869456001,21.381091188540999,21.826617359856002,22.839788816274002,23.14141111444,23.484543056069,23.813308317166001]
[null,null,null,null,"Coincident",21.082761535381,21.380298850519999,21.719478904763999,22.233117949259,22.559381751172001,22.927873969614001,23.283877158629998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.521775522306999,21.567642572825001,22.017055988399999,23.039067430395001,23.343321402349002,23.689447192052999,24.021080951020998]
[null,null,null,null,"Coincident",21.266709974413999,21.566843321604999,21.908982743454001,22.427103321372002,22.756213795766001,23.127921132314999,23.487030471861001]
[null,"Cleve 11kV","Substation Rating","MVA","Non-Coincident",7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999]
[null,null,null,null,"Coincident",7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999,7.1114450017294999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2832738536486001,2.2875300083250001,2.2961325127468002,2.3169350370319002,2.3192007608787,2.3203023265697,2.3198968236548998]
[null,null,null,null,"Coincident",2.1498951679432001,2.1552893807775,2.1712062668573999,2.1971721704165001,2.1990802258269002,2.1998841974808001,2.199258627241]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2991384621836999,2.3034241894091001,2.3120864656207001,2.3330335296875,2.3353149962020998,2.3364242157751001,2.3360158953512]
[null,null,null,null,"Coincident",2.1648330367303998,2.1702647295519002,2.1862922090966999,2.2124385285505999,2.2143598414824002,2.2151693992799002,2.2145394824625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0426138390166999,2.0470831290879001,2.056056671741,2.0775597183093999,2.0869058079444001,2.0933950242639998,2.0978885794772002]
[null,null,null,null,"Coincident",1.9256003907271999,1.9300221937057001,1.9466461297354001,1.9739157475158999,1.9825514524622001,1.9884722653174001,1.9924965372987999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0568062973118999,2.0613066408362002,2.0703425333213001,2.0919949870296,2.101406015022,2.1079403196154001,2.1124650968803]
[null,null,null,null,"Coincident",1.9389798179672,1.9434323444496,1.9601717866579,1.9876308787804,1.9963265861999999,2.0022885379567001,2.0063407713232002]
[null,"Cleve 33kV","Substation Rating","MVA","Non-Coincident",17.7,17.7,17.7,17.7,17.7,17.7,17.7]
[null,null,null,null,"Coincident",17.7,17.7,17.7,17.7,17.7,17.7,17.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3112667340569999,2.3137619535793998,2.3206449055457998,2.3398907737911001,2.3404465274063999,2.3398748309073998,2.3379377141144002]
[null,null,null,null,"Coincident",2.0891583508598002,2.092760237837,2.1065648729437001,2.1301384322105998,2.1304113258522999,2.1296580733059001,2.1276617265240998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3330695785582001,2.3355883362047001,2.3425362170385,2.3619636370997998,2.3625246332989001,2.3619475438222999,2.3599921536488999]
[null,null,null,null,"Coincident",2.1088659830387999,2.1125018476527,2.1264367058567002,2.1502326412947999,2.1505081092207998,2.1497477510262999,2.1477325721306002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0503749467896002,2.0522293865441998,2.0586002737113001,2.0775502302988,2.0843697133532002,2.0888618328542998,2.0915671326518002]
[null,null,null,null,"Coincident",1.8555608145178,1.8574397553402999,1.871052468634,1.8949102235635999,1.9008961195967,1.9047591809946001,1.9069924592178999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0697167239523999,2.0715886571711999,2.0780196427509998,2.0971483597346001,2.1040321729358999,2.1085666678934998,2.1112974875628998]
[null,null,null,null,"Coincident",1.8730648538851999,1.8749615192974001,1.8887026452346001,1.912785457235,1.9188278199486,1.9227273227168,1.9249816680966001]
[null,"Coffin Bay 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4704514288118,1.4873083154297,1.5145014526274001,1.5520266258143001,1.5766312703454,1.6044681698615,1.6353495253889001]
[null,null,null,null,"Coincident",1.2337819929584,1.3539284249428001,1.4515103053687,1.4949269144056001,1.5242120838812001,1.5548377919731,1.5864574673255001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4871042635931999,1.504152054135,1.5316531531002,1.5696032981678001,1.5944865898356,1.6226387417153001,1.6538698280133]
[null,null,null,null,"Coincident",1.247754550829,1.3692616388964001,1.4679486322832,1.5118569336011001,1.5414737570704,1.5724463007305001,1.6044240683116999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.275773743629,1.2876001959173,1.3085176100719,1.3383886506322999,1.3601399672514001,1.3833270984093999,1.4083901760121]
[null,null,null,null,"Coincident",1.0673998146573001,1.1749878478147,1.2612012534573001,1.2966134566533001,1.3215336290690001,1.3464096404468,1.371534621943]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2902218572863,1.3021822439244,1.3233365474009999,1.3535458769341,1.3755435268049001,1.3989932517871999,1.4243401682725001]
[null,null,null,null,"Coincident",1.0794880974872001,1.1882945630970001,1.2754843339374999,1.3112975796688,1.3364999725685001,1.3616577043074001,1.3870672257465999]
[null,"Collinsfield 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.60122870717119004,0.60776424519445005,0.62235687054774003,0.64781801434698005,0.65954396397991999,0.67167643931444998,0.68411235521243996]
[null,null,null,null,"Coincident",0.56245608143006998,0.57227841310607996,0.58551551629304999,0.60222453843924995,0.61309985807625,0.62436111223101998,0.63591293073176003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.60186409624006998,0.60840654113481996,0.62301458823115996,0.64850263981484002,0.66024098163752998,0.67238627878530999,0.68483533717788003]
[null,null,null,null,"Coincident",0.56305049490634995,0.57288320699517004,0.58613429938553996,0.60286097992012,0.61374779278614,0.62502094803230002,0.63658497469793995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.55629150536562,0.56206336122918998,0.57547458093222004,0.59942053125921002,0.61167261526473005,0.62386829879417005,0.63620297157909]
[null,null,null,null,"Coincident",0.51334455716287997,0.52150970164249,0.53353988074008996,0.54919358670605001,0.56039302140501002,0.57154853528689997,0.58283961895822001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.55687940400951996,0.56265735967185004,0.57608275258767006,0.60005400941598996,0.61231904163930995,0.62452761378153998,0.63687532206553998]
[null,null,null,null,"Coincident",0.51388706871681,0.52206084226466998,0.53410373506705,0.54977398414472001,0.56098525460316995,0.57215255782828001,0.58345557411534998]
[null,"Coomandook 11kV","Substation Rating","MVA","Non-Coincident",0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002]
[null,null,null,null,"Coincident",0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.36249053867644998,0.36677982337746001,0.37566929495557999,0.39073536397264003,0.39691454823594002,0.40317014723466998,0.40941975874233999]
[null,null,null,null,"Coincident",0.33416984123818999,0.33969661650195998,0.34708876695738,0.35638235465070001,0.36206251529275002,0.36780943259011001,0.37354671836087999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.37689237628092997,0.38135207531034998,0.39059472776464998,0.40625937538217,0.41268406014490999,0.41918819561918003,0.42568610571790999]
[null,null,null,null,"Coincident",0.34744649061888,0.35319284601326001,0.36087868841109,0.37054151261251,0.37644734742369002,0.38242259114839,0.38838782068361]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.29251877891382,0.29670602274338997,0.3029740063418,0.31140388961830001,0.31686863142385002,0.32216219717425998,0.32735521170068999]
[null,null,null,null,"Coincident",0.29251877891382,0.29670602274338997,0.3029740063418,0.31115320585443001,0.31665900439771999,0.32199115037352,0.32721930641752001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.30414062141916998,0.30849422546840999,0.31501123758553001,0.32377604218278,0.32945789951449,0.33496177992460002,0.34036111418606002]
[null,null,null,null,"Coincident",0.30414062141916998,0.30849422546840999,0.31501123758553001,0.32351539869175999,0.32923994395542999,0.33478393739271001,0.3402198093528]
[null,"Coonalpyn 11kV","Substation Rating","MVA","Non-Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,null,null,"Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.42487402526630003,0.43402251897944999,0.44876238793526002,0.471158407419,0.48308498856805998,0.49525258767024,0.50757930227708004]
[null,null,null,null,"Coincident",0.38151390702003002,0.39154137613098,0.40386007784988998,0.41858150417347001,0.42922964052652002,0.44008935550964001,0.45108631050781001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.42775987202308002,0.43697050450995001,0.45181049020740999,0.47435862885199997,0.48636621821404002,0.49861646258121001,0.51102690320388999]
[null,null,null,null,"Coincident",0.38410524140567998,0.39420081950303998,0.40660319281231999,0.42142461061074998,0.43214507167167998,0.44307854845569999,0.45415019742203]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.38362352528040999,0.39215827654344998,0.40691124490686997,0.42910744458194999,0.4399907545899,0.45076210928386001,0.46155989831092997]
[null,null,null,null,"Coincident",0.38362352528040999,0.39215827654344998,0.40354299014806999,0.41763406158325,0.42828785604845998,0.43883006599326002,0.44939407766842998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.38622918870161999,0.39482191005175998,0.40967508413115999,0.43202204574281,0.44297927781475999,0.45382379414524998,0.46469492435721999]
[null,null,null,null,"Coincident",0.38622918870161999,0.39482191005175998,0.40628395137442003,0.42047073276216002,0.43119689036650999,0.44181070554148999,0.45244647052944997]
[null,"Coonawarra 11kV","Substation Rating","MVA","Non-Coincident",12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999]
[null,null,null,null,"Coincident",12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999,12.448329621380999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2983899514805999,3.3477846015319002,3.4307585590729999,3.5615184587739002,3.6254252641248002,3.6891862648739,3.7517599647436]
[null,null,null,null,"Coincident",2.9756828971840998,3.0339737255689001,3.1069880883534999,3.1964365595438999,3.2529140988788998,3.3092355235066999,3.3644658145342001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5215543529186002,3.5742909751669001,3.6628788333814,3.8024857630509001,3.8707164125117002,3.9387913924375,4.0055987403847997]
[null,null,null,null,"Coincident",3.1770133955144999,3.2392480989464998,3.3172025103023999,3.4127029386070999,3.4730016684156002,3.5331337210164002,3.5921008154601002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9731791648608001,3.0062588388183,3.0651703340248,3.1633911193188999,3.2171294490179001,3.2679886272137999,3.3165666760130001]
[null,null,null,null,"Coincident",2.6425355240593,2.6798322703033,2.7353518338384002,2.8073660604485999,2.8543543000696001,2.898769168671,2.9411416863805999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1743402642015002,3.2096580621367998,3.2725554258303,3.3774216906103001,3.4347958797309999,3.4890961180278999,3.5409608889378998]
[null,null,null,null,"Coincident",2.8213257420688,2.8611459334400999,2.9204218721602002,2.9973084795418998,3.0474758770319998,3.0948957928571001,3.1401351752162001]
[null,"Copley Nepabunna 33kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.23086749225605999,0.23086749225605999,0.23086749225605999,0.23086749225605999,0.23086749225605999,0.23086749225605999,0.23086749225605999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.26262567385326002,0.26262567385326002,0.26262567385326002,0.26262567385326002,0.26262567385326002,0.26262567385326002,0.26262567385326002]
[null,null,null,null,"Coincident",0.23319896432522999,0.23319896432522999,0.23319896432522999,0.23319896432522999,0.23319896432522999,0.23319896432522999,0.23319896432522999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.23,0.23,0.23,0.23,0.23,0.23,0.23]
[null,null,null,null,"Coincident",0.20422893545727999,0.20422893545727999,0.20422893545727999,0.20422893545727999,0.20422893545727999,0.20422893545727999,0.20422893545727999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.23232271148558001,0.23232271148558001,0.23232271148558001,0.23232271148558001,0.23232271148558001,0.23232271148558001,0.23232271148558001]
[null,null,null,null,"Coincident",0.20629139151847001,0.20629139151847001,0.20629139151847001,0.20629139151847001,0.20629139151847001,0.20629139151847001,0.20629139151847001]
[null,"Cordola 11kV","Substation Rating","MVA","Non-Coincident",2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315]
[null,null,null,null,"Coincident",2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315,2.8414328657315]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8795678944800001,1.8962978135193,1.934415766846,2.0014039322142998,2.0273353703096002,2.0528452548243998,2.0773626741218001]
[null,null,null,null,"Coincident",1.3628300582196999,1.3813988870358,1.4073064704342999,1.4404078270583001,1.4583388015814001,1.4759589144431999,1.4928606282646]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.927419151716,1.9445749918737001,1.9836633767528999,2.0523569702370001,2.0789485876843998,2.1051079193671001,2.1302495190099]
[null,null,null,null,"Coincident",1.397525868824,1.4165674349149999,1.4431345903573001,1.4770786627646,1.4954661356547001,1.5135348327659,1.5308668413683999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5024496233411999,1.5144003898067999,1.5435606582125001,1.5965607924073,1.6206094639905,1.6430105573963001,1.6639985045706001]
[null,null,null,null,"Coincident",1.0938104432675999,1.1069697987028999,1.1275614272836001,1.1547940364835001,1.1715747094119,1.1871573637104,1.2017127738222999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5406999592944,1.5529549761156001,1.5828576255275,1.6372070714775999,1.6618679897232,1.6848393846786001,1.7063616566102]
[null,null,null,null,"Coincident",1.1216573782157999,1.1351517530477,1.1562676166501999,1.1841935312592999,1.2014014174314001,1.2173807850389999,1.232306756212]
[null,"Coromandel Place 11kV","Substation Rating","MVA","Non-Coincident",92.038780642435,92.038780642435,92.038780642435,92.038780642435,92.038780642435,92.038780642435,92.038780642435]
[null,null,null,null,"Coincident",92.038780642435,92.038780642435,92.038780642435,92.038780642435,92.038780642435,92.038780642435,92.038780642435]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.382859681885002,48.725620150665002,48.06755813649,47.461322523353999,46.910797220745003,46.396056901319,45.920486199952997]
[null,null,null,null,"Coincident",49.346590657694001,48.684531379695997,48.052548156603997,47.461322523353999,46.910797220745003,46.396056901319,45.920486199952997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.263901027911999,49.594935662971999,48.925133141129997,48.308081656980001,47.747734412977998,47.223810593309999,46.739755218241001]
[null,null,null,null,"Coincident",50.226984926778002,49.553113825788003,48.909855367661997,48.308081656980001,47.747734412977998,47.223810593309999,46.739755218241001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.949015102483997,46.308222393694997,45.652529724529998,45.007929599782003,44.446245327489002,43.914482074883999,43.412421471568997]
[null,null,null,null,"Coincident",46.802117616411998,46.147654989552997,45.525443885202002,44.936924861739001,44.377656398805001,43.848391662022998,43.348851643011997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.786634141297,47.134409027128001,46.467018121864001,45.810917663494003,45.239212362233999,44.697961902633999,44.186944018338998]
[null,null,null,null,"Coincident",47.637115851979999,46.970976934249997,46.337664939581998,45.738646127408003,45.169399736048,44.630692368379997,44.122240038222998]
[null,"Cowell 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1170726221315999,2.1196584360305,2.1261191200431,2.1485646698155998,2.1539771829218002,2.1582963076249002,2.1612771764041998]
[null,null,null,null,"Coincident",1.9555421167328,1.9591911524692001,1.9722586368417001,1.9988067177229001,2.0036227991049,2.0074209400079002,2.0099730716624999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1252114167418998,2.1278071714467002,2.1342926926707002,2.1568245312732,2.1622578520418001,2.166593581026,2.1695859093454999]
[null,null,null,null,"Coincident",1.9630599295246001,1.9667229934771,1.9798407139966001,2.0064908553245999,2.0113254514693,2.0151381938027,2.0177001367765]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8506580203945,1.8555221143531,1.8644463776547999,1.8847598909582,1.8940664265466001,1.9007978638378,1.9058169821077]
[null,null,null,null,"Coincident",1.7115051366761,1.7161889307056,1.7317052146522001,1.7567229074919,1.7651798585876,1.7712359707720999,1.7756954704143]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8577726206989,1.8626554139980001,1.8716139854028,1.8920055912150999,1.9013479044999999,1.9081052198763999,1.9131436334562999]
[null,null,null,null,"Coincident",1.7180847828518,1.7227865830833999,1.7383625172502,1.7634763871703001,1.7719658498516999,1.7780452439268,1.7825218875022]
[null,"Croydon 11kV","Substation Rating","MVA","Non-Coincident",58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997]
[null,null,null,null,"Coincident",58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997,58.499488926745997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.173120519259001,26.611233213452,27.358120439968001,28.573044501321,29.083065909325999,29.668353936424001,30.269573629949001]
[null,null,null,null,"Coincident",25.105402687765999,25.580603956537001,26.155053577903999,26.906455170474999,27.353966737097998,27.882758907349,28.425268399467999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.935312101983001,27.386183145244001,28.154820592827001,29.405124649948,29.929998472051,30.532330764367,31.151058671689]
[null,null,null,null,"Coincident",25.836501090626001,26.325540770713001,26.916719030370999,27.690002307575998,28.150545929318,28.694737140004001,29.253045136857999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.062919363300001,23.374569684644001,23.869616154433,24.722825483206002,25.188465476811999,25.783300238369002,26.368120018757999]
[null,null,null,null,"Coincident",22.3014642614,22.664156717609998,23.000699700190999,23.498902636421999,23.911997124111998,24.456925397565001,24.992388225708002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.734538286187998,24.055264225836002,24.564727022179,25.442782794776001,25.921982764292,26.534139803031,27.135990212751999]
[null,null,null,null,"Coincident",22.950908729818,23.324163210416,23.670506714426999,24.18321789717,24.608342174779001,25.169139390681998,25.720195516541999]
[null,"Croydon Park 11kV","Substation Rating","MVA","Non-Coincident",27.255232029117,27.255232029117,27.255232029117,27.255232029117,27.255232029117,27.255232029117,27.255232029117]
[null,null,null,null,"Coincident",27.255232029117,27.255232029117,27.255232029117,27.255232029117,27.255232029117,27.255232029117,27.255232029117]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.337456416058,18.688663487144002,19.233059798989,20.073758353228001,20.385288045926,20.714472702864001,21.002932681817999]
[null,null,null,null,"Coincident",17.784714099708001,18.164361795863002,18.591474930741999,19.112819817386999,19.386217725796001,19.683951274582,19.942257395932]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.641925950981001,18.998964357186999,19.552399659397,20.407056916087999,20.723759152812001,21.058409491420001,21.351658971908002]
[null,null,null,null,"Coincident",18.080006069751001,18.465957320491999,18.900162111629001,19.430163249804,19.708100573721001,20.010777599567,20.273372556994001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.210651377639,16.465938461951001,16.837598400931,17.440958869319999,17.713260335756999,18.014640951198,18.284168388407]
[null,null,null,null,"Coincident",15.84950381752,16.142787679272999,16.404834976168001,16.761618165912001,17.002342152168001,17.277665835863001,17.522655008971]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.479808090203999,16.739333883423001,17.117164750703999,17.730543232334998,18.007365909291,18.313750556574,18.587753145168001]
[null,null,null,null,"Coincident",16.112664146117002,16.410817603683,16.677215853993001,17.039922963030001,17.284643856953,17.564538931141001,17.813595829777999]
[null,"Crystal Brook 11kV","Substation Rating","MVA","Non-Coincident",4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996]
[null,null,null,null,"Coincident",4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996,4.0714285714285996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9694298809743001,1.9898928416377999,2.0207780203743,2.0732822789685001,2.0825117180063999,2.0911261830201,2.0988485166895998]
[null,null,null,null,"Coincident",1.8727841482609999,1.8916609706177001,1.9109736248899001,1.9395912918542,1.9474123958373999,1.9546457359135001,1.961023941471]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0162366163912999,2.0371859129202998,2.0688051286507001,2.1225572371755002,2.1320060289891001,2.1408252309110001,2.1487310985221]
[null,null,null,null,"Coincident",1.9172939391237001,1.9366194001642001,1.9563910513814,1.9856888641985,1.9936958495620001,2.0011011018440001,2.0076308959312001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8779690209401001,1.9006967638262,1.9377189848362,1.9969928581920999,2.0119163560936002,2.0245715606591999,2.0353926710068002]
[null,null,null,null,"Coincident",1.8433350857329001,1.8518250984099001,1.8724298135446,1.9036280103808001,1.9172220260905,1.928638317369,1.9382838107525]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.9226020388169001,1.9458699438372999,1.9837720587294001,2.044454673028,2.0597328523653,2.0726888286504002,2.0837671204563999]
[null,null,null,null,"Coincident",1.8871449712619,1.8958367630329001,1.9169311830608999,1.9488708562801,1.9627879560979,1.9744755742871001,1.9843503086611001]
[null,"Cudmore Park 11kV","Substation Rating","MVA","Non-Coincident",24.65028583426,24.65028583426,24.65028583426,24.65028583426,24.65028583426,24.65028583426,24.65028583426]
[null,null,null,null,"Coincident",24.65028583426,24.65028583426,24.65028583426,24.65028583426,24.65028583426,24.65028583426,24.65028583426]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.87718784508,11.915590868932,12.080347076984999,12.381397627775,12.507539919065,12.804904974160999,13.101249564570001]
[null,null,null,null,"Coincident",10.062084197629,10.165023434098,10.385756377385,10.584686857375999,10.627557701085999,10.818395050243,11.095635803236]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.382909190312001,12.422947384807999,12.59471878301,12.908587830190999,13.040101161333,13.350127787303,13.659090497999999]
[null,null,null,null,"Coincident",10.490519852823001,10.597842161263999,10.827973740193,11.035374524035999,11.080070774655001,11.279033828497999,11.568079275362001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.102545569973,10.028624335526001,10.296932957584,10.759742647087,11.021304359804001,11.269696599415999,11.510309247623001]
[null,null,null,null,"Coincident",8.7550470749678997,8.7522185900443006,9.0792272284407005,9.4440702163088002,9.5989235546173006,9.7435157094990004,9.9719314517531004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.532704038674,10.455635296029,10.735368288825001,11.217884052006999,11.490582857353999,11.749551443758,12.000409189856001]
[null,null,null,null,"Coincident",9.1278301143609006,9.1248811947669992,9.4658136045703998,9.8461913207791003,10.007638192808001,10.158386968266001,10.396528473719]
[null,"Cummins 11kV","Substation Rating","MVA","Non-Coincident",4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004]
[null,null,null,null,"Coincident",4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004,4.5947046843177004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6457121951290001,2.7062873807129,2.8840600738056001,2.952972338815,2.9935594779941002,3.0365267399604998,3.0811661709974998]
[null,null,null,null,"Coincident",2.4811979889309002,2.7062873807129,2.8840600738056001,2.952972338815,2.9935594779941002,3.0365267399604998,3.0811661709974998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6660717382341002,2.7271130679072999,2.9062537748055002,2.9756963402127998,3.0165958095127001,3.0598937173534999,3.1048766621038002]
[null,null,null,null,"Coincident",2.5002915462350002,2.7271130679072999,2.9062537748055002,2.9756963402127998,3.0165958095127001,3.0598937173534999,3.1048766621038002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3662989813645998,2.4241321473960999,2.5896580781770999,2.6499751373747999,2.6885603751629001,2.7268742877963001,2.7655152029177001]
[null,null,null,null,"Coincident",2.2128611165179,2.4241321473960999,2.5896580781770999,2.6499751373747999,2.6885603751629001,2.7268742877963001,2.7655152029177001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3845083565941998,2.4427865660582002,2.6095862681620998,2.6703674850897001,2.7092496477714998,2.7478583973705999,2.7867966658391001]
[null,null,null,null,"Coincident",2.2298897416912,2.4427865660582002,2.6095862681620998,2.6703674850897001,2.7092496477714998,2.7478583973705999,2.7867966658391001]
[null,"Curramulka 7.6kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.20772470770925999,0.2111923613999,0.21578114690479,0.22153126248598001,0.22499856480590999,0.22883514834586999,0.23262691407732999]
[null,null,null,null,"Coincident",0.20772470770925999,0.2111923613999,0.21578114690479,0.22153126248598001,0.22499856480590999,0.22883514834586999,0.23262691407732999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.20870586109891001,0.21218989367971999,0.21680035355595001,0.22257762885953,0.22606130840998001,0.22991601341939,0.23372568893077]
[null,null,null,null,"Coincident",0.20870586109891001,0.21218989367971999,0.21680035355595001,0.22257762885953,0.22606130840998001,0.22991601341939,0.23372568893077]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.19990754247222001,0.20301581884552999,0.20800111701412999,0.21426948745203001,0.21865358870706,0.22285892840717,0.22693499564649]
[null,null,null,null,"Coincident",0.19990754247222001,0.20301581884552999,0.20800111701412999,0.21426948745203001,0.21865358870706,0.22285892840717,0.22693499564649]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.20085177277142999,0.20397473057543,0.20898357597753001,0.21528155402914001,0.21968636286323001,0.22391156579168001,0.22800688566220001]
[null,null,null,null,"Coincident",0.20085177277142999,0.20397473057543,0.20898357597753001,0.21528155402914001,0.21968636286323001,0.22391156579168001,0.22800688566220001]
[null,"Curramulka South 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.10714440058831,0.10906892130640999,0.11158170662684,0.11469573476460999,0.11662880842966,0.11875224745812001,0.12082967029663]
[null,null,null,null,"Coincident",0.10714440058831,0.10906892130640999,0.11158170662684,0.11469573476460999,0.11662880842966,0.11875224745812001,0.12082967029663]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10765399816479,0.10958767224124,0.11211240880972,0.11524124781193,0.11718351551464,0.11931705399185,0.12140435741804]
[null,null,null,null,"Coincident",0.10765399816479,0.10958767224124,0.11211240880972,0.11524124781193,0.11718351551464,0.11931705399185,0.12140435741804]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3832199275667993E-2,9.5410041171897997E-2,9.787833253356E-2,0.10095177711217,0.10313927937235,0.10524234984548,0.10726461956673]
[null,null,null,null,"Coincident",9.3832199275667993E-2,9.5410041171897997E-2,9.787833253356E-2,0.10095177711217,0.10313927937235,0.10524234984548,0.10726461956673]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.4278481685976995E-2,9.5863828075228003E-2,9.8343859063869998E-2,0.10143192148438,0.10362982788929,0.10574290093475,0.10777478892577]
[null,null,null,null,"Coincident",9.4278481685976995E-2,9.5863828075228003E-2,9.8343859063869998E-2,0.10143192148438,0.10362982788929,0.10574290093475,0.10777478892577]
[null,"Darke Peak 11kV","Substation Rating","MVA","Non-Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,null,null,"Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.29926002490537001,0.29801222548827999,0.29734685702511998,0.29825203440467002,0.29676827752274998,0.29514730654214,0.29332447107998999]
[null,null,null,null,"Coincident",0.22716153316389001,0.22635999370693999,0.22667012877343001,0.22801344197295001,0.22685429591566,0.22559053393077,0.22417270564808001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.32791953579720001,0.32655223722215998,0.32582314780353999,0.32681501214028003,0.32518915894419997,0.32341295094022998,0.32141554631269997]
[null,null,null,null,"Coincident",0.24891632128159,0.24803802005600001,0.24837785611352001,0.24984981562750999,0.24857966056037001,0.24719487071557,0.24564125996368999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.24932222756936001,0.24803428515379999,0.24731120017144001,0.24808749418062001,0.24740565492771999,0.24639113979901001,0.24512970284857]
[null,null,null,null,"Coincident",0.18948188527467,0.18852343476302,0.18876545442827,0.19002326302660999,0.18947767404322,0.18867755522150001,0.18768860163739001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.27319929935287002,0.27178801336779002,0.27099568003883001,0.27184631811256998,0.27109918053088999,0.26998750739589999,0.26860526524926998]
[null,null,null,null,"Coincident",0.20762817179106,0.20657793246501999,0.20684312985084,0.20822139616561999,0.20762355725873,0.20674681271963999,0.20566314910527]
[null,"Deloraine 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.33775924884212,0.33022378932384999,0.32533028542893999,0.32406455765577002,0.31704573437116002,0.30982783351363002,0.30239979330686001]
[null,null,null,null,"Coincident",0.32936065219487998,0.32346336538794002,0.31904229111614002,0.31593633596978998,0.30924506140588998,0.3023476479892,0.29523203741907]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.33781019754139002,0.33027360135,0.32537935930311002,0.32411344060345998,0.31709355857680999,0.30987456894773002,0.30244540827131]
[null,null,null,null,"Coincident",0.32941033402262998,0.32351215764983998,0.31909041648886999,0.31598399283019002,0.30929170893275998,0.30239325508788001,0.29527657117601003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.29329160901592999,0.28470064468746997,0.27856503050810999,0.27577064884107999,0.26835431728136999,0.26046820901562001,0.25226041682986]
[null,null,null,null,"Coincident",0.28593322909661001,0.27877487639465998,0.27322762463039002,0.26892948088731,0.26186596590957001,0.25432898295964002,0.24646170404850001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.29333585007236002,0.28474358985501003,0.27860705015972997,0.27581224697911,0.26839479671592997,0.26050749888406,0.25229846860833999]
[null,null,null,null,"Coincident",0.28597636019117001,0.27881692770012001,0.27326883917042,0.26897004708140998,0.26190546662017999,0.25436734676734002,0.24649888113035001]
[null,"Direk 11kV","Substation Rating","MVA","Non-Coincident",55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998]
[null,null,null,null,"Coincident",55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998,55.421489726026998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.200501478044998,45.677403105532001,46.550754190965002,48.722856724690999,49.269764312536999,49.802936297499002,50.319337450070996]
[null,null,null,null,"Coincident",44.200501478044998,45.677403105532001,46.550754190965002,47.973886664532998,48.624584484692001,49.262037093977,49.882849074841999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.203623928379002,46.714043573308999,47.607215204924003,49.828613215921997,50.387932773343998,50.933205000839997,51.461325784914003]
[null,null,null,null,"Coincident",45.203623928379002,46.714043573308999,47.607215204924003,49.062645414632001,49.728110705067998,50.380030186946001,51.014931384326999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.852285212363,44.816016078749001,45.556667022206,47.335134030345998,48.014014836126002,48.689940829038001,49.318291441058001]
[null,null,null,null,"Coincident",42.852285212363,44.816016078749001,45.556667022206,46.583362589712003,47.350076109607002,48.114976435545003,48.833778531794003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.824810136453003,45.833107522508001,46.590567406235003,48.409396404021997,49.10368428788,49.794950299922,50.437561216340001]
[null,null,null,null,"Coincident",43.824810136453003,45.833107522508001,46.590567406235003,47.640563645429999,48.424677591090997,49.206937192683,49.942052373534999]
[null,"Dorrien TF4 11kV","Substation Rating","MVA","Non-Coincident",14.6,14.6,14.6,14.6,14.6,14.6,14.6]
[null,null,null,null,"Coincident",14.6,14.6,14.6,14.6,14.6,14.6,14.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9769903471875008,9.1494908067100997,9.3995218633974993,9.7021294107462008,9.9066886801685001,10.112522528529,10.318016330511]
[null,null,null,null,"Coincident",8.9769903471875008,9.1494908067100997,9.3995218633974993,9.7021294107462008,9.9066886801685001,10.112522528529,10.318016330511]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.2579236511181993,9.4358224816035996,9.6936782153957992,10.005755811701,10.216716726795999,10.428992108549,10.640916802231001]
[null,null,null,null,"Coincident",9.2579236511181993,9.4358224816035996,9.6936782153957992,10.005755811701,10.216716726795999,10.428992108549,10.640916802231001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.0754899983550992,8.2284500017927993,8.4654592313874009,8.7939910212610002,9.0122957933684003,9.2255204475546009,9.4364599236751001]
[null,null,null,null,"Coincident",8.0754899983550992,8.2284500017927993,8.4654592313874009,8.7574015205562006,8.9749217477256007,9.1873800274480999,9.3975237488805003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.3282110104489,8.4859578697785008,8.7303842607330004,9.0691973940864994,9.2943339749093994,9.5142314564311992,9.7317722456492]
[null,null,null,null,"Coincident",8.3282110104489,8.4859578697785008,8.7303842607330004,9.0314628315153005,9.2557903152068999,9.4748974387134997,9.6916175702430998]
[null,"Dorrien TF5 11kV","Substation Rating","MVA","Non-Coincident",16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001]
[null,null,null,null,"Coincident",16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001,16.100000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6470651451532001,4.6504710350216003,4.7126876020864996,4.8481645730212,4.8815804440938004,4.9136014376646999,4.9436099729008998]
[null,null,null,null,"Coincident",4.5669161079988996,4.5903639024206999,4.6504760081000001,4.7335505764798,4.7660990834353996,4.7972799670833002,4.8264742725580003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9826936273065998,4.9863455033213997,5.0530555843174003,5.1983172104488,5.2341465011179,5.2684801709981999,5.3006560352514001]
[null,null,null,null,"Coincident",4.8967559259427,4.9218972080616998,4.9863508355741999,5.0754253610065003,5.1103246432675,5.1437575273337002,5.1750603550966998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.1776279184460998,4.1471195044286002,4.1684012175114997,4.2547353726579002,4.2617123958545999,4.2631644507511997,4.2607545198591001]
[null,null,null,null,"Coincident",4.0781989850929001,4.0633000266266999,4.0870127319413001,4.1329537325701002,4.1397881428411996,4.1412517857682003,4.1389443835573001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4793518825984,4.4466400364426999,4.4694587947005999,4.5620283264868,4.5695092564789999,4.5710661842288003,4.5684821990847997]
[null,null,null,null,"Coincident",4.3727418185872997,4.3567668014347003,4.3821921273053004,4.4314511593857002,4.4387791764116997,4.4403485291229998,4.4378744776661998]
[null,"Dowlingville 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.12220014746813999,0.1222588528662,0.12299752139005,0.1243776407993,0.12446842979835,0.12456767036999,0.12463881768074001]
[null,null,null,null,"Coincident",0.12220014746813999,0.1222588528662,0.12299752139005,0.1243776407993,0.12446842979835,0.12456767036999,0.12463881768074001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.12348937354716,0.12354869829414999,0.12429515985870999,0.12568983969174999,0.12578158652553001,0.12588187409699,0.12595377202033001]
[null,null,null,null,"Coincident",0.12348937354716,0.12354869829414999,0.12429515985870999,0.12568983969174999,0.12578158652553001,0.12588187409699,0.12595377202033001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10811111949059,0.10764956577254001,0.10794710972762001,0.10889630620181,0.10888063851217,0.10878953139304,0.10864519375202999]
[null,null,null,null,"Coincident",0.10811111949059,0.10764956577254001,0.10794710972762001,0.10889630620181,0.10888063851217,0.10878953139304,0.10864519375202999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10925170464999,0.10878528148537001,0.10908596456453,0.11004517517434,0.1100293421887,0.10993727387864,0.10979141345837]
[null,null,null,null,"Coincident",0.10925170464999,0.10878528148537001,0.10908596456453,0.11004517517434,0.1100293421887,0.10993727387864,0.10979141345837]
[null,"East Terrace 11kV","Substation Rating","MVA","Non-Coincident",77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994]
[null,null,null,null,"Coincident",77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994,77.840301278035994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.824631252970001,37.486884712962997,37.744065246218,37.233448637753,36.784802274024003,36.368858865466002,36.005802730683001]
[null,null,null,null,"Coincident",36.698035621568998,37.353944000440997,37.630200361655,37.147686624193,36.701377906588,36.287825695107003,35.927139493033003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.078204428991,38.763002124864997,39.028937521560003,38.500938653943003,38.037019603756001,37.606916773041,37.231501588988003]
[null,null,null,null,"Coincident",37.947299266649999,38.625535884032999,38.911196482366002,38.412257155352002,37.950755328744997,37.523125095528002,37.150160520732001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.646168126166998,35.388791650396001,35.714424736978003,35.255608736244,34.866065935211999,34.504858194313002,34.189313507681]
[null,null,null,null,"Coincident",34.444328319341999,35.170679156333001,35.518653570655999,35.104761405631002,34.718082060908003,34.359722224003001,34.046891050661998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.825582706493002,36.593486400492999,36.930204592035999,36.455769713076002,36.052966211537999,35.679462343847,35.353175978574001]
[null,null,null,null,"Coincident",35.616871928823997,36.367948985593998,36.727769041729999,36.299787282371,35.899944714071999,35.529385697877998,35.205905218510999]
[null,"Edinburgh 11kV","Substation Rating","MVA","Non-Coincident",57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002]
[null,null,null,null,"Coincident",57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002,57.057998289136002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.529060224157998,28.027396833175001,28.649707429145,29.838518555834,30.004882715050002,30.164123618615001,30.331844556111999]
[null,null,null,null,"Coincident",22.986891810197001,23.619022679711001,23.929782480661999,24.520734156774999,24.714475765345998,24.901882582163001,25.095693918102]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.295408082986999,28.807617275744999,29.447251615746001,30.669156602308,30.840151970005,31.003825786446001,31.176215702115002]
[null,null,null,null,"Coincident",23.626795794439001,24.276523782576,24.595934445783001,25.203336903288001,25.402471847689998,25.595095653813001,25.794302266637999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.647910013076999,27.331783117442999,28.002149466959999,29.037253971333001,29.282436155951,29.526006778111,29.758700012959999]
[null,null,null,null,"Coincident",22.338757202663,23.223364030086,23.463481321343,23.849914005397999,24.101491264029999,24.351728701363001,24.592932227102999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.389728608207999,28.092639220029,28.781667078961998,29.845586592423999,30.097594104193998,30.347945191188,30.587116088582]
[null,null,null,null,"Coincident",22.960618559779999,23.869850875417001,24.116652498450001,24.513842609659999,24.772423220092001,25.029626711578999,25.277544807447999]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Edithburgh 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.81566594098237,0.83240226291013997,0.85391278041096996,0.88025676064292002,0.89760203106216996,0.91486612884822005,0.93223828477033999]
[null,null,null,null,"Coincident",0.81566594098237,0.83240226291013997,0.85391278041096996,0.88025676064292002,0.89760203106216996,0.91486612884822005,0.93223828477033999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.82210030776604004,0.83896865388224995,0.86064885673139002,0.88720065099949996,0.90468274928692005,0.92208303461220997,0.93959223048831997]
[null,null,null,null,"Coincident",0.82210030776604004,0.83896865388224995,0.86064885673139002,0.88720065099949996,0.90468274928692005,0.92208303461220997,0.93959223048831997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.77067765947038003,0.78390031316424003,0.80275577201933002,0.82684991671286001,0.84380569458879995,0.86011440743154,0.87638389431177999]
[null,null,null,null,"Coincident",0.77067765947038003,0.78390031316424003,0.80275577201933002,0.82684991671286001,0.84380569458879995,0.86011440743154,0.87638389431177999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.77675713696705995,0.79008409733776996,0.80908829715659003,0.83337250809722996,0.85046204133609005,0.86689940518034003,0.88329723362875001]
[null,null,null,null,"Coincident",0.77675713696705995,0.79008409733776996,0.80908829715659003,0.83337250809722996,0.85046204133609005,0.86689940518034003,0.88329723362875001]
[null,"Elizabeth Downs 11kV","Substation Rating","MVA","Non-Coincident",59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999]
[null,null,null,null,"Coincident",59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999,59.744727744165999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.981206615437998,45.521515500653997,46.707977992814001,49.134289274476998,49.896010214688999,50.646929429189001,51.379336779046]
[null,null,null,null,"Coincident",43.859488604242998,45.521515500653997,46.592625557455001,48.222358545455002,49.083197505401998,49.934665760830001,50.768746283421002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.443500472080999,45.999999802938,47.198933401815999,49.650748049260002,50.420475566332001,51.179287818935997,51.919393625575999]
[null,null,null,null,"Coincident",44.320503062406999,45.999999802938,47.082368477616001,48.729231863037,49.599119246011,50.459537427416997,51.302385110602998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.725825707924002,41.76218310166,42.672152971715001,44.709673847826998,45.580526625783001,46.453634951059001,47.282213878744997]
[null,null,null,null,"Coincident",39.725825707924002,41.76218310166,42.672152971715001,43.857142687653997,44.804703357926002,45.756452060976997,46.666122673859]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.143390540454,42.201152429098002,43.120687145437003,45.179624746016003,46.059631203923999,46.94191691759,47.779205177682002]
[null,null,null,null,"Coincident",40.143390540454,42.201152429098002,43.120687145437003,44.318132487494999,45.275653127272001,46.237405820943998,47.156638134566002]
[null,"Elizabeth Heights 11kV","Substation Rating","MVA","Non-Coincident",27.565363881402,27.565363881402,27.565363881402,27.565363881402,27.565363881402,27.565363881402,27.565363881402]
[null,null,null,null,"Coincident",27.565363881402,27.565363881402,27.565363881402,27.565363881402,27.565363881402,27.565363881402,27.565363881402]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.287798726540998,20.831244395256,21.481880609042001,22.569022773688999,22.889780448848001,23.204766215149998,23.509657019253002]
[null,null,null,null,"Coincident",19.918897388969999,20.641244374273001,21.097566235502001,21.807730291698999,22.168821024528,22.524759736343,22.871159429533002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.491599083949001,21.040503916717,21.697676073347001,22.795739085775001,23.119718920703001,23.437868865268001,23.745822439053001]
[null,null,null,null,"Coincident",20.118991961169002,20.848595257309999,21.309501083495999,22.026799067352002,22.391517124239002,22.751031405669,23.100910844603]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.335112723035,18.981213292402,19.631075461293999,20.545405967436,20.907453417047002,21.269299717488,21.608740417332999]
[null,null,null,null,"Coincident",18.072612625982,18.963680697116999,19.34134508304,19.842093981695999,20.23388832414,20.626226078108001,20.997486502627002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.519297442946002,19.171888392503998,19.828278728600001,20.751794109180999,21.117478493515002,21.482959708041001,21.825810247311001]
[null,null,null,null,"Coincident",18.254160410546,19.154179674159,19.535637874180999,20.041417028011001,20.437147126527002,20.833426095387001,21.208416003239002]
[null,"Elizabeth South 11kV","Substation Rating","MVA","Non-Coincident",25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001]
[null,null,null,null,"Coincident",25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001,25.337745098039001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.642493692594,11.052894023321,11.320220203302,11.880152772198,12.071745492406,12.260797688352,12.445147243938001]
[null,null,null,null,"Coincident",10.642493692594,11.052894023321,11.320220203302,11.723530542469,11.940148329112001,12.15459178039,12.364615292278]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.777964539005,11.193588953651,11.464317992484,12.031378076907,12.225409626654001,12.416868313196,12.603564498346]
[null,null,null,null,"Coincident",10.777964539005,11.193588953651,11.464317992484,11.872762165374001,12.092137331608001,12.309310484841999,12.522007436221999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.6224555755020003,10.086941275339001,10.2777309919,10.679855341129,10.857632025975001,11.035073350011,11.200841109608]
[null,null,null,null,"Coincident",9.6224555755020003,10.086941275339001,10.2777309919,10.53360009683,10.731291968824999,10.929001557268,11.115453240467]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7449421128691007,10.215340362219999,10.408558686692,10.815801772896,10.995841419662,11.175541436731001,11.343419293767999]
[null,null,null,null,"Coincident",9.7449421128691007,10.215340362219999,10.408558686692,10.667684810628,10.867893149721001,11.068119430779999,11.256944502028]
[null,"Eudunda 11kV","Substation Rating","MVA","Non-Coincident",2.4,2.4,2.4,2.4,2.4,2.4,2.4]
[null,null,null,null,"Coincident",2.4,2.4,2.4,2.4,2.4,2.4,2.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8331104504369,1.8601555578044999,1.8970480518357999,1.9437575489692001,1.9700967355923,1.9961070398744001,2.0214981319973999]
[null,null,null,null,"Coincident",1.8331104504369,1.8601555578044999,1.8970480518357999,1.9437575489692001,1.9700967355923,1.9961070398744001,2.0214981319973999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8935616162875,1.9214986002304999,1.9596077117737001,2.0078575653855002,2.0350653491727999,2.0619334049437001,2.0881618285656001]
[null,null,null,null,"Coincident",1.8935616162875,1.9214986002304999,1.9596077117737001,2.0078575653855002,2.0350653491727999,2.0619334049437001,2.0881618285656001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6533981654994001,1.6765082109645,1.7109685394411001,1.7558198559255001,1.7850788303973999,1.8127974537222999,1.8395772262159999]
[null,null,null,null,"Coincident",1.6533981654994001,1.6765082109645,1.7109685394411001,1.7558198559255001,1.7850788303973999,1.8127974537222999,1.8395772262159999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7079228924168,1.7317950464558001,1.7673917860152999,1.813722181063,1.8439460396301,1.8725787503169999,1.9002416493392]
[null,null,null,null,"Coincident",1.7079228924168,1.7317950464558001,1.7673917860152999,1.813722181063,1.8439460396301,1.8725787503169999,1.9002416493392]
[null,"Evanston 11kV","Substation Rating","MVA","Non-Coincident",57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998]
[null,null,null,null,"Coincident",57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998,57.667953878993998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.153448275327001,41.102911650868997,42.273492689508998,44.385999166634001,45.074896781305,45.845588636781997,46.698821850500003]
[null,null,null,null,"Coincident",39.804331996179997,41.102911650868997,41.91845984751,43.303284580125002,44.077082133419999,44.932196446719999,45.869598407765999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.422981371412,41.378818092562,42.557256746055003,44.683943584662003,45.377465477320001,46.153330660888003,47.012291267884002]
[null,null,null,null,"Coincident",40.071521622509003,41.378818092562,42.199840718918999,43.593961193588001,44.372952922208,45.233807255812003,46.177501599297997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.398118733013,37.86911021161,38.733568261141002,40.503451398517001,41.252606263646001,42.078151781951,42.944989492188]
[null,null,null,null,"Coincident",36.223750908824002,37.86911021161,38.530727974774997,39.494983173024998,40.309436624664002,41.200298649864003,42.133494940633]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.642443892000003,38.123309513530998,38.993570303909998,40.775333917365003,41.529517541890002,42.360604597698,43.233261022438001]
[null,null,null,null,"Coincident",36.466905610440001,38.123309513530998,38.789368436590998,39.760096271690998,40.580016804487997,41.476858809244,42.416319251570002]
[null,"Evanston 33kV","Substation Rating","MVA","Non-Coincident",11.875,11.875,11.875,11.875,11.875,11.875,11.875]
[null,null,null,null,"Coincident",11.875,11.875,11.875,11.875,11.875,11.875,11.875]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Findon 11kV","Substation Rating","MVA","Non-Coincident",24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002]
[null,null,null,null,"Coincident",24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002,24.821457654723002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.676219106361,20.042416226366001,20.645601625325,21.599311204071999,22.017849802760999,22.489591655140998,22.951835635856]
[null,null,null,null,"Coincident",19.393555304504002,19.797026573025999,20.281543157123,20.899888306558001,21.279387729995001,21.718406539204,22.147249169504999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.009610807337001,20.382012731225998,20.995418437504998,21.965287566874,22.390917837726999,22.870652832373999,23.340729024459002]
[null,null,null,null,"Coincident",19.722157580988,20.132465222482001,20.625191402500999,21.254013724406999,21.639943344500001,22.086400840317001,22.522509733164998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.247629243694,17.531109155892999,17.956854851968,18.648653494087,19.005455456743999,19.411590889147998,19.801026709005999]
[null,null,null,null,"Coincident",17.137702610849001,17.466642447923,17.779927302387001,18.213820585240999,18.539435966530998,18.920324417993001,19.285033489812001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.539871184092998,17.828154348868001,18.261113833376001,18.9646342359,19.327481811925001,19.740498758602001,20.136533136329]
[null,null,null,null,"Coincident",17.428081966423999,17.762595324061,18.081188442778998,18.522433565884,18.853566138522002,19.240908322178999,19.611796984556001]
[null,"Flinders Park 11kV","Substation Rating","MVA","Non-Coincident",29.4,29.4,29.4,29.4,29.4,29.4,29.4]
[null,null,null,null,"Coincident",29.4,29.4,29.4,29.4,29.4,29.4,29.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.500356119938001,21.636104105548,22.050890305544002,22.874387513037,23.202105619196001,23.635618137578,24.114567459433999]
[null,null,null,null,"Coincident",20.839321535229001,21.016049887234999,21.302065759455999,21.765852246188999,22.051277862765001,22.445820850021999,22.882526935192999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.885507614801998,22.023687352671999,22.445903919127002,23.284153030203999,23.617741788819998,24.059020131804001,24.546549220722]
[null,null,null,null,"Coincident",21.212631437469,21.392525652802,21.683665135075,22.155759765993,22.446298418943002,22.847909141287001,23.292438259741001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.760421152384001,18.86365392678,19.171306090367999,19.79385802689,20.099768708561001,20.504558853256999,20.943756245010999]
[null,null,null,null,"Coincident",18.331074276064999,18.481958711413998,18.666957949831001,19.011052662636001,19.281083468885999,19.653505215999999,20.05900569644]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.096490202161998,19.201572260224001,19.514735620465999,20.148439781985999,20.459830463879999,20.871871908437001,21.318936962058]
[null,null,null,null,"Coincident",18.659452123413999,18.813039461239999,19.001352725379999,19.351611456691,19.626479520897,20.005572729255999,20.418337234317001]
[null,"Forreston 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.94842842911627001,0.96070687683502998,0.98133614169321004,1.0142919377395001,1.0304850415896001,1.0466464806982001,1.0625971908862]
[null,null,null,null,"Coincident",0.82727185488327004,0.84175724956566,0.86083670572624005,0.88452525380117997,0.89908711171243005,0.91361959090560996,0.92796133063159003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.97776114163469996,0.99041933353450995,1.0116866141637999,1.0456616572735,1.0623555766257999,1.0790168519189001,1.0954608809299]
[null,null,null,null,"Coincident",0.85285747288976999,0.86779086755285995,0.88746040746187005,0.91188158790982998,0.92689381063377996,0.94187574602340995,0.95666104281230002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.86754824993580004,0.8802473212045,0.90130705070508998,0.93486590171370998,0.95441148217252003,0.97325013638292002,0.99167422710968001]
[null,null,null,null,"Coincident",0.7565503745944,0.77099065711653003,0.79076966384618996,0.81549051495761005,0.83307739179883,0.85005069317159998,0.86665966795171001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.89437952431560996,0.90747134868547996,0.92918240723969003,0.96377915641633005,0.98392923677730004,1.0033505272850001,1.0223444328129001]
[null,null,null,null,"Coincident",0.77994873968175005,0.79483562696909005,0.81522635293922996,0.84071176318510998,0.85884256172524998,0.87634080831727001,0.89346346053206005]
[null,"Freeling 11kV","Substation Rating","MVA","Non-Coincident",3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999]
[null,null,null,null,"Coincident",3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999,3.8887499999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.64111808782879998,0.65611231282994997,0.67478601961354001,0.69719931430866,0.71252643675928995,0.72789398974389996,0.74314688621703995]
[null,null,null,null,"Coincident",0.64111808782879998,0.65611231282994997,0.67478601961354001,0.69719931430866,0.71252643675928995,0.72789398974389996,0.74314688621703995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.64704424941694005,0.66217707322218,0.68102339002246004,0.70364386153666003,0.71911265992196005,0.73462226256001995,0.75001614886155998]
[null,null,null,null,"Coincident",0.64704424941694005,0.66217707322218,0.68102339002246004,0.70364386153666003,0.71911265992196005,0.73462226256001995,0.75001614886155998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.57778076199127004,0.59182139273973999,0.60684748123158005,0.62749799592547995,0.64274651907848002,0.65756233058256996,0.67210538154316002]
[null,null,null,null,"Coincident",0.57778076199127004,0.59182139273973999,0.60684748123158005,0.62749799592547995,0.64274651907848002,0.65756233058256996,0.67210538154316002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.58312146633744999,0.59729188136153999,0.61245686318697001,0.63329826048000004,0.64868773303670002,0.66364049418344995,0.67831797353034995]
[null,null,null,null,"Coincident",0.58312146633744999,0.59729188136153999,0.61245686318697001,0.63329826048000004,0.64868773303670002,0.66364049418344995,0.67831797353034995]
[null,"Freeling North 11kV","Substation Rating","MVA","Non-Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,null,null,"Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.3539693254582001,3.4328148188373002,3.5308370064768999,3.6486131454435,3.7294676830014,3.8107127431790002,3.8921039086390001]
[null,null,null,null,"Coincident",3.3539693254582001,3.4328148188373002,3.5308370064768999,3.6486131454435,3.7294676830014,3.8107127431790002,3.8921039086390001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.3836761722393001,3.4632200175602001,3.5621104093564,3.6809297175875999,3.7625004016351999,3.8444650672474001,3.9265771322288998]
[null,null,null,null,"Coincident",3.3836761722393001,3.4632200175602001,3.5621104093564,3.6809297175875999,3.7625004016351999,3.8444650672474001,3.9265771322288998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9393189273027001,3.0005872428299001,3.0662587485341,3.1598962763082001,3.2258524665017001,3.2892803864481999,3.3515638163935999]
[null,null,null,null,"Coincident",2.9393189273027001,3.0005872428299001,3.0662587485341,3.1598962763082001,3.2258524665017001,3.2892803864481999,3.3515638163935999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9653531239638,3.0271641064881001,3.0934172792167001,3.187884175247,3.2544245539783998,3.3184142690148999,3.3812493570498998]
[null,null,null,null,"Coincident",2.9653531239638,3.0271641064881001,3.0934172792167001,3.187884175247,3.2544245539783998,3.3184142690148999,3.3812493570498998]
[null,"Fulham Gardens 11kV","Substation Rating","MVA","Non-Coincident",55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999]
[null,null,null,null,"Coincident",55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999,55.670763956904999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.076199557644998,47.042617646788003,48.567468571871999,50.927545548495999,52.034859575197999,53.274734864612,54.510778130256]
[null,null,null,null,"Coincident",42.974417658793001,43.970250066855002,45.147789097706998,46.630962100543002,47.587860167835998,48.683887717727998,49.773973811749997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.047830000345002,48.034627401253999,49.591633573377003,52.001478600742999,53.132143077965999,54.398164199455998,55.660272489493003]
[null,null,null,null,"Coincident",43.880639370988,44.897471364363,46.099841713354003,47.614291081323003,48.591367707213998,49.710507704394999,50.823580955437002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.592244503282998,40.389117821183,41.516751033330998,43.271207478396001,44.258915609620999,45.370051361224,46.462563832508998]
[null,null,null,null,"Coincident",37.226386661089997,38.078687483602998,38.899196910721002,39.991726704897999,40.854186904019002,41.846032381545001,42.820666758648997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.427144742962,41.240822102473999,42.392234245342003,44.183687736793999,45.192224132893998,46.326790925525003,47.442341719985997]
[null,null,null,null,"Coincident",38.011396946201998,38.881670636126003,39.719482530583001,40.835051013231997,41.715698315307002,42.728459303870999,43.723646253460998]
[null,"Fullerville 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2706131779394999E-2,3.3359405210480003E-2,3.4521366289809001E-2,3.6336731827983998E-2,3.7243499962051001E-2,3.8152550343554997E-2,3.9056856181249003E-2]
[null,null,null,null,"Coincident",3.086317802075E-2,3.1710607491909001E-2,3.2740308202965002E-2,3.3951486448739E-2,3.4811516412804999E-2,3.5674212049281999E-2,3.6532942630923E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2859765783802002E-2,3.3516107905914999E-2,3.4683527189070001E-2,3.6507420237590002E-2,3.7418447830416E-2,3.8331768391325002E-2,3.9240322121370998E-2]
[null,null,null,null,"Coincident",3.1008154921718E-2,3.1859565113801003E-2,3.2894102747934001E-2,3.4110970390584E-2,3.4975040265214002E-2,3.5841788334002998E-2,3.6704552722480001E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.964596285499E-2,3.0165334421396E-2,3.1100221286125999E-2,3.2598331660167998E-2,3.3410215205799003E-2,3.4194059386019E-2,3.4970350789175E-2]
[null,null,null,null,"Coincident",2.7771718490143999E-2,2.8431594575350001E-2,2.9278228752383999E-2,3.030927919787E-2,3.1075888960562001E-2,3.1816849949219003E-2,3.2551137625916E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9785222001214001E-2,3.0307033267125999E-2,3.1246311675729999E-2,3.2751459283566001E-2,3.356715657645E-2,3.4354682791617998E-2,3.5134620751256999E-2]
[null,null,null,null,"Coincident",2.7902173548224999E-2,2.8565149339811999E-2,2.9415760501950002E-2,3.0451654210765001E-2,3.1221865051335999E-2,3.1966306635147997E-2,3.2704043559739E-2]
[null,"Gawler Belt TF1 11kV","Substation Rating","MVA","Non-Coincident",14,14,14,14,14,14,14]
[null,null,null,null,"Coincident",14,14,14,14,14,14,14]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.7017607167113002,4.8117237007954001,4.9486708602301999,5.1191688625646998,5.2317593158392999,5.3446500227650002,5.4567065112593998]
[null,null,null,null,"Coincident",4.7017607167113002,4.8117237007954001,4.9486708602301999,5.1130429946782003,5.2254473451507,5.3381482005886003,5.4500082008208999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9205421864602998,5.0356219480083002,5.1789415076192,5.3573730918153002,5.4752025834696996,5.5933463001231001,5.7106169806456002]
[null,null,null,null,"Coincident",4.9205421864602998,5.0356219480083002,5.1789415076192,5.3509621761646997,5.4685969053154002,5.5865419363462996,5.7036069856509997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.2339456923728997,4.3368346633916,4.4469450146328002,4.6468086589529998,4.7596513692505003,4.8692872362991002,4.9769051951292997]
[null,null,null,null,"Coincident",4.2339456923728997,4.3368346633916,4.4469450146328002,4.5982708521913001,4.7100111924133996,4.8185806454366,4.9251513241770004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4309588789697001,4.5386354607700996,4.6538694467367998,4.8630331096008002,4.9811265962556002,5.0958640194180997,5.2084896374258998]
[null,null,null,null,"Coincident",4.4309588789697001,4.5386354607700996,4.6538694467367998,4.8122367504919996,4.9291765717886999,5.0427979587434004,5.1543275648159002]
[null,"Gawler Belt TF2 11kV","Substation Rating","MVA","Non-Coincident",15.9,15.9,15.9,15.9,15.9,15.9,15.9]
[null,null,null,null,"Coincident",15.9,15.9,15.9,15.9,15.9,15.9,15.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.5756840025361996,5.7060859706861002,5.8684877031561999,6.0634119317003004,6.1967090466550996,6.3303577783959,6.4630093639183999]
[null,null,null,null,"Coincident",5.5756840025361996,5.7060859706861002,5.8684877031561999,6.0634119317003004,6.1967090466550996,6.3303577783959,6.4630093639183999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6939526187254996,5.8271206081051998,5.9929671247769001,6.1920259884190001,6.3281505350074001,6.4646341567008996,6.60009948121]
[null,null,null,null,"Coincident",5.6939526187254996,5.8271206081051998,5.9929671247769001,6.1920259884190001,6.3281505350074001,6.4646341567008996,6.60009948121]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.0248511354872001,5.1469598729195001,5.2776389518834996,5.4572326127219997,5.5898461642977999,5.7186965036599,5.8451746956318003]
[null,null,null,null,"Coincident",5.0248511354872001,5.1469598729195001,5.2776389518834996,5.4572326127219997,5.5898461642977999,5.7186965036599,5.8451746956318003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.131435760814,5.2561346076201998,5.3895855857498001,5.5729886973629998,5.7084151811685002,5.8399986293876998,5.9691596134145]
[null,null,null,null,"Coincident",5.131435760814,5.2561346076201998,5.3895855857498001,5.5729886973629998,5.7084151811685002,5.8399986293876998,5.9691596134145]
[null,"Georgetown 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.15030717679280001,0.15194106129860999,0.15558921763694,0.16195450358673999,0.16488599099498,0.16791910982861,0.17102808880310999]
[null,null,null,null,"Coincident",0.14038918312814999,0.1428408396502,0.14614482402295001,0.15031540026422999,0.15302988285319,0.15584069479741999,0.15872403167741]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.15323332556069999,0.15489901818929,0.1586181960743,0.16510740008336,0.16809595707703001,0.17118812403549,0.17435762796422]
[null,null,null,null,"Coincident",0.14312225046400001,0.14562163532388001,0.14898994097528001,0.15324170912495999,0.15600903669478999,0.15887456893968999,0.16181403802068001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.13681764050883999,0.13823720505907,0.14153564017522,0.14742504957996999,0.15043839997051001,0.15343787889262001,0.15647154165864]
[null,null,null,null,"Coincident",0.12605313506286001,0.12805810822471,0.13101215102006,0.13485596057221,0.13760601184874999,0.14034527825067999,0.1431178341786]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.13948117779791,0.14092837813472001,0.14429102649775,0.15029508969642,0.15336710336386999,0.15642497551602,0.15951769699603999]
[null,null,null,null,"Coincident",0.12850711120507999,0.13055111676626999,0.13356266825063001,0.13748130828541999,0.14028489698662999,0.14307749085554,0.14590402232399]
[null,"Geranium 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.8414075207614998E-2,9.9559613561314E-2,0.10195262158313,0.10602152313534,0.10767871736727,0.10935684351636001,0.11103660951928999]
[null,null,null,null,"Coincident",6.5780554927145005E-2,6.6855744080176999E-2,6.8297215344108E-2,7.0112790600370997E-2,7.1217407593785004E-2,7.2335285844874003E-2,7.3453426524700993E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10316097614333,0.10436176835244999,0.10687020063644,0.11113536143861,0.11287248871703,0.11463155754197001,0.11639234531739]
[null,null,null,null,"Coincident",6.8953411828728994E-2,7.0080461616390005E-2,7.1591460753006E-2,7.3494608400359998E-2,7.4652505449786993E-2,7.5824303399912002E-2,7.6996376436753999E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.5939359840829996E-2,8.7506140920361006E-2,9.0173915832545998E-2,9.4364815035847996E-2,9.6020797401165994E-2,9.7624908234623997E-2,9.9198549000209996E-2]
[null,null,null,null,"Coincident",6.4270185339870001E-2,6.5190177341711994E-2,6.6567334969241998E-2,6.8364411623809004E-2,6.9574107268426999E-2,7.0745649182408998E-2,7.1894343154061999E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.0084555807794994E-2,9.1726908949114005E-2,9.4523361219697996E-2,9.8916404103238001E-2,0.10065226106193,0.10233374451917,0.1039832882164]
[null,null,null,null,"Coincident",6.7370191129538001E-2,6.8334557992243999E-2,6.9778141390853005E-2,7.1661898175626002E-2,7.2929942236112003E-2,7.4157992260299996E-2,7.5362092295337996E-2]
[null,"Gladstone 11kV","Substation Rating","MVA","Non-Coincident",4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998]
[null,null,null,null,"Coincident",4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998,4.7529411764705998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2403927415485998,2.2286031757782001,2.2275105411952998,2.2487192248416998,2.2218439259235998,2.1939452937541999,2.1648247669977998]
[null,null,null,null,"Coincident",2.0159054615143002,2.0046804794634001,1.9932173282529,1.9906083681997,1.9659968946074999,1.9404944879212001,1.9139181092649]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3271607559569998,2.3149145929151,2.3137796417635998,2.3358097150414001,2.3078935645438001,2.2789144481927002,2.2486661145842999]
[null,null,null,null,"Coincident",2.0939793236934001,2.0823196100946002,2.0704125032994001,2.0677025010140002,2.0421378513757,2.0156477637574999,1.9880421103837]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9933393480999999,1.9704742055925999,1.9608905242554999,1.9715469142523001,1.9366699002431,1.8990225692094,1.8595094804412999]
[null,null,null,null,"Coincident",1.8513814501532,1.8165890309599,1.7929447371102001,1.7783264715823,1.7462921186182001,1.7117746392016999,1.6755846053772001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0705392488447001,2.0467885638259999,2.0368337167621,2.0479028173446001,2.0116750538897001,1.9725696819951,1.9315262935648001]
[null,null,null,null,"Coincident",1.923083473358,1.8869435809855,1.8623835689266,1.8471991536114001,1.8139241444231,1.778069839951,1.7404782048276]
[null,"Glanville 11kV","Substation Rating","MVA","Non-Coincident",23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999]
[null,null,null,null,"Coincident",23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999,23.942580101179999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.288891460094,12.527324463135001,12.918256105515001,13.527697961995999,13.795802024505999,14.086404502820001,14.35711701798]
[null,null,null,null,"Coincident",11.326712791362,11.57133886481,11.867322377883999,12.240618380313,12.46828077112,12.721020153254001,12.955226304386001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.364356986632,12.604254195957999,12.997586531870001,13.610770943222001,13.880521420652,14.172908475639,14.445283424107]
[null,null,null,null,"Coincident",11.396269622222,11.642397933321,11.940199067759,12.315787464052001,12.544847919302001,12.799139362548001,13.03478376306]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.890926813302,11.102830538226,11.407744832851,11.880112121083,12.132454681365999,12.405015477134,12.652720823287]
[null,null,null,null,"Coincident",10.119601969985,10.344491438418,10.562699000182,10.850494000524,11.067315999637,11.306811618966,11.523701772754]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.957807502185,11.171012518296999,11.477799277811,11.953067352193001,12.206959536722,12.481194116007,12.730420609486]
[null,null,null,null,"Coincident",10.181745987896999,10.408016492383,10.627564056912,10.917126393332,11.135279886533,11.376246237627001,11.594468304036999]
[null,"Glencoe 11kV","Substation Rating","MVA","Non-Coincident",2.1,2.1,2.1,2.1,2.1,2.1,2.1]
[null,null,null,null,"Coincident",2.1,2.1,2.1,2.1,2.1,2.1,2.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0528698449716001,1.0652044331229,1.0913444613417,1.1357498279184,1.1546326538944001,1.173436629657,1.1921309921879]
[null,null,null,null,"Coincident",0.71190248267702005,0.72379410517099996,0.73953973355577995,0.75920405149122006,0.77099090633531997,0.78270879702277996,0.79433645612125003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1254421661552001,1.1386269540698,1.1665687648476,1.2140349091083,1.2342192924591999,1.2543193906011001,1.2743023200792001]
[null,null,null,null,"Coincident",0.76097257037208998,0.77368385984689003,0.79051480452772005,0.81153454659643998,0.82413384698599002,0.83665942965040996,0.84908856123358001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.95741546261513,0.96626846905248998,0.98699827493784997,1.0240727293173,1.0415651462341999,1.0581539583523001,1.0744102139531]
[null,null,null,null,"Coincident",0.64633865092024001,0.65498959057627004,0.66803852426664001,0.68515449720984001,0.69617606260127995,0.70658634437267998,0.71674894166592995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0234082942941001,1.0328715216716,1.0550301937533999,1.0946601199453001,1.1133582559782,1.1310905034476,1.1484672719097999]
[null,null,null,null,"Coincident",0.69088954806293001,0.70013678057913997,0.71408515251575,0.73238089700595999,0.74416215799259,0.75529000073882002,0.76615308658565995]
[null,"Glenelg North 11kV","Substation Rating","MVA","Non-Coincident",27.91251198466,27.91251198466,27.91251198466,27.91251198466,27.91251198466,27.91251198466,27.91251198466]
[null,null,null,null,"Coincident",27.91251198466,27.91251198466,27.91251198466,27.91251198466,27.91251198466,27.91251198466,27.91251198466]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.066909946258999,21.493042961852002,22.223255910744999,22.900710715182999,23.093790413838001,23.272974704658999,23.629348784676001]
[null,null,null,null,"Coincident",21.066909946258999,21.493042961852002,22.223255910744999,22.900710715182999,23.093790413838001,23.272974704658999,23.629348784676001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.634164627337999,22.071771843393002,22.821646750993999,23.517342930651001,23.715621558013002,23.899630625128999,24.265600553119999]
[null,null,null,null,"Coincident",21.634164627337999,22.071771843393002,22.821646750993999,23.517342930651001,23.715621558013002,23.899630625128999,24.265600553119999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.504150080870001,18.785342434869001,19.383275455993001,19.927894118333999,20.016915292532001,20.077522192330001,20.301253156952001]
[null,null,null,null,"Coincident",18.504150080870001,18.785342434869001,19.383275455993001,19.927894118333999,20.016915292532001,20.077522192330001,20.301253156952001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.002399030504002,19.291162864112,19.905196030254,20.464479277311,20.555897465495001,20.618136286999,20.847891506591999]
[null,null,null,null,"Coincident",19.002399030504002,19.291162864112,19.905196030254,20.464479277311,20.555897465495001,20.618136286999,20.847891506591999]
[null,"Glossop 11kV","Substation Rating","MVA","Non-Coincident",15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001]
[null,null,null,null,"Coincident",15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001,15.145135697399001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.357665369752,10.664272874348001,10.955178786080999,11.335771013781001,11.521400094297,11.699843179837,11.867274762924]
[null,null,null,null,"Coincident",7.2917897868533998,7.6137150679471999,7.7967385559258,8.0166674731813004,8.1490124079852997,8.2761419039689006,8.3953682052245995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.89064317936,11.213027887638001,11.518903041001,11.919079528728,12.114260586181,12.30188587654,12.477933041924]
[null,null,null,null,"Coincident",7.6670058234778002,8.0054965201405999,8.1979379082200001,8.4291837804459,8.5683388322932998,8.7020100727614995,8.8273714411990998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.8500002472769008,10.129280201676,10.391298473725,10.745836954152001,10.932766490076,11.104153485648,11.261438343478]
[null,null,null,null,"Coincident",6.9501512136250998,7.2512703728489001,7.4160167649673001,7.6214645454759999,7.7548688814020004,7.8770956171286004,7.9891836262866001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.35685496492,10.650505920220001,10.926006953079,11.298789037249,11.495337468074,11.675543580912001,11.840921897646]
[null,null,null,null,"Coincident",7.3077874412927999,7.6244013885972999,7.7976251902552001,8.0136447650953997,8.1539137320184008,8.2824299292750005,8.4002856881594994]
[null,"Golden Grove 11kV","Substation Rating","MVA","Non-Coincident",87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004]
[null,null,null,null,"Coincident",87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004,87.662995644239004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.551142105826003,50.226147381632003,51.939267331792003,54.930232222575,56.171065883033997,57.429770331912998,58.729170561734001]
[null,null,null,null,"Coincident",47.139645558067997,48.289085891077001,49.717555432475002,51.442350787107003,52.658653222844002,53.895077953302,55.172292504745997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.339475431864997,51.025219696351002,52.765594508676003,55.804144121024997,57.064718810350001,58.343448603196997,59.663521626045998]
[null,null,null,null,"Coincident",47.889613207486001,49.057340548267,50.508536309423,52.260772275931998,53.496425461297001,54.752521076798999,56.050055458475001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.092670913604998,43.508432053452999,44.76077416711,47.213301839779,48.211926090298,49.326290231592999,50.445007010899999]
[null,null,null,null,"Coincident",41.083538624269003,41.975855648222002,42.973702727754002,44.341959516694999,45.345485616792999,46.462475465817,47.587837576159998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.778253266412001,44.200628953337997,45.472895189463998,47.964441322965001,48.978953174524001,50.111046279321997,51.247561270376004]
[null,null,null,null,"Coincident",41.737156710002999,42.643670041396,43.657392357576001,45.047417412180003,46.066909099238003,47.201669685432002,48.344935731341003]
[null,"Gomersal North 11kV","Substation Rating","MVA","Non-Coincident",0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002]
[null,null,null,null,"Coincident",0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002,0.71250000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.26054767575898002,0.26287727311176001,0.26860372755202,0.27862501036379,0.28289053670848002,0.28713608027942,0.29128588146994999]
[null,null,null,null,"Coincident",0.12817265252834001,0.12988742546075999,0.13267976301893999,0.1361738327407,0.13825630040692,0.14032879673616,0.14235382023203999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.26847369440919,0.2708741595293,0.27677481619401001,0.28710095251957002,0.29149623876813002,0.29587093435481998,0.30014697501970999]
[null,null,null,null,"Coincident",0.13207174251802001,0.13383867988522999,0.13671596204903999,0.14031632349532999,0.14246214109361999,0.14459768402081,0.14668430996217999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.23697836263857,0.23867398914603999,0.24345097448947001,0.25221625162632999,0.25646283371491002,0.26049183583851998,0.26435543695937003]
[null,null,null,null,"Coincident",0.11580071620989001,0.11705806158746,0.11948458772715,0.12263796973324,0.12470455320142,0.12666527268583,0.12854500922322001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.24418738845888999,0.24593459695527001,0.25085690109615999,0.25988882329080998,0.26426458898749,0.26841615580440997,0.27239729001953999]
[null,null,null,null,"Coincident",0.11932344437744,0.12061903896558,0.12311938150521,0.12636869130847,0.12849814150176,0.13051850726455999,0.13245542652986]
[null,"Goolwa 11kV","Substation Rating","MVA","Non-Coincident",33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997]
[null,null,null,null,"Coincident",33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997,33.670542635658997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.658999226515,14.982376029809,15.488069745923999,16.172627459723,16.534119372694001,16.886396617062001,17.237198660259001]
[null,null,null,null,"Coincident",14.22844207787,14.643746443808,15.255790670727,15.840454267299,16.096125485561998,16.345648981187999,16.725721729976001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.701229941605,15.025538352401,15.532688907889,16.219218745523001,16.581752070785999,16.935044181157,17.286856840487999]
[null,null,null,null,"Coincident",14.269432412495,14.685933217568,15.299740666176,15.886088604317999,16.142496378891,16.392738720017999,16.773906410125999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.725910410711,13.021908472328001,13.637977436085,14.234718482338,14.548933167963,14.927830701773001,15.299794407468999]
[null,null,null,null,"Coincident",12.635581560318,13.020574217657,13.637977436085,14.234718482338,14.517752640302,14.786959144179001,15.186461512797001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.762572142423,13.059422936864999,13.677266717065001,14.275726898486999,14.590846796716001,14.970835886202,15.343871172095]
[null,null,null,null,"Coincident",12.671983066084,13.058084838375001,13.677266717065001,14.275726898486999,14.559576441916001,14.829558495541001,15.230211779746]
[null,"Gulnare 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.11270155998556,0.11466969961305,0.11732207057695999,0.12067012373859,0.12284925474793,0.12510571699011,0.12742040076488001]
[null,null,null,null,"Coincident",0.11270155998556,0.11466969961305,0.11732207057695999,0.12067012373859,0.12284925474793,0.12510571699011,0.12742040076488001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11510032621617999,0.11711035618552,0.11981918083029,0.12323849473457001,0.12546400687543,0.1277684961851,0.13013244622799999]
[null,null,null,null,"Coincident",0.11510032621617999,0.11711035618552,0.11981918083029,0.12323849473457001,0.12546400687543,0.1277684961851,0.13013244622799999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10109178252666,0.10269972596058,0.10506880191964001,0.10815145082897,0.11035693017264001,0.11255376028915,0.11477728785765]
[null,null,null,null,"Coincident",0.10109178252666,0.10269972596058,0.10506880191964001,0.10815145082897,0.11035693017264001,0.11255376028915,0.11477728785765]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10324344355201,0.10488561082818,0.10730511075129,0.1104533714774,0.11270579275668,0.11494938071663,0.11722023436336]
[null,null,null,null,"Coincident",0.10324344355201,0.10488561082818,0.10730511075129,0.1104533714774,0.11270579275668,0.11494938071663,0.11722023436336]
[null,"Gumeracha 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.17123807269357,0.17463270140938,0.17901043570912001,0.18437418137888001,0.18786229548236,0.1913664975921,0.1948373973917]
[null,null,null,null,"Coincident",0.17123807269357,0.17463270140938,0.17901043570912001,0.18437418137888001,0.18786229548236,0.1913664975921,0.1948373973917]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.17475268429815,0.17821698678035999,0.1826845728025,0.18815840779106,0.19171811442132999,0.19529423925950001,0.1988363782673]
[null,null,null,null,"Coincident",0.17475268429815,0.17821698678035999,0.1826845728025,0.18815840779106,0.19171811442132999,0.19529423925950001,0.1988363782673]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.13271403411794,0.13528786122114,0.13881548678573999,0.14322264772102999,0.14639014781212001,0.14946259723561001,0.15247072500360001]
[null,null,null,null,"Coincident",0.13271403411794,0.13528786122114,0.13881548678573999,0.14322264772102999,0.14639014781212001,0.14946259723561001,0.15247072500360001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.13543795104285999,0.13806460519826,0.14166463425087999,0.14616225088171,0.14939476299029,0.15253027354397999,0.15560014225893001]
[null,null,null,null,"Coincident",0.13543795104285999,0.13806460519826,0.14166463425087999,0.14616225088171,0.14939476299029,0.15253027354397999,0.15560014225893001]
[null,"Gumeracha Weir 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.39000027166839002,0.3976131168889,0.40745788196581001,0.41954965505893999,0.42737565056652999,0.43524245875257001,0.44305925024823001]
[null,null,null,null,"Coincident",0.39000027166839002,0.3976131168889,0.40745788196581001,0.41954965505893999,0.42737565056652999,0.43524245875257001,0.44305925024823001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.39790081950257,0.40566788422545003,0.41571208259268,0.42804880841704002,0.43603334138305999,0.44405951380264003,0.45203465630369]
[null,null,null,null,"Coincident",0.39790081950257,0.40566788422545003,0.41571208259268,0.42804880841704002,0.43603334138305999,0.44405951380264003,0.45203465630369]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.34805051742512999,0.35468207904768001,0.36380766432178002,0.37524069684096001,0.38342758367117002,0.39136916191387,0.39916784239538999]
[null,null,null,null,"Coincident",0.34805051742512999,0.35468207904768001,0.36380766432178002,0.37524069684096001,0.38342758367117002,0.39136916191387,0.39916784239538999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.35510125549221999,0.36186715796942998,0.37117760753264001,0.38284224814767998,0.39119498330086999,0.39929744045402998,0.40725410505162002]
[null,null,null,null,"Coincident",0.35510125549221999,0.36186715796942998,0.37117760753264001,0.38284224814767998,0.39119498330086999,0.39929744045402998,0.40725410505162002]
[null,"Gumhaven 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.12722472810703001,0.12970732431167001,0.13291795999524,0.13686161744846001,0.1394137485727,0.14197922317471001,0.14452856529794]
[null,null,null,null,"Coincident",0.12722472810703001,0.12970732431167001,0.13291795999524,0.13686161744846001,0.1394137485727,0.14197922317471001,0.14452856529794]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.12981387673229,0.13234699621684001,0.13562297150137001,0.13964688627112001,0.14225095577942001,0.14486864031843,0.14746986406682]
[null,null,null,null,"Coincident",0.12981387673229,0.13234699621684001,0.13562297150137001,0.13964688627112001,0.14225095577942001,0.14486864031843,0.14746986406682]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.11324237606675,0.11539908927436,0.11836720399474,0.12208608060494,0.12474882447379999,0.12733178590225999,0.12986845942479999]
[null,null,null,null,"Coincident",0.11324237606675,0.11539908927436,0.11836720399474,0.12208608060494,0.12474882447379999,0.12733178590225999,0.12986845942479999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.11554697004526999,0.11774757449258,0.12077609327326,0.12457065268825999,0.12728758601956999,0.12992311325919001,0.13251141058836]
[null,null,null,null,"Coincident",0.11554697004526999,0.11774757449258,0.12077609327326,0.12457065268825999,0.12728758601956999,0.12992311325919001,0.13251141058836]
[null,"Hackham 11kV","Substation Rating","MVA","Non-Coincident",31.6,31.6,31.6,31.6,31.6,31.6,31.6]
[null,null,null,null,"Coincident",31.6,31.6,31.6,31.6,31.6,31.6,31.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.728425434489001,17.152179176743001,17.802390610456001,18.415597217197998,18.642902646888999,18.861123345225,19.226760657223]
[null,null,null,null,"Coincident",16.728425434489001,17.152179176743001,17.802390610456001,18.415597217197998,18.642902646888999,18.861123345225,19.226760657223]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.826892152848998,17.253140190848999,17.907178893682001,18.523994952041999,18.752638345059001,18.972143532250001,19.339933055547]
[null,null,null,null,"Coincident",16.826892152848998,17.253140190848999,17.907178893682001,18.523994952041999,18.752638345059001,18.972143532250001,19.339933055547]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.985642160496999,15.351866681520001,15.986187329409001,16.588611988221999,16.820186685673999,17.032733508191999,17.390873561583]
[null,null,null,null,"Coincident",14.985642160496999,15.351866681520001,15.986187329409001,16.588611988221999,16.820186685673999,17.032733508191999,17.390873561583]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.073850522475,15.442230711222001,16.080285092021001,16.686255737839002,16.919193528345001,17.132991442199,17.493239576587001]
[null,null,null,null,"Coincident",15.073850522475,15.442230711222001,16.080285092021001,16.686255737839002,16.919193528345001,17.132991442199,17.493239576587001]
[null,"Hahndorf 11kV","Substation Rating","MVA","Non-Coincident",6.9,6.9,6.9,6.9,6.9,6.9,6.9]
[null,null,null,null,"Coincident",6.9,6.9,6.9,6.9,6.9,6.9,6.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0256335175971998,5.1870218885905999,5.3790941045864997,5.5990333309339997,5.7659947621720997,5.9365470817626003,6.1103156900285001]
[null,null,null,null,"Coincident",5.0256335175971998,5.1870218885905999,5.3790941045864997,5.5990333309339997,5.7659947621720997,5.9365470817626003,6.1103156900285001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1547370790305997,5.3202713578775001,5.5172777193996003,5.7428669672461004,5.9141174727510002,6.0890511129835003,6.2672836651708996]
[null,null,null,null,"Coincident",5.1547370790305997,5.3202713578775001,5.5172777193996003,5.7428669672461004,5.9141174727510002,6.0890511129835003,6.2672836651708996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4741153221517997,4.6068636782079002,4.7470313606936001,4.9098921089010998,5.0675679626934,5.2218513757920002,5.3736375260548002]
[null,null,null,null,"Coincident",4.4741153221517997,4.6068636782079002,4.7470313606936001,4.9098921089010998,5.0675679626934,5.2218513757920002,5.3736375260548002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.5890509258585004,4.7252094560710001,4.8689779078811997,5.0360223878586003,5.1977487786041996,5.3559955802052999,5.5116809667546001]
[null,null,null,null,"Coincident",4.5890509258585004,4.7252094560710001,4.8689779078811997,5.0360223878586003,5.1977487786041996,5.3559955802052999,5.5116809667546001]
[null,"Halbury 11kV","Substation Rating","MVA","Non-Coincident",0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998]
[null,null,null,null,"Coincident",0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.11270155998556,0.11466969961305,0.11732207057695999,0.12067012373859,0.12284925474793,0.12510571699011,0.12742040076488001]
[null,null,null,null,"Coincident",0.11270155998556,0.11466969961305,0.11732207057695999,0.12067012373859,0.12284925474793,0.12510571699011,0.12742040076488001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11512068305412999,0.11713106852076,0.11984037225282999,0.12326029090274,0.12548619665144001,0.12779109353698001,0.13015546167207001]
[null,null,null,null,"Coincident",0.11512068305412999,0.11713106852076,0.11984037225282999,0.12326029090274,0.12548619665144001,0.12779109353698001,0.13015546167207001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10119287430918,0.10280242568653999,0.10517387072155999,0.1082596022798,0.11046728710280999,0.11266631404944,0.11489206514550999]
[null,null,null,null,"Coincident",0.10119287430918,0.10280242568653999,0.10517387072155999,0.1082596022798,0.11046728710280999,0.11266631404944,0.11489206514550999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10336496506504,0.1050090652354,0.10743141300318999,0.11058337935354,0.11283845181949,0.11508468056896,0.11735820709797]
[null,null,null,null,"Coincident",0.10336496506504,0.1050090652354,0.10743141300318999,0.11058337935354,0.11283845181949,0.11508468056896,0.11735820709797]
[null,"Hamley Bridge 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4440456375752002,2.5012060435887,2.5723932280844002,2.6578363253284998,2.7162657901544001,2.7748493827019001,2.8329958861204001]
[null,null,null,null,"Coincident",2.4440456375752002,2.5012060435887,2.5723932280844002,2.6578363253284998,2.7162657901544001,2.7748493827019001,2.8329958861204001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4801637527015998,2.5381688753985001,2.6104080643599001,2.697113839999,2.7564067756639998,2.8158561167506,2.8748619094033998]
[null,null,null,null,"Coincident",2.4801637527015998,2.5381688753985001,2.6104080643599001,2.697113839999,2.7564067756639998,2.8158561167506,2.8748619094033998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2025935278194,2.2561186786162,2.3134005533995001,2.3921236487378001,2.4502534803540001,2.5067337453178999,2.5621742030619998]
[null,null,null,null,"Coincident",2.2025935278194,2.2561186786162,2.3134005533995001,2.3921236487378001,2.4502534803540001,2.5067337453178999,2.5621742030619998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2351434628089,2.2894596084745999,2.3475879950072001,2.4274744605284999,2.4864633350031,2.5437782655235002,2.6000380225494002]
[null,null,null,null,"Coincident",2.2351434628089,2.2894596084745999,2.3475879950072001,2.4274744605284999,2.4864633350031,2.5437782655235002,2.6000380225494002]
[null,"Happy Valley 11kV","Substation Rating","MVA","Non-Coincident",59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002]
[null,null,null,null,"Coincident",59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002,59.671082686158002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.262354602199999,40.427682369932,42.137886060436998,43.773077073137998,44.499395748011999,45.208444682366,46.275543208799]
[null,null,null,null,"Coincident",39.262354602199999,40.427682369932,42.137886060436998,43.773077073137998,44.499395748011999,45.208444682366,46.275543208799]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.824331747814,41.006339298999002,42.741021791097999,44.399617920152998,45.136332672895001,45.855530496694001,46.937902813760999]
[null,null,null,null,"Coincident",39.824331747814,41.006339298999002,42.741021791097999,44.399617920152998,45.136332672895001,45.855530496694001,46.937902813760999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.825305591025,35.813507875345003,37.436564617122997,38.996069736513,39.691369850050002,40.345816270865001,41.349267529704001]
[null,null,null,null,"Coincident",34.825305591025,35.813507875345003,37.436564617122997,38.996069736513,39.691369850050002,40.345816270865001,41.349267529704001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.323773551734,36.326120354502002,37.972408530160997,39.554235444676003,40.259487655511002,40.923301419045998,41.941115460756002]
[null,null,null,null,"Coincident",35.323773551734,36.326120354502002,37.972408530160997,39.554235444676003,40.259487655511002,40.923301419045998,41.941115460756002]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Harrow 11kV","Substation Rating","MVA","Non-Coincident",30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998]
[null,null,null,null,"Coincident",30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998,30.491403785488998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.367222524744999,21.839478186026,22.434432452951,23.158764845993002,23.64996601647,24.146388916608998,24.656807286923001]
[null,null,null,null,"Coincident",21.367222524744999,21.839478186026,22.434432452951,23.158764845993002,23.64996601647,24.146388916608998,24.656807286923001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.848855626830002,22.331756282276999,22.940121261280002,23.680780645675,24.183053856198001,24.690666498058,25.212590078409001]
[null,null,null,null,"Coincident",21.848855626830002,22.331756282276999,22.940121261280002,23.680780645675,24.183053856198001,24.690666498058,25.212590078409001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.34029992684,18.717612549216,19.14044145766,19.726263878251999,20.147765642081001,20.617651722695999,21.088786661913002]
[null,null,null,null,"Coincident",18.34029992684,18.717612549216,19.14044145766,19.726263878251999,20.147765642081001,20.617651722695999,21.088786661913002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.753703940240001,19.139521470005999,19.571881256813001,20.170908550867999,20.601911278231999,21.0823889409,21.564143612374]
[null,null,null,null,"Coincident",18.753703940240001,19.139521470005999,19.571881256813001,20.170908550867999,20.601911278231999,21.0823889409,21.564143612374]
[null,"Hatherleigh 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.2891106631946002E-2,8.4819321380374998E-2,8.7274807537557994E-2,9.0224027235912996E-2,9.2266004778048999E-2,9.4323061805084998E-2,9.6384496830850999E-2]
[null,null,null,null,"Coincident",8.2891106631946002E-2,8.4819321380374998E-2,8.7274807537557994E-2,9.0224027235912996E-2,9.2266004778048999E-2,9.4323061805084998E-2,9.6384496830850999E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3304870039228998E-2,8.5242709761153002E-2,8.7710452846251993E-2,9.0674394017643004E-2,9.2726564397344002E-2,9.4793889533458006E-2,9.6865614521740001E-2]
[null,null,null,null,"Coincident",8.3304870039228998E-2,8.5242709761153002E-2,8.7710452846251993E-2,9.0674394017643004E-2,9.2726564397344002E-2,9.4793889533458006E-2,9.6865614521740001E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8193758166236998E-2,7.9849528149626994E-2,8.2067868174276998E-2,8.4810960090938997E-2,8.6825902944416999E-2,8.8785006138039996E-2,9.0709124888143006E-2]
[null,null,null,null,"Coincident",7.8193758166236998E-2,7.9849528149626994E-2,8.2067868174276998E-2,8.4810960090938997E-2,8.6825902944416999E-2,8.8785006138039996E-2,9.0709124888143006E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.8584074053208997E-2,8.0248109061132999E-2,8.2477522263165001E-2,8.5234306735085003E-2,8.7259307478417994E-2,8.9228189829848994E-2,9.1161913107654993E-2]
[null,null,null,null,"Coincident",7.8584074053208997E-2,8.0248109061132999E-2,8.2477522263165001E-2,8.5234306735085003E-2,8.7259307478417994E-2,8.9228189829848994E-2,9.1161913107654993E-2]
[null,"Hawker 11kV","Substation Rating","MVA","Non-Coincident",1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615]
[null,null,null,null,"Coincident",1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615,1.1224615384615]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.93134126456490995,0.93986030311271995,0.95330806406285995,0.97153204127422998,0.97945877667698,0.98716265550426996,0.99437915758536]
[null,null,null,null,"Coincident",0.93134126456490995,0.93986030311271995,0.95330806406285995,0.97153204127422998,0.97945877667698,0.98716265550426996,0.99437915758536]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.94911634980659998,0.95779797820427004,0.97150239598502997,0.99007418635652,0.99815220722554998,1.0060031181968001,1.0133573506078]
[null,null,null,null,"Coincident",0.94911634980659998,0.95779797820427004,0.97150239598502997,0.99007418635652,0.99815220722554998,1.0060031181968001,1.0133573506078]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.87307060055122998,0.88134173361238999,0.89552696776692997,0.91497657826237999,0.92614945585897002,0.93640855923820998,0.94592104093853002]
[null,null,null,null,"Coincident",0.87307060055122998,0.88134173361238999,0.89552696776692997,0.91497657826237999,0.92614945585897002,0.93640855923820998,0.94592104093853002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.88973356281573002,0.89816255433416003,0.91261852034163005,0.93243933578378002,0.94382545299428,0.95428035617753004,0.96397438805663005]
[null,null,null,null,"Coincident",0.88973356281573002,0.89816255433416003,0.91261852034163005,0.93243933578378002,0.94382545299428,0.95428035617753004,0.96397438805663005]
[null,"Hay Flat 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7443916724016996E-2,8.9648817031265995E-2,9.3089857612718999E-2,9.6337837986695998E-2,9.7566873586809003E-2,9.8747015047396997E-2,0.10068907587444]
[null,null,null,null,"Coincident",8.7443916724016996E-2,8.9648817031265995E-2,9.3089857612718999E-2,9.6337837986695998E-2,9.7566873586809003E-2,9.8747015047396997E-2,0.10068907587444]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7933763710534005E-2,9.0151015520455E-2,9.3611332266821001E-2,9.6877507312971997E-2,9.8113427776064993E-2,9.9300180202398003E-2,0.10125312014693]
[null,null,null,null,"Coincident",8.7933763710534005E-2,9.0151015520455E-2,9.3611332266821001E-2,9.6877507312971997E-2,9.8113427776064993E-2,9.9300180202398003E-2,0.10125312014693]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.3465199684302993E-2,8.5603168408631997E-2,8.9245102370900997E-2,9.2713104722722997E-2,9.4110542818223994E-2,9.5400679228977006E-2,9.7491977762025006E-2]
[null,null,null,null,"Coincident",8.3465199684302993E-2,8.5603168408631997E-2,8.9245102370900997E-2,9.2713104722722997E-2,9.4110542818223994E-2,9.5400679228977006E-2,9.7491977762025006E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.3932758527458004E-2,8.6082703814320996E-2,8.9745039314437003E-2,9.3232468866741997E-2,9.4637735189358002E-2,9.5935098740164995E-2,9.8038112396719002E-2]
[null,null,null,null,"Coincident",8.3932758527458004E-2,8.6082703814320996E-2,8.9745039314437003E-2,9.3232468866741997E-2,9.4637735189358002E-2,9.5935098740164995E-2,9.8038112396719002E-2]
[null,"Henley South 11kV","Substation Rating","MVA","Non-Coincident",57.074810505258,57.074810505258,57.074810505258,57.074810505258,57.074810505258,57.074810505258,57.074810505258]
[null,null,null,null,"Coincident",57.074810505258,57.074810505258,57.074810505258,57.074810505258,57.074810505258,57.074810505258,57.074810505258]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.685563453184997,36.35984610061,37.464320043295999,39.205762417003001,39.976556945685999,40.844491261218003,41.696485484325002]
[null,null,null,null,"Coincident",35.296102870542001,36.040461252630998,36.932586440263002,38.069080067587997,38.771091287226,39.582051044521997,40.375715582687]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.429711519584998,37.118054926592002,38.245560371916,40.023316897615999,40.810184740059,41.696218017192002,42.565978804488999]
[null,null,null,null,"Coincident",36.032129548024002,36.792009973123001,37.702738572587002,38.862931406354001,39.579581607168997,40.407452240373999,41.217666998692003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.787259689113998,31.281620529796999,32.029299304996997,33.251099232717003,33.875174998765999,34.586986540222,35.269631746876001]
[null,null,null,null,"Coincident",30.698181143315001,31.275747251148001,31.824791110553999,32.589522476307998,33.160280700161003,33.829734478005001,34.470852823400001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.429263837303001,31.933933543197998,32.697203601288003,33.944481620586998,34.581571186326002,35.308226074250001,36.005106424234]
[null,null,null,null,"Coincident",31.338327744048001,31.927937789562002,32.488430814592,33.269109059477003,33.851769256777999,34.535183098190998,35.189670630755998]
[null,"Hermitage 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.13686726401058999,0.13681998384061,0.13792566430021999,0.14069617659688,0.14115322132111999,0.14158180430024001,0.14195721997013]
[null,null,null,null,"Coincident",0.12298721787402001,0.12349864897637999,0.12464210453026001,0.12639976454068,0.12687252401637,0.12731791992194,0.12771308834610001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.14257008080056,0.14252083061862,0.14367258121147,0.14655853180638001,0.14703462010794999,0.14748106075542,0.14787211878362999]
[null,null,null,null,"Coincident",0.12811169797607,0.12864443876046999,0.12983553841375001,0.13166643443930001,0.13215889227526001,0.13262284638951999,0.13303448020545999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.12345182119355,0.12410145222522,0.12590572286866,0.12944750772845001,0.13104014830523,0.13251265192077999,0.13391007045414999]
[null,null,null,null,"Coincident",0.11090686252736,0.11197935784632999,0.11379925224781,0.11632685685676999,0.11783404189558,0.11923243240233,0.12056173912587]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.12859565981519,0.12927235887353999,0.13115180764664,0.13484116724104001,0.13650016800619999,0.13803402609101001,0.1394896705408]
[null,null,null,null,"Coincident",0.11552799324342999,0.11664517597802999,0.11854089950068,0.12117382122917,0.12274380580012,0.12420046272228,0.12558515736313999]
[null,"Hillcrest 11kV","Substation Rating","MVA","Non-Coincident",59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998]
[null,null,null,null,"Coincident",59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998,59.685440613026998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.362205072613001,40.117213589557998,41.089275921911998,42.288145996913997,43.051416678297002,43.815236041664001,44.594801969891002]
[null,null,null,null,"Coincident",39.362205072613001,40.117213589557998,41.089275921911998,42.288145996913997,43.051416678297002,43.815236041664001,44.594801969891002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.942065743862997,40.708196598712,41.694578777107999,42.911109895366003,43.685624627960998,44.460696125398002,45.251746156753001]
[null,null,null,null,"Coincident",39.942065743862997,40.708196598712,41.694578777107999,42.911109895366003,43.685624627960998,44.460696125398002,45.251746156753001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.816613230820998,35.415598259977997,36.091921437880998,37.064789023403002,37.717625665941,38.449996651233,39.172346599980003]
[null,null,null,null,"Coincident",34.816613230820998,35.415598259977997,36.091921437880998,37.064789023403002,37.717625665941,38.449996651233,39.172346599980003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.329510937679999,35.937319859208998,36.623606229246001,37.610805523323002,38.273259368277998,39.016419208774998,39.749410388759003]
[null,null,null,null,"Coincident",35.329510937679999,35.937319859208998,36.623606229246001,37.610805523323002,38.273259368277998,39.016419208774998,39.749410388759003]
[null,"Hindley Street 11kV","Substation Rating","MVA","Non-Coincident",79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002]
[null,null,null,null,"Coincident",79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002,79.988345477129002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.661623690535997,42.220472503914998,41.776695301208001,41.365240452691999,41.020473688905,40.709967104763997,40.446061977847002]
[null,null,null,null,"Coincident",42.614315100168,42.169060293728002,41.747998589487999,41.365240452691999,41.020473688905,40.709967104763997,40.446061977847002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.170697779287003,42.724282408632,42.275209686075002,41.858845015008001,41.509964206536999,41.195752398762998,40.928698135681998]
[null,null,null,null,"Coincident",43.122824663347998,42.672256705057002,42.246170541247999,41.858845015008001,41.509964206536999,41.195752398762998,40.928698135681998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.096162812229998,39.664066350862001,39.217152224475001,38.782272994872997,38.420968200733,38.088172879515,37.792961414521002]
[null,null,null,null,"Coincident",39.955727773901998,39.511723847246998,39.093325010911002,38.706578931639001,38.347301148885997,38.016598663293998,37.723477901624001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.574623681280997,40.137371084415001,39.685124005787003,39.245055434374002,38.879439249975,38.542672737314,38.243938562808999]
[null,null,null,null,"Coincident",40.432512854902001,39.983210702938997,39.559819182595,39.168458126422003,38.804893141400001,38.470244437828001,38.173625914662999]
[null,"Holden Hill 11kV","Substation Rating","MVA","Non-Coincident",46.713043478261,46.713043478261,46.713043478261,46.713043478261,46.713043478261,46.713043478261,46.713043478261]
[null,null,null,null,"Coincident",46.713043478261,46.713043478261,46.713043478261,46.713043478261,46.713043478261,46.713043478261,46.713043478261]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.126391184957001,39.768663269309997,40.618131086970998,41.682375257430003,42.308020336569001,42.925863814945998,43.550776689804003]
[null,null,null,null,"Coincident",39.126391184957001,39.768663269309997,40.618131086970998,41.682375257430003,42.308020336569001,42.925863814945998,43.550776689804003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.941697653574003,40.597353251435003,41.464522078201,42.550942716515003,43.189624839567998,43.820342793950999,44.458277455222998]
[null,null,null,null,"Coincident",39.941697653574003,40.597353251435003,41.464522078201,42.550942716515003,43.189624839567998,43.820342793950999,44.458277455222998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.557505819970999,35.063559338295001,35.639420095737997,36.500098597602999,37.037200686508001,37.644166510569001,38.232794415796]
[null,null,null,null,"Coincident",34.557505819970999,35.063559338295001,35.639420095737997,36.500098597602999,37.037200686508001,37.644166510569001,38.232794415796]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.277606937937001,35.794205479567999,36.382065887026002,37.260679003577003,37.808973098545998,38.428586732629,39.029480326672001]
[null,null,null,null,"Coincident",35.277606937937001,35.794205479567999,36.382065887026002,37.260679003577003,37.808973098545998,38.428586732629,39.029480326672001]
[null,"Hope Valley 11kV","Substation Rating","MVA","Non-Coincident",29.1,29.1,29.1,29.1,29.1,29.1,29.1]
[null,null,null,null,"Coincident",29.1,29.1,29.1,29.1,29.1,29.1,29.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.345640003873999,19.473998619465998,20.002084646242999,21.017988339184999,21.365477902498,21.729033086983002,22.120797927858]
[null,null,null,null,"Coincident",18.639173488350998,18.962044329044002,19.390995849227,19.934778903695999,20.285260964359999,20.652057767262001,21.046450209837001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.666107055803,19.796591975157,20.333425925090999,21.366158405370001,21.719404250507001,22.088981849250001,22.487236406855001]
[null,null,null,null,"Coincident",18.947937684159999,19.276156989233002,19.712214236032001,20.265005240215999,20.621293154431999,20.994166070095002,21.395091756509]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.521370276498001,16.585849027542999,16.979591006151001,17.841460737561999,18.173395477562998,18.575808811736,19.012096985673999]
[null,null,null,null,"Coincident",15.952229912061,16.205959082142002,16.509857164275001,16.970389921972,17.311175436525001,17.720767531913001,18.164301836903999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.79505234777,16.860599211075002,17.260863658365999,18.137010552585998,18.474443903516999,18.883523350303999,19.327038785001999]
[null,null,null,null,"Coincident",16.216483981225998,16.474416260590999,16.783348516958998,17.251510155123999,17.597940896672,18.014318023276001,18.465199623632]
[null,"Houghton 7.6kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1945587273778999,2.2251367193174998,2.2751328196184999,2.3537310433676999,2.3934534639697,2.4330822000704999,2.4719976498131002]
[null,null,null,null,"Coincident",2.0459195534040999,2.0837726166722002,2.1330812511369999,2.1938238760958999,2.2319410926013998,2.2699684851679001,2.3073152105968]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2940998890875002,2.3260648426985999,2.3783286744768999,2.4604919696012999,2.502016126399,2.5434423493381999,2.5841229325572002]
[null,null,null,null,"Coincident",2.1387187146066,2.1782887234478001,2.2298339071996001,2.2933317062982002,2.3331778498836,2.3729300952807,2.4119707997263999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9233564980558,1.9443745171035001,1.9837596556985,2.0503030343851001,2.0857900238534999,2.1195230841263002,2.1519673446391998]
[null,null,null,null,"Coincident",1.7926754116226999,1.8202120447418999,1.860218441307,1.9115484450425,1.9458884448802001,1.9785916118341,2.0100779364145001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0105964237,2.0325677815700001,2.0737393578671002,2.1433010222508999,2.1803976365214002,2.2156607665825998,2.2495766392888998]
[null,null,null,null,"Coincident",1.8739878826972001,1.9027735270259001,1.9445945404158,1.9982527790436999,2.0341503783361001,2.0683369010049999,2.1012513875605001]
[null,"Hoyleton 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.11022526298139,0.11142344495232,0.11409875960042,0.11876663596361001,0.12091639339632,0.12314068054098,0.12542059845562001]
[null,null,null,null,"Coincident",8.7684082504078997E-2,8.9215334755583006E-2,9.1278932761334003E-2,9.3883785521933993E-2,9.5579193316059005E-2,9.7334766366127007E-2,9.9135636940618999E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11023435855164,0.11143263939417,0.11410817480394,0.11877643635104,0.12092637117747,0.1231508418659,0.12543094791484]
[null,null,null,null,"Coincident",8.7691318020793996E-2,8.9222696628197998E-2,9.1286464917967006E-2,9.3891532625855006E-2,9.5587080321671E-2,9.7342798238147996E-2,9.9143817416911001E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10033293637314999,0.10137395037664999,0.10379280279516,0.10811170302530999,0.11032149331171,0.11252111118792001,0.11474579721634]
[null,null,null,null,"Coincident",7.8730093362396003E-2,7.9982356736435001E-2,8.1827388714087998E-2,8.4228149986359996E-2,8.5945773222354999E-2,8.7656660456225999E-2,8.9388339616357004E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10034121564822,0.10138231555413001,0.10380136757154999,0.10812062418879,0.11033059682269999,0.11253039620702,0.11475526581212001]
[null,null,null,null,"Coincident",7.8736590013672003E-2,7.9988956722002E-2,8.1834140948037995E-2,8.4235100326372006E-2,8.5952865297233005E-2,8.7663893710128005E-2,8.9395715764991002E-2]
[null,"Ingle Farm 11kV","Substation Rating","MVA","Non-Coincident",54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002]
[null,null,null,null,"Coincident",54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002,54.434679994447002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.606218930925998,39.451185486104997,40.517108339137998,41.816104167563999,42.693567225208,43.579964575218,44.491624912700999]
[null,null,null,null,"Coincident",38.606218930925998,39.451185486104997,40.517108339137998,41.816104167563999,42.693567225208,43.579964575218,44.491624912700999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.240346478376999,40.099192055749,41.182623254931002,42.502955776295003,43.394831628357998,44.295788523258999,45.222423363554]
[null,null,null,null,"Coincident",39.240346478376999,40.099192055749,41.182623254931002,42.502955776295003,43.394831628357998,44.295788523258999,45.222423363554]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.960185750036999,34.648369675371001,35.419953159210003,36.492317531509002,37.259801061818997,38.115908617122003,38.973818152969002]
[null,null,null,null,"Coincident",33.960185750036999,34.648369675371001,35.419953159210003,36.492317531509002,37.259801061818997,38.115908617122003,38.973818152969002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.517999747288997,35.217487457269002,36.001744607573002,37.09172313138,37.871812984253999,38.741982558563002,39.613983711899998]
[null,null,null,null,"Coincident",34.517999747288997,35.217487457269002,36.001744607573002,37.09172313138,37.871812984253999,38.741982558563002,39.613983711899998]
[null,"Inverness 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.70081852455131999,0.70563931478835995,0.71728774327042,0.73849643848074997,0.74615796248470001,0.75367469389198005,0.76083960219478997]
[null,null,null,null,"Coincident",9.0039426612847001E-2,9.1064737733209999E-2,9.2572536172449996E-2,9.4550505307114993E-2,9.5531584421936003E-2,9.6493873371927996E-2,9.7409932930955997E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.80628670281917003,0.81183298752633004,0.82523442122821,0.84963487346108002,0.85844940206057996,0.86709734781263004,0.87534052359794001]
[null,null,null,null,"Coincident",0.10358971668718001,0.10476932980191,0.10650404112802001,0.10877968047828999,0.10990840498682,0.11101551154504,0.11206943151941]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.63722216620756,0.63984603998246004,0.64808687967157996,0.66466941704287996,0.67151272558747999,0.67767578044610999,0.68329604728991999]
[null,null,null,null,"Coincident",8.0496666947758005E-2,8.1102088442233003E-2,8.2248645646952001E-2,8.3873984818727002E-2,8.4736442826409006E-2,8.5512799661612002E-2,8.6219501235507007E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.73311954715198002,0.73613829517370999,0.74561932232785999,0.76469741303619998,0.77257059059859001,0.77966114115794005,0.78612721798624996]
[null,null,null,null,"Coincident",9.2610839907226003E-2,9.3307373008871E-2,9.4626478876938994E-2,9.6496419975617004E-2,9.7488671748327996E-2,9.8381864737578997E-2,9.9194919846613994E-2]
[null,"Jabuk 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7776164773010997E-2,7.8688639858202E-2,8.0587532988853003E-2,8.3811260335634005E-2,8.5128638325363007E-2,8.6462488605480003E-2,8.7796402555547007E-2]
[null,null,null,null,"Coincident",7.6980041492086995E-2,7.8245408629988994E-2,7.9939929343568999E-2,8.2072353123100003E-2,8.3372586238754001E-2,8.4688271149132993E-2,8.6003057037985997E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.9773096257001005E-2,8.0708999473821E-2,8.2656647380288994E-2,8.5963145106059E-2,8.7314347257619995E-2,8.8682444631651994E-2,9.0050607310383002E-2]
[null,null,null,null,"Coincident",7.8956532219586997E-2,8.0254388121674E-2,8.1992416274493995E-2,8.4179590814684999E-2,8.5513207891258006E-2,8.6862673493038001E-2,8.8211216990584998E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.4261284876828995E-2,7.5324293918609994E-2,7.6915537111040003E-2,7.8991977698297994E-2,8.0389726162912997E-2,8.1743389721828E-2,8.3070653519405999E-2]
[null,null,null,null,"Coincident",7.4261284876828995E-2,7.5324293918609994E-2,7.6915537111040003E-2,7.8991977698297994E-2,8.0389726162912997E-2,8.1743389721828E-2,8.3070653519405999E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.6167970533610005E-2,7.7258272721427004E-2,7.8890371664959005E-2,8.1020125623934E-2,8.2453761791727004E-2,8.3842181157738005E-2,8.5203522938882004E-2]
[null,null,null,null,"Coincident",7.6167970533610005E-2,7.7258272721427004E-2,7.8890371664959005E-2,8.1020125623934E-2,8.2453761791727004E-2,8.3842181157738005E-2,8.5203522938882004E-2]
[null,"Jamestown 11kV","Substation Rating","MVA","Non-Coincident",4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999]
[null,null,null,null,"Coincident",4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999,4.1116880430284999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6197610935815998,2.6613512553890999,2.7172986938063,2.8029122192968998,2.8304657573090002,2.8573053249693001,2.8829117014986001]
[null,null,null,null,"Coincident",2.2334670050729,2.2682267246276999,2.3037965028067999,2.3508879937430001,2.3730070727861001,2.3945015266317999,2.4149258102801001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6994490578486001,2.7423043103303,2.7999535594523999,2.8881712794921999,2.9165629417736998,2.9442189161336998,2.9706041881215]
[null,null,null,null,"Coincident",2.3014046652389002,2.3372217068894998,2.3738734475496002,2.4223973687392002,2.4451892665308002,2.4673375392587,2.4883830893230998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3301710671473002,2.3621851324454002,2.4120384135495998,2.4898612005340999,2.5126017071203002,2.5326365319124,2.5507528863295001]
[null,null,null,null,"Coincident",2.0505686917518,2.0633443521553998,2.0896311053718999,2.1279007300166999,2.1466280012469001,2.1630231976040002,2.1777508900643001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4010502741063,2.4340381441141998,2.4854078636803001,2.5655978663179,2.5890300942526001,2.6096743388907,2.6283417570696002]
[null,null,null,null,"Coincident",2.1129429460438001,2.1261072168333,2.1531935612248998,2.1926272723540001,2.2119241902304001,2.2288180961165001,2.2439937759272]
[null,"James Well 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.46298596316613,0.47572968920535003,0.49125888196959999,0.50973236295672997,0.52323205496744996,0.53782450601559995,0.55251091782418005]
[null,null,null,null,"Coincident",0.46298596316613,0.47572968920535003,0.49125888196959999,0.50973236295672997,0.52323205496744996,0.53782450601559995,0.55251091782418005]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.46524153130697998,0.47804734204150001,0.49365218969648,0.51221566951398001,0.52578112912379005,0.54044467145829,0.55520263230985001]
[null,null,null,null,"Coincident",0.46524153130697998,0.47804734204150001,0.49365218969648,0.51221566951398001,0.52578112912379005,0.54044467145829,0.55520263230985001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.44556272152861998,0.45731129555522998,0.47354645045926003,0.49302338154353997,0.50847687248091999,0.52377877239643,0.53899207333073995]
[null,null,null,null,"Coincident",0.44556272152861998,0.45731129555522998,0.47354645045926003,0.49302338154353997,0.50847687248091999,0.52377877239643,0.53899207333073995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.44773340737957001,0.45953921793467001,0.47585346702530001,0.49542528553324,0.51095406255831,0.52633051004261999,0.54161792691054]
[null,null,null,null,"Coincident",0.44773340737957001,0.45953921793467001,0.47585346702530001,0.49542528553324,0.51095406255831,0.52633051004261999,0.54161792691054]
[null,"Jervois 11kV","Substation Rating","MVA","Non-Coincident",4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004]
[null,null,null,null,"Coincident",4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5737138297409001,2.6602449098130001,2.7759205867261998,2.9321306414900001,3.0141116842154001,3.0865180494623998,3.1473690206786999]
[null,null,null,null,"Coincident",2.0678006389286998,2.1472629826049001,2.2352171898276998,2.3307442541508001,2.3962036170630001,2.4540372386542999,2.5026586922441001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.7717355785947002,2.8649243669200999,2.9895001397094001,3.1577290086379,3.2460176793776001,3.3239949961845001,3.3895278460154001]
[null,null,null,null,"Coincident",2.2268973862321002,2.3124735690154998,2.4071949800088999,2.5100719043363999,2.5805677158906999,2.6428510609739999,2.6952134531098002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4582046616944,2.5569482553945999,2.6839508014237001,2.8515185023174001,2.9351185626188001,3.0070525489262998,3.0667982833469001]
[null,null,null,null,"Coincident",2.2097521635861002,2.2896740501759001,2.3815674355616001,2.4831575378760999,2.5563250460633,2.6193178763309,2.6716693238728002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6473391258776999,2.7536800596109998,2.8904541917361,3.0709145650003,3.1609468206584999,3.2384154136521999,3.3027579896796002]
[null,null,null,null,"Coincident",2.3797706726021999,2.4658417555678001,2.5648054254086001,2.6742118783577999,2.7530089005037999,2.8208484041934998,2.8772277763155998]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kadina 11kV","Substation Rating","MVA","Non-Coincident",17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002]
[null,null,null,null,"Coincident",17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002,17.360319270240002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9750562042297997,9.1566018905785,9.3639982521288996,9.6218448390721001,9.6902316460706004,9.7568454903999999,9.8193378723386999]
[null,null,null,null,"Coincident",8.9350058495175997,9.1566018905785,9.3639982521288996,9.6218448390721001,9.6902316460706004,9.7568454903999999,9.8193378723386999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.1734443244457005,9.3590029669953001,9.5709836980885008,9.8345298259062996,9.9044282813869007,9.9725145839445997,10.03638832171]
[null,null,null,null,"Coincident",9.1325086811731992,9.3590029669953001,9.5709836980885008,9.8345298259062996,9.9044282813869007,9.9725145839445997,10.03638832171]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8891930788878,8.0930679686851992,8.2943416705226003,8.5414646853608005,8.6179872706852994,8.6844372890518002,8.7447612668070995]
[null,null,null,null,"Coincident",7.8891930788878,8.0930679686851992,8.2943416705226003,8.5414646853608005,8.6179872706852994,8.6844372890518002,8.7447612668070995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.0635788598039007,8.2719602791678994,8.4776830129053007,8.7302685306247998,8.8084826008281993,8.8764014561504005,8.9380588584857996]
[null,null,null,null,"Coincident",8.0635788598039007,8.2719602791678994,8.4776830129053007,8.7302685306247998,8.8084826008281993,8.8764014561504005,8.9380588584857996]
[null,"Kalangadoo 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.63064369321534997,0.64587901743373,0.66517523835801995,0.68824525076997001,0.70440621734747999,0.72068432083064005,0.73690404020418998]
[null,null,null,null,"Coincident",0.63064369321534997,0.64587901743373,0.66517523835801995,0.68824525076997001,0.70440621734747999,0.72068432083064005,0.73690404020418998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.63372248575284995,0.64903218858314005,0.66842261335284003,0.69160525320055999,0.70784511736135003,0.72420269028828999,0.74050159407534]
[null,null,null,null,"Coincident",0.63372248575284995,0.64903218858314005,0.66842261335284003,0.69160525320055999,0.70784511736135003,0.72420269028828999,0.74050159407534]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.56466450167142002,0.57662139637094001,0.59264080628207005,0.61244963330976998,0.62700024104287999,0.64114761104393003,0.65504234613100998]
[null,null,null,null,"Coincident",0.56466450167142002,0.57662139637094001,0.59264080628207005,0.61244963330976998,0.62700024104287999,0.64114761104393003,0.65504234613100998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.56742118483917003,0.57943645290953005,0.59553406932651998,0.61543960273453002,0.6300612463045,0.64427768354216997,0.65824025250621998]
[null,null,null,null,"Coincident",0.56742118483917003,0.57943645290953005,0.59553406932651998,0.61543960273453002,0.6300612463045,0.64427768354216997,0.65824025250621998]
[null,"Kalangadoo West 11kV","Substation Rating","MVA","Non-Coincident",1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999]
[null,null,null,null,"Coincident",1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999,1.2925287356321999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.87869322635244995,0.89982050246864997,0.92658263426384002,0.95862427292128005,0.98106182725909996,1.0036867547334001,1.0263583487229999]
[null,null,null,null,"Coincident",0.87869322635244995,0.89982050246864997,0.92658263426384002,0.95862427292128005,0.98106182725909996,1.0036867547334001,1.0263583487229999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.92201410004022,0.94418298206909002,0.97226452648331996,1.0058858652447,1.0294296241465,1.0531699939571,1.0769593310112]
[null,null,null,null,"Coincident",0.92201410004022,0.94418298206909002,0.97226452648331996,1.0058858652447,1.0294296241465,1.0531699939571,1.0769593310112]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.78708482933532997,0.80555409073219997,0.82976948966830999,0.85943087819381003,0.88184545873328002,0.90381092099493998,0.92563636728484999]
[null,null,null,null,"Coincident",0.78708482933532997,0.80555409073219997,0.82976948966830999,0.85943087819381003,0.88184545873328002,0.90381092099493998,0.92563636728484999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.82588927376554,0.84526909702413999,0.87067835088839995,0.90180208967129005,0.92532174213256002,0.94837013412167004,0.97127160714486005]
[null,null,null,null,"Coincident",0.82588927376554,0.84526909702413999,0.87067835088839995,0.90180208967129005,0.92532174213256002,0.94837013412167004,0.97127160714486005]
[null,"Kapunda TF1 11kV","Substation Rating","MVA","Non-Coincident",17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001]
[null,null,null,null,"Coincident",17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.1070621828674003,4.1727703793037998,4.3050245183945997,4.5221167706024996,4.6215757239272,4.7212999121186003,4.8202871773328004]
[null,null,null,null,"Coincident",3.3566602938393002,3.4351645829145001,3.5329332955576001,3.6502811255214,3.7305283441313999,3.8109872422599,3.8908458407449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.2436225535940997,4.3115155564116998,4.4481671634394999,4.6724777622716998,4.7752437391897002,4.8782837700695003,4.9805623751838999]
[null,null,null,null,"Coincident",3.4682697006902998,3.5493842679504,3.6504038034566002,3.7716534645712998,3.8545689140079,3.9377030813355001,4.0202169889755996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7412336205268999,3.8024483685402002,3.9144854968251002,4.1125912264273001,4.2124610455646998,4.3094926941688003,4.4047384221026]
[null,null,null,null,"Coincident",3.0283815320272001,3.1019741291745002,3.1807319070043998,3.2889695664071001,3.3688932138266998,3.4465488453267001,3.5227748290313001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8656301422852999,3.9288802889146002,4.0446426668043998,4.2493354385969999,4.3525259426713996,4.4527839066599002,4.5511965678754001]
[null,null,null,null,"Coincident",3.1290756258347998,3.2051151867489001,3.2864916712987999,3.3983282474543999,3.4809093669148998,3.5611470586211,3.6399075665501002]
[null,"Kapunda TF2 11kV","Substation Rating","MVA","Non-Coincident",17.3,17.3,17.3,17.3,17.3,17.3,17.3]
[null,null,null,null,"Coincident",17.3,17.3,17.3,17.3,17.3,17.3,17.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1187877094927998,3.1917287254066999,3.2825689751406002,3.3916008514071998,3.4661612826731001,3.5409183926084999,3.6151177436449]
[null,null,null,null,"Coincident",3.1187877094927998,3.1917287254066999,3.2825689751406002,3.3916008514071998,3.4661612826731001,3.5409183926084999,3.6151177436449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.137813863091,3.2111998554193,3.3025942757814999,3.4122913006308,3.4873065875489,3.562519752974,3.6371717568938999]
[null,null,null,null,"Coincident",3.137813863091,3.2111998554193,3.3025942757814999,3.4122913006308,3.4873065875489,3.562519752974,3.6371717568938999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8106764939082001,2.8789786482900999,2.9520746675721998,3.0525313114335,3.1267093879850001,3.1987824923043,3.2695287237014998]
[null,null,null,null,"Coincident",2.8106764939082001,2.8789786482900999,2.9520746675721998,3.0525313114335,3.1267093879850001,3.1987824923043,3.2695287237014998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.827823016105,2.8965418475426001,2.9700837888367002,3.0711532681053,3.1457838677552998,3.2182966537973998,3.2894744723336999]
[null,null,null,null,"Coincident",2.827823016105,2.8965418475426001,2.9700837888367002,3.0711532681053,3.1457838677552998,3.2182966537973998,3.2894744723336999]
[null,"Karoonda 11kV","Substation Rating","MVA","Non-Coincident",0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997]
[null,null,null,null,"Coincident",0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997,0.90499654695473997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.64799289641025004,0.65502245163925998,0.67022646676888997,0.69643766484896996,0.70679718726208995,0.71729955496349995,0.72790100333052998]
[null,null,null,null,"Coincident",0.64135998731513,0.65133289230427005,0.66484050833403996,0.68198804944363001,0.69221722099085004,0.70258050844549003,0.71303276313441]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.66459889191479005,0.67180859227068002,0.68740223791677002,0.71428514557869005,0.72491014957900002,0.73568165953766995,0.74655478928409003]
[null,null,null,null,"Coincident",0.65779600247077996,0.66802448127305003,0.68187825450965001,0.69946523252072001,0.70995654517730999,0.72058541070516002,0.73130552341434996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.61580699251805004,0.62462192754273005,0.63781721074205,0.65503596254929997,0.66662670299660998,0.67785187216085996,0.68885812297945004]
[null,null,null,null,"Coincident",0.61580699251805004,0.62462192754273005,0.63781721074205,0.65503596254929997,0.66662670299660998,0.67785187216085996,0.68885812297945004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.63158816574707,0.64062899950027996,0.65416243581008005,0.67182244942234004,0.68371022365633005,0.69522305817881003,0.7065113641752]
[null,null,null,null,"Coincident",0.63158816574707,0.64062899950027996,0.65416243581008005,0.67182244942234004,0.68371022365633005,0.69522305817881003,0.7065113641752]
[null,"Keith 11kV","Substation Rating","MVA","Non-Coincident",16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001]
[null,null,null,null,"Coincident",16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001,16.590415704388001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.2611774159460003,5.2772474518596004,5.3276220070263003,5.4321747151624997,5.4607273187498002,5.4882504262312999,5.5136243919333001]
[null,null,null,null,"Coincident",4.8945811316586996,4.9215494529330996,4.9742814465484999,5.0518616822534002,5.0759132734551002,5.0990230790610998,5.1201385591572999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6599835388243998,5.6772717105678003,5.7314647419898002,5.8439427217661004,5.8746596608689998,5.9042690663246002,5.9315664214283998]
[null,null,null,null,"Coincident",5.2655986377998998,5.2946112033180999,5.3513403709998002,5.4348013194362998,5.4606760618222996,5.4855376296756999,5.5082536987815001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.7116881579373002,4.7158781401718999,4.7485637809885999,4.8294816440846997,4.8581928644563996,4.8820663736389998,4.9025266579059004]
[null,null,null,null,"Coincident",4.2895514968867001,4.3001224045301996,4.3392757965403996,4.4035036389495001,4.4275525238603004,4.4472049350797,4.4637543757013001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0688420681597997,5.0733496581155002,5.1085129256414996,5.1955644992555996,5.2264520785626001,5.2521352400119001,5.2741464483394997]
[null,null,null,null,"Coincident",4.6147067361256999,4.6260789363999004,4.6682002215700003,4.7372966427755001,4.7631684737292002,4.7843105708694003,4.8021144870062997]
[null,"Kent Town 11kV","Substation Rating","MVA","Non-Coincident",57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997]
[null,null,null,null,"Coincident",57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997,57.503264685555997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.608244970293001,33.279381222683,34.128158827245997,35.179057212819998,35.880181634686998,36.595612438052001,37.374475337397001]
[null,null,null,null,"Coincident",32.608244970293001,33.279381222683,34.128158827245997,35.179057212819998,35.880181634686998,36.595612438052001,37.374475337397001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.981664933250997,34.681068635414,35.565595729325999,36.660756687849997,37.391411625031999,38.136975511252999,38.948643176856002]
[null,null,null,null,"Coincident",33.981664933250997,34.681068635414,35.565595729325999,36.660756687849997,37.391411625031999,38.136975511252999,38.948643176856002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.358058543681999,28.857600851023001,29.415250072738001,30.225444843373001,30.784594424400002,31.420409824895,32.097378902960003]
[null,null,null,null,"Coincident",28.358058543681999,28.857600851023001,29.415250072738001,30.225444843373001,30.784594424400002,31.420409824895,32.097378902960003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.552465778727001,30.073048205763001,30.654184940349001,31.498504137885,32.081204425109,32.743799603680998,33.449281803104]
[null,null,null,null,"Coincident",29.552465778727001,30.073048205763001,30.654184940349001,31.498504137885,32.081204425109,32.743799603680998,33.449281803104]
[null,"Kersbrook 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.58905310653492005,0.59939122588090998,0.61493968858789005,0.63840497434584997,0.65148339662882004,0.66466615931258,0.67812121428066996]
[null,null,null,null,"Coincident",0.55604668474579,0.56835471419031003,0.58377921198178995,0.60249943643908999,0.61514365884764,0.62788784126437003,0.64088730042408004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.59527244814589997,0.60571971944290004,0.62143234595791996,0.64514538293984003,0.65836188984541,0.6716838387988,0.68528095495341002]
[null,null,null,null,"Coincident",0.56191753789250998,0.57435551799654005,0.58994287074942997,0.60886074711561,0.62163846977684001,0.63451720784419996,0.64765391791791005]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.49520235780360999,0.50153054527506002,0.51255340701750995,0.53112161826605997,0.54268679147858001,0.55386952498734998,0.56487072215780998]
[null,null,null,null,"Coincident",0.46734762041796002,0.47539532983943,0.486664285064,0.50139118310700004,0.51263949686608001,0.52352923902512005,0.53424657231219996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.50043080426383002,0.50682580601606997,0.51796504935799004,0.53672930752925996,0.54841658817521999,0.55971739124185005,0.57083474127283995]
[null,null,null,null,"Coincident",0.47228197093781998,0.48041464969996001,0.49180258482866002,0.50668497243412003,0.51805204816056005,0.52905676641562005,0.53988725547105998]
[null,"Keswick 11kV","Substation Rating","MVA","Non-Coincident",50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002]
[null,null,null,null,"Coincident",50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002,50.566940704555002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.106347031192001,29.043594490406001,29.257999782658,29.734172134815999,29.545068950872999,29.349732651256002,29.141110829489001]
[null,null,null,null,"Coincident",23.968025246831001,24.083155739955,24.449702537515002,24.707819657367001,24.401516087299999,24.102431346163002,23.989202186532999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.683181862350001,30.617029705943001,30.843050393712002,31.345019358192999,31.145671519131,30.939752885678001,30.719828987606]
[null,null,null,null,"Coincident",25.266491763525,25.387859445105001,25.774263896290002,26.046364497637999,25.72346694765,25.408179306272999,25.288815962830999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.959712043063,25.764325570126999,25.860160771653,26.264912825183,26.150988678055,25.966323125248,25.762665170235]
[null,null,null,null,"Coincident",21.867431094160001,21.855754285682998,22.163709507341,22.408021659462001,22.138484018288999,21.821477421535999,21.694683071943]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.366078087984,27.160106563075001,27.261133631642,27.687813106545001,27.567717124693001,27.373047325201998,27.158356211106]
[null,null,null,null,"Coincident",23.052098032278,23.039788633311002,23.364427313029001,23.621975063238999,23.337835234423,23.003654821838001,22.869991394974001]
[null,"Ki Ki 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.10733739519671,0.10862169817263,0.11126925471445,0.11574652977329,0.11759153065437999,0.11945901978373,0.12132229274633]
[null,null,null,null,"Coincident",0.10623868070648999,0.1080098623501,0.11037509190429,0.11334503295004,0.11516582695660001,0.11700771076362999,0.11884414121001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11009375542118,0.11141103853075,0.11412658274388,0.11871883155314,0.12061121095533001,0.12252665609056,0.12443777679041]
[null,null,null,null,"Coincident",0.10896682659883,0.11078349112959,0.1132094583666,0.11625566572524999,0.11812321663482001,0.12001239891835,0.12189598780216999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10211759409564999,0.10357935073006,0.10576748855587,0.10862282720784,0.1105448880851,0.11240632727351001,0.11423146382971]
[null,null,null,null,"Coincident",0.10211759409564999,0.10357935073006,0.10576748855587,0.10862282720784,0.1105448880851,0.11240632727351001,0.11423146382971]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10473991294425,0.10623920661632,0.1084835345151,0.11141219655891001,0.11338361481196001,0.11529285464739,0.11716485962068]
[null,null,null,null,"Coincident",0.10473991294425,0.10623920661632,0.1084835345151,0.11141219655891001,0.11338361481196001,0.11529285464739,0.11716485962068]
[null,"Kilburn 11kV","Substation Rating","MVA","Non-Coincident",85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005]
[null,null,null,null,"Coincident",85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005,85.054321447182005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.190974181847999,44.056974026707998,45.438331722939999,47.608841905353003,48.614880695579998,49.753528034570003,50.933207791740003]
[null,null,null,null,"Coincident",26.580248941848001,27.171575155469998,27.870585484730999,28.763513990722998,29.3361899336,29.999950059023998,30.686945147136001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.076310583735001,48.020213295688002,49.525833976092997,51.891597041364001,52.988136201342002,54.229212995533999,55.515013366788999]
[null,null,null,null,"Coincident",28.971332049863999,29.615852276974,30.377743574517002,31.350997372873,31.975189604267999,32.698659690539998,33.447454890235001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.831605795222004,41.581642461736998,42.663922479842,44.396223420605999,45.346582150033001,46.430490815642997,47.536732638190998]
[null,null,null,null,"Coincident",25.332025442690998,25.867349884751999,26.376110383975,27.073840398437,27.619324717581001,28.256670348815,28.907616000512]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.504700170813997,45.322207988845001,46.501846819318999,48.389980593948003,49.425830874243999,50.607244860689001,51.813001030942999]
[null,null,null,null,"Coincident",27.610821937802001,28.194302634288,28.748829771678999,29.509325580967001,30.103880107996002,30.798559527794001,31.508062386965999]
[null,"Kilburn Bus A CMP 11kV","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",5.7021518564734004,5.7021518564734004,5.7021518564734004,5.7021518564734004,5.7021518564734004,5.7021518564734004,5.7021518564734004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.956521277665001,11.956521277665001,11.956521277665001,11.956521277665001,11.956521277665001,11.956521277665001,11.956521277665001]
[null,null,null,null,"Coincident",6.1979909091275998,6.1979909091275998,6.1979909091275998,6.1979909091275998,6.1979909091275998,6.1979909091275998,6.1979909091275998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.45,10.45,10.45,10.45,10.45,10.45,10.45]
[null,null,null,null,"Coincident",5.4170442636497,5.4170442636497,5.4170442636497,5.4170442636497,5.4170442636497,5.4170442636497,5.4170442636497]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.358695213781999,11.358695213781999,11.358695213781999,11.358695213781999,11.358695213781999,11.358695213781999,11.358695213781999]
[null,null,null,null,"Coincident",5.8880913636712,5.8880913636712,5.8880913636712,5.8880913636712,5.8880913636712,5.8880913636712,5.8880913636712]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kilburn South 11kV","Substation Rating","MVA","Non-Coincident",36.1,36.1,36.1,36.1,36.1,36.1,36.1]
[null,null,null,null,"Coincident",36.1,36.1,36.1,36.1,36.1,36.1,36.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.004111357902001,16.282731473032001,16.647394021497,17.101419804727001,17.376816196429001,17.650187970284001,17.927439128574999]
[null,null,null,null,"Coincident",16.004111357902001,16.282731473032001,16.647394021497,17.101419804727001,17.376816196429001,17.650187970284001,17.927439128574999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.298318769921998,16.582060825355999,16.953427052786001,17.415799300726999,17.696258370252998,17.974655602898,18.257003535633]
[null,null,null,null,"Coincident",16.298318769921998,16.582060825355999,16.953427052786001,17.415799300726999,17.696258370252998,17.974655602898,18.257003535633]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.097187601870999,14.290306616766999,14.510905036666999,14.846173997757999,15.048477350818001,15.277822575259,15.498011905378]
[null,null,null,null,"Coincident",14.097187601870999,14.290306616766999,14.510905036666999,14.846173997757999,15.048477350818001,15.277822575259,15.498011905378]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.356339577782,14.55300874578,14.777662479266001,15.119094769964001,15.325117114015001,15.558678446644,15.782915569952999]
[null,null,null,null,"Coincident",14.356339577782,14.55300874578,14.777662479266001,15.119094769964001,15.325117114015001,15.558678446644,15.782915569952999]
[null,"Kilkenny 11kV","Substation Rating","MVA","Non-Coincident",55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003]
[null,null,null,null,"Coincident",55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003,55.516949854952003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.043556904102999,20.447650693903999,21.044770916592,21.946442791321001,22.245525436226,22.537379693152001,22.800693681885999]
[null,null,null,null,"Coincident",19.881483563021,20.325981159116001,20.80539031603,21.371077179739,21.636405061512001,21.903222851172998,22.141581547076001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.415030796356,21.846774572903001,22.484752553516,23.448121034366,23.767668312424,24.079492602394001,24.360823765561999]
[null,null,null,null,"Coincident",21.241867639380001,21.716779839586,22.228992412857998,22.833386217080001,23.116869073265999,23.401943783804999,23.656612096309999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.598331401589999,19.039518835989998,19.488638990195,20.229394898666001,20.592272186763001,20.958986706748998,21.247225654304]
[null,null,null,null,"Coincident",18.597535163846999,19.039518835989998,19.419562056928999,19.883584498796999,20.215324530699,20.558713927039001,20.825389377034998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.870916206711001,20.342291748480001,20.822142803837998,21.613584695534001,22.001291744591001,22.393098586886001,22.701060191113001]
[null,null,null,null,"Coincident",19.870065486659001,20.342291748480001,20.748339303776,21.244112331006999,21.598551567192999,21.965437271809002,22.250359903136999]
[null,"Kingscote 11kV","Substation Rating","MVA","Non-Coincident",8.5,8.5,8.5,8.5,8.5,8.5,8.5]
[null,null,null,null,"Coincident",8.5,8.5,8.5,8.5,8.5,8.5,8.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1314685265272999,3.1956987776532002,3.2986404525405999,3.4392201385746,3.5107049335106,3.5799367945306,3.6482030382255002]
[null,null,null,null,"Coincident",3.0853550734164998,3.1705997139603999,3.2981961306801,3.4194093626490001,3.4692746429497001,3.5175851064733998,3.5933643327156002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2113300192739,3.2771983273342,3.3827653122806001,3.5269301863761999,3.6002380500686,3.6712355235223999,3.7412427536202002]
[null,null,null,null,"Coincident",3.1640405399091001,3.2514591650178999,3.3823096589291999,3.5066141784406999,3.5577511674259998,3.6072936873154999,3.6850055027169999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9761455030730999,3.0670152653059999,3.2127152766310001,3.3534409255514999,3.4201676339546001,3.4835236003838999,3.5770322037739999]
[null,null,null,null,"Coincident",2.9761455030730999,3.0670152653059999,3.2127152766310001,3.3534409255514999,3.4201676339546001,3.4835236003838999,3.5770322037739999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.0520458100674999,3.1452330137167999,3.2946487961884001,3.4389633556458001,3.5073917878549001,3.5723635144332002,3.6682568573115999]
[null,null,null,null,"Coincident",3.0520458100674999,3.1452330137167999,3.2946487961884001,3.4389633556458001,3.5073917878549001,3.5723635144332002,3.6682568573115999]
[null,"Kingston SE 11kV","Substation Rating","MVA","Non-Coincident",3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627]
[null,null,null,null,"Coincident",3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627,3.8691564147627]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.7026386671640998,3.7580908556377,3.8337307824151998,3.9295088676132002,3.9844195664459998,4.0389772744348997,4.0925475554755]
[null,null,null,null,"Coincident",3.7026386671640998,3.7580908556377,3.8337307824151998,3.9295088676132002,3.9844195664459998,4.0389772744348997,4.0925475554755]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.7909403845659999,3.8477150146592001,3.9251588267302,4.0232210584984003,4.0794412853318001,4.1353001030821002,4.1901479454089001]
[null,null,null,null,"Coincident",3.7909403845659999,3.8477150146592001,3.9251588267302,4.0232210584984003,4.0794412853318001,4.1353001030821002,4.1901479454089001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2809333874765998,3.3095222828056001,3.3601865977154999,3.4306993577934999,3.4702560160509002,3.5065086705491,3.5406310112674002]
[null,null,null,null,"Coincident",3.2809333874765998,3.3095222828056001,3.3601865977154999,3.4306993577934999,3.4702560160509002,3.5065086705491,3.5406310112674002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3591781417824,3.3884488342790999,3.4403214080604001,3.5125157791119999,3.5530157972737002,3.5901330167322998,3.6250691180030001]
[null,null,null,null,"Coincident",3.3591781417824,3.3884488342790999,3.4403214080604001,3.5125157791119999,3.5530157972737002,3.5901330167322998,3.6250691180030001]
[null,"Kingswood 11kV","Substation Rating","MVA","Non-Coincident",69.116396272006,69.116396272006,69.116396272006,69.116396272006,69.116396272006,69.116396272006,69.116396272006]
[null,null,null,null,"Coincident",69.116396272006,69.116396272006,69.116396272006,69.116396272006,69.116396272006,69.116396272006,69.116396272006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.373545548739997,54.773559579644001,56.897930187345999,58.968275349004003,59.838482903785,60.682277442428997,62.000963079157003]
[null,null,null,null,"Coincident",53.373545548739997,54.773559579644001,56.897930187345999,58.968275349004003,59.838482903785,60.682277442428997,62.000963079157003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.879132920316003,56.318639239455003,58.502935143979997,60.631681625958002,61.526436425851998,62.394033138185002,63.749916911581003]
[null,null,null,null,"Coincident",54.879132920316003,56.318639239455003,58.502935143979997,60.631681625958002,61.526436425851998,62.394033138185002,63.749916911581003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",47.592389748277,48.841942707855999,50.955051549135,52.973112728876004,53.811289754908003,54.590549254053002,55.835866611782002]
[null,null,null,null,"Coincident",47.592389748277,48.841942707855999,50.955051549135,52.973112728876004,53.811289754908003,54.590549254053002,55.835866611782002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.934899417654997,50.219700385149999,52.392416845775003,54.467404493414001,55.329225231560997,56.130466468083,57.410912353775998]
[null,null,null,null,"Coincident",48.934899417654997,50.219700385149999,52.392416845775003,54.467404493414001,55.329225231560997,56.130466468083,57.410912353775998]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kongorong 11kV","Substation Rating","MVA","Non-Coincident",1.33,1.33,1.33,1.33,1.33,1.33,1.33]
[null,null,null,null,"Coincident",1.33,1.33,1.33,1.33,1.33,1.33,1.33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.80218654854976001,0.81158432999840002,0.83150054197459,0.86533320222357002,0.87972011725288002,0.89404695592915995,0.9082902797622]
[null,null,null,null,"Coincident",0.50428988953765996,0.51271355027748999,0.52386727061430005,0.53779687046933999,0.54614631701850003,0.55444691147376002,0.56268358863817003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.82078268779565,0.83039832686449,0.85077623275940994,0.88539319544051998,0.90011362525600003,0.91477258603960998,0.92934609595442996]
[null,null,null,null,"Coincident",0.51598024388615005,0.52459918036122999,0.53601146416668,0.55026397741263999,0.5588069792775,0.56729999656830998,0.57572761484952995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.72945940008772003,0.73620454784952005,0.75199868566693995,0.78024588900367997,0.79357344474987002,0.80621253969697004,0.81859825824994004]
[null,null,null,null,"Coincident",0.45784648151643997,0.46397454190349002,0.47321800640799999,0.48534243681088002,0.49314977577799002,0.50052410017255,0.50772297247758003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74636959211570997,0.75327110463736002,0.76943137921767002,0.79833340396410002,0.81196991662675,0.82490200872021002,0.83757485069515003]
[null,null,null,null,"Coincident",0.46846019342535999,0.47473031336760002,0.48418805814562998,0.49659355483722001,0.50458188208296995,0.51212715669294995,0.51949291191572999]
[null,"Kumorna 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.59777204597762001,0.59895288306089001,0.60402538209523005,0.61521380321371999,0.61777268830948995,0.62020158279561,0.62234619289521997]
[null,null,null,null,"Coincident",0.52204261359779003,0.52435428702176001,0.52940727809712995,0.53708319192825005,0.53905139673124003,0.54090836401903997,0.54251823825168]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.70195135487698002,0.70333798745049003,0.70929451819447997,0.72243284979749001,0.72543769566145,0.72828989624000995,0.73080826754096995]
[null,null,null,null,"Coincident",0.61302384811115995,0.61573839841995004,0.62167202137104005,0.63068568828627003,0.63299691049452,0.63517750878848001,0.63706795081630996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.54545214970277001,0.54548807071348004,0.54882607043373999,0.55771370445319002,0.56055072419789997,0.56281204946769003,0.56461546027511]
[null,null,null,null,"Coincident",0.46615438457572,0.46691870261627,0.4707902718834,0.47736098944652999,0.47955857049619,0.48126537717839002,0.48258171191691002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.64051318237580002,0.64055536367601995,0.64447510773562999,0.65491167261614003,0.65824312624801995,0.66089855376027995,0.66301626178659001]
[null,null,null,null,"Coincident",0.54739545623887997,0.54829297911190999,0.55283928285904005,0.56055514064628997,0.56313571463873002,0.56513998243804997,0.56668572710676002]
[null,"Kybunga 11kV","Substation Rating","MVA","Non-Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.1145397015258002E-2,7.1918769014676004E-2,7.3645563014816007E-2,7.6658465031058998E-2,7.8046035737624003E-2,7.9481711985543005E-2,8.0953295366805997E-2]
[null,null,null,null,"Coincident",4.2341832770198998E-2,4.3081260325470001E-2,4.4077752723737998E-2,4.5335612039027001E-2,4.6154308788152E-2,4.7002058783123003E-2,4.7871682533846001E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.4323099041862004E-2,7.5131013624117005E-2,7.6934934705191999E-2,8.0082407687999999E-2,8.1531954101093998E-2,8.3031754684724998E-2,8.4569066190210998E-2]
[null,null,null,null,"Coincident",4.4233026486850999E-2,4.5005480499764002E-2,4.6046481131118998E-2,4.7360522606646999E-2,4.8215786364011998E-2,4.9101401027537003E-2,5.0009866435921001E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3848232237459002E-2,6.4510695694232997E-2,6.6049965415103995E-2,6.8798356470650995E-2,7.0204586652906006E-2,7.1604343483223004E-2,7.3020052774033006E-2]
[null,null,null,null,"Coincident",3.7482568926171002E-2,3.8078758340237003E-2,3.8957158648427997E-2,4.0100135825514999E-2,4.0917878172600002E-2,4.1732413579960999E-2,4.2556847804608E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.6700007130676003E-2,6.7392059451347006E-2,6.9000080500015007E-2,7.1871228166579995E-2,7.3340267478975998E-2,7.4802544307817007E-2,7.6281486112200994E-2]
[null,null,null,null,"Coincident",3.9156724110285999E-2,3.9779542264774002E-2,4.0697176234686001E-2,4.1891204372825001E-2,4.2745471099877003E-2,4.3596387649564999E-2,4.4457645146220998E-2]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Lameroo 11kV","Substation Rating","MVA","Non-Coincident",2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002]
[null,null,null,null,"Coincident",2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002,2.5808471454880002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0432054164175999,1.0550147325256001,1.0800218688637,1.1227758801195,1.1399835057801999,1.1574162784352,1.1749238320974]
[null,null,null,null,"Coincident",0.92844225202493003,0.94331946214898998,0.96334510391497996,0.98864650239277996,1.0039211426336001,1.0193857725175,1.0349046225742999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0512434729905999,1.0631437816772999,1.0883436018085999,1.1314270392307999,1.1487672522673,1.1663343470898999,1.1839767991187999]
[null,null,null,null,"Coincident",0.93559604094235005,0.95058788223563995,0.97076782462055999,0.99626417422603997,1.0116565078957001,1.0272402951074,1.0428787202669001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.94533295824913,0.96256755012396999,0.99191307415800001,1.0380129653943,1.0562287714128,1.0738739905809001,1.0911840390023]
[null,null,null,null,"Coincident",0.94134101878301002,0.95481579256352,0.97498649780216995,1.0013075977009001,1.0190255508156001,1.0361846807141999,1.0530091654706]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.95261689262980997,0.96998427965918999,0.99955591542408995,1.0460110133416001,1.064367174919,1.0821483531874001,1.0995917781675999]
[null,null,null,null,"Coincident",0.94859419466228001,0.96217279362646002,0.98249891722018001,1.0090228252013,1.0268772978425,1.0441686414496001,1.0611227614229]
[null,"Langhorne Creek 11kV","Substation Rating","MVA","Non-Coincident",6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003]
[null,null,null,null,"Coincident",6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003,6.8552346570397003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.7535815745205001,3.8632801732659998,3.9952381805015,4.1468973774502,4.2571602696516999,4.3681678413381997,4.4804571027669002]
[null,null,null,null,"Coincident",3.7535815745205001,3.8632801732659998,3.9952381805015,4.1468973774502,4.2571602696516999,4.3681678413381997,4.4804571027669002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.0056859380947003,4.1227522987691003,4.2635730917924999,4.4254182789929999,4.5430868331502001,4.6615500822094997,4.7813811040146996]
[null,null,null,null,"Coincident",4.0056859380947003,4.1227522987691003,4.2635730917924999,4.4254182789929999,4.5430868331502001,4.6615500822094997,4.7813811040146996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.3696467348108001,3.4667501918413,3.5679212657463002,3.6847754820726002,3.7973310545921999,3.906937828302,4.0140370762842004]
[null,null,null,null,"Coincident",3.3696467348108001,3.4667501918413,3.5679212657463002,3.6847754820726002,3.7973310545921999,3.906937828302,4.0140370762842004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.5959646204579001,3.6995899033098998,3.8075559991672998,3.9322585750544001,4.0523737943842999,4.1693421627153002,4.2836345906554003]
[null,null,null,null,"Coincident",3.5959646204579001,3.6995899033098998,3.8075559991672998,3.9322585750544001,4.0523737943842999,4.1693421627153002,4.2836345906554003]
[null,"Largs North 11kV","Substation Rating","MVA","Non-Coincident",35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999]
[null,null,null,null,"Coincident",35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999,35.525726512738999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.891988937097999,17.208274601995001,17.728037803035001,18.54903977847,18.910661142887999,19.318158248797999,19.718103007448001]
[null,null,null,null,"Coincident",15.709168389766999,16.037764814321001,16.432012092693,16.934879845009,17.244379007096001,17.602272150632,17.952466350717]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.143636793845001,17.464634314165,17.992140670617999,18.825373496325,19.192382103279002,19.605949884093999,20.011852806800999]
[null,null,null,null,"Coincident",15.943195215813001,16.276686894933999,16.676807459334,17.187166667663998,17.501276583469,17.864501428490001,18.219912635301998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.724618613963999,14.986418086065999,15.370436768488,15.98343614595,16.310459171388999,16.680651395422998,17.03777134145]
[null,null,null,null,"Coincident",13.804601454993,14.088167425929001,14.359606570382001,14.729240345402999,15.012086105377,15.340413955228,15.656767302965999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.943978141692,15.209677762928999,15.599417351204,16.221548866989,16.553443707332001,16.929150858004,17.291590986831999]
[null,null,null,null,"Coincident",14.010255056965001,14.298045442747,14.573528343041,14.948668725224,15.235728170724,15.568947274058999,15.890013485522999]
[null,"LeFevre 11kV","Substation Rating","MVA","Non-Coincident",74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998]
[null,null,null,null,"Coincident",74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998,74.579784102060998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.989075683464,10.980949233324001,11.09421533844,11.382172461827,11.376473376571001,11.391812941034001,11.397336101215]
[null,null,null,null,"Coincident",8.5623460885099991,8.5744367941427004,8.6156068883730992,8.7065290937092996,8.6917596504572998,8.6967115121763001,8.6940383733779996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.335187171222,11.326804770733,11.443638300561,11.740664909977999,11.73478632656,11.750609025331,11.756306142744]
[null,null,null,null,"Coincident",8.8320253981036991,8.8444969121169006,8.8869636979868005,8.9807495854620996,8.9655149644167,8.9706227897742004,8.9678654579033008]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.287885116130999,10.242661791938,10.272953261355999,10.443738752657,10.416077005595,10.408206175906001,10.385559696683]
[null,null,null,null,"Coincident",8.0810004462367999,8.0673091415136007,8.0410146156254001,8.0635336905880006,8.0322690655002003,8.0197192717704997,7.9961038293083]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.611911933852999,10.565264257652,10.596509785978,10.772674330276001,10.744141349935999,10.736022620909999,10.712662869083999]
[null,null,null,null,"Coincident",8.3355193127530001,8.3213967872443995,8.2942740900217,8.3175024248675999,8.2852530903998005,8.2723080288693005,8.2479487953768]
[null,"Leigh Creek South 11kV","Substation Rating","MVA","Non-Coincident",3.3,3.3,3.3,3.3,3.3,3.3,3.3]
[null,null,null,null,"Coincident",3.3,3.3,3.3,3.3,3.3,3.3,3.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0042178034828999,1.0151725478264,1.0314964364239001,1.053042201609,1.0634713997487999,1.0736828163462,1.0833664365603]
[null,null,null,null,"Coincident",1.0042178034828999,1.0151725478264,1.0314964364239001,1.053042201609,1.0634713997487999,1.0736828163462,1.0833664365603]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0047727996999001,1.0157335983492,1.0320665085915,1.0536241813709,1.0640591433654001,1.0742762034572,1.0839651754710999]
[null,null,null,null,"Coincident",1.0047727996999001,1.0157335983492,1.0320665085915,1.0536241813709,1.0640591433654001,1.0742762034572,1.0839651754710999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.91304942908244002,0.92169930609650996,0.93653409716383995,0.95687432594663002,0.96855882145517003,0.97928770005605004,0.98923576837966998]
[null,null,null,null,"Coincident",0.91304942908244002,0.92169930609650996,0.93653409716383995,0.95687432594663002,0.96855882145517003,0.97928770005605004,0.98923576837966998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.91355403971302995,0.92220869721295995,0.93705168695282004,0.95740315707189005,0.96909411019429004,0.97982891827284002,0.98978248454746998]
[null,null,null,null,"Coincident",0.91355403971302995,0.92220869721295995,0.93705168695282004,0.95740315707189005,0.96909411019429004,0.97982891827284002,0.98978248454746998]
[null,"Linden Park 11kV","Substation Rating","MVA","Non-Coincident",55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002]
[null,null,null,null,"Coincident",55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002,55.666160152883002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.264549374788999,45.141117883846,46.261728064849997,47.674896301464997,48.677089019699999,49.689286058534002,50.728955892119998]
[null,null,null,null,"Coincident",44.264549374788999,45.141117883846,46.261728064849997,47.674896301464997,48.677089019699999,49.689286058534002,50.728955892119998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.531131145441996,46.432781705711001,47.585456924027,49.039061427420997,50.069930796507997,51.111090748911003,52.180509600104998]
[null,null,null,null,"Coincident",45.531131145441996,46.432781705711001,47.585456924027,49.039061427420997,50.069930796507997,51.111090748911003,52.180509600104998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.555061749486001,39.341147365457999,40.295829546707999,41.599155835746998,42.561736755996002,43.632133677852998,44.710520405270998]
[null,null,null,null,"Coincident",38.555061749486001,39.341147365457999,40.295829546707999,41.599155835746998,42.561736755996002,43.632133677852998,44.710520405270998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.658272762995999,40.466851360945,41.448850730884999,42.789470279253003,43.779594401988,44.880619563548002,45.989863150235003]
[null,null,null,null,"Coincident",39.658272762995999,40.466851360945,41.448850730884999,42.789470279253003,43.779594401988,44.880619563548002,45.989863150235003]
[null,"Little Swamp 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.17408809510664999,0.17570776572138999,0.1782442278601,0.18171699400097999,0.18342693476986999,0.18529454761535999,0.18731233574483999]
[null,null,null,null,"Coincident",0.12524235905368,0.13714503157058999,0.14647392745662999,0.15007583203882999,0.15204522845606999,0.15396111401779999,0.15580401528318]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.17598296321724,0.17762026319483001,0.18018433354659999,0.18369489913501,0.18542345181548001,0.18731139275992001,0.18935114357662]
[null,null,null,null,"Coincident",0.12660556399954001,0.13863779158207001,0.14806822816972001,0.15170933781144,0.15370017019457,0.15563690928137,0.15749986967162]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.16097864394788,0.1619855761399,0.16386095818252999,0.16660675259930999,0.16811871481337001,0.16961531804067001,0.17116768416075001]
[null,null,null,null,"Coincident",0.1154824928933,0.12674274480822001,0.13541748209898,0.13839337518764999,0.14005709058734001,0.14155063484041,0.1429222962908]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.16273082176747999,0.16374871394903001,0.16564450865472,0.16842018976924,0.16994860899021,0.17146150204898,0.17303076495372999]
[null,null,null,null,"Coincident",0.11673946622614,0.12812228075661,0.13689143853631,0.13989972283996999,0.14158154700955,0.14309134779857,0.14447793914719001]
[null,"Lobethal 11kV","Substation Rating","MVA","Non-Coincident",13.40027972028,13.40027972028,13.40027972028,13.40027972028,13.40027972028,13.40027972028,13.40027972028]
[null,null,null,null,"Coincident",13.40027972028,13.40027972028,13.40027972028,13.40027972028,13.40027972028,13.40027972028,13.40027972028]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7291272966074001,7.9192110831019997,8.1797259857090996,8.5466794068252998,8.7755782531275006,9.0058468545335995,9.2363733494991997]
[null,null,null,null,"Coincident",7.6400671123962001,7.8632288011778,8.1313895301185006,8.4463233732020999,8.6767852971902002,8.9086720419506999,9.1408319093879999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.0825458555483998,8.2813213267990005,8.5537484153396992,8.9374809816702001,9.1768463524969999,9.4176441112264992,9.6587115558390995]
[null,null,null,null,"Coincident",7.9894133458657004,8.2227792245168008,8.5032017489681007,8.8325361137034992,9.0735360347953993,9.3160259273663009,9.5588014312971996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.0537280179469004,7.2078635205257999,7.4313257310639003,7.7601031423639002,7.9746538059959997,8.1845532258688003,8.3926453646866008]
[null,null,null,null,"Coincident",6.9708534126085997,7.1544126516987001,7.3886748859568998,7.6711436582966996,7.8883207180071997,8.1009948804708003,8.3119220110508003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3762635766973998,7.5374470091540999,7.7711271510828004,8.1149380887377998,8.3392991984202993,8.5587963836872003,8.7764036489876993]
[null,null,null,null,"Coincident",7.2895994848534,7.4815520702125999,7.7265260728334004,8.0219108837678998,8.2490184829211994,8.4714172873965996,8.6919891760030001]
[null,"Lock 11kV","Substation Rating","MVA","Non-Coincident",1.2,1.2,1.2,1.2,1.2,1.2,1.2]
[null,null,null,null,"Coincident",1.2,1.2,1.2,1.2,1.2,1.2,1.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.68332402449762997,0.68024297640925002,0.67848668018478997,0.68032440198900002,0.67672161481922,0.67281726293349997,0.66849664291926003]
[null,null,null,null,"Coincident",0.64295503472047999,0.64046807527833005,0.64112113385166003,0.64470481294147997,0.64122051433321003,0.63745128622645997,0.63328834586393001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.69983381039003001,0.69667832112522998,0.69487959104275998,0.69676171402770004,0.69307187994803998,0.68907319504989994,0.68464818457257004]
[null,null,null,null,"Coincident",0.65848946579726997,0.65594241894937,0.65661125606529003,0.66028152039485999,0.65671303767780997,0.65285274128310999,0.64858922015421006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.62829201347478003,0.62504639858759004,0.62322422443202996,0.62518048533516002,0.62346225041783998,0.62090567229350002,0.61772685117839998]
[null,null,null,null,"Coincident",0.59188327192426005,0.58888936660188995,0.58964536177860005,0.59357436991337997,0.59187011732932004,0.58937079162627004,0.58628160406465002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.64347217142108004,0.64014813926044001,0.63828193957074997,0.64028546567678002,0.63852571650036005,0.63590736891389998,0.63265174432910998]
[null,null,null,null,"Coincident",0.60618375857837004,0.60311751753520004,0.60389177830489005,0.6079157151715,0.60617028615538004,0.60361057426546005,0.60044674886966998]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Loveday 11kV","Substation Rating","MVA","Non-Coincident",20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001]
[null,null,null,null,"Coincident",20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001,20.681463204869001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.16014636155,15.191572144732,15.504445652455001,15.941531535386,16.102755644034001,16.254055683706,16.390320301776001]
[null,null,null,null,"Coincident",12.893502775328001,15.094058397904,15.356338604384,15.689560657145,15.85031356098,16.001016232213999,16.136677738780001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.317420445303,15.373123361884,15.689735953725,16.132045356203001,16.295196219560001,16.448304413521999,16.586197500787002]
[null,null,null,null,"Coincident",13.047590258829,15.274444249203,15.53985891012,15.877063228093,16.039737255369001,16.192240941872001,16.329523709977]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.039508190123,14.058416902893001,14.358470414637001,14.784636202507,14.978970149195,15.151873049901999,15.305564766491001]
[null,null,null,null,"Coincident",11.822373979769999,14.005862761331,14.260902012556,14.593073307268,14.786462184738999,14.958392294627,15.111091453542]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.183389767684,14.226426025032,14.530065411875,14.961324215579999,15.157980605543001,15.332949831694,15.488478284991]
[null,null,null,null,"Coincident",11.963660633002,14.173243820208,14.431330990768,14.767471993308,14.963172019733999,15.137156829452,15.291680863231999]
[null,"Lower Mitcham 11kV","Substation Rating","MVA","Non-Coincident",25.741904394757,25.741904394757,25.741904394757,25.741904394757,25.741904394757,25.741904394757,25.741904394757]
[null,null,null,null,"Coincident",25.741904394757,25.741904394757,25.741904394757,25.741904394757,25.741904394757,25.741904394757,25.741904394757]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.600425718181999,23.254305005494,24.220624320096,25.142390174089002,25.541123886354999,25.929322205628999,26.521530452749001]
[null,null,null,null,"Coincident",22.600425718181999,23.254305005494,24.220624320096,25.142390174089002,25.541123886354999,25.929322205628999,26.521530452749001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.909196933244999,23.572009640865002,24.551530989473999,25.485890179818,25.89007146614,26.283573422976001,26.883872529192999]
[null,null,null,null,"Coincident",22.909196933244999,23.572009640865002,24.551530989473999,25.485890179818,25.89007146614,26.283573422976001,26.883872529192999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.159115629932,20.718281992944,21.643956929489999,22.531643838099001,22.919116519923001,23.282422941404999,23.845816311602]
[null,null,null,null,"Coincident",20.159115629932,20.718281992944,21.643956929489999,22.531643838099001,22.919116519923001,23.282422941404999,23.845816311602]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.434533213003,21.001339010753,21.939660690261999,22.839475342338002,23.232241747928999,23.600511729240001,24.171602284333002]
[null,null,null,null,"Coincident",20.434533213003,21.001339010753,21.939660690261999,22.839475342338002,23.232241747928999,23.600511729240001,24.171602284333002]
[null,"Loxton 11kV","Substation Rating","MVA","Non-Coincident",21.954282759923,21.954282759923,21.954282759923,21.954282759923,21.954282759923,21.954282759923,21.954282759923]
[null,null,null,null,"Coincident",21.954282759923,21.954282759923,21.954282759923,21.954282759923,21.954282759923,21.954282759923,21.954282759923]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.098439233503999,13.360698451785,13.600439684635001,13.948514037416,14.054885394418999,14.152921318816,14.239269124867]
[null,null,null,null,"Coincident",12.444005475888,12.872500364766999,13.062154928244,13.311871874015999,13.415146177163001,13.510218098043,13.593923723139]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.610161108838,13.88266611111,14.131773408960999,14.493446119331001,14.603973127959,14.705839060359001,14.795560250096999]
[null,null,null,null,"Coincident",12.930160330314999,13.375395397486001,13.572459270358999,13.83193200623,13.939240967182,14.038027100173,14.125002885835]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.328358130099,12.599429209966001,12.847185790144,13.207531593236,13.360630828841,13.494855636715,13.613298503063]
[null,null,null,null,"Coincident",11.739014359544999,12.17179878406,12.373064248844001,12.641197743518999,12.78909256923,12.918654512869001,13.032876719980999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.809994944201,13.091656064519,13.349091848423001,13.723515422679,13.882595846314,14.022064467529001,14.145134587904]
[null,null,null,null,"Coincident",12.197627048855001,12.647319232636001,12.856447614463001,13.135056385794,13.288729076808,13.423352667838,13.542037238821999]
[null,"Lucindale 11kV","Substation Rating","MVA","Non-Coincident",3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002]
[null,null,null,null,"Coincident",3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002,3.5971761541909002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4190132999508001,1.4498292758867,1.4887064136585999,1.5357533712613001,1.5671240869273,1.5985437345205999,1.6297030325751001]
[null,null,null,null,"Coincident",1.4190132999508001,1.4498292758867,1.4887064136585999,1.5357533712613001,1.5671240869273,1.5985437345205999,1.6297030325751001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4378718311242,1.4690973480014999,1.5084911586719001,1.5561633651828,1.5879509942204999,1.6197882054854,1.6513616071946]
[null,null,null,null,"Coincident",1.4378718311242,1.4690973480014999,1.5084911586719001,1.5561633651828,1.5879509942204999,1.6197882054854,1.6513616071946]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2933115899884999,1.3186168370869999,1.3530292851768,1.3958969755962001,1.4265846730698999,1.4561807563114999,1.4850729681671]
[null,null,null,null,"Coincident",1.2933115899884999,1.3186168370869999,1.3530292851768,1.3958969755962001,1.4265846730698999,1.4561807563114999,1.4850729681671]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3104995592186,1.3361411102765,1.3710108960284,1.4144482933533999,1.4455438269617999,1.4755332389047999,1.5048094250880999]
[null,null,null,null,"Coincident",1.3104995592186,1.3361411102765,1.3710108960284,1.4144482933533999,1.4455438269617999,1.4755332389047999,1.5048094250880999]
[null,"Lyndoch 11kV","Substation Rating","MVA","Non-Coincident",4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996]
[null,null,null,null,"Coincident",4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8994757456290001,2.9232856088425998,2.9847626847878002,3.0939095594742998,3.1390896244556998,3.1840485402827001,3.2281934584469001]
[null,null,null,null,"Coincident",2.8811810946913998,2.9176166154868999,2.9781417564889998,3.054387160448,3.0989397645529002,3.1432695194277001,3.1867805071686002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9829857200994998,3.0074813490321,3.0707290723263001,3.1830195679700002,3.229500897871,3.2757547091350001,3.3211710781794999]
[null,null,null,null,"Coincident",2.9641641512061998,3.0016490787491001,3.0639174497083999,3.1423588547022998,3.1881946517556998,3.2338011811313998,3.2785653614472001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.5635371247052001,2.5772246530851999,2.6240167217661998,2.7136036360111002,2.7543809755208,2.7927291675718,2.8294647042863001]
[null,null,null,null,"Coincident",2.5303760576913001,2.5532387136099999,2.6014164243661,2.6652699642208,2.7053583002366999,2.7430591604169998,2.7791639079280999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6373714791263998,2.6514532322718001,2.6995929943994001,2.7917601685180999,2.8337119667507,2.8731646538278,2.9109582382730999]
[null,null,null,null,"Coincident",2.6032553153631,2.6267764557733,2.6763417688921001,2.7420344024143999,2.7832773526471,2.8220640635629999,2.8592086909723]
[null,"Lyndoch South 7.6kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.32067406247259,0.32354125921447002,0.33058920314093998,0.34292308967849999,0.34817296825659,0.35339825265158997,0.35850570027070999]
[null,null,null,null,"Coincident",0.27778171494613002,0.28149805034616998,0.28754973376163001,0.29512224365595002,0.29963546413029002,0.30412707426085001,0.30851579906597998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.33755227528816001,0.34057038275983997,0.34798928496270998,0.36097234767691999,0.36649854597732001,0.37199885561558999,0.37737512631067999]
[null,null,null,null,"Coincident",0.29240235144221,0.29631429075013999,0.30268449571919998,0.31065557365659002,0.31540634092552,0.32013436042166998,0.32475407937294998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.29166567709363,0.29375260202589998,0.29963196860241997,0.31042000200163,0.31564656457219997,0.32060533641664002,0.32536053779613999]
[null,null,null,null,"Coincident",0.25096868096461,0.25369365816037998,0.25895253810980001,0.26578669379163,0.27026548929555,0.27451485146575999,0.27858870363859001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.30701707574129999,0.30921384293166998,0.31540266141564,0.3267585072602,0.33226016234894001,0.33747993193622999,0.34248541642327002]
[null,null,null,null,"Coincident",0.26417805242017001,0.26704645482680001,0.27258212827262002,0.27977598979759,0.28449052018785997,0.28896354135463997,0.29325181481064]
[null,"Lyrup 11kV","Substation Rating","MVA","Non-Coincident",6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999]
[null,null,null,null,"Coincident",6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999,6.6710344827585999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6899475094063998,4.7482957983957004,4.7979495232206002,4.8847448063848002,4.8862025477620996,4.8847066193742004,4.8788197586270998]
[null,null,null,null,"Coincident",3.5357580717992998,3.6303243779384999,3.6567180205110001,3.6993632716293998,3.7009522515443001,3.7002295569229,3.6961179330154001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.7715283224720997,4.8308915696985997,4.8814090123443998,4.9697140842123,4.9711971827447998,4.9696752329454004,4.9636859712897001]
[null,null,null,null,"Coincident",3.5972619623486999,3.6934732327712001,3.7203259881198001,3.7637130458900998,3.7653296658315001,3.7645944000640998,3.7604112551809998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4136852239086997,4.4762230721443999,4.5298142916502,4.6220453346569004,4.6409833603245998,4.6531903211387,4.6595185995351001]
[null,null,null,null,"Coincident",3.3350447400255998,3.4315436727959998,3.4619722032651001,3.5105461215412999,3.5253049733658002,3.5348726530622998,3.5399072645173999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4904605030478004,4.5540861861678001,4.6086096155228997,4.7024450013208998,4.7217124506183001,4.7341317493714001,4.7405701070589004]
[null,null,null,null,"Coincident",3.3930572574272002,3.4912347721815,3.5221926015929998,3.5716114546447999,3.5866270341041999,3.5963611419083001,3.6014833295452999]
[null,"MacGillivray 11kV","Substation Rating","MVA","Non-Coincident",2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001]
[null,null,null,null,"Coincident",2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001,2.3977859778598001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6110286181658999,1.6475545236228,1.7055771747096999,1.7597000578202,1.7767041355961,1.7926942640575001,1.8224049213608]
[null,null,null,null,"Coincident",1.6110286181658999,1.6475545236228,1.7055771747096999,1.7597000578202,1.7767041355961,1.7926942640575001,1.8224049213608]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6209393063827999,1.6576899110515999,1.7160695045279,1.7705253395263001,1.7876340225906,1.8037225187507999,1.8336159493816]
[null,null,null,null,"Coincident",1.6209393063827999,1.6576899110515999,1.7160695045279,1.7705253395263001,1.7876340225906,1.8037225187507999,1.8336159493816]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5317322786492999,1.5683132490134,1.6322468873321001,1.6928156897516,1.7154596938629001,1.7361001467724,1.7713802402034]
[null,null,null,null,"Coincident",1.5317322786492999,1.5683132490134,1.6322468873321001,1.6928156897516,1.7154596938629001,1.7361001467724,1.7713802402034]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5411551534971999,1.5779611618203,1.6422881056016001,1.7032295137647999,1.7260128187316,1.7467802470970999,1.7822773757827]
[null,null,null,null,"Coincident",1.5411551534971999,1.5779611618203,1.6422881056016001,1.7032295137647999,1.7260128187316,1.7467802470970999,1.7822773757827]
[null,"Maitland 11kV","Substation Rating","MVA","Non-Coincident",6.46875,6.46875,6.46875,6.46875,6.46875,6.46875,6.46875]
[null,null,null,null,"Coincident",6.46875,6.46875,6.46875,6.46875,6.46875,6.46875,6.46875]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.8469419849755,3.9357763461745998,4.0465266961833004,4.1802933215643003,4.2720956235732999,4.3717928409170002,4.4714135749613]
[null,null,null,null,"Coincident",3.8469419849755,3.9357763461745998,4.0465266961833004,4.1802933215643003,4.2720956235732999,4.3717928409170002,4.4714135749613]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8519716256269998,3.9409221323037,4.0518172816010001,4.1857587986386999,4.2776811265257999,4.3775086918652004,4.4772596739079997]
[null,null,null,null,"Coincident",3.8519716256269998,3.9409221323037,4.0518172816010001,4.1857587986386999,4.2776811265257999,4.3775086918652004,4.4772596739079997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.3253821434784001,3.3892815381479999,3.4965756323987001,3.6772464835576999,3.7809891862642999,3.8828137184331002,3.9836143896676002]
[null,null,null,null,"Coincident",3.3143240069339002,3.3892815381479999,3.4965756323987001,3.6267916368206001,3.7263998049187999,3.8240065645246002,3.9203466969938998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3297298766327001,3.3937128158408001,3.5011471905376998,3.6820542577511999,3.7859325976773999,3.8878902591753999,3.9888227211039999]
[null,null,null,null,"Coincident",3.3186572822530001,3.3937128158408001,3.5011471905376998,3.6315334443972,3.7312718440646,3.8290062185207998,3.9254723098033]
[null,"Mallala 11kV","Substation Rating","MVA","Non-Coincident",7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998]
[null,null,null,null,"Coincident",7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998,7.0829827915869998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.4504114378348003,4.5083779246543001,4.6375540476732002,4.8571163205375996,4.9494173970283999,5.0414741847237998,5.1325840458404999]
[null,null,null,null,"Coincident",4.2394863486593,4.3259385130943002,4.4359409634792,4.5698296343848996,4.656625546321,4.7431888738690002,4.8288547901651002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.5779875704388999,4.6376157328838001,4.7704948371729996,4.9963511136434002,5.0912981060317,5.1859938068069997,5.2797154362705001]
[null,null,null,null,"Coincident",4.3610160724039,4.4499464869845999,4.5631022833900001,4.7008290261396004,4.7901130421365004,4.8791578064478003,4.9672794341876001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.9805662759486,4.0373903931584998,4.1477381119435996,4.3487084103248002,4.4452423843578002,4.5384553019588996,4.6298396229280998]
[null,null,null,null,"Coincident",3.7555849061500002,3.8389508872202001,3.9282640223618999,4.0536062752167004,4.1436566219001003,4.2306131662095998,4.3158632391092997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.0946737597517,4.1531268052558996,4.2666377675750002,4.4733691093549002,4.5726703401334996,4.6685553126002004,4.7625592696216996]
[null,null,null,null,"Coincident",3.8632430417372001,3.9489988039780002,4.0408722022618999,4.1698075341149998,4.2624392769524997,4.3518885300334,4.4395823937504]
[null,"Mannum Town 7.6kV","Substation Rating","MVA","Non-Coincident",6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033]
[null,null,null,null,"Coincident",6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033,6.1627787307033]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.5852567258777999,4.6789669694224996,4.8338929789333998,5.0720428449202997,5.1994947064109001,5.3280879854108996,5.4584664262246996]
[null,null,null,null,"Coincident",4.5100277187537001,4.6287424210918999,4.7738837365154998,4.9467497836907999,5.0704490049894,5.1952418345869003,5.3216638311763003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.6914281967975997,4.7873082979952999,4.9458216142365004,5.1894858326540998,5.3198888378677998,5.4514596900764998,5.5848570394629]
[null,null,null,null,"Coincident",4.6144572644509996,4.7359208018752996,4.8844228597549,5.0612916146513998,5.1878550874111999,5.3155374909345996,5.4448867847587001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.9506056227153001,4.0058066844492002,4.1107866011159997,4.2855485237393998,4.3792998809563999,4.4720031659058996,4.5667739601820996]
[null,null,null,null,"Coincident",3.7769140540167001,3.8488593097955999,3.9473625858374999,4.0711826413625998,4.1600787197821001,4.2479496841761,4.3376139264041003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.0420817679049001,4.0985610084345998,4.2059717316703997,4.3847802609495998,4.4807024278052996,4.5755522543140996,4.6725174632610997]
[null,null,null,null,"Coincident",3.8643683765609,3.9379795224062,4.0387636386132,4.1654507435120998,4.256405207747,4.3463108214744999,4.4380512363260003]
[null,"Marion Bay 11kV","Substation Rating","MVA","Non-Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,null,null,"Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.53429757490114005,0.54005793320263995,0.55255410995880005,0.57402673762684997,0.58299677174525,0.59184106346695997,0.60053652714676997]
[null,null,null,null,"Coincident",0.52005627373699004,0.52875744370851996,0.54042188697993998,0.55499982846337004,0.56377418256657996,0.57238579438545001,0.58084051978239004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.53517252222495004,0.54094231349098998,0.55345895355622998,0.57496674406048998,0.58395146719810997,0.59281024202761001,0.60151994509953999]
[null,null,null,null,"Coincident",0.52090789999604004,0.52962331870413004,0.54130686326648003,0.55590867708526004,0.56469739976883004,0.57332311366690003,0.58179168423121996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.48585662820270997,0.48998987835697,0.49999118643064999,0.51813232479180005,0.52668269896914999,0.53474474727640997,0.54256433291766004]
[null,null,null,null,"Coincident",0.44712125024082,0.45310474440443999,0.46229306917236002,0.47437817086998002,0.48225677646164,0.48966836777143002,0.49686555250793002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.48665225029902998,0.49079226892152,0.50080995479317003,0.51898080045827,0.52754517643415999,0.53562042687431999,0.54345281759995001]
[null,null,null,null,"Coincident",0.44785344061505,0.45384673314282997,0.46305010439521999,0.47515499623954,0.48304650356461998,0.49047023184131,0.49767920243988001]
[null,"Marrabel 11kV","Substation Rating","MVA","Non-Coincident",2.66,2.66,2.66,2.66,2.66,2.66,2.66]
[null,null,null,null,"Coincident",2.66,2.66,2.66,2.66,2.66,2.66,2.66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0038553992624,1.0307870073642,1.0639164980466,1.1033807076233999,1.1320725809348,1.1612424677702999,1.190567083865]
[null,null,null,null,"Coincident",1.0038553992624,1.0307870073642,1.0639164980466,1.1033807076233999,1.1320725809348,1.1612424677702999,1.190567083865]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0043025919441999,1.0312461974095,1.0643904464581999,1.1038722363616,1.1325768911909,1.1617597724875,1.1910974519713]
[null,null,null,null,"Coincident",1.0043025919441999,1.0312461974095,1.0643904464581999,1.1038722363616,1.1325768911909,1.1617597724875,1.1910974519713]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.91233999730066995,0.93542758383058,0.96546826262911001,1.0020801840007001,1.0304962789993,1.0586293495387,1.0866533031506]
[null,null,null,null,"Coincident",0.91233999730066995,0.93542758383058,0.96546826262911001,1.0020801840007001,1.0304962789993,1.0586293495387,1.0866533031506]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.91274642214079005,0.93584429361786003,0.96589835479370001,1.0025265858682,1.0309553395322999,1.0591009426568001,1.087137380245]
[null,null,null,null,"Coincident",0.91274642214079005,0.93584429361786003,0.96589835479370001,1.0025265858682,1.0309553395322999,1.0591009426568001,1.087137380245]
[null,"McLaren Flat TF1 11kV","Substation Rating","MVA","Non-Coincident",15.4,15.4,15.4,15.4,15.4,15.4,15.4]
[null,null,null,null,"Coincident",15.4,15.4,15.4,15.4,15.4,15.4,15.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.2172608240280001,6.2661927117187002,6.4256509018171002,6.6579250054927996,6.7541336514996999,6.8445933122447,6.9323795553559]
[null,null,null,null,"Coincident",6.0749492944424004,6.1654644320005003,6.3715499833073999,6.5647242797822001,6.6191233213449996,6.6696550543553004,6.7715962348355001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5444850104291001,6.5959922600986998,6.7638429847869004,7.0083420387661004,7.1096142966763001,7.2048349912153,7.2972415619583]
[null,null,null,null,"Coincident",6.3946834018840004,6.4899624930678002,6.7068946501009004,6.9102360127139999,6.9674981611369997,7.0206894584940001,7.1279959631559002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.4305718030187,5.5458695783345,5.7595376340937001,5.9605099377597002,6.0274117340049003,6.1042833441396001,6.2031185085534997]
[null,null,null,null,"Coincident",5.4280329601646997,5.5458695783345,5.7595376340937001,5.9605099377597002,6.0274117340049003,6.0870574127561996,6.1982861087151999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.7163913126438999,5.8377573906720004,6.0626711312569004,6.2742209224077001,6.3446438650974004,6.4255613486151999,6.5295983627147001]
[null,null,null,null,"Coincident",5.7137188465094004,5.8377573906720004,6.0626711312569004,6.2742209224077001,6.3446438650974004,6.4074287894513002,6.5245116260953999]
[null,"McLaren Flat TF2 11kV","Substation Rating","MVA","Non-Coincident",16,16,16,16,16,16,16]
[null,null,null,null,"Coincident",16,16,16,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0247163871474001,6.1584451562905,6.3669965889886004,6.6494054719006996,6.7992689791442,6.9456402754880999,7.0926385972004002]
[null,null,null,null,"Coincident",4.5035166799931998,4.6355868874911001,4.8298559974707,5.0157052349033,5.0975869517383003,5.1777325009812998,5.3001498820388004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3188254008938998,6.4590824169909,6.6778147199979996,6.9740099776852,7.1311893825543997,7.2847060970128998,7.4388804463825]
[null,null,null,null,"Coincident",4.7233651780850998,4.8618826664135,5.0656354255254996,5.2605572785658996,5.3464362210683998,5.4304942413605,5.5588876805252001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7621436054029997,5.8731317418974998,6.0649131522238999,6.3347960654852002,6.4863328811976002,6.6303633860820002,6.7713838631616996]
[null,null,null,null,"Coincident",4.4060821628828997,4.5225917019765998,4.7185268745903999,4.9060368739765003,4.9845920044760996,5.0580328193095996,5.1761943336704999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0434345847537001,6.1598408371003996,6.3609844543460001,6.6440422612198002,6.8029766605779001,6.9540383129916998,7.1019429968568]
[null,null,null,null,"Coincident",4.6211741931362003,4.7433713867904004,4.9488715408360999,5.1455352293659002,5.2279251913282998,5.3049511717084004,5.4288809852254003]
[null,"McLaren Vale 11kV","Substation Rating","MVA","Non-Coincident",5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002]
[null,null,null,null,"Coincident",5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002,5.3947162426614002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"McLaren Vale Vineyard 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Meadows 11kV","Substation Rating","MVA","Non-Coincident",7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997]
[null,null,null,null,"Coincident",7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997,7.1122540250446997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.8426387551602996,5.9845505305767004,6.1588730640904998,6.361721717589,6.4993358942038997,6.6367101760193998,6.7758898087577997]
[null,null,null,null,"Coincident",5.8426387551602996,5.9845505305767004,6.1588730640904998,6.361721717589,6.4993358942038997,6.6367101760193998,6.7758898087577997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.0226219930799001,6.1689053789808002,6.3485979405485002,6.557695372894,6.6995487719098001,6.8411548861359002,6.9846219653523001]
[null,null,null,null,"Coincident",6.0226219930799001,6.1689053789808002,6.3485979405485002,6.557695372894,6.6995487719098001,6.8411548861359002,6.9846219653523001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.2451714409168,5.3675312523079999,5.4943126636669,5.6437403698314998,5.7849411131334998,5.9201194485780002,6.0512492561373001]
[null,null,null,null,"Coincident",5.2451714409168,5.3675312523079999,5.4943126636669,5.6437403698314998,5.7849411131334998,5.9201194485780002,6.0512492561373001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.4067496214171999,5.5328787425275996,5.6635656715609999,5.8175965174229001,5.9631469677736,6.1024894892184998,6.2376587673563]
[null,null,null,null,"Coincident",5.4067496214171999,5.5328787425275996,5.6635656715609999,5.8175965174229001,5.9631469677736,6.1024894892184998,6.2376587673563]
[null,"Melrose 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.32991005952932001,0.33310295139450002,0.3412199354805,0.35554451456941,0.36075526691338999,0.36585861717315998,0.37082990396205001]
[null,null,null,null,"Coincident",0.29117350197253,0.29614852511724998,0.30267323181056,0.31070750391634999,0.31537696188005998,0.31995502401448001,0.32441950033715]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.34727372309228,0.35063466166758001,0.35917885485723,0.37425735812880001,0.37974236022053998,0.38511430749455,0.39034724059818998]
[null,null,null,null,"Coincident",0.30649840214051,0.31173526825003001,0.31860338008847,0.32706050804175002,0.33197572661432001,0.33679473905740998,0.34149418749630001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.29970604312066002,0.30198667366607002,0.30831159456458002,0.32003012910723,0.32483503407196002,0.32926267640585999,0.33355805614535]
[null,null,null,null,"Coincident",0.26258960155240002,0.26621080685121001,0.27146635265049002,0.27830174602106,0.28258687091804002,0.28654567134251002,0.29039052829603001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.31548002378665002,0.31788068735427,0.32453849837047999,0.33687379704435999,0.34193159139772999,0.34659226721952002,0.35111371926724999]
[null,null,null,null,"Coincident",0.27641008796918998,0.28022188275955001,0.28575403585364001,0.29294918627731997,0.29745984375473,0.30162700181092,0.30567421937959]
[null,"Meningie 11kV","Substation Rating","MVA","Non-Coincident",6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002]
[null,null,null,null,"Coincident",6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002,6.9798076923077002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1099983994856002,2.1062317624717002,2.1305208200325998,2.1881689986833002,2.1945644631087,2.2005309470568002,2.2057998230816001]
[null,null,null,null,"Coincident",1.9479914190961001,1.953557860681,1.9713102417141,1.9987048726354,2.0047915624509001,2.0104640555147002,2.0154710381553]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1299944988502002,2.1261921660518999,2.1507114069194002,2.2089059076473001,2.2153619808116001,2.2213850081228999,2.2267038163981998]
[null,null,null,null,"Coincident",1.9664522056006,1.9720713994146,1.989992016772,2.0176462619955,2.0237906343450001,2.0295168846699001,2.0345713176414999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9955855774035001,2.0080923687879002,2.0340623220306,2.0721718673976999,2.0918132938290999,2.1098082009891002,2.1269474797568]
[null,null,null,null,"Coincident",1.9955855774035001,2.0080923687879002,2.0340623220306,2.0721718673976999,2.0918132938290999,2.1098082009891002,2.1269474797568]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0144974057281999,2.0271227218674999,2.0533387879820002,2.0918094910903,2.1116370560109998,2.1298024978746999,2.1471042026998002]
[null,null,null,null,"Coincident",2.0144974057281999,2.0271227218674999,2.0533387879820002,2.0918094910903,2.1116370560109998,2.1298024978746999,2.1471042026998002]
[null,"Milang 11kV","Substation Rating","MVA","Non-Coincident",6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212]
[null,null,null,null,"Coincident",6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212,6.8121212121212]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.6542060612531002,3.7692208879417999,3.9064320883761998,4.0636203798999002,4.1809014036301004,4.2994989859067996,4.4202727140481999]
[null,null,null,null,"Coincident",3.6542060612531002,3.7692208879417999,3.9064320883761998,4.0636203798999002,4.1809014036301004,4.2994989859067996,4.4202727140481999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8287063121216001,3.9492134716931,4.0929769542091003,4.2576714990323996,4.3805530739411003,4.5048140773584997,4.6313551446989996]
[null,null,null,null,"Coincident",3.8287063121216001,3.9492134716931,4.0929769542091003,4.2576714990323996,4.3805530739411003,4.5048140773584997,4.6313551446989996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2138905133542002,3.3094138162072002,3.4089358228172002,3.5237188860989002,3.6346661282000001,3.7430740464687999,3.8496855344164]
[null,null,null,null,"Coincident",3.2138905133542002,3.3094138162072002,3.4089358228172002,3.5237188860989002,3.6346661282000001,3.7430740464687999,3.8496855344164]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3673642615346,3.4674491134716998,3.5717236203045002,3.6919879490109002,3.8082332835717998,3.9218180333101,4.0335205673235999]
[null,null,null,null,"Coincident",3.3673642615346,3.4674491134716998,3.5717236203045002,3.6919879490109002,3.8082332835717998,3.9218180333101,4.0335205673235999]
[null,"Millicent 11kV","Substation Rating","MVA","Non-Coincident",12.47731092437,12.47731092437,12.47731092437,12.47731092437,12.47731092437,12.47731092437,12.47731092437]
[null,null,null,null,"Coincident",12.47731092437,12.47731092437,12.47731092437,12.47731092437,12.47731092437,12.47731092437,12.47731092437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.7283953149892,5.8210669757796003,5.9478937510146999,6.1054663891976002,6.1989715792205002,6.2912114829458003,6.3806414402882004]
[null,null,null,null,"Coincident",5.7283953149892,5.8210669757796003,5.9478937510146999,6.1054663891976002,6.1989715792205002,6.2912114829458003,6.3806414402882004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.8152577556951996,5.9093346418930004,6.0380845531266001,6.1980465417625998,6.2929695964016004,6.3866081785922004,6.4773942058180003]
[null,null,null,null,"Coincident",5.8152577556951996,5.9093346418930004,6.0380845531266001,6.1980465417625998,6.2929695964016004,6.3866081785922004,6.4773942058180003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.1900411924587999,5.2705122856982998,5.3866882922582997,5.5354788618670003,5.6349906688380003,5.7294138228667002,5.8201481927104002]
[null,null,null,null,"Coincident",5.1900411924587999,5.2705122856982998,5.3866882922582997,5.5354788618670003,5.6349906688380003,5.7294138228667002,5.8201481927104002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2687403081016004,5.3504316236163003,5.4683692633958998,5.6194160166860003,5.7204367695235003,5.8162917077024003,5.9084019268699004]
[null,null,null,null,"Coincident",5.2687403081016004,5.3504316236163003,5.4683692633958998,5.6194160166860003,5.7204367695235003,5.8162917077024003,5.9084019268699004]
[null,"Minlaton 11kV","Substation Rating","MVA","Non-Coincident",2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999]
[null,null,null,null,"Coincident",2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999,2.5874545454545999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8945749040418001,1.9160894467034,1.9632382281127001,2.0442396389847,2.0782009274701001,2.1156099387845999,2.1526436914413001]
[null,null,null,null,"Coincident",1.8706744763733001,1.9023503890522,1.9441556054816,1.9964265773787999,2.0281281042509001,2.0631548481962998,2.0977025322668998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9942889373152,2.0169358193833999,2.0665661047692998,2.1518307291788998,2.1875794460962998,2.2269573441467001,2.2659402331701002]
[null,null,null,null,"Coincident",1.969130597893,2.0024736565920001,2.0464791379637002,2.1015012016334,2.1348712226351001,2.1717414713708001,2.2081074466641999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7438231420759001,1.7621634357583,1.8083483169793,1.8896488396080999,1.9299874472753,1.9687867519947999,2.0065136634041001]
[null,null,null,null,"Coincident",1.6573233685643001,1.6833417146351,1.7249411646948001,1.7771839580593001,1.8138021506733,1.8489372284753001,1.8829583753462]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8356029067296,1.8549084748124001,1.9035241286425,1.9891036074643,2.0315652904760002,2.0724066549490998,2.1121191846052998]
[null,null,null,null,"Coincident",1.7445505334366,1.7719382601638001,1.8157271454042001,1.8707195474670999,1.9092650049619,1.9462492893112999,1.9820610150417]
[null,"Monarto Central 11kV","Substation Rating","MVA","Non-Coincident",8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993]
[null,null,null,null,"Coincident",8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.807790632506,1.8819940440217,1.9799849284094,2.1089501160137001,2.1402093590611,2.1719546627235,2.2045176104277]
[null,null,null,null,"Coincident",1.3115077145819001,1.3307834483530001,1.3581129890331001,1.3927733045752999,1.4128838569279001,1.4332969420816,1.4542137062572]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8854382820664,1.9628288549657,2.0650286127230002,2.1995330721393,2.2321349522741998,2.2652437701453998,2.2992053512458002]
[null,null,null,null,"Coincident",1.3678391777428001,1.3879428367138,1.4164462271525,1.4525952615686,1.4735695959840001,1.4948594574933001,1.5166746318858999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5656005836711,1.641799369636,1.7375241434063999,1.8610461000411,1.8887110699531999,1.9146160301113,1.9391170376814]
[null,null,null,null,"Coincident",1.1549390272822,1.1686942426644999,1.1902572380205001,1.2191886624002,1.2371853028837001,1.2540240076364999,1.2699311072323001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6328457631108,1.7123174151495,1.8121537290254,1.9409811615429,1.9698343884634,1.9968520102495,2.0224053773214998]
[null,null,null,null,"Coincident",1.2045456018719001,1.2188916269001999,1.2413807891899,1.2715548669284,1.2903244934028,1.3078864488585999,1.3244767851482]
[null,"Monarto South 11kV","Substation Rating","MVA","Non-Coincident",14.9,14.9,14.9,14.9,14.9,14.9,14.9]
[null,null,null,null,"Coincident",14.9,14.9,14.9,14.9,14.9,14.9,14.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.6849802720325,3.8603529947625002,4.0834548974637999,4.3730459527457999,4.4713060574560997,4.5708161269021996,4.6703735794646999]
[null,null,null,null,"Coincident",3.2074368022708999,3.2750383345960001,3.3604853346597001,3.4649613187805,3.5414802580322,3.6189234167233999,3.6962939799116001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8649848766977999,4.0489242389464,4.2829242650652999,4.58666131831,4.6897212509696002,4.7940922068761003,4.8985128604783004]
[null,null,null,null,"Coincident",3.3641142743222998,3.4350180189262001,3.5246389500099999,3.6342183965188002,3.7144751472083999,3.7957012637814,3.8768512386926002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.4445117723487,3.6351137494037999,3.8775621057366001,4.1903884880050999,4.2905616844564998,4.3879909497496001,4.4840588635755001]
[null,null,null,null,"Coincident",3.0486388443439001,3.1045527845119998,3.1869039071360001,3.2935805941997001,3.3719692030983999,3.4481814115656002,3.5232841271798998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.6127699268229998,3.8126824648569002,4.0669739837880003,4.3950813676119997,4.5001478430755997,4.6023363513189999,4.7030970085444999]
[null,null,null,null,"Coincident",3.1975593240839002,3.2562045588456998,3.3425783844904999,3.4544660342906002,3.5366837845993002,3.6166188212617998,3.6953901683572998]
[null,"Moonta 11kV","Substation Rating","MVA","Non-Coincident",12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999]
[null,null,null,null,"Coincident",12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999,12.800279329608999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.531512996689999,10.735032626842999,11.028739269241999,11.466729169489,11.567841375112,11.698678152717999,11.852101524603]
[null,null,null,null,"Coincident",10.298094500583,10.649646049828,10.989752722882001,11.381861555065999,11.540965560588999,11.698678152717999,11.852101524603]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.656395110503,10.862328065468001,11.159517465411,11.602701026301,11.705012215012999,11.83740044808,11.992643106044]
[null,null,null,null,"Coincident",10.420208750443001,10.775928979022,11.120068618685,11.516827056278,11.677817708529,11.83740044808,11.992643106044]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.2641309409969992,9.4480723736671006,9.7234174468303003,10.130287443618,10.248731022407,10.400799164425001,10.546266233760999]
[null,null,null,null,"Coincident",9.1076241351970992,9.4185273496769994,9.7234174468303003,10.085576526879001,10.248731022407,10.400799164425001,10.546266233760999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.3739845066639997,9.5601071069343,9.8387172071430005,10.250411846435,10.370259922801999,10.524131280657,10.671323290665001]
[null,null,null,null,"Coincident",9.2156218515915,9.5302117396411994,9.8387172071430005,10.205170750055,10.370259922801999,10.524131280657,10.671323290665001]
[null,"Moorkitabie 11kV","Substation Rating","MVA","Non-Coincident",1.4,1.4,1.4,1.4,1.4,1.4,1.4]
[null,null,null,null,"Coincident",1.4,1.4,1.4,1.4,1.4,1.4,1.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.68918014294445995,0.70267300783232001,0.72388640322585995,0.75591273166287998,0.77348064366795999,0.79113589181834998,0.80866384267276004]
[null,null,null,null,"Coincident",0.60585003143812,0.62087578971575996,0.63944944828607997,0.66162047656696998,0.67711940126073,0.69269897862948004,0.70816478024549001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.69133558283595997,0.70487064722641002,0.72615038840651003,0.75827688053310005,0.77589973692207004,0.79361020260382997,0.81119297286195002]
[null,null,null,null,"Coincident",0.60774485290011004,0.62281760486891002,0.64144935333782005,0.66368972244240998,0.67923712067521003,0.69486542382761995,0.71037959538884998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.62299350815029997,0.63516858776528995,0.65450612696173005,0.68414047547895995,0.70220245884694998,0.71984200128378995,0.73718421318942995]
[null,null,null,null,"Coincident",0.54125705335322005,0.55436076186135996,0.57142066758479004,0.59218520432687005,0.60791227680017002,0.62327682985516997,0.63838057942364002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.62494194655694002,0.63715510424565003,0.65655312240948005,0.68628015359842998,0.70439862657929997,0.72209333742722004,0.73948978783020003]
[null,null,null,null,"Coincident",0.54294985755876002,0.55609454846655004,0.57320780976285002,0.59403728846717996,0.60981354802128995,0.62522615436236995,0.64037714154304004]
[null,"Morgan 11kV","Substation Rating","MVA","Non-Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,null,null,"Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1715898619431999,1.1736769647423,1.1890138260769001,1.2222801791375,1.2309959570808999,1.2403821245851001,1.25040262737]
[null,null,null,null,"Coincident",0.83622623933569995,0.84163858725106,0.85151100675458002,0.86593639515233001,0.87167373570494,0.87788586101037003,0.88454782352817996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1953294198855999,1.1974588129942001,1.2131064403401,1.2470468590799,1.2559392420983999,1.2655155985711,1.2757391436612999]
[null,null,null,null,"Coincident",0.85317042936885001,0.85869244599260997,0.86876490723638,0.88348259275520002,0.88933618724009,0.89567418689236,0.90247113866737005]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0239611524543999,1.0216546200771,1.0317707371895,1.0588355567023999,1.0680652342376999,1.0779924921277,1.0891694744138001]
[null,null,null,null,"Coincident",0.73382098507028004,0.73512918205734001,0.74193219400485,0.75389712957112998,0.76007053422273996,0.76674009272985999,0.77429723305280995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0447093561553,1.0423560872358,1.0526771840567,1.0802904095193,1.0897071051160001,1.0998355159193001,1.1112389738921]
[null,null,null,null,"Coincident",0.74869016955224998,0.75002487412457997,0.75696573336965001,0.76917311067289995,0.77547160508687996,0.78227630676634996,0.78998657505362002]
[null,"Morphett Vale East 11kV","Substation Rating","MVA","Non-Coincident",57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997]
[null,null,null,null,"Coincident",57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997,57.350200758767997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.793115793902999,40.463539772828,41.698304970934998,42.888537468164003,43.241027229418002,43.647304373284001,44.476434299928997]
[null,null,null,null,"Coincident",39.793115793902999,40.463539772828,41.698304970934998,42.888537468164003,43.241027229418002,43.647304373284001,44.476434299928997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.070553920011001,40.745652103725,41.989026101015,43.187556914852003,43.542504239351999,43.951613952803001,44.786524584189003]
[null,null,null,null,"Coincident",40.070553920011001,40.745652103725,41.989026101015,43.187556914852003,43.542504239351999,43.951613952803001,44.786524584189003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.778364644755001,36.353058481262003,37.593278227082003,38.799124566187999,39.195592109374999,39.618438527621997,40.457056567138999]
[null,null,null,null,"Coincident",35.778364644755001,36.353058481262003,37.593278227082003,38.799124566187999,39.195592109374999,39.618438527621997,40.457056567138999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.027811873106998,36.606512482592002,37.855379056773003,39.069632572398,39.468864292505003,39.894658801534,40.73912369704]
[null,null,null,null,"Coincident",36.027811873106998,36.606512482592002,37.855379056773003,39.069632572398,39.468864292505003,39.894658801534,40.73912369704]
[null,"Morphettville 11kV","Substation Rating","MVA","Non-Coincident",28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002]
[null,null,null,null,"Coincident",28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002,28.487219730942002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.906054040531998,27.715741603156001,28.899840680493998,30.033059917864001,30.543024676819002,31.041184214735001,31.784406409586001]
[null,null,null,null,"Coincident",26.906054040531998,27.715741603156001,28.899840680493998,30.033059917864001,30.543024676819002,31.041184214735001,31.784406409586001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.400894659064999,28.225473528074001,29.431349872302999,30.585410623910001,31.104754360413001,31.612075761063998,32.368966869612002]
[null,null,null,null,"Coincident",27.400894659064999,28.225473528074001,29.431349872302999,30.585410623910001,31.104754360413001,31.612075761063998,32.368966869612002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.291147929400001,25.034889098891998,26.226253613101001,27.377305864518,27.924458452265998,28.444274811355999,29.210937480788001]
[null,null,null,null,"Coincident",24.291147929400001,25.034889098891998,26.226253613101001,27.377305864518,27.924458452265998,28.444274811355999,29.210937480788001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.737896703789001,25.49531633166,26.708591734483001,27.88081347464,28.438028977022999,28.967405498605,29.748168185415]
[null,null,null,null,"Coincident",24.737896703789001,25.49531633166,26.708591734483001,27.88081347464,28.438028977022999,28.967405498605,29.748168185415]
[null,"Mount Barker 11kV","Substation Rating","MVA","Non-Coincident",72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995]
[null,null,null,null,"Coincident",72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995,72.737673219464995]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.027409652066002,30.853726552586,31.839368424958,33.086245161824003,34.012108264018003,34.955618314097002,35.929760150588002]
[null,null,null,null,"Coincident",30.027409652066002,30.853726552586,31.839368424958,33.086245161824003,34.012108264018003,34.955618314097002,35.929760150588002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.103273512459999,30.931678091895002,31.919810175652,33.169837130395003,34.098039413689001,35.043933229651998,36.020536222837002]
[null,null,null,null,"Coincident",30.103273512459999,30.931678091895002,31.919810175652,33.169837130395003,34.098039413689001,35.043933229651998,36.020536222837002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.091375874848001,25.781838827775999,26.510277932567,27.372486512049001,28.227158128052999,29.091132794244999,29.977361924509001]
[null,null,null,null,"Coincident",25.091375874848001,25.781838827775999,26.510277932567,27.372486512049001,28.227158128052999,29.091132794244999,29.977361924509001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.154768910028999,25.846976308637,26.577255805362999,27.441642743620001,28.298473676358999,29.164631163321001,30.053099339968998]
[null,null,null,null,"Coincident",25.154768910028999,25.846976308637,26.577255805362999,27.441642743620001,28.298473676358999,29.164631163321001,30.053099339968998]
[null,"Mount Burr 11kV","Substation Rating","MVA","Non-Coincident",0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999]
[null,null,null,null,"Coincident",0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.39478061088449001,0.40391665081928002,0.41555975995865002,0.42955288568834998,0.43922570021010998,0.44897013095659,0.45874309394995999]
[null,null,null,null,"Coincident",0.39478061088449001,0.40391665081928002,0.41555975995865002,0.42955288568834998,0.43922570021010998,0.44897013095659,0.45874309394995999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.39671004687383998,0.40589073794843,0.41759075118386002,0.43165226639278997,0.44137235546638998,0.45116441077917002,0.46098513778627997]
[null,null,null,null,"Coincident",0.39671004687383998,0.40589073794843,0.41759075118386002,0.43165226639278997,0.44137235546638998,0.45116441077917002,0.46098513778627997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.36825945761179002,0.37605743241583001,0.38650487366222003,0.39942367389766997,0.40891320068013998,0.418139746333,0.42720153008543998]
[null,null,null,null,"Coincident",0.36825945761179002,0.37605743241583001,0.38650487366222003,0.39942367389766997,0.40891320068013998,0.418139746333,0.42720153008543998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.37005927510876002,0.37789536144314001,0.38839386312305002,0.40137580221949998,0.41091170776017,0.42018334688710002,0.42928941886247002]
[null,null,null,null,"Coincident",0.37005927510876002,0.37789536144314001,0.38839386312305002,0.40137580221949998,0.41091170776017,0.42018334688710002,0.42928941886247002]
[null,"Mount Gambier 11kV","Substation Rating","MVA","Non-Coincident",25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001]
[null,null,null,null,"Coincident",25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001,25.444066953928001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.133891467872999,14.303756130926001,14.547791530515999,14.888739753143,15.052082265729,15.215526344252,15.385675164828999]
[null,null,null,null,"Coincident",14.133891467872999,14.303756130926001,14.547791530515999,14.869020568261,15.036218503239001,15.203401566854,15.376362042307999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.277082460779001,14.448668029205001,14.695175760725,15.039578142784,15.204575484587,15.369675421297,15.541548026057001]
[null,null,null,null,"Coincident",14.277082460779001,14.448668029205001,14.695175760725,15.019659182089001,15.188551005716,15.357427807317,15.532140551936999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.867741600339,13.011188038364001,13.240640810675,13.551904644988999,13.744493514767001,13.944469054358001,14.143527084857]
[null,null,null,null,"Coincident",12.867741600339,13.011188038364001,13.240640810675,13.551904644988999,13.744493514767001,13.944469054358001,14.143527084857]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.998105180702,13.143004880055001,13.374782247143999,13.689199507221,13.883739502176001,14.085741001577,14.286815696566]
[null,null,null,null,"Coincident",12.998105180702,13.143004880055001,13.374782247143999,13.689199507221,13.883739502176001,14.085741001577,14.286815696566]
[null,"Mount Gambier North 11kV","Substation Rating","MVA","Non-Coincident",17.8125,17.8125,17.8125,17.8125,17.8125,17.8125,17.8125]
[null,null,null,null,"Coincident",17.8125,17.8125,17.8125,17.8125,17.8125,17.8125,17.8125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.1712064951898995,9.4332883203763007,9.8228999838111992,10.387689080177999,10.728693548041999,11.074955935569999,11.427997533081999]
[null,null,null,null,"Coincident",9.1183028857119997,9.4251204078236999,9.7877103336924005,10.210252949912,10.534016217357999,10.862362777285,11.196760183489999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.5812182655627005,9.8550168297827003,10.262046634219001,10.85208542673,11.208334982102,11.570077519881,11.938902341824001]
[null,null,null,null,"Coincident",9.5259495253256006,9.8464837591356993,10.225283780971999,10.666716763059,11.004954325738,11.347980083478999,11.697327199147001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4982195001188998,8.7181745524445002,9.0493038916913999,9.5392782398501996,9.8552836990330004,10.168240474998999,10.485153259424999]
[null,null,null,null,"Coincident",8.4358598622173009,8.6896817695674002,9.0062087555622998,9.3845823579310998,9.6859784919895002,9.9839847661998,10.285216478442999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8781444341053,9.1079328884432993,9.4538658335929,9.9657451786604003,10.295878109276,10.622826060975999,10.953906880093999]
[null,null,null,null,"Coincident",8.8129969203064,9.0781662953693996,9.4088440683918009,9.8041333983316008,10.119003873260001,10.430332939856999,10.745031642261001]
[null,"Mount Gambier West 11kV","Substation Rating","MVA","Non-Coincident",25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001]
[null,null,null,null,"Coincident",25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001,25.635966875560001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.430940712935,15.790335820963,16.237445805029001,16.814501079441001,17.203209874479999,17.594689955374999,17.989881366673998]
[null,null,null,null,"Coincident",15.430940712935,15.790335820963,16.237445805029001,16.775982595182999,17.145219594736002,17.516621123659998,17.891096569847999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.774500621661,16.141897429183,16.598962027694,17.188865064346,17.586228209150001,17.986424340696999,18.390414433018002]
[null,null,null,null,"Coincident",15.774500621661,16.141897429183,16.598962027694,17.149488990963,17.526946813355998,17.906617356967001,18.289430256620001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.07616281132,14.328866552429,14.679669791734,15.144618147880999,15.472333059432,15.789263549531,16.105200733099998]
[null,null,null,null,"Coincident",14.07616281132,14.328866552429,14.679669791734,15.123216979627999,15.435354108787999,15.736436623686,16.035821683201998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.38955946682,14.647889493186,15.006503139589,15.481803269992,15.816814541965,16.140801284321999,16.463772604822001]
[null,null,null,null,"Coincident",14.38955946682,14.647889493186,15.006503139589,15.459925618577,15.779012278915999,16.086798201160999,16.392848875277]
[null,"Mount Pleasant 11kV","Substation Rating","MVA","Non-Coincident",3.7,3.7,3.7,3.7,3.7,3.7,3.7]
[null,null,null,null,"Coincident",3.7,3.7,3.7,3.7,3.7,3.7,3.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5704241367221998,2.6414323209838999,2.7361170293615,2.8666364564823001,2.9510506052662002,3.0359860473187998,3.1208337002561]
[null,null,null,null,"Coincident",2.4690252172289999,2.5486635202644998,2.6431067352834998,2.7529411804031998,2.8353964176934001,2.9183824615085001,3.0012964309068]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5724863450200002,2.6435514979603001,2.738312170296,2.8689363109703998,2.9534181838142,3.0384217681514998,3.1233374929417002]
[null,null,null,null,"Coincident",2.4710060748694,2.5507082703836002,2.6452272556145999,2.7551498190728001,2.8376712088208,2.9207238309511001,3.0037043208404]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2581329149715001,2.3186313233255,2.4016772603678,2.5191489926548001,2.5999066518868998,2.6793236110007999,2.7580836750461999]
[null,null,null,null,"Coincident",2.1685566055786998,2.2364188856752998,2.3204324330757999,2.4199171525179,2.4991049660890998,2.5770483872693002,2.6543858079082998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2599445772447999,2.3204915224599998,2.4036040858686998,2.5211700637619998,2.6019925135134998,2.6814731875255999,2.7602964394531999]
[null,null,null,null,"Coincident",2.1702964022770002,2.238213127146,2.3222940772105001,2.4218586115792999,2.501109956209,2.5791159100924999,2.6565153772507002]
[null,"Mount Schank 11kV","Substation Rating","MVA","Non-Coincident",3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002]
[null,null,null,null,"Coincident",3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002,3.9415058732483002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5474345427591998,2.5701509363688002,2.6258193536143999,2.7251339866689999,2.7629330418281999,2.8012019289324002,2.8412421515676001]
[null,null,null,null,"Coincident",1.4609781789139,1.481274617582,1.5092437445806,1.5451070466976999,1.5648425840739999,1.5848197201431999,1.6057711140327999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8663527522702998,2.8919130547046001,2.9545507077269,3.0662987299109998,3.1088299211821,3.1518897635593999,3.1969426983553002]
[null,null,null,null,"Coincident",1.6438808353445999,1.6667182240434,1.6981888596201999,1.7385419572183001,1.7607482243182,1.7832263363142,1.8068006753329999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3998453248703,2.4109001268139001,2.4511473301953002,2.5314893556197999,2.5643835500139001,2.5969801811090001,2.6285604590322]
[null,null,null,null,"Coincident",1.3741616286322,1.3861514562448001,1.4071791970226,1.4365762851185,1.453819553502,1.4708889660454001,1.4873383578677]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7002865575161001,2.7127253312883002,2.7580111591466001,2.8484113566131,2.8854236382056002,2.9221011039797999,2.9576349773819999]
[null,null,null,null,"Coincident",1.5461955548533,1.5596864119489,1.5833466558692,1.6164240217279999,1.6358260079064,1.6550323728992,1.6735410955893]
[null,"Murray Bridge North 11kV","Substation Rating","MVA","Non-Coincident",26.104631217839,26.104631217839,26.104631217839,26.104631217839,26.104631217839,26.104631217839,26.104631217839]
[null,null,null,null,"Coincident",26.104631217839,26.104631217839,26.104631217839,26.104631217839,26.104631217839,26.104631217839,26.104631217839]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.504838175682,14.739050585157001,15.052730879346999,15.445864125027001,15.676105323290001,15.907838787293,16.136418781134001]
[null,null,null,null,"Coincident",14.504838175682,14.739050585157001,15.052730879346999,15.445864125027001,15.676105323290001,15.907838787293,16.136418781134001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.003626677107,15.245893120369001,15.570360168741001,15.977012375481999,16.21517104658,16.454873299054999,16.691313640678]
[null,null,null,null,"Coincident",15.003626677107,15.245893120369001,15.570360168741001,15.977012375481999,16.21517104658,16.454873299054999,16.691313640678]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.425637215598,14.59744520047,14.866775391017001,15.268022204736999,15.494985617896001,15.707509911033,15.908516177138001]
[null,null,null,null,"Coincident",14.425637215598,14.59744520047,14.866775391017001,15.228140123157001,15.452925155597001,15.663247120833001,15.861932975669999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.92170217556,15.099418247531,15.378010092742,15.793054874732,16.027823045127999,16.247655566898999,16.455573982800999]
[null,null,null,null,"Coincident",14.92170217556,15.099418247531,15.378010092742,15.751801338782,15.984316218885001,16.201870679691002,16.407388890642]
[null,"Murray Bridge South 11kV","Substation Rating","MVA","Non-Coincident",28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001]
[null,null,null,null,"Coincident",28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001,28.411048689139001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.299520845886999,16.592498851995,17.049355260171001,18.202168656845,18.512318971774,18.825039160330999,19.135119799089999]
[null,null,null,null,"Coincident",16.299520845886999,16.592498851995,16.975647208323998,17.449445196831999,17.740072533262001,18.032903945270998,18.322731142178998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.558379829601002,16.856010732542,17.320122653725999,18.491244325048001,18.806320256875999,19.124006875487002,19.439012024589999]
[null,null,null,null,"Coincident",16.558379829601002,16.856010732542,17.245244015850002,17.726566573144002,18.021809474514001,18.319291455238002,18.613721509760001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.775043898442,14.998947461363,15.410638878718,16.559080262434001,16.859501358292999,17.146408900145001,17.425284590423999]
[null,null,null,null,"Coincident",14.775043898442,14.998947461363,15.324100414328999,15.746874190198,16.030915110195998,16.302030408364001,16.565341037124]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.009692075162,15.237151537013,15.65538118472,16.822061409457,17.127253608730999,17.418717640029001,17.702022262818002]
[null,null,null,null,"Coincident",15.009692075162,15.237151537013,15.567468369565001,15.996956378999,16.285508262514998,16.560929247409,16.828421613928001]
[null,"Mylor 11kV","Substation Rating","MVA","Non-Coincident",4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004]
[null,null,null,null,"Coincident",4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0994186095602001,2.1565660609400998,2.2257636879159,2.3057916265656999,2.3626583805753998,2.4198644086497998,2.4783350907536001]
[null,null,null,null,"Coincident",2.0994186095602001,2.1565660609400998,2.2257636879159,2.3057916265656999,2.3626583805753998,2.4198644086497998,2.4783350907536001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1031486122005001,2.1603975965208,2.2297181657865002,2.3098882887635002,2.3668560770032001,2.4241637420901001,2.4827383080968]
[null,null,null,null,"Coincident",2.1031486122005001,2.1603975965208,2.2297181657865002,2.3098882887635002,2.3668560770032001,2.4241637420901001,2.4827383080968]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8912920915861999,1.9417778368983001,1.9942068935488,2.0553157309233998,2.1139058809205,2.1707687514079002,2.2267803867286]
[null,null,null,null,"Coincident",1.8912920915861999,1.9417778368983001,1.9942068935488,2.0553157309233998,2.1139058809205,2.1707687514079002,2.2267803867286]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8946523192525999,1.9452277617611,1.9977499682574,2.0589673767018999,2.1176616228584,2.1746255206760998,2.2307366709514]
[null,null,null,null,"Coincident",1.8946523192525999,1.9452277617611,1.9977499682574,2.0589673767018999,2.1176616228584,2.1746255206760998,2.2307366709514]
[null,"Mypolonga 11kV","Substation Rating","MVA","Non-Coincident",5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004]
[null,null,null,null,"Coincident",5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004,5.0633100000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8568934443031,2.9704699562236998,3.1190759780338002,3.3152179459681999,3.3567739546959001,3.3983685621794,3.4389049871597002]
[null,null,null,null,"Coincident",2.5290717093512001,2.5630595304939998,2.6106241756983,2.6715948311417002,2.7040622432845001,2.7365304145740001,2.7680837210184999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9832737383038999,3.1018745303553001,3.2570544314832999,3.4618731246987,3.505267445111,3.5487020717709998,3.5910317051459]
[null,null,null,null,"Coincident",2.6409501648862999,2.6764415040678999,2.7261102647956998,2.7897780769621998,2.8236817488647001,2.8575862134964001,2.8905353424392999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4005875616289001,2.5174257001085998,2.6642036865563998,2.8536040200630999,2.8960236405948998,2.935744579504,2.9733127911114998]
[null,null,null,null,"Coincident",2.1609266086299002,2.1866630416579,2.2270080722837,2.2811396613034001,2.3148119317592002,2.3463176686819001,2.3760803435682001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5067822684768002,2.6287889715457999,2.7820599705758999,2.9798387999204001,3.0241349357017002,3.0656130083769,3.1048431236292999]
[null,null,null,null,"Coincident",2.2565194423974,2.2833943771007998,2.3255241494158998,2.3820503556196999,2.4172121851098001,2.4501116401996001,2.4811909254797002]
[null,"Myponga 11kV","Substation Rating","MVA","Non-Coincident",13.260830860534,13.260830860534,13.260830860534,13.260830860534,13.260830860534,13.260830860534,13.260830860534]
[null,null,null,null,"Coincident",13.260830860534,13.260830860534,13.260830860534,13.260830860534,13.260830860534,13.260830860534,13.260830860534]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0941388432602999,6.1851746746523997,6.3703670481290002,6.5589000226456999,6.6311822266230998,6.7246799492087996,6.8973748287717003]
[null,null,null,null,"Coincident",6.0941388432602999,6.1851746746523997,6.3703670481290002,6.5589000226456999,6.6311822266230998,6.7245829720526,6.8973748287717003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3572316546921996,6.4521976349435004,6.6453850317444001,6.8420572481767996,6.9174599797217002,7.0149941345795002,7.1951445025309999]
[null,null,null,null,"Coincident",6.3572316546921996,6.4521976349435004,6.6453850317444001,6.8420572481767996,6.9174599797217002,7.0148929707788996,7.1951445025309999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7437782869217999,5.8416740181079998,6.0527105364998004,6.2661826217279,6.3577652256779,6.4627981236230001,6.6458899419263]
[null,null,null,null,"Coincident",5.7437782869217999,5.8416740181079998,6.0527105364998004,6.2661826217279,6.3577652256779,6.4627981236230001,6.6458899419263]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.9917455250523997,6.0938675569198999,6.3140148278505999,6.5367028125699003,6.6322391703432002,6.7418064908086999,6.9328026484234]
[null,null,null,null,"Coincident",5.9917455250523997,6.0938675569198999,6.3140148278505999,6.5367028125699003,6.6322391703432002,6.7418064908086999,6.9328026484234]
[null,"Nairne 11kV","Substation Rating","MVA","Non-Coincident",9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999]
[null,null,null,null,"Coincident",9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999,9.1921097770153999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.8755566953756002,8.1188424084178994,8.4095775420136007,8.7430801194261996,8.9904944128298006,9.2405784250807006,9.4955723601265003]
[null,null,null,null,"Coincident",7.8755566953756002,8.1188424084178994,8.4095775420136007,8.7430801194261996,8.9904944128298006,9.2405784250807006,9.4955723601265003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.9645094605048996,8.2105430347750996,8.5045619608765008,8.8418313801245993,9.0920401662075996,9.3449488250535993,9.6028228632451995]
[null,null,null,null,"Coincident",7.9645094605048996,8.2105430347750996,8.5045619608765008,8.8418313801245993,9.0920401662075996,9.3449488250535993,9.6028228632451995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.7942631516471996,6.9934456890996,7.2008505916934,7.4404298827586004,7.6718241480259,7.8977968296250998,8.1203363507943997]
[null,null,null,null,"Coincident",6.7942631516471996,6.9934456890996,7.2008505916934,7.4404298827586004,7.6718241480259,7.8977968296250998,8.1203363507943997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.8710029324311996,7.0724351949706996,7.2821826925454998,7.5244679815779003,7.7584757966584004,7.9870007924176001,8.2120538509183003]
[null,null,null,null,"Coincident",6.8710029324311996,7.0724351949706996,7.2821826925454998,7.5244679815779003,7.7584757966584004,7.9870007924176001,8.2120538509183003]
[null,"Nangwarry 11kV","Substation Rating","MVA","Non-Coincident",3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998]
[null,null,null,null,"Coincident",3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998,3.6199861878189998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.54805649432842996,0.55835787161261996,0.57426111790180001,0.59835161178968999,0.61137174869123001,0.62449534287599995,0.63783704761489002]
[null,null,null,null,"Coincident",0.37633268517376001,0.38514912165720999,0.39584102769266999,0.40874204707627998,0.41752353888042998,0.42637159023833998,0.43536426274571999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.55657927004723995,0.56704084309427005,0.58319139929168995,0.60765652221597999,0.62087913405904005,0.63420681203995,0.64775599239198001]
[null,null,null,null,"Coincident",0.38218499986136001,0.39113853993095998,0.40199671480566002,0.41509835674531997,0.42401640871416002,0.43300205529820002,0.44213457202180001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.51964774457354002,0.52645209567073004,0.53774542438100004,0.55605888154435001,0.56666003501661,0.57685289712747001,0.58702560075493004]
[null,null,null,null,"Coincident",0.35153677234573999,0.35719227798803999,0.36525592201573998,0.37560286530227999,0.38266953450284003,0.38945755749571997,0.39622896159097998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.52772873845942003,0.53463890338951003,0.54610785360726,0.56470610164464996,0.57547211267145004,0.58582348303575005,0.59615438143395005]
[null,null,null,null,"Coincident",0.35700348809242,0.36274694197849,0.37093598298668001,0.38144383062873999,0.38862039294669998,0.39551397585565001,0.40239068142805001]
[null,"Naracoorte 11kV","Substation Rating","MVA","Non-Coincident",29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001]
[null,null,null,null,"Coincident",29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001,29.838205128205001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.275281839911999,11.362616479809001,11.508785001716999,11.712217785353999,11.791147666257,11.867238759913,11.938430355709]
[null,null,null,null,"Coincident",11.275281839911999,11.362616479809001,11.508785001716999,11.712217785353999,11.791147666257,11.867238759913,11.938430355709]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.007142397465,12.100145789518001,12.255801877011001,12.472439158112,12.556492251672999,12.637522296835,12.713334825547999]
[null,null,null,null,"Coincident",12.007142397465,12.100145789518001,12.255801877011001,12.472439158112,12.556492251672999,12.637522296835,12.713334825547999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.8728807013562996,9.9192290222881994,10.030937347928001,10.200458239472001,10.2766545765,10.342191747020999,10.400380885768]
[null,null,null,null,"Coincident",9.8728807013562996,9.9192290222881994,10.030937347928001,10.200458239472001,10.2766545765,10.342191747020999,10.400380885768]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.513713638159,10.563070354665999,10.682029489523,10.862553711712,10.943695831426,11.013486915137999,11.075453018056001]
[null,null,null,null,"Coincident",10.513713638159,10.563070354665999,10.682029489523,10.862553711712,10.943695831426,11.013486915137999,11.075453018056001]
[null,"Naracoorte East 11kV","Substation Rating","MVA","Non-Coincident",17.7,17.7,17.7,17.7,17.7,17.7,17.7]
[null,null,null,null,"Coincident",17.7,17.7,17.7,17.7,17.7,17.7,17.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9253765500551001,5.0363219730994002,5.1977965828009003,5.4321376919553996,5.5699832443841002,5.7084055943583998,5.8457666227280001]
[null,null,null,null,"Coincident",4.5310344719647997,4.6538431133655003,4.8032900395897,4.9798584567082997,5.1062358662067,5.2331286304290998,5.3589831057878001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.4710793252899999,5.5943168491797,5.7736818966473997,6.0339866234701001,6.1871046529875002,6.3408633858287997,6.4934432088689]
[null,null,null,null,"Coincident",5.0330464625016003,5.1694615796212,5.3354663469692998,5.5315975070093,5.6719767907582996,5.8129285275058997,5.9527269390857001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.7265100520623999,4.8302117511697,4.9777464517842001,5.1926191863825997,5.3344899662538001,5.4726691817416002,5.6080163768869999]
[null,null,null,null,"Coincident",4.2752192278384999,4.3838279540532996,4.5233383811097996,4.6917929049208,4.8199181602643,4.9446907713553996,5.0668337085020001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2501795880611004,5.3653708259731001,5.5292515043519002,5.7679308751336,5.9255201036378002,6.0790087641203998,6.2293516330505003]
[null,null,null,null,"Coincident",4.7488883927560002,4.8695303275402999,5.0244976900099001,5.2116159850494004,5.3539367656909,5.4925334488002999,5.6282091055469996]
[null,"Narrung 11kV","Substation Rating","MVA","Non-Coincident",3.8,3.8,3.8,3.8,3.8,3.8,3.8]
[null,null,null,null,"Coincident",3.8,3.8,3.8,3.8,3.8,3.8,3.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4231255546187001,1.4403230607730999,1.475608173705,1.5351615754381001,1.5598059383009999,1.5847467993418001,1.6096025671501999]
[null,null,null,null,"Coincident",1.1772947705886001,1.1970633083005999,1.2234249468958001,1.2564898543241001,1.2768166490535,1.2973758207223001,1.3178506782171]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4666520803842999,1.484375575052,1.5207398888824,1.5821147410606,1.6075128557563001,1.6332165370748,1.6588325225706]
[null,null,null,null,"Coincident",1.2133025219774001,1.2336756836195999,1.2608435972042999,1.2949198001858999,1.3158682932268,1.3370562704936,1.3581573548237]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2203389097398001,1.2425872010690999,1.2804696048221,1.3399803735091,1.3634953230966,1.3862736969317,1.408619395803]
[null,null,null,null,"Coincident",1.1295347001747,1.1457033619649999,1.1699066114139001,1.2014898475516,1.2227499886266999,1.2433395860823999,1.2635276358601]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2576631731015999,1.2805919320275001,1.3196329752397999,1.3809638904332,1.4051980485655,1.4286731026565,1.4517022483499]
[null,null,null,null,"Coincident",1.1640817020683001,1.1807448850002999,1.2056883947567001,1.2382376092912,1.2601479952271,1.2813673288584,1.3021728334109]
[null,"New Osborne 11kV","Substation Rating","MVA","Non-Coincident",12.5,12.5,12.5,12.5,12.5,12.5,12.5]
[null,null,null,null,"Coincident",12.5,12.5,12.5,12.5,12.5,12.5,12.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"New Richmond 11kV","Substation Rating","MVA","Non-Coincident",51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999]
[null,null,null,null,"Coincident",51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999,51.333812582848999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.370040098643997,33.022842613296,33.941953411280998,35.499543616240999,36.178645300402998,36.946732447466999,37.707587062431998]
[null,null,null,null,"Coincident",32.360207515600003,33.022842613296,33.819140314670001,34.840077363200997,35.464088451224001,36.188843256421997,36.904845086778003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.357366067167,34.030079860058997,34.977224665911997,36.582323284608002,37.282138403970997,38.073653152115,38.857714767051]
[null,null,null,null,"Coincident",33.347233578268003,34.030079860058997,34.850665619057999,35.902742501124997,36.545786693524001,37.292647410169998,38.030488175494]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.881502950451999,29.420231535424001,29.930958079035001,30.936385529641001,31.514305911688002,32.175370927594997,32.816844962889]
[null,null,null,null,"Coincident",28.881502950451999,29.420231535424001,29.930958079035001,30.646114765985999,31.180154267611002,31.808507285009998,32.417669532521998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.762424252559001,30.31758472085,30.843889051135999,31.879983273497999,32.475530936797,33.156759247377003,33.817799028380001]
[null,null,null,null,"Coincident",29.762424252559001,30.31758472085,30.843889051135999,31.580858895144001,32.131187257287998,32.778705813240002,33.406448257260003]
[null,"Nildottie 11kV","Substation Rating","MVA","Non-Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,null,null,"Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2778209254921999,2.3036459599435002,2.3590778009751001,2.4534543483295002,2.4928158411421002,2.5317148179624001,2.5693431580785999]
[null,null,null,null,"Coincident",2.0160748520905001,2.0506912989494999,2.0964697020869001,2.1532107082794001,2.1874946234118,2.2213688810572001,2.2540857053462]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2852180294458999,2.3111269293418002,2.366738782369,2.4614218126096001,2.5009111298051998,2.5399364290119002,2.5776869651885002]
[null,null,null,null,"Coincident",2.0226219494028999,2.0573508113569998,2.1032778774569998,2.1602031470902001,2.1945983974384,2.2285826599582998,2.2614057304177]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2209065923304001,2.2430363256170001,2.2929934955730999,2.3809572068912002,2.4230861259381,2.4639522917966001,2.5028768572366]
[null,null,null,null,"Coincident",1.9106240388377,1.9393217844469,1.9813282441032001,2.0353414574843001,2.0712724748226998,2.1061101241570999,2.1392048806127999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2281188699731,2.2503204684076001,2.3004398716522001,2.388689240508,2.4309549710092,2.4719538475973999,2.5110048185215001]
[null,null,null,null,"Coincident",1.9168286901663001,1.9456196301988,1.9877625036291,2.0419511220870001,2.0779988235191,2.1129496062920001,2.1461518362329999]
[null,"Ninnes 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0183345622344999,1.0188237738849999,1.0249793449171001,1.0364803399942,1.0372369149862,1.0380639197499,1.0386568140062]
[null,null,null,null,"Coincident",1.0183345622344999,1.0188237738849999,1.0249793449171001,1.0364803399942,1.0372369149862,1.0380639197499,1.0386568140062]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0293165037594001,1.0298109911747999,1.0360329452243999,1.0476579695352,1.0484227035967,1.0492586269596,1.0498579151166001]
[null,null,null,null,"Coincident",1.0293165037594001,1.0298109911747999,1.0360329452243999,1.0476579695352,1.0484227035967,1.0492586269596,1.0498579151166001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.91093628459663001,0.90704726715755002,0.90955435048269995,0.91755220966341999,0.91742019487104998,0.91665253303391003,0.91543635476248997]
[null,null,null,null,"Coincident",0.91093628459663001,0.90704726715755002,0.90955435048269995,0.91755220966341999,0.91742019487104998,0.91665253303391003,0.91543635476248997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.92076001972392996,0.91682906227446004,0.91936318253176996,0.92744729236636003,0.92731385389775001,0.92653791342830005,0.92530861962572997]
[null,null,null,null,"Coincident",0.92076001972392996,0.91682906227446004,0.91936318253176996,0.92744729236636003,0.92731385389775001,0.92653791342830005,0.92530861962572997]
[null,"Noarlunga Centre 11kV","Substation Rating","MVA","Non-Coincident",28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001]
[null,null,null,null,"Coincident",28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001,28.272321428571001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.706922464582998,18.997094179771,19.517734803797001,20.261029479626998,20.597265430389001,20.922916739344,21.267188546118]
[null,null,null,null,"Coincident",17.636022071393,18.034493205116,18.672914007193,19.274974713296,19.475790988787999,19.67128220244,20.043498162875999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.077342956422999,19.373260434959999,19.904210395349999,20.662223236603001,21.005117080264998,21.337216692956002,21.688305512643002]
[null,null,null,null,"Coincident",17.985237394338,18.391598755522001,19.042661088988002,19.656643351043002,19.861436040276001,20.060798224774999,20.440384527361001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.488061804257999,16.680612695128001,17.093525065255001,17.721821840232,18.100440225835001,18.477665809584,18.845131353149]
[null,null,null,null,"Coincident",15.900882914934,16.199915778261001,16.772453596936,17.309704549588002,17.542950593008001,17.777657672086001,18.168347457536001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.814546076302001,17.010909715945001,17.431998268099999,18.072736106049,18.458851609838,18.843546732551999,19.218288554063999]
[null,null,null,null,"Coincident",16.215740309634,16.520694398139,17.104569182624001,17.652458376948001,17.890322984127,18.129677557297999,18.528103489768]
[null,"North Adelaide 11kV","Substation Rating","MVA","Non-Coincident",70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001]
[null,null,null,null,"Coincident",70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001,70.117696811971001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.084800400679001,24.510120906645,25.062462565579001,25.754829819895001,26.183121649429001,26.614085988271999,27.075158576001002]
[null,null,null,null,"Coincident",24.084800400679001,24.510120906645,25.062462565579001,25.754829819895001,26.183121649429001,26.614085988271999,27.075158576001002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.386841861278999,25.835155496671,26.417357139012999,27.147154260135999,27.598599850964,28.052862428857999,28.538860929011999]
[null,null,null,null,"Coincident",25.386841861278999,25.835155496671,26.417357139012999,27.147154260135999,27.598599850964,28.052862428857999,28.538860929011999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.764133892566999,21.034969818861001,21.34225869242,21.821946936473001,22.129968627438,22.511459325171,22.899095426100001]
[null,null,null,null,"Coincident",20.764133892566999,21.034969818861001,21.34225869242,21.821946936473001,22.129968627438,22.511459325171,22.899095426100001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.886657757070999,22.172135266403998,22.496036395290002,23.001656927406,23.326330490328999,23.728444846843001,24.137036831425998]
[null,null,null,null,"Coincident",21.886657757070999,22.172135266403998,22.496036395290002,23.001656927406,23.326330490328999,23.728444846843001,24.137036831425998]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Northfield 11kV","Substation Rating","MVA","Non-Coincident",26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002]
[null,null,null,null,"Coincident",26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002,26.532076395690002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.338847399999999,24.623109899999999,26.073060999999999,27.663330800000001,29.0125472,29.5979405,30.202256800000001]
[null,null,null,null,"Coincident",22.338847399999999,24.623109899999999,26.073060999999999,27.663330800000001,29.0125472,29.5979405,30.202256800000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.111544299999998,25.474819,26.9749236,28.6202006,30.016086099999999,30.621728099999999,31.2469477]
[null,null,null,null,"Coincident",23.111544299999998,25.474819,26.9749236,28.6202006,30.016086099999999,30.621728099999999,31.2469477]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.674429700000001,22.3846454,23.7027827,25.148482600000001,26.3750429,26.9072186,27.4565971]
[null,null,null,null,"Coincident",19.674429700000001,22.3846454,23.7027827,25.148482600000001,26.3750429,26.9072186,27.4565971]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.354964800000001,23.158926399999999,24.522657899999999,26.018364200000001,27.287351000000001,27.837934600000001,28.406316100000002]
[null,null,null,null,"Coincident",20.354964800000001,23.158926399999999,24.522657899999999,26.018364200000001,27.287351000000001,27.837934600000001,28.406316100000002]
[null,"North Unley 11kV","Substation Rating","MVA","Non-Coincident",26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001]
[null,null,null,null,"Coincident",26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001,26.007714843750001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.538582718829002,17.792216159241999,18.252968102046001,18.91968084893,19.204332117448999,19.477722769530999,19.765993140614]
[null,null,null,null,"Coincident",16.751326940702999,17.112097460908,17.691824043882999,18.234864762971998,18.396753090699001,18.552611664217999,18.872894476569002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.084619458029,18.346149384661,18.821246129007999,19.508715949603001,19.802229396609999,20.084131645243001,20.381376869993002]
[null,null,null,null,"Coincident",17.272853684716999,17.644856238982001,18.242631715533999,18.802579170375999,18.969507641654001,19.13021863162,19.460472955654001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.244402021947,15.410009229596,15.778725925077,16.345028606985998,16.600765600365001,16.835412260133999,17.075949891884999]
[null,null,null,null,"Coincident",14.894243801721,15.162125566816,15.685318096353001,16.174222236165999,16.300392133630002,16.409963642434001,16.678521987627999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.719012981371,15.889776114165,16.269972235625001,16.853905878643001,17.117604849121001,17.359556870961001,17.607583271115001]
[null,null,null,null,"Coincident",15.357953124687,15.634174975629,16.173656298129998,16.677781714746001,16.807879717491002,16.920862566328999,17.197782061647999]
[null,"Norwood 11kV","Substation Rating","MVA","Non-Coincident",85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003]
[null,null,null,null,"Coincident",85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003,85.596856481922003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",61.236136941533999,62.705858825881997,64.536460924240004,66.749243372701997,68.299860158570993,69.874334905989002,71.497794630388]
[null,null,null,null,"Coincident",61.236136941533999,62.705858825881997,64.536460924240004,66.749243372701997,68.299860158570993,69.874334905989002,71.497794630388]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.241509002449,63.735360712643001,65.596017551489993,67.845129359734003,69.421204100195993,71.021528501114005,72.671642112097999]
[null,null,null,null,"Coincident",62.241509002449,63.735360712643001,65.596017551489993,67.845129359734003,69.421204100195993,71.021528501114005,72.671642112097999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",52.728256793165997,53.878158584003003,55.164104282586997,56.925554688795003,58.218848973077002,59.657812113288003,61.106005952121997]
[null,null,null,null,"Coincident",52.728256793165997,53.878158584003003,55.164104282586997,56.925554688795003,58.218848973077002,59.657812113288003,61.106005952121997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",53.593946871741998,54.762727696938001,56.069785992459003,57.860155809875998,59.174683339834999,60.637271310254,62.109241528478002]
[null,null,null,null,"Coincident",53.593946871741998,54.762727696938001,56.069785992459003,57.860155809875998,59.174683339834999,60.637271310254,62.109241528478002]
[null,"Nuriootpa 11kV","Substation Rating","MVA","Non-Coincident",13.7,13.7,13.7,13.7,13.7,13.7,13.7]
[null,null,null,null,"Coincident",13.7,13.7,13.7,13.7,13.7,13.7,13.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.080536567733001,10.394604725665999,10.61288453157,10.88742262763,11.049197254319999,11.210366653803,11.369175467937]
[null,null,null,null,"Coincident",10.080536567733001,10.394604725665999,10.61288453157,10.88742262763,11.049197254319999,11.210366653803,11.369175467937]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.241470521923,10.560552721540001,10.782317325307,11.061238372718,11.225595702242,11.389338142214999,11.550682310519001]
[null,null,null,null,"Coincident",10.241470521923,10.560552721540001,10.782317325307,11.061238372718,11.225595702242,11.389338142214999,11.550682310519001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6873574339192992,8.9398387339796006,9.1003019290230007,9.3153334351012003,9.4470413422041002,9.5702444561882007,9.6881108952463002]
[null,null,null,null,"Coincident",8.6873574339192992,8.9398387339796006,9.1003019290230007,9.3153334351012003,9.4470413422041002,9.5702444561882007,9.6881108952463002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8260495336815001,9.0825616523102006,9.2455866134170996,9.4640510588350004,9.5978616589985997,9.7230316885499004,9.8427798441194998]
[null,null,null,null,"Coincident",8.8260495336815001,9.0825616523102006,9.2455866134170996,9.4640510588350004,9.5978616589985997,9.7230316885499004,9.8427798441194998]
[null,"Oaklands 11kV","Substation Rating","MVA","Non-Coincident",58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998]
[null,null,null,null,"Coincident",58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998,58.068924205378998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.522507800337003,48.540990288595999,50.184446726087998,51.812306523110003,52.425857348629997,53.012512361044998,54.009381002426998]
[null,null,null,null,"Coincident",47.522507800337003,48.540990288595999,50.184446726087998,51.812306523110003,52.425857348629997,53.012512361044998,54.009381002426998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.208324200553001,49.241504818731997,50.908678636261001,52.560030731937999,53.182435955888998,53.777557222452003,54.788812075647002]
[null,null,null,null,"Coincident",48.208324200553001,49.241504818731997,50.908678636261001,52.560030731937999,53.182435955888998,53.777557222452003,54.788812075647002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.875453504634997,42.771805831503002,44.426338366631001,45.98246008492,46.503789486088998,46.968379886751002,47.826878417233999]
[null,null,null,null,"Coincident",41.875453504634997,42.771805831503002,44.426338366631001,45.98246008492,46.503789486088998,46.968379886751002,47.826878417233999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.479774995844998,43.389062943212998,45.067472701993999,46.646051437906003,47.174904353084997,47.646199444448001,48.517087312088996]
[null,null,null,null,"Coincident",42.479774995844998,43.389062943212998,45.067472701993999,46.646051437906003,47.174904353084997,47.646199444448001,48.517087312088996]
[null,"Orroroo 11kV","Substation Rating","MVA","Non-Coincident",2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001]
[null,null,null,null,"Coincident",2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001,2.5880294659300001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3736318620934,1.3673922442396,1.3805055106896,1.4171905401761999,1.4161617498782,1.4138657123983001,1.4102168199442]
[null,null,null,null,"Coincident",1.2757142184849,1.2792368286883999,1.2885595987455001,1.3032050449632,1.3027374354759,1.3010996388972,1.29820967396]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3987591586576,1.3924054019776999,1.4057585441499001,1.4431146381633,1.4420670286171,1.4397289906446999,1.4360133504649]
[null,null,null,null,"Coincident",1.2990503468782,1.3026373947770999,1.3121307025266,1.3270440520161999,1.3265678887362,1.3249001326018,1.3219573026955]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2433016115783,1.2343187690071999,1.2411864835019999,1.2684897352755,1.2671948326157001,1.2636786081136,1.2589305180767001]
[null,null,null,null,"Coincident",1.1462656264632001,1.1449644027582999,1.1499790706669,1.1607502073514,1.1600033931528999,1.1572168009868,1.1532926452436001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2660448291572,1.2568976670508001,1.2638910098916001,1.2916937090959,1.2903751193013,1.2867945739151001,1.2819596289720001]
[null,null,null,null,"Coincident",1.1672338036964001,1.1659087772283001,1.1710151764451,1.1819833452116999,1.1812228698406,1.1783853036620999,1.1743893649121999]
[null,"Padthaway 11kV","Substation Rating","MVA","Non-Coincident",13.628013795266,13.628013795266,13.628013795266,13.628013795266,13.628013795266,13.628013795266,13.628013795266]
[null,null,null,null,"Coincident",13.628013795266,13.628013795266,13.628013795266,13.628013795266,13.628013795266,13.628013795266,13.628013795266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5447475717728998,3.5492718469555999,3.5768506754131999,3.6405432058447,3.6530840819338,3.6648036358598,3.6746811969958002]
[null,null,null,null,"Coincident",3.2168694656285002,3.2288598819683001,3.2577165938649002,3.3026264245607999,3.3123705231064999,3.3213856712847001,3.3287389988907998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6400372596941,3.6446831561661002,3.6730033570075,3.7384080661554999,3.7512860653103002,3.7633206635698002,3.7734637527014998]
[null,null,null,null,"Coincident",3.3033451543077001,3.3156578962879002,3.3452903325526999,3.391407426577,3.4014134653852999,3.4106709582265999,3.4182219575368]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2980691179654,3.3070745429750001,3.3361534981230001,3.3991640247118,3.4254860462034,3.4483721774822,3.4685181343400999]
[null,null,null,null,"Coincident",2.9289411127770002,2.9415603864606998,2.9738327718848998,3.0233296400410001,3.0452763739048998,3.0641719744604998,3.0806320882690001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3867276107438,3.395975119039,3.4258357728848998,3.4905401446045001,3.5175697530716001,3.5410711079349002,3.5617586271757]
[null,null,null,null,"Coincident",3.0076767290444,3.0206352332733002,3.0537751629930998,3.1046026029385998,3.1271393075630001,3.1465428584997999,3.1634454520832]
[null,"Palmer 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2646528245091999E-2,1.2866144831077999E-2,1.3155940986926001E-2,1.3514569021222E-2,1.3732283592559E-2,1.3947426863167999E-2,1.4155006167653E-2]
[null,null,null,null,"Coincident",1.2646528245091999E-2,1.2866144831077999E-2,1.3155940986926001E-2,1.3514569021222E-2,1.3732283592559E-2,1.3947426863167999E-2,1.4155006167653E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2899122743889E-2,1.3123125825551999E-2,1.3418710203537E-2,1.3784501268415E-2,1.4006564345677999E-2,1.4226004764529E-2,1.4437730138935999E-2]
[null,null,null,null,"Coincident",1.2899122743889E-2,1.3123125825551999E-2,1.3418710203537E-2,1.3784501268415E-2,1.4006564345677999E-2,1.4226004764529E-2,1.4437730138935999E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2284472071943E-2,1.2461536538261E-2,1.2723906983741999E-2,1.3062939202385999E-2,1.3285511513873E-2,1.3500727562225E-2,1.3704147887348E-2]
[null,null,null,null,"Coincident",1.2284472071943E-2,1.2461536538261E-2,1.2723906983741999E-2,1.3062939202385999E-2,1.3285511513873E-2,1.3500727562225E-2,1.3704147887348E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2529835068480001E-2,1.2710436118851001E-2,1.2978047001067E-2,1.3323850854715E-2,1.3550868697842999E-2,1.3770383348058E-2,1.3977866674035E-2]
[null,null,null,null,"Coincident",1.2529835068480001E-2,1.2710436118851001E-2,1.2978047001067E-2,1.3323850854715E-2,1.3550868697842999E-2,1.3770383348058E-2,1.3977866674035E-2]
[null,"Panorama 11kV","Substation Rating","MVA","Non-Coincident",58.509328028294,58.509328028294,58.509328028294,58.509328028294,58.509328028294,58.509328028294,58.509328028294]
[null,null,null,null,"Coincident",58.509328028294,58.509328028294,58.509328028294,58.509328028294,58.509328028294,58.509328028294,58.509328028294]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.963055907840001,29.604097279438999,30.725907547933001,31.783384731725,32.174447867306,32.549415527327,33.17691910181]
[null,null,null,null,"Coincident",27.963055907840001,29.604097279438999,30.725907547933001,31.783384731725,32.174447867306,32.549415527327,33.17691910181]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.272039030953,29.931213402387002,31.065419327545001,32.134581307302,32.529965569635998,32.909076506380003,33.543513801370999]
[null,null,null,null,"Coincident",28.272039030953,29.931213402387002,31.065419327545001,32.134581307302,32.529965569635998,32.909076506380003,33.543513801370999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.704180536826001,26.219669016390998,27.259786800299,28.241635308953001,28.589392245856001,28.903097751171,29.460389383371002]
[null,null,null,null,"Coincident",24.704180536826001,26.219669016390998,27.259786800299,28.241635308953001,28.589392245856001,28.903097751171,29.460389383371002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.977154094557999,26.509388253316001,27.560999017187001,28.553696648327001,28.905296191876001,29.222468046043002,29.785917578494999]
[null,null,null,null,"Coincident",24.977154094557999,26.509388253316001,27.560999017187001,28.553696648327001,28.905296191876001,29.222468046043002,29.785917578494999]
[null,"Parafield Gardens 11kV","Substation Rating","MVA","Non-Coincident",74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994]
[null,null,null,null,"Coincident",74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994,74.496640110841994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.259305042954999,35.391181832889998,36.053167909147,37.588064493402001,38.083735122561002,38.569046238097997,39.036961526348001]
[null,null,null,null,"Coincident",34.259305042954999,35.391181832889998,36.053167909147,37.206666494113001,37.784492340132999,38.352612706739002,38.903706500877]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.545384609827003,35.686713045714001,36.354226983370999,37.901940597904002,38.401750284720997,38.891113951632001,39.362936528802003]
[null,null,null,null,"Coincident",34.545384609827003,35.686713045714001,36.354226983370999,37.517357765347001,38.100008699545,38.672873109504998,39.228568767976]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.627635369496002,31.943246322341,32.406428103608,33.425743509950998,33.835238920747997,34.239702463770001,34.603832139242002]
[null,null,null,null,"Coincident",30.627635369496002,31.943246322341,32.406428103608,33.069447342623,33.544439833349998,34.01493536369,34.445709965208003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.883388971323001,32.209985827445003,32.677035370863003,33.704862488392003,34.117777357628,34.525618340884002,34.892788651876998]
[null,null,null,null,"Coincident",30.883388971323001,32.209985827445003,32.677035370863003,33.345591098622002,33.824549975876998,34.298974341240999,34.733346091366997]
[null,"Paralowie 11kV","Substation Rating","MVA","Non-Coincident",27.612735849057,27.612735849057,27.612735849057,27.612735849057,27.612735849057,27.612735849057,27.612735849057]
[null,null,null,null,"Coincident",27.612735849057,27.612735849057,27.612735849057,27.612735849057,27.612735849057,27.612735849057,27.612735849057]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.833415476778999,20.552737085015,21.003817625865999,21.704885196389,22.058247133238002,22.406298476920998,22.744556184467999]
[null,null,null,null,"Coincident",19.833415476778999,20.552737085015,21.003817625865999,21.704885196389,22.058247133238002,22.406298476920998,22.744556184467999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.224417808752001,20.957920354536999,21.417893642256001,22.132782284358001,22.493110512086002,22.848023451905998,23.192949680698]
[null,null,null,null,"Coincident",20.224417808752001,20.957920354536999,21.417893642256001,22.132782284358001,22.493110512086002,22.848023451905998,23.192949680698]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.543283925312,19.437786764051999,19.804919256677,20.297293189748999,20.677422977500999,21.057432340051999,21.415115372011002]
[null,null,null,null,"Coincident",18.543283925312,19.437786764051999,19.804919256677,20.297293189748999,20.677422977500999,21.057432340051999,21.415115372011002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.908852188918001,19.820989544330999,20.195359805001001,20.697440556158,21.085064344812,21.472565334161999,21.837299844459999]
[null,null,null,null,"Coincident",18.908852188918001,19.820989544330999,20.195359805001001,20.697440556158,21.085064344812,21.472565334161999,21.837299844459999]
[null,"Parilla 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.962703532888,1.9863694618951,2.0349769269875,2.1170512146292002,2.1509835267457,2.1853252634124001,2.2195585931237001]
[null,null,null,null,"Coincident",1.4777773035346,1.5025520492883,1.5355998444095,1.5770612076882,1.6025343312258999,1.6282995131775,1.6539655246972]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0506464268832998,2.0753727556151,2.1261581763073001,2.2119099680940999,2.2473626859557001,2.2832431734610998,2.3190103966184998]
[null,null,null,null,"Coincident",1.5439920988797999,1.5698769271309001,1.6044054954277001,1.6477246187882,1.6743391170498001,1.7012587599922,1.7280747889712]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4559138608329001,1.4824569755920001,1.5276522211631001,1.5986509841367,1.6267052736198,1.6538807983277,1.6805401242389]
[null,null,null,null,"Coincident",1.2264986924365999,1.2440553399139,1.2703362977253001,1.3046307712106,1.3277159718914999,1.3500730666787,1.3719941432524001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5211490204910001,1.5488814530907999,1.5961017628775001,1.6702817687547999,1.6995930873127001,1.7279862662657,1.7558401170928]
[null,null,null,null,"Coincident",1.2814544423433001,1.2997977508533001,1.327256280034,1.3630873866357001,1.3872069663363999,1.4105658158887999,1.4334691105516]
[null,"Paringa 11kV","Substation Rating","MVA","Non-Coincident",3.5625,3.5625,3.5625,3.5625,3.5625,3.5625,3.5625]
[null,null,null,null,"Coincident",3.5625,3.5625,3.5625,3.5625,3.5625,3.5625,3.5625]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7835309552946002,2.8671590092105999,2.9465601842406999,3.0501699065315,3.1013835297758998,3.1507082606962,3.1972806497767001]
[null,null,null,null,"Coincident",2.5700380396660001,2.6846543733071999,2.7502998810411001,2.829033363193,2.8769110146255001,2.9229898782108998,2.9664753358365998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8476962633773999,2.9332520917389,3.0144836041856999,3.1204817136932999,3.1728759014675001,3.2233376546111998,3.2709836195711999]
[null,null,null,null,"Coincident",2.6292819587199001,2.7465404014224002,2.8136991541302998,2.894247582198,2.9432288981141999,2.9903699609442,3.0348578352236002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.5031223032226002,2.5785023669611,2.6495497301884998,2.7443602138147001,2.7964933396295999,2.8447075088634999,2.8895241356749999]
[null,null,null,null,"Coincident",2.3163880407697,2.4208856720024001,2.4799572293750001,2.5527632170171999,2.6015334137271,2.6466073376716999,2.6884755936768001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5608236962859001,2.6379414037189002,2.7106265342364999,2.8076225670767001,2.8609574535808,2.9102830446283998,2.9561327738959999]
[null,null,null,null,"Coincident",2.3697848790526002,2.4766913653725,2.5371246265446001,2.6116089208778002,2.6615033568175002,2.7076163143718999,2.7504497076751999]
[null,"Paringa 33kV","Substation Rating","MVA","Non-Coincident",34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002]
[null,null,null,null,"Coincident",34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002,34.643267817427002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.490773641985001,17.022032658311002,17.527876427776999,18.180508196685999,18.522907104712999,18.855590118716002,19.179114164802002]
[null,null,null,null,"Coincident",12.854004866825999,13.455565532284,13.811726511346,14.235541428169,14.50554447521,14.767710917803001,15.022508567384]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.169906071020002,17.723043698626,18.249719414204002,18.929228236191999,19.285728010991999,19.632111766287998,19.968959363837001]
[null,null,null,null,"Coincident",13.383365813593,14.009700292870001,14.380528896149,14.821797600173999,15.102920066422,15.375883196717,15.641174068170001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.569627442292999,16.079107774055998,16.561355464931999,17.195046142081999,17.563589472088001,17.909211252315,18.240801837429]
[null,null,null,null,"Coincident",12.163579510517,12.744494826681001,13.086452337415,13.502889012335,13.793765226450001,14.06637806703,14.327737978881]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.210824704084001,16.741286744938002,17.243394634784998,17.903182322189,18.286903213439,18.646758586596999,18.992004923976001]
[null,null,null,null,"Coincident",12.664506967171,13.269345868626001,13.625386068258001,14.05897267542,14.361827919394001,14.645667657183999,14.917791041729]
[null,"Paskeville 11kV","Substation Rating","MVA","Non-Coincident",1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403]
[null,null,null,null,"Coincident",1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403,1.2285943983403]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.28805472606909999,0.28741909336804999,0.28810760575132,0.29124098248166003,0.29125496856075,0.29129573495362998,0.29132823872975999]
[null,null,null,null,"Coincident",0.27461186479631999,0.27441726175572001,0.27573795104364002,0.27850592737039997,0.27839493609018001,0.27831546834970999,0.27823332038247001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.28806583031728999,0.28743017311317998,0.28811871203798001,0.29125220955714998,0.29126619617538002,0.29130696413976997,0.29133946916890002]
[null,null,null,null,"Coincident",0.27462245083441,0.27442784029203998,0.27574858049133999,0.27851666352107002,0.27840566796222999,0.27832619715835999,0.27824404602439001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.26779892111957998,0.26626300952885001,0.26561144479542997,0.26699480396684999,0.26674578594506998,0.26632033464897997,0.26582251951764002]
[null,null,null,null,"Coincident",0.25123086799649003,0.24983884512936,0.25020048612905998,0.25208340433608001,0.25174166182870999,0.25123850814038001,0.25067165273885]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.26780924452487997,0.26627327372615001,0.2656216838755,0.26700509637417003,0.26675606875295998,0.26633060105611001,0.26583276673445]
[null,null,null,null,"Coincident",0.25124055271837997,0.24984847619003001,0.25021013113066998,0.25209312192248001,0.25175136624124,0.25124819315678998,0.25068131590350001]
[null,"Peake 11kV","Substation Rating","MVA","Non-Coincident",0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999]
[null,null,null,null,"Coincident",0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999,0.36199861878188999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.12703696656328001,0.12842101962967001,0.13140810432972,0.13655343035072001,0.13859076330135001,0.14065604256653999,0.14273972576610999]
[null,null,null,null,"Coincident",0.12573660562476,0.12769765973475,0.13035210516672999,0.13372023414317,0.13573188286030999,0.13776976887621001,0.13982409779127]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.13028261490758,0.13170202893749999,0.13476543021512,0.14004221339643999,0.14213159786008001,0.14424964263446999,0.14638656154258001]
[null,null,null,null,"Coincident",0.12894903124309001,0.13096018802948001,0.13368245148839999,0.13713663228527001,0.13919967631281999,0.14128962797191,0.14339644262731999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.11196490773055,0.11356762318959,0.11596676558947,0.11909744773623999,0.12120485509029,0.12324579493833999,0.12524693145081001]
[null,null,null,null,"Coincident",0.11196490773055,0.11356762318959,0.11596676558947,0.11909744773623999,0.12120485509029,0.12324579493833999,0.12524693145081001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.11482548231153,0.11646914530667,0.11892958303473999,0.12214025050863,0.12430149969609,0.12639458320922001,0.12844684645734999]
[null,null,null,null,"Coincident",0.11482548231153,0.11646914530667,0.11892958303473999,0.12214025050863,0.12430149969609,0.12639458320922001,0.12844684645734999]
[null,"Pellaring Flat 11kV","Substation Rating","MVA","Non-Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.4121868557868998E-2,9.5947905778032999E-2,9.8303202807663997E-2,0.10118531975229,0.10302338603926001,0.10485133846965999,0.10664118376769]
[null,null,null,null,"Coincident",9.4121868557868998E-2,9.5947905778032999E-2,9.8303202807663997E-2,0.10118531975229,0.10302338603926001,0.10485133846965999,0.10664118376769]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.6002845592342997E-2,9.7865375225247006E-2,0.10026774165214,0.10320745621852,0.10508225531291999,0.10694673843056,0.10877235286441]
[null,null,null,null,"Coincident",9.6002845592342997E-2,9.7865375225247006E-2,0.10026774165214,0.10320745621852,0.10508225531291999,0.10694673843056,0.10877235286441]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.1481446673474997E-2,8.2709470697182999E-2,8.4503949861409994E-2,8.6812905143240998E-2,8.8352641223678002E-2,8.9847988279435007E-2,9.1278704062353999E-2]
[null,null,null,null,"Coincident",8.1481446673474997E-2,8.2709470697182999E-2,8.4503949861409994E-2,8.6812905143240998E-2,8.8352641223678002E-2,8.9847988279435007E-2,9.1278704062353999E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.3109811391227001E-2,8.4362376842148007E-2,8.6192717747631001E-2,8.8547816310777003E-2,9.0118323223230004E-2,9.1643554019222001E-2,9.3102861919699006E-2]
[null,null,null,null,"Coincident",8.3109811391227001E-2,8.4362376842148007E-2,8.6192717747631001E-2,8.8547816310777003E-2,9.0118323223230004E-2,9.1643554019222001E-2,9.3102861919699006E-2]
[null,"Penfield 11kV","Substation Rating","MVA","Non-Coincident",50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001]
[null,null,null,null,"Coincident",50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001,50.639915966387001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.750326378105001,40.338019222592997,41.157017972425002,42.789471267739998,42.955789098155002,43.115159575494999,43.307428655839999]
[null,null,null,null,"Coincident",33.713753331275001,34.527987781230003,34.917247418522003,35.716646220017999,35.938397745317999,36.153388414821002,36.394882861976001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.522577427766997,42.136472302663002,42.991985756304999,44.697221273296996,44.870954311997998,45.037430252903,45.238271566747997]
[null,null,null,null,"Coincident",35.216866391556003,36.067403131079999,36.474017740359002,37.309057390474997,37.540695611288001,37.765271546485003,38.017532918755997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.079996281966999,39.014108567648002,39.923267828907001,41.354431232929997,41.662531703119001,41.972091724229998,42.330660751590997]
[null,null,null,null,"Coincident",32.424276349990002,33.671029275837,33.978539111787001,34.500935138894,34.830515914505,35.161163289164001,35.532760221282999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.777776389225998,40.753535665752999,41.703229398094997,43.198200601350997,43.520037597285999,43.843399217588001,44.217954889411999]
[null,null,null,null,"Coincident",33.869898638702999,35.172237502648997,35.493457531173,36.039144358426,36.383419349877002,36.728808494233,37.116972914294003]
[null,"Penneshaw 11kV","Substation Rating","MVA","Non-Coincident",2.09,2.09,2.09,2.09,2.09,2.09,2.09]
[null,null,null,null,"Coincident",2.09,2.09,2.09,2.09,2.09,2.09,2.09]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8704167989339999,1.9025542631017001,1.9686645758781001,2.0301800860573,2.0528244544121002,2.0820943861610002,2.1102901438355]
[null,null,null,null,"Coincident",1.8612280817080999,1.9025542631017001,1.9686645758781001,2.0301800860573,2.0488033079357,2.0662067201435002,2.0992710871385998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8708288888839,1.9029734335729001,1.9690983117634999,2.0306273750308002,2.0532767323894001,2.0825531128853001,2.1107550826449]
[null,null,null,null,"Coincident",1.8616381472012,1.9029734335729001,1.9690983117634999,2.0306273750308002,2.0492546999746,2.0666619464995999,2.0997335982310998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8371396582999,1.8771327028322999,1.9496196079523,2.0177343131957999,2.0403976749326,2.0605266955071002,2.0977447739141999]
[null,null,null,null,"Coincident",1.8371396582999,1.8771327028322999,1.9496196079523,2.0177343131957999,2.0403976749326,2.0605266955071002,2.0977447739141999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8375444166351,1.8775462724291001,1.9500491478533,2.0181788601183999,2.0408472150437,2.0609806704410998,2.0982069487296]
[null,null,null,null,"Coincident",1.8375444166351,1.8775462724291001,1.9500491478533,2.0181788601183999,2.0408472150437,2.0609806704410998,2.0982069487296]
[null,"Penola 11kV","Substation Rating","MVA","Non-Coincident",4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004]
[null,null,null,null,"Coincident",4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004,4.2637190224874004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7907828839182001,2.8081124718065,2.8589885928148,2.9495402321716999,2.9840643646917,3.0181723176160999,3.0513763520703998]
[null,null,null,null,"Coincident",2.4886263320188999,2.5154622114306999,2.5592390068689999,2.6165811313163001,2.6464934017427999,2.6760246973020001,2.7047419849968]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8756444389171998,2.8935009813687,2.9459241330564998,3.0392292481380001,3.0748031834168001,3.1099482839960002,3.144161979937]
[null,null,null,null,"Coincident",2.5642999724025,2.5919518717455001,2.6370598230237001,2.6961455950601998,2.7269674316864001,2.7573967088394999,2.7869872259436002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4590098252758001,2.4670234007418999,2.4958692842024002,2.5561192465481,2.5798496555822998,2.6010082533005998,2.6204673871539002]
[null,null,null,null,"Coincident",2.1602748457888001,2.1737195035703998,2.2015543386365,2.2422098479950998,2.2624694935085001,2.2804671384656001,2.2969681019841999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5337828929813999,2.5420401436108002,2.5717631667943999,2.6338451976692001,2.6582971961266,2.6800991801556999,2.7001500233701998]
[null,null,null,null,"Coincident",2.225964041353,2.2398175215378999,2.2684987525742,2.3103905063443002,2.3312662030136999,2.3498111166767002,2.3668138381181998]
[null,"Peterborough 11kV","Substation Rating","MVA","Non-Coincident",2.8,2.8,2.8,2.8,2.8,2.8,2.8]
[null,null,null,null,"Coincident",2.8,2.8,2.8,2.8,2.8,2.8,2.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8888773602357001,1.924463099952,1.9762053509077999,2.0559172508129002,2.0995284855539,2.1487755304098002,2.203362418097]
[null,null,null,null,"Coincident",1.6876757828527,1.7189421361032999,1.7559260016925,1.8071553014123001,1.8447193494441001,1.8871956282119,1.9343087402612]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8955389848216,1.931250227042,1.9831749607033999,2.0631679856637,2.1069330269352999,2.1563537544938001,2.2111331572488]
[null,null,null,null,"Coincident",1.6936278169682,1.7250044392663999,1.7621187382196,1.813528711587,1.8512252391494,1.893851321726,1.9411305906005001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7135466623547,1.7476595202159,1.8004248338668001,1.8802196068379,1.9245881979060999,1.9725869560422999,2.0248505916652002]
[null,null,null,null,"Coincident",1.5803375395417001,1.5998601217577,1.6346613844196001,1.6840392423863,1.7232106190204,1.7655981756054,1.811758054859]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7195899369555001,1.7538231028141,1.8067745072712,1.8868506975712001,1.9313757661871001,1.9795438046133,2.0319917617423]
[null,null,null,null,"Coincident",1.5859110170099,1.6055024507652,1.6404264492656999,1.689978451282,1.7292879761152,1.7718250236069,1.8181476978586999]
[null,"Piccadilly 11kV","Substation Rating","MVA","Non-Coincident",3.895,3.895,3.895,3.895,3.895,3.895,3.895]
[null,null,null,null,"Coincident",3.895,3.895,3.895,3.895,3.895,3.895,3.895]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8003684907971,1.8508812981270999,1.9118897401368,1.9822214891125001,2.0326659594648002,2.0833962859620998,2.1348667331081002]
[null,null,null,null,"Coincident",1.8003684907971,1.8508812981270999,1.9118897401368,1.9822214891125001,2.0326659594648002,2.0833962859620998,2.1348667331081002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8009927484601,1.8515230705418,1.9125526665471999,1.9829088022712,2.0333707636802001,2.0841186803515002,2.1356069743000998]
[null,null,null,null,"Coincident",1.8009927484601,1.8515230705418,1.9125526665471999,1.9829088022712,2.0333707636802001,2.0841186803515002,2.1356069743000998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5473194601996001,1.5840947406852,1.6222406071088999,1.6670731131337,1.7094836791136001,1.7501146223024,1.7893883589883]
[null,null,null,null,"Coincident",1.5473194601996001,1.5840947406852,1.6222406071088999,1.6670731131337,1.7094836791136001,1.7501146223024,1.7893883589883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5478559759379,1.5846440078413,1.622803100918,1.6676511521135,1.7100764234834001,1.7507214549979,1.7900088094132001]
[null,null,null,null,"Coincident",1.5478559759379,1.5846440078413,1.622803100918,1.6676511521135,1.7100764234834001,1.7507214549979,1.7900088094132001]
[null,"Pinnaroo 11kV","Substation Rating","MVA","Non-Coincident",2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998]
[null,null,null,null,"Coincident",2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998,2.4857943925233998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6532681049505999,1.6726499826015999,1.7129987957066,1.7815085019042001,1.8094962061213999,1.8378341983011,1.8661760169588]
[null,null,null,null,"Coincident",1.4092257550799001,1.4323777364925001,1.4633850841275,1.5024086678916999,1.5261981795443,1.5502706738458001,1.5743287949010001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7532527640613,1.7738067991041,1.8165957864989,1.8892487527032999,1.9189290686978999,1.9489808570122999,1.9790367032186]
[null,null,null,null,"Coincident",1.4944514703222,1.5190036136095,1.5518861919308999,1.5932698041189,1.6184980335487,1.6440263595628,1.6695394430802]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5039387972145,1.5313574661063001,1.5780435270696,1.6513842631274001,1.6803639545204001,1.7084358941058999,1.7359746075036999]
[null,null,null,null,"Coincident",1.4343150925927,1.4548465163988,1.4855804867397,1.5256857727998001,1.5526825009303999,1.5788277538177,1.6044631101124001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5948924710393999,1.6239693381714999,1.6734788310249999,1.7512549931771999,1.7819872887343,1.8117569343976001,1.8409611059647]
[null,null,null,null,"Coincident",1.5210581351523,1.5428312374279001,1.5754239054226,1.6179546379926999,1.6465840466613999,1.6743104854371,1.7014961906151]
[null,"Pinnaroo South 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9864004588303001E-2,2.0094317901826E-2,2.0576352625567E-2,2.1396603129696001E-2,2.1730121034428999E-2,2.2067872703110999E-2,2.2406110807987E-2]
[null,null,null,null,"Coincident",9.3912934031976994E-3,9.5443658521890996E-3,9.7497005743204003E-3,1.0008438625668E-2,1.0165686617006E-2,1.0324831931363E-2,1.0484087386984E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1355683073494999E-2,2.1603291661649E-2,2.2121524566040999E-2,2.3003371412640999E-2,2.3361934694338001E-2,2.3725049672580999E-2,2.4088687615727002E-2]
[null,null,null,null,"Coincident",1.0096528354961999E-2,1.0261095710622999E-2,1.0481849951307E-2,1.0760017820181E-2,1.0929074278662999E-2,1.1100170538781999E-2,1.1271385211172999E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7187871968165999E-2,1.7501228184072001E-2,1.8034783166509E-2,1.887296300717E-2,1.9204159480233001E-2,1.9524981646925E-2,1.9839709800041998E-2]
[null,null,null,null,"Coincident",9.0919666288801996E-3,9.2221130806968993E-3,9.4169323600563001E-3,9.6711553856545004E-3,9.8422846950507008E-3,1.000801659593E-2,1.0170516318031E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8478587478584999E-2,1.8815475038504999E-2,1.9389097092233E-2,2.0290219670823999E-2,2.0646287193983998E-2,2.0991201356904E-2,2.1329563879043001E-2]
[null,null,null,null,"Coincident",9.7747237712325994E-3,9.9146435122789006E-3,1.0124092657748E-2,1.0397406447045E-2,1.0581386634918E-2,1.075956409831E-2,1.0934266663912E-2]
[null,"Plympton 11kV","Substation Rating","MVA","Non-Coincident",28.429104477612,28.429104477612,28.429104477612,28.429104477612,28.429104477612,28.429104477612,28.429104477612]
[null,null,null,null,"Coincident",28.429104477612,28.429104477612,28.429104477612,28.429104477612,28.429104477612,28.429104477612,28.429104477612]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.639618208464,23.047219027013998,23.748654193309001,24.387927553564001,24.507494605729001,24.610274989289,24.898269452011]
[null,null,null,null,"Coincident",22.639618208464,23.047219027013998,23.748654193309001,24.387927553564001,24.507494605729001,24.610274989289,24.898269452011]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.193195894889001,23.610763255984999,24.329349721077001,24.984254416829,25.106745089503999,25.212038630592001,25.50707505431]
[null,null,null,null,"Coincident",23.193195894889001,23.610763255984999,24.329349721077001,24.984254416829,25.106745089503999,25.212038630592001,25.50707505431]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.790579919349,21.155138560716001,21.879639346166002,22.548201932093001,22.704214143790999,22.829703097389,23.143223281127]
[null,null,null,null,"Coincident",20.790579919349,21.155138560716001,21.879639346166002,22.548201932093001,22.704214143790999,22.829703097389,23.143223281127]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.298945432636,21.672418161130999,22.414634239522002,23.099544332996,23.259371312171002,23.387928686974,23.709114979582001]
[null,null,null,null,"Coincident",21.298945432636,21.672418161130999,22.414634239522002,23.099544332996,23.259371312171002,23.387928686974,23.709114979582001]
[null,"Point Boston 11kV","Substation Rating","MVA","Non-Coincident",2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001]
[null,null,null,null,"Coincident",2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001,2.1850000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0268672026311001,1.0630317305207999,1.1189623751769,1.1345913401867,1.1424279681620999,1.1547372200563999,1.1715420827228]
[null,null,null,null,"Coincident",0.98879956190665996,1.0630317305207999,1.1189623751769,1.1345913401867,1.1424279681620999,1.1547372200563999,1.1715420827228]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0908450475803,1.1292627670727,1.1886781097526,1.2052808204400001,1.2136057010037,1.2266818674583,1.2445337388277]
[null,null,null,null,"Coincident",1.0504056438766001,1.1292627670727,1.1886781097526,1.2052808204400001,1.2136057010037,1.2266818674583,1.2445337388277]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.99763208673207004,1.0345618260997,1.0918152419317,1.1065095433767,1.1150714204154999,1.1269216572648,1.1426022715819999]
[null,null,null,null,"Coincident",0.95792191865425003,1.0345618260997,1.0918152419317,1.1065095433767,1.1150714204154999,1.1269216572648,1.1426022715819999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0597884695611,1.0990190762008001,1.1598396038769001,1.1754494178021,1.1845447332837999,1.1971332862599,1.2137908642088]
[null,null,null,null,"Coincident",1.0176042026225001,1.0990190762008001,1.1598396038769001,1.1754494178021,1.1845447332837999,1.1971332862599,1.2137908642088]
[null,"Polda 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.64514021393775001,0.64915061888397996,0.66006152275970997,0.6803889352843,0.68731415719108002,0.69410436279203003,0.70057735990442005]
[null,null,null,null,"Coincident",0.59156961910302996,0.59829627518162998,0.60819043242396997,0.62117488643117003,0.62761088397032005,0.63392459653046995,0.63994369754032998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.66120628971633999,0.66531656670336004,0.67649918733879,0.69733281811322001,0.70443050042091004,0.71138980408051999,0.71802399973528996]
[null,null,null,null,"Coincident",0.60630161398334004,0.61319578553217002,0.62333633925791998,0.63664414812272996,0.64324042279534999,0.64971136719789002,0.65588036327065002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.59419533348593001,0.59730241590278998,0.60693117247371997,0.62567804429167995,0.63344057197203996,0.64058272704924002,0.64723775950600004]
[null,null,null,null,"Coincident",0.53847885454528999,0.54377233873162001,0.55271473258004,0.56491427849454001,0.57201025381852,0.57854666225919005,0.58463775160954001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.60899271713808001,0.61217717594611998,0.62204571966623001,0.64125944916370003,0.64921528886406998,0.65653530667904003,0.66335607094642002]
[null,null,null,null,"Coincident",0.55188871785157001,0.55731402689742005,0.56647911524559003,0.57898246927014996,0.58625515730683997,0.59295434343685005,0.59919712059236996]
[null,"Poonindie 11kV","Substation Rating","MVA","Non-Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,null,null,"Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.49433780214869999,0.51416676453886001,0.54380379024189995,0.55263924692682997,0.55609284365068001,0.55994759826602003,0.56413884421133997]
[null,null,null,null,"Coincident",0.47499838114915999,0.51416676453886001,0.54380379024189995,0.55263924692682997,0.55609284365068001,0.55994759826602003,0.56413884421133997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.52035524468921002,0.54122782318030005,0.57242467216602,0.58172514687226995,0.58536050949371998,0.58941814330678999,0.59382997829077999]
[null,null,null,null,"Coincident",0.49999797259181999,0.54122782318030005,0.57242467216602,0.58172514687226995,0.58536050949371998,0.58941814330678999,0.59382997829077999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.44779472160747003,0.46672314969995998,0.49512065216952,0.50314948557794004,0.50697017453425997,0.51068793384065003,0.51441615074571001]
[null,null,null,null,"Coincident",0.42905502893148001,0.46672314969995998,0.49512065216952,0.50314948557794004,0.50697017453425997,0.51068793384065003,0.51441615074571001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.47136256001416998,0.49128720827865002,0.52117929680978003,0.52963069493197001,0.5336524701798,0.53756589849776004,0.54149033480720998]
[null,null,null,null,"Coincident",0.45163658048068001,0.49128720827865002,0.52117929680978003,0.52963069493197001,0.5336524701798,0.53756589849776004,0.54149033480720998]
[null,"Port Adelaide 11kV","Substation Rating","MVA","Non-Coincident",33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998]
[null,null,null,null,"Coincident",33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998,33.191503579951998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.544785674092999,11.708428475889001,12.044824225346,12.584748355587999,12.812031244233999,13.069831278538,13.321892110643001]
[null,null,null,null,"Coincident",11.224441449555,11.408054241791,11.67177751919,12.011899233266,12.214207489255999,12.450289519042,12.680353470825001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.048288209020001,12.219067961458,12.570134932830999,13.133606764686,13.370802137964001,13.639845600639999,13.90289955739]
[null,null,null,null,"Coincident",11.713972817441,11.905593511161999,12.180818547229,12.53577398365,12.746905506056001,12.993283777262,13.233381504135]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.446578279402001,10.611614441657,10.862501135553,11.274010626585,11.482700296261999,11.721015105816999,11.949267077306001]
[null,null,null,null,"Coincident",10.239065904226001,10.429045914987,10.609443998213999,10.861632281009999,11.049060367475001,11.269269262898,11.479871771399001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.902184714504999,11.074418596007,11.336247206878999,11.765703854119,11.983495102696001,12.232203531856999,12.470410252572]
[null,null,null,null,"Coincident",10.685622105754,10.883887711388001,11.072153493051999,11.335340458998999,11.530942843308001,11.760755705420999,11.980543217428]
[null,"Port Adelaide North 11kV","Substation Rating","MVA","Non-Coincident",49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997]
[null,null,null,null,"Coincident",49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997,49.029029029028997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.10801827469,19.346789046262,19.803533469457999,20.599443292298002,20.887517647477001,21.232627182881998,21.612231654279999]
[null,null,null,null,"Coincident",13.576581030632999,13.775829859888001,14.024104033342001,14.368734891573,14.552246345267999,14.781180062499001,15.033529898209]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.360543131288001,21.627461096895001,22.138048265664001,23.027782923385999,23.349816563941999,23.735608905673999,24.159962575821002]
[null,null,null,null,"Coincident",15.177039319896,15.399776348403,15.677318012547,16.062575248843999,16.267719720938,16.523641003346,16.805738784098001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.916835728637,18.141371724104999,18.504476449220999,19.148408260031001,19.453762083903001,19.817409959824001,20.208498746612999]
[null,null,null,null,"Coincident",12.833452019838001,13.029541804214,13.207952422348001,13.481717987559,13.679833794214,13.924298595203,14.188148476837]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.028939519316001,20.279944660026,20.685853531919999,21.405694439579001,21.747044517403001,22.153560568755999,22.590752368463999]
[null,null,null,null,"Coincident",14.346307474291001,14.565513057860001,14.764955388768,15.070993465531,15.292463906485001,15.565747135052,15.860700630269999]
[null,"Port Augusta 11kV","Substation Rating","MVA","Non-Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,null,null,"Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.765210656603999,13.902337748500001,13.965857559903,14.092576009217,14.064226722762999,14.028871326826,13.984254323179]
[null,null,null,null,"Coincident",13.765210656603999,13.902337748500001,13.965857559903,14.092576009217,14.064226722762999,14.028871326826,13.984254323179]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.196756600823001,14.3381826927,14.403693880601001,14.534385013967,14.505146963811001,14.468683159284,14.422667391212]
[null,null,null,null,"Coincident",14.196756600823001,14.3381826927,14.403693880601001,14.534385013967,14.505146963811001,14.468683159284,14.422667391212]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.371502907868001,12.460671692529999,12.484735277081001,12.575161107913001,12.545739210424999,12.500084700118,12.442673574186999]
[null,null,null,null,"Coincident",12.371502907868001,12.460671692529999,12.484735277081001,12.575161107913001,12.545739210424999,12.500084700118,12.442673574186999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.759355446922999,12.851319715673,12.876137705121,12.969398429041,12.939054140981,12.891968339918,12.832757347704]
[null,null,null,null,"Coincident",12.759355446922999,12.851319715673,12.876137705121,12.969398429041,12.939054140981,12.891968339918,12.832757347704]
[null,"Port Augusta West TF1 11kV","Substation Rating","MVA","Non-Coincident",15.1,15.1,15.1,15.1,15.1,15.1,15.1]
[null,null,null,null,"Coincident",15.1,15.1,15.1,15.1,15.1,15.1,15.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0596397521606002,6.1158382238598001,6.1483611040854997,6.2088107262758001,6.2010123126884,6.1901428892687997,6.1752504803125996]
[null,null,null,null,"Coincident",6.0467402040081,6.1158382238598001,6.1483611040854997,6.2088107262758001,6.2010123126884,6.1901428892687997,6.1752504803125996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.1567348547460004,6.2138338084207003,6.2468778107791998,6.3082960321780002,6.3003726626859002,6.2893290758134999,6.2741980421147998]
[null,null,null,null,"Coincident",6.1436286139513001,6.2138338084207003,6.2468778107791998,6.3082960321780002,6.3003726626859002,6.2893290758134999,6.2741980421147998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.4303196816695998,5.4752215421616004,5.4916136637955999,5.5373228594950001,5.5303574323155997,5.5162722974623,5.4970726710672997]
[null,null,null,null,"Coincident",5.4303196816695998,5.4752215421616004,5.4916136637955999,5.5373228594950001,5.5303574323155997,5.5162722974623,5.4970726710672997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.5173310335202004,5.5629523675995998,5.5796071442423001,5.6260487496603,5.6189717137228996,5.6046608892791001,5.5851536225340999]
[null,null,null,null,"Coincident",5.5173310335202004,5.5629523675995998,5.5796071442423001,5.6260487496603,5.6189717137228996,5.6046608892791001,5.5851536225340999]
[null,"Port Augusta West TF2 11kV","Substation Rating","MVA","Non-Coincident",17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001]
[null,null,null,null,"Coincident",17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001,17.100000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5531510082426001,3.5456116488484999,3.5696988012725002,3.6100948781278999,3.6108606809566002,3.6098281266072001,3.6063808464853002]
[null,null,null,null,"Coincident",3.5017190916529999,3.5456116488484999,3.5696988012725002,3.6100948781278999,3.6108606809566002,3.6098281266072001,3.6063808464853002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6509305735917001,3.6431837377118002,3.6679337472137998,3.7094414882871001,3.7102283653305999,3.7091673960009999,3.7056252497867002]
[null,null,null,null,"Coincident",3.5980832962596998,3.6431837377118002,3.6679337472137998,3.7094414882871001,3.7102283653305999,3.7091673960009999,3.7056252497867002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.1998089643141001,3.2087502692126999,3.2291849613763,3.2670449925677998,3.2739708247678001,3.2767053951071001,3.2763414906346]
[null,null,null,null,"Coincident",3.1718169266341998,3.2087502692126999,3.2291849613763,3.2670449925677998,3.2739708247678001,3.2767053951071001,3.2763414906346]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2878648699045998,3.2970522315862998,3.3180492683598,3.3569511740411002,3.3640675990025,3.3668774222929998,3.3665035034920998]
[null,null,null,null,"Coincident",3.2591025161668998,3.2970522315862998,3.3180492683598,3.3569511740411002,3.3640675990025,3.3668774222929998,3.3665035034920998]
[null,"Port Broughton 11kV","Substation Rating","MVA","Non-Coincident",5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003]
[null,null,null,null,"Coincident",5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003,5.2830508474576003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1777781172867998,3.2120891106293001,3.2632946782398,3.3494091450907999,3.3656056307056001,3.3807675620755999,3.3942487144698998]
[null,null,null,null,"Coincident",3.0096650380807999,3.0412252683894998,3.0735463558606999,3.1208103896292001,3.1345925227117002,3.1473897107013,3.1585870809872998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.4541067173340001,3.4914012760504001,3.5470595028114,3.6406621860168999,3.6582670620323001,3.674747422542,3.6894008493464998]
[null,null,null,null,"Coincident",3.2713751058981999,3.3056797047362001,3.3408113222455,3.3921852730069002,3.4071658527397002,3.4210758399593,3.4332468948580002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8921536004915001,2.9255162839033,2.9807844916779,3.0702752394863002,3.0915791170347,3.1094437174294001,3.1247920689013]
[null,null,null,null,"Coincident",2.8273827978222998,2.8388146767912001,2.8687501306396999,2.9149444066584,2.9342035955946999,2.9501748107129999,2.9637234541997999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1436452799130001,3.1799090669451999,3.2399832070152002,3.3372557608989002,3.3604121499950002,3.3798301942852,3.3965131853444999]
[null,null,null,null,"Coincident",3.0732422321452,3.0856681877912,3.1182067252246002,3.1684178958002001,3.1893517972306999,3.2067118140058999,3.2214386006950999]
[null,"Port Clinton 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.58910570519252003,0.58850518858794998,0.59063656541092002,0.59775903712811995,0.59846259755401998,0.59919463322472,0.59978079605885004]
[null,null,null,null,"Coincident",0.40900621997629,0.40920270806122,0.41167504567301999,0.41629433160997997,0.41659820411821002,0.41693036420078,0.41716849560434999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.60443941378074995,0.60382326645567996,0.60601012043803004,0.61331798147463001,0.61403985472698996,0.61479094440031001,0.61539236434365996]
[null,null,null,null,"Coincident",0.4196521569153,0.41985375934729002,0.42239044891518002,0.42712996927496,0.42744175121684003,0.42778255702439,0.42802688670021]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.52962927152032002,0.52726500284629996,0.52666619659594005,0.53007520972624,0.53022343921598003,0.52999408048703001,0.52949620926370999]
[null,null,null,null,"Coincident",0.36184997511382,0.36030514603262997,0.36130103131479002,0.36447800998437002,0.36442556992885999,0.36412063266665001,0.36363753183436998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.54341488051664999,0.54098907279020003,0.54037468033781,0.54387242595440999,0.54402451367838001,0.54378918501927997,0.54327835481053]
[null,null,null,null,"Coincident",0.37126849206612,0.36968345295346,0.37070525992432002,0.37396493150398002,0.37391112649727998,0.37359825208717001,0.37310257672486002]
[null,"Portee 11kV","Substation Rating","MVA","Non-Coincident",0.7,0.7,0.7,0.7,0.7,0.7,0.7]
[null,null,null,null,"Coincident",0.7,0.7,0.7,0.7,0.7,0.7,0.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.64305496816300001,0.64804772716073,0.66030800866934003,0.68241590626503001,0.69051713865668995,0.69848672197382999,0.70624670882885998]
[null,null,null,null,"Coincident",0.29097118270532002,0.29460339349238002,0.29978066708446,0.30649123623998997,0.30997415996694999,0.31339669041122997,0.31672443728757999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.67689992750681005,0.68215546299124996,0.69506102173079998,0.71833249154403001,0.72686010409681001,0.73524913868438002,0.74341754542980998]
[null,null,null,null,"Coincident",0.30628543784126,0.31010881739694002,0.31555857875898002,0.32262233535801998,0.32628857064896,0.32989123406704002,0.33339412531411999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.63102884180329,0.63604816371884998,0.64829547644925001,0.67055553281109004,0.68065597487603002,0.69006443410644003,0.69887937191964999]
[null,null,null,null,"Coincident",0.28668802432986001,0.29013709508468999,0.29553416671796001,0.30267184123635998,0.30707006032301998,0.31115427839037002,0.31496925546795002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.66424084785716997,0.66952434430612995,0.68241625170098996,0.70584788862725001,0.71647993229386997,0.72638357301872003,0.73566245439302003]
[null,null,null,null,"Coincident",0.30177685033724999,0.30540745092274002,0.31108857863060002,0.31860191979625002,0.32323162383138998,0.3275308004968,0.33154656561037998]
[null,"Port Germein 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.84093694332975999,0.84669971199226002,0.86487413605394003,0.89883060945230997,0.91008147505600001,0.92095958731909,0.93130187694307998]
[null,null,null,null,"Coincident",0.73839830634466996,0.74891317999606999,0.76324416977461995,0.78145969135313997,0.79153209143310999,0.80128532128949004,0.81057582856286003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.84361820254157005,0.84939934532438,0.86763171706254005,0.90169645792118003,0.91298319599696998,0.92389599223839003,0.93427125741368999]
[null,null,null,null,"Coincident",0.74075262943224995,0.75130102890511996,0.7656777118818,0.78395131217290004,0.79405582728326995,0.80384015452168001,0.81316028382368999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.74577805771038996,0.74927599377050003,0.76334454357555004,0.79062852479112,0.80070494470259002,0.80975905130153003,0.81829981763237003]
[null,null,null,null,"Coincident",0.65007369666936998,0.65712908515129997,0.66867906168109004,0.68401954548220001,0.69299898206085997,0.70109703047927996,0.70875222488093004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74815591053642005,0.75166499948183996,0.76577840571643996,0.79314937969235,0.80325792745113,0.81234090233432998,0.82090890020563001]
[null,null,null,null,"Coincident",0.65214640390547995,0.65922428792112997,0.67081109061393995,0.68620048630295005,0.69520855308657004,0.70333242147531005,0.71101202384317996]
[null,"Port Giles 11kV","Substation Rating","MVA","Non-Coincident",3.5625,3.5625,3.5625,3.5625,3.5625,3.5625,3.5625]
[null,null,null,null,"Coincident",3.5625,3.5625,3.5625,3.5625,3.5625,3.5625,3.5625]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3833595747909,1.3982738233014,1.4306279019571,1.4862230730301,1.5094475516106001,1.5323464682634,1.5548600515244999]
[null,null,null,null,"Coincident",0.58190825864795004,0.59164428707801997,0.60469602054408,0.62100776404508995,0.63082568063375999,0.64046149946863995,0.64992177286890995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5045105539914001,1.5207309530097,1.5559185164525,1.6163825658252,1.6416409829222001,1.6665453262376,1.69103058968]
[null,null,null,null,"Coincident",0.63287024758037003,0.64345893167517998,0.65765370149889002,0.67539398442929,0.68607172823143003,0.69655142663928005,0.70684020580684004]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3123137792691999,1.3234778157683,1.3504916581941,1.3994914339736999,1.4225862590713001,1.4443621008909,1.4654830435507999]
[null,null,null,null,"Coincident",0.52192388449689997,0.52890840718524001,0.53963392325566995,0.55374084217121,0.56293752524677998,0.57158906333544002,0.57999032499117997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4272427552736999,1.439384508614,1.4687641520373,1.5220551988099,1.5471726077143999,1.5708555202678001,1.5938261793221]
[null,null,null,null,"Coincident",0.56763260031249996,0.57522880905728002,0.58689363750754997,0.60223600313647996,0.61223810743464002,0.62164732438723003,0.63078434635768998]
[null,"Port Julia 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.26076464060630999,0.26399271803044,0.27077006044954999,0.28222234268075003,0.28718625596526998,0.29262489685474002,0.29796654200666001]
[null,null,null,null,"Coincident",0.23392421095040999,0.23812594233317,0.24361200898845001,0.25041074574937,0.25463115044920998,0.25926717245789999,0.26380272910518998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.27448857606506999,0.27788654587230999,0.28502057702699002,0.29707558814746998,0.30230075014034002,0.30802562445615,0.31364839818876]
[null,null,null,null,"Coincident",0.24623554566917,0.25065841244122,0.25643320852133,0.26358975999320999,0.26803228285132003,0.27291229678576001,0.27768655790829999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.24066295336679999,0.24346141769761001,0.25012466813341999,0.26165247840715,0.26751665663891999,0.27316761520855998,0.27862498759870002]
[null,null,null,null,"Coincident",0.20780408981546999,0.21129843399209,0.21676479888356001,0.22357135738039,0.22841587684869999,0.23307341071087001,0.23755200038509]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.25332894531893002,0.25627469167298,0.26328862623034999,0.27542314040308002,0.28159594791598003,0.28754431410387998,0.29328890575151001]
[null,null,null,null,"Coincident",0.21874073333454999,0.22241898340363001,0.22817304082421999,0.23533782568674999,0.24043731021611001,0.24533996816400999,0.25005426416519]
[null,"Port Lincoln City 11kV","Substation Rating","MVA","Non-Coincident",28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998]
[null,null,null,null,"Coincident",28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998,28.417994268169998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.681334058313,11.141408232503,11.738561721,11.883467991965,11.911586457265001,11.947657236762,11.990382644686999]
[null,null,null,null,"Coincident",10.331926977789999,11.141408232503,11.738561721,11.883467991965,11.911586457265001,11.947657236762,11.990382644686999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.742145048814001,11.20483851813,11.805391721954001,11.951122973564001,11.979401522963,12.015677660686,12.058646312982001]
[null,null,null,null,"Coincident",10.390748723264,11.20483851813,11.805391721954001,11.951122973564001,11.979401522963,12.015677660686,12.058646312982001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.7847007464305999,10.275549975937,10.910223120336999,11.097296896611001,11.192225562141999,11.285513894089,11.381398228486001]
[null,null,null,null,"Coincident",9.4377636604780992,10.275549975937,10.910223120336999,11.097296896611001,11.192225562141999,11.285513894089,11.381398228486001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.8404070225282005,10.334050755762,10.972337222462,11.1604760475,11.255945161082,11.34976460233,11.446194825595001]
[null,null,null,null,"Coincident",9.4914947537264993,10.334050755762,10.972337222462,11.1604760475,11.255945161082,11.34976460233,11.446194825595001]
[null,"Port Lincoln Docks 11kV","Substation Rating","MVA","Non-Coincident",13.4,13.4,13.4,13.4,13.4,13.4,13.4]
[null,null,null,null,"Coincident",13.4,13.4,13.4,13.4,13.4,13.4,13.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0904657788507004,6.1415708392050998,6.2358547340235004,6.3730652031195003,6.4576493816721996,6.5560368788945,6.6676135554474003]
[null,null,null,null,"Coincident",4.6949905035372996,5.1365395057827001,5.4908918026134002,5.6398249215906997,5.7356968948722002,5.8370288153618004,5.9427126603957996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3579436948646997,6.4112931607436998,6.5097177667352,6.6529541740207998,6.7412530766402998,6.8439615049168996,6.9604383480587]
[null,null,null,null,"Coincident",4.9011826604577999,5.3621233826844001,5.7320379398302999,5.8875118262523003,5.9875942551127999,6.0933764183100001,6.2037016316158002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.3905365437402004,5.4356901146818997,5.5197851885478997,5.6422803280096998,5.7311804525758996,5.8268074378210004,5.9312488724136996]
[null,null,null,null,"Coincident",4.1436391233438998,4.5572567609060997,4.8879129834721002,5.0220311947209,5.1160545526292003,5.2105007297660997,5.3067227968627]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.6272753307677004,5.6744119328098002,5.7622002504968002,5.8900750679364,5.9828794620472001,6.0827061436137999,6.1917343829410996]
[null,null,null,null,"Coincident",4.3256173164199003,4.7573999987814002,5.1025778097679,5.2425861550304997,5.3407387819869996,5.4393327973277001,5.5397806952417996]
[null,"Port Lincoln Marina 11kV","Substation Rating","MVA","Non-Coincident",17.8,17.8,17.8,17.8,17.8,17.8,17.8]
[null,null,null,null,"Coincident",17.8,17.8,17.8,17.8,17.8,17.8,17.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.5966122372473004,5.7302258421227004,6.0015289190964998,6.0389755653792001,6.0161697885559997,5.9968071274544998,5.9800956881075003]
[null,null,null,null,"Coincident",5.3451433882329997,5.7302258421227004,6.0015289190964998,6.0389755653792001,6.0161697885559997,5.9968071274544998,5.9800956881075003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.7546305061801997,5.8920166415889001,6.1709798602274004,6.2094837986667999,6.1860341092011,6.1661247505511998,6.1489414699178999]
[null,null,null,null,"Coincident",5.4960615275647999,5.8920166415889001,6.1709798602274004,6.2094837986667999,6.1860341092011,6.1661247505511998,6.1489414699178999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.1866430886310004,5.3219503664219001,5.5912553680665003,5.6267806433010001,5.6141448534145999,5.5997641736519999,5.5857025673051002]
[null,null,null,null,"Coincident",4.9395368019415002,5.3219503664219001,5.5912553680665003,5.6267806433010001,5.6141448534145999,5.5997641736519999,5.5857025673051002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.3330860308423,5.4722136593924997,5.7491223877867004,5.7856507059795996,5.7726581492565003,5.7578714363392001,5.743412805757]
[null,null,null,null,"Coincident",5.0790027898794001,5.4722136593924997,5.7491223877867004,5.7856507059795996,5.7726581492565003,5.7578714363392001,5.743412805757]
[null,"Port Noarlunga 11kV","Substation Rating","MVA","Non-Coincident",58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003]
[null,null,null,null,"Coincident",58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003,58.044959244959003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.392940308828003,36.407327271325002,37.910068099901999,39.342681303950997,39.956654504862001,40.554198447798001,41.471934034679002]
[null,null,null,null,"Coincident",35.392940308828003,36.407327271325002,37.910068099901999,39.342681303950997,39.956654504862001,40.554198447798001,41.471934034679002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.518935515617997,36.536933590783001,38.04502402128,39.482737180160001,40.098896062163,40.698567199731002,41.619569830380001]
[null,null,null,null,"Coincident",35.518935515617997,36.536933590783001,38.04502402128,39.482737180160001,40.098896062163,40.698567199731002,41.619569830380001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.618885699669999,32.411906024494002,33.772436601469998,35.067080148648998,35.578764336771002,36.050650149802003,36.830614631750997]
[null,null,null,null,"Coincident",31.618885699669999,32.411906024494002,33.772436601469998,35.067080148648998,35.578764336771002,36.050650149802003,36.830614631750997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.731445662403999,32.527289057560999,33.892662982670998,35.191915326973003,35.705421057880997,36.178986735598997,36.961727810431]
[null,null,null,null,"Coincident",31.731445662403999,32.527289057560999,33.892662982670998,35.191915326973003,35.705421057880997,36.178986735598997,36.961727810431]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Port Pirie South 11kV","Substation Rating","MVA","Non-Coincident",40.509658862243,40.509658862243,40.509658862243,40.509658862243,40.509658862243,40.509658862243,40.509658862243]
[null,null,null,null,"Coincident",40.509658862243,40.509658862243,40.509658862243,40.509658862243,40.509658862243,40.509658862243,40.509658862243]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.214010405770001,23.760793981243001,24.457059277005001,25.428879157421001,25.880351193578999,26.327431618567001,26.765359921407001]
[null,null,null,null,"Coincident",21.790790681191002,22.297192067000001,22.830526766415002,23.483056353138998,23.890005736279001,24.292483832430001,24.685987306160001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.842504380481,24.404091523999,25.119207442101999,26.117338284247001,26.581033432634001,27.040218071776,27.490002805059]
[null,null,null,null,"Coincident",22.380752536464001,22.900864186644,23.448638340475998,24.118834452992001,24.536801546163002,24.950176297134,25.354333447586001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.787738179904999,21.276095373486999,21.931434594272002,22.851418142629001,23.273816937227998,23.674149691572001,24.059341063175999]
[null,null,null,null,"Coincident",20.141820266227999,20.462310548051001,20.919794140531,21.502766770905001,21.893022069040999,22.262178498669002,22.616661762094999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.350543484355999,21.852122415513001,22.525204229863999,23.470095327879999,23.903930108450002,24.315101434829,24.710721442069001]
[null,null,null,null,"Coincident",20.687138048710999,21.016305254837999,21.486174715869002,22.084930693419999,22.485751727471001,22.864902664195998,23.228983174772001]
[null,"Port Stanvac 11kV","Substation Rating","MVA","Non-Coincident",56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998]
[null,null,null,null,"Coincident",56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998,56.194646926807998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.229675285896999,30.518382203392001,31.160195537046,32.133940421696998,32.441784337160001,32.715980205325003,32.970729736514002]
[null,null,null,null,"Coincident",24.810301647923001,25.221943548155,25.952735082215,26.613167510288001,26.704874863956,26.777538572358001,27.051557422725999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.706863478067,31.000127756194001,31.652072384395002,32.641188243320002,32.95389160501,33.232415770762998,33.491186630896998]
[null,null,null,null,"Coincident",25.201942738296001,25.620082579784,26.362409966866,27.033267599756002,27.126422592733999,27.200233328464002,27.478577682118999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.101634303368002,27.269398291041,27.795580182906999,28.650877900124001,28.944882005050999,29.186857075060001,29.392573327729]
[null,null,null,null,"Coincident",22.753456949522,23.055608456436001,23.743294774287001,24.362367924116,24.42224372443,24.446406966493999,24.669147585785002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.529445047471999,27.699857260546999,28.234345155814999,29.10314410874,29.401789192639001,29.647583941329,29.856547511933002]
[null,null,null,null,"Coincident",23.112629877602998,23.419550973669999,24.118092710500001,24.746938191468999,24.807759156581,24.832303825625999,25.058560499668999]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Port Vincent 11kV","Substation Rating","MVA","Non-Coincident",2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001]
[null,null,null,null,"Coincident",2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001,2.6555813953488001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2374641777596,1.2681842234723,1.3060930393542001,1.3576741155851,1.3914018484638,1.4281471433474,1.4659442343180999]
[null,null,null,null,"Coincident",1.2374641777596,1.2681842234723,1.3060930393542001,1.3518523745738,1.3844351506688,1.4199772101814001,1.4564694984102999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2789215759724999,1.3106708015121,1.3498496346630999,1.4031587748300001,1.4380164507630999,1.4759927827545001,1.5150561479978999]
[null,null,null,null,"Coincident",1.2789215759724999,1.3106708015121,1.3498496346630999,1.3971419944472001,1.4308163553716999,1.4675491413238999,1.5052639904576]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1889029974842,1.2111100528684,1.2528716863685001,1.3200041648148,1.3595262382493001,1.3987573919834999,1.4385818680096001]
[null,null,null,null,"Coincident",1.1520290532185,1.1795650654103,1.2184591888956,1.2657232954315001,1.3026724080472001,1.3393006387999999,1.3764022468224999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2287335040063001,1.2516845378868,1.2948452653575999,1.3642268092248999,1.4050729471179999,1.4456184189487999,1.4867770904943001]
[null,null,null,null,"Coincident",1.1906242126344,1.2190827334879,1.2592798839168999,1.3081274277120001,1.3463144057162,1.3841697517063001,1.422514334003]
[null,"Prospect 11kV","Substation Rating","MVA","Non-Coincident",50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999]
[null,null,null,null,"Coincident",50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999,50.616385542168999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.810327216997003,35.574493454044998,36.538210650720004,37.712074413987999,38.505759712836998,39.307427394426,40.130926196232998]
[null,null,null,null,"Coincident",34.810327216997003,35.574493454044998,36.538210650720004,37.712074413987999,38.505759712836998,39.307427394426,40.130926196232998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.204038273849001,35.976847368371999,36.951464379737999,38.138604753133002,38.941266775350996,39.752001462491997,40.584814183745003]
[null,null,null,null,"Coincident",35.204038273849001,35.976847368371999,36.951464379737999,38.138604753133002,38.941266775350996,39.752001462491997,40.584814183745003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.992079541677001,31.583991765328001,32.249347522800001,33.185018179823999,33.839770840984997,34.571376237778999,35.299762423974002]
[null,null,null,null,"Coincident",30.992079541677001,31.583991765328001,32.249347522800001,33.185018179823999,33.839770840984997,34.571376237778999,35.299762423974002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.342605531115002,31.941212388392,32.614093439058003,33.560346699368999,34.222504730798001,34.962384716111998,35.699009080975998]
[null,null,null,null,"Coincident",31.342605531115002,31.941212388392,32.614093439058003,33.560346699368999,34.222504730798001,34.962384716111998,35.699009080975998]
[null,"Punyelroo 11kV","Substation Rating","MVA","Non-Coincident",1.33,1.33,1.33,1.33,1.33,1.33,1.33]
[null,null,null,null,"Coincident",1.33,1.33,1.33,1.33,1.33,1.33,1.33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.56523931610384004,0.57068497376242,0.58340366165831004,0.60573657357627997,0.61455226606135005,0.62410088944402997,0.63334945698839995]
[null,null,null,null,"Coincident",0.47122157400050002,0.47850526546048999,0.48833877156736999,0.50072361664481002,0.50795045315996001,0.51578229573695999,0.52335628590130001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.58069757904175001,0.58629216549131002,0.59935868627164002,0.62230236254156002,0.63135914811505001,0.64116890890756995,0.65067040788261998]
[null,null,null,null,"Coincident",0.48410862340664002,0.49159151052507,0.50169394506398002,0.51441749303451001,0.52184197032919,0.52988799949653997,0.53766912445867998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.53111119016708996,0.53608286399619998,0.54769752294135998,0.56836734179996995,0.57807447849353999,0.58746539746578996,0.59636622229603997]
[null,null,null,null,"Coincident",0.43036418834913998,0.43656732063565001,0.44575899311087003,0.45763637170283,0.46543378876894997,0.47297349250440002,0.48009995448033999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.54563611119251998,0.55074375122053998,0.56267604987474995,0.58391115052762999,0.59388375968056994,0.60353150313506998,0.61267574926789004]
[null,null,null,null,"Coincident",0.44213386287995998,0.44850663950504999,0.45794968743473002,0.47015189063823998,0.47816255281985998,0.4859084536819,0.49322981137706001]
[null,"Pyap 11kV","Substation Rating","MVA","Non-Coincident",15.169945987654,15.169945987654,15.169945987654,15.169945987654,15.169945987654,15.169945987654,15.169945987654]
[null,null,null,null,"Coincident",15.169945987654,15.169945987654,15.169945987654,15.169945987654,15.169945987654,15.169945987654,15.169945987654]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.4151686989527992,9.6210587360132998,9.8106195493952004,10.079619815752,10.174920082066,10.264887826223999,10.349661419902001]
[null,null,null,null,"Coincident",9.0534729650083996,9.3821652023096007,9.5368461210881001,9.7364759598478994,9.8298200295747993,9.9178362757513003,10.000684627824]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.4593310574836007,9.6661868329100997,9.8566367915501996,10.126898818220001,10.222646095592999,10.313035838326,10.398207067135001]
[null,null,null,null,"Coincident",9.0959387701166001,9.4261727561525994,9.5815792141551999,9.7821454274819004,9.8759273326216004,9.9643564237661,10.04759338052]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4893800069541001,8.6824838046442991,8.8591667727358008,9.1144992297002005,9.2276158036292006,9.3284490740976,9.4217629332450006]
[null,null,null,null,"Coincident",8.1817993627097003,8.4897389142024,8.6359197862062,8.8296977701138992,8.9402307893073996,9.0386786244886004,9.1296799111148008]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.5291999035017998,8.7232094650099992,8.9007211741290995,9.1572512818068006,9.2708984351500998,9.3722046695329002,9.4659562223887992]
[null,null,null,null,"Coincident",8.2201765355928007,8.5295604942240004,8.6764270355223996,8.8711139455548995,8.9821654258593,9.0810750359415007,9.1725031690295999]
[null,"Qualco 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8279697150601999,2.8670180576852,2.9388451437040999,3.0552630672621,3.1096539333405002,3.1637371682488999,3.2164428345676002]
[null,null,null,null,"Coincident",2.5327405948645998,2.5797359584097999,2.6408749372481002,2.7160115069992998,2.7629763345926999,2.8096402993342,2.8550587475447]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9955483684366002,3.0369106215107,3.1129940071239002,3.2363105755842998,3.2939245129865,3.3512125897388998,3.4070414665149]
[null,null,null,null,"Coincident",2.6828246838060998,2.7326048790613999,2.7973668060832999,2.8769557874396998,2.9267036372564998,2.9761327958156998,3.0242426315431001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6540138571465999,2.6926965207381999,2.7624557576929001,2.8758336938728002,2.9379563153461001,2.9976310632289001,3.0552310205082001]
[null,null,null,null,"Coincident",2.3865888313199002,2.4311667090675,2.4925513407827999,2.5693017443109998,2.6234284423658001,2.6753363391180001,2.7253612223538002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8112843066334001,2.8522592114181999,2.9261522122271999,3.0462486510015001,3.1120525089447,3.1752634382220002,3.2362766298171999]
[null,null,null,null,"Coincident",2.5280123198339002,2.5752317749235001,2.6402539116185002,2.7215523586426,2.7788864740624,2.8338703073747,2.8868595443385998]
[null,"Queenstown 11kV","Substation Rating","MVA","Non-Coincident",22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999]
[null,null,null,null,"Coincident",22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999,22.830759717313999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.546078629803,15.752031137841,16.140069027812999,16.799776855735999,17.069755514623999,17.379434625382,17.680722823006001]
[null,null,null,null,"Coincident",15.064447268186999,15.296885265426001,15.588179545748,15.981742727144001,16.219149710787999,16.500556483459,16.773316469301001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.899131096882,16.109760799907999,16.506611055857,17.181300891896001,17.457410783865001,17.774122727573999,18.082253199960999]
[null,null,null,null,"Coincident",15.4065618554,15.644278534827,15.942188127393999,16.344689154497999,16.587487666337999,16.875285205305001,17.154239588346002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.550421613973,13.712454911259,14.001792943405,14.496311731906999,14.728316128813001,14.997168460296001,15.252249413432001]
[null,null,null,null,"Coincident",13.237091204187999,13.431725491704,13.630127501702001,13.919628768809,14.124981623259,14.371208078602001,14.604380683513]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.858152579105999,14.023865663219,14.319774581084999,14.825523923764001,15.062797155767001,15.337755141362001,15.598628999701999]
[null,null,null,null,"Coincident",13.537706415126999,13.736760860101001,13.939668592781,14.235744452684999,14.445760883952,14.697579158271999,14.93604712836]
[null,"Quorn 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.801846637868,1.7973087956347,1.7983470875167999,1.8116677772480001,1.806480641202,1.8004689616989,1.7934785407474001]
[null,null,null,null,"Coincident",1.6423500175457999,1.6627738433137,1.6732725826265999,1.6914287703619,1.691033847213,1.6898249992495999,1.6876193277913001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8172859107398001,1.8127091856276001,1.8137563742000999,1.8271912033697999,1.8219596209169999,1.8158964298377001,1.8088461108825]
[null,null,null,null,"Coincident",1.6564226303525,1.6770214593713,1.6876101580056999,1.7059219185465999,1.7055236114657999,1.7043044053881,1.7020798344503001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5950377474426001,1.5893976744123,1.5888411865519001,1.5998365002041,1.5992838960849001,1.5966236963575999,1.5923113362671999]
[null,null,null,null,"Coincident",1.4622959732267999,1.4798245220371999,1.4897752989076001,1.5077375980404,1.5114011513456,1.5130988611934,1.5132155836333001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6087049611255,1.60301656066,1.602455304487,1.6135448323993999,1.6129874932457,1.6103044993758,1.605955188469]
[null,null,null,null,"Coincident",1.4748257779700999,1.4925045216098001,1.5025405625399,1.5206567731278,1.5243517178943,1.5260639747102001,1.5261816972960001]
[null,"Ramco 11kV","Substation Rating","MVA","Non-Coincident",9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005]
[null,null,null,null,"Coincident",9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005,9.3866666666667005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.1204432685265999,6.2784473330133999,6.5104061601555996,6.8452429606520999,7.0447214324366998,7.2455182630710002,7.4451077482318997]
[null,null,null,null,"Coincident",5.1409694489840998,5.2983820857447999,5.4868792811014,5.7071337668441,5.8705003585041,6.0348429343610004,6.1980687396784999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6069551894986001,6.7775189424853997,7.0279160966617997,7.3893689587529998,7.6047039053454997,7.8214620066771001,8.0369167910608006]
[null,null,null,null,"Coincident",5.5496233344216996,5.7195486472967998,5.9230294195916997,6.1607918583143002,6.3371444039067999,6.5145505143426998,6.6907510825349004]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.591150493202,5.7229304306674997,5.9221153021766,6.2175022393355999,6.4045851635868001,6.5878348042830002,6.7679197036514003]
[null,null,null,null,"Coincident",4.7154352863922,4.8460957051192004,5.0115472487070001,5.2097092176570996,5.3636580563961997,5.5142835935259997,5.6621504396877]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0355891143194,6.1778441934877,6.3928622016203001,6.7117293443659998,6.9136834256339998,7.1114995169614996,7.3058993027663997]
[null,null,null,null,"Coincident",5.0902636082555999,5.2313101785276004,5.4099134081563003,5.6238272035588004,5.7900133823041999,5.9526120913435001,6.1122328220227002]
[null,"Rapid Bay 11kV","Substation Rating","MVA","Non-Coincident",0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998]
[null,null,null,null,"Coincident",0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998,0.40949999999999998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5185199910905997E-2,3.5254995073812002E-2,3.5719871264071001E-2,3.6544780822294003E-2,3.6594577805808999E-2,3.6594584781417E-2,3.6558974475761001E-2]
[null,null,null,null,"Coincident",1.757295280131E-2,1.7730617351515002E-2,1.8104185950439999E-2,1.8418069281921998E-2,1.8331107856824E-2,1.8226937231731001E-2,1.8253404424928E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5759664366586001E-2,3.5830599066578997E-2,3.6303065233541001E-2,3.7141442989231999E-2,3.7192053002007001E-2,3.7192060091504997E-2,3.7155868380744E-2]
[null,null,null,null,"Coincident",1.7859864252465999E-2,1.8020102972501E-2,1.8399770780250999E-2,1.8718778846497999E-2,1.8630397612846999E-2,1.8524526206699001E-2,1.8551425526521999E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.1846127941689999E-2,3.1739778140974E-2,3.2035663239710001E-2,3.2686268867118E-2,3.2673973059537002E-2,3.2586955040672001E-2,3.2441765131453998E-2]
[null,null,null,null,"Coincident",1.6270267781782002E-2,1.6330183956069E-2,1.6652717620109E-2,1.691348372853E-2,1.6776520099563999E-2,1.6609541522344E-2,1.6569414639157998E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2366075777708003E-2,3.2257989616801999E-2,3.2558705595357999E-2,3.3219933581273002E-2,3.3207437021546E-2,3.3118998270128999E-2,3.2971437863020002E-2]
[null,null,null,null,"Coincident",1.6535910453948002E-2,1.6596804872284002E-2,1.692460450401E-2,1.7189628108790999E-2,1.7050428291405999E-2,1.6880723475378001E-2,1.6839941445477E-2]
[null,"Renmark 11kV","Substation Rating","MVA","Non-Coincident",29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998]
[null,null,null,null,"Coincident",29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998,29.902854831252998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.047510370013001,22.629700170265998,23.202700749866001,23.991568111565002,24.394018499268,24.807205673422999,25.224677739408001]
[null,null,null,null,"Coincident",20.830451848045001,21.682584206550999,22.161487733040001,22.770276855264001,23.155274865273,23.550091901178,23.948661643563]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.168203435774998,22.753580274867002,23.32971758943,24.122903389754001,24.527556882039001,24.943005936376998,25.362763339013]
[null,null,null,null,"Coincident",20.944482459781,21.801279583833999,22.282804736705,22.894926508480999,23.282032084802999,23.679010438593,24.079762042026999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.608642108748999,20.09819998835,20.580176034726001,21.274131758258999,21.665451203427001,22.054933421910999,22.447131083055002]
[null,null,null,null,"Coincident",18.568311072945001,19.308989575571001,19.711371345448999,20.249621158157002,20.624289494627,20.996808303935001,21.371561440699001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.715984257218999,20.208222087543,20.692836579969999,21.390591174320999,21.784052790771,22.175667123139998,22.570011763118998]
[null,null,null,null,"Coincident",18.669958213678999,19.414691358199999,19.81927585703,20.360472171133001,20.737191526943,21.111749588592001,21.488554208913001]
[null,"Riverton 11kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9459234552686999,1.9715863563225,2.0075067639609001,2.0535964442991999,2.0779563646794998,2.1017906147449001,2.1247929183576999]
[null,null,null,null,"Coincident",1.9459234552686999,1.9715863563225,2.0075067639609001,2.0535964442991999,2.0779563646794998,2.1017906147449001,2.1247929183576999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9988087055954999,2.0251690590299001,2.0620656919893001,2.1094079726163999,2.1344299336765999,2.1589119380396999,2.1825393857614999]
[null,null,null,null,"Coincident",1.9988087055954999,2.0251690590299001,2.0620656919893001,2.1094079726163999,2.1344299336765999,2.1589119380396999,2.1825393857614999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7263192788384001,1.7410499255941001,1.7670268846873001,1.8030528909982,1.8223938822714001,1.8395713431848,1.8552168386928001]
[null,null,null,null,"Coincident",1.7263192788384001,1.7410499255941001,1.7670268846873001,1.8030528909982,1.8223938822714001,1.8395713431848,1.8552168386928001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7732362461827,1.7883672344518999,1.8150501812244,1.8520552827596,1.8719219129844999,1.8895662135969999,1.9056369138808]
[null,null,null,null,"Coincident",1.7732362461827,1.7883672344518999,1.8150501812244,1.8520552827596,1.8719219129844999,1.8895662135969999,1.9056369138808]
[null,"Robe 7.6kV","Substation Rating","MVA","Non-Coincident",6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996]
[null,null,null,null,"Coincident",6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996,6.4255725190839996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.7642697033333001,3.8470860194355998,3.9535651009308999,4.0820955581403,4.1692872958037999,4.2569186694886998,4.3444973989386]
[null,null,null,null,"Coincident",3.7642697033333001,3.8470860194355998,3.9535651009308999,4.0820955581403,4.1692872958037999,4.2569186694886998,4.3444973989386]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.7669179006240001,3.8497924787428,3.9563464692212,4.0849673487529996,4.1722204265810001,4.2599134497184998,4.3475537915853]
[null,null,null,null,"Coincident",3.7669179006240001,3.8497924787428,3.9563464692212,4.0849673487529996,4.1722204265810001,4.2599134497184998,4.3475537915853]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2109412808748998,3.2724720975378001,3.3566569606439001,3.4620525209499,3.5374683429171001,3.6104366722660002,3.6823448940799]
[null,null,null,null,"Coincident",3.2109412808748998,3.2724720975378001,3.3566569606439001,3.4620525209499,3.5374683429171001,3.6104366722660002,3.6823448940799]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2132002066880001,3.2747743108290002,3.3590183987366999,3.4644881057588002,3.5399569834290001,3.6129766466479998,3.6849354565370001]
[null,null,null,null,"Coincident",3.2132002066880001,3.2747743108290002,3.3590183987366999,3.4644881057588002,3.5399569834290001,3.6129766466479998,3.6849354565370001]
[null,"Robertstown 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.96918428288193004,0.97721837035879999,0.99005724977498,1.0075664329978,1.0140861947577999,1.0200669109933,1.0253515485228999]
[null,null,null,null,"Coincident",0.96918428288193004,0.97721837035879999,0.99005724977498,1.0075664329978,1.0140861947577999,1.0200669109933,1.0253515485228999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.96941073963284996,0.97744670433099001,0.99028858364200001,1.0078018580090999,1.0143231431574999,1.0203052568294999,1.0255911291519999]
[null,null,null,null,"Coincident",0.96941073963284996,0.97744670433099001,0.99028858364200001,1.0078018580090999,1.0143231431574999,1.0203052568294999,1.0255911291519999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.87210288029550997,0.87812735153904997,0.88974369730486003,0.90631324589616002,0.91439038960468,0.92128804235294004,0.92731592285202002]
[null,null,null,null,"Coincident",0.87210288029550997,0.87812735153904997,0.88974369730486003,0.90631324589616002,0.91439038960468,0.92128804235294004,0.92731592285202002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.87230665329124002,0.87833253219502005,0.88995159220204001,0.90652501238536998,0.91460404337555001,0.92150330780906997,0.92753259676499]
[null,null,null,null,"Coincident",0.87230665329124002,0.87833253219502005,0.88995159220204001,0.90652501238536998,0.91460404337555001,0.92150330780906997,0.92753259676499]
[null,"Roonka 11kV","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1906499518792,3.2181461342661,3.28188771662,3.3946010239370001,3.4376682030402002,3.4800353217051998,3.5208783178587]
[null,null,null,null,"Coincident",2.3808803724627001,2.4126429109087,2.4571819059967002,2.5142831848179998,2.5449046769782,2.5749952743103002,2.6039502680383002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.4071439275997002,3.4365057981479001,3.5045724142068,3.6249336153340002,3.6709230156046,3.7161648544984001,3.7597791551669002]
[null,null,null,null,"Coincident",2.5424293563133999,2.5763470663799,2.6239081492139,2.6848838997123998,2.7175831405070001,2.7497154638657002,2.7806351299343]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0048992466822999,3.0288007796135998,3.0871213164250002,3.1931215848146999,3.2412189279810999,3.2860211147924998,3.3279970091412001]
[null,null,null,null,"Coincident",2.2513695622831,2.2784552172689998,2.3208385809585002,2.3768909507559002,2.4114302957568001,2.4435037814352998,2.4734629096316998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2087895493996998,3.2343128640895999,3.2965906024338998,3.4097832673187001,3.4611441414900002,3.5089862742968001,3.5538103432772998]
[null,null,null,null,"Coincident",2.4041308976554001,2.4330543854407001,2.4783135716265998,2.5381692418702002,2.5750521721064001,2.6093019279914,2.6412938616883999]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Rudall 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.34913669572292999,0.34768092973633002,0.34690466652930002,0.34796070680544,0.34622965710988002,0.34433852429916001,0.34221188292665999]
[null,null,null,null,"Coincident",0.29239079284250002,0.29135909194645998,0.29175828205894999,0.29348732661141003,0.29199533265455002,0.29036868238688002,0.28854372580239002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.35942383006063999,0.35792517067311003,0.35712603526733999,0.35821319123061002,0.35643113704029,0.35448428296764001,0.35229498119377001]
[null,null,null,null,"Coincident",0.30100593814783999,0.29994383871208002,0.30035479075726002,0.30213478072395,0.30059882592753001,0.29892424724090999,0.29704551924317002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.30915956218599999,0.30756251359072001,0.30666588821259,0.30762849278396998,0.30678301211037001,0.30552501335076998,0.30396083153223002]
[null,null,null,null,"Coincident",0.25922178355056003,0.25791056981255001,0.25824166620833999,0.25996241849953999,0.25921602235114999,0.25812141519269,0.25676847155088001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.31826879071155001,0.31662468589546999,0.31570164190873001,0.31669260913192998,0.31582221680230999,0.31452715175207002,0.31291688211551]
[null,null,null,null,"Coincident",0.26685962094581001,0.26550977296500999,0.26585062494692002,0.26762207832509999,0.2668536899956,0.26572683079654003,0.26433402336165002]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Salisbury 11kV","Substation Rating","MVA","Non-Coincident",71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994]
[null,null,null,null,"Coincident",71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994,71.319394725444994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",59.293702648217,61.414770711404998,62.732360157655002,65.484363168846002,66.366727196585003,67.231995947941996,68.069993313040996]
[null,null,null,null,"Coincident",59.293702648217,61.414770711404998,62.732360157655002,64.795948747336993,65.820913256302006,66.830007011255006,67.812558186765003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",59.651946799687998,61.785830055630001,63.111380190656,65.880010414173995,66.767705560367006,67.638202142940997,68.481262569403]
[null,null,null,null,"Coincident",59.651946799687998,61.785830055630001,63.111380190656,65.187436690254998,66.218593889581001,67.233784446046002,68.222272056563995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",54.317317593387003,56.946956240721001,58.031629132718997,60.147580437472001,61.157401131507001,62.165928524926997,63.110634214035002]
[null,null,null,null,"Coincident",54.317317593387003,56.946956240721001,58.031629132718997,59.484452555403003,60.609369331822002,61.735012361151,62.799029926403001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.645495131343999,57.291021682853,58.382248014802997,60.510983597580001,61.526905485191001,62.541526258247004,63.491939725296]
[null,null,null,null,"Coincident",54.645495131343999,57.291021682853,58.382248014802997,59.843849190790998,60.975562555008999,62.108006560055998,63.178452768701]
[null,"Salt Cliffs 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.10978584614903,0.11277668851492,0.11726549562687,0.12153385708467,0.12327250920578001,0.12496405220885,0.12767293359219001]
[null,null,null,null,"Coincident",0.10978584614903,0.11277668851492,0.11726549562687,0.12153385708467,0.12327250920578001,0.12496405220885,0.12767293359219001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11040130034228,0.11340890922716,0.11792288037671,0.12221517006433,0.12396356898591,0.12566459469801999,0.1283886619406]
[null,null,null,null,"Coincident",0.11040130034228,0.11340890922716,0.11792288037671,0.12221517006433,0.12396356898591,0.12566459469801999,0.1283886619406]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10280977235402999,0.10551931111435001,0.11008044625706,0.11444582591323001,0.11627038207856,0.11797686475287,0.12073304818066]
[null,null,null,null,"Coincident",0.10280977235402999,0.10551931111435001,0.11008044625706,0.11444582591323001,0.11627038207856,0.11797686475287,0.12073304818066]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10338611901182999,0.10611084731661,0.11069755196439,0.11508740372975,0.11692218826952,0.11863823740394,0.12140987186397]
[null,null,null,null,"Coincident",0.10338611901182999,0.10611084731661,0.11069755196439,0.11508740372975,0.11692218826952,0.11863823740394,0.12140987186397]
[null,"Sandy Creek 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3649712107354,2.3861167867067001,2.4380953731644999,2.529057786379,2.5677756408922998,2.6063121133055001,2.6439795394965002]
[null,null,null,null,"Coincident",2.2928810064118998,2.3235565850901998,2.3735087209347001,2.4360141457820998,2.4732674167736,2.5103423104849001,2.5465679625225999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4361749690843002,2.45795718895,2.5115007292189002,2.6052018081981001,2.6450853668621002,2.6847820824345998,2.7235835868334002]
[null,null,null,null,"Coincident",2.3619142971185001,2.3935134458095999,2.4449695237713001,2.509356840942,2.5477317208957002,2.5859228530461,2.6232391748399002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1382739951927001,2.1535737636024002,2.1966768698164998,2.2757666396745,2.3140838765199998,2.3504378726045001,2.3852994427179999]
[null,null,null,null,"Coincident",2.0592704848811998,2.081629709505,2.1247803377894998,2.1808565582588999,2.2176063684487,2.2524736118953999,2.2859007451418001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2026524299686998,2.2184128386634998,2.2628136787125999,2.3442846567793998,2.3837555361135001,2.4212040660937002,2.4571152366431002]
[null,null,null,null,"Coincident",2.1212703085217002,2.1443027171655999,2.1887525100637002,2.2465170545317998,2.2843733156552002,2.3202903303487998,2.3547238764882001]
[null,"Seacombe 11kV","Substation Rating","MVA","Non-Coincident",59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001]
[null,null,null,null,"Coincident",59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001,59.870019065777001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.249146563670003,49.451861995099001,51.306529351938003,53.052581181804001,53.685495218644,54.291234190541999,55.318413304962]
[null,null,null,null,"Coincident",48.249146563670003,49.451861995099001,51.306529351938003,53.052581181804001,53.685495218644,54.291234190541999,55.318413304962]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.777395378214003,49.993278565886001,51.868251480489,53.633419706704998,54.273263111492,54.885633929062998,55.924058965703999]
[null,null,null,null,"Coincident",48.777395378214003,49.993278565886001,51.868251480489,53.633419706704998,54.273263111492,54.885633929062998,55.924058965703999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.378064623446001,44.383310271364003,46.160241075563,47.839991102168,48.446673773771003,48.996325871158,49.960335080146002]
[null,null,null,null,"Coincident",43.378064623446001,44.383310271364003,46.160241075563,47.839991102168,48.446673773771003,48.996325871158,49.960335080146002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.852983100693997,44.869234535442999,46.665619809984001,48.363760337218999,48.977085186455,49.532755070466003,50.507318595088002]
[null,null,null,null,"Coincident",43.852983100693997,44.869234535442999,46.665619809984001,48.363760337218999,48.977085186455,49.532755070466003,50.507318595088002]
[null,"Seaford 11kV","Substation Rating","MVA","Non-Coincident",16.7,16.7,16.7,16.7,16.7,16.7,16.7]
[null,null,null,null,"Coincident",16.7,16.7,16.7,16.7,16.7,16.7,16.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.697161403685,11.002727384381,11.455748518332999,11.887612694196999,12.072163920893001,12.251830007325999,12.528685841265]
[null,null,null,null,"Coincident",10.697161403685,11.002727384381,11.455748518332999,11.887612694196999,12.072163920893001,12.251830007325999,12.528685841265]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.758831834636,11.066159440214999,11.521792295867,11.956146221003999,12.141761407873,12.322463291051999,12.600915232402]
[null,null,null,null,"Coincident",10.758831834636,11.066159440214999,11.521792295867,11.956146221003999,12.141761407873,12.322463291051999,12.600915232402]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.5802883258128997,9.8408317088579,10.274983821725,10.690886065208,10.869336498993,11.036372095806,11.299010243581]
[null,null,null,null,"Coincident",9.5802883258128997,9.8408317088579,10.274983821725,10.690886065208,10.869336498993,11.036372095806,11.299010243581]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.6355198482131996,9.8975652954139992,10.334220347787999,10.752520318073,10.931999540219,11.099998117476,11.36415040598]
[null,null,null,null,"Coincident",9.6355198482131996,9.8975652954139992,10.334220347787999,10.752520318073,10.931999540219,11.099998117476,11.36415040598]
[null,"Second Valley 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.23458252692395001,0.23866547387275,0.24559670184289001,0.25528907479944002,0.25981725635568997,0.26416109679291999,0.26845858163246999]
[null,null,null,null,"Coincident",0.20293043803274999,0.20790245083395001,0.21560481717194999,0.22285263989515999,0.22542743888471001,0.22789381896238001,0.23216351781120001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.24692926439186999,0.25122710830991002,0.25852314628188,0.26872565605853999,0.27349216853232999,0.27806463749609001,0.28258831103684001]
[null,null,null,null,"Coincident",0.21361123713359001,0.21884494093772999,0.22695270445643001,0.23458200045283001,0.23729231834726999,0.23988851093790001,0.24438293603315001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.21134806658081001,0.2152452403781,0.22210784667857,0.23179513215413,0.23712058143987,0.2421411001515,0.24694321514687001]
[null,null,null,null,"Coincident",0.18702650465583001,0.19181720567957999,0.19997795029802001,0.20774895378753,0.21088029431583,0.21377119620481999,0.21845731995827999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.22247190912205,0.22657420212566001,0.23379800667669001,0.24399516120393999,0.24960090384781,0.25488566656472,0.25994053036418002]
[null,null,null,null,"Coincident",0.19687023505983001,0.20191308413827,0.21050335167414999,0.21868336491049001,0.22197951668852001,0.22502257486610999,0.22995534247871]
[null,"Sheidow Park 11kV","Substation Rating","MVA","Non-Coincident",35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997]
[null,null,null,null,"Coincident",35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997,35.371847030105997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.606798026966999,29.373121555263999,30.530271645968998,31.626516605957001,32.061633905351997,32.481712620084998,33.154536756440997]
[null,null,null,null,"Coincident",28.606798026966999,29.373121555263999,30.530271645968998,31.626516605957001,32.061633905351997,32.481712620084998,33.154536756440997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.910834077446001,29.685302172595001,30.854750575855999,31.962646542283,32.402388313983003,32.826931669365003,33.506906651225997]
[null,null,null,null,"Coincident",28.910834077446001,29.685302172595001,30.854750575855999,31.962646542283,32.402388313983003,32.826931669365003,33.506906651225997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.508384070598002,26.146473091968002,27.242512995797998,28.284833105634,28.695154916629999,29.072905536013,29.697097916798999]
[null,null,null,null,"Coincident",25.508384070598002,26.146473091968002,27.242512995797998,28.284833105634,28.695154916629999,29.072905536013,29.697097916798999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.779489852504,26.424360550932999,27.532049281843001,28.585447279153001,29.000130033402002,29.381895425995999,30.012721788886999]
[null,null,null,null,"Coincident",25.779489852504,26.424360550932999,27.532049281843001,28.585447279153001,29.000130033402002,29.381895425995999,30.012721788886999]
[null,"Sherlock 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.7260170993198001E-2,1.7423700335203001E-2,1.7803150320012999E-2,1.8474521096978998E-2,1.8724948267959E-2,1.8979412424885999E-2,1.9240595875125999E-2]
[null,null,null,null,"Coincident",1.7083494449677002E-2,1.7325557476037E-2,1.7660083711355998E-2,1.8091213676770999E-2,1.8338685958065998E-2,1.8589953303611999E-2,1.8847583913776E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7702385978224999E-2,1.7870105031071001E-2,1.8259276731235001E-2,1.8947848393301998E-2,1.9204691644847002E-2,1.9465675312118999E-2,1.9733550424660001E-2]
[null,null,null,null,"Coincident",1.7521182885396999E-2,1.776944769838E-2,1.8112544678114E-2,1.8554720428144E-2,1.8808533084121001E-2,1.9066238035961001E-2,1.9330469282728E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1196490773055E-2,1.1356762318958999E-2,1.1596676558947E-2,1.1909744773624E-2,1.2120485509029E-2,1.2324579493834E-2,1.2524693145080999E-2]
[null,null,null,null,"Coincident",1.1196490773055E-2,1.1356762318958999E-2,1.1596676558947E-2,1.1909744773624E-2,1.2120485509029E-2,1.2324579493834E-2,1.2524693145080999E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1483350967053999E-2,1.1647728757287E-2,1.189378973082E-2,1.2214878923732001E-2,1.2431018951601E-2,1.2640341935495999E-2,1.2845582607520001E-2]
[null,null,null,null,"Coincident",1.1483350967053999E-2,1.1647728757287E-2,1.189378973082E-2,1.2214878923732001E-2,1.2431018951601E-2,1.2640341935495999E-2,1.2845582607520001E-2]
[null,"Smithfield West 11kV","Substation Rating","MVA","Non-Coincident",37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003]
[null,null,null,null,"Coincident",37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.065306814199001,29.072539077580998,30.237173267814999,32.031625370915997,32.753118950252002,33.472022600591004,34.182705884870003]
[null,null,null,null,"Coincident",27.732380890360002,28.992830704860999,29.887407452304,31.150404059338001,31.925714666663001,32.700313874643001,33.468428567139]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.088616312056999,29.096685127072998,30.262286598313,32.058229074483002,32.780321886642,33.499822618751999,34.211096157419]
[null,null,null,null,"Coincident",27.755413878285999,29.01691055297,29.912230286581998,31.176275869026,31.952230406632999,32.727472954046,33.496225600293997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.017846242548998,26.147784539077001,27.002514695295002,28.372253773748,28.985616952029002,29.601981246322001,30.191298976312002]
[null,null,null,null,"Coincident",24.818428005977999,26.147784539077001,26.775265595166001,27.577418271791998,28.232397157407998,28.891783835866999,29.526138494998001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.038624687525999,26.169501448559998,27.024941496562999,28.395818204843,29.009690808792001,29.626567021315999,30.21637420615]
[null,null,null,null,"Coincident",24.839040825152999,26.169501448559998,26.797503655850001,27.600322556302999,28.255845431301001,28.915779760012999,29.550661279180002]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"South End 11kV","Substation Rating","MVA","Non-Coincident",0.78,0.78,0.78,0.78,0.78,0.78,0.78]
[null,null,null,null,"Coincident",0.78,0.78,0.78,0.78,0.78,0.78,0.78]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.48443358510835999,0.49534231379742,0.50932298342772997,0.52614112731677998,0.53762927814000006,0.54916693388374005,0.56062012986426002]
[null,null,null,null,"Coincident",0.48443358510835999,0.49534231379742,0.50932298342772997,0.52614112731677998,0.53762927814000006,0.54916693388374005,0.56062012986426002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.49219556049112001,0.50327907739913003,0.51748375629890997,0.53457137369860996,0.54624359669730005,0.55796611782323002,0.56960282590528]
[null,null,null,null,"Coincident",0.49219556049112001,0.50327907739913003,0.51748375629890997,0.53457137369860996,0.54624359669730005,0.55796611782323002,0.56960282590528]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.43013434391616001,0.43800986412192999,0.44891152284156999,0.46260698462996003,0.47225725757685,0.48154246250147997,0.49057797576535001]
[null,null,null,null,"Coincident",0.43013434391616001,0.43800986412192999,0.44891152284156999,0.46260698462996003,0.47225725757685,0.48154246250147997,0.49057797576535001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.43702629420902001,0.44502800218508998,0.45610433584308002,0.47001923707688997,0.47982413427642001,0.48925811404710001,0.49843840140112]
[null,null,null,null,"Coincident",0.43702629420902001,0.44502800218508998,0.45610433584308002,0.47001923707688997,0.47982413427642001,0.48925811404710001,0.49843840140112]
[null,"Spalding 11kV","Substation Rating","MVA","Non-Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,null,null,"Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0800067427285001,1.1139059514002001,1.1556505632573,1.2132264997888,1.2450811714729999,1.2742526238022001,1.3003486395124999]
[null,null,null,null,"Coincident",1.0765818072972,1.1139059514002001,1.1556505632573,1.2017634083832001,1.2332660972997,1.2621266272502001,1.2879579717141001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0827204368476999,1.1167048228425001,1.1585543248851999,1.2162749304028,1.2482096421754001,1.2774543925641999,1.3036159787951]
[null,null,null,null,"Coincident",1.0792868957043,1.1167048228425001,1.1585543248851999,1.2047830360994001,1.2363648806898999,1.2652979274566001,1.2911941774111999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.99330237172081004,1.0224795169695,1.0632681717746999,1.1212984268916,1.1547295907951001,1.1847154201507999,1.2114095101227]
[null,null,null,null,"Coincident",0.97669658134037995,1.0108888217306,1.0504012200551001,1.0946788250840001,1.127263999967,1.1565007029884999,1.1825404708059]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.99579820688383003,1.0250486644965,1.0659398074885,1.1241158731414,1.1576310383287001,1.1876922119997999,1.2144533752519999]
[null,null,null,null,"Coincident",0.97915069173084002,1.0134288457344001,1.0530405254418,1.0974293852171999,1.1300964356978001,1.1594066007318999,1.1855117977378999]
[null,"Square Water Hole 11kV","Substation Rating","MVA","Non-Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,null,null,"Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0814191094750001,4.1849103933708003,4.3436209427100003,4.4934959236622998,4.5513974247853,4.6071096457090004,4.6987536884371996]
[null,null,null,null,"Coincident",4.0814191094750001,4.1849103933708003,4.3436209427100003,4.4934959236622998,4.5513974247853,4.6071096457090004,4.6987536884371996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.2847559074178001,4.3934031397027002,4.5600206679718003,4.7173624387590003,4.7781485997316002,4.8366364102982002,4.9328461704151998]
[null,null,null,null,"Coincident",4.2847559074178001,4.3934031397027002,4.5600206679718003,4.7173624387590003,4.7781485997316002,4.8366364102982002,4.9328461704151998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8383516959107,3.9435980000767001,4.1195333592698002,4.2894829907628997,4.3642716396371002,4.4345050836709996,4.5429673701112003]
[null,null,null,null,"Coincident",3.8383516959107,3.9435980000767001,4.1195333592698002,4.2894829907628997,4.3642716396371002,4.4345050836709996,4.5429673701112003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.0295788456570003,4.1400685335361,4.3247690137871997,4.5031855566540999,4.5817001851391002,4.6554326679228,4.7692985587052004]
[null,null,null,null,"Coincident",4.0295788456570003,4.1400685335361,4.3247690137871997,4.5031855566540999,4.5817001851391002,4.6554326679228,4.7692985587052004]
[null,"Stansbury 11kV","Substation Rating","MVA","Non-Coincident",1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999]
[null,null,null,null,"Coincident",1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999,1.8049999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.99869415750580004,1.0205748754804,1.0483257570478,1.0823819726471999,1.1070353719471,1.1340499099621,1.161467324268]
[null,null,null,null,"Coincident",0.99869415750580004,1.0205748754804,1.0483257570478,1.0823819726471999,1.1070353719471,1.1340499099621,1.161467324268]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0512568781510001,1.0742892100184001,1.1035006606944999,1.1393493042692999,1.1653002476978001,1.1937365999933001,1.2225970325427999]
[null,null,null,null,"Coincident",1.0512568781510001,1.0742892100184001,1.1035006606944999,1.1393493042692999,1.1653002476978001,1.1937365999933001,1.2225970325427999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.94361090387851998,0.96110858913291997,0.98552167356209996,1.0167118094965,1.0406869844699,1.0661807619140999,1.0918788397632]
[null,null,null,null,"Coincident",0.94361090387851998,0.96110858913291997,0.98552167356209996,1.0167118094965,1.0406869844699,1.0661807619140999,1.0918788397632]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.99327451306819003,1.0116931268522,1.0373911072901001,1.0702228252741,1.0954598484471001,1.1222954003393,1.1493460052628]
[null,null,null,null,"Coincident",0.99327451306819003,1.0116931268522,1.0373911072901001,1.0702228252741,1.0954598484471001,1.1222954003393,1.1493460052628]
[null,"Stirling East 11kV","Substation Rating","MVA","Non-Coincident",17.5,17.5,17.5,17.5,17.5,17.5,17.5]
[null,null,null,null,"Coincident",17.5,17.5,17.5,17.5,17.5,17.5,17.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7031650362558004,8.9395759604214007,9.2380984229447005,9.5818544976698998,9.8296533759294,10.078958224546,10.331625190003001]
[null,null,null,null,"Coincident",8.7031650362558004,8.9395759604214007,9.2380984229447005,9.5818544976698998,9.8296533759294,10.078958224546,10.331625190003001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7263071451969001,8.9633466966882001,9.2626629439231998,9.6073330815780995,9.8557908682476008,10.105758629717,10.359097448048001]
[null,null,null,null,"Coincident",8.7263071451969001,8.9633466966882001,9.2626629439231998,9.6073330815780995,9.8557908682476008,10.105758629717,10.359097448048001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.4209971298125001,7.5973270871357004,7.7802807825098004,7.9952110584967002,8.1984443937672999,8.3930474354147009,8.5807213290697]
[null,null,null,null,"Coincident",7.4209971298125001,7.5973270871357004,7.7802807825098004,7.9952110584967002,8.1984443937672999,8.3930474354147009,8.5807213290697]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.4407298963765998,7.6175287230209001,7.8009689005347997,8.0164706858335997,8.2202444277225002,8.4153649276475999,8.6035378546627008]
[null,null,null,null,"Coincident",7.4407298963765998,7.6175287230209001,7.8009689005347997,8.0164706858335997,8.2202444277225002,8.4153649276475999,8.6035378546627008]
[null,"Stirling North 1 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.7196648500084,1.7453361949148001,1.7829764044447001,1.8398758246824001,1.8849832588797,1.9356796238895,1.9915557919936]
[null,null,null,null,"Coincident",1.5948948242301999,1.6429710773512001,1.6880259296719999,1.7478493810136,1.7954231660936,1.8485444958304,1.9068262497374999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.954164685044,1.9833366691276999,2.0261096363141,2.0907680711408001,2.1420265212630998,2.1996360293959998,2.2631316776579999]
[null,null,null,null,"Coincident",1.8123805588368,1.8670126669697999,1.9182113649573,1.9861925625428001,2.0402536842413999,2.1006188342262,2.1668481028345998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5148792441526999,1.5507799630440999,1.5946477477483001,1.6535887642416001,1.7039475468459999,1.7548700719863,1.8067581277667]
[null,null,null,null,"Coincident",1.4131318097929999,1.4691568557968,1.5214069027823001,1.5856890060860001,1.6385162193931,1.6921935675835,1.7470815355806]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7214537594432999,1.7622500326385999,1.8120997900953999,1.8790782207654,1.9363041125122,1.9941706208040999,2.0531343230518]
[null,null,null,null,"Coincident",1.6058316700469,1.6694964977474001,1.7288715536546999,1.8019194014116999,1.8619503281668,1.92294731733,1.9853200108774001]
[null,"Stirling North 2 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9546801722036,1.9945033422191001,2.0405374436344998,2.1009040294723,2.1400535002144001,2.1779800853771998,2.2142577761008]
[null,null,null,null,"Coincident",1.8486989534767,1.9146431613487001,1.970064020735,2.0352790375473,2.0786731729365,2.1210582142052998,2.1619670788804002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9849311730185,2.0253706539607998,2.0721171878544999,2.1334180184160001,2.1731733737873999,2.2116869179703,2.2485260491112]
[null,null,null,null,"Coincident",1.8773097688639,1.9442745417953999,2.0005531049054999,2.0667774016781002,2.1108431129311001,2.1538841131318001,2.1954260911500998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7438355991736001,1.7756082413734,1.8128888801272001,1.8636390119619,1.9012178596378999,1.9362487989824,1.9692675691613]
[null,null,null,null,"Coincident",1.6588703698391001,1.7154078399795001,1.7638191647407,1.8224454970501001,1.8643552150600999,1.904006765556,1.9418699401046999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7708235294149,1.8030878910474,1.8409454920323001,1.8924810425259,1.9306414675707999,1.966214552372,1.9997443272963]
[null,null,null,null,"Coincident",1.6845433620879,1.7419558168317,1.7911163644303001,1.8506500089699001,1.8932083297190001,1.9334735351254999,1.9719226873397]
[null,"Stockwell TF1 11kV","Substation Rating","MVA","Non-Coincident",8.90625,8.90625,8.90625,8.90625,8.90625,8.90625,8.90625]
[null,null,null,null,"Coincident",8.90625,8.90625,8.90625,8.90625,8.90625,8.90625,8.90625]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3449290818308,2.3658954580058,2.4174335479681002,2.5076250932741,2.5460148303763002,2.5842247225147998,2.6215729332294999]
[null,null,null,null,"Coincident",2.2641884713510998,2.2944801835686999,2.3438072309742002,2.4055304786876999,2.4423175716346002,2.4789285194696999,2.5147008528274002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3748906329397999,2.3961249000102001,2.4483215007685999,2.5396654385350002,2.5785456877295001,2.6172437940511002,2.6550692091013999]
[null,null,null,null,"Coincident",2.2931183861746001,2.3237971406661,2.3737544480070998,2.4362663439809999,2.4735234717677002,2.5106022038071001,2.5468316062516001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1328052637471999,2.1480659023144,2.1910587704052,2.2699462646369,2.3081655034341999,2.3444265225467,2.3791989326343002]
[null,null,null,null,"Coincident",2.0456364243429999,2.0678476125507999,2.1107125482648001,2.166417498136,2.2029239944238999,2.2375603881053001,2.2707662062979002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1600564733511001,2.1755120996499002,2.2190542948076,2.2989497477484,2.3376573201527,2.3743816523715999,2.4095983553592002]
[null,null,null,null,"Coincident",2.0717738631053,2.0942688473800999,2.1376814755475002,2.194098176881,2.2310711227782001,2.2661500714553,2.2997801659411001]
[null,"Stockwell TF2 11kV","Substation Rating","MVA","Non-Coincident",8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993]
[null,null,null,null,"Coincident",8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993,8.6999999999999993]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8602162593502003,4.9036722099693,5.0104926101049001,5.1974280779397999,5.2769965501389002,5.3561922667506998,5.4336020197278998]
[null,null,null,null,"Coincident",4.1053586875079997,4.1602827123786001,4.2497210365982996,4.3616357797517002,4.4283370343196999,4.4947189078493999,4.5595802307386002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9528910497496001,4.9971756201051001,5.1060328757353002,5.2965328362544,5.3776185231389002,5.4583243467183999,5.5372101518400001]
[null,null,null,null,"Coincident",4.1836398247203004,4.2396111430075996,4.3307548806304998,4.4448036184069002,4.5127767350601999,4.5804243807051996,4.6465224817918003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.6148681566240004,4.6478884403651,4.7409144757405999,4.9116076896378003,4.9943047605302997,5.0727647236940001,5.148003701565]
[null,null,null,null,"Coincident",3.8721234414947001,3.9141663292237001,3.9953040721876998,4.1007462903830003,4.1698483352825999,4.2354105194061997,4.2982648103679004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7028646399724998,4.7365145557529003,4.8313144151456999,5.0052624138048003,5.0895363556228999,5.1694923963791997,5.2461660339716003]
[null,null,null,null,"Coincident",3.9459572400732998,3.9888018032011998,4.0714866837659001,4.1789394782297,4.2493591635766998,4.3161714899466004,4.3802242889437002]
[null,"Strathalbyn 11kV","Substation Rating","MVA","Non-Coincident",16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999]
[null,null,null,null,"Coincident",16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999,16.899999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.02331271111,11.330587533188,11.70196465824,12.130286065150001,12.436793166179999,12.74496170355,13.057687120737]
[null,null,null,null,"Coincident",11.02331271111,11.330587533188,11.70196465824,12.130286065150001,12.436793166179999,12.74496170355,13.057687120737]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.025415328197001,11.332748760722,11.704196723272,12.132599829388999,12.439165394429001,12.747392712717,13.060177780012999]
[null,null,null,null,"Coincident",11.025415328197001,11.332748760722,11.704196723272,12.132599829388999,12.439165394429001,12.747392712717,13.060177780012999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3782854187965992,9.6077136009526996,9.8458149723942991,10.124958302597999,10.389870237809999,10.64443817543,10.891342740303999]
[null,null,null,null,"Coincident",9.3782854187965992,9.6077136009526996,9.8458149723942991,10.124958302597999,10.389870237809999,10.64443817543,10.891342740303999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.3800742588380999,9.6095462027587999,9.8476929903130994,10.126889565086,10.391852030331,10.646468524942,10.893420185074]
[null,null,null,null,"Coincident",9.3800742588380999,9.6095462027587999,9.8476929903130994,10.126889565086,10.391852030331,10.646468524942,10.893420185074]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Streaky Bay 11kV","Substation Rating","MVA","Non-Coincident",7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001]
[null,null,null,null,"Coincident",7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001,7.1187169312169001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9242475736085001,2.9533018052683002,3.0140463131303998,3.1183634035580998,3.1617650287333001,3.204828161425,3.2467033470573998]
[null,null,null,null,"Coincident",2.6492487199892998,2.6892767747550002,2.7438599138491999,2.8128088425482001,2.8524734791112998,2.8918410858972998,2.9301180878155999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9256403743494999,2.9547084443572,3.0154818844465998,3.1198486604489002,3.1632709575454001,3.2063546009366002,3.2482497314567]
[null,null,null,null,"Coincident",2.6505105405045999,2.6905576603812,2.7451667970815001,2.8141485657218999,2.8538320943022,2.8932184516318999,2.9315136846456]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6403230176295001,2.6684438609430998,2.7260651670054998,2.8253857564637999,2.8758077763376999,2.9238391424910999,2.9700485223191002]
[null,null,null,null,"Coincident",2.3640318615728,2.4001465361824001,2.4527578667694998,2.5203812186776999,2.5657517744173002,2.6089964672643,2.6505951618507]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6415805868889,2.6697148239834001,2.7273635747117999,2.8267314699426001,2.8771775055076998,2.9252317486988999,2.9714631377641001]
[null,null,null,null,"Coincident",2.3651578350909999,2.4012897108931002,2.4539260999264001,2.5215816604121,2.5669738258621999,2.6102391158846001,2.6518576236678002]
[null,"Swan Reach 11kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4920126824219999,1.5159485785053,1.5573035151057,1.6224925901444001,1.6549226760404001,1.6872990039917,1.7191136541823999]
[null,null,null,null,"Coincident",1.0774431103097,1.0998543470933999,1.1283667315429,1.1629782537652,1.1856286589006999,1.2082262124204,1.2304095072303001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5827514859497001,1.6081430764768001,1.6520130704299001,1.7211667087339,1.7555690749109001,1.7899144137797001,1.8236639156825001]
[null,null,null,null,"Coincident",1.1429692950737,1.1667435020488,1.196989906377,1.2337063759311,1.2577342966103,1.2817061514300001,1.3052385538266]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3632830165409,1.3856547657244001,1.4240744900019999,1.4851334930405,1.5198646237466,1.5534227595337999,1.5860597789987001]
[null,null,null,null,"Coincident",0.98847643163551002,1.0087609160304001,1.0360658634366,1.0698495618588,1.0942956476028001,1.1178814472412999,1.1407893181293001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4461929483719,1.4699252662540001,1.5106815389095001,1.5754539292037,1.6122972813959999,1.6478963013699,1.6825181860653999]
[null,null,null,null,"Coincident",1.0485919854632999,1.0701100986778,1.0990756340182,1.1349139345289001,1.1608467426028,1.1858669450882999,1.2101679896538]
[null,"Swan Reach 33kV","Substation Rating","MVA","Non-Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,null,null,"Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9269420152429,1.9591926899656,2.013974681838,2.0996887324547999,2.1431034716411999,2.1865177165468999,2.2293887942478001]
[null,null,null,null,"Coincident",1.5993906516783001,1.6337738127474,1.6772395286716999,1.7298476783165,1.7647297002325999,1.7995887823032,1.8339816065118999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0903655102091001,2.1253513570005,2.1847793966015998,2.2777628355075001,2.3248595684200999,2.3719557651321002,2.4184627287576999]
[null,null,null,null,"Coincident",1.7350345932425999,1.7723337820414,1.8194858150169,1.8765556493469999,1.9143960072627999,1.9522114798103001,1.9895211512771001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8039906682583999,1.8329081725831999,1.883015166241,1.9630546690205,2.0082885678159998,2.0519845037394999,2.0945923750548001]
[null,null,null,null,"Coincident",1.5034142227203999,1.5336914221333999,1.5746083465277001,1.6253754224723,1.6619576572220001,1.6972438153039,1.731607609428]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.9569866886684999,1.9883566796717,2.0427132355690998,2.1295408695825002,2.1786110445987998,2.2260128224771001,2.2722342572458998]
[null,null,null,null,"Coincident",1.6309184261242,1.6637634276333,1.7081505066742,1.7632231262803,1.8029078916767001,1.8411866604506,1.8784648397982999]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Tailem Bend Town 11kV","Substation Rating","MVA","Non-Coincident",4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996]
[null,null,null,null,"Coincident",4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996,4.1669907705515996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2142186227030001,3.2541122251990999,3.3348387569907998,3.4706009124299002,3.5276078987610999,3.5854386323814,3.6436463330823998]
[null,null,null,null,"Coincident",3.0251994317998001,3.0769917440681001,3.1457030204194001,3.2318126058968999,3.2852987877359001,3.3395258491878002,3.3940666296779001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2912252204447001,3.3320745981884001,3.4147351849684,3.5537499448254999,3.6121227107068998,3.6713389593041001,3.7309412064002001]
[null,null,null,null,"Coincident",3.0976774873021999,3.1507106453949998,3.2210681139439998,3.3092407221926998,3.3640083317667999,3.4195345710276999,3.4753820454415001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0245174563393999,3.059841182754,3.1162578605412001,3.1920870410524,3.2402433247498998,3.2864693420643998,3.3319781111257001]
[null,null,null,null,"Coincident",3.0245174563393999,3.059841182754,3.1162578605412001,3.1920870410524,3.2402433247498998,3.2864693420643998,3.3319781111257001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.0969791729998,3.1331491890761001,3.1909175037375999,3.2685634079649,3.3178734251208,3.3652069303626999,3.4118060034400002]
[null,null,null,null,"Coincident",3.0969791729998,3.1331491890761001,3.1909175037375999,3.2685634079649,3.3178734251208,3.3652069303626999,3.4118060034400002]
[null,"Tantanoola 11kV","Substation Rating","MVA","Non-Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,null,null,"Coincident",1.425,1.425,1.425,1.425,1.425,1.425,1.425]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.57266493466426005,0.58514233179342001,0.60541174358288996,0.63619568932798998,0.65302579301089003,0.67001539049938996,0.68714546894310002]
[null,null,null,null,"Coincident",0.49766981557036999,0.51102069004355,0.52728497255952,0.54658970683735997,0.56044196213483,0.57440768576169998,0.58846968210299]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.60839712523500999,0.62165306616011995,0.64318721486813002,0.67589196586828004,0.69377220626415004,0.71182189229382997,0.73002082477485997]
[null,null,null,null,"Coincident",0.52872258589878995,0.54290650594904,0.5601856200134,0.58069489887285997,0.59541148407105005,0.61024861760603,0.62518803091955]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.53082481578981999,0.54052800955113001,0.55702184785923003,0.58302677753065002,0.59815399865820995,0.61293141057885003,0.62767917285066999]
[null,null,null,null,"Coincident",0.46058076565078998,0.47092276252495002,0.48456521373719003,0.50135009628779004,0.51385495355097,0.52604530216798995,0.53818246061241004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.56394633647208003,0.57425497391892,0.59177796721451004,0.61940550907423997,0.63547661329191996,0.65117608149175998,0.66684405001350999]
[null,null,null,null,"Coincident",0.4893193153598,0.50030661488969996,0.51480030499759999,0.53263250262845996,0.54591761709918996,0.55886859873831995,0.57176307133324999]
[null,"Tarlton 11kV","Substation Rating","MVA","Non-Coincident",0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004]
[null,null,null,null,"Coincident",0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004,0.66500000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.53002008243164001,0.53443501872081001,0.54456156461604999,0.56251598878209996,0.56944254406910999,0.57628634398391998,0.58289527376900996]
[null,null,null,null,"Coincident",0.50111613974424996,0.50787875706378005,0.51736431407326,0.52952422730770998,0.53614147514222998,0.54268207160888005,0.54899769232276996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.66392228077030002,0.66945258927693996,0.68213746607679004,0.70462782566383997,0.71330427875770996,0.72187706948619002,0.73015565341499999]
[null,null,null,null,"Coincident",0.62771615917539003,0.63618725765558004,0.64806920864735995,0.66330115474938001,0.67159015816706003,0.67978314531541995,0.68769431971772998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.48066956597865002,0.48417288843117001,0.49298791102034001,0.50926074565152002,0.51664170486295002,0.52354612748911999,0.53008018463266005]
[null,null,null,null,"Coincident",0.44913857760201997,0.45448298061983999,0.46290533257937999,0.47409585153174,0.48104058089766,0.48754245185306,0.49369519057050998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.60210404307193999,0.60649243119165996,0.61753444657264001,0.63791838642897003,0.64716404227552005,0.65581277119978998,0.66399756695606005]
[null,null,null,null,"Coincident",0.56260718925103004,0.56930178132133002,0.57985192330230995,0.59386957114646,0.60256878974739003,0.61071326792295999,0.61842041045902996]
[null,"Tarpeena South 11kV","Substation Rating","MVA","Non-Coincident",10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001]
[null,null,null,null,"Coincident",10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001,10.859958563457001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.8356125900881999,5.8836732656292998,5.9973479863868997,6.2008449232215996,6.2792480454512001,6.3573628956643002,6.4356996802947002]
[null,null,null,null,"Coincident",4.5221446272819996,4.5845878040308996,4.6713814638097002,4.7828193359605997,4.8446049284893,4.9061347461324001,4.9675413333131004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3804999972595002,6.4330482319862998,6.5573370781503,6.7798350909760998,6.8655589311811998,6.9509675826082997,7.0366188910877003]
[null,null,null,null,"Coincident",4.9443898710802001,5.0126635412261003,5.1075613668497004,5.2294045036201,5.2969591890750003,5.3642342172305,5.4313745085520999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5060612714166997,5.5419528366417001,5.6356764590986996,5.8121095259490003,5.8916689937826998,5.9735722711539996,6.0515254013612996]
[null,null,null,null,"Coincident",4.3022660427341997,4.3485395873629002,4.4239308515362001,4.5258758955714002,4.5875286125354,4.6509253014922001,4.7108957528332001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0201775537423998,6.0594204144162997,6.161895272642,6.3548023865356003,6.4417905435555998,6.5313413581404003,6.6165731893141002]
[null,null,null,null,"Coincident",4.7039806104504001,4.7545748448721001,4.8370056014421996,4.9484695382861004,5.0158789412146003,5.0851951556600996,5.1507652151369996]
[null,"Teal Flat 11kV","Substation Rating","MVA","Non-Coincident",3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001]
[null,null,null,null,"Coincident",3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001,3.5563299328940001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7692036934828002,2.8157229926498002,2.8774957642035002,2.9543172223796001,3.0003258842049001,3.0457898283647,3.0898691696374998]
[null,null,null,null,"Coincident",2.7692036934828002,2.8157229926498002,2.8774957642035002,2.9543172223796001,3.0003258842049001,3.0457898283647,3.0898691696374998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8463268113286002,2.8941416863320999,2.9576348473073,3.0365958051474999,3.0838858214127001,3.1306159494691999,3.1759229130508002]
[null,null,null,null,"Coincident",2.8463268113286002,2.8941416863320999,2.9576348473073,3.0365958051474999,3.0838858214127001,3.1306159494691999,3.1759229130508002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2138247049727,2.2457340688926002,2.2930167010365001,2.3541148008995001,2.3942252817509999,2.4330100664743002,2.4696691055126001]
[null,null,null,null,"Coincident",2.2138247049727,2.2457340688926002,2.2930167010365001,2.3541148008995001,2.3942252817509999,2.4330100664743002,2.4696691055126001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2754803585504999,2.3082784074160001,2.3568778744391001,2.4196775739232002,2.4609051431814,2.5007700952934999,2.5384500990931]
[null,null,null,null,"Coincident",2.2754803585504999,2.3082784074160001,2.3568778744391001,2.4196775739232002,2.4609051431814,2.5007700952934999,2.5384500990931]
[null,"Tea Tree Gully 11kV","Substation Rating","MVA","Non-Coincident",49.862835820895,49.862835820895,49.862835820895,49.862835820895,49.862835820895,49.862835820895,49.862835820895]
[null,null,null,null,"Coincident",49.862835820895,49.862835820895,49.862835820895,49.862835820895,49.862835820895,49.862835820895,49.862835820895]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.429209840883999,35.019562810318,35.984545895624002,37.941600298032,38.718842797485003,39.503172691526999,40.309643289111001]
[null,null,null,null,"Coincident",34.252074815173003,35.019562810318,35.984545895624002,37.157988898540999,37.958289703890998,38.767802723232002,39.600740074302998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.825245072133001,35.422388803708998,36.398471978186002,38.378038151745002,39.164221182056998,39.957573132439002,40.773320468324997]
[null,null,null,null,"Coincident",34.646072482644001,35.422388803708998,36.398471978186002,37.585412960672997,38.394919533916003,39.213744288184998,40.056262821571003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.215066854042998,30.776608517654999,31.506353214440999,33.098178680841002,33.79585241449,34.574346800265999,35.355062197282997]
[null,null,null,null,"Coincident",30.124175885404,30.776608517654999,31.506353214440999,32.507366537945003,33.240700288614001,34.056895698761998,34.878401606552998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.562627284388999,31.130628297013999,31.86876716291,33.478903214119001,34.184602208286996,34.972051525224998,35.761747401440999]
[null,null,null,null,"Coincident",30.470690807417,31.130628297013999,31.86876716291,32.881295027261999,33.623064231514,34.448648243360999,35.279603838893003]
[null,"Telowie 11kV","Substation Rating","MVA","Non-Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,null,null,"Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.55731164454577997,0.55585650100631001,0.56232711759469001,0.57846890003953999,0.57928083542326003,0.57960604492294998,0.57934576056414999]
[null,null,null,null,"Coincident",0.49788287669178,0.50022634875254002,0.50489541401682003,0.51169427235409004,0.51260073757875002,0.51307556587449998,0.51303006515592997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.56059958359688999,0.55913585523181997,0.56564464614003995,0.58188165931866997,0.58269838483029002,0.58302551294951999,0.58276369300624997]
[null,null,null,null,"Coincident",0.50082020730235999,0.50317750500874003,0.50787411608543997,0.51471308525127002,0.51562489829601998,0.51610252790861999,0.51605675875210999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.49481510186561001,0.49132303682320999,0.49415356097231999,0.50510877885257,0.50466702469614,0.50332726288973995,0.50142331740704005]
[null,null,null,null,"Coincident",0.43883145655394001,0.43840733522191999,0.44041374141678002,0.44461361967580998,0.44439260937354003,0.44337845337864001,0.44186369461431002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.49773433370372,0.49422166672855999,0.49706888995614001,0.50808873969727997,0.50764437934957996,0.50629671342849003,0.50438153534950003]
[null,null,null,null,"Coincident",0.44142040494031998,0.44099378144438001,0.44301202471701001,0.44723668075320999,0.44701436656933002,0.44599422741736999,0.44447053211896997]
[null,"Thebarton 11kV","Substation Rating","MVA","Non-Coincident",51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002]
[null,null,null,null,"Coincident",51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002,51.889795316090002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.083554008715002,24.337489368044999,24.863303942363999,25.812661808619001,26.187168328523999,26.714918315936,27.257195851788001]
[null,null,null,null,"Coincident",21.716458751665002,21.99268794923,22.345235717314001,22.850173554984998,23.153967065334001,23.602221794704999,24.062247504113]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.020907033017998,25.284725779034002,25.83100551731,26.817313223557999,27.206395865365,27.754686344707,28.318069797402998]
[null,null,null,null,"Coincident",22.561682354487001,22.848662634456002,23.214931870581001,23.739522331326,24.055139751285001,24.520840947488999,24.998771260586999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.374819247455001,21.534910092442999,21.948698782095001,22.758130457994,23.162029436981999,23.653459325646999,24.164605927968001]
[null,null,null,null,"Coincident",19.43024574911,19.628890281760999,19.882048800303998,20.334935802794,20.670333947119001,21.091854307822,21.531042254363001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.206745941425002,22.373067662373,22.802961370393,23.643896836351001,24.063515917503,24.574072688030999,25.105113563987]
[null,null,null,null,"Coincident",20.186487938668002,20.392863890584,20.655875560487999,21.126389321941001,21.474841455922,21.912767758405,22.369049284646]
[null,"Tintinara 11kV","Substation Rating","MVA","Non-Coincident",0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997]
[null,null,null,null,"Coincident",0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997,0.93137254901960997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0929487148432999,1.0972204048,1.1072047625187,1.1226867320225999,1.1262481709737,1.129596170216,1.1325315904005]
[null,null,null,null,"Coincident",1.0929487148432999,1.0972204048,1.1072047625187,1.1226867320225999,1.1262481709737,1.129596170216,1.1325315904005]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1132505569397,1.1176015947869999,1.1277714148710001,1.1435409664873999,1.1471685602088999,1.1505787495165001,1.1535686959896001]
[null,null,null,null,"Coincident",1.1132505569397,1.1176015947869999,1.1277714148710001,1.1435409664873999,1.1471685602088999,1.1505787495165001,1.1535686959896001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0910193488302,1.092808210629,1.1018694940161,1.1172480472043,1.1223914149920999,1.1263861411528,1.1294669802841999]
[null,null,null,null,"Coincident",1.0910193488302,1.092808210629,1.1018694940161,1.1172480472043,1.1223914149920999,1.1263861411528,1.1294669802841999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1112853523885999,1.1131074428187,1.1223370421953001,1.1380012565076001,1.1432401638567,1.1473090932243999,1.1504471598438999]
[null,null,null,null,"Coincident",1.1112853523885999,1.1131074428187,1.1223370421953001,1.1380012565076001,1.1432401638567,1.1473090932243999,1.1504471598438999]
[null,"Tonsley Park 11kV","Substation Rating","MVA","Non-Coincident",39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999]
[null,null,null,null,"Coincident",39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999,39.831349937365999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.405308840610001,17.688739242945001,18.216954463943999,18.955284647801999,19.314765384126002,19.665253804757999,20.031334696918002]
[null,null,null,null,"Coincident",16.741049972542999,17.132325542063001,17.781202530893999,18.397774461985001,18.632779652322,18.863082723775001,19.260874355719999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.636194334630002,17.923384507565,18.458606627055001,19.206730933546002,19.570980265944002,19.926117997477999,20.297055038322998]
[null,null,null,null,"Coincident",16.963123917263999,17.359589848759001,18.017074342661999,18.641825244675999,18.879947833846,19.113305929424001,19.516374360436998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.63210768705,15.912863487087,16.426982595767999,17.119232314171001,17.511190857765001,17.885657162470999,18.268080734426]
[null,null,null,null,"Coincident",15.380549177780001,15.767097986641,16.426982595767999,17.059576509978999,17.315373171440999,17.556381291097001,17.968501149632001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.839471252899999,16.123951344310999,16.644890363255001,17.346322936135,17.743480901516001,18.122914589366001,18.510411099477]
[null,null,null,null,"Coincident",15.584575761147001,15.976252230397,16.644890363255001,17.285875783744,17.545065647767,17.789270796518,18.206857521399002]
[null,"Tumby Bay 11kV","Substation Rating","MVA","Non-Coincident",5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996]
[null,null,null,null,"Coincident",5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996,5.1649903288200996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.454040693938,2.4909250888865002,2.5555095726790999,2.640710222894,2.7011558800238999,2.7641047822077001,2.8289565243996999]
[null,null,null,null,"Coincident",2.1571590175350002,2.3755710492073998,2.5555095726790999,2.640710222894,2.7011558800238999,2.7641047822077001,2.8289565243996999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4619710811847999,2.4989746703814002,2.5637678630059,2.6492438444944,2.7098848355768999,2.7730371611073998,2.8380984757937]
[null,null,null,null,"Coincident",2.1641300129240002,2.3832478568491999,2.5637678630059,2.6492438444944,2.7098848355768999,2.7730371611073998,2.8380984757937]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2256898857062,2.2617917424382998,2.3364689888307999,2.4176440019724001,2.4796182312963002,2.5417375751603002,2.6045495607800002]
[null,null,null,null,"Coincident",1.9508809702464001,2.1623082834871998,2.3364689888307999,2.4176440019724001,2.4796182312963002,2.5417375751603002,2.6045495607800002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2328823429171001,2.2691008650756999,2.3440194356988,2.4254567710141002,2.4876312739678998,2.5499513604086999,2.6129663269206]
[null,null,null,null,"Coincident",1.9571853651183999,2.1692959190538001,2.3440194356988,2.4254567710141002,2.4876312739678998,2.5499513604086999,2.6129663269206]
[null,"Two Wells 11kV","Substation Rating","MVA","Non-Coincident",16.3,16.3,16.3,16.3,16.3,16.3,16.3]
[null,null,null,null,"Coincident",16.3,16.3,16.3,16.3,16.3,16.3,16.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.1331410426820998,7.3604792026992003,7.6262164446665004,8.0487348578367008,8.2000482161768993,8.3501539063238006,8.4978520144969991]
[null,null,null,null,"Coincident",6.5717846098274997,6.8438249735656003,7.0281549927136,7.2978927478867002,7.4522860924362,7.6058821702254003,7.7575251938987]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.1457648268331999,7.3735053156203003,7.6397128426364,8.0629790023064007,8.2145601455064998,8.3649314832581005,8.5128909782490005]
[null,null,null,null,"Coincident",6.5834149406881997,6.8559367443434001,7.0405929791599,7.3108080992383,7.4654746794136004,7.6193425818760003,7.7712539738300999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.6227831446079,6.8612840457909998,7.1013818741992996,7.4376424139477004,7.5743673865375998,7.7112792027656001,7.8407249263066996]
[null,null,null,null,"Coincident",6.1256197352403996,6.4324468515586997,6.5653455847230999,6.7403153019466,6.8785471734410004,7.0172209818919997,7.1493444106292001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.6345037294661999,6.8734267145360999,7.1139494529725003,7.4508050854643004,7.5877720253070002,7.7249261394520001,7.8546009478889998]
[null,null,null,null,"Coincident",6.1364604715817004,6.4438305912229001,6.5769645202023002,6.7522438878211002,6.8907203933831997,7.0296396180140004,7.1619968704812003]
[null,"Uley 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.27402503425861002,0.28717940680124998,0.30162593881129002,0.30436913206883998,0.30408648163737001,0.30397984346520002,0.30397020273007003]
[null,null,null,null,"Coincident",0.26714578208973,0.28717940680124998,0.30162593881129002,0.30436913206883998,0.30408648163737001,0.30397984346520002,0.30397020273007003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.27447576387025002,0.28765177336019998,0.30212206772384997,0.30486977311816998,0.30458665776961003,0.30447984419382002,0.30447018760115002]
[null,null,null,null,"Coincident",0.26758519637514,0.28765177336019998,0.30212206772384997,0.30486977311816998,0.30458665776961003,0.30447984419382002,0.30447018760115002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.24091141192814,0.25173159620041002,0.26383771108206,0.26485367192176001,0.26357766879066002,0.26219927264017001,0.26077796614715998]
[null,null,null,null,"Coincident",0.23419691681381,0.25173159620041002,0.26383771108206,0.26485367192176001,0.26357766879066002,0.26219927264017001,0.26077796614715998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.24130767465438999,0.25214565648837001,0.26427168409249002,0.26528931603366002,0.26401121407097,0.26263055066792002,0.26120690634133997]
[null,null,null,null,"Coincident",0.23458213521419,0.25214565648837001,0.26427168409249002,0.26528931603366002,0.26401121407097,0.26263055066792002,0.26120690634133997]
[null,"Uley South 11kV","Substation Rating","MVA","Non-Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,null,null,"Coincident",1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001,1.2350000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.61730213724673999,0.61644637830328997,0.61984242414204005,0.62733053682527995,0.62947679445177995,0.63284604511513998,0.63732127249842996]
[null,null,null,null,"Coincident",0.36624141887201001,0.39680025168511002,0.42006225590700003,0.42726680711722997,0.43030552514428999,0.43364464344316,0.43717789244843003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.63639391154724001,0.63551168589385998,0.63901276383399996,0.64673246709285004,0.64894510366689995,0.65241855771682,0.65703219387270995]
[null,null,null,null,"Coincident",0.37756844673519002,0.40907239589206001,0.43305384187120999,0.44048121373497001,0.44361391251347998,0.44705630227227,0.45069882676597001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.57715764118295998,0.57562800949740001,0.57815080698729004,0.58452577993654997,0.58724957326379001,0.59052485973647995,0.59451897960262001]
[null,null,null,null,"Coincident",0.34145214600044999,0.37142932795827999,0.39402873247622999,0.40041826811228998,0.4034588628038,0.40641754364396998,0.40938454688865999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.59500783601690999,0.59343089624486001,0.59603171821802003,0.60260385482082002,0.60541188898299003,0.60878847274000003,0.61290612179939996]
[null,null,null,null,"Coincident",0.35201249710329002,0.38291680624500002,0.40621515979348999,0.41280230947441998,0.41593694295841999,0.41898712917889003,0.42204589519723001]
[null,"Uraidla 11kV","Substation Rating","MVA","Non-Coincident",17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999]
[null,null,null,null,"Coincident",17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999,17.329838709676999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.3554141735516003,5.5300138101104999,5.7375180532297998,5.9749056963443996,6.1541138235456998,6.3357067302388996,6.5212645682573003]
[null,null,null,null,"Coincident",5.3554141735516003,5.5300138101104999,5.7375180532297998,5.9749056963443996,6.1541138235456998,6.3357067302388996,6.5212645682573003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.4321103445771,5.6092104644137999,5.8196864255745,6.0604737540703004,6.2422483638493,6.4264419061193996,6.6146571624473003]
[null,null,null,null,"Coincident",5.4321103445771,5.6092104644137999,5.8196864255745,6.0604737540703004,6.2422483638493,6.4264419061193996,6.6146571624473003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.6481661450607001,4.7875056744125004,4.9326465345342001,5.1000340209733004,5.2620266373940998,5.4205112139112996,5.5768802254896999]
[null,null,null,null,"Coincident",4.6481661450607001,4.7875056744125004,4.9326465345342001,5.1000340209733004,5.2620266373940998,5.4205112139112996,5.5768802254896999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7147336474169999,4.8560686915930003,5.0032881487887,5.1730728315737,5.3373853831125997,5.4981396552671002,5.6567480649699]
[null,null,null,null,"Coincident",4.7147336474169999,4.8560686915930003,5.0032881487887,5.1730728315737,5.3373853831125997,5.4981396552671002,5.6567480649699]
[null,"Uraidla 33kV","Substation Rating","MVA","Non-Coincident",31,31,31,31,31,31,31]
[null,null,null,null,"Coincident",31,31,31,31,31,31,31]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.264179931520999,17.659135589815001,18.160350204448999,18.744109275292999,19.134231713937002,19.522266777635,19.912149461959999]
[null,null,null,null,"Coincident",17.264179931520999,17.659135589815001,18.160350204448999,18.744109275292999,19.134231713937002,19.522266777635,19.912149461959999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.266840859337002,17.661857392140998,18.163149258977,18.746998304598002,19.137180872809001,19.525275744346001,19.915218521282998]
[null,null,null,null,"Coincident",17.266840859337002,17.661857392140998,18.163149258977,18.746998304598002,19.137180872809001,19.525275744346001,19.915218521282998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.763935686502,15.046661940163,15.338467064523,15.689009385691,16.057862780638999,16.452075484491001,16.833814255309001]
[null,null,null,null,"Coincident",14.763935686502,15.046661940163,15.338467064523,15.689009385691,16.012033137593001,16.313773625751001,16.598102357207999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.766211251707,15.048981081960999,15.340831182241001,15.691427532493,16.060337778809,16.45461124266,16.836408850868999]
[null,null,null,null,"Coincident",14.766211251707,15.048981081960999,15.340831182241001,15.691427532493,16.014501072041,16.316288067456,16.600660622496999]
[null,"Verdun 11kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1462938997072001,1.1767791147665001,1.2138208318457999,1.2566676445406,1.2867999052004,1.3170259883076001,1.3476811508962001]
[null,null,null,null,"Coincident",1.1462938997072001,1.1767791147665001,1.2138208318457999,1.2566676445406,1.2867999052004,1.3170259883076001,1.3476811508962001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1614924847024,1.1923818998819,1.2299147490222,1.2733296629035,1.3038614438999001,1.3344882913253,1.3655499073499]
[null,null,null,null,"Coincident",1.1614924847024,1.1923818998819,1.2299147490222,1.2733296629035,1.3038614438999001,1.3344882913253,1.3655499073499]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0219104403335,1.0503402866869,1.0799150305189,1.114219083933,1.1471963133265,1.1792653153245001,1.2107346686853999]
[null,null,null,null,"Coincident",1.0219104403335,1.0503402866869,1.0799150305189,1.114219083933,1.1471963133265,1.1792653153245001,1.2107346686853999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0354598386936,1.0642666332591999,1.0942335053734,1.1289923924664,1.1624068633247999,1.1949010647002001,1.2267876667632001]
[null,null,null,null,"Coincident",1.0354598386936,1.0642666332591999,1.0942335053734,1.1289923924664,1.1624068633247999,1.1949010647002001,1.2267876667632001]
[null,"Victor Harbor 11kV","Substation Rating","MVA","Non-Coincident",59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002]
[null,null,null,null,"Coincident",59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002,59.755485232067002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.048940405250001,24.496495355490001,25.348204456884002,26.265112300352001,26.762149672319001,27.240855223724999,27.713534716773001]
[null,null,null,null,"Coincident",23.801343465778999,24.413382758413,25.348204456884002,26.231239241548,26.565241758668002,26.886756741589,27.419693659370001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.059018098231999,24.506760596086,25.35882660563,26.276118678739,26.773364333896001,27.252270486554998,27.725148055639998]
[null,null,null,null,"Coincident",23.811317403423001,24.423613170728999,25.35882660563,26.242231425452001,26.576373906111002,26.898023619679002,27.431183864331999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.391173840756998,21.96671561498,22.929310233549,23.850763345807,24.242208917410998,24.608098015079001,25.187356784685001]
[null,null,null,null,"Coincident",21.391173840756998,21.96671561498,22.929310233549,23.850763345807,24.242208917410998,24.608098015079001,25.187356784685001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.400137798372999,21.975920753006001,22.938918746230001,23.860757992820002,24.252367599439001,24.618410022698001,25.197911530317999]
[null,null,null,null,"Coincident",21.400137798372999,21.975920753006001,22.938918746230001,23.860757992820002,24.252367599439001,24.618410022698001,25.197911530317999]
[null,"Virginia 11kV","Substation Rating","MVA","Non-Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,null,null,"Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.5350026417388003,7.8209424713787996,8.150129553787,8.6499959703575993,8.8608073322383003,9.0710301655847001,9.2783459372998003]
[null,null,null,null,"Coincident",7.1694444870152001,7.5101996683443,7.7570448677656003,8.1000061465309994,8.3166034537524993,8.5331879572096998,8.7475046006867991]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3019645187685995,8.6170091754253004,8.9797030732418008,9.5304491647569005,9.7627182865740991,9.9943389755714005,10.222756703181]
[null,null,null,null,"Coincident",7.8991974628885,8.2746369364343,8.5466076555781001,8.9244777775936992,9.1631217761310992,9.4017516676530999,9.6378828615657994]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.1496904407819004,7.5004448605210996,7.8587013862150998,8.3298982927910998,8.5827199035009993,8.8381146039168001,9.0861356920832002]
[null,null,null,null,"Coincident",6.8296166138082004,7.2620196251801996,7.5035209358291004,7.7962221317443996,8.0496107717243,8.3061150416573,8.5563552428689]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.8774327205615,8.2638892204365995,8.6586114397033995,9.1777698508868006,9.4563252995690998,9.7377157438653992,10.010982041406001]
[null,null,null,null,"Coincident",7.5247796849536996,8.0011955044165006,8.2672783988189007,8.5897726378558996,8.8689528317579001,9.1515657848178993,9.4272770712506997]
[null,"Waikerie 11kV","Substation Rating","MVA","Non-Coincident",12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001]
[null,null,null,null,"Coincident",12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001,12.229254793437001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7113023931921001,7.8212554025966998,8.0206412327005001,8.3420715091217001,8.4944451497838998,8.6462205321502008,8.7949937823071007]
[null,null,null,null,"Coincident",6.2553368578177002,6.3742384810496997,6.5281065469422996,6.7168231636437996,6.8360799357322,6.9547839977227,7.0710150162768004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.7868556560073996,7.8978859553682002,8.0992253141050998,8.423804877756,8.5776714342879004,8.7309338709504001,8.8811647613211004]
[null,null,null,null,"Coincident",6.3166249626694002,6.4366915519644001,6.5920671757024003,6.7826327869591996,6.9030580047632997,7.0229250971650004,7.1402949159171003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.0025204912856003,7.0995591608769999,7.2783083204584997,7.5718655300485,7.7303511295560003,7.8823928342684999,8.0295101304126]
[null,null,null,null,"Coincident",5.7034260787143998,5.8058488395188999,5.9482092936206001,6.1271885876632997,6.2521605335467001,6.3718463389234001,6.4874806974890999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.0711293000277999,7.1691187283540003,7.3496192240319997,7.646052628054,7.8060910267569996,7.9596223951202996,8.1081811068870007]
[null,null,null,null,"Coincident",5.7593067104808,5.8627329818948999,6.0064882453627,6.1872211302973001,6.3134175176290999,6.4342759722740999,6.5510432851239999]
[null,"Walker Flat 11kV","Substation Rating","MVA","Non-Coincident",2.85,2.85,2.85,2.85,2.85,2.85,2.85]
[null,null,null,null,"Coincident",2.85,2.85,2.85,2.85,2.85,2.85,2.85]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.456374085392,1.4731690289566,1.5089133066447,1.5695759998803001,1.5950513298897,1.6202308270693999,1.6445627469074999]
[null,null,null,null,"Coincident",1.2193887736133999,1.2405643875259,1.2685067739445,1.3030859873419001,1.3240782074196,1.3448225005422001,1.3648374697587999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.520243069965,1.5377745523091,1.575086387909,1.6384094310213,1.6650019763641,1.6912857151895999,1.7166847063443]
[null,null,null,null,"Coincident",1.2728648163084,1.2949690823933,1.3241368763943999,1.3602325540499001,1.3821453836013,1.4037994134123,1.4246921349681001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3027255607871999,1.3149202324435001,1.3434090185354,1.3941085742263,1.417918532154,1.4409528617086,1.4627850735562999]
[null,null,null,null,"Coincident",1.0601810924665001,1.0754622049342,1.0981054397343,1.1273647799679001,1.1465733348788001,1.1651470256262,1.1827027155456]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3598563210632,1.3725857875251,1.4023239434442001,1.4552469176734999,1.480101056386,1.5041455517035001,1.5269352106905001]
[null,null,null,null,"Coincident",1.1066751152031,1.1226263777004,1.1462626268838001,1.1768051294371999,1.1968560715545,1.2162443076716001,1.2345698987447]
[null,"Wallaroo 11kV","Substation Rating","MVA","Non-Coincident",17.8125,17.8125,17.8125,17.8125,17.8125,17.8125,17.8125]
[null,null,null,null,"Coincident",17.8125,17.8125,17.8125,17.8125,17.8125,17.8125,17.8125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.2660968841893006,9.4605491327127993,9.6445103313259999,9.8684411865573001,9.8867226217147,9.9026978905337995,9.9139658602794007]
[null,null,null,null,"Coincident",9.2610867646054995,9.4605491327127993,9.6445103313259999,9.8684411865573001,9.8867226217147,9.9026978905337995,9.9139658602794007]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.4099715697379001,9.6074430783080995,9.7942606424368002,10.021668472039,10.040233763038,10.056457079855001,10.067900007365999]
[null,null,null,null,"Coincident",9.4048836580277992,9.6074430783080995,9.7942606424368002,10.021668472039,10.040233763038,10.056457079855001,10.067900007365999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.3294469679188001,8.5053941612995008,8.6709444529485005,8.8821083413841997,8.9142600904615996,8.9353882858722997,8.9496249409765998]
[null,null,null,null,"Coincident",8.3294469679188001,8.5053941612995008,8.6709444529485005,8.8821083413841997,8.9142600904615996,8.9353882858722997,8.9496249409765998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.4587782902955002,8.6374574157332002,8.8055782067468993,9.0200208368607004,9.0526718061433993,9.0741280590425006,9.0885857666894001]
[null,null,null,null,"Coincident",8.4587782902955002,8.6374574157332002,8.8055782067468993,9.0200208368607004,9.0526718061433993,9.0741280590425006,9.0885857666894001]
[null,"Warooka 11kV","Substation Rating","MVA","Non-Coincident",6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996]
[null,null,null,null,"Coincident",6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996,6.4423076923076996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1554016999130998,2.1932298486829001,2.2588702982506002,2.3621854633917998,2.4149255150068001,2.4676846683461999,2.5205649545526998]
[null,null,null,null,"Coincident",2.1104572818917999,2.1601380158681001,2.2224429369525001,2.2975021559563999,2.3492215826656002,2.4007924867504999,2.4524297671430002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1868550120129999,2.2252351787985001,2.2918335052884999,2.3966563263501999,2.4501660021627001,2.5036950584470001,2.5573470152640998]
[null,null,null,null,"Coincident",2.1412547297938,2.1916604440051999,2.2548745673642001,2.3310291093612001,2.3835032665088001,2.4358267336733999,2.4882175457609002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8872972423984,1.9142240353094999,1.9643533739447001,2.0471471623491002,2.0926915440667999,2.1367225584910998,2.1804030224066002]
[null,null,null,null,"Coincident",1.7471841951510001,1.7806783304842,1.8270728271033001,1.8854467895545,1.9275946574128999,1.968270872845,2.0086562988373]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.9148381639784,1.9421578937705,1.9930187590318,2.0770207393322,2.1232297403886,2.1679032899093,2.2122211734130999]
[null,null,null,null,"Coincident",1.7726804772539999,1.8066633852795999,1.8537349067808,1.9129607078752,1.9557236304782,1.9969934251485,2.0379681869514998]
[null,"Wasleys 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8819793351745,1.9259943491553,1.9808103509887001,2.0466037800778998,2.0915960026768001,2.1367069076697001,2.1814812425526999]
[null,null,null,null,"Coincident",1.8819793351745,1.9259943491553,1.9808103509887001,2.0466037800778998,2.0915960026768001,2.1367069076697001,2.1814812425526999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8852331211090001,1.9293242333926,1.9842350075396,2.0501421880022002,2.0952121984165002,2.1404010964167002,2.1852528424052999]
[null,null,null,null,"Coincident",1.8852331211090001,1.9293242333926,1.9842350075396,2.0501421880022002,2.0952121984165002,2.1404010964167002,2.1852528424052999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6914223108648001,1.7325255072134,1.7765135784543,1.8369668568980999,1.8816060937253001,1.9249785903193,1.9675525949954999]
[null,null,null,null,"Coincident",1.6914223108648001,1.7325255072134,1.7765135784543,1.8369668568980999,1.8816060937253001,1.9249785903193,1.9675525949954999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6943466395338,1.7355208998944001,1.7795850228565,1.8401428199968,1.8848592343563,1.9283067183939999,1.9709543299876]
[null,null,null,null,"Coincident",1.6943466395338,1.7355208998944001,1.7795850228565,1.8401428199968,1.8848592343563,1.9283067183939999,1.9709543299876]
[null,"Waterloo Town 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.30141330403257999,0.30675402326520002,0.31741566463446003,0.33482808969874001,0.34313687180208002,0.35156414312694001,0.36001561641189]
[null,null,null,null,"Coincident",0.28176444385434002,0.28932366959991002,0.29862253129268002,0.30969943646423997,0.31775273750006,0.32594020847204003,0.33417110920854998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.30155366517602999,0.30689687145699002,0.31756347770388998,0.33498401132826999,0.34329666263759001,0.35172785834608,0.36018326728497002]
[null,null,null,null,"Coincident",0.28189565498203001,0.28945840088266001,0.29876159283837,0.30984365626623001,0.31790070753645999,0.32609199122264998,0.33432672489760001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.27220471470635998,0.27673056847658001,0.28613240889653002,0.30184354002066999,0.31001122701666001,0.31806579561613002,0.32606377576068002]
[null,null,null,null,"Coincident",0.25421901482244003,0.26065225628902999,0.26902294242725999,0.27922467271354001,0.28714267663423998,0.29498181719326,0.30279055286168999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.27233147409121999,0.27685943544594999,0.28626565408362997,0.30198410151498001,0.31015559201225001,0.31821391143638,0.32621561605368998]
[null,null,null,null,"Coincident",0.25433739868649002,0.26077363596352998,0.269148220135,0.27935470112906002,0.28727639227945001,0.29511918334333997,0.30293155535778998]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Whitmore Square 11kV","Substation Rating","MVA","Non-Coincident",79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001]
[null,null,null,null,"Coincident",79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001,79.217232138789001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.668983409768998,43.700939270768998,43.629143822812999,43.462640235658,43.193897667027997,42.814264148489002,42.340464125254002]
[null,null,null,null,"Coincident",43.668983409768998,43.700939270768998,43.629143822812999,43.462640235658,43.193897667027997,42.814264148489002,42.340464125254002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.678354907005001,44.711049400617,44.637594461802003,44.467242285512,44.192287960442997,43.803879535252001,43.319128026512999]
[null,null,null,null,"Coincident",44.678354907005001,44.711049400617,44.637594461802003,44.467242285512,44.192287960442997,43.803879535252001,43.319128026512999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.039187180192002,40.006979603894997,39.853237310701999,39.600763928486003,39.306586890368003,38.921231146296002,38.473827892088003]
[null,null,null,null,"Coincident",39.950689356769999,39.904998521414001,39.778916882192,39.574723129219997,39.282093586854003,38.89846646222,38.452890539304001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.964659017559001,40.931706990465003,40.774411074619003,40.516101984404003,40.215125293665999,39.820862378554999,39.363117777759001]
[null,null,null,null,"Coincident",40.874115642040998,40.827368701795997,40.698372792466998,40.489459274158001,40.190065848224997,39.797571508121997,39.341696475831]
[null,"Whyalla City 11kV","Substation Rating","MVA","Non-Coincident",25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001]
[null,null,null,null,"Coincident",25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001,25.129312762973001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.645377079058999,19.828068887766999,20.306253564355,21.171542922029001,21.529066503551,21.895752222799999,22.269249265609002]
[null,null,null,null,"Coincident",14.470588409739999,14.704222393638,15.026058163461,15.436541030667,15.695437869824,15.960997166413,16.231677620904001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.068474228837001,20.255100621402999,20.743583831479999,21.627508691007002,21.992732160788002,22.367315090767999,22.748856037932999]
[null,null,null,null,"Coincident",14.782237541601001,15.020903237146999,15.349670296523,15.768993621738,16.033466251794,16.304744826819,16.581254852733]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.481171323718002,17.607647793942999,18.001764754020002,18.752592684195001,19.089430391354998,19.415719248272001,19.742883292990999]
[null,null,null,null,"Coincident",12.964507821788001,13.139628424965,13.411519695761999,13.772792106863999,14.017885388814999,14.255653749439,14.494071609891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.857658562017999,17.986858921625998,18.389463871616002,19.156462178971999,19.500554268335001,19.833870319730998,20.168080407611999]
[null,null,null,null,"Coincident",13.243720905130999,13.422613033169,13.700359952411,14.069412989296,14.319784778683999,14.562673891905,14.806226493055]
[null,"Whyalla North 11kV","Substation Rating","MVA","Non-Coincident",3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998]
[null,null,null,null,"Coincident",3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998,3.7953431372548998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.38042087742457997,0.38566962149612999,0.39674569711608998,0.41550659175396998,0.4244160857184,0.43357567292694998,0.44289848063126003]
[null,null,null,null,"Coincident",0.33548743299964001,0.34242318858486998,0.35149048901282998,0.36271163933227002,0.37044707021862999,0.37840001885947,0.38649876846928]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.40290681121317001,0.40846579827786,0.42019655905788,0.44006637347298,0.44950249019464,0.45920348268277,0.46907734331083001]
[null,null,null,null,"Coincident",0.35531743879848998,0.36266315332687998,0.37226640414338003,0.38415081470453,0.39234347177658002,0.40076650365199001,0.40934395450640998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.36512040890925002,0.36979881175480001,0.38018929215851999,0.39825886130597998,0.40767880895389003,0.41696559710747999,0.42631630774221002]
[null,null,null,null,"Coincident",0.32419604021537002,0.33039490756061002,0.33911646981643001,0.35019683045042999,0.35842126195189999,0.36653881431238,0.37471222503238]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.38670196193855999,0.39165689602323001,0.40266153739512001,0.42179916342259999,0.43177590574628999,0.44161161777845998,0.45151503062456999]
[null,null,null,null,"Coincident",0.34335863387783999,0.34992390414405,0.35916098088148002,0.37089627995433999,0.37960684151113999,0.38820420651003001,0.39686073154677998]
[null,"Whyalla Stuart 11kV","Substation Rating","MVA","Non-Coincident",29.312673267327,29.312673267327,29.312673267327,29.312673267327,29.312673267327,29.312673267327,29.312673267327]
[null,null,null,null,"Coincident",29.312673267327,29.312673267327,29.312673267327,29.312673267327,29.312673267327,29.312673267327,29.312673267327]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.681566463932,17.883700112934999,18.353176761425999,19.176788132304001,19.544367233142001,19.923378894441001,20.316425354835001]
[null,null,null,null,"Coincident",11.335297905556001,11.542646649086,11.819875084326,12.169135621658,12.400986362886,12.640071299374,12.888177471121001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.877746458829002,18.082122815135001,18.556808387094001,19.389557866570001,19.761215320209001,20.144432180517999,20.54183955841]
[null,null,null,null,"Coincident",11.461064968662001,11.670714281857,11.951018613858,12.304154256405999,12.538577421140999,12.780315045767001,13.031173997795999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.691439060112,15.826599308832,16.202437854425,16.902336078573001,17.243985941159998,17.598411421702998,17.955914202152002]
[null,null,null,null,"Coincident",10.128255727032,10.279115064289,10.505812675269,10.804229058782999,11.020811494044001,11.245881431111,11.472913646305001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.865538252116,16.002198126842998,16.382206665184999,17.089870379474,17.435310905542998,17.793668797226999,18.155138131985002]
[null,null,null,null,"Coincident",10.240630451347,10.393163598675001,10.622376458304,10.924103822477999,11.143089276789,11.370656403185,11.600207579519999]
[null,"Williamstown 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.78164302727694002,0.78863181933528004,0.80581118265605001,0.83587503109134997,0.84867161012543002,0.86140824083824996,0.87385764440985003]
[null,null,null,null,"Coincident",0.72415828188557996,0.73384651877593998,0.74962285115800997,0.76936387606922996,0.78112953884908998,0.79283886491355005,0.80427997584185995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.82278228375147,0.83013890830993997,0.84822245193944001,0.87986861394785998,0.89333869959365997,0.90674568173192005,0.91985031945594997]
[null,null,null,null,"Coincident",0.76227201442974002,0.77247016038129002,0.78907682906962995,0.80985685907466998,0.82224176951849004,0.83456737814584003,0.84661065499953003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.71093508791573001,0.71602196743812996,0.73035292346840996,0.75664875487897998,0.76938850114474,0.78147550751557004,0.79306631087809998]
[null,null,null,null,"Coincident",0.65425850239879002,0.66136233500581998,0.67507188197707002,0.69288806702602002,0.70456398621912997,0.71564178811435997,0.72626204722934995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74835286034875004,0.75370747134705995,0.76879269096709002,0.79647251854324996,0.80988278021150995,0.82260594712845003,0.83480679499420996]
[null,null,null,null,"Coincident",0.68869328578653999,0.69617100568145995,0.71060211038344001,0.72935599279621,0.74164643628941995,0.75330728251235002,0.76448650466840995]
[null,"Williamstown South 11kV","Substation Rating","MVA","Non-Coincident",4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004]
[null,null,null,null,"Coincident",4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004,4.9400000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5448810053596,2.5509627827830998,2.5894337257728002,2.6684167027580998,2.6914616268475,2.7138797790098002,2.7353313649677999]
[null,null,null,null,"Coincident",2.4138893115562001,2.4303000330233,2.4662616780855,2.5146000322363999,2.536275385238,2.5573569006274002,2.5775158200955999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5572408458974998,2.5633521609689001,2.6020099475555001,2.6813765247951,2.7045333722264,2.7270604036587001,2.74861617452]
[null,null,null,null,"Coincident",2.4256129587145998,2.4421033828868999,2.4782396845234,2.5268128057805002,2.5485934304651998,2.5697773334192,2.5900341596380998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1980168504939002,2.1903027838782001,2.2101677640365001,2.2650171443228002,2.2780997410668,2.2885399583792001,2.2972216632203]
[null,null,null,null,"Coincident",2.0709769786267,2.0712956552139001,2.0915454923126,2.1235626661431,2.1358576841968002,2.1456735536716001,2.1538307781025998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2086920599495001,2.200940528072,2.2209019873922999,2.2760177571846998,2.2891638927775002,2.2996548155732,2.3083786852491999]
[null,null,null,null,"Coincident",2.0810351876981001,2.0813554120164999,2.1017035974296001,2.1338762705396999,2.1462310023727,2.1560945450319,2.1642913870296998]
[null,"Willunga 11kV","Substation Rating","MVA","Non-Coincident",6.9,6.9,6.9,6.9,6.9,6.9,6.9]
[null,null,null,null,"Coincident",6.9,6.9,6.9,6.9,6.9,6.9,6.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9847391657597004,5.0930084756467,5.2555963942005999,5.3929381792628996,5.4030239036073002,5.3968919947396996,5.4187714346772999]
[null,null,null,null,"Coincident",4.9847391657597004,5.0930084756467,5.2555963942005999,5.3929381792628996,5.4030239036073002,5.3968919947396996,5.4187714346772999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1028786156591002,5.2137139327705002,5.3801552219059996,5.5207520384544999,5.5310767967555998,5.5247995602557998,5.5471975478870998]
[null,null,null,null,"Coincident",5.1028786156591002,5.2137139327705002,5.3801552219059996,5.5207520384544999,5.5310767967555998,5.5247995602557998,5.5471975478870998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.5654288538751997,4.6666299279606998,4.8379161237829003,4.9867810088412003,5.0112664205156996,5.0176722921421,5.0540128405589]
[null,null,null,null,"Coincident",4.5654288538751997,4.6666299279606998,4.8379161237829003,4.9867810088412003,5.0112664205156996,5.0176722921421,5.0540128405589]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.6736305541881,4.7772301167047999,4.9525758342546,5.1049688508852,5.1300345723751999,5.1365922646135003,5.1737940922780998]
[null,null,null,null,"Coincident",4.6736305541881,4.7772301167047999,4.9525758342546,5.1049688508852,5.1300345723751999,5.1365922646135003,5.1737940922780998]
[null,"Willunga 33kV","Substation Rating","MVA","Non-Coincident",9.75,9.75,9.75,9.75,9.75,9.75,9.75]
[null,null,null,null,"Coincident",9.75,9.75,9.75,9.75,9.75,9.75,9.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Wilmington 11kV","Substation Rating","MVA","Non-Coincident",2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999]
[null,null,null,null,"Coincident",2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999,2.5649999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.76071717275419004,0.76460641164948995,0.77966060861668995,0.80859855551866999,0.81654037862203999,0.82406318581391003,0.83102237327230999]
[null,null,null,null,"Coincident",0.69503298798584001,0.70371196410035997,0.71593091421531996,0.73150386716462001,0.73895987377979999,0.74603991531257996,0.75261145557104003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.76173193198682998,0.76562635893522002,0.78070063745954998,0.80967718615710005,0.81762960326124001,0.82516244550730999,0.83213091617893997]
[null,null,null,null,"Coincident",0.69596012775186,0.70465068119295005,0.71688593078540996,0.73247965728676001,0.73994560984746005,0.74703509580685001,0.75361540217627998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.68583647203399001,0.68708815720076,0.69741016705412995,0.71963255827165995,0.72602981464628003,0.73139779998278998,0.73620327416898002]
[null,null,null,null,"Coincident",0.62205460114123001,0.62701260561549998,0.63568260974486002,0.64783107153248998,0.65383697892727,0.65891729014147005,0.66349042975538997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.68675134410077998,0.68800469895390004,0.69834047785991005,0.72059251265255997,0.72699830265204002,0.73237344861653997,0.73718533306856004]
[null,null,null,null,"Coincident",0.62288439133439,0.62784900954237999,0.63653057903012,0.64869524626730002,0.65470916524667999,0.65979625334575998,0.66437549330263002]
[null,"Wirrabara Forest 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.33015653010354001,0.31966274335393002,0.31553826340474,0.31870724119194999,0.31563663395563002,0.31484823498049003,0.31646777808977]
[null,null,null,null,"Coincident",0.29081292811914,0.28363553607253,0.27933745660381998,0.27796314475544998,0.27538622586167999,0.27479854852657998,0.27631166913550997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.34682437181491999,0.33580080976012999,0.33146810682375,0.33479706939190002,0.33157144357891999,0.33074324254589998,0.33244454774596]
[null,null,null,null,"Coincident",0.30549452127738003,0.29795478100007,0.29343971443064998,0.29199602090947002,0.28928900712945999,0.28867166110115999,0.29026117109664001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.29562956473317997,0.28395566595687,0.27776110715648,0.27804579161524001,0.27430242168237001,0.27266111860075998,0.27350122047316]
[null,null,null,null,"Coincident",0.25850408730044,0.24981928910976001,0.24408163913617001,0.24131199856328001,0.23815312563786001,0.23681656986616001,0.23763357807381]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.31055432417571999,0.29829107253428,0.29178378351006001,0.29208284016826003,0.28815048745958999,0.28642632374228,0.28730883787599998]
[null,null,null,null,"Coincident",0.27155457946402001,0.26243133214893999,0.25640401884043001,0.25349455389196002,0.25017620632616,0.24877217498449999,0.24963042957754999]
[null,"Wirrabara South 11kV","Substation Rating","MVA","Non-Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.4912499746844999E-2,5.663410085817E-2,5.9413416692064999E-2,6.3551744611792998E-2,6.6340896516075998E-2,6.9354684588023005E-2,7.2585055012772001E-2]
[null,null,null,null,"Coincident",5.1818242116879E-2,5.3834944946994E-2,5.6348105041937997E-2,5.9380029172554999E-2,6.2008866252171002E-2,6.4849497669875994E-2,6.7894498173077994E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.5170342654555997E-2,5.6900027583564002E-2,5.9692393758989999E-2,6.3850153292810005E-2,6.6652401724119001E-2,6.9680341107395002E-2,7.2925879810899E-2]
[null,null,null,null,"Coincident",5.2061555866599003E-2,5.4087728171315998E-2,5.6612688867388003E-2,5.9658849467612997E-2,6.2300030312303002E-2,6.5153999980276003E-2,6.8213298353497001E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.0406055809804E-2,5.1976129874311001E-2,5.4416302954813998E-2,5.8027786339248003E-2,6.0605510040143001E-2,6.3300200117218999E-2,6.6148523137166002E-2]
[null,null,null,null,"Coincident",4.7219339746044003E-2,4.8988823778261997E-2,5.1228348220172998E-2,5.3953079431350998E-2,5.6371085573816003E-2,5.8899499066454003E-2,6.1572435843437003E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0642738606182999E-2,5.2220184989633003E-2,5.4671815959056E-2,5.8300257146927999E-2,6.0890084608849003E-2,6.3597427665265993E-2,6.6459125051577E-2]
[null,null,null,null,"Coincident",4.7441059243725998E-2,4.9218851928984002E-2,5.1468892109509001E-2,5.4206417358865999E-2,5.6635777304882999E-2,5.9176063021328003E-2,6.1861550634529999E-2]
[null,"Wirrina Cove 11kV","Substation Rating","MVA","Non-Coincident",1.95,1.95,1.95,1.95,1.95,1.95,1.95]
[null,null,null,null,"Coincident",1.95,1.95,1.95,1.95,1.95,1.95,1.95]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.68998868395607005,0.70535070462906002,0.73103099889100998,0.75622069957604998,0.76663209888493999,0.77772367210008997,0.79591407208112996]
[null,null,null,null,"Coincident",0.68998868395607005,0.70535070462906002,0.73103099889100998,0.75622069957604998,0.76663209888493999,0.77772367210008997,0.79591407208112996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.69385333837508001,0.70930140234480998,0.73512553296959005,0.76045632218308001,0.77092603615898003,0.78207973372259998,0.80037201886683995]
[null,null,null,null,"Coincident",0.69385333837508001,0.70930140234480998,0.73512553296959005,0.76045632218308001,0.77092603615898003,0.78207973372259998,0.80037201886683995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.64467340304220999,0.66072499225891002,0.68915657469899005,0.71702232211058003,0.72959423011127,0.74197314220064003,0.76125345521659005]
[null,null,null,null,"Coincident",0.64467340304220999,0.66072499225891002,0.68915657469899005,0.71702232211058003,0.72959423011127,0.74197314220064003,0.76125345521659005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.64828424474702995,0.66442573956165996,0.69301656844051995,0.72103839302608996,0.73368071679003,0.74612896366477,0.76551726649074003]
[null,null,null,null,"Coincident",0.64828424474702995,0.66442573956165996,0.69301656844051995,0.72103839302608996,0.73368071679003,0.74612896366477,0.76551726649074003]
[null,"Wongyarra 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.10804403450886001,0.109867875832,0.1133518925798,0.11895650418644001,0.12156446020491,0.12416693065524,0.12674457049157001]
[null,null,null,null,"Coincident",0.10195587462373,0.10443762604567999,0.10750373746208999,0.11114786434274,0.11362635643667,0.11610121404248,0.11855414324853999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10855141536896,0.11038382155349,0.11388419943979999,0.11951513061761999,0.12213533374417,0.12475002554205,0.12733977011995001]
[null,null,null,null,"Coincident",0.10243466514273999,0.10492807100889,0.10800858105687999,0.11166982096222999,0.11415995219437,0.11664643187062999,0.11911088017014]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.8003034937570996E-2,9.9452476449321994E-2,0.10226149412011,0.10690526335470001,0.10928257595999,0.11155865411332,0.11380429838598]
[null,null,null,null,"Coincident",9.18071951577E-2,9.3736487400451998E-2,9.627055029171E-2,9.9398383589629005E-2,0.10164715117631,0.10380297110648,0.10593143321655001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.8463262699197002E-2,9.9919510869771994E-2,0.10274171984546,0.10740729648144,0.10979577308037,0.11208253982466999,0.11433872976907]
[null,null,null,null,"Coincident",9.2238326907399998E-2,9.4176679214986E-2,9.6722642208041998E-2,9.9865163986968999E-2,0.10212449191266,0.10429043569441999,0.10642889318220999]
[null,"Woodforde 11kV","Substation Rating","MVA","Non-Coincident",47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999]
[null,null,null,null,"Coincident",47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999,47.682843137254999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.868598036502,38.805038211206998,39.96676749681,41.850245455843996,42.810595675511998,43.785342533048002,44.79122312917]
[null,null,null,null,"Coincident",37.868598036502,38.805038211206998,39.96676749681,41.367656781496997,42.360579611520002,43.370488816726002,44.413359510653002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.682099746780999,39.638656739197003,40.825342553685999,42.749281808368004,43.730262486691998,44.725949074686,45.753438223214999]
[null,null,null,null,"Coincident",38.682099746780999,39.638656739197003,40.825342553685999,42.256326055959001,43.270579076753997,44.302183377852003,45.367457253757998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.665656428030001,32.359774879094999,33.135805546039002,34.498110175233002,35.235174171520001,36.057250904885002,36.882467411828003]
[null,null,null,null,"Coincident",31.665656428030001,32.359774879094999,33.135805546039002,34.197893289166998,34.979173068413999,35.848421994882997,36.724111030404998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.345905156449,33.054934815647002,33.847636347306,35.239206309869999,35.992104080117997,36.831840850116002,37.674784843013001]
[null,null,null,null,"Coincident",32.345905156449,33.054934815647002,33.847636347306,34.932540097371003,35.730603503939001,36.618525830666002,37.513026614311997]
[null,"Woodside 11kV","Substation Rating","MVA","Non-Coincident",13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999]
[null,null,null,null,"Coincident",13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999,13.384720638540999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9731781683047007,9.2300111271378,9.5394634736355997,9.8959038004127997,10.153491385619001,10.412897297545999,10.676694220021]
[null,null,null,null,"Coincident",8.9731781683047007,9.2300111271378,9.5394634736355997,9.8959038004127997,10.153491385619001,10.412897297545999,10.676694220021]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.3429778660756995,9.6103953412052991,9.9326007370757008,10.303730566574,10.571933767493,10.842030231421001,11.116698666795999]
[null,null,null,null,"Coincident",9.3429778660756995,9.6103953412052991,9.9326007370757008,10.303730566574,10.571933767493,10.842030231421001,11.116698666795999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.9293683664880996,8.1487871143866002,8.3770280378302999,8.6418649293847007,8.8963190051040009,9.1436381308908992,9.3861671480674005]
[null,null,null,null,"Coincident",7.9293683664880996,8.1487871143866002,8.3770280378302999,8.6418649293847007,8.8963190051040009,9.1436381308908992,9.3861671480674005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.2561509144821006,8.4846122763949001,8.7222593904798007,8.9980106538006002,9.2629512080598992,9.5204627691528003,9.7729868132384006]
[null,null,null,null,"Coincident",8.2561509144821006,8.4846122763949001,8.7222593904798007,8.9980106538006002,9.2629512080598992,9.5204627691528003,9.7729868132384006]
[null,"Woods Point 11kV","Substation Rating","MVA","Non-Coincident",8.9,8.9,8.9,8.9,8.9,8.9,8.9]
[null,null,null,null,"Coincident",8.9,8.9,8.9,8.9,8.9,8.9,8.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5039343365651998,2.5555499234483001,2.6400475213446999,2.7693634221911001,2.8369481590360999,2.9058005493004,2.9751865737613001]
[null,null,null,null,"Coincident",2.0030752402192999,2.0538745043186002,2.1166563478630001,2.1918820272344002,2.2456480728119002,2.3004036457121,2.3555595241374001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5650513985351999,2.6179268399505,2.7044868900651,2.8369591867524,2.9061935597279001,2.9767265275300998,3.0478061546926001]
[null,null,null,null,"Coincident",2.0519671267991999,2.1040063202875001,2.1683205689618998,2.2453823877403001,2.3004607771327001,2.3565528466386998,2.4130549924923002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3493887981560002,2.4144881900398998,2.5110439797158,2.6517590031754001,2.7227277884372998,2.7930552998531,2.8633196824240001]
[null,null,null,null,"Coincident",2.1028405427951,2.1527952489460001,2.2185466744164999,2.2992598166728002,2.3611336353782,2.4224378399687998,2.4836663259009]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4067336488861999,2.4734220135757998,2.5723345767880001,2.7164842305744998,2.7891852512163,2.8612293455355,2.9332087701348999]
[null,null,null,null,"Coincident",2.1541675420258999,2.2053415632470998,2.2726978766279,2.3553810985485,2.4187651589391002,2.4815657018386998,2.5442886779074998]
[null,"Woodville 11kV","Substation Rating","MVA","Non-Coincident",27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001]
[null,null,null,null,"Coincident",27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001,27.265000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.196635686184001,11.396344582351,11.659158338737999,12.162771845042,12.363166013148,12.592375638556,12.815239504858001]
[null,null,null,null,"Coincident",11.196635686184001,11.396344582351,11.641535655478,11.962067335295,12.144609176422,12.360148201451,12.568941736899999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.738352124784999,11.947723351229,12.223252581809,12.751231953245,12.961321606505001,13.201620868609,13.435267350627999]
[null,null,null,null,"Coincident",11.738352124784999,11.947723351229,12.204777276612001,12.540816943374001,12.732190537077001,12.958157786824,13.177053186225001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.8237251383875002,9.9064423529913999,9.9770347633960998,10.185738549285,10.269423931435,10.376031071746,10.469954463961001]
[null,null,null,null,"Coincident",9.8237251383875002,9.9064423529913999,9.9770347633960998,10.111503079117,10.182019798892,10.27941339643,10.364470027769]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.299017319441999,10.385736564313,10.459744381829999,10.678545689401,10.766279943772,10.878044958465001,10.976512559044]
[null,null,null,null,"Coincident",10.299017319441999,10.385736564313,10.459744381829999,10.60071855334,10.674647018158,10.776752719784,10.865924567221001]
[null,"Woodville 33kV","Substation Rating","MVA","Non-Coincident",33.9,33.9,33.9,33.9,33.9,33.9,33.9]
[null,null,null,null,"Coincident",33.9,33.9,33.9,33.9,33.9,33.9,33.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Woolpunda 11kV","Substation Rating","MVA","Non-Coincident",19.018235294118,19.018235294118,19.018235294118,19.018235294118,19.018235294118,19.018235294118,19.018235294118]
[null,null,null,null,"Coincident",19.018235294118,19.018235294118,19.018235294118,19.018235294118,19.018235294118,19.018235294118,19.018235294118]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.2374475387511996,8.4281761018061996,8.6052565950420998,8.8515693365757002,8.9449279246126991,9.0329404768299995,9.1133759228432005]
[null,null,null,null,"Coincident",7.3193822805197,7.5946624596595997,7.7297746210621003,7.9008276002233,7.9852050142972004,8.0646688802225999,8.1372477732403006]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.6501651626362008,8.8504497245585991,9.0364024127384006,9.2950560655726004,9.3930921625638994,9.4855143733863994,9.5699798452052995]
[null,null,null,null,"Coincident",7.6861024385433003,7.9751748732214001,8.1170565065930997,8.2966796865096004,8.3852846292788001,8.4687298423115003,8.5449451273217996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.7462683847845,7.9303748946872998,8.1001041617826992,8.3411882785103,8.4516474924262006,8.5501882842564001,8.6386805491003003]
[null,null,null,null,"Coincident",6.8985855849524,7.1653719039258004,7.2962715937261997,7.4668188583005,7.5665040062294002,7.6553639745834001,7.7350915604591997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.1343766509316993,8.3277073775534998,8.5059405239742993,8.7591035842514007,8.8750970931158992,8.9785750358377001,9.0715009941414007]
[null,null,null,null,"Coincident",7.2442227301231998,7.5243757400689999,7.6618338460156004,7.8409259737242003,7.9456056077724,8.0389176924918999,8.1226398385328995]
[null,"Wudinna 11kV","Substation Rating","MVA","Non-Coincident",5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997]
[null,null,null,null,"Coincident",5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997,5.4556390010228997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9148060927332,1.8974524713383001,1.8994711316924999,1.9270441378059,1.9152878583927999,1.9023951320279,1.8878887582448001]
[null,null,null,null,"Coincident",1.7620085059274999,1.7549840811773001,1.7563833687562,1.7655489407206999,1.7550952231187,1.7435925568670001,1.7305873306469]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.939491919023,1.9219145734167,1.9239592584942,1.9518877379068,1.9399798956423,1.926920955265,1.9122275642040001]
[null,null,null,null,"Coincident",1.7847244540663001,1.7776094698961999,1.7790267971974001,1.7883105324151001,1.7777220446879001,1.7660710851849999,1.752898194596]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7533896152262001,1.7389921173902001,1.7429810884143999,1.7719292938824001,1.7686112749353,1.7628600881101,1.755107513265]
[null,null,null,null,"Coincident",1.5945909637911,1.5887366175613,1.5928897723069,1.6054969181414001,1.6027352120375999,1.5977633884322,1.5909560654153001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7759944479683001,1.7614113364913999,1.7654517336344,1.7947731415767001,1.7914123464762,1.7855870149115001,1.7777344932798]
[null,null,null,null,"Coincident",1.6151485521991,1.6092187312909001,1.6134254288244001,1.6261951069452001,1.6233977967155999,1.6183618759808001,1.611466792436]
[null,"Yankalilla 11kV","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.4385563336939002,7.5494889356736001,7.7497227708584999,8.0355274118573004,8.1574396776744003,8.2726156000966995,8.3847296959103996]
[null,null,null,null,"Coincident",6.4973029349214002,6.6401897812498003,6.8693401761126998,7.0826024897612996,7.1463713964949003,7.2060862988974002,7.3214765892241003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.5530517174774996,7.6656918108395997,7.8690076754906002,8.1592114647369005,8.2830002225821993,8.3999489502167997,8.5137887231448008]
[null,null,null,null,"Coincident",6.5973104040752997,6.7423965863467004,6.9750740987343001,7.1916189781595001,7.2563694255472004,7.3170034687563001,7.4341698638785996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.6460982482321,6.7653483756939004,6.9774399762166999,7.2783525099843001,7.4423690173586996,7.5969952377598,7.7461563848040997]
[null,null,null,null,"Coincident",5.9383332020867998,6.0874736651420998,6.3431830930027999,6.5865887348304,6.6829909793070996,6.7719767354289999,6.9190853976806004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.7483959973461003,6.8694816408000996,7.0848377873060997,7.3903820122908002,7.5569230865456998,7.7139293371104003,7.8653863950828002]
[null,null,null,null,"Coincident",6.0297369245977999,6.1811729802102002,6.4408183262473004,6.6879705045164002,6.7858565869158998,6.8762120252505001,7.0255850062740999]
[null,"Yankalilla 33kV","Substation Rating","MVA","Non-Coincident",17.8125,17.8125,17.8125,17.8125,17.8125,17.8125,17.8125]
[null,null,null,null,"Coincident",17.8125,17.8125,17.8125,17.8125,17.8125,17.8125,17.8125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2163288436815001,1.2147527033348999,1.2131575258689,1.2115946287357999,1.2100572929522999,1.2087369548288001,1.2078820385342]
[null,null,null,null,"Coincident",0.91533859092839998,0.91415247905457997,0.91295204094806004,0.91177589514917001,0.91061898534049002,0.90962537539378996,0.90898201494032005]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2163314146755,1.2147552709974001,1.2131600901596,1.2115971897229001,1.2100598506899001,1.2087395097756,1.2078845916739001]
[null,null,null,null,"Coincident",0.91534052570947999,0.91415441132854003,0.91295397068460005,0.91177782239965,0.91062091014558,0.90962729809866005,0.90898393628528995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0948105023251,1.0933796668621001,1.0919297942796,1.0907959761266,1.0900846467064,1.0893733172863,1.0886619878662001]
[null,null,null,null,"Coincident",0.82389093026747995,0.82281416642733995,0.82172307635450004,0.82086983052711004,0.82033452523324002,0.81979921993936999,0.81926391464550996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0948128164619,1.0933819779744001,1.0919321023273001,1.0907982817776001,1.0900869508540001,1.0893756199303,1.0886642890066001]
[null,null,null,null,"Coincident",0.82389267175265002,0.82281590563651996,0.82172481325739999,0.82087156562648,0.82033625920111997,0.81980095277576004,0.8192656463504]
[null,"Yankalilla Hill 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.13107120901107,0.13364555941428999,0.1378988461506,0.14173052138171999,0.14245125180264001,0.14296010058191,0.14439870868638]
[null,null,null,null,"Coincident",0.13107120901107,0.13364555941428999,0.1378988461506,0.14173052138171999,0.14245125180264001,0.14296010058191,0.14439870868638]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.13180598792865,0.13439477001687999,0.13867190047485001,0.14252505589372,0.14324982669485001,0.14376152805600001,0.14520820092857001]
[null,null,null,null,"Coincident",0.13180598792865,0.13439477001687999,0.13867190047485001,0.14252505589372,0.14324982669485001,0.14376152805600001,0.14520820092857001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.12017383576326,0.12267470124903,0.12725691155669,0.13146630937449999,0.13259588693037,0.13341969677300999,0.13517700370312999]
[null,null,null,null,"Coincident",0.12017383576326,0.12267470124903,0.12725691155669,0.13146630937449999,0.13259588693037,0.13341969677300999,0.13517700370312999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.12084752452854999,0.1233624097464,0.1279703077055,0.13220330320578999,0.13333921311930999,0.13416764120046001,0.13593479950903001]
[null,null,null,null,"Coincident",0.12084752452854999,0.1233624097464,0.1279703077055,0.13220330320578999,0.13333921311930999,0.13416764120046001,0.13593479950903001]
[null,"Yongala 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.8364945121160004E-2,7.4695533546185994E-2,7.1483295997986002E-2,6.9031751238379999E-2,6.5231436680867005E-2,6.1630898364053999E-2,5.8246874817329E-2]
[null,null,null,null,"Coincident",7.4986451729512002E-2,7.1453254691402998E-2,6.8022786848339997E-2,6.498519839097E-2,6.1382021665632003E-2,5.7969570547881002E-2,5.4763121877319E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.8942113738246E-2,7.5245676441489995E-2,7.2009780321201006E-2,6.9540179596692994E-2,6.5711875198897998E-2,6.2084818421337999E-2,5.8675871074978E-2]
[null,null,null,null,"Coincident",7.5538737277315998E-2,7.1979517756255995E-2,6.8523784044917005E-2,6.5463823330072002E-2,6.1834108711746001E-2,5.8396524421381997E-2,5.5166459814611997E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.1351967341643993E-2,6.7813392986438001E-2,6.4817606802065997E-2,6.2581023898864996E-2,5.9069885999646E-2,5.5742576881957002E-2,5.2651813510786002E-2]
[null,null,null,null,"Coincident",7.0475081363050002E-2,6.6483882509213998E-2,6.3026256613271006E-2,6.0029124221978002E-2,5.6642496873826997E-2,5.3434096275290999E-2,5.0454076874619003E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.1877484411212E-2,6.8312847968373003E-2,6.5294997406026997E-2,6.3041941761612E-2,5.9504943848037999E-2,5.6153128640297E-2,5.3039601371086001E-2]
[null,null,null,null,"Coincident",7.0994140046578003E-2,6.6973545463319004E-2,6.3490453676298006E-2,6.0471246992030998E-2,5.7059676666888E-2,5.3827645755926003E-2,5.0825678101813002E-2]
[null,"Yorketown 11kV","Substation Rating","MVA","Non-Coincident",2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001]
[null,null,null,null,"Coincident",2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001,2.5973577235772001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2464555452021999,1.2445934009515001,1.2475073715041001,1.2549660475529001,1.247369295395,1.2378976870095999,1.2270021682004999]
[null,null,null,null,"Coincident",1.2464555452021999,1.2445934009515001,1.2475073715041001,1.2549660475529001,1.247369295395,1.2378976870095999,1.2270021682004999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3120580306703,1.3100978794817,1.3131652158816001,1.3210164512069,1.3130198726574001,1.3030497618954999,1.2915807985562999]
[null,null,null,null,"Coincident",1.3120580306703,1.3100978794817,1.3131652158816001,1.3210164512069,1.3130198726574001,1.3030497618954999,1.2915807985562999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0862284177527,1.0858305192219,1.0907407909014999,1.1000322004184,1.0971604361914999,1.0910445794957,1.0826144715762001]
[null,null,null,null,"Coincident",1.0862284177527,1.0858305192219,1.0907407909014999,1.1000322004184,1.0971604361914999,1.0910445794957,1.0826144715762001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1433979528114999,1.1429791123924999,1.1481478176983999,1.1579282455041,1.1549053368005999,1.1484675950592,1.1395938002113]
[null,null,null,null,"Coincident",1.1433979528114999,1.1429791123924999,1.1481478176983999,1.1579282455041,1.1549053368005999,1.1484675950592,1.1395938002113]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"ACR 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Angas Creek 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ardrossan West 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Baroota 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Berri 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Blanche 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brinkworth 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clare North 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dalrymple 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Davenport West 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dorrien 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Florieton SWER 19kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hummocks 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kadina 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Keith 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kincraig 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Leigh Creek South 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mannum 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Metro East 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Metro North 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Metro South 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Metro West 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mobilong 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Barker 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Gambier 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Gunson 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Neuroodla 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North West Bend 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Penola West 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Lincoln Terminal 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Pirie Bungama 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Snuggery Rural 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tailem Bend 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Templers 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Waterloo 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Whyalla Central 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Wudinna 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yadnarie 66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,null,null,"MWh","Non-Coincident"]
[null,"Aldgate 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Aldinga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Allendale East 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Alma 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"American River 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Angaston 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Angle Vale 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ardrossan 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Arno Bay 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ascot Park 11kV",null,"MWh","Non-Coincident",0,0,0,0.26,0.47,0.7,1.63]
[null,"Athol Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Auburn 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Balaklava 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Balhannah 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Baroota Town 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Barossa South TF1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Barossa South TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beachport 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Belvedere Road 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Berri 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Binnies 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Birdwood 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Black Point 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Blackpool 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Blackwood 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,"Booleroo Centre 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Boothby 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Booyoolie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bordertown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brinkworth Town 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brukunga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bungama Napperby 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Burnside 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Burra TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cadell 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caloote 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caltowie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cambrai 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Campbell Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Campbelltown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cape Jervis 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cape Jervis 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caralue 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cavan 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"CBD 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ceduna 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Chain of Ponds 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cheltenham 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cheltenham 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clare 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clarence Gardens 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clarendon 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clearview 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cleve 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cleve 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coffin Bay 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Collinsfield 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coomandook 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coonalpyn 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coonawarra 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Copley Nepabunna 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cordola 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coromandel Place 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cowell 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Croydon 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Croydon Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Crystal Brook 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cudmore Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cummins 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Curramulka 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Curramulka South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Darke Peak 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Deloraine 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Direk 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dorrien TF4 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dorrien TF5 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dowlingville 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"East Terrace 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Edinburgh 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Edithburgh 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Elizabeth Downs 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Elizabeth Heights 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Elizabeth South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Eudunda 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Evanston 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Evanston 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Findon 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Flinders Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Forreston 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Freeling 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Freeling North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Fulham Gardens 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Fullerville 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gawler Belt TF1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gawler Belt TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Georgetown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Geranium 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gladstone 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Glanville 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Glencoe 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Glenelg North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Glossop 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Golden Grove 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gomersal North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Goolwa 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gulnare 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gumeracha 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gumeracha Weir 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gumhaven 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hackham 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hahndorf 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Halbury 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hamley Bridge 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Happy Valley 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Harrow 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hatherleigh 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hawker 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hay Flat 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Henley South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hermitage 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hillcrest 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hindley Street 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Holden Hill 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hope Valley 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Houghton 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hoyleton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ingle Farm 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Inverness 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Jabuk 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jamestown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"James Well 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jervois 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,"Kadina East 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kalangadoo 11kV",null,"MWh","Non-Coincident",0,0,0.01,0.06,0.12,0.2,0.3]
[null,"Kalangadoo West 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kanmantoo 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kapunda TF1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kapunda TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Karoonda 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Keith 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kent Town 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kersbrook 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Keswick 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ki Ki 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kilburn 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kilburn Bus A CMP 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Kilburn South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kilkenny 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kingscote 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kingston SE 11kV",null,"MWh","Non-Coincident",0,0,0.03,0.1,0.19,0.28999999999999998,0.44]
[null,"Kingswood 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Kongorong 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kumorna 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kybunga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Lameroo 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Langhorne Creek 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Largs North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"LeFevre 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Leigh Creek South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Linden Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Little Swamp 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lobethal 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lock 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Loveday 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lower Mitcham 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Loxton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lucindale 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lyndoch 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lyndoch South 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lyrup 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"MacGillivray 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Maitland 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mallala 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mannum Town 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Marion Bay 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Marrabel 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"McLaren Flat TF1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"McLaren Flat TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"McLaren Vale 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"McLaren Vale Vineyard 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Meadows 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Melrose 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Meningie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Milang 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Millicent 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Minlaton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Monarto Central 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Monarto South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Moonta 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Moorkitabie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morgan 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morphett Vale East 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morphettville 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Barker 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Burr 11kV",null,"MWh","Non-Coincident",0.01,0.03,0.06,0.13,0.2,0.28999999999999998,0.41]
[null,"Mount Gambier 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Gambier North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Gambier West 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Pleasant 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mount Schank 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Murray Bridge North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Murray Bridge South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mylor 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mypolonga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Myponga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nairne 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0.02,0.21]
[null,"Nangwarry 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Naracoorte 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Naracoorte East 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Narrung 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"New Osborne 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"New Richmond 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nildottie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ninnes 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Noarlunga Centre 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North Adelaide 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Northfield 11kV",null,"MWh","Non-Coincident",0,0,0.53,7.14,24.81,37.6,53.59]
[null,"North Unley 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Norwood 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nuriootpa 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Oaklands 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Orroroo 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Padthaway 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Palmer 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Panorama 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Parafield Gardens 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Paralowie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Parilla 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Paringa 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Paringa 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Paskeville 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Peake 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pellaring Flat 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Penfield 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Penneshaw 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Penola 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Peterborough 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Piccadilly 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pinnaroo 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pinnaroo South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Plympton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Point Boston 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Polda 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Poonindie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Adelaide 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Adelaide North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Augusta 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Augusta West TF1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Augusta West TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Broughton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Clinton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Portee 11kV",null,"MWh","Non-Coincident",0,0,0,0.06,0.06,7.0000000000000007E-2,0.09]
[null,"Port Germein 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Giles 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Julia 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Lincoln City 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Lincoln Docks 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Lincoln Marina 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Noarlunga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,"Port Pirie South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Stanvac 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Port Vincent 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Prospect 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Punyelroo 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pyap 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Qualco 11kV",null,"MWh","Non-Coincident",0,0,0,0,0.04,0.12,0.3]
[null,"Queenstown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Quorn 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ramco 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rapid Bay 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Renmark 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Riverton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Robe 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Robertstown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Roonka 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Rudall 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Salisbury 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Salt Cliffs 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sandy Creek 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Seacombe 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Seaford 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Second Valley 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sheidow Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sherlock 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Smithfield West 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"South End 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Spalding 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Square Water Hole 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stansbury 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stirling East 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stirling North 1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stirling North 2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stockwell TF1 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stockwell TF2 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stony Point 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Strathalbyn 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Streaky Bay 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Swan Reach 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Swan Reach 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,"Tailem Bend Town 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tantanoola 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tarlton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tarpeena South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Teal Flat 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tea Tree Gully 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Telowie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Thebarton 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tintinara 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tonsley Park 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tumby Bay 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Two Wells 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Uley 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Uley South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Uraidla 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Uraidla 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Verdun 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Victor Harbor 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Virginia 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Waikerie 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Walker Flat 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wallaroo 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Warooka 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wasleys 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Waterloo Town 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Whitmore Square 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Whyalla City 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Whyalla North 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Whyalla Stuart 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Williamstown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Williamstown South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Willunga 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Willunga 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wilmington 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wirrabara Forest 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wirrabara South 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wirrina Cove 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wongyarra 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woodforde 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woodside 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woods Point 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woodville 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woodville 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woolpunda 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wudinna 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yankalilla 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yankalilla 33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yankalilla Hill 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yongala 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yorketown 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.2 Reliability & Cust serv","index":22,"n_rows":76,"n_cols":9,"rows_kept":76,"cut":false,"hidden":false,"merged":[[6,1,6,7],[17,1,17,3],[29,1,29,3],[71,4,71,8],[41,1,41,3],[53,1,53,3],[56,1,56,8],[68,1,68,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. There are no further instructions."]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,18,17,17,16,15]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,94,94,94,94,94]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,189,188,188,187,186]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,302,296,290,284,278]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E13:E17)","v":603},{"$f":"SUM(F13:F17)","v":595},{"$f":"SUM(G13:G17)","v":589},{"$f":"SUM(H13:H17)","v":581},{"$f":"SUM(I13:I17)","v":573}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.86,0.87,0.87,0.88,0.88]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1.28,1.29,1.3,1.3,1.31]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,1.49,1.48,1.47,1.46,1.45]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E25:E29)","v":3.7700000000000005},{"$f":"SUM(F25:F29)","v":3.78},{"$f":"SUM(G25:G29)","v":3.7800000000000002},{"$f":"SUM(H25:H29)","v":3.7800000000000002},{"$f":"SUM(I25:I29)","v":3.7800000000000002}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E37:E41)","v":0},{"$f":"SUM(F37:F41)","v":0},{"$f":"SUM(G37:G41)","v":0},{"$f":"SUM(H37:H41)","v":0},{"$f":"SUM(I37:I41)","v":0}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E49:E53)","v":0},{"$f":"SUM(F49:F53)","v":0},{"$f":"SUM(G49:G53)","v":0},{"$f":"SUM(H49:H53)","v":0},{"$f":"SUM(I49:I53)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS (STPIS)"]
[null,null,"FORECAST"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},6876,6907,6938,6969,7000,7031,7062]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},648222,654631,661094,667609,674179,680803,687482]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},142301,144475,146679,148915,151182,153482,155814]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},138696,138775,138853,138928,139002,139073,139143]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C62:C66)","v":936095},944788,953564,962421,971363,980389,989501]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Number of calls received",null,null,70120,69419,68725,68038,67357]
[null,"Number of calls answered within 30 seconds",null,null,61895,61276,60663,60057,59456]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E75/E74),\"\")","v":0.88270108385624646},{"$f":"IFERROR((F75/F74),\"\")","v":0.88269782048142442},{"$f":"IFERROR((G75/G74),\"\")","v":0.8826918879592579},{"$f":"IFERROR((H75/H74),\"\")","v":0.88269790411240778},{"$f":"IFERROR((I75/I74),\"\")","v":0.88269964517422095}]

{"sheet":"7.1  Policies and Procedures","index":23,"n_rows":386,"n_cols":5,"rows_kept":386,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"SA Power Networks Corporate Strategic Plan 2023 - 2027","Represents our view of internal and external business environments, corporate objectives and strategic directions for the next 5 years","Balanced corporate directions that set the tone and priorities of almost all aspects of our Regulatory Proposal. ","No"]
[null,"Human Relations and Ethics Policy","SA Power Networks will endeavour to be recognised as an employer of choice with a reputation for very high ethical standards and professionalism. SA Power Networks recognises that committed employees are key stakeholders in the achievement of its Strategic Intent.  SA Power Networks’ employees should perform their roles in a professional, courteous and ethical manner which reflects the values that underpin SA Power Networks’ Ethics Policy.","How we achieve our business plans.  ","No"]
[null,"Customer Service Policy","SA Power Networks is committed to providing our customers with value for money services which are targeted to their needs and expectations and delivered in a way which reinforces their vital importance to our business.","How we achieve our business plans.  ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Governance framework"]
[null,"Corporate Governance Policy","The Corporate Governance Policy explains the Board approved Corporate Governance Model and details the Policies and Directives that emanate from the Model. The Policies and Directives provide approved direction to SA Power Networks’ managers, employees and directors in the manner in which we must conduct ourselves in our business operations. Compliance with the Policies and Directives is mandatory","Corporate governance applies to all aspects of the day to day operations and set the tone of our Regulatory Proposal. ","No"]
[null,"Risk Management Policy","SA Power Networks will apply a risk management approach to all business activities in order to ensure that the organisation maximises opportunities while not exposing the business to unacceptable levels of risk. ","How we achieve our business plans.  ","No"]
[null,"Compliance Policy","SA Power Networks will conduct its business activities in compliance with all relevant legal, regulatory and contractual obligations and requirements of relevant standards and internal policies (including directives, procedures and instructions).","How we achieve our business plans. ","No"]
[null,"Sustainability Policy","\nEnsures that environmental and sustainability considerations are incorporated into all SA Power Networks’ business activities as a fundamental part of sound management practice. \n","How we achieve our business plans. ","No"]
[null,"Risk Management Framework","This document outlines SA Power Networks Framework for the management of risk across the business. It is closely aligned to the requirements of AS/NZS ISO 31000:2018 Risk Management – Principles and Guidelines. This document is designed to outline the risk management activities of SA Power Networks as they relate to the principles and guidelines described in AS/NZS ISO 31000:2018.","Supports Risk Management Policy. ","No"]
[null,"Ring Fencing Directive","This Directive contains information relating to the responsibilities of all SA Power Networks (SAPN) staff and contractors and all Enerven staff, and other third parties to appropriately follow the AER Ring-fencing guideline.","How we achieve our business plans","No"]
[null,"Critical Infrastructure Risk Management Program","The Critical Infrastructure Risk Management Program (CIRMP) provides an holistic approach towards identifying, preventing and mitigating material risks relating to the management of critical infrastructure in accordance with the Security of Critical Infrastructure Act and Rules. ","Supports Risk Management Policy. ","No"]
[null,"Expenditure Governance Procedures (5.1.2)","This document describes SA Power Networks’ robust planning and governance processes employed in its business planning and annual budget cycles. ","Attachment 5 and 6","Yes"]
[null,"Negotiated services framework and criteria (Attachment 16)","This document specifies the Negotiated Distribution Service Criteria, information disclosure process, and identifies the timetable that will apply to each classification of negotiated distribution service. ","Attachment 16","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Accounting Practices and Guideline Manual","Sets out the required accounting treatments for items in the Income Statement, the Balance Sheet, the Statement of Changes in Equity (or Statement of Recognised Income and Expense) and the Cash Flow Statement","How we achieve our business plans. ","Yes"]
[null,"Finance Policy","Obligations in regard to the following financial management areas: \n• business plans and budgets; \n• accounts and financial statements; and\n• management reporting. ","How we achieve our business plans. ","No"]
[null,"Cost Allocation Method","This AER approved document describes the principles and policies for allocating costs within the categories of distribution services that SA Power Networks provides.","Available at the following link https://www.sapowernetworks.com.au/public/download.jsp?id=309684#:~:text=SA%20Power%20Networks%20employs%20a,its%20integrated%20business%20management%20system.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Policy","SA Power Networks will manage its assets to satisfy customer service needs; meet Licence and Regulatory obligations; to provide a safe environment for employees, contractors and the community; and to deliver optimal returns to shareholders. \n\nAsset management includes risk management for the whole of life consideration of procurement, operation, maintenance, condition and performance monitoring, disposal or replacement and legal compliance. It includes assets owned or leased and those owned by clients if part of an asset management contract. It also includes long term planning and financial links, provision of assets for current and future services. ","How we achieve our business plans","No"]
[null,"Connections Policy 2025-2030 ","The SA Power Networks Connection Policy sets out the circumstances in which it may require a retail customer or real estate developer to pay a connection charge, for the provision of a connection service.","Attachment 17","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset Management Strategies"]
[null,"Strategic Asset Management Plan (SAMP)","The Plan outlines SA Power Networks strategic direction and priorities for electricity distribution assets. ","Supporting Document 5.2.2","Yes"]
[null,"Network Strategy","This strategy sets out SA Power Networks' strategies to adapt our network business into the future in response to increased distributed energy resources on the network.","Supporting Document 5.2.4","Yes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset Management Plans"]
[null,"Public Lighting Asset Management Plan","The Plan outlines SA Power Networks approach to managing pubic lighting assets","Attachment 15","No"]
[null,"Metering Asset Management Strategy and Asset Plan","The Plan outlines SA Power Networks approach to managing metering assets","Attachment 19","No"]
[null,"Reliability  Management Strategy 2025-30","The document outlines SA Power Networks approach to reliability and resiliance of the network ","Key contents and information are covered in 5.9 supporting documents","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Expenditure Forecasting Methodology","This document describes the methodology which SA Power Networks is proposing to use when developing its operating and capital expenditure forecasts for the 2025-2030 regulatory control period.","How we achieve our business plans. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Future Operating Model 2016 - 2031","The SA Power Networks Future Operating Model (FOM) 2016 - 2031 represents a ‘living document’ vision that offers long-term directional insights into our most likely future development paths. These insights will help to guide our staff and decision makers in the coming years.","How we achieve our business plans. ","No"]
[null,"Customer Strategy 2022 - 2026","The SA Power Networks Customer Strategy provides our customer service and experience vision. This strategy outlines SA Power Networks customer vision and initiatives. It provides an overview of key customer segments, their current and future needs, and outlines our roadmap in response to this which we expect to deliver improved customer satisfaction. ","How we achieve our business plans. ","No"]
[null,"SA Power Network’s Connection Policy","The SA Power Networks Connection Policy sets out the circumstances in which it may require a retail customer or real estate developer to pay a connection charge, for the provision of a connection service.","Attachment 17","No"]
[null,"Sustainability Policy","The SA Power Networks Sustainability Policy sets out the commitment and approach to conducting electricity distribution operations and business activities in a manner which is sustainable and prevents or minimises pollution and other adverse impacts on the environment.","How we achieve our business plans. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"Procurement Directive","Establishes the \nprinciples and direction which must be \nfollowed when making procurement \ndecisions on behalf of the SA Power \nNetworks Group","How we achieve our business plans. ","No"]
[null,"Supplier Management Framework and Strategic Supplier Management Program","Sets out the governance, performance management and reviews required for procurement at SA Power Networks","How we achieve our business plans. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Information technology policies or strategies"]
[null,"IT Investment Plan 2025-30","The IT Investment Plan provides the overview, rationalse and portfolio summary of the proposed IT expenditure for the 2020-25 RCP and supports our regulatory proposal","Attachment 5 Capex, Attachment 6 Opex, relating to the IT sections\nSupporting Document 5.12.1","Yes"]
[null,"IT Asset Management Plan","The IT Asset Management Plan provides alignment with SA Power Networks' Asset Management Policy to enable the delivery of essential energy services; Describe how we manage our IT Assets to deliver the most value to our customers and stakeholders; and provide a framework for ensuring IT Assets are prudently managed throughout the entire asset lifecycle. ","How we achieve our business plans. ","No"]
[null,"Cyber Security Policy","The SA Power Networks Cyber Security Policy sets out the circumstances in which SA Power Networks manages its cyber security risk. This includes via appropriate investments in cyber security to ensure that the organisation can prevent, detect and respond to increasing cyber security threats. SA Power Networks recognises that it's business is becoming increasingly reliant on digital technology, and that cyber security plays a critical role in ensuring the safety, integrity and availability of it's information and business systems.","How we achieve our business plans. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Distribution Annual Planning Report","SA Power Networks produces each year a Distribution Annual Planning Report (DAPR) in accordance with the requirements of Section 5.13.2 of the National Electricity Rules (NER).  The information contained within the DAPR complies with the requirements of Schedule 5.8 of the NER. ","Available from our website www.sapowernetworks.com.au","No"]
[null,"Network Strategy 2020-2030","This strategy sets out SA Power Networks' strategies to adapt our network business into the future in response to increased distributed energy resources on the network.","Supporting Document 5.2.4","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Self insurance guidelines or policy"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Land and easement acquisition polices"]
[null,"30 Year Property Strategy","The document describes SA Power Networks' property strategy.","How we achieve our business plans.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"Refer to Asset Management Plans",null,null,"No"]
[null,"Bushfire Risk Management Policy & Manuals","This manual details the policies and procedures which govern SA Power Networks bushfire risk management practices. It is a self contained document except where it specifically refers to other related documents. It supersedes all previous bushfire related letters and documents including all previous Bushfire Risk Management Manuals."," Capital Expenditure","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"Organisational Resilience Policy","This policy addresses the \nresilience of the organisation through four \nkey areas:\n• Risk Management;\n• Business Continuity;\n• Crisis and Emergency; and\n• IT Disaster Recovery\nThese areas are interrelated and \ncomplimentary in managing risk to plan, \nprevent and respond to incidents. ","How we achieve our business plans","No"]

{"sheet":"7.2 Contingent projects","index":24,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.2 CONTINGENT PROJECTS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($, nominal)\")","v":"Proposed annual revenue requirement for 2025-26 \n($, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2025-26"}]
[null,null,null,null,null,{"$f":"+E9*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$9","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":25,"n_rows":298,"n_cols":5,"rows_kept":298,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"State Government SA","Aboriginal Heritage Act 1988 (SA)","Business as usual","No"]
[null,"State Government SA","Adelaide Parklands Act 2005 SA","Capex and Opex","No"]
[null,"State Government SA","Building and Construction Industry Security of Payment Act 2009 (SA)","Business as usual","No"]
[null,"State Government SA","Building and Construction Industry Security of Payment Regulations 2011 (SA)","Business as usual","No"]
[null,"State Government SA","Building Work Contractors Act 1995 (SA)","Business as usual","No"]
[null,"State Government SA","Building Work Contractors Regulations 2011 (SA)","Business as usual","No"]
[null,"State Government SA","Business Names (Commonwealth Powers) Act 2012 SA","Business as usual","No"]
[null,"State Government SA","Children’s Protection Act 1993 (SA) ","Business as usual","No"]
[null,"State Government SA","Civil Liability Act 1936 (SA)","Business as usual","No"]
[null,"State Government SA","Civil Liability Regulations 2013 (SA)","Business as usual","No"]
[null,"State Government SA","Civil Liability Regulations 2013 SA","Business as usual","No"]
[null,"State Government SA","Construction Industry Long Service Leave Act 1987 (SA)","Opex","No"]
[null,"State Government SA","Construction Industry Training Fund Act 1993 SA","Opex","No"]
[null,"State Government SA","Dangerous Substances (Goods Transport) Regulations 2008 SA","Business as usual","No"]
[null,"State Government SA","Dangerous Substances Act 1979 SA","Business as usual","No"]
[null,"State Government SA","Dangerous Substances Regulations 2002 SA","Business as usual","No"]
[null,"State Government SA","Electricity (General) Regulations 2012 (SA)","Capex and Opex","Yes"]
[null,"State Government SA","Electricity (Principles of Vegetation Clearance) Regulations 2010 (SA) ","Opex","No"]
[null,"State Government SA","Electricity Act 1996 (SA)","Capex / Opex\n\nComply with and adapt to:\n- distribution licence conditions\n- changes in vegetation cleareance practices\n- report 'prescribed fires'\n- change in penalties\n- enhanced powers of Essential Services Commission of SA and the Office of the Technical Regulator","Yes"]
[null,"State Government SA","Electricity Corporations (Restructuring and Disposal) Act 1999 SA","Opex","No"]
[null,"State Government SA","Electricity Corporations (Restructuring and Disposal) Regulations 2012 SA","Opex","No"]
[null,"State Government SA","Electronic Communication Act 2000 (SA)","Business as usual","No"]
[null,"State Government SA","Electronic Communication Regulations 1997 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Management Act 2004 (SA)","Opex","No"]
[null,"State Government SA","Emergency Management Regulations 2009 (SA)","Opex","No"]
[null,"State Government SA","Emergency Services Funding (Remissions - Land) Regulations 2014 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Services Funding (Remissions - Motor Vehicles and Vessels) Regulations 2014 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Services Funding Act 1998 (SA)","Business as usual","No"]
[null,"State Government SA","Energy Products (Safety and Efficiency) Act 2000 SA","Business as usual","No"]
[null,"State Government SA","Energy Products (Safety and Efficiency) Regulations 2012 SA","Business as usual","No"]
[null,"State Government SA","Environment Protection Act 1993 (SA)","Capex / Opex - Environmental","No"]
[null,"State Government SA","Environment Protection Regulations 2009 (SA)","Capex / Opex - Environmental","No"]
[null,"State Government SA","Equal Opportunity Act 1984 (SA)","Business as usual","No"]
[null,"State Government SA","Essential Services Act 1981 (SA)","Business as usual","No"]
[null,"State Government SA","Essential Services Commission Act 2002 (SA)","Business as usual","No"]
[null,"State Government SA","Essential Services Commission Regulations 2004 (SA)","Business as usual","No"]
[null,"State Government SA","Fair Trading Act 1987 (SA)","Business as usual","No"]
[null,"State Government SA","Fair Trading Regulations 2010 (SA)","Business as usual","No"]
[null,"State Government SA","Fair Work (Clothing Outworker Code of Practice) Regulations 2007","Business as usual","No"]
[null,"State Government SA","Fair Work (General) Regulations 2009","Capex and Opex","No"]
[null,"State Government SA","Fair Work (Representation) Regulations 2009","Capex and Opex","No"]
[null,"State Government SA","Fair Work Act 1994 (SA)","Capex and Opex","No"]
[null,"State Government SA","Fences Act 1975 SA","Business as usual","No"]
[null,"State Government SA","Fences Regulations 2003 SA","Business as usual","No"]
[null,"State Government SA","Fire & Emergency Services Act 2005 (SA)","Business as usual","No"]
[null,"State Government SA","Fire & Emergency Services Regulations 2005  (SA)","Business as usual","No"]
[null,"State Government SA","Foreign Acquisitions and Takeovers (Notices) Regulations 1975 (Cth)","Business as usual","No"]
[null,"State Government SA","Freedom of Information (Exempt Agency) Regulations 2008 (SA)","Business as usual","No"]
[null,"State Government SA","Freedom of Information (Fees and Charges) Regulations 2003 (SA)","Business as usual","No"]
[null,"State Government SA","Freedom of Information (General) Regulations 2002 (SA)","Business as usual","No"]
[null,"State Government SA","Freedom of Information Act 1991 (SA)","Business as usual","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) (Expiation Fees) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) (Fees) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) (Savings, Transitional and Declaratory) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) Act 2013  (SA)","Opex\nComply with and adapt to:\n- overarching primary duty of care \n- reasonably practicable’ defence \n- Eexcutive Officers  proactive duty to exercise due diligence\n- increase in penalties","No"]
[null,"State Government SA","Highways Act 1926 SA","Business as usual","No"]
[null,"State Government SA","Labour Hire Licensing Act 2017","Business as usual","No"]
[null,"State Government SA","Labour Hire Licensing Regulation 2017","Business as usual","No"]
[null,"State Government SA","Land Tax Act 1936 SA","Opex","No"]
[null,"State Government SA","Land Tax Regulations 2010 SA","Business as usual","No"]
[null,"State Government SA","Landlord and Tenant Act 1936 SA","Business as usual","No"]
[null,"State Government SA","Law of Property Act 1936 (SA)","Business as usual","No"]
[null,"State Government SA","Mines and Works Inspection Act 1920 (SA)","Business as usual","No"]
[null,"State Government SA","Mines and Works Inspection Regulations 1998 (SA)","Opex","No"]
[null,"State Government SA","Misrepresentation Act 1972 SA","Business as usual","No"]
[null,"State Government SA","Motor Vehicles Act 1959 SA","Opex","No"]
[null,"State Government SA","Motor Vehicles Regulations 2010 SA","Opex","No"]
[null,"State Government SA","National Electricity (South Australia) Act 1996 (SA) ","Capex and Opex","No"]
[null,"State Government SA","National Electricity (South Australia) Regulations 1998 (SA)","Opex","No"]
[null,"State Government SA","National Energy Retail Law  (Local Provisions) Regulations 2013 (SA)","Capex and Opex","No"]
[null,"State Government SA","National Energy Retail Law (South Australia) Act 2011 (SA)","Capex and Opex","Yes"]
[null,"State Government SA","National Energy Retail Regulations 2012 (SA)","Business as usual","No"]
[null,"State Government SA","Native Title (South Australia) Act 1994 (SA)","Opex","No"]
[null,"State Government SA","Native Title (South Australia) Regulations 2001 (SA)","Opex","No"]
[null,"State Government SA","Native Vegetation Act 1991 SA","Capex and Opex","No"]
[null,"State Government SA","Native Vegetation Regulations 2017 (SA)","Capex and Opex","No"]
[null,"State Government SA","Partnership Act 1981 SA","Business as usual","No"]
[null,"State Government SA","Payroll Tax Act 2009 (SA)","Opex","No"]
[null,null,null,null,"No"]
[null,"State Government SA","Planning, Development and Infrastructure Act 2016","Capex and Opex","No"]
[null,"State Government SA","Planning, Development and Infrastructure (General) Regulations 2016","Capex and Opex","No"]
[null,"State Government SA","Plumbers, Gas Fitters and Electricians Act 1995 (SA)","Opex","No"]
[null,"State Government SA","Plumbers, Gas Fitters and Electricians Regulations 2010 (SA)","Opex","No"]
[null,"State Government SA","Race Discrimination Commissioner (Cth) (Allowances) Regulations 1987 ","Business as usual","No"]
[null,"State Government SA","Racial Vilification Act 1996 (SA)","Business as usual","No"]
[null,"State Government SA","Real Property Act 1886 (SA)","Business as usual","No"]
[null,"State Government SA","Real Property Regulations 2009 (SA)","Opex","No"]
[null,"State Government SA","Retail and Commercial Leases Act 1995 SA","Business as usual","No"]
[null,"State Government SA","Return to Work Act 2014","Opex","No"]
[null,"Sate Government SA ","Return to Work Regulations 2015","Opex","No"]
[null,"State Government SA","Road Traffic (Light Vehicle Mass and Loading Requirements) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Road Traffic (Miscellaneous) Regulations 1999 (SA)","Opex","No"]
[null,"State Government SA","Road Traffic (Oversize or Overmass Vehicle Exemptions) Regulations 1999 (SA)","Opex","No"]
[null,"State Government SA","Road Traffic Act 1961 (SA)","Capex / Opex\nComply with and adapt to:\n - requirement to obtain a permit from Comissioner of Highways on main roads\n- increased penalties","No"]
[null,"State Government SA","Sale of Goods Act 1895 SA","Business as usual","No"]
[null,"State Government SA","Stamp Duties Act 1923 SA","Opex","No"]
[null,"State Government SA","State Records Act 1997 (SA)","Business as usual","No"]
[null,"State Government SA","State Records Regulations 2013 (SA)","Business as usual","No"]
[null,"State Government SA","Surveillance Devices Act 2016 (SA) ","Business as usual","No"]
[null,"State Government SA","Surveillance Devices Regulations 2017 (SA) ","Business as usual","No"]
[null,"State Government SA","Telecommunications (Interception) Act 2012 (SA)","Opex","No"]
[null,"State Government SA","Training and Skills Development Act 2008 SA","Business as usual","No"]
[null,"State Government SA","Work Health & Safety Act 2012  (SA)","Capex and Opex","No"]
[null,"State Government SA","Work Health & Safety Regulations 2012 (SA)","Capex and Opex","No"]
[null,"State Government SA","Workers Rehabilitation & Compensation Act 1986 (SA)","Opex","No"]
[null,"State Government SA","Workers Rehabilitation and Compensation Regulations 2010 (SA)","Opex","No"]
[null,"Commonwealth Government","A New Tax System (Goods and Services Tax) Act 1999  (Cth)","Capex and Opex","No"]
[null,"Commonwealth Government","A New Tax System (Goods and Services Tax) Regulations 1999 (Cth)","Capex and Opex","No"]
[null,"Commonwealth Government","Aboriginal and Torres Strait Islander Heritage Protection Act 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Aboriginal and Torres Strait Islander Heritage Protection Regulations 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Affirmative Action (Equal Employment Opportunity for Women) Regulations 1986 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Age Discrimination Act 2004 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Human Rights Commission Act 1986 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Human Rights Commission Regulations 1989 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Modern Slavery Act 2018 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Securities and Investments Commission Act 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Securities and Investments Commission Regulations 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Building and Construction Industry (Improving Productivity) Act 2016","Business as usual","No"]
[null,"Commonwealth Government","Climate Change Act 2022","Business as usual","No"]
[null,"Commonwealth Government","Competition and Consumer Act 2010 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Competition and Consumer Regulations 2010 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Corporations Act 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Corporations Regulations 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Designs Act 2003 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Disability Discrimination Act 1992 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Disability Discrimination Regulations 1996 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Electronic Transactions Act 1999 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Electronic Transactions Act Regulations 2020 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Environment Protection and Biodiversity Conservation Act 1999 (Cth)","Capex and Opex","No"]
[null,"Commonwealth Government","Equal Employment Opportunity (Commonwealth Authorities) Act 1987 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fair Work (Transitional Provisions and Consequential Amendments) Regulations 2009 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fair Work Act 2009 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fair Work Regulations 2009  (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Foreign Acquisitions and Takeovers Act 1975 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Foreign Acquisitions and Takeovers Regulations 1989 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fringe Benefits Tax Act 1986 (Cth)","Opex","No"]
[null,"Commonwealth Government","Fringe Benefits Tax Assessment Act 1986 (Cth)","Opex","No"]
[null,"Commonwealth Government","Fringe Benefits Tax Regulations 1992 (Cth)","Opex","No"]
[null,"Commonwealth Government","National Harmonisation of Work Health and Safety Regulations 2011 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Income Tax (Excluded STBs) Regulations 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Act 1986 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Assessment Act 1936 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Assessment Act 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Assessment Regulations 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Regulations 1936 (Cth)","Opex","No"]
[null,"Commonwealth Government","Law Reform (Contributory Negligence and Apportionment of Liability) Act 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","National Greenhouse and Energy Reporting Act 2007 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Native Title (Indigenous Land Use Agreements) Regulations 1999 (Cth)","Opex","No"]
[null,"Commonwealth Government","Native Title Act 1993 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Patents Act 1990 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Personal Property Securities Act 2000 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Privacy Act 1988 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Privacy Amendment (Notifiable Data Breaches) Act 2017 ","Business as usual","No"]
[null,"Commonwealth Government","Privacy Regulation 2013 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Racial Discrimination Act 1975 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Racial Discrimination Regulations 1987 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Security of Critical Infrastructure Act 2018 (Cth)","Capex and Opex","Yes"]
[null,"Commonwealth Government","Sex Discrimination Amendment (Sexual Orientation, Gender Identity and Intersex Status) Act 2013","Business as usual","No"]
[null,"Commonwealth Government","Sex Discrimination Act 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Sex Discrimination Regulations 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Superannuation Guarantee (Administration) Act 1992  (Cth)","Opex","No"]
[null,"Commonwealth Government","Superannuation Guarantee (Administration) Regulations 1993  (Cth)","Opex","No"]
[null,"Commonwealth Government","Superannuation Industry (Supervision) Act 1993 (Cth)","Opex","No"]
[null,"Commonwealth Government","Superannuation Industry (Supervision) Regulations 1994  (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications (Interception and Access) Act 1979 (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications (Interception and Access) Regulations 1987 (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications Act 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications Regulations 2001 (Cth)","Opex","No"]
[null,"Commonwealth Government","Trade Marks Act 1995 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Workplace Gender Equality Act 2012 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Workplace Relations Acts and Regulations (Cth)","Capex and Opex","No"]
[null,"Commonwealth Government","Security Legislation Amendment (Critical Infrastructure Protection) Act 2022","Capex and Opex","Yes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"ACMA","Carrier licences for telecommunications and radio communications permits us to operate our radio and operational telecommunications","Opex","No"]
[null,"ESCoSA","Electricity Distribution Licence - Licenses and imposes obligations on DNSPs","Opex","Yes"]
[null,"ESCoSA","Electricity Generation Licence- Kangaroo Island Power Station - Permits us to operate the Kingscote Generator in SA","Opex","No"]
[]
[null,"RULES"]
[null,"Equal Opportunity Tribunal Rules (SA)","Equal Opportunity Tribunal Rules (SA)","Business as usual","No"]
[null,"Industrial Proceedings Rules 2010","Industrial Proceedings Rules 2010","Business as usual","No"]
[null,"Fair Work Commission Rules 2013 (Cth)","Fair Work Commission Rules 2013 (Cth)","Business as usual","No"]
[null,"National Electricity Rules\n\n\nNational Energy Retail Rules","National Electricity Rules - Details the technical operational requirements for the operation of the National Electricity Market\nNational Energy Retail Rules","Capex and Opex","Yes"]
[null,"ORDERS"]
[null,"N/A"]
[]
[]
[null,"CODES"]
[null,"AEMO","National Metrology procedures","Opex","No"]
[null,"AEMO","MSATS","Opex","No"]
[null,"ESCoSA (ESC Act)","ESCOSA Electricity Distribution Code (SA)","Capex and Opex","No"]
[null,"ESCoSA (ESC Act)","ESCOSA Electricity Metering Code (SA)","Opex","No"]
[null,"ESCoSA (ESC Act)","ESCOSA Electricity Transmission Code (SA)","Capex and Opex","No"]
[null,"Building Code of Australia","Building Code of Australia published by the Australian Building Codes Board as in force from time to time\nBuilding and Construction Industry (Fair and Lawful Building Sites) Code 2014\nCode for the Tendering and Performance of Building Work ","Capex and Opex","No"]
[null,"State Government SA","Approved Code of Working Hours","Capex and Opex","No"]
[null,"Commonwealth Government","National Harmonisation of Work Health and Safety Code of Practice","Capex and Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"AER","Compliance Procedures and Guidelines","Opex","No"]
[null,"AER","Confidentiality","Confidentiality template supporting document 20.2","No"]
[null,"AER","Consumer Engagement","Attachment 0 Customer and Stakeholder engagement","No"]
[null,"AER","Cost Allocation Guideline (Distribution) - cost must be in acordance with this","Capex and Opex","No"]
[null,"AER","Distribution Annual Planning Report Template v1.0 (June 2017)","Business as ususal/Capex","No"]
[null,"AER","Distribution Reliability Measures Guideline (Nov 2018)","Business as ususal ","No"]
[null,"AER","Electricity Distribution Service Classification Guideline (Sept 2018)","Discussed in Attachment 13","No"]
[null,"AER","Expenditure Forecasts Assessment Guideline for Electricity Distribution","Business as usual","No"]
[null,"AER","National Electricity Connection Charge Guideline","Connections capex","No"]
[null,"AER","Rate of Return Binding Instrument","Discussed in Attachment 3 Rate of Return","No"]
[null,"AER","Restricted Asset Exemptin Guideline (Sept 2018)","Business as usual","No"]
[null,"AER","Ring Fencing Guidelines (Oct 2017)","Capex and Opex","No"]
[null,"AER","RIT-D Application","Capex - augex and repex","No"]
[null,"AER","Shared Assets","Discussed in Attachment 1 - Annual Revenue requirements and control mechanism","No"]
[null,"AER Scheme","Demand Management Incentive Scheme and Innovation allowance mechanism","Discussed in Attachment 12 - Demand Management Incentives and Allowances","No"]
[null,"AER Scheme","Capital Expenditure Incentive Guideline for Electricity Network Service Providers","Discussed in Attachment 1, 5 and 9","No"]
[null,"AER Scheme","Efficiency Benefit Sharing Scheme for Electricity Network Service Providers","Discussed in Attachment 1, 8","No"]
[null,"AER Scheme","Service Target Performance Incentive Scheme ","Discussed in Attachement 10","No"]
[null,"ESCoSA (ESC Act)","Electricity Industry Guideline No.1 - Information requirements - Details SA Power Networks reporting requirements for both Operational and Financial Perfromance","Opex","No"]
[null,"ESCoSA (ESC Act)","Energy Industry Guideline No.4 - Compliance Systems and Reporting - Details SA Power Networks compliance reporting obligations and system for compliance","Opex","No"]
[null,"SAPN Real Estate Guidelines","To hold only such real property as is necessary for the efficient and effective operation of the business, ensure prudent provision for planned expansion of SA Power Networks’ operations, and appropriate legal tenure is obtained in all cases, to deliver optimal returns to shareholders and to meet the obligations to the Treasurer of South Australia under the Distribution Network Land Lease","Capex/Opex","No"]
[null,"SAPN Easement Guideilines","To provide adequate legal protection for electricity distribution network assets constructed on, under or over private and public property, to secure the right of access to those assets for maintenance purposes by the acquisition and registration of easements.\nThese Guidelines do not extend to land owned or leased by SA Power Networks (although it is possible to have an easement in favour of oneself), which are the subject of another document, “SA POWER NETWORKS Real Estate Guidelines” dated 28 April 2008","Business as usual","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[]
[]
[]
[null,"OTHER"]
[null,"Rules ","Security of Critical Infrastructure (Critical infrastructure risk management program) Rules (LIN 23/006) 2023","Business as usual","Yes"]
[null,"AER Regulatory Information Notice 11 October 2023 ","Reset 2025-30 information requirements","Capex/Opex, RIN templates 1-7                                                      ","Yes"]
[null,"AER Framework and Approach for SA Power Networks - RCP commencing 1 July 2025","Sets parameters for our 2025-30 Regulatory Control Period.","Capex/Opex                                                      ","Yes"]

{"sheet":"7.4 Shared Assets","index":26,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,8,2],[30,2,30,8],[31,2,31,8],[32,2,32,8],[39,2,39,8],[40,2,40,8],[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.4 SHARED ASSETS"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service",{"$f":"CONCATENATE(\"Shared asset unregulated revenue  \n($, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  \n($, real June 2025)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", FRCP_y5)","v":"Total 2025-26 to 2029-30"}]
[null,"Fibre Access","Rental of overhead and underground distribution assets for telecommunication services.",null,null,null,null,null,null,null,{"$f":"SUM(F10:J10)","v":0}]
[null,"Pole Rental","Rental of overhead and underground distribution assets for telecommunication services.",null,null,null,null,null,null,null,0]
[null,"Duct Space Rental","Rental of underground distribution assets for telecommunication services.",null,null,null,null,null,null,null,0]
[null,"Facilities Access","Facilities Access Agreements for access to other assets - e.g. towers, base stations etc",null,null,null,null,null,null,null,0]
[null,"Property Rentals","Rental fees received for lease of properties.",303704,303704,303704,303704,303704,303704,303704,1518520]
[null,"Unregulated Services - Vehicle revenue","Unregulated construction and maintenance services provided to external groups, e.g. ElectraNet. Relates specifically to use of regulated heavy vehicles in undertaking work.",3164674,3164674,3164674,3164674,3164674,3164674,3164674,15823370]
[null,"Unregulated Services - Property/IT revenue","Unregulated construction and maintenance services provided to external groups, e.g. ElectraNet. Relates specifically to use of infrastructure assets of property and IT in undertaking work.",8239934,8239934,8239934,8239934,8239934,8239934,8239934,41199670]
[null,"HV Test Equipment Hire","Hire of high voltage test equipment by electrical contractors for compliance testing for new subdivisions. Ceased in December 2015, as not cost effective to continue to provide this service.","                            -  ","                            -  ","                            -  ","                            -  ","                            -  ","                            -  ","                            -  ",0]
[null,"Training - Overheads revenue only","Electrical related training programs provided to external groups, principally electrical contractors requiring accreditation to work on SA Power Networks' assets. Relates to corporate infrastructure assets e.g. property, IT. Ceases from 2020 as service wil","                            -  ","                            -  ","                            -  ","                            -  ","                            -  ","                            -  ","                            -  ",0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]
[]
[null,"Unregulated Services - Vehicle revenue","Allocated only transfer costs including a margin for regulated vehicles when used by Enerven."]
[null,"Unregulated Services - Property/IT revenue","Partial internal allocation based on CAM apportionment for property and IT of revenue recived for overheads"]

{"sheet":"7.7 TSS-LRMC","index":27,"n_rows":155,"n_cols":22,"rows_kept":155,"cut":false,"hidden":false,"merged":[[69,1,70,1],[89,1,90,1],[6,3,7,4],[11,1,12,1],[23,1,24,1],[35,1,36,1],[49,1,50,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is SA Power Networks using the 'Average Incremental Cost' approach?"}]
[null,null,null,null,null,"YES"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C13,4)+1)&\"-\"&MID(C13,3,2)+2),VALUE(LEFT(C13,4)+1))","v":"2024-25"},"2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42","2042-43"]
[null,"Replacement expenditure",null,null,11388678.560000001,12353240.310000001,13850299.07,12773407.810000001,13453146.539999999,13060000,13321200,13587624,13859376.48,14136564.01,13592952.9,13592952.9,13592952.9,13592952.9,13592952.9,13592952.9,13592952.9,13592952.9]
[null,"Connections"]
[null,"Augmentation Expenditure",null,null,82684234.530000001,88354041.959999993,90202615.290000007,102510008.26000001,107439348.27,104985500,106149822,107337430.44,108548791.05,109784378.87,107361184.47,107361184.47,107361184.47,107361184.47,107361184.47,107361184.47,107361184.47,107361184.47]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C14:C20)","v":0},{"$f":"SUM(D14:D20)","v":0},94072913.090000004,100707282.27,104052914.36000001,115283416.07000001,120892494.81,118045500,119471022,120925054.44,122408167.53,123920942.88000001,120954137.37,120954137.37,120954137.37,120954137.37,120954137.37,120954137.37,120954137.37,120954137.37]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C25,4)+1)&\"-\"&MID(C25,3,2)+2),VALUE(LEFT(C25,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D25,4)+1)&\"-\"&MID(D25,3,2)+2),VALUE(LEFT(D25,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E25,4)+1)&\"-\"&MID(E25,3,2)+2),VALUE(LEFT(E25,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F25,4)+1)&\"-\"&MID(F25,3,2)+2),VALUE(LEFT(F25,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G25,4)+1)&\"-\"&MID(G25,3,2)+2),VALUE(LEFT(G25,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H25,4)+1)&\"-\"&MID(H25,3,2)+2),VALUE(LEFT(H25,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I25,4)+1)&\"-\"&MID(I25,3,2)+2),VALUE(LEFT(I25,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J25,4)+1)&\"-\"&MID(J25,3,2)+2),VALUE(LEFT(J25,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K25,4)+1)&\"-\"&MID(K25,3,2)+2),VALUE(LEFT(K25,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L25,4)+1)&\"-\"&MID(L25,3,2)+2),VALUE(LEFT(L25,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M25,4)+1)&\"-\"&MID(M25,3,2)+2),VALUE(LEFT(M25,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N25,4)+1)&\"-\"&MID(N25,3,2)+2),VALUE(LEFT(N25,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O25,4)+1)&\"-\"&MID(O25,3,2)+2),VALUE(LEFT(O25,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P25,4)+1)&\"-\"&MID(P25,3,2)+2),VALUE(LEFT(P25,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q25,4)+1)&\"-\"&MID(Q25,3,2)+2),VALUE(LEFT(Q25,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R25,4)+1)&\"-\"&MID(R25,3,2)+2),VALUE(LEFT(R25,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S25,4)+1)&\"-\"&MID(S25,3,2)+2),VALUE(LEFT(S25,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T25,4)+1)&\"-\"&MID(T25,3,2)+2),VALUE(LEFT(T25,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U25,4)+1)&\"-\"&MID(U25,3,2)+2),VALUE(LEFT(U25,4)+1))","v":"2042-43"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Export services",null,null,29530000,11140000,15310000,9370000,10060000]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C26:C32)","v":0},{"$f":"SUM(D26:D32)","v":0},29530000,11140000,15310000,9370000,10060000,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C37,4)+1)&\"-\"&MID(C37,3,2)+2),VALUE(LEFT(C37,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D37,4)+1)&\"-\"&MID(D37,3,2)+2),VALUE(LEFT(D37,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E37,4)+1)&\"-\"&MID(E37,3,2)+2),VALUE(LEFT(E37,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F37,4)+1)&\"-\"&MID(F37,3,2)+2),VALUE(LEFT(F37,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G37,4)+1)&\"-\"&MID(G37,3,2)+2),VALUE(LEFT(G37,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H37,4)+1)&\"-\"&MID(H37,3,2)+2),VALUE(LEFT(H37,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I37,4)+1)&\"-\"&MID(I37,3,2)+2),VALUE(LEFT(I37,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J37,4)+1)&\"-\"&MID(J37,3,2)+2),VALUE(LEFT(J37,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K37,4)+1)&\"-\"&MID(K37,3,2)+2),VALUE(LEFT(K37,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L37,4)+1)&\"-\"&MID(L37,3,2)+2),VALUE(LEFT(L37,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M37,4)+1)&\"-\"&MID(M37,3,2)+2),VALUE(LEFT(M37,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N37,4)+1)&\"-\"&MID(N37,3,2)+2),VALUE(LEFT(N37,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O37,4)+1)&\"-\"&MID(O37,3,2)+2),VALUE(LEFT(O37,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P37,4)+1)&\"-\"&MID(P37,3,2)+2),VALUE(LEFT(P37,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q37,4)+1)&\"-\"&MID(Q37,3,2)+2),VALUE(LEFT(Q37,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R37,4)+1)&\"-\"&MID(R37,3,2)+2),VALUE(LEFT(R37,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S37,4)+1)&\"-\"&MID(S37,3,2)+2),VALUE(LEFT(S37,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T37,4)+1)&\"-\"&MID(T37,3,2)+2),VALUE(LEFT(T37,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U37,4)+1)&\"-\"&MID(U37,3,2)+2),VALUE(LEFT(U37,4)+1))","v":"2042-43"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C37:C43)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C51,4)+1)&\"-\"&MID(C51,3,2)+2),VALUE(LEFT(C51,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D51,4)+1)&\"-\"&MID(D51,3,2)+2),VALUE(LEFT(D51,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E51,4)+1)&\"-\"&MID(E51,3,2)+2),VALUE(LEFT(E51,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F51,4)+1)&\"-\"&MID(F51,3,2)+2),VALUE(LEFT(F51,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G51,4)+1)&\"-\"&MID(G51,3,2)+2),VALUE(LEFT(G51,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H51,4)+1)&\"-\"&MID(H51,3,2)+2),VALUE(LEFT(H51,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I51,4)+1)&\"-\"&MID(I51,3,2)+2),VALUE(LEFT(I51,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J51,4)+1)&\"-\"&MID(J51,3,2)+2),VALUE(LEFT(J51,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K51,4)+1)&\"-\"&MID(K51,3,2)+2),VALUE(LEFT(K51,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L51,4)+1)&\"-\"&MID(L51,3,2)+2),VALUE(LEFT(L51,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M51,4)+1)&\"-\"&MID(M51,3,2)+2),VALUE(LEFT(M51,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N51,4)+1)&\"-\"&MID(N51,3,2)+2),VALUE(LEFT(N51,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O51,4)+1)&\"-\"&MID(O51,3,2)+2),VALUE(LEFT(O51,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P51,4)+1)&\"-\"&MID(P51,3,2)+2),VALUE(LEFT(P51,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q51,4)+1)&\"-\"&MID(Q51,3,2)+2),VALUE(LEFT(Q51,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R51,4)+1)&\"-\"&MID(R51,3,2)+2),VALUE(LEFT(R51,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S51,4)+1)&\"-\"&MID(S51,3,2)+2),VALUE(LEFT(S51,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T51,4)+1)&\"-\"&MID(T51,3,2)+2),VALUE(LEFT(T51,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U51,4)+1)&\"-\"&MID(U51,3,2)+2),VALUE(LEFT(U51,4)+1))","v":"2042-43"}]
[null,"Consumption - Opex",null,null,null,545667.44999999995,581000.64,601368.02,1481999.43,1563993.11,1576713.63,1677415.73,1728563.45,1709627.65,1728854,1724716.23,1736431.26,1748380.6,1724945.96,1724945.96,1724945.96,1724945.96]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C52:C66)","v":0},{"$f":"SUM(D52:D66)","v":0},0,545667.44999999995,581000.64,601368.02,1481999.43,1563993.11,1576713.63,1677415.73,1728563.45,1709627.65,1728854,1724716.23,1736431.26,1748380.6,1724945.96,1724945.96,1724945.96,1724945.96]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C71,4)+1)&\"-\"&MID(C71,3,2)+2),VALUE(LEFT(C71,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D71,4)+1)&\"-\"&MID(D71,3,2)+2),VALUE(LEFT(D71,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E71,4)+1)&\"-\"&MID(E71,3,2)+2),VALUE(LEFT(E71,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F71,4)+1)&\"-\"&MID(F71,3,2)+2),VALUE(LEFT(F71,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G71,4)+1)&\"-\"&MID(G71,3,2)+2),VALUE(LEFT(G71,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H71,4)+1)&\"-\"&MID(H71,3,2)+2),VALUE(LEFT(H71,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I71,4)+1)&\"-\"&MID(I71,3,2)+2),VALUE(LEFT(I71,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J71,4)+1)&\"-\"&MID(J71,3,2)+2),VALUE(LEFT(J71,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K71,4)+1)&\"-\"&MID(K71,3,2)+2),VALUE(LEFT(K71,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L71,4)+1)&\"-\"&MID(L71,3,2)+2),VALUE(LEFT(L71,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M71,4)+1)&\"-\"&MID(M71,3,2)+2),VALUE(LEFT(M71,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N71,4)+1)&\"-\"&MID(N71,3,2)+2),VALUE(LEFT(N71,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O71,4)+1)&\"-\"&MID(O71,3,2)+2),VALUE(LEFT(O71,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P71,4)+1)&\"-\"&MID(P71,3,2)+2),VALUE(LEFT(P71,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q71,4)+1)&\"-\"&MID(Q71,3,2)+2),VALUE(LEFT(Q71,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R71,4)+1)&\"-\"&MID(R71,3,2)+2),VALUE(LEFT(R71,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S71,4)+1)&\"-\"&MID(S71,3,2)+2),VALUE(LEFT(S71,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T71,4)+1)&\"-\"&MID(T71,3,2)+2),VALUE(LEFT(T71,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U71,4)+1)&\"-\"&MID(U71,3,2)+2),VALUE(LEFT(U71,4)+1))","v":"2042-43"}]
[null,"Export Services - Opex",null,null,921572.9,1263128.2,1395767.3,1593211.2,1719678.3,1844310.54,1966676.73,2087909.9,2209143.08,2329243.23,2329243.23,2329243.23,2329243.23,2329243.23,2329243.23,2329243.23,2329243.23,2329243.23]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C72:C86)","v":0},{"$f":"SUM(D72:D86)","v":0},{"$f":"SUM(E72:E86)","v":921572.9},{"$f":"SUM(F72:F86)","v":1263128.2},{"$f":"SUM(G72:G86)","v":1395767.3},{"$f":"SUM(H72:H86)","v":1593211.2},{"$f":"SUM(I72:I86)","v":1719678.3},{"$f":"SUM(J72:J86)","v":1844310.54},{"$f":"SUM(K72:K86)","v":1966676.73},{"$f":"SUM(L72:L86)","v":2087909.9},{"$f":"SUM(M72:M86)","v":2209143.08},{"$f":"SUM(N72:N86)","v":2329243.23},{"$f":"SUM(O72:O86)","v":2329243.23},{"$f":"SUM(P72:P86)","v":2329243.23},{"$f":"SUM(Q72:Q86)","v":2329243.23},{"$f":"SUM(R72:R86)","v":2329243.23},{"$f":"SUM(S72:S86)","v":2329243.23},{"$f":"SUM(T72:T86)","v":2329243.23},{"$f":"SUM(U72:U86)","v":2329243.23},{"$f":"SUM(V72:V86)","v":2329243.23}]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2025"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C91,4)+1)&\"-\"&MID(C91,3,2)+2),VALUE(LEFT(C91,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D91,4)+1)&\"-\"&MID(D91,3,2)+2),VALUE(LEFT(D91,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E91,4)+1)&\"-\"&MID(E91,3,2)+2),VALUE(LEFT(E91,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F91,4)+1)&\"-\"&MID(F91,3,2)+2),VALUE(LEFT(F91,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G91,4)+1)&\"-\"&MID(G91,3,2)+2),VALUE(LEFT(G91,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H91,4)+1)&\"-\"&MID(H91,3,2)+2),VALUE(LEFT(H91,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I91,4)+1)&\"-\"&MID(I91,3,2)+2),VALUE(LEFT(I91,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J91,4)+1)&\"-\"&MID(J91,3,2)+2),VALUE(LEFT(J91,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K91,4)+1)&\"-\"&MID(K91,3,2)+2),VALUE(LEFT(K91,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L91,4)+1)&\"-\"&MID(L91,3,2)+2),VALUE(LEFT(L91,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M91,4)+1)&\"-\"&MID(M91,3,2)+2),VALUE(LEFT(M91,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N91,4)+1)&\"-\"&MID(N91,3,2)+2),VALUE(LEFT(N91,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O91,4)+1)&\"-\"&MID(O91,3,2)+2),VALUE(LEFT(O91,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P91,4)+1)&\"-\"&MID(P91,3,2)+2),VALUE(LEFT(P91,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q91,4)+1)&\"-\"&MID(Q91,3,2)+2),VALUE(LEFT(Q91,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R91,4)+1)&\"-\"&MID(R91,3,2)+2),VALUE(LEFT(R91,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S91,4)+1)&\"-\"&MID(S91,3,2)+2),VALUE(LEFT(S91,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T91,4)+1)&\"-\"&MID(T91,3,2)+2),VALUE(LEFT(T91,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U91,4)+1)&\"-\"&MID(U91,3,2)+2),VALUE(LEFT(U91,4)+1))","v":"2042-43"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C92:C106)","v":0},{"$f":"SUM(D92:D106)","v":0},{"$f":"SUM(E92:E106)","v":0},{"$f":"SUM(F92:F106)","v":0},{"$f":"SUM(G92:G106)","v":0},{"$f":"SUM(H92:H106)","v":0},{"$f":"SUM(I92:I106)","v":0},{"$f":"SUM(J92:J106)","v":0},{"$f":"SUM(K92:K106)","v":0},{"$f":"SUM(L92:L106)","v":0},{"$f":"SUM(M92:M106)","v":0},{"$f":"SUM(N92:N106)","v":0},{"$f":"SUM(O92:O106)","v":0},{"$f":"SUM(P92:P106)","v":0},{"$f":"SUM(Q92:Q106)","v":0},{"$f":"SUM(R92:R106)","v":0},{"$f":"SUM(S92:S106)","v":0},{"$f":"SUM(T92:T106)","v":0},{"$f":"SUM(U92:U106)","v":0},{"$f":"SUM(V92:V106)","v":0}]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C114,4)+1)&\"-\"&MID(C114,3,2)+2),VALUE(LEFT(C114,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D114,4)+1)&\"-\"&MID(D114,3,2)+2),VALUE(LEFT(D114,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E114,4)+1)&\"-\"&MID(E114,3,2)+2),VALUE(LEFT(E114,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F114,4)+1)&\"-\"&MID(F114,3,2)+2),VALUE(LEFT(F114,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G114,4)+1)&\"-\"&MID(G114,3,2)+2),VALUE(LEFT(G114,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H114,4)+1)&\"-\"&MID(H114,3,2)+2),VALUE(LEFT(H114,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I114,4)+1)&\"-\"&MID(I114,3,2)+2),VALUE(LEFT(I114,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J114,4)+1)&\"-\"&MID(J114,3,2)+2),VALUE(LEFT(J114,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K114,4)+1)&\"-\"&MID(K114,3,2)+2),VALUE(LEFT(K114,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L114,4)+1)&\"-\"&MID(L114,3,2)+2),VALUE(LEFT(L114,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M114,4)+1)&\"-\"&MID(M114,3,2)+2),VALUE(LEFT(M114,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N114,4)+1)&\"-\"&MID(N114,3,2)+2),VALUE(LEFT(N114,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O114,4)+1)&\"-\"&MID(O114,3,2)+2),VALUE(LEFT(O114,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P114,4)+1)&\"-\"&MID(P114,3,2)+2),VALUE(LEFT(P114,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q114,4)+1)&\"-\"&MID(Q114,3,2)+2),VALUE(LEFT(Q114,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R114,4)+1)&\"-\"&MID(R114,3,2)+2),VALUE(LEFT(R114,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S114,4)+1)&\"-\"&MID(S114,3,2)+2),VALUE(LEFT(S114,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T114,4)+1)&\"-\"&MID(T114,3,2)+2),VALUE(LEFT(T114,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U114,4)+1)&\"-\"&MID(U114,3,2)+2),VALUE(LEFT(U114,4)+1))","v":"2042-43"}]
[null,"ST Incremental MW",null,null,2.2000000000000002,1.2,1.93,1.1499999999999999,0.55000000000000004,1.41,1.44,0.89,1.25,1.42,1.55,1.79,1.94,1.53,2.42,1.1299999999999999,1.94,1.77]
[null,"HV Bus Incremental MW",null,null,2.14,1.17,1.88,1.1200000000000001,0.53,1.37,1.4,0.87,1.22,1.38,1.51,1.74,1.89,1.49,2.36,1.1000000000000001,1.89,1.72]
[null,"HV line Incremental MW",null,null,5.3,2.9,4.66,2.78,1.32,3.4,3.46,2.16,3.02,3.41,3.73,4.3099999999999996,4.6900000000000004,3.69,5.84,2.73,4.68,4.26]
[null,"LV Bus Incremental MW",null,null,24.34,13.32,21.4,12.77,6.08,15.65,15.92,9.91,13.9,15.69,17.16,19.809999999999999,21.54,16.97,26.84,12.54,21.5,19.57]
[null,"LV line Incremental MW",null,null,65.66,35.92,57.72,34.450000000000003,16.399999999999999,42.21,42.94,26.73,37.479999999999997,42.33,46.28,53.44,58.1,45.77,72.38,33.82,57.99,52.79]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C115:C124)","v":0},{"$f":"-SUM(D115:D124)","v":0},-99.64,-54.510000000000005,-87.59,-52.27,-24.88,-64.039999999999992,-65.16,-40.56,-56.87,-64.22999999999999,-70.23,-81.09,-88.16,-69.45,-109.84,-51.32,-88,-80.11]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C129,4)+1)&\"-\"&MID(C129,3,2)+2),VALUE(LEFT(C129,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D129,4)+1)&\"-\"&MID(D129,3,2)+2),VALUE(LEFT(D129,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E129,4)+1)&\"-\"&MID(E129,3,2)+2),VALUE(LEFT(E129,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F129,4)+1)&\"-\"&MID(F129,3,2)+2),VALUE(LEFT(F129,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G129,4)+1)&\"-\"&MID(G129,3,2)+2),VALUE(LEFT(G129,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H129,4)+1)&\"-\"&MID(H129,3,2)+2),VALUE(LEFT(H129,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I129,4)+1)&\"-\"&MID(I129,3,2)+2),VALUE(LEFT(I129,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J129,4)+1)&\"-\"&MID(J129,3,2)+2),VALUE(LEFT(J129,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K129,4)+1)&\"-\"&MID(K129,3,2)+2),VALUE(LEFT(K129,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L129,4)+1)&\"-\"&MID(L129,3,2)+2),VALUE(LEFT(L129,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M129,4)+1)&\"-\"&MID(M129,3,2)+2),VALUE(LEFT(M129,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N129,4)+1)&\"-\"&MID(N129,3,2)+2),VALUE(LEFT(N129,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O129,4)+1)&\"-\"&MID(O129,3,2)+2),VALUE(LEFT(O129,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P129,4)+1)&\"-\"&MID(P129,3,2)+2),VALUE(LEFT(P129,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q129,4)+1)&\"-\"&MID(Q129,3,2)+2),VALUE(LEFT(Q129,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R129,4)+1)&\"-\"&MID(R129,3,2)+2),VALUE(LEFT(R129,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S129,4)+1)&\"-\"&MID(S129,3,2)+2),VALUE(LEFT(S129,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T129,4)+1)&\"-\"&MID(T129,3,2)+2),VALUE(LEFT(T129,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U129,4)+1)&\"-\"&MID(U129,3,2)+2),VALUE(LEFT(U129,4)+1))","v":"2042-43"}]
[null,"Incremental export between 10 - 4pm for systems below 30 kW kWh",null,null,28321551,27709940,27467392,30167285,28938802,31416364,34237573,35800034,39083727,39413689,43077748,46490333,46722225,49736632,52291867,54694027,52895389,54965997]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C130:C139)","v":0},{"$f":"-SUM(D130:D139)","v":0},{"$f":"-SUM(E130:E139)","v":-28321551},{"$f":"-SUM(F130:F139)","v":-27709940},{"$f":"-SUM(G130:G139)","v":-27467392},{"$f":"-SUM(H130:H139)","v":-30167285},{"$f":"-SUM(I130:I139)","v":-28938802},{"$f":"-SUM(J130:J139)","v":-31416364},{"$f":"-SUM(K130:K139)","v":-34237573},{"$f":"-SUM(L130:L139)","v":-35800034},{"$f":"-SUM(M130:M139)","v":-39083727},{"$f":"-SUM(N130:N139)","v":-39413689},{"$f":"-SUM(O130:O139)","v":-43077748},{"$f":"-SUM(P130:P139)","v":-46490333},{"$f":"-SUM(Q130:Q139)","v":-46722225},{"$f":"-SUM(R130:R139)","v":-49736632},{"$f":"-SUM(S130:S139)","v":-52291867},{"$f":"-SUM(T130:T139)","v":-54694027},{"$f":"-SUM(U130:U139)","v":-52895389},{"$f":"-SUM(V130:V139)","v":-54965997}]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C144,4)+1)&\"-\"&MID(C144,3,2)+2),VALUE(LEFT(C144,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D144,4)+1)&\"-\"&MID(D144,3,2)+2),VALUE(LEFT(D144,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E144,4)+1)&\"-\"&MID(E144,3,2)+2),VALUE(LEFT(E144,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F144,4)+1)&\"-\"&MID(F144,3,2)+2),VALUE(LEFT(F144,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G144,4)+1)&\"-\"&MID(G144,3,2)+2),VALUE(LEFT(G144,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H144,4)+1)&\"-\"&MID(H144,3,2)+2),VALUE(LEFT(H144,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I144,4)+1)&\"-\"&MID(I144,3,2)+2),VALUE(LEFT(I144,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J144,4)+1)&\"-\"&MID(J144,3,2)+2),VALUE(LEFT(J144,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K144,4)+1)&\"-\"&MID(K144,3,2)+2),VALUE(LEFT(K144,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L144,4)+1)&\"-\"&MID(L144,3,2)+2),VALUE(LEFT(L144,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M144,4)+1)&\"-\"&MID(M144,3,2)+2),VALUE(LEFT(M144,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N144,4)+1)&\"-\"&MID(N144,3,2)+2),VALUE(LEFT(N144,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O144,4)+1)&\"-\"&MID(O144,3,2)+2),VALUE(LEFT(O144,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P144,4)+1)&\"-\"&MID(P144,3,2)+2),VALUE(LEFT(P144,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q144,4)+1)&\"-\"&MID(Q144,3,2)+2),VALUE(LEFT(Q144,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R144,4)+1)&\"-\"&MID(R144,3,2)+2),VALUE(LEFT(R144,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S144,4)+1)&\"-\"&MID(S144,3,2)+2),VALUE(LEFT(S144,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T144,4)+1)&\"-\"&MID(T144,3,2)+2),VALUE(LEFT(T144,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U144,4)+1)&\"-\"&MID(U144,3,2)+2),VALUE(LEFT(U144,4)+1))","v":"2042-43"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C145:C154)","v":0},{"$f":"-SUM(D145:D154)","v":0},{"$f":"-SUM(E145:E154)","v":0},{"$f":"-SUM(F145:F154)","v":0},{"$f":"-SUM(G145:G154)","v":0},{"$f":"-SUM(H145:H154)","v":0},{"$f":"-SUM(I145:I154)","v":0},{"$f":"-SUM(J145:J154)","v":0},{"$f":"-SUM(K145:K154)","v":0},{"$f":"-SUM(L145:L154)","v":0},{"$f":"-SUM(M145:M154)","v":0},{"$f":"-SUM(N145:N154)","v":0},{"$f":"-SUM(O145:O154)","v":0},{"$f":"-SUM(P145:P154)","v":0},{"$f":"-SUM(Q145:Q154)","v":0},{"$f":"-SUM(R145:R154)","v":0},{"$f":"-SUM(S145:S154)","v":0},{"$f":"-SUM(T145:T154)","v":0},{"$f":"-SUM(U145:U154)","v":0},{"$f":"-SUM(V145:V154)","v":0}]

{"sheet":"7.8 Export Services","index":28,"n_rows":57,"n_cols":9,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2025-26 TO 2029-30"}]
[null,"7.8 EXPORT SERVICES"]
[null," TEMPLATE DATE - OCTOBER 2023 - FINAL RIN"]
[]
[null,"Expenditure must only be related to DER integration, and must exclude amounts relating to DMIA"]
[]
[null,"Export service related overvoltage complaint management\nexamples include but not limited to: complaint processing, analysis, transformer tapping "]
[]
[null,"7.8.1 - OPEX FOR PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"Export service related overvoltage complaint management","                                   -   ","                                   -  ","                                   -  ","                                   -  ","                                   -  ","                                   -  ","                                   -  "]
[null,"Other opex","                                   -  ","                                   -  ",1932693,2422948,2707212,3053917,3283615]
[]
[]
[null,"ICT capex\nexamples include but not limited to: establishing systems for network visibility, hosting capacity assessments, generation of dynamic operating envelopes"]
[null,"Network monitoring capex\nexamples include but not limited to: implementing transformer monitors"]
[]
[null,"7.8.2 - CAPEX FOR THE PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2025)"}]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"ICT capex","                                   -   ","                                   -  ",3733010,4272936,1933632,1905767,1637949]
[null,"Network monitoring capex","                                   -  ","                                   -  ",2288048,2644383,412123,377448,365925]
[null,"Other capex",9224375,6261121,29093979,10494380,14171780,8308901,9064876]
[]
[]
[]
[]
[null,"7.8.3 - EXPORT VOLUMES - NET METERED VOLUME OF ENERGY EXPORTED"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"VOLUMES\nMWh"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},1858,1956,2054,2222,2379,2547,2705]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1289513,1357058,1425427,1541709,1650985,1767340,1877430]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},449489,473033,496865,537398,575489,616047,654421]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},347693,365906,384340,415693,445158,476531,506215]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},{"$f":"SUM(C35:C38)","v":2088553},{"$f":"SUM(D35:D38)","v":2197953},2308686,2497022,2674011,2862465,3040771]
[]
[]
[null,"7.8.4 EXPORT SERVICES - CUSTOMER NUMBERS"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"CUSTOMER NUMBERS"]
[null,null,{"$f":"CRCP_y4","v":"2023-24"},{"$f":"CRCP_y5","v":"2024-25"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"FRCP_y2","v":"2026-27"},{"$f":"FRCP_y3","v":"2027-28"},{"$f":"FRCP_y4","v":"2028-29"},{"$f":"FRCP_y5","v":"2029-30"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},299,{"$f":"C53","v":322},{"$f":"D53","v":340},356,370,383,395]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},238184,{"$f":"C54","v":256306},{"$f":"D54","v":270571},283765,294837,304868,314442]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},58951,{"$f":"C55","v":63436},66967,70232,72973,75455,77825]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},49584,{"$f":"C56","v":53357},56326,59073,61378,63466,65459]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C57,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},322,340,356,370,383,395,407]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},256306,270571,283765,294837,304868,314442,323869]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},63436,66967,70232,72973,75455,77825,80158]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},53357,56326,59073,61378,63466,65459,67422]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]

{"sheet":"AER Sheet Heading","index":29,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"dms_Header_Span","v":"2022-23 to 2029-30"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2025)"}]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C15:C35)","v":0},{"$f":"SUM(D15:D35)","v":0},0,0,0,0,0]
[null,null,{"$f":"SUM(C15:C36)","v":0},{"$f":"SUM(D15:D36)","v":0},0,0,0,0,0]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C46:C66)","v":0},{"$f":"SUM(D46:D66)","v":0},{"$f":"SUM(E46:E66)","v":0},{"$f":"SUM(F46:F66)","v":0},{"$f":"SUM(G46:G66)","v":0},{"$f":"SUM(H46:H66)","v":0},{"$f":"SUM(I46:I66)","v":0}]
[null,null,{"$f":"SUM(C46:C67)","v":0},{"$f":"SUM(D46:D67)","v":0},{"$f":"SUM(E46:E67)","v":0},{"$f":"SUM(F46:F67)","v":0},{"$f":"SUM(G46:G67)","v":0},{"$f":"SUM(H46:H67)","v":0},{"$f":"SUM(I46:I67)","v":0}]

{"sheet":"AER CF","index":30,"n_rows":77,"n_cols":25,"rows_kept":77,"cut":false,"hidden":true,"merged":[[3,1,3,22],[39,38,39,59],[40,38,40,59],[41,38,41,59],[39,69,39,90],[40,69,40,90],[41,69,41,90]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[null,"CELLS FLAGED \"Y\" and greyed out will be greyed out in the worksheets."]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":false},"=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",null,null,"=INDEX(dms_CF_F10, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6.1","dms_CF_3.6.6.2","dms_CF_3.6.6.3","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.8 (set from dms_MAIFI_flag)","dms_CF_7.12","dms_CF_8.1_A  (and 8.4)","dms_CF_8.1_B  (and 8.4)","dms_CF_8.1_Neg  (and 8.4)","dms_CF_4.4.1","dms_CF_MAIFI_flag (set from dms_MAIFI_flag)","9.5 TUOS (set from Jurisdiction)","dms_CF_F10"]
[null,"Amadeus","NT","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"APA GasNet","Vic","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C7=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ausgrid (Tx Assets)","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C8=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C9=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","Y","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C10=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co.","NSW","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C13=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co. (Vic)","Vic","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C14=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C15=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C16=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C17=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C18=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Energex","Qld","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C19=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C20=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C21=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C22=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution (Tx Assets)","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C23=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C25=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"JGN","Vic","Gas","Distribution","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C26=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Power and Water","NT","Electricity","Distribution",null,"N","N",null,null,"N","Y","N","N","N","Y",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","Y","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C27=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C28=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C29=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Roma to Brisbane Pipeline","Qld","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","N","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C31=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C32=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C33=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C34=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"United Energy","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C35=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE","dms_H2"]
[null,"TOP HEADER","dms_H1"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,5.1109999999999998,"dms_NUM"]
[null,5.45E-2,"dms_NUM%"]
[null,5.5555000000000003,"dms_NUM3d"]
[null,"Text description","dms_Row_Locked"]
[null,"Text description - not locked","dms_Row1"]
[null,"Text description","dms_Row2"]
[null,"Total","dms_T1"]
[null,"Total","dms_T2"]
[null,"EXPENSES","dms_BH"]
[null,2019,"dms_BY1"]
[null,2019,"dms_BY2"]
[null,"VOLUMES","dms_GH"]
[null,2019,"dms_GY1"]
[null,2019,"dms_GY2"]

{"sheet":"AER NRs","index":31,"n_rows":232,"n_cols":16,"rows_kept":232,"cut":false,"hidden":true,"merged":[[33,67,33,88],[34,67,34,88],[35,67,35,88],[36,10,40,10],[44,10,45,10],[33,10,35,10],[33,36,33,57],[34,36,34,57],[35,36,35,57],[208,1,213,1],[199,1,200,1],[32,1,55,1],[100,1,107,1],[110,1,115,1],[191,1,192,1],[195,1,196,1],[160,1,174,1],[4,1,28,1],[176,1,177,1],[179,1,184,1],[65,1,78,1],[135,1,150,1],[84,1,97,1],[152,1,158,1],[118,1,132,1]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Tariff cap"]
[null,null,"Final decision","Weighted average price cap"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Reallocated"]
[null,null,"Recast"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[null,null,null,null,null,null,null,null,null,null,null,null,"GAS ARR & RESET"]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140201_UOM","dms_E050201_UOM","dms_E050202_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number per km","per metre per connection","metres per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","per service per connection","number per connection"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number per connection","number per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","dms_E020202_UOM","Spare"]
[null,null,"number","number","Length of mains replaced"]
[null,null,"number","number","Number of services replaced"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)",""]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":{"$error":"#NAME?"}}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]
[]
[]
[]
[null,"PTRM input sheet","DMS_50_01_01a","DMS_50_01_01aa","DMS_50_01_01b","DMS_50_01_01bb","DMS_50_01_01c","DMS_50_01_01d","DMS_50_01_01dd"]

{"sheet":"AER lookups","index":32,"n_rows":101,"n_cols":37,"rows_kept":101,"cut":false,"hidden":true,"merged":[[17,60,17,81],[22,1,22,4],[4,24,4,35],[5,24,5,27],[5,29,7,33],[5,34,7,34],[5,35,7,35],[5,36,7,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Template number",5]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_MAIFI_flag_List","dms_Public_Lighting_List","Name"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Australian Distribution Co."]
[null,"Australian Transmission Co.","Australian Transmission Co.",11222333444,"NSW","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Australian Transmission Co."]
[null,"Directlink","Directlink",16779340889,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"Level 25","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO",{"$f":"B12","v":"Directlink"}]
[null,"ElectraNet","ElectraNet",41094482416,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"52-55 East Terrace","Rymill Park","ADELAIDE","SA",5000,"PO Box 7096","Hutt Street Post Office","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","ElectraNet"]
[null,"Energex","Energex",40078849055,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"26 Reddacliff Street",null,"NEWSTEAD","Qld",4006,"26 Reddacliff Street",null,"NEWSTEAD","QLD",4006,"YES","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Energex"]
[null,"Ergon Energy","Ergon Energy",50087646062,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"22 Walker Street",null,"TOWNSVILLE","Qld",4810,"Po Box 264",null,"FORTITUDE VALLEY","QLD",4006,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Ergon Energy"]
[null,"Murraylink","Murraylink",79181207909,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Murraylink"]
[null,"Powerlink","Queensland Electricity Transmission Corporation Limited trading as Powerlink Queensland",82078849233,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,5,"33 Harold St",null,"VIRGINIA","Qld",4014,"PO Box 1193",null,"VIRGINIA","QLD",4014,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Powerlink"]
[null,"SA Power Networks","SA Power Networks",13332330749,"SA","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"1 Anzac Highway",null,"KESWICK","SA",5035,"GPO Box 77",null,"ADELAIDE","SA",5000,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","SA Power Networks"]
[]
[]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"EBSS","Efficiency Benefit Sharing Scheme","EFFICIENCY BENEFIT SHARING SCHEME",5]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"Profitability","Profitability","PROFITABILITY",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88",1988,"PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2015-16"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2020-21"},{"$f":"FRCP_y1","v":"2025-26"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2025-26"}]
[null,"1988-89",1989,"PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2016-17"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2021-22"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2026-27"}]
[null,"1989-90",1990,"PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2017-18"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2022-23"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2027-28"}]
[null,"1990-91",1991,"PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2018-19"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2023-24"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2028-29"}]
[null,"1991-92",1992,"PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2019-20"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2024-25"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2029-30"}]
[null,"1992-93",1993,"PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2020-21"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2025-26"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2030-31"}]
[null,"1993-94",1994,"PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2021-22"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2026-27"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2031-32"}]
[null,"1994-95",1995,"PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2022-23"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2027-28"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2032-33"}]
[null,"1995-96",1996,"PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2023-24"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2028-29"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2033-34"}]
[null,"1996-97",1997,"PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2024-25"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2029-30"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2034-35"}]
[null,"1997-98",1998,"PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2025-26"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2030-31"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2035-36"}]
[null,"1998-99",1999,"PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2026-27"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2031-32"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2036-37"}]
[null,"1999-00",2000,"PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2027-28"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2032-33"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2037-38"}]
[null,"2000-01",2001,"PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2028-29"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2033-34"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2038-39"}]
[null,"2001-02",2002,"PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2029-30"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2034-35"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2039-40"}]
[null,"2002-03",2003,"PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2030-31"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2035-36"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2040-41"}]
[null,"2003-04",2004,"PRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+16)","v":"2031-32"},"CRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+16)","v":"2036-37"},"FRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+16)","v":"2041-42"}]
[null,"2004-05",2005,"PRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+17)","v":"2032-33"},"CRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+17)","v":"2037-38"},"FRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+17)","v":"2042-43"}]
[null,"2005-06",2006,"PRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+18)","v":"2033-34"},"CRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+18)","v":"2038-39"},"FRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+18)","v":"2043-44"}]
[null,"2006-07",2007,"PRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+19)","v":"2034-35"},"CRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+19)","v":"2039-40"},"FRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+19)","v":"2044-45"}]
[null,"2007-08",2008,"PRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+20)","v":"2035-36"},"CRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+20)","v":"2040-41"},"FRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+20)","v":"2045-46"}]
[null,"2008-09",2009,"PRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+21)","v":"2036-37"},"CRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+21)","v":"2041-42"},"FRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+21)","v":"2046-47"}]
[null,"2009-10",2010,"PRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+22)","v":"2037-38"},"CRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+22)","v":"2042-43"},"FRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+22)","v":"2047-48"}]
[null,"2010-11",2011,"PRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+23)","v":"2038-39"},"CRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+23)","v":"2043-44"},"FRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+23)","v":{"$error":"#REF!"}}]
[null,"2011-12",2012,"PRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+24)","v":"2039-40"},"CRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+24)","v":"2044-45"},"FRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+24)","v":{"$error":"#REF!"}}]
[null,"2012-13",2013]
[null,"2013-14",2014]
[null,"2014-15",2015]
[null,"2015-16",2016]
[null,"2016-17",2017]
[null,"2017-18",2018]
[null,"2018-19",2019]
[null,"2019-20",2020]
[null,"2020-21",2021]
[null,"2021-22",2022,null,"CRY - FRY"]
[null,"2022-23",2023,"dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2022-23"}]
[null,"2023-24",2024,"dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2023-24"}]
[null,"2024-25",2025,"dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2024-25"}]
[null,"2025-26",2026,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2025-26"}]
[null,"2026-27",2027,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2026-27"}]
[null,"2027-28",2028,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2027-28"}]
[null,"2028-29",2029,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2028-29"}]
[null,"2029-30",2030,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2029-30"}]
[null,"2030-31",2031,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2030-31"}]
[null,"2031-32",2032,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2031-32"}]
[null,"2032-33",2033,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2032-33"}]
[null,"2033-34",2034,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2033-34"}]
[null,"2034-35",2035,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2034-35"}]
[null,"2035-36",2036,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2035-36"}]
[null,"2036-37",2037,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2036-37"}]
[null,"2037-38",2038,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2037-38"}]
[null,"2038-39",2039,"dms_y17",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+16),0)","v":"2038-39"}]
[null,"2039-40",2040,"dms_y18",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+17),0)","v":"2039-40"}]
[null,"2040-41",2041,"dms_y19",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+18),0)","v":"2040-41"}]
[null,"2041-42",2042,"dms_y20",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+19),0)","v":"2041-42"}]
[null,"2042-43",2043,"dms_y21",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+20),0)","v":"2042-43"}]
[null,"2043-44",2044,"dms_y22",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+21),0)","v":"2043-44"}]
[null,"2044-45",2045,"dms_y23",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+22),0)","v":"2044-45"}]
[null,"2045-46",2046,"dms_y24",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+23),0)","v":"2045-46"}]
[null,"2046-47",2047,"dms_y25",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+24),0)","v":"2046-47"}]
[null,"2047-48",2048,"dms_y26",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+25),0)","v":"2047-48"}]

{"sheet":"AER ETL","index":33,"n_rows":145,"n_cols":10,"rows_kept":145,"cut":false,"hidden":true,"merged":[[32,37,32,58],[33,37,33,58],[34,37,34,58],[32,68,32,89],[33,68,33,89],[34,68,34,89],[12,4,12,8],[71,1,73,1],[11,0,15,0],[18,0,25,0],[26,0,31,0],[34,0,59,0],[14,2,14,4]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"SA Power Networks"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Regulatory proposal","dms_Source",{"$f":"IF(dms_Model=\"Reset\", \"Make sure you have set Reg Proposal as source\",\"\")","v":"Make sure you have set Reg Proposal as source"}]
[null,"Data quality","Consolidated","For DB purposes this is always Consoldiated"]
[null,"Data status","Public","For DB purposes this is always Public"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"31/01/2024"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality","Consolidated","dms_DataQuality","Always Consolidated"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)","v":"2030"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)"]
[null,"Reporting Period Type","Financial","dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM",{"$f":"IF(dms_SingleYearModel=\"yes\",\"This is set to an historical template (EB, CA or ARR), apply UOM Named Range to cell !\",\"This is not an historical template, make sure UOM Named Range is not applied\")","v":"This is not an historical template, make sure UOM Named Range is not applied"},null,null,null,null,{"$f":"IFERROR(dms_dollar_nom_UOM, \"NR not applied\")","v":"NR not applied"}]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"2022-23"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"2022"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))","v":"June 2025"},"dms_DollarReal","=IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year","v":"June 2020"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2025-26"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2022-23"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":36},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":39},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":34},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":29},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":43},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2020-21"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2015-16"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2029-30"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2024-25"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2019-20"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2029-30"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2028-29"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2025"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2020"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":"2023"},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2030"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2030"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2025-26 to 2029-30"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_y1&\" to \"&FRCP_final_year,CRY))","v":"2022-23 to 2029-30"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"2022-23"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2029-30"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C50,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"2022-23"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(dms_SingleYearModel=\"yes\",(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(PRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(PRCP_y4,4))))","v":"1-Jul-2018"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060101_StartDateTxt)","v":43282},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"Does the NSP report MAIFI or MAIFIe",{"$f":"INDEX(dms_MAIFI_flag_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_MAIFI_Flag"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes","Must be present for ARRs","=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","0","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2017"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]