{"text_format":"1","workbook":"xlsx","n_sheets":34,"sheets":["Instructions","CONTENTS","Business & other details","2.1 Expenditure summary","2.2 Repex","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","5.4 MD & utilisation-Spatial","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.7 TSS-LRMC","7.8 Export Services","AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":901,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[13,2,13,4],[16,2,16,4],[10,1,11,1],[10,2,10,3],[11,2,11,4],[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List)),\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by AusNet Electricity Services Pty Ltd to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nBusinesses must use the macro at the top of  \neach worksheet to identify confidential\ninformation in the workbook.\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the NON-CONFIDENTIAL macro."]
[]
[null,"PROTECTED (SOCI) INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify information in the \nconfidential workbook that is protected \ninformation under the SOCI Act. All \ninformation marked Protected (SOCI) is also \ndeemed to be confidential information."]
[null,null,"-Do this by selecting the cell or cells that contain protected information and then run the PROTECTED (SOCI) macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as protected..\n\n-To reverse this, select the cell or cells and run the NON-PROTECTED macro."]
[]
[null,"RESPONSES","\nPlease return locked template files as provided by AER,with confidential/protected information marked using the appropriate macro. \n\n"]
[]
[]
[null,"ORDER OF MAGNITUDE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. \n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," PLEASE DO NOT ENTER TEXT into cells that are to contain numbers \n(including 'numbers stored as text')"]

{"sheet":"CONTENTS","index":1,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[[6,3,6,4],[8,3,8,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"DRAFT RIN ONLY - DO NOT USE FOR SUBMISSION"]
[]
[null,null,null,"TEMPLATE","MARCH 2024 - PRELIMINARY RIN"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 FORECAST price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[null,null,null,null,"7.8 Export Services"]

{"sheet":"Business & other details","index":2,"n_rows":77,"n_cols":81,"rows_kept":77,"cut":false,"hidden":false,"merged":[[10,16,10,93],[11,16,11,93],[18,37,18,58],[27,37,27,51],[19,37,19,48],[0,7,2,15],[6,21,6,75],[27,21,27,35],[45,37,45,44],[45,46,45,53],[45,55,45,62],[45,64,45,71],[3,21,3,57],[8,16,8,93],[26,68,26,89],[28,68,28,71],[28,80,28,82],[27,68,27,82],[28,37,28,40],[25,37,25,58],[28,49,28,51],[28,60,28,66],[18,21,18,35],[19,21,19,35],[48,25,48,34],[44,55,44,62],[44,64,44,71],[46,64,46,71],[52,25,52,34],[48,73,48,80],[48,64,48,71],[49,73,49,80],[48,55,48,62],[25,21,25,35],[25,60,25,66],[26,60,26,66],[34,60,34,66],[26,37,26,58],[25,68,25,89],[46,73,46,80],[44,73,44,80],[28,21,28,35],[26,21,26,35],[45,73,45,80],[35,21,35,35],[36,21,36,35],[36,60,36,66],[35,60,35,66],[34,21,34,35],[34,68,34,89],[44,25,44,34],[27,60,27,66],[35,68,35,89],[36,68,36,89],[34,37,34,58],[44,46,44,53],[56,25,56,34],[48,46,48,53],[48,37,48,44],[52,37,52,44],[50,73,50,80],[54,73,54,80],[52,73,52,80],[56,37,56,44],[52,46,52,53],[53,46,53,53],[49,46,49,53],[49,37,49,44],[54,64,54,71],[50,46,50,53],[53,55,53,62],[50,37,50,44],[53,37,53,44],[52,64,52,71],[50,64,50,71],[52,55,52,62],[50,55,50,62],[49,64,49,71],[49,55,49,62],[54,55,54,62],[76,25,76,34],[76,37,76,52],[58,25,58,34],[66,25,66,34],[68,25,68,34],[58,37,58,44],[64,25,64,34],[64,37,64,52],[35,37,35,58],[36,37,36,58],[46,37,46,44],[46,46,46,53],[46,55,46,62],[44,37,44,44],[66,37,66,52],[68,37,68,52],[70,37,70,52],[72,37,74,81],[70,25,70,34],[72,25,74,34],[54,46,54,53],[54,37,54,44],[53,73,53,80],[53,64,53,71]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRAFT TEMPLATE ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DO NOT USE FOR SUBMISSIONS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AusNet (D)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":91064651118}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Level 32\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,"Level 32"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 Southbank Boulevard",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,"2 Southbank Boulevard\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOUTHBANK\t\t\t\t\t\t\t\t\t\t\t\t\t\t",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,"SOUTHBANK\t\t\t\t\t\t\t\t\t\t\t\t\t\t"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},null,null,null,null,null,null,null,null,null,"Post code",null,3006,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},null,null,null,null,null,null,null,null,null,"Post code",null,3006]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2026-27",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2030-31"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2034-35"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2035-36"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2036-37"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2037-38"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2038-39"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2039-40"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2040-41"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2030-31"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2034-35"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2035-36"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2020-21"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2030-31"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2022-23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2028-29"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Regulatory proposal"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Public"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"2025-01-31",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"2.1 Expenditure summary","index":3,"n_rows":127,"n_cols":37,"rows_kept":127,"cut":false,"hidden":false,"merged":[[8,1,9,1],[26,1,27,1],[40,1,41,1],[97,1,98,1],[114,1,115,1],[53,1,54,1],[65,1,66,1],[83,1,84,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX (excluding dual function assets)"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Replacement expenditure",202337645.83202738,182373282.0864667,189927211.81239775,246090263.91853431,292044137.60136026,296490874.72187698,292321337.16585636]
[null,"Connections",152624493.34874564,163524825.65499631,176209034.53184786,165713118.14278477,164081983.53856844,162623482.39045596,163012305.9848423,null,null,null,null,null,null,null,"ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO",{"$f":"B12","v":"Connections"}]
[null,"Augmentation Expenditure",53097372.76516486,56991303.950017229,145041405.39663395,173294951.54451269,193586677.76260912,181686982.70448032,217598167.67457101,null,null,null,null,null,null,null,"ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Augmentation Expenditure"]
[null,"Export services",13057852,4866491.9999999991,{"$f":"SUM('7.8 Export Services'!E24:E26)","v":22738079.075647291},{"$f":"SUM('7.8 Export Services'!F24:F26)","v":20660059.97195654},{"$f":"SUM('7.8 Export Services'!G24:G26)","v":6102959.8240485098},{"$f":"SUM('7.8 Export Services'!H24:H26)","v":35145635.185019903},{"$f":"SUM('7.8 Export Services'!I24:I26)","v":4872036.031709536}]
[null,"ICT",74822064.796950504,66490120.573587686,81492175.880357653,89281461.505135,84716722.974924579,66127821.870889053,65057030.81161999]
[null,"Property",9577478.0397610292,3074459.8585923645,73981666.957825169,30865206.374365617,19568733.815473676,18694641.638046566,30632857.348922793]
[null,"Fleet",1183470.2008500001,3853124.8385267924,25188919.926498096,25273729.094505765,30059774.750529815,32632861.354057297,31069692.779272992]
[null,"Other non-network",1417146.6926343373,8558517.405777676,895786.46942066622,904744.33411487297,913791.77745602163,922929.69523058191,932158.99218288786]
[null,"Network overheads",38775249.079901889,41523505.50461103,41493729.382437669,41604134.089731798,41785724.029504754,42042834.570900127,42219722.445647627]
[null,"Corporate overheads",6603892.8444947237,7072244.7785120914,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"capital contributions (included in the above)",101752968.9089205,105283066.89218506,117752101.08593863,106024669.29738495,102584595.23637715,102210755.61606802,103889366.38410564]
[null,"Total",{"$f":"SUM(C11:C21)","v":553496665.60053039},538327876.65108788,756968009.43306613,793687668.97564149,832860506.07447517,836368064.13095677,847715309.23462558]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY (excluding dual function assets)"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"}]
[null,"Vegetation management",62340245.578933224,58218454.627778918]
[null,"Maintenance",35269803.792722665,32937847.016297016]
[null,"Emergency response",50499806.747079514,24229032.491080444,null," "]
[null,"Non-network",52460938.35051237,48992344.042387314]
[null,"Export services",54068.301049233247,21627.3204196933]
[null,"Metering",4494306,4494306]
[null,"Network overheads",94343640.234860316,88105859.824986294]
[null,"Corporate overheads",32311611.000945505,30175242.999759421]
[null,"Total",{"$f":"SUM(C29:C36)","v":331774420.0061028},{"$f":"SUM(D29:D36)","v":287174714.32270914}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Connections",8708283.8780560829,8864708.6562869549,8992016.3985718023,9057896.0208479017,9151956.4091671854,9271687.6803706232,9362500.76749295]
[null,"Metering",11265347.633035913,9360287.1593412794,17361654.920394383,16534754.744360328,34206856.784653597,48917185.724169217,48976277.91521398]
[null,"Public lighting",{"$f":"SUM('4.1 Public lighting'!D16,'4.1 Public lighting'!D21,'4.1 Public lighting'!D26)","v":10071565.118531734},{"$f":"SUM('4.1 Public lighting'!E16,'4.1 Public lighting'!E21,'4.1 Public lighting'!E26)","v":8330239.7009401955},{"$f":"SUM('4.1 Public lighting'!F16,'4.1 Public lighting'!F21,'4.1 Public lighting'!F26)","v":9332613.1996251047},{"$f":"SUM('4.1 Public lighting'!G16,'4.1 Public lighting'!G21,'4.1 Public lighting'!G26)","v":9486722.0995063037},{"$f":"SUM('4.1 Public lighting'!H16,'4.1 Public lighting'!H21,'4.1 Public lighting'!H26)","v":9647298.211344108},{"$f":"SUM('4.1 Public lighting'!I16,'4.1 Public lighting'!I21,'4.1 Public lighting'!I26)","v":9814660.870401185},{"$f":"SUM('4.1 Public lighting'!J16,'4.1 Public lighting'!J21,'4.1 Public lighting'!J26)","v":9984042.8250676729}]
[null,"Fee and quoted",9634352.70189864,9807412.2284248825,9980780.9687629584,10160063.301708465,10343341.290404728,10530532.19535473,10721897.289966406]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D17","v":2244113.2540260935},{"$f":"'2.10 Overheads'!E17","v":1856902.6088855749},{"$f":"'2.10 Overheads'!F17","v":1870002.1534657835},{"$f":"'2.10 Overheads'!G17","v":1888476.861992287},{"$f":"'2.10 Overheads'!H17","v":2706134.4017950636},{"$f":"'2.10 Overheads'!I17","v":3394046.6049527554},{"$f":"'2.10 Overheads'!J17","v":3415064.9845639369}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D32","v":0},{"$f":"'2.10 Overheads'!E32","v":0},{"$f":"'2.10 Overheads'!F32","v":0},{"$f":"'2.10 Overheads'!G32","v":0},{"$f":"'2.10 Overheads'!H32","v":0},{"$f":"'2.10 Overheads'!I32","v":0},{"$f":"'2.10 Overheads'!J32","v":0}]
[null,"capital contributions (included in the above)",{"$f":"'4.1 Public lighting'!D16","v":4358526.5173333436},{"$f":"'4.1 Public lighting'!E16","v":4480565.2598186778},{"$f":"'4.1 Public lighting'!F16","v":4031427.5915476866},{"$f":"'4.1 Public lighting'!G16","v":4144307.5641110213},{"$f":"'4.1 Public lighting'!H16","v":4260348.1759061301},{"$f":"'4.1 Public lighting'!I16","v":4379637.9248315012},{"$f":"'4.1 Public lighting'!J16","v":4502267.786726784}]
[null,"Total",{"$f":"SUM(C43:C48)","v":41923662.58554846},38219550.353878886,47537067.640820034,47127913.028415285,66055587.097364686,81928113.07524851,82459783.782304943]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Connections",{"$f":"SUM('3.2 Operating expenditure'!C73)","v":5427975.533428343},{"$f":"SUM('3.2 Operating expenditure'!D73)","v":4688284.6665305989},{"$f":"SUM('3.2 Operating expenditure'!E73)","v":5235580.8084106538},{"$f":"SUM('3.2 Operating expenditure'!F73)","v":5370151.3407006143},{"$f":"SUM('3.2 Operating expenditure'!G73)","v":5513867.41459521},{"$f":"SUM('3.2 Operating expenditure'!H73)","v":5668802.5175859164},{"$f":"SUM('3.2 Operating expenditure'!I73)","v":5774190.1565493587}]
[null,"Metering",{"$f":"'3.2 Operating expenditure'!K72","v":12500000},{"$f":"'3.2 Operating expenditure'!L72","v":11910620.869754987},{"$f":"'3.2 Operating expenditure'!M72","v":11321241.739509974},{"$f":"'3.2 Operating expenditure'!N72","v":11619964.875153653},{"$f":"'3.2 Operating expenditure'!O72","v":12374765.280047774},{"$f":"'3.2 Operating expenditure'!P72","v":12982798.983951945},{"$f":"'3.2 Operating expenditure'!Q72","v":13365072.837744256}]
[null,"Public lighting",{"$f":"'3.2 Operating expenditure'!K74","v":4328501.6932231933},{"$f":"'3.2 Operating expenditure'!L74","v":4395084.9111169707},{"$f":"'3.2 Operating expenditure'!M74","v":3601785.6147425449},{"$f":"'3.2 Operating expenditure'!N74","v":3532822.3228559569},{"$f":"'3.2 Operating expenditure'!O74","v":3494894.3245605328},{"$f":"'3.2 Operating expenditure'!P74","v":3487713.2049801005},{"$f":"'3.2 Operating expenditure'!Q74","v":3291368.4255929077}]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D14","v":1306840.7233057984},{"$f":"'2.10 Overheads'!E14","v":1323486.5277792427},{"$f":"'2.10 Overheads'!F14","v":1100353.1536856364},{"$f":"'2.10 Overheads'!G14","v":1088505.4807139891},{"$f":"'2.10 Overheads'!H14","v":1092506.3811401331},{"$f":"'2.10 Overheads'!I14","v":1101497.4512450253},{"$f":"'2.10 Overheads'!J14","v":1059062.8563982269}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D29","v":""},{"$f":"'2.10 Overheads'!E29","v":0},{"$f":"'2.10 Overheads'!F29","v":0},{"$f":"'2.10 Overheads'!G29","v":0},{"$f":"'2.10 Overheads'!H29","v":0},{"$f":"'2.10 Overheads'!I29","v":0},{"$f":"'2.10 Overheads'!J29","v":0}]
[null,"Total",{"$f":"SUM(C56:C61)","v":23563317.949957334},22317476.975181803,21258961.31634881,21611444.019424215,22476033.400343649,23240812.157762986,23489694.276284751]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Export services"]
[null,"ICT"]
[null,"Property"]
[null,"Fleet"]
[null,"Other non-network"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Metering"]
[null,"capital contributions (included in the above)"]
[null,"Total",{"$f":"SUM(C68:C78)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"}]
[null,"Vegetation management",0,0]
[null,"Maintenance",0,0]
[null,"Emergency response",0,0]
[null,"Non-network",0,0]
[null,"Export services",0,0]
[null,"Metering",0,0]
[null,"Network overheads",0,0]
[null,"Corporate overheads",0,0]
[null,"Total",{"$f":"SUM(C86:C93)","v":0},{"$f":"SUM(D86:D93)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES (TOTAL) CAPITAL CONTRIBUTIONS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Replacement expenditure",0,0,0,0,0,0,0]
[null,"Connections",97159783.439607605,99399191.260743797,112254264.38868171,102084954.50472322,99232870.345413983,98974580.6423347,100605400.97402054]
[null,"Augmentation Expenditure",0,0,0,0,0,0,0]
[null,"Export services",0,0,0,0,0,0,0]
[null,"ICT",0,0,0,0,0,0,0]
[null,"Property",0,0,0,0,0,0,0]
[null,"Fleet",0,0,0,0,0,0,0]
[null,"Other non-network",0,0,0,0,0,0,0]
[null,"Network overheads",4593185.4693128895,5883875.6314412709,5497836.6972569311,3939714.7926617265,3351724.890963167,3236174.9737333385,3283965.4100851147]
[null,"Corporate overheads",0,0,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C100:C110)","v":101752968.9089205},105283066.89218506,117752101.08593865,106024669.29738495,102584595.23637715,102210755.61606804,103889366.38410565]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES (TOTAL) CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Replacement expenditure",21771530.691526145,21100588.737404197,16666095.295070155,18833133.228842963,20328043.183260005,20294343.77981291,19834602.774602618]
[null,"Connections",10563891.094666958,13285113.951844277,11109861.870527748,8809138.1652943194,7865616.4698654497,7592844.2793084178,7518402.0176999038]
[null,"Augmentation Expenditure",5713277.3095317399,6593893.8670169925,13717772.216839777,13961862.695594512,13592064.376379298,14155646.511778789,14866717.653345093]
[null,"Export services",1239926.7542000001,561551.93399999989,0,0,0,0,0]
[null,"ICT",6090516.0744717708,7054601.7928576544,0,0,0,0,0]
[null,"Property",0,0,0,0,0,0,0]
[null,"Fleet",0,0,0,0,0,0,0]
[null,"Other non-network",0,0,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"capital contributions (included in the above)",4593185.4693128895,5883875.6314412709,{"$f":"SUM(E108:E109)","v":5497836.6972569311},3939714.7926617265,3351724.890963167,3236174.9737333385,3283965.4100851147]
[null,"Total",{"$f":"SUM(C117:C125)","v":45379141.924396612},48595750.283123121,41493729.382437676,41604134.089731798,41785724.029504754,42042834.570900112,42219722.445647612]

{"sheet":"2.2 Repex","index":4,"n_rows":557,"n_cols":10,"rows_kept":557,"cut":false,"hidden":false,"merged":[[508,1,515,1],[410,1,416,1],[417,1,422,1],[423,1,431,1],[432,1,439,1],[440,1,455,1],[456,1,484,1],[324,1,331,1],[379,1,409,1],[485,1,498,1],[499,1,507,1],[332,1,372,1],[248,1,255,1],[256,1,271,1],[272,1,300,1],[301,1,314,1],[315,1,323,1],[516,1,556,1],[11,1,41,1],[42,1,48,1],[49,1,54,1],[55,1,63,1],[64,1,71,1],[72,1,87,1],[88,1,116,1],[117,1,130,1],[131,1,139,1],[140,1,147,1],[195,1,225,1],[226,1,232,1],[233,1,238,1],[239,1,247,1],[148,1,188,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.2 REPEX"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE; MATERIAL TYPE","˂ = 1 kV; wood",5898159.5463000005,5646755.28452498,8916415.5829982813,8675485.0259472728,8490615.0526424646,8349536.2361249113,8218147.9370505298]
[null,null,"> 1 kV & < = 11 kV; wood",106760.4725,91325.716323456261,112241.85286436413,110292.6409524639,108551.17116765909,107470.37580494661,106412.65269565227]
[null,null,"˃ 11 kV & < = 22 kV; wood",12399947.358999999,11100885.483625874,13518966.899404909,13327566.256957892,13164414.456803642,13086038.323402751,13001318.654774789]
[null,null,"> 22 kV & < = 66 kV; wood",966887.44479999994,942326.17838311428,1206500.8707591479,1226220.2303745013,1251517.4489114219,1262957.2781439612,1283567.4294184675]
[null,null,"> 66 kV & < = 132 kV; wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; concrete",2428835.7579999999,2316836.7706855466,3614852.3019664958,3520183.1810012264,3448279.1095116632,3394155.6059757932,3344059.3930518539]
[null,null,"> 1 kV & < = 11 kV; concrete",36527.156800000004,32581.362372544194,39760.659966709223,39180.607130942371,38682.362810525316,38431.399025936757,38165.379959705984]
[null,null,"˃ 11 kV & < = 22 kV; concrete",10157991.1939,12396684.157992346,18173989.930898968,28757176.552836906,31970901.544922367,35166582.175088249,18228165.786961932]
[null,null,"> 22 kV & < = 66 kV; concrete",1728254.7884000002,1600678.7577168855,1837309.8768812297,1873184.6435099167,1911225.186302009,1928695.250163476,1959867.1547580133]
[null,null,"> 66 kV & < = 132 kV; concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; steel",2373539.5567999999,1969403.6090170254,1518772.3873233537,1586507.0552581993,1665134.0682456025,1752198.2022544846,1844472.7802678111]
[null,null,"> 1 kV & < = 11 kV; steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; steel",1810.4156000000003,1501.2375532386973,1759.1719944160591,1724.432904493164,1692.6380610876604,1670.6956970746269,1649.9960185021953]
[null,null,"> 22 kV & < = 66 kV; steel",0,0,2394.6239653524326,2417.5471393259527,2469.0964343129945,2491.6658691952493,2533.1661394429543]
[null,null,"> 66 kV & < = 132 kV; steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; steel",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV;  composite pole",1649.3132000000003,1573.9456390251823,2906.0543493914738,2827.0001309383788,2766.2111234846043,2719.6894327510267,2676.3095738162547]
[null,null,"> 1 kV & < = 11 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; composite pole",0,-9.2924144900155987,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; composite pole",200156.29829999999,170034.45102058112,200432.40083251658,196689.26616281155,193346.63113728652,191023.79167689392,188878.2995207319]
[null,null,"> 66 kV & < = 132 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"> 132 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 132 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",7210924,7100989.4593547909,3557413.0439892444,3652553.6741871843,3764623.275505227,3899970.3894231417,4033184.1162350359]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",4582646,4465737.3327661883,7124203.0379693368,7346319.0868792776,7590101.893291817,7878072.1096650874,8162849.5176540995]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",256723.99999999994,251756.20787902019,892117.06967570027,915538.82941948145,946773.15913859243,978344.61404013447,1009445.1976761866]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING OF/ STAKED WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",861101.8,716967.20000000007,271147.97969981836,279915.64143666282,289180.26332888217,299306.24892203545,308844.36107219162]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",865841.20000000007,765392.79999999993,406721.96954972745,419873.46215499437,433770.39499332319,448959.37338305305,463266.54160828749]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",477735.63710471801,1174788.3747201071,9385194.0660230797,9524615.0037687942,9707101.3267730363,9934656.4677515309,10018671.835226029]
[null,null,"> 1 kV & < = 11 kV",9028.2691856757829,213546.84773871847,2325264.6251309663,2386731.982770347,2526559.1639748486,2549653.8522725785,2571215.7559002265]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",7561048.1269781357,10256328.528194392,919151.16400964279,8679170.7674343977,8720102.5738959163,8799810.9985945597,8874229.2089426387]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",4434476.5530481935,4437982.1314179339,4118128.799514534,4123190.7583280774,4142636.1236338336,4180502.9946615933,4215856.6575149428]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",19347006.379636943,16310093.49801857,14108533.337906791,33715938.013038367,57692384.937794074,38864948.008340262,51439786.851498865]
[null,null,"> 22 kV & < = 66 kV",864682.03404633119,513793.61991027615,8673.394658027617,8684.0558997395601,8725.0107449562074,8804.764034102267,8879.2241312634087]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",2029655.0307441961,1651093.5196035069,2298932.63747461,3836264.1004864192,6166970.06719869,5445423.2900102492,3137985.2150385263]
[null,null,"> 11 kV & < = 22 kV",3265841.0285049984,1073329.4173303621,1145392.6801564703,1911334.3071552783,3072557.3505593627,2713062.5208674422,1563432.1933384838]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",5668.9407508062268,6017.0630661311025,6421.0482641277895,10714.901577204706,17224.694538424254,15209.373773635638,8764.5693438045855]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",7552587.1066269213,4706884.1953640031,6583003.6956996024,6620363.7968279822,6674801.6321686646,6743623.6941695409,6808528.4447147399]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",624773.89337307727,480479.8046359974,351309.87080085481,354992.22829308576,359244.71724919934,363395.78249534796,367343.57421364606]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",6001439.3113477593,4522685.7935423404,1746052.0224644686,1804230.2456934401,1835257.6685541861,1920206.337097116,1959361.6416462637]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",95915.902129834722,72282.241881070018,27905.664993335049,28835.47807246865,29331.362992745209,30689.025339278822,31314.811282310624]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",1245.6610666212302,938.73041403987054,362.411233679676,374.48672821387862,380.92679211357421,398.55877063998474,406.68586080922898]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",1003535.6967967286,756264.68981087068,291967.5501331889,301695.87041730591,306884.14689649816,321088.90959683765,327636.29661443509]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",2032607.4454591926,1531773.3531095588,591364.53055681125,611068.71876299637,621577.29303132463,650348.27399179502,663609.65337545925]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",3736.983199863691,2816.1912421196116,1087.2337010390279,1123.4601846416356,1142.7803763407226,1195.6763119199541,1220.0575824276868]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,2540.5216981132075,11275.168128128129,11289.027441291693,11342.267583552693,11445.944607295725,11542.740630932396]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,24433.841037735849,108440.58758523229,108573.88156771715,109085.92646534501,110083.05548781477,111014.0054798498]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,3810.7825471698116,16912.752192192194,16933.541161937541,17013.401375329038,17168.91691094359,17314.110946398596]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,261.5242924528302,1160.6790720131899,1162.1057660153213,1167.5863688951301,1178.2590036922072,1188.223300243041]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",0,114809.16438679244,509538.11261379032,510164.43128072604,512570.41594496206,517255.70262087887,521630.0288066949]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,12553.166037735848,55712.595456633106,55781.076768735416,56044.14570696625,56556.432177225935,57034.718411665956]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0,0,0,0,3120704.5235989415,3149230.1561150816,7645557.6964156013]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",9543698.0780005008,8689336.0090795532,4366111.9111146023,8742928.4784186054,8784131.9384235851,4432212.8203080632,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,-87287,95389.058877098869,159177.18343908686,159927.87838912348,161389.74184127522,162754.5820359436]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",12758459,12853913,20962814.53071782,10650097.264986251,9609500.9505930711,11154111.530623866,10392389.731984828]
[null,null,"˂ = 11 kV  ; Switch",0,230749,1591523.9514450105,1593480.2352537957,2731109.5300226398,5306234.3589213705,8194383.452900474]
[null,null,"˂ = 11 kV ;  Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",9263059.6777527202,7751397.1494246228,2765661.3505396098,3271346.3191722189,4576295.7534015384,7980577.4543583337,4050021.2384481556]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",1545449.0164734931,986905.86284862447,0,1324835.1033453455,1711392.6258971386,2878393.4448519684,4063829.6052153371]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",391269,823449.00000000012,0,3410843.5930628837,4283661.8255375363,4322817.779628884,4359374.9696494676]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",20152239.200000003,11314006,4362508.7891624561,3275903.3528868943,4388470.4387548398,4428584.4239454335,7815563.1066579763]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",2577,-1439833.9999999998,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",3370459.5999999996,9724724.0000000019,8043885.9194597779,12517693.705649789,14674982.12098597,22201416.288795386,22010929.674541015]
[null,null,"Local Network Wiring Assets",19814,0,0,0,0,0,0]
[null,null,"Communications Network Assets",3487601,3732896,3750208.1773696626,3601643.7242891425,4695344.1535542244,8273316.8734353855,11624598.383432504]
[null,null,"Master Station Assets",0,0,7977286.8402417833,7987092.4338487359,8024760.3321368108,8098112.795509615,8166596.8869901001]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",0,0,0,0,0,0,0]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,-722535,0,0,0,0,0]
[null,"OTHER: ","Zone Substation Batteries",1716386.5125608174,1866346.0579699199,3926213.6633813893,5628817.0660000509,5266105.1795970565,6099873.5125326365,9075806.6682211831]
[null,null,"Zone Substation Protection Relays",2205259.3404369112,2344928.9390203529,6664665.5736521659,10679446.655847942,13732731.563556978,17281033.518237717,14363832.589900937]
[null,null,"Zone Substation Property",20578398.089881357,15338438.129411863,5527524.4194520414,7878526.6700116582,9107781.7102313563,13048303.763806287,10943610.857179163]
[null,null,"Zone Substation Current transformers",575888.20000000007,0,0,1564767.6189925317,1572147.2140084719,1586517.8451749114,1599934.7036440384]
[null,null,"Zone Substation Voltage transformers",495312.81332151423,542134.27627165744,782620.51301960892,644244.67863078963,863230.35248135985,911200.96757074061,960495.54921272292]
[null,null,"Zone Substation Surge Arresters",0,174646.00000000003,947346.91615666507,948511.38460949436,605323.72137374384,610856.84439088113,616022.73637943715]
[null,null,"Reactive Plant",985520,299294,671158.22372677387,1284505.927997665,675152.34166843339,681323.75182444346,687085.56810510135]
[null,null,"Power Transformer Bushings",0,113245,1025651.1651739434,1026911.8843519803,1547632.3497692421,1561778.8962768542,1574986.5424909478]
[null,null,"Line Surge Arresters",6972438,6032196,956468.71485814964,957644.39572602976,962160.73906287143,970955.62606880732,979166.80015322589]
[null,null,"NERs & NEDs",0,13338,112354.59249019616,112492.69752463921,113023.22393629704,114056.34287704127,0]
[null,null,"ZSS - SOCI",1925732,4350068,5698062.0287441323,6280707.1860171957,6310327.6068924405,1324619.8786940726,1335821.9193719518]
[null,null,"Upgrade oil control ",0,0,3459392.3277780511,5712448.8858645484,6349674.1297195898,7547746.3346392876,6461903.762222602]
[null,null,"Capitalised insurance costs - Repex major projects",0,0,230672.80217857071,279310.09879719221,314415.9128163046,320879.50846834615,321198.96246580931]
[null,null,"SAPS",959345,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE; MATERIAL TYPE","˂ = 1 kV; wood",441,429,705.3977059276757,685.68710345876309,668.12363119641282,651.27121849638343,635.85487644059526]
[null,null,"> 1 kV & < = 11 kV; wood",8,7,7.2490801147797441,7.1066984097609494,6.9532479841520054,6.8123779417863553,6.6810649573577088]
[null,null,"˃ 11 kV & < = 22 kV; wood",917,819,817.33650680051051,802.89638819466381,787.31261595209867,773.29987601774644,760.00341104861832]
[null,null,"> 22 kV & < = 66 kV; wood",57,66,49.468612800657269,50.176786786598292,50.975530140875719,50.975530140875719,51.374901818014436]
[null,null,"> 66 kV & < = 132 kV; wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; concrete",185,181,290.85879699767895,283.32708232419981,276.68243207602899,270.32280846540607,264.56522264254363]
[null,null,"> 1 kV & < = 11 kV; concrete",2,2,2.4258923660708303,2.3823529306488922,2.3353750684099648,2.2929957461869512,2.252894737582003]
[null,null,"˃ 11 kV & < = 22 kV; concrete",712,632,942.75087779858848,1401.6524912886341,1531.7334851769069,1653.2047669800427,910.9270000718609]
[null,null,"> 22 kV & < = 66 kV; concrete",57,65,75.183392999246067,76.472319061637563,77.667775804025197,77.667775804025197,78.265504175219007]
[null,null,"> 66 kV & < = 132 kV; concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; steel",300,323,296.53215787958504,309.78105000129113,323.99505056225979,338.21280292362803,353.39191192385931]
[null,null,"> 1 kV & < = 11 kV; steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; steel",0,0,0.11900244525572443,0.11650924334061659,0.11382425666280814,0.11133105474770029,0.10902963759529305]
[null,null,"> 22 kV & < = 66 kV; steel",58,67,9.8598356694055089E-2,9.9420009666505549E-2,0.10106331561140647,0.10106331561140647,0.10188496858385693]
[null,null,"> 66 kV & < = 132 kV; steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; steel",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV;  composite pole",0,0,0.22905728755285043,0.22255261812944291,0.21674487757282906,0.21116944663847975,0.20605863494865956]
[null,null,"> 1 kV & < = 11 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; composite pole",17,16,13.350318225704665,13.079245672665751,12.789223588982901,12.516283666921497,12.266238943221541]
[null,null,"> 66 kV & < = 132 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"> 132 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 132 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",2078,1832,949.2240030665364,974.2240030665364,1000.2240030665364,1027.6012834938731,1054.6012834938731]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",1340,1037,1464.7207794937742,1505.7207794937742,1545.7207794937742,1587.274642958713,1628.274642958713]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",153,85,205.05521743968939,210.05521743968939,216.05521743968939,221.12407354741384,226.12407354741384]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING OF/ STAKED WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,206,212.4,218.4,224,229.20000000000002]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,309,318.59999999999997,327.59999999999997,336,343.8]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",0,0,68.628553142856902,69.562553142856899,70.562553142856899,71.562553142856856,71.562553142856856]
[null,null,"> 1 kV & < = 11 kV",0,0,18.193062428571402,18.6510624285714,19.65106242857145,19.65106242857145,19.65106242857145]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",0,0,85.061541857142856,135.06154185714286,135.06154185714286,135.06154185714286,135.06154185714286]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",107,107,30.113519142856873,30.113519142856873,30.113519142856873,30.113519142856873,30.113519142856873]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,68.399555143575355,83.657927869900547,98.123934340872864,87.348482641352376,102.31843494891154]
[null,null,"> 22 kV & < = 66 kV",0,0,6.3423571428571426E-2,6.3423571428571426E-2,6.3423571428571426E-2,6.3423571428571426E-2,6.3423571428571426E-2]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",3,3,1.9986394771250109,3.3310657952083518,5.3297052723333627,4.6634921132916922,2.6648526361666813]
[null,null,"> 11 kV & < = 22 kV",2,2,0.99577821031131697,1.6596303505188614,2.6554085608301783,2.323482490726406,1.3277042804150891]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",0,0,5.5823125636723049E-3,9.3038542727871733E-3,1.4886166836459479E-2,1.3025395981902043E-2,7.4430834182297395E-3]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",1440,2253,2191.4857573044683,2208.586549808741,2222.0871754700088,2226.5873840237646,2231.0875925775208]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",160,250,205.51424269553186,207.41345019125905,208.91282452999104,209.41261597623503,209.91240742247905]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",271,231,102.44859430908161,105.73220310103936,107.04564661782246,110.98597716817174,112.29942068495484]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",4,4,1.6373487817345374,1.6898279093542341,1.7108195604021128,1.7737945135457487,1.7947861645936274]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,2.126426989265633E-2,2.1945817004600444E-2,2.221843584937809E-2,2.3036292383711025E-2,2.3308911228488671E-2]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",45,39,17.131027432271257,17.680098824331232,17.899727381155223,18.558613051627194,18.778241608451186]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",92,78,34.697972397341971,35.810086897256774,36.254932697222699,37.589470097120461,38.034315897086387]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,6.3792809677968992E-2,6.5837451013801326E-2,6.6655307548134271E-2,6.9108877151133077E-2,6.9926733685466008E-2]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0.16037735849056603,0.16037735849056603,0.16037735849056603,0.16037735849056603,0.16037735849056603]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",2,2,1.5424528301886791,1.5424528301886791,1.5424528301886791,1.5424528301886791,1.5424528301886791]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0.24056603773584906,0.24056603773584906,0.24056603773584906,0.24056603773584906,0.24056603773584906]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,1.6509433962264151E-2,1.6509433962264151E-2,1.6509433962264151E-2,1.6509433962264151E-2,1.6509433962264151E-2]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",10,10,7.2476415094339615,7.2476415094339615,7.2476415094339615,7.2476415094339615,7.2476415094339615]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",1,1,0.79245283018867918,0.79245283018867918,0.79245283018867918,0.79245283018867918,0.79245283018867918]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0,0,0,0,1,1,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",0,0,1,2,2,1,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,2,3,3,3,3]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",0,0,4010,2096,1895,2161,2006]
[null,null,"˂ = 11 kV  ; Switch",0,0,102,102,174,335,513]
[null,null,"˂ = 11 kV ;  Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,169,124,165,267,177]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,7,9,15,21]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,16,20,20,20]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",6,4,4,3,4,4,7]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",16,12,102,214,242,331,339]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",0,0,20309.230982189725,20787.411610406143,50949.654671398144,81308.174422211843,85376.05706065608]
[null,null,"Master Station Assets",0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",0,0,0,0,0,0,0]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B149),\"\",B149)","v":"OTHER: "},"Zone Substation Batteries",0,0,3,5,4,6,11]
[null,null,"Zone Substation Protection Relays",0,0,37,64,90,109,71]
[null,null,"Zone Substation Property",0,0,5,5,6,6,7]
[null,null,"Zone Substation Current transformers",0,0,0,4,4,4,4]
[null,null,"Zone Substation Voltage transformers",0,0,2.4325618125316399,2,2.66724247122196,2.7899615417780801,2.9162322207907101]
[null,null,"Zone Substation Surge Arresters",0,14,36,36,14,14,14]
[null,null,"Reactive Plant",1,0,3,4,3,3,3]
[null,null,"Power Transformer Bushings",0,0,6,6,9,9,9]
[null,null,"Line Surge Arresters",378,379,299,299,299,299,299]
[null,null,"NERs & NEDs",0,0,1,1,1,1,0]
[null,null,"ZSS - SOCI",0,0,0,0,0,0,0]
[null,null,"Upgrade oil control ",0,0,4,6,7,8,7]
[null,null,"Capitalised insurance costs - Repex major projects",0,0,0,0,0,0,0]
[null,null,"SAPS",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,{"$f":"IF(ISBLANK(C169),\"\",C169)","v":""},0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,"",0,0,0,0,0,0,0]
[null,null,{"$f":"IF(ISBLANK(C189),\"\",C189)","v":""},0,0,0,0,0,0,0]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE; MATERIAL TYPE","˂ = 1 kV; wood",626,610,996.25650292535465,969.01418578296284,944.80606327244186,921.5940269617895,900.42009908313889]
[null,null,"> 1 kV & < = 11 kV; wood",10,9,9.6749724808505739,9.4890513404098407,9.2886230525619702,9.1053736879733069,8.9339596949397126]
[null,null,"˃ 11 kV & < = 22 kV; wood",1631,1451,1760.0873845990991,2204.5488794832982,2319.0461011290054,2426.5046429977892,1670.9304111204792]
[null,null,"> 22 kV & < = 66 kV; wood",114,131,124.65200579990334,126.64910584823585,128.64330594490093,128.64330594490093,129.64040599323346]
[null,null,"> 66 kV & < = 132 kV; wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; concrete",1.85,1.81,2.9085879699767894,2.8332708232419983,2.7668243207602901,2.7032280846540608,2.6456522264254363]
[null,null,"> 1 kV & < = 11 kV; concrete",0.02,0.02,2.4258923660708302E-2,2.3823529306488924E-2,2.3353750684099648E-2,2.2929957461869512E-2,2.2528947375820032E-2]
[null,null,"˃ 11 kV & < = 22 kV; concrete",8.120000000000001,6.32,9.427508777985885,14.016524912886341,15.31733485176907,16.532047669800427,9.1092700007186096]
[null,null,"> 22 kV & < = 66 kV; concrete",0.57000000000000006,0.65,0.75183392999246068,0.76472319061637561,0.77667775804025196,0.77667775804025196,0.78265504175219014]
[null,null,"> 66 kV & < = 132 kV; concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; steel",300,323,296.53215787958504,309.78105000129113,323.99505056225979,338.21280292362803,353.39191192385931]
[null,null,"> 1 kV & < = 11 kV; steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; steel",0,0,0.11900244525572443,0.11650924334061659,0.11382425666280814,0.11133105474770029,0.10902963759529305]
[null,null,"> 22 kV & < = 66 kV; steel",58,67,9.8598356694055089E-2,9.9420009666505549E-2,0.10106331561140647,0.10106331561140647,0.10188496858385693]
[null,null,"> 66 kV & < = 132 kV; steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; steel",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV;  composite pole",0,0,0.22905728755285043,0.22255261812944291,0.21674487757282906,0.21116944663847975,0.20605863494865956]
[null,null,"> 1 kV & < = 11 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; composite pole",17,16,13.350318225704665,13.079245672665751,12.789223588982901,12.516283666921497,12.266238943221541]
[null,null,"> 66 kV & < = 132 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"> 132 kV; composite pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"> 132 kV; pole - other technology",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",2078,1832,949.2240030665364,974.2240030665364,1000.2240030665364,1027.6012834938731,1054.6012834938731]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",1340,1037,1464.7207794937742,1505.7207794937742,1545.7207794937742,1587.274642958713,1628.274642958713]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",153,85,205.05521743968939,210.05521743968939,216.05521743968939,221.12407354741384,226.12407354741384]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING OF/ STAKED WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,206,212.4,218.4,224,229.20000000000002]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,309,318.59999999999997,327.59999999999997,336,343.8]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",0,0,68.628553142856902,69.562553142856899,70.562553142856899,71.562553142856856,71.562553142856856]
[null,null,"> 1 kV & < = 11 kV",0,0,18.193062428571402,18.6510624285714,19.65106242857145,19.65106242857145,19.65106242857145]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",0,0,85.061541857142856,135.06154185714286,135.06154185714286,135.06154185714286,135.06154185714286]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",107,107,30.113519142856873,30.113519142856873,30.113519142856873,30.113519142856873,30.113519142856873]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,68.399555143575355,83.657927869900547,98.123934340872864,87.348482641352376,102.31843494891154]
[null,null,"> 22 kV & < = 66 kV",0,0,6.3423571428571426E-2,6.3423571428571426E-2,6.3423571428571426E-2,6.3423571428571426E-2,6.3423571428571426E-2]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",3,3,1.9986394771250109,3.3310657952083518,5.3297052723333627,4.6634921132916922,2.6648526361666813]
[null,null,"> 11 kV & < = 22 kV",2,2,0.99577821031131697,1.6596303505188614,2.6554085608301783,2.323482490726406,1.3277042804150891]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",0,0,5.5823125636723049E-3,9.3038542727871733E-3,1.4886166836459479E-2,1.3025395981902043E-2,7.4430834182297395E-3]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",1680,2318,2242.4857573044683,2272.586549808741,2263.0871754700088,2289.5873840237646,2271.0875925775208]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",187,257,211.51424269553186,214.41345019125905,212.91282452999104,216.41261597623503,213.91240742247905]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",271,231,102.44859430908161,105.73220310103936,107.04564661782246,110.98597716817174,112.29942068495484]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",4,4,1.6373487817345374,1.6898279093542341,1.7108195604021128,1.7737945135457487,1.7947861645936274]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,2.126426989265633E-2,2.1945817004600444E-2,2.221843584937809E-2,2.3036292383711025E-2,2.3308911228488671E-2]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",45,39,17.131027432271257,17.680098824331232,17.899727381155223,18.558613051627194,18.778241608451186]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",92,78,34.697972397341971,35.810086897256774,36.254932697222699,37.589470097120461,38.034315897086387]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,6.3792809677968992E-2,6.5837451013801326E-2,6.6655307548134271E-2,6.9108877151133077E-2,6.9926733685466008E-2]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0.16037735849056603,0.16037735849056603,0.16037735849056603,0.16037735849056603,0.16037735849056603]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",2,2,1.5424528301886791,1.5424528301886791,1.5424528301886791,1.5424528301886791,1.5424528301886791]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0.24056603773584906,0.24056603773584906,0.24056603773584906,0.24056603773584906,0.24056603773584906]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,1.6509433962264151E-2,1.6509433962264151E-2,1.6509433962264151E-2,1.6509433962264151E-2,1.6509433962264151E-2]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",10,10,7.2476415094339615,7.2476415094339615,7.2476415094339615,7.2476415094339615,7.2476415094339615]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",1,1,0.79245283018867918,0.79245283018867918,0.79245283018867918,0.79245283018867918,0.79245283018867918]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0,0,0,0,1,1,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",0,0,1,2,2,1,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,2,3,3,3,3]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",0,0,4010,2096,1895,2161,2006]
[null,null,"˂ = 11 kV  ; Switch",0,0,102,102,174,335,513]
[null,null,"˂ = 11 kV ;  Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,169,124,165,267,177]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,7,9,15,21]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,16,20,20,20]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",6,4,4,3,4,4,7]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",16,12,102,214,242,331,339]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",0,0,20309.230982189725,20787.411610406143,50949.654671398144,81308.174422211843,85376.05706065608]
[null,null,"Master Station Assets",0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",0,0,0,0,0,0,0]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B149),\"\",B149)","v":"OTHER: "},"Zone Substation Batteries",0,0,3,5,4,6,11]
[null,null,"Zone Substation Protection Relays",0,0,37,64,90,109,71]
[null,null,"Zone Substation Property",0,0,5,5,6,6,7]
[null,null,"Zone Substation Current transformers",0,0,0,4,4,4,4]
[null,null,"Zone Substation Voltage transformers",0,0,2.4325618125316399,2,2.66724247122196,2.7899615417780801,2.9162322207907101]
[null,null,"Zone Substation Surge Arresters",0,14,36,36,14,14,14]
[null,null,"Reactive Plant",1,0,3,4,3,3,3]
[null,null,"Power Transformer Bushings",0,0,6,6,9,9,9]
[null,null,"Line Surge Arresters",378,379,299,299,299,299,299]
[null,null,"NERs & NEDs",0,0,1,1,1,1,0]
[null,null,"ZSS - SOCI",0,0,0,0,0,0,0]
[null,null,"Upgrade oil control ",0,0,4,6,7,8,7]
[null,null,"Capitalised insurance costs - Repex major projects",0,0,0,0,0,0,0]
[null,null,"SAPS",0,0,0,0,0,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C169),\"\",C169)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C189),\"\",C189)","v":""}]

{"sheet":"2.3 Augex (b)","index":5,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[68,1,69,2],[60,1,61,2],[45,1,46,2],[6,1,6,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.3 AUGEX PROJECT DATA"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,null,null,"VOLUMES"]
[null,"PROJECT TYPE","UNITS",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV feeder augmentations - overhead conductor","Circuit Line Length in KM",2.9202437934117391,4.2832693804266988,0,2.75,53.9,9.75,0]
[null,"HV feeder augmentations - underground asset (cable)","Circuit Line Length in KM",2.2868002364675597,3.3541656536047268,9,9,2.95,15,0]
[null,"LV feeder augmentations - overhead conductor","Circuit Line Length in KM",2.742935242055383,5.7944624550566024,0.9,30.048749999999998,35.46,24.513749999999998,11.3775]
[null,"LV feeder augmentations - underground asset (cable)","Circuit Line Length in KM",5.1000334310178941,10.773842481757724,0,2.5874999999999995,0.86249999999999993,0.86249999999999993,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",18.714349135712069,27.194609873051338,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",null,null,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",8.5349721058393058E-2,0.12402527868455518,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV feeder augmentations - overhead conductor","Circuit Line Length in KM",3.6844328827141037,5.4041441972654845,99,12,0,3,0]
[null,"HV feeder augmentations - underground asset (cable)","Circuit Line Length in KM",null,9.9434417561515623E-2,0.03,0.03,0.03,0.03,0.03]
[null,"LV feeder augmentations - overhead conductor","Circuit Line Length in KM",2.1547331162813128,4.551882943325821,0,0,0,0,0]
[null,"LV feeder augmentations - underground asset (cable)","Circuit Line Length in KM",8.2724989180594385E-2,0.17475689420313306,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",7.1978265906584848,10.459465335788972,33,248,293,279,100]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",null,null,5,11,7,2,0]
[null,"Distribution Substation Augmentations - Indoor","Number",3.2826815791689619E-2,4.7702030263290431E-2,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2026)"}]
[null,"PROJECT TYPE",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"HV feeder augmentations - overhead conductor",null,5122865.9179999996,7513966.7359999996,37541993.976866849,20258082.432805482,22521984.426303055,10223408.852410568,47729726.695343561]
[null,"HV feeder augmentations - underground asset (cable)",null,1647846.0730000001,2416979.2420000001,8755240.4228365161,7151358.2174856765,2154067.5826628702,31371895.507257473,20669742.83390712]
[null,"HV feeder non-material projects",null,220876.0091,323970.02230000001,675018.51833896071,338678.55908527563,0,9618005.5610427614,3873445.182079318]
[null,"LV feeder augmentations - overhead conductor",null,2773650.98,5859349.5829999996,5733676.23265211,5929957.2870785007,5962730.8051052941,7588961.8136502346,11286893.351195354]
[null,"LV feeder augmentations - underground asset (cable)",null,801924.30740000005,1694068.537,209679.42419200117,526395.26910896623,148809.46625964594,277189.32157949771,0]
[null,"LV feeder non-material projects",null,26269.712449999999,55494.880149999997,0,0,0,0,0]
[null,"Distribution substation augmentations - pole mounted",null,2444385.9950000001,3552040.3629999999,10194478.188203661,9913967.9541776385,9969383.2061889414,12970551.316100722,19593464.694566488]
[null,"Distribution substation augmentations - ground mounted",null,0,0,0,1173340.9650450589,518036.808809251,589833.05573727551,0]
[null,"Distribution substation augmentations - indoor",null,11148.00527,16199.636549999999,0,0,0,0,0]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,15444179.76516486,12105333.950017229,35577593.971533291,40229423.437030822,49792337.800143182,15364190.563421294,19069500.887306131]
[null,"Subtransmission Lines",null,10818702,17041760.999999996,23126178.039905954,65394321.757866137,70912658.630847737,50616479.759540617,47659726.476408705]
[null,"HV Feeders",null,6991588,10254916.000000002,53054325.672182441,33794927.15610639,30726085.425817344,57315778.851253405,78431229.49878706]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,3601845,7608912.9999999991,10194478.188203661,11087308.919222698,10487420.014998192,13560384.371837998,19593464.694566488]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,2455534,3568240.0000000005,10330512.959044201,12318138.43353603,9265622.9308136702,8444353.5780361667,11756648.20365349]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,13785523.999999998,6412140.0000000009,12758316.565764457,10470831.840750661,22402552.959988993,36385795.580390818,41087597.913849145]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,6735751.0000000009,12794932,54996996.063905172,85845396.750556126,74749503.943964198,40761980.860285275,62303872.631982602]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,46361621.765164852,44196371.950017229,90044409.332728833,87449554.793956593,118837173.81864494,140925001.84419507,155294295.04258844]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,287455,429166.99999999994,29966916.66046321,36651519.68328324,36106464.351711214,0,0]
[null,"Subtransmission Lines",null,6230098,7003487,10159011.127907084,39259081.937531173,24480066.201766938,0,0]
[null,"HV Feeders",null,218198,5362278,14871068.275534876,9934795.1297417227,0,12142705.019161899,28598961.968111325]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,0,0,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,14162973.390486045,28619275.841123372,33704910.663871266]

{"sheet":"2.5 Connections","index":6,"n_rows":212,"n_cols":17,"rows_kept":212,"cut":false,"hidden":false,"merged":[[11,16,11,93],[12,16,12,93],[139,1,140,1],[139,2,140,3],[103,1,104,1],[103,2,104,2],[103,3,104,3],[121,1,122,1],[121,2,122,3],[6,1,6,2],[10,1,11,1],[10,2,11,2],[10,3,11,3],[55,1,56,1],[55,2,56,2],[55,3,56,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.5 CONNECTIONS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL SERVICE CLASSIFICATIONS"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2026)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,null,null,null,null,"DRAFT TEMPLATE ONLY"]
[null,"RESIDENTIAL","Underground connections","0's",15763.255563757839,15893.598032578268,16359.470872091593,16374.974320822019,16375.885077787212,16388.766633426669,16383.735709344302,null,null,null,null,null,"DO NOT USE FOR SUBMISSIONS"]
[null,null,"Overhead connections","0's",805.14329947093256,811.80083065050371,835.59632096800203,836.38819405624236,836.43471299168721,837.0926670651919,836.83570144037662]
[null,null,"Distribution substations installed","MVA",25.46063063529753,26.923144070363218,31.290625115506263,31.724801612276796,31.914133061405281,32.248591476988857,32.538736940000561]
[null,null,"Distribution substations installed","Number of substations",127.30315317648767,134.61572035181612,156.45312557753132,158.62400806138402,159.57066530702642,161.2429573849443,162.69368470000282]
[null,null,"Distribution substations installed ","$",2134415.562130555,2257020.9869664013,2623155.653605015,2659553.5372510548,2675425.5711063482,2703463.8886693637,2727787.3628363861]
[null,null,"Augmentation HV ","km added",14.642836408184296,15.483952454412515,17.995764175651448,18.245466372959775,18.354354070056694,18.546706723644988,18.713574253766854]
[null,null,"Augmentation HV","$",884745.96380571078,935567.67663838947,1087335.7644771573,1102423.210998002,1109002.397422618,1120624.6835115645,1130707.1135579066]
[null,null,"Augmentation LV","km added",10.814362825076406,11.435563106793792,13.290643812781534,13.475059597035036,13.555477832325501,13.697538518403187,13.820777347558826]
[null,null,"Augmentation LV","$",716289.17469634395,757434.3669106008,880305.61225164868,892520.38921452418,897846.88993569219,907256.27754671534,915418.99972039205]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",10,10,10,10,10,10,10]
[null,null,"Volume of GSL breaches for residential customers","0's",6879.75,6879.75,6879.75,6879.75,6879.75,6879.75,6879.75]
[null,null,"Volume of customer complaints relating to connection services","0's",56,56,56,56,56,56,56]
[null,null,"GSL payments","$",664067.5,664067.5,664067.5,664067.5,664067.5,664067.5,664067.5]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1839.0441949840911,1830.5978251262361,1973.7659995639231,2052.6447472255823,2121.2141333128234,2209.52670546933,2289.4305847113255]
[null,null,"Overhead connections","0's",366.78861992129703,365.10403161615613,393.65824323427609,409.39023438209642,423.06607238554761,440.67959497044956,456.61604373740425]
[null,null,"Distribution substations installed","MVA",404.87068585914483,400.48585048919722,538.68018323071112,550.92091621098507,585.54155935291055,551.14859488471927,495.12453528470218]
[null,null,"Distribution substations installed","Number of substations",404.87068585914483,400.48585048919722,538.68018323071112,550.92091621098507,585.54155935291055,551.14859488471927,495.12453528470218]
[null,null,"Distribution substations installed ","$",19643311.871697668,19430570.639283776,26135413.621882744,26729303.334988195,28409010.249289688,26740349.734124765,24022202.647959631]
[null,null,"Augmentation HV ","km added",180.25311388392015,178.30093444266421,239.8266503509646,245.27636630467427,260.6898772081708,245.37773148456736,220.43517192658868]
[null,null,"Augmentation HV","$",10790576.066595653,10673711.839938898,14356854.412376277,14683093.295426663,15605799.473831927,14689161.36637741,13196013.312473131]
[null,null,"Augmentation LV","km added",41.164266161097231,40.718448430781443,54.769029254768313,56.01357673129818,59.533548462366873,56.036725420131795,50.340612114456192]
[null,null,"Augmentation LV","$",3541104.1750903907,3502753.2660769196,4711436.7932786271,4818497.4231946552,5121298.5600910857,4820488.7600098383,4330487.7836878505]
[null,"SUBDIVISION","Underground connections","0's",310.77647107202944,310.77647107202944,319.27265372291072,318.98646651782838,319.02223991846375,319.25476702259306,319.14744682068726]
[null,null,"Overhead connections","0's",138.37474458069033,138.37474458069033,142.15771148346496,142.0302852298978,142.04621351159375,142.14974734261702,142.10196249752937]
[null,null,"Distribution substations installed","MVA",201.37089012839311,203.44531447105703,173.16663335170313,173.51809483955455,174.46111942102698,176.3714411135179,177.97780191080406]
[null,null,"Distribution substations installed","Number of substations",566.75077723809773,572.58916633086483,487.3709600290656,488.36013513417657,491.01424226040206,496.39077063202382,500.91181252544879]
[null,null,"Distribution substations installed ","$",13301105.168998232,13438126.64379685,11438135.872090461,11461350.877048643,11523640.263201319,11649822.303327573,11755926.884235151]
[null,null,"Augmentation HV ","km added",143.35738914164202,144.83418679370857,123.27857530907286,123.52878327731538,124.20012927876616,125.56010107052579,126.70368090856297]
[null,null,"Augmentation HV","$",6297050.0332804043,6361919.1604302162,5415077.3908539563,5426067.9097534874,5455557.1421264438,5515294.6308449293,5565526.9871977353]
[null,null,"Augmentation LV","km added",450.72466433438842,455.36780920472268,387.59560848937946,388.38227810700545,390.49303223672217,394.76886924111579,398.36435630826384]
[null,null,"Augmentation LV","$",10786383.812106442,10897499.858397359,9275629.5092644971,9294455.4602285251,9344968.3475357573,9447294.2744195387,9533338.6082813106]
[null,null,"Cost per lot","$",1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",8.5,9.5,9.5,11.5,2,1,1]
[null,null,"Distribution substations installed","MVA",5.5620980323926652,11.512847373966022,10.240146548397529,5.1186955038033695,2.8931734478808684,3.2020880247277108,5.1139639675844073]
[null,null,"Distribution substations installed","Number of substations",11.12419606478533,23.025694747932043,20.480293096795059,10.237391007606739,5.7863468957617368,6.4041760494554216,10.227927935168815]
[null,null,"Distribution substations installed ","$",500229.7014928555,1035412.9272213549,920952.02589308925,460352.10256783495,260198.81019211982,287981.17678525479,459926.56980364595]
[null,null,"Augmentation HV ","km added",3.7724045599222258,7.8084056912163327,6.9452165906592462,3.4716738444638082,1.9622488931099782,2.1717652934928338,3.4684647552489292]
[null,null,"Augmentation HV","$",2220013.7644555983,4595150.8746217489,4087174.6875172863,2043037.4308976645,1154759.3803358471,1278057.2094368488,2041148.9212971607]
[null,null,"Augmentation LV","km added",6.2517495920090752E-6,1.2940339859866322E-5,1.1509835251594481E-5,5.7533690239104831E-6,3.2519016775797451E-6,3.5991189629495124E-6,5.7480508185400997E-6]
[null,null,"Augmentation LV","$",-2.304811682920679E-2,-4.7706719616707173E-2,-4.2432925960878318E-2,-2.1210753801483313E-2,-1.198867751801066E-2,-1.3268751910073869E-2,-2.1191147351017833E-2]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2026)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Underground connections","0's",1890.2013052524123,2020.5437740728412,2051.7397816079292,2081.8849762576247,2080.9655149829064,2081.950652062962,2082.4103827003205]
[null,null,"Overhead connections","0's",96.546231165231802,103.20376234480301,104.79716773847495,106.33690052941266,106.28993700202022,106.34025506708355,106.36373683077974]
[null,null,"Distribution substations installed","MVA",18.710397134657534,20.051657772601509,24.320456115286099,24.703565967982446,24.819986428768441,25.061635049762252,25.281386672658755]
[null,null,"Distribution substations installed","Number of substations",93.551985673287675,100.25828886300755,121.60228057643052,123.51782983991224,124.09993214384221,125.30817524881128,126.4069333632938]
[null,null,"Distribution substations installed ","$",1568529.9940092901,1680970.5544772584,2038832.4529013874,2070949.3176921196,2080709.0776451014,2100966.9646002473,2119389.1824326478]
[null,null,"Augmentation HV ","km added",10.76066372036856,11.532045245966856,13.987102887186522,14.207435799585751,14.27439116240742,14.413367343954555,14.539750194033903]
[null,null,"Augmentation HV","$",650178.25297463383,696786.48325889267,845125.38963125495,858438.29223459342,862483.85317376419,870881.03881876892,878517.31319792324]
[null,null,"Augmentation LV","km added",7.9472117605343051,8.5169101073462876,10.330075490644996,10.492800798131135,10.542250205776874,10.644890077547508,10.738229233809706]
[null,null,"Augmentation LV","$",526383.46291566896,564117.42517164163,684212.40968422522,694990.51821329922,698265.79905644385,705064.14956777019,711246.46731383959]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",10,10,10,10,10,10,10]
[null,null,"Volume of GSL breaches for residential customers","0's",6879.75,6879.75,6879.75,6879.75,6879.75,6879.75,6879.75]
[null,null,"Volume of customer complaints relating to connection services","0's",56,56,56,56,56,56,56]
[null,null,"GSL payments","$",664067.5,664067.5,664067.5,664067.5,664067.5,664067.5,664067.5]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",488.26683553915166,479.82046568129698,580.66547087516199,660.96984107977039,729.36102434914312,816.51527818950285,896.95376588510464]
[null,null,"Overhead connections","0's",97.382498609444013,95.697910304303178,115.81096706601615,131.82729185110489,145.46758814989758,162.85008965451885,178.89316353544928]
[null,null,"Distribution substations installed","MVA",395.95971419173065,391.41481321225359,529.47887508749477,541.65219507850668,576.17658854976492,541.66110603090647,485.54411964328006]
[null,null,"Distribution substations installed","Number of substations",395.95971419173065,391.41481321225359,529.47887508749477,541.65219507850668,576.17658854976492,541.66110603090647,485.54411964328006]
[null,null,"Distribution substations installed ","$",19210973.839687675,18990466.62470765,25688989.191076528,26279608.194746777,27954645.316039048,26280040.531843971,23557384.870635003]
[null,null,"Augmentation HV ","km added",176.28584619356039,174.26240369090942,235.73012150225154,241.1498244131426,256.52048384960528,241.15379167225475,216.16986003322685]
[null,null,"Augmentation HV","$",10553081.674033077,10431951.393558152,14111621.998918453,14436064.197215127,15356205.138301432,14436301.691094169,12940676.961042803]
[null,null,"Augmentation LV","km added",40.258264263990142,39.796172242687028,53.833508085499467,55.071201506328038,58.581387280547695,55.072107506266157,49.366546089990685]
[null,null,"Augmentation LV","$",3463166.5024514524,3423415.618043392,4630959.7624135865,4737430.7808164358,5039390.0930944029,4737508.7183205551,4246694.9801783767]
[null,"SUBDIVISION","Underground connections","0's",310.77647107202944,310.77647107202944,319.27265372291072,318.98646651782838,319.02223991846375,319.25476702259306,319.14744682068726]
[null,null,"Overhead connections","0's",138.37474458069033,138.37474458069033,142.15771148346496,142.0302852298978,142.04621351159375,142.14974734261702,142.10196249752937]
[null,null,"Distribution substations installed","MVA",201.37089012839311,203.44531447105703,173.16663335170313,173.51809483955455,174.46111942102698,176.3714411135179,177.97780191080406]
[null,null,"Distribution substations installed","Number of substations",566.75077723809773,572.58916633086483,487.3709600290656,488.36013513417657,491.01424226040206,496.39077063202382,500.91181252544879]
[null,null,"Distribution substations installed ","$",13301105.168998232,13438126.64379685,11438135.872090461,11461350.877048643,11523640.263201319,11649822.303327573,11755926.884235151]
[null,null,"Augmentation HV ","km added",143.35738914164202,144.83418679370857,123.27857530907286,123.52878327731538,124.20012927876616,125.56010107052579,126.70368090856297]
[null,null,"Augmentation HV","$",6297050.0332804043,6361919.1604302162,5415077.3908539563,5426067.9097534874,5455557.1421264438,5515294.6308449293,5565526.9871977353]
[null,null,"Augmentation LV","km added",450.72466433438842,455.36780920472268,387.59560848937946,388.38227810700545,390.49303223672217,394.76886924111579,398.36435630826384]
[null,null,"Augmentation LV","$",10786383.812106442,10897499.858397359,9275629.5092644971,9294455.4602285251,9344968.3475357573,9447294.2744195387,9533338.6082813106]
[null,null,"Cost per lot","$",1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178,1647.9508141003178]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",8.5,9.5,9.5,11.5,2,1,1]
[null,null,"Distribution substations installed","MVA",5.5620980323926652,11.512847373966022,10.240146548397529,5.1186955038033695,2.8931734478808684,3.2020880247277108,5.1139639675844073]
[null,null,"Distribution substations installed","Number of substations",11.12419606478533,23.025694747932043,20.480293096795059,10.237391007606739,5.7863468957617368,6.4041760494554216,10.227927935168815]
[null,null,"Distribution substations installed ","$",500229.7014928555,1035412.9272213549,920952.02589308925,460352.10256783495,260198.81019211982,287981.17678525479,459926.56980364595]
[null,null,"Augmentation HV ","km added",3.7724045599222258,7.8084056912163327,6.9452165906592462,3.4716738444638082,1.9622488931099782,2.1717652934928338,3.4684647552489292]
[null,null,"Augmentation HV","$",2220013.7644555983,4595150.8746217489,4087174.6875172863,2043037.4308976645,1154759.3803358471,1278057.2094368488,2041148.9212971607]
[null,null,"Augmentation LV","km added",6.2517495920090752E-6,1.2940339859866322E-5,1.1509835251594481E-5,5.7533690239104831E-6,3.2519016775797451E-6,3.5991189629495124E-6,5.7480508185400997E-6]
[null,null,"Augmentation LV","$",-2.304811682920679E-2,-4.7706719616707173E-2,-4.2432925960878318E-2,-2.1210753801483313E-2,-1.198867751801066E-2,-1.3268751910073869E-2,-2.1191147351017833E-2]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL SERVICE CLASSIFICATIONS INCLUDING CAPITAL CONTRIBUTIONS"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Simple connection LV",null,12158005.325156156,12588748.828401113,13621369.009502111,13765299.822429515,13878003.265307676,14041296.49681145,14173280.447399192]
[null,null,"Complex connection LV",null,11871328.000298487,12668037.835336482,15190492.735046875,15423050.900994971,15500119.792797381,15652710.380451255,15790785.403641302]
[null,null,"Complex connection HV",null,7204192.642089583,7687681.1895643733,9218449.3587228283,9359578.7949526254,9406348.5534196608,9498949.144423509,9582740.8706816919]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,903017.25983758224,914164.62376030523,932718.33159847592,940276.63139252644,950511.76576200593,964132.25687416946,975026.81585792208]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,8650633.74083375,7442589.4223886831,9007480.1058692541,9268254.5400871113,9491070.7302409802,9933793.3741694558,10421097.308392614]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,15114349.795052361,13003659.995446466,15737830.218085473,16193454.179804109,16582757.661939733,17356280.747414906,18207696.070154499]
[null,null,"Complex connection HV (customer connected at HV)",null,19735747.982049707,16979688.838378109,20549865.206248872,21144801.79333286,21653139.599202495,22663176.873729035,23774922.894265406]
[null,null,"Complex connection sub-transmission",null,814581.82756060315,6493221.1617513327,12160951.28001887,12083961.750521723,14393091.131274279,8860256.4529813137,981296.48589644022]
[null,"SUBDIVISION","Complex connection LV",null,7236682.3791467482,7228144.1922907559,6943926.4521381855,7053625.5056146756,7110584.2118919659,7194099.1138212131,7263576.3574423706]
[null,null,"Complex connection HV (no upstream asset works)",null,54967808.908318259,54902955.236575514,52744117.027221553,53577360.258442387,54010002.610044986,54644358.372772977,55172088.021631032]
[null,null,"Complex connection HV (with upstream asset works)",null,2864980.0647472525,2861599.8231047564,2749078.9030307941,2792508.417394646,2815058.1922014649,2848121.4823392346,2875627.3071771171]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,878566.86167471053,875048.87221570418,874088.12858181843,874986.36878760916,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,18932882.440036487,28743994.292069636,25470684.174354568,12293855.199877899,7443252.4336529588,8237995.3750380669,13156668.769795638]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES EXCLUDING CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Simple connection LV",null,1738865.6717985792,1880865.2162673194,1314326.5396796183,1334200.8838737588,1341006.4390164276,1351908.3402517708,1361653.6972080735]
[null,null,"Complex connection LV",null,4777781.8859091913,5167945.9235190442,3611299.9614028702,3665907.5617627497,3684606.7969087106,3714561.3282385059,3741338.0889122491]
[null,null,"Complex connection HV",null,2899428.0258375853,3136201.6108051804,2191540.8798125037,2224679.8574150861,2236027.6099367794,2254205.7121843053,2270455.3636318906]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,21040.080417871366,17752.239759052492,19649.639045670905,19936.164485989571,20260.437866719658,20739.158410047283,21194.215058650749]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,5654439.5029406194,4770845.1567513011,5280763.8103888407,5357766.4043028429,5444913.6098902728,5573567.8876924468,5695862.5861363597]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,9879412.202945672,8335599.9892582167,9226527.6517854128,9361066.250275474,9513329.4703320935,9738113.667142218,9951786.4344490413]
[null,null,"Complex connection HV (customer connected at HV)",null,12900163.890076678,10884312.120461049,12047651.864234162,12223327.292529939,12422146.863250505,12715661.59056245,12994667.432254363]
[null,null,"Complex connection sub-transmission",null,532446.96309293865,3726334.4380275188,6524722.4821644742,6529244.0444996133,7835352.3399990015,4796134.1213045316,536347.54330748483]
[null,"SUBDIVISION","Complex connection LV",null,2231645.4859474176,2231637.9250506773,1814347.4532534913,1816170.297840684,1826145.5176542862,1846220.1380517806,1862999.3375981068]
[null,null,"Complex connection HV (no upstream asset works)",null,16950952.963771243,16950895.533321016,13781274.191488104,13795120.0075249,13870888.978415838,14023370.162486626,14150820.254389893]
[null,null,"Complex connection HV (with upstream asset works)",null,883501.51268852514,883498.51935300219,718294.51836589887,719016.17687318509,722965.33539778669,730912.81522803602,737555.64818435954]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,666241.83699512354,663574.04714105418,593603.4740782564,594213.47951052256,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,-3004481.7981363977,5476171.6745380694,2411392.1254061824,2351538.175807429,2528031.7732383446,3541402.7180164647,5660057.2621536553]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - TYPE 1 CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Simple connection LV",null,2272898.4955967623,2418483.513214868,3900310.7379701016,3962580.3679611166,3980736.9464156968,4021647.8031793693,4059020.1893750904]
[null,null,"Complex connection LV",null,6245113.3729842007,6645129.0103715872,10716661.036856228,10887755.742467165,10937643.536019759,11050051.960403871,11152737.93131871]
[null,null,"Complex connection HV",null,3789887.686494451,4032639.7788900556,6503475.4820645638,6607305.4174544206,6637580.1495848652,6705795.9333486147,6768111.5829618592]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,7046.2571631235751,6352.3022900624428,10517.052471116391,11149.566503110345,11732.746868109438,12508.27927154152,13246.551428428809]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1893654.1144206875,1707156.4504591923,2826416.8085910855,2996402.4862899687,3153129.9335096702,3361551.2404003069,3559959.0014409367]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,3308584.2648836784,2982736.3543694951,4938303.2031528251,5235301.4428034537,5509134.959599168,5873287.764059877,6219944.9445928978]
[null,null,"Complex connection HV (customer connected at HV)",null,4320224.5623886762,3894744.6489563081,6448250.0933170533,6836059.1944916165,7193620.6741318246,7669117.673555892,8121769.5470362296]
[null,null,"Complex connection sub-transmission",null,178314.82357312113,1925340.6356054232,4420739.2193258693,4362931.7038774043,5203474.13049741,3173373.9941649665,335221.44114670227]
[null,"SUBDIVISION","Complex connection LV",null,391438.97792157199,418468.27101229533,441344.54530565866,444099.88561819744,446408.63161082362,451218.12008015672,455363.59364841488]
[null,null,"Complex connection HV (no upstream asset works)",null,2973260.6476777992,3178567.5742079904,3352329.3351932955,3373258.1271233456,3390794.7139032516,3427326.2388864206,3458814.0929880631]
[null,null,"Complex connection HV (with upstream asset works)",null,154969.47489943195,165670.28803616433,174726.93393719714,175817.76460426711,176731.78996794755,178635.85150669585,180277.03160964197]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,212325.02467958693,211474.82507464997,280484.65450356196,280772.88927708665,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,16435495.907539288,23267822.617531568,23059292.048948385,9942317.0240704697,4915220.6604146138,4696592.6570216017,7496611.5076419814]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Simple connection LV",null,15189.346044587168,15257.928080414102,15304.562045497893,15772.60227873308,15767.99802931512,15769.592764904892,15782.449282093781]
[null,null,"Complex connection LV",null,872.06880007443112,941.43078003031837,1006.3489513127721,1021.8863872599278,1036.9004569436004,1036.4425114630528,1036.9331673350682]
[null,null,"Complex connection HV",null,377.09407894736842,369.04000278434842,394.48786641810381,400.57852706658537,406.46402861953914,406.2845144109524,406.47685106300969]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1690.1539554128326,1624.3461801865012,1624.2741709971988,1675.8982451665599,1674.8729206912265,1675.6697315186323,1677.7949931936275]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,180.78888326273866,182.62032381013788,179.46123397197923,217.17902711843172,247.21426404772518,272.793761005818,305.07914866845294]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,91.383329045536399,96.137890963110962,94.474832722565296,114.33083236832611,130.14245876737712,143.60842377138746,160.60461025301424]
[null,null,"Complex connection HV (customer connected at HV)",null,306.81991252894267,283.20465822269699,278.3055925587862,336.79773896446721,383.37590086742011,423.04417295446717,473.1118323902798]
[null,null,"Complex connection sub-transmission",null,22.344996140982762,19.523761722940385,19.1860264918623,23.218399180414135,26.429437233929139,29.164116448065755,33.615715934404264]
[null,"SUBDIVISION","Complex connection LV",null,88.989166537477715,152.00750113453586,152.00750113453586,156.16316803392516,156.0231876752089,156.04068522004846,156.15441926150538]
[null,null,"Complex connection HV (no upstream asset works)",null,177.14253190967105,276.26850332578636,276.26850332578636,283.82128766896608,283.56687809109059,283.59867928832512,283.8053870703489]
[null,null,"Complex connection HV (with upstream asset works)",null,13.8683015528512,20.875211192397551,20.875211192397551,21.445909503484376,21.426685981426711,21.429088921683928,21.44470803335577]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,7.5,7.5,7.5,7.5,0,0]
[null,null,"Complex connection HV (large capacity)",null,2,1,2,2,4,2,1]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Simple connection LV",null,628.16287902180011,676.2767536029769,722.91071868676761,734.07203501989011,744.85739122389691,744.5284261109208,744.88088873196682]
[null,null,"Complex connection LV",null,872.06880007443112,941.43078003031837,1006.3489513127721,1021.8863872599278,1036.9004569436004,1036.4425114630528,1036.9331673350682]
[null,null,"Complex connection HV",null,377.09407894736842,369.04000278434842,394.48786641810381,400.57852706658537,406.46402861953914,406.2845144109524,406.47685106300969]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,2.3371209782003461,4.1626994297094093,4.0906902404070431,4.9504403095388296,5.6350720144236721,6.218138319302251,6.9540605978703338]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,180.78888326273866,182.62032381013788,179.46123397197923,217.17902711843172,247.21426404772518,272.793761005818,305.07914866845294]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,91.383329045536399,96.137890963110962,94.474832722565296,114.33083236832611,130.14245876737712,143.60842377138746,160.60461025301424]
[null,null,"Complex connection HV (customer connected at HV)",null,306.81991252894267,283.20465822269699,278.3055925587862,336.79773896446721,383.37590086742011,423.04417295446717,473.1118323902798]
[null,null,"Complex connection sub-transmission",null,22.344996140982762,19.523761722940385,19.1860264918623,23.218399180414135,26.429437233929139,29.164116448065755,33.615715934404264]
[null,"SUBDIVISION","Complex connection LV",null,88.989166537477715,152.00750113453586,152.00750113453586,156.16316803392516,156.0231876752089,156.04068522004846,156.15441926150538]
[null,null,"Complex connection HV (no upstream asset works)",null,177.14253190967105,276.26850332578636,276.26850332578636,283.82128766896608,283.56687809109059,283.59867928832512,283.8053870703489]
[null,null,"Complex connection HV (with upstream asset works)",null,13.8683015528512,20.875211192397551,20.875211192397551,21.445909503484376,21.426685981426711,21.429088921683928,21.44470803335577]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,7.5,7.5,7.5,7.5,0,0]
[null,null,"Complex connection HV (large capacity)",null,2,1,2,2,4,2,1]
[]
[null,"EXISTING CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RESIDENTIAL","Simple connection LV",null,719149.4017065065,733122.87774138222,747564.39400949317,762001.30602818611,776439.81278246886,790891.17605394043,805336.93270586024]
[null,null,"Complex connection LV",null,59616.069041492956,60517.33732653605,61434.143047526297,62365.962838200219,63297.324683393592,64229.177184458982,65161.258658264647]
[null,null,"Complex connection HV",null,15618.60631700983,15983.573360319793,16354.631064278237,16731.574269789635,17108.337961092446,17485.293989047314,17862.339774106476]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,76862.727238745327,77312.740212783538,77814.37726099111,78314.988984723357,78816.397519283011,79319.93131551765,79823.516761138933]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,6884.9488822274452,6964.0951534516425,7080.9592178222929,7227.8585191222364,7400.3373173802729,7605.1015033009444,7840.262913810805]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,5144.3866480598599,5167.5621626262382,5210.5936768383772,5269.4368174495667,5341.7459230647664,5431.0512151615931,5536.3586969499402]
[null,null,"Complex connection HV (customer connected at HV)",null,1399.1414126438626,1557.6349830656025,1774.6206998930234,2038.1845786233971,2341.416729440818,2694.7165396940513,3095.1558764856891]
[null,null,"Complex connection sub-transmission",null,122.80262071593984,141.98864720780213,165.20704638821627,191.63648362214542,220.80060007021117,254.41631600461545,290.28176974221759]
[null,"SUBDIVISION","Complex connection LV",null,5199.9205903992133,5351.9280915337495,5508.0912595676746,5664.1144472428832,5820.1551324629318,5976.3095517244374,6132.4114783514242]
[null,null,"Complex connection HV (no upstream asset works)",null,5569.1303961237227,5845.3988994495094,6129.2201871184752,6412.7870652095662,6696.3857444978912,6980.1911315682401,7263.9011150468859]
[null,null,"Complex connection HV (with upstream asset works)",null,89.793666013254551,110.66887720565211,132.1147867091365,153.54147269056321,174.97056161224714,196.4152696456029,217.85276885818706]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,41.5,49,56.5,64,64,64,64]
[null,null,"Complex connection HV (large capacity)",null,7.5,9.5,11.5,15.5,17.5,18.5,19.5]

{"sheet":"2.6 Non-network","index":7,"n_rows":117,"n_cols":11,"rows_kept":117,"cut":false,"hidden":false,"merged":[[83,1,87,1],[61,4,61,10],[63,1,67,1],[68,1,72,1],[73,1,77,1],[78,1,82,1],[56,1,57,3],[56,4,56,10],[6,1,6,2],[13,1,17,1],[20,1,30,1],[33,1,37,1],[40,1,50,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.6 NON-NETWORK EXPENDITURE"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,{"$f":"'3.2 Operating expenditure'!C28+'3.2 Operating expenditure'!C35","v":50868799.833754711},{"$f":"'3.2 Operating expenditure'!D28+'3.2 Operating expenditure'!D35","v":43890656.559563279},{"$f":"'3.2 Operating expenditure'!E28+'3.2 Operating expenditure'!E35","v":49501191.893741876},{"$f":"'3.2 Operating expenditure'!F28+'3.2 Operating expenditure'!F35","v":53834572.502820127},{"$f":"'3.2 Operating expenditure'!G28+'3.2 Operating expenditure'!G35","v":56790606.136548512},{"$f":"'3.2 Operating expenditure'!H28+'3.2 Operating expenditure'!H35","v":59832848.3441002},{"$f":"'3.2 Operating expenditure'!I28+'3.2 Operating expenditure'!I35","v":60959006.489688039}]
[null,"MOTOR VEHICLES","Car",null,93729.804579265197,197819.99319968658,228162.8994266275,260679.89044232463,260223.74266674253,275054.73835579905,278956.10669076978]
[null,null,"Light commercial vehicle",null,811681.91699608066,2221152.5677682161,2789300.9672340648,3500636.2175501725,3564982.1584898839,3816034.1652377294,3744071.218201465]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,0,2066717.7361074551,2262481.3993989737,2253958.6763127982,2051749.8324288731,1977262.9413546377,1679732.5095820157]
[null,null,"Heavy commercial vehicle",null,65015.508137221201,1182140.8931944454,1292621.4268431363,1296981.437160685,1291557.7253546128,1302473.1142403777,1243022.6624872573]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,5274324.5854435628,5424915.0229435638,6177267.9354435634,6167439.927943564,6157189.2104435638,6225351.1979435636,6157189.2104435638]
[null,"OTHER","Other expenditure",null,"-   "," -   "," -   "," -   "," -   "," -   "," -   "]
[null,"OTHER - DNSP nominated","General furniture and equipment",null,0,0,0,0,0,0,0]
[null,null,"Plant",null,0,464184.5547834966,516780.88826933678,528211.07625550299,534152.59461641591,579447.46578665974,591807.51726662857]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,74822064.796950504,66490120.573587686,81492175.880357653,89281461.505135,84716722.974924579,66127821.870889053,65057030.81161999]
[null,"MOTOR VEHICLES","Car",null,120000,302235,735274.07710790855,735274.07710790855,735274.07710790855,735274.07710790855,735274.07710790855]
[null,null,"Light commercial vehicle",null,563470.20085000014,1603605,3506119.0612713005,5070725.3655416649,3506119.0612713005,3506119.0612713005,5123880.0331153758]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,0,0,643041.28440367046,1629798.2336149609,6845152.5811828366,709991.15084676386,6527405.2165809441]
[null,null,"Heavy commercial vehicle",null,500000,421800.35598820919,2572165.1376146819,814899.11680747953,977878.9401689755,7691570.8008399485,725267.24628677161]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,9577478.0397610292,3074459.8585923645,73981666.957825169,30865206.374365617,19568733.815473676,18694641.638046566,30632857.348922793]
[null,"OTHER","Other expenditure",null,270684,7820556.7088367119,125948.08094514182,127207.56175459323,128479.63737213917,129764.43374586057,131062.07808331917]
[null,"OTHER - DNSP nominated","General furniture and equipment",null,1146462.6926343373,737960.69694096409,769838.38847552438,777536.77236027969,785312.14008388261,793165.26148472133,801096.91409956862]
[null,null,"Running Costs",null,0,0,14479603.20249198,16257027.131634735,15930938.994886499,16516866.217765938,15540308.718559418]
[null,null,"Plant",null,0,1525484.2860032492,3252717.1636085659,766005.16979903064,2064411.0959122805,3473040.0462254197,2417557.4876225716]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Number of devices",null,null,1305.2610064013959,1340.1815292480237,1361.9003910184877,1361.9003910184877,1361.9003910184877,1361.9003910184877,1361.9003910184877]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  or PER CENT"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","UNITS",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"CAR","Average kilometres travelled ","0's",14930.5,17961.817460317459,17961.817460317459,17961.817460317459,17961.817460317459,18127.592633928572,18078.406593406595]
[null,null,"Number purchased","0's",2,5,10,10,10,10,10]
[null,null,"Number leased","0's",0,14,14,14,14,15,15]
[null,null,"Number in fleet","0's",49,63,63,63,64,64,66]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",21230,32396.962025316454,32396.962025316454,32444.779874213837,32444.779874213837,32828.179104477611,32912.802359882007]
[null,null,"Number purchased","0's",6,13,34,30,26,39,52]
[null,null,"Number leased","0's",0,188,188,182,178,194,183]
[null,null,"Number in fleet","0's",128,316,318,318,335,339,343]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",0,1000,1000,1000,1000,1000,1000]
[null,null,"Number purchased","0's",0,0,5,21,2,18,0]
[null,null,"Number leased","0's",0,102,100,96,75,79,60]
[null,null,"Number in fleet","0's",0,102,103,103,112,114,117]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",11177.5,24645.576923076922,24645.576923076922,24645.576923076922,24645.576923076922,24674.764705882353,24682.241379310344]
[null,null,"Number purchased","0's",2,3,3,1,15,4,2]
[null,null,"Number leased","0's",0,73,64,61,60,49,46]
[null,null,"Number in fleet","0's",2,78,78,78,85,87,88]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998,0.96189999999999998]
[]
[]
[]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"RECURRENT"]
[null,"Business Systems (TAM - Systems)",null,null,null,null,8300651.8624719614,10476126.105212018,17818189.737266909,15094670.180045171,15655363.237077698]
[null,"Hardware (TAM -Infrastructure)",null,null,null,null,7178084.3993209433,6473348.7001496973,5853459.2434272394,6459819.2980678873,6757741.4167958917]
[null,"Cyber security",null,null,null,null,3533584.5532005187,3553831.910887544,3578881.3308998067,3609086.5163712157,3634521.129846069]
[null,"Metering systems",null,null,null,null,0,1645292.5513368261,2540563.9077375173,891132.47317807819,0]
[null,"ICT expenditure",null,null,18966353.317281179,16854321.27981969]
[]
[]
[]
[]
[]
[null,"NON-RECURRENT"]
[null,"Innovation initiatives",null,null,null,null,1701355.5256150649,1711104.2533902994,1723165.0852480554,1737708.3226972525,1749954.6180740332]
[null,"Market systems",null,null,null,null,8179593.8731493503,12065478.709803391,0,0,0]
[null,"Customer engagement platform",null,null,null,null,9815512.6477792207,9871755.3080209568,9941337.030277241,4455662.3658903902,11217657.80816688]
[null,"ADMS Energy Management (IT portion)",null,null,null,null,7901487.8177888365,9317172.1602950487,8289712.1535591939,1670873.3872088965,729147.75753084722]
[null,"Field Enablement ERP",null,null,null,null,10531499.764808893,3251509.4045794024,1656889.505046207,3341746.7744177929,0]
[null,"Network Model Management Geospatial and asset model tools",null,null,null,null,15876346.183640132,7656890.0340615567,11957219.261416793,2924028.427615569,4290754.1116238311]
[null,"Asset Risk Management",null,null,null,null,3380898.800901731,18756335.085239816,17231650.852480549,22166920.270304691,17723899.336903673]
[null,"Cyber security",null,null,null,null,1897665.7785706492,1908539.3595507182,1921991.8258536002,1938213.1291623197,1951872.4586210372]
[null,"Conductor clearance compliance (3D Model/LiDAR)",null,null,null,null,3195494.6731103458,2594077.9226077292,2203663.0417114552,1837960.7259297862,1346118.9369800254]
[null,"ICT expenditure",null,null,55855711.479669318,49635799.293767996]

{"sheet":"2.10 Overheads","index":8,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[6,1,6,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.10 OVERHEADS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",94343640.234860316,88105859.824986294,95531924.958761469,97777785.987923175,100321229.80391398,103090202.39066666,104867243.4320308]
[null,"Alternative Control Services","Total  ",1306840.7233057984,1323486.5277792427,1100353.1536856364,1088505.4807139891,1092506.3811401331,1101497.4512450253,1059062.8563982269]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",38775249.079901889,41523505.50461103,41493729.382437684,41604134.08973179,41785724.029504776,42042834.570900112,42219722.445647649]
[null,"Alternative Control Services","Total  ",2244113.2540260935,1856902.6088855749,1870002.1534657835,1888476.861992287,2706134.4017950636,3394046.6049527554,3415064.9845639369]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",""]
[null,"Unregulated Distribution Services","Total  ",""]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",32311611.000945505,30175242.999759421,36955422.722545721,37724604.27792991,38595704.512990467,39544045.756477639,40152661.861583754]
[null,"Alternative Control Services","Total  ",""]
[null,"CAPEX"]
[null,"Standard Control Services","Total",6603892.8444947237,7072244.7785120914,0,0,0,0,0]
[null,"Alternative Control Services","Total",0,0,0,0,0,0,0]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",""]
[null,"Unregulated Distribution Services","Total",""]

{"sheet":"2.11 Labour","index":9,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.11 LABOUR"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"OPEX"]
[null,"In-house labour expenditure",101981478.77930422,88272332.852289826,98263194.945376739,100790428.55681579,103536894.98532683,106474713.16485487,108468818.75676008]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Non-labour expenditure",229792941.22679862,198902381.47041929,221414602.44664305,227109170.24161071,233297731.20525393,239917461.45768788,244410741.94906366]
[null,"Total",{"$f":"SUM(C13:C16)","v":331774420.00610286},287174714.32270908,319677797.39201981,327899598.79842651,336834626.19058073,346392174.62254274,352879560.70582372]
[null,"CAPEX"]
[null,"In-house labour expenditure",32614861.826139547,31440629.474270951,62396906.647547886,57187640.887540959,58892042.181247994,58904075.701892249,60312810.843323432]
[null,"Labour expenditure outsourced to related parties",null,null,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",null,null,0,0,0,0,0]
[null,"Non-labour expenditure",408814274.24953753,394095740.43239433,603476584.61397505,644290714.0648278,681102640.36958385,683725576.62315679,692976285.23928535]
[null,"Total",{"$f":"SUM(C19:C22)","v":441429136.0756771},425536369.90666527,665873491.26152289,701478354.95236874,739994682.55083179,742629652.32504904,753289096.08260882]

{"sheet":"2.14 Forecast price changes","index":10,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[[6,1,6,2],[12,4,12,8],[8,1,8,2],[9,1,9,2],[12,2,12,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There is ONE table on this worksheet."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. FORECAST price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"AusNet (D) must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. FORECAST price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"FORECAST"]
[null,"DESCRIPTION",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"OPEX"]
[null,"Labour Price Growth - WPI",9.9000000000000008E-3,1.3100000000000001E-2,9.3135243940020672E-3,8.3583556288052887E-3,1.0254990531688098E-2,1.2240188084018007E-2,1.0182353043552642E-2]
[null,"Output Growth",1.0262778660566177E-2,1.0175565888402944E-2,8.8570970664913658E-3,1.1168733924288432E-2,1.7979845685405664E-2,1.805624606729786E-2,1.7876088572783985E-2]
[null,"Productivity",5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3]
[null,"CAPEX"]
[null,"Labour Price Growth - WPI",8.2681564533859629E-3,8.100515567042995E-3,9.3135243940020672E-3,8.3583556288052887E-3,1.0254990531688098E-2,1.2240188084018007E-2,1.0182353043552642E-2]
[]
[]
[null,"CPI adjusted to $2026",4.0519877675840865E-2,0.03,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2]

{"sheet":"2.16 Opex Summary","index":11,"n_rows":62,"n_cols":12,"rows_kept":62,"cut":false,"hidden":false,"merged":[[9,1,9,7],[9,9,9,10],[6,9,6,11],[7,1,7,7],[7,9,7,10],[7,11,8,11],[8,1,8,7],[8,9,8,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.16 OPEX SUMMARY"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nAusNet (D)'s total forecast opex must reconcile to Table 2.16.1 (and if AusNet (D) owns any dual function assets Table 2.16.3). If AusNet (D) did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if AusNet (D) owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has AusNet (D) used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If AusNet (D) does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2022-23"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y1","v":"2021-22"},{"$f":"CRCP_y2","v":"2022-23"},{"$f":"CRCP_y3","v":"2023-24"},{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Base year total opex, excluding category specific",null,270740074.44554257,270740074.44554257,270740074.44554257,270740074.44554257,285946044.00352263,285946044.00352263,285946044.00352263,285946044.00352263,285946044.00352263]
[null,"Increment from base year to final year",null,null,null,null,15205969.55798004,0,0,0,0,0]
[null,"Price growth",null,null,null,null,null,1576593.9500673767,2999298.0940018017,4753472.0884540323,6859936.4061701065,8624957.0947207976]
[null,"Output growth",null,null,null,null,null,2533882.8336028312,5756949.6353463596,11015279.897667596,16420985.08539442,21866648.799072038]
[null,"Productivity growth",null,null,null,null,null,-1437613.1897677737,-2882229.787422773,-4338726.6151123075,-5812344.9311188441,-7290999.5713190483]
[null,"Step changes",null,null,null,null,null,19612755.580869403,23985787.824271008,27021647.565258428,30065096.057784095,31000104.129036989]
[null,"Category specific",null,"-","-","-","-",11446134.213725287,12093749.028707443,12436909.250790374,12912458.000790376,12732806.250790374]
[null,"Total opex",{"$f":"SUM(C16:C22)","v":0},270740074.44554257,270740074.44554257,270740074.44554257,285946044.00352263,319677797.39201975,327899598.79842651,336834626.19058073,346392174.6225428,352879560.70582372]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y1","v":"2021-22"},{"$f":"CRCP_y2","v":"2022-23"},{"$f":"CRCP_y3","v":"2023-24"},{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C29:C35)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y1","v":"2021-22"},{"$f":"CRCP_y2","v":"2022-23"},{"$f":"CRCP_y3","v":"2023-24"},{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Base year total opex, excluding category specific",null,0,0,0,0,0,0,0,0,0]
[null,"Increment from base year to final year",null,null,null,null,0,0,0,0,0,0]
[null,"Price growth",null,null,null,null,null,0,0,0,0,0]
[null,"Output growth",null,null,null,null,null,0,0,0,0,0]
[null,"Productivity growth",null,null,null,null,null,0,0,0,0,0]
[null,"Step changes",null,null,null,null,null,0,0,0,0,0]
[null,"Category specific",null,0,0,0,0,0,0,0,0,0]
[null,"Total opex",{"$f":"SUM(C42:C48)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y1","v":"2021-22"},{"$f":"CRCP_y2","v":"2022-23"},{"$f":"CRCP_y3","v":"2023-24"},{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C55:C61)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":12,"n_rows":133,"n_cols":11,"rows_kept":133,"cut":false,"hidden":false,"merged":[[55,1,55,3],[29,1,29,3],[30,1,30,3],[132,1,132,2],[106,1,106,3],[80,1,80,3],[81,1,81,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"2.17 STEP CHANGES"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Flexible services and non-network solutions","Increases due to additonal personnel to manage new flexible services and payments to third parties for non-network solutions",null,0,0,536841.69999999984,1073683.3999999997,1667590.9499999997,2318564.3499999996,2855406.05]
[null,"ESV more frequent pole inspections ","More frequent pole inspections due to a recent Energy Safe Victoria direction",null,1604812.1743500002,1604812.1743500002,1604812.1743500002,1604812.1743500002,1604812.1743500002,1604812.1743500002,1604812.1743500002]
[null,"Fleet Electrification","Progressive electrification of AusNet owned fleet",null,0,0,-46331.480487689303,-92662.960975378606,-138994.44146306789,-185325.92195075721,-231657.40243844647]
[null,"Digital (SaaS, Licenses, etc.)","Costs associated with progressively transitioning digital systems to cloud and opex with assosciated capex related to ADMS",null,0,0,3608100.3843999994,7354790.469399998,8685270.1943999976,10024204.119399998,10239786.219399998]
[null,"EFD Rollout ","Software that allows to identify faults on SWER network",null,0,0,1570762.0503253217,1569847.2309887789,1568259.4465593148,1566533.7617618253,1564895.674030385]
[null,"Digital Efficiencies","Efficiencies realised above productivity adjustment due to digital capex program",null,0,0,-770544.80114239978,-770544.80114239978,-770544.80114239978,-770544.80114239978,-770544.80114239978]
[null,"Preparedness and Response ","Uplifting resposne to emergencies and major event days through Victorian Government Network Outage Review and NOUS review",null,570658.49999999988,1719016,1813768.6833443195,1877725.6549461565,1845581.8311865409,1812984.0242615701,1807591.2594408798]
[null,"Resilience (Hazard tree program)","Expansion of annual ‘hazard tree’ management program to reduce climate increase-related and resilience related vegetation outages",null,0,0,3000000,3000000,3000000,3000000,3000000]
[null,"Customer relationship management and broad communications","Customer relationship managers, living and working in the regions, dedicated to local customer engagement, community energy support, planned and unplanned outage management, connections management and supporting complex enquiries. Broad communications to build customer agency, improve understanding of tariffs and services, provide necessary information related to preparedness for extreme weather events and community resilience",null,159961.85714285701,159961.85714285701,3286850.518656028,3120249.116348993,3111394.9498912599,3101771.7918812595,3092637.1126531493]
[null,"Emergency Backstop Mechanism","To comply with the obligation for emergency backstop to make sure that solar exports can be safely managed, enabling rooftop solar systems to be turned down or switched off when there is too much power in the grid. ",null,3163217.3901602505,3250139.4702565256,3250139.4702565256,3250139.4702565256,4321859.3823065246,5351636.951381525,5456662.4212065255]
[null,"Insurance","Bushfire Liability premium increase, major external factor",null,0,0,1758356.8811672982,1997748.0700983368,2126417.8791702595,2240459.6078410745,2380515.4215368945]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E10:E29)","v":5498649.9216531068},6733929.5017493824,19612755.580869399,23985787.824271008,27021647.565258428,30065096.057784095,31000104.129036985]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$30,0)-ROUND('2.16 Opex Summary'!H$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$30,0)-ROUND('2.16 Opex Summary'!I$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$30,0)-ROUND('2.16 Opex Summary'!J$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$30,0)-ROUND('2.16 Opex Summary'!K$21,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$30,0)-ROUND('2.16 Opex Summary'!L$21,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Augex","Investments in resilience - reclosers, SAPS, community hubs, mobile generation, emergency vehicles",null,3316464.7773295618,2325480.4301642193,11051058.860025719,8459068.5017156415,6007968.526864389,5465186.5068842089,5017030.2283983035]
[null,"Repex","Investments in resilience - undergrounding, covered conductors and pole hardening",null,2116693.1246068738,6244535.3520488422,9544970.6858595833,41817465.490228653,70527538.948564082,53519256.812468596,48768407.472024761]
[null,"Augex","Reliability upgrade (10 worst served feeders)",null,0,0,20761405.813375562,4872854.3460153677,0,0,0]
[null,"Augex","Reliability upgrade to BN11",null,5307035.0113655832,1725969.8428105323,16116947.735488581,10744631.823659051,0,0,0]
[null,"Augex","Reliability upgrade - regional reliability fund",null,0,0,6191025.8357906528,6191025.8357906528,18573077.507371955,31883783.054321859,31883783.054321859]
[null,"Repex","Repex (volume and/or unit rate increases)",null,46523785.353415772,27834195.953733172,24801678.491785254,48751120.533785328,65717447.139755026,83637050.448979467,84415811.586333096]
[null,"Augex","Enabling large renewables",null,6524846.5999999996,8953960.5999999978,14374705.679001195,45187886.972824171,23880765.041211523,27891255.210324373,40058329.006881267]
[null,"Augex","Demand driven augex",null,0,7630301.5999999996,51229531.164797664,71331446.429860428,100403303.06062409,59054152.371430323,73563633.582157552]
[null,"Augex","Under frequency load shedding (UFLS) compliance",null,0,0,0,0,4376293.1082708202,8833307.9035050608,8911865.6054144967]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E36:E55)","v":63788824.866717793},54714443.77875676,154071324.26612422,237355499.93387926,289486393.33266187,270283992.3079139,292618860.53553134]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E61:E80)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$30,0)-ROUND('2.16 Opex Summary'!H$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$30,0)-ROUND('2.16 Opex Summary'!I$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$30,0)-ROUND('2.16 Opex Summary'!J$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$30,0)-ROUND('2.16 Opex Summary'!K$47,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$30,0)-ROUND('2.16 Opex Summary'!L$47,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E87:E106)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE \n($, real June 2024)"]
[null,"CATEGORY","DESCRIPTION",{"$f":"CRCP_y3","v":"2023-24"},{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"GSL Payments",null,28351374.904699687,7477785.8363803709,7274141.7106110742,10521193.218731793,10214015.072941206,10108739.089011736,10108739.089011736,10108739.089011736]
[null,"Innovation",null,277295.04167538619,1322974.7863408248,203076.34032550416,310000,1230000,1659999.9999999998,2110000,1940000]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D113:D132)","v":28628669.946375072},{"$f":"SUM(E113:E132)","v":8800760.6227211952},{"$f":"SUM(F113:F132)","v":7477218.0509365788},10831193.218731793,11444015.072941206,11768739.089011736,12218739.089011736,12048739.089011736]

{"sheet":"3.1 Revenue","index":13,"n_rows":54,"n_cols":17,"rows_kept":54,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[29,2,29,8],[29,10,29,16],[42,2,42,8],[42,10,42,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.1 REVENUE"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DREV0101","Revenue from Fixed Customer Charges ",131073469.17477681,130739436.16923767,137085031.74609423,142525000.60603088,148304142.90430573,154350841.73677874,161717657.01380917,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",228220245.26903269,227638639.4342894,189907421.01049203,193014637.67892352,195910464.76650357,197599479.86589119,198188209.22778249,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",255806993.12037349,255155084.08578473,257466841.73241726,278753227.42784822,300848152.22753274,325750556.1755445,351183132.04761678,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",16799496.33061526,16756683.805043235,18132611.501344211,18909043.329149809,19764459.435268342,20667107.381651442,21754244.143905278,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",103840266.19301349,103575635.39907162,118623643.54439925,130033335.3537405,142654583.60046646,155938847.47054824,170088606.4612087,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",55166423.396749109,55025835.020412713,55932744.005555406,57948791.846298426,60139337.901483767,62367699.90351247,65097326.890182696,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",51541264.20669128,51409914.334740527,50548416.284549087,52029502.709032267,53612295.949181579,55219519.944601573,57311429.024489798,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,70513360.666019693,71042210.871014863,46887859.174869798,43864584.816110939,41036247.654510938,38390278.367432557,35914918.087471642]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,7286944.3646469116,7284726.947080181,10074605.237028589,10148416.399973275,10253801.13669472,10387947.38803984,10489693.866533656]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,10015527.38875098,9718597.1859435439,10492131.337767724,10718905.837883532,10974326.619696923,11276575.979385458,11372051.582090098]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,9634352.70189864,9807412.2284248825,10549685.483982446,10739186.909905847,10932911.743957797,11130772.53048995,11333045.43549449]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":842448157.69125211},840301228.24857974,827696709.82485151,873213538.9510237,921233436.78474212,971894052.47852814,{"$f":"SUM(I13:I25)","v":1025340604.8089949},null,{"$f":"SUM(K13:K25)","v":97450185.121316224},97852947.232463464,78004281.233648553,75471093.963873595,73197287.154860377,71185574.265347809,69109708.971589893]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DREV0201","Revenue from residential Customers ",474144060.94493926,472935732.7704193,473251178.17778158,507567164.35184675,544050472.56501961,582165779.84660053,620292715.67288589,null,63313970.167582162,63788824.943839043,42100624.462933764,39386025.403253466,36846460.518215992,34470643.808813989,32248016.984065462]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",98138403.631672785,97888303.698175296,83123235.793118849,86282800.679460004,89493321.58374016,92605086.332838535,96881638.347460493,null,7199390.4984375406,7253385.9271758245,4787234.7119360426,4478559.4128574776,4189787.1362949531,3919634.5586185707,3666901.1034061848]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",233608301.95965147,233012964.98021728,236364293.48278156,243870415.72419938,251367662.63756993,259862037.91640106,269699792.29987216,null,0,0,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",26968341.893005684,26899614.664271735,27146222.593281832,27831936.884399261,28812027.697946195,29908928.421307307,31233635.995040309,null,0,0,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",9589049.2619828898,9564612.135496432,7811779.777887526,7661221.3111181129,7509952.3004665915,7352219.9613805497,7232822.4937361619,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",0,0,0,0,0,0,0,null,26936824.455296531,26810736.361448608,31116422.058778755,31606509.147762652,32161039.50034944,32795295.897915252,33194790.884118244]
["DREV02","Total revenue by customer class",{"$f":"SUM(C33:C38)","v":842448157.69125211},840301228.24857986,827696709.82485139,873213538.95102358,921233436.78474236,971894052.47852802,1025340604.808995,null,{"$f":"SUM(K33:K38)","v":97450185.121316239},97852947.232463479,78004281.233648568,75471093.963873595,73197287.154860377,71185574.265347809,69109708.971589893]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nFORECAST ($, real \", dms_DollarReal,\")\")","v":"REVENUE \nFORECAST ($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DREV0301","EBSS",-4926338.4206430474,-7616232.7125162762,-15046680.033141483,15015527.070290489,0,-6115299.0211547827,46361348.663272567,null,0,0,0,0,0,0,0]
["DREV0306","CESS",18214343.269634634,18214343.269634634,-23432035.227848962,-23432035.227848962,-23432035.227848962,-23432035.227848962,-23432035.227848962,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",10609867.741849998,13483624,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0307","CSIS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0308","ESIS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0309","DMIS/DMIA/DMIAM",441748.446,35097.301999999996,866011.50266386324,917060.34573095292,944450.67142425198,976067.66460265534,1050303.8831826781,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",288267.59999999998,320808,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV03","Total revenue rewards and penalties - incentive schemes",{"$f":"SUM(C46:C53)","v":24627888.636841584},24437639.859118357,-37612703.758326575,-7499447.8118275199,-22487584.556424711,-28571266.58440109,23979617.318606284,null,{"$f":"SUM(K46:K53)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":14,"n_rows":76,"n_cols":17,"rows_kept":76,"cut":false,"hidden":false,"merged":[[10,2,10,8],[10,10,10,16],[67,2,67,8],[67,10,67,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.2 OPERATING EXPENDITURE"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DOPEX0101","Maintenance - Routine",22299435.239908837,19240415.672980096,21181740.284463581,21439329.756692648,21876701.207874458,22359017.010064952,22731866.410241358]
["DOPEX0102","Maintenance - Condition based",84247679.667323977,72690647.043042034,76961997.267955095,77935175.068583474,79587572.518042311,81409770.558677495,82818402.503490105]
["DOPEX0103","Maintenance - Emergency",28319858.470011,24434961.823060289,24862326.215498496,25189459.944151696,25744913.365417033,26357445.257320698,26830956.901450902]
["DOPEX0104","Maintenance - SCADA/Network Control",0,0,0,0,0,0,0]
["DOPEX0105","Maintenance - AMI",0,0,0,0,0,0,0]
["DOPEX0106","Maintenance - Public Lighting",0,0,0,0,0,0,0,null,4328501.6932231933,4395084.9111169707,3601785.6147425449,3532822.3228559569,3494894.3245605328,3487713.2049801005,3291368.4255929077]
["DOPEX0107","Maintenance - Alternative control -other",0,0,0,0,0,0,0]
["DOPEX0108","Maintenance - Bushfire costs",0,0,0,0,0,0,0]
["DOPEX0109","Network Operating Costs ",66668037.426109135,57021769.289903946,61599957.273118243,62673413.931484506,64077537.887902193,65600948.729693286,66850309.863871336]
["DOPEX0110","Billing & Revenue Collection",621246.39512126823,536024.28711205779,545399.28411236312,552575.5434804525,564760.40083008492,578197.3758116134,588584.69474102603]
["DOPEX0111","Advertising, marketing & promotions",138582.75908794085,119572.08159193461,121663.38217886178,123264.20567010534,125982.30780134656,128979.72248473049,131296.84388465979]
["DOPEX0112","Customer Service",13091588.571829312,11295694.408028493,14780105.193519026,14764729.835933622,15012648.409697071,15286183.994320573,15495942.345066022]
["DOPEX0113","Regulatory",3879341.1634036419,3347176.0929445578,3405717.7795534134,3450529.5620997828,3526617.2771478575,3610523.7763514346,3675386.8551825113]
["DOPEX0114","Regulatory Reset",0,0,0,0,0,0,0]
["DOPEX0115","IT",43013179.712656468,37112664.432280399,41033890.941394418,45277443.038453259,48080987.730661169,50955045.951323666,51951495.214701608]
["DOPEX0116","License fee",1329281.2591270746,1146931.4669518885,1166991.1532772246,1182346.1994610729,1208418.1455475232,1237169.2484312968,1259395.000554573]
["DOPEX0117","GSL payments",7477785.8363803709,7274141.7106110752,11118533.963725287,10793915.778707441,10682662.750790376,10682662.750790376,10682662.750790376]
["DOPEX0118","Non-network alternatives costs",1798031.6401277666,1551379.0271833725,1578512.4501939986,1599282.2148202695,1634548.0275752973,1673437.7601421592,1703501.0783969662]
["DOPEX0119","Metering Cost",4494306,4494306,3998135,4105997.9999999995,4375656,4591383,4724415,null,12500000,{"$f":"AVERAGE(K32,M32)","v":11910620.869754987},11321241.739509974,11619964.875153653,12374765.280047774,12982798.983951945,13365072.837744256]
["DOPEX0120","Other - Standard Control Services",46486377.442868672,40109411.539316416,44829909.1059689,45320559.898912035,46185992.063719966,47145117.18722558,47876043.864152037]
["DOPEX0121","Recoverable works",0,0,0,0,0,0,0]
["DOPEX0122","Software as a Service (SaaS)",7855620.1210982455,6777992.1272828775,8467300.9523474574,8557129.46436687,8709618.405887343,8877802.3927765321,9007511.2749864329]
["DOPEX0123","Export Services",54068.301049233247,21627.3204196933,4025617.1447134786,4934446.3556093629,5440009.6916868445,5898489.9071284318,6551790.1043139193]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C14:C62)","v":331774420.00610292},287174714.32270908,319677797.39201987,327899598.79842657,336834626.19058096,346392174.62254286,352879560.70582378,null,{"$f":"SUM(K14:K61)","v":16828501.693223193},16305705.780871958,14923027.354252519,15152787.19800961,15869659.604608307,16470512.188932046,16656441.263337165]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DOPEX0201","Opex for network services",321835293.81648326,277977574.48534149,310427833.98666698,318406784.24756199,326927991.57120758,336114397.0895108,342363036.48398542]
["DOPEX0202","Opex for metering",4494306,4494306,3998135,4105997.9999999995,4375656,4591383,4724415,null,{"$f":"K32","v":12500000},11910620.869754987,11321241.739509974,11619964.875153653,12374765.280047774,12982798.983951945,13365072.837744256]
["DOPEX0203","Opex for connection services",5427975.533428343,4688284.6665305989,5235580.8084106538,5370151.3407006143,5513867.41459521,5668802.5175859164,5774190.1565493587]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,{"$f":"K19","v":4328501.6932231933},{"$f":"L19","v":4395084.9111169707},3601785.6147425449,3532822.3228559569,3494894.3245605328,3487713.2049801005,3291368.4255929077]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",16844.656191341954,14549.170836989504,16247.596942273483,16665.210163989414,17111.204778190437,17592.015446141297,17919.06528898302]

{"sheet":"3.3 Assets (RAB)","index":15,"n_rows":161,"n_cols":25,"rows_kept":161,"cut":false,"hidden":false,"merged":[[121,2,121,8],[121,10,121,16],[121,18,121,24],[138,2,138,8],[138,10,138,16],[138,18,138,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[24,2,24,8],[24,10,24,16],[24,18,24,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.3 ASSETS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - BENCHMARKING ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",5649699020.0593214,6037264631.378808,6130387534.8676386,6431722233.6966743,6803364371.4568405,7196409335.0373268,7579779209.2020617,null,5664404884.5254173,6052184112.9745483,6144924753.7637386,6445877189.893136,6817137064.9536619,7209799765.8345089,7592787377.2996044,null,{"$f":"S29+S38+S47+S56+S65+S74+S83+S92+S101+S110","v":212419400.12633294},{"$f":"T29+T38+T47+T56+T65+T74+T83+T92+T101+T110","v":191611371.70618218},167614486.58680898,142264024.58324754,142368593.193964,166161153.49796051,203913183.91300926]
["DRAB0102","Inflation addition",228925113.1981217,0,0,0,0,0,0,null,229520993.02740541,0,0,0,0,0,0,null,{"$f":"S30+S39+S48+S57+S66+S75+S84+S93+S102+S111","v":6765942.280550004},0,0,0,0,0,0]
["DRAB0103","Actual straight line depreciation",306688305.78217065,305876109.1236605,312041024.51939654,327390483.19746882,349487843.09304494,363826438.38937545,374241211.96833813,null,307070568.48180991,306258371.82329977,312423287.21903586,327772745.89710814,349870105.7926842,364208701.08901477,374623474.66797733,null,{"$f":"S31+S40+S49+S58+S67+S76+S85+S94+S103+S112","v":46662935.255318895},47628170.224548668,49616180.962911345,23378605.048401441,18557944.35810931,20342463.645766996,21615349.444335185]
["DRAB0104","Gross capex ",498986372.93331903,489618222.29268515,707367220.6439606,743082489.04210043,781780406.58033681,784672486.89594901,795508818.52825642,null,498986372.93331903,489618222.29268515,707367220.6439606,743082489.04210043,781780406.58033681,784672486.89594901,795508818.52825642,null,{"$f":"S32+S41+S50+S59+S68+S77+S86+S95+S104+S113","v":23023373.168289959},{"$f":"T32+T41+T50+T59+T68+T77+T86+T95+T104+T113","v":18938499.299392194},27987459.28792356,27324215.431381322,45964942.728428163,61515994.597170547,61754281.21739421]
["DRAB0108","Capital contributions included in gross capex",47443127.394682318,56738461.901460938,68151312.296833187,55419489.363843992,51504495.742238656,50515178.381060563,51682875.677736454,null,47443127.394682318,56738461.901460938,68151312.296833187,55419489.363843992,51504495.742238656,50515178.381060563,51682875.677736454,null,{"$f":"S33+S42+S51+S60+S69+S78+S87+S96+S105+S114","v":4358526.5173333436},4480565.2598186778,4031427.5915476866,4144307.5641110213,4260348.1759061301,4379637.9248315012,4502267.786726784]
["DRAB0106","Disposals ",1626885.2115873441,1626885.2115873443,36154220.279113159,681891.69533639157,915598.61974006123,700593.47935779823,735595.28820336401,null,1626885.2115873441,1626885.2115873443,36154220.279113159,681891.69533639157,915598.61974006123,700593.47935779823,735595.28820336401,null,{"$f":"S34+S43+S52+S61+S70+S79+S88+S97+S106+S115","v":0},0,0,0,0,0,0]
["DRAB0109","Capex timing adjustment",15412443.576484881,10882896.711637365,10314035.280418718,12051512.974716693,13172494.455171837,13739597.518579675,14637041.286908019,null,15412443.576484881,10882896.711637365,10314035.280418718,12051512.974716693,13172494.455171837,13739597.518579675,14637041.286908019,null,{"$f":"S35+S44+S53+S62+S71+S80+S89+S98+S107+S116","v":424117.90366149537},258714.21164178586,309687.26297402382,303265.79184759408,645910.10958380252,958137.38847669959,1008802.0444772616]
["DRAB0107","Closing value",{"$f":"C14+C15-C16+C17-C18-C19+C20","v":6037264631.378808},6173524294.1464233,6431722233.6966753,6803364371.4568424,7196409335.037324,7579779209.2020617,7963265386.0829487,null,{"$f":"K14+K15-K16+K17-K18-K19+K20","v":6052184112.9745483},6188061513.0425243,6445877189.893136,6817137064.9536648,7209799765.834506,7592787377.2996044,7975891291.4808521,null,{"$f":"S14+S15-S16+S17-S18-S19+S20","v":191611371.70618218},158699849.73284882,142264024.58324751,142368593.19396397,166161153.49796054,203913183.91300926,240558649.94381875]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",2685355287.2872877,2833721206.7606225,2850540024.824327,2944809557.0192928,3048633150.0822306,3168245775.3275061,3301066829.7263813,null,2685355287.2872877,2833721206.7606225,2850540024.824327,2944809557.0192928,3048633150.0822306,3168245775.3275061,3301066829.7263813,null,0,0,0,0,0,0,0]
["DRAB0202","Inflation addition",108810267.75705339,0,0,0,0,0,0,null,108810267.75705339,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Actual straight line depreciation",98103706.82108812,100599558.38279003,101729251.97330031,105649227.65666562,109838684.07105771,114427710.25738437,119372685.55050956,null,98103706.82108812,100599558.38279003,101729251.97330031,105649227.65666562,109838684.07105771,114427710.25738437,119372685.55050956,null,0,0,0,0,0,0,0]
["DRAB0204","Gross capex ",154104050.3236782,152033309.72796568,220172661.5270986,230225803.53130788,248603049.53888997,266540530.38713652,273814248.52463448,null,154104050.3236782,152033309.72796568,220172661.5270986,230225803.53130788,248603049.53888997,266540530.38713652,273814248.52463448,null,0,0,0,0,0,0,0]
["DRAB0208","Capital contributions included in gross capex",21004192.677794669,22498569.735307582,27469636.055956982,24364351.353123933,23222194.851008002,23838226.220933422,25217421.32962653,null,21004192.677794669,22498569.735307582,27469636.055956982,24364351.353123933,23222194.851008002,23838226.220933422,25217421.32962653,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0209","Capex timing adjustment",4559500.891486072,3268878.3705423158,3295758.6971245706,3611368.5414200425,4070454.6284514666,4546460.4900563061,4896742.4154874086,null,4559500.891486072,3268878.3705423158,3295758.6971245706,3611368.5414200425,4070454.6284514666,4546460.4900563061,4896742.4154874086,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"C29+C30-C31+C32-C33-C34+C35","v":2833721206.7606225},2865925266.7410331,2944809557.0192928,3048633150.0822306,3168245775.3275061,3301066829.7263813,3435187713.7863669,null,{"$f":"K29+K30-K31+K32-K33-K34+K35","v":2833721206.7606225},2865925266.7410331,2944809557.0192928,3048633150.0822306,3168245775.3275061,3301066829.7263813,3435187713.7863669,null,{"$f":"S29+S30-S31+S32-S33-S34+S35","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",1213429315.9458208,1298443318.7536089,1323191745.6381872,1390124346.4968154,1462621456.3974402,1544314468.8108392,1633700380.0315042,null,1213429315.9458208,1298443318.7536089,1323191745.6381872,1390124346.4968154,1462621456.3974402,1544314468.8108392,1633700380.0315042,null,0,0,0,0,0,0,0]
["DRAB0302","Inflation addition",49168007.450403921,0,0,0,0,0,0,null,49168007.450403921,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Actual straight line depreciation",44330042.442881726,45457840.864027575,47221686.181836307,49504771.922645599,51944809.559111007,54617565.998561203,57497635.542945728,null,44330042.442881726,45457840.864027575,47221686.181836307,49504771.922645599,51944809.559111007,54617565.998561203,57497635.542945728,null,0,0,0,0,0,0,0]
["DRAB0304","Gross capex ",89753811.838163495,88547763.967242151,128233719.96455905,134088905.56112801,144792244.48572943,155239453.87135333,159475837.84507498,null,89753811.838163495,88547763.967242151,128233719.96455905,134088905.56112801,144792244.48572943,155239453.87135333,159475837.84507498,null,0,0,0,0,0,0,0]
["DRAB0308","Capital contributions included in gross capex",12233334.253419366,13103694.486998986,15998960.057511013,14190369.443983311,13525150.719586831,13883941.832127735,14687217.398303665,null,12233334.253419366,13103694.486998986,15998960.057511013,14190369.443983311,13525150.719586831,13883941.832127735,14687217.398303665,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0309","Capex timing adjustment",2655560.2155221263,1903871.40101286,1919527.1334166825,2103345.7061256319,2370728.206367448,2647965.1800006032,2851977.5856409073,null,2655560.2155221263,1903871.40101286,1919527.1334166825,2103345.7061256319,2370728.206367448,2647965.1800006032,2851977.5856409073,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"C38+C39-C40+C41-C42-C43+C44","v":1298443318.7536089},1330333418.7708375,1390124346.4968154,1462621456.3974402,1544314468.8108392,1633700380.0315042,1723843342.5209706,null,{"$f":"K38+K39-K40+K41-K42-K43+K44","v":1298443318.7536089},1330333418.7708375,1390124346.4968154,1462621456.3974402,1544314468.8108392,1633700380.0315042,1723843342.5209706,null,{"$f":"S38+S39-S40+S41-S42-S43+S44","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",377658736.4972536,426091373.41901618,451948418.00845832,506961948.097247,567271784.08842492,627992488.12568462,688600410.62700486,null,377658736.4972536,423046134.9461413,448809612.32725692,495271145.66198391,544778226.45193911,599318376.15865529,658068976.0971843,null,0,0,0,0,0,0,0]
["DRAB0402","Inflation addition",15302685.806081334,0,0,0,0,0,0,null,15302685.806081334,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Actual straight line depreciation",13779516.215497794,14130523.827689486,14563571.322688809,15955113.350918356,17481167.211217768,19047026.996934392,20643565.592236739,null,13796953.475447305,14147961.087638995,16016988.269895457,17266558.701987904,18602031.491826769,20064875.115797628,21641184.616884157,null,0,0,0,0,0,0,0]
["DRAB0404","Gross capex ",50916208.413022272,49884646.615236223,79649394.615539193,87809979.285556242,88673057.004634991,89445279.96093379,90522585.437018678,null,49123739.610761493,48463649.745429873,70184427.155213296,73389066.676676318,79247180.371567696,84965110.150905207,87283752.879879728,null,0,0,0,0,0,0,0]
["DRAB0408","Capital contributions included in gross capex",5560458.608847349,5834589.5929232929,10072293.20406167,11545029.943459962,10471185.756157547,9790330.4626791961,10266755.579645444,null,6695505.3398730233,7171867.8319643876,8756494.3684538454,7766622.9352316046,7402537.7701315666,7598910.0559002757,8038556.0045276638,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0409","Capex timing adjustment",1553717.5270040615,1111626.7236847493,0,0,0,0,0,null,1453431.8473651567,1042020.1776429097,1050588.8178629801,1151195.7504984289,1297538.5971068442,1449274.9593215883,1560934.309345752,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"C47+C48-C49+C50-C51-C52+C53","v":426091373.41901618},457122533.33732438,506961948.097247,567271784.08842492,627992488.12568462,688600410.62700486,748212674.89214134,null,{"$f":"K47+K48-K49+K50-K51-K52+K53","v":423046134.9461413},451231975.94961071,495271145.66198391,544778226.45193911,599318376.15865529,658068976.0971843,717233922.66499794,null,{"$f":"S47+S48-S49+S50-S51-S52+S53","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",243653673.47775745,254811326.16725034,269879646.02936155,270082626.32915592,277621321.93740213,287454749.13035905,293687846.43097937,null,243653673.47775745,254811326.16725034,269879646.02936155,270082626.32915592,277621321.93740213,287454749.13035905,293687846.43097937,null,0,0,0,0,0,0,0]
["DRAB0502","Inflation addition",9872817.0445880033,0,0,0,0,0,0,null,9872817.0445880033,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Actual straight line depreciation",7769153.5522057386,7934105.6362109827,8444912.5848781932,8637087.9823153615,8996549.8398833964,9414993.7739465125,9762729.13115911,null,7769153.5522057386,7934105.6362109827,8444912.5848781932,8637087.9823153615,8996549.8398833964,9414993.7739465125,9762729.13115911,null,0,0,0,0,0,0,0]
["DRAB0504","Gross capex ",9602260.5377253015,10487923.899868354,10492122.070091199,17033529.916285984,19414737.764171705,16009243.985862575,14718177.524477275,null,9602260.5377253015,10487923.899868354,10492122.070091199,17033529.916285984,19414737.764171705,16009243.985862575,14718177.524477275,null,0,0,0,0,0,0,0]
["DRAB0508","Capital contributions included in gross capex",848154.12558728806,1744548.2432250543,1989645.2312752453,1136621.2451105863,918803.57203401753,648893.18742701609,467194.19368490536,null,848154.12558728806,1744548.2432250543,1989645.2312752453,1136621.2451105863,918803.57203401753,648893.18742701609,467194.19368490536,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0509","Capex timing adjustment",299882.78497262287,220643.75603909377,145416.04585665651,278874.91938616708,334042.84070260078,287740.27613132633,280709.11171989515,null,299882.78497262287,220643.75603909377,145416.04585665651,278874.91938616708,334042.84070260078,287740.27613132633,280709.11171989515,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"C56+C57-C58+C59-C60-C61+C62","v":254811326.16725034},255841239.94372174,270082626.32915592,277621321.93740213,287454749.13035905,293687846.43097937,298456809.74233258,null,{"$f":"K56+K57-K58+K59-K60-K61+K62","v":254811326.16725034},255841239.94372174,270082626.32915592,277621321.93740213,287454749.13035905,293687846.43097937,298456809.74233258,null,{"$f":"S56+S57-S58+S59-S60-S61+S62","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",2457203.7127429694,3199734.1522835633,4044238.0279146014,4606650.5403605504,5753486.5685856938,7083139.8196876654,8125961.1307305666,null,2457203.7127429694,3199734.1522835633,4044238.0279146014,4606650.5403605504,5753486.5685856938,7083139.8196876654,8125961.1307305666,null,0,0,0,0,0,0,0]
["DRAB0602","Inflation addition",99565.59386496713,0,0,0,0,0,0,null,99565.59386496713,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Actual straight line depreciation",78350.52384339647,80014.036104291547,126549.87925418903,141860.1546253032,170497.8475775354,203834.53865930217,231538.00198601783,null,78350.52384339647,80014.036104291547,126549.87925418903,141860.1546253032,170497.8475775354,203834.53865930217,231538.00198601783,null,0,0,0,0,0,0,0]
["DRAB0604","Gross capex ",764995.18137238431,835554.42121967138,835888.88204568624,1357031.3215858613,1546737.9560103221,1275428.2659259012,1172571.2753338483,null,764995.18137238431,835554.42121967138,835888.88204568624,1357031.3215858613,1546737.9560103221,1275428.2659259012,1172571.2753338483,null,0,0,0,0,0,0,0]
["DRAB0608","Capital contributions included in gross capex",67570.945048434063,138985.08528232187,158511.53054910462,90552.612287383119,73199.461988381387,51696.17713003941,37220.53838572208,null,67570.945048434063,138985.08528232187,158511.53054910462,90552.612287383119,73199.461988381387,51696.17713003941,37220.53838572208,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0609","Capex timing adjustment",23891.133195072885,17578.299350102407,11585.040203556069,22217.473551969277,26612.604657566175,22923.76090634265,22363.600424021948,null,23891.133195072885,17578.299350102407,11585.040203556069,22217.473551969277,26612.604657566175,22923.76090634265,22363.600424021948,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"C65+C66-C67+C68-C69-C70+C71","v":3199734.1522835633},3833867.7514667232,4606650.5403605504,5753486.5685856938,7083139.8196876654,8125961.1307305666,9052137.4661166966,null,{"$f":"K65+K66-K67+K68-K69-K70+K71","v":3199734.1522835633},3833867.7514667232,4606650.5403605504,5753486.5685856938,7083139.8196876654,8125961.1307305666,9052137.4661166966,null,{"$f":"S65+S66-S67+S68-S69-S70+S71","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",620666344.89940739,698329563.76130235,782862165.3428601,823782815.08001482,912430361.33761823,1016491021.1308911,1095311080.8475003,null,620666344.89940739,698329563.76130235,782862165.3428601,823782815.08001482,912430361.33761823,1016491021.1308911,1095311080.8475003,null,0,0,0,0,0,0,0]
["DRAB0702","Inflation addition",25149324.372835245,0,0,0,0,0,0,null,25149324.372835245,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Actual straight line depreciation",19081245.058195323,19486371.706370588,23398762.226223972,24729554.814707235,27218786.955103189,30116463.211134031,32524490.681369409,null,19081245.058195323,19486371.706370588,23398762.226223972,24729554.814707235,27218786.955103189,30116463.211134031,32524490.681369409,null,0,0,0,0,0,0,0]
["DRAB0704","Gross capex ",75097162.631434709,75627670.246315196,112460690.3765633,119293420.71196264,135313165.36675814,111426886.9313821,104599175.87653796,null,75097162.631434709,75627670.246315196,112460690.3765633,119293420.71196264,135313165.36675814,111426886.9313821,104599175.87653796,null,0,0,0,0,0,0,0]
["DRAB0708","Capital contributions included in gross capex",5873370.0529595343,12080796.518682608,13778065.053086998,7870971.7741071768,6362609.3674898576,4493510.9075420815,3235266.2132079666,null,5873370.0529595343,12080796.518682608,13778065.053086998,7870971.7741071768,6362609.3674898576,4493510.9075420815,3235266.2132079666,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",0,0,35444757.116972484,0,0,0,0,null,0,0,35444757.116972484,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0709","Capex timing adjustment",2371346.9687799173,1603639.3098532152,1081543.7568748146,1954652.1344552934,2328890.7491077632,2003146.9039032906,1996618.2249731869,null,2371346.9687799173,1603639.3098532152,1081543.7568748146,1954652.1344552934,2328890.7491077632,2003146.9039032906,1996618.2249731869,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"C74+C75-C76+C77-C78-C79+C80","v":698329563.76130235},743993705.0924176,823782815.08001482,912430361.33761823,1016491021.1308911,1095311080.8475003,1166147118.0544341,null,{"$f":"K74+K75-K76+K77-K78-K79+K80","v":698329563.76130235},743993705.0924176,823782815.08001482,912430361.33761823,1016491021.1308911,1095311080.8475003,1166147118.0544341,null,{"$f":"S74+S75-S76+S77-S78-S79+S80","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0802","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[null,"Actual straight line depreciation"]
["DRAB0804","Gross capex ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0808","Capital contributions included in gross capex",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0806","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0809","Capex timing adjustment",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0807","Closing value",{"$f":"C83+C84-C85+C86-C87-C88+C89","v":0},0,0,0,0,0,0,null,{"$f":"K83+K84-K85+K86-K87-K88+K89","v":0},0,0,0,0,0,0,null,{"$f":"S83+S84-S85+S86-S87-S88+S89","v":0},0,0,0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,166978349.11244208,142558707.53125787,118568654.27805707,90264839.43214044,87534623.088704795,108594803.33232948,143713329.99104843]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,6765942.280550004,0,0,0,0,0,0]
["DRAB0903","Actual straight line depreciation",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,43990449.997691132,44844103.445440076,46720917.732806891,20320761.345275983,15349738.026620723,16987564.703994039,18113254.245472513]
["DRAB0904","Gross capex ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,12380748.23229542,10251980.752610395,18107415.623916231,17287279.209992733,35764008.160661608,51147953.974236295,51214657.877796836]
["DRAB0908","Capital contributions included in gross capex",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0909","Capex timing adjustment",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,424117.90366149537,258714.21164178586,309687.26297402382,303265.79184759408,645910.10958380252,958137.38847669959,1008802.0444772616]
["DRAB0907","Closing value",{"$f":"C92+C93-C94+C95-C96-C97+C98","v":0},0,0,0,0,0,0,null,{"$f":"K92+K93-K94+K95-K96-K97+K98","v":0},0,0,0,0,0,0,null,{"$f":"S92+S93-S94+S95-S96-S97+S98","v":142558707.53125787},108225299.05006997,90264839.43214044,87534623.088704795,108594803.33232948,143713329.99104843,177823535.66784999]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",283646894.86742508,267854825.42815414,201109383.2303758,235044256.03673965,250354594.84239551,271854103.70382166,304579913.70786631,null,298352759.33352053,282774307.02389407,215646602.12647635,249199212.23320091,264127288.33921751,285244534.5010044,317588081.80540979,null,45441051.01389087,49052664.174924299,49045832.308751903,{"$f":"U108","v":51999185.151107088},{"$f":"V108","v":54833970.105259195},57566350.165631033,60199853.921960823]
["DRAB1002","Inflation addition",11493337.48316016,0,0,0,0,0,0,null,12089217.312443841,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1003","Actual straight line depreciation",57524880.425266497,54316185.024335489,34344468.073456533,36827448.631323524,38149829.490631551,36319534.077104449,37683529.87814115,null,57907143.12490578,54698447.723974772,34726730.773095816,37209711.330962814,38532092.190270841,36701796.776743732,38065792.577780433,null,2672485.2576277647,2784066.7791085881,2895263.2301044529,3057843.7031254573,3208206.3314885884,3354898.9417729545,3502095.1988626709]
["DRAB1004","Gross capex ",29237893.168165918,27418560.533902086,67174857.62632449,51254993.79844524,58840945.061494738,67810502.090185881,69146709.208124056,null,29237893.168165918,27418560.533902086,67174857.62632449,51254993.79844524,58840945.061494738,67810502.090185881,69146709.208124056,null,10642624.935994539,8686518.546781797,9880043.6640073285,10036936.22138859,10200934.567766555,10368040.622934248,10539623.339597372]
["DRAB1008","Capital contributions included in gross capex",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,4358526.5173333436,4480565.2598186778,4031427.5915476866,4144307.5641110213,4260348.1759061301,4379637.9248315012,4502267.786726784]
["DRAB1006","Disposals ",0,0,43647.498914373093,16076.032110091744,249782.95651376146,34777.816131498475,69779.624977064217,null,0,0,43647.498914373093,16076.032110091744,249782.95651376146,34777.816131498475,69779.624977064217,null,0,0,0,0,0,0,0]
["DRAB1009","Capex timing adjustment",1001580.3346695014,691922.02405129094,1148130.7524102181,898869.67064425349,1058176.2470767349,1269619.807094723,1360644.6020974219,null,1001580.3346695014,691922.02405129094,1148130.7524102181,898869.67064425349,1058176.2470767349,1269619.807094723,1360644.6020974219,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"C101+C102-C103+C104-C105-C106+C107","v":267854825.42815414},241649122.96177202,235044256.03673965,250354594.84239551,271854103.70382166,304579913.70786631,337333958.01496959,null,{"$f":"K101+K102-K103+K104-K105-K106+K107","v":282774307.02389407},256186341.85787266,249199212.23320091,264127288.33921751,285244534.5010044,317588081.80540979,349959863.41287374,null,{"$f":"S101+S102-S103+S104-S105-S106+S107","v":49052664.174924299},50474550.682778828,51999185.151107088,54833970.105259195,57566350.165631033,60199853.921960823,62735114.27596873]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",222831563.37162694,257858521.40944386,249950719.44735461,268000836.53231108,301171773.83922982,301647700.95556593,285238221.22991472,null,222831563.37162694,257858521.40944386,249950719.44735461,268000836.53231108,301171773.83922982,301647700.95556593,285238221.22991472,null,0,0,0,0,0,0,0]
["DRAB1102","Inflation addition",9029107.690134706,0,0,0,0,0,0,null,9029107.690134706,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1103","Actual straight line depreciation",66003973.483242489,63854072.386182517,80758405.330551565,84633973.333198324,94566653.837853774,98661461.416787937,95527418.565342993,null,66003973.483242489,63854072.386182517,80758405.330551565,84633973.333198324,94566653.837853774,98661461.416787937,95527418.565342993,null,0,0,0,0,0,0,0]
["DRAB1104","Gross capex ",91302459.642017603,86203789.750742167,97812853.042065069,116439737.52470845,94022346.03571482,81405331.213197544,85298345.394194081,null,91302459.642017603,86203789.750742167,97812853.042065069,116439737.52470845,94022346.03571482,81405331.213197544,85298345.394194081,null,0,0,0,0,0,0,0]
["DRAB1108","Capital contributions included in gross capex",721000,0,0,0,0,0,0,null,721000,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1106","Disposals ",1626885.2115873441,1626885.2115873443,665815.6632262998,665815.6632262998,665815.6632262998,665815.6632262998,665815.6632262998,null,1626885.2115873441,1626885.2115873443,665815.6632262998,665815.6632262998,665815.6632262998,665815.6632262998,665815.6632262998,null,0,0,0,0,0,0,0]
["DRAB1109","Capex timing adjustment",3047249.4004944172,2134343.3731455789,1661485.0366692394,2030988.7786349058,1686050.5817014128,1512466.1411654949,1667051.437219426,null,3047249.4004944172,2134343.3731455789,1661485.0366692394,2030988.7786349058,1686050.5817014128,1512466.1411654949,1667051.437219426,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"C110+C111-C112+C113-C114-C115+C116","v":257858521.40944386},280715696.93556172,268000836.53231108,301171773.83922982,301647700.95556593,285238221.22991472,276010383.83275896,null,{"$f":"K110+K111-K112+K113-K114-K115+K116","v":257858521.40944386},280715696.93556172,268000836.53231108,301171773.83922982,301647700.95556593,285238221.22991472,276010383.83275896,null,{"$f":"S110+S111-S112+S113-S114-S115+S116","v":0},0,0,0,0,0,0]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED BENCHMARKING ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nFORECAST\n($, real \", dms_DollarReal, \")\")","v":" VALUE \nFORECAST\n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",{"$f":"IFERROR(AVERAGE(C29,C36),\"\")","v":2759538247.0239553},2849823236.7508278,2897674790.9218102,2996721353.5507617,3108439462.7048683,3234656302.5269437,3368127271.7563744,null,{"$f":"IFERROR(AVERAGE(K29,K36),\"\")","v":2759538247.0239553},2849823236.7508278,2897674790.9218102,2996721353.5507617,3108439462.7048683,3234656302.5269437,3368127271.7563744,null,{"$f":"IFERROR(AVERAGE(S29,S36),\"\")","v":0},0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",{"$f":"IFERROR(AVERAGE(C38,C45),\"\")","v":1255936317.3497148},1314388368.7622232,1356658046.0675013,1426372901.4471278,1503467962.6041398,1589007424.4211717,1678771861.2762375,null,{"$f":"IFERROR(AVERAGE(K38,K45),\"\")","v":1255936317.3497148},1314388368.7622232,1356658046.0675013,1426372901.4471278,1503467962.6041398,1589007424.4211717,1678771861.2762375,null,{"$f":"IFERROR(AVERAGE(S38,S45),\"\")","v":0},0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",{"$f":"IFERROR(AVERAGE(C47,C54),\"\")","v":401875054.95813489},441606953.37817025,479455183.05285263,537116866.0928359,597632136.10705471,658296449.37634468,718406542.7595731,null,{"$f":"IFERROR(AVERAGE(K47,K54),\"\")","v":400352435.72169745},437139055.44787598,472040378.99462044,520024686.05696154,572048301.30529714,628693676.12791979,687651449.38109112,null,{"$f":"IFERROR(AVERAGE(S47,S54),\"\")","v":0},0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",{"$f":"IFERROR(AVERAGE(C56,C63),\"\")","v":249232499.82250389},255326283.05548602,269981136.1792587,273851974.13327903,282538035.53388059,290571297.78066921,296072328.08665597,null,{"$f":"IFERROR(AVERAGE(K56,K63),\"\")","v":249232499.82250389},255326283.05548602,269981136.1792587,273851974.13327903,282538035.53388059,290571297.78066921,296072328.08665597,null,{"$f":"IFERROR(AVERAGE(S56,S63),\"\")","v":0},0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",{"$f":"IFERROR(AVERAGE(C65,C72),\"\")","v":2828468.9325132663},3516800.9518751432,4325444.2841375759,5180068.5544731226,6418313.1941366792,7604550.475209116,8589049.2984236311,null,{"$f":"IFERROR(AVERAGE(K65,K72),\"\")","v":2828468.9325132663},3516800.9518751432,4325444.2841375759,5180068.5544731226,6418313.1941366792,7604550.475209116,8589049.2984236311,null,{"$f":"IFERROR(AVERAGE(S65,S72),\"\")","v":0},0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",{"$f":"IFERROR(AVERAGE(C74,C81),\"\")","v":659497954.33035493},721161634.42685997,803322490.21143746,868106588.20881653,964460691.2342546,1055901050.9891957,1130729099.4509673,null,{"$f":"IFERROR(AVERAGE(K74,K81),\"\")","v":659497954.33035493},721161634.42685997,803322490.21143746,868106588.20881653,964460691.2342546,1055901050.9891957,1130729099.4509673,null,{"$f":"IFERROR(AVERAGE(S74,S81),\"\")","v":0},0,0,0,0,0,0]
["DRAB1207","Easements ",{"$f":"IFERROR(AVERAGE(C83,C90),\"\")","v":0},0,0,0,0,0,0,null,{"$f":"IFERROR(AVERAGE(K83,K90),\"\")","v":0},0,0,0,0,0,0,null,{"$f":"IFERROR(AVERAGE(S83,S90),\"\")","v":0},0,0,0,0,0,0]
["DRAB1208","Meters",{"$f":"IFERROR(AVERAGE(C92,C99),\"\")","v":0},{"$f":"IFERROR(AVERAGE(D92,D99),\"\")","v":0},0,0,0,0,0,null,{"$f":"IFERROR(AVERAGE(K92,K99),\"\")","v":0},{"$f":"IFERROR(AVERAGE(L92,L99),\"\")","v":0},0,0,0,0,0,null,{"$f":"IFERROR(AVERAGE(S92,S99),\"\")","v":154768528.32184997},{"$f":"IFERROR(AVERAGE(T92,T99),\"\")","v":125392003.29066393},104416746.85509875,88899731.260422617,98064713.210517138,126154066.66168895,160768432.82944921]
["DRAB1209","“Other” assets with long lives",{"$f":"IFERROR(AVERAGE(C101,C108),\"\")","v":275750860.1477896},{"$f":"IFERROR(AVERAGE(D101,D108),\"\")","v":254751974.1949631},{"$f":"IFERROR(AVERAGE(E101,E108),\"\")","v":218076819.63355774},242699425.43956757,261104349.2731086,288217008.70584399,320956935.86141795,null,{"$f":"IFERROR(AVERAGE(K101,K108),\"\")","v":290563533.1787073},{"$f":"IFERROR(AVERAGE(L101,L108),\"\")","v":269480324.4408834},232422907.17983863,256663250.28620923,274685911.42011094,301416308.15320706,333773972.60914177,null,{"$f":"IFERROR(AVERAGE(S101,S108),\"\")","v":47246857.594407588},{"$f":"IFERROR(AVERAGE(T101,T108),\"\")","v":49763607.42885156},50522508.729929492,53416577.628183141,56200160.135445118,58883102.043795928,61467484.098964781]
["DRAB1210","“Other” assets with short lives",{"$f":"IFERROR(AVERAGE(C110,C117),\"\")","v":240345042.39053541},{"$f":"IFERROR(AVERAGE(D110,D117),\"\")","v":269287109.17250276},258975777.98983285,284586305.18577045,301409737.39739788,293442961.0927403,280624302.53133684,null,{"$f":"IFERROR(AVERAGE(K110,K117),\"\")","v":240345042.39053541},{"$f":"IFERROR(AVERAGE(L110,L117),\"\")","v":269287109.17250276},258975777.98983285,284586305.18577045,301409737.39739788,293442961.0927403,280624302.53133684,null,{"$f":"IFERROR(AVERAGE(S110,S117),\"\")","v":0},{"$f":"IFERROR(AVERAGE(T110,T117),\"\")","v":0},0,0,0,0,0]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)"]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"FORECAST\n( years )",null,null,null,null,null,null,null,"FORECAST\n( years )",null,null,null,null,null,null,null,"FORECAST\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",63.8,63.8,63.8,63.8,63.8,63.8,63.8,null,63.8,63.8,63.8,63.8,63.8,63.8,63.8]
["DRAB1402","Underground network assets less than 33kV (cables)",50,50,50,50,50,50,50,null,50,50,50,50,50,50,50]
["DRAB1403","Distribution substations including transformers",52.2,52.2,52.2,52.2,52.2,52.2,52.2,null,52.2,52.2,52.2,52.2,52.2,52.2,52.2]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",71.7,71.7,71.7,71.7,71.7,71.7,71.7,null,71.7,71.7,71.7,71.7,71.7,71.7,71.7]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",50,50,50,50,50,50,50,null,50,50,50,50,50,50,50]
["DRAB1406","Zone substations and transformers",45.9,45.9,45.9,45.9,45.9,45.9,45.9,null,45.9,45.9,45.9,45.9,45.9,45.9,45.9]
["DRAB1407","Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.368160145942658,{"$f":"$S149","v":13.368160145942658},{"$f":"$S149","v":13.368160145942658},13.368160145942658,13.368160145942658,13.368160145942658,13.368160145942658]
["DRAB1408","“Other” assets with long lives",15,15,15,15,15,15,15,null,15,15,15,15,15,15,15,null,23.353651984007712,24.567634250368094,25.429551434890577,25.58189948731566,26.696341106966543,26.511673326622528,25.878454580742581]
["DRAB1409","“Other” assets with short lives",5,5,5,5,5,5,5,null,5,5,5,5,5,5,5]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",26.068014059290995,{"$f":"$C153","v":26.068014059290995},{"$f":"$C153","v":26.068014059290995},26.068014059290995,26.068014059290995,26.068014059290995,26.068014059290995,null,26.068014059290995,{"$f":"$K153","v":26.068014059290995},{"$f":"$K153","v":26.068014059290995},26.068014059290995,26.068014059290995,26.068014059290995,26.068014059290995]
["DRAB1502","Underground network assets less than 33kV (cables)",27.59012754355814,{"$f":"$C154","v":27.59012754355814},27.59012754355814,27.59012754355814,27.59012754355814,27.59012754355814,27.59012754355814,null,27.59012754355814,{"$f":"$K154","v":27.59012754355814},27.59012754355814,27.59012754355814,27.59012754355814,27.59012754355814,27.59012754355814]
["DRAB1503","Distribution substations including transformers",23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,null,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561,23.978009915976561]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,null,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601,36.119408726195601]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,null,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345,20.599581042600345]
["DRAB1506","Zone substations and transformers",12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,null,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995,12.059999999999995]
["DRAB1507","Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.463297523971792,4.4846583448554149,5.872079574036694,10.098409440008338,11.210730643209491,12.161681768465142,12.507460523680821]
["DRAB1508","“Other” assets with long lives",8.9214534289210619,8.9765536074607102,12.680233299976607,13.532614580686991,13.952908275745349,14.061394777133007,13.991024982339681,null,10.519609523222542,10.947695804529834,13.909381591324477,14.489427456372271,14.70469623524977,14.661258444108809,14.486258940072393,null,20.99106649286454,21.031053783910721,20.895688282605271,20.769272587097966,20.651305918212906,20.544356269675852,20.449755794899957]
["DRAB1509","“Other” assets with short lives",3.7171199861813311,3.6689841186181287,3.8245377808834164,3.8544715886784675,3.72755121718173,3.5802435054881561,3.4772905819504563,null,3.7171199861813311,3.6689841186181287,3.8245377808834164,3.8544715886784675,3.72755121718173,3.5802435054881561,3.4772905819504563]

{"sheet":"3.4 Operational data","index":16,"n_rows":110,"n_cols":10,"rows_kept":110,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.4 OPERATIONAL DATA"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped for ease of navigation. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DOPED01","TOTAL ENERGY DELIVERED"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",1943.7214340450948,1914.1255404120718,1907.0248630686651,1897.4710069813805,1882.3109782524148,1851.4284998706989,1797.527324373129]
["DOPED0202","Energy Delivery at On-peak times","GWh",2049.3075586684754,2118.7548992024176,2193.7470927343729,2272.2496736898802,2351.7720469169753,2443.552634042906,2522.4047234829986]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",436.86109240432774,455.7972303272112,457.82257106372629,461.86911242534597,465.19357084401753,468.59509039282466,472.55925250173624]
["DOPED0204","Energy Delivery at Off-peak times","GWh",3196.745680692381,3410.9609820133273,3618.6600534217787,3848.8169436478865,4102.7422245886528,4364.8367203050502,4605.8270459704872]
["DOPED0205","Controlled load energy deliveries","GWh",0,0,0,0,0,0,0]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",255.52130627130282,253.22134868527201,250.92139109924122,248.60987593740123,246.30991835137041,244.0099607653396,241.71000317930881]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh"]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh"]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh"]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",5914.6044504948159,6083.9885010295293,6276.260853495457,6506.5108899776042,6780.6466695427625,7062.01594750412,7282.758112997275]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh"]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh"]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh"]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",1355.9857388451408,1361.5892444992141,1366.3326120014422,1370.4731809623484,1373.3518421758879,1376.0768506175959,1379.006389285827]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh"]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh"]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh"]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",936.66146946031961,1043.5418130276712,1133.1972970139411,1212.0553149764037,1267.5228273041062,1320.8897663829864,1375.8607237623237]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",3724.4031711422085,3913.3489298177356,4167.5552046735957,4446.5293572922665,4733.8718948724318,5021.912301020976,5256.898321874829]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",987.48463505791347,1005.7434827609273,1020.2945979483247,1030.3344749297637,1040.2212764542312,1048.0716287531018,1058.1529632737509]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",2398.3066287106694,2404.5134276098215,2417.024360955792,2439.2676597677314,2460.800449884583,2485.5432646593408,2506.9712843991852]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",771.96263717079,829.25416045181453,823.30180781007221,812.88512069213323,813.43511774218211,816.89571094339919,818.00577995989431]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.4.2 - CUSTOMER NUMBERS (Benchmarking)"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"3.4.2.1 - Distribution customer numbers by customer type or class"]
["DOPCN0101","Residential customer numbers","number",742654,757541,772526,787511,802495,817477,832461]
["DOPCN0102","Non residential customers not on demand tariff customer numbers","number",61762,62283,62797,63309,63823,64339,64856]
["DOPCN0103","Low voltage demand tariff customer numbers","number",12520,12589,12697,12857,13059,13305,13603]
["DOPCN0104","High voltage demand tariff customer numbers","number",125,187,299,465,671,920,1220]
["DOPCN0105","Unmetered Customer Numbers","number",5539,5338,5139,4940,4740,4541,4342]
["DOPCN0106","Other Customer Numbers","number",0,0,0,0,0,0,0]
[null,"Total customer numbers",null,{"$f":"SUM(D48:D53)","v":822600},{"$f":"SUM(E48:E53)","v":837938},853458,869082,884788,900582,916482]
[]
[]
[null,"Table 3.4.2.2 Distribution customer numbers by location on the network"]
["DOPCN0201",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},"number",0,0,null,null,null,null,{"$f":"+(J54/E54)^(0.2)-1","v":1.8081183534125911E-2}]
["DOPCN0202",{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},"number",{"$f":"('6.2 Reliability & Cust serv'!C63/'6.2 Reliability & Cust serv'!$C$67)*'3.4 Operational data'!$D$54","v":356478},{"$f":"('6.2 Reliability & Cust serv'!D63/'6.2 Reliability & Cust serv'!D$67)*'3.4 Operational data'!E$54","v":361899},{"$f":"('6.2 Reliability & Cust serv'!E63/'6.2 Reliability & Cust serv'!E$67)*'3.4 Operational data'!F$54","v":372929},{"$f":"('6.2 Reliability & Cust serv'!F63/'6.2 Reliability & Cust serv'!F$67)*'3.4 Operational data'!G$54","v":380943},{"$f":"('6.2 Reliability & Cust serv'!G63/'6.2 Reliability & Cust serv'!G$67)*'3.4 Operational data'!H$54","v":388386.43895988527},{"$f":"('6.2 Reliability & Cust serv'!H63/'6.2 Reliability & Cust serv'!H$67)*'3.4 Operational data'!I$54","v":392563},{"$f":"('6.2 Reliability & Cust serv'!I63/'6.2 Reliability & Cust serv'!I$67)*'3.4 Operational data'!J$54","v":399960}]
["DOPCN0203",{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},"number",{"$f":"('6.2 Reliability & Cust serv'!C64/'6.2 Reliability & Cust serv'!$C$67)*'3.4 Operational data'!$D$54","v":327761},{"$f":"('6.2 Reliability & Cust serv'!D64/'6.2 Reliability & Cust serv'!D$67)*'3.4 Operational data'!E$54","v":336145},{"$f":"('6.2 Reliability & Cust serv'!E64/'6.2 Reliability & Cust serv'!E$67)*'3.4 Operational data'!F$54","v":337766},{"$f":"('6.2 Reliability & Cust serv'!F64/'6.2 Reliability & Cust serv'!F$67)*'3.4 Operational data'!G$54","v":342235},{"$f":"('6.2 Reliability & Cust serv'!G64/'6.2 Reliability & Cust serv'!G$67)*'3.4 Operational data'!H$54","v":348149.39348340331},{"$f":"('6.2 Reliability & Cust serv'!H64/'6.2 Reliability & Cust serv'!H$67)*'3.4 Operational data'!I$54","v":357105},{"$f":"('6.2 Reliability & Cust serv'!I64/'6.2 Reliability & Cust serv'!I$67)*'3.4 Operational data'!J$54","v":363059}]
["DOPCN0204",{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},"number",{"$f":"('6.2 Reliability & Cust serv'!C65/'6.2 Reliability & Cust serv'!$C$67)*'3.4 Operational data'!$D$54","v":138361},{"$f":"('6.2 Reliability & Cust serv'!D65/'6.2 Reliability & Cust serv'!D$67)*'3.4 Operational data'!E$54","v":139894},{"$f":"('6.2 Reliability & Cust serv'!E65/'6.2 Reliability & Cust serv'!E$67)*'3.4 Operational data'!F$54","v":142763},{"$f":"('6.2 Reliability & Cust serv'!F65/'6.2 Reliability & Cust serv'!F$67)*'3.4 Operational data'!G$54","v":145904},{"$f":"('6.2 Reliability & Cust serv'!G65/'6.2 Reliability & Cust serv'!G$67)*'3.4 Operational data'!H$54","v":148252.16755671139},{"$f":"('6.2 Reliability & Cust serv'!H65/'6.2 Reliability & Cust serv'!H$67)*'3.4 Operational data'!I$54","v":150914},{"$f":"('6.2 Reliability & Cust serv'!I65/'6.2 Reliability & Cust serv'!I$67)*'3.4 Operational data'!J$54","v":153463}]
["DOPCN0205",{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},"number"]
[null,"Total customer numbers",null,{"$f":"SUM(D58:D62)","v":822600},{"$f":"SUM(E58:E62)","v":837938},853458,869082,884787.99999999988,900582,916482.01808118355]
[]
[]
[null," 3.4.2.4 - Unmetered Supply"]
["DOPCN0301","Number of unmetered connections reported in customer numbers in the economic benchmarking RIN",null,{"$f":"D52","v":5539},{"$f":"E52","v":5338},5139,4940,4740,4541,4342]
["DOPCN0302","Unmetered connections not reported in customer numbers in the economic benchmarking RIN",null,0,0,0,0,0,0,0]
["DOPCN0303","Total unmetered connections",null,{"$f":"SUM(D67:D68)","v":5539},{"$f":"SUM(E67:E68)","v":5338},5139,4940,4740,4541,4342]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2320.96,2371.7600000000002,2430.12,2496.8000000000002,2565.9,2637.62,2704.66]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2080.85,2127.69,2185.36,2252.4699999999998,2317.2199999999998,2385.06,2449.19]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2020.08,2065.12,2116.7800000000002,2175.9499999999998,2237.1799999999998,2300.7199999999998,2360]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1793.43,1834.7,1885.49,1944.72,2001.83,2061.61,2117.85]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2040.77,2080.77,2126.67,2178.33,2232.7199999999998,2289.77,2347.17]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1872.2,1908.55,1948.6,1993.46,2042.52,2093.02,2144.0300000000002]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",1816.35,1852.43,1893.74,1940.33,1989.45,2040.93,2092.7199999999998]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1655.57,1688.13,1724.02,1764.21,1808.08,1853.2,1898.84]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2418.09,2473.4,2537.6799999999998,2610.65,2685.84,2765.48,2842.88]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2105.84,2160.56,2224.39,2296.5,2368.0300000000002,2442.96,2515.4899999999998]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2042,2087.4899999999998,2139.62,2199.35,2261.16,2325.29,2385.17]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",1813.17,1854.82,1906.15,1966.12,2023.91,2084.39,2141.31]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2092.41,2136.65,2186.48,2242.46,2298.52,2356.86,2415.5500000000002]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",1789.63,1830.28,1874.69,1926.77,1980.56,2037.21,2093.33]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",1836.96,1873.55,1915.45,1962.66,2012.44,2064.59,2117.0700000000002]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",1674.25,1707.27,1743.65,1784.38,1828.84,1874.55,1920.81]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.98878037627384363,0.98872728243174723,0.98866584875616692,0.98862258363649325,0.98857605692592077,0.98854009754963457,0.98849825466328445]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.98884276541735106,0.9,0.9,0.9,0.9,0.9,0.9]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor"]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0.99075917286484694,0.99075917286484694,0.99075917286484694,0.99075917286484694,0.99075917286484694,0.99075917286484694,0.99075917286484694]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor"]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.9,0.9,0.9,0.9,0.9,0.9,0.9]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.96726272015158243,0.96726272015158243,0.96726272015158243,0.96726272015158243,0.96726272015158243,0.96726272015158243,0.96726272015158243]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0.99168753718261449,0.99168753718261449,0.99168753718261449,0.99168753718261449,0.99168753718261449,0.99168753718261449,0.99168753718261449]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor"]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor"]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.98878037627384363,0.98872728243174723,0.98866584875616692,0.98862258363649325,0.98857605692592077,0.98854009754963457,0.98849825466328445]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor"]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor"]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor"]

{"sheet":"3.5 Physical assets","index":17,"n_rows":96,"n_cols":10,"rows_kept":96,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",6571.5849320000552,6571.5849320000552,6571.5849320000552,6600.7336820000555,6606.1449320000556,6595.1986820000557,6582.0624320000552]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",48.956077000000086,48.956077000000086,48.956077000000086,48.956077000000086,48.956077000000086,48.956077000000086,48.956077000000086]
["DPA0104","Overhead 11 kV","km",0,0,0,0,0,0,0]
["DPA0105","Overhead SWER","km",0.8006040000000002,93.800604000000007,99.800604000000007,12.800604,0.8006040000000002,0.8006040000000002,0.8006040000000002]
["DPA0106","Overhead 22 kV","km",6416.3880630000704,6416.3880630000704,6416.3880630000704,6427.6380630000704,6478.78806300007,6434.6380630000704,6424.8880630000704]
["DPA0107","Overhead 33 kV","km",22520.538553999566,22520.538553999566,22520.538553999566,22520.538553999566,22520.538553999566,22520.538553999566,22520.538553999566]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",0,0,9.2496999999999989,28.709699999999998,76.809699999999992,172.05969999999999,192.90969999999999]
["DPA0112","Overhead 110kV","km",0,0,0,0,0,0,0]
["DPA0110","Overhead 132 kV","km",2390.4482739999994,2390.4482739999994,2390.4482739999994,2390.4482739999994,2390.4482739999994,2390.4482739999994,2390.4482739999994]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D14:D27)","v":37948.716503999698},38041.716503999698,38056.966203999698,38029.82495399969,38122.486203999688,38162.639953999693,38160.603703999688]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",5745.8172939998794,5745.8172939998794,5745.8172939998794,5748.4047939998791,5746.6797939998796,5746.6797939998796,5745.8172939998794]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",14.757923000000003,14.757923000000003,14.757923000000003,14.757923000000003,14.757923000000003,14.757923000000003,14.757923000000003]
["DPA0204","Underground 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0205","Underground 11 kV","km",0.31809500000000002,0.31809500000000002,0.31809500000000002,0.31809500000000002,0.31809500000000002,0.31809500000000002,0.31809500000000002]
["DPA0206","Underground SWER","km",59.560240000000007,59.560240000000007,59.560240000000007,59.560240000000007,59.560240000000007,59.560240000000007,59.560240000000007]
["DPA0207","Underground 22 kV","km",2706.2090399999856,2706.2090399999856,2715.2390399999858,2717.5390399999856,2709.1890399999857,2722.8390399999857,2706.2390399999858]
["DPA0208","Underground 33 kV","km",0,0,0,0,0,0,0]
["DPA0209","Underground 66 kV","km",13.776541999999997,13.776541999999997,13.776541999999997,14.966541999999997,14.966541999999997,14.966541999999997,14.966541999999997]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",0,0,0,0,0,0,0]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D30:D41)","v":8540.4391339998638},8540.4391339998638,8549.4691339998644,8555.5466339998638,8545.4716339998649,8559.1216339998646,8541.6591339998649]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.11285300205533302,0.11285300205533302,0.11285300205533302,0.11285300205533302,0.11285300205533302,0.11285300205533302,0.11285300205533302]
["DPA0302","Overhead 6.6 kV","MVA",2.8164215945194551,2.8164215945194551,2.8164215945194551,2.8164215945194551,2.8164215945194551,2.8164215945194551,2.8164215945194551]
["DPA0303","Overhead 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0304","Overhead 11 kV","MVA",6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598]
["DPA0305","Overhead SWER","MVA",0.48988953096195981,0.48988953096195981,0.48988953096195981,0.48988953096195981,0.48988953096195981,0.48988953096195981,0.48988953096195981]
["DPA0306","Overhead 22 kV","MVA",4.42905741029921,4.42905741029921,4.42905741029921,37.99966616259919,43.99966616259919,43.99966616259919,37.99966616259919]
["DPA0307","Overhead 33 kV","MVA",0,0,0,0,0,0,0]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",42.001221118621217,42.001221118621217,115.1630472303306,232.33304723033061,293.60607659888723,479.82254999181299,423.92557936036957]
["DPA0310","Overhead 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0311","Overhead 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.22678316798963885,0.22678316798963885,0.22678316798963885,0.22678316798963885,0.22678316798963885,0.22678316798963885,0.22678316798963885]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",3.6646434118328939,3.6646434118328939,3.6646434118328939,3.6646434118328939,3.6646434118328939,3.6646434118328939,3.6646434118328939]
["DPA0404","Underground 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0405","Underground 11 kV","MVA",6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598,6.0015560482261598]
["DPA0406","Underground SWER","MVA",0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859]
["DPA0407","Underground 12.7 kV","MVA",0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859,0.1415302876549859]
["DPA0408","Underground 22 kV","MVA",11.247310716516905,11.247310716516905,11.247310716516905,23.247310716516907,77.247310716516907,32.489357823123022,35.247310716516907]
["DPA0409","Underground 33 kV","MVA",0,0,0,0,0,0,0]
["DPA0410","Underground 66 kV","MVA",43.438905092191099,43.438905092191099,43.438905092191099,160.60890509219109,160.60890509219109,160.60890509219109,160.60890509219109]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",6598.9189999999999,6598.9189999999999,6598.9189999999999,6598.9189999999999,6598.9189999999999,6598.9189999999999,6598.9189999999999]
["DPA0503","Cold spare capacity included in DPA0501","MVA",124.36499999999999,124.36499999999999,124.36499999999999,124.36499999999999,124.36499999999999,124.36499999999999,124.36499999999999]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",0,0,0,0,0,0,0]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",0,0,0,0,0,0,0]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",3345.5,3378.5,3378.5,3411.5,3477.5,3477.5,3543.5]
["DPA0604","Total zone substation transformer  capacity ","MVA",3436,3469,3469,3502,3568,3568,3634]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",90.5,90.5,90.5,90.5,90.5,90.5,90.5]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DPA0701","Public lighting luminaires","0's",{"$f":"SUM('4.1 Public lighting'!D23:D24)","v":164582.70830448897},{"$f":"SUM('4.1 Public lighting'!E23:E24)","v":167487.65367298821},{"$f":"SUM('4.1 Public lighting'!F23:F24)","v":172908.5960805983},{"$f":"SUM('4.1 Public lighting'!G23:G24)","v":177655.58533019404},{"$f":"SUM('4.1 Public lighting'!H23:H24)","v":183448.97089746979},{"$f":"SUM('4.1 Public lighting'!I23:I24)","v":189398.29674839281},{"$f":"SUM('4.1 Public lighting'!J23:J24)","v":198552.17169572573}]
["DPA0702","Public lighting poles","0's",114715.44400000002,{"$f":"D95+'4.1 Public lighting'!E15","v":119583.48043200003},{"$f":"E95+'4.1 Public lighting'!F15","v":124587.82188409603},{"$f":"F95+'4.1 Public lighting'!G15","v":129732.28489685073},{"$f":"G95+'4.1 Public lighting'!H15","v":135020.79287396255},{"$f":"H95+'4.1 Public lighting'!I15","v":140457.37907443353},{"$f":"I95+'4.1 Public lighting'!J15","v":146046.18968851768}]
["DPA0703","Public lighting columns","0's",0,0,0,0,0,0,0]

{"sheet":"3.6 Quality of service","index":18,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DQS0201","Energy Not Supplied (planned)","GWh",2.2879999999999998,2.2879999999999998,2.2879999999999998,2.2879999999999998,2.2879999999999998,2.2879999999999998,2.2879999999999998]
["DQS0202","Energy Not Supplied (unplanned)","GWh",7.165,7.165,7.165,7.165,7.165,7.165,7.165]
["DQS02","Total",null,{"$f":"SUM(D10:D11)","v":9.4529999999999994},9.4529999999999994,9.4529999999999994,9.4529999999999994,9.4529999999999994,9.4529999999999994,9.4529999999999994]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DQS03","System losses","%",{"$f":"(SUM('3.4 Operational data'!D22:D34)-SUM('3.4 Operational data'!D15:D20))/SUM('3.4 Operational data'!D22:D34)","v":3.9610651681444425E-2},{"$f":"(SUM('3.4 Operational data'!E22:E34)-SUM('3.4 Operational data'!E15:E20))/SUM('3.4 Operational data'!E22:E34)","v":3.9610651681444405E-2},{"$f":"(SUM('3.4 Operational data'!F22:F34)-SUM('3.4 Operational data'!F15:F20))/SUM('3.4 Operational data'!F22:F34)","v":3.9610651681444439E-2},{"$f":"(SUM('3.4 Operational data'!G22:G34)-SUM('3.4 Operational data'!G15:G20))/SUM('3.4 Operational data'!G22:G34)","v":3.9610651681444488E-2},{"$f":"(SUM('3.4 Operational data'!H22:H34)-SUM('3.4 Operational data'!H15:H20))/SUM('3.4 Operational data'!H22:H34)","v":3.9610651681444356E-2},{"$f":"(SUM('3.4 Operational data'!I22:I34)-SUM('3.4 Operational data'!I15:I20))/SUM('3.4 Operational data'!I22:I34)","v":3.9610651681444377E-2},{"$f":"(SUM('3.4 Operational data'!J22:J34)-SUM('3.4 Operational data'!J15:J20))/SUM('3.4 Operational data'!J22:J34)","v":3.9610651681444467E-2}]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DQS04","Overall utilisation","%",{"$f":"'3.4 Operational data'!D87/'3.5 Physical assets'!D86","v":0.70375145518044246},{"$f":"'3.4 Operational data'!E87/'3.5 Physical assets'!E86","v":0.71300086480253677},{"$f":"'3.4 Operational data'!F87/'3.5 Physical assets'!F86","v":0.73153070049005475},{"$f":"'3.4 Operational data'!G87/'3.5 Physical assets'!G86","v":0.74547401484865794},{"$f":"'3.4 Operational data'!H87/'3.5 Physical assets'!H86","v":0.75275784753363228},{"$f":"'3.4 Operational data'!I87/'3.5 Physical assets'!I86","v":0.7750784753363229},{"$f":"'3.4 Operational data'!J87/'3.5 Physical assets'!J86","v":0.78230049532195933}]

{"sheet":"3.7 Operating Environment","index":19,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DOEF0101","Customer density","Customer / km",{"$f":"'3.4 Operational data'!D54/'3.5 Physical assets'!D28","v":21.676622446856669}]
["DOEF0102","Energy density","MWh/customer",{"$f":"SUM('3.4 Operational data'!D15:D20)*1000/'3.4 Operational data'!D54","v":9.5820047071256766}]
["DOEF0103","Demand density","kVA / customer",{"$f":"'3.4 Operational data'!D87*1000/'3.4 Operational data'!D54","v":2.9395696571845367}]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DOEF0201","Rural proportion","%",0.92766641878217171]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",11056.47]
["DOEF0203","Rural vegetation maintenance spans","0's",64200.33]
["DOEF0204","Total vegetation maintenance spans","0's",75256.800000000003]
["DOEF0205","Total number of spans","0's",318414]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",1]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",2.5722666666666667]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",6.2523999999999997]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",0.95634194971838815]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",0.73610443202965425]
["DOEF0212","Tropical proportion","Spans",0]
["DOEF0213","Standard vehicle access","km",780.27,780.27,780.27,780.27,780.27,780.27,780.27]
["DOEF0214","Bushfire risk","Spans",56895]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"FORECAST"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
["DOEF0301","Route Line length","km",40316.133365684647,40467.977406274309,40620.393342299816,40773.383327710624,40926.949524568692,41081.09410307902,41235.819241620338]

{"sheet":"4.1 Public lighting","index":20,"n_rows":165,"n_cols":10,"rows_kept":165,"cut":false,"hidden":false,"merged":[[216,1,216,2],[217,1,217,2],[218,1,218,2],[219,1,219,2],[210,1,210,2],[211,1,211,2],[212,1,212,2],[213,1,213,2],[214,1,214,2],[215,1,215,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[155,1,155,2],[156,1,156,2],[157,1,157,2],[158,1,158,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[99,1,99,2],[97,1,97,2],[100,1,100,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[6,1,6,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[58,1,58,2],[59,1,59,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"4.1 PUBLIC LIGHTING"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. There are no further instructions."]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"PUBLIC LIGHT INSTALLATION "]
[null,"Major road light installed","number",1196.2440000000031,1229.7388320000032,1264.171519296003,1299.568321836291,1335.9562348477073,1373.3630094234431,1411.8171736872996]
[null,"Minor road light installed","number",3539.2000000000085,3638.297600000009,3740.1699328000095,3844.8946909184097,3952.5517422641251,4063.2231910475202,4176.9934403968509]
[null,"Number of poles installed ","number",{"$f":"SUM(D13:D14)","v":4735.4440000000113},{"$f":"SUM(E13:E14)","v":4868.0364320000117},{"$f":"SUM(F13:F14)","v":5004.3414520960123},{"$f":"SUM(G13:G14)","v":5144.4630127547007},5288.5079771118326,5436.5862004709634,5588.8106140841501]
[null,"Total expenditure","$",{"$f":"D13*D39+D14*AVERAGE(D41:D43)","v":4358526.5173333436},{"$f":"E13*E39+E14*AVERAGE(E41:E43)","v":4480565.2598186778},4031427.5915476866,4144307.5641110213,4260348.1759061301,4379637.9248315012,4502267.786726784]
[null,"PUBLIC LIGHT REPLACEMENT"]
[null,"Major road light installed","number",1075.5852764026927,1086.4497741441339,1097.424014287004,1107.2596442627976,1117.3706718779135,1127.7648082662527,1138.4499804734655]
[null,"Minor road light installed","number",3412.0587696636444,3446.5240097612568,3481.3373835972293,3516.6921636712855,3553.0368775874135,3590.3992434931952,3628.8077556443386]
[null,"Number of poles replaced","number",817.28493309949044,817.28493309949044,817.28493309949044,817.28493309949044,817.28493309949044,817.28493309949044,817.28493309949044]
[null,"Total expenditure","$",5713038.6011983911,3849674.4411215172,5301185.608077419,5342414.5353952814,5386950.0354379788,5435022.9455696847,5481775.038340888]
[null,"PUBLIC LIGHT MAINTENANCE"]
[null,"Major road light installed","number",44107.686894965125,44529.186140188154,45476.376714022699,46538.242692782893,47709.384660847827,48981.268091782164,48263.520312999375]
[null,"Minor road light installed","number",120475.02140952383,122958.46753280004,127432.21936657559,131117.34263741114,135739.58623662195,140417.02865661064,150288.65138272636]
[null,"Number of poles maintained","number",{"$f":"'3.5 Physical assets'!D95","v":114715.44400000002},{"$f":"'3.5 Physical assets'!E95","v":119583.48043200003},{"$f":"'3.5 Physical assets'!F95","v":124587.82188409603},{"$f":"'3.5 Physical assets'!G95","v":129732.28489685073},{"$f":"'3.5 Physical assets'!H95","v":135020.79287396255},{"$f":"'3.5 Physical assets'!I95","v":140457.37907443353},{"$f":"'3.5 Physical assets'!J95","v":146046.18968851768}]
[null,"Total expenditure","$",0,0,0,0,0,0,0]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","number of days",{"$f":"AVERAGE(20,9,6)","v":11.666666666666666},11.666666666666666,11.666666666666666,11.666666666666666,11.666666666666666,11.666666666666666,11.666666666666666]
[null,"GSO breaches","number",{"$f":"AVERAGE(387,465,540)","v":464},464,464,464,464,464,464]
[null,"GSL payments ","$",12586,12586,12586,12586,12586,12586,12586]
[null,"Customer complaints ","number",{"$f":"AVERAGE(47,54,56)","v":52.333333333333336},52.333333333333336,52.333333333333336,52.333333333333336,52.333333333333336,52.333333333333336,52.333333333333336]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"PUBLIC LIGHT INSTALLATION"]
[null,"LED 18W",null,536,536,{"$f":"AVERAGE(655,443,678)","v":592},{"$f":"AVERAGE(655,443,678)","v":592},592,592,592]
[null,"LED 14W",null,536,536,{"$f":"F39","v":592},{"$f":"G39","v":592},592,592,592]
[null,"LED 70W",null,944,944,{"$f":"F40","v":592},592,592,592,592]
[null,"LED 155W",null,1049,1049,{"$f":"F43","v":1020.6666666666666},{"$f":"G43","v":1020.6666666666666},1020.6666666666666,1020.6666666666666,1020.6666666666666]
[null,"LED 275W",null,1158,1158,{"$f":"AVERAGE(1018,1003,1041)","v":1020.6666666666666},{"$f":"AVERAGE(1018,1003,1041)","v":1020.6666666666666},1020.6666666666666,1020.6666666666666,1020.6666666666666]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"PUBLIC LIGHT REPLACEMENT"]
[null,"LED 18W",null,536,536,671.65440478820256,672.58584195592687,673.73818791582994,675.12771403775434,676.2977800139364]
[null,"LED 14W",null,536,536,659.40871887728997,660.34015604501417,661.49250200491724,662.88202812684187,664.05209410302371]
[null,"LED 70W",null,944,944,1039.5075890068645,1040.4390261745884,1041.5913721344914,1042.9808982564159,1044.150964232598]
[null,"LED 155W",null,1049,1049,1039.507589006864,1040.4390261745884,1041.5913721344916,1042.9808982564161,1044.150964232598]
[null,"LED 275W",null,1158,1158,1881.2040752244391,1882.1355123921633,1883.2878583520665,1884.6773844739917,1885.8474504501733]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"PUBLIC LIGHT MAINTENANCE"]
[null,"LED 18W",null,16,16,13.680386307432116,13.752711132705365,13.80805234351164,13.902779224096449,13.9476345776309]
[null,"LED 14W",null,16,16,15.733222805609813,15.822752279034894,15.895860666678761,16.008840892206038,16.077139111105534]
[null,"LED70W",null,21,21,23.454937896032437,23.588921900673327,23.728025803040978,23.929055281209155,24.069692452042883]
[null,"LED155W",null,22,22,23.075692025080141,23.140990534342606,23.235878696894339,23.407026871523392,23.522215346525059]
[null,"LED275W",null,34,34,24.874950933101559,24.884521526017835,24.968063195119292,25.16165199303007,25.205730718235184]

{"sheet":"5.4 MD & utilisation-Spatial","index":21,"n_rows":11580,"n_cols":12,"rows_kept":11580,"cut":false,"hidden":false,"merged":[[11566,1,11566,2],[11567,1,11567,2],[11568,1,11568,2],[11569,1,11569,2],[11570,1,11570,2],[11571,1,11571,2],[11572,1,11572,2],[11579,1,11579,2],[11573,1,11573,2],[11574,1,11574,2],[11575,1,11575,2],[11576,1,11576,2],[11577,1,11577,2],[11578,1,11578,2],[11531,1,11531,2],[11532,1,11532,2],[11533,1,11533,2],[11534,1,11534,2],[11535,1,11535,2],[11536,1,11536,2],[11537,1,11537,2],[11538,1,11538,2],[11539,1,11539,2],[11540,1,11540,2],[11541,1,11541,2],[11542,1,11542,2],[11543,1,11543,2],[11544,1,11544,2],[11545,1,11545,2],[11546,1,11546,2],[11547,1,11547,2],[11548,1,11548,2],[11549,1,11549,2],[11550,1,11550,2],[11551,1,11551,2],[11552,1,11552,2],[11553,1,11553,2],[11554,1,11554,2],[11555,1,11555,2],[11556,1,11556,2],[11557,1,11557,2],[11558,1,11558,2],[11559,1,11559,2],[11560,1,11560,2],[11561,1,11561,2],[11562,1,11562,2],[11563,1,11563,2],[11500,1,11500,2],[11501,1,11501,2],[11502,1,11502,2],[11503,1,11503,2],[11504,1,11504,2],[11505,1,11505,2],[11506,1,11506,2],[11507,1,11507,2],[11508,1,11508,2],[11509,1,11509,2],[11510,1,11510,2],[11511,1,11511,2],[11512,1,11512,2],[11513,1,11513,2],[11514,1,11514,2],[11515,1,11515,2],[11516,1,11516,2],[11517,1,11517,2],[11518,1,11518,2],[11519,1,11519,2],[11520,1,11520,2],[11521,1,11521,2],[11522,1,11522,2],[11523,1,11523,2],[11524,1,11524,2],[11525,1,11525,2],[11526,1,11526,2],[11527,1,11527,2],[11528,1,11528,2],[11529,1,11529,2],[11530,1,11530,2],[11564,1,11564,2],[11565,1,11565,2],[11467,1,11467,2],[11468,1,11468,2],[11469,1,11469,2],[11470,1,11470,2],[11471,1,11471,2],[11472,1,11472,2],[11473,1,11473,2],[11474,1,11474,2],[11475,1,11475,2],[11476,1,11476,2],[11477,1,11477,2],[11478,1,11478,2],[11479,1,11479,2],[11480,1,11480,2],[11481,1,11481,2],[11482,1,11482,2],[11483,1,11483,2],[11484,1,11484,2],[11485,1,11485,2],[11486,1,11486,2],[11487,1,11487,2],[11488,1,11488,2],[11489,1,11489,2],[11490,1,11490,2],[11491,1,11491,2],[11492,1,11492,2],[11493,1,11493,2],[11494,1,11494,2],[11495,1,11495,2],[11496,1,11496,2],[11497,1,11497,2],[11498,1,11498,2],[11499,1,11499,2],[11434,1,11434,2],[11435,1,11435,2],[11436,1,11436,2],[11437,1,11437,2],[11438,1,11438,2],[11439,1,11439,2],[11440,1,11440,2],[11441,1,11441,2],[11442,1,11442,2],[11443,1,11443,2],[11444,1,11444,2],[11445,1,11445,2],[11446,1,11446,2],[11447,1,11447,2],[11448,1,11448,2],[11449,1,11449,2],[11450,1,11450,2],[11451,1,11451,2],[11452,1,11452,2],[11453,1,11453,2],[11454,1,11454,2],[11455,1,11455,2],[11456,1,11456,2],[11457,1,11457,2],[11458,1,11458,2],[11459,1,11459,2],[11460,1,11460,2],[11461,1,11461,2],[11462,1,11462,2],[11463,1,11463,2],[11464,1,11464,2],[11465,1,11465,2],[11466,1,11466,2],[11401,1,11401,2],[11402,1,11402,2],[11403,1,11403,2],[11404,1,11404,2],[11405,1,11405,2],[11406,1,11406,2],[11407,1,11407,2],[11408,1,11408,2],[11409,1,11409,2],[11410,1,11410,2],[11411,1,11411,2],[11412,1,11412,2],[11413,1,11413,2],[11414,1,11414,2],[11415,1,11415,2],[11416,1,11416,2],[11417,1,11417,2],[11418,1,11418,2],[11419,1,11419,2],[11420,1,11420,2],[11421,1,11421,2],[11422,1,11422,2],[11423,1,11423,2],[11424,1,11424,2],[11425,1,11425,2],[11426,1,11426,2],[11427,1,11427,2],[11428,1,11428,2],[11429,1,11429,2],[11430,1,11430,2],[11431,1,11431,2],[11432,1,11432,2],[11433,1,11433,2],[11368,1,11368,2],[11369,1,11369,2],[11370,1,11370,2],[11371,1,11371,2],[11372,1,11372,2],[11373,1,11373,2],[11374,1,11374,2],[11375,1,11375,2],[11376,1,11376,2],[11377,1,11377,2],[11378,1,11378,2],[11379,1,11379,2],[11380,1,11380,2],[11381,1,11381,2],[11382,1,11382,2],[11383,1,11383,2],[11384,1,11384,2],[11385,1,11385,2],[11386,1,11386,2],[11387,1,11387,2],[11388,1,11388,2],[11389,1,11389,2],[11390,1,11390,2],[11391,1,11391,2],[11392,1,11392,2],[11393,1,11393,2],[11394,1,11394,2],[11395,1,11395,2],[11396,1,11396,2],[11397,1,11397,2],[11398,1,11398,2],[11399,1,11399,2],[11400,1,11400,2],[11335,1,11335,2],[11336,1,11336,2],[11337,1,11337,2],[11338,1,11338,2],[11339,1,11339,2],[11340,1,11340,2],[11341,1,11341,2],[11342,1,11342,2],[11343,1,11343,2],[11344,1,11344,2],[11345,1,11345,2],[11346,1,11346,2],[11347,1,11347,2],[11348,1,11348,2],[11349,1,11349,2],[11350,1,11350,2],[11351,1,11351,2],[11352,1,11352,2],[11353,1,11353,2],[11354,1,11354,2],[11355,1,11355,2],[11356,1,11356,2],[11357,1,11357,2],[11358,1,11358,2],[11359,1,11359,2],[11360,1,11360,2],[11361,1,11361,2],[11362,1,11362,2],[11363,1,11363,2],[11364,1,11364,2],[11365,1,11365,2],[11366,1,11366,2],[11367,1,11367,2],[11302,1,11302,2],[11303,1,11303,2],[11304,1,11304,2],[11305,1,11305,2],[11306,1,11306,2],[11307,1,11307,2],[11308,1,11308,2],[11309,1,11309,2],[11310,1,11310,2],[11311,1,11311,2],[11312,1,11312,2],[11313,1,11313,2],[11314,1,11314,2],[11315,1,11315,2],[11316,1,11316,2],[11317,1,11317,2],[11318,1,11318,2],[11319,1,11319,2],[11320,1,11320,2],[11321,1,11321,2],[11322,1,11322,2],[11323,1,11323,2],[11324,1,11324,2],[11325,1,11325,2],[11326,1,11326,2],[11327,1,11327,2],[11328,1,11328,2],[11329,1,11329,2],[11330,1,11330,2],[11331,1,11331,2],[11332,1,11332,2],[11333,1,11333,2],[11334,1,11334,2],[11269,1,11269,2],[11270,1,11270,2],[11271,1,11271,2],[11272,1,11272,2],[11273,1,11273,2],[11274,1,11274,2],[11275,1,11275,2],[11276,1,11276,2],[11277,1,11277,2],[11278,1,11278,2],[11279,1,11279,2],[11280,1,11280,2],[11281,1,11281,2],[11282,1,11282,2],[11283,1,11283,2],[11284,1,11284,2],[11285,1,11285,2],[11286,1,11286,2],[11287,1,11287,2],[11288,1,11288,2],[11289,1,11289,2],[11290,1,11290,2],[11291,1,11291,2],[11292,1,11292,2],[11293,1,11293,2],[11294,1,11294,2],[11295,1,11295,2],[11296,1,11296,2],[11297,1,11297,2],[11298,1,11298,2],[11299,1,11299,2],[11300,1,11300,2],[11301,1,11301,2],[11236,1,11236,2],[11237,1,11237,2],[11238,1,11238,2],[11239,1,11239,2],[11240,1,11240,2],[11241,1,11241,2],[11242,1,11242,2],[11243,1,11243,2],[11244,1,11244,2],[11245,1,11245,2],[11246,1,11246,2],[11247,1,11247,2],[11248,1,11248,2],[11249,1,11249,2],[11250,1,11250,2],[11251,1,11251,2],[11252,1,11252,2],[11253,1,11253,2],[11254,1,11254,2],[11255,1,11255,2],[11256,1,11256,2],[11257,1,11257,2],[11258,1,11258,2],[11259,1,11259,2],[11260,1,11260,2],[11261,1,11261,2],[11262,1,11262,2],[11263,1,11263,2],[11264,1,11264,2],[11265,1,11265,2],[11266,1,11266,2],[11267,1,11267,2],[11268,1,11268,2],[11203,1,11203,2],[11204,1,11204,2],[11205,1,11205,2],[11206,1,11206,2],[11207,1,11207,2],[11208,1,11208,2],[11209,1,11209,2],[11210,1,11210,2],[11211,1,11211,2],[11212,1,11212,2],[11213,1,11213,2],[11214,1,11214,2],[11215,1,11215,2],[11216,1,11216,2],[11217,1,11217,2],[11218,1,11218,2],[11219,1,11219,2],[11220,1,11220,2],[11221,1,11221,2],[11222,1,11222,2],[11223,1,11223,2],[11224,1,11224,2],[11225,1,11225,2],[11226,1,11226,2],[11227,1,11227,2],[11228,1,11228,2],[11229,1,11229,2],[11230,1,11230,2],[11231,1,11231,2],[11232,1,11232,2],[11233,1,11233,2],[11234,1,11234,2],[11235,1,11235,2],[11170,1,11170,2],[11171,1,11171,2],[11172,1,11172,2],[11173,1,11173,2],[11174,1,11174,2],[11175,1,11175,2],[11176,1,11176,2],[11177,1,11177,2],[11178,1,11178,2],[11179,1,11179,2],[11180,1,11180,2],[11181,1,11181,2],[11182,1,11182,2],[11183,1,11183,2],[11184,1,11184,2],[11185,1,11185,2],[11186,1,11186,2],[11187,1,11187,2],[11188,1,11188,2],[11189,1,11189,2],[11190,1,11190,2],[11191,1,11191,2],[11192,1,11192,2],[11193,1,11193,2],[11194,1,11194,2],[11195,1,11195,2],[11196,1,11196,2],[11197,1,11197,2],[11198,1,11198,2],[11199,1,11199,2],[11200,1,11200,2],[11201,1,11201,2],[11202,1,11202,2],[11137,1,11137,2],[11138,1,11138,2],[11139,1,11139,2],[11140,1,11140,2],[11141,1,11141,2],[11142,1,11142,2],[11143,1,11143,2],[11144,1,11144,2],[11145,1,11145,2],[11146,1,11146,2],[11147,1,11147,2],[11148,1,11148,2],[11149,1,11149,2],[11150,1,11150,2],[11151,1,11151,2],[11152,1,11152,2],[11153,1,11153,2],[11154,1,11154,2],[11155,1,11155,2],[11156,1,11156,2],[11157,1,11157,2],[11158,1,11158,2],[11159,1,11159,2],[11160,1,11160,2],[11161,1,11161,2],[11162,1,11162,2],[11163,1,11163,2],[11164,1,11164,2],[11165,1,11165,2],[11166,1,11166,2],[11167,1,11167,2],[11168,1,11168,2],[11169,1,11169,2],[11104,1,11104,2],[11105,1,11105,2],[11106,1,11106,2],[11107,1,11107,2],[11108,1,11108,2],[11109,1,11109,2],[11110,1,11110,2],[11111,1,11111,2],[11112,1,11112,2],[11113,1,11113,2],[11114,1,11114,2],[11115,1,11115,2],[11116,1,11116,2],[11117,1,11117,2],[11118,1,11118,2],[11119,1,11119,2],[11120,1,11120,2],[11121,1,11121,2],[11122,1,11122,2],[11123,1,11123,2],[11124,1,11124,2],[11125,1,11125,2],[11126,1,11126,2],[11127,1,11127,2],[11128,1,11128,2],[11129,1,11129,2],[11130,1,11130,2],[11131,1,11131,2],[11132,1,11132,2],[11133,1,11133,2],[11134,1,11134,2],[11135,1,11135,2],[11136,1,11136,2],[11067,1,11067,2],[11068,1,11068,2],[11069,1,11069,2],[11070,1,11070,2],[11071,1,11071,2],[11072,1,11072,2],[11073,1,11073,2],[11077,5,11077,11],[11079,1,11079,2],[11080,1,11080,2],[11081,1,11081,2],[11082,1,11082,2],[11083,1,11083,2],[11084,1,11084,2],[11085,1,11085,2],[11086,1,11086,2],[11087,1,11087,2],[11088,1,11088,2],[11089,1,11089,2],[11090,1,11090,2],[11091,1,11091,2],[11092,1,11092,2],[11093,1,11093,2],[11094,1,11094,2],[11095,1,11095,2],[11096,1,11096,2],[11097,1,11097,2],[11098,1,11098,2],[11099,1,11099,2],[11100,1,11100,2],[11101,1,11101,2],[11102,1,11102,2],[11103,1,11103,2],[11034,1,11034,2],[11035,1,11035,2],[11036,1,11036,2],[11037,1,11037,2],[11038,1,11038,2],[11039,1,11039,2],[11040,1,11040,2],[11041,1,11041,2],[11042,1,11042,2],[11043,1,11043,2],[11044,1,11044,2],[11045,1,11045,2],[11046,1,11046,2],[11047,1,11047,2],[11048,1,11048,2],[11049,1,11049,2],[11050,1,11050,2],[11051,1,11051,2],[11052,1,11052,2],[11053,1,11053,2],[11054,1,11054,2],[11055,1,11055,2],[11056,1,11056,2],[11057,1,11057,2],[11058,1,11058,2],[11059,1,11059,2],[11060,1,11060,2],[11061,1,11061,2],[11062,1,11062,2],[11063,1,11063,2],[11064,1,11064,2],[11065,1,11065,2],[11066,1,11066,2],[10995,2,10996,2],[10995,3,10996,3],[10997,2,10998,2],[10997,3,10998,3],[10999,2,11000,2],[10999,3,11000,3],[11001,2,11002,2],[11001,3,11002,3],[11003,2,11004,2],[11003,3,11004,3],[11005,2,11006,2],[11005,3,11006,3],[11007,2,11008,2],[11007,3,11008,3],[11009,2,11010,2],[11009,3,11010,3],[11011,2,11012,2],[11011,3,11012,3],[11013,2,11014,2],[11013,3,11014,3],[11015,2,11016,2],[11015,3,11016,3],[11022,5,11022,11],[11024,1,11024,2],[11025,1,11025,2],[11026,1,11026,2],[11027,1,11027,2],[11028,1,11028,2],[11029,1,11029,2],[11030,1,11030,2],[11031,1,11031,2],[11032,1,11032,2],[11033,1,11033,2],[10961,2,10962,2],[10961,3,10962,3],[10963,2,10964,2],[10963,3,10964,3],[10965,2,10966,2],[10965,3,10966,3],[10967,2,10968,2],[10967,3,10968,3],[10969,2,10970,2],[10969,3,10970,3],[10971,2,10972,2],[10971,3,10972,3],[10973,2,10974,2],[10973,3,10974,3],[10975,2,10976,2],[10975,3,10976,3],[10977,2,10978,2],[10977,3,10978,3],[10979,2,10980,2],[10979,3,10980,3],[10981,2,10982,2],[10981,3,10982,3],[10983,2,10984,2],[10983,3,10984,3],[10985,2,10986,2],[10985,3,10986,3],[10987,2,10988,2],[10987,3,10988,3],[10989,2,10990,2],[10989,3,10990,3],[10991,2,10992,2],[10991,3,10992,3],[10993,2,10994,2],[10993,3,10994,3],[10927,2,10928,2],[10927,3,10928,3],[10929,2,10930,2],[10929,3,10930,3],[10931,2,10932,2],[10931,3,10932,3],[10933,2,10934,2],[10933,3,10934,3],[10935,2,10936,2],[10935,3,10936,3],[10937,2,10938,2],[10937,3,10938,3],[10939,2,10940,2],[10939,3,10940,3],[10941,2,10942,2],[10941,3,10942,3],[10943,2,10944,2],[10943,3,10944,3],[10945,2,10946,2],[10945,3,10946,3],[10947,2,10948,2],[10947,3,10948,3],[10949,2,10950,2],[10949,3,10950,3],[10951,2,10952,2],[10951,3,10952,3],[10953,2,10954,2],[10953,3,10954,3],[10955,2,10956,2],[10955,3,10956,3],[10957,2,10958,2],[10957,3,10958,3],[10959,2,10960,2],[10959,3,10960,3],[10893,2,10894,2],[10893,3,10894,3],[10895,2,10896,2],[10895,3,10896,3],[10897,2,10898,2],[10897,3,10898,3],[10899,2,10900,2],[10899,3,10900,3],[10901,2,10902,2],[10901,3,10902,3],[10903,2,10904,2],[10903,3,10904,3],[10905,2,10906,2],[10905,3,10906,3],[10907,2,10908,2],[10907,3,10908,3],[10909,2,10910,2],[10909,3,10910,3],[10911,2,10912,2],[10911,3,10912,3],[10913,2,10914,2],[10913,3,10914,3],[10915,2,10916,2],[10915,3,10916,3],[10917,2,10918,2],[10917,3,10918,3],[10919,2,10920,2],[10919,3,10920,3],[10921,2,10922,2],[10921,3,10922,3],[10923,2,10924,2],[10923,3,10924,3],[10925,2,10926,2],[10925,3,10926,3],[10859,2,10860,2],[10859,3,10860,3],[10861,2,10862,2],[10861,3,10862,3],[10863,2,10864,2],[10863,3,10864,3],[10865,2,10866,2],[10865,3,10866,3],[10867,2,10868,2],[10867,3,10868,3],[10869,2,10870,2],[10869,3,10870,3],[10871,2,10872,2],[10871,3,10872,3],[10873,2,10874,2],[10873,3,10874,3],[10875,2,10876,2],[10875,3,10876,3],[10877,2,10878,2],[10877,3,10878,3],[10879,2,10880,2],[10879,3,10880,3],[10881,2,10882,2],[10881,3,10882,3],[10883,2,10884,2],[10883,3,10884,3],[10885,2,10886,2],[10885,3,10886,3],[10887,2,10888,2],[10887,3,10888,3],[10889,2,10890,2],[10889,3,10890,3],[10891,2,10892,2],[10891,3,10892,3],[10825,2,10826,2],[10825,3,10826,3],[10827,2,10828,2],[10827,3,10828,3],[10829,2,10830,2],[10829,3,10830,3],[10831,2,10832,2],[10831,3,10832,3],[10833,2,10834,2],[10833,3,10834,3],[10835,2,10836,2],[10835,3,10836,3],[10837,2,10838,2],[10837,3,10838,3],[10839,2,10840,2],[10839,3,10840,3],[10841,2,10842,2],[10841,3,10842,3],[10843,2,10844,2],[10843,3,10844,3],[10845,2,10846,2],[10845,3,10846,3],[10847,2,10848,2],[10847,3,10848,3],[10849,2,10850,2],[10849,3,10850,3],[10851,2,10852,2],[10851,3,10852,3],[10853,2,10854,2],[10853,3,10854,3],[10855,2,10856,2],[10855,3,10856,3],[10857,2,10858,2],[10857,3,10858,3],[10791,2,10792,2],[10791,3,10792,3],[10793,2,10794,2],[10793,3,10794,3],[10795,2,10796,2],[10795,3,10796,3],[10797,2,10798,2],[10797,3,10798,3],[10799,2,10800,2],[10799,3,10800,3],[10801,2,10802,2],[10801,3,10802,3],[10803,2,10804,2],[10803,3,10804,3],[10805,2,10806,2],[10805,3,10806,3],[10807,2,10808,2],[10807,3,10808,3],[10809,2,10810,2],[10809,3,10810,3],[10811,2,10812,2],[10811,3,10812,3],[10813,2,10814,2],[10813,3,10814,3],[10815,2,10816,2],[10815,3,10816,3],[10817,2,10818,2],[10817,3,10818,3],[10819,2,10820,2],[10819,3,10820,3],[10821,2,10822,2],[10821,3,10822,3],[10823,2,10824,2],[10823,3,10824,3],[10757,2,10758,2],[10757,3,10758,3],[10759,2,10760,2],[10759,3,10760,3],[10761,2,10762,2],[10761,3,10762,3],[10763,2,10764,2],[10763,3,10764,3],[10765,2,10766,2],[10765,3,10766,3],[10767,2,10768,2],[10767,3,10768,3],[10769,2,10770,2],[10769,3,10770,3],[10771,2,10772,2],[10771,3,10772,3],[10773,2,10774,2],[10773,3,10774,3],[10775,2,10776,2],[10775,3,10776,3],[10777,2,10778,2],[10777,3,10778,3],[10779,2,10780,2],[10779,3,10780,3],[10781,2,10782,2],[10781,3,10782,3],[10783,2,10784,2],[10783,3,10784,3],[10785,2,10786,2],[10785,3,10786,3],[10787,2,10788,2],[10787,3,10788,3],[10789,2,10790,2],[10789,3,10790,3],[10723,2,10724,2],[10723,3,10724,3],[10725,2,10726,2],[10725,3,10726,3],[10727,2,10728,2],[10727,3,10728,3],[10729,2,10730,2],[10729,3,10730,3],[10731,2,10732,2],[10731,3,10732,3],[10733,2,10734,2],[10733,3,10734,3],[10735,2,10736,2],[10735,3,10736,3],[10737,2,10738,2],[10737,3,10738,3],[10739,2,10740,2],[10739,3,10740,3],[10741,2,10742,2],[10741,3,10742,3],[10743,2,10744,2],[10743,3,10744,3],[10745,2,10746,2],[10745,3,10746,3],[10747,2,10748,2],[10747,3,10748,3],[10749,2,10750,2],[10749,3,10750,3],[10751,2,10752,2],[10751,3,10752,3],[10753,2,10754,2],[10753,3,10754,3],[10755,2,10756,2],[10755,3,10756,3],[10689,2,10690,2],[10689,3,10690,3],[10691,2,10692,2],[10691,3,10692,3],[10693,2,10694,2],[10693,3,10694,3],[10695,2,10696,2],[10695,3,10696,3],[10697,2,10698,2],[10697,3,10698,3],[10699,2,10700,2],[10699,3,10700,3],[10701,2,10702,2],[10701,3,10702,3],[10703,2,10704,2],[10703,3,10704,3],[10705,2,10706,2],[10705,3,10706,3],[10707,2,10708,2],[10707,3,10708,3],[10709,2,10710,2],[10709,3,10710,3],[10711,2,10712,2],[10711,3,10712,3],[10713,2,10714,2],[10713,3,10714,3],[10715,2,10716,2],[10715,3,10716,3],[10717,2,10718,2],[10717,3,10718,3],[10719,2,10720,2],[10719,3,10720,3],[10721,2,10722,2],[10721,3,10722,3],[10655,2,10656,2],[10655,3,10656,3],[10657,2,10658,2],[10657,3,10658,3],[10659,2,10660,2],[10659,3,10660,3],[10661,2,10662,2],[10661,3,10662,3],[10663,2,10664,2],[10663,3,10664,3],[10665,2,10666,2],[10665,3,10666,3],[10667,2,10668,2],[10667,3,10668,3],[10669,2,10670,2],[10669,3,10670,3],[10671,2,10672,2],[10671,3,10672,3],[10673,2,10674,2],[10673,3,10674,3],[10675,2,10676,2],[10675,3,10676,3],[10677,2,10678,2],[10677,3,10678,3],[10679,2,10680,2],[10679,3,10680,3],[10681,2,10682,2],[10681,3,10682,3],[10683,2,10684,2],[10683,3,10684,3],[10685,2,10686,2],[10685,3,10686,3],[10687,2,10688,2],[10687,3,10688,3],[10621,2,10622,2],[10621,3,10622,3],[10623,2,10624,2],[10623,3,10624,3],[10625,2,10626,2],[10625,3,10626,3],[10627,2,10628,2],[10627,3,10628,3],[10629,2,10630,2],[10629,3,10630,3],[10631,2,10632,2],[10631,3,10632,3],[10633,2,10634,2],[10633,3,10634,3],[10635,2,10636,2],[10635,3,10636,3],[10637,2,10638,2],[10637,3,10638,3],[10639,2,10640,2],[10639,3,10640,3],[10641,2,10642,2],[10641,3,10642,3],[10643,2,10644,2],[10643,3,10644,3],[10645,2,10646,2],[10645,3,10646,3],[10647,2,10648,2],[10647,3,10648,3],[10649,2,10650,2],[10649,3,10650,3],[10651,2,10652,2],[10651,3,10652,3],[10653,2,10654,2],[10653,3,10654,3],[10587,2,10588,2],[10587,3,10588,3],[10589,2,10590,2],[10589,3,10590,3],[10591,2,10592,2],[10591,3,10592,3],[10593,2,10594,2],[10593,3,10594,3],[10595,2,10596,2],[10595,3,10596,3],[10597,2,10598,2],[10597,3,10598,3],[10599,2,10600,2],[10599,3,10600,3],[10601,2,10602,2],[10601,3,10602,3],[10603,2,10604,2],[10603,3,10604,3],[10605,2,10606,2],[10605,3,10606,3],[10607,2,10608,2],[10607,3,10608,3],[10609,2,10610,2],[10609,3,10610,3],[10611,2,10612,2],[10611,3,10612,3],[10613,2,10614,2],[10613,3,10614,3],[10615,2,10616,2],[10615,3,10616,3],[10617,2,10618,2],[10617,3,10618,3],[10619,2,10620,2],[10619,3,10620,3],[10553,2,10554,2],[10553,3,10554,3],[10555,2,10556,2],[10555,3,10556,3],[10557,2,10558,2],[10557,3,10558,3],[10559,2,10560,2],[10559,3,10560,3],[10561,2,10562,2],[10561,3,10562,3],[10563,2,10564,2],[10563,3,10564,3],[10565,2,10566,2],[10565,3,10566,3],[10567,2,10568,2],[10567,3,10568,3],[10569,2,10570,2]],"merged_total":11555,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"DEMAND"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"bdl","Substation Rating","MVA","Non-Coincident",81,81,81,81,81,81,81]
[null,null,null,null,"Coincident",81,81,81,81,81,81,81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.3,0.31,0.31,0.32,0.32,0.33,0.33]
[null,null,null,null,"Coincident",0.04,0.04,0.04,0.04,0.05,0.05,0.05]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",59.47,60.33,61.26,62.23,63.25,64.319999999999993,65.39]
[null,null,null,null,"Coincident",49.29,50.01,50.78,51.58,52.43,53.31,54.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",66.900000000000006,68.52,70.400000000000006,72.44,74.28,76.25,78.099999999999994]
[null,null,null,null,"Coincident",49.98,50.71,51.49,52.3,53.16,54.06,54.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",53.95,54.66,55.48,57.08,58.6,60.16,61.63]
[null,null,null,null,"Coincident",44.72,45.31,45.99,47.31,48.57,49.87,51.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.33,57.68,59.22,60.91,62.48,64.12,65.66]
[null,null,null,null,"Coincident",45.34,45.94,46.63,47.97,49.25,50.56,51.8]
[null,"bge","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,0.08,0.08]
[null,null,null,null,"Coincident",3.61,3.67,3.73,3.8,3.87,3.94,4]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.87,31.36,31.9,32.479999999999997,33.049999999999997,33.65,34.200000000000003]
[null,null,null,null,"Coincident",31.32,31.82,32.369999999999997,32.96,33.54,34.14,34.700000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.87,31.36,31.9,32.479999999999997,33.049999999999997,33.65,34.200000000000003]
[null,null,null,null,"Coincident",31.33,31.83,32.369999999999997,32.96,33.54,34.15,34.71]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.11,28.61,29.14,29.7,30.26,30.85,31.4]
[null,null,null,null,"Coincident",26.36,26.83,27.33,27.85,28.38,28.93,29.45]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.11,28.61,29.14,29.7,30.26,30.85,31.4]
[null,null,null,null,"Coincident",26.37,26.84,27.33,27.86,28.38,28.94,29.45]
[null,"bn","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.12,0.12,0.12,0.12,0.13,0.14000000000000001,0.14000000000000001]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.69,35.08,35.46,36.4,37.85,39.49,40.840000000000003]
[null,null,null,null,"Coincident",30.79,31.14,31.47,32.31,33.6,35.049999999999997,36.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.25,34.21,35.270000000000003,36.42,37.86,39.49,40.840000000000003]
[null,null,null,null,"Coincident",30.84,31.18,31.52,32.36,33.65,35.1,36.299999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.090000000000003,32.409999999999997,33.01,34.19,35.42,36.880000000000003,37.9]
[null,null,null,null,"Coincident",28.48,28.77,29.3,30.35,31.44,32.74,33.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.43,30.13,31.01,32.19,33.42,34.880000000000003,35.9]
[null,null,null,null,"Coincident",28.53,28.81,29.34,30.39,31.49,32.78,33.69]
[null,"bra","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.11]
[null,null,null,null,"Coincident",0.02,0.02,0.03,0.03,0.03,0.03,0.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",76.680000000000007,77.66,78.63,79.67,80.930000000000007,82.28,83.48]
[null,null,null,null,"Coincident",63.61,64.42,65.23,66.09,67.14,68.260000000000005,69.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",63.46,64.41,65.37,66.44,67.709999999999994,69.06,70.260000000000005]
[null,null,null,null,"Coincident",63.61,64.42,65.23,66.09,67.14,68.260000000000005,69.25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",68.099999999999994,69.040000000000006,70.03,70.989999999999995,71.930000000000007,73.12,74.290000000000006]
[null,null,null,null,"Coincident",56.49,57.27,58.09,58.89,59.67,60.66,61.63]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.72,55.62,56.58,57.59,58.69,59.83,60.96]
[null,null,null,null,"Coincident",56.49,57.27,58.09,58.89,59.67,60.66,61.63]
[null,"brt","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident",40,40,40,40,40,40,40]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0.03,0.03,0.03,0.03,0.03,0.03,0.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.84,16,16.170000000000002,16.34,16.52,16.72,16.920000000000002]
[null,null,null,null,"Coincident",10.5,10.6,10.72,10.83,10.95,11.08,11.21]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.84,20.03,20.239999999999998,20.45,20.67,20.92,21.16]
[null,null,null,null,"Coincident",10.68,10.79,10.9,11.02,11.14,11.27,11.41]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.67,14.82,14.98,15.14,15.3,15.49,15.67]
[null,null,null,null,"Coincident",8.99,9.08,9.18,9.27,9.3699999999999992,9.49,9.6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.14,17.309999999999999,17.48,17.649999999999999,17.829999999999998,18.04,18.25]
[null,null,null,null,"Coincident",9.14,9.23,9.33,9.43,9.5299999999999994,9.65,9.76]
[null,"bwa","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.26,0.26,0.27,0.27,0.27,0.28000000000000003,0.28000000000000003]
[null,null,null,null,"Coincident",0.36,0.36,0.37,0.37,0.38,0.38,0.39]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.67,11.83,12.03,12.16,12.34,12.51,12.68]
[null,null,null,null,"Coincident",6.88,6.97,7.09,7.17,7.27,7.38,7.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.41,13.6,13.77,13.94,14.11,14.29,14.47]
[null,null,null,null,"Coincident",6.88,6.97,7.09,7.17,7.28,7.38,7.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.78,10.92,11.07,11.22,11.38,11.54,11.71]
[null,null,null,null,"Coincident",6.36,6.44,6.53,6.61,6.71,6.8,6.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.12,11.24,11.39,11.56,11.77,11.96,12.13]
[null,null,null,null,"Coincident",6.36,6.44,6.53,6.61,6.71,6.8,6.9]
[null,"bwn","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.64,36.04,36.43,36.799999999999997,37.200000000000003,37.619999999999997,38.01]
[null,null,null,null,"Coincident",29.74,30.07,30.4,30.7,31.04,31.39,31.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.3,52.82,53.4,53.97,54.61,55.29,55.95]
[null,null,null,null,"Coincident",29.83,30.16,30.49,30.8,31.13,31.48,31.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.409999999999997,32.74,33.1,33.5,33.909999999999997,34.340000000000003,34.76]
[null,null,null,null,"Coincident",27.04,27.32,27.62,27.95,28.29,28.65,29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.95,45.75,46.66,47.6,48.51,49.48,50.39]
[null,null,null,null,"Coincident",27.12,27.4,27.7,28.04,28.38,28.74,29.09]
[null,"bwr","Substation Rating","MVA","Non-Coincident",81,81,81,81,81,81,81]
[null,null,null,null,"Coincident",81,81,81,81,81,81,81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.04,0.04,0.04,0.04,0.04,0.05,0.05]
[null,null,null,null,"Coincident",0.03,0.03,0.03,0.04,0.04,0.04,0.04]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.48,55.13,55.88,56.95,58.6,60.4,61.99]
[null,null,null,null,"Coincident",45.6,46.15,46.78,47.67,49.05,50.56,51.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",74.17,75.930000000000007,78.17,81.31,84.18,87.17,89.22]
[null,null,null,null,"Coincident",45.79,46.34,46.97,47.87,49.25,50.77,52.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.7,50.32,51.69,53.41,54.89,56.6,58.19]
[null,null,null,null,"Coincident",38.450000000000003,38.93,39.99,41.32,42.47,43.79,45.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.78,54.01,55.44,57.37,59.18,61.11,62.84]
[null,null,null,null,"Coincident",38.61,39.090000000000003,40.159999999999997,41.49,42.64,43.97,45.21]
[null,"cf","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.67,7.66,7.66,7.65,7.64,7.64,7.64]
[null,null,null,null,"Coincident",1.52,1.52,1.52,1.52,1.51,1.51,1.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.37,6.36,6.36,6.35,6.34,6.34,6.34]
[null,null,null,null,"Coincident",1.52,1.52,1.52,1.52,1.51,1.51,1.51]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.95,6.94,6.93,6.93,6.92,6.92,6.92]
[null,null,null,null,"Coincident",1.27,1.27,1.27,1.27,1.27,1.27,1.27]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.65,5.64,5.63,5.63,5.63,5.62,5.62]
[null,null,null,null,"Coincident",1.27,1.27,1.27,1.27,1.27,1.27,1.27]
[null,"cln","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.45,0.48,0.51,0.54,0.56999999999999995,0.6,0.64]
[null,null,null,null,"Coincident",7.0000000000000007E-2,0.08,0.08,0.09,0.09,0.1,0.1]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",92.1,97.98,103.89,110.4,116.89,123.79,130.9]
[null,null,null,null,"Coincident",90.46,96.24,102.04,108.44,114.81,121.59,128.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",102.18,107.98,114.2,120.4,126.89,133.79,140.9]
[null,null,null,null,"Coincident",90.57,96.35,102.16,108.56,114.95,121.73,128.72]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",75.239999999999995,80.599999999999994,86.37,92.34,98.54,104.91,111.36]
[null,null,null,null,"Coincident",73.900000000000006,79.17,84.83,90.7,96.79,103.04,109.38]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",90.44,95.98,101.61,107.54,113.7,120.02,126.48]
[null,null,null,null,"Coincident",73.989999999999995,79.260000000000005,84.93,90.81,96.9,103.17,109.51]
[null,"cnr","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.41,2.4500000000000002,2.48,2.4900000000000002,2.5099999999999998,2.5299999999999998,2.5499999999999998]
[null,null,null,null,"Coincident",2.13,2.17,2.19,2.2000000000000002,2.2200000000000002,2.2400000000000002,2.2599999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.69,3.74,3.78,3.79,3.81,3.83,3.85]
[null,null,null,null,"Coincident",2.14,2.1800000000000002,2.2000000000000002,2.21,2.23,2.25,2.2599999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.19,2.23,2.2599999999999998,2.27,2.2799999999999998,2.2999999999999998,2.3199999999999998]
[null,null,null,null,"Coincident",1.94,1.97,2,2.0099999999999998,2.02,2.0299999999999998,2.0499999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.84,2.88,2.9,2.91,2.93,2.94,2.96]
[null,null,null,null,"Coincident",1.94,1.98,2.0099999999999998,2.02,2.02,2.04,2.06]
[null,"cpk","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.3,0.31,0.31,0.31,0.32,0.32,0.33]
[null,null,null,null,"Coincident",0.54,0.54,0.55000000000000004,0.55000000000000004,0.56000000000000005,0.56999999999999995,0.57999999999999996]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.12,49.5,50.02,50.71,51.51,52.35,53.14]
[null,null,null,null,"Coincident",42.65,42.98,43.43,44.03,44.73,45.46,46.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.99,46.38,46.89,47.59,48.38,49.22,50.02]
[null,null,null,null,"Coincident",42.83,43.16,43.62,44.22,44.92,45.65,46.34]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.95,43.39,43.94,44.58,45.25,45.94,46.67]
[null,null,null,null,"Coincident",37.29,37.68,38.15,38.71,39.29,39.89,40.520000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.01,39.44,40,40.64,41.3,41.99,42.72]
[null,null,null,null,"Coincident",37.450000000000003,37.840000000000003,38.31,38.869999999999997,39.46,40.06,40.700000000000003]
[null,"cre","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.36,0.37,0.38,0.39,0.4,0.41,0.42]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.03,0.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.930000000000007,72.040000000000006,73.650000000000006,75.25,77.3,79.5,81.650000000000006]
[null,null,null,null,"Coincident",68.09,70.14,71.709999999999994,73.27,75.260000000000005,77.41,79.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",72.08,74.45,76.55,78.150000000000006,80.2,82.4,84.55]
[null,null,null,null,"Coincident",68.099999999999994,70.16,71.73,73.290000000000006,75.28,77.42,79.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.52,65.53,67.12,69.06,70.89,72.989999999999995,74.959999999999994]
[null,null,null,null,"Coincident",61.85,63.8,65.349999999999994,67.239999999999995,69.02,71.069999999999993,72.989999999999995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",65.67,67.84,70.03,71.959999999999994,73.790000000000006,75.89,77.86]
[null,null,null,null,"Coincident",61.86,63.82,65.37,67.260000000000005,69.040000000000006,71.08,73]
[null,"cyn","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.15,0.15,0.16,0.16,0.16,0.16,0.17]
[null,null,null,null,"Coincident",0.03,0.03,0.03,0.03,0.03,0.04,0.04]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",70.44,71.400000000000006,72.61,74,75.430000000000007,76.92,78.430000000000007]
[null,null,null,null,"Coincident",58.94,59.74,60.75,61.91,63.11,64.36,65.62]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.59,78.12,79.77,81.55,83.79,86.39,88.87]
[null,null,null,null,"Coincident",59.04,59.85,60.86,62.03,63.22,64.47,65.739999999999995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.78,61.88,63.06,64.34,65.63,66.88,68.52]
[null,null,null,null,"Coincident",50.85,51.77,52.76,53.83,54.91,55.96,57.33]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.59,64.42,66.66,69.09,71.41,73.739999999999995,76.150000000000006]
[null,null,null,null,"Coincident",50.95,51.87,52.86,53.93,55.01,56.06,57.43]
[null,"drn","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.05,7.15,7.25,7.36,7.48,7.61,7.74]
[null,null,null,null,"Coincident",7.02,7.12,7.22,7.33,7.44,7.58,7.71]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",68.540000000000006,69.44,70.42,71.48,72.64,73.95,75.25]
[null,null,null,null,"Coincident",60.12,60.91,61.76,62.69,63.71,64.86,66]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.36,58.27,59.27,60.36,61.57,62.84,64.11]
[null,null,null,null,"Coincident",60.26,61.05,61.91,62.84,63.86,65.010000000000005,66.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",61.73,62.53,63.42,64.400000000000006,65.459999999999994,66.599999999999994,67.75]
[null,null,null,null,"Coincident",54.14,54.84,55.63,56.48,57.41,58.41,59.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.26,48.1,49.03,50.01,51.52,53.13,54.64]
[null,null,null,null,"Coincident",54.27,54.97,55.76,56.62,57.55,58.55,59.56]
[null,"elm","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.05,0.05,0.05,0.05,0.05,0.05,0.05]
[null,null,null,null,"Coincident",0.04,0.04,0.04,0.04,0.04,0.04,0.04]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",76.62,77.540000000000006,78.55,79.64,80.77,81.89,83.07]
[null,null,null,null,"Coincident",68.39,69.209999999999994,70.11,71.08,72.09,73.09,74.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.959999999999994,77.69,78.489999999999995,79.42,81.39,83.45,85.37]
[null,null,null,null,"Coincident",69.06,69.89,70.8,71.78,72.8,73.81,74.87]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",70.37,70.989999999999995,71.73,72.61,73.55,74.540000000000006,75.64]
[null,null,null,null,"Coincident",62.81,63.36,64.02,64.81,65.650000000000006,66.53,67.510000000000005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",66.150000000000006,66.91,67.72,68.64,69.739999999999995,70.89,71.959999999999994]
[null,null,null,null,"Coincident",63.43,63.99,64.650000000000006,65.45,66.290000000000006,67.19,68.180000000000007]
[null,"epg","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.38,0.4,0.42,0.44,0.46,0.48,0.5]
[null,null,null,null,"Coincident",0.27,0.28000000000000003,0.3,0.31,0.32,0.34,0.35]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",93.32,97.85,102.68,107.52,112.46,117.5,122.56]
[null,null,null,null,"Coincident",70.44,73.86,77.5,81.150000000000006,84.88,88.69,92.51]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",101.82,106.35,111.18,116.02,120.96,126,131.06]
[null,null,null,null,"Coincident",70.44,73.86,77.510000000000005,81.16,84.89,88.7,92.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",79.680000000000007,83.71,88.01,92.29,96.52,101.03,105.54]
[null,null,null,null,"Coincident",60.14,63.18,66.430000000000007,69.66,72.849999999999994,76.260000000000005,79.66]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",89.18,93.21,97.51,101.79,106.02,110.53,115.04]
[null,null,null,null,"Coincident",60.15,63.19,66.44,69.67,72.86,76.260000000000005,79.67]
[null,"fgy","Substation Rating","MVA","Non-Coincident",93,93,93,93,93,93,93]
[null,null,null,null,"Coincident",93,93,93,93,93,93,93]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.08,0.08,0.08,0.09,0.09,0.09,0.09]
[null,null,null,null,"Coincident",0.1,0.1,0.1,0.1,0.1,0.11,0.11]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.41,46.1,46.69,47.61,48.69,49.88,50.95]
[null,null,null,null,"Coincident",44.83,45.51,46.1,47.01,48.07,49.25,50.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.17,47.71,48.09,48.55,49.09,49.88,50.95]
[null,null,null,null,"Coincident",44.99,45.67,46.26,47.17,48.24,49.42,50.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.07,42.97,43.97,45.13,46.22,47.37,48.38]
[null,null,null,null,"Coincident",38.39,39.21,40.119999999999997,41.18,42.18,43.23,44.15]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.07,42.96,43.97,45.13,46.22,47.37,48.38]
[null,null,null,null,"Coincident",38.520000000000003,39.35,40.26,41.33,42.32,43.38,44.3]
[null,"ftr","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.22,0.22,0.23,0.23,0.23,0.24,0.24]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.260000000000002,19.48,19.7,19.93,20.18,20.440000000000001,20.7]
[null,null,null,null,"Coincident",18.13,18.34,18.55,18.77,19,19.25,19.489999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.23,19.46,19.68,19.91,20.149999999999999,20.420000000000002,20.68]
[null,null,null,null,"Coincident",18.18,18.38,18.59,18.809999999999999,19.04,19.29,19.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.29,17.5,17.71,17.93,18.16,18.420000000000002,18.670000000000002]
[null,null,null,null,"Coincident",16.28,16.48,16.68,16.88,17.100000000000001,17.34,17.579999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.32,18.53,18.739999999999998,18.96,19.190000000000001,19.440000000000001,19.690000000000001]
[null,null,null,null,"Coincident",16.32,16.52,16.71,16.920000000000002,17.14,17.38,17.62]
[null,"hpk","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.39,0.4,0.4,0.41,0.42,0.44,0.44]
[null,null,null,null,"Coincident",7.66,7.76,7.85,8.0299999999999994,8.2899999999999991,8.5399999999999991,8.6]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63.57,64.36,65.09,66.66,68.75,70.84,71.34]
[null,null,null,null,"Coincident",59.25,59.99,60.67,62.13,64.08,66.03,66.489999999999995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.16,54.94,55.67,56.48,57.31,58.13,58.98]
[null,null,null,null,"Coincident",59.39,60.13,60.81,62.28,64.23,66.19,66.650000000000006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",55.69,56.39,56.86,58.5,60.59,62.69,63.18]
[null,null,null,null,"Coincident",51.91,52.56,53,54.53,56.47,58.43,58.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.15,46.86,47.33,48.02,48.84,49.7,50.52]
[null,null,null,null,"Coincident",52.03,52.68,53.12,54.66,56.61,58.57,59.03]
[null,"klk","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.7,6.87,7.08,7.32,7.56,7.79,8.02]
[null,null,null,null,"Coincident",6.28,6.44,6.64,6.86,7.09,7.3,7.52]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.2,11.37,11.58,11.82,12.06,12.31,12.63]
[null,null,null,null,"Coincident",6.44,6.61,6.81,7.04,7.27,7.49,7.71]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.02,6.18,6.36,6.59,6.81,7.01,7.2]
[null,null,null,null,"Coincident",5.22,5.36,5.51,5.71,5.9,6.07,6.24]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.32,8.5299999999999994,8.7799999999999994,9.07,9.35,9.66,9.9700000000000006]
[null,null,null,null,"Coincident",5.35,5.49,5.65,5.86,6.05,6.23,6.4]
[null,"klo","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.33,0.36,0.41,0.48,0.55000000000000004,0.61,0.68]
[null,null,null,null,"Coincident",0.14000000000000001,0.16,0.18,0.21,0.24,0.26,0.28999999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",68.209999999999994,76.33,86.83,100.16,114.42,128.88999999999999,143.5]
[null,null,null,null,"Coincident",60.63,67.849999999999994,77.180000000000007,89.03,101.71,114.57,127.56]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",69.209999999999994,77.33,88.02,103.16,117.42,131.88999999999999,146.5]
[null,null,null,null,"Coincident",60.84,68.08,77.45,89.34,102.06,114.97,128]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",57.76,65.52,76.84,91.07,104.48,118.23,132.1]
[null,null,null,null,"Coincident",51.34,58.24,68.3,80.95,92.87,105.09,117.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.17,70.52,81.84,96.07,109.48,123.23,137.1]
[null,null,null,null,"Coincident",51.52,58.44,68.540000000000006,81.23,93.19,105.46,117.83]
[null,"kms","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.09,0.09,0.1,0.1,0.1,0.11,0.11]
[null,null,null,null,"Coincident",0.03,0.03,0.03,0.03,0.04,0.04,0.04]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.69,16.04,16.53,17.09,17.73,18.5,19.25]
[null,null,null,null,"Coincident",13.69,13.99,14.42,14.91,15.47,16.14,16.8]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.190000000000001,17.61,18.25,19,19.73,20.5,21.25]
[null,null,null,null,"Coincident",13.69,14,14.43,14.91,15.47,16.14,16.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.43,14.68,15.13,15.81,16.489999999999998,17.18,17.87]
[null,null,null,null,"Coincident",12.59,12.81,13.2,13.79,14.39,14.99,15.59]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.09,16.54,17.13,17.809999999999999,18.489999999999998,19.18,19.87]
[null,null,null,null,"Coincident",12.59,12.81,13.2,13.8,14.39,14.99,15.59]
[null,"ldl","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.06,0.06,0.06,0.06,0.06,0.06,7.0000000000000007E-2]
[null,null,null,null,"Coincident",1.43,1.44,1.46,1.49,1.52,1.54,1.57]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63.77,64.510000000000005,65.37,66.48,67.67,68.930000000000007,70.19]
[null,null,null,null,"Coincident",53.73,54.35,55.08,56.01,57.02,58.08,59.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",69.52,70.84,73.11,75.91,78.58,81.39,84.01]
[null,null,null,null,"Coincident",54.02,54.64,55.37,56.31,57.32,58.39,59.46]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.35,58.92,59.76,60.9,62.01,63.22,64.400000000000006]
[null,null,null,null,"Coincident",49.16,49.64,50.35,51.31,52.25,53.27,54.26]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",63.28,64.87,67.08,69.680000000000007,72.099999999999994,74.62,77.05]
[null,null,null,null,"Coincident",49.43,49.91,50.62,51.59,52.53,53.55,54.55]
[null,"lga","Substation Rating","MVA","Non-Coincident",73,73,73,73,73,73,73]
[null,null,null,null,"Coincident",73,73,73,73,73,73,73]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.19,36.61,37.049999999999997,37.54,38.03,38.549999999999997,39.06]
[null,null,null,null,"Coincident",33.159999999999997,33.54,33.94,34.39,34.840000000000003,35.32,35.79]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.03,40.46,40.93,41.44,41.95,42.5,43.04]
[null,null,null,null,"Coincident",33.270000000000003,33.659999999999997,34.07,34.520000000000003,34.97,35.44,35.909999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.869999999999997,34.24,34.65,35.090000000000003,35.549999999999997,36.020000000000003,36.5]
[null,null,null,null,"Coincident",28.68,28.99,29.34,29.71,30.1,30.5,30.91]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.89,37.299999999999997,37.74,38.22,38.71,39.21,39.729999999999997]
[null,null,null,null,"Coincident",28.78,29.1,29.45,29.82,30.21,30.61,31.02]
[null,"llg","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.53,24.32,25.38,26.45,27.51,28.14,28.75]
[null,null,null,null,"Coincident",22.45,23.2,24.21,25.23,26.25,26.85,27.43]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.53,24.23,24.95,25.69,26.4,27.11,27.8]
[null,null,null,null,"Coincident",22.49,23.25,24.26,25.28,26.3,26.9,27.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.84,21.57,22.59,23.63,24.66,25.26,25.83]
[null,null,null,null,"Coincident",18.38,19.02,19.920000000000002,20.84,21.75,22.27,22.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.84,20.43,21.06,21.74,22.38,23.04,23.66]
[null,null,null,null,"Coincident",18.41,19.059999999999999,19.96,20.88,21.79,22.32,22.82]
[null,"lyd","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.39,0.4,0.41,0.41,0.42,0.42,0.43]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.93,21.23,21.54,21.83,22.16,22.5,22.82]
[null,null,null,null,"Coincident",20.48,20.77,21.08,21.36,21.68,22.02,22.33]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.55,20.85,21.16,21.46,21.79,22.13,22.44]
[null,null,null,null,"Coincident",20.51,20.8,21.11,21.39,21.71,22.05,22.36]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.64,18.87,19.04,19.260000000000002,19.55,19.84,20.12]
[null,null,null,null,"Coincident",18.239999999999998,18.46,18.63,18.850000000000001,19.13,19.41,19.690000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.07,17.3,17.47,17.690000000000001,17.97,18.27,18.55]
[null,null,null,null,"Coincident",18.27,18.489999999999998,18.66,18.87,19.16,19.440000000000001,19.72]
[null,"mby","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.4600000000000009,9.5399999999999991,9.6199999999999992,9.6999999999999993,9.8000000000000007,9.8800000000000008,9.98]
[null,null,null,null,"Coincident",4,4.04,4.07,4.1100000000000003,4.1500000000000004,4.18,4.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.34,10.37,10.47,10.56,10.66,10.76,10.87]
[null,null,null,null,"Coincident",5.18,5.22,5.27,5.31,5.36,5.41,5.46]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.7899999999999991,8.8699999999999992,8.94,9.02,9.1,9.18,9.27]
[null,null,null,null,"Coincident",3.44,3.47,3.5,3.53,3.56,3.59,3.63]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.3699999999999992,9.4499999999999993,9.5399999999999991,9.6199999999999992,9.7100000000000009,9.7899999999999991,9.8800000000000008]
[null,null,null,null,"Coincident",4.45,4.49,4.5199999999999996,4.5599999999999996,4.5999999999999996,4.6399999999999997,4.6900000000000004]
[null,"mdi","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.17,0.17,0.17,0.17,0.18,0.18,0.18]
[null,null,null,null,"Coincident",0.16,0.16,0.16,0.16,0.17,0.17,0.17]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.16,0.17,0.17,0.17,0.17,0.17,0.17]
[null,null,null,null,"Coincident",0.18,0.18,0.18,0.18,0.19,0.19,0.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.15]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.14000000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.13,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,null,null,null,"Coincident",0.15,0.15,0.15,0.15,0.15,0.15,0.16]
[null,"mfa","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.04,0.04,0.04,0.04,0.04,0.05,0.05]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.4,31.74,32.119999999999997,32.58,33.1,33.700000000000003,34.229999999999997]
[null,null,null,null,"Coincident",28.61,28.92,29.26,29.68,30.16,30.7,31.19]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.61,30.2,30.87,31.64,32.33,33.049999999999997,33.72]
[null,null,null,null,"Coincident",28.62,28.93,29.27,29.69,30.16,30.71,31.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.09,29.48,29.92,30.36,30.79,31.27,31.75]
[null,null,null,null,"Coincident",26.5,26.86,27.26,27.66,28.05,28.49,28.93]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.72,26.1,26.74,27.47,28.08,28.72,29.31]
[null,null,null,null,"Coincident",26.51,26.87,27.27,27.67,28.06,28.5,28.93]
[null,"mjg","Substation Rating","MVA","Non-Coincident",20,20,20,20,20,20,20]
[null,null,null,null,"Coincident",20,20,20,20,20,20,20]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.69,15.02,15.33,15.63,15.96,16.28,16.61]
[null,null,null,null,"Coincident",2.0699999999999998,2.11,2.16,2.2000000000000002,2.25,2.29,2.34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.190000000000001,16.510000000000002,16.829999999999998,17.14,17.46,17.78,18.11]
[null,null,null,null,"Coincident",2.34,2.4,2.4500000000000002,2.4900000000000002,2.5499999999999998,2.6,2.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.53,13.82,14.1,14.38,14.66,14.96,15.25]
[null,null,null,null,"Coincident",1.76,1.8,1.83,1.87,1.91,1.95,1.98]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.53,14.82,15.1,15.38,15.67,15.96,16.25]
[null,null,null,null,"Coincident",1.99,2.04,2.08,2.12,2.16,2.21,2.25]
[null,"moe","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.98,1.99,2.0099999999999998,2.02,2.06,2.1,2.11]
[null,null,null,null,"Coincident",1.79,1.81,1.82,1.83,1.87,1.91,1.92]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.130000000000003,33.409999999999997,33.590000000000003,33.83,34.479999999999997,35.19,35.42]
[null,null,null,null,"Coincident",33.130000000000003,33.409999999999997,33.590000000000003,33.83,34.479999999999997,35.19,35.42]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.65,42.27,43.18,44.14,45.21,46.36,47.38]
[null,null,null,null,"Coincident",33.130000000000003,33.409999999999997,33.590000000000003,33.83,34.479999999999997,35.19,35.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.01,31.27,31.61,31.98,32.619999999999997,33.28,33.49]
[null,null,null,null,"Coincident",31.01,31.27,31.61,31.98,32.619999999999997,33.28,33.49]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36,36.69,37.700000000000003,38.74,39.67,40.61,41.56]
[null,null,null,null,"Coincident",31.01,31.27,31.61,31.98,32.619999999999997,33.28,33.49]
[null,"msd","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident",26,26,26,26,26,26,26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.1,0.11,0.11,0.11,0.11,0.11,0.11]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.55,17.73,17.96,18.2,18.489999999999998,18.79,19.11]
[null,null,null,null,"Coincident",17.43,17.600000000000001,17.829999999999998,18.07,18.36,18.66,18.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.45,18.64,18.87,19.12,19.420000000000002,19.73,20.03]
[null,null,null,null,"Coincident",17.47,17.649999999999999,17.88,18.12,18.41,18.71,19.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.53,15.68,15.87,16.079999999999998,16.329999999999998,16.600000000000001,16.89]
[null,null,null,null,"Coincident",15.42,15.57,15.76,15.97,16.21,16.48,16.77]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.99,15.24,15.51,15.77,16.05,16.34,16.63]
[null,null,null,null,"Coincident",15.46,15.61,15.8,16.010000000000002,16.260000000000002,16.53,16.809999999999999]
[null,"mwl","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.2,0.2,0.2,0.21,0.21,0.21,0.21]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.33,36.65,36.96,37.409999999999997,37.85,38.340000000000003,38.83]
[null,null,null,null,"Coincident",34.51,34.82,35.11,35.54,35.96,36.42,36.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.950000000000003,34.26,34.58,35.119999999999997,35.86,36.56,37.22]
[null,null,null,null,"Coincident",34.630000000000003,34.93,35.229999999999997,35.659999999999997,36.08,36.54,37.01]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.979999999999997,33.21,33.479999999999997,33.86,34.26,34.93,35.590000000000003]
[null,null,null,null,"Coincident",31.33,31.55,31.81,32.17,32.549999999999997,33.18,33.81]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.55,31.05,31.76,32.51,33.15,33.93,34.590000000000003]
[null,null,null,null,"Coincident",31.43,31.65,31.91,32.270000000000003,32.65,33.29,33.92]
[null,"myt","Substation Rating","MVA","Non-Coincident",20,20,20,20,20,20,20]
[null,null,null,null,"Coincident",20,20,20,20,20,20,20]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.03,0.03,0.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.28,17.45,17.61,17.79,17.98,18.170000000000002,18.36]
[null,null,null,null,"Coincident",17.84,18.010000000000002,18.18,18.36,18.559999999999999,18.75,18.95]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.46,18.64,18.8,18.98,19.16,19.37,19.559999999999999]
[null,null,null,null,"Coincident",17.93,18.11,18.27,18.46,18.66,18.850000000000001,19.05]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.04,16.21,16.37,16.54,16.71,16.899999999999999,17.079999999999998]
[null,null,null,null,"Coincident",15.3,15.46,15.62,15.78,15.94,16.12,16.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.36,17.53,17.690000000000001,17.86,18.03,18.23,18.41]
[null,null,null,null,"Coincident",15.38,15.55,15.7,15.86,16.02,16.21,16.38]
[null,"nla","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.61,8.7100000000000009,8.7899999999999991,8.8699999999999992,8.9499999999999993,9.0299999999999994,9.11]
[null,null,null,null,"Coincident",7.46,7.54,7.61,7.68,7.75,7.82,7.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.75,10.86,10.95,11.04,11.13,11.23,11.33]
[null,null,null,null,"Coincident",7.47,7.55,7.62,7.69,7.76,7.83,7.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.18,8.27,8.34,8.4,8.4700000000000006,8.5500000000000007,8.6199999999999992]
[null,null,null,null,"Coincident",6.55,6.62,6.68,6.72,6.78,6.84,6.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.0399999999999991,9.1300000000000008,9.19,9.26,9.34,9.43,9.51]
[null,null,null,null,"Coincident",6.56,6.63,6.68,6.73,6.79,6.85,6.91]
[null,"nrn","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.3,0.3,0.3,0.3,0.31,0.31,0.31]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.59,22.72,22.88,23.1,23.35,23.61,23.85]
[null,null,null,null,"Coincident",18.37,18.48,18.61,18.79,18.989999999999998,19.2,19.399999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.69,21.82,21.97,22.34,22.8,23.31,23.75]
[null,null,null,null,"Coincident",18.46,18.57,18.7,18.88,19.09,19.3,19.489999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.56,20.68,20.84,21.03,21.24,21.47,21.69]
[null,null,null,null,"Coincident",16.72,16.82,16.95,17.100000000000001,17.27,17.46,17.64]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.350000000000001,18.45,18.739999999999998,19.190000000000001,19.670000000000002,20.14,20.62]
[null,null,null,null,"Coincident",16.809999999999999,16.899999999999999,17.03,17.190000000000001,17.36,17.55,17.73]
[null,"ofr","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.97,1.02,1.07,1.1299999999999999,1.18,1.24,1.28]
[null,null,null,null,"Coincident",0.05,0.05,0.05,0.05,0.06,0.06,0.06]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",64.03,66.760000000000005,70.349999999999994,74.05,77.680000000000007,81.349999999999994,84.06]
[null,null,null,null,"Coincident",62.88,65.56,69.09,72.72,76.290000000000006,79.89,82.55]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",64.03,66.430000000000007,69.05,71.83,74.5,77.239999999999995,80.099999999999994]
[null,null,null,null,"Coincident",62.89,65.569999999999993,69.099999999999994,72.73,76.3,79.900000000000006,82.57]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",55.7,57.95,61.26,64.63,68.08,71.63,74.08]
[null,null,null,null,"Coincident",54.7,56.91,60.16,63.47,66.86,70.349999999999994,72.75]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",55.7,57.41,59.64,61.94,64.349999999999994,66.92,69.41]
[null,null,null,null,"Coincident",54.71,56.92,60.17,63.48,66.87,70.36,72.760000000000005]
[null,"phi","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident",26,26,26,26,26,26,26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.99,0.99,1,1.01,1.03,1.05,1.07]
[null,null,null,null,"Coincident",2.96,2.98,3,3.05,3.1,3.15,3.2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.11,24.24,24.46,24.8,25.22,25.64,26.06]
[null,null,null,null,"Coincident",19.36,19.46,19.64,19.91,20.25,20.59,20.93]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.89,24,24.19,24.41,24.77,25.19,25.6]
[null,null,null,null,"Coincident",20.18,20.28,20.47,20.75,21.1,21.46,21.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.17,22.45,22.8,23.15,23.51,23.89,24.27]
[null,null,null,null,"Coincident",17.8,18.03,18.309999999999999,18.59,18.88,19.18,19.489999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.12,20.48,20.87,21.26,21.7,22.15,22.62]
[null,null,null,null,"Coincident",18.55,18.79,19.079999999999998,19.37,19.670000000000002,19.989999999999998,20.309999999999999]
[null,"phm","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.36,3.48,3.67,3.87,4.0599999999999996,4.25,4.3899999999999997]
[null,null,null,null,"Coincident",0.03,0.03,0.03,0.04,0.04,0.04,0.04]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.15,55.09,58.09,61.14,64.23,67.25,69.44]
[null,null,null,null,"Coincident",44.67,46.3,48.82,51.38,53.98,56.52,58.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.93,53.82,54.81,55.9,57.06,58.33,59.99]
[null,null,null,null,"Coincident",44.7,46.33,48.85,51.42,54.01,56.55,58.4]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.03,50.96,53.97,56.99,60.02,63,65.16]
[null,null,null,null,"Coincident",41.2,42.83,45.36,47.89,50.44,52.94,54.76]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.49,48.33,49.27,50.32,51.74,53.33,54.82]
[null,null,null,null,"Coincident",41.23,42.86,45.39,47.93,50.47,52.98,54.8]
[null,"ruba","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident",40,40,40,40,40,40,40]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",2.5499999999999998,2.58,2.61,2.63,2.66,2.69,2.72]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.86,13.01,13.14,13.27,13.41,13.55,13.7]
[null,null,null,null,"Coincident",13.49,13.65,13.78,13.92,14.07,14.21,14.37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.86,15.01,15.14,15.27,15.41,15.55,15.7]
[null,null,null,null,"Coincident",13.72,13.88,14.02,14.16,14.31,14.46,14.62]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.79,10.91,11.04,11.15,11.27,11.39,11.54]
[null,null,null,null,"Coincident",10.46,10.58,10.7,10.81,10.93,11.04,11.19]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.79,12.91,13.04,13.15,13.27,13.4,13.54]
[null,null,null,null,"Coincident",10.64,10.76,10.89,11,11.11,11.23,11.38]
[null,"rve","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.24,0.24,0.24,0.24,0.24,0.24,0.24]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.71,23.65,23.63,23.63,23.7,23.76,23.83]
[null,null,null,null,"Coincident",19.37,19.32,19.3,19.3,19.36,19.41,19.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.13,27.07,27.05,27.06,27.12,27.19,27.25]
[null,null,null,null,"Coincident",19.39,19.34,19.329999999999998,19.329999999999998,19.38,19.43,19.489999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.05,22.07,22.12,22.17,22.28,22.38,22.49]
[null,null,null,null,"Coincident",18.010000000000002,18.03,18.07,18.11,18.2,18.28,18.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.48,24.6,24.78,24.99,25.21,25.45,25.63]
[null,null,null,null,"Coincident",18.03,18.05,18.09,18.13,18.22,18.3,18.39]
[null,"rwn","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.25,0.27,0.28000000000000003,0.28999999999999998,0.3,0.3,0.3]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.03,0.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.19,44.32,46.52,48.76,49.2,49.65,50.08]
[null,null,null,null,"Coincident",38.72,40.67,42.69,44.75,45.15,45.57,45.96]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.94,42.28,42.7,43.18,43.73,44.3,44.85]
[null,null,null,null,"Coincident",38.92,40.89,42.92,44.98,45.39,45.81,46.2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.880000000000003,39.11,41.35,43.56,43.95,44.37,44.78]
[null,null,null,null,"Coincident",33.85,35.89,37.950000000000003,39.979999999999997,40.33,40.72,41.1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.93,34.39,34.880000000000003,35.32,35.799999999999997,36.340000000000003,36.86]
[null,null,null,null,"Coincident",34.020000000000003,36.08,38.15,40.19,40.549999999999997,40.93,41.31]
[null,"rwt","Substation Rating","MVA","Non-Coincident",150,150,150,150,150,150,150]
[null,null,null,null,"Coincident",150,150,150,150,150,150,150]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.5,0.5,0.51,0.51,0.52,0.53,0.54]
[null,null,null,null,"Coincident",0.14000000000000001,0.14000000000000001,0.14000000000000001,0.15,0.15,0.15,0.15]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",105.82,106.88,108.21,109.63,111.14,112.79,114.39]
[null,null,null,null,"Coincident",85.38,86.24,87.31,88.46,89.68,91.01,92.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",93,94.25,95.57,96.99,98.51,100.16,101.76]
[null,null,null,null,"Coincident",85.42,86.28,87.35,88.5,89.72,91.05,92.34]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",92.76,93.51,94.58,95.75,97,98.35,99.73]
[null,null,null,null,"Coincident",74.849999999999994,75.45,76.31,77.260000000000005,78.27,79.36,80.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",83.88,84.8,85.87,87.04,88.29,89.64,91.03]
[null,null,null,null,"Coincident",74.88,75.489999999999995,76.349999999999994,77.290000000000006,78.3,79.39,80.510000000000005]
[null,"sle","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.25,0.26,0.27,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28999999999999998]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.03,0.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.81,31.8,32.86,33.97,34.24,34.53,34.82]
[null,null,null,null,"Coincident",27.28,28.15,29.09,30.07,30.31,30.57,30.83]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.06,30.33,30.76,31.29,31.86,32.46,33.08]
[null,null,null,null,"Coincident",27.43,28.32,29.26,30.25,30.49,30.75,31.01]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.23,29.23,30.28,31.36,31.59,31.83,32.08]
[null,null,null,null,"Coincident",24.99,25.88,26.81,27.76,27.97,28.18,28.4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.83,24.39,25.04,25.74,26.46,27.2,27.9]
[null,null,null,null,"Coincident",25.14,26.03,26.96,27.92,28.13,28.34,28.57]
[null,"smg","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.05,0.05,0.05,0.05,0.05,0.05,0.05]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.27,46.55,46.99,47.44,47.92,48.37,48.82]
[null,null,null,null,"Coincident",38.82,39.06,39.43,39.799999999999997,40.21,40.58,40.96]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.74,45.02,45.46,45.91,46.39,46.84,47.29]
[null,null,null,null,"Coincident",38.82,39.06,39.43,39.799999999999997,40.21,40.590000000000003,40.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.75,41.94,42.23,42.57,42.96,43.41,43.86]
[null,null,null,null,"Coincident",35.03,35.19,35.43,35.72,36.049999999999997,36.42,36.799999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38.909999999999997,39.1,39.4,39.74,40.119999999999997,40.57,41.02]
[null,null,null,null,"Coincident",35.03,35.19,35.43,35.72,36.049999999999997,36.42,36.799999999999997]
[null,"smr","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.11,0.11,0.11,0.11,0.11,0.12,0.12]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.21,36.78,37.43,38.17,38.94,39.729999999999997,40.54]
[null,null,null,null,"Coincident",34.35,34.89,35.51,36.21,36.94,37.69,38.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.659999999999997,38.47,39.39,40.46,41.56,42.92,44.21]
[null,null,null,null,"Coincident",34.35,34.89,35.51,36.21,36.94,37.69,38.46]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.51,32.89,33.44,34.06,34.69,35.340000000000003,36.01]
[null,null,null,null,"Coincident",30.84,31.2,31.72,32.31,32.909999999999997,33.520000000000003,34.159999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.630000000000003,33.43,34.369999999999997,35.6,36.67,37.85,38.85]
[null,null,null,null,"Coincident",30.84,31.2,31.72,32.31,32.909999999999997,33.53,34.159999999999997]
[null,"tgn","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.15,0.16,0.16,0.16,0.16,0.17,0.17]
[null,null,null,null,"Coincident",3.99,4.04,4.08,4.16,4.26,4.37,4.46]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.88,47.41,47.96,48.88,50.07,51.28,52.37]
[null,null,null,null,"Coincident",40.18,40.64,41.11,41.9,42.92,43.95,44.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.33,41.16,42.18,43.31,44.4,45.54,46.59]
[null,null,null,null,"Coincident",40.58,41.04,41.51,42.31,43.34,44.39,45.33]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.42,42.92,43.3,44.25,45.42,46.62,47.72]
[null,null,null,null,"Coincident",36.36,36.79,37.11,37.93,38.93,39.96,40.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38.14,38.99,39.909999999999997,40.99,42,43.07,44.08]
[null,null,null,null,"Coincident",36.72,37.15,37.479999999999997,38.299999999999997,39.31,40.35,41.3]
[null,"tt","Substation Rating","MVA","Non-Coincident",84,84,84,84,84,84,84]
[null,null,null,null,"Coincident",84,84,84,84,84,84,84]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.85,0.86,0.87,0.88,0.9,0.91,0.92]
[null,null,null,null,"Coincident",0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",81.5,82.65,83.8,84.95,86.04,87.38,88.5]
[null,null,null,null,"Coincident",61.95,62.83,63.7,64.58,65.41,66.42,67.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",140.47,144.30000000000001,149.03,153.61000000000001,157.75,162.34,166.33]
[null,null,null,null,"Coincident",62.01,62.89,63.76,64.64,65.459999999999994,66.48,67.34]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",73.36,74.290000000000006,75.209999999999994,76.17,77.19,78.349999999999994,80.11]
[null,null,null,null,"Coincident",55.77,56.47,57.17,57.9,58.68,59.56,60.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",128.08000000000001,131.80000000000001,135.83000000000001,140.32,144.58000000000001,148.97999999999999,152.78]
[null,null,null,null,"Coincident",55.82,56.52,57.22,57.95,58.73,59.61,60.95]
[null,"wgi","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.14000000000000001,0.15,0.15,0.15,0.15,0.16,0.16]
[null,null,null,null,"Coincident",0.06,0.06,0.06,0.06,0.06,7.0000000000000007E-2,7.0000000000000007E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.65,46.42,47.29,48.19,49.02,49.87,50.91]
[null,null,null,null,"Coincident",44.39,45.14,45.98,46.86,47.66,48.49,49.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.72,46.99,48.3,49.66,51.06,52.53,54.03]
[null,null,null,null,"Coincident",44.47,45.22,46.06,46.94,47.75,48.58,49.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.909999999999997,41.47,42.19,42.95,43.7,44.54,45.39]
[null,null,null,null,"Coincident",39.78,40.32,41.02,41.76,42.49,43.31,44.13]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38.9,39.94,40.99,42.07,43.18,44.35,45.67]
[null,null,null,null,"Coincident",39.85,40.39,41.1,41.84,42.57,43.39,44.21]
[null,"wgl","Substation Rating","MVA","Non-Coincident",84,84,84,84,84,84,84]
[null,null,null,null,"Coincident",84,84,84,84,84,84,84]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.06,1.0900000000000001,1.1299999999999999,1.17,1.21,1.25,1.29]
[null,null,null,null,"Coincident",0.05,0.05,0.05,0.05,0.05,0.05,0.06]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",71.7,73.36,76.040000000000006,79.099999999999994,81.75,84.47,87.19]
[null,null,null,null,"Coincident",64.989999999999995,66.489999999999995,68.92,71.69,74.099999999999994,76.56,79.03]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",63.81,65.61,67.540000000000006,69.61,71.72,73.97,76.180000000000007]
[null,null,null,null,"Coincident",65.13,66.63,69.069999999999993,71.849999999999994,74.25,76.73,79.2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",64.12,65.69,68.31,71.33,73.91,76.52,79.14]
[null,null,null,null,"Coincident",58.12,59.54,61.91,64.650000000000006,66.989999999999995,69.349999999999994,71.73]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.97,59.11,61.56,64.290000000000006,66.819999999999993,69.45,72.03]
[null,null,null,null,"Coincident",58.24,59.67,62.05,64.790000000000006,67.13,69.5,71.88]
[null,"wn","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.77,0.78,0.78,0.79,0.8,0.81,0.83]
[null,null,null,null,"Coincident",0.06,0.06,0.06,0.06,0.06,0.06,0.06]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.48,47.95,48.44,48.98,49.56,50.28,51]
[null,null,null,null,"Coincident",42.97,43.4,43.84,44.33,44.86,45.51,46.16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.91,52.4,53.15,53.87,54.69,55.58,56.49]
[null,null,null,null,"Coincident",43.07,43.5,43.94,44.43,44.96,45.61,46.27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.32,44.81,45.31,45.85,46.38,46.98,47.63]
[null,null,null,null,"Coincident",40.11,40.56,41.01,41.5,41.98,42.52,43.11]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.08,43.99,44.98,46.12,47.24,48.44,49.62]
[null,null,null,null,"Coincident",40.21,40.65,41.1,41.59,42.08,42.62,43.21]
[null,"wo","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident",99,99,99,99,99,99,99]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.04,0.04,0.04,0.04,0.05,0.05,0.05]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.27,47.54,47.98,48.54,49.03,49.56,50.06]
[null,null,null,null,"Coincident",36.11,36.31,36.65,37.08,37.450000000000003,37.86,38.24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.77,45.03,45.48,46.03,46.52,47.06,47.56]
[null,null,null,null,"Coincident",36.24,36.450000000000003,36.79,37.22,37.590000000000003,38,38.380000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.37,43.78,44.22,44.67,45.17,45.7,46.19]
[null,null,null,null,"Coincident",33.130000000000003,33.44,33.78,34.119999999999997,34.5,34.909999999999997,35.28]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.770000000000003,40.18,40.83,41.94,43,43.86,44.66]
[null,null,null,null,"Coincident",33.25,33.57,33.909999999999997,34.25,34.630000000000003,35.04,35.42]
[null,"wots","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.31,0.31,0.32,0.33,0.34,0.35,0.36]
[null,null,null,null,"Coincident",0.1,0.1,0.1,0.11,0.11,0.11,0.12]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.869999999999997,37.68,38.56,39.57,40.6,41.7,42.81]
[null,null,null,null,"Coincident",34.56,35.32,36.14,37.090000000000003,38.06,39.090000000000003,40.130000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.79,36.6,37.619999999999997,39.01,40.32,41.75,43.13]
[null,null,null,null,"Coincident",48.3,49.36,50.51,51.84,53.19,54.63,56.08]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.520000000000003,34.21,35.24,36.729999999999997,38.08,39.47,40.83]
[null,null,null,null,"Coincident",31.42,32.07,33.03,34.43,35.69,37,38.270000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.86,33.92,35.24,36.729999999999997,38.08,39.47,40.83]
[null,null,null,null,"Coincident",43.91,44.81,46.16,48.12,49.88,51.71,53.49]
[null,"wt","Substation Rating","MVA","Non-Coincident",109,109,109,109,109,109,109]
[null,null,null,null,"Coincident",109,109,109,109,109,109,109]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.09,0.09,0.09,0.09,0.1,0.1,0.1]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.069999999999993,69.86,70.709999999999994,71.39,72.349999999999994,73.42,74.48]
[null,null,null,null,"Coincident",54.93,55.56,56.24,56.78,57.54,58.39,59.24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",64.97,65.650000000000006,66.44,67.290000000000006,68.25,69.319999999999993,70.38]
[null,null,null,null,"Coincident",55.23,55.86,56.54,57.09,57.85,58.71,59.56]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",64.239999999999995,64.92,65.680000000000007,66.22,67.06,68.040000000000006,69.03]
[null,null,null,null,"Coincident",51.09,51.63,52.24,52.67,53.34,54.11,54.9]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",57.6,58.15,58.84,59.52,60.31,61.2,62.05]
[null,null,null,null,"Coincident",51.37,51.91,52.52,52.95,53.62,54.41,55.2]
[null,"wyk","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.27,0.27,0.27,0.27,0.28000000000000003,0.28000000000000003,0.28000000000000003]
[null,null,null,null,"Coincident",0.81,0.81,0.82,0.82,0.83,0.83,0.84]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.42,31.53,31.66,31.82,32.07,32.35,32.65]
[null,null,null,null,"Coincident",29,29.1,29.22,29.37,29.6,29.85,30.13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.78,30.19,30.69,31.24,31.75,32.270000000000003,32.72]
[null,null,null,null,"Coincident",29,29.1,29.22,29.37,29.6,29.85,30.13]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.69,28.79,28.96,29.16,29.39,29.64,29.89]
[null,null,null,null,"Coincident",26.48,26.57,26.73,26.91,27.12,27.35,27.58]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.06,27.42,27.8,28.32,28.78,29.26,29.69]
[null,null,null,null,"Coincident",26.48,26.57,26.73,26.91,27.12,27.35,27.58]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"CLN",null,"MWh","Non-Coincident",6.7325188485881649,21.872809446708533,53.202794092211349,117.83789885684723,265.22176776634217,572.31378962689359,1203.8002186114275]
[null,"LLG",null,"MWh","Non-Coincident",8.098689289493219,34.340260886301479,66.857371852496513,91.556973220460691,114.61045506899204,138.83151602452628,165.34064162106748]
[null,"OFR",null,"MWh","Non-Coincident",0,0,0,0,0.63769426962554376,1.4156259719462678,2.5854550780246441]
[null,"KLO",null,"MWh","Non-Coincident",1.1065958970027902E-2,0.13338978338345686,0.67012530962971895,10.855379582032965,81.422191558185077,261.14121965325648,621.30846321883894]
[null,"EPG",null,"MWh","Non-Coincident",1.2039233106075834E-2,2.633667698254951E-2,6.395309878436288E-2,0.13804394705777789,0.26585165596910432,0.46780739710487101,0.79637028650643638]
[null,"DRN",null,"MWh","Non-Coincident",1.2039233106075834E-2,2.633667698254951E-2,6.395309878436288E-2,0.13804394705777789,0.26585165596910432,0.46780739710487101,0.79637028650643638]
[null,"WGI",null,"MWh","Non-Coincident",6.9,9.1999999999999993,12,15.7,20.5,26.8,35.299999999999997]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.2 Reliability & Cust serv","index":22,"n_rows":76,"n_cols":9,"rows_kept":76,"cut":false,"hidden":false,"merged":[[6,1,6,7],[17,1,17,3],[29,1,29,3],[71,4,71,8],[41,1,41,3],[53,1,53,3],[56,1,56,8],[68,1,68,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. There are no further instructions."]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,88.03,88.03,88.03,88.03,88.03]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,184.24,184.24,184.24,184.24,184.24]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,295.08,295.08,295.08,295.08,295.08]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E13:E17)","v":567.34999999999991},{"$f":"SUM(F13:F17)","v":567.34999999999991},{"$f":"SUM(G13:G17)","v":567.34999999999991},{"$f":"SUM(H13:H17)","v":567.34999999999991},{"$f":"SUM(I13:I17)","v":567.34999999999991}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.81200000000000006,0.81200000000000006,0.81200000000000006,0.81200000000000006,0.81200000000000006]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1.506,1.506,1.506,1.506,1.506]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,2.1459999999999999,2.1459999999999999,2.1459999999999999,2.1459999999999999,2.1459999999999999]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E25:E29)","v":4.4640000000000004},{"$f":"SUM(F25:F29)","v":4.4640000000000004},{"$f":"SUM(G25:G29)","v":4.4640000000000004},{"$f":"SUM(H25:H29)","v":4.4640000000000004},{"$f":"SUM(I25:I29)","v":4.4640000000000004}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E37:E41)","v":0},{"$f":"SUM(F37:F41)","v":0},{"$f":"SUM(G37:G41)","v":0},{"$f":"SUM(H37:H41)","v":0},{"$f":"SUM(I37:I41)","v":0}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E49:E53)","v":0},{"$f":"SUM(F49:F53)","v":0},{"$f":"SUM(G49:G53)","v":0},{"$f":"SUM(H49:H53)","v":0},{"$f":"SUM(I49:I53)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS (STPIS)"]
[null,null,"FORECAST"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},356478,361899,372929,380943,388386,392563,399960]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},327761,336145,337766,342235,348149,357105,363059]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},138361,139894,142763,145904,148252,150914,153463]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C62:C66)","v":822600},837938,853458,869082,884787,900582,916482]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Number of calls received",null,null,125486,128462,131572,134854,138242]
[null,"Number of calls answered within 30 seconds",null,null,100388,102765,105257,107886,110563]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E75/E74),\"\")","v":0.79999362478682878},{"$f":"IFERROR((F75/F74),\"\")","v":0.79996419174541888},{"$f":"IFERROR((G75/G74),\"\")","v":0.79999543975921927},{"$f":"IFERROR((H75/H74),\"\")","v":0.80002076319575244},{"$f":"IFERROR((I75/I74),\"\")","v":0.79977864903574891}]

{"sheet":"7.1  Policies and Procedures","index":23,"n_rows":386,"n_cols":5,"rows_kept":386,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"Asset Management Strategy","The document sets out the significant Asset Management Drivers  as well as Electricity Distribution Asset Management Objectives and Network Performance and Process and System Strategies","Provides an overview of the asset management system and interdependencies.","No"]
[null,"Consumer Energy Resources (CER) Integration Strategy","The document provides an overview of the strategy for effective CER intgration ands sets out plans to effciently ingreate CER.  Inlcudes the transition to the role of the Distribution System Operator (DSO).","Provides an overview of the CER strategy that the relevant expenditure is based on.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Governance framework"]
[null,"AMS 01-09 Asset Risk Management","This document outlines the various components and methods used in risk identification, evaluation and management.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"AMS 20-13 Enhanced Network Safety","The objective of the Enhanced Safety Strategy is to optimise the output of the Electricity Safety Management Scheme (ESMS), the Bushfire Mitigation program and the Occupational Health & Safety Management System to identify and prioritise opportunities to develop and implement network asset management initiatives and programs that continuously reduce network related health and safety risks 'so far as is practicable’ for customers, public and personnel. ","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"BFM 10-01 Bushfire Mitigation Plan","This document outlines the initiatives and controls implemented by AusNet Services to reduce bushfire risk on its electricity distribution network.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"QMS 10-01-1 Health, Safety, Enviornment and Quality Policy","High level document that shows AusNet Services commitment to providing a safe and healthy work enviornment","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"ESMS 10-01 Electricity Safety Management Scheme","This document (ESMS 10-01 Overview) contains a summary of the structure of the ESMS for AusNet Services' electricity distribution supply network.  It also outlines the period of application, the location of ESMS records, exemptions and lists officers responsible for the operation of this ESMS.","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"ESMS 10-03 Electricity Safety Management System","This document describe the assets forming AusNet Services' electricity distribution supply network, their location and the associated planning, design, construction, commissioning, operation, augmentation, inspection, testing, maintenance, refurbishment, replacement and decommissioning processes necessary to ensure the safety of consumers, the general public, AusNet Services' staff and contractors.","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Cost Estimating Methodology","The purpose of this document is to describe the principles, methodologies and procedures AusNet  follow to prepare cost estimates for major capital projects developed for the Electricity Distribution Price Review (EDPR) submission for the regulatory period 2026-2031.","Cost Estimating","No"]
[null,"Cost Allocation Methodology","The CAM establishes a method for attributing direct costs and allocating indirect costs between various categories of Essential Energy’s distribution services, that is, between direct control services (standard control services and alternative control services), negotiated services and unregulated distribution services.   ","Cost Allocation","No"]
[null,"Asset Capitalisation Policy (Property, Plant & Equipment)","The document describes property strategy, asset management plan and expenditure program to meet our strategic objectives and operational requirements. ","RIN Supporting Information, Chapter 6 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"​Asset Risk Assessment Overview ","This document describes the methodologies used by AusNet to determine the asset risk and the mitigating methods for regulated network assets. The results of the risk assessment can be reported in a risk matrix.  The document is not intended to be prescriptive for every asset class, it details accepted methods.  The unique characteristics of an asset class will determine the specific methods used.   ","Determines Risk approach.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset Management Strategies"]
[null,"Poles – Asset Strategy","This document is part of the suite of Asset Management Strategies relating to the AusNet electricity distribution network. The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of galvanised steel, steel reinforced concrete, wood, and glass reinforced concrete poles in AusNet’s electricity distribution network. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Conductor – Asset Strategy","This document is part of the suite of Asset Management Strategies relating to AusNet’s electricity distribution network. The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of zone substation circuit breakers (CBs).  "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"MV Switches & ACRs (lines) - Asset Strategy","This document is part of the Asset Management Strategies related to AusNet’s electricity distribution network. The purpose of this strategy is to outline the inspection, maintenance, replacement, and monitoring activities identified for the effective economic lifecycle management of Medium Voltage Switches and Automatic Circuit Reclosers (ACRs). This encompasses all associated switchgear, instrumentation, and control components.  "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Power Transformers – Asset Strategy","The purpose of this document is to outline the inspection, maintenance, replacement, and monitoring activities identified for economic life cycle management of the fleet of zone substation power transformers and regulators in AusNet’s Victorian electricity distribution network. This document is intended to be used to inform asset management decisions and communicate the basis for activities.  "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Circuit Breakers (Z/S) - Asset Strategy","This document is part of the suite of Asset Management Strategies relating to AusNet’s electricity distribution network. The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of zone substation circuit breakers (CBs).  "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Fuses (MV Fuse Switch disconnectors) – Asset Strategy","The purpose of this document is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of medium voltage (MV) Fuse Switch Disconnectors (FSDs) in AusNets Victorian electricity distribution network. This document intends to be used to inform asset management decisions and communicate the basis for activities. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Crossarms – Asset Strategy","The purpose of this document is to outline the inspection, maintenance, replacement and monitoring activities identified for the economic life cycle management of crossarms in AusNet’s’ Victorian electricity distribution network. This document is intended to be used to inform asset management decisions and communicate the basis for activities"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Distribution Transformers – Asset Strategy","The purpose of this document is to outline the inspection, maintenance, replacement, and monitoring activities identified for economic life cycle management of distribution transformers in AusNet. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Services – Asset Strategy","The purpose of this document is to outline the maintenance, replacement and performance of the service cables connecting customers to low voltage (LV) circuits in AusNet Service’s electricity distribution network.   "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Protection & Control – Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of protection and control schemes and Supervisory Control and Data Acquisition (SCADA) Remote Terminal Units (RTU) in AusNet’ Victorian electricity distribution network. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Instrument transformers – Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of Instrument Transformer.  "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Comms – Asset Strategy","This docuement outlines various communications related technologies, their condition and the strategies aimed at enhancing the reliability of the electricity distribution network and supporting Information Technology systems to efficiently deliver existing and future communication services. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Z/S Civil Infrastructure - Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of civil infrastructure facilities in AusNet’s Victorian electricity distribution network. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Indoor Switchboards - Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of indoor switchboards in AusNet’s Victorian electricity distribution network."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Neutral Earthing Device - Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of Neutral Earthing Devices. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"HV Switches, Disconnectors & Earth Switches - Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of zone substation HV switches, Disconnectors and earth switches. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Insulators - High & Medium Voltage - Asset Strategy","The purpose of this strategy is to outline the inspection, maintenance, replacement and monitoring activities identified for economic life cycle management of high (HV) and medium voltage (MV) Insulators in AusNets’ Victorian electricity distribution network."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[]
[]
[]
[null,"Asset Management Plans"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Asset Capitalisation Policy (Property, Plant & Equipment)","The document describes property strategy, asset management plan and expenditure program to meet our strategic objectives and operational requirements. ","RIN Supporting Information, Chapter 6 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Resilience Strategy","This document is our Resilience Strategy which describes our vision and approach for ensuring that we factor resilience into our decision-making, so that we deliver optimal outcomes for our customers when disruptive events occur. ","Resilience capex forecast","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"Procurement Principles","This document defines the priciples to ensure an integrated, consistent and compliant approach to procuremnt is undertaken across the organisation","Business as usual","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Information technology policies or strategies"]
[null,"Digital Investment Strategy","This document outlines the strategic direction and forecast expenditure of AusNet Services’ information, communication and technology (ICT) capabilities for our electricity distribution services in the 2026-31 regulatory  period.  ","Digital forecast","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Distribution Annual Planning Report","AusNet Services produces each year a Distribution Annual Planning Report (DAPR) in accordance with the requirements of Section 5.13.2 of the National Electricity Rules (NER).  The information contained within the DAPR complies with the requirements of Schedule 5.8 of the NER ","Chapter 6 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Self insurance guidelines or policy"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Land and easement acquisition polices"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"BFM 10-01 Bushfire Mitigation Plan","This plan details the policies and procedures which govern AusNet Services bushfire risk management practices. It is a self contained document except where it specifically refers to other related documents. ","Chapter 6 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"Network Contingency Plan","The objective of this Plan is to provide the framework for network contingency planning and provide an overview of the suite of contingency plans established for the electricity distribution network. The Network Contingency Plan is applicable to events that directly impact or are likely to directly impact or impede the safe and reliable operation of the distribution network or which interrupt or are likely to interrupt power supply which require a Level 2 or greater response under the SPIRACS Crisis & Emergency Management Guide 30-4006-041. It does not cover the broader business continuity planning undertaken under SPIRACS.","This document underpins expenditure required for network contigency if a plan is enacted for the electricity distribution network.","No"]

{"sheet":"7.2 Contingent projects","index":24,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"7.2 CONTINGENT PROJECTS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($, nominal)\")","v":"Proposed annual revenue requirement for 2026-27 \n($, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2026-27"}]
[null,null,null,null,null,{"$f":"+E9*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$9","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":25,"n_rows":295,"n_cols":5,"rows_kept":295,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"National Electricity Law (NEL)","Impose obligations including registration, distribution losses, network connections, economic regulation and metering.","Submission document","No"]
[null,"Electricity Industry Act 2000","Sets out key obligations relating to distribution of electricity in Victoria including matters such as licences and compliance with industry codes, standards, rules and guidelines.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"Electricity Safety Amendment (Bushfire Mitigation Civil Penalties Scheme) Act 2017 ","Amended the Electricity Safety Act 1998 (Vic) (ESA) to provide for significant financial penalties if AusNet Services fails to achieve the REFCL milestones prescribed by the Regulations by the applicable deadline","Chapter 6 Capex, Chapter 7Opex, Chapter 15 Cost pass Through","Yes"]
[null,"Electricity Safety (Bushfire Mitigation) Regulations 2013 (amendments as at 1 May 2016)","Requires the preparation of bushfire mitigation plans and specifies inspection of assets.","Chapter 6 Capex, Chapter 7 Opex, Chapter 15 Cost pass Through","Yes"]
[null,"Electricity Safety (Electric Line Clearance) Regulations 2015","Prescribes line clearance requirements including vegetation clearing","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Electricity Safety (Management) Regulations 2009","Sets out requirements for Electricity Safety Management Schemes.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Electricity Distribution Code of Practice","Regulates connection and distribution of electricity to customers, connection of embedded generating units, and transfer between distribution systems to ensure that they are undertaken in a safe, efficient and reliable manner. Sets out obligations in relation to smart meters.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"Electricity System Code","Requires particular power quality and connection characteristics.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Public Lighting Code","Regulates the provision of public lighting by specifying minimum standards and certain obligations of distributors and public lighting customers.","Chapter 18: Alternative Control Service - Public lighting","No"]
[null,"Electricity Industry Guideline No.14","Sets out customer contributions, requirements for undergrounding network assets and contestability of connection works.","Chapter 6 Capex, Chapter 7 Opex, TSS","No"]
[null,"Electricity Industry Guideline No.15","Sets out arrangement for connecting embedded generation units to distribution systems","Chapter 6 Capex, Chapter 7 Opex, TSS","No"]
[null,"Electricity Distribution Licence","Sets out obligations of AusNet Services in relation to distribution of electricity in Victoria including requirements to connect customers, offer services, undertake network augmentation and comply with orders, codes and guidelines.","Chapter 4 Demandand Energy Forecasts,  Chapte 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"Emergency Management Act 2013","Establishes arrangments for management of emergencies in Victoria ","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Terrorism (Community Protection) Act 2003","Obliges providers of essential services including electricity to plan for the protection of services from the effects of terrorist acts.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Energy and Water Ombudsman Charter 2006","Describes how electricity licence holders must participate in a customer dispute resolution scheme and how this scheme operates in Victoria.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Occupational Health and Safety Act 2004","Sets out duties of employers and persons who manage or control workplaces to provide for the health, safety and welfare of employees and other persons including the public. Describes the principle of eliminating or reducing risks so far as is practicable.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Occupational Health and Safety Regulations 2017","Detail many aspects of OH&S including manual handling, exposure to noise, prevention of falls, work in confined spaces, operating plant, and asbestos control & handling. ","Chapter 6 Capex, Chapter 7 Opex Chapter 17 Metering","No"]
[null,"National Greenhouse and Energy Reporting Act 2007","Provides for reporting and dissemination of information related to greenhouse emissions including annual reporting.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"National Greenhouse and Energy Reporting Regulations 2008","Sets out requirements for reporting greenhouse emissions.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Environment Protection Act 1970","Legislative framework for the protection of the environment in Victoria.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Environmental Protection (Residential Noise) Regulations 2018","Prescribes items and times during which noise resulting from their use is deemed to be unreasonable on residential properties.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Aboriginal Heritage Act 2006","Promotes the recognition, protection and conservation of Aboriginal culture in Victoria; recognition of Aboriginal people as the primary guardians of their cultural heritage; and management of Aboriginal cultural heritage as an integral part of land management.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Land Act 1958","Defines Crown Land and conditions relating to Crown Land which prohibit a number of activities including refuelling of vehicles, removal of vegetation and disposal of waste.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"National Measurement Act 1960 and Regulations","The National Measurement Act establishes a national system of units and standards of measuremnet of physical quantities and provides for a national system of trade measurements. The National Trade Measurement Regulations were amended in remove the exemption for electricity meters.  Electricity meters installed prior to 1 January 2013 are exempt, whilst electricity meters installed after 1 January 2013 must comply with the National Measurement Act and Regulations.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Privacy Act 1988","Obligations to protect the privacy of individuals and the responsible and transparent handling of personal information in accordance with the Australian Privacy Principles (APPs).","Submission document","No"]
[null,"AMI Cost Recovery Order in Council (CROIC)","The Order in Council made on 28 August 2007 under section 15A and 46D of the Electricity Industry Act 2000 as amended from time to time establishing  \n- conditions for cost recovery for AMI deployments;\n- obligations requiring Victorian Distribution Businesses to deploy an AMI meter to every eligible customer; and\nrequirements to pay rebates to customers without an AMI meter installed or operating as remotely read interval meters","Chapter 6 Capex, Chapter 7 Opex, Chapter 17  Metering, TSS","No"]
[null,"AMI Specifications Order","The Order in Council made on 12 November 2007 under section 15A and 46D of the Electricity Industry Act 2000 requiring the deployment of AMI Meters and AMI System inaccordance with the Minimum AMI Functionality Specification and the Minimum AMI Service Levels Specification in Victoria.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"AMI Tariff Order","Provides the regulatory framework for applying AMI tariffs, transfer between and consent to AMI tariffs, assignment of AMI tariffs, customer access to meter data.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"Electricity Customer Transfer Code","The purpose of this Code is to facilitate and regulate aspects of the process by which customers can choose to change retailer.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Customer Metering Code","The purpose of this Code is to regulate customer metering to the extent not regulated by AEMO Procedures.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"Default Use-Of-System Agreement","This agreement sets out the rights and obligations of the parties in respect of:\n(a) the provision of the Distribution Services by the Distributor to the Retailer in respect of Customers, and the payment for those Distribution Services by the Retailer; and\n(b) the provision of Retail Services by the Retailer, and the payment for those Retail Services by the Distributor","Chapter 4 Demand Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering, TSS","No"]
[null,"Metrology Procedures","Establishes obligations on the application of metering installations to connection points and sets out provisions for metering installations and metering data services.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"MPB Service Level Procedure","Details the technical requirements and performances associated with the provision, installation and maintenance of a metering installation. ","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"MDP Service Level Procedure","Details the obligations, technical requirements and performances associated with the processes of meter reading, data collection, data processing, adjustment, aggregation and delivery of metering data","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"NMI Procedures","Establishes conditions and describes processes for creating and abolishing NMIs","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"CATS Procedures","Establishes the conditions and processes for governing AEMO's Market Settlement and Transfer System (MSATS)","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"B2B Procedures","Define the transactions and conditions for information exchange as defined under chapter 7 of the Rules","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"Other Metering Services procedures and guidelines","Various procedures and guidelines that instruct participants on how metering and related interaction to other participants is to be undertaken.","Chapter 6 Capex, Chapter 7 Opex, Chapter 17 Metering","No"]
[null,"Direction under Section 141(2)(d) of the Electricity Safety Act 1998 Fitting of Spacers in Aerial Lines","Direction from Energy Safe Victoria under Section 141(2)( d) of the Electricity Safety Act 1998 which requires the fitting of spacers in overhead lines.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"National Electricity (Victoria) Act 2005","This Act provides for the regulation of the national electricity wholesale market. It is part of a national scheme which gives effect to the National Electricity Law and the National Electricity Rules made under that Law. The lead legislation under the national scheme is the National Electricity (South Australia) Act 1996. The economic regulator is the Australian Energy Regulator (AER) and the rule-maker is the Australian Energy Market Commission (AEMC). The national electricity wholesale market is administered by the Australian Energy Market Operator (AEMO).","Chapter 13 Incentive Scheme","No"]
[null,"Superannuation Guarantee (Administration) Act 1992, No. 111","The Act sets out relevant superannuation payment requirements.","Chapter 7 Opex","No"]
[null,"Roads Management Act 2004 (Vic)","Safety obligations when carrying out works on public roadways.","Chapter 6 Capex, Chapter 18 Public Lighting","No"]
[null,"Fair Work Act 2009","Sets out our obligations in relation to the negotiation of employment terms and conditions.","Chapter 7 Opex","No"]
[null,"The Security of Critical Infrastructure Act 2018 (Cth) ","May result in additional cyber security obligations being imposed on AusNet Services","Chapter 7 Opex","Yes"]
[null,"National Electricity Amendment (Five Minute Settlement) Rule 2017 No. 15","Aligns operational dispatch and financial settlement to occur at five minute intervals","Chapter 7Opex","Yes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"Electricity Distribution Licence (2005)","The Licence authorisesAusNet  to distribute or supply electricity to supply points located in the Licensee’s distribution area.","Chapter 6 Capex","No"]
[]
[]
[]
[null,"RULES"]
[null,"National Electricity Rules\n","National Electricity Rules - Details the technical operational requirements for the operation of the National Electricity Market\nNational Energy Retail Rules","Chapter 6 Capex, Chapter 7 Opex","No"]
[]
[]
[]
[null,"ORDERS"]
[]
[]
[]
[null,"CODES"]
[null,"Building Code of Australia","Building Code of Australia published by the Australian Building Codes Board as in force from time to time\nBuilding and Construction Industry (Fair and Lawful Building Sites) Code 2014\nCode for the Tendering and Performance of Building Work ","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"National Harmonisation of Work Health and Safety Code of Practice","Achieving the standards of health, safety and welfare.","Chapter 6 Capex, Chapter 7 Opex","No"]
[null,"Electricity Distribution Code (2014)","The purpose of this Code is to regulate the following activities so that they are undertaken in a safe, efficient and reliable manner:\n(a) the distribution of electricity by a distributor for supply to its customers;\n(b) the connection of a customer’s electrical installation to the distribution system;\n(c) the connection of embedded generating units to the distribution system; and\n(d) the transfer of electricity between distribution systems.","Chapter 6 Capex, Chapter 13 incentive Schemes, Chapter 15 Cost Pass through","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[]
[]
[]
[null,"OTHER"]

{"sheet":"7.4 Shared Assets","index":26,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8],[30,2,30,8],[31,2,31,8],[32,2,32,8],[39,2,39,8],[40,2,40,8],[7,1,8,1],[7,2,8,2],[27,2,27,8],[28,2,28,8],[29,2,29,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"7.4 SHARED ASSETS"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service",{"$f":"CONCATENATE(\"Shared asset unregulated revenue  \n($, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  \n($, real June 2026)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", FRCP_y5)","v":"Total 2026-27 to 2030-31"}]
[null,"Leasing Access to third parties - various communications equipment installed on distribution assets","Poles shared for communication services, including distribution poles.",2316302,2374210,2433565,2494404,2556764,2620683,2686200,{"$f":"SUM(F10:J10)","v":12791616}]
[null,"Leasing Access to third parties - providing access to distribution assets for the construction and operation of fibre optic cable (FOC).","Assets shared to facilitate the construction, operation, and maintenance of the Fibre Optic Cable (FOC), including fibre optic cable, poles and other structures, fixtures and fittings, polemounted patch connectors and enclosures, and Pits.",264880.01380000002,256666.68,250406.5171,244299.041,238340.52789999999,232527.34419999999,226855.94560000001,1192429.3758]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]

{"sheet":"7.7 TSS-LRMC","index":27,"n_rows":155,"n_cols":22,"rows_kept":155,"cut":false,"hidden":false,"merged":[[69,1,70,1],[89,1,90,1],[6,3,7,4],[11,1,12,1],[23,1,24,1],[35,1,36,1],[49,1,50,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is AusNet (D) using the 'Average Incremental Cost' approach?"}]
[null,null,null,null,null,"YES"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2026"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C13,4)+1)&\"-\"&MID(C13,3,2)+2),VALUE(LEFT(C13,4)+1))","v":"2025-26"},"2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42","2042-43","2043-44"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure",4233500,3946000,47277725.060212523,63981022.713837437,88063113.49477081,53213451.58208096,65022321.149098277]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C14:C20)","v":4233500},{"$f":"SUM(D14:D20)","v":3946000},47277725.060212523,63981022.713837437,88063113.49477081,53213451.58208096,65022321.149098277,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2026"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C25,4)+1)&\"-\"&MID(C25,3,2)+2),VALUE(LEFT(C25,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D25,4)+1)&\"-\"&MID(D25,3,2)+2),VALUE(LEFT(D25,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E25,4)+1)&\"-\"&MID(E25,3,2)+2),VALUE(LEFT(E25,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F25,4)+1)&\"-\"&MID(F25,3,2)+2),VALUE(LEFT(F25,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G25,4)+1)&\"-\"&MID(G25,3,2)+2),VALUE(LEFT(G25,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H25,4)+1)&\"-\"&MID(H25,3,2)+2),VALUE(LEFT(H25,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I25,4)+1)&\"-\"&MID(I25,3,2)+2),VALUE(LEFT(I25,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J25,4)+1)&\"-\"&MID(J25,3,2)+2),VALUE(LEFT(J25,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K25,4)+1)&\"-\"&MID(K25,3,2)+2),VALUE(LEFT(K25,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L25,4)+1)&\"-\"&MID(L25,3,2)+2),VALUE(LEFT(L25,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M25,4)+1)&\"-\"&MID(M25,3,2)+2),VALUE(LEFT(M25,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N25,4)+1)&\"-\"&MID(N25,3,2)+2),VALUE(LEFT(N25,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O25,4)+1)&\"-\"&MID(O25,3,2)+2),VALUE(LEFT(O25,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P25,4)+1)&\"-\"&MID(P25,3,2)+2),VALUE(LEFT(P25,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q25,4)+1)&\"-\"&MID(Q25,3,2)+2),VALUE(LEFT(Q25,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R25,4)+1)&\"-\"&MID(R25,3,2)+2),VALUE(LEFT(R25,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S25,4)+1)&\"-\"&MID(S25,3,2)+2),VALUE(LEFT(S25,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T25,4)+1)&\"-\"&MID(T25,3,2)+2),VALUE(LEFT(T25,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U25,4)+1)&\"-\"&MID(U25,3,2)+2),VALUE(LEFT(U25,4)+1))","v":"2043-44"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Export services","                                         -  ","                                         -  ",8300000,6400000,0,20263500,0]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C26:C32)","v":0},{"$f":"SUM(D26:D32)","v":0},8300000,6400000,0,20263500,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2026"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C37,4)+1)&\"-\"&MID(C37,3,2)+2),VALUE(LEFT(C37,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D37,4)+1)&\"-\"&MID(D37,3,2)+2),VALUE(LEFT(D37,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E37,4)+1)&\"-\"&MID(E37,3,2)+2),VALUE(LEFT(E37,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F37,4)+1)&\"-\"&MID(F37,3,2)+2),VALUE(LEFT(F37,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G37,4)+1)&\"-\"&MID(G37,3,2)+2),VALUE(LEFT(G37,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H37,4)+1)&\"-\"&MID(H37,3,2)+2),VALUE(LEFT(H37,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I37,4)+1)&\"-\"&MID(I37,3,2)+2),VALUE(LEFT(I37,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J37,4)+1)&\"-\"&MID(J37,3,2)+2),VALUE(LEFT(J37,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K37,4)+1)&\"-\"&MID(K37,3,2)+2),VALUE(LEFT(K37,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L37,4)+1)&\"-\"&MID(L37,3,2)+2),VALUE(LEFT(L37,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M37,4)+1)&\"-\"&MID(M37,3,2)+2),VALUE(LEFT(M37,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N37,4)+1)&\"-\"&MID(N37,3,2)+2),VALUE(LEFT(N37,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O37,4)+1)&\"-\"&MID(O37,3,2)+2),VALUE(LEFT(O37,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P37,4)+1)&\"-\"&MID(P37,3,2)+2),VALUE(LEFT(P37,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q37,4)+1)&\"-\"&MID(Q37,3,2)+2),VALUE(LEFT(Q37,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R37,4)+1)&\"-\"&MID(R37,3,2)+2),VALUE(LEFT(R37,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S37,4)+1)&\"-\"&MID(S37,3,2)+2),VALUE(LEFT(S37,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T37,4)+1)&\"-\"&MID(T37,3,2)+2),VALUE(LEFT(T37,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U37,4)+1)&\"-\"&MID(U37,3,2)+2),VALUE(LEFT(U37,4)+1))","v":"2043-44"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C37:C43)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2026"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C51,4)+1)&\"-\"&MID(C51,3,2)+2),VALUE(LEFT(C51,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D51,4)+1)&\"-\"&MID(D51,3,2)+2),VALUE(LEFT(D51,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E51,4)+1)&\"-\"&MID(E51,3,2)+2),VALUE(LEFT(E51,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F51,4)+1)&\"-\"&MID(F51,3,2)+2),VALUE(LEFT(F51,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G51,4)+1)&\"-\"&MID(G51,3,2)+2),VALUE(LEFT(G51,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H51,4)+1)&\"-\"&MID(H51,3,2)+2),VALUE(LEFT(H51,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I51,4)+1)&\"-\"&MID(I51,3,2)+2),VALUE(LEFT(I51,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J51,4)+1)&\"-\"&MID(J51,3,2)+2),VALUE(LEFT(J51,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K51,4)+1)&\"-\"&MID(K51,3,2)+2),VALUE(LEFT(K51,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L51,4)+1)&\"-\"&MID(L51,3,2)+2),VALUE(LEFT(L51,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M51,4)+1)&\"-\"&MID(M51,3,2)+2),VALUE(LEFT(M51,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N51,4)+1)&\"-\"&MID(N51,3,2)+2),VALUE(LEFT(N51,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O51,4)+1)&\"-\"&MID(O51,3,2)+2),VALUE(LEFT(O51,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P51,4)+1)&\"-\"&MID(P51,3,2)+2),VALUE(LEFT(P51,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q51,4)+1)&\"-\"&MID(Q51,3,2)+2),VALUE(LEFT(Q51,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R51,4)+1)&\"-\"&MID(R51,3,2)+2),VALUE(LEFT(R51,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S51,4)+1)&\"-\"&MID(S51,3,2)+2),VALUE(LEFT(S51,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T51,4)+1)&\"-\"&MID(T51,3,2)+2),VALUE(LEFT(T51,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U51,4)+1)&\"-\"&MID(U51,3,2)+2),VALUE(LEFT(U51,4)+1))","v":"2043-44"}]
[null,"Based on 0.5% of capex",387681.24393333332,427141.24393333332,236388.62530106262,556293.73887024983,996609.30634410388,1262676.5642545086,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C52:C66)","v":387681.24393333332},{"$f":"SUM(D52:D66)","v":427141.24393333332},236388.62530106262,556293.73887024983,996609.30634410388,1262676.5642545086,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17,1587788.17]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2026"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C71,4)+1)&\"-\"&MID(C71,3,2)+2),VALUE(LEFT(C71,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D71,4)+1)&\"-\"&MID(D71,3,2)+2),VALUE(LEFT(D71,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E71,4)+1)&\"-\"&MID(E71,3,2)+2),VALUE(LEFT(E71,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F71,4)+1)&\"-\"&MID(F71,3,2)+2),VALUE(LEFT(F71,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G71,4)+1)&\"-\"&MID(G71,3,2)+2),VALUE(LEFT(G71,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H71,4)+1)&\"-\"&MID(H71,3,2)+2),VALUE(LEFT(H71,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I71,4)+1)&\"-\"&MID(I71,3,2)+2),VALUE(LEFT(I71,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J71,4)+1)&\"-\"&MID(J71,3,2)+2),VALUE(LEFT(J71,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K71,4)+1)&\"-\"&MID(K71,3,2)+2),VALUE(LEFT(K71,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L71,4)+1)&\"-\"&MID(L71,3,2)+2),VALUE(LEFT(L71,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M71,4)+1)&\"-\"&MID(M71,3,2)+2),VALUE(LEFT(M71,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N71,4)+1)&\"-\"&MID(N71,3,2)+2),VALUE(LEFT(N71,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O71,4)+1)&\"-\"&MID(O71,3,2)+2),VALUE(LEFT(O71,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P71,4)+1)&\"-\"&MID(P71,3,2)+2),VALUE(LEFT(P71,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q71,4)+1)&\"-\"&MID(Q71,3,2)+2),VALUE(LEFT(Q71,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R71,4)+1)&\"-\"&MID(R71,3,2)+2),VALUE(LEFT(R71,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S71,4)+1)&\"-\"&MID(S71,3,2)+2),VALUE(LEFT(S71,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T71,4)+1)&\"-\"&MID(T71,3,2)+2),VALUE(LEFT(T71,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U71,4)+1)&\"-\"&MID(U71,3,2)+2),VALUE(LEFT(U71,4)+1))","v":"2043-44"}]
[null,"Based on 0.5% of capex","                                         -  ","                                         -  ",41500,73500,73500,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5,174817.5]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C72:C86)","v":0},{"$f":"SUM(D72:D86)","v":0},{"$f":"SUM(E72:E86)","v":41500},{"$f":"SUM(F72:F86)","v":73500},{"$f":"SUM(G72:G86)","v":73500},{"$f":"SUM(H72:H86)","v":174817.5},{"$f":"SUM(I72:I86)","v":174817.5},{"$f":"SUM(J72:J86)","v":174817.5},{"$f":"SUM(K72:K86)","v":174817.5},{"$f":"SUM(L72:L86)","v":174817.5},{"$f":"SUM(M72:M86)","v":174817.5},{"$f":"SUM(N72:N86)","v":174817.5},{"$f":"SUM(O72:O86)","v":174817.5},{"$f":"SUM(P72:P86)","v":174817.5},{"$f":"SUM(Q72:Q86)","v":174817.5},{"$f":"SUM(R72:R86)","v":174817.5},{"$f":"SUM(S72:S86)","v":174817.5},{"$f":"SUM(T72:T86)","v":174817.5},{"$f":"SUM(U72:U86)","v":174817.5},{"$f":"SUM(V72:V86)","v":174817.5}]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"FORECAST \n($, real \", dms_DollarReal)","v":"FORECAST \n($, real June 2026"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C91,4)+1)&\"-\"&MID(C91,3,2)+2),VALUE(LEFT(C91,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D91,4)+1)&\"-\"&MID(D91,3,2)+2),VALUE(LEFT(D91,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E91,4)+1)&\"-\"&MID(E91,3,2)+2),VALUE(LEFT(E91,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F91,4)+1)&\"-\"&MID(F91,3,2)+2),VALUE(LEFT(F91,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G91,4)+1)&\"-\"&MID(G91,3,2)+2),VALUE(LEFT(G91,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H91,4)+1)&\"-\"&MID(H91,3,2)+2),VALUE(LEFT(H91,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I91,4)+1)&\"-\"&MID(I91,3,2)+2),VALUE(LEFT(I91,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J91,4)+1)&\"-\"&MID(J91,3,2)+2),VALUE(LEFT(J91,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K91,4)+1)&\"-\"&MID(K91,3,2)+2),VALUE(LEFT(K91,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L91,4)+1)&\"-\"&MID(L91,3,2)+2),VALUE(LEFT(L91,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M91,4)+1)&\"-\"&MID(M91,3,2)+2),VALUE(LEFT(M91,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N91,4)+1)&\"-\"&MID(N91,3,2)+2),VALUE(LEFT(N91,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O91,4)+1)&\"-\"&MID(O91,3,2)+2),VALUE(LEFT(O91,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P91,4)+1)&\"-\"&MID(P91,3,2)+2),VALUE(LEFT(P91,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q91,4)+1)&\"-\"&MID(Q91,3,2)+2),VALUE(LEFT(Q91,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R91,4)+1)&\"-\"&MID(R91,3,2)+2),VALUE(LEFT(R91,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S91,4)+1)&\"-\"&MID(S91,3,2)+2),VALUE(LEFT(S91,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T91,4)+1)&\"-\"&MID(T91,3,2)+2),VALUE(LEFT(T91,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U91,4)+1)&\"-\"&MID(U91,3,2)+2),VALUE(LEFT(U91,4)+1))","v":"2043-44"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C92:C106)","v":0},{"$f":"SUM(D92:D106)","v":0},{"$f":"SUM(E92:E106)","v":0},{"$f":"SUM(F92:F106)","v":0},{"$f":"SUM(G92:G106)","v":0},{"$f":"SUM(H92:H106)","v":0},{"$f":"SUM(I92:I106)","v":0},{"$f":"SUM(J92:J106)","v":0},{"$f":"SUM(K92:K106)","v":0},{"$f":"SUM(L92:L106)","v":0},{"$f":"SUM(M92:M106)","v":0},{"$f":"SUM(N92:N106)","v":0},{"$f":"SUM(O92:O106)","v":0},{"$f":"SUM(P92:P106)","v":0},{"$f":"SUM(Q92:Q106)","v":0},{"$f":"SUM(R92:R106)","v":0},{"$f":"SUM(S92:S106)","v":0},{"$f":"SUM(T92:T106)","v":0},{"$f":"SUM(U92:U106)","v":0},{"$f":"SUM(V92:V106)","v":0}]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C114,4)+1)&\"-\"&MID(C114,3,2)+2),VALUE(LEFT(C114,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D114,4)+1)&\"-\"&MID(D114,3,2)+2),VALUE(LEFT(D114,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E114,4)+1)&\"-\"&MID(E114,3,2)+2),VALUE(LEFT(E114,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F114,4)+1)&\"-\"&MID(F114,3,2)+2),VALUE(LEFT(F114,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G114,4)+1)&\"-\"&MID(G114,3,2)+2),VALUE(LEFT(G114,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H114,4)+1)&\"-\"&MID(H114,3,2)+2),VALUE(LEFT(H114,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I114,4)+1)&\"-\"&MID(I114,3,2)+2),VALUE(LEFT(I114,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J114,4)+1)&\"-\"&MID(J114,3,2)+2),VALUE(LEFT(J114,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K114,4)+1)&\"-\"&MID(K114,3,2)+2),VALUE(LEFT(K114,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L114,4)+1)&\"-\"&MID(L114,3,2)+2),VALUE(LEFT(L114,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M114,4)+1)&\"-\"&MID(M114,3,2)+2),VALUE(LEFT(M114,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N114,4)+1)&\"-\"&MID(N114,3,2)+2),VALUE(LEFT(N114,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O114,4)+1)&\"-\"&MID(O114,3,2)+2),VALUE(LEFT(O114,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P114,4)+1)&\"-\"&MID(P114,3,2)+2),VALUE(LEFT(P114,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q114,4)+1)&\"-\"&MID(Q114,3,2)+2),VALUE(LEFT(Q114,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R114,4)+1)&\"-\"&MID(R114,3,2)+2),VALUE(LEFT(R114,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S114,4)+1)&\"-\"&MID(S114,3,2)+2),VALUE(LEFT(S114,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T114,4)+1)&\"-\"&MID(T114,3,2)+2),VALUE(LEFT(T114,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U114,4)+1)&\"-\"&MID(U114,3,2)+2),VALUE(LEFT(U114,4)+1))","v":"2043-44"}]
[null,"MW",162.34583705867473,189.4891304360489,39.850000000000136,85.632000000000062,137.87699999999995,192.44799999999987,247.1840000000002,303.06600000000026,362.41300000000001,423.64200000000028,482.42399999999998,541.6579999999999,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C115:C124)","v":-162.34583705867473},{"$f":"-SUM(D115:D124)","v":-189.4891304360489},-39.850000000000136,-85.632000000000062,-137.87699999999995,-192.44799999999987,-247.1840000000002,-303.06600000000026,-362.41300000000001,-423.64200000000028,-482.42399999999998,-541.6579999999999,0,0,0,0,0,0,0,0]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C129,4)+1)&\"-\"&MID(C129,3,2)+2),VALUE(LEFT(C129,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D129,4)+1)&\"-\"&MID(D129,3,2)+2),VALUE(LEFT(D129,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E129,4)+1)&\"-\"&MID(E129,3,2)+2),VALUE(LEFT(E129,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F129,4)+1)&\"-\"&MID(F129,3,2)+2),VALUE(LEFT(F129,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G129,4)+1)&\"-\"&MID(G129,3,2)+2),VALUE(LEFT(G129,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H129,4)+1)&\"-\"&MID(H129,3,2)+2),VALUE(LEFT(H129,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I129,4)+1)&\"-\"&MID(I129,3,2)+2),VALUE(LEFT(I129,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J129,4)+1)&\"-\"&MID(J129,3,2)+2),VALUE(LEFT(J129,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K129,4)+1)&\"-\"&MID(K129,3,2)+2),VALUE(LEFT(K129,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L129,4)+1)&\"-\"&MID(L129,3,2)+2),VALUE(LEFT(L129,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M129,4)+1)&\"-\"&MID(M129,3,2)+2),VALUE(LEFT(M129,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N129,4)+1)&\"-\"&MID(N129,3,2)+2),VALUE(LEFT(N129,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O129,4)+1)&\"-\"&MID(O129,3,2)+2),VALUE(LEFT(O129,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P129,4)+1)&\"-\"&MID(P129,3,2)+2),VALUE(LEFT(P129,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q129,4)+1)&\"-\"&MID(Q129,3,2)+2),VALUE(LEFT(Q129,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R129,4)+1)&\"-\"&MID(R129,3,2)+2),VALUE(LEFT(R129,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S129,4)+1)&\"-\"&MID(S129,3,2)+2),VALUE(LEFT(S129,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T129,4)+1)&\"-\"&MID(T129,3,2)+2),VALUE(LEFT(T129,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U129,4)+1)&\"-\"&MID(U129,3,2)+2),VALUE(LEFT(U129,4)+1))","v":"2043-44"}]
[null,"Export MWh","                                         -  ","                                         -  ",209081,585775,669460,716647,895396,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C130:C139)","v":0},{"$f":"-SUM(D130:D139)","v":0},{"$f":"-SUM(E130:E139)","v":-209081},{"$f":"-SUM(F130:F139)","v":-585775},{"$f":"-SUM(G130:G139)","v":-669460},{"$f":"-SUM(H130:H139)","v":-716647},{"$f":"-SUM(I130:I139)","v":-895396},{"$f":"-SUM(J130:J139)","v":0},{"$f":"-SUM(K130:K139)","v":0},{"$f":"-SUM(L130:L139)","v":0},{"$f":"-SUM(M130:M139)","v":0},{"$f":"-SUM(N130:N139)","v":0},{"$f":"-SUM(O130:O139)","v":0},{"$f":"-SUM(P130:P139)","v":0},{"$f":"-SUM(Q130:Q139)","v":0},{"$f":"-SUM(R130:R139)","v":0},{"$f":"-SUM(S130:S139)","v":0},{"$f":"-SUM(T130:T139)","v":0},{"$f":"-SUM(U130:U139)","v":0},{"$f":"-SUM(V130:V139)","v":0}]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,"FORECAST (MWh)"]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C144,4)+1)&\"-\"&MID(C144,3,2)+2),VALUE(LEFT(C144,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D144,4)+1)&\"-\"&MID(D144,3,2)+2),VALUE(LEFT(D144,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E144,4)+1)&\"-\"&MID(E144,3,2)+2),VALUE(LEFT(E144,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F144,4)+1)&\"-\"&MID(F144,3,2)+2),VALUE(LEFT(F144,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G144,4)+1)&\"-\"&MID(G144,3,2)+2),VALUE(LEFT(G144,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H144,4)+1)&\"-\"&MID(H144,3,2)+2),VALUE(LEFT(H144,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I144,4)+1)&\"-\"&MID(I144,3,2)+2),VALUE(LEFT(I144,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J144,4)+1)&\"-\"&MID(J144,3,2)+2),VALUE(LEFT(J144,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K144,4)+1)&\"-\"&MID(K144,3,2)+2),VALUE(LEFT(K144,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L144,4)+1)&\"-\"&MID(L144,3,2)+2),VALUE(LEFT(L144,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M144,4)+1)&\"-\"&MID(M144,3,2)+2),VALUE(LEFT(M144,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N144,4)+1)&\"-\"&MID(N144,3,2)+2),VALUE(LEFT(N144,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O144,4)+1)&\"-\"&MID(O144,3,2)+2),VALUE(LEFT(O144,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P144,4)+1)&\"-\"&MID(P144,3,2)+2),VALUE(LEFT(P144,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q144,4)+1)&\"-\"&MID(Q144,3,2)+2),VALUE(LEFT(Q144,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R144,4)+1)&\"-\"&MID(R144,3,2)+2),VALUE(LEFT(R144,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S144,4)+1)&\"-\"&MID(S144,3,2)+2),VALUE(LEFT(S144,4)+1))","v":"2041-42"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T144,4)+1)&\"-\"&MID(T144,3,2)+2),VALUE(LEFT(T144,4)+1))","v":"2042-43"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U144,4)+1)&\"-\"&MID(U144,3,2)+2),VALUE(LEFT(U144,4)+1))","v":"2043-44"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C145:C154)","v":0},{"$f":"-SUM(D145:D154)","v":0},{"$f":"-SUM(E145:E154)","v":0},{"$f":"-SUM(F145:F154)","v":0},{"$f":"-SUM(G145:G154)","v":0},{"$f":"-SUM(H145:H154)","v":0},{"$f":"-SUM(I145:I154)","v":0},{"$f":"-SUM(J145:J154)","v":0},{"$f":"-SUM(K145:K154)","v":0},{"$f":"-SUM(L145:L154)","v":0},{"$f":"-SUM(M145:M154)","v":0},{"$f":"-SUM(N145:N154)","v":0},{"$f":"-SUM(O145:O154)","v":0},{"$f":"-SUM(P145:P154)","v":0},{"$f":"-SUM(Q145:Q154)","v":0},{"$f":"-SUM(R145:R154)","v":0},{"$f":"-SUM(S145:S154)","v":0},{"$f":"-SUM(T145:T154)","v":0},{"$f":"-SUM(U145:U154)","v":0},{"$f":"-SUM(V145:V154)","v":0}]

{"sheet":"7.8 Export Services","index":28,"n_rows":57,"n_cols":9,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2026-27 TO 2030-31"}]
[null,"7.8 EXPORT SERVICES"]
[null," TEMPLATE DATE - SEPTEMBER 2024 - FINAL RIN"]
[]
[null,"Expenditure must only be related to DER integration, and must exclude amounts relating to DMIA"]
[]
[null,"Export service related overvoltage complaint management\nexamples include but not limited to: complaint processing, analysis, transformer tapping "]
[]
[null,"7.8.1 - OPEX FOR PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"Export service related overvoltage complaint management"]
[null,"Other opex",54068.301049233247,21627.3204196933,4025617.1447134786,4934446.3556093629,5440009.6916868445,5898489.9071284318,6551790.1043139193]
[]
[]
[null,"ICT capex\nexamples include but not limited to: establishing systems for network visibility, hosting capacity assessments, generation of dynamic operating envelopes"]
[null,"Network monitoring capex\nexamples include but not limited to: implementing transformer monitors"]
[]
[null,"7.8.2 - CAPEX FOR THE PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($, real June 2026)"}]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"ICT capex",6301455,156374,11451431.422409091,11517047.859357784,4418372.0134565514,10025240.323253378,3365297.3424500641]
[null,"Network monitoring capex"]
[null,"Other capex",6756397.0000000009,4710118,11286647.6532382,9143012.1125987563,1684587.810591958,25120394.861766525,1506738.6892594718]
[]
[]
[]
[]
[null,"7.8.3 - EXPORT VOLUMES - NET METERED VOLUME OF ENERGY EXPORTED"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"VOLUMES\nMWh"]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},78754.181100659553,80660.679583358971,87369.117035077841,366262.21356470109,446785.50849363155,491707.32048252801,540653.7532548192]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},57014.481398471806,63356.671986966554,79991.40350533434,181289.58839710339,195491.40782071269,208411.54742062755,318342.95942428836]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},44390.799633303228,52294.74016229964,58272.091674470124,65519.906731653449,68413.937515005877,73200.547322926664,97646.269170313404]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},{"$f":"SUM(C35:C38)","v":180159.46213243456},{"$f":"SUM(D35:D38)","v":196312.09173262515},225632.61221488228,613071.708693458,710690.85382935009,773319.4152260822,956642.98184942093]
[]
[]
[null,"7.8.4 EXPORT SERVICES - CUSTOMER NUMBERS"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"CUSTOMER NUMBERS"]
[null,null,{"$f":"CRCP_y4","v":"2024-25"},{"$f":"CRCP_y5","v":"2025-26"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"FRCP_y2","v":"2027-28"},{"$f":"FRCP_y3","v":"2028-29"},{"$f":"FRCP_y4","v":"2029-30"},{"$f":"FRCP_y5","v":"2030-31"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,{"$f":"C53","v":0},{"$f":"D53","v":0},0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},96690.025578418557,{"$f":"C54","v":107078.74019165183},115650.98039645453,122950.21170689368,128763.35175914642,133595.46904726417,138395.94043976467]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},90548.393285171958,100277.22943863372,108304.97141880222,115140.56447427253,120584.46097263745,125109.64807427605,129605.19938892346]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},41914.581136409462,46418.030369714448,50134.048184743253,53298.22381883378,55818.187268216134,57912.882878459772,59993.860171311841]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C57,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},107078.74019165183,115650.98039645453,122950.21170689368,128763.35175914642,133595.46904726417,138395.94043976467,142871.09202531978]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},100277.22943863372,108304.97141880222,115140.56447427253,120584.46097263745,125109.64807427605,129605.19938892346,133796.09481330164]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},46418.030369714448,50134.048184743253,53298.22381883378,55818.187268216134,57912.882878459772,59993.860171311841,61933.813161378559]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]

{"sheet":"AER Sheet Heading","index":29,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2022-23 to 2030-31"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2026)"}]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C15:C35)","v":0},{"$f":"SUM(D15:D35)","v":0},0,0,0,0,0]
[null,null,{"$f":"SUM(C15:C36)","v":0},{"$f":"SUM(D15:D36)","v":0},0,0,0,0,0]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C46:C66)","v":0},{"$f":"SUM(D46:D66)","v":0},{"$f":"SUM(E46:E66)","v":0},{"$f":"SUM(F46:F66)","v":0},{"$f":"SUM(G46:G66)","v":0},{"$f":"SUM(H46:H66)","v":0},{"$f":"SUM(I46:I66)","v":0}]
[null,null,{"$f":"SUM(C46:C67)","v":0},{"$f":"SUM(D46:D67)","v":0},{"$f":"SUM(E46:E67)","v":0},{"$f":"SUM(F46:F67)","v":0},{"$f":"SUM(G46:G67)","v":0},{"$f":"SUM(H46:H67)","v":0},{"$f":"SUM(I46:I67)","v":0}]

{"sheet":"AER CF","index":30,"n_rows":77,"n_cols":25,"rows_kept":77,"cut":false,"hidden":true,"merged":[[3,1,3,22],[39,38,39,59],[40,38,40,59],[41,38,41,59],[39,69,39,90],[40,69,40,90],[41,69,41,90]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[null,"CELLS FLAGED \"Y\" and greyed out will be greyed out in the worksheets."]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":true},"=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",null,null,"=INDEX(dms_CF_F10, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6.1","dms_CF_3.6.6.2","dms_CF_3.6.6.3","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.8 (set from dms_MAIFI_flag)","dms_CF_7.12","dms_CF_8.1_A  (and 8.4)","dms_CF_8.1_B  (and 8.4)","dms_CF_8.1_Neg  (and 8.4)","dms_CF_4.4.1","dms_CF_MAIFI_flag (set from dms_MAIFI_flag)","9.5 TUOS (set from Jurisdiction)","dms_CF_F10"]
[null,"Amadeus","NT","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"APA GasNet","Vic","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C7=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ausgrid (Tx Assets)","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C8=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C9=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","Y","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C10=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co.","NSW","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C13=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co. (Vic)","Vic","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C14=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C15=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C16=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C17=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C18=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Energex","Qld","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C19=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C20=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C21=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C22=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution (Tx Assets)","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C23=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C25=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"JGN","Vic","Gas","Distribution","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C26=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Power and Water","NT","Electricity","Distribution",null,"N","N",null,null,"N","Y","N","N","N","Y",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","Y","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C27=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C28=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C29=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Roma to Brisbane Pipeline","Qld","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","N","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C31=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C32=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C33=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C34=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"United Energy","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C35=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE","dms_H2"]
[null,"TOP HEADER","dms_H1"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,5.1109999999999998,"dms_NUM"]
[null,5.45E-2,"dms_NUM%"]
[null,5.5555000000000003,"dms_NUM3d"]
[null,"Text description","dms_Row_Locked"]
[null,"Text description - not locked","dms_Row1"]
[null,"Text description","dms_Row2"]
[null,"Total","dms_T1"]
[null,"Total","dms_T2"]
[null,"EXPENSES","dms_BH"]
[null,2019,"dms_BY1"]
[null,2019,"dms_BY2"]
[null,"VOLUMES","dms_GH"]
[null,2019,"dms_GY1"]
[null,2019,"dms_GY2"]

{"sheet":"AER NRs","index":31,"n_rows":232,"n_cols":16,"rows_kept":232,"cut":false,"hidden":true,"merged":[[4,1,28,1],[176,1,177,1],[179,1,184,1],[65,1,78,1],[135,1,150,1],[84,1,97,1],[152,1,158,1],[118,1,132,1],[208,1,213,1],[199,1,200,1],[32,1,55,1],[100,1,107,1],[110,1,115,1],[191,1,192,1],[195,1,196,1],[160,1,174,1],[33,67,33,88],[34,67,34,88],[35,67,35,88],[36,10,40,10],[44,10,45,10],[33,10,35,10],[33,36,33,57],[34,36,34,57],[35,36,35,57]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Tariff cap"]
[null,null,"Final decision","Weighted average price cap"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Reallocated"]
[null,null,"Recast"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[null,null,null,null,null,null,null,null,null,null,null,null,"GAS ARR & RESET"]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140201_UOM","dms_E050201_UOM","dms_E050202_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number per km","per metre per connection","metres per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","per service per connection","number per connection"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number per connection","number per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","dms_E020202_UOM","Spare"]
[null,null,"number","number","Length of mains replaced"]
[null,null,"number","number","Number of services replaced"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)",""]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"_xlfn.SINGLE(dms_060701_StartDateTxt)","v":"1-Jul-2019"}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]
[]
[]
[]
[null,"PTRM input sheet","DMS_50_01_01a","DMS_50_01_01aa","DMS_50_01_01b","DMS_50_01_01bb","DMS_50_01_01c","DMS_50_01_01d","DMS_50_01_01dd"]

{"sheet":"AER lookups","index":32,"n_rows":99,"n_cols":38,"rows_kept":99,"cut":false,"hidden":true,"merged":[[5,37,7,37],[17,1,17,4],[4,25,4,36],[5,25,5,28],[5,30,7,34],[5,35,7,35],[5,36,7,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Template number",5]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_UID_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_MAIFI_flag_List","dms_Public_Lighting_List","Name"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"EDDVIC100","Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic",8001,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"YES","YES",{"$f":"B10","v":"AusNet (D)"}]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"UID_123","Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"123 Straight Street",null,"MELBOURNE","Vic",3000,"PO Box 123",null,"MELBOURNE","Vic",3000,"NO","NO","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"YES","YES","Australian Distribution Co. (Vic)"]
[null,"CitiPower","CitiPower",76064651056,"EDDVIC200","Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"40 Market Street",null,"MELBOURNE","Vic",3000,"Locked Bag 14090",null,"MELBOURNE","Vic",8001,"YES","YES","NO","NO","NO","CBD","Urban","Short rural","Long rural",null,"YES","YES","CitiPower"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"EDDVIC300","Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"Level 16","567 Collins Street","MELBOURNE","Vic",3000,"PO Box 16182",null,"MELBOURNE","Vic",8001,"NO","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"YES","YES","Jemena Electricity"]
[null,"Powercor Australia","Powercor Australia",89064651109,"EDDVIC400","Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"40 Market Street",null,"MELBOURNE","Vic",3000,"Locked bag 14090",null,"MELBOURNE","Vic",8001,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"YES","YES","Powercor Australia"]
[null,"United Energy","United Energy",70064651029,"EDDVIC500","Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"43-45 Centreway",null,"MOUNT WAVERLEY","Vic",3149,"PO Box 449",null,"MOUNT WAVERLEY","Vic",3170,"NO","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"YES","YES","United Energy"]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"EBSS","Efficiency Benefit Sharing Scheme","EFFICIENCY BENEFIT SHARING SCHEME",5]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"Profitability","Profitability","PROFITABILITY",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"Reset_outputs","Reset Outputs","AER RESET DECISION OUTPUTS",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88","1988","PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2016-17"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2021-22"},{"$f":"FRCP_y1","v":"2026-27"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2026-27"}]
[null,"1988-89","1989","PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2017-18"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2022-23"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2027-28"}]
[null,"1989-90","1990","PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2018-19"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2023-24"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2028-29"}]
[null,"1990-91","1991","PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2019-20"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2024-25"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2029-30"}]
[null,"1991-92","1992","PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2020-21"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2025-26"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2030-31"}]
[null,"1992-93","1993","PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2021-22"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2026-27"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2031-32"}]
[null,"1993-94","1994","PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2022-23"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2027-28"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2032-33"}]
[null,"1994-95","1995","PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2023-24"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2028-29"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2033-34"}]
[null,"1995-96","1996","PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2024-25"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2029-30"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2034-35"}]
[null,"1996-97","1997","PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2025-26"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2030-31"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2035-36"}]
[null,"1997-98","1998","PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2026-27"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2031-32"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2036-37"}]
[null,"1998-99","1999","PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2027-28"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2032-33"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2037-38"}]
[null,"1999-00","2000","PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2028-29"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2033-34"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2038-39"}]
[null,"2000-01","2001","PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2029-30"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2034-35"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2039-40"}]
[null,"2001-02","2002","PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2030-31"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2035-36"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2040-41"}]
[null,"2002-03","2003","PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2031-32"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2036-37"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2041-42"}]
[null,"2003-04","2004","PRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+16)","v":"2032-33"},"CRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+16)","v":"2037-38"},"FRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+16)","v":"2042-43"}]
[null,"2004-05","2005","PRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+17)","v":"2033-34"},"CRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+17)","v":"2038-39"},"FRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+17)","v":"2043-44"}]
[null,"2005-06","2006","PRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+18)","v":"2034-35"},"CRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+18)","v":"2039-40"},"FRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+18)","v":"2044-45"}]
[null,"2006-07","2007","PRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+19)","v":"2035-36"},"CRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+19)","v":"2040-41"},"FRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+19)","v":"2045-46"}]
[null,"2007-08","2008","PRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+20)","v":"2036-37"},"CRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+20)","v":"2041-42"},"FRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+20)","v":"2046-47"}]
[null,"2008-09","2009","PRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+21)","v":"2037-38"},"CRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+21)","v":"2042-43"},"FRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+21)","v":"2047-48"}]
[null,"2009-10",2010,"PRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+22)","v":"2038-39"},"CRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+22)","v":"2043-44"},"FRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+22)","v":"2048-49"}]
[null,"2010-11",2011,"PRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+23)","v":"2039-40"},"CRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+23)","v":"2044-45"},"FRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+23)","v":"2049-50"}]
[null,"2011-12",2012,"PRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+24)","v":"2040-41"},"CRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+24)","v":"2045-46"},"FRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+24)","v":0}]
[null,"2012-13",2013]
[null,"2013-14",2014]
[null,"2014-15",2015]
[null,"2015-16",2016]
[null,"2016-17",2017]
[null,"2017-18",2018]
[null,"2018-19",2019]
[null,"2019-20",2020]
[null,"2020-21",2021]
[null,"2021-22",2022,null,"CRY - FRY"]
[null,"2022-23",2023,"dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2022-23"}]
[null,"2023-24",2024,"dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2023-24"}]
[null,"2024-25",2025,"dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2024-25"}]
[null,"2025-26",2026,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2025-26"}]
[null,"2026-27",2027,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2026-27"}]
[null,"2027-28",2028,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2027-28"}]
[null,"2028-29",2029,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2028-29"}]
[null,"2029-30",2030,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2029-30"}]
[null,"2030-31",2031,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2030-31"}]
[null,"2031-32",2032,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2031-32"}]
[null,"2032-33",2033,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2032-33"}]
[null,"2033-34",2034,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2033-34"}]
[null,"2034-35",2035,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2034-35"}]
[null,"2035-36",2036,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2035-36"}]
[null,"2036-37",2037,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2036-37"}]
[null,"2037-38",2038,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2037-38"}]
[null,"2038-39",2039,"dms_y17",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+16),0)","v":"2038-39"}]
[null,"2039-40",2040,"dms_y18",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+17),0)","v":"2039-40"}]
[null,"2040-41",2041,"dms_y19",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+18),0)","v":"2040-41"}]
[null,"2041-42",2042,"dms_y20",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+19),0)","v":"2041-42"}]
[null,"2042-43",2043,"dms_y21",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+20),0)","v":"2042-43"}]
[null,"2043-44",2044,"dms_y22",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+21),0)","v":"2043-44"}]
[null,"2044-45",2045,"dms_y23",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+22),0)","v":"2044-45"}]
[null,"2045-46",2046,"dms_y24",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+23),0)","v":"2045-46"}]
[null,"2046-47",2047,"dms_y25",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+24),0)","v":"2046-47"}]
[null,"2047-48",2048,"dms_y26",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+25),0)","v":"2047-48"}]
[null,"2048-49","2049"]
[null,"2049-50","2050"]

{"sheet":"AER ETL","index":33,"n_rows":147,"n_cols":10,"rows_kept":147,"cut":false,"hidden":true,"merged":[[12,0,16,0],[13,4,13,8],[15,2,15,4],[19,0,26,0],[27,0,32,0],[72,1,74,1],[33,68,33,89],[34,37,34,58],[34,68,34,89],[35,0,60,0],[35,37,35,58],[35,68,35,89],[33,37,33,58]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"AusNet (D)"}]
[null,"Unique ID",{"$f":"INDEX(dms_UID_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"EDDVIC100"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Final decision","dms_Source",{"$f":"IF(dms_Model=\"Reset\", \"Make sure you have set Reg Proposal as source\",\"\")","v":"Make sure you have set Reg Proposal as source"}]
[null,"Data quality","Consolidated","For DB purposes this is always Consoldiated"]
[null,"Data status","Public","For DB purposes this is always Public"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"2025-01-31"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality","Consolidated","dms_DataQuality","Always Consolidated"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)","v":"2031"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM",{"$f":"IF(dms_SingleYearModel=\"yes\",\"This is set to an historical template (EB, CA or ARR), apply UOM Named Range to cell !\",\"This is not an historical template, make sure UOM Named Range is not applied\")","v":"This is not an historical template, make sure UOM Named Range is not applied"},null,null,null,null,{"$f":"IFERROR(dms_dollar_nom_UOM, \"NR not applied\")","v":"NR not applied"}]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"2022-23"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"2022"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))","v":"June 2026"},"dms_DollarReal","=IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year","v":"June 2021"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2026-27"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2022-23"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":36},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":40},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":35},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":30},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":44},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2026-27"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2021-22"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2016-17"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2030-31"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2020-21"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2030-31"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2028-29"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2026"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2021"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":"2023"},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2031"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2031"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2026-27 to 2030-31"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_y1&\" to \"&FRCP_final_year,CRY))","v":"2022-23 to 2030-31"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"2022-23"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2030-31"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C51,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"2022-23"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":2},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(dms_SingleYearModel=\"yes\",(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(PRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(PRCP_y4,4))))","v":"1-Jul-2019"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060701_StartDateTxt)","v":43647},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"Does the NSP report MAIFI or MAIFIe","NO","dms_MAIFI_Flag"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?",{"$f":"IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")","v":"no"},"Must be present for ARRs","=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row",{"$f":"IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")","v":"0"},"dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2018"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":{"$error":"#NAME?"}},"dms_DeterminationRef"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]