{"text_format":"1","workbook":"xlsx","n_sheets":40,"sheets":["AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL","Instructions","CONTENTS","Business & other details","CPI series","2.1 Expenditure summary","2.2 Repex","2.3 Augex (a)","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","4.2 Metering","4.3 Fee-based services","4.4 Quoted services","5.4 MD & utilisation-Spatial","6.1 Telephone answering","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.7 TSS-LRMC","8.2 Capex"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":2,"defined_names":861,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AER Sheet Heading","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":true,"merged":[[10,2,10,8],[11,2,11,8],[41,2,41,8],[42,2,42,8]]}
[null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]

{"sheet":"AER CF","index":1,"n_rows":67,"n_cols":24,"rows_kept":67,"cut":false,"hidden":true,"merged":[[33,37,33,58],[33,68,33,89],[3,1,3,21],[31,37,31,58],[31,68,31,89],[32,37,32,58],[32,68,32,89]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.6.1","dms_CF_6.8","dms_CF_7.12","dms_CF_8.1_A","dms_CF_8.1_B","dms_CF_8.1_Neg","dms_CF_4.4.1","dms_CF_MAIFI_flag","Spare1","Spare2"]
[null,"ActewAGL Distribution","ACT","Electricity","Distribution",null,"Y",null,"Y","Y","N","Y","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","N","N","N","Y","Y","N","Y","Y","Y","N","N","N"]
[null,"Energex","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N","N","N"]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"Power and Water","NT","Electricity","Distribution",null,"N",null,"N","Y","N","N","Y","Y","Y","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","Y","N","Y","Y","Y","Y","N","N","N","N","N"]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"United Energy","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,null,"dms_NUM"]
[null,null,"dms_NUM%"]
[null,null,"dms_Row_Locked"]
[null,null,"dms_Row1"]
[null,null,"dms_Row2"]
[null,null,"dms_T1"]
[null,null,"dms_T2"]
[null,null,"dms_BH"]
[null,null,"dms_BY1"]
[null,null,"dms_BY2"]
[null,null,"dms_GH"]
[null,null,"dms_GY1"]
[null,null,"dms_GY2"]

{"sheet":"AER NRs","index":2,"n_rows":226,"n_cols":15,"rows_kept":226,"cut":false,"hidden":true,"merged":[[193,1,194,1],[197,1,198,1],[206,1,211,1],[133,1,148,1],[150,1,156,1],[158,1,172,1],[174,1,175,1],[177,1,182,1],[189,1,190,1],[116,1,130,1],[4,1,26,1],[30,1,53,1],[31,10,33,10],[31,36,31,57],[34,10,38,10],[42,10,43,10],[63,1,76,1],[82,1,95,1],[98,1,105,1],[108,1,113,1],[31,67,31,88],[32,36,32,57],[32,67,32,88],[33,36,33,57],[33,67,33,88]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Weighted average price cap"]
[null,null,"Final decision"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140102_UOM","dms_S140201_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number","number per km"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","number"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km","number"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","Spare","Spare"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)",""]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":"2015-01-01"}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]

{"sheet":"AER lookups","index":3,"n_rows":88,"n_cols":38,"rows_kept":88,"cut":false,"hidden":true,"merged":[[22,1,22,4],[6,25,6,36],[8,25,8,28],[8,31,8,35],[8,36,10,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Data in these columns used for data validation and database purposes."]
[null,"Date last modified:","2017-01-16","added (Albury and Victora) for AGN"]
[null,null,"2016-10-17","updated TransGrid's correct legal name, corrected TasNetworks (T) to June financial year"]
[null,null,"2017-02-01","inserted Power and Water, added NRs (dms_FeederCat_1 and dms_FeederCat_2)"]
[null,null,"2017-03-03","inserted AEMO as a business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,"2018-03-28","major changes to accommodate STPIS"]
[null,null,"Template Version",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","MAIFI flag","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_DeterminationRef_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_MAIFI_flag_List","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_Public_Lighting_List","Name"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic",8001,"NO","YES","YES","YES","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES",{"$f":"B13","v":"AusNet (D)"}]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"distribution determination","123 Straight Street",null,"MELBOURNE","Vic",3000,"PO Box 123",null,"MELBOURNE","Vic",3000,"NO","NO","NO","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co. (Vic)"]
[null,"CitiPower","CitiPower",76064651056,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked Bag 14090",null,"MELBOURNE","Vic",8001,"YES","YES","NO","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","CitiPower"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","Level 16","567 Collins Street","MELBOURNE","Vic",3000,"PO Box 16182",null,"MELBOURNE","Vic",8001,"NO","YES","YES","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","Jemena Electricity"]
[null,"Powercor Australia","Powercor Australia",89064651109,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked bag 14090",null,"MELBOURNE","Vic",8001,"NO","NO","YES","YES","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","Powercor Australia"]
[null,"United Energy","United Energy",70064651029,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","43-45 Centreway",null,"MOUNT WAVERLEY","Vic",3149,"PO Box 449",null,"MOUNT WAVERLEY","Vic",3170,"NO","NO","YES","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","United Energy"]
[]
[]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88","1988","PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2011-12"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2016-17"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2021-22"}]
[null,"1988-89","1989","PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2012-13"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2017-18"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2022-23"}]
[null,"1989-90","1990","PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2013-14"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2018-19"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2023-24"}]
[null,"1990-91","1991","PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2014-15"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2019-20"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2024-25"}]
[null,"1991-92","1992","PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2015-16"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2020-21"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2025-26"}]
[null,"1992-93","1993","PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2016-17"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2021-22"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2026-27"}]
[null,"1993-94","1994","PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2017-18"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2022-23"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2027-28"}]
[null,"1994-95","1995","PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2018-19"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2023-24"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2028-29"}]
[null,"1995-96","1996","PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2019-20"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2024-25"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2029-30"}]
[null,"1996-97","1997","PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2020-21"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2025-26"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2030-31"}]
[null,"1997-98","1998","PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2021-22"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2026-27"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2031-32"}]
[null,"1998-99","1999","PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2022-23"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2027-28"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2032-33"}]
[null,"1999-00","2000","PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2023-24"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2028-29"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2033-34"}]
[null,"2000-01","2001","PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2024-25"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2029-30"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2034-35"}]
[null,"2001-02","2002","PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2025-26"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2030-31"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2035-36"}]
[null,"2002-03","2003","PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2026-27"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2031-32"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2036-37"}]
[null,"2003-04","2004"]
[null,"2004-05","2005"]
[null,"2005-06","2006",null,"CRY - FRY"]
[null,"2006-07","2007","dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2019-20"}]
[null,"2007-08","2008","dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2020-21"}]
[null,"2008-09","2009","dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2021-22"}]
[null,"2009-10",2010,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2022-23"}]
[null,"2010-11",2011,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2023-24"}]
[null,"2011-12",2012,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2024-25"}]
[null,"2012-13",2013,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2025-26"}]
[null,"2013-14",2014,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2026-27"}]
[null,"2014-15",2015,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2027-28"}]
[null,"2015-16",2016,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2028-29"}]
[null,"2016-17",2017,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2029-30"}]
[null,"2017-18",2018,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2030-31"}]
[null,"2018-19",2019,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2031-32"}]
[null,"2019-20",2020,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2032-33"}]
[null,"2020-21",2021,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2033-34"}]
[null,"2021-22",2022,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2034-35"}]
[null,"2022-23",2023]
[null,"2023-24",2024]
[null,"2024-25",2025]
[null,"2025-26",2026]
[null,"2026-27",2027]
[null,"2027-28",2028]
[null,"2028-29",2029]
[null,"2029-30",2030]
[null,"2030-31",2031]
[null,"2031-32",2032]
[null,"2032-33",2033]
[null,"2033-34",2034]
[null,"2034-35",2035]
[null,"2035-36",2036]
[null,"2036-37","2037"]

{"sheet":"AER ETL","index":4,"n_rows":145,"n_cols":8,"rows_kept":145,"cut":false,"hidden":true,"merged":[[71,1,73,1],[32,68,32,89],[33,37,33,58],[33,68,33,89],[34,0,59,0],[34,37,34,58],[34,68,34,89],[32,37,32,58],[11,0,15,0],[12,4,12,8],[14,2,14,4],[18,0,25,0],[26,0,31,0]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"AusNet (D)"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Regulatory proposal","dms_Source"]
[null,"Data quality",{"$f":"dms_Selected_Quality","v":"Consolidated"},"dms_DQ_1"]
[null,"Data status",{"$f":"dms_Selected_Status","v":"Confidential"},"dms_DQ_2"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"2020-01-31"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality",{"$f":"dms_Selected_Quality","v":"Consolidated"},"dms_DataQuality","=IF(dms_DQ_2=\"Confidential\",\"Consolidated\",\"Public\")"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"dms_RYE_result","v":"2026"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM","If the cover sheet is attached to an ABC RIN apply the NAMED RANGE to the cell"]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"NO"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"CRY not present"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year)","v":"June 2021"},"dms_DollarReal","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_RYE,2)&RIGHT(dms_RYE,2))))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year)","v":"June 2016"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2021-22"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2019-20"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":33},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":35},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":30},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":25},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":39},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2021-22"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2016-17"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2011-12"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2020-21"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2015-16"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2017-18"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2021"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2016"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":0},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2026"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2026"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2021-22 to 2025-26"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","v":"2021-22 to 2025-26"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"not an ABC"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2025-26"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C50,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"CRY not present"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":2},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text","2015-01-01","dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",42005,"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes",null,"=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","0","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2013"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2016-20 Distribution Determination"},"dms_DeterminationRef"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]

{"sheet":"Instructions","index":5,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4],[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[26,2,26,4],[10,2,10,4],[12,1,14,1],[12,2,12,4],[13,2,13,3],[14,2,14,4],[16,2,16,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",dms_TradingNameFull,\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by AusNet Electricity Services Pty Ltd to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify confidential information\nin the confidential workbook. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selection as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return selection to NON-CONFIDENTIAL macro."]
[]
[null,"RESPONSES","\nPlease return two (2) files to the AER: \n\n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,"AMENDMENTS","\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]
[]
[null,"UNITS OF MEASURE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," \nPLEASE DO NOT ENTER TEXT into cells that are to contain numeric data."]
[]
[]
[null,"NAVIGATION","\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]

{"sheet":"CONTENTS","index":6,"n_rows":48,"n_cols":5,"rows_kept":48,"cut":false,"hidden":false,"merged":[[6,3,6,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[null,null,null,null,"CPI series"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (a)"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 Forecast price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[null,null,null,null,"4.2 Metering"]
[null,null,null,null,"4.3 Fee-based services"]
[null,null,null,null,"4.4 Quoted services"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.1 Telephone answering"]
[null,null,null,null,"6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[]
[null,null,null,"FINANCIAL","8.2 Capex"]

{"sheet":"Business & other details","index":7,"n_rows":74,"n_cols":81,"rows_kept":74,"cut":false,"hidden":false,"merged":[[69,25,71,34],[69,37,71,81],[73,25,73,34],[73,37,73,52],[63,25,63,34],[63,37,63,52],[65,25,65,34],[65,37,65,52],[67,25,67,34],[67,37,67,52],[53,25,53,34],[53,37,53,44],[55,25,55,34],[55,37,55,44],[61,25,61,34],[61,37,61,52],[50,37,50,44],[50,46,50,53],[50,55,50,62],[50,64,50,71],[50,73,50,80],[51,37,51,44],[51,46,51,53],[51,55,51,62],[51,64,51,71],[51,73,51,80],[49,25,49,34],[49,37,49,44],[49,46,49,53],[49,55,49,62],[49,64,49,71],[49,73,49,80],[46,37,46,44],[46,46,46,53],[46,55,46,62],[46,64,46,71],[46,73,46,80],[47,37,47,44],[47,46,47,53],[47,55,47,62],[47,64,47,71],[47,73,47,80],[45,25,45,34],[45,37,45,44],[45,46,45,53],[45,55,45,62],[45,64,45,71],[45,73,45,80],[42,37,42,44],[42,46,42,53],[42,55,42,62],[42,64,42,71],[42,73,42,80],[43,37,43,44],[43,46,43,53],[43,55,43,62],[43,64,43,71],[43,73,43,80],[33,21,33,35],[33,37,33,58],[33,60,33,66],[33,68,33,89],[41,25,41,34],[41,37,41,44],[41,46,41,53],[41,55,41,62],[41,64,41,71],[41,73,41,80],[31,21,31,35],[31,37,31,58],[31,60,31,66],[31,68,31,89],[32,21,32,35],[32,37,32,58],[32,60,32,66],[32,68,32,89],[25,21,25,35],[25,37,25,40],[25,49,25,51],[25,60,25,66],[25,68,25,71],[25,80,25,82],[24,21,24,35],[24,37,24,51],[24,60,24,66],[24,68,24,82],[16,21,16,35],[16,37,16,48],[22,21,22,35],[22,37,22,58],[22,60,22,66],[22,68,22,89],[0,7,2,15],[3,21,3,57],[6,21,6,75],[8,16,8,93],[15,21,15,35],[15,37,15,58],[23,21,23,35],[23,37,23,58],[23,60,23,66],[23,68,23,89]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AusNet (D)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":91064651118}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Level 32"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Level 32"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":"2 Southbank Boulevard"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":"2 Southbank Boulevard"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SOUTHBANK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SOUTHBANK"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},null,null,null,null,null,null,null,null,null,"Post code",null,3006,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},null,null,null,null,null,null,null,null,null,"Post code",null,3006]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Charlotte Eddy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,"Namrata Powale"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"03 9695 6309",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,"03 9695 6968"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"charlotte.eddy@ausnetservices.com.au",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,"namrata.powale@ausnetservices.com.au"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2021-22",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2030-31"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2034-35"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2035-36"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2020-21"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2030-31"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2011-12"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2012-13"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2013-14"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2014-15"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2015-16"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2020-21"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2025-26"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2017-18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2017-18"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Reporting"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Confidential"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"2020-01-31",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"CPI series","index":8,"n_rows":13,"n_cols":12,"rows_kept":13,"cut":false,"hidden":false,"merged":[[9,2,9,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"CPI SERIES"]
[]
[]
[]
[null,"NOMINATED CPI SERIES"]
[]
[null,"Name of CPI series","Actual / Forecast annual inflation"]
[]
[null,null,{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Series data",1.0232558139534831E-2,1.9337016574585641E-2,2.0776874435411097E-2,1.5929203539823078E-2,0.02,2.4500000000000001E-2,2.4500000000000001E-2,2.4500000000000001E-2,2.4500000000000001E-2,2.4500000000000001E-2]

{"sheet":"2.1 Expenditure summary","index":9,"n_rows":119,"n_cols":9,"rows_kept":119,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,7,8],[22,1,23,1],[22,2,22,3],[35,1,36,1],[35,2,35,8],[99,1,100,1],[99,2,99,8],[111,1,112,1],[111,2,111,8],[47,1,48,1],[47,2,47,8],[59,1,60,1],[59,2,59,8],[72,1,73,1],[72,2,72,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure",133914630.9154004,160792424.43609089,148475694.19769377,150722818.0612911,147984662.92283458,132012503.70489204,123609643.3338408]
[null,"Connections",102870322.24100851,105193995.13286962,106971646.23061639,105593271.36136366,104324989.29624884,105697030.47208519,107016530.21664727]
[null,"Augmentation Expenditure",125073930.47554509,104209177.0338901,43428451.772343919,41260902.571705468,39112979.575283088,44851875.409484647,47349535.067849144]
[null,"Non-network",84369506.16971983,61005466.648324244,55888624.266389839,39745938.037413381,44092777.780731678,38940567.454876393,45979809.186532825]
[null,"Public lighting",0,0,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",26676237.028954912,25606188.581280082,25081027.813311782,24655280.391756963,24655280.391756963,24655280.391756963,24655280.391756963]
[null,"Capitalised corporate overheads",5052559.5892935973,4849889.1924366541,4750422.1622389918,4669784.3190882141,4669784.3190882141,4669784.3190882141,4669784.3190882141]
[null,"capcons (included in the above)",68462514.291257992,70471995.830687955,72320594.377096742,70447447.43860355,68807592.119885251,69877527.723339319,70807211.973137051]
[null,"Total",{"$f":"SUM(C10:C17)","v":477957186.41992235},461657141.02489156,384595866.44259471,366647994.74261874,364840474.28594339,350827041.75218338,353280582.51571518]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"}]
[null,"Vegetation management",31189806.760730568,31189806.760730568]
[null,"Maintenance",30800552.26545481,30800552.26545481]
[null,"Emergency response",18217976.834046442,18217976.834046442,null," "]
[null,"Non-network",31985560.845507219,31985560.845507219]
[null,"Metering",7330810.7737233983,7330810.7737233983]
[null,"Network overheads",64060192.302748092,64060192.302748092]
[null,"Corporate overheads",20763454.791556746,20763454.791556746]
[null,"Total",{"$f":"SUM(C25:C31)","v":204348354.57376727},{"$f":"SUM(D25:D31)","v":204348354.57376727}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Connections",3378459.9167490196,2737575.7199020153,6021502.3069754681,5994607.0659371363,6080860.7260709964,6128821.0282291453,6202670.7123706872]
[null,"Metering",7949980.9359768517,15002757.864204407,12899261.903426304,11353353.561256366,10742742.634374902,11440223.656994503,12163563.174776629]
[null,"Public lighting",3156348.6402891725,5078133.4681722177,7000346.7280869102,6963654.9141876763,6701493.1702350955,5538750.8654166395,3738917.4987989259]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Network overheads",1252952.5759543246,2053403.7902760697,2199229.7979369434,2036077.9036444151,1956271.7693063386,1934553.7883432256,1870560.4212664852]
[null,"Corporate overheads",154056.93538675006,187153.69878996554,308569.29793107492,307056.93982888525,302515.6260402124,274845.60991743533,232005.85336128093]
[null,"Total",{"$f":"SUM(C38:C43)","v":15891799.00435612},25059024.541344676,28428910.034356702,26654750.384854481,25783883.926027544,25317194.948900945,24207717.660574008]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Metering",16554898.187668698,16588507.318503393,10995508.299065977,11256836.493501576,11385041.741312673,11346971.558551952,11404708.810775677]
[null,"Public lighting",8589233.2387688234,8326637.6155471932,7863349.7467969749,7733448.8846003013,7337143.5510646179,7237510.1244625803,7207299.587155167]
[null,"Fee and quoted",2385611.5110410214,2468434.6851211688,3035940.5826577786,7225132.6791684087,6780052.2605440132,3731255.6419243533,3235001.6042864057]
[null,"Network overheads",0,0,0,0,0,0,0]
[null,"Corporate overheads",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C50:C55)","v":27529742.937478542},27383579.619171754,21894798.628520727,26215418.057270288,25502237.552921306,22315737.324938886,21847010.002217252]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure",0,0,0,0,0,0,0]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Augmentation expenditure",0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0]
[null,"capcons (included in the above)",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C62:C67)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"}]
[null,"Vegetation management",0,0]
[null,"Maintenance",0,0]
[null,"Emergency response",0,0]
[null,"Non-network",0,0]
[null,"Metering",0,0]
[null,"Network overheads",0,0]
[null,"Corporate overheads",0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",{"$f":"SUM(C75:C95)","v":0},{"$f":"SUM(D75:D95)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure",0,0,0,0,0,0,0]
[null,"Connections",65435429.196657516,67530800.030283228,68994861.128409073,67343581.488704428,65825088.154600084,66776173.285481147,67626670.22237587]
[null,"Augmentation Expenditure",0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",2545045.7659000969,2472833.6616157023,2796136.56655491,2609599.8780486328,2507563.8283736804,2607488.3044106062,2674065.6648476538]
[null,"Capitalised corporate overheads",482039.3287003783,468362.13878902898,529596.68213275587,494266.07185048587,474940.13691148983,493866.13344756461,506476.08591353428]
[null,"Total",{"$f":"SUM(C102:C107)","v":68462514.291257992},70471995.830687955,72320594.377096727,70447447.438603535,68807592.119885266,69877527.723339304,70807211.973137066]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure",11610167.595990155,13265250.686627032,15867850.254920095,15928544.818464365,16072452.532390706,14972316.010866061,14373683.723714823]
[null,"Connections",6343433.9859455554,5961310.5642133486,6637496.6344098495,6396768.7942489646,6365338.3828328876,6626577.3682721592,6806185.4712800849]
[null,"Augmentation Expenditure",10951622.651712455,8508707.6523327008,4641272.5884212554,4360495.2741557853,4248017.9716455126,5086915.5077308882,5505939.6918742023]
[null,"Non-network",2823572.3846003385,2720808.8705436443,2684830.4977995693,2639255.8239760664,2639255.823976066,2639255.823976066,2639255.8239760655]
[null,"capcons (included in the above)",3027085.0946004749,2941195.8004047312,3325733.2486876659,3103865.9498991184,2982503.9652851699,3101354.4378581708,3180541.7507611881]
[null,"Total",{"$f":"SUM(C114:C117)","v":31728796.618248504},30456077.773716725,29831449.975550767,29325064.71084518,29325064.710845172,29325064.710845176,29325064.710845176]

{"sheet":"2.2 Repex","index":10,"n_rows":524,"n_cols":11,"rows_kept":524,"cut":false,"hidden":false,"merged":[[9,4,9,10],[11,1,30,1],[31,1,37,1],[38,1,43,1],[44,1,52,1],[53,1,60,1],[61,1,76,1],[77,1,105,1],[106,1,119,1],[120,1,128,1],[129,1,136,1],[182,4,182,10],[184,1,203,1],[204,1,210,1],[211,1,216,1],[217,1,225,1],[226,1,233,1],[234,1,249,1],[250,1,278,1],[279,1,292,1],[293,1,301,1],[302,1,309,1],[355,4,355,10],[357,1,376,1],[452,1,465,1],[466,1,474,1],[475,1,482,1],[377,1,383,1],[384,1,389,1],[390,1,398,1],[399,1,406,1],[407,1,422,1],[423,1,451,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.2 REPEX"]
[]
[null,"There are THREE sub-tables on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($0's, real June 2021)"}]
[null,"ASSET GROUP","ASSET CATEGORY","UNITS",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,1639492.0500096737,1903214.075777682,2010746,2219938,2133532,2083080,2233684]
[null,null,"˂ = 1 kV; Wood",null,1296180.1418259833,1504678.4097868407,1589693,1747602,1501801,1105983,1066037]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,10120351.998374021,11748270.676284511,12412050,12590440,12964740,11890720,10789400]
[null,null,"> 22 kV & < = 66 kV; Wood",null,2232723.9514320004,2591870.84906345,2738312,2589321,3077239,2843341,2440327]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,6480899.0783997793,7523390.1558914464,7948463,8738010,7509005,5529914,5330183]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,10120351.998374021,11748270.676284511,12412050,12590440,12964740,11890720,10789400]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,744241.58893235645,863957.26519494283,912771,863107,1025746,947781,813442]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,7596757.1585034514,8818740.6302112434,9317001,9383520,9454022,9516618,9575428]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,3183789.4129078579,3695920.8340915372,3904741,3932619,3962166,3988400,4013047]
[null,null,"> 22 kV & < = 66 kV",null,151895.98933948006,176329.36064762826,186292,187623,189032,190284,191460]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",737771.66711387376,856446.61805637053,904836,998972,960090,937386,1005158]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",885325.83746363467,1027735.7523633688,1085803,1198767,1152107,1124863,1206189]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",16394.545432165232,19031.705357942701,20107,22199,21335,20831,22337]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",112183.63367858547,130229.03690671221,137587,138569,139610,140535,141403]
[null,null,"> 1 kV & < = 11 kV","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",2243671.0428415723,2604578.8450914868,2751738,2771384,2792206,2810694,2828063]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",2804588.3958694311,3255723.0831036693,3439672,3464230,3490258,3513368,3535079]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",6057911.3264532043,7032362.3138341876,7429692,7482737,7538957,7588874,7635771]
[null,null,"> 22 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",1509965.6013242672,1752852.5291498059,1851889,2826513,5027156,9996573,21233280]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV","per km",2337544.8385421047,2713552.7979221079,2866869,3813465,4665427,4641067,4669747]
[null,null,"> 22 kV & < = 33 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",576676.72907166893,669438.6032162566,707262,712312,717663,722415,726880]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",64075.46390743048,74382.382531154668,78585,79146,79740,80268,80764]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,912083.67291633121,1058797.7444423267,1118620,1126606,1135071,1142586,1149647]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,174654.45913122402,202748.6653649355,214204,215733,217354,218793,220145]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,77624.385250559222,90110.728278055452,95202,95881,96602,97241,97842]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,172007.78411889952,199676.25697025296,210958,212465,214061,215478,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,57335.656251277018,66558.436816291476,70319,70821,71354,71826,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,57335.656251277018,66558.436816291476,70319,70821,71354,71826,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,402330.5685324535,467047.82810144435,0,0,1088676,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,1501175.1505208567,1742648.0821679598,1841108,1594919,1526833,633563,199222]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,2916969.3478945913,3386181.178183984,3577501,3696528,3811709,3918110,3976290]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,88209.454569720168,102398.46881402859,108184,108956,164662,165752,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,3746152.4082021532,4348743.2545078397,4594448,6333326,6194082,4127209,464852]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,4626310.4618616858,5370479.9543741345,5673913,5714422,5757357,5795477,5720107]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,388314.76009149448,450777.49369629769,476246.5,519917,449198.25,464570.75,545960.25]
[null,null,"Poles / Columns ; Minor Road",null,1164944.2802744834,1352332.4810888933,1428739.5,1559751,1347594.75,1393712.25,1637880.75]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,6562534.2444222495,7618156.8228304517,8048584,9568398,9480150,7736161,2305227]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,12106736.224583136,14054176.593426125,14848240,9481289,8807600,8395914,8419833]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"OTHER BY: \nenter DNSP defined asset group here","Insulators",null,406626.63648221822,472034.944075835,498705,502266,506040,509390,512538]
[null,null,"Site Repairs",null,3727812.4017165662,4327453.1491407426,4571955,7651160,7375025,3659775,1856325]
[null,null,"Switchboards",null,5289146.0023558186,6139936.5251374375,6486844,9569513,9160997,3801378,1195334]
[null,null,"Voltage Transformers",null,893914.89309512766,1037706.40856472,1096337,1713477,1659626,917799,166019]
[null,null,"Current Transformers",null,458797.77038966806,532598.11448056786,562690,477195,467435,319967,33204]
[null,null,"Capacitor Banks",null,260032.96618314052,301860.81195273559,318916,443055,433039,285343,33204]
[null,null,"NER's",null,72900.160043717566,84626.583410898733,89408,90046,199591,54794,0]
[null,null,"Surge Arrestors",null,839692.30067535257,974761.7903716258,1029836,1037188,722902,727688,732185]
[null,null,"Pole Top Capacitior",null,55218.968533472231,64101.267317648257,67723,68207,68719,69174,0]
[null,null,"Electrical Earths",null,159606.08142713882,185279.66680293271,195748,197145,198626,199942,201177]
[null,null,"Line Voltage Regulator",null,1190825.1905960168,1382376.4894252506,1460481,1470908,1481959,1491772,0]
[null,null,"Low Conductor",null,680445.79524341866,789899.53949662123,834529,840488,846803,852409,857677]
[null,null,"REFCL",null,20669387.673668556,29331011.249774773,10968320,4942519,0,0,0]
[null,null,"Top Down Adjustment",null,0,0,-888189,-894530,-901251,-907218,-912824]
[null,null,"Support",null,4982205.0837823432,5783622.338278329,6110398,6113380,6098462,6101438,6104416]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,1948.7,1948.7,1860.5,2039.5,1945.5,1887,2011]
[null,null,"˂ = 1 kV; Wood",null,737.375,737.375,792.125,817.375,791.5,673.375,612.5]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,884.85,884.85,950.55,980.84999999999991,949.8,808.05,735]
[null,null,"> 22 kV & < = 66 kV; Wood",null,17.696999999999999,17.696999999999999,19.011000000000003,19.617000000000001,18.996000000000002,16.161000000000001,14.700000000000001]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,265.45499999999998,265.45499999999998,285.16499999999996,294.255,284.94,242.41499999999999,220.5]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,884.85,884.85,950.55,980.84999999999991,949.8,808.05,735]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,159.273,159.273,171.09900000000002,176.553,170.964,145.44900000000001,132.30000000000001]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,4880,3732,2980,2980,2980,2980,2980]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,2045,1564,1114,1114,1114,1114,1114]
[null,null,"> 22 kV & < = 66 kV",null,98,75,41,41,41,41,41]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,876.21402877697835,876.21402877697835,836.55575539568349,917.04136690647488,874.77517985611507,848.47122302158266,904.22661870503589]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,1051.4568345323742,1051.4568345323742,1003.8669064748201,1100.4496402877699,1049.730215827338,1018.1654676258993,1085.0719424460431]
[null,null,"> 22 kV & < = 66 kV",null,21.02913669064748,21.02913669064748,20.0773381294964,22.008992805755391,20.994604316546759,20.363309352517984,21.701438848920862]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",null,3,3,4,4,4,4,4]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,40,45,51.4,51.4,51.4,51.4,51.4]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,45,53,59.969565217391306,59.969565217391306,59.969565217391306,59.969565217391306,59.969565217391306]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,110,130,152.23043478260871,152.23043478260871,152.23043478260871,152.23043478260871,152.23043478260871]
[null,null,"> 22 kV & < = 66 kV",null,0.2,0.2,0.2,0.2,0.2,0.2,0.2]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,1.6,4.3059375000000006,7.0633593750000001,13.267558593750001,27.227006835937502,58.635765380859382]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV",null,0,0,2.1907766990291266,2.7067961165048544,3.1228155339805825,3.0728155339805827,3.0728155339805827]
[null,null,"> 22 kV & < = 33 kV",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,">  132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0.45922330097087383,0.79320388349514581,1.1271844660194177,1.1271844660194177,1.1271844660194177]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",null,3955.5,3711.9375,817.2,817.2,817.2,817.2,817.2]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,439.5,412.4375,90.8,90.8,90.8,90.8,90.8]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,94,94,94,94,94,94,94]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,18,18,18,18,18,18,18]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,8,8,8,8,8,8,8]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,3,3,3,3,3,3,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,1,1,1,1,1,1,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,1,1,1,1,1,1,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,2,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0,0,1,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,311,284,274,281,287.5,293.5,296]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,2,2,2,3,3,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,5.3,4,4,4,4,4,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,1837,1837,1837,1837,1837,1837,1836]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,83.375,90.375,77.5,79.625,93]
[null,null,"Poles / Columns ; Minor Road",null,0,0,250.125,271.125,232.5,238.875,279]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,21,21,24.8,24.8,24.8,24.8,6.2]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,50,50,50,50,50,50,50]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},"Insulators",null,null,118.2,236.4,236.4,236.4,236.4,236.4]
[null,null,"Site Repairs",null,10,10,10,10,10,10,10]
[null,null,"Switchboards",null,0,1,1,0,0,0,0]
[null,null,"Voltage Transformers",null,6,2,2,2,2,2,0]
[null,null,"Current Transformers",null,2,2,2,1,1,1,0]
[null,null,"Capacitor Banks",null,2,2,2,2,2,2,0]
[null,null,"NER's",null,0,1,1,1,3,1,0]
[null,null,"Surge Arrestors",null,2761,1611,433,433,406,406,406]
[null,null,"Pole Top Capacitior",null,0,2,2,2,2,2,0]
[null,null,"Electrical Earths",null,101,101,101,101,101,101,101]
[null,null,"Line Voltage Regulator",null,3,3,3,3,3,3,0]
[null,null,"Low Conductor",null,203,203,203,203,203,203,203]
[null,null,"REFCL",null,3,2,2,1,1,0,0]
[null,null,"Top Down Adjustment",null,0,20,41,41,41,41,41]
[null,null,"Support",null,0,0,0,0,0,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C158),\"\",C158)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C178),\"\",C178)","v":""}]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,2707.2712989873571,2707.2712989873571,2707.2712989873571,2707.2712989873571,2707.2712989873571,2707.2712989873571,2707.2712989873571]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0.36720186250280162,0.36720186250280162,0.36720186250280162,0.36720186250280162,0.36720186250280162,0.36720186250280162,0.36720186250280162]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,2946.8854508221616,2946.8854508221616,2946.8854508221616,2946.8854508221616,2946.8854508221616,2946.8854508221616,2946.8854508221616]
[null,null,"> 22 kV & < = 66 kV; Wood",null,75.128947653948742,75.128947653948742,75.128947653948742,75.128947653948742,75.128947653948742,75.128947653948742,75.128947653948742]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,782.57922425106017,782.57922425106017,782.57922425106017,782.57922425106017,782.57922425106017,782.57922425106017,782.57922425106017]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0.12158188758453964,0.12158188758453964,0.12158188758453964,0.12158188758453964,0.12158188758453964,0.12158188758453964,0.12158188758453964]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,3061.6065602691278,3061.6065602691278,3061.6065602691278,3061.6065602691278,3061.6065602691278,3061.6065602691278,3061.6065602691278]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,384.72472825531833,384.72472825531833,384.72472825531833,384.72472825531833,384.72472825531833,384.72472825531833,384.72472825531833]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0.20386457918215728,0.20386457918215728,0.20386457918215728,0.20386457918215728,0.20386457918215728,0.20386457918215728,0.20386457918215728]
[null,null,"> 1 kV & < = 11 kV; Steel",null,1.2280998745913098E-3,1.2280998745913098E-3,1.2280998745913098E-3,1.2280998745913098E-3,1.2280998745913098E-3,1.2280998745913098E-3,1.2280998745913098E-3]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,3.0088446927487088E-2,3.0088446927487088E-2,3.0088446927487088E-2,3.0088446927487088E-2,3.0088446927487088E-2,3.0088446927487088E-2,3.0088446927487088E-2]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,4.5910901642623747,4.5910901642623747,4.5910901642623747,4.5910901642623747,4.5910901642623747,4.5910901642623747,4.5910901642623747]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,11423.36295225018,11423.36295225018,11423.36295225018,11423.36295225018,11423.36295225018,11423.36295225018,11423.36295225018]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,5563.5838810478017,5563.5838810478017,5563.5838810478017,5563.5838810478017,5563.5838810478017,5563.5838810478017,5563.5838810478017]
[null,null,"> 22 kV & < = 66 kV",null,97.713877164396081,97.713877164396081,97.713877164396081,97.713877164396081,97.713877164396081,97.713877164396081,97.713877164396081]
[null,null,"> 66 kV & < = 132 kV",null,3.0535586613873775,3.0535586613873775,3.0535586613873775,3.0535586613873775,3.0535586613873775,3.0535586613873775,3.0535586613873775]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,7120.8987983553643,7120.8987983553643,7120.8987983553643,7120.8987983553643,7120.8987983553643,7120.8987983553643,7120.8987983553643]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",null,243.72558736042444,243.72558736042444,243.72558736042444,243.72558736042444,243.72558736042444,243.72558736042444,243.72558736042444]
[null,null,"> 1 kV & < = 11 kV",null,0.71081086204347366,0.71081086204347366,0.71081086204347366,0.71081086204347366,0.71081086204347366,0.71081086204347366,0.71081086204347366]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,1761.084756824265,1761.084756824265,1761.084756824265,1761.084756824265,1761.084756824265,1761.084756824265,1761.084756824265]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,3737.2149545365078,3737.2149545365078,3737.2149545365078,3737.2149545365078,3737.2149545365078,3737.2149545365078,3737.2149545365078]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,9426.6288152065626,9426.6288152065626,9426.6288152065626,9426.6288152065626,9426.6288152065626,9426.6288152065626,9426.6288152065626]
[null,null,"> 22 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,">  132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",null,8031.6851454536591,8031.6851454536591,8031.6851454536591,8031.6851454536591,8031.6851454536591,8031.6851454536591,8031.6851454536591]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,897.58547816628129,897.58547816628129,897.58547816628129,897.58547816628129,897.58547816628129,897.58547816628129,897.58547816628129]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,2977.7675495513236,2977.7675495513236,2977.7675495513236,2977.7675495513236,2977.7675495513236,2977.7675495513236,2977.7675495513236]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,3.2130968130195448,3.2130968130195448,3.2130968130195448,3.2130968130195448,3.2130968130195448,3.2130968130195448,3.2130968130195448]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,559.38394943597814,559.38394943597814,559.38394943597814,559.38394943597814,559.38394943597814,559.38394943597814,559.38394943597814]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,229.79987547176063,229.79987547176063,229.79987547176063,229.79987547176063,229.79987547176063,229.79987547176063,229.79987547176063]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,69.933303663381082,69.933303663381082,69.933303663381082,69.933303663381082,69.933303663381082,69.933303663381082,69.933303663381082]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,24.191012464387281,24.191012464387281,24.191012464387281,24.191012464387281,24.191012464387281,24.191012464387281,24.191012464387281]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,37.386110172234886,37.386110172234886,37.386110172234886,37.386110172234886,37.386110172234886,37.386110172234886,37.386110172234886]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,4.3983659026158684,4.3983659026158684,4.3983659026158684,4.3983659026158684,4.3983659026158684,4.3983659026158684,4.3983659026158684]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,8.7967318052317367,8.7967318052317367,8.7967318052317367,8.7967318052317367,8.7967318052317367,8.7967318052317367,8.7967318052317367]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,17.473043579818217,17.473043579818217,17.473043579818217,17.473043579818217,17.473043579818217,17.473043579818217,17.473043579818217]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,3.3196856654793874,3.3196856654793874,3.3196856654793874,3.3196856654793874,3.3196856654793874,3.3196856654793874,3.3196856654793874]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,17,17,17,17,17,17,17]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,4.6828220950016881,4.6828220950016881,4.6828220950016881,4.6828220950016881,4.6828220950016881,4.6828220950016881,4.6828220950016881]
[null,null,"˂ = 11 kV  ; Switch",null,0.43964865046141605,0.43964865046141605,0.43964865046141605,0.43964865046141605,0.43964865046141605,0.43964865046141605,0.43964865046141605]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0.22385456812651849,0.22385456812651849,0.22385456812651849,0.22385456812651849,0.22385456812651849,0.22385456812651849,0.22385456812651849]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,1016.8679992327842,1016.8679992327842,1016.8679992327842,1016.8679992327842,1016.8679992327842,1016.8679992327842,1016.8679992327842]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,7.382336694730169,7.382336694730169,7.382336694730169,7.382336694730169,7.382336694730169,7.382336694730169,7.382336694730169]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,1.8010626263192466,1.8010626263192466,1.8010626263192466,1.8010626263192466,1.8010626263192466,1.8010626263192466,1.8010626263192466]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,470,470,470,470,470,470,470]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,0,0,0,0,0,0,0]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,0,0,0,0,0,0,0]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},"Insulators",null,0,0,0,0,0,0,0]
[null,null,"Site Repairs",null,0,0,0,0,0,0,0]
[null,null,"Switchboards",null,0,0,0,0,0,0,0]
[null,null,"Voltage Transformers",null,0,0,0,0,0,0,0]
[null,null,"Current Transformers",null,0,0,0,0,0,0,0]
[null,null,"Capacitor Banks",null,0,0,0,0,0,0,0]
[null,null,"NER's",null,0,0,0,0,0,0,0]
[null,null,"Surge Arrestors",null,0,0,0,0,0,0,0]
[null,null,"Pole Top Capacitior",null,0,0,0,0,0,0,0]
[null,null,"Electrical Earths",null,0,0,0,0,0,0,0]
[null,null,"Line Voltage Regulator",null,0,0,0,0,0,0,0]
[null,null,"Low Conductor",null,0,0,0,0,0,0,0]
[null,null,"REFCL",null,0,0,0,0,0,0,0]
[null,null,"Top Down Adjustment",null,0,0,0,0,0,0,0]
[null,null,"Support",null,0,0,0,0,0,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C158),\"\",C158)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C178),\"\",C178)","v":""}]

{"sheet":"2.3 Augex (a)","index":11,"n_rows":150,"n_cols":32,"rows_kept":150,"cut":false,"hidden":false,"merged":[[5,1,5,3],[9,11,9,22],[9,23,9,24],[9,25,11,25],[9,26,11,26],[9,27,9,28],[10,11,10,13],[10,14,10,16],[10,17,10,19],[10,21,10,22],[9,29,10,29],[9,30,9,31],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,6,11,6],[10,7,10,8],[10,9,10,10],[11,14,11,15],[11,17,11,18],[11,23,11,24],[11,27,11,29],[11,30,11,31],[9,1,9,10],[12,14,12,15],[12,17,12,18],[13,14,13,15],[13,17,13,18],[14,14,14,15],[14,17,14,18],[15,14,15,15],[15,17,15,18],[16,14,16,15],[16,17,16,18],[17,14,17,15],[17,17,17,18],[18,14,18,15],[18,17,18,18],[19,14,19,15],[19,17,19,18],[20,14,20,15],[20,17,20,18],[21,14,21,15],[21,17,21,18],[22,14,22,15],[22,17,22,18],[23,14,23,15],[23,17,23,18],[24,14,24,15],[24,17,24,18],[25,14,25,15],[25,17,25,18],[26,14,26,15],[26,17,26,18],[27,14,27,15],[27,17,27,18],[28,14,28,15],[28,17,28,18],[29,14,29,15],[29,17,29,18],[30,14,30,15],[30,17,30,18],[31,14,31,15],[31,17,31,18],[32,14,32,15],[32,17,32,18],[33,14,33,15],[33,17,33,18],[34,14,34,15],[34,17,34,18],[35,14,35,15],[35,17,35,18],[36,14,36,15],[36,17,36,18],[37,14,37,15],[37,17,37,18],[38,14,38,15],[38,17,38,18],[39,14,39,15],[39,17,39,18],[60,14,60,15],[60,17,60,18],[61,14,61,15],[61,17,61,18],[62,14,62,15],[62,17,62,18],[63,14,63,15],[63,17,63,18],[64,14,64,15],[64,17,64,18],[65,14,65,15],[65,17,65,18],[66,14,66,15],[66,17,66,18],[67,14,67,15],[67,17,67,18],[68,14,68,15],[68,17,68,18],[69,14,69,15],[69,17,69,18],[70,14,70,15],[70,17,70,18],[71,14,71,15],[71,17,71,18],[72,14,72,15],[72,17,72,18],[73,14,73,15],[73,17,73,18],[74,14,74,15],[74,17,74,18],[75,14,75,15],[75,17,75,18],[80,14,80,15],[80,17,80,18],[81,14,81,15],[81,17,81,18],[82,14,82,15],[82,17,82,18],[83,14,83,15],[83,17,83,18],[84,14,84,15],[84,17,84,18],[85,14,85,15],[85,17,85,18],[86,14,86,15],[86,17,86,18],[87,14,87,15],[87,17,87,18],[92,1,92,10],[92,11,92,22],[92,23,92,24],[92,25,94,25],[92,26,94,26],[92,27,92,28],[93,17,93,19],[93,21,93,22],[94,7,94,10],[94,23,94,24],[92,29,93,29],[92,30,92,31],[93,1,94,1],[93,3,94,3],[93,4,94,4],[93,5,94,5],[93,6,94,6],[93,7,93,10],[93,11,93,13],[93,14,93,16],[94,27,94,29],[94,30,94,31],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[147,1,147,2],[148,1,148,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are TWO tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation.  Both ROWS and COLUMNS have been grouped. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"2.3.1 - AUGEX ASSET DATA - SUBTRANSMISSION SUBSTATIONS, SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON-RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"SUBSTATION ID","SUBSTATION TYPE\n(drop down)","PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)","SUBSTATION RATING\nNORMAL CYCLIC\n(MVA)",null,"SUBSTATION RATING\nN-1 EMERGENCY\n(MVA)",null,"TRANSFORMERS",null,null,"SWITCHGEAR",null,null,"CAPACITORS",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"PRE","POST","PRE","POST","UNITS ADDED ","MVA ADDED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"UNITS ADDED ",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"MVAR ADDED",null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"}]
[null,"CLN 3rd 20/33MVA Transformer (RIT-D?)","Zone substation","Clyde North Augmentation","Substation upgrade - capacity","Demand growth",66,87,131,44,87,1,33,1423966.02,1,null,2287263.33,null,null,null,0,null,928717.05,372674.2,2973954,{"$f":"IF(SUM(N13,Q13,T13,U13,W13,X13,Y13)<>0,SUM(N13,Q13,T13,U13,W13,X13,Y13),\"\")","v":7986574.6000000006},"2021, 2022, 2023, 2024"]
[null,"KMS","Zone substation","REFCL Driven Augmentation","Substation upgrade - capacity","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,1236216,null,320497,61383,408727,{"$f":"IF(SUM(N14,Q14,T14,U14,W14,X14,Y14)<>0,SUM(N14,Q14,T14,U14,W14,X14,Y14),\"\")","v":2026823},"2022, 2023, 2024, 2025, 2026"]
[null,"WGI","Zone substation","REFCL Driven Augmentation","Substation upgrade - capacity","Safety",66,null,null,null,null,2,2,276291,null,null,null,null,null,null,4250023,null,1123412,191733,1475537,{"$f":"IF(SUM(N15,Q15,T15,U15,W15,X15,Y15)<>0,SUM(N15,Q15,T15,U15,W15,X15,Y15),\"\")","v":7316996},"2022, 2023, 2024, 2025, 2026"]
[null,"RWN","Zone substation","REFCL Driven Augmentation","Substation upgrade - capacity","Safety",66,null,null,null,null,2,1.5,276290,null,null,null,6,null,604574,2488332,null,847362,179352,1046370.0104172337,5442280.0104172342,"2022, 2023, 2024, 2025, 2026"]
[null,"BGE","Zone substation","REFCL Driven Augmentation","Substation upgrade - capacity","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,1040410,null,93637,null,208082,1342129,"2022, 2023, 2024, 2025, 2026"]
[null,"WOTS","Zone substation","REFCL Driven Augmentation","New substation establishment","Safety",66,null,null,null,null,2,40,2315305.2373489202,3,null,1627224.1315341603,6,null,215849.50350433664,13175111.8579983,null,1454118.8727602367,2936744.3594614416,8710756.6724310983,30435110.635038495,"2022, 2023, 2024, 2025, 2026"]
[null,"ELM","Zone substation","REFCL Driven Augmentation","New substation establishment","Safety",66,null,null,null,null,2,40,2315378.192613441,3,null,1627275.4053640794,6,null,215856.30492186503,7308258,null,984783.17981688376,2936836.8962717587,6974319.5531213768,22362707.532109402,"2022, 2023, 2024, 2025, 2026"]
[null,"LDL","Zone substation","REFCL Driven Augmentation","Substation upgrade - capacity","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,1535473,null,132435,null,230321,1898229,"2022, 2023, 2024, 2025, 2026"]
[null,"BDL","Zone substation","REFCL Driven Augmentation","New substation establishment","Safety",66,null,null,null,null,2,40,2315300.7779537789,3,null,1465261.6362333819,6,null,215849.08776726158,9486184.2215776704,null,1146047.1131229706,2936738.7031430798,6452481.4602018567,24017862.999999996,"2022, 2023, 2024, 2025, 2026"]
[null,"WGI","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,4175839.2554303636,null,2160173.1191390781,null,4320738.979670763,10656751.354240205,"2021, 2022"]
[null,"SMR","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,6954079.7669907883,null,5049192.8608166287,null,5253610.735742934,17256883.36355035,"2021, 2022"]
[null,"WN","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,10951116.246873081,null,2190710.0566940634,null,4422639.7513276292,17564466.054894775,"2021, 2022"]
[null,"MYT","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,3279462.9486486972,null,1270354.615840774,null,2885985.8075642963,7435803.3720537666,"2021, 2022"]
[null,"KLK","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,7070996.4291722802,null,5309890.5620500082,null,8257925.487651539,20638812.478873827,"2021, 2022"]
[null,"KMS","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,2260116.2615938243,null,1314007.3521569851,null,3221092.4330579988,6795216.0468088081,"2021, 2022"]
[null,"RUBA","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,2944671.6804801021,null,2617887.8836462707,null,3477049.8063473967,9039609.3704737686,"2021, 2022"]
[null,"BWA","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,2766780.6781812902,null,1453152.0468243507,null,3429562.9929786497,7649495.7179842908,"2021, 2022"]
[null,"WYK","Zone substation","CPA1","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,4479996.3587197755,null,1968207.4316774304,null,4387782.0739824707,10835985.864379678,"2021, 2022"]
[null,"RWN","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,3692029.4169881437,null,1922051.5500634366,null,6467032.1135330517,12081113.080584632,"2021, 2022"]
[null,"ELM","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,5706344.1747391578,null,3463292.6202249639,null,11769637.66072271,20939274.45568683,"2021, 2022"]
[null,"FGY","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,10854379.762210773,null,5916792.5606089216,null,19693677.30249716,36464849.625316858,"2021, 2022"]
[null,"WOTS","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,5974976.029545567,null,2934182.3058272693,null,9763243.7294538599,18672402.064826697,"2021, 2022"]
[null,"MOE","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,4826724.0973863676,null,2927969.5723496592,null,9900715.3928667791,17655409.062602807,"2021, 2022"]
[null,"BGE","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,4042483.0142064043,null,2450256.9862634121,null,8299923.7374470662,14792663.737916883,"2021, 2022"]
[null,"LDL","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,4258529.0120310104,null,2591735.7678791452,null,8812690.0480656475,15662954.827975802,"2021, 2022"]
[null,"BDL","Zone substation","CPA2","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,5768853.3145909859,null,2948535.0318143675,null,9522848.2045088075,18240236.550914161,"2021, 2022"]
[null,"LLG","Zone substation","CPA3","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,3065772.789745728,null,1861362.0509170489,null,6024495.436632283,10951630.27729506,"2021, 2022, 2023"]
[null,"SLE","Zone substation","CPA3","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,3092724.5912802066,null,1877725.6447058395,null,6078045.2053162782,11048495.441302326,"2021, 2022, 2023"]
[null,"MSD","Zone substation","CPA3","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,4202263.9847750254,null,2551374.5621848362,null,8261092.8133953866,15014731.360355249,"2021, 2022, 2023"]
[null,"BN","Zone substation","CPA3","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,3348774.1367359692,null,2033184.2973039811,null,6580390.9396488275,11962349.373688778,"2021, 2022, 2023"]
[null,"KLO","Zone substation","CPA3","REFCL Station work","Safety",66,null,null,null,null,null,null,null,null,null,null,null,null,null,3586001.1517529897,null,2177214.9849928864,null,7070045.5057976972,12833261.642543573,"2021, 2022, 2023"]
[null,"BGE","Zone substation","DER Hosting Capacity - BGE","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"BRA","Zone substation","DER Hosting Capacity - BRA","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"BRT","Zone substation","DER Hosting Capacity - BRT","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"BWN","Zone substation","DER Hosting Capacity - BWN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"BWR","Zone substation","DER Hosting Capacity - BWR","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"CF","Zone substation","DER Hosting Capacity - CF","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"CLN","Zone substation","DER Hosting Capacity - CLN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"CPK","Zone substation","DER Hosting Capacity - CPK","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"CRE","Zone substation","DER Hosting Capacity - CRE","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"CYN","Zone substation","DER Hosting Capacity - CYN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"DRN","Zone substation","DER Hosting Capacity - DRN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"EPG","Zone substation","DER Hosting Capacity - EPG","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"FGY","Zone substation","DER Hosting Capacity - FGY","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"FTR","Zone substation","DER Hosting Capacity - FTR","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"HPK","Zone substation","DER Hosting Capacity - HPK","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"KLK","Zone substation","DER Hosting Capacity - KLK","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"KLO","Zone substation","DER Hosting Capacity - KLO","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"KMS","Zone substation","DER Hosting Capacity - KMS","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"LDL","Zone substation","DER Hosting Capacity - LDL","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"LGA","Zone substation","DER Hosting Capacity - LGA","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"LLG","Zone substation","DER Hosting Capacity - LLG","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"LYD","Zone substation","DER Hosting Capacity - LYD","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"MJG","Zone substation","DER Hosting Capacity - MJG","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"MSD","Zone substation","DER Hosting Capacity - MSD","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"MWTS","Zone substation","DER Hosting Capacity - MWTS","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"MYT","Zone substation","DER Hosting Capacity - MYT","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"NLA","Zone substation","DER Hosting Capacity - NLA","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"NRN","Zone substation","DER Hosting Capacity - NRN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"OFR","Zone substation","DER Hosting Capacity - OFR","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"PHI","Zone substation","DER Hosting Capacity - PHI","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"PHM","Zone substation","DER Hosting Capacity - PHM","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"RUBA","Zone substation","DER Hosting Capacity - RUBA","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"RWN","Zone substation","DER Hosting Capacity - RWN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"RWT","Zone substation","DER Hosting Capacity - RWT","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"SLE","Zone substation","DER Hosting Capacity - SLE","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"SMG","Zone substation","DER Hosting Capacity - SMG","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"SMR","Zone substation","DER Hosting Capacity - SMR","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"TGN","Zone substation","DER Hosting Capacity - TGN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"TT","Zone substation","DER Hosting Capacity - TT","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"WGI","Zone substation","DER Hosting Capacity - WGI","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"WGL","Zone substation","DER Hosting Capacity - WGL","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"WN","Zone substation","DER Hosting Capacity - WN","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"WT","Zone substation","DER Hosting Capacity - WT","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"WYK","Zone substation","DER Hosting Capacity - WYK","Substation upgrade - voltage","Voltage issues",66,null,null,null,null,null,null,null,null,null,null,null,null,null,331929.28355373122,null,null,null,null,331929.28355373122,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,"All","Other","Top Down Adjustment","Other","Other",66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-4477388,-4477388,"2021, 2022, 2023, 2024, 2025. 2026"]
[null,null,null,"Non material projects - [forecast]"]
[]
[]
[null,"2.3.2 - AUGEX ASSET DATA - SUBTRANSMISSION LINES"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"LINE ID",null,"PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)\n(drop down)","ROUTE LINE LENGTH ADDED",null,null,null,"POLES/TOWERS (INCLUDING STRUCTURES, AND CIVIL WORKS)",null,null,"OVERHEAD LINES",null,null,"UNDERGROUND CABLES",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"KM ADDED",null,null,null,"POLES/TOWERS ADDED","POLES/TOWERS UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N96,Q96,T96,U96,W96,X96,Y96)<>0,SUM(N96,Q96,T96,U96,W96,X96,Y96),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N97,Q97,T97,U97,W97,X97,Y97)<>0,SUM(N97,Q97,T97,U97,W97,X97,Y97),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N98,Q98,T98,U98,W98,X98,Y98)<>0,SUM(N98,Q98,T98,U98,W98,X98,Y98),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,"Non material projects - [forecast]"]

{"sheet":"2.3 Augex (b)","index":12,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,9,9],[29,1,30,1],[29,2,30,2],[29,3,29,9],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[45,1,46,2],[45,3,45,9],[47,1,47,2],[63,1,63,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[60,1,61,2],[60,3,60,9],[62,1,62,2],[68,3,68,9],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[68,1,69,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,"PROJECT TYPE","Units","VOLUMES (0's)"]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",99.18,82.08,34.200000000000003,37.9,32.9,25.2,26.3]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",190.82,157.91999999999999,65.8,65.900000000000006,64.900000000000006,64.099999999999994,63.8]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",138.33000000000001,114.48,47.7,52.8,45.8,35.1,36.700000000000003]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",148.76999999999998,123.11999999999999,51.3,56.8,49.3,37.799999999999997,39.5]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",286.52,237.11999999999998,98.8,98.8,97.4,96.2,95.7]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",207.35,171.6,71.5,79.2,68.7,52.7,55]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,"PROJECT TYPE",null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,16574034,12870980,5202620,5432024,4877091,4099639,4081826]
[null,"HV Feeder Augmentations - Underground Cables",null,0,0,0,0,0,0,0]
[null,"HV Feeder Non-Material Projects",null,8340396,6435490,2601310,2716012,2438545,2049819,2040913]
[null,"LV Feeder Augmentations - Overhead Lines",null,12092946,9391080,3777320,3799935,3823903,3845184,3865177]
[null,"LV Feeder Augmentations - Underground Cables",null,0,0,0,0,0,0,0]
[null,"LV Feeder Non-Material Projects",null,0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted",null,8340396,6435490,2601310,2716012,2438545,2049819,2040913]
[null,"Distribution Substation Augmentations - Ground Mounted",null,0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,96949942,79243029,28362031,25707768,24640130,31907673,34416286]
[null,"Subtransmission Lines",null,0,0,0,0,0,0,0]
[null,"HV Feeders",null,11897078,10534194,7803930,8148035,7315636,6149458,6122740]
[null,"HV Feeders - Land Purchases and Easements",null,0,0]
[null,"Distribution Substations",null,8340396,6435490,2601310,2716012,2438545,2049819,2040913]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,null,0,0,0]
[null,"LV Feeders",null,5947844,5774806,3777320,3799935,3823903,3845184,3865177]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,1938670.03653726,2221657.9235388702,883861.04031377134,889152.66016103642,894766.03048614401,899740.5884573455,904418.87801977166]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,105462734,87869508,35673024,35865591,35431236,34817785,7238066]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,19611196,16339669,7755428.0403137701,5395311.6601610333,3681744.0304861399,10034089.588457299,40201469]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,96801963.5,80596451,30000000,30000000,30000000,30000000,2200000]
[null,"Subtransmission Lines",null,0,0,0,0,0,0,0]
[null,"HV Feeders",null,4273136.5,5095683,3121572,3259214,2926255,2459783,2449096]
[null,"HV Feeders - Land Purchases and Easements",null,null,0]
[null,"Distribution Substations",null,1480582.5,1987055,1040524,1086405,975418,819928,816365]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,5395626.5,2263751,1510928,1519974,1529561,1538074,1546071]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]

{"sheet":"2.5 Connections","index":13,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,10],[54,1,55,1],[54,2,55,2],[54,3,55,3],[54,4,54,10],[102,1,103,1],[102,2,103,3],[102,4,102,10],[159,4,159,10],[177,4,177,10],[195,4,195,10],[120,1,121,1],[120,2,121,3],[120,4,120,10],[138,1,139,1],[138,2,139,3],[138,4,138,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Underground connections","0's",13998.365930571821,11672.274898541447,16506.858352125117,16442.877209588129,16665.497995590697,16807.729463388045,17003.456215146594]
[null,null,"Overhead connections","0's",774.79952343030823,646.05205161743027,913.64278144968478,910.10147105731096,922.42337203889394,930.29578186249387,941.12911732016266]
[null,null,"Distribution substations installed","MVA added",80.361416406338336,80.453459991686273,89.79633388472736,90.425987981782527,91.752970421762541,93.230684237793284,94.510402262061163]
[null,null,"Distribution substations installed","0's",401.80708203169166,402.26729995843135,448.98166942363679,452.12993990891255,458.76485210881265,466.15342118896638,472.55201131030577]
[null,null,"Distribution substations installed ","total spend $0s",3504225.9313556394,3508239.5679117735,3915643.3001187374,3943099.887040107,4000964.0522648604,4065400.9836284667,4121204.1449713153]
[null,null,"Augmentation HV ","net circuit KM added",78.902075550608984,78.992447650179116,88.165657565259679,88.783877319941325,90.086762129788681,91.537641076036806,92.794119778747898]
[null,null,"Augmentation HV","total spend $0s",1625017.1395241094,1626878.3860085832,1815804.003394872,1828536.4656316314,1855369.8554005679,1885251.2386034168,1911128.8776021893]
[null,null,"Augmentation LV","net circuit KM added",19.727553434347232,19.750148789549275,22.043687806126371,22.198258686037242,22.524013484319784,22.886770632837642,23.200922707721315]
[null,null,"Augmentation LV","total spend $0s",1556557.7241004582,1558340.5591988692,1739307.0375642579,1751503.101199162,1777206.0424745183,1805828.5700158717,1830616.0247973141]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006]
[null,null,"Volume of GSL breaches for residential customers","0's",540.5,540.5,540.5,540.5,540.5,540.5,540.5]
[null,null,"Volume of customer complaints relating to connection services","0's",258.75,258.75,258.75,258.75,258.75,258.75,258.75]
[null,null,"GSL payments","$0's",120697.5,120697.5,120697.5,120697.5,120697.5,120697.5,120697.5]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1560.9607252943626,1310.4765147675378,1815.0908984478042,1806.1566941225112,1821.8350525494884,1830.5556739329327,1849.2763143814923]
[null,null,"Overhead connections","0's",215.81277470563745,181.18173523246233,250.94789176268313,249.71268104021922,251.8803140755202,253.08599559422947,255.67424352001146]
[null,null,"Distribution substations installed","MVA added",498.27307531696869,493.81829219379648,511.71034604458413,512.82973873186324,508.97720876714442,507.62696253570175,511.21534885347648]
[null,null,"Distribution substations installed","0's",498.27307531696869,493.81829219379648,511.71034604458413,512.82973873186324,508.97720876714442,507.62696253570175,511.21534885347648]
[null,null,"Distribution substations installed ","total spend $0s",10946090.509932531,10848227.587603558,11241281.217352111,11265872.0978915,11181239.506296594,11151577.222315736,11230407.091647888]
[null,null,"Augmentation HV ","net circuit KM added",141.0836305920914,139.82228012454365,144.88832932740806,145.20527999603311,144.11445462072743,143.73213887869372,144.74817324771232]
[null,null,"Augmentation HV","total spend $0s",5709868.0327584408,5658819.2705276255,5863849.9482499091,5876677.4214524962,5832530.0677613523,5817057.1711205645,5858177.6196055952]
[null,null,"Augmentation LV","net circuit KM added",28.961317456270908,28.702390384710885,29.742337107073368,29.807399998448538,29.58347791867924,29.50499703803349,29.713566195094003]
[null,null,"Augmentation LV","total spend $0s",2406292.9941749303,2384779.6635318105,2471185.142706384,2476590.987241365,2457986.0970251821,2451465.3994236421,2468794.6698269472]
[null,"SUBDIVISION","Underground connections","0's",451.15847621874548,456.18642610088341,448.60873742809662,449.11715506942187,453.31119663296778,459.14320960298932,460.30204078645158]
[null,null,"Overhead connections","0's",60.563222771164035,61.23817151943166,60.220947480936594,60.289197137089438,60.852202570686558,61.635088229109783,61.790648979528157]
[null,null,"Distribution substations installed","MVA added",259.81852157176723,257.36370732405925,258.1647213123947,260.92272661879309,265.07173223140552,270.49502728511396,274.91233822387682]
[null,null,"Distribution substations installed","0's",721.7197324684978,714.90078872500374,717.12583256663493,724.78697558230215,736.31201699440101,751.37675922902667,763.64709488357505]
[null,null,"Distribution substations installed ","total spend $0s",14236692.30804643,14102181.362073036,14146072.727543773,14297196.953382719,14524540.700602083,14821708.825908616,15063754.297816068]
[null,null,"Augmentation HV ","net circuit KM added",206.07365348716928,204.12663085923154,204.76195076665016,206.94944774103172,210.24020907612626,214.54166618124603,218.04523243292394]
[null,null,"Augmentation HV","total spend $0s",8640825.932615079,8559185.7843953539,8585825.2341194358,8677548.6556432359,8815532.7957851607,8995896.1827246975,9142803.395810131]
[null,null,"Augmentation LV","net circuit KM added",299.63678198390909,296.80575732445919,297.72953001139842,300.91021101021431,305.69506885127839,311.94950624785787,317.04378831330189]
[null,null,"Augmentation LV","total spend $0s",12904914.495459456,12782986.436684949,12822771.964547252,12959759.206418164,13165835.980114048,13435205.378909675,13654608.597817019]
[null,null,"Cost per lot","$0's",2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",1,1,1,1,1,1,1]
[null,null,"Distribution substations installed","MVA added",17.565939882331087,20.791118409041513,22.492440452755876,19.392937590139546,16.260809589202093,16.328832396554613,16.391342575214395]
[null,null,"Distribution substations installed","0's",35.131879764662173,41.582236818083025,44.984880905511751,38.785875180279092,32.521619178404187,32.657664793109227,32.78268515042879]
[null,null,"Distribution substations installed ","total spend $0's",1192289.1890107396,1411198.3686951306,1526675.7011541042,1316296.7644641036,1103703.3946170488,1108320.4466140301,1112563.3286185479]
[null,null,"Augmentation HV ","net circuit KM added",60.898773437773123,72.080037731639351,77.978294607097851,67.232731098135616,56.374060580934554,56.609886592028282,56.826601053836605]
[null,null,"Augmentation HV","total spend $0s",8807213.6545416042,10424254.162994545,11277263.272358827,9723234.0478034504,8152847.226351589,8186952.5120208152,8218293.8750636224]
[null,null,"Augmentation LV","net circuit KM added",4.5169559697422798E-2,5.346287590896389E-2,5.7837704021372255E-2,4.9867553803215975E-2,4.1813510372233957E-2,4.1988426162569009E-2,4.2149166621979879E-2]
[null,null,"Augmentation LV","total spend $0s",33295.584944622213,39408.790746133134,42633.583327919689,36758.591067918474,30821.759073090801,30950.693771464419,31069.179487424532]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Underground connections","0's",2195.4380321125186,2268.8248694116569,2247.7411591861937,2249.1646523595386,2262.0312587398698,2287.6314575800038,2303.7683822120262]
[null,null,"Overhead connections","0's",121.51592188961072,125.57783074721888,124.41086249422047,124.48965182133081,125.20180926464167,126.61876192607612,127.51192914120199]
[null,null,"Distribution substations installed","MVA added",99.206761134456528,101.91066510066041,101.95040343502511,102.93835476780501,104.44653569081758,106.31912251164219,107.81105369449529]
[null,null,"Distribution substations installed","0's",496.0338056722826,509.55332550330201,509.7520171751255,514.69177383902502,522.23267845408782,531.59561255821097,539.05526847247631]
[null,null,"Distribution substations installed ","total spend $0s",4325992.7522351108,4443898.7177840164,4445631.5406731199,4488711.9744691029,4554477.4491948532,4636133.1440505609,4701190.0354363071]
[null,null,"Augmentation HV ","net circuit KM added",97.405194086956371,100.05999591304989,100.09901261037197,101.06902302314484,102.54981580222953,104.38839696989704,105.85323509956071]
[null,null,"Augmentation HV","total spend $0s",2006095.6415329035,2060772.2573169172,2061575.8204859917,2081553.5401501812,2112051.0096946005,2149917.2621222641,2180086.1398193417]
[null,null,"Augmentation LV","net circuit KM added",24.3538101846367,25.017579097132163,25.027334277536252,25.269861893144736,25.640098271221401,26.099790972274374,26.466038276593686]
[null,null,"Augmentation LV","total spend $0s",1921581.9883763001,1973955.1643608953,1974724.8746779151,1993860.9644439062,2023073.6235785577,2059344.630367002,2088242.5407118618]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006,8.2025000000000006]
[null,null,"Volume of GSL breaches for residential customers","0's",540.5,540.5,540.5,540.5,540.5,540.5,540.5]
[null,null,"Volume of customer complaints relating to connection services","0's",258.75,258.75,258.75,258.75,258.75,258.75,258.75]
[null,null,"GSL payments","$0's",120697.5,120697.5,120697.5,120697.5,120697.5,120697.5,120697.5]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",345.04528847338213,341.75077585269423,346.14345934694478,343.94711759981948,338.01699488258123,334.72248226189328,334.94211643660583]
[null,null,"Overhead connections","0's",47.704711526617828,47.249224147305753,47.856540653055184,47.552882400180465,46.733005117418735,46.27751773810666,46.307883563394135]
[null,null,"Distribution substations installed","MVA added",518.42551373301842,515.34117834337303,526.04221784800063,527.29357013204447,523.00286584672222,521.45414080107446,525.06012771188466]
[null,null,"Distribution substations installed","0's",518.42551373301842,515.34117834337303,526.04221784800063,527.29357013204447,523.00286584672222,521.45414080107446,525.06012771188466]
[null,null,"Distribution substations installed ","total spend $0s",11388800.392977279,11321043.542345585,11556124.570742521,11583614.347010769,11489355.917677384,11455333.440115504,11534549.960250074]
[null,null,"Augmentation HV ","net circuit KM added",146.78969683942211,145.91638207229764,148.94633006509625,149.30064446041115,148.08575212856033,147.64723806257371,148.66825595506378]
[null,null,"Augmentation HV","total spend $0s",5940801.1688118726,5905456.7985939188,6028083.37910078,6042423.0188652538,5993254.4876914667,5975507.1598350462,6016829.2990565626]
[null,null,"Augmentation LV","net circuit KM added",30.132645379446142,29.953373368201497,30.575354000023641,30.648086829757162,30.398696575549366,30.308679434504867,30.518271597598762]
[null,null,"Augmentation LV","total spend $0s",2503614.4706469113,2488719.3960232865,2540397.5573889068,2546440.6698577558,2525719.7194927791,2518240.5149925663,2535654.7833333737]
[null,"SUBDIVISION","Underground connections","0's",451.15847621874548,456.18642610088341,448.60873742809662,449.11715506942187,453.31119663296778,459.14320960298932,460.30204078645158]
[null,null,"Overhead connections","0's",60.563222771164035,61.23817151943166,60.220947480936594,60.289197137089438,60.852202570686558,61.635088229109783,61.790648979528157]
[null,null,"Distribution substations installed","MVA added",259.81852157176723,257.36370732405925,258.1647213123947,260.92272661879309,265.07173223140552,270.49502728511396,274.91233822387682]
[null,null,"Distribution substations installed","0's",721.7197324684978,714.90078872500374,717.12583256663493,724.78697558230215,736.31201699440101,751.37675922902667,763.64709488357505]
[null,null,"Distribution substations installed ","total spend $0s",14236692.30804643,14102181.362073036,14146072.727543773,14297196.953382719,14524540.700602083,14821708.825908616,15063754.297816068]
[null,null,"Augmentation HV ","net circuit KM added",206.07365348716928,204.12663085923154,204.76195076665016,206.94944774103172,210.24020907612626,214.54166618124603,218.04523243292394]
[null,null,"Augmentation HV","total spend $0s",8640825.932615079,8559185.7843953539,8585825.2341194358,8677548.6556432359,8815532.7957851607,8995896.1827246975,9142803.395810131]
[null,null,"Augmentation LV","net circuit KM added",299.63678198390909,296.80575732445919,297.72953001139842,300.91021101021431,305.69506885127839,311.94950624785787,317.04378831330189]
[null,null,"Augmentation LV","total spend $0s",12904914.495459456,12782986.436684949,12822771.964547252,12959759.206418164,13165835.980114048,13435205.378909675,13654608.597817019]
[null,null,"Cost per lot","$0's",2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492,2070.2165973900492]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",1,1,1,1,1,1,1]
[null,null,"Distribution substations installed","MVA added",17.565939882331087,20.791118409041513,22.492440452755876,19.392937590139546,16.260809589202093,16.328832396554613,16.391342575214395]
[null,null,"Distribution substations installed","0's",35.131879764662173,41.582236818083025,44.984880905511751,38.785875180279092,32.521619178404187,32.657664793109227,32.78268515042879]
[null,null,"Distribution substations installed ","total spend $0s",1192289.1890107396,1411198.3686951306,1526675.7011541042,1316296.7644641036,1103703.3946170488,1108320.4466140301,1112563.3286185479]
[null,null,"Augmentation HV ","net circuit KM added",60.898773437773123,72.080037731639351,77.978294607097851,67.232731098135616,56.374060580934554,56.609886592028282,56.826601053836605]
[null,null,"Augmentation HV","total spend $0s",8807213.6545416042,10424254.162994545,11277263.272358827,9723234.0478034504,8152847.226351589,8186952.5120208152,8218293.8750636224]
[null,null,"Augmentation LV","net circuit KM added",4.5169559697422798E-2,5.346287590896389E-2,5.7837704021372255E-2,4.9867553803215975E-2,4.1813510372233957E-2,4.1988426162569009E-2,4.2149166621979879E-2]
[null,null,"Augmentation LV","total spend $0s",33295.584944622213,39408.790746133134,42633.583327919689,36758.591067918474,30821.759073090801,30950.693771464419,31069.179487424532]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,8734926.959127076,8271833.2388965897,11386692.586135451,11416661.26363242,11584639.988599019,11736432.190148495,11891584.43765014]
[null,null,"Complex connection LV",null,12983186.355117278,13337046.199729953,13342246.754557056,13471539.920835147,13668915.520610712,13913980.911143443,14109229.907829661]
[null,null,"Complex connection HV",null,5136339.9033491155,5276332.0740199639,5278389.4901693882,5329539.7726208726,5407624.4693467366,5504575.9502770677,5581819.3314731661]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,400311.43102881918,331580.06436116376,678504.50265623466,675761.5228115418,684530.35130120697,689490.49968177581,697731.83662005363]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,4411766.8383354442,4385519.3481369792,4476584.486660515,4487233.4118456738,4450719.8021222968,4437540.2544011809,4468226.9645478912]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,10720489.235523943,10656708.45416281,10877994.59031805,10903871.227049032,10815144.017671559,10783118.027937565,10857686.00894301]
[null,null,"Complex connection HV (customer connected at HV)",null,6528696.0868634665,6489854.0780202802,6624615.6452822099,6640374.31946724,6586340.1264435183,6566836.5432337709,6612247.8742933981]
[null,null,"Complex connection sub-transmission",null,121740.84915603814,121016.56071059946,123529.46488224206,123823.31749099176,122815.73979788928,122452.05572530429,123298.84257691297]
[null,"SUBDIVISION","Complex connection LV",null,21513150.142432321,21309889.854585066,21376214.357137859,21604579.070674203,21948119.5548012,22397172.070577726,22762928.418033369]
[null,null,"Complex connection HV (no upstream asset works)",null,23526422.281699479,23304140.220107652,23376671.590192921,23626407.433122706,24002097.57830929,24493173.921981554,24893158.964873116]
[null,null,"Complex connection HV (with upstream asset works)",null,108685.09155434262,107658.21437235021,107993.28778486866,109146.99329215857,110882.5703100645,113151.19733431497,114999.00957225364]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,12165327.864638193,14398931.899620028,15577185.987005357,13430618.892178863,11261457.190575602,11308566.525986051,11351858.079035157]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,2994837.7911338955,3100621.5339195235,3085723.9951033541,3118970.1997832535,3159967.8267268185,3208798.6170726982,3249621.9702251274]
[null,null,"Complex connection LV",null,6940486.614970725,7185638.6739766262,7151113.8763212292,7228161.4009860121,7323172.7174218334,7436337.2593537373,7530944.69918619]
[null,null,"Complex connection HV",null,2745758.8125186046,2842744.5807744768,2829086.0619022916,2859567.198394184,2897155.0757095776,2941924.6366224848,2979352.734400162]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,31806.968478888059,31782.475514820089,32303.759524476158,32402.975650097815,32105.058511877771,31956.88882971519,32148.30398058963]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,2686192.0259945719,2684123.5231501069,2728147.490757898,2736526.5843414911,2711366.605903904,2698853.2405077824,2715018.8129129219]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,6527383.1901076287,6522356.7770422222,6629333.9787255395,6649694.9782656357,6588556.8248024005,6558149.6423865864,6597431.6015893016]
[null,null,"Complex connection HV (customer connected at HV)",null,3975126.5221648542,3972065.4749877974,4037213.7739757909,4049613.467226875,4012380.7985954061,3993863.0566818342,4017785.4698942159]
[null,null,"Complex connection sub-transmission",null,74124.338439458821,74067.258974021373,75282.081832115262,75513.299393107067,74819.020377016757,74473.719325318729,74919.801492353115]
[null,"SUBDIVISION","Complex connection LV",null,4552092.0814501513,4529163.6301827347,4525659.3070713822,4574301.7068248298,4645444.5122173345,4737914.6026897067,4813546.5492582405]
[null,null,"Complex connection HV (no upstream asset works)",null,4978091.9978866624,4953017.8258936536,4949185.5565707879,5002380.073869193,5080180.6595987361,5181304.4086767044,5264014.2443436235]
[null,null,"Complex connection HV (with upstream asset works)",null,22997.308221280833,22881.472985218239,22863.769037833918,23109.511926979609,23468.927552600406,23936.089273802991,24318.184177748335]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,-1121089.7016161999,-1196463.9252195465,-1414861.7973030596,-1204417.4739015161,-1031220.8510539149,-1068009.4126744752,-1089784.12795027]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,2607440.4499578741,2654348.1385086179,2671489.7300829147,2694033.8585577202,2738204.3095959718,2795119.8643670622,2838546.9545042398]
[null,null,"Complex connection LV",null,6042699.7401465522,6151407.5257533276,6191132.8782358272,6243378.5198491337,6345742.8031888781,6477643.6517897053,6578285.2086434709]
[null,null,"Complex connection HV",null,2390581.0908305114,2433587.4932454876,2449303.4282670971,2469972.5742266891,2510469.3936371594,2562651.3136545834,2602466.5970730041]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,20432.382768230367,20146.081460960508,20703.091915182631,20729.96879572756,20595.53142530378,20587.643217756729,20759.586759377769]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1725574.8123408721,1701395.8249868718,1748436.9959026168,1750706.8275041829,1739353.1962183928,1738687.0138933987,1753208.1516349688]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,4193106.0454163137,4134351.6771205878,4248660.6115925107,4254176.2487833966,4226587.1928691585,4224968.3855509795,4260254.4073537085]
[null,null,"Complex connection HV (customer connected at HV)",null,2553569.5646986128,2517788.6030324828,2587401.8713064189,2590760.852240365,2573959.3278481117,2572973.4865519363,2594462.4043991822]
[null,null,"Complex connection sub-transmission",null,47616.510716579323,46949.301736578076,48247.383050126788,48310.018097884691,47996.719420872527,47978.336399985565,48379.041084559853]
[null,"SUBDIVISION","Complex connection LV",null,16961058.060982171,16780726.224402335,16850555.050066475,17030277.363849375,17302675.042583864,17659257.46788802,17949381.868775126]
[null,null,"Complex connection HV (no upstream asset works)",null,18548330.283812813,18351122.394213997,18427486.033622131,18624027.359253511,18921916.918710556,19311869.513304848,19629144.720529493]
[null,null,"Complex connection HV (with upstream asset works)",null,85687.783333061787,84776.741387131959,85129.51874703473,86037.481365178959,87413.642757464098,89215.108060511979,90680.8253945053]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,13286417.566254392,15595395.824839575,16992047.784308415,14635036.366080379,12292678.041629517,12376575.938660527,12441642.206985427]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,13321.058028725298,10817.679976144647,15933.799354880577,15865.335374576447,16091.767826067857,16224.939210819241,16420.826007449916]
[null,null,"Complex connection LV",null,1137.7594581680419,1175.7913074030625,1164.8649271675822,1165.602635450814,1172.2706000618036,1185.5375964130139,1193.9003642785967]
[null,null,"Complex connection HV",null,314.34796710879158,324.85566661116837,321.83685152664145,322.04067061818,323.88294149992942,327.54843801828639,329.85896073824819]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1390.7509885293857,1109.3215040749358,1678.7876902246899,1671.0754522072993,1695.5558216515678,1709.1678900992715,1730.2310607705763]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,146.33369951230608,144.93649677985249,146.79943375645729,145.8679652681549,143.35300034973844,141.95579761728484,142.04894446611507]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,105.23635792221965,104.23155501398713,105.57129222496383,104.90142361947548,103.09277838465694,102.08797547642442,102.15496233697326]
[null,null,"Complex connection HV (customer connected at HV)",null,127.26712412467012,126.05197017058352,127.67217544269899,126.86207280664125,124.67479568928538,123.45964173519877,123.54065199880455]
[null,null,"Complex connection sub-transmission",null,7.1853299114186093,7.1167239606412194,7.2081985616777393,7.1624612611594793,7.0389705497601778,6.9703645989827878,6.9749383290346145]
[null,"SUBDIVISION","Complex connection LV",null,272.30074221844154,275.33540643713945,270.76182451711441,271.06868454166744,273.60003592005722,277.11999962255555,277.81942257035729]
[null,null,"Complex connection HV (no upstream asset works)",null,234.33068875246923,236.94219451152986,233.00636021062456,233.27043117979747,235.44880685053559,238.47794115281536,239.07983543981726]
[null,null,"Complex connection HV (with upstream asset works)",null,5.0902680189987164,5.1469966716457431,5.0615001812942833,5.0672364850463998,5.1145564330615585,5.1803570567282025,5.1934317558051983]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,1,1,1,1,1,1,1]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,864.84652872529603,893.755726144645,885.45024298618978,886.01099811187532,891.07952644277827,901.16418507477954,907.52098633638366]
[null,null,"Complex connection LV",null,1137.7594581680419,1175.7913074030625,1164.8649271675822,1165.602635450814,1172.2706000618036,1185.5375964130139,1193.9003642785967]
[null,null,"Complex connection HV",null,314.34796710879158,324.85566661116837,321.83685152664145,322.04067061818,323.88294149992942,327.54843801828639,329.85896073824819]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,6.7274885293855524,6.6632540749356588,6.7489000142021833,6.7060770445689215,6.5904550265591118,6.5262205721092181,6.5305028690725448]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,146.33369951230608,144.93649677985249,146.79943375645729,145.8679652681549,143.35300034973844,141.95579761728484,142.04894446611507]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,105.23635792221965,104.23155501398713,105.57129222496383,104.90142361947548,103.09277838465694,102.08797547642442,102.15496233697326]
[null,null,"Complex connection HV (customer connected at HV)",null,127.26712412467012,126.05197017058352,127.67217544269899,126.86207280664125,124.67479568928538,123.45964173519877,123.54065199880455]
[null,null,"Complex connection sub-transmission",null,7.1853299114186093,7.1167239606412194,7.2081985616777393,7.1624612611594793,7.0389705497601778,6.9703645989827878,6.9749383290346145]
[null,"SUBDIVISION","Complex connection LV",null,272.30074221844154,275.33540643713945,270.76182451711441,271.06868454166744,273.60003592005722,277.11999962255555,277.81942257035729]
[null,null,"Complex connection HV (no upstream asset works)",null,234.33068875246923,236.94219451152986,233.00636021062456,233.27043117979747,235.44880685053559,238.47794115281536,239.07983543981726]
[null,null,"Complex connection HV (with upstream asset works)",null,5.0902680189987164,5.1469966716457431,5.0615001812942833,5.0672364850463998,5.1145564330615585,5.1803570567282025,5.1934317558051983]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,1,1,1,1,1,1,1]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,645115.99077867775,654894.33395056566]
[null,null,"Complex connection LV",null,55054.836576467176,56136.543678786358]
[null,null,"Complex connection HV",null,13853.731158351582,14156.507834303415]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,71830.413263894501,72560.41882198106]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,6527.5388059161623,6637.5531153096626]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,4900.0884296099339,4978.923282715833]
[null,null,"Complex connection HV (customer connected at HV)",null,719.87705480426234,816.56386025766096]
[null,null,"Complex connection sub-transmission",null,35.252042441359777,42.368766402000993]
[null,"SUBDIVISION","Complex connection LV",null,5091.2722978090032,5366.6077042461429]
[null,null,"Complex connection HV (no upstream asset works)",null,4694.1855765183691,4931.1277710298991]
[null,null,"Complex connection HV (with upstream asset works)",null,20.226302951911798,25.373299623557543]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0]
[null,null,"Complex connection HV (small capacity)",null,33,33]
[null,null,"Complex connection HV (large capacity)",null,3.5,4.5]

{"sheet":"2.6 Non-network","index":14,"n_rows":118,"n_cols":11,"rows_kept":118,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,4,8,10],[12,1,16,1],[19,1,29,1],[32,1,36,1],[39,1,49,1],[55,1,56,3],[55,4,55,10],[57,1,57,3],[58,1,58,3],[59,1,59,3],[62,4,62,10],[64,1,68,1],[69,1,73,1],[74,1,78,1],[79,1,83,1],[84,1,88,1],[94,4,94,10],[97,1,97,3],[98,1,98,3],[99,1,99,3],[100,1,100,3],[101,1,101,3],[102,1,102,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[106,1,106,3],[108,1,108,3],[109,1,109,3],[116,1,116,3],[117,1,117,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[113,1,113,3],[114,1,114,3],[115,1,115,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.6 NON NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2021)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,24578686.025925349,24578686.025925349,29103570.396610584,29373633.864282925,29303164.923866794,29766257.85671721,30110577.429352943]
[null,"MOTOR VEHICLES","Car",null,95657.718964652857,95657.718964652857,95657.718964652857,95657.718964652857,95657.718964652857,95657.718964652857,95657.718964652857]
[null,null,"Light commercial vehicle",null,951482.42810883932,951482.42810883932,951482.42810883932,951482.42810883932,951482.42810883932,951482.42810883932,951482.42810883932]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,304372.13410196122,304372.13410196122,304372.13410196122,304372.13410196122,304372.13410196122,304372.13410196122,304372.13410196122]
[null,null,"Heavy commercial vehicle",null,151588.23937314167,151588.23937314167,151588.23937314167,151588.23937314167,151588.23937314167,151588.23937314167,151588.23937314167]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,5903774.2990332739,5903774.2990332739,5903774.2990332739,5903774.2990332739,5903774.2990332739,5903774.2990332739,5903774.2990332739]
[null,"OTHER","Other expenditure",null,0,0,0,0,0,0,0]
[null,"OTHER - DNSP nominated"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,61136772.729486287,53837866.259191543,45435736.398980513,31676147.239958487,36245473.02684658,27536544.12636824,26953136.876349084]
[null,"MOTOR VEHICLES","Car",null,804734.72066120047,1039496.5145140061,1688171.4181812874,1791467.7878379286,2161262.5904644052,2761993.8317558179,2999889.0871549714]
[null,null,"Light commercial vehicle",null,677056.8370242439,874571.71182611806,918638.75053506996,641474.37821133947,799121.22307672573,1554965.8607360395,2045018.5100070809]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,141219.21371453573,182416.48666290249,0,0,254549.82018766738,411464.15804039757,313830.16381820064]
[null,null,"Heavy commercial vehicle",null,98807.822045944456,127632.60237993546,181098.13540828307,211556.11931921635,224600.73272344487,239012.53181885241,293269.69431510539]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,18571114.13782401,2327558.4328926932,4766583.0498622246,2188507.4005018608,892170.99185464915,2625977.2932714764,9479194.6064198725]
[null,"OTHER","Other expenditure",null,0,0,1277847.1304252069,1280934.4849754327,1284206.6451347689,1287111.9296042204,1289841.4413576575]
[null,"OTHER - DNSP nominated","General furniture and equipment",null,1685092.4385715781,1634660.719044741,1585908.8262617646,1589740.4761629333,1593801.4843649913,1597407.1709711596,1600794.7098074527]
[null,null,"Land purchases - REFCL",null,863013.55258521601,869063.9218123079,34640.556735496219,366110.15044618322,637591.26607844396,926090.55231018353,1004834.0973034032]
[null,null,"Live line equipment - REFCL",null,391694.71780683642,112200,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Employee numbers",null,null,910,910,910,910,910,910,910]
[null,"User numbers",null,null,2150,2150,2150,2150,2150,2150,2150]
[null,"Number of devices",null,null,1832,1832,1832,1832,1832,1832,1832]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"CAR","Average kilometres travelled ","0's",24987,24987,24987,24987,24987,24987,24987]
[null,null,"Number purchased","0's",22,22,37,38,44,58,64]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",280,280,280,280,280,280,280]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",24944,24944,24944,24944,24944,24944,24944]
[null,null,"Number purchased","0's",11,11,12,9,11,19,24]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",78,78,78,78,78,78,78]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",12530,12530,12530,12530,12530,12530,12530]
[null,null,"Number purchased","0's",1,1,0,0,1,1,1]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",8,8,8,8,8,8,8]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",9783,9783,9783,9783,9783,9783,9783]
[null,null,"Number purchased","0's",1,1,1,1,2,2,2]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",23,23,23,23,23,23,23]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[]
[]
[null,"Table 2.6.4 intentionally omitted"]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RECURRENT"]
[null,"Metering Lifecycle",null,null,0,0,2247797.746676066,4025680.3677909821,668444.95092762157,0,676627.57834240654]
[null,"CLCOE - Apps",null,null,0,0,1143234.2566474215,1294885.6588104134,1593968.8988307291,1749850.1990633307,1466801.0289094367]
[null,"Corporate Communications",null,null,0,0,4466327.2935256185,1781386.2298666979,1794140.0358077481,1805463.8807672358,1816102.6213917823]
[null,"CLCOE - Infra",null,null,0,0,7284807.8015085356,1656144.0676932523,9769721.3400398325,2397898.4499623142,2653230.5347932647]
[null,"Corporate Enablement",null,null,0,0,1056410.9073380711,1772659.3889793127,1428280.5721951837,1796619.0857692671,1084323.4249321632]
[null,"ICT Expenditure",null,null,24279171.991757546,10495159.728894679,0,0,0,0,0]
[null,"CLIENT DEVICES",null,null,0,0,0,0,0,0,0]
[null,"CLCOE - Infra",null,null,0,0,670016.63602844253,152323.04094344252,898565.34386991744,220545.53761169451,244029.61841857276]
[null,"Workforce Collaboration ",null,null,0,0,1379466.343686814,1111078.5542701005,1119033.3032340484,1126096.1630874719,849548.78445975052]
[]
[null,"NON-RECURRENT"]
[null,"Outage Management",null,null,0,0,2864314.107219588,2883794.5120859039,1936293.9948787936,974257.52743047499,979998.36403554748]
[null,"5 min Settlement",null,null,0,0,7024367.958362706,0,0,0,0]
[null,"Customer Information Services ",null,null,0,0,990233.2561303426,1329290.5376617925,2008211.3576946438,1347257.552885439,1016397.2260325841]
[null,"DER",null,null,0,0,1349808.261498691,1746042.0632563434,2076399.938277476,2489837.3334206091,2907199.7743953359]
[null,"Corporate Enablement",null,null,0,0,452747.53171631624,759711.16670541978,612120.24522650742,769979.60818682867,464710.03925664135]
[null,"Workforce Collaboration ",null,null,0,0,591199.86158006312,476176.52325861453,479585.70138602081,482612.64132320223,364093.33619703603]
[null,"IM",null,null,0,0,3155612.427514948,2541659.1784540731,2559856.1462911479,2576012.8640169981,1943394.0627043317]
[null,"Future Distribution Network Management",null,null,0,0,7141673.6110680457,5592412.5004917514,5632451.2874643626,6477715.3283081744,7330371.1045675194]
[null,"Cyber Security",null,null,0,0,3617718.3984788465,4552903.4496903792,3668399.9107225491,3322397.9545352063,3156309.9741546148]
[null,"ICT Expenditure",null,null,36857600.737728745,43342706.530296862,0,0,0,0,0]

{"sheet":"2.10 Overheads","index":15,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,3,8,9],[23,3,23,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE ($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE ($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",64060192.302748092,64060192.302748092,75158756.751601577,76272271.965273723,77407949.311964855,78488822.36002183,79323174.835277423]
[null,"Alternative Control Services","Total  ",0,0,0,0,0,0,0]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",26676237.028954912,25606188.581280082,25081027.813311782,24655280.391756963,24655280.391756963,24655280.391756963,24655280.391756963]
[null,"Alternative Control Services","Total  ",1252952.5759543246,2053403.7902760697,2199229.7979369434,2036077.9036444151,1956271.7693063386,1934553.7883432256,1870560.4212664852]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ","           99,655 ","                      99,655 ",0,0,0,0,0]
[null,"Unregulated Distribution Services","Total  ","         354,584 ","                    354,584 ",0,0,0,0,0]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",20763454.791556746,20763454.791556746,24360767.457991909,24721684.61992494,25089785.064181726,25440122.112229902,25710555.891421817]
[null,"Alternative Control Services","Total  ",0,0,0,0,0,0,0]
[null,"CAPEX"]
[null,"Standard Control Services","Total",5052559.5892935973,4849889.1924366541,4750422.1622389918,4669784.3190882141,4669784.3190882141,4669784.3190882141,4669784.3190882141]
[null,"Alternative Control Services","Total",154056.93538675006,187153.69878996554,308569.29793107492,307056.93982888525,302515.6260402124,274845.60991743533,232005.85336128093]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",0,0,0,0,0,0,0]

{"sheet":"2.11 Labour","index":16,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[8,2,8,8],[9,2,9,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"($0's, real \", dms_DollarReal,\")\")","v":"($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"In-house labour expenditure",85452786.437000751,85452786.437000751,100257663.28037669,101743031.56179839,103257962.91432223,104699788.33539827,105812768.82013123]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Controllable non-labour expenditure",112725078.76927596,112725078.76927596,132254938.21475291,134214362.40097401,136212784.72473511,138114769.32862121,139582957.99795952]
[null,"Uncontrollable non-labour expenditure",6170489.3674905337,6170489.3674905337,7239539.7631310243,7346797.2273926195,7456189.4215268381,7560302.6845517531,7640670.2715388937]
[null,"Total",{"$f":"SUM(C13:C17)","v":204348354.57376724},204348354.57376724,239752141.25826061,243304191.19016501,246926937.06058419,250374860.34857121,253036397.08962962]
[null,"CAPEX"]
[null,"In-house labour expenditure",53753537.052876346,51339725.436592236,41147105.288093708,36852222.943760879,36150251.812696747,34086119.608516589,33719026.135495812]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Controllable non-labour expenditure",355741135.07578802,339845419.75761133,271128166.77740431,259348324.36025426,259882630.35336137,246863394.42032745,248754344.40708226]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C20:C24)","v":409494672.12866437},391185145.19420356,312275272.06549799,296200547.30401516,296032882.16605812,280949514.02884406,282473370.5425781]

{"sheet":"2.14 Forecast price changes","index":17,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[11,4,11,8],[12,2,12,8],[5,1,5,2],[7,1,7,2],[8,1,8,2],[11,1,13,1],[11,2,11,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet. It has been grouped for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"AusNet (D) must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"Labour Price Growth - WPI",5.8999999999999999E-3,6.3E-3,5.7119806869430053E-3,6.1253168643765543E-3,6.4260393123064192E-3,5.6447897708409673E-3,5.2535999999999998E-3]
[null,"Output Growth",1.54E-2,1.4999999999999999E-2,1.5140462319952797E-2,1.413053499470506E-2,1.540262676058754E-2,1.3609423254243923E-2,1.0767590159900552E-2]
[null,"Productivity",0,0,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3]
[null,"Materials",0,0,0,0,0,0,0]
[null,"CAPEX"]
[null,"Labour Price Growth - WPI",5.8999999999999999E-3,6.3E-3,5.7119806869430053E-3,6.1253168643765543E-3,6.4260393123064192E-3,5.6447897708409673E-3,5.2535999999999998E-3]
[null,"Materials",0,0,0,0,0,0,0]
[]
[null,"CPI"]
[null,"CPI",1.5929203539823078E-2,2.0000000000000018E-2,2.4500000000000001E-2,2.4500000000000001E-2,2.4500000000000001E-2,2.4500000000000001E-2,2.4500000000000001E-2]

{"sheet":"2.16 Opex Summary","index":18,"n_rows":67,"n_cols":12,"rows_kept":67,"cut":false,"hidden":false,"merged":[[5,1,5,6],[7,9,7,11],[8,1,8,7],[8,9,8,10],[8,11,9,11],[9,1,9,7],[9,9,9,10],[42,2,42,11],[43,2,43,11],[56,2,56,11],[57,2,57,11],[10,1,10,7],[10,9,10,10],[14,2,14,11],[15,2,15,11],[28,2,28,11],[29,2,29,11]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nAusNet (D)'s total forecast opex must reconcile to Table 2.16.1 (and if AusNet (D) owns any dual function assets Table 2.16.3). If AusNet (D) did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if AusNet (D) owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has AusNet (D) used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If AusNet (D) does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,2018]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,2017,2018,2019,2020,2021,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Base year total opex, excluding category specific",null,0,209074291.26305607,209074291.26305607,209074291.26305607,215352771.60235175,215352771.60235175,215352771.60235175,215352771.60235175,215352771.60235175]
[null,"Increment from base year to final year",null,null,null,null,6278480.3392956834]
[null,"Price growth",null,null,null,null,null,1248715.0167740425,2632114.5495564053,4136442.8225302561,5504438.0418435996,6804616.3914554827]
[null,"Output growth",null,null,null,null,null,3260540.5239428082,6349663.5812518038,9764463.4422981944,12828179.175845889,15285138.136121929]
[null,"Productivity growth",null,null,null,null,null,-1099310.1357153137,-2237737.13358824,-3421639.7988773794,-4638771.6647188878,-5876998.5836075591]
[null,"Step changes",null,null,null,null,null,3414108.8585961103,3534225.023217781,3241400.4531045449,3335427.1263571596,3383601.436909006]
[null,"Category specific",null,0,0,0,0,17575315.392311204,17673153.567375511,17853498.539176799,17992816.066891722,18087268.106399026]
[null,"Total opex",{"$f":"SUM(C18:C24)","v":0},0,209074291.26305607,209074291.26305607,215352771.60235175,239752141.25826061,243304191.19016498,246926937.06058419,250374860.34857124,253036397.08962965]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C32:C38)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,2017,2018,2019,2020,2021,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Base year total opex, excluding category specific",null,0,0,0,0,0,0,0,0,0]
[null,"Increment from base year to final year",null,null,null,null,0,0,0,0,0,0]
[null,"Price growth",null,null,null,null,null,0,0,0,0,0]
[null,"Output growth",null,null,null,null,null,0,0,0,0,0]
[null,"Productivity growth",null,null,null,null,null,0,0,0,0,0]
[null,"Step changes",null,null,null,null,null,0,0,0,0,0]
[null,"Category specific",null,0,0,0,0,0,0,0,0,0]
[null,"Total opex",{"$f":"SUM(C46:C52)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C60:C66)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":19,"n_rows":89,"n_cols":11,"rows_kept":89,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,4,8,10],[9,4,9,10],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,1,21,3],[22,1,22,3],[25,4,25,10],[26,4,26,10],[27,2,27,3],[28,2,28,3],[29,2,29,3],[30,2,30,3],[31,2,31,3],[32,2,32,3],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,2,36,3],[37,2,37,3],[38,1,38,3],[41,4,41,10],[42,4,42,10],[43,2,43,3],[44,2,44,3],[45,2,45,3],[46,2,46,3],[47,2,47,3],[48,2,48,3],[49,2,49,3],[50,2,50,3],[51,2,51,3],[52,2,52,3],[53,2,53,3],[54,1,54,3],[55,1,55,3],[58,4,58,10],[59,4,59,10],[60,2,60,3],[61,2,61,3],[62,2,62,3],[63,2,63,3],[64,2,64,3],[65,2,65,3],[66,2,66,3],[76,3,76,10],[88,1,88,2],[67,2,67,3],[68,2,68,3],[69,2,69,3],[70,2,70,3],[71,1,71,3],[75,3,75,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"REFCL - step change","Step change for increases in ongoing cost as a result of the REFCL program",null,0,419982.46805052977,864536.83135857875,1106357.9606394647,1323607.1946628315,1324793.166336746,1325979.1380106609]
[null,"IT Opex - step change","Additional opex due to transition to cloud based solutions. This is a capex/opex tradeoff.",null,0,264576.01012872654,529152.02025745308,529152.02025745308,529152.02025745308,529152.02025745308,529152.02025745308]
[null,"Security","Uplift in Cyber Security Capabilities as a result of a direction by AEMO. ",null,0,474642.83134073881,1067946.3705166625,1067946.3705166625,901821.37954740366,830624.95484629297,807913.34518458252]
[null,"5 minute meter data - step change","Increase in ongoing opex to handle greater data flows to meet the new 5 minute settlement rules. ",null,0,317491.21215447184,952473.63646341546,830768.67180420121,486819.85863685684,650856.98491666722,720556.93345630937]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E12:E21)","v":0},1476692.5216744668,3414108.8585961098,3534225.0232177814,3241400.4531045454,3335427.1263571596,3383601.436909006]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$22,0)-ROUND('2.16 Opex Summary'!H$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$22,0)-ROUND('2.16 Opex Summary'!I$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$22,0)-ROUND('2.16 Opex Summary'!J$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$22,0)-ROUND('2.16 Opex Summary'!K$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$22,0)-ROUND('2.16 Opex Summary'!L$23,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Overhead Cable","Proactive replacement of bare SWER conductor in Codified Areas with HV ABC",null,0,742824.00292600226,1851889.3688037151,2826512.7909066286,5027155.5395918889,9996573.3198547587,21233279.338129483]
[null,"REFCL","Tranche 3 REFCL Construction, Testing and Commissioning",null,16147558.913359912,33957333.02349519,27399588.893316165,10135210.374957033,0,0,0]
[null,"REFCL Augmentation","Augmentation to address the capacitive current seen by REFCL's",null,0,0,0,12005835.724716794,21343613.480876435,30775991.688868444,33637208.861343749]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E29:E38)","v":16147558.913359912},34700157.026421189,29251478.262119878,24967558.890580453,26370769.020468324,40772565.008723199,54870488.199473232]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E45:E54)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$22,0)-ROUND('2.16 Opex Summary'!H$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$22,0)-ROUND('2.16 Opex Summary'!I$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$22,0)-ROUND('2.16 Opex Summary'!J$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$22,0)-ROUND('2.16 Opex Summary'!K$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$22,0)-ROUND('2.16 Opex Summary'!L$51,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E62:E71)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Category","Description",{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"GSL payments - bottom-up forecast","Payments for failure to meet Guaranteed Service Levels",6993101.5629132744,9347020.9637976438,9347020.9637976438,9347020.9637976438,9347020.9637976438,9347020.9637976438,9347020.9637976438,9347020.9637976438]
[null,"Metering - reallocation","Reallocation of costs from the ACS metering business to reflect additional usage of AMI systems by the distribution business. ",0,0,0,5671139.6291159382,5737071.6991435383,5875638.6976210754,6048396.8233351503,6107144.4485612055]
[null,"Innovation - step change","Expenditure on proposed innovation programs.",0,0,0,242388.11852068987,242388.11852068987,242388.11852068987,242388.11852068987,242388.11852068987]
[null,"Debt Raising Costs","Forecast Based on AER's benchmark methodology.",2222100.8372093025,2344316.3832558137,2344316.3832558137,2314766.680876933,2346672.785913642,2388450.7592373937,2355010.1612382396,2390714.5755194849]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D86:D88)","v":0},0,0,0,0,0,0,0]

{"sheet":"3.1 Revenue","index":20,"n_rows":53,"n_cols":17,"rows_kept":53,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[9,2,9,8],[9,10,9,16],[10,2,10,8],[10,10,10,16],[29,2,29,8],[29,10,29,16],[30,2,30,8],[30,10,30,16],[31,2,31,8],[31,10,31,16],[43,2,43,8],[43,10,43,16],[44,2,44,8],[44,10,44,16],[45,2,45,8],[45,10,45,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DREV0101","Revenue from Fixed Customer Charges ",103214640.78606175,100228137.79100305,96022897.262767643,99256473.630711645,102585023.99651928,106019928.65690881,109536722.2647613,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",242242287.59937176,229765552.5555245,192784725.98031032,193258480.54816142,193947089.56810215,194875948.93711138,195669916.03067315,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",180522713.32530242,171514593.1053316,173442521.63690126,175827438.96011806,178021788.17698464,180036259.7078608,181911601.09310263,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",12843036.443085339,12385745.751874458,14424173.442967005,14902779.918599883,15354602.618015088,15789393.451435823,16199653.986574208,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",50504677.319165044,48301674.16010464,50653900.397889882,51325969.799309745,51931066.972352006,52484038.605353169,53004752.503199607,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",9922514.860315498,9573627.1912125573,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",43180921.881932259,40741088.540079087,41162907.135085389,42199077.870533317,43290345.513244674,44404207.801155515,45524785.182506859,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",42056062.104185037,40951447.174859434,47601172.173002347,49707113.33262486,51907506.519182138,54165739.532450289,56847183.471924573,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,48974689.611457631,51932266.498839393,53452899.668418288,53929133.897884734,54409611.097194202,54894369.068738826,55383445.951708063]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,4011432.8202974531,3354192.2198143657,7051178.0972610395,7026054.3810398877,7127990.4519614,7186470.5626941221,7273712.6807704559]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,10421659.555353427,10475906.571795451,12488290.050153334,11507860.99334896,11659599.034052985,12002113.077305723,12227567.461332344]
["DREV0113","Revenue from other Sources",-2644062.4044263558,-907657.88475013373,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":681842791.91499257},652554208.38523924,616092298.02892387,626477334.06005895,637037423.36439991,647775516.69227576,658694614.53274226,null,{"$f":"SUM(K13:K25)","v":63407781.987108506},65762365.29044921,72992367.81583266,72463049.272273585,73197200.583208591,74082952.70873867,74884726.093810856]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DREV0201","Revenue from residential Customers ",367971179.7832886,352736121.42737734,316670080.89894396,319890143.36837083,323187247.98479557,326718157.97131759,330237565.55836844,null,43664543.654902838,46301441.328708611,47657197.821356952,48081795.720138364,48510176.539105833,48942373.981876768,49378422.052348219]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",90457356.177433431,86378547.663018733,79891095.95809941,80894076.825128272,81908707.051193416,82851331.652583256,83744161.690757558,null,5310145.9565547928,5630825.1701307772,5795701.8470613314,5847338.1777463676,5899434.5580883687,5951995.0868620556,6005023.8993598465]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",191903248.54213035,183660884.14999411,192752567.593622,198615613.74889386,204563166.19777513,210537066.74708089,216765753.0111967,null,0,0,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",21588492.551824819,20192903.461264137,20619941.400683176,20832904.376590312,21049389.886644859,21260733.385571185,21467716.965900742,null,0,0,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",9922514.860315498,9585751.6835848242,6158612.1775751337,6244595.7410756741,6328912.2439911067,6408226.9357227599,6479417.3065187838,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV02","Total revenue by customer class",{"$f":"SUM(C34:C39)","v":681842791.91499269},652554208.38523912,616092298.02892363,626477334.06005895,637037423.36440015,647775516.69227564,658694614.53274226,null,{"$f":"SUM(K34:K39)","v":48974689.611457631},51932266.498839386,53452899.668418281,53929133.897884734,54409611.097194202,54894369.068738826,55383445.951708063]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DREV0301","EBSS",9280182.2592477351,3620542.7184919724,17543720.869361512,17839443.075159844,18140150.062901162,18445925.857560687,18756855.900463779,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",7585867.7430104753,2791303.0114647103,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",930675.98230088502,161262,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",-3805105.2525014756,-1952505.858932341,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",0,0,9185412.9461824577,9340245.0138972066,9497686.9772511944,9657782.8294258565,9820577.3051648606,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C48:C52)","v":13991620.73205762},4620601.8710243423,26729133.815543972,27179688.089057051,27637837.040152356,28103708.686986543,28577433.205628641,null,{"$f":"SUM(K48:K52)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":21,"n_rows":85,"n_cols":17,"rows_kept":85,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[10,2,10,8],[10,10,10,16],[11,2,11,8],[11,10,11,16],[80,2,80,8],[81,2,81,8],[82,2,82,8],[67,2,67,8],[67,10,67,16],[68,2,68,8],[68,10,68,16],[69,2,69,8],[69,10,69,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPEX0101"," OPERATING"]
["DOPEX0102","Network Operating Costs ",49577494.883611463,49577494.883611463,54975097.631658487,56115972.590946317,57342053.583223969,58192916.708854303,58876436.330791332,null,0,0,0,0,0,0,0]
["DOPEX0103","Billing & Revenue Collection",89161.936060291526,89161.936060291526,96327.602796089224,97748.786657469842,99343.502530787664,100686.63396328197,101765.23631106726,null,0,0,0,0,0,0,0]
["DOPEX0104","Advertising, marketing & promotions",876393.5119159522,876393.5119159522,946826.5252991356,960795.67368675501,976470.50878432463,989672.46160298504,1000274.2962120626,null,0,0,0,0,0,0,0]
["DOPEX0105","Customer Service",5556490.5957369516,5556490.5957369516,6003048.4161360217,6091615.2991525,6190996.5390009824,6274699.2657839311,6341916.7810917655,null,0,0,0,0,0,0,0]
["DOPEX0106","Regulatory",3010431.6213352666,3010431.6213352666,3252370.6222426575,3300354.9642733037,3354198.3788985191,3399547.3867223966,3435964.9294328154,null,0,0,0,0,0,0,0]
["DOPEX0107","IT",24578686.025925349,24578686.025925349,29103570.396610584,29373633.864282925,29303164.923866794,29766257.85671721,30110577.429352943,null,13147482.291531537,13170877.51808268,7477400.7017182205,7444846.3028122727,7341010.6616969686,7199985.9752871115,7171824.3211069899]
["DOPEX0108","Licence fee",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0109","GSL payments",0,0,9347020.9637976438,9347020.9637976438,9347020.9637976438,9347020.9637976438,9347020.9637976438,null,0,0,0,0,0,0,0]
["DOPEX0110","Non-network alternatives costs",11405973.76483082,11405973.76483082,12322636.305006735,12504440.184040355,12708443.015485408,12880262.09612303,13018241.49209762,null,0,0,0,0,0,0,0]
["DOPEX0111","AMI Cost",7826503.6235760972,7826503.6235760972,14126634.940749779,14317316.440100472,14595865.252708385,14886521.480323782,15039947.233418563,null,2220381.0506310631,2227921.762696892,2323083.0733659398,2613060.3758322331,2840940.5166249326,2940029.380469434,3022351.9505647472]
["DOPEX0112","Other - Standard Control Services",25664800.566426858,25664800.566426858,27727400.548277516,28136480.947181083,28595511.635132287,28982125.047453843,29292595.135582827,null,0,0,0,0,0,0,0]
["DOPEX0113"," MAINTENANCE"]
["DOPEX0114","Routine",10788022.722547591,10788022.722547591,11655022.46463166,11826976.601867137,12019927.000182025,12182437.293849476,12312941.263936361,null,0,0,0,0,0,0,0]
["DOPEX0115","Condition based",45477068.484882221,45477068.484882221,49131918.651699565,49856793.846759401,50670179.089266501,51355243.622840986,51905385.02853027,null,0,0,0,0,0,0,0]
["DOPEX0116","Emergency",19449835.237456329,19449835.237456329,21012957.838153824,21322975.690696798,21670847.914619952,21963839.366113313,22199126.293227274,null,0,0,0,0,0,0,0]
["DOPEX0117","SCADA/Network Control",47491.59946206805,47491.59946206805,51308.35120089358,52065.336722843276,52914.753086572739,53630.164425036717,54204.675847099461,null,0,0,0,0,0,0,0]
["DOPEX0118","Other - Standard Control Services",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0119","AMI",0,0,0,0,0,0,0,null,1187034.8455060965,1189708.0377238197,1195024.5239818159,1198929.8148570708,1203090.5629907704,1206956.2027954073,1210532.5391039404]
["DOPEX0120","Public Lighting",0,0,0,0,0,0,0,null,8589233.2387688234,8326637.6155471932,7863349.7467969749,7733448.8846003013,7337143.5510646179,7237510.1244625803,7207299.587155167]
["DOPEX0121","Alternative control -other",0,0,0,0,0,0,0,null,2385611.5110410214,2468434.6851211688,3035940.5826577786,7225132.6791684087,6780052.2605440132,3731255.6419243533,3235001.6042864057]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C14:C62)","v":204348354.57376727},204348354.57376727,239752141.25826058,243304191.19016504,246926937.06058416,250374860.34857121,253036397.08962968,null,{"$f":"SUM(K14:K62)","v":27529742.937478542},27383579.61917175,21894798.628520727,26215418.057270288,25502237.552921303,22315737.324938886,21847010.002217252]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPEX0201","Opex for network services",178869778.53363988,178869778.53363988,205359272.52579275,208418714.6397042,211462527.75367266,214336201.37891945,216619027.7149514,null,2385611.5110410214,2468434.6851211688,3035940.5826577786,7225132.6791684087,6780052.2605440132,3731255.6419243533,3235001.6042864057]
["DOPEX0202","Opex for metering",7826503.6235760972,7826503.6235760972,14126634.940749779,14317316.440100472,14595865.252708385,14886521.480323782,15039947.233418563,null,16554898.187668698,16588507.318503393,10995508.299065977,11256836.493501576,11385041.741312673,11346971.558551952,11404708.810775677]
["DOPEX0203","Opex for connection services",2567218.5808889205,2567218.5808889205,2947407.5749855996,2991318.048327581,3035004.2073142636,3076248.4487206251,3109012.5871617179,null,0,0,0,0,0,0,0]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,8589233.2387688234,8326637.6155471932,7863349.7467969749,7733448.8846003013,7337143.5510646179,7237510.1244625803,7207299.587155167]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",15016313.165993532,15016313.165993532,17240135.103135709,17496978.608351346,17752510.041960806,17993758.079764161,18185403.842656337,null,0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",68540.669668842893,68540.669668842893,78691.113596795141,79863.45368140655,81029.804928042489,82130.960843249602,83005.711441656997,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.2.4 - OPEX FOR HIGH VOLTAGE CUSTOMERS"]
[null,null,"End user costs (not standard control services)"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPEX0401","Opex for high voltage customers",246463.01107263716,246463.01107263716,246463.01107263716,246463.01107263716,246463.01107263716,246463.01107263716,246463.01107263716]

{"sheet":"3.3 Assets (RAB)","index":22,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[8,18,8,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[21,2,21,8],[21,10,21,16],[21,18,21,24],[22,2,22,8],[22,10,22,16],[22,18,22,24],[97,2,97,8],[97,10,97,16],[97,18,97,24],[98,2,98,8],[98,10,98,16],[98,18,98,24],[114,2,114,8],[114,10,114,16],[114,18,114,24],[115,2,115,8],[115,10,115,16],[115,18,115,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",4277916371.4887838,4489715967.2293768,4701674067.712842,4768559208.5437651,4809608785.121047,4846810453.1765003,4862731663.172883,null,4290385688.1048713,4501899298.3991327,4715140468.7922983,4781711502.8155107,4822446972.5850821,4859334533.8328247,4874941637.0214968,null,301260036.19125086,280151279.95133829,268393749.8817693,255115640.94897166,237285158.97669107,217560227.17388594,196363584.73454937]
["DRAB0102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0103","Straight line depreciation",-204326161.26316842,-209570219.33720917,-247333650.70376915,-256733809.10817823,-260238162.81581804,-266112731.11656284,-270801953.64600003,null,-204612146.70949966,-209854262.73866326,-247647757.51147977,-257047915.91588888,-260552269.62352866,-266426837.92427349,-271116060.45371062,null,-39222561.283461817,-31780567.324871637,-35854330.394526385,-38108419.581015095,-39025829.86287117,-40068459.384002186,-40756581.149857879]
["DRAB0105","Actual additions (recognised in RAB)",417449399.26365411,394281004.45803565,315881754.82668602,299446348.97745442,299102794.16326547,283696904.40493977,285069531.64142323,null,417449399.26365417,395612329.98709971,315881754.82668602,299446348.97745442,299102794.16326535,283696904.40493989,285069531.64142317,null,18113805.04354924,15325634.478939008,22576221.461728759,20277937.608734496,19300898.060066033,18871816.944665607,17705529.982165534]
["DRAB0106","Disposals ",-1323642.2598920304,-1309842.1498963325,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,null,-1323642.2598920304,-1309842.1498963325,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":4489715967.2293768},4673116910.2003069,4768559208.5437651,4809608785.121047,4846810453.1765003,4862731663.172883,4875336277.8763123,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":4501899298.3991327},4686347523.497673,4781711502.8155107,4822446972.5850821,4859334533.8328247,4874941637.0214968,4887232144.9172153,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":280151279.95133829},263696347.10540566,255115640.94897166,237285158.97669107,217560227.17388594,196363584.73454937,173312533.56685704]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",2331015871.9862885,2353559847.6169648,2418958472.3440499,2423635470.9607983,2423545168.1223111,2419310278.6107135,2412897194.2477441,null,2331015871.9862885,2353559847.6169648,2418958472.3440499,2423635470.9607983,2423545168.1223111,2419310278.6107135,2412897194.2477441,null,0,{"$f":"S31","v":0},0,0,0,0,0]
["DRAB0202","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-86970087.644984454,-86301575.97916013,-81742453.957454666,-84180393.042360485,-85248943.955377132,-87534393.86129491,-89822869.489798769,null,-86970087.644984454,-86301575.97916013,-81742453.957454666,-84180393.042360485,-85248943.955377132,-87534393.86129491,-89822869.489798769,null,0,0,0,0,0,0,0]
["DRAB0205","Actual additions (recognised in RAB)",109514063.27566047,110127606.57392997,86419452.574203148,84090090.203873187,81014054.44377926,81121309.498325557,85618873.897041097,null,109514063.27566047,110127606.57392997,86419452.574203148,84090090.203873187,81014054.44377926,81121309.498325557,85618873.897041097,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":2353559847.6169648},2377385878.2117343,2423635470.9607983,2423545168.1223111,2419310278.6107135,2412897194.2477441,2408693198.6549869,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":2353559847.6169648},2377385878.2117343,2423635470.9607983,2423545168.1223111,2419310278.6107135,2412897194.2477441,2408693198.6549869,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",824037837.74292135,888395138.79743814,970181673.38278663,1016485756.5273188,1059955585.9246492,1100417715.5614021,1140190919.9731352,null,824037837.74292135,888395138.79743814,970181673.38278663,1016485756.5273188,1059955585.9246492,1100417715.5614021,1140190919.9731352,null,0,{"$f":"S38","v":0},0,0,0,0,0]
["DRAB0302","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-29722478.869407676,-29494011.537713986,-27935907.92275222,-28769086.259099398,-29134269.079917848,-29915333.44785342,-30697431.872187745,null,-29722478.869407676,-29494011.537713986,-27935907.92275222,-28769086.259099398,-29134269.079917848,-29915333.44785342,-30697431.872187745,null,0,0,0,0,0,0,0]
["DRAB0305","Actual additions (recognised in RAB)",94079779.923924461,94606853.952122077,74239991.067284465,72238915.656429723,69596398.716670841,69688537.859586641,73552241.352714851,null,94079779.923924461,94606853.952122077,74239991.067284465,72238915.656429723,69596398.716670841,69688537.859586641,73552241.352714851,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":888395138.79743814},953507981.21184623,1016485756.5273188,1059955585.9246492,1100417715.5614021,1140190919.9731352,1183045729.4536622,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":888395138.79743814},953507981.21184623,1016485756.5273188,1059955585.9246492,1100417715.5614021,1140190919.9731352,1183045729.4536622,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",349237542.22501969,362876954.09559989,231027560.34948084,239854116.13441205,247757328.87130287,254758868.24618787,261448823.12634596,null,349237542.22501969,362876954.09559989,231027560.34948084,239854116.13441205,247757328.87130287,254758868.24618787,261448823.12634596,null,0,{"$f":"S45","v":0},0,0,0,0,0]
["DRAB0402","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-12843984.605609704,-12745256.942144904,-12071953.112661434,-12431994.742190026,-12589801.315101847,-12927322.918257238,-13265291.368545581,null,-12843984.605609704,-12745256.942144904,-12071953.112661434,-12431994.742190026,-12589801.315101847,-12927322.918257238,-13265291.368545581,null,0,0,0,0,0,0,0]
["DRAB0405","Actual additions (recognised in RAB)",26483396.4761899,26631767.470173385,20898508.897592627,20335207.479080867,19591340.689986836,19617277.798415329,20704907.803052846,null,26483396.4761899,26631767.470173385,20898508.897592627,20335207.479080867,19591340.689986836,19617277.798415329,20704907.803052846,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":362876954.09559989},376763464.62362832,239854116.13441205,247757328.87130287,254758868.24618787,261448823.12634596,268888439.56085324,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":362876954.09559989},376763464.62362832,239854116.13441205,247757328.87130287,254758868.24618787,261448823.12634596,268888439.56085324,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",274797021.40201426,264830634.81831989,230796718.93723765,222246476.25771537,213250744.22865275,203617822.72117764,193261454.7052418,null,274797021.40201426,264830634.81831989,230796718.93723765,222246476.25771537,213250744.22865275,203617822.72117764,193261454.7052418,null,0,{"$f":"S52","v":0},0,0,0,0,0]
["DRAB0502","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-10284482.056720302,-11046121.003828671,-8758643.3124220204,-9262740.7664636336,-9908604.5666732509,-10575450.565797724,-11105386.363370143,null,-10284482.056720302,-11046121.003828671,-8758643.3124220204,-9262740.7664636336,-9908604.5666732509,-10575450.565797724,-11105386.363370143,null,0,0,0,0,0,0,0]
["DRAB0505","Actual additions (recognised in RAB)",318095.47302593786,313332.80406063638,208400.63289972919,267008.73740099923,275683.0591981539,219082.54986187376,167079.06640266068,null,318095.47302593786,313332.80406063638,208400.63289972919,267008.73740099923,275683.0591981539,219082.54986187376,167079.06640266068,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":264830634.81831989},254097846.61855185,222246476.25771537,213250744.22865275,203617822.72117764,193261454.7052418,182323147.40827432,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":264830634.81831989},254097846.61855185,222246476.25771537,213250744.22865275,203617822.72117764,193261454.7052418,182323147.40827432,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",180817.86914344897,499680.85611626948,739040.96858728479,947689.56275708531,1215263.0926384937,1491485.7850443628,1710656.4773126696,null,180817.86914344897,499680.85611626948,739040.96858728479,947689.56275708531,1215263.0926384937,1491485.7850443628,1710656.4773126696,null,0,{"$f":"S59","v":0},0,0,0,0,0]
["DRAB0602","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-1297.1761595997095,-1393.2412680770017,-1104.722944009339,-1168.3044832537389,-1249.7669350680173,-1333.8758602835053,-1400.7163758231488,null,-1297.1761595997095,-1393.2412680770017,-1104.722944009339,-1168.3044832537389,-1249.7669350680173,-1333.8758602835053,-1400.7163758231488,null,0,0,0,0,0,0,0]
["DRAB0605","Actual additions (recognised in RAB)",320160.16313242022,315366.58069513639,209753.3171138099,268741.83436466212,277472.45934093685,220504.56812859038,168163.54111121385,null,320160.16313242022,315366.58069513639,209753.3171138099,268741.83436466212,277472.45934093685,220504.56812859038,168163.54111121385,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":499680.85611626948},813654.19554332888,947689.56275708531,1215263.0926384937,1491485.7850443628,1710656.4773126696,1877419.3020480603,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":499680.85611626948},813654.19554332888,947689.56275708531,1215263.0926384937,1491485.7850443628,1710656.4773126696,1877419.3020480603,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",305856118.3710919,365049713.50185734,331124544.06449687,367345005.22720021,416034677.18052953,466223491.51938397,503831910.01446891,null,305856118.3710919,365049713.50185734,331124544.06449687,367345005.22720021,416034677.18052953,466223491.51938397,503831910.01446891,null,0,{"$f":"S66","v":0},0,0,0,0,0]
["DRAB0702","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-10277527.84859455,-11038651.787195377,-8752720.8529186733,-9256477.4440377075,-9901904.5211082529,-10568299.609254405,-11097877.072414912,null,-10277527.84859455,-11038651.787195377,-8752720.8529186733,-9256477.4440377075,-9901904.5211082529,-10568299.609254405,-11097877.072414912,null,0,0,0,0,0,0,0]
["DRAB0705","Actual additions (recognised in RAB)",69471122.979359984,68432938.390821248,44973182.015622012,57946149.397367075,60090718.859962694,48176718.104339361,37041952.96979738,null,69471122.979359984,68432938.390821248,44973182.015622012,57946149.397367075,60090718.859962694,48176718.104339361,37041952.96979738,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":365049713.50185734},422444000.10548317,367345005.22720021,416034677.18052953,466223491.51938397,503831910.01446891,529775985.91185135,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":365049713.50185734},422444000.10548317,367345005.22720021,416034677.18052953,466223491.51938397,503831910.01446891,529775985.91185135,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",0,{"$f":"C72","v":0},0,0,0,0,0,null,0,{"$f":"K72","v":0},0,0,0,0,0,null,0,{"$f":"S72","v":0},0,0,0,0,0]
["DRAB0802","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0804","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",{"$f":"SUM(C68+C69+C70+C71)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(K68+K69+K70+K71)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(S68+S69+S70+S71)","v":0},0,0,0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",0,{"$f":"C79","v":0},0,0,0,0,0,null,0,{"$f":"K79","v":0},0,0,0,0,0,null,270869393.62086433,247681737.12275246,231920707.134987,212825410.5936994,189550926.09943604,164997407.08062443,140538088.35504508]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0903","Straight line depreciation",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-37805311.935799249,-30186619.834386546,-33978829.290832952,-35900054.065428957,-36490138.869828105,-37244596.257699199,-37741812.787988678]
["DRAB0905","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,14617655.437687365,9728187.0702574309,14883532.749545339,12625569.571165619,11936619.851016479,12785277.53211985,13596829.434034845]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":247681737.12275246},227223304.35862333,212825410.5936994,189550926.09943604,164997407.08062443,140538088.35504508,116393105.00109124]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",78387055.362492323,117563487.45061609,345770775.50937724,324725223.61937743,289428429.97824943,250444419.12248167,212935137.56235111,null,90856371.978579864,129746818.62037234,359237176.58883405,337877517.89112359,302266617.44228494,262968499.77880657,225145111.41096535,null,30390642.570386503,32469542.828585811,36473042.746782295,42290230.355272278,47734232.877255015,52562820.093261503,55825496.379504271]
["DRAB1002","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1003","Straight line depreciation",-7038446.6418092595,-9084539.7800441347,-55600752.511486277,-59345846.228430934,-61584804.632151589,-63777273.367895789,-66205186.837024033,null,-7324432.0881405482,-9368583.1814982221,-55914859.319196917,-59659953.036141574,-61898911.439862229,-64091380.17560643,-66519293.644734673,null,-1417249.3476625688,-1593947.4904850901,-1875501.1036934357,-2208365.515586135,-2535690.9930430655,-2823863.1263029892,-3014768.3618691978]
["DRAB1005","Actual additions (recognised in RAB)",46214878.729933023,30854783.989109635,34555200.621486507,24049052.587302927,22600793.776383843,26267991.807765212,29344083.442763735,null,46214878.729933023,32186109.518173657,34555200.621486507,24049052.587302927,22600793.776383843,26267991.807765212,29344083.442763735,null,3496149.6058618752,5597447.4086815771,7692688.7121834178,7652368.0375688747,7364278.2090495555,6086539.4125457574,4108700.5481306878]
["DRAB1006","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":117563487.45061609},139333731.65968159,324725223.61937743,289428429.97824943,250444419.12248167,212935137.56235111,176074034.16809082,null,129746818.62037234,152564344.95704779,337877517.89112359,302266617.44228494,262968499.77880657,225145111.41096535,187969901.20899442,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":32469542.828585811},36473042.746782295,42290230.355272278,47734232.877255015,52562820.093261503,55825496.379504271,56919428.565765761]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",114404106.52981253,136940510.09246555,172912478.88544673,173156666.98280618,158258784.45133394,150383568.33872935,136292763.7949031,null,114404106.52981253,136940510.09246555,172912478.88544673,173156666.98280618,158258784.45133394,150383568.33872935,136292763.7949031,null,0,{"$f":"S93","v":0},0,0,0,0,0]
["DRAB1102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1103","Straight line depreciation",-47187856.419882871,-49858669.065853909,-52470114.311129838,-53486102.321112797,-51868584.978553034,-50813323.470349088,-48606509.926282972,null,-47187856.419882871,-49858669.065853909,-52470114.311129838,-53486102.321112797,-51868584.978553034,-50813323.470349088,-48606509.926282972,null,0,0,0,0,0,0,0]
["DRAB1105","Actual additions (recognised in RAB)",71047902.2424279,62998354.697123587,54377265.700483702,40251183.081634976,45656332.157942861,38385482.218517251,38472229.568539418,null,71047902.2424279,62998354.697123587,54377265.700483702,40251183.081634976,45656332.157942861,38385482.218517251,38472229.568539418,null,0,0,0,0,0,0,0]
["DRAB1106","Disposals ",-1323642.2598920304,-1309842.1498963325,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,null,-1323642.2598920304,-1309842.1498963325,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,-1662963.2919944129,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":136940510.09246555},148770353.57383889,173156666.98280618,158258784.45133394,150383568.33872935,136292763.7949031,124495520.14516513,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":136940510.09246555},148770353.57383889,173156666.98280618,158258784.45133394,150383568.33872935,136292763.7949031,124495520.14516513,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":0},0,0,0,0,0,0]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",2342287859.8016267,2365472862.9143496,2421296971.6524239,2423590319.5415545,2421427723.3665123,2416103736.4292288,2410795196.4513655,null,2342287859.8016267,2365472862.9143496,2421296971.6524239,2423590319.5415545,2421427723.3665123,2416103736.4292288,2410795196.4513655,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",856216488.27017975,920951560.00464225,993333714.95505273,1038220671.2259841,1080186650.7430258,1120304317.7672687,1161618324.7133987,null,856216488.27017975,920951560.00464225,993333714.95505273,1038220671.2259841,1080186650.7430258,1120304317.7672687,1161618324.7133987,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",356057248.16030979,294967019.54492098,235440838.24194646,243805722.50285745,251258098.55874538,258103845.6862669,265168631.34359962,null,356057248.16030979,294967019.54492098,235440838.24194646,243805722.50285745,251258098.55874538,258103845.6862669,265168631.34359962,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",269813828.11016709,259464240.71843588,226521597.59747651,217748610.24318406,208434283.47491521,198439638.71320972,187792301.05675805,null,269813828.11016709,259464240.71843588,226521597.59747651,217748610.24318406,208434283.47491521,198439638.71320972,187792301.05675805,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",340249.36262985924,656667.52582979924,843365.26567218499,1081476.3276977895,1353374.4388414281,1601071.1311785162,1794037.8896803651,null,340249.36262985924,656667.52582979924,843365.26567218499,1081476.3276977895,1353374.4388414281,1601071.1311785162,1794037.8896803651,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",335452915.93647462,363799826.88552594,349234774.64584851,391689841.20386487,441129084.34995675,485027700.76692641,516803947.96316016,null,335452915.93647462,363799826.88552594,349234774.64584851,391689841.20386487,441129084.34995675,485027700.76692641,516803947.96316016,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,259275565.37180841,237452520.74068791,222373058.8643432,201188168.34656772,177274166.59003025,152767747.71783477,128465596.67806816]
["DRAB1209","“Other” assets with long lives",97975271.406554207,233248829.28798634,335247999.56437731,307076826.79881346,269936424.55036557,231689778.34241641,194504585.86522096,null,110301595.2994761,245955801.52154753,348557347.23997879,320072067.6667043,282617558.61054575,244056805.59488595,206557506.30997989,null,31430092.699486159,34471292.787684053,39381636.551027283,45012231.616263643,50148526.485258259,54194158.236382887,56372462.472635016]
["DRAB1210","“Other” assets with short lives",125672308.31113905,142855431.83315223,173034572.93412644,165707725.71707004,154321176.39503163,143338166.06681621,130394141.97003412,null,125672308.31113905,142855431.83315223,173034572.93412644,165707725.71707004,154321176.39503163,143338166.06681621,130394141.97003412,null,0,0,0,0,0,0,0]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",68462514.291257992,70471995.830687955,72320594.377096742,70447447.43860355,68807592.119885251,69877527.723339319,70807211.973137051,null,68462514.291257992,70471995.830687955,72320594.377096742,70447447.43860355,68807592.119885251,69877527.723339319,70807211.973137051,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)","                     64 ","                      64 ","                      64 ","                      64 ","                      64 ","                      64 ","                      64 ",null,"                     64 ","                      64 ","                      64 ","                      64 ","                      64 ","                      64 ","                      64 ",null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)","                    50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ",null,"                    50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ",null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers","                     52 ","                      52 ","                      52 ","                      52 ","                      52 ","                      52 ","                      52 ",null,"                     52 ","                      52 ","                      52 ","                      52 ","                      52 ","                      52 ","                      52 ",null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ","                     72 ","                      72 ","                      72 ","                      72 ","                      72 ","                      72 ","                      72 ",null,"                     72 ","                      72 ","                      72 ","                      72 ","                      72 ","                      72 ","                      72 ",null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)","                     50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ",null,"                     50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ","                      50 ",null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers","                     46 ","                      46 ","                      46 ","                      46 ","                      46 ","                      46 ","                      46 ",null,"                     46 ","                      46 ","                      46 ","                      46 ","                      46 ","                      46 ","                      46 ",null,0,0,0,0,0,0,0]
["DRAB1407","Meters","                      -   ","                       -   ","                       -   ","                       -   ","                       -   ","                       -   ","                       -   ",null,"                      -   ","                       -   ","                       -   ","                       -   ","                       -   ","                       -   ","                       -   ",null,14.768157511119092,14.764933835947648,14.034908348725091,14.308705628423926,14.118701200182608,13.868757208858524,13.51652885306726]
["DRAB1408","“Other” assets with long lives",10.119613805676611,9.8888497289345327,10.584878412266356,10,10,10,9.0051501443060982,null,10.119613805676611,12.967737727376523,10.584878412266356,10,10,10,9.0051501443060982,null,29.762461706682615,29.355054450641102,28.619004868274757,28.103904583825901,27.693728085675296,27.608447591592334,27.801971089396705]
["DRAB1409","“Other” assets with short lives",5,5,5,5,5,5,5,null,5,5,5,5,5,5,5,null,0,0,0,0,0,0,0]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",35,35,34,34,33,33,32,null,35,35,34,34,33,33,32,null,0,0,0,0,0,0,0]
["DRAB1502","Underground network assets less than 33kV (cables)",26,25,24,23,22,21,20,null,26,25,24,23,22,21,20,null,0,0,0,0,0,0,0]
["DRAB1503","Distribution substations including transformers",24,23,22,21,20,19,19,null,24,23,22,21,20,19,19,null,0,0,0,0,0,0,0]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",38,38,37,37,36,36,35,null,38,38,37,37,36,36,35,null,0,0,0,0,0,0,0]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",18,17,16,15,14,13,12,null,18,17,16,15,14,13,12,null,0,0,0,0,0,0,0]
["DRAB1506","Zone substations and transformers",13,12,11,10,10,9,8,null,13,12,11,10,10,9,8,null,0,0,0,0,0,0,0]
["DRAB1507","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,7.9224887482071367,7.0187366074176518,5.8866002127094177,5.81506282727561,5.6562185878062019,5.9081877221342545,6.8145629381571116]
["DRAB1508","“Other” assets with long lives",9.095668604200549,6.5165615414332958,6.0765708174079229,5.598987996541501,5.335733932870764,5.4748240619660296,6.157860642016546,null,12.461844606923933,7.8794912886481061,7.4894917732050743,7.1330696780177565,7.0328421286976708,7.3777187481127076,8.3454327761914868,null,25.211008781783256,24.599617710958345,23.829332840406249,23.174869607120062,22.542961516142189,22.098542362740986,21.759507638947355]
["DRAB1509","“Other” assets with short lives",3.8593164612431945,3.6522874674735601,3.5987985697427707,3.4715656141747391,3.512591685725845,3.5092630048374605,3.5609462916773924,null,3.8593164612431945,3.6522874674735601,3.5987985697427707,3.4715656141747391,3.512591685725845,3.5092630048374605,3.5609462916773924,null,0,0,0,0,0,0,0]

{"sheet":"3.4 Operational data","index":23,"n_rows":87,"n_cols":10,"rows_kept":87,"cut":false,"hidden":false,"merged":[[8,3,8,9],[9,3,9,9],[43,3,43,9],[44,3,44,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPED01","Total energy delivered","GWh"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",2139.106292987603,2091.1028599342217,2049.6552460249613,2015.3264015327504,1988.4587723500376,1966.8636081540637,1947.1368627226866]
["DOPED0202","Energy Delivery at On-peak times","GWh",2120.240408196189,2127.3204846171025,2128.2282988651991,2123.3138654545946,2120.2905171096718,2116.8836869040997,2114.1318905015755]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",469.40639832002074,476.67077136331039,482.4019172572535,488.44664528023037,494.8270171624365,501.18286108904516,507.357120617156]
["DOPED0204","Energy Delivery at Off-peak times","GWh",2340.8046117156541,2345.4413920260595,2343.9254501527307,2336.369703270037,2330.5535042616216,2324.4540921259345,2319.8021185637813]
["DOPED0205","Controlled load energy deliveries","GWh",0,0,0,0,0,0,0]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",295.3994447683616,295.46143717484938,295.35962712359105,295.07064223778917,294.88952293544457,294.71170317900231,294.54598423588351]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",0,0,0,0,0,0,0]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",0,0,0,0,0,0,0]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",0,0,0,0,0,0,0]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",6493.2740040315748,6396.4384752360538,6297.1162578442081,6200.1928904280903,6122.2444874589573,6057.0056648864684,5995.7185574795203]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",1043.2451643649051,1048.6815875746429,1054.7772361140912,1060.1594524664786,1066.0202046240761,1071.0628995312322,1076.4736764858794]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",322.48841906178831,382.9846270258746,437.34126185794963,485.08589719772885,525.6861960328456,559.28705002864342,592.62451748602689]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",3031.617397657481,2970.514116160025,2925.1894998938355,2871.1470369780809,2825.3672401844324,2784.982201687525,2747.662161730429]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",942.35156095666389,948.28648167118354,940.09740949631669,938.29476260229694,936.55281180784095,934.11156240803575,933.08702893184636]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",2393.6870027059203,2423.389187423365,2445.2852886760147,2466.6691369907976,2490.3796208737226,2513.9862600856995,2536.7982032430477]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",997.3011946677625,993.80715986096959,988.99834135756805,982.41632120422571,976.71966095321659,971.0159272708853,965.42658273575921]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2050.6966891748002,2079.1943012281931,2107.873191577035,2136.4334658101334,2165.3843494392599,2194.5421509696162,2223.3154070373589]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1962.4724966286194,1989.340722087406,2016.4070366430965,2043.3341248117777,2070.6560729888856,2098.1115322433257,2125.2548256206992]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",0,0,0,0,0,0,0]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",0,0,0,0,0,0,0]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2206.7960140317664,2222.5373934940844,2262.3332519106125,2278.6221885822329,2320.0186291116952,2379.0905451729659,2400.4955301506634]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1957.1840823245859,1968.2185976070373,2011.8429086400104,2038.1592544390846,2069.6790825272769,2120.2401160115369,2121.3590592527371]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",1986.6460284692885,1979.2879330583744,1999.526458677022,2048.7870613375844,2063.7573198604127,2102.4122303662598,2157.222763022678]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1798.8624616176244,1801.7063572280299,1809.9186783776549,1864.680782605079,1884.4578699687627,1915.6547251132677,1964.5277221430356]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2071.2036560665483,2099.9862442404751,2128.9519234928052,2157.7978004682345,2187.0381929336527,2216.4875724793123,2245.5485611077324]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",1982.0972215949057,2009.23412930828,2036.5711070095274,2063.7674660598955,2091.3626337187743,2119.0926475657589,2146.5073738769061]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",0,0,0,0,0,0,0]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",0,0,0,0,0,0,0]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2427.4756154349434,2444.791132843493,2488.5665771016738,2506.4844074404564,2552.0204920228648,2616.9995996902626,2640.5450831657299]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2152.9024905570445,2165.0404573677411,2213.0271995040116,2241.9751798829934,2276.6469907800047,2332.2641276126906,2333.4949651780112]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2185.3106313162175,2177.2167263642118,2199.4791045447246,2253.6657674713429,2270.1330518464542,2312.653453402886,2372.9450393249458]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",1978.7487077793869,1981.876992950833,1990.9105462154207,2051.1488608655873,2072.9036569656391,2107.2201976245947,2160.9804943573395]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.99009900990098998,0.99009900990098998,0.99009900990098998,0.99009900990098998,0.99009900990098998,0.99009900990098998,0.99009900990098998]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.9,0.9,0.9,0.9,0.9,0.9,0.9]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0.99859932928511697,0.99859932928511697,0.99859932928511697,0.99859932928511697,0.99859932928511697,0.99859932928511697,0.99859932928511697]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.94395604099999997,0.94395604099999997,0.94395604099999997,0.94395604099999997,0.94395604099999997,0.94395604099999997,0.94395604099999997]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.98963820508626754,0.98934569399718209,0.98905318290809641,0.98876067181901084,0.98846816072992516,0.98817564964083948,0.9878831385517538]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0.97385478604789388,0.97688086690000175,0.97990694775210962,0.98293302860421738,0.98595910945632514,0.98898519030843257,0.99201127116054133]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.96347682107695887,0.95937318218168033,0.95526954328640201,0.95116590439112381,0.94706226549584516,0.94295862660056629,0.93885498770528875]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW ",0,0,0,0,0,0,0]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW ",0,0,0,0,0,0,0]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA",1207.268925518925,1231.3566799804694,1255.9250398007166,1280.9835941471076,1306.5421235127328,1332.6106035337125,1359.1992088827428]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA",556.98260073260064,564.60217649424931,572.32598878808244,580.15546357992582,588.0920463429552,596.13720232455898,604.29241681685141]

{"sheet":"3.5 Physical assets","index":24,"n_rows":95,"n_cols":10,"rows_kept":95,"cut":false,"hidden":false,"merged":[[8,3,8,9],[75,3,75,9],[91,3,91,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",7454.3,7454.3,7454.3,7454.3,7454.3,7454.3,7454.3]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",51.7,51.7,51.7,51.7,51.7,51.7,51.7]
["DPA0104","Overhead 11 kV","km",3.2,3.2,3.2,3.2,3.2,3.2,3.2]
["DPA0105","Overhead SWER","km",6494.9,6494.9,6492.2,6486.7,6475,6449.4,6392.4]
["DPA0106","Overhead 22 kV","km",22744.2,22744.2,22742.600000000002,22741.000000000004,22739.400000000005,22737.800000000007,22736.200000000008]
["DPA0107","Overhead 33 kV","km",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",2720.2,2720.2,2720.2,2720.2,2720.2,2720.2,2720.2]
["DPA0110","Overhead 132 kV","km",0,0,0,0,0,0,0]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0112","Overhead 110kV","km",0,0,0,0,0,0,0]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D13:D26)","v":39468.800000000003},39468.800000000003,39464.5,39457.4,39444.100000000006,39416.900000000009,39358.300000000003]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",4695.194306041667,4947.888612083334,5200.582918125001,5453.277224166668,5705.971530208335,5958.665836250002,6211.360142291669]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",13.297862605000001,14.695725210000001,16.093587814999999,17.49145042,18.889313025,20.28717563,21.685038235]
["DPA0204","Underground 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0205","Underground 11 kV","km",2.0481588374999999,2.0963176749999999,2.1444765124999998,2.1926353499999998,2.2407941874999997,2.2889530249999996,2.3371118624999996]
["DPA0206","Underground SWER","km",29.629361666666668,33.258723333333336,39.594022500000001,48.686743541666672,63.983663802083342,93.240032304687503,153.90515935221356]
["DPA0207","Underground 22 kV","km",2142.6713039850001,2257.4426079700002,2373.8139119550001,2490.18521594,2606.556519925,2722.9278239099999,2839.2991278949999]
["DPA0208","Underground 33 kV","km",1.1395908333333333E-2,1.2791816666666666E-2,1.4187724999999998E-2,1.5583633333333331E-2,1.6979541666666664E-2,1.8375449999999998E-2,1.9771358333333332E-2]
["DPA0209","Underground 66 kV","km",12.694112951666666,13.788225903333332,14.882338854999999,15.976451806666665,17.070564758333333,18.164677709999999,19.258790661666666]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",0,0,0,0,0,0,0]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D29:D40)","v":6895.5465019958328},7269.1830039916676,7647.1254434875009,8027.8253048583356,8414.7293654479163,8815.5928742796896,9247.8651416563825]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
["DPA0302","Overhead 6.6 kV","MVA",2.57,2.57,2.57,2.57,2.57,2.57,2.57]
["DPA0303","Overhead 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0304","Overhead 11 kV","MVA",6,6,6,6,6,6,6]
["DPA0305","Overhead SWER","MVA",0.35,0.35,0.35,0.35,0.35,0.35,0.35]
["DPA0306","Overhead 22 kV","MVA",4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996]
["DPA0307","Overhead 33 kV","MVA",1.43,1.43,1.43,1.43,1.43,1.43,1.43]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",39.74,39.74,39.74,39.74,39.74,39.74,39.74]
["DPA0310","Overhead 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0311","Overhead 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.18,0.18,0.18,0.18,0.18,0.18,0.18]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",3.49,3.49,3.49,3.49,3.49,3.49,3.49]
["DPA0404","Underground 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0405","Underground 11 kV","MVA",6,6,6,6,6,6,6]
["DPA0406","Underground SWER","MVA",1.43,1.43,1.43,1.43,1.43,1.43,1.43]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",11.07,11.07,11.07,11.07,11.07,11.07,11.07]
["DPA0409","Underground 33 kV","MVA",1.43,1.43,1.43,1.43,1.43,1.43,1.43]
["DPA0410","Underground 66 kV","MVA",55.2,55.2,55.2,55.2,55.2,55.2,55.2]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",6006.8180000000002,6104.518,6202.2179999999998,6299.9179999999997,6397.6179999999995,6495.3179999999993,6593.0179999999991]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",368.19988000000001,373.79988000000003,379.39988000000005,384.99988000000008,390.5998800000001,396.19988000000012,401.79988000000014]
["DPA0503","Cold spare capacity included in DPA0501","MVA",62.902000000000001,62.902000000000001,62.902000000000001,62.902000000000001,62.902000000000001,62.902000000000001,62.902000000000001]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",0,0,0,0,0,0,0]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",0,0,0,0,0,0,0]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",3443.9,3463.3,3482.7000000000003,3502.1000000000004,3521.5000000000005,3540.9000000000005,3560.3000000000006]
["DPA0604","Total zone substation transformer  capacity ","MVA",3534.4,3553.8,3573.2000000000003,3592.6000000000004,3612.0000000000005,3631.4000000000005,3650.8000000000006]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",90.5,90.5,90.5,90.5,90.5,90.5,90.5]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DPA0701","Public lighting luminaires","0's",178957.92590226419,182195.93717952899,187600.34843500599,192160.6981822683,196768.54864784333,201417.4282378614,206271.37005096188]
["DPA0702","Public lighting poles","0's",178957.92590226419,182195.93717952899,187600.34843500599,192160.6981822683,196768.54864784333,201417.4282378614,206271.37005096188]

{"sheet":"3.6 Quality of service","index":25,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[6,3,6,9],[13,3,13,9],[18,3,18,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DQS0201","Energy Not Supplied (planned)","GWh",3.0126491680397165,3.0126491680397165,3.0126491680397165,3.0126491680397165,3.0126491680397165,3.0126491680397165,3.0126491680397165]
["DQS0202","Energy Not Supplied (unplanned)","GWh",2.9797214896634729,2.9797214896634729,2.9797214896634729,2.9797214896634729,2.9797214896634729,2.9797214896634729,2.9797214896634729]
["DQS02","Total",null,{"$f":"SUM(D9:D10)","v":5.992370657703189},5.992370657703189,5.992370657703189,5.992370657703189,5.992370657703189,5.992370657703189,5.992370657703189]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DQS03","System losses","%",6.2864226299878798E-2,6.2864226299878798E-2,6.2864226299878798E-2,6.2864226299878798E-2,6.2864226299878798E-2,6.2864226299878798E-2,6.2864226299878798E-2]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DQS04","Overall utilisation","%",0.52478776813651096,0.52227575673885052,0.51976374534119052,0.51725173394352997,0.51473972254586953,0.51222771114820898,0.50971569975054853]

{"sheet":"3.7 Operating Environment","index":26,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[8,3,8,9],[15,3,15,9],[33,3,33,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOEF0101","Customer density","Customer / km",19.187687391884548]
["DOEF0102","Energy density","MWh/customer",9.9501225592470703]
["DOEF0103","Demand density","kVA / customer",2.3714246222736675]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOEF0201","Rural proportion","%",0.93160574154659614]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",9123.25]
["DOEF0203","Rural vegetation maintenance spans","0's",61531.807638888902]
["DOEF0204","Total vegetation maintenance spans","0's",70655.057638888873]
["DOEF0205","Total number of spans","0's",313873.91875000001]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",0.75902777777777874]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",5.631571146223715]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",6.4894567374601158]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",2.7367096637445895E-2]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",4.3467568827692357E-2]
["DOEF0212","Tropical proportion","Spans",0]
["DOEF0213","Standard vehicle access","km",2089.3116385328117,2107.0821537705615,2125.3208246713202,2143.7173674973055,2162.2731487705028,2180.9895468413615,2199.8679519911807]
["DOEF0214","Bushfire risk","Spans",52258.734722222223]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOEF0301","Route Line length","km",39204.933981567439,39361.116792444285,39517.921797211951,39675.35147453782,39833.408312963656,39992.094810944982,40151.413476890535]

{"sheet":"4.1 Public lighting","index":27,"n_rows":165,"n_cols":10,"rows_kept":165,"cut":false,"hidden":false,"merged":[[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[5,1,5,2],[8,3,8,9],[31,3,31,9],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[95,1,95,2],[93,1,93,2],[96,1,96,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[156,1,156,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[212,1,212,2],[213,1,213,2],[214,1,214,2],[215,1,215,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's",4443.134708044643,3238.011277264799,5404.4112554765306,4560.3497472627787,4607.8504655750294,4648.8795900180703,4853.9418131004786]
[null,"Number of poles installed ","0's",3554.5077664357145,2590.4090218118395,4323.5290043812247,3648.279797810223,3686.2803724600235,3719.1036720144566,3883.1534504803831]
[null,"Total expenditure","$0's",2363301.640978395,2363264.7295210287,2368715.6530517163,2369071.6530517167,2119391.6930777859,2369783.6530517172,2370139.6530517167]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's",2648.90548972735,5292.9002477630202,8254.1792933897232,8181.1792933897232,8111.815620092284,5352.7369619435985,2178.8753089046172]
[null,"Number of poles replaced","0's",817,817,817,817,817,817,817]
[null,"Total expenditure","$0's",1132847.9648834807,3234182.6791605493,5323973.0591317015,5283296.3845171584,5244886.5159717696,3716755.7594940397,1738560.8950789711]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's",178957.92590226419,182195.93717952899,187600.34843500599,192160.6981822683,196768.54864784333,201417.4282378614,206271.37005096188]
[null,"Number of poles maintained","0's",178957.92590226419,182195.93717952899,187600.34843500599,192160.6981822683,196768.54864784333,201417.4282378614,206271.37005096188]
[null,"Total expenditure","$0's",8589233.2387688234,8326637.6155471932,7863349.7467969749,7733448.8846003013,7337143.5510646179,7237510.1244625803,7207299.587155167]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days",1.7,1.7,1.7,1.7,1.7,1.7,1.7]
[null,"GSO breaches","0's",33,33,33,33,33,33,33]
[null,"GSL payments ","$0's",825,825,825,825,825,825,825]
[null,"Customer complaints ","0's",0,0,0,0,0,0,0]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"LIGHT INSTALLATION"]
[null,"Mercury Vapour 80W",null,288.27999999999997,288.27999999999997,0,0,0,0,0]
[null,"HP Sodium 150W",null,436.07,436.07,0,0,0,0,0]
[null,"HP Sodium 250W",null,443.02,443.02,0,0,0,0,0]
[null,"T5 2X14W",null,451.38,451.38,415.98484478423143,416.78005682944001,416.78005682944001,416.78005682944001,416.78005682944001]
[null,"T5 2X24W",null,496.49,496.49,458.02964951375588,458.94659020699112,458.94659020699112,458.94659020699112,458.94659020699112]
[null,"LED 18W standard output power",null,585.89,585.89,535.51943566977832,536.30084535140986,536.29109322963518,536.28134128519355,536.27158951808178]
[null,"LED 70W-125W (L1)",null,1040.28,1040.28,940.50125456849059,940.68679419240902,941.75695954580601,942.82834236487872,943.90094403466799]
[null,"LED 155W-250W (L2)",null,1050.54,1050.54,1048.6634160290798,1049.3418834864242,1049.3296053145966,1049.3173272864337,1049.305049401934]
[null,"LED 275W-400W (L4)",null,0,0,1157.6700557355093,1157.983225324956,1157.983225324956,1157.983225324956,1157.983225324956]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"Mercury Vapour 80W",null,288.27999999999997,288.27999999999997,0,0,0,0,0]
[null,"HP Sodium 150W",null,436.07,436.07,0,0,0,0,0]
[null,"HP Sodium 250W",null,443.02,443.02,0,0,0,0,0]
[null,"T5 2X14W",null,451.38,451.38,415.98484478423143,416.78005682944001,416.78005682944001,416.78005682944001,416.78005682944001]
[null,"T5 2X24W",null,496.49,496.49,458.02964951375588,458.94659020699112,458.94659020699112,458.94659020699112,458.94659020699112]
[null,"LED 18W standard output power",null,585.89,585.89,535.51943566977832,536.30084535140986,536.29109322963518,536.28134128519355,536.27158951808178]
[null,"LED 70W-125W (L1)",null,1040.28,1040.28,940.50125456849059,940.68679419240902,941.75695954580601,942.82834236487872,943.90094403466799]
[null,"LED 155W-250W (L2)",null,1050.54,1050.54,1048.6634160290798,1049.3418834864242,1049.3296053145966,1049.3173272864337,1049.305049401934]
[null,"LED 275W-400W (L4)",null,0,0,1157.6700557355093,1157.983225324956,1157.983225324956,1157.983225324956,1157.983225324956]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"Mercury Vapour 80W",null,37.206089097210651,36.878956265360721,37.224374623231171,36.495142930587591,36.621527928970856,40.804985489386425,41.330641903751875]
[null,"HP Sodium 150W",null,92.944819454026572,92.558839969039795,93.380922935975718,93.822679541522348,92.866960055043805,94.294337485708425,95.618890037140901]
[null,"HP Sodium 250W",null,94.537800203558518,94.099350513064508,94.899714175886643,95.380652493922312,94.294463807393242,95.089471632161647,96.458224039534713]
[null,"T5 2X14W",null,53.868778480098193,49.801894181156342,46.610394104312483,49.376704242403378,46.04730455821511,46.336590060151963,46.995783326713045]
[null,"T5 2X24W",null,58.511777926703324,54.345581527245045,51.059620228288324,51.276667296042653,50.199647650678834,50.309200526883167,49.989888688548376]
[null,"LED 18W standard output power",null,18.014413650278296,17.198217393337579,16.310738257511417,16.354475328553988,16.074558569804076,16.188512789830863,16.402403718245953]
[null,"LED 70W-125W (L1)",null,15.294148880998158,17.800474943755702,20.58925566303083,20.6418248316185,20.427104656722612,20.609949482247849,20.915364064545344]
[null,"LED 155W-250W (L2)",null,15.582093336215523,18.420106229783723,21.522520448697961,21.664560148579199,21.339276277028265,21.526486449589406,21.834867502248237]
[null,"LED 275W-400W (L4)",null,16.153325826041023,25.212369609723158,34.115361513851163,34.142402863056617,33.235274087010779,33.480591040104677,33.943092953575231]

{"sheet":"4.2 Metering","index":28,"n_rows":92,"n_cols":11,"rows_kept":92,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,4,8,10],[10,1,13,1],[14,1,17,1],[18,1,21,1],[26,4,26,10],[27,2,27,3],[28,1,30,1],[31,1,33,1],[34,1,36,1],[37,1,39,1],[40,1,42,1],[43,1,45,1],[46,1,48,1],[49,1,51,1],[54,1,56,1],[64,4,64,10],[65,2,65,3],[84,1,86,1],[87,1,89,1],[66,1,68,1],[69,1,71,1],[72,1,74,1],[75,1,77,1],[78,1,80,1],[81,1,83,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.2 METERING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.2.1 - METERING DESCRIPTOR METRIC"]
[null,null,null,null,"VOLUMES (0's)"]
[null,"ASSET CATEGORY","ASSET SUBCATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Meter Type 4","Single phase meter population ",null,632200,646017,660883,675906,691187,706517,722055]
[null,null,"Multi phase meter population ",null,133226,135266.5,137446.5,139644.5,141876.5,144111.5,146377.5]
[null,null,"Current transformer connected meter population ",null,4370,4440,4516,4594,4672,4752,4832]
[null,null,"Direct connect meter population ",null,761056,776843.5,793813.5,810956.5,828391.5,845876.5,863600.5]
[null,"Meter Type 5","Single phase meter population ",null,902,902,902,902,902,902,902]
[null,null,"Multi phase meter population ",null,303,303,303,303,303,303,303]
[null,null,"Current transformer connected meter population ",null,39,39,39,39,39,39,39]
[null,null,"Direct connect meter population ",null,1166,1166,1166,1166,1166,1166,1166]
[null,"Meter Type 6","Single phase meter population ",null,2662,2342,2142,1982,1862,1782,1702]
[null,null,"Multi phase meter population ",null,1259,1179,1129,1089,1059,1039,1019]
[null,null,"Current transformer connected meter population ",null,29,29,29,29,29,29,29]
[null,null,"Direct connect meter population ",null,3892,3492,3242,3042,2892,2792,2692]
[]
[]
[null,"4.2.2 - COST METRICS"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"}]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Meter purchase ",null,"Meter Type 4",1575289.0502222227,1740727.4938666672,1891429.6333333335,1916968.5142222226,1955126.1868444451,1967041.3130666672,1993712.798933334]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4",84943.003811893883,84943.003811893883,84943.003811893883,84943.003811893883,84943.003811893883,84943.003811893883,84943.003811893883]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",75434.45860906993,75434.45860906993,75434.45860906993,75434.45860906993,75434.45860906993,75434.45860906993,75434.45860906993]
[null,"Meter investigation ",null,"Meter Type 4",721708.54006591171,721708.54006591171,721708.54006591171,721708.54006591171,721708.54006591171,721708.54006591171,721708.54006591171]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",8499.7793797912509,8499.7793797912509,8499.7793797912509,8499.7793797912509,8499.7793797912509,8499.7793797912509,8499.7793797912509]
[null,"Scheduled meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",2371641.2821282349,2379181.9941940643,2474343.304863112,2764320.6073294049,2992200.7481221044,3091289.6119666062,3173612.1820619185]
[null,null,null,"Meter Type 6",86236.77401393895,86236.77401393895,86236.77401393895,86236.77401393895,86236.77401393895,86236.77401393895,86236.77401393895]
[null,"Special meter reading ",null,"Meter Type 4",420903.03460979153,420903.03460979153,420903.03460979153,420903.03460979153,420903.03460979153,420903.03460979153,420903.03460979153]
[null,null,null,"Meter Type 5",182578.38301295848,182578.38301295848,182578.38301295848,182578.38301295848,182578.38301295848,182578.38301295848,182578.38301295848]
[null,null,null,"Meter Type 6",940203.84531058336,940203.84531058336,940203.84531058336,940203.84531058336,940203.84531058336,940203.84531058336,940203.84531058336]
[null,"New meter installation ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4",3862276.9032009253,3870219.0850055059,4267069.2574333986,4893563.842684947,5548947.2651909878,6229056.72865126,6814198.3631117269]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4",1187034.8455060967,1189708.0377238195,1195024.5239818159,1198929.8148570708,1203090.5629907707,1206956.2027954075,1210532.5391039401]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4",1960266.9554352791,1960266.9554352791,1960266.9554352791,1960266.9554352791,1960266.9554352791,1960266.9554352791,1960266.9554352791]
[null,"Remote meter re-configuration ",null,"Meter Type 4",26368.876475832643,26368.876475832643,26368.876475832643,26368.876475832643,26368.876475832643,26368.876475832643,26368.876475832643]
[null,"Other metering ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 7",0,0,0,0,0,0,0]
[null,"IT infrastructure capex ",null,"Meter Type 4",0,0,1376038.3268840984,928594.06670351967,166773.5397088631,1378.2937166021745,171660.21743136176]
[null,"IT infrastructure opex ",null,"Meter Type 4",7728014.5418095021,7751409.7683606483,2057932.9519961884,2025378.5530902389,1921542.9119749367,1780518.2255650794,1752356.5713849552]
[null,"Communications infrastructure capex ",null,"Meter Type 4",2512414.9825537042,9391811.2853322364,5364724.6857754756,3614227.1376456777,3071895.642630605,3242747.3215599735,3183991.7953002066]
[null,"Communications infrastructure opex ",null,"Meter Type 4",2304748.9400331443,2304748.9400331443,2304748.9400331443,2304748.9400331443,2304748.9400331443,2304748.9400331443,2304748.9400331443]
[]
[null,"VOLUMES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Meter purchase ",null,"Meter Type 4",14051,15527.5,16872,17099,17441,17545,17784]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4",134,134,134,134,134,134,134]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",119,119,119,119,119,119,119]
[null,"Meter investigation ",null,"Meter Type 4",2802,2802,2802,2802,2802,2802,2802]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",33,33,33,33,33,33,33]
[null,"Scheduled meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",89149,89149,89149,89149,89149,89149,89149]
[null,null,null,"Meter Type 6",3101,3101,3101,3101,3101,3101,3101]
[null,"Special meter reading ",null,"Meter Type 4",9000,9000,9000,9000,9000,9000,9000]
[null,null,null,"Meter Type 5",3904,3904,3904,3904,3904,3904,3904]
[null,null,null,"Meter Type 6",20104,20104,20104,20104,20104,20104,20104]
[null,"New meter installation ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4",4663.5,4620,5053,5811.5,6744,7702.5,8469.5]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4",123,123,123,123,123,123,123]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4",745855,745855,745855,745855,745855,745855,745855]
[null,"Remote meter re-configuration ",null,"Meter Type 4",10033,10033,10033,10033,10033,10033,10033]

{"sheet":"4.3 Fee-based services","index":29,"n_rows":43,"n_cols":16,"rows_kept":43,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,1,9,1],[8,2,8,8],[8,9,8,15]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.3 ANCILLARY SERVICES - FEE BASED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.3.1 - COST METRICS FOR FEE-BASED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"COMMON FEE-BASED SERVICES"]
[null,"Energisation",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"De-energisation",83140,83140,83140,83140,83140,83140,83140,51600,51600,51600,51600,51600,51600,51600]
[null,"Re-energisation",167792,167792,167792,167792,167792,167792,167792,114660,114660,114660,114660,114660,114660,114660]
[null,"MISCELLANEOUS FEE-BASED SERVICES"]
[null,"Single Phase Overhead – Business Hours",33000,26513.2483681456,44306.675739599901,44103.447030061063,44755.206202511807,45117.608989785658,45675.63990635363,76.042740159804154,60.583620718733734,91.867234379394105,91.445851840980382,92.797235388831112,93.548655829260966,94.705699460893186]
[null,"Single Phase Overhead – After Hours",999.99999999999989,803.42908808475374,2945.7475118712805,2932.2357677498462,2975.5682436925199,2999.6627416679798,3036.7636560694227,1.910870750293266,1.5224000152414752,2.308522953236674,2.2979340716991739,2.3318928597253383,2.350775232161844,2.3798504710058519]
[null,"Single Phase underground – Business Hours",2586934.8639777177,2078426.63430178,1453389.8030090567,1446723.3011965896,1468102.9267145314,1479990.8083218422,1498295.8702648852,11477.685129830877,9144.3275344026606,6933.0957020958531,6901.2945328786627,7003.2816181629933,7059.9903006568647,7147.3108157871875]
[null,"Single Phase underground with a directly connected meter on group metering panel - Business Hours",0,0,3195732.5812148168,3181074.189501375,3228083.9907951527,3254223.2209558799,3294472.6314935242,0,0,6933.0957020958531,6901.2945328786627,7003.2816181629933,7059.9903006568647,7147.3108157871875]
[null,"Single Phase underground – After Hours",19999.999999999989,16068.430569048818,106945.19702558046,106454.65391847347,108027.83700990264,108902.58639790471,110249.53299957424,69.374054652332973,55.270646559358156,83.810795418490386,83.426366672392888,84.659238553493452,85.34476201821488,86.400336922108437]
[null,"Multi-phase overhead with a directly connected meter – Business Hours",9500.0000000000036,7632.5800422835673,13679.005420128007,13616.261678402812,13817.482309464589,13929.368602187693,14101.652074258471,20.482566200132883,16.318560054614444,24.744988224315843,24.631486321037489,24.995489550306367,25.197889133526186,25.509545745735917]
[null,"Multi-phase overhead with a directly connected meter– After Hours",350.00000000000011,281.20033868248635,964.67649405419263,960.25165387522475,974.4422186818166,982.33271022574297,994.48255670333629,0.62577396350327841,0.4985571585251905,0.75599752524523134,0.75252986718004222,0.76365072680680623,0.76983434599618561,0.77935593579938245]
[null,"Multi-phase overhead with a CT connected meter ",2500.0000000000009,2008.5748935049676,5119.1196794118414,5095.6389720679617,5170.9421436608545,5212.8135594066571,5277.2875240866615,4.0148477625016907,3.198648728014033,4.8503375814735863,4.8280897411412642,4.8994390797101817,4.9391120145310188,5.0002007394482604]
[null,"Multi-phase overhead connection with a CT connected meter – After Hours",650.00000000000057,522.52439330823825,1858.9509106442838,1850.4241550626498,1877.7696574485394,1892.9747925704376,1916.3877898943274,0.86511766029695414,0.68924344517787017,1.0451486453175445,1.0403546903001901,1.0557290149316216,1.0642777217767174,1.0774410938140166]
[null,"Multi-phase underground with a directly connected meter – Business Hours",620000.00000000012,498120.86785059789,376208.31297283247,374482.69648983108,380016.78846670024,383093.95322666195,387832.19788628299,1838.2343920971803,1464.530275591195,1110.3854844536525,1105.2922969073234,1121.6262671808367,1130.7085733524725,1144.6935862041507]
[null,"Multi-phase underground with a directly connected meter on group metering panel – Business Hours",0,0,655257.1265176218,652251.55099169083,661890.50122644904,667250.12266197917,675502.91366456659,0,0,1110.3854844536525,1105.2922969073234,1121.6262671808367,1130.7085733524725,1144.693586204151]
[null,"Multi-phase underground with a directly connected meter – After Hours",7999.9999999999964,6427.4167791233431,29523.566769602578,29388.146174953734,29822.443154457258,30063.928725400394,30435.770276358195,19.151580356771934,15.258157163467608,23.137024227085647,23.030897836474107,23.371247626014746,23.560495000798593,23.851899729782954]
[null,"Multi-phase underground with a CT connected meter – Business Hours",80000,64274.180416131603,167117.81924292899,166351.27248267794,168809.60567408442,170176.53204546723,172281.3369826524,164.40103273030198,130.97910190729243,198.61288762490582,197.70187725962774,200.62350857399787,202.24804625059554,204.74952328252007]
[null,"Multi-phase underground connection with a CT connected meter – After Hours",12000.000000000002,9641.1714497208104,42785.28274515699,42589.032458842215,43218.411666592867,43568.370345783194,44107.239718114841,19.911393836002521,15.863504255720605,24.054954891267528,23.944618077255598,24.298470792034195,24.495226304715334,24.798192128756561]
[null,"95mm2 overhead service from LVABC – Business Hours",100491.55933003168,80737.73063344309,141249.83144644028,140601.93763612263,142679.74807248666,143835.08937859148,145614.09381960126,140.51000000000002,111.94500000000001,169.75013098583625,168.97151016880514,171.46856513959477,172.85702228702158,174.99498049761456]
[null,"95mm2 overhead service from LVABC – After Hours",6294.3745092583968,5057.0847299759689,17892.815466010543,17810.74354938684,18073.950084435415,18220.302887682697,18445.658187935012,7.025500000000001,5.5972499999999998,8.4875065492918136,8.448575508440257,8.5734282569797404,8.6428511143510782,8.7497490248807299]
[null,"Establish temporary supply connection – Business Hours",71828.682499595117,57709.349095955084,114616.37748881067,114090.64771783965,115776.67525419671,116714.1704279105,118157.73352796536,196.714,156.72299999999998,237.65018338017077,236.56011423632719,240.05599119543274,241.99983120183023,244.99297269666044]
[null,"Establish temporary supply connection – After Hours",6516.2678456967124,5235.3690471439195,21660.647787377056,21561.293335161419,21879.925361622161,22057.096837506251,22329.906993909903,14.051,11.1945,16.975013098583627,16.897151016880517,17.146856513959481,17.28570222870216,17.499498049761463]
[null,"Appointment – inspection of group or CT metering prior to connection – Business Hours",0,0,6031.3932583243195,6031.3932583243195,6031.3932583243195,6031.3932583243195,6031.3932583243195,0,0,12,12,12,12,12]
[null,"Service truck - Disconnect / Reconnect at pole or pit – Business Hours",109542.81215306757,110467.54291831146,166152.58390299056,166152.58390299056,166152.58390299056,166152.58390299056,166152.58390299056,300,300,300,300,300,300,300]
[null,"Service truck - Disconnect / Reconnect at pole or pit – After Hours",13912.74894106479,14030.199777955031,0,0,0,0,0,30,30,0,0,0,0,0]
[null,"Meter equipment test – Single Phase",28394.010342098325,39502.548856203852,49170.070436468683,49674.68496563255,50208.173849109175,50683.683552117618,51131.351776718402,165,165,165,165,165,165,165]
[null,"Meter equipment test – Single Phase Each Additional Meter at same site",556.68483674589584,576.34014153274393,577.20970180321342,583.13339480016748,589.3960451607104,594.97807527459179,600.23327300229209,9,9,9,9,9,9,9]
[null,"Meter equipment test – Multi Phase",4893.1036015117161,6889.9347647253171,8631.6232044636163,8718.0781770350059,8811.3633195289112,8896.9010413634896,8976.3641386391737,24,24,24,24,24,24,24]
[null,"Meter equipment test – Multi Phase  Each Additional Meter at same site",121.29512159300718,124.7939832758294,124.1867975704764,125.43066166455924,126.77279428930503,128.00346151080947,129.14673055093573,1,1,1,1,1,1,1]
[null,"Wasted Truck Visit – customer not ready for their requested works",145973.10143423532,117705.78282554835,174838.09994539715,175821.78035263033,180340.5614605727,183519.83335789331,187424.6221978633,703,560,849,845,857,864,875]
[null,"Manual assessment of PV & small generator installation enquiry, 4.6kW to 15kW",64053.427516411983,97456.831938934818,127199.69628603775,128504.78580832326,129887.99653767637,131116.12121809667,132269.9430848159,400,400,400,400,400,400,400]
[null,"Manual assessment of PV & small generator installation enquiry, 15kW to 30kW",84919.888188425,107978.45261094786,127199.69628603775,128504.78580832326,129887.99653767637,131116.12121809667,132269.9430848159,400,400,400,400,400,400,400]

{"sheet":"4.4 Quoted services","index":30,"n_rows":34,"n_cols":16,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,1,9,1],[8,2,8,8],[8,9,8,15]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.4 ANCILLARY SERVICES - QUOTED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.4.1 - COST METRICS FOR QUOTED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Processing access permit applications;",6000,6000,6000,6000,6000,6000,6000,12,12,12,12,12,12,12]
[null,"Clearance assessment",12000,12000,12000,12000,12000,12000,12000,12,12,12,12,12,12,12]
[null,"Property admin;",10000,10000,10000,10000,10000,10000,10000,2,2,2,2,2,2,2]
[null,"Conveyancing inquiries",60000,60000,60000,60000,60000,60000,60000,12,12,12,12,12,12,12]
[null,"Fitting of tiger tails, possum guards, HiVis flags, and aerial markers;",35000,35000,35000,35000,35000,35000,35000,10,10,10,10,10,10,10]
[null,"High load escorts.",108000,108000,108000,108000,108000,108000,108000,36,36,36,36,36,36,36]
[null,"Site visit assessing location of underground cables;",5000,5000,5000,5000,5000,5000,5000,12,12,12,12,12,12,12]
[null,"De-energising shared network lines for safe approach.",24000,24000,24000,24000,24000,24000,24000,6,6,6,6,6,6,6]
[null,"Abolishment of connection with a capacity greater 100A;",150000,150000,150000,150000,150000,150000,150000,30,30,30,30,30,30,30]
[null,"Establishing premises connection assets with a capacity greater 100A;",120000,120000,120000,120000,120000,120000,120000,12,12,12,12,12,12,12]
[null,"Rectification of damage to overhead or underground cables;",80000,80000,80000,80000,80000,80000,80000,8,8,8,8,8,8,8]
[null,"Upgrade from a single phase connection to multi-phase connection, where only the required multiphase isn’t available at the point of connection.",0,0,180000,225000,270000,315000,315000,0,0,12,15,18,21,21]
[null,"Creating a community PV generator opportunity map.",0,1500,1500,1500,1500,1500,1500,0,1,1,1,1,1,1]
[null,"Augmenting shared network to create greater generation hosting capacity",0,40000,40000,80000,80000,80000,80000,0,1,1,2,2,2,2]
[null,"Training days to individual employees of third party service providers",4000,4000,4000,4000,6000,6000,3000,2,2,2,2,3,3,3]
[null,"Authorisation or re-authorisation of individual employees of third party service providers to become accredited to undertake design, construct, audit or tie in distributor’s network assets for customer connections;",20000,20000,40000,40000,40000,40000,40000,20,20,40,40,40,40,40]
[null,"Assessing new public lighting assets for use as standard lighting.",4000,4000,4000,4000,4000,4000,4000,2,2,2,2,2,2,2]
[null,"Relocating power lines",1200000,1200000,1200000,4800000,4800000,1200000,1200000,24,24,24,96,96,24,24]
[null,"Complex requests for de-identified metering data from multiple sites and other analysis by third party",6000,6000,6000,6000,6000,6000,6000,2,2,2,2,2,2,2]
[null,"Provision and maintenance of reserve feeder and backup supply;",30000,30000,30000,30000,30000,30000,30000,3,3,3,3,3,3,3]
[null,"Provision and maintenance of isolation transformer or harmonic filtering equipment at a customer’s premises.",0,0,0,500000,0,500000,0,0,0,0,1,0,1,0]
[null,"Manual assessment of connection applications and preparing offers;",0,0,125000,125000,125000,125000,125000,0,0,125,125,125,125,125]
[null,"Site inspection required to provide a connection offer",0,0,125000,125000,125000,125000,125000,0,0,250,250,250,250,250]
[null,"Manual Aassessment of PV & small generator installation enquiry greater than 30 kW;",182700,182700,182700,182700,182700,182700,182700,150,150,150,150,150,150,150]

{"sheet":"5.4 MD & utilisation-Spatial","index":31,"n_rows":11579,"n_cols":12,"rows_kept":11579,"cut":false,"hidden":false,"merged":[[5,1,5,2],[11,2,12,2],[11,3,12,3],[13,2,14,2],[13,3,14,3],[15,2,16,2],[15,3,16,3],[17,2,18,2],[17,3,18,3],[19,2,20,2],[19,3,20,3],[21,2,22,2],[21,3,22,3],[23,2,24,2],[23,3,24,3],[25,2,26,2],[25,3,26,3],[27,2,28,2],[27,3,28,3],[29,2,30,2],[29,3,30,3],[31,2,32,2],[31,3,32,3],[33,2,34,2],[33,3,34,3],[35,2,36,2],[35,3,36,3],[37,2,38,2],[37,3,38,3],[39,2,40,2],[39,3,40,3],[9,5,9,11],[41,2,42,2],[41,3,42,3],[43,2,44,2],[43,3,44,3],[45,2,46,2],[45,3,46,3],[47,2,48,2],[47,3,48,3],[49,2,50,2],[49,3,50,3],[51,2,52,2],[51,3,52,3],[53,2,54,2],[53,3,54,3],[55,2,56,2],[55,3,56,3],[57,2,58,2],[57,3,58,3],[59,2,60,2],[59,3,60,3],[61,2,62,2],[61,3,62,3],[63,2,64,2],[63,3,64,3],[65,2,66,2],[65,3,66,3],[67,2,68,2],[67,3,68,3],[69,2,70,2],[69,3,70,3],[71,2,72,2],[71,3,72,3],[73,2,74,2],[73,3,74,3],[75,2,76,2],[75,3,76,3],[77,2,78,2],[77,3,78,3],[79,2,80,2],[79,3,80,3],[81,2,82,2],[81,3,82,3],[83,2,84,2],[83,3,84,3],[85,2,86,2],[85,3,86,3],[87,2,88,2],[87,3,88,3],[89,2,90,2],[89,3,90,3],[91,2,92,2],[91,3,92,3],[93,2,94,2],[93,3,94,3],[95,2,96,2],[95,3,96,3],[97,2,98,2],[97,3,98,3],[99,2,100,2],[99,3,100,3],[101,2,102,2],[101,3,102,3],[103,2,104,2],[103,3,104,3],[105,2,106,2],[105,3,106,3],[107,2,108,2],[107,3,108,3],[109,2,110,2],[109,3,110,3],[111,2,112,2],[111,3,112,3],[113,2,114,2],[113,3,114,3],[115,2,116,2],[115,3,116,3],[117,2,118,2],[117,3,118,3],[119,2,120,2],[119,3,120,3],[121,2,122,2],[121,3,122,3],[123,2,124,2],[123,3,124,3],[125,2,126,2],[125,3,126,3],[127,2,128,2],[127,3,128,3],[129,2,130,2],[129,3,130,3],[131,2,132,2],[131,3,132,3],[133,2,134,2],[133,3,134,3],[135,2,136,2],[135,3,136,3],[137,2,138,2],[137,3,138,3],[139,2,140,2],[139,3,140,3],[141,2,142,2],[141,3,142,3],[143,2,144,2],[143,3,144,3],[145,2,146,2],[145,3,146,3],[147,2,148,2],[147,3,148,3],[149,2,150,2],[149,3,150,3],[151,2,152,2],[151,3,152,3],[153,2,154,2],[153,3,154,3],[155,2,156,2],[155,3,156,3],[157,2,158,2],[157,3,158,3],[159,2,160,2],[159,3,160,3],[161,2,162,2],[161,3,162,3],[163,2,164,2],[163,3,164,3],[165,2,166,2],[165,3,166,3],[167,2,168,2],[167,3,168,3],[169,2,170,2],[169,3,170,3],[171,2,172,2],[171,3,172,3],[173,2,174,2],[173,3,174,3],[175,2,176,2],[175,3,176,3],[177,2,178,2],[177,3,178,3],[179,2,180,2],[179,3,180,3],[181,2,182,2],[181,3,182,3],[183,2,184,2],[183,3,184,3],[185,2,186,2],[185,3,186,3],[187,2,188,2],[187,3,188,3],[189,2,190,2],[189,3,190,3],[191,2,192,2],[191,3,192,3],[193,2,194,2],[193,3,194,3],[195,2,196,2],[195,3,196,3],[197,2,198,2],[197,3,198,3],[199,2,200,2],[199,3,200,3],[201,2,202,2],[201,3,202,3],[203,2,204,2],[203,3,204,3],[205,2,206,2],[205,3,206,3],[207,2,208,2],[207,3,208,3],[209,2,210,2],[209,3,210,3],[211,2,212,2],[211,3,212,3],[213,2,214,2],[213,3,214,3],[215,2,216,2],[215,3,216,3],[217,2,218,2],[217,3,218,3],[219,2,220,2],[219,3,220,3],[221,2,222,2],[221,3,222,3],[223,2,224,2],[223,3,224,3],[225,2,226,2],[225,3,226,3],[227,2,228,2],[227,3,228,3],[229,2,230,2],[229,3,230,3],[231,2,232,2],[231,3,232,3],[233,2,234,2],[233,3,234,3],[235,2,236,2],[235,3,236,3],[237,2,238,2],[237,3,238,3],[239,2,240,2],[239,3,240,3],[241,2,242,2],[241,3,242,3],[243,2,244,2],[243,3,244,3],[245,2,246,2],[245,3,246,3],[247,2,248,2],[247,3,248,3],[249,2,250,2],[249,3,250,3],[251,2,252,2],[251,3,252,3],[253,2,254,2],[253,3,254,3],[255,2,256,2],[255,3,256,3],[257,2,258,2],[257,3,258,3],[259,2,260,2],[259,3,260,3],[261,2,262,2],[261,3,262,3],[263,2,264,2],[263,3,264,3],[265,2,266,2],[265,3,266,3],[267,2,268,2],[267,3,268,3],[269,2,270,2],[269,3,270,3],[271,2,272,2],[271,3,272,3],[273,2,274,2],[273,3,274,3],[275,2,276,2],[275,3,276,3],[277,2,278,2],[277,3,278,3],[279,2,280,2],[279,3,280,3],[281,2,282,2],[281,3,282,3],[283,2,284,2],[283,3,284,3],[285,2,286,2],[285,3,286,3],[287,2,288,2],[287,3,288,3],[289,2,290,2],[289,3,290,3],[291,2,292,2],[291,3,292,3],[293,2,294,2],[293,3,294,3],[295,2,296,2],[295,3,296,3],[297,2,298,2],[297,3,298,3],[299,2,300,2],[299,3,300,3],[301,2,302,2],[301,3,302,3],[303,2,304,2],[303,3,304,3],[305,2,306,2],[305,3,306,3],[307,2,308,2],[307,3,308,3],[309,2,310,2],[309,3,310,3],[311,2,312,2],[311,3,312,3],[313,2,314,2],[313,3,314,3],[315,2,316,2],[315,3,316,3],[317,2,318,2],[317,3,318,3],[319,2,320,2],[319,3,320,3],[321,2,322,2],[321,3,322,3],[323,2,324,2],[323,3,324,3],[325,2,326,2],[325,3,326,3],[327,2,328,2],[327,3,328,3],[329,2,330,2],[329,3,330,3],[331,2,332,2],[331,3,332,3],[333,2,334,2],[333,3,334,3],[335,2,336,2],[335,3,336,3],[337,2,338,2],[337,3,338,3],[339,2,340,2],[339,3,340,3],[341,2,342,2],[341,3,342,3],[343,2,344,2],[343,3,344,3],[345,2,346,2],[345,3,346,3],[347,2,348,2],[347,3,348,3],[349,2,350,2],[349,3,350,3],[351,2,352,2],[351,3,352,3],[353,2,354,2],[353,3,354,3],[355,2,356,2],[355,3,356,3],[357,2,358,2],[357,3,358,3],[359,2,360,2],[359,3,360,3],[361,2,362,2],[361,3,362,3],[363,2,364,2],[363,3,364,3],[365,2,366,2],[365,3,366,3],[367,2,368,2],[367,3,368,3],[369,2,370,2],[369,3,370,3],[371,2,372,2],[371,3,372,3],[373,2,374,2],[373,3,374,3],[375,2,376,2],[375,3,376,3],[377,2,378,2],[377,3,378,3],[379,2,380,2],[379,3,380,3],[381,2,382,2],[381,3,382,3],[383,2,384,2],[383,3,384,3],[385,2,386,2],[385,3,386,3],[387,2,388,2],[387,3,388,3],[389,2,390,2],[389,3,390,3],[391,2,392,2],[391,3,392,3],[393,2,394,2],[393,3,394,3],[395,2,396,2],[395,3,396,3],[397,2,398,2],[397,3,398,3],[399,2,400,2],[399,3,400,3],[401,2,402,2],[401,3,402,3],[403,2,404,2],[403,3,404,3],[405,2,406,2],[405,3,406,3],[407,2,408,2],[407,3,408,3],[409,2,410,2],[409,3,410,3],[411,2,412,2],[411,3,412,3],[413,2,414,2],[413,3,414,3],[415,2,416,2],[415,3,416,3],[417,2,418,2],[417,3,418,3],[419,2,420,2],[419,3,420,3],[421,2,422,2],[421,3,422,3],[423,2,424,2],[423,3,424,3],[425,2,426,2],[425,3,426,3],[427,2,428,2],[427,3,428,3],[429,2,430,2],[429,3,430,3],[431,2,432,2],[431,3,432,3],[433,2,434,2],[433,3,434,3],[435,2,436,2],[435,3,436,3],[437,2,438,2],[437,3,438,3],[439,2,440,2],[439,3,440,3],[441,2,442,2],[441,3,442,3],[443,2,444,2],[443,3,444,3],[445,2,446,2],[445,3,446,3],[447,2,448,2],[447,3,448,3],[449,2,450,2],[449,3,450,3],[451,2,452,2],[451,3,452,3],[453,2,454,2],[453,3,454,3],[455,2,456,2],[455,3,456,3],[457,2,458,2],[457,3,458,3],[459,2,460,2],[459,3,460,3],[461,2,462,2],[461,3,462,3],[463,2,464,2],[463,3,464,3],[465,2,466,2],[465,3,466,3],[467,2,468,2],[467,3,468,3],[469,2,470,2],[469,3,470,3],[471,2,472,2],[471,3,472,3],[473,2,474,2],[473,3,474,3],[475,2,476,2],[475,3,476,3],[477,2,478,2],[477,3,478,3],[479,2,480,2],[479,3,480,3],[481,2,482,2],[481,3,482,3],[483,2,484,2],[483,3,484,3],[485,2,486,2],[485,3,486,3],[487,2,488,2],[487,3,488,3],[489,2,490,2],[489,3,490,3],[491,2,492,2],[491,3,492,3],[493,2,494,2],[493,3,494,3],[495,2,496,2],[495,3,496,3],[497,2,498,2],[497,3,498,3],[499,2,500,2],[499,3,500,3],[501,2,502,2],[501,3,502,3],[503,2,504,2],[503,3,504,3],[505,2,506,2],[505,3,506,3],[507,2,508,2],[507,3,508,3],[509,2,510,2],[509,3,510,3],[511,2,512,2],[511,3,512,3],[513,2,514,2],[513,3,514,3],[515,2,516,2],[515,3,516,3],[517,2,518,2],[517,3,518,3],[519,2,520,2],[519,3,520,3],[521,2,522,2],[521,3,522,3],[523,2,524,2],[523,3,524,3],[525,2,526,2],[525,3,526,3],[527,2,528,2],[527,3,528,3],[529,2,530,2],[529,3,530,3],[531,2,532,2],[531,3,532,3],[533,2,534,2],[533,3,534,3],[535,2,536,2],[535,3,536,3],[537,2,538,2],[537,3,538,3],[539,2,540,2],[539,3,540,3],[541,2,542,2],[541,3,542,3],[543,2,544,2],[543,3,544,3],[545,2,546,2],[545,3,546,3],[547,2,548,2],[547,3,548,3],[549,2,550,2],[549,3,550,3],[551,2,552,2],[551,3,552,3],[553,2,554,2],[553,3,554,3],[555,2,556,2],[555,3,556,3],[557,2,558,2],[557,3,558,3],[559,2,560,2],[559,3,560,3],[561,2,562,2],[561,3,562,3],[563,2,564,2],[563,3,564,3],[565,2,566,2],[565,3,566,3],[567,2,568,2],[567,3,568,3],[569,2,570,2],[569,3,570,3],[571,2,572,2],[571,3,572,3],[573,2,574,2],[573,3,574,3],[575,2,576,2],[575,3,576,3],[577,2,578,2],[577,3,578,3],[579,2,580,2],[579,3,580,3],[581,2,582,2],[581,3,582,3],[583,2,584,2],[583,3,584,3],[585,2,586,2],[585,3,586,3],[587,2,588,2],[587,3,588,3],[589,2,590,2],[589,3,590,3],[591,2,592,2],[591,3,592,3],[593,2,594,2],[593,3,594,3],[595,2,596,2],[595,3,596,3],[597,2,598,2],[597,3,598,3],[599,2,600,2],[599,3,600,3],[601,2,602,2],[601,3,602,3],[603,2,604,2],[603,3,604,3],[605,2,606,2],[605,3,606,3],[607,2,608,2],[607,3,608,3],[609,2,610,2],[609,3,610,3],[611,2,612,2],[611,3,612,3],[613,2,614,2],[613,3,614,3],[615,2,616,2],[615,3,616,3],[617,2,618,2],[617,3,618,3],[619,2,620,2],[619,3,620,3],[621,2,622,2],[621,3,622,3],[623,2,624,2],[623,3,624,3],[625,2,626,2],[625,3,626,3],[627,2,628,2],[627,3,628,3],[629,2,630,2],[629,3,630,3],[631,2,632,2],[631,3,632,3],[633,2,634,2],[633,3,634,3],[635,2,636,2],[635,3,636,3],[637,2,638,2],[637,3,638,3],[639,2,640,2],[639,3,640,3],[641,2,642,2],[641,3,642,3],[643,2,644,2],[643,3,644,3],[645,2,646,2],[645,3,646,3],[647,2,648,2],[647,3,648,3],[649,2,650,2],[649,3,650,3],[651,2,652,2],[651,3,652,3],[653,2,654,2],[653,3,654,3],[655,2,656,2],[655,3,656,3],[657,2,658,2],[657,3,658,3],[659,2,660,2],[659,3,660,3],[661,2,662,2],[661,3,662,3],[663,2,664,2],[663,3,664,3],[665,2,666,2],[665,3,666,3],[667,2,668,2],[667,3,668,3],[669,2,670,2],[669,3,670,3],[671,2,672,2],[671,3,672,3],[673,2,674,2],[673,3,674,3],[675,2,676,2],[675,3,676,3],[677,2,678,2],[677,3,678,3],[679,2,680,2],[679,3,680,3],[681,2,682,2],[681,3,682,3],[683,2,684,2],[683,3,684,3],[685,2,686,2],[685,3,686,3],[687,2,688,2],[687,3,688,3],[689,2,690,2],[689,3,690,3],[691,2,692,2],[691,3,692,3],[693,2,694,2],[693,3,694,3],[695,2,696,2],[695,3,696,3],[697,2,698,2],[697,3,698,3],[699,2,700,2],[699,3,700,3],[701,2,702,2],[701,3,702,3],[703,2,704,2],[703,3,704,3],[705,2,706,2],[705,3,706,3],[707,2,708,2],[707,3,708,3],[709,2,710,2],[709,3,710,3],[711,2,712,2],[711,3,712,3],[713,2,714,2],[713,3,714,3],[715,2,716,2],[715,3,716,3],[717,2,718,2],[717,3,718,3],[719,2,720,2],[719,3,720,3],[721,2,722,2],[721,3,722,3],[723,2,724,2],[723,3,724,3],[725,2,726,2],[725,3,726,3],[727,2,728,2],[727,3,728,3],[729,2,730,2],[729,3,730,3],[731,2,732,2],[731,3,732,3],[733,2,734,2],[733,3,734,3],[735,2,736,2],[735,3,736,3],[737,2,738,2],[737,3,738,3],[739,2,740,2],[739,3,740,3],[741,2,742,2],[741,3,742,3],[743,2,744,2],[743,3,744,3],[745,2,746,2],[745,3,746,3],[747,2,748,2],[747,3,748,3],[749,2,750,2],[749,3,750,3],[751,2,752,2],[751,3,752,3],[753,2,754,2],[753,3,754,3],[755,2,756,2],[755,3,756,3],[757,2,758,2],[757,3,758,3],[759,2,760,2],[759,3,760,3],[761,2,762,2],[761,3,762,3],[763,2,764,2],[763,3,764,3],[765,2,766,2],[765,3,766,3],[767,2,768,2],[767,3,768,3],[769,2,770,2],[769,3,770,3],[771,2,772,2],[771,3,772,3],[773,2,774,2],[773,3,774,3],[775,2,776,2],[775,3,776,3],[777,2,778,2],[777,3,778,3],[779,2,780,2],[779,3,780,3],[781,2,782,2],[781,3,782,3],[783,2,784,2],[783,3,784,3],[785,2,786,2],[785,3,786,3],[787,2,788,2],[787,3,788,3],[789,2,790,2],[789,3,790,3],[791,2,792,2],[791,3,792,3],[793,2,794,2],[793,3,794,3],[795,2,796,2],[795,3,796,3],[797,2,798,2],[797,3,798,3],[799,2,800,2],[799,3,800,3],[801,2,802,2],[801,3,802,3],[803,2,804,2],[803,3,804,3],[805,2,806,2],[805,3,806,3],[807,2,808,2],[807,3,808,3],[809,2,810,2],[809,3,810,3],[811,2,812,2],[811,3,812,3],[813,2,814,2],[813,3,814,3],[815,2,816,2],[815,3,816,3],[817,2,818,2],[817,3,818,3],[819,2,820,2],[819,3,820,3],[821,2,822,2],[821,3,822,3],[823,2,824,2],[823,3,824,3],[825,2,826,2],[825,3,826,3],[827,2,828,2],[827,3,828,3],[829,2,830,2],[829,3,830,3],[831,2,832,2],[831,3,832,3],[833,2,834,2],[833,3,834,3],[835,2,836,2],[835,3,836,3],[837,2,838,2],[837,3,838,3],[839,2,840,2],[839,3,840,3],[841,2,842,2],[841,3,842,3],[843,2,844,2],[843,3,844,3],[845,2,846,2],[845,3,846,3],[847,2,848,2],[847,3,848,3],[849,2,850,2],[849,3,850,3],[851,2,852,2],[851,3,852,3],[853,2,854,2],[853,3,854,3],[855,2,856,2],[855,3,856,3],[857,2,858,2],[857,3,858,3],[859,2,860,2],[859,3,860,3],[861,2,862,2],[861,3,862,3],[863,2,864,2],[863,3,864,3],[865,2,866,2],[865,3,866,3],[867,2,868,2],[867,3,868,3],[869,2,870,2],[869,3,870,3],[871,2,872,2],[871,3,872,3],[873,2,874,2],[873,3,874,3],[875,2,876,2],[875,3,876,3],[877,2,878,2],[877,3,878,3],[879,2,880,2],[879,3,880,3],[881,2,882,2],[881,3,882,3],[883,2,884,2],[883,3,884,3],[885,2,886,2],[885,3,886,3],[887,2,888,2],[887,3,888,3],[889,2,890,2],[889,3,890,3],[891,2,892,2],[891,3,892,3],[893,2,894,2],[893,3,894,3],[895,2,896,2],[895,3,896,3],[897,2,898,2],[897,3,898,3],[899,2,900,2],[899,3,900,3],[901,2,902,2],[901,3,902,3],[903,2,904,2],[903,3,904,3],[905,2,906,2],[905,3,906,3],[907,2,908,2],[907,3,908,3],[909,2,910,2],[909,3,910,3],[911,2,912,2],[911,3,912,3],[913,2,914,2],[913,3,914,3],[915,2,916,2],[915,3,916,3],[917,2,918,2],[917,3,918,3],[919,2,920,2],[919,3,920,3],[921,2,922,2],[921,3,922,3],[923,2,924,2],[923,3,924,3],[925,2,926,2],[925,3,926,3],[927,2,928,2],[927,3,928,3],[929,2,930,2],[929,3,930,3],[931,2,932,2],[931,3,932,3],[933,2,934,2],[933,3,934,3],[935,2,936,2],[935,3,936,3],[937,2,938,2],[937,3,938,3],[939,2,940,2],[939,3,940,3],[941,2,942,2],[941,3,942,3],[943,2,944,2],[943,3,944,3],[945,2,946,2],[945,3,946,3],[947,2,948,2],[947,3,948,3],[949,2,950,2],[949,3,950,3],[951,2,952,2],[951,3,952,3],[953,2,954,2],[953,3,954,3],[955,2,956,2],[955,3,956,3],[957,2,958,2],[957,3,958,3],[959,2,960,2],[959,3,960,3],[961,2,962,2],[961,3,962,3],[963,2,964,2],[963,3,964,3],[965,2,966,2],[965,3,966,3],[967,2,968,2],[967,3,968,3],[969,2,970,2],[969,3,970,3],[971,2,972,2],[971,3,972,3],[973,2,974,2],[973,3,974,3],[975,2,976,2],[975,3,976,3],[977,2,978,2],[977,3,978,3],[979,2,980,2],[979,3,980,3],[981,2,982,2],[981,3,982,3],[983,2,984,2],[983,3,984,3],[985,2,986,2],[985,3,986,3],[987,2,988,2],[987,3,988,3],[989,2,990,2],[989,3,990,3],[991,2,992,2],[991,3,992,3],[993,2,994,2],[993,3,994,3],[995,2,996,2],[995,3,996,3],[997,2,998,2],[997,3,998,3],[999,2,1000,2],[999,3,1000,3],[1001,2,1002,2],[1001,3,1002,3],[1003,2,1004,2],[1003,3,1004,3],[1005,2,1006,2],[1005,3,1006,3],[1007,2,1008,2],[1007,3,1008,3]],"merged_total":11556,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"BDL","Substation Rating","MVA","Non-Coincident",81,81,81,81,81,81,81]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",55.741888240354399,56.4166549614053,57.140535447645995,57.819443128236401,58.476471392155297,59.1334996560741,59.790527919993004]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",56.299307122757945,56.98082151101935,57.711940802122456,58.397637559518763,59.061236106076848,59.72483465263484,60.388433199192932]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",54.754095799180895,55.412465572572998,56.119949111154796,56.786086511872895,57.431002514852501,58.0759185178322,58.720834520811799]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",55.301636757172702,55.966590228298728,56.681148602266347,57.353947376991627,58.005312540001029,58.656677703010523,59.308042866019917]
[null,null,null,null,"Coincident"]
[null,"BGE","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.8379999999999996,3.8380000000000001,3.8380000000000001,3.8380000000000001,3.8380000000000001,3.8380000000000001,3.8380000000000001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.2480005172728,33.444163187626302,33.5679200215516,33.731892019806104,33.9124820225991,34.020666188963901,34.175879392353899]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.580480522445527,33.778604819502569,33.903599221767116,34.069210940004162,34.25160684282509,34.360872850853539,34.517638186277438]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.265148828533402,31.450062812833302,31.562570960705099,31.715867867382201,31.886520097385002,31.984766490959597,32.130041921559503]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.577800316818735,31.764563440961634,31.87819667031215,32.033026546056021,32.205385298358856,32.304614155869196,32.451342340775099]
[null,null,null,null,"Coincident"]
[null,"BN","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.955946615295801,37.098150563109201,37.268690438074501,37.348567460668797,37.479009151876099,37.637566998770701,37.716122768134703]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.325506081448758,37.469132068740294,37.641377342455243,37.722053135275488,37.85379924339486,38.013942668758411,38.093283995816051]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.166311856600998,36.3032655851027,36.468555240756302,36.543724796607698,36.669527301878801,36.823445962837297,36.8973625462651]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.527974975167005,36.666298240953729,36.833240793163867,36.909162044573776,37.036222574897593,37.191680422465673,37.266336171727751]
[null,null,null,null,"Coincident"]
[null,"BRA","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.02,2.02,2.02,2.02,2.02,2.02,2.02]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",70.257056012691592,70.813282310064508,71.354405827073009,71.9011707046336,72.450390139651603,72.999609574669591,73.548829009687594]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",70.959626572818507,71.521415133165149,72.067949885343737,72.620182411679934,73.17489404104812,73.729605670416291,74.284317299784476]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",66.451556639762302,66.973281343369493,67.479903266612297,67.991547442401597,68.505433024575595,69.019318606749707,69.533204188923804]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.116072206159927,67.64301415680319,68.154702299278426,68.671462916825618,69.190487354821357,69.70951179281721,70.228536230813049]
[null,null,null,null,"Coincident"]
[null,"BRT","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9408449907047114,9.0356469973030116,9.1588959689846394,9.1963497021578604,9.2376150080949184,9.32845045682323,9.4453593208028188]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.0302534406117587,9.1260034672760426,9.250484928674485,9.2883131991794396,9.3299911581758685,9.4217349613914632,9.539812914010847]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.9426183802392014,9.0374378785546714,9.1607043419534602,9.1981720415757096,9.2394520626831316,9.3303022265817912,9.4472258057317386]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.0320445640415929,9.1278122573402189,9.2523113853729946,9.2901537619914674,9.3318465833099626,9.4236052488476094,9.5416980637890561]
[null,null,null,null,"Coincident"]
[null,"BWA","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.3792945054259,10.44835192663,10.546546304838301,10.615103023447301,10.7091364958945,10.7744456170589,10.868891695227399]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.483087450480159,10.552835445896299,10.652011767886684,10.721254053681774,10.816227860853445,10.88219007322949,10.977580612179674]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.281366184303101,10.349588473195499,10.4469477190919,10.5147549228616,10.6080701572601,10.6726610403759,10.7663888804957]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.384179846146132,10.453084357927455,10.55141719628282,10.619902472090217,10.714150858832701,10.779387650779659,10.874052769300658]
[null,null,null,null,"Coincident"]
[null,"BWN","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.426109072448899,27.969997311578602,28.516013038424401,29.091135577891599,29.666595419351101,30.244182748526697,30.821526593423098]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.700370163173389,28.249697284694388,28.801173168808646,29.382046933670516,29.963261373544611,30.546624576011965,31.129741859357328]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.606415045254501,26.1130975436634,26.621907529788199,27.157159970112701,27.692548066979601,28.2300636515624,28.767335751866099]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.862479195707046,26.374228519100036,26.888126605086082,27.428731569813827,27.969473547649397,28.512364288078025,29.055009109384759]
[null,null,null,null,"Coincident"]
[null,"BWR","Substation Rating","MVA","Non-Coincident",81,81,81,81,81,81,81]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",58.269733947175894,58.474970040261603,58.705883904400203,58.860108358165,59.0682803896661,59.302130192220197,59.456515174621806]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",58.852431286647651,59.059719740664221,59.292942743444208,59.448709441746651,59.658963193562762,59.895151494142397,60.051080326368023]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",56.912719740271697,57.108243337034899,57.329444704851099,57.473747884488198,57.671964827982002,57.895859542528697,58.040289436922997]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",57.481846937674412,57.679325770405249,57.90273915189961,58.048485363333079,58.248684476261822,58.474818137953982,58.620692331292226]
[null,null,null,null,"Coincident"]
[null,"CF","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4489240340563498,1.4490211782409899,1.4491183224256299,1.4481438677899601,1.4478851295731698,1.4476263913563701,1.44736765313958]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4634132743969133,1.4635113900233998,1.4636095056498861,1.4626253064678596,1.4623639808689015,1.4621026552699337,1.4618413296709758]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.45244988701057,1.4525480210933999,1.45264615517622,1.4516617708584099,1.4514003961020001,1.4511390213455899,1.4508776465891799]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4669743858806756,1.4670735013043339,1.4671726167279822,1.4661783885669939,1.4659144000630202,1.4656504115590459,1.4653864230550717]
[null,null,null,null,"Coincident"]
[null,"CLN","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",76.690932849330792,80.11241873633341,83.599942407844196,87.529484773100606,91.537723961765607,95.545963150430495,99.554202339095397]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",77.457842177824105,80.913542923696738,84.435941831922634,88.404779620831619,92.453101201383262,96.501422781934806,100.54974436248635]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",72.040714042921195,75.214208863428993,78.416763897069202,82.057709766596702,85.771316800478104,89.484923834359506,93.198530868240894]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",72.761121183350411,75.96635095206328,79.200931536039889,82.878286864262662,86.629029968482882,90.379773072703102,94.130516176923308]
[null,null,null,null,"Coincident"]
[null,"CNR","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.85715436684483,2.8541732834809199,2.851192200117,2.8482111167530801,2.84523003338917,2.8422489500252501,2.83926786666134]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8857259105132784,2.8827150163157294,2.8797041221181701,2.8766932279206108,2.8736823337230617,2.8706714395255029,2.8676605453279533]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8166478234532,2.8137328077469803,2.81081779204077,2.8079027763345499,2.80498776062834,2.8020727449221199,2.79915772921591]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8448143016877321,2.84187013582445,2.8389259699611777,2.8359818040978952,2.8330376382346234,2.8300934723713409,2.8271493065080691]
[null,null,null,null,"Coincident"]
[null,"CPK","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.731129844709997,48.281789073591305,48.832448302472599,49.414860916289001,50.001108257943599,50.587355599598297,51.173602941252902]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.208441143157096,48.764606964327221,49.320772785497326,49.909009525451893,50.501119340523033,51.09322915559428,51.685338970665434]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.710227566796199,45.226603769868802,45.742979972941505,46.2885683191437,46.837684497692095,47.386800676240398,47.935916854788793]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.157329842464165,45.678869807567487,46.200409772670923,46.751454002335137,47.306061342669018,47.8606686830028,48.415276023336681]
[null,null,null,null,"Coincident"]
[null,"CRE","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.018827208634903,58.8724703402359,60.726113471836797,62.440315660279303,64.093325134224102,65.746334608168809,67.399344082113601]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.589015480721251,59.461195043638263,61.333374606555168,63.064718816882099,64.734258385566349,66.403797954250493,68.073337522934736]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",53.560164978952002,55.276926422711597,56.993687866471198,58.5827023895881,60.115656040870803,61.648609692153499,63.181563343436103]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.095766628741522,55.829695686938713,57.563624745135911,59.168529413483981,60.716812601279514,62.265095789075033,63.813378976870467]
[null,null,null,null,"Coincident"]
[null,"CYN","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",75.523894235877393,75.912412616382497,76.3286011861329,76.702795091818501,77.102575015566899,77.476809309323301,77.878713792324902]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.279133178236165,76.671536742546323,77.091887197994225,77.469823042736692,77.873600765722571,78.25157740241653,78.657500930248148]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",72.694311158429599,73.058343565052098,73.450046160919896,73.800966045338086,74.177693356364699,74.528875037399402,74.907726907679205]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",73.42125427001389,73.788927000702614,74.184546622529098,74.538975705791472,74.919470289928341,75.274163787773404,75.656804176755998]
[null,null,null,null,"Coincident"]
[null,"DRN","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",75.616089317951804,77.601387717193603,79.586686116435502,81.568979752511595,83.610337260707112,85.651694768902701,87.693052277098289]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.372250211131316,78.377401594365537,80.382552977599858,82.384669550036705,84.446440633314182,86.508211716591731,88.56998279986928]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",70.906751987942002,72.760053358303992,74.613354728665897,76.467473783598194,78.381676408627399,80.295879033656604,82.210081658685795]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",71.615819507821428,73.487653891887035,75.359488275952558,77.232148521434183,79.165493172713667,81.098837823993165,83.032182475272649]
[null,null,null,null,"Coincident"]
[null,"ELM","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",79.9873774223406,80.792135055924689,81.625796887307402,82.357178978655298,83.101293003372803,83.816502830291711,84.560616855009101]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",80.787251196564,81.60005640648393,82.442054856180476,83.180750768441854,83.932305933406525,84.654667858594635,85.406223023559193]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",74.273261871564486,75.016680341904902,75.789003010043899,76.465094849018797,77.155251825631694,77.816504604446109,78.506661581059006]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",75.015994490280136,75.76684714532395,76.54689304014434,77.229745797508983,77.926804343888008,78.594669650490573,79.291728196869599]
[null,null,null,null,"Coincident"]
[null,"EPG","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",9.8979999999999997,9.8979999999999997,9.8979999999999997,9.8979999999999997,9.8979999999999997,9.8979999999999997,9.8979999999999997]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",71.815204532593398,73.655826147217894,75.582019803599991,77.472186046713389,79.359822467953094,81.251354983137901,83.199328140115597]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",72.533356577919335,74.392384408690077,76.337840001635996,78.246907907180528,80.153420692632622,82.063868532969281,84.031321421516751]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",69.00856144206,70.755551820056596,72.588114239810807,74.387738320038693,76.185053641060108,77.98626505602661,79.843917112786002]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",69.698647056480596,71.46310733825716,73.313995382208915,75.131615703239078,76.946904177470714,78.766127706586872,80.64235628391387]
[null,null,null,null,"Coincident"]
[null,"FGY","Substation Rating","MVA","Non-Coincident",93,93,93,93,93,93,93]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",78.207071745382905,78.869767464052003,79.532463182721003,80.209934344187999,80.887259991996402,81.564585639804903,82.241911287613306]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",78.989142462836739,79.65846513869252,80.327787814548216,81.012033687629881,81.696132591916367,82.380231496202953,83.064330400489439]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",74.246407235018893,74.863648004862796,75.480888774706699,76.111666941147803,76.742311786636506,77.37295663212511,78.003601477613799]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",74.988871307369081,75.612284484911427,76.235697662453774,76.872783610559281,77.509734904502878,78.146686198446361,78.783637492389943]
[null,null,null,null,"Coincident"]
[null,"FTR","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.821872893471301,21.988430492922301,22.154988092373301,22.319085971173699,22.481991575139897,22.644897179106103,22.807802783072301]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.040091622406013,22.208314797851525,22.376537973297033,22.542276830885438,22.706811490891297,22.871346150897164,23.035880810903024]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.637060256036502,21.802501486137199,21.9679427162378,22.130979218263199,22.2928501014338,22.454720984604499,22.616591867775202]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.853430858596866,22.020526500998571,22.18762214340018,22.352289010445833,22.515778602448137,22.679268194450543,22.842757786452953]
[null,null,null,null,"Coincident"]
[null,"HPK","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.8879999999999999,8.8879999999999999,8.8879999999999999,8.8879999999999999,8.8879999999999999,8.8879999999999999,8.8879999999999999]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",55.857050006064306,56.3673562965595,56.876378436354699,57.4118477397775,57.955907069407004,58.4986822483365,59.043135877331601]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",56.415620506124952,56.931029859525097,57.445142220718246,57.985966217175275,58.535466140101072,59.083669070819866,59.633567236104916]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.758054003649498,52.237819054251801,52.716299954154103,53.219161716838101,53.729863998917097,54.239282130296296,54.7503787117409]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.275634543685996,52.76019724479432,53.243462953695641,53.751353334006481,54.267162638906271,54.781674951599257,55.297882498858307]
[null,null,null,null,"Coincident"]
[null,"KLK","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.1403046293397505,5.1741239594221495,5.2069065357636202,5.2630679822991695,5.3337558256319895,5.3655016482325202,5.3950431520558606]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1917076756331477,5.2258651990163711,5.2589756011212563,5.3156986621221609,5.3870933838883097,5.419156664714845,5.4489935835764189]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.00665936944214,5.0392571051114503,5.0708180870398403,5.1257579391623107,5.1952241880820402,5.2257484162694903,5.2540683256797402]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0567259631365618,5.0896496761625647,5.1215262679102391,5.1770155185539339,5.2471764299628605,5.2780059004321851,5.3066090089365376]
[null,null,null,null,"Coincident"]
[null,"KLO","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.534756582148901,30.184844078873898,30.835767027217202,31.470384234154899,32.101131493737604,32.731878753320302,33.363461464521201]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.830104147970392,30.486692519662636,31.144124697489374,31.78508807649645,32.422142808674984,33.059197540853503,33.697096079166414]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.157942204518697,28.7668702119547,29.376633671008999,29.971457918373797,30.562590694511098,31.153723470648501,31.745691698404102]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.439521626563884,29.054538914074246,29.670400007719088,30.271172497557536,30.868216601456208,31.465260705354986,32.063148615388144]
[null,null,null,null,"Coincident"]
[null,"KMS","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.653283285377499,14.061327202926401,14.4973056502576,15.127908566970399,15.763303948183299,16.451963896096,17.168558373790997]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.789816118231274,14.201940474955666,14.642278706760175,15.279187652640104,15.920936987665133,16.616483535056961,17.340243957528909]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.3287167117054,13.725515063622801,14.1502479453224,14.7607387575485,15.3759272916322,16.044380392415601,16.740768022981399]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.462003878822454,13.862770214259029,14.291750424775625,14.908346145123986,15.529686564548522,16.204824196339757,16.908175703211214]
[null,null,null,null,"Coincident"]
[null,"LDL","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.2720000000000002,7.2720000000000002,7.2720000000000002,7.2720000000000002,7.2720000000000002,7.2720000000000002,7.2720000000000002]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",67.142121512439303,67.675327810927001,68.205615000973907,68.794282814568206,69.379055748825706,69.964280313756504,70.552423987127995]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.8135427275637,68.352081089036275,68.88767115098365,69.482225642713885,70.072846306313963,70.663923116894068,71.257948226999275]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.466240310811102,63.957601941314302,64.446044463376694,64.988841041207294,65.527711694243806,66.067033977953599,66.6092753701042]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64.100902713919211,64.59717796072745,65.090504908010459,65.638729451619369,66.182988811186249,66.727704317733142,67.275368123805237]
[null,null,null,null,"Coincident"]
[null,"LGA","Substation Rating","MVA","Non-Coincident",73,73,73,73,73,73,73]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8180000000000001,1.8180000000000001,1.8180000000000001,1.8180000000000001,1.8180000000000001,1.8180000000000001,1.8180000000000001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.043536469037299,33.330901078872898,33.618265688708505,33.898044393718898,34.177269078216398,34.456493762713798,34.735718447211298]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.373971833727673,33.66421008966163,33.954448345595587,34.237024837656087,34.519041768998562,34.801058700340938,35.083075631683414]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.7803184407991,33.063894934394703,33.3474714279903,33.623609524480699,33.899204373372399,34.174799222264099,34.450394071155699]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.10812162520709,33.394533883738653,33.680946142270201,33.959845619725506,34.238196417106124,34.516547214486742,34.794898011867254]
[null,null,null,null,"Coincident"]
[null,"LLG","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.060589792868502,25.566464471611301,26.072339150354001,26.644912667465601,27.233415485849001,27.821918304232497,28.410421122615897]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.311195690797188,25.822129116327414,26.33306254185754,26.911361794140255,27.505749640707492,28.100137487274822,28.694525333842055]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.343026954263003,24.825459386428001,25.307891818593099,25.8528633168204,26.412770661742002,26.9726780066636,27.532585351585201]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.586457223805635,25.073713980292283,25.56097073677903,26.111391949988604,26.676898368359421,27.242404786730237,27.807911205101053]
[null,null,null,null,"Coincident"]
[null,"LYD","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001,0.20200000000000001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.973442219088902,25.297322745651599,25.622164805507399,25.954890643102001,26.287083152175001,26.619275661248,26.952429703614001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.223176641279792,25.550295973108113,25.878386453562474,26.214439549533022,26.549953983696749,26.88546841786048,27.221954000650143]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.201756593531801,23.497983750949,23.795172441659201,24.0996249794246,24.403454430742201,24.707283882059698,25.0120748666703]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.43377415946712,23.732963588458489,24.033124166075794,24.340621229218847,24.647488975049622,24.954356720880295,25.262195615337003]
[null,null,null,null,"Coincident"]
[null,"MBY","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.59396127194003,1.5919505437374901,1.58993981553494,1.5879290873323901,1.58591835912984,1.5839076309272899,1.5818969027247398]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6099008846594303,1.607870049174865,1.6058392136902895,1.603808378205714,1.6017775427211385,1.5997467072365628,1.5977158717519873]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.59396127194003,1.5919505437374901,1.58993981553494,1.5879290873323901,1.58591835912984,1.5839076309272899,1.5818969027247398]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6099008846594303,1.607870049174865,1.6058392136902895,1.603808378205714,1.6017775427211385,1.5997467072365628,1.5977158717519873]
[null,null,null,null,"Coincident"]
[null,"WYK","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.8910891089108911,0.8910891089108911,0.8910891089108911,0.8910891089108911,0.8910891089108911,0.8910891089108911,0.8910891089108911]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.088039723615701,33.290231371227101,33.517581289056899,33.698871397023893,33.902739058038804,34.080386956248802,34.282790089535304]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.418920120851858,33.623133684939376,33.852757101947468,34.035860110994136,34.241766448619195,34.421190825811287,34.625617990430655]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.3437184788182,31.5334054910204,31.7482507734411,31.918450191534802,32.111306710425204,32.277943466510898,32.469335457672898]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.657155663606382,31.848739545930602,32.065733281175511,32.237634693450147,32.432419777529454,32.600722901176006,32.794028812249628]
[null,null,null,null,"Coincident"]
[null,"MFA","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.9390000000000001,3.9390000000000001,3.9390000000000001,3.9390000000000001,3.9390000000000001,3.9390000000000001,3.9390000000000001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.609267737875804,36.8827129040654,37.156158070254996,37.425509661253095,37.694186146016797,37.9628626307804,38.231539115544003]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.975360415254563,37.251540033106053,37.527719650957543,37.799764757865624,38.071128007476965,38.342491257088206,38.61385450669944]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.827369788150101,36.091703618174897,36.3560374481997,36.616518959488204,36.8763651521922,37.136211344896104,37.3960575376001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.185643486031601,36.452620654356643,36.719597822681699,36.982684149083084,37.245128803714124,37.507573458345064,37.770018112976103]
[null,null,null,null,"Coincident"]
[null,"MJG","Substation Rating","MVA","Non-Coincident",20,20,20,20,20,20,20]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0823449146447199,2.0845497655589602,2.0867546164731898,2.0884002279254599,2.0901011493303399,2.0918020707352198,2.0935029921401003]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1031683637911671,2.1053952632145498,2.1076221626379219,2.1092842302047146,2.1110021608236433,2.1127200914425721,2.1144380220615013]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0822019023397802,2.0844062934027603,2.0866106844657404,2.0882559527036602,2.0899565193585499,2.09165708601344,2.0933576526683302]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1030239213631781,2.1052503563367879,2.1074767913103978,2.1091385122306967,2.1108560845521356,2.1125736568735745,2.1142912291950133]
[null,null,null,null,"Coincident"]
[null,"MOE","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",10.907999999999999,10.907999999999999,10.907999999999999,10.907999999999999,10.907999999999999,10.907999999999999,10.907999999999999]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.0249451208363,36.261822132585699,36.5141660687732,36.807882510959701,37.114736237461599,37.419380403329505,37.724024569197496]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.385194572044661,36.624440353911559,36.879307729460933,37.1759613360693,37.485883599836214,37.793574207362802,38.101264814889468]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.763763740428494,34.992791556594497,35.237286297198601,35.520734421937497,35.817169644086896,36.111395305602201,36.4056209671175]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.111401377832777,35.342719472160439,35.589659160170591,35.87594176615687,36.175341340527766,36.472509258658221,36.769677176788676]
[null,null,null,null,"Coincident"]
[null,"MSD","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.677721306118698,16.819622753916999,16.988347552321098,17.075795648395097,17.212009761116001,17.375047224442699,17.461551508561801]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.844498519179886,16.987818981456169,17.158231027844309,17.246553604879047,17.38412985872716,17.548797696687128,17.63616702364742]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.486465454703499,16.626045968392098,16.792449832686501,16.877696413364799,17.0117327712593,17.1725924797597,17.2569190090524]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.651330109250534,16.792306428076021,16.960374331013366,17.046473377498447,17.181850098971893,17.344318404557299,17.429488199142924]
[null,null,null,null,"Coincident"]
[null,"MYT","Substation Rating","MVA","Non-Coincident",20,20,20,20,20,20,20]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.24837355,12.31947499,12.389015880000001,12.46011732,12.52965822,12.637595170000001,12.76384796]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.3708572855,12.442669739899999,12.512906038800001,12.5847184932,12.654954802200001,12.763971121700001,12.8914864396]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.15020337,12.22035758,12.28895125,12.35910546,12.42769912,12.534688840000001,12.659994409999999]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.2717054037,12.3425611558,12.411840762500001,12.482696514600001,12.5519761112,12.6600357284,12.7865943541]
[null,null,null,null,"Coincident"]
[null,"NLA","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.832326112554,12.869959038808499,12.8565851512384,12.877141596250299,12.9149901499944,12.903284718937702,12.889910831367601]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.960649373679541,12.998658629196584,12.985151002750785,13.005913012212803,13.044140051494345,13.032317566127078,13.018809939681278]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.639206700808099,12.6770518674897,12.663890220346701,12.6846589057857,12.7227196999568,12.7112265093271,12.698064862184099]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.765598767816181,12.803822386164597,12.790529122550168,12.811505494843557,12.849946896956368,12.83833877442037,12.825045510805939]
[null,null,null,null,"Coincident"]
[null,"NRN","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.8680000000000003,6.8680000000000003,6.8680000000000003,6.8680000000000003,6.8680000000000003,6.8680000000000003,6.8680000000000003]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.6144615908118,26.903621793962898,27.195209466208301,27.498371313643201,27.8039095738418,28.109447834040299,28.414986094238799]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.880606206719918,27.172658011902527,27.467161560870384,27.773355026779633,28.081948669580218,28.390542312380703,28.699135955181188]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.722718879309401,25.999289852945999,26.278288295676898,26.568016172293301,26.8599186954883,27.1518212186832,27.443723741878198]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.979946068102496,26.25928275147546,26.541071178633668,26.833696334016235,27.128517882443184,27.423339430870033,27.718160979296979]
[null,null,null,null,"Coincident"]
[null,"OFR","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.853185551123097,54.548214110623796,56.244602488384899,57.910334547519696,59.632995901440594,61.357017073621904,63.081038245803207]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.38171740663433,55.093696251730037,56.807048513268747,58.489437892994893,60.229325860454999,61.970587244358121,63.711848628261237]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.737117999091303,51.326577695987602,52.917397211144198,54.483859801345702,56.108608286250302,57.7347165894152,59.360824892580204]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",50.234489179082217,51.839843472947479,53.446571183255642,55.028698399359158,56.669694369112804,58.312063755309353,59.954433141506009]
[null,null,null,null,"Coincident"]
[null,"PHI","Substation Rating","MVA","Non-Coincident",26,26,26,26,26,26,26]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.905340405768797,25.205309348722302,25.5333133869458,25.767783091503599,26.052186978507301,26.364625960781101,26.597074378045399]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.154393809826484,25.457362442209526,25.788646520815259,26.025460922418635,26.312708848292374,26.628272220388912,26.863045121825852]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.921565681731,24.206331602622701,24.519132618784401,24.7392372056777,25.009541938611299,25.307881766815001,25.5262310300092]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.160781338548311,24.448394918648926,24.764323944972244,24.986629577734476,25.259637357997413,25.560960584483151,25.781493340309293]
[null,null,null,null,"Coincident"]
[null,"PHM","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.0571643201718,58.399784670590698,59.744081976604399,61.024457489234898,62.2849903001431,63.547200066646298,64.811086788744205]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.627735963373517,58.983782517296603,60.341522796370441,61.634702064127247,62.907840203144531,64.182672067312765,65.459197656631645]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",54.281817134902397,55.529812562908198,56.779484946508703,57.970582025077199,59.143488962330096,60.318072855177903,61.494333703620498]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.824635306251423,56.085110688537277,57.34727979597379,58.550287845327972,59.734923851953397,60.92125358372968,62.109277040656707]
[null,null,null,null,"Coincident"]
[null,"WOTS","Substation Rating","MVA","Non-Coincident",70.400000000000006,70.400000000000006,70.400000000000006,70.400000000000006,70.400000000000006,70.400000000000006,70.400000000000006]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",49.504950495049506,49.504950495049506,49.504950495049506,49.504950495049506,49.504950495049506,49.504950495049506,49.504950495049506]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.711363970000001,35.042371090000003,35.350153579999997,35.677805670000005,35.982339339999996,36.310097650000003,36.614631320000001]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.058477609699999,35.392794800900006,35.703655115799997,36.034583726700006,36.342162733399995,36.673198626500003,36.980777633199999]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.013446129999998,34.334045949999997,34.63142113,34.948787689999996,35.243031960000003,35.560500879999999,35.854745149999999]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.353580591300002,34.677386409499995,34.977735341299997,35.298275566899996,35.595462279600007,35.916105888799997,36.213292601500001]
[null,null,null,null,"Coincident"]
[null,"RWN","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.931194769070601,46.376974701749504,46.822754634428399,47.2853999572189,47.758662567024999,48.231925176830998,48.705187786637097]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.390506716761308,46.840744448766998,47.290982180772687,47.758253956791087,48.236249192695247,48.714244428599308,49.192239664503468]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.438302388967401,42.846495483595199,43.254688578223004,43.678406344069401,44.1119628268195,44.545519309569599,44.979075792319705]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.862685412857076,43.274960438431151,43.687235464005234,44.115190407510099,44.553082455087697,44.990974502665296,45.428866550242901]
[null,null,null,null,"Coincident"]
[null,"SLE","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.318239379052194,33.715017335526795,34.1121984383525,34.480305099302001,34.8454760104961,35.210646921690099,35.575817832884198]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.651421772842717,34.052167508882064,34.453320422736027,34.825108150295023,35.193930770601064,35.562753390906998,35.931576011213039]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.332865191929997,32.712778512328605,33.093094979078202,33.446351371675597,33.796861509298793,34.147371646922103,34.497881784545299]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.656193843849294,33.039906297451893,33.424025928868986,33.780814885392353,34.134830124391783,34.488845363391327,34.842860602390751]
[null,null,null,null,"Coincident"]
[null,"SMG","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.433898350827597,37.824446809823904,38.214995268820296,38.529242912245202,38.860716352222397,39.192189792199599,39.523663232176794]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.808237334335871,38.202691277922142,38.597145221508498,38.914535341367653,39.249323515744621,39.584111690121595,39.918899864498563]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.666323299228402,36.036201465005497,36.4060796307826,36.7059140534625,37.021561665809102,37.337209278155697,37.652856890502299]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.022986532220685,36.396563479655555,36.770140427090425,37.072973193997129,37.391777282467196,37.710581370937255,38.029385459407322]
[null,null,null,null,"Coincident"]
[null,"SMR","Substation Rating","MVA","Non-Coincident",38.5,38.5,38.5,38.5,38.5,38.5,38.5]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.784209089744401,33.947739384472904,34.0826417527621,34.239123350427796,34.363581260778197,34.517230354281203,34.641688264631703]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.122051180641847,34.287216778317635,34.423468170289723,34.581514583932076,34.707217073385976,34.862402657824013,34.98810514727802]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.161653750586197,33.321076767718303,33.451871858411202,33.6044955912527,33.7251884464225,33.875072484744905,33.995765339914797]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.493270288092056,33.654287535395483,33.786390576995316,33.940540547165227,34.062440330886723,34.213823209592356,34.335722993313944]
[null,null,null,null,"Coincident"]
[null,"TGN","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",10.1,10.1,10.1,10.1,10.1,10.1,10.1]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.471755060311104,52.0738052674862,52.675855474661304,53.213453789556503,53.7328990169447,54.2534167938542,54.773123296104799]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.986472610914213,52.594543320161065,53.202614029407918,53.745588327452069,54.270228007114149,54.795950961792741,55.320854529065848]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.4450534462703,50.015381432790399,50.585709419310497,51.095783180565199,51.5885196702095,52.082328709375098,52.575326473881802]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.939503980733001,50.515535247118301,51.091566513503601,51.606741012370854,52.104404866911594,52.603151996468846,53.101079738620619]
[null,null,null,null,"Coincident"]
[null,"TT","Substation Rating","MVA","Non-Coincident",84,84,84,84,84,84,84]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",79.8442274321973,80.233596572610409,80.623238600405301,80.99952867615491,81.37153195813849,81.705384798230895,82.039510525705097]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",80.642669706519271,81.03593253833651,81.429470986409356,81.809523962916458,82.185247277719881,82.522438646213203,82.859905630962146]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",78.221108530294188,78.5931864581772,78.965537273441996,79.326062095561198,79.682519830295305,80.000827123138194,80.319407303362894]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",79.003319615597135,79.37911832275897,79.755192646176411,80.119322716516805,80.47934502859826,80.800835394369571,81.122601376396517]
[null,null,null,null,"Coincident"]
[null,"WGI","Substation Rating","MVA","Non-Coincident",40.5,40.5,40.5,40.5,40.5,40.5,40.5]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.12,12.12,12.12,12.12,12.12,12.12,12.12]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.5442271933778,41.027517088038401,41.510806982699094,41.9979882504608,42.485530001248996,42.973071752037299,43.460613502825602]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.94966946531158,41.437792258918783,41.925915052526086,42.417968132965406,42.910385301261485,43.40280246955767,43.895219637853856]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.273165365713801,39.739123859646199,40.205082353578504,40.674744062576401,41.144748824306603,41.614753586036798,42.084758347767]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.665897019370938,40.136515098242661,40.607133177114292,41.081491503202166,41.556196312549673,42.030901121897166,42.505605931244673]
[null,null,null,null,"Coincident"]
[null,"WGL","Substation Rating","MVA","Non-Coincident",84,84,84,84,84,84,84]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",77.0001403310375,78.943088149116505,80.739016983649904,82.616934990649995,84.430121429068507,86.16376896559791,87.898068342374003]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",77.770141734347874,79.732519030607676,81.546407153486399,83.443104340556502,85.274422643359188,87.025406655253889,88.777049025797737]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",74.023095861702203,75.883054236665103,77.649781990915002,79.450226135619403,81.186763792716604,82.843762547924797,84.501413143379494]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",74.763326820319222,76.641884779031756,78.426279810824155,80.244728396975603,81.998631430643769,83.67220017340405,85.346427274813294]
[null,null,null,null,"Coincident"]
[null,"WN","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.323,2.323,2.323,2.323,2.323,2.323,2.323]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.805573565880898,49.1210471640657,49.459608082751402,49.696144476497196,49.9730035247429,50.272949893489596,50.507022834889597]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",49.29362930153971,49.612257635706356,49.954204163578915,50.193105921262166,50.472733559990331,50.775679392424493,51.012093063238495]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",47.573063001963497,47.876258692625001,48.202541703787503,48.428364407530495,48.694616356598495,48.9839556261675,49.207421468389704]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.048793631983131,48.355021279551252,48.684567120825378,48.9126480516058,49.181562520164483,49.473795182429178,49.6994956830736]
[null,null,null,null,"Coincident"]
[null,"WO","Substation Rating","MVA","Non-Coincident",99,99,99,99,99,99,99]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.593696530936,41.993328442724099,42.392960354512198,42.791258633999,43.189547134873798,43.848641252076,44.267141063661597]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.009633496245364,42.413261727151344,42.816889958057317,43.219171220338993,43.621442606222537,44.28712766459676,44.709812474298211]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.890326716807998,41.279319223735101,41.668311730662204,42.0560244587491,42.443727803094504,43.018829929869597,43.425717326575196]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.299229983976076,41.692112415972453,42.084994847968829,42.476584703336592,42.868165081125447,43.449018229168296,43.859974499840945]
[null,null,null,null,"Coincident"]
[null,"WT","Substation Rating","MVA","Non-Coincident",109,109,109,109,109,109,109]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.328595044373699,69.969398746044902,70.610202447716006,71.243400574094807,71.873065355047004,72.504350448397702,73.1356355417483]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",70.021880994817437,70.669092733505352,71.316304472193167,71.955834579835752,72.59179600859747,73.229393952881679,73.866991897165789]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",65.114477233313409,65.721432917000399,66.328388600687489,66.9283400132868,67.524996437417101,68.12327317394579,68.721549910474394]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",65.765622005646549,66.378647246170402,66.99167248669437,67.597623413419669,68.200246401791276,68.804505905685247,69.408765409579132]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Clyde North",null,"MWh","Non-Coincident",3.7,5.0999999999999996,7.2,11.7,28.2,35,44.9]
[null,"Maffra",null,"MWh","Non-Coincident",47.5,52.4,57.7,63.3,69.400000000000006,75,80.8]
[null,"Thomastown",null,"MWh","Non-Coincident",86.7,95.4,105,115.4,126.7,137,147.6]
[null,"Watsonia",null,"MWh","Non-Coincident",33.200000000000003,35.700000000000003,38.5,41.3,44.4,47.3,50.2]
[null,"Benalla",null,"MWh","Non-Coincident",26.8,29.1,31.6,34.200000000000003,37,39.6,42.3]
[null,"Bayswater",null,"MWh","Non-Coincident",38.4,41.4,44.5,47.9,51.3,54.6,57.9]
[null,"Traralgon",null,"MWh","Non-Coincident",22.4,24.6,27,29.7,32.6,35.200000000000003,38]
[null,"Warragul",null,"MWh","Non-Coincident",39.4,47.9,58.1,70.5,85,97.1,110]
[null,"Newmerella",null,"MWh","Non-Coincident",16.7,18.399999999999999,20.2,22.1,24.2,26.1,28.1]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.1 Telephone answering","index":32,"n_rows":1833,"n_cols":4,"rows_kept":1833,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"6.1 TELEPHONE ANSWERING"]
[]
[null,"6.1.1 - TELEPHONE ANSWERING DATA"]
["C10 starts at first day of PRCP_y5 and goes for 5 full years","Date","Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) "]
[null,"2015-01-01",118,112]
[null,{"$f":"B8+1","v":"2015-01-02"},300,281]
[null,"2015-01-03",1049,651]
[null,"2015-01-04",311,232]
[null,"2015-01-05",341,288]
[null,"2015-01-06",266,252]
[null,"2015-01-07",1344,1011]
[null,"2015-01-08",1624,1137]
[null,"2015-01-09",391,377]
[null,"2015-01-10",264,231]
[null,"2015-01-11",191,163]
[null,"2015-01-12",268,253]
[null,"2015-01-13",338,289]
[null,"2015-01-14",373,332]
[null,"2015-01-15",215,206]
[null,"2015-01-16",256,242]
[null,"2015-01-17",123,112]
[null,"2015-01-18",182,139]
[null,"2015-01-19",246,234]
[null,"2015-01-20",346,299]
[null,"2015-01-21",322,314]
[null,"2015-01-22",377,332]
[null,"2015-01-23",406,346]
[null,"2015-01-24",146,127]
[null,"2015-01-25",93,89]
[null,"2015-01-26",110,90]
[null,"2015-01-27",302,248]
[null,"2015-01-28",251,235]
[null,"2015-01-29",292,262]
[null,"2015-01-30",275,254]
[null,"2015-01-31",152,121]
[null,"2015-02-01",112,108]
[null,"2015-02-02",284,247]
[null,"2015-02-03",227,202]
[null,"2015-02-04",239,216]
[null,"2015-02-05",247,230]
[null,"2015-02-06",228,214]
[null,"2015-02-07",185,170]
[null,"2015-02-08",140,127]
[null,"2015-02-09",241,231]
[null,"2015-02-10",268,251]
[null,"2015-02-11",471,385]
[null,"2015-02-12",511,450]
[null,"2015-02-13",667,573]
[null,"2015-02-14",575,411]
[null,"2015-02-15",210,190]
[null,"2015-02-16",340,304]
[null,"2015-02-17",269,231]
[null,"2015-02-18",274,262]
[null,"2015-02-19",316,291]
[null,"2015-02-20",284,247]
[null,"2015-02-21",189,167]
[null,"2015-02-22",163,143]
[null,"2015-02-23",1001,754]
[null,"2015-02-24",350,313]
[null,"2015-02-25",248,205]
[null,"2015-02-26",313,292]
[null,"2015-02-27",232,200]
[null,"2015-02-28",911,203]
[null,"2015-03-01",1700,850]
[null,"2015-03-02",555,480]
[null,"2015-03-03",259,230]
[null,"2015-03-04",287,241]
[null,"2015-03-05",525,408]
[null,"2015-03-06",431,373]
[null,{"$f":"B72+1","v":"2015-03-07"},135,104]
[null,"2015-03-08",79,77]
[null,"2015-03-09",104,98]
[null,"2015-03-10",229,203]
[null,"2015-03-11",222,202]
[null,"2015-03-12",222,209]
[null,"2015-03-13",238,212]
[null,"2015-03-14",180,150]
[null,"2015-03-15",162,135]
[null,"2015-03-16",257,241]
[null,"2015-03-17",240,221]
[null,"2015-03-18",218,196]
[null,"2015-03-19",426,366]
[null,"2015-03-20",319,281]
[null,"2015-03-21",149,131]
[null,"2015-03-22",165,144]
[null,"2015-03-23",213,198]
[null,"2015-03-24",249,229]
[null,"2015-03-25",299,271]
[null,"2015-03-26",270,246]
[null,"2015-03-27",196,184]
[null,"2015-03-28",107,84]
[null,"2015-03-29",75,71]
[null,"2015-03-30",180,173]
[null,"2015-03-31",297,275]
[null,"2015-04-01",201,192]
[null,"2015-04-02",248,236]
[null,"2015-04-03",88,85]
[null,"2015-04-04",75,71]
[null,"2015-04-05",93,89]
[null,"2015-04-06",78,72]
[null,"2015-04-07",505,442]
[null,"2015-04-08",344,313]
[null,"2015-04-09",278,255]
[null,"2015-04-10",210,193]
[null,"2015-04-11",122,99]
[null,"2015-04-12",69,65]
[null,"2015-04-13",223,208]
[null,"2015-04-14",223,199]
[null,"2015-04-15",289,268]
[null,"2015-04-16",257,243]
[null,"2015-04-17",187,181]
[null,"2015-04-18",144,130]
[null,"2015-04-19",137,117]
[null,"2015-04-20",176,166]
[null,"2015-04-21",317,272]
[null,"2015-04-22",254,237]
[null,"2015-04-23",211,196]
[null,"2015-04-24",142,132]
[null,"2015-04-25",125,113]
[null,"2015-04-26",102,100]
[null,"2015-04-27",245,235]
[null,"2015-04-28",208,193]
[null,"2015-04-29",202,195]
[null,"2015-04-30",753,280]
[null,"2015-05-01",203,190]
[null,"2015-05-02",108,94]
[null,"2015-05-03",69,67]
[null,"2015-05-04",236,203]
[null,"2015-05-05",381,360]
[null,"2015-05-06",325,287]
[null,"2015-05-07",237,227]
[null,"2015-05-08",236,223]
[null,"2015-05-09",120,106]
[null,{"$f":"B136+1","v":"2015-05-10"},157,138]
[null,"2015-05-11",272,244]
[null,"2015-05-12",283,245]
[null,"2015-05-13",300,249]
[null,"2015-05-14",242,231]
[null,"2015-05-15",181,172]
[null,"2015-05-16",145,122]
[null,"2015-05-17",173,132]
[null,"2015-05-18",195,185]
[null,"2015-05-19",238,227]
[null,"2015-05-20",228,218]
[null,"2015-05-21",346,306]
[null,"2015-05-22",177,171]
[null,"2015-05-23",104,92]
[null,"2015-05-24",141,124]
[null,"2015-05-25",234,205]
[null,"2015-05-26",218,186]
[null,"2015-05-27",218,203]
[null,"2015-05-28",292,250]
[null,"2015-05-29",235,224]
[null,"2015-05-30",95,87]
[null,"2015-05-31",140,131]
[null,"2015-06-01",303,263]
[null,"2015-06-02",302,273]
[null,"2015-06-03",261,213]
[null,"2015-06-04",283,238]
[null,"2015-06-05",195,178]
[null,"2015-06-06",114,97]
[null,"2015-06-07",191,163]
[null,"2015-06-08",181,160]
[null,"2015-06-09",353,288]
[null,"2015-06-10",252,228]
[null,"2015-06-11",421,370]
[null,"2015-06-12",212,199]
[null,"2015-06-13",85,72]
[null,"2015-06-14",145,120]
[null,"2015-06-15",192,159]
[null,"2015-06-16",252,218]
[null,"2015-06-17",255,221]
[null,"2015-06-18",215,198]
[null,"2015-06-19",217,198]
[null,"2015-06-20",83,66]
[null,"2015-06-21",116,104]
[null,"2015-06-22",274,245]
[null,"2015-06-23",273,232]
[null,"2015-06-24",232,226]
[null,"2015-06-25",210,200]
[null,"2015-06-26",198,184]
[null,"2015-06-27",84,75]
[null,"2015-06-28",83,76]
[null,"2015-06-29",235,221]
[null,"2015-06-30",314,268]
[null,"2015-07-01",322,306]
[null,"2015-07-02",413,383]
[null,"2015-07-03",204,193]
[null,"2015-07-04",184,152]
[null,"2015-07-05",109,97]
[null,"2015-07-06",261,229]
[null,"2015-07-07",246,199]
[null,"2015-07-08",228,211]
[null,"2015-07-09",204,200]
[null,"2015-07-10",195,188]
[null,"2015-07-11",154,126]
[null,"2015-07-12",282,239]
[null,{"$f":"B200+1","v":"2015-07-13"},562,443]
[null,"2015-07-14",337,271]
[null,"2015-07-15",267,243]
[null,"2015-07-16",188,180]
[null,"2015-07-17",187,175]
[null,"2015-07-18",119,107]
[null,"2015-07-19",133,111]
[null,"2015-07-20",294,259]
[null,"2015-07-21",408,381]
[null,"2015-07-22",431,373]
[null,"2015-07-23",274,244]
[null,"2015-07-24",181,169]
[null,"2015-07-25",139,117]
[null,"2015-07-26",242,215]
[null,"2015-07-27",246,221]
[null,"2015-07-28",213,199]
[null,"2015-07-29",344,275]
[null,"2015-07-30",406,346]
[null,"2015-07-31",286,250]
[null,"2015-08-01",142,128]
[null,"2015-08-02",156,115]
[null,"2015-08-03",365,345]
[null,"2015-08-04",212,175]
[null,"2015-08-05",268,241]
[null,"2015-08-06",218,207]
[null,"2015-08-07",180,164]
[null,"2015-08-08",121,114]
[null,"2015-08-09",142,120]
[null,"2015-08-10",198,186]
[null,"2015-08-11",210,196]
[null,"2015-08-12",204,188]
[null,"2015-08-13",176,164]
[null,"2015-08-14",160,140]
[null,"2015-08-15",173,120]
[null,"2015-08-16",83,76]
[null,"2015-08-17",233,219]
[null,"2015-08-18",298,260]
[null,"2015-08-19",257,243]
[null,"2015-08-20",345,314]
[null,"2015-08-21",187,171]
[null,"2015-08-22",100,91]
[null,"2015-08-23",106,90]
[null,"2015-08-24",192,163]
[null,"2015-08-25",195,190]
[null,"2015-08-26",174,158]
[null,"2015-08-27",338,295]
[null,"2015-08-28",218,201]
[null,"2015-08-29",111,92]
[null,"2015-08-30",163,146]
[null,"2015-08-31",150,141]
[null,"2015-09-01",189,161]
[null,"2015-09-02",209,195]
[null,"2015-09-03",235,219]
[null,"2015-09-04",182,174]
[null,"2015-09-05",72,63]
[null,"2015-09-06",77,75]
[null,"2015-09-07",263,236]
[null,"2015-09-08",218,201]
[null,"2015-09-09",288,256]
[null,"2015-09-10",248,237]
[null,"2015-09-11",178,172]
[null,"2015-09-12",114,98]
[null,"2015-09-13",107,95]
[null,"2015-09-14",326,275]
[null,{"$f":"B264+1","v":"2015-09-15"},287,253]
[null,"2015-09-16",204,187]
[null,"2015-09-17",224,205]
[null,"2015-09-18",235,214]
[null,"2015-09-19",129,115]
[null,"2015-09-20",198,154]
[null,"2015-09-21",394,306]
[null,"2015-09-22",378,338]
[null,"2015-09-23",322,274]
[null,"2015-09-24",293,247]
[null,"2015-09-25",398,372]
[null,"2015-09-26",144,136]
[null,"2015-09-27",155,153]
[null,"2015-09-28",229,209]
[null,"2015-09-29",339,274]
[null,"2015-09-30",251,222]
[null,"2015-10-01",247,197]
[null,"2015-10-02",131,118]
[null,"2015-10-03",134,112]
[null,"2015-10-04",67,65]
[null,"2015-10-05",482,284]
[null,"2015-10-06",1017,891]
[null,"2015-10-07",263,227]
[null,"2015-10-08",342,226]
[null,"2015-10-09",283,221]
[null,"2015-10-10",205,181]
[null,"2015-10-11",253,211]
[null,"2015-10-12",240,216]
[null,"2015-10-13",323,257]
[null,"2015-10-14",317,289]
[null,"2015-10-15",297,242]
[null,"2015-10-16",244,218]
[null,"2015-10-17",149,143]
[null,"2015-10-18",223,189]
[null,"2015-10-19",234,205]
[null,"2015-10-20",356,313]
[null,"2015-10-21",314,265]
[null,"2015-10-22",234,215]
[null,"2015-10-23",188,180]
[null,"2015-10-24",94,87]
[null,"2015-10-25",235,194]
[null,"2015-10-26",325,280]
[null,"2015-10-27",276,251]
[null,"2015-10-28",277,251]
[null,"2015-10-29",274,237]
[null,"2015-10-30",215,201]
[null,"2015-10-31",306,267]
[null,"2015-11-01",305,285]
[null,"2015-11-02",602,247]
[null,"2015-11-03",124,107]
[null,"2015-11-04",371,322]
[null,"2015-11-05",307,275]
[null,"2015-11-06",254,237]
[null,"2015-11-07",180,163]
[null,"2015-11-08",98,95]
[null,"2015-11-09",234,205]
[null,"2015-11-10",210,200]
[null,"2015-11-11",230,217]
[null,"2015-11-12",658,538]
[null,"2015-11-13",272,219]
[null,"2015-11-14",117,99]
[null,"2015-11-15",108,107]
[null,"2015-11-16",216,208]
[null,"2015-11-17",234,219]
[null,{"$f":"B328+1","v":"2015-11-18"},274,248]
[null,"2015-11-19",348,311]
[null,"2015-11-20",453,357]
[null,"2015-11-21",175,146]
[null,"2015-11-22",115,111]
[null,"2015-11-23",193,182]
[null,"2015-11-24",382,301]
[null,"2015-11-25",911,533]
[null,"2015-11-26",1447,864]
[null,"2015-11-27",240,215]
[null,"2015-11-28",131,109]
[null,"2015-11-29",123,86]
[null,"2015-11-30",739,321]
[null,"2015-12-01",505,418]
[null,"2015-12-02",243,224]
[null,"2015-12-03",210,201]
[null,"2015-12-04",273,244]
[null,"2015-12-05",131,118]
[null,"2015-12-06",123,110]
[null,"2015-12-07",253,228]
[null,"2015-12-08",585,443]
[null,"2015-12-09",289,270]
[null,"2015-12-10",263,228]
[null,"2015-12-11",281,259]
[null,"2015-12-12",200,155]
[null,"2015-12-13",106,104]
[null,"2015-12-14",276,253]
[null,"2015-12-15",433,379]
[null,"2015-12-16",235,231]
[null,"2015-12-17",428,320]
[null,"2015-12-18",788,635]
[null,"2015-12-19",1292,876]
[null,"2015-12-20",1956,1132]
[null,"2015-12-21",442,401]
[null,"2015-12-22",337,309]
[null,"2015-12-23",214,206]
[null,"2015-12-24",216,202]
[null,"2015-12-25",201,194]
[null,"2015-12-26",275,256]
[null,"2015-12-27",115,109]
[null,"2015-12-28",129,125]
[null,"2015-12-29",189,184]
[null,"2015-12-30",148,146]
[null,"2015-12-31",493,471]
[null,"2016-01-01",137,135]
[null,"2016-01-02",319,227]
[null,"2016-01-03",377,315]
[null,"2016-01-04",327,292]
[null,"2016-01-05",320,282]
[null,"2016-01-06",213,203]
[null,"2016-01-07",211,193]
[null,"2016-01-08",153,139]
[null,"2016-01-09",116,108]
[null,"2016-01-10",158,148]
[null,"2016-01-11",352,316]
[null,"2016-01-12",318,287]
[null,"2016-01-13","???","???"]
[null,"2016-01-14",471,674]
[null,"2016-01-15",290,236]
[null,"2016-01-16",146,124]
[null,"2016-01-17",116,111]
[null,"2016-01-18",316,288]
[null,"2016-01-19",297,240]
[null,"2016-01-20",522,468]
[null,{"$f":"B392+1","v":"2016-01-21"},260,239]
[null,"2016-01-22",311,265]
[null,"2016-01-23",122,105]
[null,"2016-01-24",133,125]
[null,"2016-01-25",192,184]
[null,"2016-01-26",116,110]
[null,"2016-01-27",700,355]
[null,"2016-01-28",578,435]
[null,"2016-01-29",448,341]
[null,"2016-01-30",276,232]
[null,"2016-01-31",369,298]
[null,"2016-02-01",338,311]
[null,"2016-02-02",393,295]
[null,"2016-02-03",408,330]
[null,"2016-02-04",236,216]
[null,"2016-02-05",379,256]
[null,"2016-02-06",137,119]
[null,"2016-02-07",149,143]
[null,"2016-02-08",248,239]
[null,"2016-02-09",225,188]
[null,"2016-02-10",241,218]
[null,"2016-02-11",241,210]
[null,"2016-02-12",225,208]
[null,"2016-02-13",206,174]
[null,"2016-02-14",138,136]
[null,"2016-02-15",381,298]
[null,"2016-02-16",225,208]
[null,"2016-02-17",245,211]
[null,"2016-02-18",225,210]
[null,"2016-02-19",294,279]
[null,"2016-02-20",145,136]
[null,"2016-02-21",140,124]
[null,"2016-02-22",252,233]
[null,"2016-02-23",466,383]
[null,"2016-02-24",1009,348]
[null,"2016-02-25",306,259]
[null,"2016-02-26",233,192]
[null,"2016-02-27",108,103]
[null,"2016-02-28",123,109]
[null,"2016-02-29",358,308]
[null,"2016-03-01",314,290]
[null,"2016-03-02",273,257]
[null,"2016-03-03",302,225]
[null,"2016-03-04",311,265]
[null,"2016-03-05",156,146]
[null,"2016-03-06",149,142]
[null,"2016-03-07",280,244]
[null,"2016-03-08",621,326]
[null,"2016-03-09",422,343]
[null,"2016-03-10",454,368]
[null,"2016-03-11",330,273]
[null,"2016-03-12",141,122]
[null,"2016-03-13",71,71]
[null,"2016-03-14",122,117]
[null,"2016-03-15",321,274]
[null,"2016-03-16",290,252]
[null,"2016-03-17",268,254]
[null,"2016-03-18","???","???"]
[null,"2016-03-19",283,320]
[null,"2016-03-20",206,176]
[null,"2016-03-21",225,186]
[null,"2016-03-22",233,200]
[null,"2016-03-23",242,214]
[null,"2016-03-24",227,212]
[null,{"$f":"B456+1","v":"2016-03-25"},118,107]
[null,"2016-03-26",113,104]
[null,"2016-03-27",121,109]
[null,"2016-03-28",170,153]
[null,"2016-03-29",233,203]
[null,"2016-03-30",281,257]
[null,"2016-03-31",324,275]
[null,"2016-04-01",215,185]
[null,"2016-04-02",80,76]
[null,"2016-04-03",104,99]
[null,"2016-04-04",238,219]
[null,"2016-04-05",285,268]
[null,"2016-04-06",319,307]
[null,"2016-04-07",248,209]
[null,"2016-04-08",237,211]
[null,"2016-04-09",117,105]
[null,"2016-04-10",115,95]
[null,"2016-04-11",217,174]
[null,"2016-04-12",256,237]
[null,"2016-04-13",202,187]
[null,"2016-04-14",192,164]
[null,"2016-04-15",178,162]
[null,"2016-04-16",114,104]
[null,"2016-04-17",137,128]
[null,"2016-04-18",184,177]
[null,"2016-04-19",162,157]
[null,"2016-04-20",233,221]
[null,"2016-04-21",192,173]
[null,"2016-04-22",185,168]
[null,"2016-04-23",127,116]
[null,"2016-04-24",69,67]
[null,"2016-04-25",57,54]
[null,"2016-04-26",258,211]
[null,"2016-04-27",208,195]
[null,"2016-04-28",222,201]
[null,"2016-04-29",308,274]
[null,"2016-04-30",152,127]
[null,"2016-05-01","???","???"]
[null,"2016-05-02",552,731]
[null,"2016-05-03","???","???"]
[null,"2016-05-04",470,385]
[null,"2016-05-05",334,293]
[null,"2016-05-06",368,270]
[null,"2016-05-07",140,132]
[null,"2016-05-08",124,120]
[null,"2016-05-09",610,467]
[null,"2016-05-10",384,336]
[null,"2016-05-11",286,250]
[null,"2016-05-12",301,267]
[null,"2016-05-13",230,213]
[null,"2016-05-14",102,96]
[null,"2016-05-15",131,108]
[null,"2016-05-16",227,208]
[null,"2016-05-17",256,224]
[null,"2016-05-18",218,178]
[null,"2016-05-19",230,210]
[null,"2016-05-20",193,166]
[null,"2016-05-21",83,74]
[null,"2016-05-22",109,102]
[null,"2016-05-23",244,223]
[null,"2016-05-24",176,156]
[null,"2016-05-25",204,190]
[null,"2016-05-26",230,219]
[null,"2016-05-27",267,208]
[null,{"$f":"B520+1","v":"2016-05-28"},173,142]
[null,"2016-05-29",133,116]
[null,"2016-05-30",228,205]
[null,"2016-05-31",245,218]
[null,"2016-06-01",196,166]
[null,"2016-06-02",270,232]
[null,"2016-06-03",171,142]
[null,"2016-06-04",138,128]
[null,"2016-06-05",149,125]
[null,"2016-06-06",232,199]
[null,"2016-06-07",301,265]
[null,"2016-06-08",230,209]
[null,"2016-06-09",260,239]
[null,"2016-06-10",188,166]
[null,"2016-06-11",117,107]
[null,"2016-06-12",102,93]
[null,"2016-06-13",76,74]
[null,"2016-06-14",207,190]
[null,"2016-06-15",210,182]
[null,"2016-06-16",186,161]
[null,"2016-06-17",171,147]
[null,"2016-06-18",151,145]
[null,"2016-06-19",87,84]
[null,"2016-06-20",302,246]
[null,"2016-06-21",241,206]
[null,"2016-06-22",208,169]
[null,"2016-06-23",409,391]
[null,"2016-06-24",339,305]
[null,"2016-06-25",185,162]
[null,"2016-06-26",102,95]
[null,"2016-06-27",287,242]
[null,"2016-06-28",267,234]
[null,"2016-06-29",242,200]
[null,"2016-06-30",416,335]
[null,"2016-07-01",266,207]
[null,"2016-07-02",122,118]
[null,"2016-07-03",75,66]
[null,"2016-07-04",188,177]
[null,"2016-07-05",335,277]
[null,"2016-07-06",340,241]
[null,"2016-07-07",272,204]
[null,"2016-07-08",231,202]
[null,"2016-07-09",148,140]
[null,"2016-07-10",149,127]
[null,"2016-07-11",701,549]
[null,"2016-07-12",858,763]
[null,"2016-07-13",553,408]
[null,"2016-07-14",188,170]
[null,"2016-07-15",232,196]
[null,"2016-07-16",234,110]
[null,"2016-07-17",138,125]
[null,"2016-07-18",344,293]
[null,"2016-07-19",219,194]
[null,"2016-07-20",166,157]
[null,"2016-07-21",240,215]
[null,"2016-07-22",337,315]
[null,"2016-07-23",412,308]
[null,"2016-07-24",122,107]
[null,"2016-07-25",465,394]
[null,"2016-07-26",540,384]
[null,"2016-07-27",232,197]
[null,"2016-07-28",226,183]
[null,"2016-07-29",236,203]
[null,"2016-07-30",124,106]
[null,{"$f":"B584+1","v":"2016-07-31"},131,107]
[null,"2016-08-01",261,237]
[null,"2016-08-02",252,238]
[null,"2016-08-03",216,184]
[null,"2016-08-04",176,161]
[null,"2016-08-05",185,170]
[null,"2016-08-06",119,114]
[null,"2016-08-07",159,150]
[null,"2016-08-08",224,197]
[null,"2016-08-09",271,231]
[null,"2016-08-10",299,225]
[null,"2016-08-11",232,195]
[null,"2016-08-12",165,150]
[null,"2016-08-13",126,101]
[null,"2016-08-14",140,96]
[null,"2016-08-15",157,149]
[null,"2016-08-16",183,174]
[null,"2016-08-17",305,269]
[null,"2016-08-18",357,218]
[null,"2016-08-19",213,196]
[null,"2016-08-20",113,95]
[null,"2016-08-21",177,148]
[null,"2016-08-22",271,213]
[null,"2016-08-23",222,187]
[null,"2016-08-24",193,144]
[null,"2016-08-25",397,297]
[null,"2016-08-26",255,190]
[null,"2016-08-27",101,91]
[null,"2016-08-28",52,50]
[null,"2016-08-29",153,127]
[null,"2016-08-30",161,146]
[null,"2016-08-31",245,197]
[null,"2016-09-01",197,150]
[null,"2016-09-02",127,123]
[null,"2016-09-03",126,119]
[null,"2016-09-04",92,88]
[null,"2016-09-05",137,130]
[null,"2016-09-06",199,181]
[null,"2016-09-07",162,136]
[null,"2016-09-08",241,205]
[null,"2016-09-09",200,180]
[null,"2016-09-10",179,164]
[null,"2016-09-11",72,68]
[null,"2016-09-12",388,243]
[null,"2016-09-13",217,188]
[null,"2016-09-14",242,210]
[null,"2016-09-15",332,213]
[null,"2016-09-16",157,147]
[null,"2016-09-17",144,128]
[null,"2016-09-18",149,135]
[null,"2016-09-19",197,186]
[null,"2016-09-20",238,211]
[null,"2016-09-21",280,197]
[null,"2016-09-22",238,202]
[null,"2016-09-23",236,170]
[null,"2016-09-24",97,83]
[null,"2016-09-25",75,74]
[null,"2016-09-26",288,251]
[null,"2016-09-27",282,229]
[null,"2016-09-28",249,206]
[null,"2016-09-29",305,247]
[null,"2016-09-30",221,184]
[null,"2016-10-01",141,120]
[null,"2016-10-02",333,314]
[null,{"$f":"B648+1","v":"2016-10-03"},372,291]
[null,"2016-10-04",1331,322]
[null,"2016-10-05",767,576]
[null,"2016-10-06",359,304]
[null,"2016-10-07",316,259]
[null,"2016-10-08",108,94]
[null,"2016-10-09","???","???"]
[null,"2016-10-10",1634,361]
[null,"2016-10-11",1039,481]
[null,"2016-10-12",697,506]
[null,"2016-10-13",483,349]
[null,"2016-10-14",300,380]
[null,"2016-10-15",326,222]
[null,"2016-10-16",300,276]
[null,"2016-10-17",541,299]
[null,"2016-10-18",363,260]
[null,"2016-10-19",224,191]
[null,"2016-10-20",339,199]
[null,"2016-10-21",512,295]
[null,"2016-10-22",378,297]
[null,"2016-10-23",275,258]
[null,"2016-10-24",247,199]
[null,"2016-10-25",258,228]
[null,"2016-10-26",252,217]
[null,"2016-10-27",232,195]
[null,"2016-10-28",209,178]
[null,"2016-10-29",133,115]
[null,"2016-10-30",285,265]
[null,"2016-10-31",205,190]
[null,"2016-11-01",69,65]
[null,"2016-11-02",354,279]
[null,"2016-11-03",246,191]
[null,"2016-11-04",308,201]
[null,"2016-11-05",223,205]
[null,"2016-11-06",86,82]
[null,"2016-11-07",294,252]
[null,"2016-11-08",254,191]
[null,"2016-11-09",201,175]
[null,"2016-11-10",298,249]
[null,"2016-11-11",240,205]
[null,"2016-11-12",253,245]
[null,"2016-11-13",119,116]
[null,"2016-11-14",274,227]
[null,"2016-11-15",213,190]
[null,"2016-11-16",237,203]
[null,"2016-11-17",214,200]
[null,"2016-11-18",241,212]
[null,"2016-11-19",163,156]
[null,"2016-11-20",144,135]
[null,"2016-11-21",595,526]
[null,"2016-11-22",367,321]
[null,"2016-11-23",237,196]
[null,"2016-11-24",250,193]
[null,"2016-11-25",210,199]
[null,"2016-11-26",164,134]
[null,"2016-11-27",77,75]
[null,"2016-11-28",203,164]
[null,"2016-11-29",270,202]
[null,"2016-11-30",252,224]
[null,"2016-12-01",322,248]
[null,"2016-12-02",215,197]
[null,"2016-12-03",133,124]
[null,"2016-12-04",117,106]
[null,"2016-12-05",268,236]
[null,{"$f":"B712+1","v":"2016-12-06"},225,202]
[null,"2016-12-07",236,205]
[null,"2016-12-08",329,268]
[null,"2016-12-09",257,220]
[null,"2016-12-10",108,97]
[null,"2016-12-11",86,78]
[null,"2016-12-12",267,234]
[null,"2016-12-13",273,225]
[null,"2016-12-14",293,246]
[null,"2016-12-15",269,216]
[null,"2016-12-16",157,145]
[null,"2016-12-17",160,140]
[null,"2016-12-18",93,85]
[null,"2016-12-19",222,198]
[null,"2016-12-20",450,351]
[null,"2016-12-21",223,196]
[null,"2016-12-22",199,181]
[null,"2016-12-23",203,190]
[null,"2016-12-24",484,356]
[null,"2016-12-25",241,215]
[null,"2016-12-26",205,195]
[null,"2016-12-27",131,117]
[null,"2016-12-28",376,315]
[null,"2016-12-29",956,480]
[null,"2016-12-30",505,399]
[null,"2016-12-31",153,138]
[null,"2017-01-01",98,91]
[null,"2017-01-02",92,86]
[null,"2017-01-03",164,160]
[null,"2017-01-04",235,199]
[null,"2017-01-05",251,212]
[null,"2017-01-06",446,315]
[null,"2017-01-07",379,358]
[null,"2017-01-08",152,147]
[null,"2017-01-09",271,233]
[null,"2017-01-10",232,193]
[null,"2017-01-11",178,160]
[null,"2017-01-12",203,186]
[null,"2017-01-13",395,307]
[null,"2017-01-14",115,104]
[null,"2017-01-15",160,151]
[null,"2017-01-16",211,178]
[null,"2017-01-17",385,268]
[null,"2017-01-18",294,241]
[null,"2017-01-19",197,152]
[null,"2017-01-20",509,420]
[null,"2017-01-21",144,122]
[null,"2017-01-22",140,131]
[null,"2017-01-23",318,272]
[null,"2017-01-24",296,249]
[null,"2017-01-25",333,217]
[null,"2017-01-26",109,103]
[null,"2017-01-27",200,155]
[null,"2017-01-28",129,113]
[null,"2017-01-29",97,91]
[null,"2017-01-30",327,285]
[null,"2017-01-31",260,179]
[null,"2017-02-01",263,185]
[null,"2017-02-02",275,209]
[null,"2017-02-03",204,152]
[null,"2017-02-04",182,158]
[null,"2017-02-05",186,158]
[null,"2017-02-06",294,253]
[null,"2017-02-07",253,214]
[null,{"$f":"B776+1","v":"2017-02-08"},316,234]
[null,"2017-02-09",502,341]
[null,"2017-02-10",330,284]
[null,"2017-02-11",252,172]
[null,"2017-02-12",125,122]
[null,"2017-02-13",268,189]
[null,"2017-02-14",199,172]
[null,"2017-02-15",261,228]
[null,"2017-02-16",256,221]
[null,"2017-02-17",196,175]
[null,"2017-02-18",140,119]
[null,"2017-02-19",176,142]
[null,"2017-02-20",215,175]
[null,"2017-02-21",222,192]
[null,"2017-02-22",336,275]
[null,"2017-02-23",290,237]
[null,"2017-02-24",222,186]
[null,"2017-02-25",94,88]
[null,"2017-02-26",101,92]
[null,"2017-02-27",217,184]
[null,"2017-02-28",416,322]
[null,"2017-03-01",401,302]
[null,"2017-03-02",296,232]
[null,"2017-03-03",361,276]
[null,"2017-03-04",105,99]
[null,"2017-03-05",107,104]
[null,"2017-03-06",323,281]
[null,"2017-03-07",221,182]
[null,"2017-03-08",199,158]
[null,"2017-03-09",275,209]
[null,"2017-03-10",215,178]
[null,"2017-03-11",195,163]
[null,"2017-03-12",227,220]
[null,"2017-03-13",168,162]
[null,"2017-03-14",296,276]
[null,"2017-03-15",315,285]
[null,"2017-03-16",241,224]
[null,"2017-03-17",207,172]
[null,"2017-03-18",150,130]
[null,"2017-03-19",123,116]
[null,"2017-03-20",321,268]
[null,"2017-03-21",428,304]
[null,"2017-03-22",295,252]
[null,"2017-03-23",240,222]
[null,"2017-03-24",233,186]
[null,"2017-03-25",157,140]
[null,"2017-03-26",220,192]
[null,"2017-03-27",1425,858]
[null,"2017-03-28",381,281]
[null,"2017-03-29",301,248]
[null,"2017-03-30",313,284]
[null,"2017-03-31",229,203]
[null,"2017-04-01",126,115]
[null,"2017-04-02",112,104]
[null,"2017-04-03",221,192]
[null,"2017-04-04",239,219]
[null,"2017-04-05",406,287]
[null,"2017-04-06",259,245]
[null,"2017-04-07",268,253]
[null,"2017-04-08",313,274]
[null,"2017-04-09",325,252]
[null,"2017-04-10",519,400]
[null,"2017-04-11",325,264]
[null,"2017-04-12",409,290]
[null,{"$f":"B840+1","v":"2017-04-13"},285,197]
[null,"2017-04-14",125,119]
[null,"2017-04-15",83,73]
[null,"2017-04-16",224,130]
[null,"2017-04-17",113,109]
[null,"2017-04-18",258,208]
[null,"2017-04-19",284,230]
[null,"2017-04-20",213,184]
[null,"2017-04-21",245,188]
[null,"2017-04-22",126,114]
[null,"2017-04-23",86,82]
[null,"2017-04-24",232,214]
[null,"2017-04-25",160,159]
[null,"2017-04-26",403,233]
[null,"2017-04-27",312,189]
[null,"2017-04-28",237,191]
[null,"2017-04-29",134,105]
[null,"2017-04-30",127,98]
[null,"2017-05-01",317,239]
[null,"2017-05-02",316,250]
[null,"2017-05-03",285,224]
[null,"2017-05-04",240,189]
[null,"2017-05-05",222,203]
[null,"2017-05-06",144,124]
[null,"2017-05-07",134,126]
[null,"2017-05-08",221,192]
[null,"2017-05-09",187,167]
[null,"2017-05-10",228,200]
[null,"2017-05-11",248,206]
[null,"2017-05-12",173,165]
[null,"2017-05-13",104,92]
[null,"2017-05-14",55,51]
[null,"2017-05-15",184,175]
[null,"2017-05-16",240,175]
[null,"2017-05-17",268,209]
[null,"2017-05-18",211,185]
[null,"2017-05-19",198,160]
[null,"2017-05-20",100,88]
[null,"2017-05-21",70,66]
[null,"2017-05-22",211,206]
[null,"2017-05-23",219,207]
[null,"2017-05-24",367,304]
[null,"2017-05-25",262,224]
[null,"2017-05-26",174,165]
[null,"2017-05-27",162,108]
[null,"2017-05-28",455,351]
[null,"2017-05-29",240,214]
[null,"2017-05-30",247,232]
[null,"2017-05-31",356,302]
[null,"2017-06-01",266,254]
[null,"2017-06-02",186,164]
[null,"2017-06-03",102,95]
[null,"2017-06-04",73,66]
[null,"2017-06-05",224,196]
[null,"2017-06-06",221,210]
[null,"2017-06-07",185,176]
[null,"2017-06-08",223,212]
[null,"2017-06-09",241,196]
[null,"2017-06-10",171,149]
[null,"2017-06-11",101,99]
[null,"2017-06-12",90,87]
[null,"2017-06-13",218,200]
[null,"2017-06-14",253,222]
[null,"2017-06-15",238,214]
[null,{"$f":"B904+1","v":"2017-06-16"},229,198]
[null,"2017-06-17",131,117]
[null,"2017-06-18",64,60]
[null,"2017-06-19",229,185]
[null,"2017-06-20",280,247]
[null,"2017-06-21",192,169]
[null,"2017-06-22",219,212]
[null,"2017-06-23",272,217]
[null,"2017-06-24",158,125]
[null,"2017-06-25",78,72]
[null,"2017-06-26",196,181]
[null,"2017-06-27",215,172]
[null,"2017-06-28",239,200]
[null,"2017-06-29",204,169]
[null,"2017-06-30",191,178]
[null,"2017-07-01",166,133]
[null,"2017-07-02",199,172]
[null,"2017-07-03",366,318]
[null,"2017-07-04",245,223]
[null,"2017-07-05",235,212]
[null,"2017-07-06",309,267]
[null,"2017-07-07",197,189]
[null,"2017-07-08",104,99]
[null,"2017-07-09",106,86]
[null,"2017-07-10",276,214]
[null,"2017-07-11",262,231]
[null,"2017-07-12",308,276]
[null,"2017-07-13",197,186]
[null,"2017-07-14",232,206]
[null,"2017-07-15",140,121]
[null,"2017-07-16",97,80]
[null,"2017-07-17",214,193]
[null,"2017-07-18",265,228]
[null,"2017-07-19",371,300]
[null,"2017-07-20",288,223]
[null,"2017-07-21",244,221]
[null,"2017-07-22",213,170]
[null,"2017-07-23",272,251]
[null,"2017-07-24",190,169]
[null,"2017-07-25",243,194]
[null,"2017-07-26",266,214]
[null,"2017-07-27",222,193]
[null,"2017-07-28",284,214]
[null,"2017-07-29",348,311]
[null,"2017-07-30",118,112]
[null,"2017-07-31",267,230]
[null,"2017-08-01",255,239]
[null,"2017-08-02",170,156]
[null,"2017-08-03",245,212]
[null,"2017-08-04",234,194]
[null,"2017-08-05",144,138]
[null,"2017-08-06",163,159]
[null,"2017-08-07",279,253]
[null,"2017-08-08",205,190]
[null,"2017-08-09",220,205]
[null,"2017-08-10",351,323]
[null,"2017-08-11",183,172]
[null,"2017-08-12",183,170]
[null,"2017-08-13",83,80]
[null,"2017-08-14",247,191]
[null,"2017-08-15",235,208]
[null,"2017-08-16",247,216]
[null,"2017-08-17",280,257]
[null,"2017-08-18",231,216]
[null,{"$f":"B968+1","v":"2017-08-19"},140,119]
[null,"2017-08-20",108,106]
[null,"2017-08-21",206,187]
[null,"2017-08-22",257,200]
[null,"2017-08-23",219,194]
[null,"2017-08-24",286,250]
[null,"2017-08-25",188,166]
[null,"2017-08-26",101,94]
[null,"2017-08-27",103,99]
[null,"2017-08-28",242,219]
[null,"2017-08-29",220,207]
[null,"2017-08-30",260,230]
[null,"2017-08-31",302,238]
[null,"2017-09-01",165,133]
[null,"2017-09-02",119,109]
[null,"2017-09-03",131,126]
[null,"2017-09-04",268,232]
[null,"2017-09-05",329,292]
[null,"2017-09-06",225,205]
[null,"2017-09-07",206,187]
[null,"2017-09-08",216,206]
[null,"2017-09-09",111,106]
[null,"2017-09-10",64,59]
[null,"2017-09-11",196,169]
[null,"2017-09-12",164,137]
[null,"2017-09-13",206,183]
[null,"2017-09-14",171,148]
[null,"2017-09-15",219,174]
[null,"2017-09-16",316,261]
[null,"2017-09-17",216,188]
[null,"2017-09-18",406,326]
[null,"2017-09-19",326,236]
[null,"2017-09-20",211,179]
[null,"2017-09-21",233,195]
[null,"2017-09-22",206,159]
[null,"2017-09-23",257,193]
[null,"2017-09-24",262,220]
[null,"2017-09-25",274,213]
[null,"2017-09-26",240,207]
[null,"2017-09-27",249,207]
[null,"2017-09-28",229,184]
[null,"2017-09-29",152,133]
[null,"2017-09-30",116,110]
[null,"2017-10-01",75,72]
[null,"2017-10-02",197,169]
[null,"2017-10-03",228,200]
[null,"2017-10-04",221,187]
[null,"2017-10-05",246,188]
[null,"2017-10-06",293,248]
[null,"2017-10-07",136,113]
[null,"2017-10-08",79,75]
[null,"2017-10-09",247,216]
[null,"2017-10-10",209,192]
[null,"2017-10-11",241,228]
[null,"2017-10-12",342,259]
[null,"2017-10-13",146,132]
[null,"2017-10-14",102,82]
[null,"2017-10-15",82,74]
[null,"2017-10-16",181,158]
[null,"2017-10-17",239,193]
[null,"2017-10-18",304,266]
[null,"2017-10-19",355,294]
[null,"2017-10-20",250,219]
[null,"2017-10-21",124,114]
[null,{"$f":"B1032+1","v":"2017-10-22"},96,91]
[null,"2017-10-23",202,190]
[null,"2017-10-24",422,295]
[null,"2017-10-25",258,225]
[null,"2017-10-26",225,206]
[null,"2017-10-27",241,218]
[null,"2017-10-28",239,205]
[null,"2017-10-29",157,134]
[null,"2017-10-30",296,263]
[null,"2017-10-31",202,180]
[null,"2017-11-01",232,206]
[null,"2017-11-02",226,181]
[null,"2017-11-03",201,177]
[null,"2017-11-04",98,91]
[null,"2017-11-05",73,71]
[null,"2017-11-06",173,162]
[null,"2017-11-07",80,77]
[null,"2017-11-08",214,167]
[null,"2017-11-09",249,187]
[null,"2017-11-10",226,192]
[null,"2017-11-11",121,105]
[null,"2017-11-12",148,134]
[null,"2017-11-13",309,273]
[null,"2017-11-14",303,235]
[null,"2017-11-15",364,308]
[null,"2017-11-16",355,273]
[null,"2017-11-17",455,350]
[null,"2017-11-18",199,179]
[null,"2017-11-19",98,92]
[null,"2017-11-20",284,223]
[null,"2017-11-21",349,203]
[null,"2017-11-22",270,234]
[null,"2017-11-23",654,413]
[null,"2017-11-24",310,266]
[null,"2017-11-25",377,243]
[null,"2017-11-26",254,224]
[null,"2017-11-27",366,316]
[null,"2017-11-28",269,213]
[null,"2017-11-29",417,295]
[null,"2017-11-30",324,275]
[null,"2017-12-01",422,397]
[null,"2017-12-02",344,329]
[null,"2017-12-03",346,310]
[null,"2017-12-04",230,212]
[null,"2017-12-05",283,250]
[null,"2017-12-06",221,200]
[null,"2017-12-07",223,202]
[null,"2017-12-08",232,221]
[null,"2017-12-09",334,256]
[null,"2017-12-10",131,119]
[null,"2017-12-11",286,261]
[null,"2017-12-12",230,209]
[null,"2017-12-13",448,385]
[null,"2017-12-14",326,295]
[null,"2017-12-15",276,262]
[null,"2017-12-16",174,145]
[null,"2017-12-17",154,145]
[null,"2017-12-18",269,257]
[null,"2017-12-19",0,0]
[null,"2017-12-20",504,1013]
[null,"2017-12-21",17,427]
[null,"2017-12-22",241,212]
[null,"2017-12-23",185,155]
[null,"2017-12-24",79,78]
[null,{"$f":"B1096+1","v":"2017-12-25"},75,72]
[null,"2017-12-26",105,98]
[null,"2017-12-27",222,215]
[null,"2017-12-28",311,293]
[null,"2017-12-29",444,349]
[null,"2017-12-30",149,139]
[null,"2017-12-31",90,85]
[null,"2018-01-01",69,69]
[null,"2018-01-02",235,211]
[null,"2018-01-03",174,168]
[null,"2018-01-04",168,151]
[null,"2018-01-05",172,166]
[null,"2018-01-06",697,452]
[null,"2018-01-07",153,138]
[null,"2018-01-08",281,256]
[null,"2018-01-09",218,199]
[null,"2018-01-10",269,239]
[null,"2018-01-11",293,231]
[null,"2018-01-12",348,300]
[null,"2018-01-13",185,174]
[null,"2018-01-14",145,118]
[null,"2018-01-15",200,178]
[null,"2018-01-16",216,183]
[null,"2018-01-17",179,171]
[null,"2018-01-18",561,398]
[null,"2018-01-19",573,461]
[null,"2018-01-20",234,214]
[null,"2018-01-21",151,134]
[null,"2018-01-22",297,279]
[null,"2018-01-23",302,284]
[null,"2018-01-24",287,245]
[null,"2018-01-25",320,232]
[null,"2018-01-26",282,271]
[null,"2018-01-27",375,306]
[null,"2018-01-28",1695,452]
[null,"2018-01-29",754,534]
[null,"2018-01-30",362,322]
[null,"2018-01-31",365,323]
[null,"2018-02-01",289,230]
[null,"2018-02-02",193,177]
[null,"2018-02-03",124,120]
[null,"2018-02-04",159,122]
[null,"2018-02-05",242,220]
[null,"2018-02-06",295,219]
[null,"2018-02-07",487,340]
[null,"2018-02-08",322,294]
[null,"2018-02-09",239,210]
[null,"2018-02-10",194,172]
[null,"2018-02-11",194,130]
[null,"2018-02-12",403,237]
[null,"2018-02-13",243,216]
[null,"2018-02-14",0,0]
[null,"2018-02-15",493,350]
[null,"2018-02-16",261,222]
[null,"2018-02-17",160,141]
[null,"2018-02-18",76,71]
[null,"2018-02-19",499,355]
[null,"2018-02-20",555,402]
[null,"2018-02-21",391,282]
[null,"2018-02-22",295,206]
[null,"2018-02-23",312,241]
[null,"2018-02-24",330,311]
[null,"2018-02-25",163,137]
[null,"2018-02-26",255,212]
[null,{"$f":"B1160+1","v":"2018-02-27"},289,208]
[null,"2018-02-28",696,388]
[null,"2018-03-01",362,261]
[null,"2018-03-02",244,224]
[null,"2018-03-03",180,156]
[null,"2018-03-04",102,102]
[null,"2018-03-05",232,190]
[null,"2018-03-06",468,246]
[null,"2018-03-07",297,261]
[null,"2018-03-08",352,298]
[null,"2018-03-09",304,252]
[null,"2018-03-10",208,179]
[null,"2018-03-11",88,86]
[null,"2018-03-12",88,85]
[null,"2018-03-13",232,197]
[null,"2018-03-14",210,179]
[null,"2018-03-15",189,173]
[null,"2018-03-16",226,193]
[null,"2018-03-17",181,156]
[null,"2018-03-18",989,864]
[null,"2018-03-19",317,270]
[null,"2018-03-20",334,278]
[null,"2018-03-21",881,758]
[null,"2018-03-22",279,224]
[null,"2018-03-23",250,203]
[null,"2018-03-24",592,358]
[null,"2018-03-25",414,338]
[null,"2018-03-26",356,299]
[null,"2018-03-27",238,206]
[null,"2018-03-28",258,221]
[null,"2018-03-29",226,197]
[null,"2018-03-30",168,163]
[null,"2018-03-31",106,98]
[null,"2018-04-01",89,78]
[null,"2018-04-02",84,81]
[null,"2018-04-03",221,189]
[null,"2018-04-04",295,261]
[null,"2018-04-05",286,229]
[null,"2018-04-06",305,249]
[null,"2018-04-07",214,131]
[null,"2018-04-08",167,119]
[null,"2018-04-09",246,195]
[null,"2018-04-10",286,245]
[null,"2018-04-11",323,298]
[null,"2018-04-12",320,256]
[null,"2018-04-13",397,283]
[null,"2018-04-14",1237,970]
[null,"2018-04-15",323,260]
[null,"2018-04-16",319,250]
[null,"2018-04-17",289,238]
[null,"2018-04-18",180,140]
[null,"2018-04-19",206,158]
[null,"2018-04-20",203,184]
[null,"2018-04-21",155,117]
[null,"2018-04-22",49,47]
[null,"2018-04-23",205,178]
[null,"2018-04-24",217,187]
[null,"2018-04-25",95,83]
[null,"2018-04-26",175,132]
[null,"2018-04-27",157,139]
[null,"2018-04-28",90,82]
[null,"2018-04-29",104,88]
[null,"2018-04-30",245,216]
[null,"2018-05-01",266,209]
[null,{"$f":"B1224+1","v":"2018-05-02"},225,180]
[null,"2018-05-03",206,182]
[null,"2018-05-04",216,177]
[null,"2018-05-05",116,103]
[null,"2018-05-06",87,80]
[null,"2018-05-07",231,163]
[null,"2018-05-08",242,212]
[null,"2018-05-09",169,153]
[null,"2018-05-10",230,190]
[null,"2018-05-11",442,426]
[null,"2018-05-12",283,187]
[null,"2018-05-13",101,89]
[null,"2018-05-14",263,206]
[null,"2018-05-15",253,226]
[null,"2018-05-16",202,169]
[null,"2018-05-17",295,213]
[null,"2018-05-18",221,190]
[null,"2018-05-19",91,77]
[null,"2018-05-20",93,83]
[null,"2018-05-21",326,235]
[null,"2018-05-22",230,198]
[null,"2018-05-23",249,212]
[null,"2018-05-24",246,203]
[null,"2018-05-25",251,209]
[null,"2018-05-26",146,129]
[null,"2018-05-27",73,69]
[null,"2018-05-28",238,222]
[null,"2018-05-29",277,241]
[null,"2018-05-30",250,216]
[null,"2018-05-31",211,166]
[null,"2018-06-01",192,158]
[null,"2018-06-02",129,74]
[null,"2018-06-03",121,103]
[null,"2018-06-04",235,204]
[null,"2018-06-05",196,181]
[null,"2018-06-06",186,153]
[null,"2018-06-07",193,179]
[null,"2018-06-08",245,215]
[null,"2018-06-09",195,155]
[null,"2018-06-10",85,77]
[null,"2018-06-11",100,94]
[null,"2018-06-12",293,263]
[null,"2018-06-13",216,194]
[null,"2018-06-14",328,293]
[null,"2018-06-15",323,295]
[null,"2018-06-16",215,174]
[null,"2018-06-17",183,167]
[null,"2018-06-18",297,225]
[null,"2018-06-19",337,233]
[null,"2018-06-20",201,161]
[null,"2018-06-21",256,223]
[null,"2018-06-22",268,237]
[null,"2018-06-23",161,126]
[null,"2018-06-24",129,114]
[null,"2018-06-25",236,200]
[null,"2018-06-26",257,184]
[null,"2018-06-27",227,176]
[null,"2018-06-28",251,218]
[null,"2018-06-29",211,176]
[null,"2018-06-30",236,200]
[null,"2018-07-01",94,79]
[null,"2018-07-02",255,202]
[null,"2018-07-03",303,252]
[null,"2018-07-04",370,277]
[null,{"$f":"B1288+1","v":"2018-07-05"},463,309]
[null,"2018-07-06",204,168]
[null,"2018-07-07",218,204]
[null,"2018-07-08",174,162]
[null,"2018-07-09",237,188]
[null,"2018-07-10",268,228]
[null,"2018-07-11",203,191]
[null,"2018-07-12",361,296]
[null,"2018-07-13",177,159]
[null,"2018-07-14",157,150]
[null,"2018-07-15",111,99]
[null,"2018-07-16",207,170]
[null,"2018-07-17",1240,520]
[null,"2018-07-18",385,352]
[null,"2018-07-19",396,309]
[null,"2018-07-20",231,221]
[null,"2018-07-21",153,126]
[null,"2018-07-22",136,111]
[null,"2018-07-23",515,360]
[null,"2018-07-24",653,478]
[null,"2018-07-25",313,247]
[null,"2018-07-26",227,198]
[null,"2018-07-27",342,237]
[null,"2018-07-28",158,139]
[null,"2018-07-29",212,203]
[null,"2018-07-30",235,192]
[null,"2018-07-31",271,264]
[null,"2018-08-01",185,161]
[null,"2018-08-02",203,174]
[null,"2018-08-03",210,189]
[null,"2018-08-04",107,101]
[null,"2018-08-05",67,66]
[null,"2018-08-06",214,201]
[null,"2018-08-07",180,164]
[null,"2018-08-08",204,176]
[null,"2018-08-09",204,159]
[null,"2018-08-10",847,648]
[null,"2018-08-11",350,257]
[null,"2018-08-12",161,124]
[null,"2018-08-13",221,183]
[null,"2018-08-14",254,225]
[null,"2018-08-15",335,312]
[null,"2018-08-16",172,161]
[null,"2018-08-17",179,171]
[null,"2018-08-18",191,167]
[null,"2018-08-19",314,242]
[null,"2018-08-20",257,201]
[null,"2018-08-21",206,178]
[null,"2018-08-22",356,254]
[null,"2018-08-23",288,232]
[null,"2018-08-24",254,210]
[null,"2018-08-25",117,96]
[null,"2018-08-26",78,76]
[null,"2018-08-27",199,174]
[null,"2018-08-28",189,152]
[null,"2018-08-29",450,249]
[null,"2018-08-30",319,272]
[null,"2018-08-31",356,292]
[null,"2018-09-01",133,127]
[null,"2018-09-02",37,37]
[null,"2018-09-03",439,184]
[null,"2018-09-04",220,172]
[null,"2018-09-05",199,177]
[null,"2018-09-06",242,211]
[null,{"$f":"B1352+1","v":"2018-09-07"},188,176]
[null,"2018-09-08",131,109]
[null,"2018-09-09",89,85]
[null,"2018-09-10",193,179]
[null,"2018-09-11",201,157]
[null,"2018-09-12",159,142]
[null,"2018-09-13",192,165]
[null,"2018-09-14",151,134]
[null,"2018-09-15",182,162]
[null,"2018-09-16",96,87]
[null,"2018-09-17",175,151]
[null,"2018-09-18",227,191]
[null,"2018-09-19",224,182]
[null,"2018-09-20",183,160]
[null,"2018-09-21",158,138]
[null,"2018-09-22",111,99]
[null,"2018-09-23",101,94]
[null,"2018-09-24",232,199]
[null,"2018-09-25",263,183]
[null,"2018-09-26",179,162]
[null,"2018-09-27",210,185]
[null,"2018-09-28",147,126]
[null,"2018-09-29",131,105]
[null,"2018-09-30",113,49]
[null,"2018-10-01",209,188]
[null,"2018-10-02",252,193]
[null,"2018-10-03",255,205]
[null,"2018-10-04",218,177]
[null,"2018-10-05",184,165]
[null,"2018-10-06",118,106]
[null,"2018-10-07",71,63]
[null,"2018-10-08",191,182]
[null,"2018-10-09",191,169]
[null,"2018-10-10",252,228]
[null,"2018-10-11",200,175]
[null,"2018-10-12",190,169]
[null,"2018-10-13",114,100]
[null,"2018-10-14",119,110]
[null,"2018-10-15",237,214]
[null,"2018-10-16",366,256]
[null,"2018-10-17",255,223]
[null,"2018-10-18",235,226]
[null,"2018-10-19",235,174]
[null,"2018-10-20",103,92]
[null,"2018-10-21",254,191]
[null,"2018-10-22",271,227]
[null,"2018-10-23",171,163]
[null,"2018-10-24",183,164]
[null,"2018-10-25",189,170]
[null,"2018-10-26",192,177]
[null,"2018-10-27",98,93]
[null,"2018-10-28",87,79]
[null,"2018-10-29",206,190]
[null,"2018-10-30",188,167]
[null,"2018-10-31",206,180]
[null,"2018-11-01",476,222]
[null,"2018-11-02",636,491]
[null,"2018-11-03",243,172]
[null,"2018-11-04",89,86]
[null,"2018-11-05",175,146]
[null,"2018-11-06",295,237]
[null,"2018-11-07",261,233]
[null,"2018-11-08",253,225]
[null,"2018-11-09",194,153]
[null,{"$f":"B1416+1","v":"2018-11-10"},136,107]
[null,"2018-11-11",73,69]
[null,"2018-11-12",211,170]
[null,"2018-11-13",229,218]
[null,"2018-11-14",216,205]
[null,"2018-11-15",230,212]
[null,"2018-11-16",199,160]
[null,"2018-11-17",152,134]
[null,"2018-11-18",101,93]
[null,"2018-11-19",376,286]
[null,"2018-11-20",787,595]
[null,"2018-11-21",400,358]
[null,"2018-11-22",285,260]
[null,"2018-11-23",330,264]
[null,"2018-11-24",235,178]
[null,"2018-11-25",209,164]
[null,"2018-11-26",226,209]
[null,"2018-11-27",198,187]
[null,"2018-11-28",260,242]
[null,"2018-11-29",220,194]
[null,"2018-11-30",174,163]
[null,"2018-12-01",171,152]
[null,"2018-12-02",407,343]
[null,"2018-12-03",281,262]
[null,"2018-12-04",218,198]
[null,"2018-12-05",176,160]
[null,"2018-12-06",358,275]
[null,"2018-12-07",353,300]
[null,"2018-12-08",168,149]
[null,"2018-12-09",298,211]
[null,"2018-12-10",578,505]
[null,"2018-12-11",244,223]
[null,"2018-12-12",273,218]
[null,"2018-12-13",426,363]
[null,"2018-12-14",285,252]
[null,"2018-12-15",286,224]
[null,"2018-12-16",314,228]
[null,"2018-12-17",236,220]
[null,"2018-12-18",301,251]
[null,"2018-12-19",214,203]
[null,"2018-12-20",243,222]
[null,"2018-12-21",198,180]
[null,"2018-12-22",314,163]
[null,"2018-12-23",142,134]
[null,"2018-12-24",141,139]
[null,"2018-12-25",125,97]
[null,"2018-12-26",90,80]
[null,"2018-12-27",331,302]
[null,"2018-12-28",238,210]
[null,"2018-12-29",218,146]
[null,"2018-12-30",123,114]
[null,"2018-12-31",226,213]
[null,"2019-01-01",80,77]
[null,"2019-01-02",154,147]
[null,"2019-01-03",244,203]
[null,"2019-01-04",519,446]
[null,"2019-01-05",177,143]
[null,"2019-01-06",97,92]
[null,"2019-01-07",150,141]
[null,"2019-01-08",199,185]
[null,"2019-01-09",173,164]
[null,"2019-01-10",189,174]
[null,"2019-01-11",174,166]
[null,"2019-01-12",162,131]
[null,{"$f":"B1480+1","v":"2019-01-13"},212,181]
[null,"2019-01-14",406,302]
[null,"2019-01-15",463,419]
[null,"2019-01-16",330,299]
[null,"2019-01-17",303,264]
[null,"2019-01-18",297,248]
[null,"2019-01-19",123,98]
[null,"2019-01-20",78,72]
[null,"2019-01-21",189,176]
[null,"2019-01-22",287,253]
[null,"2019-01-23",347,285]
[null,"2019-01-24",945,645]
[null,"2019-01-25",3011,1883]
[null,"2019-01-26",316,270]
[null,"2019-01-27",203,161]
[null,"2019-01-28",129,112]
[null,"2019-01-29",385,317]
[null,"2019-01-30",0,0]
[null,"2019-01-31",1472,821]
[null,"2019-02-01",336,299]
[null,"2019-02-02",196,154]
[null,"2019-02-03",935,460]
[null,"2019-02-04",356,290]
[null,"2019-02-05",346,303]
[null,"2019-02-06",403,356]
[null,"2019-02-07",562,378]
[null,"2019-02-08",347,284]
[null,"2019-02-09",336,222]
[null,"2019-02-10",92,82]
[null,"2019-02-11",402,290]
[null,"2019-02-12",500,424]
[null,"2019-02-13",183,173]
[null,"2019-02-14",212,194]
[null,"2019-02-15",180,172]
[null,"2019-02-16",85,78]
[null,"2019-02-17",128,112]
[null,"2019-02-18",363,272]
[null,"2019-02-19",199,180]
[null,"2019-02-20",183,161]
[null,"2019-02-21",196,171]
[null,"2019-02-22",126,121]
[null,"2019-02-23",95,79]
[null,"2019-02-24",167,108]
[null,"2019-02-25",314,226]
[null,"2019-02-26",233,211]
[null,"2019-02-27",286,255]
[null,"2019-02-28",336,252]
[null,"2019-03-01",409,322]
[null,"2019-03-02",264,221]
[null,"2019-03-03",301,168]
[null,"2019-03-04",483,379]
[null,"2019-03-05",789,386]
[null,"2019-03-06",513,432]
[null,"2019-03-07",261,229]
[null,"2019-03-08",301,265]
[null,"2019-03-09",136,105]
[null,"2019-03-10",93,89]
[null,"2019-03-11",110,89]
[null,"2019-03-12",271,230]
[null,"2019-03-13",180,147]
[null,"2019-03-14",308,206]
[null,"2019-03-15",299,260]
[null,"2019-03-16",129,110]
[null,"2019-03-17",140,128]
[null,{"$f":"B1544+1","v":"2019-03-18"},275,244]
[null,"2019-03-19",382,211]
[null,"2019-03-20",264,217]
[null,"2019-03-21",209,171]
[null,"2019-03-22",603,401]
[null,"2019-03-23",167,141]
[null,"2019-03-24",147,136]
[null,"2019-03-25",509,423]
[null,"2019-03-26",334,298]
[null,"2019-03-27",375,274]
[null,"2019-03-28",229,182]
[null,"2019-03-29",518,394]
[null,"2019-03-30",334,234]
[null,"2019-03-31",215,191]
[null,"2019-04-01",186,146]
[null,"2019-04-02",340,257]
[null,"2019-04-03",264,233]
[null,"2019-04-04",157,141]
[null,"2019-04-05",212,190]
[null,"2019-04-06",161,146]
[null,"2019-04-07",133,105]
[null,"2019-04-08",246,183]
[null,"2019-04-09",200,167]
[null,"2019-04-10",198,178]
[null,"2019-04-11",218,173]
[null,"2019-04-12",166,133]
[null,"2019-04-13",88,75]
[null,"2019-04-14",94,76]
[null,"2019-04-15",304,238]
[null,"2019-04-16",184,148]
[null,"2019-04-17",417,285]
[null,"2019-04-18",166,145]
[null,"2019-04-19",76,64]
[null,"2019-04-20",104,91]
[null,"2019-04-21",208,174]
[null,"2019-04-22",84,79]
[null,"2019-04-23",186,168]
[null,"2019-04-24",317,235]
[null,"2019-04-25",65,63]
[null,"2019-04-26",381,223]
[null,"2019-04-27",208,152]
[null,"2019-04-28",194,168]
[null,"2019-04-29",293,236]
[null,"2019-04-30",464,312]
[null,"2019-05-01",204,182]
[null,"2019-05-02",432,332]
[null,"2019-05-03",272,201]
[null,"2019-05-04",145,118]
[null,"2019-05-05",97,82]
[null,"2019-05-06",219,149]
[null,"2019-05-07",209,194]
[null,"2019-05-08",287,214]
[null,"2019-05-09",240,176]
[null,"2019-05-10",192,160]
[null,"2019-05-11",147,123]
[null,"2019-05-12",58,55]
[null,"2019-05-13",163,154]
[null,"2019-05-14",165,141]
[null,"2019-05-15",170,148]
[null,"2019-05-16",217,177]
[null,"2019-05-17",194,147]
[null,"2019-05-18",84,79]
[null,"2019-05-19",162,137]
[null,"2019-05-20",312,254]
[null,{"$f":"B1608+1","v":"2019-05-21"},183,164]
[null,"2019-05-22",209,196]
[null,"2019-05-23",181,153]
[null,"2019-05-24",235,187]
[null,"2019-05-25",149,86]
[null,"2019-05-26",175,139]
[null,"2019-05-27",527,394]
[null,"2019-05-28",352,245]
[null,"2019-05-29",267,212]
[null,"2019-05-30",148,130]
[null,"2019-05-31",279,227]
[null,"2019-06-01",81,71]
[null,"2019-06-02",96,85]
[null,"2019-06-03",310,218]
[null,"2019-06-04",170,163]
[null,"2019-06-05",236,172]
[null,"2019-06-06",186,152]
[null,"2019-06-07",158,142]
[null,"2019-06-08",129,101]
[null,"2019-06-09",158,136]
[null,"2019-06-10",96,88]
[null,"2019-06-11",154,118]
[null,"2019-06-12",227,195]
[null,"2019-06-13",255,199]
[null,"2019-06-14",173,141]
[null,"2019-06-15",128,106]
[null,"2019-06-16",127,107]
[null,"2019-06-17",206,148]
[null,"2019-06-18",210,174]
[null,"2019-06-19",211,177]
[null,"2019-06-20",200,181]
[null,"2019-06-21",211,183]
[null,"2019-06-22",142,103]
[null,"2019-06-23",130,83]
[null,"2019-06-24",214,192]
[null,"2019-06-25",230,197]
[null,"2019-06-26",205,170]
[null,"2019-06-27",196,172]
[null,"2019-06-28",214,186]
[null,"2019-06-29",653,283]
[null,"2019-06-30",278,228]
[null,"2019-07-01",202,189]
[null,"2019-07-02",164,151]
[null,"2019-07-03",237,231]
[null,"2019-07-04",226,182]
[null,"2019-07-05",154,134]
[null,"2019-07-06",151,112]
[null,"2019-07-07",105,87]
[null,"2019-07-08",331,272]
[null,"2019-07-09",210,191]
[null,"2019-07-10",591,376]
[null,"2019-07-11",857,658]
[null,"2019-07-12",302,248]
[null,"2019-07-13",406,259]
[null,"2019-07-14",466,328]
[null,"2019-07-15",520,419]
[null,"2019-07-16",220,168]
[null,"2019-07-17",176,155]
[null,"2019-07-18",266,229]
[null,"2019-07-19",155,134]
[null,"2019-07-20",119,105]
[null,"2019-07-21",176,151]
[null,"2019-07-22",238,220]
[null,"2019-07-23",248,226]
[null,{"$f":"B1672+1","v":"2019-07-24"},264,220]
[null,"2019-07-25",168,150]
[null,"2019-07-26",222,179]
[null,"2019-07-27",134,87]
[null,"2019-07-28",53,38]
[null,"2019-07-29",194,167]
[null,"2019-07-30",182,158]
[null,"2019-07-31",149,122]
[null,"2019-08-01",204,155]
[null,"2019-08-02",201,184]
[null,"2019-08-03",170,101]
[null,"2019-08-04",69,65]
[null,"2019-08-05",125,114]
[null,"2019-08-06",229,206]
[null,"2019-08-07",154,139]
[null,"2019-08-08",315,221]
[null,"2019-08-09",542,450]
[null,"2019-08-10",232,188]
[null,"2019-08-11",223,156]
[null,"2019-08-12",243,215]
[null,"2019-08-13",204,177]
[null,"2019-08-14",218,185]
[null,"2019-08-15",350,267]
[null,"2019-08-16",431,352]
[null,"2019-08-17",116,92]
[null,"2019-08-18",158,136]
[null,"2019-08-19",198,181]
[null,"2019-08-20",224,193]
[null,"2019-08-21",252,219]
[null,"2019-08-22",359,260]
[null,"2019-08-23",180,162]
[null,"2019-08-24",141,106]
[null,"2019-08-25",59,54]
[null,"2019-08-26",203,179]
[null,"2019-08-27",172,154]
[null,"2019-08-28",211,182]
[null,"2019-08-29",183,170]
[null,"2019-08-30",210,153]
[null,"2019-08-31",111,89]
[null,"2019-09-01",97,84]
[null,"2019-09-02",205,184]
[null,"2019-09-03",173,162]
[null,"2019-09-04",162,132]
[null,"2019-09-05",185,178]
[null,"2019-09-06",183,166]
[null,"2019-09-07",327,275]
[null,"2019-09-08",201,168]
[null,"2019-09-09",623,484]
[null,"2019-09-10",189,171]
[null,"2019-09-11",232,151]
[null,"2019-09-12",221,207]
[null,"2019-09-13",166,146]
[null,"2019-09-14",73,69]
[null,"2019-09-15",66,65]
[null,"2019-09-16",190,180]
[null,"2019-09-17",168,164]
[null,"2019-09-18",188,151]
[null,"2019-09-19",224,194]
[null,"2019-09-20",194,174]
[null,"2019-09-21",261,186]
[null,"2019-09-22",115,106]
[null,"2019-09-23",147,144]
[null,"2019-09-24",208,190]
[null,"2019-09-25",896,664]
[null,{"$f":"B1736+1","v":"2019-09-26"},157,147]
[null,"2019-09-27",176,153]
[null,"2019-09-28",66,63]
[null,"2019-09-29",127,93]
[null,"2019-09-30",320,266]
[null,"2019-10-01",440,393]
[null,"2019-10-02",186,180]
[null,"2019-10-03",156,153]
[null,"2019-10-04",206,199]
[null,"2019-10-05",93,78]
[null,"2019-10-06",72,67]
[null,"2019-10-07",251,239]
[null,"2019-10-08",203,192]
[null,"2019-10-09",159,151]
[null,"2019-10-10",125,116]
[null,"2019-10-11",194,184]
[null,"2019-10-12",81,76]
[null,"2019-10-13",119,107]
[null,"2019-10-14",158,151]
[null,"2019-10-15",166,164]
[null,"2019-10-16",187,176]
[null,"2019-10-17",541,320]
[null,"2019-10-18",221,197]
[null,"2019-10-19",89,85]
[null,"2019-10-20",49,49]
[null,"2019-10-21",152,141]
[null,"2019-10-22",217,208]
[null,"2019-10-23",180,171]
[null,"2019-10-24",180,173]
[null,"2019-10-25",220,188]
[null,"2019-10-26",470,277]
[null,"2019-10-27",184,167]
[null,"2019-10-28",229,216]
[null,"2019-10-29",266,216]
[null,"2019-10-30",230,208]
[null,"2019-10-31",200,192]
[null,"2019-11-01",243,222]
[null,"2019-11-02",154,146]
[null,"2019-11-03",286,203]
[null,"2019-11-04",317,249]
[null,"2019-11-05",134,128]
[null,"2019-11-06",224,209]
[null,"2019-11-07",203,188]
[null,"2019-11-08",279,252]
[null,"2019-11-09",183,129]
[null,"2019-11-10",70,67]
[null,"2019-11-11",185,170]
[null,"2019-11-12",319,249]
[null,"2019-11-13",151,144]
[null,"2019-11-14",138,135]
[null,"2019-11-15",138,135]
[null,"2019-11-16",154,116]
[null,"2019-11-17",89,86]
[null,"2019-11-18",204,162]
[null,"2019-11-19",122,120]
[null,"2019-11-20",241,225]
[null,"2019-11-21",0,0]
[null,"2019-11-22",932,606]
[null,"2019-11-23",313,238]
[null,"2019-11-24",68,67]
[null,"2019-11-25",221,207]
[null,"2019-11-26",286,264]
[null,"2019-11-27",211,191]
[null,"2019-11-28",168,167]
[null,{"$f":"B1800+1","v":"2019-11-29"},163,150]
[null,"2019-11-30",108,102]
[null,"2019-12-01",175,135]
[null,"2019-12-02",262,230]
[null,"2019-12-03",246,221]
[null,"2019-12-04",407,287]
[null,"2019-12-05",150,145]
[null,"2019-12-06",339,304]
[null,"2019-12-07",166,134]
[null,"2019-12-08",71,67]
[null,"2019-12-09",281,254]
[null,"2019-12-10",138,138]
[null,"2019-12-11",154,147]
[null,"2019-12-12",225,185]
[null,"2019-12-13",170,161]
[null,"2019-12-14",129,113]
[null,"2019-12-15",66,66]
[null,"2019-12-16",185,176]
[null,"2019-12-17",228,216]
[null,"2019-12-18",571,439]
[null,"2019-12-19",346,313]
[null,"2019-12-20",625,374]
[null,"2019-12-21",187,173]
[null,"2019-12-22",119,102]
[null,"2019-12-23",182,177]
[null,"2019-12-24",225,171]
[null,"2019-12-25",86,79]
[null,"2019-12-26",72,70]
[null,"2019-12-27",421,408]
[null,"2019-12-28",162,147]
[null,"2019-12-29",203,172]
[null,"2019-12-30",0,0]
[null,"2019-12-31",733,625]

{"sheet":"6.2 Reliability & Cust serv","index":33,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[[5,1,5,7],[8,4,8,8],[16,1,16,3],[20,4,20,8],[28,1,28,3],[32,4,32,8],[70,4,70,8],[40,1,40,3],[44,4,44,8],[52,1,52,3],[55,1,55,8],[58,2,58,8],[67,1,67,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,76.747701561442938,76.747701561442938,76.747701561442938,76.747701561442938,76.747701561442938]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,188.09697493108868,188.09697493108868,188.09697493108868,188.09697493108868,188.09697493108868]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,270.86873903162251,270.86873903162251,270.86873903162251,270.86873903162251,270.86873903162251]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E12:E16)","v":535.71341552415413},{"$f":"SUM(F12:F16)","v":535.71341552415413},{"$f":"SUM(G12:G16)","v":535.71341552415413},{"$f":"SUM(H12:H16)","v":535.71341552415413},{"$f":"SUM(I12:I16)","v":535.71341552415413}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.82843788617166569,0.82843788617166569,0.82843788617166569,0.82843788617166569,0.82843788617166569]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1.9773349256486792,1.9773349256486792,1.9773349256486792,1.9773349256486792,1.9773349256486792]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,2.5820701403108997,2.5820701403108997,2.5820701403108997,2.5820701403108997,2.5820701403108997]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E24:E28)","v":5.3878429521312441},{"$f":"SUM(F24:F28)","v":5.3878429521312441},{"$f":"SUM(G24:G28)","v":5.3878429521312441},{"$f":"SUM(H24:H28)","v":5.3878429521312441},{"$f":"SUM(I24:I28)","v":5.3878429521312441}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E36:E40)","v":0},{"$f":"SUM(F36:F40)","v":0},{"$f":"SUM(G36:G40)","v":0},{"$f":"SUM(H36:H40)","v":0},{"$f":"SUM(I36:I40)","v":0}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,2.6958910251838715,2.6958910251838715,2.6958910251838715,2.6958910251838715,2.6958910251838715]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,5.7582886006054448,5.7582886006054448,5.7582886006054448,5.7582886006054448,5.7582886006054448]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,10.556527448521333,10.556527448521333,10.556527448521333,10.556527448521333,10.556527448521333]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E48:E52)","v":19.010707074310648},{"$f":"SUM(F48:F52)","v":19.010707074310648},{"$f":"SUM(G48:G52)","v":19.010707074310648},{"$f":"SUM(H48:H52)","v":19.010707074310648},{"$f":"SUM(I48:I52)","v":19.010707074310648}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},314998.48904970684,320638.93723421206,326143.41190689901,331656.87942890119,337224.38252020173,342874.6662367126,348543.78988796449]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},299949.21408801718,305320.18588267727,310561.68039593921,315811.73811879836,321113.24982352491,326493.58725071274,331891.86452147283]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},128340.3939472567,130638.49177059026,132881.18966446447,135127.55153090984,137395.92920534156,139698.03433695171,142007.81545664009]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C61:C65)","v":743288.09708498069},756597.61488747958,769586.28196730267,782596.16907860932,795733.5615490682,809066.28782437707,822443.46986607742]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Number of calls received",null,null,113708,115982,118302,120668,123081]
[null,"Number of calls answered within 30 seconds",null,null,90966,92786,94642,96534,98465]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E74/E73),\"\")","v":0.79999648221760999},{"$f":"IFERROR((F74/F73),\"\")","v":0.80000344881102237},{"$f":"IFERROR((G74/G73),\"\")","v":0.80000338117698766},{"$f":"IFERROR((H74/H73),\"\")","v":0.79999668511950139},{"$f":"IFERROR((I74/I73),\"\")","v":0.80000162494617366}]

{"sheet":"7.1  Policies and Procedures","index":34,"n_rows":216,"n_cols":5,"rows_kept":216,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"AusNet Services Corporate Strategic Plan: Energising Futures","Represents our view of internal and external business environments, corporate objectives and strategic directions ","Balanced corporate directions that set the tone and priorities of aspects of our Regulatory Proposal. ","No"]
[]
[]
[null,"Governance framework"]
[null,"AMS 01-01 Asset Management System Overview","The document provides an overview of the systems, policies, strategies, plans, standards, processes and procedures which have been integrated in AusNet Services ISO 55001 certified asset management system to enable performance management of the  gas and electricity networks and the assets forming those networks. ","Provides an overview of the asset management system and interdependencies.","No"]
[]
[null,"AMS 01-04 ISO 55001 Accreditation","Certificate demonstrates AusNet Services' achievement of the standard necessary to demonstrate compliance with the requirements of Asset Management systems.","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"AMS 01-09 Asset Risk Management","This document outlines the various components and methods used in risk identification, evaluation and management.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"AMS 20-13 Enhanced Network Safety","The objective of the Enhanced Safety Strategy is to optimise the output of the Electricity Safety Management Scheme (ESMS), the Bushfire Mitigation program and the Occupational Health & Safety Management System to identify and prioritise opportunities to develop and implement network asset management initiatives and programs that continuously reduce network related health and safety risks 'so far as is practicable’ for customers, public and personnel. ","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"BFM 10-01 Bushfire Mitigation Plan","This document outlines the initiatives and controls implemented by AusNet Services to reduce bushfire risk on its electricity distribution network.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"QMS 10-01-1 Health, Safety, Enviornment and Quality Policy","High level document that shows AusNet Services commitment to providing a safe and healthy work enviornment","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"ESMS 10-01 Electricity Safety Management Scheme","This document (ESMS 10-01 Overview) contains a summary of the structure of the ESMS for AusNet Services' electricity distribution supply network.  It also outlines the period of application, the location of ESMS records, exemptions and lists officers responsible for the operation of this ESMS.","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[null,"ESMS 10-03 Electricity Safety Management System","This document describe the assets forming AusNet Services' electricity distribution supply network, their location and the associated planning, design, construction, commissioning, operation, augmentation, inspection, testing, maintenance, refurbishment, replacement and decommissioning processes necessary to ensure the safety of consumers, the general public, AusNet Services' staff and contractors.","Applies to all aspects of the day to day operations and our Proposal. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Unit Rates","This document lists the unit rates used in estimating the cost of replacing, installing or maitaining network assets.","Chapter 9 Capex","No"]
[null,"Project Cost Estimating","This document outlines the method used for estimating the cost of projects.","Chapter 9 Capex","No"]
[null,"Top down adjustment","This document identifies areas of potential overlaps between programs an projects.","Chapter 9 Capex","No"]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Strategy","High level document that directs the content and implementation of asset management strategies, objectives and plans for the network and guides asset management decisions.","Underpins all asset related expenditure.","No"]
[]
[null,"Asset Management Strategies"]
[null,"Security Infrastructure","This document includes Strategies for the management of infrastructure physical security associated with the AusNet Services electricity distribution network in eastern Victoria.  The scope of infrastructure covered by this document includes:\n\n• Zone substations\n• Voltage regulators and ground-type substations\n• Kiosk substations\n• Indoor substations\n• Cable distribution cabinets\n• Pole mounted installations\n• Tower mounted installations\n• Underground cables.\n\nThis document does not include information technology security strategies: please refer to the Information and Communication Technology Strategy  for information on this topic.\n","Chapter 9 Capex","No"]
[null,"Power Transformers and Station Voltage Regulators","The purpose of this document is to define the asset management strategies for the power transformers and station voltage regulators located within zone-substations within the AusNet Services’ electricity distribution network for the next 20 years. \n","Chapter 9 Capex\n","No"]
[]
[]
[null,"Asset Management Plans"]
[null,"Asset Management Plan 2019/20 to 2023/24","Document sets the framework for AusNet Services’ holistic approach to management of the network assets, and in so doing establishes the linkages with and between the underpinning detailed strategies, processes and plans. The document provides context for management strategies, by taking into account the demand for network services, the condition of network assets, and expected trends into the future.  It therefore also has regard to the network augmentation planning process.\n","This strategy provides a high level overview of AusNet Services approach to  managing the distribution network, meeting regulatory obligations and informing stakeholders by:\n• presenting a distribution network overview including network summary, planning and regulatory framework;\n• presenting an overview of the asset management system in regard to the distribution network;\n• describing asset management drivers including network safety, demand and utilisation and reliability;\n• Summating the process and systems and plant asset management strategies\n","No"]
[null,"Asset Risk Assessment Overview","This document describes the risk assessment process used by AusNet Services to identify and assess the highest risks associated with network assets. These risk assessments are used to inform the development of optimised inspection, maintenance and replacement programs, forecast future asset replacement capital and operational expenditure and assist in the prioritisation of work.","Chapter 9 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Asset Management System Overview","The document provides an overview of the systems, policies, strategies, plans, standards, processes and procedures which have been integrated in AusNet Services ISO 55001 certified asset management system to enable performance management of the  gas and electricity networks and the assets forming those networks. ","Provides an overview of the asset management system and interdependencies.","No"]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Augmentation","It summarises the proposed augmentations works within the 2022-26 Electricity Distribution Price Review period to ensure that AusNet Services achieves its regulatory and business performance targets.","Describes expenditure required for network reinforecement and demand side management.","No"]
[null,"Network Support Services","This asset management strategy guides the commercial application of demand management and non-network solutions, known as Network Support Services, to manage constraints within the electricity distribution network within the context of strengthened regulatory obligations and dedicated revenues established in the  Electricity Distribution Price Review.","This document supports demand management activities to be undertaken during the fortchoming regualtory period.","No"]
[null,"Zone Substation Capacitor Banks","This asset management strategy applies to all 22 kV, 11 kV and 6.6 kV capacitor banks located in zone substations and capacitor bank stations within the AusNet Services’ electricity distribution network.  There are no capacitor banks that operate at 66 kV sub transmission voltage level. This strategy does not include the management of pole top capacitors ."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Pole-Top Capacitors","The purpose of this document is to define the asset management strategies for the AusNet Services electricity distribution network’s population of pole-top capacitors.  "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Surge Diverters in Zone Substations","This asset management strategy applies to all surge arresters located within AusNet Services’ electricity distribution zone substations that operate at 66 kV, 22 kV, 11 kV and 6.6 kV. Surge arresters mounted on medium voltage structures in the distribution network are not covered in this document. For medium voltage surge arresters in the distribution network refer AMS 20-67 “Line Surge Arresters”.\n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Neutral Earthing Devices","This asset management strategy applies to all neutral earthing resistors, neutral earthing compensators and ground fault neutralisers associated with the AusNet Services electricity distribution network that operate at voltages between earth potential and 22 kV, 11 kV and 6.6 kV. The power transformer medium voltage winding neutral points within zone substations are directly connected to earth or via neutral earthing resistors (NERs), or in stations with delta-connected phases, through neutral earthing compensators (NECs). "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Service Cables","The purpose of this document is to optimise the maintenance, replacement and performance of the 456,500 service cables connecting customers to low voltage (LV) circuits in AusNet Service’s electricity distribution network."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Communication Systems","This document describes the Asset Management Strategies for Communication Systems in the AusNet Services electricity distribution network.","This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Line Surge Arresters","The purpose of this document is to define the asset management strategy for the AusNet Services electricity distribution network’s population of line surge arresters.  This asset management strategy applies to all line surge arresters associated with the AusNet Services electricity distribution network that operate at 22 kV, 11 kV and 6.6 kV. \n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"MV Fuse Switch Disconnectors","The purpose of this document is to define the asset management strategy for the AusNet Services electricity distribution network’s population of medium voltage (MV) fuse switch disconnectors (FSD). This asset management strategy applies to the 103,500 MV fuse switch disconnectors protecting distribution substations and sections of single wire earth return (SWER) lines and single-phase spurs on medium voltage feeders in the AusNet Services electricity distribution network. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Instrument Transformers","This asset management strategy (AMS) applies to 1297 independent single-phase and three-phase post type current transformers (CTs) and 608 voltage transformers (VTs), magnetic voltage transformers (MVTs) and capacitive voltage transformers (CVTs) in the AusNet Services’ electricity distribution network. Toroidal current transformers that are built into transformers, Gas Insulated Switchgear (GIS) and bulk oil circuit breaker bushings are not included in this assessment. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Distribution Transformers","The purpose of this strategy is to identify the issues and define the company’s approach to the management of distribution transformers. The AusNet Services electricity distribution network in Victoria includes 62,561 distribution transformers to convert electrical energy from 22 kV, 11 kV or 6.6 kV to 420/230 V in urban areas or 460/230 V in rural areas.\n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"MV Switches and ACRs","This asset management strategy applies to all MV switches and ACRs associated with the AusNet Services electricity distribution network that operate at 22 kV, 12.7 kV, 11 kV and 6.6 kV."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Circuit Breakers","This document summarises the key strategies used to manage the fleet of high voltage and medium voltage circuit breakers to maintain the reliability, safety and security of the distribution network. This asset management strategy applies to the 957 circuit breakers operating at 66 kV, 22 kV, 11 kV and 6.6 kV located in zone substations.\n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Civil Infrastructure","The scope of this asset management strategy includes civil infrastructure in zone substations and voltage regulator stations supporting the electricity distribution network. The strategy also includes shared civil infrastructure in terminal stations and power stations which connected to the electricity distribution network. \nCivil infrastructure  includes buildings, environmental systems, security fence and overall switchyard including switchyard surface, access roads, stations lights, cable ducts and trenches, signage and name plates, support structures and foundations that all contribute to the overall function of the stations.\n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Conductor","This strategy applies to all bare overhead conductors including those operating at LV (415 V), those operating at MV (22 kV, 11 kV and 6.6 kV) and those operating at HV (66 kV) circuits.\nThe scope of this AMS has been extended to include conductor ties, vibration dampers, armour rods, joints and spreaders which are all installed on bare overhead conductors. Aerial Bundled Cable (ABC) has been removed from the scope of this strategy and included in a separate document, AMS 20-65 .\n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Public Lighting","The purpose of this document is to define the asset management strategies for the AusNet Services electricity distribution network’s population of public lighting.  This strategy is to assist personnel involved in managing the assets, meeting regulatory obligations and informing other stakeholders."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Protection and Control Systems","This asset management strategy applies to all protection and control systems located within zone substations that operate at 66 kV, 22 kV, 11 kV and 6.6 kV in the AusNet Services’ electricity distribution network. Protection and control systems associated with Automatic Circuit Reclosers, Sectionalisers, medium voltage fuses and low voltage fuses, Distribution Feeder Automation and line voltage regulators are not covered by this document. "," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Power Transformers and Station Voltage Regulators","The purpose of this document is to define the asset management strategies for the power transformers and station voltage regulators located within zone-substations within the AusNet Services’ electricity distribution network for the next 20 years. \n"," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"HV Switches, Disconnectors and Earth Switches","The purpose of this document is to define the asset management strategies for the AusNet Services electricity distribution network’s population of High Voltage (HV) switches, disconnectors and earth switches located in zone substations.  This asset management strategy applies to all HV switches, disconnectors and earth switches associated with the AusNet Services electricity distribution network that operate at 66 kV, 22 kV, 11 kV and 6.6 kV in zone substations and power station switchyards."," This strategy is intended to assist in managing the assets, meeting regulatory obligations and informing stakeholders by:\n• presenting an overview of the asset population;\n• describing the condition and life cycle phase of the current fleet;\n• understanding asset behaviour through failure mode effect and criticality analysis;\n• requirements to achieve network reliability targets taking account of risk, costs and customer expectations; and\n• methods for effective and economic management of the asset population throughout the life-cycle.\n• outlining strategies to manage  the emerging performance risks through inspection, maintenance, refurbishment and replacement activities;\n","No"]
[null,"Infrastructure Security","This document includes Strategies for the management of infrastructure physical security associated with the AusNet Services electricity distribution network in eastern Victoria.  The scope of infrastructure covered by this document includes:\n\n• Zone substations\n• Voltage regulators and ground-type substations\n• Kiosk substations\n• Indoor substations\n• Cable distribution cabinets\n• Pole mounted installations\n• Tower mounted installations\n• Underground cables.\n\nThis document does not include information technology security strategies: please refer to the Information and Communication Technology Strategy  for information on this topic.\n","Identifies expenditure required to ensure network and site security including upgrades, maintenance and replacements.","No"]
[null,"Steady State Voltage Complaince","This document presents the current and estimated future levels of voltage compliance, the work that has been carried out to-date to improve voltage compliance levels and the need for further augmentation","Chapter 9 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"Procurement Principles","This document defines the priciples to ensure an integrated, consistent and compliant approach to procuremnt is undertaken across the organisation","Business as usual","No"]
[]
[null,"Information technology policies or strategies"]
[null,"Technology Strategy","The technology Strategy document provides the overview, rationalse and portfolio summary of the proposed IT expenditure for the 2022-26 regulatory proposal","Chapter 9 Capex","Yes"]
[null,"ICT Program Classification","This document provides the overview, rationale and  summary of the proposed IT expenditure programs for the forthcoming period and supports our regulatory proposal","Chapter 9 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Demand Side Engagement Strategy","The Demand Side Engagement Strategy is designed to assist non-network providers in understanding our framework and processes for assessing demand side options. This engagement strategy also discusses our consultation process with non-network\nproviders","RIN Supporting Information","Yes"]
[null,"Distribution Annual Planning Report","AusNet Services produces each year a Distribution Annual Planning Report (DAPR) in accordance with the requirements of Section 5.13.2 of the National Electricity Rules (NER).  The information contained within the DAPR complies with the requirements of Schedule 5.8 of the NER ","Chapter 9 Capex","No"]
[]
[null,"Self insurance guidelines or policy"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Land and easement acquisition polices"]
[null,"Asset Capitalisation Policy (Property, Plant & Equipment)","The document describes property strategy, asset management plan and expenditure program to meet our strategic objectives and operational requirements. ","RIN Supporting Information, Chapter 9 Capex","No"]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"Refer to Asset Management Plans"]
[null,"BFM 10-01 Bushfire Mitigation Plan","This plan details the policies and procedures which govern AusNet Services bushfire risk management practices. It is a self contained document except where it specifically refers to other related documents. ","Chapter 9 Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"Network Contingency Plan","The objective of this Plan is to provide the framework for network contingency planning and provide an overview of the suite of contingency plans established for the electricity distribution network. The Network Contingency Plan is applicable to events that directly impact or are likely to directly impact or impede the safe and reliable operation of the distribution network or which interrupt or are likely to interrupt power supply which require a Level 2 or greater response under the SPIRACS Crisis & Emergency Management Guide 30-4006-041. It does not cover the broader business continuity planning undertaken under SPIRACS.","This document underpins expenditure required for network contigency if a plan is enacted for the electricity distribution network.","No"]

{"sheet":"7.2 Contingent projects","index":35,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2021-22 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2021-22"}]
[null,null,null,null,null,{"$f":"+E8*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":36,"n_rows":296,"n_cols":5,"rows_kept":296,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"National Electricity Law (NEL)","Impose obligations including registration, distribution losses, network connections, economic regulation and metering.","Submission document","No"]
[null,"Electricity Industry Act 2000","Sets out key obligations relating to distribution of electricity in Victoria including matters such as licences and compliance with industry codes, standards, rules and guidelines.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"Electricity Safety Amendment (Bushfire Mitigation Civil Penalties Scheme) Act 2017 ","Amended the Electricity Safety Act 1998 (Vic) (ESA) to provide for significant financial penalties if AusNet Services fails to achieve the REFCL milestones prescribed by the Regulations by the applicable deadline","Chapter 9 Capex, Chapter 10 Opex, Chapter 17 Cost pass Through","Yes"]
[null,"Electricity Safety (Bushfire Mitigation) Regulations 2013 (amendments as at 1 May 2016)","Requires the preparation of bushfire mitigation plans and specifies inspection of assets.","Chapter 9 Capex, Chapter 10 Opex, Chapter 17 Cost pass Through","Yes"]
[null,"Electricity Safety (Electric Line Clearance) Regulations 2015","Prescribes line clearance requirements including vegetation clearing","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Electricity Safety (Management) Regulations 2009","Sets out requirements for Electricity Safety Management Schemes.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Electricity Distribution Code ","Regulates connection and distribution of electricity to customers, connection of embedded generating units, and transfer between distribution systems to ensure that they are undertaken in a safe, efficient and reliable manner. Sets out obligations in relation to smart meters.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"Electricity System Code","Requires particular power quality and connection characteristics.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Public Lighting Code","Regulates the provision of public lighting by specifying minimum standards and certain obligations of distributors and public lighting customers.","Chapter 18 Alternative Control Services","No"]
[null,"Electricity Industry Guideline No.14","Sets out customer contributions, requirements for undergrounding network assets and contestability of connection works.","Chapter 9 Capex, Chapter 10 Opex, TSS","No"]
[null,"Electricity Industry Guideline No.15","Sets out arrangement for connecting embedded generation units to distribution systems","Chapter 9 Capex, Chapter 10 Opex, TSS","No"]
[null,"Electricity Distribution Licence","Sets out obligations of AusNet Services in relation to distribution of electricity in Victoria including requirements to connect customers, offer services, undertake network augmentation and comply with orders, codes and guidelines.","Chapter 7 Demand Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"Emergency Management Act 2013","Establishes arrangments for management of emergencies in Victoria ","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Terrorism (Community Protection) Act 2003","Obliges providers of essential services including electricity to plan for the protection of services from the effects of terrorist acts.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Energy and Water Ombudsman Charter 2006","Describes how electricity licence holders must participate in a customer dispute resolution scheme and how this scheme operates in Victoria.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Occupational Health and Safety Act 2004","Sets out duties of employers and persons who manage or control workplaces to provide for the health, safety and welfare of employees and other persons including the public. Describes the principle of eliminating or reducing risks so far as is practicable.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Occupational Health and Safety Regulations 2017","Detail many aspects of OH&S including manual handling, exposure to noise, prevention of falls, work in confined spaces, operating plant, and asbestos control & handling. ","Chapter 9 Capex, Chapter 10 Opex Chapter 19 Metering","No"]
[null,"National Greenhouse and Energy Reporting Act 2007","Provides for reporting and dissemination of information related to greenhouse emissions including annual reporting.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"National Greenhouse and Energy Reporting Regulations 2008","Sets out requirements for reporting greenhouse emissions.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Environment Protection Act 1970","Legislative framework for the protection of the environment in Victoria.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Environmental Protection (Residential Noise) Regulations 2018","Prescribes items and times during which noise resulting from their use is deemed to be unreasonable on residential properties.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Aboriginal Heritage Act 2006","Promotes the recognition, protection and conservation of Aboriginal culture in Victoria; recognition of Aboriginal people as the primary guardians of their cultural heritage; and management of Aboriginal cultural heritage as an integral part of land management.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Land Act 1958","Defines Crown Land and conditions relating to Crown Land which prohibit a number of activities including refuelling of vehicles, removal of vegetation and disposal of waste.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"National Measurement Act 1960 and Regulations","The National Measurement Act establishes a national system of units and standards of measuremnet of physical quantities and provides for a national system of trade measurements. The National Trade Measurement Regulations were amended in remove the exemption for electricity meters.  Electricity meters installed prior to 1 January 2013 are exempt, whilst electricity meters installed after 1 January 2013 must comply with the National Measurement Act and Regulations.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Privacy Act 1988","Obligations to protect the privacy of individuals and the responsible and transparent handling of personal information in accordance with the Australian Privacy Principles (APPs).","Submission document","No"]
[null,"AMI Cost Recovery Order in Council (CROIC)","The Order in Council made on 28 August 2007 under section 15A and 46D of the Electricity Industry Act 2000 as amended from time to time establishing  \n- conditions for cost recovery for AMI deployments;\n- obligations requiring Victorian Distribution Businesses to deploy an AMI meter to every eligible customer; and\nrequirements to pay rebates to customers without an AMI meter installed or operating as remotely read interval meters","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"AMI Specifications Order","The Order in Council made on 12 November 2007 under section 15A and 46D of the Electricity Industry Act 2000 requiring the deployment of AMI Meters and AMI System inaccordance with the Minimum AMI Functionality Specification and the Minimum AMI Service Levels Specification in Victoria.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"AMI Tariff Order","Provides the regulatory framework for applying AMI tariffs, transfer between and consent to AMI tariffs, assignment of AMI tariffs, customer access to meter data.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"Electricity Customer Transfer Code","The purpose of this Code is to facilitate and regulate aspects of the process by which customers can choose to change retailer.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Customer Metering Code","The purpose of this Code is to regulate customer metering to the extent not regulated by AEMO Procedures.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"Default Use-Of-System Agreement","This agreement sets out the rights and obligations of the parties in respect of:\n(a) the provision of the Distribution Services by the Distributor to the Retailer in respect of Customers, and the payment for those Distribution Services by the Retailer; and\n(b) the provision of Retail Services by the Retailer, and the payment for those Retail Services by the Distributor","Chapter 7 Demand Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering, TSS","No"]
[null,"Metrology Procedures","Establishes obligations on the application of metering installations to connection points and sets out provisions for metering installations and metering data services.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"MPB Service Level Procedure","Details the technical requirements and performances associated with the provision, installation and maintenance of a metering installation. ","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"MDP Service Level Procedure","Details the obligations, technical requirements and performances associated with the processes of meter reading, data collection, data processing, adjustment, aggregation and delivery of metering data","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"NMI Procedures","Establishes conditions and describes processes for creating and abolishing NMIs","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"CATS Procedures","Establishes the conditions and processes for governing AEMO's Market Settlement and Transfer System (MSATS)","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"B2B Procedures","Define the transactions and conditions for information exchange as defined under chapter 7 of the Rules","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"Other Metering Services procedures and guidelines","Various procedures and guidelines that instruct participants on how metering and related interaction to other participants is to be undertaken.","Chapter 9 Capex, Chapter 10 Opex, Chapter 19 Metering","No"]
[null,"Direction under Section 141(2)(d) of the Electricity Safety Act 1998 Fitting of Spacers in Aerial Lines","Direction from Energy Safe Victoria under Section 141(2)( d) of the Electricity Safety Act 1998 which requires the fitting of spacers in overhead lines.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"National Electricity (Victoria) Act 2005","This Act provides for the regulation of the national electricity wholesale market. It is part of a national scheme which gives effect to the National Electricity Law and the National Electricity Rules made under that Law. The lead legislation under the national scheme is the National Electricity (South Australia) Act 1996. The economic regulator is the Australian Energy Regulator (AER) and the rule-maker is the Australian Energy Market Commission (AEMC). The national electricity wholesale market is administered by the Australian Energy Market Operator (AEMO).","Chapter 16 Incentive Scheme","No"]
[null,"Superannuation Guarantee (Administration) Act 1992, No. 111","The Act sets out relevant superannuation payment requirements.","Chapter 10 Opex","No"]
[null,"Roads Management Act 2004 (Vic)","Safety obligations when carrying out works on public roadways.","Chapter 9 Capex, Chapter 18 Public Lighting","No"]
[null,"Fair Work Act 2009","Sets out our obligations in relation to the negotiation of employment terms and conditions.","Chapter 10 Opex","No"]
[null,"The Security of Critical Infrastructure Act 2018 (Cth) ","May result in additional cyber security obligations being imposed on AusNet Services","Chapter 10 Opex","Yes"]
[null,"National Electricity Amendment (Five Minute Settlement) Rule 2017 No. 15","Aligns operational dispatch and financial settlement to occur at five minute intervals","Chapter 10 Opex","Yes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"Electricity Distribution Licence (2005)","The Licence authorisesAusNet Services to distribute or supply electricity to supply points located in the Licensee’s distribution area.","Chapter 9 Capex","No"]
[]
[]
[]
[null,"RULES"]
[null,"National Electricity Rules\n\n\nNational Energy Retail Rules","National Electricity Rules - Details the technical operational requirements for the operation of the National Electricity Market\nNational Energy Retail Rules","Chapter 9 Capex, Chapter 10 Opex","No"]
[]
[]
[]
[null,"ORDERS"]
[]
[]
[]
[null,"CODES"]
[null,"Building Code of Australia","Building Code of Australia published by the Australian Building Codes Board as in force from time to time\nBuilding and Construction Industry (Fair and Lawful Building Sites) Code 2014\nCode for the Tendering and Performance of Building Work ","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"National Harmonisation of Work Health and Safety Code of Practice","Achieving the standards of health, safety and welfare.","Chapter 9 Capex, Chapter 10 Opex","No"]
[null,"Electricity Distribution Code (2014)","The purpose of this Code is to regulate the following activities so that they are undertaken in a safe, efficient and reliable manner:\n(a) the distribution of electricity by a distributor for supply to its customers;\n(b) the connection of a customer’s electrical installation to the distribution system;\n(c) the connection of embedded generating units to the distribution system; and\n(d) the transfer of electricity between distribution systems.","Chapter 9 Capex, Chapter 16 incentive Schemes, Chapter 17 Cost Pass through","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"AER","Compliance Procedures and Guidelines","Chapter 10 Opex","No"]
[null,"AER","Confidentiality","Confidentiality template","No"]
[null,"AER","Consumer Engagement","Chapter 2 Customer Forum, Chapter 3 Understanding our Customer's Views","Yes"]
[null,"AER","Cost Allocation Guideline (Distribution) ","Cost allocation methodology","No"]
[null,"AER","Distribution Annual Planning Report Template v1.0 (June 2017)","Chapter 9 Capex","No"]
[null,"AER","Electricity Distribution Service Classification Guideline (Sept 2018)","Classification of services","No"]
[null,"AER","Expenditure Forecasts Assessment Guideline for Electricity Distribution","Expenditure Forecasting methodology","No"]
[null,"AER","Ring Fencing Guidelines (Oct 2017)","Chapter 9 capex, Chapter 10 Opex","Yes"]
[null,"AER","RIT-D Application","Chapter 9 Capex","No"]
[null,"AER","Shared Assets","Chapter 8 Revenue","No"]
[null,"AER Scheme","Demand Management Incentive Scheme and Innovation allowance mechanism","Chapter 11 Innovation, Chapter 16 incentive Schemes","No"]
[null,"AER Scheme","Capital Expenditure Incentive Guideline for Electricity Network Service Providers","Chapter 9 Capex","No"]
[null,"AER Scheme","Efficiency Benefit Sharing Scheme for Electricity Network Service Providers","Chapter 10 Opex","No"]
[null,"AER Scheme","Service Target Performance Incentive Scheme ","Chapter 16 Incentive Schemes","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[]
[]
[]
[null,"OTHER"]
[null,"AER Regulatory Information Notice 4 October 2019","Reset 2022-26 information requirements","Chapter 9 Capex, Chapter 10 Opex, RIN templates                                                   ","Yes"]
[null,"AER - Final framework and approach for AusNet Services, CitiPower, Jemena, Powercor and United Energy - January 2019","Sets parameters for our 2022-26 Regulatory Control Period.","Chapter 9 Capex, Chapter 10 Opex","Yes"]

{"sheet":"7.4 Shared Assets","index":37,"n_rows":28,"n_cols":19,"rows_kept":28,"cut":false,"hidden":false,"merged":[[6,1,7,1],[6,2,7,2],[6,3,6,10],[6,11,6,18],[25,1,26,1],[25,2,26,8],[27,2,27,8],[28,2,28,8],[29,2,29,8],[30,2,30,8],[31,2,31,8],[32,2,32,8],[39,2,39,8],[40,2,40,8],[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service","Shared asset unregulated revenue  ($0's, nominal)",null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Shared asset unregulated revenue  ($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  ($0's, real June 2021)"}]
[null,null,null,{"$f":"PRCP_y1","v":"2011-12"},{"$f":"PRCP_y2","v":"2012-13"},{"$f":"PRCP_y3","v":"2013-14"},{"$f":"PRCP_y4","v":"2014-15"},{"$f":"PRCP_y5","v":"2015-16"},{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},{"$f":"CONCATENATE(\"Total \",dms_Header_Span)","v":"Total 2021-22 to 2025-26"}]
[null,"Asset Inspection Services","1. Unmanned Aerial Vehicle (UAV/Drone) x 8\n2. HiMast Camera x 4\n3. Pole Camera x 45 incl wireless controller\n",3025134,2479056,2812631,2850607,3134540,4138188,2404806,"                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ",{"$f":"SUM(N9:R9)","v":0}]
[null,"Contestable Metering (MDP and MP)","Contestable installation and connections",15429024,15553656,16250415,17816631,19941785,10494691,"                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ",0]
[null,"LV CT Testing","Test Equipment",172628,324538,606281,1260869,1611307,1115123,333390,"                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ",0]
[null,"Non-Invasive Testing Services (Thermographic)","Thermographic Test Equipment\n(Thermovision Testing Services, TTS Business Acquisition)",757338,865286,835106,776533,809032,883130,448749,"                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ",0]
[null,"Utility Materials Management","Material sales",7867848,9480464,9313721,9619581,8788596,4267125,"                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ",0]
[null,"Facilities Access Agreements (FAA) Distribution Poles","70,000 distribution poles at all stages in their lifecycle (0-40 years old)",2489468,1229700,1422425,2012512,2027800,2039036,2091365,2148148,2356693,2344933,2334633,2324379,2314169,2304004,2293884,11571069]
[null,"Leasing Access to third parties – Various communication equipment on AMI communication towers or monopoles","4 x AMI monopole","                              -  ","                              -  ","                              -  ","                              -  ",50000,100000,100000,143899,257159,255876,254752,253633,252519,251410,250306,1262620]
[null,"Leasing Access to third parties – wireless equipment installed on distribution poles","19 x distribution poles",249965,297298,315272,211540,245233,321960,278793,281694,320991,319390,317987,316590,315199,313815,312437,1576028]
[null,"Leasing to third parties – wireless base stations installed monopole within zone sub station","1 x monopole (combined in FY19 with 4 AMI monopoles)","                              -  ","                              -  ","                              -  ","                              -  ",37000,74000,74000,"                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ","                              -  ",0]
[null,"Site leasing","Zone substation",14045,14570,15155,15796,50951,45966,13077,26023,6212,6181,6033,6007,5980,5954,5928,29902]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]
[]
[null,"Utility materials management","Revenue apportioned by allocation of corporate IT systems to distribution network (49%)"]

{"sheet":"7.7 TSS-LRMC","index":38,"n_rows":152,"n_cols":22,"rows_kept":152,"cut":false,"hidden":false,"merged":[[5,3,6,4],[10,1,11,1],[10,2,10,21],[21,1,22,1],[21,2,21,21],[32,1,33,1],[32,2,32,21],[109,2,109,21],[124,2,124,21],[139,2,139,21],[46,1,47,1],[46,2,46,21],[66,1,67,1],[66,2,66,21],[86,1,87,1],[86,2,86,21]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is AusNet (D) using the 'Average Incremental Cost' approach?"},null,"YES / NO?"]
[null,null,null,null,null,"YES"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C12,4)+1)&\"-\"&MID(C12,3,2)+2),VALUE(LEFT(C12,4)+1))","v":"2020-21"},"2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39"]
[null,"Replacement expenditure",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",6190060.2133333338,4177864.1800000006,7271500,9556700,7338500,4233500,3946000,13755300,17496400,12726200,6832100,0,0,0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex",{"$f":"SUM(C13:C18)","v":6190060.2133333338},{"$f":"SUM(D13:D18)","v":4177864.1800000006},7271500,9556700,7338500,4233500,3946000,13755300,17496400,12726200,6832100,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C23,4)+1)&\"-\"&MID(C23,3,2)+2),VALUE(LEFT(C23,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D23,4)+1)&\"-\"&MID(D23,3,2)+2),VALUE(LEFT(D23,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E23,4)+1)&\"-\"&MID(E23,3,2)+2),VALUE(LEFT(E23,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F23,4)+1)&\"-\"&MID(F23,3,2)+2),VALUE(LEFT(F23,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G23,4)+1)&\"-\"&MID(G23,3,2)+2),VALUE(LEFT(G23,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H23,4)+1)&\"-\"&MID(H23,3,2)+2),VALUE(LEFT(H23,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I23,4)+1)&\"-\"&MID(I23,3,2)+2),VALUE(LEFT(I23,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J23,4)+1)&\"-\"&MID(J23,3,2)+2),VALUE(LEFT(J23,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K23,4)+1)&\"-\"&MID(K23,3,2)+2),VALUE(LEFT(K23,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L23,4)+1)&\"-\"&MID(L23,3,2)+2),VALUE(LEFT(L23,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M23,4)+1)&\"-\"&MID(M23,3,2)+2),VALUE(LEFT(M23,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N23,4)+1)&\"-\"&MID(N23,3,2)+2),VALUE(LEFT(N23,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O23,4)+1)&\"-\"&MID(O23,3,2)+2),VALUE(LEFT(O23,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P23,4)+1)&\"-\"&MID(P23,3,2)+2),VALUE(LEFT(P23,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q23,4)+1)&\"-\"&MID(Q23,3,2)+2),VALUE(LEFT(Q23,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R23,4)+1)&\"-\"&MID(R23,3,2)+2),VALUE(LEFT(R23,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S23,4)+1)&\"-\"&MID(S23,3,2)+2),VALUE(LEFT(S23,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T23,4)+1)&\"-\"&MID(T23,3,2)+2),VALUE(LEFT(T23,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U23,4)+1)&\"-\"&MID(U23,3,2)+2),VALUE(LEFT(U23,4)+1))","v":"2038-39"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C34,4)+1)&\"-\"&MID(C34,3,2)+2),VALUE(LEFT(C34,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D34,4)+1)&\"-\"&MID(D34,3,2)+2),VALUE(LEFT(D34,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E34,4)+1)&\"-\"&MID(E34,3,2)+2),VALUE(LEFT(E34,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F34,4)+1)&\"-\"&MID(F34,3,2)+2),VALUE(LEFT(F34,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G34,4)+1)&\"-\"&MID(G34,3,2)+2),VALUE(LEFT(G34,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H34,4)+1)&\"-\"&MID(H34,3,2)+2),VALUE(LEFT(H34,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I34,4)+1)&\"-\"&MID(I34,3,2)+2),VALUE(LEFT(I34,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J34,4)+1)&\"-\"&MID(J34,3,2)+2),VALUE(LEFT(J34,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K34,4)+1)&\"-\"&MID(K34,3,2)+2),VALUE(LEFT(K34,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L34,4)+1)&\"-\"&MID(L34,3,2)+2),VALUE(LEFT(L34,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M34,4)+1)&\"-\"&MID(M34,3,2)+2),VALUE(LEFT(M34,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N34,4)+1)&\"-\"&MID(N34,3,2)+2),VALUE(LEFT(N34,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O34,4)+1)&\"-\"&MID(O34,3,2)+2),VALUE(LEFT(O34,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P34,4)+1)&\"-\"&MID(P34,3,2)+2),VALUE(LEFT(P34,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q34,4)+1)&\"-\"&MID(Q34,3,2)+2),VALUE(LEFT(Q34,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R34,4)+1)&\"-\"&MID(R34,3,2)+2),VALUE(LEFT(R34,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S34,4)+1)&\"-\"&MID(S34,3,2)+2),VALUE(LEFT(S34,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T34,4)+1)&\"-\"&MID(T34,3,2)+2),VALUE(LEFT(T34,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U34,4)+1)&\"-\"&MID(U34,3,2)+2),VALUE(LEFT(U34,4)+1))","v":"2038-39"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C48,4)+1)&\"-\"&MID(C48,3,2)+2),VALUE(LEFT(C48,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D48,4)+1)&\"-\"&MID(D48,3,2)+2),VALUE(LEFT(D48,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E48,4)+1)&\"-\"&MID(E48,3,2)+2),VALUE(LEFT(E48,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F48,4)+1)&\"-\"&MID(F48,3,2)+2),VALUE(LEFT(F48,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G48,4)+1)&\"-\"&MID(G48,3,2)+2),VALUE(LEFT(G48,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H48,4)+1)&\"-\"&MID(H48,3,2)+2),VALUE(LEFT(H48,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I48,4)+1)&\"-\"&MID(I48,3,2)+2),VALUE(LEFT(I48,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J48,4)+1)&\"-\"&MID(J48,3,2)+2),VALUE(LEFT(J48,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K48,4)+1)&\"-\"&MID(K48,3,2)+2),VALUE(LEFT(K48,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L48,4)+1)&\"-\"&MID(L48,3,2)+2),VALUE(LEFT(L48,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M48,4)+1)&\"-\"&MID(M48,3,2)+2),VALUE(LEFT(M48,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N48,4)+1)&\"-\"&MID(N48,3,2)+2),VALUE(LEFT(N48,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O48,4)+1)&\"-\"&MID(O48,3,2)+2),VALUE(LEFT(O48,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P48,4)+1)&\"-\"&MID(P48,3,2)+2),VALUE(LEFT(P48,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q48,4)+1)&\"-\"&MID(Q48,3,2)+2),VALUE(LEFT(Q48,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R48,4)+1)&\"-\"&MID(R48,3,2)+2),VALUE(LEFT(R48,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S48,4)+1)&\"-\"&MID(S48,3,2)+2),VALUE(LEFT(S48,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T48,4)+1)&\"-\"&MID(T48,3,2)+2),VALUE(LEFT(T48,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U48,4)+1)&\"-\"&MID(U48,3,2)+2),VALUE(LEFT(U48,4)+1))","v":"2038-39"}]
[null,"Opex",61900.602133333341,103679.24393333335,176394.24393333335,271961.24393333338,345346.24393333332,387681.24393333332,427141.24393333332,564694.24393333332,739658.24393333332,866920.24393333332,935241.24393333332,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C49:C63)","v":61900.602133333341},{"$f":"SUM(D49:D63)","v":103679.24393333335},176394.24393333335,271961.24393333338,345346.24393333332,387681.24393333332,427141.24393333332,564694.24393333332,739658.24393333332,866920.24393333332,935241.24393333332,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C68,4)+1)&\"-\"&MID(C68,3,2)+2),VALUE(LEFT(C68,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D68,4)+1)&\"-\"&MID(D68,3,2)+2),VALUE(LEFT(D68,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E68,4)+1)&\"-\"&MID(E68,3,2)+2),VALUE(LEFT(E68,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F68,4)+1)&\"-\"&MID(F68,3,2)+2),VALUE(LEFT(F68,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G68,4)+1)&\"-\"&MID(G68,3,2)+2),VALUE(LEFT(G68,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H68,4)+1)&\"-\"&MID(H68,3,2)+2),VALUE(LEFT(H68,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I68,4)+1)&\"-\"&MID(I68,3,2)+2),VALUE(LEFT(I68,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J68,4)+1)&\"-\"&MID(J68,3,2)+2),VALUE(LEFT(J68,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K68,4)+1)&\"-\"&MID(K68,3,2)+2),VALUE(LEFT(K68,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L68,4)+1)&\"-\"&MID(L68,3,2)+2),VALUE(LEFT(L68,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M68,4)+1)&\"-\"&MID(M68,3,2)+2),VALUE(LEFT(M68,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N68,4)+1)&\"-\"&MID(N68,3,2)+2),VALUE(LEFT(N68,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O68,4)+1)&\"-\"&MID(O68,3,2)+2),VALUE(LEFT(O68,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P68,4)+1)&\"-\"&MID(P68,3,2)+2),VALUE(LEFT(P68,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q68,4)+1)&\"-\"&MID(Q68,3,2)+2),VALUE(LEFT(Q68,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R68,4)+1)&\"-\"&MID(R68,3,2)+2),VALUE(LEFT(R68,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S68,4)+1)&\"-\"&MID(S68,3,2)+2),VALUE(LEFT(S68,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T68,4)+1)&\"-\"&MID(T68,3,2)+2),VALUE(LEFT(T68,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U68,4)+1)&\"-\"&MID(U68,3,2)+2),VALUE(LEFT(U68,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C88,4)+1)&\"-\"&MID(C88,3,2)+2),VALUE(LEFT(C88,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D88,4)+1)&\"-\"&MID(D88,3,2)+2),VALUE(LEFT(D88,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E88,4)+1)&\"-\"&MID(E88,3,2)+2),VALUE(LEFT(E88,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F88,4)+1)&\"-\"&MID(F88,3,2)+2),VALUE(LEFT(F88,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G88,4)+1)&\"-\"&MID(G88,3,2)+2),VALUE(LEFT(G88,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H88,4)+1)&\"-\"&MID(H88,3,2)+2),VALUE(LEFT(H88,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I88,4)+1)&\"-\"&MID(I88,3,2)+2),VALUE(LEFT(I88,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J88,4)+1)&\"-\"&MID(J88,3,2)+2),VALUE(LEFT(J88,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K88,4)+1)&\"-\"&MID(K88,3,2)+2),VALUE(LEFT(K88,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L88,4)+1)&\"-\"&MID(L88,3,2)+2),VALUE(LEFT(L88,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M88,4)+1)&\"-\"&MID(M88,3,2)+2),VALUE(LEFT(M88,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N88,4)+1)&\"-\"&MID(N88,3,2)+2),VALUE(LEFT(N88,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O88,4)+1)&\"-\"&MID(O88,3,2)+2),VALUE(LEFT(O88,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P88,4)+1)&\"-\"&MID(P88,3,2)+2),VALUE(LEFT(P88,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q88,4)+1)&\"-\"&MID(Q88,3,2)+2),VALUE(LEFT(Q88,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R88,4)+1)&\"-\"&MID(R88,3,2)+2),VALUE(LEFT(R88,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S88,4)+1)&\"-\"&MID(S88,3,2)+2),VALUE(LEFT(S88,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T88,4)+1)&\"-\"&MID(T88,3,2)+2),VALUE(LEFT(T88,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U88,4)+1)&\"-\"&MID(U88,3,2)+2),VALUE(LEFT(U88,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C111,4)+1)&\"-\"&MID(C111,3,2)+2),VALUE(LEFT(C111,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D111,4)+1)&\"-\"&MID(D111,3,2)+2),VALUE(LEFT(D111,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E111,4)+1)&\"-\"&MID(E111,3,2)+2),VALUE(LEFT(E111,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F111,4)+1)&\"-\"&MID(F111,3,2)+2),VALUE(LEFT(F111,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G111,4)+1)&\"-\"&MID(G111,3,2)+2),VALUE(LEFT(G111,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H111,4)+1)&\"-\"&MID(H111,3,2)+2),VALUE(LEFT(H111,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I111,4)+1)&\"-\"&MID(I111,3,2)+2),VALUE(LEFT(I111,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J111,4)+1)&\"-\"&MID(J111,3,2)+2),VALUE(LEFT(J111,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K111,4)+1)&\"-\"&MID(K111,3,2)+2),VALUE(LEFT(K111,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L111,4)+1)&\"-\"&MID(L111,3,2)+2),VALUE(LEFT(L111,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M111,4)+1)&\"-\"&MID(M111,3,2)+2),VALUE(LEFT(M111,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N111,4)+1)&\"-\"&MID(N111,3,2)+2),VALUE(LEFT(N111,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O111,4)+1)&\"-\"&MID(O111,3,2)+2),VALUE(LEFT(O111,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P111,4)+1)&\"-\"&MID(P111,3,2)+2),VALUE(LEFT(P111,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q111,4)+1)&\"-\"&MID(Q111,3,2)+2),VALUE(LEFT(Q111,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R111,4)+1)&\"-\"&MID(R111,3,2)+2),VALUE(LEFT(R111,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S111,4)+1)&\"-\"&MID(S111,3,2)+2),VALUE(LEFT(S111,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T111,4)+1)&\"-\"&MID(T111,3,2)+2),VALUE(LEFT(T111,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U111,4)+1)&\"-\"&MID(U111,3,2)+2),VALUE(LEFT(U111,4)+1))","v":"2038-39"}]
[null,"Zone substation",{"$f":"SUM('5.4 MD & utilisation-Spatial'!F1135,'5.4 MD & utilisation-Spatial'!F1157,'5.4 MD & utilisation-Spatial'!F1179,'5.4 MD & utilisation-Spatial'!F1201,'5.4 MD & utilisation-Spatial'!F1223,'5.4 MD & utilisation-Spatial'!F1245,'5.4 MD & utilisation-Spatial'!F1267,'5.4 MD & utilisation-Spatial'!F1289,'5.4 MD & utilisation-Spatial'!F1311,'5.4 MD & utilisation-Spatial'!F1333,'5.4 MD & utilisation-Spatial'!F1355,'5.4 MD & utilisation-Spatial'!F1377,'5.4 MD & utilisation-Spatial'!F1399,'5.4 MD & utilisation-Spatial'!F1421,'5.4 MD & utilisation-Spatial'!F1443,'5.4 MD & utilisation-Spatial'!F1465,'5.4 MD & utilisation-Spatial'!F1487,'5.4 MD & utilisation-Spatial'!F1509,'5.4 MD & utilisation-Spatial'!F1531,'5.4 MD & utilisation-Spatial'!F1553,'5.4 MD & utilisation-Spatial'!F1575,'5.4 MD & utilisation-Spatial'!F1597,'5.4 MD & utilisation-Spatial'!F1619,'5.4 MD & utilisation-Spatial'!F1641,'5.4 MD & utilisation-Spatial'!F1663,'5.4 MD & utilisation-Spatial'!F1685,'5.4 MD & utilisation-Spatial'!F1707,'5.4 MD & utilisation-Spatial'!F1729,'5.4 MD & utilisation-Spatial'!F1751,'5.4 MD & utilisation-Spatial'!F1773,'5.4 MD & utilisation-Spatial'!F1795,'5.4 MD & utilisation-Spatial'!F1817,'5.4 MD & utilisation-Spatial'!F1839,'5.4 MD & utilisation-Spatial'!F1861,'5.4 MD & utilisation-Spatial'!F1883,'5.4 MD & utilisation-Spatial'!F1905,'5.4 MD & utilisation-Spatial'!F1927,'5.4 MD & utilisation-Spatial'!F1949,'5.4 MD & utilisation-Spatial'!F1971,'5.4 MD & utilisation-Spatial'!F1993,'5.4 MD & utilisation-Spatial'!F2015,'5.4 MD & utilisation-Spatial'!F2037,'5.4 MD & utilisation-Spatial'!F2059,'5.4 MD & utilisation-Spatial'!F2081,'5.4 MD & utilisation-Spatial'!F2103,'5.4 MD & utilisation-Spatial'!F2125,'5.4 MD & utilisation-Spatial'!F2147,'5.4 MD & utilisation-Spatial'!F2169,'5.4 MD & utilisation-Spatial'!F2191,'5.4 MD & utilisation-Spatial'!F2213,'5.4 MD & utilisation-Spatial'!F2235)","v":1962.4724966320512},{"$f":"SUM('5.4 MD & utilisation-Spatial'!G1135,'5.4 MD & utilisation-Spatial'!G1157,'5.4 MD & utilisation-Spatial'!G1179,'5.4 MD & utilisation-Spatial'!G1201,'5.4 MD & utilisation-Spatial'!G1223,'5.4 MD & utilisation-Spatial'!G1245,'5.4 MD & utilisation-Spatial'!G1267,'5.4 MD & utilisation-Spatial'!G1289,'5.4 MD & utilisation-Spatial'!G1311,'5.4 MD & utilisation-Spatial'!G1333,'5.4 MD & utilisation-Spatial'!G1355,'5.4 MD & utilisation-Spatial'!G1377,'5.4 MD & utilisation-Spatial'!G1399,'5.4 MD & utilisation-Spatial'!G1421,'5.4 MD & utilisation-Spatial'!G1443,'5.4 MD & utilisation-Spatial'!G1465,'5.4 MD & utilisation-Spatial'!G1487,'5.4 MD & utilisation-Spatial'!G1509,'5.4 MD & utilisation-Spatial'!G1531,'5.4 MD & utilisation-Spatial'!G1553,'5.4 MD & utilisation-Spatial'!G1575,'5.4 MD & utilisation-Spatial'!G1597,'5.4 MD & utilisation-Spatial'!G1619,'5.4 MD & utilisation-Spatial'!G1641,'5.4 MD & utilisation-Spatial'!G1663,'5.4 MD & utilisation-Spatial'!G1685,'5.4 MD & utilisation-Spatial'!G1707,'5.4 MD & utilisation-Spatial'!G1729,'5.4 MD & utilisation-Spatial'!G1751,'5.4 MD & utilisation-Spatial'!G1773,'5.4 MD & utilisation-Spatial'!G1795,'5.4 MD & utilisation-Spatial'!G1817,'5.4 MD & utilisation-Spatial'!G1839,'5.4 MD & utilisation-Spatial'!G1861,'5.4 MD & utilisation-Spatial'!G1883,'5.4 MD & utilisation-Spatial'!G1905,'5.4 MD & utilisation-Spatial'!G1927,'5.4 MD & utilisation-Spatial'!G1949,'5.4 MD & utilisation-Spatial'!G1971,'5.4 MD & utilisation-Spatial'!G1993,'5.4 MD & utilisation-Spatial'!G2015,'5.4 MD & utilisation-Spatial'!G2037,'5.4 MD & utilisation-Spatial'!G2059,'5.4 MD & utilisation-Spatial'!G2081,'5.4 MD & utilisation-Spatial'!G2103,'5.4 MD & utilisation-Spatial'!G2125,'5.4 MD & utilisation-Spatial'!G2147,'5.4 MD & utilisation-Spatial'!G2169,'5.4 MD & utilisation-Spatial'!G2191,'5.4 MD & utilisation-Spatial'!G2213,'5.4 MD & utilisation-Spatial'!G2235)","v":1989.3407220880847},{"$f":"SUM('5.4 MD & utilisation-Spatial'!H1135,'5.4 MD & utilisation-Spatial'!H1157,'5.4 MD & utilisation-Spatial'!H1179,'5.4 MD & utilisation-Spatial'!H1201,'5.4 MD & utilisation-Spatial'!H1223,'5.4 MD & utilisation-Spatial'!H1245,'5.4 MD & utilisation-Spatial'!H1267,'5.4 MD & utilisation-Spatial'!H1289,'5.4 MD & utilisation-Spatial'!H1311,'5.4 MD & utilisation-Spatial'!H1333,'5.4 MD & utilisation-Spatial'!H1355,'5.4 MD & utilisation-Spatial'!H1377,'5.4 MD & utilisation-Spatial'!H1399,'5.4 MD & utilisation-Spatial'!H1421,'5.4 MD & utilisation-Spatial'!H1443,'5.4 MD & utilisation-Spatial'!H1465,'5.4 MD & utilisation-Spatial'!H1487,'5.4 MD & utilisation-Spatial'!H1509,'5.4 MD & utilisation-Spatial'!H1531,'5.4 MD & utilisation-Spatial'!H1553,'5.4 MD & utilisation-Spatial'!H1575,'5.4 MD & utilisation-Spatial'!H1597,'5.4 MD & utilisation-Spatial'!H1619,'5.4 MD & utilisation-Spatial'!H1641,'5.4 MD & utilisation-Spatial'!H1663,'5.4 MD & utilisation-Spatial'!H1685,'5.4 MD & utilisation-Spatial'!H1707,'5.4 MD & utilisation-Spatial'!H1729,'5.4 MD & utilisation-Spatial'!H1751,'5.4 MD & utilisation-Spatial'!H1773,'5.4 MD & utilisation-Spatial'!H1795,'5.4 MD & utilisation-Spatial'!H1817,'5.4 MD & utilisation-Spatial'!H1839,'5.4 MD & utilisation-Spatial'!H1861,'5.4 MD & utilisation-Spatial'!H1883,'5.4 MD & utilisation-Spatial'!H1905,'5.4 MD & utilisation-Spatial'!H1927,'5.4 MD & utilisation-Spatial'!H1949,'5.4 MD & utilisation-Spatial'!H1971,'5.4 MD & utilisation-Spatial'!H1993,'5.4 MD & utilisation-Spatial'!H2015,'5.4 MD & utilisation-Spatial'!H2037,'5.4 MD & utilisation-Spatial'!H2059,'5.4 MD & utilisation-Spatial'!H2081,'5.4 MD & utilisation-Spatial'!H2103,'5.4 MD & utilisation-Spatial'!H2125,'5.4 MD & utilisation-Spatial'!H2147,'5.4 MD & utilisation-Spatial'!H2169,'5.4 MD & utilisation-Spatial'!H2191,'5.4 MD & utilisation-Spatial'!H2213,'5.4 MD & utilisation-Spatial'!H2235)","v":2016.4070366410076},{"$f":"SUM('5.4 MD & utilisation-Spatial'!I1135,'5.4 MD & utilisation-Spatial'!I1157,'5.4 MD & utilisation-Spatial'!I1179,'5.4 MD & utilisation-Spatial'!I1201,'5.4 MD & utilisation-Spatial'!I1223,'5.4 MD & utilisation-Spatial'!I1245,'5.4 MD & utilisation-Spatial'!I1267,'5.4 MD & utilisation-Spatial'!I1289,'5.4 MD & utilisation-Spatial'!I1311,'5.4 MD & utilisation-Spatial'!I1333,'5.4 MD & utilisation-Spatial'!I1355,'5.4 MD & utilisation-Spatial'!I1377,'5.4 MD & utilisation-Spatial'!I1399,'5.4 MD & utilisation-Spatial'!I1421,'5.4 MD & utilisation-Spatial'!I1443,'5.4 MD & utilisation-Spatial'!I1465,'5.4 MD & utilisation-Spatial'!I1487,'5.4 MD & utilisation-Spatial'!I1509,'5.4 MD & utilisation-Spatial'!I1531,'5.4 MD & utilisation-Spatial'!I1553,'5.4 MD & utilisation-Spatial'!I1575,'5.4 MD & utilisation-Spatial'!I1597,'5.4 MD & utilisation-Spatial'!I1619,'5.4 MD & utilisation-Spatial'!I1641,'5.4 MD & utilisation-Spatial'!I1663,'5.4 MD & utilisation-Spatial'!I1685,'5.4 MD & utilisation-Spatial'!I1707,'5.4 MD & utilisation-Spatial'!I1729,'5.4 MD & utilisation-Spatial'!I1751,'5.4 MD & utilisation-Spatial'!I1773,'5.4 MD & utilisation-Spatial'!I1795,'5.4 MD & utilisation-Spatial'!I1817,'5.4 MD & utilisation-Spatial'!I1839,'5.4 MD & utilisation-Spatial'!I1861,'5.4 MD & utilisation-Spatial'!I1883,'5.4 MD & utilisation-Spatial'!I1905,'5.4 MD & utilisation-Spatial'!I1927,'5.4 MD & utilisation-Spatial'!I1949,'5.4 MD & utilisation-Spatial'!I1971,'5.4 MD & utilisation-Spatial'!I1993,'5.4 MD & utilisation-Spatial'!I2015,'5.4 MD & utilisation-Spatial'!I2037,'5.4 MD & utilisation-Spatial'!I2059,'5.4 MD & utilisation-Spatial'!I2081,'5.4 MD & utilisation-Spatial'!I2103,'5.4 MD & utilisation-Spatial'!I2125,'5.4 MD & utilisation-Spatial'!I2147,'5.4 MD & utilisation-Spatial'!I2169,'5.4 MD & utilisation-Spatial'!I2191,'5.4 MD & utilisation-Spatial'!I2213,'5.4 MD & utilisation-Spatial'!I2235)","v":2043.3341248119743},{"$f":"SUM('5.4 MD & utilisation-Spatial'!J1135,'5.4 MD & utilisation-Spatial'!J1157,'5.4 MD & utilisation-Spatial'!J1179,'5.4 MD & utilisation-Spatial'!J1201,'5.4 MD & utilisation-Spatial'!J1223,'5.4 MD & utilisation-Spatial'!J1245,'5.4 MD & utilisation-Spatial'!J1267,'5.4 MD & utilisation-Spatial'!J1289,'5.4 MD & utilisation-Spatial'!J1311,'5.4 MD & utilisation-Spatial'!J1333,'5.4 MD & utilisation-Spatial'!J1355,'5.4 MD & utilisation-Spatial'!J1377,'5.4 MD & utilisation-Spatial'!J1399,'5.4 MD & utilisation-Spatial'!J1421,'5.4 MD & utilisation-Spatial'!J1443,'5.4 MD & utilisation-Spatial'!J1465,'5.4 MD & utilisation-Spatial'!J1487,'5.4 MD & utilisation-Spatial'!J1509,'5.4 MD & utilisation-Spatial'!J1531,'5.4 MD & utilisation-Spatial'!J1553,'5.4 MD & utilisation-Spatial'!J1575,'5.4 MD & utilisation-Spatial'!J1597,'5.4 MD & utilisation-Spatial'!J1619,'5.4 MD & utilisation-Spatial'!J1641,'5.4 MD & utilisation-Spatial'!J1663,'5.4 MD & utilisation-Spatial'!J1685,'5.4 MD & utilisation-Spatial'!J1707,'5.4 MD & utilisation-Spatial'!J1729,'5.4 MD & utilisation-Spatial'!J1751,'5.4 MD & utilisation-Spatial'!J1773,'5.4 MD & utilisation-Spatial'!J1795,'5.4 MD & utilisation-Spatial'!J1817,'5.4 MD & utilisation-Spatial'!J1839,'5.4 MD & utilisation-Spatial'!J1861,'5.4 MD & utilisation-Spatial'!J1883,'5.4 MD & utilisation-Spatial'!J1905,'5.4 MD & utilisation-Spatial'!J1927,'5.4 MD & utilisation-Spatial'!J1949,'5.4 MD & utilisation-Spatial'!J1971,'5.4 MD & utilisation-Spatial'!J1993,'5.4 MD & utilisation-Spatial'!J2015,'5.4 MD & utilisation-Spatial'!J2037,'5.4 MD & utilisation-Spatial'!J2059,'5.4 MD & utilisation-Spatial'!J2081,'5.4 MD & utilisation-Spatial'!J2103,'5.4 MD & utilisation-Spatial'!J2125,'5.4 MD & utilisation-Spatial'!J2147,'5.4 MD & utilisation-Spatial'!J2169,'5.4 MD & utilisation-Spatial'!J2191,'5.4 MD & utilisation-Spatial'!J2213,'5.4 MD & utilisation-Spatial'!J2235)","v":2070.6560729844423},{"$f":"SUM('5.4 MD & utilisation-Spatial'!K1135,'5.4 MD & utilisation-Spatial'!K1157,'5.4 MD & utilisation-Spatial'!K1179,'5.4 MD & utilisation-Spatial'!K1201,'5.4 MD & utilisation-Spatial'!K1223,'5.4 MD & utilisation-Spatial'!K1245,'5.4 MD & utilisation-Spatial'!K1267,'5.4 MD & utilisation-Spatial'!K1289,'5.4 MD & utilisation-Spatial'!K1311,'5.4 MD & utilisation-Spatial'!K1333,'5.4 MD & utilisation-Spatial'!K1355,'5.4 MD & utilisation-Spatial'!K1377,'5.4 MD & utilisation-Spatial'!K1399,'5.4 MD & utilisation-Spatial'!K1421,'5.4 MD & utilisation-Spatial'!K1443,'5.4 MD & utilisation-Spatial'!K1465,'5.4 MD & utilisation-Spatial'!K1487,'5.4 MD & utilisation-Spatial'!K1509,'5.4 MD & utilisation-Spatial'!K1531,'5.4 MD & utilisation-Spatial'!K1553,'5.4 MD & utilisation-Spatial'!K1575,'5.4 MD & utilisation-Spatial'!K1597,'5.4 MD & utilisation-Spatial'!K1619,'5.4 MD & utilisation-Spatial'!K1641,'5.4 MD & utilisation-Spatial'!K1663,'5.4 MD & utilisation-Spatial'!K1685,'5.4 MD & utilisation-Spatial'!K1707,'5.4 MD & utilisation-Spatial'!K1729,'5.4 MD & utilisation-Spatial'!K1751,'5.4 MD & utilisation-Spatial'!K1773,'5.4 MD & utilisation-Spatial'!K1795,'5.4 MD & utilisation-Spatial'!K1817,'5.4 MD & utilisation-Spatial'!K1839,'5.4 MD & utilisation-Spatial'!K1861,'5.4 MD & utilisation-Spatial'!K1883,'5.4 MD & utilisation-Spatial'!K1905,'5.4 MD & utilisation-Spatial'!K1927,'5.4 MD & utilisation-Spatial'!K1949,'5.4 MD & utilisation-Spatial'!K1971,'5.4 MD & utilisation-Spatial'!K1993,'5.4 MD & utilisation-Spatial'!K2015,'5.4 MD & utilisation-Spatial'!K2037,'5.4 MD & utilisation-Spatial'!K2059,'5.4 MD & utilisation-Spatial'!K2081,'5.4 MD & utilisation-Spatial'!K2103,'5.4 MD & utilisation-Spatial'!K2125,'5.4 MD & utilisation-Spatial'!K2147,'5.4 MD & utilisation-Spatial'!K2169,'5.4 MD & utilisation-Spatial'!K2191,'5.4 MD & utilisation-Spatial'!K2213,'5.4 MD & utilisation-Spatial'!K2235)","v":2098.1115322442556},{"$f":"SUM('5.4 MD & utilisation-Spatial'!L1135,'5.4 MD & utilisation-Spatial'!L1157,'5.4 MD & utilisation-Spatial'!L1179,'5.4 MD & utilisation-Spatial'!L1201,'5.4 MD & utilisation-Spatial'!L1223,'5.4 MD & utilisation-Spatial'!L1245,'5.4 MD & utilisation-Spatial'!L1267,'5.4 MD & utilisation-Spatial'!L1289,'5.4 MD & utilisation-Spatial'!L1311,'5.4 MD & utilisation-Spatial'!L1333,'5.4 MD & utilisation-Spatial'!L1355,'5.4 MD & utilisation-Spatial'!L1377,'5.4 MD & utilisation-Spatial'!L1399,'5.4 MD & utilisation-Spatial'!L1421,'5.4 MD & utilisation-Spatial'!L1443,'5.4 MD & utilisation-Spatial'!L1465,'5.4 MD & utilisation-Spatial'!L1487,'5.4 MD & utilisation-Spatial'!L1509,'5.4 MD & utilisation-Spatial'!L1531,'5.4 MD & utilisation-Spatial'!L1553,'5.4 MD & utilisation-Spatial'!L1575,'5.4 MD & utilisation-Spatial'!L1597,'5.4 MD & utilisation-Spatial'!L1619,'5.4 MD & utilisation-Spatial'!L1641,'5.4 MD & utilisation-Spatial'!L1663,'5.4 MD & utilisation-Spatial'!L1685,'5.4 MD & utilisation-Spatial'!L1707,'5.4 MD & utilisation-Spatial'!L1729,'5.4 MD & utilisation-Spatial'!L1751,'5.4 MD & utilisation-Spatial'!L1773,'5.4 MD & utilisation-Spatial'!L1795,'5.4 MD & utilisation-Spatial'!L1817,'5.4 MD & utilisation-Spatial'!L1839,'5.4 MD & utilisation-Spatial'!L1861,'5.4 MD & utilisation-Spatial'!L1883,'5.4 MD & utilisation-Spatial'!L1905,'5.4 MD & utilisation-Spatial'!L1927,'5.4 MD & utilisation-Spatial'!L1949,'5.4 MD & utilisation-Spatial'!L1971,'5.4 MD & utilisation-Spatial'!L1993,'5.4 MD & utilisation-Spatial'!L2015,'5.4 MD & utilisation-Spatial'!L2037,'5.4 MD & utilisation-Spatial'!L2059,'5.4 MD & utilisation-Spatial'!L2081,'5.4 MD & utilisation-Spatial'!L2103,'5.4 MD & utilisation-Spatial'!L2125,'5.4 MD & utilisation-Spatial'!L2147,'5.4 MD & utilisation-Spatial'!L2169,'5.4 MD & utilisation-Spatial'!L2191,'5.4 MD & utilisation-Spatial'!L2213,'5.4 MD & utilisation-Spatial'!L2235)","v":2125.2548256169894},2152.3177853011653,2178.8513270103831,2205.3356058747563,2231.9528373200997,0,0,0,0,0,0,0,0,0]
[]
[]
[null,"Note: These are in MW"]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"SUM(C112:C121)","v":1962.4724966320512},{"$f":"SUM(D112:D121)","v":1989.3407220880847},2016.4070366410076,2043.3341248119743,2070.6560729844423,2098.1115322442556,2125.2548256169894,2152.3177853011653,2178.8513270103831,2205.3356058747563,2231.9528373200997,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C126,4)+1)&\"-\"&MID(C126,3,2)+2),VALUE(LEFT(C126,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D126,4)+1)&\"-\"&MID(D126,3,2)+2),VALUE(LEFT(D126,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E126,4)+1)&\"-\"&MID(E126,3,2)+2),VALUE(LEFT(E126,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F126,4)+1)&\"-\"&MID(F126,3,2)+2),VALUE(LEFT(F126,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G126,4)+1)&\"-\"&MID(G126,3,2)+2),VALUE(LEFT(G126,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H126,4)+1)&\"-\"&MID(H126,3,2)+2),VALUE(LEFT(H126,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I126,4)+1)&\"-\"&MID(I126,3,2)+2),VALUE(LEFT(I126,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J126,4)+1)&\"-\"&MID(J126,3,2)+2),VALUE(LEFT(J126,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K126,4)+1)&\"-\"&MID(K126,3,2)+2),VALUE(LEFT(K126,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L126,4)+1)&\"-\"&MID(L126,3,2)+2),VALUE(LEFT(L126,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M126,4)+1)&\"-\"&MID(M126,3,2)+2),VALUE(LEFT(M126,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N126,4)+1)&\"-\"&MID(N126,3,2)+2),VALUE(LEFT(N126,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O126,4)+1)&\"-\"&MID(O126,3,2)+2),VALUE(LEFT(O126,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P126,4)+1)&\"-\"&MID(P126,3,2)+2),VALUE(LEFT(P126,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q126,4)+1)&\"-\"&MID(Q126,3,2)+2),VALUE(LEFT(Q126,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R126,4)+1)&\"-\"&MID(R126,3,2)+2),VALUE(LEFT(R126,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S126,4)+1)&\"-\"&MID(S126,3,2)+2),VALUE(LEFT(S126,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T126,4)+1)&\"-\"&MID(T126,3,2)+2),VALUE(LEFT(T126,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U126,4)+1)&\"-\"&MID(U126,3,2)+2),VALUE(LEFT(U126,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C141,4)+1)&\"-\"&MID(C141,3,2)+2),VALUE(LEFT(C141,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D141,4)+1)&\"-\"&MID(D141,3,2)+2),VALUE(LEFT(D141,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E141,4)+1)&\"-\"&MID(E141,3,2)+2),VALUE(LEFT(E141,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F141,4)+1)&\"-\"&MID(F141,3,2)+2),VALUE(LEFT(F141,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G141,4)+1)&\"-\"&MID(G141,3,2)+2),VALUE(LEFT(G141,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H141,4)+1)&\"-\"&MID(H141,3,2)+2),VALUE(LEFT(H141,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I141,4)+1)&\"-\"&MID(I141,3,2)+2),VALUE(LEFT(I141,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J141,4)+1)&\"-\"&MID(J141,3,2)+2),VALUE(LEFT(J141,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K141,4)+1)&\"-\"&MID(K141,3,2)+2),VALUE(LEFT(K141,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L141,4)+1)&\"-\"&MID(L141,3,2)+2),VALUE(LEFT(L141,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M141,4)+1)&\"-\"&MID(M141,3,2)+2),VALUE(LEFT(M141,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N141,4)+1)&\"-\"&MID(N141,3,2)+2),VALUE(LEFT(N141,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O141,4)+1)&\"-\"&MID(O141,3,2)+2),VALUE(LEFT(O141,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P141,4)+1)&\"-\"&MID(P141,3,2)+2),VALUE(LEFT(P141,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q141,4)+1)&\"-\"&MID(Q141,3,2)+2),VALUE(LEFT(Q141,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R141,4)+1)&\"-\"&MID(R141,3,2)+2),VALUE(LEFT(R141,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S141,4)+1)&\"-\"&MID(S141,3,2)+2),VALUE(LEFT(S141,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T141,4)+1)&\"-\"&MID(T141,3,2)+2),VALUE(LEFT(T141,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U141,4)+1)&\"-\"&MID(U141,3,2)+2),VALUE(LEFT(U141,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]

{"sheet":"8.2 Capex","index":39,"n_rows":61,"n_cols":5,"rows_kept":61,"cut":false,"hidden":false,"merged":[[8,2,8,3],[7,2,7,4]]}
[null,{"$f":"IF(dms_DataQuality=\"backcast\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))&\" BACKCAST\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"AusNet Electricity Services Pty Ltd"}]
[null,{"$f":"CONCATENATE(\"Annual Reporting RIN Response \",IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(CRY),CONCATENATE(FRCP_y1,\" to \",dms_MultiYear_FinalYear_Result)))","v":"Annual Reporting RIN Response 2021-22 to 2025-26"}]
[null,"8.2 - CAPEX"]
[]
[null,"8.2.7 - IMMEDIATE EXPENSING OF CAPEX"]
[null,"ESTIMATED - AS INCURRED"]
[null,null,"Estimate"]
[null,null,"CALENDAR YEARS",null,"6 MONTHS"]
[null,null,2019,2020,"1 January 2021 \nto \n30 June 2021"]
[null,"Subtransmission",29945141.311838422,29766073.591931444,14858804.015609318]
[null,"Distribution system assets",112666018.93479224,111533174.02901542,55613281.986701354]
[null,"SCADA/Network control",1726851.3226822596,1639573.2482068455,807975.50365250453]
[null,"Non-network general assets - IT",2415309.782106753,2267481.988392177,1113735.8338158808]
[null,"Non-network general assets - Other",769220.30417945143,722140.57085095148,354699.10452486284]
[null,"Land",0,0,0]
[null,"Non- Network Leasehold Land & Buildings - 1 Apr 2019 ",0,0,0]
[null,"Non- Network Leasehold Land & Buildings - CY20 ",0,0,0]
[null,"Non- Network Leasehold Land & Buildings - Jan-Jun 2021 ",0,0,0]
[null,"Non-network - Metering related IT ",0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",{"$f":"SUM(C11:C60)","v":147522541.65559915},{"$f":"SUM(D11:D60)","v":145928443.42839682},72748496.44430393]