{"text_format":"1","workbook":"xlsx","n_sheets":35,"sheets":["Cover page","Instructions","CONTENTS","Business & other details","2.1 Expenditure summary","2.2 Repex","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","5.4 MD & utilisation-Spatial","6.2 Reliability & Cust serv","7.1 Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.7 TSS-LRMC","7.8 Export Services","AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":723,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover page","index":0,"n_rows":34,"n_cols":2,"rows_kept":34,"cut":false,"hidden":false,"merged":[[26,1,26,2],[29,1,32,7]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2023-01-31"]
[]
[]
[null,"RIN.10: 2024-2029 - Reset RIN - workbook 1 - forecast data"]
[]
[]
[]
[null,"Ausgrid’s 2024-29 Regulatory Proposal"]

{"sheet":"Instructions","index":1,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[26,2,26,4],[10,2,10,4],[12,1,14,1],[12,2,12,4],[13,2,13,3],[14,2,14,4],[16,2,16,4],[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List)),\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by Ausgrid to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify confidential information\nin the confidential workbook. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selection as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return selection to NON-CONFIDENTIAL macro."]
[]
[null,"RESPONSES","\nPlease return two (2) files to the AER: \n\n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,"AMENDMENTS","\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]
[]
[null,"UNITS OF MEASURE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," PLEASE DO NOT ENTER TEXT into cells that are to contain numbers \n(including 'numbers stored as text')"]
[]
[]
[null,"NAVIGATION","\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]

{"sheet":"CONTENTS","index":2,"n_rows":43,"n_cols":5,"rows_kept":43,"cut":false,"hidden":false,"merged":[[6,3,6,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"TEMPLATE","FINAL RIN OCTOBER 2022"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 Forecast price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[null,null,null,null,"7.8 Export Services"]

{"sheet":"Business & other details","index":3,"n_rows":74,"n_cols":79,"rows_kept":74,"cut":false,"hidden":false,"merged":[[24,68,24,82],[25,37,25,40],[22,37,22,58],[23,37,23,58],[25,49,25,51],[24,60,24,66],[25,21,25,35],[0,7,2,15],[6,21,6,75],[24,21,24,35],[22,21,22,35],[16,21,16,35],[16,37,16,48],[15,21,15,35],[15,37,15,58],[24,37,24,51],[23,21,23,35],[3,21,3,57],[8,16,8,93],[22,68,22,89],[23,68,23,89],[22,60,22,66],[23,60,23,66],[46,73,46,80],[33,21,33,35],[33,60,33,66],[32,60,32,66],[46,37,46,44],[25,68,25,71],[25,80,25,82],[31,60,31,66],[32,37,32,58],[32,68,32,89],[33,68,33,89],[25,60,25,66],[31,21,31,35],[31,68,31,89],[42,37,42,44],[42,46,42,53],[42,55,42,62],[42,64,42,71],[41,25,41,34],[45,25,45,34],[51,37,51,44],[49,25,49,34],[47,73,47,80],[31,37,31,58],[41,46,41,53],[33,37,33,58],[43,37,43,44],[43,46,43,53],[43,55,43,62],[45,46,45,53],[45,37,45,44],[49,37,49,44],[49,73,49,80],[41,37,41,44],[45,55,45,62],[42,73,42,80],[32,21,32,35],[47,46,47,53],[47,37,47,44],[43,73,43,80],[41,73,41,80],[46,46,46,53],[45,73,45,80],[45,64,45,71],[49,46,49,53],[50,46,50,53],[49,64,49,71],[41,55,41,62],[41,64,41,71],[47,64,47,71],[49,55,49,62],[47,55,47,62],[46,64,46,71],[46,55,46,62],[43,64,43,71],[69,25,71,34],[50,73,50,80],[50,64,50,71],[53,25,53,34],[73,25,73,34],[73,37,73,52],[55,25,55,34],[63,25,63,34],[65,25,65,34],[55,37,55,44],[61,25,61,34],[61,37,61,52],[63,37,63,52],[65,37,65,52],[67,37,67,52],[69,37,71,81],[67,25,67,34],[51,64,51,71],[51,73,51,80],[51,55,51,62],[50,55,50,62],[53,37,53,44],[50,37,50,44],[51,46,51,53]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ausgrid"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":67505337385}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"570 George St"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 4009"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SYDNEY"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SYDNEY"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NSW"},null,null,null,null,null,null,null,null,null,"Post code",null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NSW"},null,null,null,null,null,null,null,null,null,"Post code"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2024-25",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2028-29"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2033-34"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2034-35"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2035-36"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2036-37"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2037-38"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2038-39"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2023-24"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2028-29"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2033-34"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2014-15"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2015-16"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2018-19"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2023-24"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2028-29"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2022-23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2028-29"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Regulatory proposal"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Public"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"dd/mm/yy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"2.1 Expenditure summary","index":4,"n_rows":111,"n_cols":9,"rows_kept":111,"cut":false,"hidden":false,"merged":[[7,1,8,1],[23,1,24,1],[37,1,38,1],[89,1,90,1],[102,1,103,1],[49,1,50,1],[61,1,62,1],[75,1,76,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX (including dual function assets)"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure",{"$f":"SUM('2.2 Repex'!D12:D182)","v":395566981.49172598},{"$f":"SUM('2.2 Repex'!E12:E182)","v":363892822.3634069},{"$f":"SUM('2.2 Repex'!F12:F182)","v":332589886.13017797},{"$f":"SUM('2.2 Repex'!G12:G182)","v":322525124.54208779},{"$f":"SUM('2.2 Repex'!H12:H182)","v":335465457.39884502},{"$f":"SUM('2.2 Repex'!I12:I182)","v":350191287.30961293},{"$f":"SUM('2.2 Repex'!J12:J182)","v":347145816.29996777}]
[null,"Connections",{"$f":"SUM('2.5 Connections'!E123:E136)","v":12928193.012},{"$f":"SUM('2.5 Connections'!F123:F136)","v":9153896.9830000009},{"$f":"SUM('2.5 Connections'!G123:G136)","v":14304769.071999999},{"$f":"SUM('2.5 Connections'!H123:H136)","v":11381958.975},{"$f":"SUM('2.5 Connections'!I123:I136)","v":11201084.748000002},{"$f":"SUM('2.5 Connections'!J123:J136)","v":12093701.290999999},{"$f":"SUM('2.5 Connections'!K123:K136)","v":11760673.915000001}]
[null,"Augmentation Expenditure",{"$f":"SUM('2.3 Augex (b)'!D47:D55)","v":23232705.040000003},{"$f":"SUM('2.3 Augex (b)'!E47:E55)","v":29096786.440000005},{"$f":"SUM('2.3 Augex (b)'!F47:F55)","v":45742254.350000001},{"$f":"SUM('2.3 Augex (b)'!G47:G55)","v":39583340.100000001},{"$f":"SUM('2.3 Augex (b)'!H47:H55)","v":40874874.730000004},{"$f":"SUM('2.3 Augex (b)'!I47:I55)","v":38798225.100000001},{"$f":"SUM('2.3 Augex (b)'!J47:J55)","v":36755837.630000003}]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E32:E50)","v":162807985},{"$f":"SUM('2.6 Non-network'!F32:F50)","v":187402595},{"$f":"SUM('2.6 Non-network'!G32:G50)","v":177633603},{"$f":"SUM('2.6 Non-network'!H32:H50)","v":148587561},{"$f":"SUM('2.6 Non-network'!I32:I50)","v":121945978},{"$f":"SUM('2.6 Non-network'!J32:J50)","v":86415668},{"$f":"SUM('2.6 Non-network'!K32:K50)","v":66757045}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C23:C25)","v":0},{"$f":"SUM('7.8 Export Services'!D23:D25)","v":0},{"$f":"SUM('7.8 Export Services'!E23:E25)","v":10191492.26},{"$f":"SUM('7.8 Export Services'!F23:F25)","v":9715388.8099999987},{"$f":"SUM('7.8 Export Services'!G23:G25)","v":5448028.96},{"$f":"SUM('7.8 Export Services'!H23:H25)","v":5250526.0199999996},{"$f":"SUM('7.8 Export Services'!I23:I25)","v":4980558.66}]
[null,"Public lighting"]
[null,"Metering"]
[null,"Capitalised network overheads",{"$f":"'2.10 Overheads'!D15","v":158403726},{"$f":"'2.10 Overheads'!E15","v":153329857},{"$f":"'2.10 Overheads'!F15","v":137923302},{"$f":"'2.10 Overheads'!G15","v":140390232},{"$f":"'2.10 Overheads'!H15","v":144593861},{"$f":"'2.10 Overheads'!I15","v":141358290},{"$f":"'2.10 Overheads'!J15","v":138536973}]
[null,"Capitalised corporate overheads",{"$f":"'2.10 Overheads'!D30","v":5819014},{"$f":"'2.10 Overheads'!E30","v":3529789},{"$f":"'2.10 Overheads'!F30","v":5007249},{"$f":"'2.10 Overheads'!G30","v":6531585},{"$f":"'2.10 Overheads'!H30","v":4071473},{"$f":"'2.10 Overheads'!I30","v":2650098},{"$f":"'2.10 Overheads'!J30","v":2514286}]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C10:C18)","v":758758604.54372597},746405746.78640687,723392555.81217802,678715190.42708778,663600757.83684504,636757795.720613,608451190.50496781]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"}]
[null,"Vegetation management",39645413.700199999,40880795.226199999]
[null,"Maintenance",45778424.371699996,45194210.349600002]
[null,"Emergency response",23306063.280499998,25877622.102400001,null," "]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E12:E30)","v":142429858.16},{"$f":"SUM('2.6 Non-network'!F12:F30)","v":144615024.50999999}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C13:C14)","v":0},{"$f":"SUM('7.8 Export Services'!D13:D14)","v":0}]
[null,"Metering",0,0]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D12","v":125056607.1573},{"$f":"'2.10 Overheads'!E12","v":122392471.23360001}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D27","v":32345733.370900001},{"$f":"'2.10 Overheads'!E27","v":31656657.981699999}]
[null,"Total",{"$f":"SUM(C26:C33)","v":408562100.04059994},{"$f":"SUM(D26:D33)","v":410616781.40350002}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Connections",20689980.91,18640639.690000001,11910787.810000001,11314183.59,10868549.33,10300063.789999999,10073584.210000001]
[null,"Metering",113710.3,193814.47,6079653.2699999996,5039795.7699999996,4004696.65,2816407.23,2149134.5699999998]
[null,"Public lighting",{"$f":"'4.1 Public lighting'!D14+'4.1 Public lighting'!D18","v":32875536},{"$f":"'4.1 Public lighting'!E14+'4.1 Public lighting'!E18","v":26822221},{"$f":"'4.1 Public lighting'!F14+'4.1 Public lighting'!F18","v":22918764},{"$f":"'4.1 Public lighting'!G14+'4.1 Public lighting'!G18","v":21311037},{"$f":"'4.1 Public lighting'!H14+'4.1 Public lighting'!H18","v":8028330},{"$f":"'4.1 Public lighting'!I14+'4.1 Public lighting'!I18","v":6496673},{"$f":"'4.1 Public lighting'!J14+'4.1 Public lighting'!J18","v":5306967}]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D16","v":12785353.789999999},{"$f":"'2.10 Overheads'!E16","v":11456299.24},{"$f":"'2.10 Overheads'!F16","v":9151111.0999999996},{"$f":"'2.10 Overheads'!G16","v":9142836.1199999992},{"$f":"'2.10 Overheads'!H16","v":6439058.0599999996},{"$f":"'2.10 Overheads'!I16","v":6391378.54},{"$f":"'2.10 Overheads'!J16","v":6368190.1399999997}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D31","v":448722.97},{"$f":"'2.10 Overheads'!E31","v":398461.93},{"$f":"'2.10 Overheads'!F31","v":326665.23},{"$f":"'2.10 Overheads'!G31","v":434490.28},{"$f":"'2.10 Overheads'!H31","v":259705.31},{"$f":"'2.10 Overheads'!I31","v":158684.21},{"$f":"'2.10 Overheads'!J31","v":148838.62}]
[null,"Total",{"$f":"SUM(C40:C45)","v":66913303.969999999},57511436.329999998,50386981.409999996,47242342.759999998,29600339.349999998,26163206.77,24046714.540000003]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Connections",31378119.739999998,27278941.57,29704415.809999999,30323214.460000001,29451474.25,29018649.239999998,29029678.879999999]
[null,"Metering",{"$f":"'3.2 Operating expenditure'!K71","v":36310020.689999998},{"$f":"'3.2 Operating expenditure'!L71","v":36108509.149999999},{"$f":"'3.2 Operating expenditure'!M71","v":43805897.549999997},{"$f":"'3.2 Operating expenditure'!N71","v":41347392.770000003},{"$f":"'3.2 Operating expenditure'!O71","v":37211283.380000003},{"$f":"'3.2 Operating expenditure'!P71","v":32631193.440000001},{"$f":"'3.2 Operating expenditure'!Q71","v":28061272.91}]
[null,"Public lighting",{"$f":"'3.2 Operating expenditure'!K73","v":13125924.720000001},{"$f":"'3.2 Operating expenditure'!L73","v":13829940.09},{"$f":"'3.2 Operating expenditure'!M73","v":10907530.140000001},{"$f":"'3.2 Operating expenditure'!N73","v":10434198.050000001},{"$f":"'3.2 Operating expenditure'!O73","v":10263379.52},{"$f":"'3.2 Operating expenditure'!P73","v":10270661.539999999},{"$f":"'3.2 Operating expenditure'!Q73","v":10295190.939999999}]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D13","v":18912019.940000001},{"$f":"'2.10 Overheads'!E13","v":16746081.67},{"$f":"'2.10 Overheads'!F13","v":19774852.859999999},{"$f":"'2.10 Overheads'!G13","v":19884908.690000001},{"$f":"'2.10 Overheads'!H13","v":19068311.949999999},{"$f":"'2.10 Overheads'!I13","v":18523250.989999998},{"$f":"'2.10 Overheads'!J13","v":18252570.280000001}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D28","v":15495549.300000001},{"$f":"'2.10 Overheads'!E28","v":13773596.460000001},{"$f":"'2.10 Overheads'!F28","v":12731381.699999999},{"$f":"'2.10 Overheads'!G28","v":12379211.77},{"$f":"'2.10 Overheads'!H28","v":11550036.869999999},{"$f":"'2.10 Overheads'!I28","v":10689383.439999999},{"$f":"'2.10 Overheads'!J28","v":9878211.6899999995}]
[null,"Total",{"$f":"SUM(C52:C57)","v":115221634.38999999},107737068.94,116924078.06,114368925.73999999,107544485.97000001,101133138.64999999,95516924.700000003]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure",47268164,51156238,26367258,19735422,21658472,35333635,32399470]
[null,"Connections",9162,170130,101432,50720,430357,939610,51674]
[null,"Augmentation expenditure",8280437,3721711,8172158,4817298,3735095,3622072,3320851]
[null,"Non-network",19732328,22713195,20085340,16855276,13440451,9499972,7313959]
[null,"Export services"]
[null,"Capitalised network overheads",8084584,9715449,4034513,3558186,3271433,3062794,3379044]
[null,"Capitalised corporate overheads",705264,427810,531140,700034,426796,268897,253643]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C64:C70)","v":84079939},87904533,59291841,45716936,42962604,52726980,46718641]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"}]
[null,"Vegetation management",1902979.8574000001,1962278.1712]
[null,"Maintenance",2197364.3695999999,2169322.0972000002]
[null,"Emergency response",1118691.0374,1242125.8611000001]
[null,"Non-network",6836633.1909999996,6941521.1775000002]
[null,"Export services",0,0]
[null,"Metering",0,0]
[null,"Network overheads",6002717.1430000002,5874838.6201999998]
[null,"Corporate overheads",1552595.2017000001,1519519.5833999999]
[null,"Total",{"$f":"SUM(C78:C85)","v":19610980.800099999},{"$f":"SUM(D78:D85)","v":19709605.510600001}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure"]
[null,"Connections",160058597,118969953,123681105,114757042,108775961,107479316,106136582]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total",{"$f":"SUM(C92:C98)","v":160058597},118969953,123681105,114757042,108775961,107479316,106136582]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure",139371203,132575407,113416786,115216606,119210222,116703286,114580906]
[null,"Connections",8613958,6449670,7819630,6444484,6336315,6710469,6683706]
[null,"Augmentation Expenditure",8586941,13163777,12755360,13861552,14764830,14299521,13824911]
[null,"Non-network",7650638,4670793,7023271,9375879,6717612,4735607,4486475]
[null,"Export services",null,null,1915503,2023297,1636356,1559505,1475260]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C105:C109)","v":164222740},156859647,142930550,146921818,148665335,144008388,141051258]

{"sheet":"2.2 Repex","index":5,"n_rows":523,"n_cols":10,"rows_kept":523,"cut":false,"hidden":false,"merged":[[474,1,481,1],[376,1,382,1],[383,1,388,1],[389,1,397,1],[398,1,405,1],[406,1,421,1],[422,1,450,1],[292,1,300,1],[301,1,308,1],[356,1,375,1],[451,1,464,1],[465,1,473,1],[309,1,349,1],[136,1,176,1],[225,1,232,1],[233,1,248,1],[249,1,277,1],[278,1,291,1],[482,1,522,1],[5,1,5,2],[11,1,29,1],[30,1,36,1],[37,1,42,1],[43,1,51,1],[52,1,59,1],[60,1,75,1],[76,1,104,1],[105,1,118,1],[119,1,127,1],[128,1,135,1],[183,1,202,1],[203,1,209,1],[210,1,215,1],[216,1,224,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.2 REPEX"]
[]
[null,"There are THREE sub-tables on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",27097128.960000001,20769242.219999999,15942390.02,16136094.689999999,16236887.380000001,16227702.73,16322837.789999999]
[null,null,"> 1 kV & < = 11 kV; Wood",9597736.6950000003,7510880.0829999996,6472135.392,6546287.2709999997,6584284.6710000001,6578922.9309999999,6614839.3990000002]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",1593541.004,1978067.9339999999,2550710.9010000001,2525378.648,2531390.6519999998,2523961.773,2538621.7459999998]
[null,null,"> 66 kV & < = 132 kV; Wood",284761.73680000001,401864.21220000001,531346.88639999996,537762.08929999999,541072.2206,540758.80980000005,543899.70920000004]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",112048.65300000001,61093.092519999998,76322.921270000006,255849.47260000001,524187.52889999998,325793.26669999998,110208.0882]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",70166.170310000001,53633.287190000003,40544.555529999998,41036.165309999997,41292.541709999998,41268.577310000001,41510.073640000002]
[null,null,"> 1 kV & < = 11 kV; Steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",11851031.6,15792613.33,1617741.9180000001,1632918.291,1641006.5549999999,1638184.15,1645317.2]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",5716564.2680000002,4846110.3099999996,5356100.693,5424566.7290000003,5459246.1940000001,5457858.0259999996,5491540.1689999998]
[null,null,"> 1 kV & < = 11 kV",2726361.42,2311221.84,2554448.023,2587101.0559999999,2603640.4920000001,2602978.443,2619042.2349999999]
[null,null,"˃ 11 kV & < = 22 kV",351788.57030000002,298222.17290000001,329606.19650000002,333819.49099999998,335953.61190000002,335868.1862,337940.93349999998]
[null,null,"> 22 kV & < = 66 kV",891987.03610000003,1314813.399,1646916.054,1664086.2860000001,1672053.754,1670270.067,1678246.7]
[null,null,"> 66 kV & < = 132 kV",599965.93669999996,642455.99820000003,999781.91850000003,1009699.274,1014325.5550000001,1013018.752,1017583.572]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",401493.5281,223412.0698,223861.91250000001,215864.16190000001,217152.84020000001,217091.61859999999,218382.57490000001]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",502912.24599999998,620901.35530000005,702839.35840000003,712818.43489999999,719022.69409999996,718866.50419999997,724120.08100000001]
[null,null,"> 1 kV & < = 11 kV",101199.5194,124942.11320000001,141430.2513,143438.31080000001,144686.7752,144655.3456,145712.50709999999]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",11415.79945,14094.07984,15954.02225,16180.541160000001,16321.374040000001,16317.82862,16437.081590000002]
[null,null,"> 66 kV & < = 132 kV",1542.6756009999999,1904.605384,2155.9489520000002,2186.559616,2205.5910859999999,2205.1119760000001,2221.2272419999999]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",3340938.0010000002,3129842.338,9386636.5510000009,10389541.49,13268418.5,12546940.880000001,12083235.449999999]
[null,null,"> 1 kV & < = 11 kV",5088107.5690000001,7541219.0389999999,13944105.630000001,16626210.59,18530500,17446704.41,16749517.85]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",1427872.4580000001,956435.10719999997,953428.38939999999,903664.13049999997,1036705.504,909223.83519999997,784828.04]
[null,null,"> 66 kV & < = 132 kV",235406.68780000001,139520.18400000001,203453.92230000001,59751.605369999997,15399.687400000001,66200.388850000003,99779.840899999996]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",19271275.27,22690621.77,28272572.32,28569381.98,28726589.59,28836802.93,29051915.719999999]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",53013509.210000001,43006143.990000002,35912113.920000002,35899931.57,35707386.399999999,35588477.259999998,33974660.399999999]
[null,null,"> 1 kV & < = 11 kV",24361375.469999999,18611917.359999999,16385621.390000001,16621554.189999999,17241576.989999998,15353150.99,13796206.300000001]
[null,null,"> 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",1794893.1359999999,1663943.1059999999,5802949.9220000003,5924588.0659999996,3714394.5860000001,1190272.973,361585.02230000001]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",17723683.879999999,35466500.950000003,16084577.529999999,5457654.9649999999,7642082.2149999999,39903516.509999998,49001442.799999997]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",7807595.0710000005,5432398.5,5891350.574,5648686.3130000001,5662717.2510000002,5611719.2989999996,5623014.8039999995]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",14235888.34,1488305.834,8376040.5329999998,8453958.3440000005,8498431.2569999993,8529598.9940000009,8575404.1199999992]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",1022298.519,106877.2678,601494.87219999998,607090.25619999995,610283.91669999994,612522.11430000002,615811.44270000001]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",177311.70680000001,175451.8474,155962.92670000001,156708.22020000001,157109.74220000001,157415.76939999999,157848.3216]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",228238.663,224530.41279999999,391399.51899999997,395709.95150000002,397288.61739999999,394102.42349999998,395483.978]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",46846.734830000001,46085.604299999999,80336.033729999996,81220.764129999996,81544.790470000007,80890.813739999998,81174.382320000004]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",410829.59330000001,404154.74300000002,704519.1287,712277.90720000002,715119.50569999998,709384.35690000001,711871.15480000002]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",1311708.575,1290396.92,2249408.9989999998,2274181.4509999999,2283254.1889999998,2264942.84,2272882.7599999998]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",522121.83439999999,322179.62310000003,386613.83970000001,390262.73369999998,391606.62469999999,388184.32819999999,389226.58110000001]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",73455.217640000003,49141.8,46327.032079999997,48887.458910000001,53299.244169999998,51603.684500000003,47185.733630000002]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",730745.13269999996,781797.81420000002,995110.47849999997,1005400.964,1009258.904,1000828.786,1004005.9350000001]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",1631904.6259999999,1764591.02,2139537.1549999998,2162256.665,2170859.4240000001,2152969.7790000001,2160138.1120000002]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",2079095.4920000001,1705613.274,1305871.912,1315164.176,1317683.2990000001,1305074.102,1306770.2139999999]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",6090871.2999999998,4996726.2120000003,3831029.8689999999,3874726.0040000002,3915335.0049999999,3868454.4079999998,3837922.9840000002]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",380679.45620000002,312295.38819999999,239103.3075,240804.70800000001,241265.9558,238957.2297,239267.78529999999]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",1112755.334,912863.4425,698917.36349999998,703890.68799999997,705238.95090000005,698490.36690000002,699398.14469999995]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",5440369.0159999998,4296282.5789999999,3285841.9989999998,3309222.2250000001,3341528.1230000001,3348309.0460000001,3456766.5950000002]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",477743.9387,391885.37170000002,299603.52360000001,301734.36739999999,302311.8566,299418.5062,299807.05820000003]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",748600.20050000004,798544.08070000005,1277723.1610000001,1289181.0330000001,1292834.0970000001,1281446.808,1284440.1599999999]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",4441261.9239999996,3656209.04,2291890.773,2050614.621,2057859.9720000001,2055593.5830000001,2062478.8389999999]
[null,null,"˂ = 11 kV  ; Switch",12022288.73,11255499.98,10521150.23,10124462.390000001,10364535.630000001,9877984.1390000004,9937535.9839999992]
[null,null,"˂ = 11 kV ;  Circuit Breaker",14918551.17,15126501.539999999,15707844.59,15889943.09,14601622.4,12099900.970000001,10820331.16]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",1446940.16,992382.68019999994,945097.46230000001,952403.77379999997,955904.71680000005,955041.98259999999,958452.79749999999]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",5197002.9989999998,3602356.824,8923028.2640000004,7837276.0700000003,9406190.0600000005,2772419.8760000002,120616.2582]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",22762.175729999999,208383.88759999999,402908.59669999999,72349.494409999999,38058.554479999999,52637.255440000001,91992.834489999994]
[null,null,"> 66 kV & < = 132 kV ; Switch",392973.81469999999,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",819252.35179999995,48211.783799999997,99635.637449999995,475346.14669999998,2652851.37,3468755.6690000002,4764689.4340000004]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",20487289.280000001,16573693.83,14580895.4,13231150.17,13259852.109999999,12007726.369999999,10272871.52]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",107144.6424,96467.818679999997,222635.7107,224123.49419999999,224688.5619,223837.71100000001,224367.1]
[null,null,"Master Station Assets",328006.6874,853026.35199999996,1027416.535,929081.00950000004,1006182.639,970718.19539999997,906362.85450000002]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",90398.662840000005,58994.149850000002,89054.213829999993,89649.326759999996,89875.353690000004,89535.013590000002,89746.769]
[null,null,"AFLC",141958.2616,90066.094840000005,127082.3202,139984.55009999999,164467.92989999999,156787.91649999999,131048.51300000001]
[null,null,"Other",46947372,53179918.700000003,25434840.059999999,19453610.010000002,20700693.43,22845872.52,21809150.25]
[null,"OTHER: ","DISTRIBUTION SUBSTATIONS - OTHER",4966932.5190000003,3745522.2609999999,6531085.6160000004,6576824.1330000004,6595193.3389999997,6570847.0889999997,6587737.4649999999]
[null,null,"DISTRIBUTION VOLTAGE REGULATION",0,0,0,0,0,0,0]
[null,null,"OVERHEAD CONDUCTORS - OTHER",11060615.779999999,6007367.2029999997,6854168.5049999999,6907409.2779999999,6930772.5619999999,6906891.8370000003,6927929.3339999998]
[null,null,"TOWERS - > = 33 KV ; REFURBISHMENT",410554.17959999997,508881.26260000002,96091.671310000005,96733.812690000006,96977.701270000005,96610.465989999997,96838.955249999999]
[null,null,"TRANSFORMERS - OTHER",1641670.835,1201846.7830000001,1600055.76,1493184.014,14956.164280000001,14899.528259999999,14934.7665]
[null,null,"UNDERGROUND CABLES - OTHER",492613.49209999997,421097.04560000001,478470.39850000001,482494.11379999999,483810.0048,451885.77840000001,354518.14179999998]
[null,null,"ZONE & SUBTRANSMISSION SUBSTATIONS - OTHER",8491156.0720000006,6043226.0800000001,5246986.7489999998,4869064.4170000004,4808078.7589999996,4826105.5360000003,4838140.9460000005]
[null,null,"DISTRIBUTION SUBSTATIONS - NOT AGE RELATED",5933840.3389999997,4995869.7560000001,3661839.9180000001,3158286.8530000001,3176922.8420000002,3169618.8420000002,3185924.1910000001]
[null,null,"OVERHEAD CONDUCTORS - NOT AGE RELATED",3716472.35,3175886.4109999998,1109770.2290000001,1117258.4539999999,1120125.6850000001,1115909.3259999999,1118592.4110000001]
[null,null,"ZONE & SUBTRANSMISSION SUBSTATIONS - NOT AGE RELATED",9164194.3330000006,7112161.3300000001,9704161.8289999999,9945583.5480000004,9826148.6099999994,9885775.8129999992,9747069.3210000005]
[null,null,"FIELD DEVICES - NOT AGE RELATED",1118236.392,936036.9253,584968.10160000005,591749.63139999995,594796.76520000002,593703.47160000005,596752.64919999999]
[null,null,"UNDERGROUND CABLES - NOT AGE RELATED",2439940.4419999998,2263586.3760000002,2310383.6290000002,2331351.7319999998,2337110.0090000001,2311484.7519999999,2315829.6639999999]
[null,null,"SWITCHGEAR - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"TRANSFORMERS - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"LAND (I.E. STRATEGIC SYSTEM PROPERTY)",0,0,829484.54619999998,0,0,0,0]
[null,null,"SUBSTATION BUILDINGS",6067716.1310000001,6066017.5149999997,5035039.5559999999,6327839.8770000003,7208250.8310000002,6436175.4189999998,6092951.4179999996]
[null,null,"SUPPORT COSTS (I.E. GIS DATA CAPTURE AND SWITCHING)"]
[null,null,"BALANCING ITEM (I.E. MULTI-NODE DISCREPANCY)"]
[null,null,"Switchgear - < = 11 KV ;  CIRCUIT BREAKER REFURBISHMENT",2069.5159250000002,1873.0525029999999,4309.4458759999998,4335.0530319999998,4346.0517490000002,4339.2764370000004,4350.1866060000002]
[null,null,"NETWORK RESILIENCE - OTHER",null,null,9063651.6079999991,13944285.189999999,17430430.690000001,15338903.02,13944549.76]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",1917.8,1594.6,1345.38,1345.38,1345.38,1345.38,1345.38]
[null,null,"> 1 kV & < = 11 kV; Wood",688,598.9,548.11,548.11,548.11,548.11,548.11]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",58.2,57.1,74.400000000000006,74.36,73.400000000000006,72.8,72.8]
[null,null,"> 66 kV & < = 132 kV; Wood",12.3,12.1,15.6,15.6,15.6,15.6,15.6]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",3.5,2.1,2.2599999999999998,7.7,15.7,9.6199999999999992,3.22]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",5,4.2,3.51,3.51,3.51,3.51,3.51]
[null,null,"> 1 kV & < = 11 kV; Steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",33,40,6.3,6.3,6.3,6.3,6.3]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",1272.0999999999999,1300,1300,1300,1300,1300,1300]
[null,null,"> 1 kV & < = 11 kV",606.70000000000005,620,620,620,620,620,620]
[null,null,"˃ 11 kV & < = 22 kV",78.3,80,80,80,80,80,80]
[null,null,"> 22 kV & < = 66 kV",143.80000000000001,145.69999999999999,157,157,157,157,157]
[null,null,"> 66 kV & < = 132 kV",43.8,48.4,45.5,45.5,45.5,45.5,45.5]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",40,22,21,20,20,20,20]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",501.2,661,660.96,660.96,660.96,660.96,660.96]
[null,null,"> 1 kV & < = 11 kV",100.9,133,133,133,133,133,133]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",11.4,15,15,15,15,15,15]
[null,null,"> 66 kV & < = 132 kV",1.5,2,2.0299999999999998,2.0299999999999998,2.0299999999999998,2.0299999999999998,2.0299999999999998]
[null,null,"> 132 kV"]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",181.2,157.4,597.41,589.45000000000005,602.46,602.13,602.19000000000005]
[null,null,"> 1 kV & < = 11 kV",145.5,186.8,195.59,195.59,195.59,195.59,195.59]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",3.3,3.7,3.78,4.05,4.4000000000000004,4.07,3.75]
[null,null,"> 66 kV & < = 132 kV",0.1,0.4,0.03,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",584.29999999999995,636.9,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",88.5,78.900000000000006,58.96,58.8,57.73,57.73,56.68]
[null,null,"> 1 kV & < = 11 kV",48.5,42.3,47.25,46.56,46.56,46.19,46.02]
[null,null,"> 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",6.1,4.4000000000000004,14.23,11.19,8.02,4.54,0.37]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",6.1,29.5,18.14,5.44,6.82,41.81,23.33]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",319.5,234.3,299.11,295.11,295.11,295.11,295.11]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",23819.1,448.7,12175.65,12175.65,12175.65,12175.65,12175.65]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",1710.5,32.200000000000003,874.35,874.35,874.35,874.35,874.35]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",24.6,22.5,17.5,17.5,17.5,17.5,17.5]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",8.1,11.3,16.2,16.2,16.2,16.2,16.2]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",1.1000000000000001,1.5,2.16,2.16,2.16,2.16,2.16]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",14.7,20.399999999999999,29.16,29.16,29.16,29.16,29.16]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",30.4,42.2,60.48,60.48,60.48,60.48,60.48]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",10,6.8,7.63,7.63,7.63,7.63,7.63]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0.9,0.9,0.87,0.87,0.87,0.87,0.87]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",7.1,7,7.46,7.46,7.46,7.46,7.46]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",15.9,13.2,13.54,13.54,13.54,13.54,13.54]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",2.2999999999999998,1.5,1.22,1.22,1.22,1.22,1.22]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",11.6,5.5,4.6900000000000004,4.75,5.17,4.7699999999999996,3.97]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0.4,0.3,0.22,0.22,0.22,0.22,0.22]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",1.2,0.8,0.65,0.65,0.65,0.65,0.65]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",7.9,4.8,3.44,3.06,3.06,3.06,3.06]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0.5,0.4,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",6.5,8.1,12.5,12.5,12.5,12.5,12.5]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",944.9,990.3,464.5,391.5,391.5,391.5,391.5]
[null,null,"˂ = 11 kV  ; Switch",504.2,431.7,404,371,374,363,363]
[null,null,"˂ = 11 kV ;  Circuit Breaker",191.4,152,177.7,151.9,155.11000000000001,144.44,136.21]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",26.3,17.7,13.5,13.5,13.5,13.5,13.5]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",7,7.1,27.52,10.24,9.9700000000000006,1.42,1]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",0.1,0.1,0,0,0.01,0.03,7.0000000000000007E-2]
[null,null,"> 66 kV & < = 132 kV ; Switch",2,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",9.4,3.1,1.53,0.66,1.54,2.5,3.7]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",5143.8,3777.1,970.54,870.42,961.67,870.34,729.67]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",2.4,2,0,0,0,0,0]
[null,null,"Master Station Assets",0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",0,0,0,0,0,0,0]
[null,null,"AFLC",5.0999999999999996,1.4,0.87,1.01,1.7,1.4,0.8]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"DISTRIBUTION SUBSTATIONS - OTHER",853,423.8,2266,2266,2266,2266,2266]
[null,null,"DISTRIBUTION VOLTAGE REGULATION",0,0,0,0,0,0,0]
[null,null,"OVERHEAD CONDUCTORS - OTHER",220.2,154.9,135.37,135.37,135.37,135.37,135.37]
[null,null,"TOWERS - > = 33 kV TOWER REFURBISHMENT",6,4,0,0,0,0,0]
[null,null,"TRANSFORMERS - OTHER",10,8,8,10,0,0,0]
[null,null,"UNDERGROUND CABLES - OTHER",120.1,200.9,201.5,202.5,202.5,155.5,2.5]
[null,null,"ZONE & SUBTRANSMISION SUBSTATIONS - OTHER",125.1,85.5,454.62,459.17,472.4,469.8,455.6]
[null,null,"DISTRIBUTION SUBSTATIONS - NOT AGE RELATED",781.5,221.2,157,135,135,135,135]
[null,null,"OVERHEAD CONDUCTORS - NOT AGE RELATED",280.10000000000002,151.80000000000001,146.27000000000001,146.27000000000001,146.27000000000001,146.27000000000001,146.27000000000001]
[null,null,"ZONE & SUBTRANSMISSION SUBSTATIONS - NOT AGE RELATED",233.9,171.4,370.01,358.02,358.5,363.5,363]
[null,null,"FIELD DEVICES - NOT AGE RELATED",11,9,5,5,5,5,5]
[null,null,"UNDERGROUND CABLES - NOT AGE RELATED",162.9,129.5,93.52,93.52,93.52,93.52,93.52]
[null,null,"SWITCHGEAR - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"TRANSFORMERS - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"LAND (I.E. STRATEGIC SYSTEM PROPERTY)",0,0,0,0,0,0,0]
[null,null,"SUBSTATION BUILDINGS",69.599999999999994,57.7,147.75,147.68,147.97,147.93,147.80000000000001]
[null,null,"SUPPORT COSTS (I.E. GIS DATA CAPTURE AND SWITCHING)",0,0,0,0,0,0,0]
[null,null,"BALANCING ITEM (I.E. MULTI-NODE DISCREPANCY)",0,0,0,0,0,0,0]
[null,null,"Switchgear - < = 11 KV ;  CIRCUIT BREAKER REFURBISHMENT",0.1,0.1,0,0,0,0,0]
[null,null,"NETWORK RESILIENCE - OTHER",0,0,0,0,0,0,0]
[]
[]
[null,null,{"$f":"IF(ISBLANK(C159),\"\",C159)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",414,442,472,503,536,570,606]
[null,null,"> 1 kV & < = 11 kV; Wood",137,147,157,167,178,189,201]
[null,null,"˃ 11 kV & < = 22 kV; Wood",2,2,2,3,3,3,3]
[null,null,"> 22 kV & < = 66 kV; Wood",24,25,27,29,30,32,34]
[null,null,"> 66 kV & < = 132 kV; Wood",4,4,4,5,5,5,6]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,1,1,1,1]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",1,1,1,1,1,1,1]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",8,9,9,10,10,11,11]
[null,null,"> 1 kV & < = 11 kV; Steel",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",386,406,427,449,472,496,520]
[null,null,"> 1 kV & < = 11 kV",185,195,205,216,227,238,250]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",35,37,39,41,43,45,47]
[null,null,"> 66 kV & < = 132 kV",4,4,4,5,5,5,5]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",1479,1559,1644,1731,1823,1918,2017]
[null,null,"> 1 kV & < = 11 kV",365,382,398,416,433,452,471]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",0,0,0,0,0,1,1]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",65,69,74,80,85,91,97]
[null,null,"> 66 kV & < = 132 kV",8,8,9,9,10,11,11]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",310,350,393,438,468,486,505]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",434,460,487,516,546,578,611]
[null,null,"> 1 kV & < = 11 kV",277,284,291,298,306,313,321]
[null,null,"> 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",13,14,15,16,18,20,21]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",3,3,4,4,4,5,5]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",305,318,332,346,360,375,390]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",7307,7604,7911,8226,8551,8884,9226]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",178,185,193,200,208,217,225]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",13,13,14,15,15,16,17]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",3,3,3,3,3,3,3]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",21,23,24,25,26,28,29]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",76,80,84,88,93,97,102]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",14,14,15,16,17,18,18]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",4,4,5,5,5,5,6]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",10,11,12,12,13,14,15]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",20,21,22,24,25,26,28]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",7,7,8,8,9,9,9]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",39,41,43,46,48,51,54]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",2,2,2,2,2,3,3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",5,6,6,6,7,7,7]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",33,35,37,39,42,44,47]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",9,9,10,10,11,12,12]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",19,21,22,23,25,26,27]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",208,218,228,238,248,259,270]
[null,null,"˂ = 11 kV  ; Switch",480,502,524,548,572,596,621]
[null,null,"˂ = 11 kV ;  Circuit Breaker",125,130,136,142,148,155,161]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,1,1,1,1]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",1,1,1,1,1,1,1]
[null,null,"> 22 kV & < = 33 kV ; Switch",11,12,12,12,13,13,14]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",36,39,41,44,46,49,52]
[null,null,"> 33 kV & < = 66 kV ; Switch",2,2,2,2,2,2,2]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",2,2,2,3,3,3,3]
[null,null,"> 66 kV & < = 132 kV ; Switch",13,14,14,15,15,16,16]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",20,21,22,24,25,27,28]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",380,406,433,462,492,523,556]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",101,108,115,122,130,139,147]
[null,null,"Master Station Assets",0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",21,22,24,26,28,30,32]
[null,null,"Communications Linear Assets",89,95,102,109,116,123,131]
[null,null,"AFLC",73,77,81,86,90,94,98]
[null,null,"Other",35,42,50,60,72,86,103]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"DISTRIBUTION SUBSTATIONS - OTHER",156,164,173,181,190,200,209]
[null,null,"DISTRIBUTION VOLTAGE REGULATION",8,10,11,13,14,16,18]
[null,null,"OVERHEAD CONDUCTORS - OTHER",0,0,0,0,0,0,0]
[null,null,"TOWERS - > = 33 kV TOWER REFURBISHMENT",0,0,0,0,0,0,0]
[null,null,"TRANSFORMERS - OTHER",0,0,0,0,0,0,0]
[null,null,"UNDERGROUND CABLES - OTHER",0,0,0,0,0,0,0]
[null,null,"ZONE & SUBTRANSMISION SUBSTATIONS - OTHER",24,25,26,27,27,28,29]
[null,null,"DISTRIBUTION SUBSTATIONS - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"OVERHEAD CONDUCTORS - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"ZONE & SUBTRANSMISSION SUBSTATIONS - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"FIELD DEVICES - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"UNDERGROUND CABLES - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"SWITCHGEAR - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"TRANSFORMERS - NOT AGE RELATED",0,0,0,0,0,0,0]
[null,null,"LAND (I.E. STRATEGIC SYSTEM PROPERTY)",0,0,0,0,0,0,0]
[null,null,"SUBSTATION BUILDINGS",0,0,0,0,0,0,0]
[null,null,"SUPPORT COSTS (I.E. GIS DATA CAPTURE AND SWITCHING)",0,0,0,0,0,0,0]
[null,null,"BALANCING ITEM (I.E. MULTI-NODE DISCREPANCY)",0,0,0,0,0,0,0]
[null,null,"Switchgear - < = 11 KV ;  CIRCUIT BREAKER REFURBISHMENT",0,0,0,0,0,0,0]
[null,null,"NETWORK RESILIENCE - OTHER"]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]

{"sheet":"2.3 Augex (b)","index":6,"n_rows":78,"n_cols":10,"rows_kept":78,"cut":false,"hidden":false,"merged":[[67,1,68,2],[59,1,60,2],[44,1,45,2],[5,1,5,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,null,null,"VOLUMES (0's)"]
[null,"PROJECT TYPE","UNITS",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0.626,5.3,3.8420000000000001,3.7869999999999999,3.8279999999999998,3.8279999999999998,3.8279999999999998]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",1.1859999999999999,10.052,8.6489999999999991,8.5259999999999998,8.6180000000000003,8.6180000000000003,8.6180000000000003]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",1.2999999999999999E-2,0.03,3.5000000000000003E-2,3.5000000000000003E-2,3.5000000000000003E-2,3.5000000000000003E-2,3.5000000000000003E-2]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",11.832000000000001,27.594000000000001,32.779000000000003,32.779000000000003,32.779000000000003,32.779000000000003,32.779000000000003]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",0.56699999999999995,1.48,1.746,1.746,1.746,1.746,1.746]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0.36899999999999999,0.86199999999999999,1.0229999999999999,1.0229999999999999,1.0229999999999999,1.0229999999999999,1.0229999999999999]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",2.0030000000000001,16.971,12.302,12.125999999999999,12.257999999999999,12.257999999999999,12.257999999999999]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0.443,1.048,1.2430000000000001,1.2430000000000001,1.2430000000000001,1.2430000000000001,1.2430000000000001]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.09,0.21,0.25,0.25,0.25,0.25,0.25]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",2.39,8.1530000000000005,9.4920000000000009,9.4920000000000009,9.4920000000000009,9.4920000000000009,9.4920000000000009]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",2.0419999999999998,7.8849999999999998,9.0060000000000002,9.0060000000000002,9.0060000000000002,9.0060000000000002,9.0060000000000002]
[null,"Distribution Substation Augmentations - Indoor","Number",0.1,0.40699999999999997,0.47,0.47,0.47,0.47,0.47]
[]
[null,"COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,"PROJECT TYPE",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,2738456.69,6213026.29,9803115.5199999996,10055929.189999999,10538096.75,10306106.279999999,10740104.99]
[null,"HV Feeder Augmentations - Underground Cables",null,3019517.79,9251594.8499999996,11312862.460000001,9051551.5,8945424.0199999996,8974598.1999999993,8962582.3599999994]
[null,"HV Feeder Non-Material Projects",null,0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines",null,2219991.12,3012052.53,4635148.6100000003,3754216.68,3669400,3681478.39,3674265.4]
[null,"LV Feeder Augmentations - Underground Cables",null,2073350.59,1982688.08,4713359.46,4774098.22,5225652.87,4937912.5999999996,4835870.5599999996]
[null,"LV Feeder Non-Material Projects",null,0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted",null,921357.35,1272016.54,1774051.71,1671459.56,1504078.39,1466565.45,1432721.34]
[null,"Distribution Substation Augmentations - Ground Mounted",null,5011145.76,3817566.67,3706872.49,4719713.8499999996,4622510.25,4409577.99,4587231.2]
[null,"Distribution Substation Augmentations - Indoor",null,139816.17000000001,112886.64,46435.25,37553.65,36667.660000000003,36769.06,36664.26]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,4644722.58,3279200.05,9127145.3499999996,5187823.83,5842732.1699999999,4649324.13,2429179.33]
[null,"Subtransmission Lines",null,2464346.9900000002,155754.79999999999,623263.51,330993.61,490312.63,335893,57218.2]
[null,"HV Feeders",null,5757974.4800000004,15464621.140000001,21115977.98,19107480.690000001,19483520.760000002,19280704.48,19702687.350000001]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,6072319.2800000003,5202469.8499999996,5527359.4500000002,6428727.0700000003,6163256.2999999998,5912912.5,6056616.79]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,4293341.71,4994740.5999999996,9348508.0600000005,8528314.9000000004,8895052.8699999992,8619390.9900000002,8510135.9600000009]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,0,0,277313.63,897645.47,2193579.73,1814692.66,384038.81]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,23232705.030000001,29096786.43,45464940.729999997,38685694.630000003,38681295.009999998,36983532.450000003,36371798.82]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,0,0,236168.33,764265.9,1867194.65,1544577.61,326820.61]
[null,"Subtransmission Lines",null,0,0,41145.300000000003,133379.57,326385.08,270115.05,57218.2]
[null,"HV Feeders",null,0,0,0,0,0,0,0]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,0,0,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]

{"sheet":"2.5 Connections","index":7,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[138,1,139,1],[138,2,139,3],[102,1,103,1],[102,2,103,2],[102,3,103,3],[120,1,121,1],[120,2,121,3],[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,10,3],[54,1,55,1],[54,2,55,2],[54,3,55,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Underground connections","0's",9062.8619999999992,8879.3389999999999,8737.3340000000007,8368.6039999999994,8266.1229999999996,8299.9480000000003,8585.6219999999994]
[null,null,"Overhead connections","0's",5166.1589999999997,5062.1019999999999,4980.576,4770.3630000000003,4711.9390000000003,4731.2219999999998,4894.085]
[null,null,"Distribution substations installed","MVA added",12.94,12.68,12.476000000000001,11.949,11.803000000000001,11.851000000000001,12.259]
[null,null,"Distribution substations installed","0's",31.356000000000002,30.724,30.23,28.954000000000001,28.599,28.716000000000001,29.704999999999998]
[null,null,"Distribution substations installed ","total spend $0s",2687855.5660000001,2594222.568,2495374.9,2392672.057,2364447.287,2373700.696,2457198.594]
[null,null,"Augmentation HV ","net circuit KM added",5.2999999999999999E-2,5.0999999999999997E-2,4.9000000000000002E-2,4.7E-2,4.7E-2,4.7E-2,4.9000000000000002E-2]
[null,null,"Augmentation HV","total spend $0s",14955.324000000001,14431.921,13873.808999999999,13288.244000000001,13125.498,13179.215,13632.883]
[null,null,"Augmentation LV","net circuit KM added",86.192999999999998,83.176000000000002,79.959999999999994,76.584999999999994,75.647000000000006,75.956999999999994,78.570999999999998]
[null,null,"Augmentation LV","total spend $0s",22378346.34,21603521.739,20796403.763999999,19968914.989999998,19745059.942000002,19817744.572999999,20534250.669]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",0,0,0,0,0,0,0]
[null,null,"Volume of GSL breaches for residential customers","0's",0,0,0,0,0,0,0]
[null,null,"Volume of customer complaints relating to connection services","0's",0,0,0,0,0,0,0]
[null,null,"GSL payments","$0's",0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",628.86500000000001,608.94000000000005,693.91,654.92499999999995,656.68700000000001,677.69600000000003,685.70500000000004]
[null,null,"Overhead connections","0's",222.804,210.791,252.18600000000001,239.01400000000001,241.07,247.161,252.971]
[null,null,"Distribution substations installed","MVA added",242.70599999999999,246.66399999999999,249.44399999999999,237.14500000000001,239.25,245.40899999999999,251.00800000000001]
[null,null,"Distribution substations installed","0's",252.66800000000001,256.78899999999999,259.68299999999999,246.88,249.07,255.482,261.31099999999998]
[null,null,"Distribution substations installed ","total spend $0s",36501304.237999998,36562317.053000003,36307312.564000003,34890570.159000002,35320660.645999998,36137051.719999999,37228599.916000001]
[null,null,"Augmentation HV ","net circuit KM added",191.761,52.225000000000001,78.721999999999994,63.420999999999999,42.850999999999999,33.22,18.361000000000001]
[null,null,"Augmentation HV","total spend $0s",61439623.478,18365456.226,29964204.188999999,20904981.346999999,14184576.625,12681183.790999999,6435288.1119999997]
[null,null,"Augmentation LV","net circuit KM added",54.44,53.948,54.387,51.734000000000002,52.207999999999998,53.561999999999998,54.802]
[null,null,"Augmentation LV","total spend $0s",17710843.011,17856859.317000002,18478663.41,19289809.377,20016716.783,20103680.405999999,21794424.530000001]
[null,"SUBDIVISION","Underground connections","0's",104.88,102.768,101.113,96.844999999999999,95.659000000000006,96.05,99.356999999999999]
[null,null,"Overhead connections","0's",2.1619999999999999,2.1190000000000002,2.085,1.9970000000000001,1.972,1.98,2.0489999999999999]
[null,null,"Distribution substations installed","MVA added",23.94,23.457999999999998,23.08,22.106000000000002,21.835000000000001,21.925000000000001,22.678999999999998]
[null,null,"Distribution substations installed","0's",41.087000000000003,40.26,39.610999999999997,37.939,37.475000000000001,37.628,38.923000000000002]
[null,null,"Distribution substations installed ","total spend $0s",11850185.664999999,11435455.606000001,10993223.221000001,10529237.289999999,10400282.585999999,10442846.245999999,10802319.884]
[null,null,"Augmentation HV ","net circuit KM added",62.914000000000001,60.713000000000001,58.365000000000002,55.901000000000003,55.216999999999999,55.442999999999998,57.350999999999999]
[null,null,"Augmentation HV","total spend $0s",17643895.27,17026398.302000001,16367952.763,15677118.086999999,15485115.754000001,15548489.34,16083714.306]
[null,null,"Augmentation LV","net circuit KM added",10.574,10.204000000000001,9.8089999999999993,9.3949999999999996,9.2799999999999994,9.3179999999999996,9.6389999999999993]
[null,null,"Augmentation LV","total spend $0s",2729999.9440000001,2634456.037,2532576.2510000002,2425684.966,2395976.88,2405782.5320000001,2488596.6779999998]
[null,null,"Cost per lot","$0's",0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",29781.062999999998,30731.252,36289.659,46724.65,51083.834000000003,49358.682999999997,59230.082000000002]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Underground connections","0's",1,0,1,1,1,1,1]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",6516.09,6723.991,7940.1689999999999,10223.343000000001,11177.130999999999,10799.668,12959.528]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",125069.429,129059.871,152403.12100000001,196226.215,214533.174,207288.179,248744.39499999999]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",0,0,0,0,0,0,0]
[null,null,"Volume of GSL breaches for residential customers","0's",0,0,0,0,0,0,0]
[null,null,"Volume of customer complaints relating to connection services","0's",0,0,0,0,0,0,0]
[null,null,"GSL payments","$0's",0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",193,162,242,228,227,235,237]
[null,null,"Overhead connections","0's",101,85,126,120,121,124,127]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",909524.95600000001,938544.08499999996,1108299.9469999999,1426988.5209999999,1560119.6610000001,1507432.892,1808909.149]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",7661593.3049999997,3719262.1540000001,7887163.7740000002,3118989.0830000001,2167219.6540000001,3364918.67,1286194.537]
[null,null,"Augmentation LV","net circuit KM added",2.0920000000000001,1.5529999999999999,2.6160000000000001,2.516,2.5539999999999998,2.63,2.7080000000000002]
[null,null,"Augmentation LV","total spend $0s",4195708.1679999996,4329575.6310000001,5112672.4019999998,6582807.1629999997,7196951.2929999996,6953903.1979999999,8344636.2240000004]
[null,"SUBDIVISION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Cost per lot","$0's",0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",29781.062999999998,30731.252,36289.659,46724.65,51083.834000000003,49358.682999999997,59230.082000000002]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,19996663.671999998,19296825.059,18550577.488000002,17767621.771000002,17550016.416999999,17621840.708999999,18228436.557999998]
[null,null,"Complex connection LV",null,2381682.6680000001,2306696.6809999999,2245826.2749999999,2201293.219,2195043.5249999999,2195903.8640000001,2305814.111]
[null,null,"Complex connection HV",null,2702810.89,2608654.4890000001,2509248.7089999998,2405960.2999999998,2377572.7850000001,2386879.9109999998,2470831.477]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,11028959.654999999,10532635.693,11419251.602,10883651.233999999,10994794.237,11287333.187000001,11562392.424000001]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,9694288.6449999996,9725413.9649999999,9753246.5999999996,9569055.5130000003,9749705.1089999992,9926902.0889999997,10365628.692]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,36174734.883000001,36194354.968000002,35908251.972999997,34610787.928999998,35011506.968999997,35763060.255999997,36778981.976999998]
[null,null,"Complex connection HV (customer connected at HV)",null,1617386.699,1638831.6129999999,1747557.3289999999,1926037.6950000001,2028524.781,2014927.39,2250223.9539999999]
[null,null,"Complex connection sub-transmission",null,57136400.844999999,14693396.356000001,25921872.659000002,18095828.511,11737422.958000001,9929692.9940000009,4501085.51]
[null,"SUBDIVISION","Complex connection LV",null,2729999.9440000001,2634456.037,2532576.2510000002,2425684.966,2395976.88,2405782.5320000001,2488596.6779999998]
[null,null,"Complex connection HV (no upstream asset works)",null,11850185.664999999,11435455.606000001,10993223.221000001,10529237.289999999,10400282.585999999,10442846.245999999,10802319.884]
[null,null,"Complex connection HV (with upstream asset works)",null,17643895.27,17026398.302000001,16367952.763,15677118.086999999,15485115.754000001,15548489.34,16083714.306]
[null,"EMBEDDED GENERATION","Simple connection LV",null,29781.062999999998,30731.252,36289.659,46724.65,51083.834000000003,49358.682999999997,59230.082000000002]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection LV",null,125069.429,129059.871,152403.12100000001,196226.215,214533.174,207288.179,248744.39499999999]
[null,null,"Complex connection HV",null,6516.09,6723.991,7940.1689999999999,10223.343000000001,11177.130999999999,10799.668,12959.528]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1958230.064,1453752.3629999999,2448620.412,2355302.6570000001,2390764.196,2461814.639,2535520.3870000001]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,722776.48600000003,745837.25399999996,880737.94499999995,1133991.6969999999,1239787.649,1197918.8049999999,1437494.3640000001]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,866093.98400000005,893727.41299999994,1055377.2169999999,1358848.007,1485621.9669999999,1435451.058,1722531.4410000001]
[null,null,"Complex connection HV (customer connected at HV)",null,644728.53,665299.11499999999,785632.75399999996,1011539.272,1105911.0020000001,1068563.3049999999,1282268.649]
[null,null,"Complex connection sub-transmission",null,8574997.3660000004,5228765.7240000004,8937767.7949999999,5269103.1339999996,4702205.7949999999,5662506.9539999999,4461925.0690000001]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,29781.062999999998,30731.252,36289.659,46724.65,51083.834000000003,49358.682999999997,59230.082000000002]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,19996663.671999998,19296825.059,18550577.488000002,17767621.771000002,17550016.416999999,17621840.708999999,18228436.557999998]
[null,null,"Complex connection LV",null,2256613.2390000001,2177636.81,2093423.155,2005067.003,1980510.351,1988615.6850000001,2057069.716]
[null,null,"Complex connection HV",null,2696294.8,2601930.4980000001,2501308.54,2395736.9580000001,2366395.6540000001,2376080.2429999998,2457871.949]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,9070729.591,9078883.3300000001,8970631.1899999995,8528348.5769999996,8604030.0399999991,8825518.5490000006,9026872.0370000005]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,8971512.1600000001,8979576.7109999992,8872508.6539999992,8435063.8159999996,8509917.4600000009,8728983.284,8928134.3279999997]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,35308640.898000002,35300627.555,34852874.755999997,33251939.921999998,33525885.002999999,34327609.197999999,35056450.537]
[null,null,"Complex connection HV (customer connected at HV)",null,972658.16899999999,973532.49800000002,961924.57499999995,914498.424,922613.77899999998,946364.08499999996,967955.30500000005]
[null,null,"Complex connection sub-transmission",null,48561403.479000002,9464630.6319999993,16984104.864,12826725.377,7035217.1639999999,4267186.04,39160.440999999999]
[null,"SUBDIVISION","Complex connection LV",null,2729999.9440000001,2634456.037,2532576.2510000002,2425684.966,2395976.88,2405782.5320000001,2488596.6779999998]
[null,null,"Complex connection HV (no upstream asset works)",null,11850185.664999999,11435455.606000001,10993223.221000001,10529237.289999999,10400282.585999999,10442846.245999999,10802319.884]
[null,null,"Complex connection HV (with upstream asset works)",null,17643895.27,17026398.302000001,16367952.763,15677118.086999999,15485115.754000001,15548489.34,16083714.306]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,14183,13897,13673,13096,12936,12989,13436]
[null,null,"Complex connection LV",null,20,20,20,19,19,19,19]
[null,null,"Complex connection HV",null,26,25,25,24,24,24,25]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,509,462,568,540,545,558,572]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,182,186,203,193,195,200,205]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,146,148,150,143,144,148,151]
[null,null,"Complex connection HV (customer connected at HV)",null,6,7,7,7,7,7,7]
[null,null,"Complex connection sub-transmission",null,9,15,18,11,7,12,4]
[null,"SUBDIVISION","Complex connection LV",null,11,11,10,10,10,10,10]
[null,null,"Complex connection HV (no upstream asset works)",null,19,19,19,18,18,18,18]
[null,null,"Complex connection HV (with upstream asset works)",null,77,75,74,71,70,70,73]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection LV",null,1,1,1,1,1,1,1]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,200,148,250,238,240,246,252]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,87,90,106,101,102,104,107]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,2,2,2,2,2,2,2]
[null,null,"Complex connection HV (customer connected at HV)",null,2,3,3,3,3,3,3]
[null,null,"Complex connection sub-transmission",null,3,3,7,4,1,4,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,0,0]
[null,null,"Complex connection LV",null,1,1]
[null,null,"Complex connection HV",null,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,239,200]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,101,87]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,2,2]
[null,null,"Complex connection HV (customer connected at HV)",null,3,2]
[null,null,"Complex connection sub-transmission",null,3,3]
[null,"SUBDIVISION","Complex connection LV",null,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0]

{"sheet":"2.6 Non-network","index":8,"n_rows":111,"n_cols":11,"rows_kept":111,"cut":false,"hidden":false,"merged":[[84,1,88,1],[62,4,62,10],[64,1,68,1],[69,1,73,1],[74,1,78,1],[79,1,83,1],[55,1,56,3],[55,4,55,10],[5,1,5,2],[12,1,16,1],[19,1,29,1],[32,1,36,1],[39,1,49,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.6 NON-NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,76588797,77003649,112053213,115656877,116530438,117870050,119138178]
[null,"MOTOR VEHICLES","Car",null,624314,674347,679477,684565,686803,691157,696062]
[null,null,"Light commercial vehicle",null,6943124,7499552,7556609,7613194,7638077,7686500,7741050]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,6167461,6661727,6712410,6762674,6784777,6827790,6876246]
[null,null,"Heavy commercial vehicle",null,2535091,2738256,2759089,2779749,2788835,2806515,2826432]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,46922468.159999996,47176629.509999998,44628928.390000001,44984883.890000001,45141415.07,45446023.859999999,45789174.950000003]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","Office furniture and equipment"]
[null,null,"Plant and equipment"]
[null,null,"Crane borer plant HCV",null,1267546,1369128,1379544,1389875,1394417,1403258,1413216]
[null,null,"Other fleet assets",null,1381057,1491736,1503086,1514341,1519291,1528922,1539773]
[null,null,"EWP Hired"]
[null,null,"Car Hired"]
[null,null,"LCV Hired"]
[null,null,"Other Hire"]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,92365295,56028404,72595757,97517491,62468901,39234271,36837893]
[null,"MOTOR VEHICLES","Car",null,2432750,1500902,1462158,0,63135,1898947,1211290]
[null,null,"Light commercial vehicle",null,9320517,8388728,8741627,10855995,8943585,2667146,7560910]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,9593134,22123251,12318847,10514145,10312332,10202997,9657226]
[null,null,"Heavy commercial vehicle",null,2365877,4070513,2357773,2928949,2457018,2809461,1035898]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,37392272,84470791,68021932,14790214,29599460,24661936,7990908]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","Crane borer plant HCV",null,2264011,5935902,5600314,4987412,3030041,589078,0]
[null,null,"Other fleet assets",null,3694077,3126274,4726335,5234990,3362302,2690428,847971]
[null,null,"Minor Assets",null,3380052,1757830,1808860,1758365,1709204,1661404,1614949]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Employee numbers",null,null,2482,2482,2678,2650,2697,2687,2680]
[null,"User numbers",null,null,2502,2502,2699,2671,2719,2708,2702]
[null,"Number of devices",null,null,6046,6046,6523,6456,6570,6545,6529]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","UNITS",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"CAR","Average kilometres travelled ","0's",8751,9189,9648,10130,10637,11169,11727]
[null,null,"Number purchased","0's",68,45,48,48,2,68,45]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",163,163,163,163,163,163,163]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",100,100,96.6,96.6,96.6,96.6,96.6]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",15713,16499,17324,18190,19100,20055,21057]
[null,null,"Number purchased","0's",138,131,151,199,170,51,154]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",889,889,880,871,862,853,844]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",100,100,96.6,96.6,96.6,96.6,96.6]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's"]
[null,null,"Number purchased","0's"]
[null,null,"Number leased","0's"]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%"]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",8120,8283,8448,8617,8790,8965,9145]
[null,null,"Number purchased","0's",9,38,22,22,23,25,22]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",179,179,179,179,179,179,179]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",100,100,96.6,96.6,96.6,96.6,96.6]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",6846,7188,7548,7925,8321,8737,9174]
[null,null,"Number purchased","0's",15,23,14,19,16,19,8]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",230,230,230,230,230,230,230]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",100,100,96.6,96.6,96.6,96.6,96.6]
[]
[]
[null,"Table 2.6.4 intentionally omitted"]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RECURRENT"]
[null,"ICT Asset Extension",null,null,5335938,3824148,8127239,7020408,9195588,7059942,6847610]
[null,"ICT Asset Remediation",null,null,2089247,730380,220996,215757,210666,205718,200909]
[null,"ICT Asset Replacement",null,null,17315222,7421045,12263743,19013297,13183187,8718098,9296506]
[null,"ICT Capability Growth",null,null,3765914,5720053,3237501,1240911,629349,1798784,1050683]
[null,"ICT - OTI",null,null,0,0,1304839,1321237,1331574,1337810,1347678]
[null,"ICT - Resilience",null,null,0,0,1258841,1936706,2420893,2130403,1936743]
[]
[]
[]
[]
[null,"NON-RECURRENT"]
[null,"Complying with Regulatory requirements",null,null,13714820,7793153,6581511,5375007,4804390,6991316,6756451]
[null,"Maintaining existing functionalities",null,null,13172223,2175614,1082963,12077506,6290430,655417,3148036]
[null,"New or expanded ICT functionality",null,null,36971931,28364011,38518124,49316662,24402823,10336784,6253276]

{"sheet":"2.10 Overheads","index":9,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",125056607.1573,122392471.23360001,136072857.45989999,138348914.15849999,139898108.51100001,141122757.71110001,142548604.77869999]
[null,"Alternative Control Services","Total  ",18912019.940000001,16746081.67,19774852.859999999,19884908.690000001,19068311.949999999,18523250.989999998,18252570.280000001]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",158403726,153329857,137923302,140390232,144593861,141358290,138536973]
[null,"Alternative Control Services","Total  ",12785353.789999999,11456299.24,9151111.0999999996,9142836.1199999992,6439058.0599999996,6391378.54,6368190.1399999997]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total  ",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",32345733.370900001,31656657.981699999,34533981.200900003,35787472.2663,36426411.863300003,36765385.457999997,36603307.230899997]
[null,"Alternative Control Services","Total  ",15495549.300000001,13773596.460000001,12731381.699999999,12379211.77,11550036.869999999,10689383.439999999,9878211.6899999995]
[null,"CAPEX"]
[null,"Standard Control Services","Total",5819014,3529789,5007249,6531585,4071473,2650098,2514286]
[null,"Alternative Control Services","Total",448722.97,398461.93,326665.23,434490.28,259705.31,158684.21,148838.62]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",5356950.3075999999,5385966.8909,5426943.3613,5467581.3748000003,5485451.9128,5520227.8788000001,5559404.0652999999]

{"sheet":"2.11 Labour","index":10,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"In-house labour expenditure",205601465.12189999,206635446.2421,228794934.9086,232994742.67289999,234804526.9368,236818740.4154,238723255.30779999]
[null,"Labour expenditure outsourced to related parties",7964614.7279000003,8004669.2150999997,8791949.9012000002,8953336.7756999992,9022881.7269000001,9100282.3214999996,9173467.5059999991]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Controllable non-labour expenditure",153242558.5544,154013223.8425,179917997.46520001,183220609.92469999,184643774.12509999,186227695.7958,187725353.5377]
[null,"Uncontrollable non-labour expenditure",41753461.635799997,41963442.099799998,46090659.1774,46936708.974600002,47301289.3781,47707051.975000001,48090715.830300003]
[null,"Total",{"$f":"SUM(C12:C16)","v":408562100.03999996},410616781.39950001,463595541.45239997,472105398.34789997,475772472.16689998,479853770.50770003,483712792.18180001]
[null,"CAPEX"]
[null,"In-house labour expenditure",365074739,353068991,298380509,308215258,312432410,300229898,292485030]
[null,"Labour expenditure outsourced to related parties",21456076,21106763,20832340,19545716,19110449,18337422,17522245]
[null,"Labour expenditure outsourced to unrelated parties",0,0,0,0,0,0,0]
[null,"Controllable non-labour expenditure",372227789,372229995,404179713,350954227,332057905,318190480,298443917]
[null,"Uncontrollable non-labour expenditure"]
[null,"Total",{"$f":"SUM(C19:C23)","v":758758604},746405749,723392562,678715201,663600764,636757800,608451192]

{"sheet":"2.14 Forecast price changes","index":11,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[[5,1,5,2],[11,4,11,8],[7,1,7,2],[8,1,8,2],[11,2,11,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"Ausgrid must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,"DESCRIPTION",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"CPI","6.30%","4.20%","2.87%","2.87%","2.87%","2.87%","2.87%"]
[null,"Labour - EGWWS (real) (Average of BISOE and KPMG, plus super guarantee increases)","0.00%","0.00%","1.65%","1.50%","0.66%","0.50%","0.71%"]
[]
[null,"CAPEX"]
[null,"CPI","8.00%","4.75%","2.87%","2.87%","2.87%","2.87%","2.87%"]
[null,"Labour - EGWWS (real) (Average of BISOE and KPMG)","-3.96%","-0.23%","1.40%","1.25%","0.66%","0.50%","0.71%"]
[null,"Contract Costs - Construction WPI (real) (BISOE Construction WPI - NSW)","-4.43%","-0.98%","1.30%","1.27%","0.90%","0.44%","0.77%"]

{"sheet":"2.16 Opex Summary","index":12,"n_rows":63,"n_cols":12,"rows_kept":63,"cut":false,"hidden":false,"merged":[[10,1,10,7],[10,9,10,10],[5,1,5,6],[7,9,7,11],[8,1,8,7],[8,9,8,10],[8,11,9,11],[9,1,9,7],[9,9,9,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nAusgrid's total forecast opex must reconcile to Table 2.16.1 (and if Ausgrid owns any dual function assets Table 2.16.3). If Ausgrid did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if Ausgrid owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has Ausgrid used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If Ausgrid does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2022-23"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y1","v":"2019-20"},{"$f":"CRCP_y2","v":"2020-21"},{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Base year total opex, excluding category specific",null,null,null,408562100.03979999,408562100.03979999,408562100.03979999,408562100.03979999,408562100.03979999,408562100.03979999,408562100.03979999]
[null,"Increment from base year to final year",null,null,null,null,44687088.839400001,44687088.839400001,44687088.839400001,44687088.839400001,44687088.839400001,44687088.839400001]
[null,"Price growth",null,null,null,null,null,4447604.1283999998,8543137.7409000006,10413712.9606,11904424.311899999,13995998.3727]
[null,"Output growth",null,null,null,null,null,1295680.959,2960939.1055000001,4952465.3801999995,8802401.8325999994,12473009.8344]
[null,"Productivity growth",null,null,null,null,null,-2294962.3698,-4635913.8256000001,-6994142.9326999998,-9408263.5800000001,-11873623.528000001]
[null,"Step changes",null,null,null,null,null,6898029.8595000003,11988046.4487,14151247.8804,15306019.068,15868218.6259]
[null,"Category specific",null,null,null,null,null,9013310.6776000001,9080997.8620999996,9110888.2730999999,9119465.1221999992,9109618.1381999999]
[null,"Total opex",{"$f":"SUM(C17:C23)","v":0},0,0,408562100.03979999,453249188.87919998,472608852.13390005,481186396.21079993,484883360.44080007,488973235.63390005,492822410.32239991]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y1","v":"2019-20"},{"$f":"CRCP_y2","v":"2020-21"},{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C30:C36)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,2017,2018,2019,2020,2021,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Base year total opex, excluding category specific",null,null,null,19610980.801899999,19610980.801899999,19610980.801899999,19610980.801899999,19610980.801899999,19610980.801899999,19610980.801899999]
[null,"Increment from base year to final year",null,null,null,null,2144980.2642999999,2144980.2642999999,2144980.2642999999,2144980.2642999999,2144980.2642999999,2144980.2642999999]
[null,"Price growth",null,null,null,null,null,213484.9982,410070.6116,499858.22210000001,571412.36699999997,671807.92189999996]
[null,"Output growth",null,null,null,null,null,62192.686000000002,142125.07709999999,237718.3382,422515.288,598704.47210000001]
[null,"Productivity growth",null,null,null,null,null,-110158.19379999999,-222523.86360000001,-335718.86080000002,-451596.65179999999,-569933.92929999996]
[null,"Step changes",null,null,null,null,null,331105.43329999998,575426.22950000002,679259.8983,734688.91529999999,761674.49399999995]
[null,"Category specific",null,null,null,null,null,1215506.855,1207726.3362,1191719.5845999999,1173044.5374,1158993.9558000001]
[null,"Total opex",{"$f":"SUM(C43:C49)","v":0},0,0,19610980.801899999,21755961.066199999,23468092.844900001,23868785.456999999,24028798.248599999,24206025.522099998,24377207.980700001]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y1","v":"2019-20"},{"$f":"CRCP_y2","v":"2020-21"},{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C56:C62)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":13,"n_rows":84,"n_cols":11,"rows_kept":84,"cut":false,"hidden":false,"merged":[[5,1,5,2],[36,1,36,3],[20,1,20,3],[21,1,21,3],[83,1,83,2],[67,1,67,3],[51,1,51,3],[52,1,52,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Cyber security","Uplift our capability to respond to the frequency and severity of cyber attacks",null,null,null,2353241.1713,3991990.6683999998,4357664.1205000002,4742602.0657000002,5147865.8108000001]
[null,"Insurance premiums","Insurance premium increases",null,null,null,812483.64659999998,1813461.3328,2341358.5462000002,2464243.9125999999,2058735.855]
[null,"Community resilience","Delivery of community resilience programs",null,null,null,1097356.1222000001,1688240.1880000001,2110300.2349999999,1857064.2068,1688240.1880000001]
[null,"Smart meter data","Purchase of smart meter data to improve safety and reduce CER curtailment",null,null,null,3599849.5,4308742.9400000004,5006559.92,5648994.5999999996,6302505.7400000002]
[null,"Network innovation program","Enable research and development through partnership",null,null,null,1000000,1000000,1000000,1000000,1000000]
[null,"ICT enablement for CER integration","Delivering some projects in the CER ICT program as opex rather than capex",null,null,null,941720.62919999997,2092232.5294000001,2241986.2686000001,2499735.4928000001,2577492.2420000001]
[null,"Property","Remove opex associated with property disposals in the current period",null,null,null,-2906621.2099000001,-2906621.2099000001,-2906621.2099000001,-2906621.2099000001,-2906621.2099000001]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E11:E20)","v":0},0,6898029.8593999995,11988046.4487,14151247.880400002,15306019.068,15868218.6259]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$21,0)-ROUND('2.16 Opex Summary'!H$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$21,0)-ROUND('2.16 Opex Summary'!I$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$21,0)-ROUND('2.16 Opex Summary'!J$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$21,0)-ROUND('2.16 Opex Summary'!K$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$21,0)-ROUND('2.16 Opex Summary'!L$22,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"N/A","N/A",null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E27:E36)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Cyber security","Uplift our capability to respond to the frequency and severity of cyber attacks",null,null,null,112955.5762,191615.5521,209167.87779999999,227644.89920000001,247097.5589]
[null,"Insurance premiums","Insurance premium increases",null,null,null,38999.214999999997,87046.144,112385.2102,118283.7078,98819.320999999996]
[null,"Community resilience","Delivery of community resilience programs",null,null,null,52673.0939,81035.528999999995,101294.41130000001,89139.081900000005,81035.528999999995]
[null,"Smart meter data","Purchase of smart data to improve safety and reduce CER curtailment",null,null,null,172792.77600000001,206819.6611,240314.8762,271151.74080000003,302520.27549999999]
[null,"Network innovation program","Enable research and development through partnership",null,null,null,48000,48000,48000,48000,48000]
[null,"ICT enablement for CER integration","Delivering some projects in the CER ICT program as opex rather than capex",null,null,null,45202.590199999999,100427.1614,107615.3409,119987.3037,123719.62760000001]
[null,"Property","Remove opex associated with property disposals in the current period",null,null,null,-139517.8181,-139517.8181,-139517.8181,-139517.8181,-139517.8181]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E42:E51)","v":0},0,331105.43319999997,575426.2294999999,679259.8983,734688.91529999999,761674.49389999988]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$21,0)-ROUND('2.16 Opex Summary'!H$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$21,0)-ROUND('2.16 Opex Summary'!I$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$21,0)-ROUND('2.16 Opex Summary'!J$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$21,0)-ROUND('2.16 Opex Summary'!K$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$21,0)-ROUND('2.16 Opex Summary'!L$48,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"N/A","N/A",null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E58:E67)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE \n($0's, real June 2024)"]
[null,"CATEGORY","DESCRIPTION",{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Debt raising costs - distribution",null,null,null,null,null,7797804,7873272,7919169,7946421]
[null,"Debt raising costs - dual function assets",null,null,null,null,null,1215507,1207726,1191720,1173045]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D74:D83)","v":0},0,0,0,9013311,9080998,9110889,9119466]

{"sheet":"3.1 Revenue","index":14,"n_rows":50,"n_cols":17,"rows_kept":50,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[28,2,28,8],[28,10,28,16],[41,2,41,8],[41,10,41,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DREV0101","Revenue from Fixed Customer Charges ",456643081.76999998,468874369.16000003,459621011.63999999,463126251.79000002,470878789.00999999,478469296.13,489512675.31999999]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",215673785.66,188168468.66,169500160.84999999,161362748.27000001,147690730.87,132423205.88,114939053.19]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",131480766.34,120333973.14,150959181.63,158740306.69999999,166996630.06999999,175622825.83000001,183307517.58000001]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",132129838.81999999,113854771.28,68239645.579999998,68059011.180000007,67712721.25,64333429.079999998,62363513.25]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",53057640.340000004,46942815.979999997,60579193.18,60066981.630000003,59528419.460000001,57809690.630000003,56034648.399999999]
["DREV0106","Revenue from controlled load customer charges",0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",9062695.6999999993,8784689.0999999996,8866499.4499999993,8998511.9900000002,9505244.7400000002,9942076.6999999993,10398984.130000001]
["DREV0108","Revenue from Contracted Maximum Demand charges",0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",491017460.47000003,511037591.95999998,578911097.71000004,627941009.27999997,681061608.37,741831377.48000002,802971163.84000003]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,74199241.930000007,69707210.400000006,66295548.649999999,64253712.939999998,60927455.310000002,56656773.18,51892829.789999999]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,58276255.210000001,58944348.630000003,62639756.149999999,63045438.350000001,63574076.939999998,64101931.479999997,64557748.68]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,38065560.229999997,38352369.229999997,31330368.43,32224753.629999999,32647787.170000002,32623156.620000001,32536779.620000001]
["DREV0113","Revenue from other Sources",102727003.18000001,115471347.84999999,150619173.46000001,166152875.63,181398407.31,198023565.16999999,216167032.18000001]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C12:C24)","v":1591792272.28},1573468027.1299999,1647295963.5,1714447696.4700003,1784772551.0799999,1858455466.9000001,1935694587.8900001,null,{"$f":"SUM(K12:K24)","v":170541057.37},167003928.25999999,160265673.22999999,159523904.91999999,157149319.42000002,153381861.28,148987358.09]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DREV0201","Revenue from residential Customers ",661379178.17999995,642498304.52999997,649355150.48000002,669786921.30999994,696127002.24000001,716059750.25999999,739195886.24000001]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",136731965.71000001,135423277.72,137254000.47999999,139823870.16999999,140979112.72999999,142640452.5,143520135.99000001]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",588218372.24000001,581366784.00999999,607188494.62,629780287.80999994,650588670.24000001,679244254.65999997,707198800.61000001]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",93109423.829999998,89341557.290000007,93762379.670000002,101311110.67,107671459.54000001,114119874.29000001,120861576.67]
["DREV0205","Revenue from unmetered supplies",9062695.6999999993,8784689.0999999996,8866499.4499999993,8998511.9900000002,9505244.7400000002,9942076.6999999993,10398984.130000001]
["DREV0206","Revenue from Other Customers",103290636.61,116053414.47,150869438.81,164746994.52000001,179901061.59,196449058.47999999,214519204.25999999]
["DREV02","Total revenue by customer class",{"$f":"SUM(C32:C37)","v":1591792272.27},1573468027.1199999,1647295963.51,1714447696.47,1784772551.0799999,1858455466.8900001,1935694587.9000003,null,{"$f":"SUM(K32:K37)","v":0},0,0,0,0,0,0]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DREV0301","EBSS",0,0,149181506.96000001,195460623.22999999,58547734.770000003,-4890123.8499999996,0,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",11315550.130000001,4573326.54,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",22074531,22051285.690000001,1403669.25,35264331.329999998,35198686.409999996,35173993.909999996,35179032.5,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C45:C49)","v":33390081.130000003},26624612.23,150585176.21000001,230724954.56,93746421.180000007,30283870.059999995,35179032.5,null,{"$f":"SUM(K45:K49)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":15,"n_rows":75,"n_cols":17,"rows_kept":75,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[66,2,66,8],[66,10,66,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are TWO tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DOPEX0101","Vegetation management",39645413.700199999,40880795.226199999,41191816.576800004,41500268.957000002,41635910.675999999,41899868.693599999,42197225.452500001]
["DOPEX0102","Maintenance",45778424.371699996,45194210.349600002,45538048.189900003,45879046.002700001,46028999.552900001,46320808.313100003,46649539.783200003]
["DOPEX0103","Emergency response",23306063.280499998,25877622.102400001,28986481.6307,29203538.075399999,29298988.4954,29484734.472800002,29693982.982500002]
["DOPEX0104","Non-network",142429858.15939999,144615024.50600001,177272356.39410001,181386158.8881,182484053.06830001,184260215.85910001,186020131.95410001]
["DOPEX0105","Network overheads",125056607.1573,122392471.23360001,136072857.45989999,138348914.15849999,139898108.51100001,141122757.71110001,142548604.77869999]
["DOPEX0106","Corporate overheads",32345733.370900001,31656657.981699999,34533981.200900003,35787472.2663,36426411.863300003,36765385.457999997,36603307.230899997]
["DOPEX0107","Connections",null,null,null,null,null,null,null,null,31378119.739999998,27278941.57,29704415.809999999,30323214.460000001,29451474.25,29018649.239999998,29029678.879999999]
["DOPEX0108","Metering",null,null,null,null,null,null,null,null,34193785.530000001,34014825.490000002,33452092.41,31594897.109999999,28476244.329999998,25003351.850000001,21526499.239999998]
["DOPEX0109","Public lighting",null,null,null,null,null,null,null,null,11209539.710000001,11810768.83,9315030.7400000002,8910805.1300000008,8764926.1099999994,8771144.9600000009,8792093.0600000005]
["DOPEX0110","Fee and quoted"]
["DOPEX0111","Network overheads",null,null,null,null,null,null,null,null,18912019.940000001,16746081.67,19774852.859999999,19884908.690000001,19068311.949999999,18523250.989999998,18252570.280000001]
["DOPEX0112","Corporate overheads",null,null,null,null,null,null,null,null,15495549.300000001,13773596.460000001,12731381.699999999,12379211.77,11550036.869999999,10689383.439999999,9878211.6899999995]
["DOPEX0113"]
["DOPEX0114"]
["DOPEX0115"]
["DOPEX0116"]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C13:C61)","v":408562100.03999996},410616781.39950001,463595541.45230001,472105398.34799999,475772472.1669001,479853770.50770003,483712792.18190002,null,{"$f":"SUM(K13:K61)","v":111189014.21999998},103624214.02000001,104977773.52,103093037.16,97310993.510000005,92005780.480000004,87479053.150000006]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DOPEX0201","Opex for network services",408562100.04000002,410616781.39950001,463595541.45240003,472105398.34789997,475772472.16689998,479853770.50779998,483712792.18180001]
["DOPEX0202","Opex for metering",null,null,null,null,null,null,null,null,36310020.689999998,36108509.149999999,43805897.549999997,41347392.770000003,37211283.380000003,32631193.440000001,28061272.91]
["DOPEX0203","Opex for connection services",null,null,null,null,null,null,null,null,61753068.810000002,53685764.780000001,50264345.829999998,51311446.350000001,49836330.600000001,49103925.479999997,49122589.299999997]
["DOPEX0204","Opex for public lighting",null,null,null,null,null,null,null,null,13125924.720000001,13829940.09,10907530.140000001,10434198.050000001,10263379.52,10270661.539999999,10295190.939999999]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP"]
["DOPEX0207","Opex for transmission connection point planning"]

{"sheet":"3.3 Assets (RAB)","index":16,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[97,2,97,8],[97,10,97,16],[97,18,97,24],[114,2,114,8],[114,10,114,16],[114,18,114,24],[8,2,8,8],[8,10,8,16],[8,18,8,24],[21,2,21,8],[21,10,21,16],[21,18,21,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",18361002553.41,18334058785.759998,18545906743.950001,18685180786.32,18746683689.529999,18764331527.25,18744070243.18,null,18361002553.41,18334058785.759998,18545906743.950001,18685180786.32,18746683689.529999,18764331527.25,18744070243.18,null,184565586.61000001,151986823.71000001,116020621.72,95251723.180000007,69616372.340000004,44101767.68,18904452.66]
["DRAB0102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0103","Straight line depreciation",-625935674.83000004,-638652497.05999994,-588253450.72000003,-622058556.11000001,-653415615.75999999,-664978446.96000004,-648159844.70000005,null,-625827085.32000005,-637771809.65999997,-587622347.63,-621961334.36000001,-653317038,-664880183.60000002,-648061694.75,null,-32449163.399999999,-29833418.440000001,-25728860.530000001,-29841065.710000001,-28856249.84,-27536285.640000001,-15971986.619999999]
["DRAB0105","Actual additions (recognised in RAB)",768434592.48000002,854143146.29999995,733330201.51999998,688200155.63999999,673115288.63,646126658.84000003,617671275.25999999,null,768326002.97000003,852938940.21000004,732699098.44000006,688102933.88999999,673016710.88,646028395.48000002,617573125.30999994,null,40208.21,-6132783.54,5119431.59,4333195.6100000003,3398033.93,2377706.66,1830082.79]
["DRAB0106","Disposals ",-169442685.30000001,-3642691.04,-5802708.4400000004,-4638696.32,-2051835.16,-1409495.94,-582483.76,null,-169442685.30000001,-3319172.36,-5802708.4400000004,-4638696.32,-2051835.16,-1409495.94,-582483.76,null,-169807.72,0,-159469.60999999999,-127480.73,-56388.75,-38736.050000000003,-16007.99]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":18334058785.759998},18545906743.959995,18685180786.310001,18746683689.529999,18764331527.240002,18744070243.190002,18712999189.98,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":18334058785.760002},18545906743.949997,18685180786.32,18746683689.529999,18764331527.25,18744070243.190002,18712999189.980003,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":151986823.70000002},116020621.73,95251723.170000002,69616372.350000009,44101767.68,18904452.649999999,4746540.8400000008]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",2202955414.8899999,2231851376.5900002,2249002992.2399998,2275786970.52,2304175789.3800001,2334709059.9200001,2362339238.96,null,2202955414.8899999,2231851376.5900002,2249002992.2399998,2275786970.52,2304175789.3800001,2334709059.9200001,2362339238.96,null,0,0,0,0,0,0,0]
["DRAB0202","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-41720888.619999997,-44095166.869999997,-45387164.990000002,-46729187.770000003,-48124877.939999998,-49585878.539999999,-51020775.810000002,null,-41720888.619999997,-44095166.869999997,-45387164.990000002,-46729187.770000003,-48124877.939999998,-49585878.539999999,-51020775.810000002,null,0,0,0,0,0,0,0]
["DRAB0205","Actual additions (recognised in RAB)",70616850.319999993,61246782.520000003,72171143.280000001,75118006.620000005,78658148.489999995,77216057.569999993,75916151.959999993,null,70616850.319999993,61246782.520000003,72171143.280000001,75118006.620000005,78658148.489999995,77216057.569999993,75916151.959999993,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":2231851376.5900002},2249002992.2400002,2275786970.5300002,2304175789.3699999,2334709059.9299998,2362339238.9500003,2387234615.1100001,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":2231851376.5900002},2249002992.2400002,2275786970.5300002,2304175789.3699999,2334709059.9299998,2362339238.9500003,2387234615.1100001,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",5016730439.1499996,5087819649.3199997,5148779759.6899996,5210763251.46,5277772934.0699997,5351034517.5100002,5415869762.5799999,null,5016730439.1499996,5087819649.3199997,5148779759.6899996,5210763251.46,5277772934.0699997,5351034517.5100002,5415869762.5799999,null,0,0,0,0,0,0,0]
["DRAB0302","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-128035555.43000001,-134993073.53999999,-139905347.71000001,-143632433.93000001,-147517638.81999999,-151588389.78,-155580924.30000001,null,-128035555.43000001,-134993073.53999999,-139905347.71000001,-143632433.93000001,-147517638.81999999,-151588389.78,-155580924.30000001,null,0,0,0,0,0,0,0]
["DRAB0305","Actual additions (recognised in RAB)",199124765.59,195953183.91,201888839.47999999,210642116.53999999,220779222.25,216423634.84999999,212706773.63999999,null,199124765.59,195953183.91,201888839.47999999,210642116.53999999,220779222.25,216423634.84999999,212706773.63999999,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":5087819649.3099995},5148779759.6899996,5210763251.4599991,5277772934.0699997,5351034517.5,5415869762.5800009,5472995611.9200001,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":5087819649.3099995},5148779759.6899996,5210763251.4599991,5277772934.0699997,5351034517.5,5415869762.5800009,5472995611.9200001,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",3172778066.5700002,3135420051.2199998,3093673118.5599999,3058448365.1900001,3019437918.3600001,2982705118.6700001,2938363279.8099999,null,3172778066.5700002,3135420051.2199998,3093673118.5599999,3058448365.1900001,3019437918.3600001,2982705118.6700001,2938363279.8099999,null,0,0,0,0,0,0,0]
["DRAB0402","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-107916702.84999999,-112731234.53,-112573729.40000001,-114156716.98999999,-115755635.25,-117437162.41,-118992105.42,null,-107916702.84999999,-112731234.53,-112573729.40000001,-114156716.98999999,-115755635.25,-117437162.41,-118992105.42,null,0,0,0,0,0,0,0]
["DRAB0405","Actual additions (recognised in RAB)",70558687.510000005,66744333.189999998,77348976.030000001,75146270.159999996,79022835.560000002,73095323.549999997,70716285.109999999,null,70558687.510000005,66744333.189999998,77348976.030000001,75146270.159999996,79022835.560000002,73095323.549999997,70716285.109999999,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,4239968.67,0,0,0,0,0,null,0,4239968.67,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":3135420051.2300005},3093673118.5499997,3058448365.1900001,3019437918.3600001,2982705118.6700001,2938363279.8100004,2890087459.5,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":3135420051.2300005},3093673118.5499997,3058448365.1900001,3019437918.3600001,2982705118.6700001,2938363279.8100004,2890087459.5,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",1047925203.09,1049575792.65,1139066250.5,1129002809.28,1116927735.3900001,1104137972.3900001,1096331734.0699999,null,1047925203.09,1049575792.65,1139066250.5,1129002809.28,1116927735.3900001,1104137972.3900001,1096331734.0699999,null,0,0,0,0,0,0,0]
["DRAB0502","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-30508330.190000001,-31808283.030000001,-30802121.260000002,-31245979.460000001,-31655946.140000001,-32059293.82,-32578976.609999999,null,-30508330.190000001,-31808283.030000001,-30802121.260000002,-31245979.460000001,-31655946.140000001,-32059293.82,-32578976.609999999,null,0,0,0,0,0,0,0]
["DRAB0505","Actual additions (recognised in RAB)",32158919.75,51125612.170000002,20738680.030000001,19170905.57,18866183.149999999,24253055.5,27945793.27,null,32158919.75,51125612.170000002,20738680.030000001,19170905.57,18866183.149999999,24253055.5,27945793.27,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,70173128.719999999,0,0,0,0,0,null,0,70173128.719999999,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":1049575792.65},1139066250.51,1129002809.27,1116927735.3899999,1104137972.4000001,1096331734.0700002,1091698550.73,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":1049575792.65},1139066250.51,1129002809.27,1116927735.3899999,1104137972.4000001,1096331734.0700002,1091698550.73,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",1752522796.1600001,1737914089.1099999,1697780812.3800001,1666253863.1400001,1625095009.1700001,1582504971.25,1561932376.23,null,1752522796.1600001,1737914089.1099999,1697780812.3800001,1666253863.1400001,1625095009.1700001,1582504971.25,1561932376.23,null,0,0,0,0,0,0,0]
["DRAB0602","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-58030146.880000003,-60534721.530000001,-65692548.789999999,-66436921.899999999,-66985346.850000001,-67514503.230000004,-68539524.069999993,null,-58030146.880000003,-60534721.530000001,-65692548.789999999,-66436921.899999999,-66985346.850000001,-67514503.230000004,-68539524.069999993,null,0,0,0,0,0,0,0]
["DRAB0605","Actual additions (recognised in RAB)",43421439.82,90574573.519999996,34165599.549999997,25278067.93,24395308.93,46941908.210000001,50096752.18,null,43421439.82,90574573.519999996,34165599.549999997,25278067.93,24395308.93,46941908.210000001,50096752.18,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,-70173128.719999999,0,0,0,0,0,null,0,-70173128.719999999,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":1737914089.0999999},1697780812.3799999,1666253863.1400001,1625095009.1700001,1582504971.2500002,1561932376.23,1543489604.3400002,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":1737914089.0999999},1697780812.3799999,1666253863.1400001,1625095009.1700001,1582504971.2500002,1561932376.23,1543489604.3400002,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",4126788669.7800002,4083770331.98,4026446086.0900002,3990060584.5700002,3943661529.6300001,3897990974.5500002,3845003039.77,null,4126788669.7800002,4083770331.98,4026446086.0900002,3990060584.5700002,3943661529.6300001,3897990974.5500002,3845003039.77,null,0,0,0,0,0,0,0]
["DRAB0702","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-117836657.67,-124408128.87,-118234265.55,-120677661.91,-122978261.68000001,-125355046.75,-127570543.94,null,-117836657.67,-124408128.87,-118234265.55,-120677661.91,-122978261.68000001,-125355046.75,-127570543.94,null,0,0,0,0,0,0,0]
["DRAB0705","Actual additions (recognised in RAB)",74818319.870000005,70389107.560000002,81848764.040000007,74278606.969999999,77307706.599999994,72367111.980000004,68284457.120000005,null,74818319.870000005,70389107.560000002,81848764.040000007,74278606.969999999,77307706.599999994,72367111.980000004,68284457.120000005,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",0,-3305224.59,0,0,0,0,0,null,0,-3305224.59,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":4083770331.98},4026446086.0799999,3990060584.5799999,3943661529.6300001,3897990974.5500002,3845003039.7800002,3785716952.9499998,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":4083770331.98},4026446086.0799999,3990060584.5799999,3943661529.6300001,3897990974.5500002,3845003039.7800002,3785716952.9499998,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",104360123.86,104468713.37,105025882.09999999,105656985.18000001,105754206.93000001,105852784.68000001,105951048.04000001,null,104360123.86,104468713.37,105025882.09999999,105656985.18000001,105754206.93000001,105852784.68000001,105951048.04000001,null,0,0,0,0,0,0,0]
["DRAB0802","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",108589.51,880687.41,631103.07999999996,97221.75,98577.75,98263.360000000001,98149.95,null,108589.51,880687.41,631103.07999999996,97221.75,98577.75,98263.360000000001,98149.95,null,0,0,0,0,0,0,0]
["DRAB0804","Disposals ",0,-323518.68,0,0,0,0,0,null,0,-323518.68,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",{"$f":"SUM(C68+C69+C70+C71)","v":104468713.37},105025882.09999999,105656985.17999999,105754206.93000001,105852784.68000001,105951048.04000001,106049197.99000001,null,{"$f":"SUM(K68+K69+K70+K71)","v":104468713.37},105025882.09999999,105656985.17999999,105754206.93000001,105852784.68000001,105951048.04000001,106049197.99000001,null,{"$f":"SUM(S68+S69+S70+S71)","v":0},0,0,0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,158544764.25,135801288.41,112347758.62,87782619.680000007,63217480.740000002,38652341.799999997,14087202.859999999]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0903","Straight line depreciation",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-22743475.850000001,-23449120.68,-24565138.940000001,-24565138.940000001,-24565138.940000001,-24565138.940000001,-14087202.859999999]
["DRAB0905","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,-4409.1099999999997,0,0,0,0,0]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":135801288.40000001},112347758.61999999,87782619.680000007,63217480.74000001,38652341.799999997,14087202.859999996,0]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",761841600.61000001,660073634.72000003,840989671.47000003,981506970.40999997,1067663668.51,1154263373.01,1216902171.5999999,null,761841600.61000001,660073634.72000003,840989671.47000003,981506970.40999997,1067663668.51,1154263373.01,1216902171.5999999,null,24927044,18903604.399999999,10132943.1,10574160.300000001,7625123.3099999996,6683801.1299999999,5242478.1900000004]
["DRAB1002","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1003","Straight line depreciation",-45068482.68,-47336998.399999999,-7461738.3300000001,-14546696.75,-16431506.9,-21707816.469999999,-24039064.59,null,-45068482.68,-47336998.399999999,-7461738.3300000001,-14546696.75,-16431506.9,-21707816.469999999,-24039064.59,null,-5893840.0899999999,-4463550.08,-2325608.38,-4244677.1500000004,-2542922.9700000002,-2718312.14,-2310012.15]
["DRAB1005","Actual additions (recognised in RAB)",112743202.08,232506951.59,153781745.72,105342091.16,105083046.56999999,85756111,66706025.93,null,112743202.08,232506951.59,153781745.72,105342091.16,105083046.56999999,85756111,66706025.93,null,40208.21,-4307111.2300000004,2926295.19,1423120.9,1657989.55,1315725.24,834705.55]
["DRAB1006","Disposals ",-169442685.30000001,-4253916.4400000004,-5802708.4400000004,-4638696.32,-2051835.16,-1409495.94,-582483.76,null,-169442685.30000001,-4253916.4400000004,-5802708.4400000004,-4638696.32,-2051835.16,-1409495.94,-582483.76,null,-169807.72,0,-159469.60999999999,-127480.73,-56388.75,-38736.050000000003,-16007.99]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":660073634.71000004},840989671.47000003,981506970.41999996,1067663668.4999999,1154263373.02,1216902171.5999999,1258986649.1800001,null,{"$f":"SUM(K81+K82+K83+K84+K85)","v":660073634.71000004},840989671.47000003,981506970.41999996,1067663668.4999999,1154263373.02,1216902171.5999999,1258986649.1800001,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":18903604.400000002},10132943.089999998,10574160.300000001,7625123.3200000003,6683801.1399999997,5242478.18,3751163.6000000006]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",175100239.30000001,243165146.80000001,245142170.93000001,267700986.56,286194898.10000002,251132755.25,201377592.12,null,175100239.30000001,243165146.80000001,245142170.93000001,267700986.56,286194898.10000002,251132755.25,201377592.12,null,1093778.3700000001,-2718069.1,-6460079.9900000002,-3105056.8,-1226231.71,-1234375.25,-425228.4]
["DRAB1102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1103","Straight line depreciation",-96818910.510000005,-82744890.299999997,-68196534.680000007,-84632957.379999995,-103966402.17,-99730355.959999993,-69837929.959999993,null,-96818910.510000005,-82744890.299999997,-68196534.680000007,-84632957.379999995,-103966402.17,-99730355.959999993,-69837929.959999993,null,-3811847.47,-1920747.68,1161886.78,-1031249.62,-1748187.93,-252834.57,425228.4]
["DRAB1105","Actual additions (recognised in RAB)",164883818.02000001,84721914.430000007,90755350.310000002,103126868.92,68904259.319999993,49975192.82,45200886.100000001,null,164883818.02000001,84721914.430000007,90755350.310000002,103126868.92,68904259.319999993,49975192.82,45200886.100000001,null,0,-1821263.21,2193136.41,2910074.71,1740044.39,1061981.42,995377.24]
["DRAB1106","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":243165146.81},245142170.93000001,267700986.56,286194898.10000002,251132755.25,201377592.11000001,176740548.26000002,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":243165146.81},245142170.93000001,267700986.56,286194898.10000002,251132755.25,201377592.11000001,176740548.26000002,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":-2718069.1},-6460079.9900000002,-3105056.8,-1226231.71,-1234375.2499999998,-425228.40000000014,995377.24]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",2217403395.7399998,2240427184.4099998,2262394981.3800001,2289981379.9499998,2319442424.6500001,2348524149.4400001,2374786927.0300002,null,2217403395.7399998,2240427184.4099998,2262394981.3800001,2289981379.9499998,2319442424.6500001,2348524149.4400001,2374786927.0300002,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",5052275044.2399998,5118299704.5,5179771505.5799999,5244268092.7700005,5314403725.79,5383452140.04,5444432687.25,null,5052275044.2399998,5118299704.5,5179771505.5799999,5244268092.7700005,5314403725.79,5383452140.04,5444432687.25,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",3154099058.8899999,3114546584.8899999,3076060741.8699999,3038943141.77,3001071518.52,2960534199.2399998,2914225369.6500001,null,3154099058.8899999,3114546584.8899999,3076060741.8699999,3038943141.77,3001071518.52,2960534199.2399998,2914225369.6500001,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",1048750497.87,1094321021.5799999,1134034529.8900001,1122965272.3299999,1110532853.8900001,1100234853.23,1094015142.4100001,null,1048750497.87,1094321021.5799999,1134034529.8900001,1122965272.3299999,1110532853.8900001,1100234853.23,1094015142.4100001,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",1745218442.6300001,1717847450.75,1682017337.76,1645674436.1600001,1603799990.21,1572218673.74,1552710990.28,null,1745218442.6300001,1717847450.75,1682017337.76,1645674436.1600001,1603799990.21,1572218673.74,1552710990.28,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",4105279500.8800001,4055108209.0300002,4008253335.3299999,3966861057.0999999,3920826252.0900002,3871497007.1599998,3815359996.3600001,null,4105279500.8800001,4055108209.0300002,4008253335.3299999,3966861057.0999999,3920826252.0900002,3871497007.1599998,3815359996.3600001,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",104414418.61,104747297.73,105341433.64,105705596.05,105803495.81,105901916.36,106000123.02,null,104414418.61,104747297.73,105341433.64,105705596.05,105803495.81,105901916.36,106000123.02,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,147173026.33000001,124074523.51000001,100065189.15000001,75500050.209999993,50934911.270000003,26369772.329999998,7043601.4299999997]
["DRAB1209","“Other” assets with long lives",710957617.65999997,750531653.09000003,911248320.94000006,1024585319.46,1110963520.76,1185582772.3099999,1237944410.3900001,null,710957617.65999997,750531653.09000003,911248320.94000006,1024585319.46,1110963520.76,1185582772.3099999,1237944410.3900001,null,21915324.199999999,14518273.75,10353551.699999999,9099641.8000000007,7154462.2199999997,5963139.6600000001,4496820.9000000004]
["DRAB1210","“Other” assets with short lives",209132693.05000001,244153658.87,256421578.75,276947942.32999998,268663826.67000002,226255173.68000001,189059070.19,null,209132693.05000001,244153658.87,256421578.75,276947942.32999998,268663826.67000002,226255173.68000001,189059070.19,null,-812145.37,-4589074.55,-4782568.4000000004,-2165644.25,-1230303.48,-829801.82,285074.42]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",55,56,55,55,55,55,55,null,55,56,55,55,55,55,55,null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)",56,56,56,56,56,56,56,null,56,56,56,56,56,56,56,null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers",47,47,47,47,47,47,47,null,47,47,47,47,47,47,47,null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",48,48,48,48,48,48,48,null,48,48,48,48,48,48,48,null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",46,46,46,46,46,46,46,null,46,46,46,46,46,46,46,null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers",42,42,42,42,42,42,42,null,42,42,42,42,42,42,42,null,0,0,0,0,0,0,0]
["DRAB1407","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,20,20,20,20,20,22,22]
["DRAB1408","“Other” assets with long lives",20,21,25,27,29,31,33,null,20,21,25,27,29,31,33,null,18,20,18,19,18,18,18]
["DRAB1409","“Other” assets with short lives",5,5,6,6,6,6,6,null,5,5,6,6,6,6,6,null,5,5,5,5,5,5,5]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",40,40,39,39,39,38,38,null,40,40,39,39,39,38,38,null,0,0,0,0,0,0,0]
["DRAB1502","Underground network assets less than 33kV (cables)",41,40,40,40,39,39,38,null,41,40,40,40,39,39,38,null,0,0,0,0,0,0,0]
["DRAB1503","Distribution substations including transformers",29,29,28,27,27,27,26,null,29,29,28,27,27,27,26,null,0,0,0,0,0,0,0]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",30,30,30,29,29,28,28,null,30,30,30,29,29,28,28,null,0,0,0,0,0,0,0]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",30,29,28,28,27,26,26,null,30,29,28,28,27,26,26,null,0,0,0,0,0,0,0]
["DRAB1506","Zone substations and transformers",27,26,26,25,24,24,23,null,27,26,26,25,24,24,23,null,0,0,0,0,0,0,0]
["DRAB1507","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,6,5,4,3,2,1,0]
["DRAB1508","“Other” assets with long lives",18,20,21,22,23,24,25,null,18,20,21,22,23,24,25,null,5,4,4,5,4,4,3]
["DRAB1509","“Other” assets with short lives",4,4,4,4,4,4,4,null,4,4,4,4,4,4,4,null,3,5,3,2,2,1,1]

{"sheet":"3.4 Operational data","index":17,"n_rows":87,"n_cols":10,"rows_kept":87,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DOPED01","TOTAL ENERGY DELIVERED"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",4297,4044,3750,3452,3055,2649,2224]
["DOPED0202","Energy Delivery at On-peak times","GWh",2698,2700,3104,3310,3555,3735,3941]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",7815,7833,0,0,0,0,0]
["DOPED0204","Energy Delivery at Off-peak times","GWh",8793,8779,17003,17998,19175,20191,21006]
["DOPED0205","Controlled load energy deliveries","GWh",960,952,938,927,916,907,893]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",143,141,136,131,133,136,138]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",3301,3209,3947,4071,4216,4295,4395]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",9737,9370,0,0,0,0,0]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",11171,11006,19966,20646,21461,22118,22548]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",0,0,0,0,0,0,0]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",42,75,61,64,66,69,70]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",123,199,0,0,0,0,0]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",195,249,484,508,528,546,559]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",130,152,170,180,188,194,201]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",928,1085,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",3,3,1216,1287,1343,1388,1436]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",0,0,0,0,0,0,0]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",8697,8540,8437,8528,8654,8805,8931]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",1342,1299,1298,1344,1378,1411,1453]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",8923,8842,9103,9524,9881,10211,10452]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",5600,5625,5958,6290,6786,7056,7228]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",143,141,136,131,133,136,138]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",6157,6263,6311,6333,6378,6418,6451]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5664,5781,5835,5860,5904,5944,5978]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5477,5557,5580,5600,5635,5670,5691]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",4939,5021,5044,5064,5099,5135,5156]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",6613,6751,6853,6934,7015,7092,7135]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",6104,6252,6359,6444,6525,6601,6644]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5866,5943,5999,6056,6119,6174,6199]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5324,5402,5459,5516,5579,5634,5660]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",6292,6400,6449,6472,6517,6558,6593]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5787,5906,5962,5986,6032,6073,6107]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5624,5706,5730,5750,5786,5823,5845]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5070,5154,5179,5199,5235,5272,5293]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",6724,6867,6973,7058,7139,7219,7263]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",6216,6366,6478,6565,6650,6728,6773]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5985,6068,6128,6184,6246,6304,6331]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5439,5520,5581,5639,5705,5764,5790]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.97874546397096995,0.97883508296647004,0.97869842334787005,0.97895088539927,0.97877984084880998,0.97875843899226,0.97887669887015005]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.96509999999999996,0.96509999999999996,0.96509999999999996,0.96509999999999996,0.96509999999999996,0.96509999999999996,0.96509999999999996]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor"]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor"]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor"]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.98450000000000004,0.98450000000000004,0.98450000000000004,0.98440000000000005,0.98440000000000005,0.98440000000000005,0.98440000000000005]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.9,0.9,0.9,0.9,0.9,0.9,0.9]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0.9,0.9,0.9,0.9,0.9,0.9,0.9]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0.97889999999999999,0.97850000000000004,0.97750000000000004,0.9778,0.97699999999999998,0.97699999999999998,0.9768]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor"]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.98719999999999997,0.9879,0.9879,0.9879,0.9879,0.9879,0.9879]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor"]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0.95989999999999998,0.96250000000000002,0.97009999999999996,0.96630000000000005,0.96499999999999997,0.96319999999999995,0.96450000000000002]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor"]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW "]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW ",2047,2392,2380,2772,3271,3782,4286]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA",0,0,0,0,0,0,0]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA",3399,3467,3587,3746,3883,3984,4062]

{"sheet":"3.5 Physical assets","index":18,"n_rows":95,"n_cols":10,"rows_kept":95,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",13086,13087,13091,13093,13090,13094,13095]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0104","Overhead 11 kV","km",9759,9753,9750,9744,9741,9736,9732]
["DPA0105","Overhead SWER","km",119,119,119,119,119,119,119]
["DPA0106","Overhead 22 kV","km",126,126,126,126,126,126,126]
["DPA0107","Overhead 33 kV","km",1281.58,1263.73,1263.73,1263.73,1263.93,1263.93,1263.93]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",474.16,476.26,476.26,476.26,476.26,476.26,476.26]
["DPA0110","Overhead 132 kV","km",1092.3399999999999,1092.3399999999999,1092.3399999999999,1091.8800000000001,1091.8800000000001,1091.8800000000001,1091.8800000000001]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0112","Overhead 110kV","km",0,0,0,0,0,0,0]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D13:D26)","v":25938.080000000002},25917.329999999998,25918.329999999998,25913.87,25908.07,25907.07,25904.07]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",7047,7175,7302,7439,7572,7701,7834]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",0,0,0,0,0,0,0]
["DPA0204","Underground 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0205","Underground 11 kV","km",8770,8850,8931,9015,9101,9182,9266]
["DPA0206","Underground SWER","km",0,0,0,0,0,0,0]
["DPA0207","Underground 22 kV","km",0,0,0,0,0,0,0]
["DPA0208","Underground 33 kV","km",587.95000000000005,550.27,552.29,554.30999999999995,543.39,541.52,541.52]
["DPA0209","Underground 66 kV","km",9.58,9.58,9.58,9.58,9.58,9.58,9.58]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",590.28,569.34,538.16999999999996,527.35,527.35,527.35,472.92]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D29:D40)","v":17004.810000000001},17154.190000000002,17333.04,17545.240000000002,17753.32,17961.45,18124.02]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.24099999999999999,0.24399999999999999,0.248,0.251,0.255,0.25800000000000001,0.26200000000000001]
["DPA0302","Overhead 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0303","Overhead 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0304","Overhead 11 kV","MVA",4.16,4.1980000000000004,4.2370000000000001,4.2750000000000004,4.3129999999999997,4.351,4.3890000000000002]
["DPA0305","Overhead SWER","MVA",0.35199999999999998,0.35199999999999998,0.35199999999999998,0.35199999999999998,0.35199999999999998,0.35199999999999998,0.35199999999999998]
["DPA0306","Overhead 22 kV","MVA",2.726,2.726,2.726,2.726,2.726,2.726,2.726]
["DPA0307","Overhead 33 kV","MVA",29.704000000000001,29.888999999999999,30.068999999999999,30.251999999999999,30.434000000000001,30.616,30.798999999999999]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",72.119,72.097999999999999,72.078000000000003,72.058000000000007,72.037999999999997,72.016999999999996,71.997]
["DPA0310","Overhead 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0311","Overhead 132 kV","MVA",220.61600000000001,220.61600000000001,220.61600000000001,220.61600000000001,220.61600000000001,220.61600000000001,220.61600000000001]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.23599999999999999,0.23599999999999999,0.23599999999999999,0.23599999999999999,0.23599999999999999,0.23499999999999999,0.23499999999999999]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0404","Underground 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0405","Underground 11 kV","MVA",6.4610000000000003,6.3869999999999996,6.3120000000000003,6.2380000000000004,6.1639999999999997,6.09,6.016]
["DPA0406","Underground SWER","MVA",0,0,0,0,0,0,0]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0409","Underground 33 kV","MVA",25.783999999999999,25.588999999999999,25.603999999999999,25.675000000000001,25.667000000000002,25.664999999999999,25.664999999999999]
["DPA0410","Underground 66 kV","MVA",98.968999999999994,98.968999999999994,98.968999999999994,98.968999999999994,98.968999999999994,98.968999999999994,98.968999999999994]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",185.14099999999999,185.173,189.88900000000001,193.583,193.583,193.583,205.012]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",16721,16955,17182,17423,17671,17901,18141]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",1948,2041,2111,2172,2222,2257,2271]
["DPA0503","Cold spare capacity included in DPA0501","MVA",649,691,699,752,797,825,863]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",7741,7741,7741,7861,7861,7861,7861]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",5651,5621,5621,5593,5593,5593,5547]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",7718,7519,7519,7519,7519,7519,7519]
["DPA0604","Total zone substation transformer  capacity ","MVA",22689,22690,22690,22782,22782,22782,22782]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",1579,1809,1809,1809,1809,1809,1855]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DPA0701","Public lighting luminaires","0's",257566,258592,259618,260644,261670,262696,263722]
["DPA0702","Public lighting poles","0's",252964,253785,254606,255427,256248,257069,257890]

{"sheet":"3.6 Quality of service","index":19,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"FORECAST"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DQS0201","Energy Not Supplied (planned)","GWh",4.09,4.09,4.09,4.09,4.09,4.09,4.09]
["DQS0202","Energy Not Supplied (unplanned)","GWh",5.52,5.52,5.52,5.52,5.52,5.52,5.52]
["DQS02","Total",null,{"$f":"SUM(D9:D10)","v":9.61},9.61,9.61,9.61,9.61,9.61,9.61]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"FORECAST"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DQS03","System losses","%","3.60%","3.55%","3.53%","3.51%","3.49%","3.47%","3.45%"]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"FORECAST"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DQS04","Overall utilisation","%","45.8%","46.2%","46.6%","46.8%","47.2%","47.5%","47.7%"]

{"sheet":"3.7 Operating Environment","index":20,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DOEF0101","Customer density","Customer / km",44.858085799999998]
["DOEF0102","Energy density","MWh/customer",13.6]
["DOEF0103","Demand density","kVA / customer",3.2170000000000001]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DOEF0201","Rural proportion","%","45.96%"]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",855208]
["DOEF0203","Rural vegetation maintenance spans","0's",288335]
["DOEF0204","Total vegetation maintenance spans","0's",1176490]
["DOEF0205","Total number of spans","0's",1176490]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",1]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",0.66613273799999995]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",1.9834634120000001]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",0.46078417500000002]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",0.39330384099999999]
["DOEF0212","Tropical proportion","Spans",1226]
["DOEF0213","Standard vehicle access","km",7764.6557000000003,7925.1076999999996,8085.5598,8246.0118000000002,8406.4637999999995,8566.9158000000007,8727.3678]
["DOEF0214","Bushfire risk","Spans",295644]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DOEF0301","Route Line length","km",39976.569000000003,40129.502999999997,40282.436000000002,40435.370000000003,40588.303,40741.237000000001,40894.171000000002]

{"sheet":"4.1 Public lighting","index":21,"n_rows":212,"n_cols":10,"rows_kept":212,"cut":false,"hidden":false,"merged":[[212,1,212,2],[213,1,213,2],[214,1,214,2],[215,1,215,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2],[205,1,205,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[156,1,156,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[88,1,88,2],[95,1,95,2],[93,1,93,2],[96,1,96,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[97,1,97,2],[98,1,98,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[5,1,5,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[54,1,54,2],[55,1,55,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[63,1,63,2],[64,1,64,2],[61,1,61,2],[62,1,62,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's",130,215,175,175,175,175,175]
[null,"Number of poles installed ","0's",130,215,175,175,175,175,175]
[null,"Total expenditure","$0's",1209460,2014610,1619390,1636399,1646501,1653179,1663271]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's",36490,20010,20295,21508,4588,3409,2825]
[null,"Number of poles replaced","0's",172,88,128,127,127,128,128]
[null,"Total expenditure","$0's",31666076,24807611,21299374,19674638,6381829,4843494,3643696]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's",16000,15000,14000,14000,14000,14000,14000]
[null,"Number of poles maintained","0's",4418,4142,3866,3866,3866,3866,3866]
[null,"Total expenditure","$0's",13125925,13829940,10907530,10434198,10263380,10270662,10295191]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days",4.5,4.5,4.5,4.5,4.5,4.5,4.5]
[null,"GSO breaches","0's",115,60,60,60,60,60,60]
[null,"GSL payments ","$0's",1500,1000,750,750,750,750,750]
[null,"Customer complaints ","0's",300,250,250,250,250,250,250]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"LIGHT INSTALLATION"]
[null,"16W LED PH",null,433.84,433.84,433.84,433.84,433.84,433.84,433.84]
[null,"17W LED ALD",null,402.51,402.51,402.51,402.51,402.51,402.51,402.51]
[null,"17W LED ALD RRW",null,402.51,402.51,402.51,402.51,402.51,402.51,402.51]
[null,"17W LED ALD RRW ZHAGA",null,423.77,423.77,423.77,423.77,423.77,423.77,423.77]
[null,"17W LED ALD ZHAGA",null,423.77,423.77,423.77,423.77,423.77,423.77,423.77]
[null,"17W LED SY RRW",null,542.5,542.5,542.5,542.5,542.5,542.5,542.5]
[null,"1x17W LED",null,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005]
[null,"1x22W LED",null,531.14,531.14,531.14,531.14,531.14,531.14,531.14]
[null,"1x25W LED GE",null,457.93,457.93,457.93,457.93,457.93,457.93,457.93]
[null,"25W LED PH",null,435.03,435.03,435.03,435.03,435.03,435.03,435.03]
[null,"28W LED SY",null,565.22,565.22,565.22,565.22,565.22,565.22,565.22]
[null,"1x29W LED",null,594.72,594.72,594.72,594.72,594.72,594.72,594.72]
[null,"49W LED PH",null,465.83,465.83,465.83,465.83,465.83,465.83,465.83]
[null,"49W LED PH ZHAGA",null,531,531,531,531,531,531,531]
[null,"70W LED PH FLOOD",null,684.29,684.29,684.29,684.29,684.29,684.29,684.29]
[null,"76W LED PH",null,553.96,553.96,553.96,553.96,553.96,553.96,553.96]
[null,"76W LED PH ZHAGA",null,619.13,619.13,619.13,619.13,619.13,619.13,619.13]
[null,"100W LED ALD",null,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33]
[null,"140W LED PH",null,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995]
[null,"140W LED PH ZHAGA",null,660.6,660.6,660.6,660.6,660.6,660.6,660.6]
[null,"150W LED SY FLOOD",null,1061.08,1061.08,1061.08,1061.08,1061.08,1061.08,1061.08]
[null,"175W LED SY FLOOD",null,1208,1208,1208,1208,1208,1208,1208]
[null,"200W LED ALD",null,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33]
[null,"224W LED PH",null,692.59,692.59,692.59,692.59,692.59,692.59,692.59]
[null,"224W LED PH ZHAGA",null,757.75,757.75,757.75,757.75,757.75,757.75,757.75]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"16W LED PH",null,433.84,433.84,433.84,433.84,433.84,433.84,433.84]
[null,"17W LED ALD",null,402.51,402.51,402.51,402.51,402.51,402.51,402.51]
[null,"17W LED ALD RRW",null,402.51,402.51,402.51,402.51,402.51,402.51,402.51]
[null,"17W LED ALD RRW ZHAGA",null,423.77,423.77,423.77,423.77,423.77,423.77,423.77]
[null,"17W LED ALD ZHAGA",null,423.77,423.77,423.77,423.77,423.77,423.77,423.77]
[null,"17W LED SY RRW",null,542.5,542.5,542.5,542.5,542.5,542.5,542.5]
[null,"1x17W LED",null,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005,512.20000000000005]
[null,"1x22W LED",null,531.14,531.14,531.14,531.14,531.14,531.14,531.14]
[null,"1x25W LED GE",null,457.93,457.93,457.93,457.93,457.93,457.93,457.93]
[null,"25W LED PH",null,435.03,435.03,435.03,435.03,435.03,435.03,435.03]
[null,"28W LED SY",null,565.22,565.22,565.22,565.22,565.22,565.22,565.22]
[null,"1x29W LED",null,594.72,594.72,594.72,594.72,594.72,594.72,594.72]
[null,"49W LED PH",null,465.83,465.83,465.83,465.83,465.83,465.83,465.83]
[null,"49W LED PH ZHAGA",null,531,531,531,531,531,531,531]
[null,"70W LED PH FLOOD",null,684.29,684.29,684.29,684.29,684.29,684.29,684.29]
[null,"76W LED PH",null,553.96,553.96,553.96,553.96,553.96,553.96,553.96]
[null,"76W LED PH ZHAGA",null,619.13,619.13,619.13,619.13,619.13,619.13,619.13]
[null,"100W LED ALD",null,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33]
[null,"140W LED PH",null,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995,595.42999999999995]
[null,"140W LED PH ZHAGA",null,660.6,660.6,660.6,660.6,660.6,660.6,660.6]
[null,"150W LED SY FLOOD",null,1061.08,1061.08,1061.08,1061.08,1061.08,1061.08,1061.08]
[null,"175W LED SY FLOOD",null,1208,1208,1208,1208,1208,1208,1208]
[null,"200W LED ALD",null,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33,1007.33]
[null,"224W LED PH",null,692.59,692.59,692.59,692.59,692.59,692.59,692.59]
[null,"224W LED PH ZHAGA",null,757.75,757.75,757.75,757.75,757.75,757.75,757.75]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"MBF1x1000",null,90.47,90.47,60.49,60.49,60.49,60.49,60.49]
[null,"MBF1x125",null,47.8,47.8,35.18,35.18,35.18,35.18,35.18]
[null,"MBF1x250",null,64.709999999999994,64.709999999999994,47.88,47.88,47.88,47.88,47.88]
[null,"MBF1x400",null,64.709999999999994,64.709999999999994,47.88,47.88,47.88,47.88,47.88]
[null,"MBF1x42",null,42.62,42.62,31.37,31.37,31.37,31.37,31.37]
[null,"MBF1x50",null,47.92,47.92,35.21,35.21,35.21,35.21,35.21]
[null,"MBF1x80",null,45.4,45.4,33.74,33.74,33.74,33.74,33.74]
[null,"MBF2x80",null,57.81,57.81,42.53,42.53,42.53,42.53,42.53]
[null,"MBI1x100",null,64.63,64.63,44.92,44.92,44.92,44.92,44.92]
[null,"MBI1x1000",null,80.48,80.48,46.77,46.77,46.77,46.77,46.77]
[null,"MBI1x150",null,64.52,64.52,44.92,44.92,44.92,44.92,44.92]
[null,"MBI1x250",null,61.84,61.84,44.59,44.59,44.59,44.59,44.59]
[null,"MBI1x400",null,61.74,61.74,44.57,44.57,44.57,44.57,44.57]
[null,"MBI1x70",null,49.45,49.45,33.159999999999997,33.159999999999997,33.159999999999997,33.159999999999997,33.159999999999997]
[null,"MBI1x70 II",null,70.09,70.09,35.51,35.51,35.51,35.51,35.51]
[null,"SON1x100",null,76.05,76.05,53.71,53.71,53.71,53.71,53.71]
[null,"SON1x1000",null,83.47,83.47,54.99,54.99,54.99,54.99,54.99]
[null,"SON1x150",null,72.349999999999994,72.349999999999994,53.07,53.07,53.07,53.07,53.07]
[null,"SON1x150 AR",null,72.36,72.36,53.07,53.07,53.07,53.07,53.07]
[null,"SON1x250",null,74.12,74.12,53.37,53.37,53.37,53.37,53.37]
[null,"SON1x250 AR",null,74.13,74.13,53.37,53.37,53.37,53.37,53.37]
[null,"SON1x400",null,74.89,74.89,53.5,53.5,53.5,53.5,53.5]
[null,"SON1x400 AR",null,100.59,100.59,53.5,53.5,53.5,53.5,53.5]
[null,"SON1x50",null,55.26,55.26,39.409999999999997,39.409999999999997,39.409999999999997,39.409999999999997,39.409999999999997]
[null,"SON1x600",null,83.62,83.62,54.99,54.99,54.99,54.99,54.99]
[null,"SON1x70",null,53.33,53.33,39.08,39.08,39.08,39.08,39.08]
[null,"SON2x250",null,106.15,106.15,74.459999999999994,74.459999999999994,74.459999999999994,74.459999999999994,74.459999999999994]
[null,"SON2x400",null,107.7,107.7,74.709999999999994,74.709999999999994,74.709999999999994,74.709999999999994,74.709999999999994]
[null,"SON4x250",null,164.83,164.83,112.6,112.6,112.6,112.6,112.6]
[null,"SON4x600",null,202.06,202.06,118.49,118.49,118.49,118.49,118.49]
[null,"TF1x20",null,49.2,49.2,37.36,37.36,37.36,37.36,37.36]
[null,"TF1x40",null,77.92,77.92,61.5,61.5,61.5,61.5,61.5]
[null,"TF1x80",null,48.85,48.85,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997]
[null,"TF2x14 T5",null,49.87,49.87,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997]
[null,"TF2x20",null,61.99,61.99,47.91,47.91,47.91,47.91,47.91]
[null,"TF2x26",null,49.47,49.47,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997]
[null,"TF2x40",null,49.47,49.47,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997]
[null,"TF4x20",null,49.29,49.29,37.36,37.36,37.36,37.36,37.36]
[null,"TF4x40",null,51.14,51.14,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997,37.369999999999997]
[null,"LED TRIAL",null,27.28,27.28,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x100",null,36.29,36.29,30.81,30.81,30.81,30.81,30.81]
[null,"LED1x17",null,27.35,27.35,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x200",null,36.299999999999997,36.299999999999997,30.81,30.81,30.81,30.81,30.81]
[null,"LED1x22",null,27.28,27.28,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x25 GE",null,27.28,27.28,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x28",null,27.35,27.35,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x29",null,27.28,27.28,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x298",null,36.32,36.32,30.81,30.81,30.81,30.81,30.81]
[null,"LED1x33",null,27.39,27.39,22.6,22.6,22.6,22.6,22.6]
[null,"LED1x42",null,27.43,27.43,22.6,22.6,22.6,22.6,22.6]
[null,"Decorative luminaires",null,0,0,24.24,24.24,24.24,24.24,24.24]
[null,"Floodlight luminaires",null,0,0,30.81,30.81,30.81,30.81,30.81]
[null,"Major road luminaires - smart controller",null,0,0,21.81,21.81,21.81,21.81,21.81]
[null,"Minor road luminaires - smart controller",null,0,0,17.47,17.47,17.47,17.47,17.47]
[null,"Floodlight luminaires - smart controller",null,0,0,21.81,21.81,21.81,21.81,21.81]
[null,"Decorative luminaires - smart controller",null,0,0,17.47,17.47,17.47,17.47,17.47]

{"sheet":"5.4 MD & utilisation-Spatial","index":22,"n_rows":11579,"n_cols":12,"rows_kept":11579,"cut":false,"hidden":false,"merged":[[11563,1,11563,2],[11564,1,11564,2],[11560,1,11560,2],[11561,1,11561,2],[11562,1,11562,2],[11557,1,11557,2],[11558,1,11558,2],[11559,1,11559,2],[11541,1,11541,2],[11542,1,11542,2],[11543,1,11543,2],[11544,1,11544,2],[11535,1,11535,2],[11475,1,11475,2],[11466,1,11466,2],[11467,1,11467,2],[11468,1,11468,2],[11469,1,11469,2],[11470,1,11470,2],[11471,1,11471,2],[11472,1,11472,2],[11473,1,11473,2],[11474,1,11474,2],[11565,1,11565,2],[11566,1,11566,2],[11567,1,11567,2],[11568,1,11568,2],[11569,1,11569,2],[11570,1,11570,2],[11571,1,11571,2],[11578,1,11578,2],[11572,1,11572,2],[11573,1,11573,2],[11574,1,11574,2],[11575,1,11575,2],[11576,1,11576,2],[11577,1,11577,2],[11537,1,11537,2],[11538,1,11538,2],[11539,1,11539,2],[11530,1,11530,2],[11531,1,11531,2],[11532,1,11532,2],[11533,1,11533,2],[11534,1,11534,2],[11536,1,11536,2],[11509,1,11509,2],[11510,1,11510,2],[11511,1,11511,2],[11555,1,11555,2],[11556,1,11556,2],[11550,1,11550,2],[11551,1,11551,2],[11552,1,11552,2],[11553,1,11553,2],[11554,1,11554,2],[11545,1,11545,2],[11546,1,11546,2],[11547,1,11547,2],[11548,1,11548,2],[11549,1,11549,2],[11540,1,11540,2],[11504,1,11504,2],[11505,1,11505,2],[11506,1,11506,2],[11507,1,11507,2],[11508,1,11508,2],[11499,1,11499,2],[11500,1,11500,2],[11501,1,11501,2],[11502,1,11502,2],[11503,1,11503,2],[11512,1,11512,2],[11513,1,11513,2],[11514,1,11514,2],[11515,1,11515,2],[11516,1,11516,2],[11517,1,11517,2],[11518,1,11518,2],[11519,1,11519,2],[11520,1,11520,2],[11521,1,11521,2],[11522,1,11522,2],[11523,1,11523,2],[11524,1,11524,2],[11525,1,11525,2],[11526,1,11526,2],[11527,1,11527,2],[11528,1,11528,2],[11529,1,11529,2],[11476,1,11476,2],[11477,1,11477,2],[11478,1,11478,2],[11479,1,11479,2],[11480,1,11480,2],[11481,1,11481,2],[11482,1,11482,2],[11483,1,11483,2],[11484,1,11484,2],[11485,1,11485,2],[11486,1,11486,2],[11487,1,11487,2],[11488,1,11488,2],[11489,1,11489,2],[11490,1,11490,2],[11491,1,11491,2],[11492,1,11492,2],[11493,1,11493,2],[11494,1,11494,2],[11495,1,11495,2],[11496,1,11496,2],[11497,1,11497,2],[11498,1,11498,2],[11433,1,11433,2],[11434,1,11434,2],[11435,1,11435,2],[11436,1,11436,2],[11437,1,11437,2],[11438,1,11438,2],[11439,1,11439,2],[11440,1,11440,2],[11441,1,11441,2],[11442,1,11442,2],[11443,1,11443,2],[11444,1,11444,2],[11445,1,11445,2],[11462,1,11462,2],[11463,1,11463,2],[11464,1,11464,2],[11465,1,11465,2],[11456,1,11456,2],[11457,1,11457,2],[11458,1,11458,2],[11459,1,11459,2],[11460,1,11460,2],[11461,1,11461,2],[11451,1,11451,2],[11452,1,11452,2],[11453,1,11453,2],[11454,1,11454,2],[11455,1,11455,2],[11446,1,11446,2],[11447,1,11447,2],[11448,1,11448,2],[11449,1,11449,2],[11450,1,11450,2],[11429,1,11429,2],[11420,1,11420,2],[11421,1,11421,2],[11422,1,11422,2],[11423,1,11423,2],[11424,1,11424,2],[11431,1,11431,2],[11432,1,11432,2],[11367,1,11367,2],[11368,1,11368,2],[11369,1,11369,2],[11370,1,11370,2],[11371,1,11371,2],[11372,1,11372,2],[11373,1,11373,2],[11374,1,11374,2],[11375,1,11375,2],[11376,1,11376,2],[11377,1,11377,2],[11378,1,11378,2],[11379,1,11379,2],[11425,1,11425,2],[11398,1,11398,2],[11399,1,11399,2],[11390,1,11390,2],[11391,1,11391,2],[11392,1,11392,2],[11393,1,11393,2],[11394,1,11394,2],[11337,1,11337,2],[11338,1,11338,2],[11395,1,11395,2],[11396,1,11396,2],[11397,1,11397,2],[11385,1,11385,2],[11386,1,11386,2],[11387,1,11387,2],[11388,1,11388,2],[11389,1,11389,2],[11380,1,11380,2],[11381,1,11381,2],[11382,1,11382,2],[11383,1,11383,2],[11384,1,11384,2],[11339,1,11339,2],[11401,1,11401,2],[11402,1,11402,2],[11403,1,11403,2],[11404,1,11404,2],[11430,1,11430,2],[11400,1,11400,2],[11364,1,11364,2],[11365,1,11365,2],[11366,1,11366,2],[11361,1,11361,2],[11362,1,11362,2],[11363,1,11363,2],[11345,1,11345,2],[11346,1,11346,2],[11347,1,11347,2],[11348,1,11348,2],[11405,1,11405,2],[11406,1,11406,2],[11409,1,11409,2],[11410,1,11410,2],[11411,1,11411,2],[11412,1,11412,2],[11413,1,11413,2],[11414,1,11414,2],[11415,1,11415,2],[11416,1,11416,2],[11417,1,11417,2],[11418,1,11418,2],[11419,1,11419,2],[11426,1,11426,2],[11427,1,11427,2],[11341,1,11341,2],[11342,1,11342,2],[11343,1,11343,2],[11334,1,11334,2],[11335,1,11335,2],[11336,1,11336,2],[11359,1,11359,2],[11360,1,11360,2],[11354,1,11354,2],[11355,1,11355,2],[11356,1,11356,2],[11357,1,11357,2],[11358,1,11358,2],[11349,1,11349,2],[11350,1,11350,2],[11351,1,11351,2],[11352,1,11352,2],[11353,1,11353,2],[11344,1,11344,2],[11428,1,11428,2],[11321,1,11321,2],[11322,1,11322,2],[11323,1,11323,2],[11324,1,11324,2],[11325,1,11325,2],[11326,1,11326,2],[11327,1,11327,2],[11328,1,11328,2],[11329,1,11329,2],[11330,1,11330,2],[11331,1,11331,2],[11332,1,11332,2],[11333,1,11333,2],[11407,1,11407,2],[11408,1,11408,2],[11340,1,11340,2],[11267,1,11267,2],[11268,1,11268,2],[11269,1,11269,2],[11270,1,11270,2],[11271,1,11271,2],[11272,1,11272,2],[11273,1,11273,2],[11274,1,11274,2],[11275,1,11275,2],[11276,1,11276,2],[11277,1,11277,2],[11278,1,11278,2],[11279,1,11279,2],[11280,1,11280,2],[11311,1,11311,2],[11312,1,11312,2],[11313,1,11313,2],[11253,1,11253,2],[11254,1,11254,2],[11255,1,11255,2],[11256,1,11256,2],[11257,1,11257,2],[11258,1,11258,2],[11259,1,11259,2],[11260,1,11260,2],[11261,1,11261,2],[11262,1,11262,2],[11307,1,11307,2],[11308,1,11308,2],[11309,1,11309,2],[11310,1,11310,2],[11301,1,11301,2],[11302,1,11302,2],[11303,1,11303,2],[11304,1,11304,2],[11305,1,11305,2],[11314,1,11314,2],[11315,1,11315,2],[11316,1,11316,2],[11317,1,11317,2],[11318,1,11318,2],[11319,1,11319,2],[11320,1,11320,2],[11281,1,11281,2],[11214,1,11214,2],[11217,1,11217,2],[11218,1,11218,2],[11219,1,11219,2],[11220,1,11220,2],[11221,1,11221,2],[11222,1,11222,2],[11223,1,11223,2],[11224,1,11224,2],[11225,1,11225,2],[11226,1,11226,2],[11227,1,11227,2],[11228,1,11228,2],[11229,1,11229,2],[11230,1,11230,2],[11231,1,11231,2],[11232,1,11232,2],[11248,1,11248,2],[11249,1,11249,2],[11235,1,11235,2],[11236,1,11236,2],[11237,1,11237,2],[11238,1,11238,2],[11239,1,11239,2],[11240,1,11240,2],[11241,1,11241,2],[11242,1,11242,2],[11243,1,11243,2],[11244,1,11244,2],[11245,1,11245,2],[11246,1,11246,2],[11247,1,11247,2],[11293,1,11293,2],[11250,1,11250,2],[11251,1,11251,2],[11252,1,11252,2],[11282,1,11282,2],[11283,1,11283,2],[11284,1,11284,2],[11285,1,11285,2],[11286,1,11286,2],[11287,1,11287,2],[11294,1,11294,2],[11295,1,11295,2],[11296,1,11296,2],[11297,1,11297,2],[11288,1,11288,2],[11306,1,11306,2],[11289,1,11289,2],[11290,1,11290,2],[11291,1,11291,2],[11292,1,11292,2],[11299,1,11299,2],[11300,1,11300,2],[11298,1,11298,2],[11266,1,11266,2],[11185,1,11185,2],[11186,1,11186,2],[11187,1,11187,2],[11188,1,11188,2],[11189,1,11189,2],[11190,1,11190,2],[11191,1,11191,2],[11141,1,11141,2],[11142,1,11142,2],[11143,1,11143,2],[11144,1,11144,2],[11145,1,11145,2],[11197,1,11197,2],[11198,1,11198,2],[11199,1,11199,2],[11200,1,11200,2],[11201,1,11201,2],[11192,1,11192,2],[11193,1,11193,2],[11194,1,11194,2],[11195,1,11195,2],[11196,1,11196,2],[11263,1,11263,2],[11264,1,11264,2],[11265,1,11265,2],[11158,1,11158,2],[11159,1,11159,2],[11160,1,11160,2],[11161,1,11161,2],[11162,1,11162,2],[11163,1,11163,2],[11164,1,11164,2],[11202,1,11202,2],[11203,1,11203,2],[11204,1,11204,2],[11205,1,11205,2],[11206,1,11206,2],[11215,1,11215,2],[11216,1,11216,2],[11207,1,11207,2],[11208,1,11208,2],[11209,1,11209,2],[11210,1,11210,2],[11211,1,11211,2],[11212,1,11212,2],[11213,1,11213,2],[11111,1,11111,2],[11112,1,11112,2],[11113,1,11113,2],[11114,1,11114,2],[11115,1,11115,2],[11116,1,11116,2],[11117,1,11117,2],[11118,1,11118,2],[11119,1,11119,2],[11120,1,11120,2],[11121,1,11121,2],[11122,1,11122,2],[11123,1,11123,2],[11124,1,11124,2],[11125,1,11125,2],[11126,1,11126,2],[11127,1,11127,2],[11128,1,11128,2],[11129,1,11129,2],[11130,1,11130,2],[11131,1,11131,2],[11132,1,11132,2],[11133,1,11133,2],[11134,1,11134,2],[11135,1,11135,2],[11233,1,11233,2],[11234,1,11234,2],[11169,1,11169,2],[11170,1,11170,2],[11171,1,11171,2],[11172,1,11172,2],[11173,1,11173,2],[11174,1,11174,2],[11175,1,11175,2],[11176,1,11176,2],[11177,1,11177,2],[11178,1,11178,2],[11179,1,11179,2],[11180,1,11180,2],[11181,1,11181,2],[11146,1,11146,2],[11147,1,11147,2],[11148,1,11148,2],[11149,1,11149,2],[11150,1,11150,2],[11151,1,11151,2],[11152,1,11152,2],[11153,1,11153,2],[11154,1,11154,2],[11155,1,11155,2],[11136,1,11136,2],[11137,1,11137,2],[11138,1,11138,2],[11139,1,11139,2],[11140,1,11140,2],[11156,1,11156,2],[11157,1,11157,2],[11165,1,11165,2],[11166,1,11166,2],[11167,1,11167,2],[11168,1,11168,2],[11182,1,11182,2],[11183,1,11183,2],[11184,1,11184,2],[11063,1,11063,2],[11064,1,11064,2],[11065,1,11065,2],[11078,1,11078,2],[11079,1,11079,2],[11066,1,11066,2],[11067,1,11067,2],[11068,1,11068,2],[11069,1,11069,2],[11070,1,11070,2],[11071,1,11071,2],[11072,1,11072,2],[11107,1,11107,2],[11108,1,11108,2],[11109,1,11109,2],[11110,1,11110,2],[11103,1,11103,2],[11104,1,11104,2],[11105,1,11105,2],[11106,1,11106,2],[11090,1,11090,2],[11091,1,11091,2],[11092,1,11092,2],[11093,1,11093,2],[11094,1,11094,2],[11095,1,11095,2],[11096,1,11096,2],[11097,1,11097,2],[11098,1,11098,2],[11099,1,11099,2],[11100,1,11100,2],[11101,1,11101,2],[11102,1,11102,2],[11014,2,11015,2],[11014,3,11015,3],[11021,5,11021,11],[11023,1,11023,2],[11024,1,11024,2],[11025,1,11025,2],[11026,1,11026,2],[11027,1,11027,2],[11028,1,11028,2],[11029,1,11029,2],[11030,1,11030,2],[11031,1,11031,2],[11032,1,11032,2],[10962,2,10963,2],[10962,3,10963,3],[10964,2,10965,2],[10964,3,10965,3],[10956,2,10957,2],[10956,3,10957,3],[10958,2,10959,2],[10958,3,10959,3],[10960,2,10961,2],[10960,3,10961,3],[11080,1,11080,2],[11081,1,11081,2],[11082,1,11082,2],[11083,1,11083,2],[11084,1,11084,2],[11085,1,11085,2],[11086,1,11086,2],[11087,1,11087,2],[11088,1,11088,2],[11089,1,11089,2],[11076,5,11076,11],[11033,1,11033,2],[11034,1,11034,2],[11035,1,11035,2],[11036,1,11036,2],[11037,1,11037,2],[11038,1,11038,2],[11039,1,11039,2],[11040,1,11040,2],[11041,1,11041,2],[11042,1,11042,2],[11043,1,11043,2],[11044,1,11044,2],[11045,1,11045,2],[11046,1,11046,2],[11047,1,11047,2],[11048,1,11048,2],[11049,1,11049,2],[11050,1,11050,2],[11051,1,11051,2],[11052,1,11052,2],[11053,1,11053,2],[11054,1,11054,2],[11055,1,11055,2],[11056,1,11056,2],[11057,1,11057,2],[11058,1,11058,2],[11059,1,11059,2],[11060,1,11060,2],[11061,1,11061,2],[11062,1,11062,2],[10942,2,10943,2],[10942,3,10943,3],[10944,2,10945,2],[10944,3,10945,3],[10946,2,10947,2],[10946,3,10947,3],[10948,2,10949,2],[10948,3,10949,3],[10950,2,10951,2],[10950,3,10951,3],[10952,2,10953,2],[10952,3,10953,3],[10954,2,10955,2],[10954,3,10955,3],[10994,2,10995,2],[10994,3,10995,3],[10996,2,10997,2],[10996,3,10997,3],[10998,2,10999,2],[10998,3,10999,3],[11000,2,11001,2],[11000,3,11001,3],[11002,2,11003,2],[11002,3,11003,3],[11004,2,11005,2],[11004,3,11005,3],[11006,2,11007,2],[11006,3,11007,3],[11008,2,11009,2],[11008,3,11009,3],[11010,2,11011,2],[11010,3,11011,3],[11012,2,11013,2],[11012,3,11013,3],[10906,2,10907,2],[10906,3,10907,3],[10908,2,10909,2],[10908,3,10909,3],[10910,2,10911,2],[10910,3,10911,3],[10912,2,10913,2],[10912,3,10913,3],[10914,2,10915,2],[10914,3,10915,3],[10916,2,10917,2],[10916,3,10917,3],[10918,2,10919,2],[10918,3,10919,3],[10920,2,10921,2],[10920,3,10921,3],[10966,2,10967,2],[10966,3,10967,3],[10968,2,10969,2],[10968,3,10969,3],[10970,2,10971,2],[10970,3,10971,3],[10972,2,10973,2],[10972,3,10973,3],[10974,2,10975,2],[10974,3,10975,3],[10976,2,10977,2],[10976,3,10977,3],[10992,2,10993,2],[10992,3,10993,3],[10926,2,10927,2],[10926,3,10927,3],[10928,2,10929,2],[10928,3,10929,3],[10930,2,10931,2],[10930,3,10931,3],[10932,2,10933,2],[10932,3,10933,3],[10934,2,10935,2],[10934,3,10935,3],[10936,2,10937,2],[10936,3,10937,3],[10984,2,10985,2],[10984,3,10985,3],[10922,2,10923,2],[10922,3,10923,3],[10924,2,10925,2],[10924,3,10925,3],[10990,2,10991,2],[10990,3,10991,3],[10986,2,10987,2],[10986,3,10987,3],[10988,2,10989,2],[10988,3,10989,3],[10978,2,10979,2],[10978,3,10979,3],[10980,2,10981,2],[10980,3,10981,3],[10982,2,10983,2],[10982,3,10983,3],[10938,2,10939,2],[10938,3,10939,3],[10940,2,10941,2],[10940,3,10941,3],[10872,2,10873,2],[10872,3,10873,3],[10874,2,10875,2],[10874,3,10875,3],[10876,2,10877,2],[10876,3,10877,3],[10878,2,10879,2],[10878,3,10879,3],[10880,2,10881,2],[10880,3,10881,3],[10900,2,10901,2],[10900,3,10901,3],[10902,2,10903,2],[10902,3,10903,3],[10882,2,10883,2],[10882,3,10883,3],[10884,2,10885,2],[10884,3,10885,3],[10886,2,10887,2],[10886,3,10887,3],[10894,2,10895,2],[10894,3,10895,3],[10896,2,10897,2],[10896,3,10897,3],[10898,2,10899,2],[10898,3,10899,3],[10888,2,10889,2],[10888,3,10889,3],[10890,2,10891,2],[10890,3,10891,3],[10892,2,10893,2],[10892,3,10893,3],[10904,2,10905,2],[10904,3,10905,3],[10838,2,10839,2],[10838,3,10839,3],[10840,2,10841,2],[10840,3,10841,3],[10842,2,10843,2],[10842,3,10843,3],[10844,2,10845,2],[10844,3,10845,3],[10846,2,10847,2],[10846,3,10847,3],[10866,2,10867,2],[10866,3,10867,3],[10868,2,10869,2],[10868,3,10869,3],[10848,2,10849,2],[10848,3,10849,3],[10850,2,10851,2],[10850,3,10851,3],[10852,2,10853,2],[10852,3,10853,3],[10860,2,10861,2],[10860,3,10861,3],[10862,2,10863,2],[10862,3,10863,3],[10864,2,10865,2],[10864,3,10865,3],[10854,2,10855,2],[10854,3,10855,3],[10856,2,10857,2],[10856,3,10857,3],[10858,2,10859,2],[10858,3,10859,3],[10870,2,10871,2],[10870,3,10871,3],[10804,2,10805,2],[10804,3,10805,3],[10806,2,10807,2],[10806,3,10807,3],[10808,2,10809,2],[10808,3,10809,3],[10810,2,10811,2],[10810,3,10811,3],[10812,2,10813,2],[10812,3,10813,3],[10832,2,10833,2],[10832,3,10833,3],[10834,2,10835,2],[10834,3,10835,3],[10814,2,10815,2],[10814,3,10815,3],[10816,2,10817,2],[10816,3,10817,3],[10818,2,10819,2],[10818,3,10819,3],[10826,2,10827,2],[10826,3,10827,3],[10828,2,10829,2],[10828,3,10829,3],[10830,2,10831,2],[10830,3,10831,3],[10820,2,10821,2],[10820,3,10821,3],[10822,2,10823,2],[10822,3,10823,3],[10824,2,10825,2],[10824,3,10825,3],[10836,2,10837,2],[10836,3,10837,3],[10770,2,10771,2],[10770,3,10771,3],[10772,2,10773,2],[10772,3,10773,3],[10774,2,10775,2],[10774,3,10775,3],[10776,2,10777,2],[10776,3,10777,3],[10778,2,10779,2],[10778,3,10779,3],[10798,2,10799,2],[10798,3,10799,3],[10800,2,10801,2],[10800,3,10801,3],[10780,2,10781,2],[10780,3,10781,3],[10782,2,10783,2],[10782,3,10783,3],[10784,2,10785,2],[10784,3,10785,3],[10792,2,10793,2],[10792,3,10793,3],[10794,2,10795,2],[10794,3,10795,3],[10796,2,10797,2],[10796,3,10797,3],[10786,2,10787,2],[10786,3,10787,3],[10788,2,10789,2],[10788,3,10789,3],[10790,2,10791,2],[10790,3,10791,3],[10802,2,10803,2],[10802,3,10803,3],[10736,2,10737,2],[10736,3,10737,3],[10738,2,10739,2],[10738,3,10739,3],[10740,2,10741,2],[10740,3,10741,3],[10742,2,10743,2],[10742,3,10743,3],[10744,2,10745,2],[10744,3,10745,3],[10764,2,10765,2],[10764,3,10765,3],[10766,2,10767,2],[10766,3,10767,3],[10746,2,10747,2],[10746,3,10747,3],[10748,2,10749,2],[10748,3,10749,3],[10750,2,10751,2],[10750,3,10751,3],[10758,2,10759,2],[10758,3,10759,3],[10760,2,10761,2],[10760,3,10761,3],[10762,2,10763,2],[10762,3,10763,3],[10752,2,10753,2],[10752,3,10753,3],[10754,2,10755,2],[10754,3,10755,3],[10756,2,10757,2],[10756,3,10757,3],[10768,2,10769,2],[10768,3,10769,3],[10702,2,10703,2],[10702,3,10703,3],[10704,2,10705,2],[10704,3,10705,3],[10706,2,10707,2],[10706,3,10707,3],[10708,2,10709,2],[10708,3,10709,3],[10710,2,10711,2],[10710,3,10711,3],[10730,2,10731,2],[10730,3,10731,3],[10732,2,10733,2],[10732,3,10733,3],[10712,2,10713,2],[10712,3,10713,3],[10714,2,10715,2],[10714,3,10715,3],[10716,2,10717,2],[10716,3,10717,3],[10724,2,10725,2],[10724,3,10725,3],[10726,2,10727,2],[10726,3,10727,3],[10728,2,10729,2],[10728,3,10729,3],[10718,2,10719,2],[10718,3,10719,3],[10720,2,10721,2],[10720,3,10721,3],[10722,2,10723,2],[10722,3,10723,3],[10734,2,10735,2],[10734,3,10735,3],[10668,2,10669,2],[10668,3,10669,3],[10670,2,10671,2],[10670,3,10671,3],[10672,2,10673,2],[10672,3,10673,3],[10674,2,10675,2],[10674,3,10675,3],[10676,2,10677,2],[10676,3,10677,3],[10696,2,10697,2],[10696,3,10697,3],[10698,2,10699,2],[10698,3,10699,3],[10678,2,10679,2],[10678,3,10679,3],[10680,2,10681,2],[10680,3,10681,3],[10682,2,10683,2],[10682,3,10683,3],[10690,2,10691,2],[10690,3,10691,3],[10692,2,10693,2],[10692,3,10693,3],[10694,2,10695,2],[10694,3,10695,3],[10684,2,10685,2],[10684,3,10685,3],[10686,2,10687,2],[10686,3,10687,3],[10688,2,10689,2],[10688,3,10689,3],[10700,2,10701,2],[10700,3,10701,3],[10634,2,10635,2],[10634,3,10635,3],[10636,2,10637,2],[10636,3,10637,3],[10638,2,10639,2],[10638,3,10639,3],[10640,2,10641,2],[10640,3,10641,3],[10642,2,10643,2],[10642,3,10643,3],[10662,2,10663,2],[10662,3,10663,3],[10664,2,10665,2],[10664,3,10665,3],[10644,2,10645,2],[10644,3,10645,3],[10646,2,10647,2],[10646,3,10647,3],[10648,2,10649,2],[10648,3,10649,3],[10656,2,10657,2],[10656,3,10657,3],[10658,2,10659,2],[10658,3,10659,3],[10660,2,10661,2],[10660,3,10661,3],[10650,2,10651,2],[10650,3,10651,3],[10652,2,10653,2],[10652,3,10653,3],[10654,2,10655,2],[10654,3,10655,3],[10666,2,10667,2],[10666,3,10667,3],[10600,2,10601,2],[10600,3,10601,3],[10602,2,10603,2],[10602,3,10603,3],[10604,2,10605,2],[10604,3,10605,3],[10606,2,10607,2],[10606,3,10607,3],[10608,2,10609,2],[10608,3,10609,3],[10628,2,10629,2],[10628,3,10629,3],[10630,2,10631,2],[10630,3,10631,3],[10610,2,10611,2],[10610,3,10611,3],[10612,2,10613,2],[10612,3,10613,3],[10614,2,10615,2],[10614,3,10615,3],[10622,2,10623,2],[10622,3,10623,3],[10624,2,10625,2],[10624,3,10625,3],[10626,2,10627,2],[10626,3,10627,3],[10616,2,10617,2],[10616,3,10617,3],[10618,2,10619,2],[10618,3,10619,3],[10620,2,10621,2],[10620,3,10621,3],[10632,2,10633,2],[10632,3,10633,3],[10566,2,10567,2],[10566,3,10567,3],[10568,2,10569,2],[10568,3,10569,3],[10570,2,10571,2],[10570,3,10571,3],[10572,2,10573,2],[10572,3,10573,3],[10574,2,10575,2],[10574,3,10575,3],[10594,2,10595,2],[10594,3,10595,3],[10596,2,10597,2],[10596,3,10597,3],[10576,2,10577,2],[10576,3,10577,3],[10578,2,10579,2],[10578,3,10579,3],[10580,2,10581,2],[10580,3,10581,3],[10588,2,10589,2],[10588,3,10589,3],[10590,2,10591,2],[10590,3,10591,3],[10592,2,10593,2],[10592,3,10593,3],[10582,2,10583,2],[10582,3,10583,3],[10584,2,10585,2],[10584,3,10585,3],[10586,2,10587,2]],"merged_total":11555,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"DEMAND"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Alexandria 132_33kV","Substation Rating","MVA","Non-Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,null,null,"Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.369999999999997,55.64,57.47,61.6,66.64,73.98,73.98]
[null,null,null,null,"Coincident",18.57,26.93,27.82,29.81,32.25,35.799999999999997,35.799999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.37,61.55,63.59,68.17,73.77,81.92,81.92]
[null,null,null,null,"Coincident",20.51,29.79,30.78,32.99,35.71,39.65,39.65]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.47,54.74,56.57,60.7,65.739999999999995,73.08,73.08]
[null,null,null,null,"Coincident",18.14,26.49,27.38,29.38,31.82,35.369999999999997,35.369999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.55,60.74,62.78,67.36,72.959999999999994,81.11,81.11]
[null,null,null,null,"Coincident",20.11,29.4,30.38,32.6,35.31,39.26,39.26]
[null,"Argenton 132_33kV","Substation Rating","MVA","Non-Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,null,null,"Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-6.2009999999999996,-6.9189999999999996,-7.3920000000000003,-7.726,-8.0820000000000007,-8.4190000000000005,-8.7449999999999992]
[null,null,null,null,"Coincident",-6.032,-7.8840000000000003,-9.0210000000000008,-9.6880000000000006,-10.3,-10.92,-11.52]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",111.2,110.1,109.6,109.5,109.3,109.1,109]
[null,null,null,null,"Coincident",101.9,100.9,100.4,100.3,100.1,99.95,99.85]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",113.4,112.3,111.8,111.7,111.4,111.3,111.1]
[null,null,null,null,"Coincident",103.9,102.9,102.4,102.3,102.1,101.9,101.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",95.19,94.27,93.81,93.72,93.49,93.32,93.21]
[null,null,null,null,"Coincident",87.21,86.36,85.94,85.85,85.65,85.49,85.39]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",97.77,96.82,96.35,96.25,96.01,95.84,95.73]
[null,null,null,null,"Coincident",89.57,88.7,88.27,88.18,87.96,87.8,87.7]
[null,"Awaba 132_33kV","Substation Rating","MVA","Non-Coincident",68.59,68.59,68.59,68.59,68.59,68.59,68.59]
[null,null,null,null,"Coincident",68.59,68.59,68.59,68.59,68.59,68.59,68.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident",-1.6120000000000001,-1.6120000000000001,-1.6120000000000001,-1.6120000000000001,-1.6120000000000001,-1.6120000000000001,-1.6120000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.22,14.22,14.22,14.22,14.22,14.22,14.22]
[null,null,null,null,"Coincident",6.69,6.69,6.69,6.69,6.69,6.69,6.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.01,15.01,15.01,15.01,15.01,15.01,15.01]
[null,null,null,null,"Coincident",6.9770000000000003,6.9770000000000003,6.9770000000000003,6.9770000000000003,6.9770000000000003,6.9770000000000003,6.9770000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.67,13.67,13.67,13.67,13.67,13.67,13.67]
[null,null,null,null,"Coincident",6.4029999999999996,6.4029999999999996,6.4029999999999996,6.4029999999999996,6.4029999999999996,6.4029999999999996,6.4029999999999996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.43,14.43,14.43,14.43,14.43,14.43,14.43]
[null,null,null,null,"Coincident",6.6779999999999999,6.6779999999999999,6.6779999999999999,6.6779999999999999,6.6779999999999999,6.6779999999999999,6.6779999999999999]
[null,"Bankstown 132_33kV","Substation Rating","MVA","Non-Coincident",139.4,139.4,139.4,139.4,139.4,139.4,139.4]
[null,null,null,null,"Coincident",139.4,139.4,139.4,139.4,139.4,139.4,139.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.56200000000000006,-1.206,-0.73699999999999999,-0.78200000000000003,-0.84199999999999997,-1.002,-1.151]
[null,null,null,null,"Coincident",-3.6280000000000001,-4.7149999999999999,-5.46,-6.0090000000000003,-6.6070000000000002,-7.2039999999999997,-7.7919999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",72.87,73.849999999999994,74.400000000000006,74.7,74.83,75.180000000000007,75.25]
[null,null,null,null,"Coincident",68.8,69.73,70.25,70.53,70.66,70.98,71.06]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.739999999999995,74.78,75.37,75.680000000000007,75.819999999999993,76.19,76.28]
[null,null,null,null,"Coincident",69.62,70.61,71.16,71.459999999999994,71.599999999999994,71.95,72.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",65.48,66.47,67.03,67.33,67.459999999999994,67.81,67.88]
[null,null,null,null,"Coincident",61.83,62.76,63.29,63.57,63.7,64.02,64.099999999999994]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",65.930000000000007,66.97,67.56,67.87,68.010000000000005,68.38,68.459999999999994]
[null,null,null,null,"Coincident",62.26,63.24,63.79,64.09,64.22,64.569999999999993,64.64]
[null,"Beresfield 132_33kV","Substation Rating","MVA","Non-Coincident",150.1,150.1,150.1,150.1,150.1,150.1,150.1]
[null,null,null,null,"Coincident",150.1,150.1,150.1,150.1,150.1,150.1,150.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.56499999999999995,-1.1950000000000001,-1.919,-1.9450000000000001,-2.2949999999999999,-2.6259999999999999,-3.4089999999999998]
[null,null,null,null,"Coincident",-5.5380000000000003,-7.2229999999999999,-8.2810000000000006,-8.9390000000000001,-9.5719999999999992,-10.199999999999999,-10.83]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",116.5,102.9,104.8,106.3,110.4,115.8,117.7]
[null,null,null,null,"Coincident",107.6,95,96.78,98.1,101.9,106.9,108.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",116.5,106.8,108.8,110.3,110.4,115.8,117.7]
[null,null,null,null,"Coincident",107.6,98.62,100.5,101.8,101.9,106.9,108.7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",104.9,91.36,93.32,94.75,98.9,104.3,106.2]
[null,null,null,null,"Coincident",96.85,84.35,86.16,87.48,91.32,96.3,98.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",108.9,94.83,96.86,98.35,102.7,108.3,110.2]
[null,null,null,null,"Coincident",100.5,87.56,89.44,90.81,94.79,99.97,101.7]
[null,"Bunnerong North 132_33kV","Substation Rating","MVA","Non-Coincident",312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002]
[null,null,null,null,"Coincident",312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002,312.60000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.5999999999999996,-5.4960000000000004,-6.2640000000000002,-7.0229999999999997,-7.9509999999999996,-8.1199999999999992,-8.2200000000000006]
[null,null,null,null,"Coincident",-4.2850000000000001,-5.5179999999999998,-6.4470000000000001,-7.2510000000000003,-8.1920000000000002,-9.1340000000000003,-10.06]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",191.4,191.9,192.1,192.2,193.5,194.8,194.8]
[null,null,null,null,"Coincident",184.1,184.6,184.8,185,186.1,187.4,187.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",191.4,191.9,192.1,192.3,193.5,194.8,194.9]
[null,null,null,null,"Coincident",184.1,184.6,184.8,185,186.1,187.4,187.5]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",182.7,183.2,183.5,183.6,184.8,186.1,186.2]
[null,null,null,null,"Coincident",175.8,176.3,176.5,176.6,177.8,179.1,179.1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",182.7,183.2,183.5,183.6,184.8,186.2,186.2]
[null,null,null,null,"Coincident",175.8,176.3,176.5,176.6,177.8,179.1,179.2]
[null,"Canterbury 132_33kV","Substation Rating","MVA","Non-Coincident",186.6,186.6,186.6,186.6,186.6,186.6,186.6]
[null,null,null,null,"Coincident",186.6,186.6,186.6,186.6,186.6,186.6,186.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.504,-2.6059999999999999,-2.7130000000000001,-2.851,-3.032,-3.198,-3.347]
[null,null,null,null,"Coincident",-9.1329999999999991,-11.86,-13.76,-15.19,-16.77,-18.350000000000001,-19.899999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",154,156.30000000000001,157.80000000000001,165.7,166.2,167,167.5]
[null,null,null,null,"Coincident",150.30000000000001,152.6,154,161.69999999999999,162.19999999999999,163,163.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",154,156.4,157.9,165.9,166.4,167.3,167.8]
[null,null,null,null,"Coincident",150.30000000000001,152.6,154.1,161.9,162.4,163.30000000000001,163.80000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",140.19999999999999,142.5,143.9,151.80000000000001,152.30000000000001,153.19999999999999,153.69999999999999]
[null,null,null,null,"Coincident",136.80000000000001,139,140.5,148.19999999999999,148.69999999999999,149.5,150]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",141.6,144,145.6,151.80000000000001,152.30000000000001,153.19999999999999,153.69999999999999]
[null,null,null,null,"Coincident",138.19999999999999,140.5,142.1,148.19999999999999,148.69999999999999,149.5,150]
[null,"Eraring 132_33kV","Substation Rating","MVA","Non-Coincident",57.16,57.16,57.16,57.16,57.16,57.16,57.16]
[null,null,null,null,"Coincident",57.16,57.16,57.16,57.16,57.16,57.16,57.16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.61799999999999999,-0.69199999999999995,-0.74199999999999999,-0.77900000000000003,-0.81899999999999995,-0.85699999999999998,-0.89300000000000002]
[null,null,null,null,"Coincident",-0.79600000000000004,-1.04,-1.1910000000000001,-1.2809999999999999,-1.3640000000000001,-1.448,-1.5309999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.12,20.2,20.23,20.22,20.18,20.14,20.07]
[null,null,null,null,"Coincident",17.38,17.45,17.48,17.47,17.440000000000001,17.399999999999999,17.34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.45,20.54,20.57,20.55,20.52,20.47,20.41]
[null,null,null,null,"Coincident",17.670000000000002,17.739999999999998,17.77,17.760000000000002,17.73,17.690000000000001,17.63]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.93,19.010000000000002,19.03,19.02,18.989999999999998,18.940000000000001,18.88]
[null,null,null,null,"Coincident",16.350000000000001,16.420000000000002,16.440000000000001,16.43,16.399999999999999,16.36,16.309999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.28,19.36,19.39,19.38,19.34,19.3,19.23]
[null,null,null,null,"Coincident",16.66,16.73,16.75,16.739999999999998,16.71,16.670000000000002,16.61]
[null,"Gosford 132_33kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.08,-1.28,-1.4350000000000001,-1.5429999999999999,-1.659,-1.645,-1.603]
[null,null,null,null,"Coincident",-1.583,-2.0720000000000001,-2.3740000000000001,-2.5529999999999999,-2.7210000000000001,-2.89,-3.056]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.83,29.65,29.74,30.22,30.74,30.98,31.01]
[null,null,null,null,"Coincident",22.12,21.99,22.05,22.41,22.8,22.97,23]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.17,29.99,30.08,30.57,31.1,31.34,31.37]
[null,null,null,null,"Coincident",22.37,22.24,22.3,22.67,23.06,23.24,23.26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.02,25.9,26.02,26.5,27.02,27.26,27.29]
[null,null,null,null,"Coincident",19.3,19.21,19.29,19.649999999999999,20.04,20.21,20.239999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.41,26.29,26.41,26.89,27.43,27.67,27.7]
[null,null,null,null,"Coincident",19.579999999999998,19.489999999999998,19.579999999999998,19.940000000000001,20.34,20.52,20.54]
[null,"Gosford 132_66kV","Substation Rating","MVA","Non-Coincident",225.4,225.4,225.4,225.4,225.4,225.4,225.4]
[null,null,null,null,"Coincident",225.4,225.4,225.4,225.4,225.4,225.4,225.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-7.4039999999999999,-8.7880000000000003,-9.141,-9.86,-10.34,-11.06,-11.76]
[null,null,null,null,"Coincident",-10.62,-13.87,-15.93,-17.23,-18.5,-19.78,-21.03]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",156.5,157.5,157.80000000000001,158.1,157.9,157.6,157.1]
[null,null,null,null,"Coincident",149.80000000000001,150.69999999999999,150.9,151.30000000000001,151.1,150.80000000000001,150.30000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",156.6,157.6,157.9,158.19999999999999,158,157.69999999999999,157.1]
[null,null,null,null,"Coincident",149.80000000000001,150.80000000000001,151,151.30000000000001,151.19999999999999,150.9,150.30000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",134.9,135.9,136,136.4,136.19999999999999,135.9,135.30000000000001]
[null,null,null,null,"Coincident",129.1,130,130.1,130.5,130.30000000000001,130,129.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",135,135.9,136.1,136.4,136.19999999999999,135.9,135.4]
[null,null,null,null,"Coincident",129.19999999999999,130,130.19999999999999,130.5,130.30000000000001,130,129.5]
[null,"Homebush 132_33kV","Substation Rating","MVA","Non-Coincident",285.8,285.8,285.8,285.8,285.8,285.8,285.8]
[null,null,null,null,"Coincident",280.5,280.5,280.5,280.5,280.5,280.5,280.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.14199999999999999,-0.29499999999999998,-0.442,-0.60299999999999998,-0.82299999999999995,-1.024,-1.2110000000000001]
[null,null,null,null,"Coincident",-3.3130000000000002,-4.258,-4.992,-5.6539999999999999,-6.444,-7.234,-8.0079999999999991]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.69,58.1,58.45,69.62,71.13,71.69,72.260000000000005]
[null,null,null,null,"Coincident",45.51,48.17,58.47,59.46,59.66,59.82,59.81]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.76,58.18,58.53,69.709999999999994,71.22,71.78,72.349999999999994]
[null,null,null,null,"Coincident",48.16,51.14,62.58,59.46,59.66,59.82,59.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",53.02,56.84,57.48,68.790000000000006,70.3,70.86,71.430000000000007]
[null,null,null,null,"Coincident",38.840000000000003,41.56,51.88,52.88,53.07,53.24,53.23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",53.08,56.91,57.55,68.87,70.39,70.95,71.52]
[null,null,null,null,"Coincident",41.5,44.54,56.04,57.14,57.36,57.55,57.53]
[null,"Kooragang 132_33kV","Substation Rating","MVA","Non-Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,null,null,"Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident",-10.79,-10.79,-10.79,-10.79,-10.79,-10.79,-10.79]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",71.66,71.66,71.66,71.66,71.66,71.66,71.66]
[null,null,null,null,"Coincident",41.75,41.75,41.75,41.75,41.75,41.75,41.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",74.45,74.45,74.45,74.45,74.45,74.45,74.45]
[null,null,null,null,"Coincident",44.69,44.69,44.69,44.69,44.69,44.69,44.69]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",68.260000000000005,68.260000000000005,68.260000000000005,68.260000000000005,68.260000000000005,68.260000000000005,68.260000000000005]
[null,null,null,null,"Coincident",40.93,40.93,40.93,40.93,40.93,40.93,40.93]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",71.180000000000007,71.180000000000007,71.180000000000007,71.180000000000007,71.180000000000007,71.180000000000007,71.180000000000007]
[null,null,null,null,"Coincident",43.91,43.91,43.91,43.91,43.91,43.91,43.91]
[null,"Kuring-gai 132_33kV","Substation Rating","MVA","Non-Coincident",274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998]
[null,null,null,null,"Coincident",260.89999999999998,260.89999999999998,260.89999999999998,260.89999999999998,260.89999999999998,260.89999999999998,260.89999999999998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.184,-0.36799999999999999,-0.55100000000000005,-0.78300000000000003,-1.0880000000000001,-1.371,-1.6220000000000001]
[null,null,null,null,"Coincident",-9.5749999999999993,-12.62,-14.55,-15.76,-16.95,-18.14,-19.309999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",147.4,149.80000000000001,150.9,151.30000000000001,151.69999999999999,152,152.1]
[null,null,null,null,"Coincident",152,154.19999999999999,155.19999999999999,155.6,155.9,155.80000000000001,155.80000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",149.30000000000001,151.69999999999999,152.80000000000001,153.19999999999999,153.69999999999999,153.9,154]
[null,null,null,null,"Coincident",169,171.5,172.7,173.1,173.5,173.4,173.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",140.9,143.69999999999999,145.19999999999999,145.69999999999999,146.19999999999999,146.4,146.5]
[null,null,null,null,"Coincident",132.5,134.6,135.6,135.9,136.19999999999999,136.19999999999999,136.1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",142.69999999999999,145.5,147,147.6,148,148.30000000000001,148.4]
[null,null,null,null,"Coincident",147.4,149.69999999999999,150.9,151.30000000000001,151.6,151.6,151.5]
[null,"Kurri 132_33kV","Substation Rating","MVA","Non-Coincident",156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999]
[null,null,null,null,"Coincident",156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999,156.19999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.325,-2.1589999999999998,-2.7330000000000001,-3.1619999999999999,-3.63,-4.07,-4.33]
[null,null,null,null,"Coincident",-7.19,-9.3930000000000007,-10.78,-11.64,-12.48,-13.31,-14.13]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",152.9,152.6,152.4,153.80000000000001,153.9,154.1,154.1]
[null,null,null,null,"Coincident",138.1,137.80000000000001,137.6,138.9,139,139.1,139.19999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",153.6,153.30000000000001,153.1,154.6,154.69999999999999,154.80000000000001,154.9]
[null,null,null,null,"Coincident",138.69999999999999,138.4,138.19999999999999,139.5,139.6,139.80000000000001,139.80000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",136.80000000000001,136.6,136.4,137.80000000000001,137.9,138.1,138.19999999999999]
[null,null,null,null,"Coincident",123.5,123.3,123.1,124.4,124.5,124.7,124.7]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",137.19999999999999,136.9,136.69999999999999,138.19999999999999,138.30000000000001,138.5,138.5]
[null,null,null,null,"Coincident",123.8,123.6,123.4,124.7,124.8,125,125]
[null,"Macquarie 132_33kV","Substation Rating","MVA","Non-Coincident",142.9,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,null,null,"Coincident",null,142.9,142.9,142.9,142.9,142.9,142.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident",null,"Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.93,32.76,41.94,53.28,65.34,77.489999999999995,84.96]
[null,null,null,null,"Coincident",14.34,29.48,37.75,47.95,58.81,69.739999999999995,76.459999999999994]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.7,36.4,46.6,59.2,72.599999999999994,86.1,94.4]
[null,null,null,null,"Coincident",15.93,32.76,41.94,53.28,65.34,77.489999999999995,84.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.93,32.76,41.94,53.28,65.34,77.489999999999995,84.96]
[null,null,null,null,"Coincident",14.34,29.48,37.75,47.95,58.81,69.739999999999995,76.459999999999994]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.7,36.4,46.6,59.2,72.599999999999994,86.1,94.4]
[null,null,null,null,"Coincident",15.93,32.76,41.94,53.28,65.34,77.489999999999995,84.96]
[null,"Merewether 132_33kV","Substation Rating","MVA","Non-Coincident",274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998]
[null,null,null,null,"Coincident",274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998,274.39999999999998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.1859999999999999,-6.1070000000000002,-7.2839999999999998,-8.4540000000000006,-9.8379999999999992,-11.15,-12.42]
[null,null,null,null,"Coincident",-9.8379999999999992,-12.8,-14.78,-16.170000000000002,-17.64,-19.11,-20.55]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",185.2,184.4,184,183.6,183,182.6,181.6]
[null,null,null,null,"Coincident",182.7,181.9,181.5,181.1,180.5,180.1,179.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",186.2,185.4,185,184.6,184,183.5,182.6]
[null,null,null,null,"Coincident",183.7,182.9,182.5,182.1,181.5,181,180.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",158.9,158.30000000000001,157.9,157.5,156.9,156.5,155.5]
[null,null,null,null,"Coincident",156.80000000000001,156.1,155.80000000000001,155.4,154.80000000000001,154.30000000000001,153.4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",159.4,158.69999999999999,158.30000000000001,157.9,157.30000000000001,156.80000000000001,155.9]
[null,null,null,null,"Coincident",157.19999999999999,156.5,156.19999999999999,155.80000000000001,155.19999999999999,154.69999999999999,153.80000000000001]
[null,"Mitchell Line 132_66kV","Substation Rating","MVA","Non-Coincident",141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001]
[null,null,null,null,"Coincident",141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001,141.30000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.14499999999999999,-1.4E-2,-0.13300000000000001,-0.221,-0.33200000000000002,-0.44,-0.54100000000000004]
[null,null,null,null,"Coincident",-1.5509999999999999,-2.2480000000000002,-2.7029999999999998,-3.0139999999999998,-3.3279999999999998,-3.6419999999999999,-3.95]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",81.45,81.209999999999994,81.11,81.14,81.12,81.08,81.010000000000005]
[null,null,null,null,"Coincident",65.61,65.42,65.34,65.37,65.349999999999994,65.319999999999993,65.260000000000005]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",83.82,83.58,83.48,83.51,83.49,83.45,83.37]
[null,null,null,null,"Coincident",67.53,67.33,67.25,67.28,67.260000000000005,67.23,67.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",76.42,76.2,76.11,76.14,76.12,76.08,76.010000000000005]
[null,null,null,null,"Coincident",61.56,61.38,61.31,61.34,61.32,61.29,61.23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",78.95,78.72,78.63,78.66,78.64,78.599999999999994,78.52]
[null,null,null,null,"Coincident",63.6,63.42,63.34,63.37,63.35,63.32,63.26]
[null,"Morisset 132_33kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.72,21.72,21.72,21.72,21.72,21.72,21.72]
[null,null,null,null,"Coincident",8.2590000000000003,8.2590000000000003,8.2590000000000003,8.2590000000000003,8.2590000000000003,8.2590000000000003,8.2590000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.25,23.25,23.25,23.25,23.25,23.25,23.25]
[null,null,null,null,"Coincident",8.8420000000000005,8.8420000000000005,8.8420000000000005,8.8420000000000005,8.8420000000000005,8.8420000000000005,8.8420000000000005]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.55,19.55,19.55,19.55,19.55,19.55,19.55]
[null,null,null,null,"Coincident",7.4329999999999998,7.4329999999999998,7.4329999999999998,7.4329999999999998,7.4329999999999998,7.4329999999999998,7.4329999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.24,21.24,21.24,21.24,21.24,21.24,21.24]
[null,null,null,null,"Coincident",8.0749999999999993,8.0749999999999993,8.0749999999999993,8.0749999999999993,8.0749999999999993,8.0749999999999993,8.0749999999999993]
[null,"Munmorah 132_33kV","Substation Rating","MVA","Non-Coincident",80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995]
[null,null,null,null,"Coincident",80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995,80.989999999999995]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.1000000000000002E-2,-8.2000000000000003E-2,-0.122,-0.17299999999999999,-0.24,-0.30199999999999999,-0.35699999999999998]
[null,null,null,null,"Coincident",-2.246,-2.9380000000000002,-3.3679999999999999,-3.6280000000000001,-3.8730000000000002,-4.1189999999999998,-4.3609999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.2,25.82,26.11,26.28,26.35,26.44,26.43]
[null,null,null,null,"Coincident",30.03,22.98,23.16,23.2,23.27,23.25,23.19]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.45,28.12,28.43,28.62,28.69,28.78,28.77]
[null,null,null,null,"Coincident",31.78,24.29,24.48,24.52,24.6,24.57,24.51]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.54,24.16,24.45,24.62,24.69,24.78,24.77]
[null,null,null,null,"Coincident",26.84,19.739999999999998,19.899999999999999,19.940000000000001,20.010000000000002,19.989999999999998,19.93]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.94,26.61,26.92,27.11,27.18,27.28,27.27]
[null,null,null,null,"Coincident",28.78,21.25,21.41,21.46,21.53,21.51,21.45]
[null,"Muswellbrook 132_33kV","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.107,-0.22,-0.29699999999999999,-0.36499999999999999,-0.441,-0.51200000000000001,-0.57699999999999996]
[null,null,null,null,"Coincident",-1.133,-1.4730000000000001,-1.696,-1.8520000000000001,-2.0110000000000001,-2.1709999999999998,-2.3279999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.08,26.21,26.3,26.33,26.34,26.35,26.32]
[null,null,null,null,"Coincident",22.81,22.92,23,23.03,23.04,23.05,23.02]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.62,26.75,26.84,26.88,26.89,26.89,26.86]
[null,null,null,null,"Coincident",23.28,23.4,23.48,23.51,23.52,23.52,23.5]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.82,23.93,24.01,24.05,24.06,24.06,24.03]
[null,null,null,null,"Coincident",20.83,20.93,21.01,21.04,21.04,21.05,21.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.41,24.53,24.61,24.65,24.66,24.66,24.63]
[null,null,null,null,"Coincident",21.35,21.45,21.53,21.56,21.57,21.57,21.54]
[null,"Ourimbah 132_33kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.4E-2,-2.1999999999999999E-2,-0.03,-4.2000000000000003E-2,-5.6000000000000001E-2,-6.9000000000000006E-2,-0.08]
[null,null,null,null,"Coincident",-0.45200000000000001,-0.58899999999999997,-0.68600000000000005,-0.76200000000000001,-0.84499999999999997,-0.92900000000000005,-1.0109999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.79,13.58,13.52,13.62,13.7,13.8,13.85]
[null,null,null,null,"Coincident",11.52,11.35,11.3,11.39,11.45,11.53,11.57]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.83,14.61,14.54,14.66,14.74,14.85,14.9]
[null,null,null,null,"Coincident",12.4,12.21,12.15,12.25,12.32,12.41,12.45]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.59,12.41,12.36,12.46,12.54,12.64,12.69]
[null,null,null,null,"Coincident",10.53,10.37,10.33,10.42,10.48,10.57,10.61]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.55,13.35,13.29,13.41,13.5,13.6,13.65]
[null,null,null,null,"Coincident",11.32,11.16,11.11,11.21,11.28,11.37,11.41]
[null,"Ourimbah 132_66kV","Substation Rating","MVA","Non-Coincident",91.8,91.8,91.8,91.8,91.8,91.8,91.8]
[null,null,null,null,"Coincident",91.8,91.8,91.8,91.8,91.8,91.8,91.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-6.7000000000000004E-2,-0.13400000000000001,-0.20499999999999999,-0.29899999999999999,-0.42299999999999999,-0.53800000000000003,-0.64]
[null,null,null,null,"Coincident",-3.6589999999999998,-4.78,-5.4989999999999997,-5.9669999999999996,-6.4340000000000002,-6.9020000000000001,-7.3639999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.83,50.91,51.1,51.34,51.47,51.67,51.73]
[null,null,null,null,"Coincident",45.12,45.05,45.04,45,45.09,44.92,44.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.52,51.6,51.79,52.04,52.17,52.37,52.44]
[null,null,null,null,"Coincident",46.21,46.14,46.13,46.08,46.18,46,45.76]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.38,48.45,48.64,48.87,49,49.21,49.27]
[null,null,null,null,"Coincident",40.76,40.67,40.65,40.61,40.700000000000003,40.520000000000003,40.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.11,49.18,49.37,49.61,49.74,49.94,50.01]
[null,null,null,null,"Coincident",41.96,41.87,41.85,41.8,41.9,41.72,41.48]
[null,"Peakhurst 132_33kV","Substation Rating","MVA","Non-Coincident",233.2,233.2,233.2,233.2,233.2,233.2,233.2]
[null,null,null,null,"Coincident",233.2,233.2,233.2,233.2,233.2,233.2,233.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.14199999999999999,-0.28799999999999998,-0.45100000000000001,-0.67900000000000005,-0.98099999999999998,-1.26,-1.5089999999999999]
[null,null,null,null,"Coincident",-8.0939999999999994,-10.55,-12.19,-13.35,-14.58,-15.81,-17.02]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",115.6,118.6,119.6,120,120.3,120.1,120.2]
[null,null,null,null,"Coincident",117.6,120.7,121.2,121.7,121.5,121.6,121.7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",116.9,120.1,121.2,121.6,121.9,121.7,121.8]
[null,null,null,null,"Coincident",118.9,122.2,122.8,123.3,123.1,123.2,123.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",110.5,113.8,114.9,115.4,115.7,115.5,115.6]
[null,null,null,null,"Coincident",102.5,105.6,106,106.5,106.4,106.4,106.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",111.8,115.3,116.5,117,117.4,117.1,117.2]
[null,null,null,null,"Coincident",103.7,107,107.5,108,107.8,107.9,108]
[null,"Port Hacking 132_33kV","Substation Rating","MVA","Non-Coincident",159.1,159.1,159.1,159.1,159.1,159.1,159.1]
[null,null,null,null,"Coincident",159.1,159.1,159.1,159.1,159.1,159.1,159.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-24.09,-23.12,-22.77,-22.44,-21.73,-21.2,-20.68]
[null,null,null,null,"Coincident",-17.649999999999999,-16.05,-15,-14.29,-13.55,-12.82,-12.1]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",100.7,102.4,102.9,102.9,103,102.9,102.6]
[null,null,null,null,"Coincident",94.41,96,96.44,96.43,96.49,96.4,96.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",109.5,111.4,111.9,111.9,112,111.9,111.6]
[null,null,null,null,"Coincident",102.7,104.4,104.9,104.9,105,104.9,104.6]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",90.22,91.89,92.34,92.33,92.39,92.3,92.03]
[null,null,null,null,"Coincident",84.55,86.12,86.55,86.53,86.59,86.5,86.25]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",99.95,101.8,102.3,102.3,102.4,102.3,102]
[null,null,null,null,"Coincident",93.67,95.41,95.89,95.87,95.94,95.84,95.56]
[null,"Pyrmont 132_33kV","Substation Rating","MVA","Non-Coincident",170,170,170,170,170,170,170]
[null,null,null,null,"Coincident",170,170,170,170,170,170,170]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.58299999999999996,-0.85599999999999998,-1.1080000000000001,-1.377,-1.7330000000000001,-2.0710000000000002,-2.403]
[null,null,null,null,"Coincident",-0.95199999999999996,-1.224,-1.4550000000000001,-1.6850000000000001,-1.972,-2.2599999999999998,-2.5419999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",103.1,107.3,109.4,110.3,111.1,111.9,111.8]
[null,null,null,null,"Coincident",90.67,94.34,96.23,96.98,97.72,98.46,98.31]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",106.1,107.3,109.5,110.3,111.2,112,111.9]
[null,null,null,null,"Coincident",93.29,94.36,96.27,97.03,97.78,98.53,98.38]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",99.03,103.3,105.4,106.3,107.1,108,107.8]
[null,null,null,null,"Coincident",87.1,90.81,92.73,93.48,94.21,94.95,94.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",101.7,103.3,105.4,106.3,107.1,108,107.8]
[null,null,null,null,"Coincident",89.41,90.81,92.73,93.49,94.23,94.97,94.82]
[null,"Rozelle 132_33kV","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.59,26.34,44.34,44.34,51.63,51.63,51.63]
[null,null,null,null,"Coincident",5.71,7.6769999999999996,12.92,12.92,15.05,15.05,15.05]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.17,28.66,48.65,48.65,56.74,56.74,56.74]
[null,null,null,null,"Coincident",6.17,8.3529999999999998,14.18,14.18,16.54,16.54,16.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.39,25.14,43.14,43.14,50.43,50.43,50.43]
[null,null,null,null,"Coincident",5.36,7.3280000000000003,12.57,12.57,14.7,14.7,14.7]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.059999999999999,27.56,47.55,47.55,55.65,55.65,55.65]
[null,null,null,null,"Coincident",5.8479999999999999,8.0329999999999995,13.86,13.86,16.22,16.22,16.22]
[null,"Singleton 132_66kV","Substation Rating","MVA","Non-Coincident",284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998]
[null,null,null,null,"Coincident",284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998,284.39999999999998]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-11.31,-11,-10.79,-10.85,-10.68,-10.52,-10.36]
[null,null,null,null,"Coincident",-4.2089999999999996,-3.1579999999999999,-2.4889999999999999,-2.0579999999999998,-1.633,-1.2090000000000001,-0.79200000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",162.4,155.4,155.5,155.6,155.6,155.6,155.5]
[null,null,null,null,"Coincident",141.9,135.80000000000001,135.9,136,136,136,135.9]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",165,157.6,157.80000000000001,157.80000000000001,157.80000000000001,157.80000000000001,157.69999999999999]
[null,null,null,null,"Coincident",144.19999999999999,137.80000000000001,137.9,138,138,137.9,137.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",150,143,143.19999999999999,143.30000000000001,143.30000000000001,143.19999999999999,143.19999999999999]
[null,null,null,null,"Coincident",131.1,125,125.2,125.2,125.2,125.2,125.1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",152,144.6,144.80000000000001,144.9,144.9,144.80000000000001,144.80000000000001]
[null,null,null,null,"Coincident",132.80000000000001,126.4,126.6,126.6,126.6,126.6,126.5]
[null,"Surry Hills 132_33kV","Substation Rating","MVA","Non-Coincident",346.7,346.7,346.7,346.7,346.7,346.7,346.7]
[null,null,null,null,"Coincident",346.7,346.7,346.7,346.7,346.7,346.7,346.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.6150000000000002,-3.9420000000000002,-5.1120000000000001,-6.0209999999999999,-7.6609999999999996,-9.2140000000000004,-10.74]
[null,null,null,null,"Coincident",-3.9020000000000001,-4.907,-5.8609999999999998,-6.9249999999999998,-8.2929999999999993,-9.6590000000000007,-11]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",154.5,138.30000000000001,138.1,138.80000000000001,139.69999999999999,140.1,141.6]
[null,null,null,null,"Coincident",140.30000000000001,125.6,125.4,126.1,127,127.3,128.69999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",154.6,138.30000000000001,138.1,138.80000000000001,139.80000000000001,140.19999999999999,141.69999999999999]
[null,null,null,null,"Coincident",140.5,125.7,125.5,126.1,127,127.3,128.69999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",148.9,132.80000000000001,132.6,133.30000000000001,134.30000000000001,134.69999999999999,136.19999999999999]
[null,null,null,null,"Coincident",135.30000000000001,120.6,120.5,121.1,122,122.3,123.7]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",149.1,132.80000000000001,132.69999999999999,133.4,134.4,134.69999999999999,136.30000000000001]
[null,null,null,null,"Coincident",135.4,120.7,120.5,121.2,122.1,122.4,123.8]
[null,"Sydney East 132_33kV","Substation Rating","MVA","Non-Coincident",128.80000000000001,128.80000000000001,128.80000000000001,128.80000000000001,128.80000000000001,128.80000000000001,128.80000000000001]
[null,null,null,null,"Coincident",118.1,118.1,118.1,118.1,118.1,118.1,118.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.106,-0.21199999999999999,-0.32600000000000001,-0.47899999999999998,-0.67700000000000005,-0.86,-1.022]
[null,null,null,null,"Coincident",-6.2320000000000002,-8.1180000000000003,-9.3559999999999999,-10.199999999999999,-11.08,-11.95,-12.8]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",80.489999999999995,82.24,83.01,83.57,84.07,84.21,84.24]
[null,null,null,null,"Coincident",79.03,79.87,80.150000000000006,80.510000000000005,80.72,80.86,80.83]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",81.22,83.03,83.83,84.4,84.92,84.21,84.24]
[null,null,null,null,"Coincident",80.16,81.06,81.36,81.75,81.97,82.13,82.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",77.209999999999994,79.12,80,80.61,81.11,81.260000000000005,81.290000000000006]
[null,null,null,null,"Coincident",69.17,69.97,70.23,70.59,70.8,70.94,70.92]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",77.91,79.89,80.8,81.44,81.95,82.1,82.14]
[null,null,null,null,"Coincident",70.17,71.02,71.3,71.7,71.91,72.069999999999993,72.040000000000006]
[null,"Tomago 132_33kV","Substation Rating","MVA","Non-Coincident",153.1,153.1,153.1,153.1,153.1,153.1,153.1]
[null,null,null,null,"Coincident",153.1,153.1,153.1,153.1,153.1,153.1,153.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.9740000000000002,-3.988,-4.5789999999999997,-4.9210000000000003,-5.3280000000000003,-5.6429999999999998,-6.6029999999999998]
[null,null,null,null,"Coincident",-7.8609999999999998,-10.26,-11.8,-12.8,-13.8,-14.8,-15.78]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",131.4,132,132.80000000000001,134,135.9,137.30000000000001,138]
[null,null,null,null,"Coincident",124,124.6,125.4,126.5,128.30000000000001,129.6,130.30000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",132,132.6,133.5,134.69999999999999,136.6,138,138.80000000000001]
[null,null,null,null,"Coincident",124.6,125.2,126,127.1,129,130.30000000000001,131]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",119.4,120,120.9,122.1,124,125.4,126.1]
[null,null,null,null,"Coincident",112.7,113.3,114.1,115.2,117,118.3,119]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",119.8,120.4,121.3,122.5,124.4,125.8,126.6]
[null,null,null,null,"Coincident",113.1,113.7,114.5,115.6,117.4,118.8,119.5]
[null,"Waratah (Comsteel) 132_33kV","Substation Rating","MVA","Non-Coincident",38.119999999999997,38.119999999999997,38.119999999999997,38.119999999999997,38.119999999999997,38.119999999999997,38.119999999999997]
[null,null,null,null,"Coincident",35.67,35.67,35.67,35.67,35.67,35.67,35.67]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",64.13,64.13,64.13,64.13,64.13,64.13,64.13]
[null,null,null,null,"Coincident",27.12,27.12,27.12,27.12,27.12,27.12,27.12]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.319999999999993,67.319999999999993,67.319999999999993,67.319999999999993,67.319999999999993,67.319999999999993,67.319999999999993]
[null,null,null,null,"Coincident",28.76,28.76,28.76,28.76,28.76,28.76,28.76]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",56.48,56.48,56.48,56.48,56.48,56.48,56.48]
[null,null,null,null,"Coincident",24.93,24.93,24.93,24.93,24.93,24.93,24.93]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",60.08,60.08,60.08,60.08,60.08,60.08,60.08]
[null,null,null,null,"Coincident",26.7,26.7,26.7,26.7,26.7,26.7,26.7]
[null,"Waratah (Domestic) 132_33kV","Substation Rating","MVA","Non-Coincident",38.119999999999997,38.119999999999997,60,60,60,60,60]
[null,null,null,null,"Coincident",35.67,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident",-3.0049999999999999,-3.0049999999999999,-3.0049999999999999,-3.0049999999999999,-3.0049999999999999,-3.0049999999999999,-3.0049999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.69,34.69,34.69,34.69,34.69,34.69,34.69]
[null,null,null,null,"Coincident",7.7089999999999996,7.7089999999999996,7.7089999999999996,7.7089999999999996,7.7089999999999996,7.7089999999999996,7.7089999999999996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.89,37.89,37.89,37.89,37.89,37.89,37.89]
[null,null,null,null,"Coincident",8.5310000000000006,8.5310000000000006,8.5310000000000006,8.5310000000000006,8.5310000000000006,8.5310000000000006,8.5310000000000006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.32,31.32,31.32,31.32,31.32,31.32,31.32]
[null,null,null,null,"Coincident",7.0730000000000004,7.0730000000000004,7.0730000000000004,7.0730000000000004,7.0730000000000004,7.0730000000000004,7.0730000000000004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.83,34.83,34.83,34.83,34.83,34.83,34.83]
[null,null,null,null,"Coincident",7.9619999999999997,7.9619999999999997,7.9619999999999997,7.9619999999999997,7.9619999999999997,7.9619999999999997,7.9619999999999997]
[null,"Warringah 132_33kV","Substation Rating","MVA","Non-Coincident",229.8,229.8,229.8,229.8,229.8,229.8,229.8]
[null,null,null,null,"Coincident",217.4,217.4,217.4,217.4,217.4,217.4,217.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.41,-0.85799999999999998,-1.321,-1.8779999999999999,-2.6240000000000001,-3.323,-2.1789999999999998]
[null,null,null,null,"Coincident",-11.27,-14.6,-16.920000000000002,-18.71,-20.69,-22.67,-24.62]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",190.1,195.1,196.2,196.4,196.8,204.5,206.8]
[null,null,null,null,"Coincident",165.2,167.6,168.1,168.3,176.3,176.6,176.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",191.6,195.1,196.2,196.4,196.8,204.5,206.9]
[null,null,null,null,"Coincident",165.7,168,168.6,168.7,176.8,177.1,176.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",182,187.8,189.3,189.8,190.2,197.9,200.3]
[null,null,null,null,"Coincident",150.69999999999999,153,153.5,153.69999999999999,161.69999999999999,162,161.69999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",183.4,189.3,190.8,191.3,191.7,197.9,200.3]
[null,null,null,null,"Coincident",151.1,153.4,154,154.1,162.19999999999999,162.5,162.19999999999999]
[null,"Willoughby 132_33kV","Substation Rating","MVA","Non-Coincident",225.4,225.4,225.4,225.4,225.4,225.4,225.4]
[null,null,null,null,"Coincident",225.4,225.4,225.4,225.4,225.4,225.4,225.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.2989999999999999,-3.13,-3.1230000000000002,-3.9809999999999999,-4.4660000000000002,-5.1870000000000003,-5.89]
[null,null,null,null,"Coincident",-3.2440000000000002,-4.1479999999999997,-4.8869999999999996,-5.5960000000000001,-6.4630000000000001,-7.33,-8.18]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",146.69999999999999,155.9,167.3,172.1,175,177.2,178.6]
[null,null,null,null,"Coincident",137.80000000000001,146.5,157.1,161.69999999999999,164.4,166.5,167.8]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",146.69999999999999,156,167.4,172.3,175.3,177.5,178.9]
[null,null,null,null,"Coincident",137.9,146.6,157.30000000000001,161.9,164.7,166.7,168.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",139.9,149.30000000000001,160.69999999999999,165.5,168.5,170.7,172]
[null,null,null,null,"Coincident",131.4,140.30000000000001,151,155.5,158.30000000000001,160.30000000000001,161.6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",139.9,149.4,160.80000000000001,165.7,168.6,170.9,172.3]
[null,null,null,null,"Coincident",131.5,140.30000000000001,151.1,155.6,158.4,160.5,161.80000000000001]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Aberdeen 66_11kV","Substation Rating","MVA","Non-Coincident",25.53,25.53,25.53,25.53,25.53,25.53,25.53]
[null,null,null,null,"Coincident",25.53,25.53,25.53,25.53,25.53,25.53,25.53]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.4999999999999999E-2,-2.8000000000000001E-2,-0.04,-5.2999999999999999E-2,-6.9000000000000006E-2,-8.4000000000000005E-2,-9.7000000000000003E-2]
[null,null,null,null,"Coincident",-0.31,-0.39900000000000002,-0.45900000000000002,-0.503,-0.54900000000000004,-0.59399999999999997,-0.63900000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.6429999999999998,6.6369999999999996,6.633,6.6390000000000002,6.6360000000000001,6.6319999999999997,6.6479999999999997]
[null,null,null,null,"Coincident",5.157,5.1529999999999996,5.15,5.1539999999999999,5.1520000000000001,5.149,5.1609999999999996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6719999999999997,6.6669999999999998,6.6630000000000003,6.6680000000000001,6.6660000000000004,6.6609999999999996,6.6779999999999999]
[null,null,null,null,"Coincident",5.18,5.1760000000000002,5.173,5.1769999999999996,5.1749999999999998,5.1719999999999997,5.1840000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.9859999999999998,5.98,5.976,5.9809999999999999,5.9790000000000001,5.9749999999999996,5.9909999999999997]
[null,null,null,null,"Coincident",4.6470000000000002,4.6429999999999998,4.6399999999999997,4.6440000000000001,4.6420000000000003,4.6379999999999999,4.6509999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0119999999999996,6.0069999999999997,6.0030000000000001,6.008,6.0060000000000002,6.0010000000000003,6.0179999999999998]
[null,null,null,null,"Coincident",4.6680000000000001,4.6630000000000003,4.66,4.665,4.6630000000000003,4.6589999999999998,4.6719999999999997]
[null,"Adamstown 132_11kV","Substation Rating","MVA","Non-Coincident",63.03,63.03,63.03,63.03,63.03,63.03,63.03]
[null,null,null,null,"Coincident",63.03,63.03,63.03,63.03,63.03,63.03,63.03]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.36499999999999999,-0.67500000000000004,-0.65400000000000003,-0.77600000000000002,-0.91700000000000004,-1.05,-1.1779999999999999]
[null,null,null,null,"Coincident",-2.0830000000000002,-2.7250000000000001,-3.1419999999999999,-3.4209999999999998,-3.706,-3.9910000000000001,-4.2709999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.770000000000003,33.99,34.049999999999997,34.06,34.049999999999997,34.119999999999997,34.06]
[null,null,null,null,"Coincident",31.64,31.84,31.91,31.91,31.91,31.96,31.91]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.78,34,34.07,34.08,34.07,34.130000000000003,34.07]
[null,null,null,null,"Coincident",31.65,31.85,31.92,31.93,31.92,31.98,31.92]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.9,29.09,29.15,29.16,29.15,29.22,29.16]
[null,null,null,null,"Coincident",27.07,27.26,27.32,27.32,27.31,27.37,27.32]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.9,29.1,29.16,29.17,29.16,29.22,29.16]
[null,null,null,null,"Coincident",27.07,27.26,27.32,27.33,27.32,27.38,27.32]
[null,"Argenton 132_11kV","Substation Rating","MVA","Non-Coincident",60.8,60.8,60.8,60.8,60.8,60.8,60.8]
[null,null,null,null,"Coincident",60.8,60.8,60.8,60.8,60.8,60.8,60.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.73299999999999998,-1,-1.1850000000000001,-1.327,-1.484,-1.3109999999999999,-1.4179999999999999]
[null,null,null,null,"Coincident",-2.222,-2.895,-3.3239999999999998,-3.6040000000000001,-3.8809999999999998,-4.1589999999999998,-4.4320000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.090000000000003,37.270000000000003,37.340000000000003,37.39,37.729999999999997,37.78,37.72]
[null,null,null,null,"Coincident",34.53,34.700000000000003,34.76,34.81,35.119999999999997,35.18,35.119999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.729999999999997,37.92,37.99,38.04,38.380000000000003,38.44,38.380000000000003]
[null,null,null,null,"Coincident",35.130000000000003,35.299999999999997,35.36,35.42,35.74,35.79,35.729999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.119999999999997,33.28,33.340000000000003,33.4,33.74,33.79,33.729999999999997]
[null,null,null,null,"Coincident",30.84,30.99,31.04,31.1,31.41,31.46,31.4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.700000000000003,33.86,33.92,33.979999999999997,34.32,34.380000000000003,34.31]
[null,null,null,null,"Coincident",31.37,31.53,31.58,31.64,31.95,32.01,31.95]
[null,"Auburn 33_11kV","Substation Rating","MVA","Non-Coincident",30.6,30.6,30.6,30.6,30.6,30.6,30.6]
[null,null,null,null,"Coincident",30.6,30.6,30.6,30.6,30.6,30.6,30.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.7290000000000001,-1.986,-2.2090000000000001,-2.4289999999999998,-2.7050000000000001,-2.9660000000000002,-3.2069999999999999]
[null,null,null,null,"Coincident",-0.73599999999999999,-0.93700000000000006,-1.1100000000000001,-1.2849999999999999,-1.504,-1.722,-1.9359999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.28,31.15,31.21,31.42,31.58,31.68,31.69]
[null,null,null,null,"Coincident",23.82,25.35,25.39,25.57,25.69,25.78,25.78]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.42,32.36,32.42,32.64,32.799999999999997,32.909999999999997,32.92]
[null,null,null,null,"Coincident",24.75,26.33,26.38,26.56,26.69,26.78,26.79]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.56,28.46,28.53,28.74,28.89,29,29]
[null,null,null,null,"Coincident",21.61,23.15,23.21,23.39,23.51,23.59,23.6]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.59,29.56,29.63,29.86,30.02,30.12,30.13]
[null,null,null,null,"Coincident",22.45,24.05,24.11,24.3,24.43,24.51,24.52]
[null,"Avoca 66_11kV","Substation Rating","MVA","Non-Coincident",63.67,63.67,63.67,63.67,63.67,63.67,63.67]
[null,null,null,null,"Coincident",59.83,59.83,59.83,59.83,59.83,59.83,59.83]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-6.0999999999999999E-2,-0.121,-0.183,-0.26200000000000001,-0.36599999999999999,-0.46300000000000002,-0.55000000000000004]
[null,null,null,null,"Coincident",-3.2050000000000001,-4.1909999999999998,-4.8120000000000003,-5.1989999999999998,-5.5739999999999998,-5.95,-6.3209999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.14,43.03,43.49,43.79,43.88,43.88,43.87]
[null,null,null,null,"Coincident",37.909999999999997,38.69,38.85,38.92,38.94,38.9,38.81]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.18,43.07,43.53,43.82,43.92,43.92,43.91]
[null,null,null,null,"Coincident",38.119999999999997,38.909999999999997,39.07,39.14,39.159999999999997,39.119999999999997,39.03]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.799999999999997,40.79,41.32,41.65,41.74,41.74,41.73]
[null,null,null,null,"Coincident",33.19,33.97,34.119999999999997,34.19,34.21,34.17,34.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.840000000000003,40.83,41.35,41.68,41.78,41.78,41.77]
[null,null,null,null,"Coincident",33.380000000000003,34.159999999999997,34.31,34.380000000000003,34.4,34.36,34.28]
[null,"Avondale 33_11kV","Substation Rating","MVA","Non-Coincident",23.59,23.59,23.59,23.59,23.59,23.59,23.59]
[null,null,null,null,"Coincident",23.59,23.59,23.59,23.59,23.59,23.59,23.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.624,-0.70599999999999996,-0.76100000000000001,-0.80100000000000005,-0.84499999999999997,-0.88700000000000001,-0.92600000000000005]
[null,null,null,null,"Coincident",-0.79600000000000004,-1.04,-1.1910000000000001,-1.2809999999999999,-1.3640000000000001,-1.448,-1.5309999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.95,14.06,14.1,14.09,14.05,14,13.93]
[null,null,null,null,"Coincident",12.69,12.8,12.84,12.82,12.79,12.74,12.68]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.08,14.2,14.24,14.22,14.19,14.14,14.06]
[null,null,null,null,"Coincident",12.82,12.92,12.96,12.95,12.91,12.87,12.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.49,12.6,12.64,12.62,12.58,12.53,12.46]
[null,null,null,null,"Coincident",11.37,11.47,11.5,11.49,11.46,11.41,11.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.61,12.72,12.76,12.74,12.71,12.66,12.58]
[null,null,null,null,"Coincident",11.48,11.58,11.61,11.6,11.57,11.52,11.45]
[null,"Baerami 33_11kV","Substation Rating","MVA","Non-Coincident",2.44,2.44,2.44,2.44,2.44,2.44,2.44]
[null,null,null,null,"Coincident",2.44,2.44,2.44,2.44,2.44,2.44,2.44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.0999999999999999E-2,-1.2999999999999999E-2,-1.6E-2,-1.9E-2,-1.4999999999999999E-2,-1.7000000000000001E-2,-1.9E-2]
[null,null,null,null,"Coincident",-3.2000000000000001E-2,-3.9E-2,-4.5999999999999999E-2,-5.1999999999999998E-2,-0.06,-6.7000000000000004E-2,-7.3999999999999996E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.872,0.86299999999999999,0.85899999999999999,0.86899999999999999,0.872,0.876,0.88100000000000001]
[null,null,null,null,"Coincident",0.71799999999999997,0.71099999999999997,0.70799999999999996,0.71599999999999997,0.71899999999999997,0.72199999999999998,0.72599999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.92200000000000004,0.91300000000000003,0.90900000000000003,0.91900000000000004,0.92300000000000004,0.92700000000000005,0.93200000000000005]
[null,null,null,null,"Coincident",0.76,0.753,0.749,0.75800000000000001,0.76100000000000001,0.76400000000000001,0.76800000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.77900000000000003,0.77200000000000002,0.76700000000000002,0.77800000000000002,0.78100000000000003,0.78500000000000003,0.79]
[null,null,null,null,"Coincident",0.64200000000000002,0.63600000000000001,0.63300000000000001,0.64100000000000001,0.64400000000000002,0.64700000000000002,0.65100000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.82499999999999996,0.81599999999999995,0.81200000000000006,0.82299999999999995,0.82699999999999996,0.83099999999999996,0.83599999999999997]
[null,null,null,null,"Coincident",0.68,0.67300000000000004,0.66900000000000004,0.67800000000000005,0.68100000000000005,0.68500000000000005,0.68899999999999995]
[null,"Balgowlah North 132_11kV","Substation Rating","MVA","Non-Coincident",43.92,43.92,43.92,43.92,43.92,43.92,43.92]
[null,null,null,null,"Coincident",43.92,43.92,43.92,43.92,43.92,43.92,43.92]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.3999999999999997E-2,-8.8999999999999996E-2,-0.13700000000000001,-0.20399999999999999,-0.29099999999999998,-0.372,-0.44400000000000001]
[null,null,null,null,"Coincident",-2.371,-3.1040000000000001,-3.5830000000000002,-3.9039999999999999,-4.234,-4.5640000000000001,-4.8899999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.549999999999997,38.64,39.03,39.270000000000003,39.36,39.42,39.46]
[null,null,null,null,"Coincident",27.94,28.56,28.77,28.86,28.91,28.96,28.98]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.590000000000003,38.69,39.08,39.32,39.42,39.47,39.520000000000003]
[null,null,null,null,"Coincident",28.18,28.81,29.02,29.11,29.16,29.22,29.23]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.51,36.619999999999997,37.01,37.270000000000003,37.36,37.409999999999997,37.46]
[null,null,null,null,"Coincident",25.05,25.64,25.84,25.94,25.98,26.04,26.06]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.549999999999997,36.67,37.06,37.32,37.409999999999997,37.46,37.51]
[null,null,null,null,"Coincident",25.26,25.87,26.07,26.16,26.21,26.27,26.28]
[null,"Bankstown 132_11kV","Substation Rating","MVA","Non-Coincident",63.52,63.52,63.52,63.52,63.52,63.52,63.52]
[null,null,null,null,"Coincident",63.52,63.52,63.52,63.52,63.52,63.52,63.52]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.2189999999999999,-3.2730000000000001,-2.7389999999999999,-3.113,-3.5670000000000002,-3.9969999999999999,-4.4160000000000004]
[null,null,null,null,"Coincident",-2.863,-3.7040000000000002,-4.3010000000000002,-4.7699999999999996,-5.2960000000000003,-5.8209999999999997,-6.3369999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.4,52.07,51.95,52.33,52.66,53.15,54.53]
[null,null,null,null,"Coincident",48.54,49.17,49.06,49.41,49.73,50.19,51.49]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.39,53.07,52.94,53.33,53.67,54.17,55.57]
[null,null,null,null,"Coincident",49.47,50.11,49.99,50.36,50.68,51.15,52.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.13,45.92,45.85,46.23,46.57,47.06,48.43]
[null,null,null,null,"Coincident",42.62,43.36,43.3,43.66,43.98,44.44,45.73]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.03,46.83,46.77,47.16,47.5,48,49.4]
[null,null,null,null,"Coincident",43.47,44.23,44.17,44.53,44.85,45.33,46.65]
[null,"Bass Hill 33_11kV","Substation Rating","MVA","Non-Coincident",20.69,20.69,20.69,20.69,20.69,20.69,20.69]
[null,null,null,null,"Coincident",20.69,20.69,20.69,20.69,20.69,20.69,20.69]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.248,-0.48299999999999998,-0.504,-0.59099999999999997,-0.68700000000000006,-0.77700000000000002,-0.86499999999999999]
[null,null,null,null,"Coincident",-1.016,-1.329,-1.5289999999999999,-1.6579999999999999,-1.786,-1.915,-2.0409999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.36,20.07,19.89,19.920000000000002,19.940000000000001,19.920000000000002,19.88]
[null,null,null,null,"Coincident",19.64,19.36,19.190000000000001,19.22,19.23,19.22,19.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.51,20.22,20.04,20.07,20.079999999999998,20.07,20.03]
[null,null,null,null,"Coincident",19.79,19.510000000000002,19.34,19.36,19.38,19.37,19.329999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.190000000000001,17.940000000000001,17.79,17.809999999999999,17.829999999999998,17.82,17.78]
[null,null,null,null,"Coincident",17.55,17.309999999999999,17.16,17.190000000000001,17.2,17.190000000000001,17.149999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.32,18.079999999999998,17.920000000000002,17.95,17.96,17.95,17.91]
[null,null,null,null,"Coincident",17.68,17.440000000000001,17.29,17.309999999999999,17.329999999999998,17.32,17.28]
[null,"Beacon Hill 33_11kV","Substation Rating","MVA","Non-Coincident",26.67,26.67,26.67,26.67,26.67,26.67,26.67]
[null,null,null,null,"Coincident",26.67,26.67,26.67,26.67,26.67,26.67,26.67]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-7.0000000000000007E-2,-9.2999999999999999E-2,-0.11899999999999999,-0.153,-0.19700000000000001,-0.23699999999999999,-0.27200000000000002]
[null,null,null,null,"Coincident",-1.234,-1.609,-1.8540000000000001,-2.0209999999999999,-2.1909999999999998,-2.3620000000000001,-2.5289999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.59,18.37,18.48,18.440000000000001,18.54,18.62,18.75]
[null,null,null,null,"Coincident",18.55,18.47,18.39,18.37,18.309999999999999,18.25,18.13]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.77,18.600000000000001,18.72,18.670000000000002,18.78,18.87,19]
[null,null,null,null,"Coincident",18.600000000000001,18.52,18.440000000000001,18.420000000000002,18.36,18.3,18.18]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.93,17.760000000000002,17.91,17.88,17.989999999999998,18.059999999999999,18.190000000000001]
[null,null,null,null,"Coincident",16.86,16.809999999999999,16.75,16.73,16.670000000000002,16.61,16.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.07,17.95,18.11,18.07,18.190000000000001,18.27,18.41]
[null,null,null,null,"Coincident",16.87,16.829999999999998,16.77,16.739999999999998,16.690000000000001,16.63,16.510000000000002]
[null,"Belmore Park 132_11kV","Substation Rating","MVA","Non-Coincident",125.6,125.6,125.6,125.6,125.6,125.6,125.6]
[null,null,null,null,"Coincident",null,125.6,125.6,125.6,125.6,125.6,125.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident",null,"Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.9,32.76,32.64,33.01,33.58,34.06,34.79]
[null,null,null,null,"Coincident",4.2080000000000002,4.1900000000000004,4.1749999999999998,4.2220000000000004,4.2949999999999999,4.3559999999999999,4.45]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.64,33.520000000000003,33.409999999999997,33.81,34.43,34.950000000000003,35.74]
[null,null,null,null,"Coincident",4.3019999999999996,4.2880000000000003,4.274,4.3250000000000002,4.4039999999999999,4.47,4.5720000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.32,31.21,31.11,31.48,32.049999999999997,32.53,33.26]
[null,null,null,null,"Coincident",4.0060000000000002,3.992,3.9790000000000001,4.0259999999999998,4.0990000000000002,4.1609999999999996,4.2539999999999996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.03,31.95,31.86,32.26,32.880000000000003,33.4,34.19]
[null,null,null,null,"Coincident",4.0970000000000004,4.0869999999999997,4.0750000000000002,4.1260000000000003,4.2050000000000001,4.2720000000000002,4.3730000000000002]
[null,"Belrose 33_11kV","Substation Rating","MVA","Non-Coincident",40.29,40.29,40.29,40.29,40.29,40.29,40.29]
[null,null,null,null,"Coincident",40.29,40.29,40.29,40.29,40.29,40.29,40.29]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5659999999999998,-2.8119999999999998,-2.472,-2.5259999999999998,-2.59,-2.65,-2.7050000000000001]
[null,null,null,null,"Coincident",-2.16,-2.84,-3.2480000000000002,-3.4729999999999999,-3.6680000000000001,-3.8650000000000002,-4.0579999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.090000000000003,36.229999999999997,36.630000000000003,36.69,36.700000000000003,36.700000000000003,36.659999999999997]
[null,null,null,null,"Coincident",32.01,33.04,33.409999999999997,33.47,33.479999999999997,33.479999999999997,33.44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.43,37.61,38.03,38.090000000000003,38.1,38.1,38.06]
[null,null,null,null,"Coincident",33.229999999999997,34.31,34.69,34.74,34.75,34.76,34.71]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.42,31.46,31.81,31.87,31.89,31.89,31.84]
[null,null,null,null,"Coincident",27.75,28.7,29.02,29.07,29.09,29.09,29.05]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.58,32.659999999999997,33.03,33.090000000000003,33.1,33.11,33.06]
[null,null,null,null,"Coincident",28.81,29.79,30.13,30.18,30.2,30.2,30.15]
[null,"Berkeley Vale 132_11kV","Substation Rating","MVA","Non-Coincident",59.9,59.9,59.9,59.9,59.9,59.9,59.9]
[null,null,null,null,"Coincident",59.9,59.9,59.9,59.9,59.9,59.9,59.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1339999999999999,-2.8980000000000001,-3.3140000000000001,-3.085,-3.3780000000000001,-3.6549999999999998,-3.9260000000000002]
[null,null,null,null,"Coincident",-2.0350000000000001,-2.6509999999999998,-3.0579999999999998,-3.34,-3.633,-3.9260000000000002,-4.2130000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.95,43.65,44.47,45.37,46.25,46.48,46.64]
[null,null,null,null,"Coincident",42.78,42.49,43.29,44.16,45.03,45.25,45.41]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.51,44.21,45.04,45.95,46.85,47.08,47.24]
[null,null,null,null,"Coincident",43.33,43.04,43.85,44.73,45.61,45.83,45.99]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.85,39.630000000000003,40.479999999999997,41.38,42.27,42.5,42.66]
[null,null,null,null,"Coincident",38.79,38.58,39.409999999999997,40.28,41.15,41.37,41.53]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.36,40.14,41,41.91,42.81,43.04,43.21]
[null,null,null,null,"Coincident",39.29,39.07,39.92,40.799999999999997,41.68,41.9,42.06]
[null,"Berowra 132_11kV","Substation Rating","MVA","Non-Coincident",44.56,44.56,44.56,44.56,44.56,44.56,44.56]
[null,null,null,null,"Coincident",42.33,42.33,42.33,42.33,42.33,42.33,42.33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.04,-0.08,-0.115,-0.158,-0.21299999999999999,-0.27,-0.318]
[null,null,null,null,"Coincident",-2.028,-2.6560000000000001,-3.0379999999999998,-3.2559999999999998,-3.452,-3.6480000000000001,-3.8410000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.48,23.4,23.89,24.74,26.03,27.12,27.04]
[null,null,null,null,"Coincident",23.13,23.49,23.99,25.29,26.37,26.29,26.18]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.21,24.13,24.63,25.51,26.83,27.96,27.88]
[null,null,null,null,"Coincident",24.74,25.13,25.66,27.04,28.2,28.12,28]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.45,22.55,23.15,24.06,25.34,26.44,26.36]
[null,null,null,null,"Coincident",20.49,20.87,21.38,22.68,23.76,23.68,23.58]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.14,23.24,23.87,24.8,26.13,27.25,27.17]
[null,null,null,null,"Coincident",21.91,22.32,22.87,24.26,25.41,25.33,25.22]
[null,"Blackwattle Bay 33_5kV","Substation Rating","MVA","Non-Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,null,null,"Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Blakehurst 33_11kV","Substation Rating","MVA","Non-Coincident",31.59,31.59,31.59,31.59,31.59,31.59,31.59]
[null,null,null,null,"Coincident",31.59,31.59,31.59,31.59,31.59,31.59,31.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5999999999999999E-2,-5.0999999999999997E-2,-8.1000000000000003E-2,-0.127,-0.185,-0.24,-0.28799999999999998]
[null,null,null,null,"Coincident",-1.56,-2.036,-2.3639999999999999,-2.6070000000000002,-2.8730000000000002,-3.1389999999999998,-3.4009999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.04,24.21,24.62,24.7,24.83,24.79,24.74]
[null,null,null,null,"Coincident",22.06,23.79,24,24.11,24.06,24,24.03]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.07,25.31,25.74,25.83,25.96,25.91,25.86]
[null,null,null,null,"Coincident",22.82,24.58,24.8,24.92,24.87,24.81,24.84]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.02,23.23,23.67,23.77,23.89,23.85,23.8]
[null,null,null,null,"Coincident",19.46,21.17,21.38,21.49,21.44,21.38,21.41]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22,24.28,24.75,24.85,24.98,24.93,24.88]
[null,null,null,null,"Coincident",20.14,21.88,22.09,22.21,22.16,22.1,22.13]
[null,"Botany 33_11kV","Substation Rating","MVA","Non-Coincident",55.16,55.16,55.16,55.16,55.16,55.16,55.16]
[null,null,null,null,"Coincident",55.16,55.16,55.16,55.16,55.16,55.16,55.16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.7999999999999999E-2,-3.5000000000000003E-2,-0.06,-9.8000000000000004E-2,-0.14899999999999999,-0.19500000000000001,-0.23499999999999999]
[null,null,null,null,"Coincident",-1.1679999999999999,-1.494,-1.7410000000000001,-1.958,-2.2109999999999999,-2.464,-2.7120000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.96,26.22,26.21,26.21,26.45,26.55,26.83]
[null,null,null,null,"Coincident",27.57,27.44,27.24,27.12,27.84,28.74,28.12]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.35,26.62,26.61,26.6,26.85,26.95,27.23]
[null,null,null,null,"Coincident",28.85,28.71,28.5,28.37,29.13,30.07,29.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.58,26.54,27.01,27.24,27.48,27.59,27.86]
[null,null,null,null,"Coincident",25.39,25.27,25.08,24.96,25.68,26.57,25.95]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.97,26.94,27.42,27.65,27.9,28,28.28]
[null,null,null,null,"Coincident",26.56,26.44,26.24,26.11,26.87,27.8,27.15]
[null,"Brandy Hill 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-6.8000000000000005E-2,-0.13200000000000001,-0.17299999999999999,-0.19900000000000001,-0.22600000000000001,-0.251,-0.27600000000000002]
[null,null,null,null,"Coincident",-0.60499999999999998,-0.79900000000000004,-0.91500000000000004,-0.97799999999999998,-1.0309999999999999,-1.085,-1.1379999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.73,12.75,12.83,12.97,13.18,13.41,13.47]
[null,null,null,null,"Coincident",10.66,10.67,10.74,10.85,11.03,11.23,11.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.86,12.88,12.97,13.1,13.32,13.55,13.61]
[null,null,null,null,"Coincident",10.77,10.78,10.85,10.97,11.15,11.34,11.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.19,11.2,11.29,11.42,11.64,11.87,11.93]
[null,null,null,null,"Coincident",9.3629999999999995,9.3770000000000007,9.4480000000000004,9.5609999999999999,9.74,9.9329999999999998,9.984]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.3,11.32,11.41,11.54,11.76,11.99,12.05]
[null,null,null,null,"Coincident",9.4610000000000003,9.4749999999999996,9.5470000000000006,9.6609999999999996,9.8409999999999993,10.039999999999999,10.09]
[null,"Branxton 66_11kV","Substation Rating","MVA","Non-Coincident",15.07,15.07,15.07,15.07,15.07,15.07,15.07]
[null,null,null,null,"Coincident",15.07,15.07,15.07,15.07,15.07,15.07,15.07]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.3999999999999997E-2,-7.4999999999999997E-2,-9.8000000000000004E-2,-0.121,-0.14799999999999999,-0.17399999999999999,-0.19700000000000001]
[null,null,null,null,"Coincident",-0.93100000000000005,-1.2170000000000001,-1.391,-1.4910000000000001,-1.581,-1.671,-1.76]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.02,18.3,18.38,18.399999999999999,18.399999999999999,18.399999999999999,18.36]
[null,null,null,null,"Coincident",15,15.23,15.29,15.32,15.32,15.32,15.29]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.29,18.579999999999998,18.66,18.68,18.68,18.68,18.649999999999999]
[null,null,null,null,"Coincident",15.23,15.46,15.53,15.55,15.55,15.55,15.52]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.3,16.57,16.64,16.670000000000002,16.670000000000002,16.670000000000002,16.63]
[null,null,null,null,"Coincident",13.57,13.79,13.85,13.87,13.88,13.87,13.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.559999999999999,16.829999999999998,16.91,16.93,16.93,16.93,16.899999999999999]
[null,null,null,null,"Coincident",13.78,14.01,14.07,14.09,14.1,14.09,14.06]
[null,"Broadmeadow 132_11kV","Substation Rating","MVA","Non-Coincident",59.54,59.54,59.54,59.54,59.54,59.54,59.54]
[null,null,null,null,"Coincident",59.54,59.54,59.54,59.54,59.54,59.54,59.54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.77400000000000002,-1.3360000000000001,-1.752,-2.085,-2.4660000000000002,-2.8279999999999998,-3.1829999999999998]
[null,null,null,null,"Coincident",-1.43,-1.8520000000000001,-2.145,-2.37,-2.6139999999999999,-2.8580000000000001,-3.0979999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.34,29.87,29.57,29.43,29.25,29.06,31.39]
[null,null,null,null,"Coincident",28.17,27.73,27.45,27.32,27.16,26.98,29.15]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.65,30.18,29.88,29.74,29.55,29.37,31.72]
[null,null,null,null,"Coincident",28.46,28.02,27.74,27.61,27.44,27.26,29.45]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.35,25.9,25.6,25.46,25.28,25.1,27.43]
[null,null,null,null,"Coincident",24.46,24.04,23.77,23.64,23.47,23.3,25.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.62,26.17,25.87,25.73,25.55,25.36,27.71]
[null,null,null,null,"Coincident",24.72,24.29,24.02,23.89,23.72,23.54,25.73]
[null,"Brookvale 33_11kV","Substation Rating","MVA","Non-Coincident",54.33,54.33,54.33,54.33,54.33,54.33,54.33]
[null,null,null,null,"Coincident",54.33,54.33,54.33,54.33,54.33,54.33,54.33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.843,-3.3170000000000002,-3.7919999999999998,-4.3360000000000003,-5.056,-5.7389999999999999,-5.6719999999999997]
[null,null,null,null,"Coincident",-1.345,-1.68,-1.9950000000000001,-2.3450000000000002,-2.7909999999999999,-3.2360000000000002,-3.6720000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.94,44.11,43.8,43.47,43.14,43.6,43.4]
[null,null,null,null,"Coincident",37.58,37.729999999999997,37.47,37.19,36.9,37.299999999999997,37.119999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.94,44.11,43.8,43.48,43.14,43.6,43.4]
[null,null,null,null,"Coincident",37.58,37.74,37.47,37.19,36.9,37.299999999999997,37.119999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.34,41.54,41.24,40.909999999999997,40.58,41.04,40.840000000000003]
[null,null,null,null,"Coincident",35.36,35.53,35.28,35,34.71,35.1,34.93]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.44,41.65,41.34,41.01,40.68,41.14,40.93]
[null,null,null,null,"Coincident",35.450000000000003,35.619999999999997,35.36,35.08,34.79,35.19,35.020000000000003]
[null,"Burwood 132_11kV","Substation Rating","MVA","Non-Coincident",83.6,83.6,83.6,83.6,83.6,83.6,83.6]
[null,null,null,null,"Coincident",83.6,83.6,83.6,83.6,83.6,83.6,83.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.2879999999999998,-4.0179999999999998,-4.617,-5.1890000000000001,-5.907,-6.5860000000000003,-7.2510000000000003]
[null,null,null,null,"Coincident",-3.0049999999999999,-3.8780000000000001,-4.5410000000000004,-5.1210000000000004,-5.8049999999999997,-6.4880000000000004,-7.1589999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",87.45,92.43,94.46,96.23,96.84,97.48,97.97]
[null,null,null,null,"Coincident",84.51,89.32,91.28,92.99,93.57,94.2,94.67]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",87.5,92.44,94.47,96.23,96.84,97.49,97.98]
[null,null,null,null,"Coincident",84.55,89.32,91.29,92.99,93.58,94.2,94.68]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",78.150000000000006,83.08,85.09,86.85,87.46,88.1,88.59]
[null,null,null,null,"Coincident",75.52,80.28,82.22,83.92,84.51,85.13,85.61]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",78.16,83.11,85.12,86.89,87.5,88.15,88.64]
[null,null,null,null,"Coincident",75.53,80.31,82.26,83.97,84.56,85.18,85.66]
[null,"Campbell St 132_11kV","Substation Rating","MVA","Non-Coincident",62.8,62.8,62.8,62.8,62.8,62.8,62.8]
[null,null,null,null,"Coincident",62.8,62.8,62.8,62.8,62.8,62.8,62.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.73799999999999999,-1.17,-1.6379999999999999,-2.198,-2.948,-3.2080000000000002,-3.802]
[null,null,null,null,"Coincident",-1.2210000000000001,-1.512,-1.8089999999999999,-2.1619999999999999,-2.6219999999999999,-3.08,-3.5289999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.23,32.92,32.47,32.08,32.159999999999997,31.92,32.46]
[null,null,null,null,"Coincident",15.47,29.57,29.17,28.82,28.89,28.67,29.16]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.64,33.64,33.18,32.78,32.869999999999997,32.619999999999997,33.17]
[null,null,null,null,"Coincident",15.84,30.22,29.81,29.45,29.52,29.3,29.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.72,30.46,30.04,29.65,29.73,29.49,30.03]
[null,null,null,null,"Coincident",13.22,27.36,26.98,26.63,26.7,26.49,26.97]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.07,31.13,30.7,30.3,30.38,30.13,30.68]
[null,null,null,null,"Coincident",13.54,27.96,27.57,27.21,27.29,27.07,27.56]
[null,"Camperdown 33_11kV","Substation Rating","MVA","Non-Coincident",58.3,58.3,58.3,58.3,58.3,58.3,58.3]
[null,null,null,null,"Coincident",58.3,58.3,58.3,58.3,58.3,58.3,58.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.081,-1.389,-1.673,-1.9770000000000001,-2.38,-2.7610000000000001,-3.1360000000000001]
[null,null,null,null,"Coincident",-0.95199999999999996,-1.224,-1.4550000000000001,-1.6850000000000001,-1.972,-2.2599999999999998,-2.5419999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.22,37.39,37.57,37.520000000000003,37.46,37.4,37.229999999999997]
[null,null,null,null,"Coincident",30.67,33.51,33.67,33.619999999999997,33.57,33.51,33.369999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.79,38.049999999999997,38.229999999999997,38.18,38.11,38.049999999999997,37.880000000000003]
[null,null,null,null,"Coincident",31.18,34.1,34.26,34.21,34.159999999999997,34.1,33.950000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.83,35.06,35.25,35.200000000000003,35.14,35.08,34.92]
[null,null,null,null,"Coincident",28.53,31.42,31.59,31.55,31.49,31.44,31.29]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.369999999999997,35.68,35.880000000000003,35.83,35.770000000000003,35.700000000000003,35.54]
[null,null,null,null,"Coincident",29.01,31.97,32.15,32.11,32.049999999999997,32,31.85]
[null,"Camperdown 33_5kV","Substation Rating","MVA","Non-Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,null,null,"Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Campsie 33_11kV","Substation Rating","MVA","Non-Coincident",87.01,87.01,87.01,87.01,87.01,87.01,87.01]
[null,null,null,null,"Coincident",87.01,87.01,87.01,87.01,87.01,87.01,87.01]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.9950000000000001,-2.097,-2.2050000000000001,-2.3439999999999999,-2.5259999999999998,-2.6930000000000001,-2.8439999999999999]
[null,null,null,null,"Coincident",-4.57,-5.9320000000000004,-6.867,-7.5629999999999997,-8.32,-9.0760000000000005,-9.8209999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",82.47,83.39,84.12,84.65,84.86,85.68,86.22]
[null,null,null,null,"Coincident",79.84,80.73,81.430000000000007,81.94,82.15,82.94,83.47]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",84.7,85.64,86.39,86.93,87.15,87.99,88.55]
[null,null,null,null,"Coincident",81.99,82.9,83.63,84.15,84.36,85.18,85.72]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",73.290000000000006,74.2,74.930000000000007,75.459999999999994,75.67,76.489999999999995,77.03]
[null,null,null,null,"Coincident",70.95,71.83,72.540000000000006,73.05,73.25,74.040000000000006,74.569999999999993]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",75.260000000000005,76.2,76.95,77.489999999999995,77.709999999999994,78.55,79.11]
[null,null,null,null,"Coincident",72.86,73.77,74.489999999999995,75.010000000000005,75.22,76.040000000000006,76.58]
[null,"Cardiff 33_11kV","Substation Rating","MVA","Non-Coincident",22.86,22.86,22.86,22.86,22.86,22.86,22.86]
[null,null,null,null,"Coincident",22.86,22.86,22.86,22.86,22.86,22.86,22.86]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.083,-1.2270000000000001,-1.3280000000000001,-1.4079999999999999,-1.496,-1.579,-1.659]
[null,null,null,null,"Coincident",-1.3979999999999999,-1.8149999999999999,-2.081,-2.2530000000000001,-2.4220000000000002,-2.5910000000000002,-2.7570000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.100000000000001,18.8,18.649999999999999,18.66,18.62,18.64,18.559999999999999]
[null,null,null,null,"Coincident",17.739999999999998,17.45,17.32,17.32,17.29,17.309999999999999,17.23]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.45,19.14,18.989999999999998,19,18.96,18.98,18.89]
[null,null,null,null,"Coincident",18.059999999999999,17.77,17.63,17.64,17.600000000000001,17.62,17.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.82,16.54,16.399999999999999,16.41,16.37,16.39,16.309999999999999]
[null,null,null,null,"Coincident",15.61,15.35,15.23,15.23,15.2,15.22,15.14]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.12,16.84,16.7,16.71,16.670000000000002,16.690000000000001,16.600000000000001]
[null,null,null,null,"Coincident",15.9,15.63,15.51,15.51,15.48,15.49,15.42]
[null,"Careel Bay 33_11kV","Substation Rating","MVA","Non-Coincident",21.68,21.68,21.68,21.68,21.68,21.68,21.68]
[null,null,null,null,"Coincident",19.7,19.7,19.7,19.7,19.7,19.7,19.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1999999999999999E-2,-4.3999999999999997E-2,-6.6000000000000003E-2,-9.5000000000000001E-2,-0.13100000000000001,-0.16500000000000001,-0.19500000000000001]
[null,null,null,null,"Coincident",-1.204,-1.579,-1.8120000000000001,-1.954,-2.089,-2.2240000000000002,-2.3570000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.34,13.34,13.33,13.37,13.4,13.36,13.32]
[null,null,null,null,"Coincident",10.73,10.83,10.89,10.89,10.89,10.85,10.82]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.53,13.52,13.52,13.56,13.59,13.55,13.51]
[null,null,null,null,"Coincident",10.73,10.83,10.89,10.89,10.89,10.85,10.82]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.76,12.75,12.75,12.78,12.82,12.78,12.74]
[null,null,null,null,"Coincident",9.2669999999999995,9.3580000000000005,9.4039999999999999,9.4060000000000006,9.4060000000000006,9.3640000000000008,9.3330000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.94,12.93,12.93,12.97,13,12.96,12.92]
[null,null,null,null,"Coincident",9.2669999999999995,9.3580000000000005,9.4039999999999999,9.4060000000000006,9.4060000000000006,9.3640000000000008,9.3330000000000002]
[null,"Caringbah 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.623,-0.80600000000000005,-0.96799999999999997,-1.139,-1.3580000000000001,-1.5640000000000001,-1.766]
[null,null,null,null,"Coincident",-0.91,-1.149,-1.3460000000000001,-1.5369999999999999,-1.77,-2.0009999999999999,-2.2290000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.65,28.87,29.03,29.17,29.23,29.24,29.24]
[null,null,null,null,"Coincident",25.89,27.03,27.18,27.31,27.36,27.37,27.37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.53,30.79,30.96,31.11,31.17,31.18,31.18]
[null,null,null,null,"Coincident",27.64,28.82,28.98,29.12,29.18,29.19,29.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.45,26.68,26.84,26.98,27.04,27.05,27.05]
[null,null,null,null,"Coincident",23.83,24.97,25.13,25.26,25.31,25.32,25.32]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.16,28.44,28.61,28.76,28.82,28.83,28.83]
[null,null,null,null,"Coincident",25.43,26.62,26.78,26.92,26.98,26.98,26.98]
[null,"Castle Cove 132_11kV","Substation Rating","MVA","Non-Coincident",96.25,96.25,96.25,96.25,96.25,96.25,96.25]
[null,null,null,null,"Coincident",90.65,90.65,90.65,90.65,90.65,90.65,90.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.9000000000000002E-2,-9.8000000000000004E-2,-0.16200000000000001,-0.25600000000000001,-0.379,-0.495,-0.59299999999999997]
[null,null,null,null,"Coincident",-3.0819999999999999,-3.988,-4.6349999999999998,-5.1539999999999999,-5.7350000000000003,-6.3150000000000004,-6.8840000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.43,50.97,54.31,54.53,55.35,56.2,57.19]
[null,null,null,null,"Coincident",48.61,47.87,49.94,50.09,50.38,51.93,52.31]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.86,52.52,56.16,56.4,57.29,58.23,59.3]
[null,null,null,null,"Coincident",57.31,56.34,59.04,59.24,59.61,61.64,62.14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",47.85,49.74,53.34,53.69,54.5,55.36,56.34]
[null,null,null,null,"Coincident",44.59,43.92,46.03,46.19,46.47,48.03,48.41]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.13,51.19,55.1,55.48,56.37,57.31,58.38]
[null,null,null,null,"Coincident",52.08,51.21,53.95,54.16,54.53,56.55,57.05]
[null,"Cessnock South 33_11kV","Substation Rating","MVA","Non-Coincident",28.48,28.48,28.48,28.48,28.48,28.48,28.48]
[null,null,null,null,"Coincident",28.48,28.48,28.48,28.48,28.48,28.48,28.48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.67800000000000005,-0.92700000000000005,-1.0940000000000001,-1.2150000000000001,-1.3460000000000001,-1.47,-1.417]
[null,null,null,null,"Coincident",-1.7250000000000001,-2.2589999999999999,-2.5910000000000002,-2.7909999999999999,-2.9809999999999999,-3.17,-3.3570000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.840000000000003,33.979999999999997,34.08,34.130000000000003,34.15,34.32,34.32]
[null,null,null,null,"Coincident",23.42,23.52,23.58,23.62,23.63,23.75,23.75]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.36,34.49,34.590000000000003,34.65,34.67,34.83,34.840000000000003]
[null,null,null,null,"Coincident",23.78,23.87,23.94,23.98,23.99,24.11,24.11]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.5,30.61,30.71,30.76,30.78,30.94,30.95]
[null,null,null,null,"Coincident",21.11,21.19,21.25,21.28,21.3,21.41,21.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.96,31.08,31.17,31.22,31.24,31.41,31.42]
[null,null,null,null,"Coincident",21.42,21.51,21.57,21.61,21.62,21.74,21.74]
[null,"Charlestown 132_11kV","Substation Rating","MVA","Non-Coincident",60.17,60.17,60.17,60.17,60.17,60.17,60.17]
[null,null,null,null,"Coincident",60.17,60.17,60.17,60.17,60.17,60.17,60.17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.4630000000000001,-1.6659999999999999,-1.8109999999999999,-1.93,-2.0649999999999999,-2.1930000000000001,-2.3140000000000001]
[null,null,null,null,"Coincident",-2.3769999999999998,-3.0920000000000001,-3.55,-3.8460000000000001,-4.1390000000000002,-4.4329999999999998,-4.7229999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.21,41.14,41.11,41.09,41.03,41.01,40.840000000000003]
[null,null,null,null,"Coincident",39.24,39.17,39.14,39.130000000000003,39.07,39.049999999999997,38.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.22,41.15,41.12,41.1,41.03,41.02,40.85]
[null,null,null,null,"Coincident",39.25,39.18,39.15,39.14,39.07,39.06,38.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.93,35.86,35.83,35.81,35.74,35.729999999999997,35.56]
[null,null,null,null,"Coincident",34.21,34.14,34.11,34.1,34.04,34.020000000000003,33.86]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.93,35.86,35.83,35.81,35.74,35.729999999999997,35.56]
[null,null,null,null,"Coincident",34.21,34.14,34.11,34.1,34.04,34.020000000000003,33.86]
[null,"Charmhaven 132_11kV","Substation Rating","MVA","Non-Coincident",63.25,63.25,63.25,63.25,63.25,63.25,63.25]
[null,null,null,null,"Coincident",63.25,63.25,63.25,63.25,63.25,63.25,63.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.6930000000000001,-2.073,-2.323,-2.4990000000000001,-2.6859999999999999,-2.8639999999999999,-3.0350000000000001]
[null,null,null,null,"Coincident",-3.4820000000000002,-4.5679999999999996,-5.2270000000000003,-5.6020000000000003,-5.9379999999999997,-6.2759999999999998,-6.61]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.86,51.23,51.27,51.81,52.3,52.3,52.27]
[null,null,null,null,"Coincident",48.53,48.89,48.92,49.43,49.9,49.9,49.88]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.36,51.75,51.78,52.32,52.82,52.82,52.79]
[null,null,null,null,"Coincident",49.01,49.37,49.41,49.93,50.4,50.4,50.37]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.04,45.48,45.55,46.09,46.58,46.58,46.56]
[null,null,null,null,"Coincident",42.97,43.4,43.46,43.98,44.44,44.45,44.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.48,45.94,46.01,46.55,47.04,47.05,47.02]
[null,null,null,null,"Coincident",43.4,43.83,43.9,44.42,44.89,44.89,44.87]
[null,"Chatswood 33_11kV","Substation Rating","MVA","Non-Coincident",70.510000000000005,70.510000000000005,70.510000000000005,70.510000000000005,70.510000000000005,70.510000000000005,70.510000000000005]
[null,null,null,null,"Coincident",67.14,67.14,67.14,67.14,67.14,67.14,67.14]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.5000000000000003E-2,-7.0999999999999994E-2,-0.12,-0.189,-0.28799999999999998,-0.379,-0.45900000000000002]
[null,null,null,null,"Coincident",-2.1890000000000001,-2.83,-3.3130000000000002,-3.7280000000000002,-4.2149999999999999,-4.702,-5.181]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.05,49.16,51.42,43.28,44.03,44.76,45.75]
[null,null,null,null,"Coincident",43.56,46.96,47.98,41.89,42.73,43.6,44.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.72,52.13,54.52,45.89,46.69,47.46,48.51]
[null,null,null,null,"Coincident",47.49,51.19,52.3,45.66,46.58,47.53,48.74]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.29,47.45,49.75,41.62,42.37,43.1,44.09]
[null,null,null,null,"Coincident",39.369999999999997,42.85,43.91,37.82,38.659999999999997,39.53,40.65]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.85,50.32,52.75,44.13,44.93,45.7,46.75]
[null,null,null,null,"Coincident",42.91,46.7,47.86,41.22,42.14,43.09,44.3]
[null,"City Central 132_11kV","Substation Rating","MVA","Non-Coincident",128,128,128,128,128,128,128]
[null,null,null,null,"Coincident",128,128,128,128,128,128,128]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.52700000000000002,-0.99,-1.4990000000000001,-1.9910000000000001,-2.7509999999999999,-3.4729999999999999,-3.6669999999999998]
[null,null,null,null,"Coincident",-1.4590000000000001,-1.782,-2.145,-2.6150000000000002,-3.234,-3.8519999999999999,-4.4530000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",101.8,109,109.7,110.5,111.3,112.5,113.2]
[null,null,null,null,"Coincident",86.69,92.78,93.4,94.05,94.71,95.81,96.37]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",101.9,109,109.7,110.5,111.3,112.6,113.3]
[null,null,null,null,"Coincident",86.71,92.78,93.42,94.07,94.73,95.84,96.41]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",97.35,104.6,105.4,106.1,106.9,108.2,108.9]
[null,null,null,null,"Coincident",82.88,89.04,89.71,90.36,91.02,92.11,92.68]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",97.35,104.7,105.4,106.1,106.9,108.2,108.9]
[null,null,null,null,"Coincident",82.88,89.09,89.76,90.36,91.02,92.12,92.69]
[null,"City East 33_11kV","Substation Rating","MVA","Non-Coincident",75.55,"NC","NC","NC","NC","NC","NC"]
[null,null,null,null,"Coincident",70.66,"NC","NC","NC","NC","NC","NC"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.113]
[null,null,null,null,"Coincident",-0.51700000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.84]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.46]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.55]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.14]
[null,null,null,null,"Coincident"]
[null,"City North 132_11kV","Substation Rating","MVA","Non-Coincident",167.9,167.9,167.9,167.9,167.9,167.9,167.9]
[null,null,null,null,"Coincident",167.9,167.9,167.9,167.9,167.9,167.9,167.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.59899999999999998,-1.0820000000000001,-1.637,-2.3039999999999998,-3.177,-4,-3.7650000000000001]
[null,null,null,null,"Coincident",-1.6539999999999999,-2.0190000000000001,-2.423,-2.9390000000000001,-3.6150000000000002,-4.2889999999999997,-4.9459999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",115.9,117.7,120.1,121.2,122.2,124.5,125.5]
[null,null,null,null,"Coincident",94.79,96.25,98.23,99.11,99.98,101.8,102.7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",115.9,117.7,120.1,121.2,122.2,124.5,125.6]
[null,null,null,null,"Coincident",94.83,96.3,98.23,99.11,99.99,101.8,102.7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",110.9,112.8,115.2,116.3,117.4,119.6,120.7]
[null,null,null,null,"Coincident",90.7,92.24,94.26,95.14,96.01,97.85,98.72]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",110.9,112.8,115.3,116.4,117.4,119.6,120.7]
[null,null,null,null,"Coincident",90.71,92.26,94.3,95.18,96.06,97.86,98.73]
[null,"City South 132_11kV","Substation Rating","MVA","Non-Coincident",130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001]
[null,null,null,null,"Coincident",130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001,130.30000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.63700000000000001,-1.2330000000000001,-1.921,-2.758,-3.8650000000000002,-4.6550000000000002,-5.609]
[null,null,null,null,"Coincident",-1.67,-2.0529999999999999,-2.4790000000000001,-3.024,-3.7429999999999999,-4.4610000000000003,-5.1609999999999996]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",114,113.1,112.8,113.4,114.3,115.2,115.8]
[null,null,null,null,"Coincident",99.94,99.17,98.88,99.38,100.3,101,101.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",114,113.1,112.8,113.4,114.4,115.2,115.8]
[null,null,null,null,"Coincident",99.95,99.17,98.88,99.39,100.3,101,101.6]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",108.9,108.1,107.9,108.4,109.4,110.3,110.9]
[null,null,null,null,"Coincident",95.49,94.81,94.56,95.07,95.94,96.69,97.23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",109,108.2,107.9,108.5,109.5,110.3,110.9]
[null,null,null,null,"Coincident",95.54,94.85,94.6,95.11,95.99,96.69,97.23]
[null,"Clovelly 132_11kV","Substation Rating","MVA","Non-Coincident",92.98,92.98,92.98,92.98,92.98,92.98,92.98]
[null,null,null,null,"Coincident",87.64,87.64,87.64,87.64,87.64,87.64,87.64]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.8000000000000001E-2,-2.8000000000000001E-2,-5.2999999999999999E-2,-9.2999999999999999E-2,-0.15,-0.20200000000000001,-0.247]
[null,null,null,null,"Coincident",-1.6739999999999999,-2.1469999999999998,-2.5350000000000001,-2.9049999999999998,-3.3610000000000002,-3.8170000000000002,-4.266]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.84,52.99,53.9,54.19,54.2,54.14,54.01]
[null,null,null,null,"Coincident",36.409999999999997,37.369999999999997,37.71,37.76,38.08,38.049999999999997,37.909999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.97,53.12,54.04,54.33,54.34,54.27,54.15]
[null,null,null,null,"Coincident",36.68,37.65,38,38.049999999999997,38.369999999999997,38.340000000000003,38.200000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.93,51.81,53.23,53.78,53.79,53.73,53.6]
[null,null,null,null,"Coincident",33.340000000000003,34.25,34.58,34.630000000000003,34.94,34.92,34.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",50.06,51.94,53.36,53.92,53.93,53.86,53.74]
[null,null,null,null,"Coincident",33.590000000000003,34.520000000000003,34.840000000000003,34.9,35.21,35.18,35.04]
[null,"Concord 33_11kV","Substation Rating","MVA","Non-Coincident",54.41,54.41,54.41,54.41,54.41,54.41,54.41]
[null,null,null,null,"Coincident",54.41,54.41,54.41,54.41,54.41,54.41,54.41]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1,-1.43,-1.772,-2.0870000000000002,-2.4809999999999999,-2.8540000000000001,-3.22]
[null,null,null,null,"Coincident",-1.647,-2.129,-2.4910000000000001,-2.8039999999999998,-3.1709999999999998,-3.5390000000000001,-3.9]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.64,54.14,55.25,56.42,56.65,56.85,56.83]
[null,null,null,null,"Coincident",48.94,52.32,53.39,54.53,54.75,54.94,54.93]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53,56.59,57.75,58.97,59.22,59.42,59.4]
[null,null,null,null,"Coincident",51.22,54.69,55.81,56.99,57.23,57.42,57.41]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.7,48.21,49.33,50.5,50.74,50.93,50.92]
[null,null,null,null,"Coincident",43.2,46.6,47.67,48.81,49.03,49.22,49.21]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.78,50.39,51.55,52.78,53.02,53.22,53.21]
[null,null,null,null,"Coincident",45.21,48.7,49.82,51.01,51.24,51.44,51.42]
[null,"Cronulla 132_11kV","Substation Rating","MVA","Non-Coincident",64.17,64.17,64.17,64.17,64.17,64.17,64.17]
[null,null,null,null,"Coincident",53.46,53.46,53.46,53.46,53.46,53.46,53.46]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-6.0999999999999999E-2,-0.123,-0.19400000000000001,-0.29299999999999998,-0.42599999999999999,-0.54900000000000004,-0.65800000000000003]
[null,null,null,null,"Coincident",-3.35,-4.3639999999999999,-5.0519999999999996,-5.5510000000000002,-6.0880000000000001,-6.625,-7.1539999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",61.7,64.569999999999993,65.48,65.7,65.62,65.489999999999995,65.25]
[null,null,null,null,"Coincident",44.87,46.07,46.26,46.42,46.19,47.07,46.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.51,65.42,66.34,66.56,66.48,66.349999999999994,66.11]
[null,null,null,null,"Coincident",45.98,47.21,47.4,47.57,47.34,48.23,48.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.54,61.69,62.79,63.11,63.03,62.89,62.66]
[null,null,null,null,"Coincident",39.200000000000003,40.380000000000003,40.56,40.72,40.49,41.36,41.28]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59.31,62.49,63.61,63.93,63.86,63.72,63.48]
[null,null,null,null,"Coincident",40.17,41.38,41.56,41.72,41.49,42.39,42.3]
[null,"Croudace Bay 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.47099999999999997,-0.625,-0.72799999999999998,-0.80100000000000005,-0.88100000000000001,-0.95599999999999996,-1.0289999999999999]
[null,null,null,null,"Coincident",-1.4379999999999999,-1.8779999999999999,-2.1480000000000001,-2.3050000000000002,-2.4500000000000002,-2.5939999999999999,-2.7370000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.98,20.6,20.420000000000002,20.399999999999999,20.37,20.309999999999999,20.23]
[null,null,null,null,"Coincident",18.87,18.53,18.37,18.350000000000001,18.32,18.27,18.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.83,23.34,23.1,23.08,23.04,22.96,22.85]
[null,null,null,null,"Coincident",21.44,20.99,20.78,20.75,20.72,20.65,20.55]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.89,16.579999999999998,16.440000000000001,16.420000000000002,16.39,16.329999999999998,16.25]
[null,null,null,null,"Coincident",15.19,14.92,14.78,14.77,14.74,14.69,14.61]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.5,18.100000000000001,17.920000000000002,17.89,17.850000000000001,17.78,17.670000000000002]
[null,null,null,null,"Coincident",16.64,16.28,16.11,16.09,16.059999999999999,15.99,15.9]
[null,"Crows Nest 132_11kV","Substation Rating","MVA","Non-Coincident",65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005]
[null,null,null,null,"Coincident",61.64,61.64,61.64,61.64,61.64,61.64,61.64]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1000000000000001E-2,-4.2000000000000003E-2,-8.1000000000000003E-2,-0.14599999999999999,-0.24399999999999999,-0.33,-0.40400000000000003]
[null,null,null,null,"Coincident",-1.6359999999999999,-2.0670000000000002,-2.452,-2.8580000000000001,-3.3719999999999999,-3.8849999999999998,-4.3879999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.93,46.79,48.32,46.79,46.87,47.71,48.84]
[null,null,null,null,"Coincident",46.91,47.75,45.33,44.83,45.17,46.67,47.55]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.94,46.8,48.32,46.8,46.88,47.72,48.85]
[null,null,null,null,"Coincident",47.16,48,45.57,45.07,45.41,46.92,47.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.25,45.17,46.72,45.22,45.29,46.14,47.27]
[null,null,null,null,"Coincident",43.75,44.65,42.26,41.76,42.1,43.61,44.49]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.26,45.17,46.73,45.22,45.3,46.15,47.28]
[null,null,null,null,"Coincident",43.99,44.89,42.49,41.99,42.33,43.84,44.73]
[null,"Croydon 132_11kV","Substation Rating","MVA","Non-Coincident",65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005]
[null,null,null,null,"Coincident",62.57,62.57,62.57,62.57,62.57,62.57,62.57]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.5999999999999997E-2,-7.1999999999999995E-2,-0.12,-0.19,-0.28499999999999998,-0.373,-0.45100000000000001]
[null,null,null,null,"Coincident",-2.2210000000000001,-2.879,-3.351,-3.7280000000000002,-4.1550000000000002,-4.5819999999999999,-5.0030000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.369999999999997,40.700000000000003,41.5,44.39,46.69,47.06,47.51]
[null,null,null,null,"Coincident",35.880000000000003,37.619999999999997,39.770000000000003,42.23,42.5,43.12,43.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.369999999999997,40.700000000000003,41.51,44.4,46.7,47.07,47.51]
[null,null,null,null,"Coincident",35.94,37.67,39.81,42.27,42.53,43.15,43.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.03,39.909999999999997,41.1,44.18,46.48,46.85,47.3]
[null,null,null,null,"Coincident",32.28,33.99,36.130000000000003,38.590000000000003,38.86,39.47,39.72]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38.03,39.92,41.1,44.19,46.49,46.86,47.3]
[null,null,null,null,"Coincident",32.340000000000003,34.04,36.17,38.630000000000003,38.89,39.51,39.75]
[null,"Dalley St 132_11kV","Substation Rating","MVA","Non-Coincident",130,130,130,130,130,130,130]
[null,null,null,null,"Coincident",123.6,123.6,123.6,123.6,123.6,123.6,123.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.19800000000000001,-0.42199999999999999,-0.66300000000000003,-0.91100000000000003,-1.2589999999999999,-1.585,-1.899]
[null,null,null,null,"Coincident",-0.65800000000000003,-0.80900000000000005,-0.97,-1.173,-1.4370000000000001,-1.7010000000000001,-1.958]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.72,16.88,19.3,19.21,19.07,18.899999999999999,18.78]
[null,null,null,null,"Coincident",12.35,14.15,14.86,14.53,14.19,15.05,14.87]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.17,16.899999999999999,19.36,19.260000000000002,19.12,18.95,18.829999999999998]
[null,null,null,null,"Coincident",13.27,15.21,15.96,15.61,15.24,16.170000000000002,15.98]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.16,15.37,17.82,17.739999999999998,17.61,17.440000000000001,17.32]
[null,null,null,null,"Coincident",10.78,12.61,13.32,13,12.65,13.51,13.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.56,15.38,17.86,17.77,17.64,17.46,17.34]
[null,null,null,null,"Coincident",11.64,13.61,14.38,14.03,13.66,14.59,14.4]
[null,"Darling Harbour 132_11kV","Substation Rating","MVA","Non-Coincident",70.3,70.3,70.3,70.3,70.3,70.3,70.3]
[null,null,null,null,"Coincident",70.3,70.3,70.3,70.3,70.3,70.3,70.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.89100000000000001,-1.1579999999999999,-1.3009999999999999,-1.4610000000000001,-1.3260000000000001,-1.26,-1.3320000000000001]
[null,null,null,null,"Coincident",-1.4279999999999999,-1.8149999999999999,-2.1800000000000002,-2.5859999999999999,-3.1080000000000001,-3.6309999999999998,-4.1420000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",61.13,59.63,59.41,60.59,61.59,62.44,63.01]
[null,null,null,null,"Coincident",58.34,56.91,56.7,57.83,58.79,59.59,60.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",63.17,61.62,61.39,62.61,63.64,64.510000000000005,65.09]
[null,null,null,null,"Coincident",60.29,58.81,58.59,59.75,60.74,61.56,62.13]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",57.53,56.1,55.91,57.1,58.1,58.95,59.52]
[null,null,null,null,"Coincident",54.91,53.54,53.36,54.49,55.45,56.26,56.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59.45,57.98,57.78,59,60.03,60.9,61.49]
[null,null,null,null,"Coincident",56.74,55.34,55.15,56.31,57.3,58.12,58.69]
[null,"Darlinghurst 33_11kV","Substation Rating","MVA","Non-Coincident",80.59,80.59,80.59,80.59,80.59,80.59,80.59]
[null,null,null,null,"Coincident",80.59,80.59,80.59,80.59,80.59,80.59,80.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.754,-1.196,-1.66,-2.206,-2.9460000000000002,-3.6469999999999998,-4.3369999999999997]
[null,null,null,null,"Coincident",-1.139,-1.421,-1.704,-2.0339999999999998,-2.4649999999999999,-2.895,-3.3159999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.19,24.41,23.9,23.61,23.26,23.01,23.76]
[null,null,null,null,"Coincident",37,21.92,21.46,21.2,20.89,20.66,21.34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.02,24.9,24.38,24.08,23.73,23.47,24.24]
[null,null,null,null,"Coincident",37.74,22.36,21.9,21.63,21.31,21.08,21.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.89,22.15,21.66,21.37,21.02,20.77,21.52]
[null,null,null,null,"Coincident",34.93,19.899999999999999,19.45,19.190000000000001,18.88,18.66,19.329999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.68,22.6,22.09,21.8,21.45,21.19,21.95]
[null,null,null,null,"Coincident",35.64,20.3,19.850000000000001,19.579999999999998,19.260000000000002,19.03,19.72]
[null,"Dee Why West 33_11kV","Substation Rating","MVA","Non-Coincident",58.78,58.78,58.78,58.78,58.78,58.78,58.78]
[null,null,null,null,"Coincident",53.45,53.45,53.45,53.45,53.45,53.45,53.45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.5999999999999999E-2,-9.0999999999999998E-2,-0.14799999999999999,-0.23,-0.34399999999999997,-0.44800000000000001,-0.53900000000000003]
[null,null,null,null,"Coincident",-2.7450000000000001,-3.5640000000000001,-4.1349999999999998,-4.5709999999999997,-5.0540000000000003,-5.5380000000000003,-6.0129999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.58,48.05,48.8,49.04,49.23,49.27,49.28]
[null,null,null,null,"Coincident",32.21,32.81,32.99,33.14,33.24,33.229999999999997,33.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.68,49.19,49.96,50.21,50.4,50.44,50.45]
[null,null,null,null,"Coincident",34.64,35.28,35.479999999999997,35.630000000000003,35.74,35.729999999999997,35.75]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.31,45.85,46.66,46.93,47.12,47.16,47.17]
[null,null,null,null,"Coincident",29.43,30.02,30.21,30.36,30.46,30.44,30.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.36,46.94,47.77,48.05,48.23,48.28,48.29]
[null,null,null,null,"Coincident",31.65,32.28,32.49,32.64,32.75,32.74,32.76]
[null,"Denman 66_11kV","Substation Rating","MVA","Non-Coincident",15.34,15.34,15.34,15.34,15.34,15.34,15.34]
[null,null,null,null,"Coincident",15.34,15.34,15.34,15.34,15.34,15.34,15.34]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.0999999999999999E-2,-2.1000000000000001E-2,-0.03,-4.1000000000000002E-2,-5.5E-2,-6.7000000000000004E-2,-7.8E-2]
[null,null,null,null,"Coincident",-0.30099999999999999,-0.38500000000000001,-0.442,-0.48499999999999999,-0.53,-0.57399999999999995,-0.61799999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.5720000000000001,7.6280000000000001,7.6639999999999997,7.6829999999999998,7.7,7.7149999999999999,7.7240000000000002]
[null,null,null,null,"Coincident",5.8179999999999996,5.8620000000000001,5.8890000000000002,5.9039999999999999,5.9169999999999998,5.9290000000000003,5.9349999999999996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.6829999999999998,7.74,7.7759999999999998,7.7960000000000003,7.8129999999999997,7.8280000000000003,7.8369999999999997]
[null,null,null,null,"Coincident",5.9039999999999999,5.9480000000000004,5.976,5.9909999999999997,6.0039999999999996,6.0149999999999997,6.0220000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.806,6.8570000000000002,6.89,6.9089999999999998,6.9260000000000002,6.9409999999999998,6.9489999999999998]
[null,null,null,null,"Coincident",5.23,5.2690000000000001,5.2949999999999999,5.3090000000000002,5.3220000000000001,5.3339999999999996,5.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.9059999999999997,6.9569999999999999,6.9909999999999997,7.01,7.0270000000000001,7.0430000000000001,7.0510000000000002]
[null,null,null,null,"Coincident",5.3070000000000004,5.3460000000000001,5.3719999999999999,5.3869999999999996,5.4,5.4119999999999999,5.4180000000000001]
[null,"Double Bay 132_11kV","Substation Rating","MVA","Non-Coincident",87.79,87.79,87.79,87.79,87.79,87.79,87.79]
[null,null,null,null,"Coincident",81.28,81.28,81.28,81.28,81.28,81.28,81.28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.03,-5.8999999999999997E-2,-0.111,-0.19400000000000001,-0.315,-0.42099999999999999,-0.51200000000000001]
[null,null,null,null,"Coincident",-2.1560000000000001,-2.7610000000000001,-3.258,-3.734,-4.3170000000000002,-4.899,-5.4710000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63.05,62.76,62.85,63.04,63.79,64.45,65.010000000000005]
[null,null,null,null,"Coincident",55.76,55.21,55.02,55.72,56.31,56.7,57.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",63.54,63.24,63.33,63.52,64.28,64.94,65.5]
[null,null,null,null,"Coincident",56.9,56.34,56.15,56.86,57.46,57.87,58.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",61.14,61.49,62,62.4,63.15,63.81,64.37]
[null,null,null,null,"Coincident",51.63,51.14,50.99,51.68,52.28,52.67,53.27]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",61.61,61.96,62.47,62.88,63.64,64.3,64.86]
[null,null,null,null,"Coincident",52.69,52.19,52.03,52.74,53.35,53.75,54.36]
[null,"Drummoyne 132_11kV","Substation Rating","MVA","Non-Coincident",61.77,61.77,61.77,61.77,61.77,61.77,61.77]
[null,null,null,null,"Coincident",56.15,56.15,56.15,56.15,56.15,56.15,56.15]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-5.6000000000000001E-2,-0.113,-0.185,-0.29099999999999998,-0.438,-0.57099999999999995,-0.68899999999999995]
[null,null,null,null,"Coincident",-3.3559999999999999,-4.351,-5.0570000000000004,-5.6109999999999998,-6.2329999999999997,-6.8550000000000004,-7.4669999999999996]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",58.42,63.7,63.97,63.92,64.680000000000007,65.239999999999995,65.97]
[null,null,null,null,"Coincident",55.43,59.7,60.05,60.54,61.01,61.6,61.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",59.34,64.66,64.930000000000007,64.88,65.650000000000006,66.22,66.959999999999994]
[null,null,null,null,"Coincident",55.75,60.04,60.38,60.88,61.35,61.94,62.33]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",55.57,61.1,61.54,61.58,62.34,62.9,63.63]
[null,null,null,null,"Coincident",48.75,53,53.34,53.83,54.3,54.89,55.28]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.45,62.01,62.46,62.5,63.27,63.85,64.58]
[null,null,null,null,"Coincident",49.03,53.3,53.64,54.13,54.6,55.19,55.58]
[null,"Dulwich Hill 33_11kV","Substation Rating","MVA","Non-Coincident",61.9,"NC","NC","NC","NC","NC","NC"]
[null,null,null,null,"Coincident",61.9,"NC","NC","NC","NC","NC","NC"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1E-3]
[null,null,null,null,"Coincident",-2.9510000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.03]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.31]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.58]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.8]
[null,null,null,null,"Coincident"]
[null,"Edgeworth 33_11kV","Substation Rating","MVA","Non-Coincident",22.86,22.86,22.86,22.86,22.86,22.86,22.86]
[null,null,null,null,"Coincident",22.86,22.86,22.86,22.86,22.86,22.86,22.86]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.73699999999999999,-1.03,-1.216,-1.337,-1.4590000000000001,-1.5760000000000001,-1.6890000000000001]
[null,null,null,null,"Coincident",-1.885,-2.4700000000000002,-2.823,-3.0209999999999999,-3.1949999999999998,-3.37,-3.5430000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.58,32.81,32.909999999999997,32.86,32.76,32.72,32.9]
[null,null,null,null,"Coincident",27.9,28.1,28.19,28.14,28.05,28.02,28.17]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.89,33.130000000000003,33.229999999999997,33.18,33.07,33.03,33.21]
[null,null,null,null,"Coincident",28.17,28.37,28.46,28.41,28.32,28.29,28.44]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.12,29.33,29.42,29.37,29.27,29.23,29.41]
[null,null,null,null,"Coincident",24.94,25.12,25.2,25.15,25.06,25.03,25.18]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.41,29.62,29.71,29.66,29.55,29.51,29.69]
[null,null,null,null,"Coincident",25.18,25.36,25.44,25.4,25.3,25.27,25.42]
[null,"Empire Bay 66_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5000000000000001E-2,-0.05,-7.1999999999999995E-2,-9.9000000000000005E-2,-0.13300000000000001,-0.16600000000000001,-0.19500000000000001]
[null,null,null,null,"Coincident",-1.2509999999999999,-1.6439999999999999,-1.8779999999999999,-2.0049999999999999,-2.1139999999999999,-2.2240000000000002,-2.3319999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.14,13.36,13.54,13.65,13.64,13.6,13.54]
[null,null,null,null,"Coincident",12.58,12.79,12.9,12.9,12.87,12.83,12.77]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.18,13.4,13.58,13.7,13.68,13.64,13.58]
[null,null,null,null,"Coincident",12.72,12.94,13.05,13.05,13.02,12.98,12.91]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.18,12.34,12.47,12.56,12.55,12.5,12.45]
[null,null,null,null,"Coincident",10.83,11.01,11.11,11.11,11.08,11.04,10.98]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.22,12.38,12.51,12.6,12.59,12.54,12.49]
[null,null,null,null,"Coincident",10.96,11.14,11.23,11.24,11.21,11.17,11.1]
[null,"Enfield 33_11kV","Substation Rating","MVA","Non-Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,null,null,"Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Engadine 132_11kV","Substation Rating","MVA","Non-Coincident",68.569999999999993,68.569999999999993,68.569999999999993,68.569999999999993,68.569999999999993,68.569999999999993,68.569999999999993]
[null,null,null,null,"Coincident",59.84,59.84,59.84,59.84,59.84,59.84,59.84]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.9000000000000002E-2,-9.7000000000000003E-2,-0.14399999999999999,-0.20200000000000001,-0.27700000000000002,-0.34699999999999998,-0.4]
[null,null,null,null,"Coincident",-2.6680000000000001,-3.4980000000000002,-4.008,-4.3079999999999998,-4.5860000000000003,-4.8639999999999999,-5.1379999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.42,31.9,31.91,31.87,31.81,31.69,31.61]
[null,null,null,null,"Coincident",31.34,31.89,32.020000000000003,31.95,31.84,31.64,31.47]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.48,31.96,31.96,31.92,31.87,31.75,31.66]
[null,null,null,null,"Coincident",31.57,32.119999999999997,32.26,32.18,32.07,31.87,31.7]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.1,31.04,31.36,31.48,31.43,31.31,31.22]
[null,null,null,null,"Coincident",27.39,27.91,28.02,27.95,27.84,27.64,27.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.15,31.1,31.42,31.54,31.48,31.36,31.27]
[null,null,null,null,"Coincident",27.59,28.11,28.23,28.16,28.04,27.85,27.68]
[null,"Epping 66_11kV","Substation Rating","MVA","Non-Coincident",74.91,74.91,74.91,74.91,74.91,74.91,74.91]
[null,null,null,null,"Coincident",74.91,74.91,74.91,74.91,74.91,74.91,74.91]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.5369999999999999,-2.1669999999999998,-2.641,-3.05,-3.548,-4.0199999999999996,-4.484]
[null,null,null,null,"Coincident",-2.3210000000000002,-3.0230000000000001,-3.5259999999999998,-3.927,-4.3849999999999998,-4.8449999999999998,-5.2960000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",70.75,73.31,73.739999999999995,74.11,74.459999999999994,74.84,75.13]
[null,null,null,null,"Coincident",67.64,70.09,70.5,70.849999999999994,71.180000000000007,71.55,71.83]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",70.75,73.31,73.75,74.12,74.459999999999994,74.849999999999994,75.14]
[null,null,null,null,"Coincident",67.64,70.09,70.510000000000005,70.86,71.19,71.56,71.83]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.81,66.5,67,67.36,67.709999999999994,68.099999999999994,68.38]
[null,null,null,null,"Coincident",61.01,63.57,64.05,64.400000000000006,64.73,65.099999999999994,65.38]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",63.88,66.5,67,67.36,67.709999999999994,68.099999999999994,68.38]
[null,null,null,null,"Coincident",61.07,63.58,64.05,64.400000000000006,64.73,65.099999999999994,65.38]
[null,"Erina 66_11kV","Substation Rating","MVA","Non-Coincident",46.94,46.94,46.94,46.94,46.94,46.94,46.94]
[null,null,null,null,"Coincident",46.94,46.94,46.94,46.94,46.94,46.94,46.94]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.6220000000000001,-2.1040000000000001,-2.5129999999999999,-2.8220000000000001,-2.8180000000000001,-3.0939999999999999,-3.3650000000000002]
[null,null,null,null,"Coincident",-1.96,-2.5430000000000001,-2.93,-3.2029999999999998,-3.488,-3.7730000000000001,-4.0529999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.89,38.68,38.57,38.92,38.880000000000003,38.869999999999997,38.770000000000003]
[null,null,null,null,"Coincident",38.159999999999997,37.96,37.85,38.19,38.159999999999997,38.15,38.049999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39,38.799999999999997,38.68,39.03,39,38.99,38.89]
[null,null,null,null,"Coincident",38.270000000000003,38.07,37.96,38.31,38.270000000000003,38.26,38.159999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.97,33.75,33.630000000000003,33.979999999999997,33.950000000000003,33.94,33.840000000000003]
[null,null,null,null,"Coincident",33.340000000000003,33.130000000000003,33.01,33.35,33.32,33.31,33.21]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.04,33.83,33.700000000000003,34.049999999999997,34.020000000000003,34.01,33.909999999999997]
[null,null,null,null,"Coincident",33.409999999999997,33.200000000000003,33.08,33.42,33.39,33.380000000000003,33.28]
[null,"Flemington 132_11kV","Substation Rating","MVA","Non-Coincident",49.3,49.3,49.3,49.3,49.3,49.3,49.3]
[null,null,null,null,"Coincident",49.3,49.3,49.3,49.3,49.3,49.3,49.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.2329999999999997,-4.8650000000000002,-5.4279999999999999,-6.0030000000000001,-6.585,-7.2510000000000003,-7.3860000000000001]
[null,null,null,null,"Coincident",-0.96099999999999997,-1.236,-1.458,-1.669,-1.927,-2.1850000000000001,-2.4369999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.49,42.91,42.41,42.06,41.52,41.58,41.42]
[null,null,null,null,"Coincident",37.74,38.11,37.67,37.35,36.880000000000003,36.93,36.79]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.26,44.68,44.17,43.8,43.24,43.3,43.14]
[null,null,null,null,"Coincident",39.31,39.69,39.229999999999997,38.9,38.409999999999997,38.46,38.32]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.11,38.6,38.15,37.79,37.25,37.31,37.159999999999997]
[null,null,null,null,"Coincident",33.85,34.29,33.880000000000003,33.57,33.090000000000003,33.14,33]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.69,40.200000000000003,39.729999999999997,39.36,38.799999999999997,38.86,38.700000000000003]
[null,null,null,null,"Coincident",35.25,35.71,35.29,34.96,34.46,34.51,34.369999999999997]
[null,"Galston 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.26,-0.28499999999999998,-0.32500000000000001,-0.35799999999999998,-0.39500000000000002,-0.42899999999999999,-0.46100000000000002]
[null,null,null,null,"Coincident",-0.54900000000000004,-0.71899999999999997,-0.82899999999999996,-0.90100000000000002,-0.97399999999999998,-1.046,-1.117]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.75,13.62,13.59,13.64,13.68,13.7,13.72]
[null,null,null,null,"Coincident",12.52,12.41,12.38,12.42,12.46,12.48,12.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.27,14.13,14.1,14.15,14.2,14.22,14.24]
[null,null,null,null,"Coincident",12.99,12.87,12.84,12.89,12.93,12.95,12.97]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.31,12.22,12.2,12.25,12.29,12.31,12.33]
[null,null,null,null,"Coincident",11.22,11.13,11.11,11.16,11.19,11.21,11.23]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.78,12.68,12.66,12.71,12.75,12.78,12.8]
[null,null,null,null,"Coincident",11.64,11.55,11.53,11.58,11.62,11.64,11.66]
[null,"Gateshead 33_11kV","Substation Rating","MVA","Non-Coincident",24.41,24.41,24.41,24.41,24.41,24.41,24.41]
[null,null,null,null,"Coincident",24.08,24.08,24.08,24.08,24.08,24.08,24.08]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.8000000000000001E-2,-5.2999999999999999E-2,-7.9000000000000001E-2,-0.112,-0.154,-0.19400000000000001,-0.22900000000000001]
[null,null,null,null,"Coincident",-1.492,-1.95,-2.2410000000000001,-2.4249999999999998,-2.605,-2.7839999999999998,-2.9609999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.16,15.45,15.66,15.78,15.81,15.76,15.7]
[null,null,null,null,"Coincident",15.45,15.22,15.04,15.02,14.96,14.9,14.78]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.850000000000001,17.16,17.399999999999999,17.54,17.559999999999999,17.510000000000002,17.45]
[null,null,null,null,"Coincident",17.170000000000002,16.91,16.71,16.690000000000001,16.62,16.55,16.43]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.19,14.45,14.65,14.77,14.79,14.75,14.69]
[null,null,null,null,"Coincident",13.46,13.27,13.11,13.09,13.03,12.97,12.85]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.76,16.059999999999999,16.28,16.41,16.440000000000001,16.38,16.32]
[null,null,null,null,"Coincident",14.96,14.74,14.57,14.55,14.48,14.41,14.28]
[null,"Gore Hill 33_11kV","Substation Rating","MVA","Non-Coincident",96.9,96.9,96.9,96.9,96.9,96.9,96.9]
[null,null,null,null,"Coincident",96.9,96.9,96.9,96.9,96.9,96.9,96.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.7989999999999999,-2.177,-2.5649999999999999,-3.0070000000000001,-3.5960000000000001,-4.1550000000000002,-4.7030000000000003]
[null,null,null,null,"Coincident",-1.0549999999999999,-1.3180000000000001,-1.5740000000000001,-1.8680000000000001,-2.2480000000000002,-2.6269999999999998,-2.9990000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.55,45.42,45,45.13,45.43,45.64,45.9]
[null,null,null,null,"Coincident",38.950000000000003,38.83,38.479999999999997,38.58,38.85,39.020000000000003,39.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.02,46.88,46.45,46.58,46.9,47.11,47.38]
[null,null,null,null,"Coincident",40.200000000000003,40.08,39.72,39.83,40.1,40.28,40.51]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.82,42.75,42.36,42.48,42.79,42.99,43.26]
[null,null,null,null,"Coincident",36.619999999999997,36.549999999999997,36.22,36.32,36.58,36.76,36.99]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.2,44.12,43.72,43.85,44.17,44.38,44.65]
[null,null,null,null,"Coincident",37.79,37.72,37.380000000000003,37.49,37.76,37.94,38.18]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Green Square 132_11kV","Substation Rating","MVA","Non-Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,null,null,"Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.5389999999999999,-2.0619999999999998,-2.5760000000000001,-3.145,-3.8919999999999999,-4.5970000000000004,-5.2839999999999998]
[null,null,null,null,"Coincident",-1.4259999999999999,-1.796,-2.1429999999999998,-2.5289999999999999,-3.0230000000000001,-3.5169999999999999,-4]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",62.2,62.15,62.09,62.11,62.15,62.49,62.4]
[null,null,null,null,"Coincident",56.44,56.39,56.34,56.35,56.39,56.7,56.62]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.79,62.74,62.68,62.69,62.74,63.08,62.99]
[null,null,null,null,"Coincident",56.97,56.92,56.87,56.88,56.92,57.23,57.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.63,58.65,58.62,58.64,58.68,59.02,58.94]
[null,null,null,null,"Coincident",53.2,53.21,53.19,53.21,53.25,53.55,53.48]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59.18,59.2,59.18,59.19,59.24,59.58,59.49]
[null,null,null,null,"Coincident",53.7,53.72,53.69,53.71,53.75,54.06,53.98]
[null,"Greenacre 132_11kV","Substation Rating","MVA","Non-Coincident",62.3,62.3,62.3,62.3,62.3,62.3,62.3]
[null,null,null,null,"Coincident",62.3,62.3,62.3,62.3,62.3,62.3,62.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",65.41,69.97,69.84,70.599999999999994,71.290000000000006,74.73,75.77]
[null,null,null,null,"Coincident",62.37,66.709999999999994,66.59,67.31,67.959999999999994,71.25,72.239999999999995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",66.37,70.959999999999994,70.84,71.650000000000006,72.38,76.069999999999993,77.19]
[null,null,null,null,"Coincident",63.28,67.66,67.540000000000006,68.319999999999993,69.010000000000005,72.53,73.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.97,63.59,63.49,64.25,64.94,68.38,69.42]
[null,null,null,null,"Coincident",56.22,60.63,60.54,61.26,61.91,65.19,66.19]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59.82,64.489999999999995,64.400000000000006,65.209999999999994,65.94,69.62,70.739999999999995]
[null,null,null,null,"Coincident",57.04,61.48,61.4,62.17,62.86,66.38,67.45]
[null,"Greenacre Park 132_11kV","Substation Rating","MVA","Non-Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,null,null,"Coincident","NC","NC","NC","NC","NC","NC","NC"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Gwawley Bay 132_11kV","Substation Rating","MVA","Non-Coincident",45.1,45.1,45.1,45.1,45.1,45.1,45.1]
[null,null,null,null,"Coincident",45.1,45.1,45.1,45.1,45.1,45.1,45.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.7320000000000002,-3.21,-3.585,-3.9,-4.2690000000000001,-4.6189999999999998,-4.9630000000000001]
[null,null,null,null,"Coincident",-1.6240000000000001,-2.1040000000000001,-2.44,-2.702,-2.9910000000000001,-3.2789999999999999,-3.5630000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.11,38.79,38.78,38.630000000000003,38.51,38.299999999999997,39.549999999999997]
[null,null,null,null,"Coincident",36.29,36.94,36.93,36.79,36.68,36.47,37.659999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.58,39.28,39.26,39.11,38.99,38.770000000000003,40.04]
[null,null,null,null,"Coincident",36.74,37.4,37.39,37.25,37.130000000000003,36.92,38.130000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.5,34.18,34.17,34.020000000000003,33.9,33.69,34.94]
[null,null,null,null,"Coincident",31.9,32.549999999999997,32.54,32.4,32.29,32.08,33.270000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.909999999999997,34.61,34.590000000000003,34.450000000000003,34.33,34.11,35.380000000000003]
[null,null,null,null,"Coincident",32.299999999999997,32.96,32.94,32.799999999999997,32.69,32.479999999999997,33.69]
[null,"Harbord 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.9000000000000001E-2,-5.8999999999999997E-2,-9.1999999999999998E-2,-0.14000000000000001,-0.20300000000000001,-0.26100000000000001,-0.315]
[null,null,null,null,"Coincident",-1.59,-2.0699999999999998,-2.391,-2.6179999999999999,-2.859,-3.1,-3.3370000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.74,23.45,23.3,23.27,23.27,23.41,23.46]
[null,null,null,null,"Coincident",14.49,14.77,14.91,14.97,15.09,15.08,15.01]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.64,24.35,24.19,24.15,24.15,24.31,24.35]
[null,null,null,null,"Coincident",15.75,16.05,16.2,16.260000000000002,16.399999999999999,16.38,16.32]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.53,22.27,22.13,22.1,22.11,22.25,22.3]
[null,null,null,null,"Coincident",13.26,13.52,13.65,13.71,13.84,13.82,13.76]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.39,23.12,22.97,22.94,22.95,23.1,23.14]
[null,null,null,null,"Coincident",14.4,14.68,14.82,14.89,15.02,15.01,14.94]
[null,"Homebush Bay 132_11kV","Substation Rating","MVA","Non-Coincident",53.18,53.18,53.18,53.18,53.18,53.18,53.18]
[null,null,null,null,"Coincident",53.18,53.18,53.18,53.18,53.18,53.18,53.18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.42,-1.7729999999999999,-2.1150000000000002,-2.4929999999999999,-2.9969999999999999,-3.4740000000000002,-3.9409999999999998]
[null,null,null,null,"Coincident",-0.99299999999999999,-1.266,-1.5189999999999999,-1.796,-2.153,-2.5110000000000001,-2.8610000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.74,51.1,48.12,48.35,48.52,48.7,48.81]
[null,null,null,null,"Coincident",43.43,45.54,42.88,43.08,43.23,43.39,43.49]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",49.09,51.48,48.47,48.7,48.88,49.05,49.16]
[null,null,null,null,"Coincident",43.74,45.87,43.19,43.39,43.55,43.71,43.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.12,47.56,44.62,44.84,45.01,45.19,45.3]
[null,null,null,null,"Coincident",40.21,42.38,39.75,39.96,40.11,40.270000000000003,40.369999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.45,47.91,44.94,45.17,45.34,45.52,45.63]
[null,null,null,null,"Coincident",40.5,42.69,40.049999999999997,40.25,40.4,40.56,40.659999999999997]
[null,"Hornsby 132_11kV","Substation Rating","MVA","Non-Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,null,null,"Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.4000000000000004,-4.9740000000000002,-5.4130000000000003,-5.8010000000000002,-6.2709999999999999,-5.6509999999999998,-5.931]
[null,null,null,null,"Coincident",-3.9140000000000001,-5.09,-5.9119999999999999,-6.5410000000000004,-7.2380000000000004,-7.9359999999999999,-8.6210000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",78.84,79.239999999999995,79.44,79.599999999999994,80.69,81.12,81.16]
[null,null,null,null,"Coincident",75.13,75.52,75.7,75.86,76.900000000000006,77.31,77.34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",78.84,79.25,79.44,79.61,80.7,81.13,81.17]
[null,null,null,null,"Coincident",75.14,75.52,75.709999999999994,75.86,76.91,77.319999999999993,77.349999999999994]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",69.78,70.23,70.45,70.61,71.7,72.14,72.17]
[null,null,null,null,"Coincident",66.5,66.930000000000007,67.14,67.290000000000006,68.33,68.75,68.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",69.83,70.290000000000006,70.5,70.67,71.760000000000005,72.14,72.17]
[null,null,null,null,"Coincident",66.55,66.98,67.19,67.349999999999994,68.39,68.75,68.78]
[null,"Hunters Hill 66_11kV","Substation Rating","MVA","Non-Coincident",72.25,72.25,72.25,72.25,72.25,72.25,72.25]
[null,null,null,null,"Coincident",72.25,72.25,72.25,72.25,72.25,72.25,72.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.673,-4.1470000000000002,-4.3369999999999997,-4.6230000000000002,-4.96,-5.2779999999999996,-5.5860000000000003]
[null,null,null,null,"Coincident",-3.129,-4.0919999999999996,-4.7439999999999998,-5.2149999999999999,-5.7210000000000001,-6.2270000000000003,-6.7249999999999996]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",67.53,68.489999999999995,69.209999999999994,69.56,70.069999999999993,70.5,71.12]
[null,null,null,null,"Coincident",65,65.92,66.61,66.95,67.44,67.86,68.45]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.25,74.290000000000006,75.08,75.459999999999994,76,76.48,77.150000000000006]
[null,null,null,null,"Coincident",70.510000000000005,71.510000000000005,72.260000000000005,72.63,73.150000000000006,73.61,74.25]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.54,59.43,60.12,60.47,60.98,61.42,62.03]
[null,null,null,null,"Coincident",56.34,57.2,57.87,58.21,58.69,59.12,59.71]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",63.5,64.47,65.22,65.599999999999994,66.150000000000006,66.63,67.290000000000006]
[null,null,null,null,"Coincident",61.12,62.05,62.78,63.14,63.67,64.13,64.77]
[null,"Hurstville North 132_11kV","Substation Rating","MVA","Non-Coincident",59.56,59.56,59.56,59.56,59.56,59.56,59.56]
[null,null,null,null,"Coincident",59.56,59.56,59.56,59.56,59.56,59.56,59.56]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.51600000000000001,-0.83,-1.0609999999999999,-1.2529999999999999,-0.65300000000000002,-0.73599999999999999,-0.81499999999999995]
[null,null,null,null,"Coincident",-1.361,-1.7689999999999999,-2.0510000000000002,-2.2650000000000001,-2.4980000000000002,-2.7320000000000002,-2.9620000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.43,26.68,26.56,27.4,27.57,27.82,27.74]
[null,null,null,null,"Coincident",25.77,26.01,25.89,26.71,26.88,27.12,27.04]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.48,26.73,26.61,27.46,27.63,27.89,27.8]
[null,null,null,null,"Coincident",25.81,26.06,25.94,26.77,26.94,27.19,27.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.96,24.24,24.15,24.98,25.15,25.4,25.32]
[null,null,null,null,"Coincident",23.36,23.63,23.54,24.35,24.52,24.76,24.68]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.98,24.27,24.17,25.02,25.19,25.45,25.36]
[null,null,null,null,"Coincident",23.38,23.66,23.57,24.39,24.56,24.81,24.72]
[null,"Jannali 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-5.3999999999999999E-2,-0.108,-0.159,-0.221,-0.30099999999999999,-0.376,-0.44400000000000001]
[null,null,null,null,"Coincident",-2.6680000000000001,-3.51,-4.0199999999999996,-4.3109999999999999,-4.5720000000000001,-4.835,-5.0940000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.369999999999997,34.950000000000003,35.31,35.47,35.409999999999997,35.24,35.11]
[null,null,null,null,"Coincident",33.17,33.72,34.11,33.85,33.67,33.5,33.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.89,35.479999999999997,35.840000000000003,36.01,35.950000000000003,35.78,35.64]
[null,null,null,null,"Coincident",33.49,34.049999999999997,34.450000000000003,34.18,34,33.83,33.57]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.729999999999997,33.4,33.81,34,33.94,33.770000000000003,33.64]
[null,null,null,null,"Coincident",28.54,29.01,29.36,29.1,28.92,28.75,28.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.229999999999997,33.909999999999997,34.32,34.51,34.46,34.28,34.15]
[null,null,null,null,"Coincident",28.82,29.29,29.65,29.38,29.2,29.03,28.78]
[null,"Jesmond 132_11kV","Substation Rating","MVA","Non-Coincident",57.48,57.48,57.48,57.48,57.48,57.48,57.48]
[null,null,null,null,"Coincident",57.48,57.48,57.48,57.48,57.48,57.48,57.48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.89700000000000002,-1.1000000000000001,-1.32,-1.488,-1.6759999999999999,-1.853,-2.024]
[null,null,null,null,"Coincident",-2.9350000000000001,-3.851,-4.4269999999999996,-4.7830000000000004,-5.1280000000000001,-5.4740000000000002,-5.8150000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.97,50.31,50.46,50.65,50.54,50.79,51]
[null,null,null,null,"Coincident",46.25,46.57,46.7,46.88,46.78,47.01,47.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.73,51.09,51.23,51.43,51.32,51.57,51.79]
[null,null,null,null,"Coincident",46.96,47.28,47.42,47.6,47.5,47.73,47.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.76,45.1,45.24,45.43,45.33,45.57,45.79]
[null,null,null,null,"Coincident",41.42,41.74,41.87,42.05,41.95,42.18,42.38]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.44,45.79,45.94,46.13,46.02,46.27,46.49]
[null,null,null,null,"Coincident",42.06,42.38,42.51,42.7,42.6,42.82,43.03]
[null,"Jewells 33_11kV","Substation Rating","MVA","Non-Coincident",16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002]
[null,null,null,null,"Coincident",16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002,16.920000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.55600000000000005,-0.73199999999999998,-0.84699999999999998,-0.92800000000000005,-1.014,-1.095,-1.173]
[null,null,null,null,"Coincident",-1.3360000000000001,-1.7450000000000001,-1.9950000000000001,-2.1429999999999998,-2.2789999999999999,-2.415,-2.5499999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.97,16.920000000000002,16.89,16.850000000000001,16.78,16.68,16.559999999999999]
[null,null,null,null,"Coincident",15.45,15.4,15.38,15.34,15.28,15.19,15.08]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.239999999999998,17.190000000000001,17.16,17.12,17.05,16.95,16.829999999999998]
[null,null,null,null,"Coincident",15.7,15.65,15.63,15.59,15.53,15.44,15.32]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.86,14.8,14.77,14.73,14.67,14.57,14.44]
[null,null,null,null,"Coincident",13.53,13.48,13.45,13.41,13.36,13.27,13.15]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.1,15.04,15.01,14.97,14.9,14.8,14.67]
[null,null,null,null,"Coincident",13.75,13.7,13.67,13.63,13.57,13.48,13.36]
[null,"Killarney 33_11kV","Substation Rating","MVA","Non-Coincident",21.09,21.09,21.09,21.09,21.09,21.09,21.09]
[null,null,null,null,"Coincident",21.09,21.09,21.09,21.09,21.09,21.09,21.09]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5000000000000001E-2,-0.05,-7.2999999999999995E-2,-0.10199999999999999,-0.13800000000000001,-0.17199999999999999,-0.20200000000000001]
[null,null,null,null,"Coincident",-1.26,-1.6519999999999999,-1.89,-2.0259999999999998,-2.149,-2.2719999999999998,-2.3929999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.92,14.96,15.01,15.05,15.04,14.98,14.97]
[null,null,null,null,"Coincident",12.19,12.09,12.04,12.03,11.99,11.95,11.92]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.22,15.26,15.31,15.35,15.34,15.29,15.27]
[null,null,null,null,"Coincident",12.35,12.24,12.19,12.19,12.15,12.1,12.08]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14,14.04,14.08,14.12,14.11,14.06,14.04]
[null,null,null,null,"Coincident",10.45,10.36,10.31,10.31,10.27,10.220000000000001,10.199999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.29,14.32,14.37,14.41,14.4,14.34,14.33]
[null,null,null,null,"Coincident",10.58,10.49,10.45,10.44,10.4,10.36,10.33]
[null,"Kingsford 132_11kV","Substation Rating","MVA","Non-Coincident",62.24,62.24,62.24,62.24,62.24,62.24,62.24]
[null,null,null,null,"Coincident",62.24,62.24,62.24,62.24,62.24,62.24,62.24]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5779999999999998,-2.9020000000000001,-2.931,-3.1389999999999998,-3.415,-2.952,-3.069]
[null,null,null,null,"Coincident",-2.601,-3.363,-3.94,-4.4370000000000003,-5.0250000000000004,-5.6120000000000001,-6.19]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",66.739999999999995,68.88,68.63,68.83,69.67,69.8,69.790000000000006]
[null,null,null,null,"Coincident",63.21,65.239999999999995,65,65.19,65.989999999999995,66.11,66.099999999999994]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.25,69.41,69.150000000000006,69.349999999999994,70.2,70.34,70.319999999999993]
[null,null,null,null,"Coincident",63.69,65.739999999999995,65.489999999999995,65.680000000000007,66.489999999999995,66.62,66.599999999999994]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",62.83,65.05,64.83,65.03,65.87,66.010000000000005,65.989999999999995]
[null,null,null,null,"Coincident",59.51,61.61,61.4,61.59,62.39,62.52,62.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",63.31,65.540000000000006,65.319999999999993,65.52,66.38,66.510000000000005,66.489999999999995]
[null,null,null,null,"Coincident",59.96,62.08,61.87,62.06,62.87,62.99,62.98]
[null,"Kirrawee 132_11kV","Substation Rating","MVA","Non-Coincident",42.87,42.87,42.87,42.87,42.87,42.87,42.87]
[null,null,null,null,"Coincident",42.87,42.87,42.87,42.87,42.87,42.87,42.87]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.8000000000000001E-2,-9.5000000000000001E-2,-0.151,-0.22700000000000001,-0.33,-0.42499999999999999,-0.50900000000000001]
[null,null,null,null,"Coincident",-2.4390000000000001,-3.1539999999999999,-3.6549999999999998,-4.04,-4.4660000000000002,-4.891,-5.3090000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.29,40.25,40.72,40.98,41.09,41.15,41.37]
[null,null,null,null,"Coincident",38.15,38.729999999999997,38.94,38.909999999999997,38.880000000000003,38.85,38.69]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.95,45.03,45.55,45.84,45.96,46.03,46.28]
[null,null,null,null,"Coincident",42.36,43.01,43.24,43.2,43.17,43.14,42.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.32,38.200000000000003,38.61,38.840000000000003,38.950000000000003,39.01,39.24]
[null,null,null,null,"Coincident",33.29,33.85,34.04,34,33.97,33.950000000000003,33.79]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.75,42.73,43.19,43.44,43.57,43.64,43.89]
[null,null,null,null,"Coincident",36.96,37.58,37.799999999999997,37.76,37.72,37.69,37.520000000000003]
[null,"Kogarah 132_11kV","Substation Rating","MVA","Non-Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,null,null,"Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.5449999999999999,-3.5790000000000002,-3.681,-3.8290000000000002,-4.0259999999999998,-4.2069999999999999,-4.367]
[null,null,null,null,"Coincident",-4.3869999999999996,-5.6580000000000004,-6.585,-7.3470000000000004,-8.2189999999999994,-9.0909999999999993,-9.9480000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",75.72,78.03,78.73,79.28,79.709999999999994,79.98,80.28]
[null,null,null,null,"Coincident",73.849999999999994,76.11,76.790000000000006,77.33,77.75,78.010000000000005,78.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.86,79.209999999999994,79.92,80.48,80.91,81.19,81.489999999999995]
[null,null,null,null,"Coincident",74.97,77.260000000000005,77.95,78.5,78.92,79.19,79.48]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",66.33,68.66,69.37,69.930000000000007,70.349999999999994,70.62,70.92]
[null,null,null,null,"Coincident",64.7,66.97,67.67,68.209999999999994,68.62,68.88,69.17]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.33,69.7,70.42,70.98,71.41,71.69,71.989999999999995]
[null,null,null,null,"Coincident",65.680000000000007,67.98,68.69,69.239999999999995,69.66,69.930000000000007,70.22]
[null,"Kotara 33_11kV","Substation Rating","MVA","Non-Coincident",30.81,30.81,30.81,30.81,30.81,30.81,30.81]
[null,null,null,null,"Coincident",30.81,30.81,30.81,30.81,30.81,30.81,30.81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.204,-1.407,-1.542,-1.639,-1.7410000000000001,-1.8380000000000001,-1.9319999999999999]
[null,null,null,null,"Coincident",-1.304,-1.706,-1.958,-2.1139999999999999,-2.2639999999999998,-2.415,-2.5630000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.67,27.58,27.57,27.64,27.69,27.78,27.77]
[null,null,null,null,"Coincident",26.16,26.07,26.07,26.13,26.18,26.27,26.26]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.18,28.09,28.08,28.15,28.21,28.3,28.29]
[null,null,null,null,"Coincident",26.64,26.55,26.55,26.61,26.67,26.75,26.74]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.13,23.04,23.03,23.1,23.16,23.25,23.24]
[null,null,null,null,"Coincident",21.87,21.78,21.78,21.84,21.89,21.98,21.97]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.56,23.47,23.46,23.53,23.59,23.68,23.67]
[null,null,null,null,"Coincident",22.28,22.19,22.18,22.25,22.3,22.38,22.38]
[null,"Kurnell South 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-7.2999999999999995E-2,-7.8E-2,-8.3000000000000004E-2,-0.09,-9.8000000000000004E-2,-0.106,-0.113]
[null,null,null,null,"Coincident",-0.27200000000000002,-0.35199999999999998,-0.40500000000000003,-0.441,-0.47699999999999998,-0.51300000000000001,-0.54900000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3869999999999996,7.4290000000000003,7.7210000000000001,7.6479999999999997,7.6550000000000002,7.6459999999999999,7.6349999999999998]
[null,null,null,null,"Coincident",4.593,5.2380000000000004,5.4039999999999999,5.4009999999999998,5.3879999999999999,5.3730000000000002,5.3579999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.4489999999999998,7.5010000000000003,7.7960000000000003,7.7229999999999999,7.73,7.72,7.71]
[null,null,null,null,"Coincident",4.9480000000000004,5.6420000000000003,5.8209999999999997,5.8179999999999996,5.8049999999999997,5.7880000000000003,5.7709999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.1120000000000001,7.1630000000000003,7.46,7.39,7.3970000000000002,7.3879999999999999,7.3769999999999998]
[null,null,null,null,"Coincident",4.3310000000000004,4.976,5.1420000000000003,5.1390000000000002,5.1269999999999998,5.1109999999999998,5.0960000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.1719999999999997,7.2320000000000002,7.5330000000000004,7.4619999999999997,7.4690000000000003,7.4589999999999996,7.4489999999999998]
[null,null,null,null,"Coincident",4.6660000000000004,5.36,5.5389999999999997,5.5359999999999996,5.5229999999999997,5.5060000000000002,5.4889999999999999]
[null,"Kurri 132_11kV","Substation Rating","MVA","Non-Coincident",57.27,57.27,57.27,57.27,57.27,57.27,57.27]
[null,null,null,null,"Coincident",57.27,57.27,57.27,57.27,57.27,57.27,57.27]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.36,-0.51100000000000001,-0.63600000000000001,-0.72899999999999998,-0.83099999999999996,-0.92600000000000005,-1.0169999999999999]
[null,null,null,null,"Coincident",-2.0920000000000001,-2.746,-3.1459999999999999,-3.3769999999999998,-3.589,-3.8,-4.0090000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.02,41.47,41.76,42.08,42.1,42.12,42.07]
[null,null,null,null,"Coincident",37.450000000000003,37.869999999999997,38.14,38.43,38.450000000000003,38.46,38.42]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.07,41.53,41.83,42.15,42.17,42.18,42.14]
[null,null,null,null,"Coincident",37.51,37.93,38.200000000000003,38.49,38.51,38.520000000000003,38.479999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.61,37.03,37.299999999999997,37.619999999999997,37.64,37.65,37.61]
[null,null,null,null,"Coincident",33.43,33.81,34.06,34.35,34.369999999999997,34.380000000000003,34.340000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.630000000000003,37.049999999999997,37.33,37.65,37.67,37.68,37.64]
[null,null,null,null,"Coincident",33.450000000000003,33.840000000000003,34.090000000000003,34.380000000000003,34.4,34.409999999999997,34.369999999999997]
[null,"Lake Munmorah 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.75600000000000001,-0.86399999999999999,-0.94,-1.0009999999999999,-1.264,-1.135,-1.196]
[null,null,null,null,"Coincident",-1.9379999999999999,-2.544,-2.9089999999999998,-3.1110000000000002,-3.29,-3.4689999999999999,-3.6459999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.04,29.9,30.57,31.27,32.03,32.19,32.200000000000003]
[null,null,null,null,"Coincident",26.61,27.4,28.01,28.65,29.35,29.5,29.5]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.44,30.31,30.99,31.7,32.47,32.630000000000003,32.64]
[null,null,null,null,"Coincident",26.97,27.77,28.39,29.04,29.75,29.9,29.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.83,25.61,26.24,26.94,27.69,27.86,27.86]
[null,null,null,null,"Coincident",22.75,23.47,24.04,24.68,25.37,25.53,25.53]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.17,25.96,26.6,27.3,28.07,28.24,28.24]
[null,null,null,null,"Coincident",23.06,23.79,24.37,25.02,25.72,25.87,25.88]
[null,"Leichhardt 132_11kV","Substation Rating","MVA","Non-Coincident",62.51,62.51,62.51,62.51,62.51,62.51,62.51]
[null,null,null,null,"Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.04,-0.08,-0.127,-0.19500000000000001,-0.28399999999999997,-0.36699999999999999,-0.44]
[null,null,null,null,"Coincident",-2.69,-3.4950000000000001,-4.05,-4.4669999999999996,-4.9210000000000003,-5.3739999999999997,-5.82]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.44,57.2,57.43,51.86,52.11,52.39,52.57]
[null,null,null,null,"Coincident",38.01,42.43,40.83,37.08,37.200000000000003,37.39,37.549999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.18,58.03,58.27,52.62,52.87,53.15,53.34]
[null,null,null,null,"Coincident",38.96,43.49,41.85,38,38.130000000000003,38.32,38.49]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.68,54.44,54.68,49.11,49.36,49.63,49.82]
[null,null,null,null,"Coincident",36.49,40.93,39.340000000000003,35.590000000000003,35.71,35.9,36.07]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.39,55.23,55.47,49.82,50.07,50.35,50.54]
[null,null,null,null,"Coincident",37.4,41.95,40.32,36.479999999999997,36.6,36.79,36.97]
[null,"Leightonfield 33_11kV","Substation Rating","MVA","Non-Coincident",22.9,22.9,22.9,22.9,22.9,22.9,22.9]
[null,null,null,null,"Coincident",22.9,22.9,22.9,22.9,22.9,22.9,22.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.1539999999999999,-1.544,-1.8049999999999999,-1.988,-2.1850000000000001,-2.3719999999999999,-2.556]
[null,null,null,null,"Coincident",-1.0269999999999999,-1.349,-1.5569999999999999,-1.6950000000000001,-1.835,-1.9750000000000001,-2.113]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.94,26.03,26.08,26.16,26.27,26.4,26.42]
[null,null,null,null,"Coincident",22.99,23.07,23.12,23.19,23.29,23.4,23.41]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.49,27.59,27.64,27.72,27.84,27.98,27.99]
[null,null,null,null,"Coincident",24.37,24.45,24.5,24.57,24.68,24.8,24.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.82,23.9,23.95,24.02,24.14,24.27,24.28]
[null,null,null,null,"Coincident",21.12,21.19,21.23,21.29,21.4,21.51,21.52]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.25,25.33,25.38,25.46,25.58,25.72,25.73]
[null,null,null,null,"Coincident",22.38,22.45,22.49,22.57,22.67,22.79,22.81]
[null,"Lemington 66_11kV","Substation Rating","MVA","Non-Coincident",6.74,6.74,6.74,6.74,6.74,6.74,6.74]
[null,null,null,null,"Coincident",6.74,6.74,6.74,6.74,6.74,6.74,6.74]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.9E-2,-2.1999999999999999E-2,-2.1000000000000001E-2,-2.4E-2,-2.8000000000000001E-2,-3.1E-2,-3.4000000000000002E-2]
[null,null,null,null,"Coincident",-7.9000000000000001E-2,-0.1,-0.11600000000000001,-0.13,-0.14799999999999999,-0.16500000000000001,-0.182]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.0979999999999999,3.1030000000000002,3.11,3.13,3.1469999999999998,3.1640000000000001,3.1760000000000002]
[null,null,null,null,"Coincident",1.3320000000000001,1.335,1.337,1.3460000000000001,1.353,1.36,1.3660000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2040000000000002,3.21,3.2160000000000002,3.238,3.254,3.2719999999999998,3.2850000000000001]
[null,null,null,null,"Coincident",1.3779999999999999,1.38,1.383,1.3919999999999999,1.4,1.407,1.413]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.653,2.6589999999999998,2.665,2.6859999999999999,2.702,2.7189999999999999,2.7309999999999999]
[null,null,null,null,"Coincident",1.141,1.143,1.1459999999999999,1.155,1.1619999999999999,1.169,1.175]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7440000000000002,2.75,2.7559999999999998,2.778,2.794,2.8119999999999998,2.8250000000000002]
[null,null,null,null,"Coincident",1.18,1.1830000000000001,1.1850000000000001,1.1950000000000001,1.202,1.2090000000000001,1.2150000000000001]
[null,"Lidcombe 33_11kV","Substation Rating","MVA","Non-Coincident",26.2,26.2,26.2,26.2,26.2,26.2,26.2]
[null,null,null,null,"Coincident",26.2,26.2,26.2,26.2,26.2,26.2,26.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.397,-1.708,-1.956,-1.9019999999999999,-2.1110000000000002,-2.3090000000000002,-2.5019999999999998]
[null,null,null,null,"Coincident",-0.93,-1.1919999999999999,-1.391,-1.5649999999999999,-1.7689999999999999,-1.9730000000000001,-2.1720000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.09,24.66,25.15,25.4,25.5,25.54,25.53]
[null,null,null,null,"Coincident",18.850000000000001,23.14,23.61,23.84,23.93,23.97,23.96]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.08,27.09,27.64,27.91,28.02,28.06,28.06]
[null,null,null,null,"Coincident",20.72,25.43,25.94,26.2,26.3,26.34,26.33]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.079999999999998,22.69,23.21,23.45,23.55,23.59,23.59]
[null,null,null,null,"Coincident",16.97,21.29,21.78,22.01,22.1,22.14,22.14]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.87,24.93,25.5,25.77,25.88,25.92,25.92]
[null,null,null,null,"Coincident",18.649999999999999,23.4,23.93,24.19,24.29,24.33,24.32]
[null,"Lindfield 33_11kV","Substation Rating","MVA","Non-Coincident",36.81,36.81,36.81,36.81,36.81,36.81,36.81]
[null,null,null,null,"Coincident",36.81,36.81,36.81,36.81,36.81,36.81,36.81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.0870000000000002,-1.9870000000000001,-2.036,-2.0950000000000002,-2.169,-2.238,-2.2999999999999998]
[null,null,null,null,"Coincident",-2.1659999999999999,-2.85,-3.2879999999999998,-3.5710000000000002,-3.8540000000000001,-4.1369999999999996,-4.4160000000000004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.39,37.24,37.53,37.61,37.69,37.67,37.65]
[null,null,null,null,"Coincident",32.94,33.71,33.97,34.049999999999997,34.119999999999997,34.1,34.08]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.200000000000003,38.07,38.369999999999997,38.46,38.53,38.520000000000003,38.5]
[null,null,null,null,"Coincident",33.68,34.46,34.729999999999997,34.81,34.880000000000003,34.869999999999997,34.85]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.87,32.700000000000003,32.97,33.06,33.130000000000003,33.119999999999997,33.1]
[null,null,null,null,"Coincident",28.85,29.6,29.85,29.92,29.99,29.98,29.96]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.590000000000003,33.43,33.71,33.799999999999997,33.880000000000003,33.86,33.840000000000003]
[null,null,null,null,"Coincident",29.5,30.26,30.52,30.6,30.67,30.65,30.63]
[null,"Lisarow 33_11kV","Substation Rating","MVA","Non-Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,null,null,"Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.085,-1.2889999999999999,-1.448,-1.5589999999999999,-1.677,-1.663,-1.62]
[null,null,null,null,"Coincident",-1.583,-2.0720000000000001,-2.3740000000000001,-2.5529999999999999,-2.7210000000000001,-2.89,-3.056]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.93,24.84,24.97,25.46,26,26.24,26.27]
[null,null,null,null,"Coincident",23.64,23.55,23.68,24.14,24.65,24.88,24.91]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.95,24.85,24.99,25.48,26.02,26.26,26.29]
[null,null,null,null,"Coincident",23.66,23.56,23.69,24.16,24.67,24.9,24.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.49,22.44,22.59,23.08,23.61,23.86,23.89]
[null,null,null,null,"Coincident",21.33,21.27,21.42,21.88,22.39,22.62,22.65]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.5,22.44,22.59,23.08,23.62,23.87,23.9]
[null,null,null,null,"Coincident",21.33,21.28,21.42,21.89,22.4,22.63,22.66]
[null,"Long Jetty 66_11kV","Substation Rating","MVA","Non-Coincident",76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994]
[null,null,null,null,"Coincident",71.69,71.69,71.69,71.69,71.69,71.69,71.69]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-6.8000000000000005E-2,-0.13500000000000001,-0.20599999999999999,-0.30099999999999999,-0.42499999999999999,-0.54,-0.64300000000000002]
[null,null,null,null,"Coincident",-3.6589999999999998,-4.78,-5.4989999999999997,-5.9669999999999996,-6.4340000000000002,-6.9020000000000001,-7.3639999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.229999999999997,40.31,40.479999999999997,40.71,40.83,41.01,41.07]
[null,null,null,null,"Coincident",37.32,37.229999999999997,37.22,37.17,37.270000000000003,37.090000000000003,36.85]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.7,44.79,44.98,45.23,45.36,45.57,45.63]
[null,null,null,null,"Coincident",41.46,41.37,41.35,41.31,41.41,41.21,40.950000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.020000000000003,38.090000000000003,38.25,38.47,38.590000000000003,38.78,38.83]
[null,null,null,null,"Coincident",32.729999999999997,32.619999999999997,32.6,32.549999999999997,32.65,32.47,32.229999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.24,42.32,42.51,42.75,42.88,43.09,43.15]
[null,null,null,null,"Coincident",36.36,36.25,36.22,36.17,36.28,36.07,35.81]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Macquarie Park 132_11kV","Substation Rating","MVA","Non-Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,null,null,"Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.1890000000000001,-1.583,-1.9139999999999999,-2.226,-2.6120000000000001,-2.976,-3.3279999999999998]
[null,null,null,null,"Coincident",-1.133,-1.4730000000000001,-1.7470000000000001,-2.008,-2.3260000000000001,-2.6459999999999999,-2.9580000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",97.93,80.88,82.53,83.08,83.61,84.15,84.48]
[null,null,null,null,"Coincident",85.14,70.31,71.75,72.22,72.69,73.150000000000006,73.44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",99.58,82.24,83.92,84.47,85.02,85.56,85.9]
[null,null,null,null,"Coincident",86.57,71.5,72.959999999999994,73.44,73.91,74.38,74.680000000000007]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",93.88,76.900000000000006,78.599999999999994,79.14,79.680000000000007,80.209999999999994,80.540000000000006]
[null,null,null,null,"Coincident",81.61,66.86,68.33,68.8,69.27,69.73,70.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",95.46,78.2,79.92,80.47,81.02,81.56,81.900000000000006]
[null,null,null,null,"Coincident",82.99,67.98,69.48,69.959999999999994,70.44,70.91,71.2]
[null,"Maitland 33_11kV","Substation Rating","MVA","Non-Coincident",36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997]
[null,null,null,null,"Coincident",36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997,36.659999999999997]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.24199999999999999,-0.39700000000000002,-0.50600000000000001,-0.59499999999999997,-0.69399999999999995,-0.78700000000000003,-0.875]
[null,null,null,null,"Coincident",-1.4079999999999999,-1.83,-2.1030000000000002,-2.2850000000000001,-2.468,-2.65,-2.8290000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.83,28.62,28.54,29.3,29.32,29.33,29.31]
[null,null,null,null,"Coincident",26.04,25.85,25.78,26.47,26.48,26.49,26.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.58,29.36,29.27,30.05,30.07,30.08,30.06]
[null,null,null,null,"Coincident",26.71,26.52,26.44,27.14,27.16,27.17,27.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.43,25.23,25.16,25.93,25.94,25.96,25.93]
[null,null,null,null,"Coincident",22.97,22.79,22.72,23.42,23.43,23.44,23.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.09,25.89,25.81,26.58,26.6,26.62,26.59]
[null,null,null,null,"Coincident",23.56,23.38,23.31,24.01,24.03,24.04,24.02]
[null,"Manly 33_11kV","Substation Rating","MVA","Non-Coincident",22.86,22.86,22.86,22.86,22.86,22.86,22.86]
[null,null,null,null,"Coincident",22.86,22.86,22.86,22.86,22.86,22.86,22.86]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-8.9999999999999993E-3,-1.7000000000000001E-2,-3.6999999999999998E-2,-5.8999999999999997E-2,-9.9000000000000005E-2,-0.13600000000000001,-0.19900000000000001]
[null,null,null,null,"Coincident",-0.76900000000000002,-0.96299999999999997,-1.147,-1.3540000000000001,-1.621,-1.8879999999999999,-2.15]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.489999999999998,19.93,20.13,20.239999999999998,20.38,20.48,20.53]
[null,null,null,null,"Coincident",14,14.12,14.18,14.31,14.43,14.54,14.63]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.45,20.91,21.12,21.24,21.39,21.49,21.54]
[null,null,null,null,"Coincident",15.32,15.46,15.52,15.67,15.8,15.92,16.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.63,19.260000000000002,19.600000000000001,19.77,19.91,20.010000000000002,20.059999999999999]
[null,null,null,null,"Coincident",12.98,13.11,13.17,13.3,13.42,13.53,13.62]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.55,20.21,20.56,20.74,20.89,20.99,21.05]
[null,null,null,null,"Coincident",14.21,14.35,14.42,14.57,14.69,14.81,14.91]
[null,"Maroubra 132_11kV","Substation Rating","MVA","Non-Coincident",102.8,102.8,102.8,102.8,102.8,102.8,102.8]
[null,null,null,null,"Coincident",102.8,102.8,102.8,102.8,102.8,102.8,102.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.2000000000000001E-2,-6.4000000000000001E-2,-0.109,-0.17799999999999999,-0.27200000000000002,-0.35799999999999998,-0.433]
[null,null,null,null,"Coincident",-2.13,-2.758,-3.226,-3.625,-4.0910000000000002,-4.5579999999999998,-5.016]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.91,44.84,45.08,45,45.15,45.22,45.29]
[null,null,null,null,"Coincident",40.44,40.9,40.950000000000003,41.07,41.18,41.4,41.49]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.79,49.83,50.09,50,50.17,50.24,50.33]
[null,null,null,null,"Coincident",41.34,41.81,41.86,41.98,42.1,42.32,42.41]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.72,43.97,44.42,44.45,44.6,44.67,44.75]
[null,null,null,null,"Coincident",38.08,38.590000000000003,38.659999999999997,38.78,38.89,39.11,39.200000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.46,48.86,49.36,49.39,49.56,49.63,49.72]
[null,null,null,null,"Coincident",38.93,39.450000000000003,39.520000000000003,39.64,39.76,39.979999999999997,40.07]
[null,"Marrickville 132_11kV","Substation Rating","MVA","Non-Coincident",72.67,72.67,72.67,72.67,72.67,72.67,72.67]
[null,null,null,null,"Coincident",71.89,71.89,71.89,71.89,71.89,71.89,71.89]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-5.5E-2,-0.111,-0.183,-0.29099999999999998,-0.436,-0.56799999999999995,-0.68500000000000005]
[null,null,null,null,"Coincident",-3.6789999999999998,-4.7549999999999999,-5.54,-6.1870000000000003,-6.9249999999999998,-7.6609999999999996,-8.3849999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.2,53.18,53.49,53.89,54.41,54.97,55.43]
[null,null,null,null,"Coincident",41.12,44.56,44.92,45.37,45.85,46.17,46.54]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.26,53.25,53.56,53.96,54.48,55.04,55.5]
[null,null,null,null,"Coincident",41.78,45.28,45.64,46.11,46.59,46.91,47.29]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.49,52.12,52.9,53.53,54.05,54.61,55.07]
[null,null,null,null,"Coincident",36.75,40.22,40.6,41.05,41.53,41.85,42.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.56,52.19,52.97,53.6,54.12,54.68,55.14]
[null,null,null,null,"Coincident",37.340000000000003,40.869999999999997,41.25,41.71,42.2,42.52,42.9]
[null,"Maryland 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.93500000000000005,-1.129,-1.173,-1.2549999999999999,-1.345,-1.431,-1.512]
[null,null,null,null,"Coincident",-1.895,-2.4750000000000001,-2.8319999999999999,-3.0430000000000001,-3.2370000000000001,-3.4319999999999999,-3.625]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.59,30.99,31.13,31.11,31.04,30.96,30.96]
[null,null,null,null,"Coincident",27.03,27.38,27.5,27.49,27.42,27.35,27.35]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.07,31.47,31.62,31.6,31.52,31.44,31.44]
[null,null,null,null,"Coincident",27.45,27.8,27.93,27.91,27.85,27.78,27.78]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.34,27.71,27.84,27.82,27.74,27.66,27.67]
[null,null,null,null,"Coincident",24.15,24.48,24.59,24.57,24.51,24.44,24.44]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.76,28.14,28.27,28.25,28.17,28.09,28.1]
[null,null,null,null,"Coincident",24.53,24.86,24.97,24.96,24.89,24.82,24.82]
[null,"Mascot 33_11kV","Substation Rating","MVA","Non-Coincident",78.44,78.44,78.44,78.44,78.44,78.44,78.44]
[null,null,null,null,"Coincident",78.44,78.44,78.44,78.44,78.44,78.44,78.44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.1020000000000001,-1.4450000000000001,-1.76,-2.0910000000000002,-2.4889999999999999,-2.8809999999999998,-3.2679999999999998]
[null,null,null,null,"Coincident",-0.875,-1.109,-1.3149999999999999,-1.5309999999999999,-1.8029999999999999,-2.0750000000000002,-2.3410000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.549999999999997,39.450000000000003,39.369999999999997,39.35,39.53,39.71,40.08]
[null,null,null,null,"Coincident",34.58,34.49,34.42,34.4,34.56,34.72,35.04]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.56,42.45,42.36,42.34,42.54,42.73,43.13]
[null,null,null,null,"Coincident",37.21,37.11,37.03,37.01,37.19,37.36,37.71]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.49,36.44,36.39,36.369999999999997,36.549999999999997,36.74,37.11]
[null,null,null,null,"Coincident",31.9,31.86,31.81,31.8,31.96,32.119999999999997,32.44]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.26,39.22,39.159999999999997,39.14,39.33,39.53,39.93]
[null,null,null,null,"Coincident",34.33,34.28,34.229999999999997,34.21,34.39,34.56,34.909999999999997]
[null,"Matraville 33_11kV","Substation Rating","MVA","Non-Coincident",58.48,58.48,58.48,58.48,58.48,58.48,58.48]
[null,null,null,null,"Coincident",57.02,57.02,57.02,57.02,57.02,57.02,57.02]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.2000000000000001E-2,-6.4000000000000001E-2,-0.10299999999999999,-0.158,-0.22800000000000001,-0.29899999999999999,-0.35299999999999998]
[null,null,null,null,"Coincident",-1.881,-2.4489999999999998,-2.8380000000000001,-3.1269999999999998,-3.4430000000000001,-3.758,-4.069]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.05,45.09,46.17,46.96,47.17,47.36,47.65]
[null,null,null,null,"Coincident",32.119999999999997,32.9,33.46,33.67,33.92,34.08,34.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.66,46.77,47.89,48.71,48.93,49.12,49.42]
[null,null,null,null,"Coincident",35.659999999999997,36.53,37.15,37.380000000000003,37.65,37.840000000000003,38.15]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.22,43.2,44.24,45.01,45.23,45.41,45.7]
[null,null,null,null,"Coincident",29.59,30.32,30.86,31.07,31.31,31.48,31.76]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.75,44.8,45.89,46.69,46.91,47.1,47.4]
[null,null,null,null,"Coincident",32.85,33.659999999999997,34.25,34.49,34.76,34.94,35.25]
[null,"Mayfield West 132_11kV","Substation Rating","MVA","Non-Coincident",62.59,62.59,62.59,62.59,62.59,62.59,62.59]
[null,null,null,null,"Coincident",62.59,62.59,62.59,62.59,62.59,62.59,62.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.40500000000000003,-0.41,-0.41399999999999998,-0.51300000000000001,-0.629,-0.73799999999999999,-0.84299999999999997]
[null,null,null,null,"Coincident",-1.175,-1.5269999999999999,-1.77,-1.9530000000000001,-2.153,-2.3519999999999999,-2.5470000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.83,26.04,26.1,26.19,26.22,26.31,26.45]
[null,null,null,null,"Coincident",23.26,23.45,23.5,23.58,23.61,23.69,23.82]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.72,26.94,27,27.09,27.12,27.21,27.36]
[null,null,null,null,"Coincident",24.06,24.25,24.31,24.39,24.42,24.51,24.64]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.57,23.81,23.89,23.98,24,24.1,24.24]
[null,null,null,null,"Coincident",21.23,21.44,21.51,21.59,21.61,21.7,21.83]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.38,24.63,24.71,24.8,24.83,24.93,25.07]
[null,null,null,null,"Coincident",21.96,22.18,22.25,22.33,22.36,22.45,22.58]
[null,"Meadowbank 132_11kV","Substation Rating","MVA","Non-Coincident",103.8,103.8,103.8,103.8,103.8,103.8,103.8]
[null,null,null,null,"Coincident",103.8,103.8,103.8,103.8,103.8,103.8,103.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.47,-3.58,-3.698,-3.8490000000000002,-4.0460000000000003,-4.0869999999999997,-4.2309999999999999]
[null,null,null,null,"Coincident",-3.6379999999999999,-4.6909999999999998,-5.4720000000000004,-6.1269999999999998,-6.8879999999999999,-7.649,-8.3979999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",81.42,84.36,85.91,86.66,87.45,88.32,88.78]
[null,null,null,null,"Coincident",73.73,76.400000000000006,77.8,78.48,79.2,79.98,80.400000000000006]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",87.26,90.41,92.07,92.87,93.72,94.65,95.15]
[null,null,null,null,"Coincident",79.03,81.88,83.38,84.11,84.88,85.72,86.17]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",72.67,75.5,77,77.739999999999995,78.540000000000006,79.400000000000006,79.86]
[null,null,null,null,"Coincident",65.81,68.37,69.73,70.400000000000006,71.13,71.91,72.33]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",77.89,80.91,82.52,83.31,84.17,85.09,85.59]
[null,null,null,null,"Coincident",70.540000000000006,73.28,74.73,75.45,76.23,77.06,77.510000000000005]
[null,"Medowie 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.33500000000000002,-0.5,-0.60299999999999998,-0.66800000000000004,-0.73199999999999998,-0.79200000000000004,-0.85099999999999998]
[null,null,null,null,"Coincident",-1.103,-1.4470000000000001,-1.65,-1.758,-1.847,-1.9370000000000001,-2.0259999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.36,16.54,16.64,16.62,16.559999999999999,16.489999999999998,16.420000000000002]
[null,null,null,null,"Coincident",14.48,14.65,14.74,14.71,14.66,14.6,14.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.579999999999998,16.760000000000002,16.87,16.84,16.78,16.71,16.64]
[null,null,null,null,"Coincident",14.68,14.84,14.93,14.91,14.86,14.8,14.73]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.47,14.62,14.71,14.68,14.63,14.56,14.48]
[null,null,null,null,"Coincident",12.81,12.95,13.02,13,12.95,12.89,12.82]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.66,14.82,14.91,14.88,14.82,14.76,14.68]
[null,null,null,null,"Coincident",12.98,13.12,13.2,13.17,13.12,13.06,12.99]
[null,"Menai 132_11kV","Substation Rating","MVA","Non-Coincident",60.72,60.72,60.72,60.72,60.72,60.72,60.72]
[null,null,null,null,"Coincident",60.72,60.72,60.72,60.72,60.72,60.72,60.72]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.58399999999999996,-1.0660000000000001,-1.415,-1.637,-1.859,-2.069,-2.2749999999999999]
[null,null,null,null,"Coincident",-3.03,-4.0179999999999998,-4.6079999999999997,-4.9329999999999998,-5.2149999999999999,-5.4980000000000002,-5.7770000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.95,49.75,49.7,49.63,49.5,49.29,49.07]
[null,null,null,null,"Coincident",46.27,46.08,46.03,45.98,45.86,45.66,45.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.46,50.26,50.21,50.15,50.01,49.8,49.58]
[null,null,null,null,"Coincident",46.75,46.56,46.51,46.45,46.33,46.13,45.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.92,43.71,43.64,43.58,43.45,43.24,43.02]
[null,null,null,null,"Coincident",40.68,40.49,40.43,40.369999999999997,40.25,40.049999999999997,39.85]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.37,44.16,44.1,44.03,43.9,43.68,43.47]
[null,null,null,null,"Coincident",41.1,40.9,40.85,40.79,40.67,40.47,40.26]
[null,"Merriwa 33_11kV","Substation Rating","MVA","Non-Coincident",6.94,6.94,6.94,6.94,6.94,6.94,6.94]
[null,null,null,null,"Coincident",6.94,6.94,6.94,6.94,6.94,6.94,6.94]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.7999999999999999E-2,-3.5000000000000003E-2,-4.8000000000000001E-2,-0.04,-0.05,-0.06,-6.9000000000000006E-2]
[null,null,null,null,"Coincident",-0.247,-0.32100000000000001,-0.36799999999999999,-0.39900000000000002,-0.42899999999999999,-0.45800000000000002,-0.48799999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.964,3.948,3.9540000000000002,3.9529999999999998,3.944,3.9390000000000001,3.9220000000000002]
[null,null,null,null,"Coincident",3.2170000000000001,3.2050000000000001,3.2090000000000001,3.2090000000000001,3.202,3.1970000000000001,3.1840000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.9990000000000001,3.984,3.9889999999999999,3.9889999999999999,3.98,3.9750000000000001,3.9580000000000002]
[null,null,null,null,"Coincident",3.246,3.234,3.238,3.238,3.23,3.226,3.2120000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.609,3.5939999999999999,3.6,3.6,3.5910000000000002,3.5859999999999999,3.569]
[null,null,null,null,"Coincident",2.9289999999999998,2.9169999999999998,2.9220000000000002,2.9220000000000002,2.915,2.91,2.8969999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.6419999999999999,3.6269999999999998,3.633,3.6320000000000001,3.6230000000000002,3.6179999999999999,3.601]
[null,null,null,null,"Coincident",2.956,2.944,2.9489999999999998,2.948,2.9409999999999998,2.9369999999999998,2.923]
[null,"Metford 33_11kV","Substation Rating","MVA","Non-Coincident",41.59,41.59,41.59,41.59,41.59,41.59,41.59]
[null,null,null,null,"Coincident",41.59,41.59,41.59,41.59,41.59,41.59,41.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.625,-0.91300000000000003,-1.109,-1.256,-1.419,-1.5720000000000001,-1.72]
[null,null,null,null,"Coincident",-2.238,-2.919,-3.35,-3.621,-3.8860000000000001,-4.1509999999999998,-4.4130000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.43,45.5,45.49,44,43.99,43.95,44.07]
[null,null,null,null,"Coincident",41.72,41.79,41.78,40.409999999999997,40.4,40.369999999999997,40.479999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.1,46.17,46.16,44.65,44.63,44.59,44.72]
[null,null,null,null,"Coincident",42.33,42.4,42.39,41,40.99,40.96,41.07]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.9,40.97,40.96,39.47,39.450000000000003,39.42,39.54]
[null,null,null,null,"Coincident",37.56,37.619999999999997,37.61,36.25,36.24,36.200000000000003,36.31]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.5,41.57,41.56,40.049999999999997,40.03,39.99,40.119999999999997]
[null,null,null,null,"Coincident",38.11,38.17,38.159999999999997,36.78,36.76,36.729999999999997,36.85]
[null,"Milperra 132_11kV","Substation Rating","MVA","Non-Coincident",61.18,61.18,61.18,61.18,61.18,61.18,61.18]
[null,null,null,null,"Coincident",61.18,61.18,61.18,61.18,61.18,61.18,61.18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.234,-5.2610000000000001,-5.7050000000000001,-6.18,-6.7039999999999997,-7.2,-7.6870000000000003]
[null,null,null,null,"Coincident",-2.2930000000000001,-2.9830000000000001,-3.4449999999999998,-3.778,-4.1289999999999996,-4.4800000000000004,-4.8239999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",56,56.49,56.6,57.17,57.61,58.1,58.7]
[null,null,null,null,"Coincident",50.54,50.98,51.08,51.59,51.99,52.44,52.98]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.98,58.48,58.6,59.18,59.64,60.15,60.77]
[null,null,null,null,"Coincident",52.32,52.77,52.88,53.41,53.83,54.28,54.84]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.47,51.99,52.13,52.69,53.14,53.63,54.22]
[null,null,null,null,"Coincident",46.45,46.92,47.04,47.55,47.95,48.4,48.94]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",53.28,53.82,53.96,54.54,55.01,55.52,56.13]
[null,null,null,null,"Coincident",48.09,48.57,48.7,49.22,49.64,50.1,50.66]
[null,"Miranda 33_11kV","Substation Rating","MVA","Non-Coincident",41.97,41.97,41.97,41.97,41.97,41.97,41.97]
[null,null,null,null,"Coincident",41.97,41.97,41.97,41.97,41.97,41.97,41.97]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.1E-2,-6.2E-2,-9.6000000000000002E-2,-0.14000000000000001,-0.19800000000000001,-0.252,-0.3]
[null,null,null,null,"Coincident",-1.67,-2.1859999999999999,-2.524,-2.754,-2.992,-3.23,-3.464]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.71,30.35,30.75,30.86,30.98,31.17,31.3]
[null,null,null,null,"Coincident",30.91,31.02,30.97,31.07,31.26,31.31,31.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.27,30.92,31.33,31.44,31.57,31.75,31.89]
[null,null,null,null,"Coincident",33.03,33.15,33.1,33.21,33.409999999999997,33.46,33.43]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.42,29.24,29.76,29.93,30.05,30.23,30.36]
[null,null,null,null,"Coincident",27.35,27.52,27.49,27.6,27.79,27.83,27.8]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.96,29.79,30.32,30.49,30.61,30.8,30.93]
[null,null,null,null,"Coincident",29.24,29.41,29.38,29.5,29.7,29.75,29.71]
[null,"Mitchell Line 66_11kV","Substation Rating","MVA","Non-Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,null,null,"Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.20200000000000001,-0.254,-0.29199999999999998,-0.32300000000000001,-0.35899999999999999,-0.39200000000000002,-0.42299999999999999]
[null,null,null,null,"Coincident",-0.58399999999999996,-0.76100000000000001,-0.874,-0.94699999999999995,-1.0189999999999999,-1.091,-1.161]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.516,8.32,8.2349999999999994,8.25,8.2490000000000006,8.2469999999999999,8.2260000000000009]
[null,null,null,null,"Coincident",7.2160000000000002,7.0490000000000004,6.9770000000000003,6.99,6.9889999999999999,6.9870000000000001,6.97]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.5220000000000002,8.3260000000000005,8.2409999999999997,8.2560000000000002,8.2550000000000008,8.2530000000000001,8.2319999999999993]
[null,null,null,null,"Coincident",7.2210000000000001,7.0540000000000003,6.9820000000000002,6.9950000000000001,6.9939999999999998,6.992,6.9740000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6509999999999998,7.4720000000000004,7.3959999999999999,7.4109999999999996,7.41,7.4080000000000004,7.3869999999999996]
[null,null,null,null,"Coincident",6.4829999999999997,6.3310000000000004,6.266,6.2789999999999999,6.2779999999999996,6.2759999999999998,6.258]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.657,7.4770000000000003,7.4009999999999998,7.4160000000000004,7.415,7.4130000000000003,7.3920000000000003]
[null,null,null,null,"Coincident",6.4870000000000001,6.335,6.27,6.2830000000000004,6.282,6.2809999999999997,6.2629999999999999]
[null,"Mitchells Flat 66_11kV","Substation Rating","MVA","Non-Coincident",6.69,6.69,6.69,6.69,6.69,6.69,6.69]
[null,null,null,null,"Coincident",6.69,6.69,6.69,6.69,6.69,6.69,6.69]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.6E-2,-2.3E-2,-2.7E-2,-0.03,-3.3000000000000002E-2,-3.5999999999999997E-2,-3.9E-2]
[null,null,null,null,"Coincident",-0.108,-0.14299999999999999,-0.16400000000000001,-0.17399999999999999,-0.182,-0.191,-0.19900000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0379999999999998,2.052,2.0579999999999998,2.0539999999999998,2.0470000000000002,2.04,2.0310000000000001]
[null,null,null,null,"Coincident",1.579,1.589,1.5940000000000001,1.591,1.585,1.58,1.573]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0459999999999998,2.0590000000000002,2.0649999999999999,2.0609999999999999,2.0550000000000002,2.048,2.0379999999999998]
[null,null,null,null,"Coincident",1.5840000000000001,1.595,1.599,1.5960000000000001,1.591,1.5860000000000001,1.579]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.804,1.8149999999999999,1.82,1.8160000000000001,1.81,1.8029999999999999,1.7929999999999999]
[null,null,null,null,"Coincident",1.397,1.4059999999999999,1.41,1.407,1.401,1.3959999999999999,1.389]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.81,1.8220000000000001,1.827,1.823,1.8160000000000001,1.8089999999999999,1.8]
[null,null,null,null,"Coincident",1.4019999999999999,1.411,1.415,1.4119999999999999,1.407,1.401,1.3939999999999999]
[null,"Mona Vale 33_11kV","Substation Rating","MVA","Non-Coincident",59.57,59.57,59.57,59.57,59.57,59.57,59.57]
[null,null,null,null,"Coincident",57.41,57.41,57.41,57.41,57.41,57.41,57.41]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.5999999999999997E-2,-7.1999999999999995E-2,-0.114,-0.17499999999999999,-0.25600000000000001,-0.33,-0.39400000000000002]
[null,null,null,null,"Coincident",-2.0960000000000001,-2.714,-3.1419999999999999,-3.4689999999999999,-3.8250000000000002,-4.181,-4.53]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.200000000000003,36.49,36.840000000000003,37.090000000000003,37.43,37.57,37.67]
[null,null,null,null,"Coincident",31.58,32.15,32.25,32.53,32.659999999999997,32.880000000000003,32.880000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.729999999999997,38.06,38.43,38.700000000000003,39.049999999999997,39.200000000000003,39.299999999999997]
[null,null,null,null,"Coincident",34.049999999999997,34.659999999999997,34.770000000000003,35.08,35.22,35.450000000000003,35.450000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.75,35.229999999999997,35.71,36.04,36.380000000000003,36.520000000000003,36.619999999999997]
[null,null,null,null,"Coincident",28.25,28.82,28.93,29.21,29.34,29.55,29.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.21,36.75,37.26,37.6,37.950000000000003,38.1,38.200000000000003]
[null,null,null,null,"Coincident",30.46,31.07,31.19,31.49,31.63,31.86,31.86]
[null,"Moonan 33_11kV","Substation Rating","MVA","Non-Coincident",3.14,3.14,3.14,3.14,3.14,3.14,3.14]
[null,null,null,null,"Coincident",2.86,2.86,2.86,2.86,2.86,2.86,2.86]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1E-3,-1E-3,-2E-3,-3.0000000000000001E-3,-4.0000000000000001E-3,-5.0000000000000001E-3,-6.0000000000000001E-3]
[null,null,null,null,"Coincident",-4.2000000000000003E-2,-5.3999999999999999E-2,-6.3E-2,-7.0999999999999994E-2,-0.08,-0.09,-9.9000000000000005E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.81799999999999995,0.8,0.78800000000000003,0.78500000000000003,0.78800000000000003,0.78900000000000003,0.78900000000000003]
[null,null,null,null,"Coincident",0.52800000000000002,0.52,0.51400000000000001,0.51700000000000002,0.51800000000000002,0.52100000000000002,0.52]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.90900000000000003,0.88900000000000001,0.876,0.872,0.876,0.876,0.876]
[null,null,null,null,"Coincident",0.58699999999999997,0.57699999999999996,0.57099999999999995,0.57399999999999995,0.57499999999999996,0.57899999999999996,0.57799999999999996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.81799999999999995,0.8,0.78800000000000003,0.78500000000000003,0.78800000000000003,0.78900000000000003,0.78900000000000003]
[null,null,null,null,"Coincident",0.49099999999999999,0.48299999999999998,0.47799999999999998,0.48099999999999998,0.48199999999999998,0.48499999999999999,0.48399999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.90900000000000003,0.88900000000000001,0.876,0.872,0.876,0.876,0.876]
[null,null,null,null,"Coincident",0.54600000000000004,0.53700000000000003,0.53100000000000003,0.53400000000000003,0.53600000000000003,0.53900000000000003,0.53800000000000003]
[null,"Morisset 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.80100000000000005,-1.018,-1.1879999999999999,-1.3089999999999999,-1.4390000000000001,-1.403,-1.506]
[null,null,null,null,"Coincident",-1.9790000000000001,-2.585,-2.9620000000000002,-3.19,-3.4049999999999998,-3.621,-3.8330000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.880000000000003,34.630000000000003,35,35.11,35.31,35.229999999999997,35.11]
[null,null,null,null,"Coincident",30.56,32.19,32.53,32.64,32.82,32.74,32.64]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.409999999999997,35.18,35.56,35.68,35.880000000000003,35.79,35.67]
[null,null,null,null,"Coincident",31.05,32.700000000000003,33.049999999999997,33.159999999999997,33.35,33.270000000000003,33.159999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.3,31,31.35,31.47,31.67,31.58,31.47]
[null,null,null,null,"Coincident",27.24,28.82,29.14,29.25,29.44,29.35,29.25]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.77,31.5,31.85,31.97,32.18,32.090000000000003,31.97]
[null,null,null,null,"Coincident",27.67,29.28,29.61,29.72,29.91,29.82,29.72]
[null,"Mortdale 33_11kV","Substation Rating","MVA","Non-Coincident",64.25,64.25,64.25,64.25,64.25,64.25,64.25]
[null,null,null,null,"Coincident",64.25,64.25,64.25,64.25,64.25,64.25,64.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.59599999999999997,-1.278,-0.20399999999999999,-0.50700000000000001,-0.40400000000000003,-0.51,-0.79300000000000004]
[null,null,null,null,"Coincident",-3.331,-4.3529999999999998,-5.0199999999999996,-5.4690000000000003,-5.931,-6.3929999999999998,-6.8490000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.72,53.78,53.86,54.23,54.23,54.31,54.54]
[null,null,null,null,"Coincident",48.56,49.54,49.61,49.95,49.95,50.03,50.24]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.23,54.3,54.38,54.75,54.75,54.84,55.07]
[null,null,null,null,"Coincident",49.03,50.02,50.09,50.44,50.44,50.52,50.73]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.39,46.44,46.5,46.87,46.87,46.96,47.19]
[null,null,null,null,"Coincident",41.82,42.78,42.84,43.18,43.18,43.26,43.47]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.83,46.89,46.95,47.33,47.33,47.41,47.64]
[null,null,null,null,"Coincident",42.22,43.19,43.26,43.6,43.6,43.68,43.89]
[null,"Mosman 132_11kV","Substation Rating","MVA","Non-Coincident",89.05,89.05,89.05,89.05,89.05,89.05,89.05]
[null,null,null,null,"Coincident",82.46,82.46,82.46,82.46,82.46,82.46,82.46]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-5.8999999999999997E-2,-0.11799999999999999,-0.20200000000000001,-0.33200000000000002,-0.50800000000000001,-0.67,-0.82599999999999996]
[null,null,null,null,"Coincident",-3.516,-4.5380000000000003,-5.3109999999999999,-5.9779999999999998,-6.7619999999999996,-7.5449999999999999,-8.3160000000000007]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",84.33,86.53,87.2,86.79,87.58,88.33,89.62]
[null,null,null,null,"Coincident",65.98,66.959999999999994,65.650000000000006,66.34,66.81,67.59,67.319999999999993]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",84.34,86.53,87.2,86.8,87.59,88.33,89.62]
[null,null,null,null,"Coincident",66.010000000000005,67,65.69,66.38,66.849999999999994,67.63,67.36]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",80.56,83.01,83.84,83.52,84.31,85.06,86.35]
[null,null,null,null,"Coincident",59.9,60.87,59.55,60.24,60.71,61.49,61.22]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",80.569999999999993,83.01,83.85,83.53,84.32,85.06,86.35]
[null,null,null,null,"Coincident",59.92,60.89,59.57,60.26,60.73,61.51,61.24]
[null,"Mt Hutton 33_11kV","Substation Rating","MVA","Non-Coincident",26.01,26.01,26.01,26.01,26.01,26.01,26.01]
[null,null,null,null,"Coincident",26.01,26.01,26.01,26.01,26.01,26.01,26.01]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.221,-0.373,-0.47399999999999998,-0.54600000000000004,-0.624,-0.69899999999999995,-0.77]
[null,null,null,null,"Coincident",-1.3120000000000001,-1.72,-1.968,-2.109,-2.2360000000000002,-2.363,-2.488]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.94,22.41,22.15,22.12,22.06,21.98,21.88]
[null,null,null,null,"Coincident",19.73,19.27,19.05,19.02,18.97,18.899999999999999,18.809999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.08,22.54,22.28,22.25,22.19,22.11,22.01]
[null,null,null,null,"Coincident",19.84,19.38,19.16,19.13,19.079999999999998,19.010000000000002,18.920000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.190000000000001,18.73,18.510000000000002,18.48,18.420000000000002,18.34,18.239999999999998]
[null,null,null,null,"Coincident",16.5,16.11,15.92,15.89,15.84,15.77,15.68]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.3,18.84,18.62,18.59,18.53,18.45,18.350000000000001]
[null,null,null,null,"Coincident",16.600000000000001,16.2,16.010000000000002,15.98,15.93,15.86,15.78]
[null,"Mt Thorley 66_11kV","Substation Rating","MVA","Non-Coincident",20.25,20.25,20.25,20.25,20.25,20.25,20.25]
[null,null,null,null,"Coincident",20.25,20.25,20.25,20.25,20.25,20.25,20.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5000000000000001E-2,-4.4999999999999998E-2,-3.5000000000000003E-2,-4.5999999999999999E-2,-6.0999999999999999E-2,-7.3999999999999996E-2,-8.5999999999999993E-2]
[null,null,null,null,"Coincident",-0.29199999999999998,-0.38,-0.442,-0.49199999999999999,-0.54800000000000004,-0.60399999999999998,-0.65900000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.9109999999999996,7.91,7.9180000000000001,7.9889999999999999,8.0389999999999997,8.0909999999999993,8.1129999999999995]
[null,null,null,null,"Coincident",6.1890000000000001,6.1879999999999997,6.194,6.25,6.2880000000000003,6.3289999999999997,6.3470000000000004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.968,7.9669999999999996,7.9749999999999996,8.0470000000000006,8.0960000000000001,8.1489999999999991,8.1709999999999994]
[null,null,null,null,"Coincident",6.2329999999999997,6.2320000000000002,6.2389999999999999,6.2939999999999996,6.3330000000000002,6.3739999999999997,6.3920000000000003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.2130000000000001,7.2149999999999999,7.2240000000000002,7.2949999999999999,7.3449999999999998,7.3970000000000002,7.4189999999999996]
[null,null,null,null,"Coincident",5.6429999999999998,5.6440000000000001,5.6509999999999998,5.7060000000000004,5.7450000000000001,5.7859999999999996,5.8029999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.2649999999999997,7.266,7.2759999999999998,7.3470000000000004,7.3970000000000002,7.4489999999999998,7.4720000000000004]
[null,null,null,null,"Coincident",5.6829999999999998,5.6840000000000002,5.6909999999999998,5.7469999999999999,5.7859999999999996,5.827,5.8449999999999998]
[null,"Muswellbrook 33_11kV","Substation Rating","MVA","Non-Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,null,null,"Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.104,-0.214,-0.29399999999999998,-0.35899999999999999,-0.432,-0.501,-0.56599999999999995]
[null,null,null,null,"Coincident",-1.0489999999999999,-1.3660000000000001,-1.5720000000000001,-1.712,-1.855,-1.9970000000000001,-2.137]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.02,19.11,19.170000000000002,19.21,19.22,19.22,19.190000000000001]
[null,null,null,null,"Coincident",15.55,15.63,15.68,15.71,15.72,15.72,15.7]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.29,19.38,19.45,19.489999999999998,19.5,19.5,19.47]
[null,null,null,null,"Coincident",15.77,15.85,15.91,15.94,15.95,15.95,15.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.21,17.29,17.350000000000001,17.38,17.39,17.399999999999999,17.37]
[null,null,null,null,"Coincident",14.08,14.14,14.19,14.22,14.22,14.23,14.21]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.37,17.45,17.52,17.55,17.559999999999999,17.57,17.54]
[null,null,null,null,"Coincident",14.21,14.27,14.33,14.36,14.36,14.37,14.34]
[null,"Narrabeen 33_11kV","Substation Rating","MVA","Non-Coincident",21.05,21.05,21.05,21.05,21.05,21.05,21.05]
[null,null,null,null,"Coincident",19.62,19.62,19.62,19.62,19.62,19.62,19.62]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1000000000000001E-2,-4.1000000000000002E-2,-6.2E-2,-8.6999999999999994E-2,-0.12,-0.15,-0.17699999999999999]
[null,null,null,null,"Coincident",-1.125,-1.474,-1.69,-1.82,-1.9430000000000001,-2.0659999999999998,-2.1869999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.65,13.82,13.95,14.05,14.06,14.04,14.02]
[null,null,null,null,"Coincident",11.46,11.58,11.64,11.68,11.68,11.66,11.64]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.22,14.39,14.53,14.63,14.65,14.62,14.6]
[null,null,null,null,"Coincident",12.25,12.37,12.44,12.48,12.48,12.46,12.44]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.95,13.1,13.23,13.33,13.34,13.31,13.3]
[null,null,null,null,"Coincident",10.26,10.36,10.41,10.45,10.45,10.43,10.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.49,13.65,13.78,13.88,13.9,13.87,13.85]
[null,null,null,null,"Coincident",10.96,11.07,11.13,11.17,11.17,11.15,11.13]
[null,"Nelson Bay 33_11kV","Substation Rating","MVA","Non-Coincident",45.73,45.73,45.73,45.73,45.73,45.73,45.73]
[null,null,null,null,"Coincident",45.73,45.73,45.73,45.73,45.73,45.73,45.73]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.5000000000000003E-2,-6.4000000000000001E-2,-9.8000000000000004E-2,-0.14599999999999999,-0.20899999999999999,-0.26600000000000001,-0.318]
[null,null,null,null,"Coincident",-1.762,-2.294,-2.649,-2.9,-3.1659999999999999,-3.4319999999999999,-3.6930000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.56,26.68,27.09,27.35,27.39,27.34,27.33]
[null,null,null,null,"Coincident",23.58,23.88,23.91,23.91,23.87,23.81,23.72]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.66,26.8,27.22,27.48,27.52,27.48,27.46]
[null,null,null,null,"Coincident",23.77,24.07,24.1,24.11,24.07,24,23.91]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.17,25.39,25.88,26.18,26.22,26.17,26.16]
[null,null,null,null,"Coincident",20.440000000000001,20.74,20.77,20.78,20.74,20.68,20.58]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.26,25.51,26.02,26.32,26.36,26.31,26.3]
[null,null,null,null,"Coincident",20.6,20.92,20.95,20.95,20.91,20.85,20.75]
[null,"New Lambton 33_11kV","Substation Rating","MVA","Non-Coincident",23.59,23.59,23.59,23.59,23.59,23.59,23.59]
[null,null,null,null,"Coincident",23.59,23.59,23.59,23.59,23.59,23.59,23.59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.151,-0.27300000000000002,-0.26200000000000001,-0.30299999999999999,-0.34699999999999998,-0.38900000000000001,-0.43]
[null,null,null,null,"Coincident",-0.77700000000000002,-1.0169999999999999,-1.1639999999999999,-1.248,-1.325,-1.4019999999999999,-1.4790000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.59,21.92,22.06,22.07,22.07,22.05,22.05]
[null,null,null,null,"Coincident",20.55,20.86,21,21.01,21.01,20.99,20.99]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.62,22.96,23.11,23.13,23.12,23.1,23.1]
[null,null,null,null,"Coincident",21.54,21.86,22,22.02,22.01,21.99,22]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.89,19.18,19.3,19.32,19.309999999999999,19.29,19.3]
[null,null,null,null,"Coincident",17.98,18.260000000000002,18.38,18.39,18.39,18.37,18.37]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.79,20.09,20.22,20.239999999999998,20.23,20.21,20.22]
[null,null,null,null,"Coincident",18.84,19.13,19.25,19.27,19.260000000000002,19.25,19.25]
[null,"Newcastle CBD 33_11kV","Substation Rating","MVA","Non-Coincident",76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994]
[null,null,null,null,"Coincident",76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994,76.209999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.8479999999999999,-4.4160000000000004,-4.9210000000000003,-5.44,-6.1020000000000003,-6.7270000000000003,-7.3380000000000001]
[null,null,null,null,"Coincident",-1.577,-2.0089999999999999,-2.3730000000000002,-2.738,-3.1880000000000002,-3.637,-4.077]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.55,44.95,44.49,44.36,44.12,44.01,43.67]
[null,null,null,null,"Coincident",41.99,41.43,41.01,40.89,40.67,40.57,40.25]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.55,45.05,44.58,44.45,44.21,44.09,43.75]
[null,null,null,null,"Coincident",41.99,41.52,41.09,40.97,40.75,40.64,40.33]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.94,39.4,38.979999999999997,38.85,38.61,38.5,38.159999999999997]
[null,null,null,null,"Coincident",36.81,36.32,35.93,35.81,35.590000000000003,35.49,35.17]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40,39.46,39.03,38.9,38.659999999999997,38.549999999999997,38.200000000000003]
[null,null,null,null,"Coincident",36.869999999999997,36.369999999999997,35.979999999999997,35.86,35.64,35.53,35.22]
[null,"Newdell 66_11kV","Substation Rating","MVA","Non-Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,null,null,"Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.7E-2,-4.4999999999999998E-2,-5.8000000000000003E-2,-7.0000000000000007E-2,-8.4000000000000005E-2,-9.6000000000000002E-2,-0.108]
[null,null,null,null,"Coincident",-0.06,-7.8E-2,-9.0999999999999998E-2,-0.10199999999999999,-0.114,-0.126,-0.13700000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.8279999999999998,3.7709999999999999,3.7440000000000002,3.7429999999999999,3.7410000000000001,3.7389999999999999,3.835]
[null,null,null,null,"Coincident",2.2250000000000001,2.1920000000000002,2.1760000000000002,2.1760000000000002,2.1739999999999999,2.173,2.2290000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.9359999999999999,3.8780000000000001,3.85,3.85,3.847,3.8450000000000002,3.944]
[null,null,null,null,"Coincident",2.2879999999999998,2.254,2.2370000000000001,2.2370000000000001,2.2360000000000002,2.2349999999999999,2.2919999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.6960000000000002,3.641,3.6139999999999999,3.6139999999999999,3.6120000000000001,3.61,3.706]
[null,null,null,null,"Coincident",2.1480000000000001,2.1160000000000001,2.101,2.101,2.0990000000000002,2.0979999999999999,2.1539999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8010000000000002,3.7440000000000002,3.7170000000000001,3.7170000000000001,3.714,3.7120000000000002,3.8109999999999999]
[null,null,null,null,"Coincident",2.2090000000000001,2.1760000000000002,2.16,2.16,2.1589999999999998,2.1579999999999999,2.2149999999999999]
[null,"Newport 33_11kV","Substation Rating","MVA","Non-Coincident",22.38,22.38,22.38,22.38,22.38,22.38,22.38]
[null,null,null,null,"Coincident",20.75,20.75,20.75,20.75,20.75,20.75,20.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.3E-2,-4.7E-2,-7.0999999999999994E-2,-0.10100000000000001,-0.14099999999999999,-0.17799999999999999,-0.21099999999999999]
[null,null,null,null,"Coincident",-1.248,-1.6359999999999999,-1.879,-2.028,-2.1709999999999998,-2.3140000000000001,-2.4550000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.23,17.600000000000001,17.86,18.02,18.07,18.05,17.98]
[null,null,null,null,"Coincident",12.91,13.09,13.18,13.19,13.2,13.18,13.15]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.579999999999998,17.96,18.23,18.39,18.43,18.420000000000002,18.350000000000001]
[null,null,null,null,"Coincident",13.08,13.26,13.36,13.36,13.38,13.35,13.32]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.37,16.72,16.97,17.12,17.170000000000002,17.149999999999999,17.079999999999998]
[null,null,null,null,"Coincident",11.49,11.65,11.73,11.73,11.75,11.72,11.69]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.71,17.059999999999999,17.32,17.47,17.52,17.5,17.43]
[null,null,null,null,"Coincident",11.64,11.8,11.88,11.89,11.9,11.88,11.85]
[null,"Noraville 33_11kV","Substation Rating","MVA","Non-Coincident",30.1,30.1,30.1,30.1,30.1,30.1,30.1]
[null,null,null,null,"Coincident",30.1,30.1,30.1,30.1,30.1,30.1,30.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.1000000000000002E-2,-8.2000000000000003E-2,-0.122,-0.17299999999999999,-0.24,-0.30199999999999999,-0.35699999999999998]
[null,null,null,null,"Coincident",-2.246,-2.9380000000000002,-3.3679999999999999,-3.6280000000000001,-3.8730000000000002,-4.1189999999999998,-4.3609999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.46,26.25,26.59,26.79,26.86,26.95,26.94]
[null,null,null,null,"Coincident",22.7,23.07,23.28,23.33,23.41,23.38,23.32]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.98,26.79,27.13,27.34,27.4,27.5,27.49]
[null,null,null,null,"Coincident",24.15,24.54,24.77,24.82,24.9,24.87,24.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.05,24.85,25.19,25.39,25.46,25.55,25.54]
[null,null,null,null,"Coincident",19.97,20.3,20.49,20.54,20.62,20.59,20.53]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.54,25.35,25.7,25.91,25.98,26.07,26.06]
[null,null,null,null,"Coincident",21.24,21.6,21.8,21.85,21.93,21.9,21.84]
[null,"North Head 33_11kV","Substation Rating","MVA","Non-Coincident",23.64,23.64,23.64,23.64,23.64,23.64,23.64]
[null,null,null,null,"Coincident",23.64,23.64,23.64,23.64,23.64,23.64,23.64]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1E-3,-2E-3,-4.0000000000000001E-3,-8.0000000000000002E-3,-1.4E-2,-0.02,-2.4E-2]
[null,null,null,null,"Coincident",-0.17,-0.218,-0.26,-0.30399999999999999,-0.35799999999999998,-0.41299999999999998,-0.46700000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.600000000000001,16.600000000000001,16.61,16.63,16.649999999999999,16.670000000000002,16.690000000000001]
[null,null,null,null,"Coincident",6.7549999999999999,6.758,6.7640000000000002,6.7789999999999999,6.7880000000000003,6.7949999999999999,6.7880000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.84,17.84,17.86,17.88,17.899999999999999,17.920000000000002,17.95]
[null,null,null,null,"Coincident",7.3819999999999997,7.3860000000000001,7.3920000000000003,7.4080000000000004,7.4180000000000001,7.4260000000000002,7.4189999999999996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.600000000000001,16.600000000000001,16.61,16.63,16.649999999999999,16.670000000000002,16.690000000000001]
[null,null,null,null,"Coincident",5.9009999999999998,5.9039999999999999,5.91,5.9249999999999998,5.9340000000000002,5.9409999999999998,5.9349999999999996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.84,17.84,17.86,17.88,17.899999999999999,17.920000000000002,17.95]
[null,null,null,null,"Coincident",6.4489999999999998,6.4530000000000003,6.4589999999999996,6.4749999999999996,6.4850000000000003,6.4930000000000003,6.4859999999999998]
[null,"North Sydney 132_11kV","Substation Rating","MVA","Non-Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,null,null,"Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.3120000000000001,-1.9079999999999999,-2.5550000000000002,-3.3340000000000001,-4.3849999999999998,-4.1360000000000001,-4.8330000000000002]
[null,null,null,null,"Coincident",-1.6240000000000001,-2.0190000000000001,-2.4220000000000002,-2.9009999999999998,-3.5249999999999999,-4.1479999999999997,-4.758]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",64.150000000000006,67.88,67.319999999999993,64.599999999999994,65.61,65.760000000000005,65.760000000000005]
[null,null,null,null,"Coincident",55.63,58.87,58.39,56.03,56.9,57.03,57.03]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",64.489999999999995,68.239999999999995,67.680000000000007,64.95,65.959999999999994,66.11,66.11]
[null,null,null,null,"Coincident",55.93,59.19,58.7,56.33,57.21,57.34,57.34]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.27,64.09,63.57,60.85,61.85,62,62]
[null,null,null,null,"Coincident",52.28,55.58,55.13,52.77,53.65,53.77,53.78]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",60.6,64.430000000000007,63.9,61.17,62.18,62.33,62.33]
[null,null,null,null,"Coincident",52.56,55.88,55.42,53.05,53.93,54.06,54.06]
[null,"Nulkaba 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.19800000000000001,-0.27900000000000003,-0.33600000000000002,-0.38,-0.42899999999999999,-0.47499999999999998,-0.51900000000000002]
[null,null,null,null,"Coincident",-0.89200000000000002,-1.169,-1.347,-1.4630000000000001,-1.58,-1.696,-1.8109999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.079999999999998,19.73,19.579999999999998,19.66,19.72,19.77,19.91]
[null,null,null,null,"Coincident",18.86,18.53,18.39,18.47,18.52,18.57,18.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.079999999999998,19.73,19.579999999999998,19.670000000000002,19.73,19.77,19.920000000000002]
[null,null,null,null,"Coincident",18.86,18.53,18.39,18.48,18.53,18.57,18.71]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.170000000000002,17.86,17.73,17.809999999999999,17.87,17.920000000000002,18.059999999999999]
[null,null,null,null,"Coincident",17.07,16.77,16.649999999999999,16.73,16.79,16.829999999999998,16.97]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.170000000000002,17.86,18.170000000000002,17.809999999999999,17.87,17.920000000000002,18.059999999999999]
[null,null,null,null,"Coincident",17.07,16.77,17.07,16.73,16.79,16.829999999999998,16.97]
[null,"Olympic Park 132_11kV","Substation Rating","MVA","Non-Coincident",56.81,56.81,56.81,56.81,56.81,56.81,56.81]
[null,null,null,null,"Coincident",56.81,56.81,56.81,56.81,56.81,56.81,56.81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.1870000000000001,-1.2210000000000001,-1.2609999999999999,-1.3089999999999999,-1.377,-1.4410000000000001,-1.5029999999999999]
[null,null,null,null,"Coincident",-0.84399999999999997,-1.0820000000000001,-1.2909999999999999,-1.508,-1.782,-2.056,-2.3250000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.950000000000003,42.4,43.69,44.7,45.68,46.63,47.46]
[null,null,null,null,"Coincident",31.8,36.5,37.61,38.47,39.32,40.14,40.85]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.1,42.58,43.88,44.89,45.87,46.83,47.66]
[null,null,null,null,"Coincident",31.94,36.65,37.770000000000003,38.64,39.479999999999997,40.31,41.02]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.85,39.31,40.6,41.6,42.58,43.53,44.36]
[null,null,null,null,"Coincident",29.14,33.83,34.950000000000003,35.81,36.65,37.47,38.18]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.99,39.47,40.770000000000003,41.78,42.76,43.72,44.55]
[null,null,null,null,"Coincident",29.26,33.979999999999997,35.090000000000003,35.96,36.81,37.630000000000003,38.35]
[null,"Paddington 33_11kV","Substation Rating","MVA","Non-Coincident",69.83,69.83,69.83,69.83,69.83,69.83,69.83]
[null,null,null,null,"Coincident",66.47,66.47,66.47,66.47,66.47,66.47,66.47]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.7000000000000001E-2,-3.3000000000000002E-2,-6.7000000000000004E-2,-0.127,-0.20899999999999999,-0.28299999999999997,-0.34699999999999998]
[null,null,null,null,"Coincident",-1.373,-1.7390000000000001,-2.0659999999999998,-2.411,-2.8490000000000002,-3.286,-3.7149999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.79,33.78,33.75,34.03,34.6,35.299999999999997,35.880000000000003]
[null,null,null,null,"Coincident",29.89,29.27,29.49,29.75,30.27,30.49,30.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.159999999999997,34.159999999999997,34.14,34.42,34.99,35.700000000000003,36.29]
[null,null,null,null,"Coincident",30.86,30.21,30.43,30.7,31.24,31.47,31.58]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.51,32.619999999999997,32.68,33,33.56,34.26,34.840000000000003]
[null,null,null,null,"Coincident",27.97,27.38,27.62,27.88,28.4,28.62,28.73]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.87,32.99,33.049999999999997,33.369999999999997,33.94,34.659999999999997,35.24]
[null,null,null,null,"Coincident",28.87,28.26,28.51,28.77,29.31,29.54,29.65]
[null,"Paxton 33_11kV","Substation Rating","MVA","Non-Coincident",25.45,25.45,25.45,25.45,25.45,25.45,25.45]
[null,null,null,null,"Coincident",25.45,25.45,25.45,25.45,25.45,25.45,25.45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.311,-0.35199999999999998,-0.38400000000000001,-0.40600000000000003,-0.42899999999999999,-0.45100000000000001,-0.47199999999999998]
[null,null,null,null,"Coincident",-0.56799999999999995,-0.748,-0.85499999999999998,-0.91100000000000003,-0.95699999999999996,-1.004,-1.0489999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.0809999999999995,8.2249999999999996,8.3070000000000004,8.3089999999999993,8.3030000000000008,8.2889999999999997,8.282]
[null,null,null,null,"Coincident",6.1029999999999998,6.2110000000000003,6.274,6.2750000000000004,6.27,6.26,6.2549999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.9789999999999992,9.1379999999999999,9.23,9.2319999999999993,9.2249999999999996,9.2089999999999996,9.202]
[null,null,null,null,"Coincident",6.7809999999999997,6.9009999999999998,6.9710000000000001,6.9720000000000004,6.9669999999999996,6.9550000000000001,6.9489999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.2030000000000003,7.3289999999999997,7.4020000000000001,7.4039999999999999,7.3979999999999997,7.3840000000000003,7.3769999999999998]
[null,null,null,null,"Coincident",5.4390000000000001,5.5350000000000001,5.59,5.5910000000000002,5.5869999999999997,5.5759999999999996,5.5709999999999997]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.0030000000000001,8.1430000000000007,8.2249999999999996,8.2260000000000009,8.2200000000000006,8.2040000000000006,8.1959999999999997]
[null,null,null,null,"Coincident",6.0439999999999996,6.15,6.2110000000000003,6.2130000000000001,6.2080000000000002,6.1959999999999997,6.19]
[null,"Peats Ridge 33_11kV","Substation Rating","MVA","Non-Coincident",17.09,17.09,17.09,17.09,17.09,17.09,17.09]
[null,null,null,null,"Coincident",17.09,17.09,17.09,17.09,17.09,17.09,17.09]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-7.3999999999999996E-2,-8.3000000000000004E-2,-9.2999999999999999E-2,-0.106,-0.122,-0.13700000000000001,-0.15]
[null,null,null,null,"Coincident",-0.45200000000000001,-0.58899999999999997,-0.68600000000000005,-0.76200000000000001,-0.84499999999999997,-0.92900000000000005,-1.0109999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.18,10.99,10.94,11.07,11.17,11.28,11.34]
[null,null,null,null,"Coincident",9.8249999999999993,9.6579999999999995,9.6150000000000002,9.7260000000000009,9.8109999999999999,9.9130000000000003,9.9629999999999992]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.7,11.5,11.45,11.58,11.69,11.81,11.87]
[null,null,null,null,"Coincident",10.28,10.11,10.06,10.18,10.27,10.37,10.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.24,10.06,10.02,10.15,10.25,10.36,10.42]
[null,null,null,null,"Coincident",8.9939999999999998,8.8420000000000005,8.8070000000000004,8.9179999999999993,9.0030000000000001,9.1050000000000004,9.1539999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.71,10.53,10.49,10.62,10.72,10.84,10.9]
[null,null,null,null,"Coincident",9.4109999999999996,9.2520000000000007,9.2149999999999999,9.3309999999999995,9.42,9.5259999999999998,9.5790000000000006]
[null,"Pelican 33_11kV","Substation Rating","MVA","Non-Coincident",25.64,25.64,25.64,25.64,25.64,25.64,25.64]
[null,null,null,null,"Coincident",25.64,25.64,25.64,25.64,25.64,25.64,25.64]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.6E-2,-3.1E-2,-4.7E-2,-6.9000000000000006E-2,-9.8000000000000004E-2,-0.125,-0.14899999999999999]
[null,null,null,null,"Coincident",-0.85299999999999998,-1.111,-1.2809999999999999,-1.3959999999999999,-1.5149999999999999,-1.6339999999999999,-1.752]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.62,11.82,11.92,12.35,12.37,12.37,12.35]
[null,null,null,null,"Coincident",12.04,11.84,12.16,12.17,12.16,12.13,12.07]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.65,11.86,11.95,12.38,12.41,12.4,12.39]
[null,null,null,null,"Coincident",12.19,11.99,12.31,12.32,12.31,12.28,12.21]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.89,11.09,11.18,11.6,11.63,11.63,11.61]
[null,null,null,null,"Coincident",10.47,10.29,10.62,10.63,10.62,10.59,10.52]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.92,11.12,11.21,11.64,11.66,11.66,11.64]
[null,null,null,null,"Coincident",10.6,10.41,10.75,10.75,10.74,10.72,10.65]
[null,"Pennant Hills 132_11kV","Substation Rating","MVA","Non-Coincident",106.9,106.9,106.9,106.9,106.9,106.9,106.9]
[null,null,null,null,"Coincident",106.9,106.9,106.9,106.9,106.9,106.9,106.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.84099999999999997,-1.224,-1.492,-1.7070000000000001,-1.948,-2.1749999999999998,-2.3889999999999998]
[null,null,null,null,"Coincident",-5.5270000000000001,-7.2690000000000001,-8.3360000000000003,-8.9589999999999996,-9.5329999999999995,-10.11,-10.67]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",95.32,96.32,96.99,97.41,97.8,97.9,98.31]
[null,null,null,null,"Coincident",87.31,88.24,88.85,89.23,89.59,89.68,90.05]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",98.84,99.89,100.6,101,101.4,101.5,101.9]
[null,null,null,null,"Coincident",90.55,91.5,92.13,92.53,92.91,93,93.39]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",81.77,82.68,83.3,83.72,84.12,84.22,84.62]
[null,null,null,null,"Coincident",74.900000000000006,75.739999999999995,76.31,76.69,77.06,77.150000000000006,77.52]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",84.79,85.74,86.39,86.82,87.23,87.34,87.75]
[null,null,null,null,"Coincident",77.67,78.55,79.13,79.53,79.91,80,80.39]
[null,"Port Botany 33_11kV","Substation Rating","MVA","Non-Coincident",59.16,59.16,59.16,59.16,59.16,59.16,59.16]
[null,null,null,null,"Coincident",59.16,59.16,59.16,59.16,59.16,59.16,59.16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.38500000000000001,-0.51,-0.61699999999999999,-0.71699999999999997,-0.84099999999999997,-0.95799999999999996,-1.071]
[null,null,null,null,"Coincident",-0.36099999999999999,-0.46700000000000003,-0.55200000000000005,-0.63400000000000001,-0.73499999999999999,-0.83599999999999997,-0.93500000000000005]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.149999999999999,16.96,16.850000000000001,16.91,16.96,17,17.03]
[null,null,null,null,"Coincident",14.7,14.54,14.44,14.5,14.54,14.58,14.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.52,18.32,18.2,18.260000000000002,18.32,18.37,18.399999999999999]
[null,null,null,null,"Coincident",15.88,15.71,15.6,15.66,15.7,15.75,15.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.55,16.38,16.27,16.329999999999998,16.38,16.420000000000002,16.45]
[null,null,null,null,"Coincident",14.19,14.04,13.95,14,14.04,14.08,14.1]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.87,17.690000000000001,17.57,17.64,17.690000000000001,17.739999999999998,17.77]
[null,null,null,null,"Coincident",15.32,15.17,15.06,15.12,15.17,15.21,15.23]
[null,"Potts Hill 132_11kV","Substation Rating","MVA","Non-Coincident",54.87,54.87,54.87,54.87,54.87,54.87,54.87]
[null,null,null,null,"Coincident",54.87,54.87,54.87,54.87,54.87,54.87,54.87]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.1990000000000001,-1.8029999999999999,-1.45,-1.6240000000000001,-1.825,-2.0139999999999998,-2.1960000000000002]
[null,null,null,null,"Coincident",-2.3210000000000002,-3.0350000000000001,-3.508,-3.839,-4.1849999999999996,-4.5330000000000004,-4.8739999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.12,44.28,44.52,44.82,45.28,45.51,45.69]
[null,null,null,null,"Coincident",45.78,42.13,42.35,42.65,43.08,43.3,43.46]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.62,45.29,45.53,45.84,46.31,46.54,46.73]
[null,null,null,null,"Coincident",46.25,43.09,43.32,43.62,44.06,44.28,44.45]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.06,39.26,39.520000000000003,39.82,40.28,40.51,40.68]
[null,null,null,null,"Coincident",40.97,37.36,37.6,37.89,38.32,38.54,38.71]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.51,40.229999999999997,40.49,40.81,41.27,41.51,41.69]
[null,null,null,null,"Coincident",41.4,38.28,38.53,38.82,39.26,39.49,39.659999999999997]
[null,"Punchbowl 33_11kV","Substation Rating","MVA","Non-Coincident",57.27,57.27,57.27,57.27,57.27,57.27,57.27]
[null,null,null,null,"Coincident",56.17,56.17,56.17,56.17,56.17,56.17,56.17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.9E-2,-7.8E-2,-0.128,-0.19900000000000001,-0.30099999999999999,-0.39300000000000002,-0.47399999999999998]
[null,null,null,null,"Coincident",-2.6120000000000001,-3.3860000000000001,-3.931,-4.351,-4.82,-5.2889999999999997,-5.7510000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.64,39.729999999999997,40.479999999999997,41.21,41.46,41.72,42.19]
[null,null,null,null,"Coincident",39.24,40.61,41.4,41.71,41.84,42.24,42.36]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.67,39.76,40.51,41.24,41.49,41.75,42.22]
[null,null,null,null,"Coincident",39.47,40.85,41.64,41.95,42.09,42.49,42.61]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.35,38.65,39.549999999999997,40.35,40.6,40.86,41.33]
[null,null,null,null,"Coincident",34.979999999999997,36.32,37.090000000000003,37.4,37.53,37.93,38.06]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.369999999999997,38.68,39.57,40.380000000000003,40.630000000000003,40.89,41.36]
[null,null,null,null,"Coincident",35.18,36.53,37.31,37.619999999999997,37.75,38.15,38.28]
[null,"Pymble 33_11kV","Substation Rating","MVA","Non-Coincident",41.48,41.48,41.48,41.48,41.48,41.48,41.48]
[null,null,null,null,"Coincident",39.43,39.43,39.43,39.43,39.43,39.43,39.43]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.5000000000000003E-2,-6.9000000000000006E-2,-0.107,-0.157,-0.22700000000000001,-0.28899999999999998,-0.34399999999999997]
[null,null,null,null,"Coincident",-1.895,-2.4809999999999999,-2.87,-3.1419999999999999,-3.4249999999999998,-3.7090000000000001,-3.988]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.9,32.619999999999997,33.1,33.22,33.380000000000003,33.47,33.549999999999997]
[null,null,null,null,"Coincident",33.06,33.659999999999997,34,34.119999999999997,34.200000000000003,34.26,34.28]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.68,33.42,33.909999999999997,34.03,34.19,34.29,34.369999999999997]
[null,null,null,null,"Coincident",36.35,37.01,37.369999999999997,37.520000000000003,37.6,37.659999999999997,37.69]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.6,31.42,31.96,32.119999999999997,32.270000000000003,32.369999999999997,32.450000000000003]
[null,null,null,null,"Coincident",29.08,29.66,29.99,30.12,30.19,30.25,30.28]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.34,32.19,32.74,32.9,33.06,33.159999999999997,33.24]
[null,null,null,null,"Coincident",31.97,32.61,32.97,33.11,33.200000000000003,33.26,33.29]
[null,"RNS Hospital 132_11kV","Substation Rating","MVA","Non-Coincident",53.54,53.54,53.54,53.54,53.54,53.54,53.54]
[null,null,null,null,"Coincident",53.54,53.54,53.54,53.54,53.54,53.54,53.54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-7.2999999999999995E-2,-0.128,-0.17799999999999999,-0.22600000000000001,-0.28799999999999998,-0.34699999999999998,-0.40300000000000002]
[null,null,null,null,"Coincident",-0.13,-0.16900000000000001,-0.20300000000000001,-0.23899999999999999,-0.28499999999999998,-0.33100000000000002,-0.376]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.45,13.79,13.97,14.03,14.09,14.15,14.17]
[null,null,null,null,"Coincident",11.55,11.84,12,12.05,12.1,12.15,12.17]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.61,13.95,14.13,14.2,14.25,14.31,14.34]
[null,null,null,null,"Coincident",11.68,11.97,12.13,12.19,12.24,12.29,12.31]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.53,12.88,13.08,13.14,13.19,13.25,13.28]
[null,null,null,null,"Coincident",10.76,11.06,11.23,11.28,11.33,11.38,11.4]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.68,13.03,13.23,13.29,13.35,13.41,13.43]
[null,null,null,null,"Coincident",10.88,11.19,11.36,11.41,11.46,11.51,11.53]
[null,"Rathmines 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.47,-0.61799999999999999,-0.71399999999999997,-0.78,-0.84899999999999998,-0.91400000000000003,-0.97699999999999998]
[null,null,null,null,"Coincident",-1.3759999999999999,-1.7989999999999999,-2.052,-2.19,-2.31,-2.431,-2.5489999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.079999999999998,18.21,18.27,18.22,18.13,18.03,17.91]
[null,null,null,null,"Coincident",15.76,15.87,15.92,15.88,15.8,15.71,15.6]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.28,18.399999999999999,18.46,18.420000000000002,18.329999999999998,18.23,18.100000000000001]
[null,null,null,null,"Coincident",15.93,16.04,16.09,16.05,15.97,15.88,15.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.73,15.83,15.87,15.83,15.74,15.64,15.51]
[null,null,null,null,"Coincident",13.71,13.79,13.83,13.79,13.72,13.63,13.52]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.9,16,16.04,16,15.91,15.81,15.68]
[null,null,null,null,"Coincident",13.85,13.94,13.98,13.94,13.86,13.78,13.66]
[null,"Raymond Terr NEW 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.2000000000000001E-2,-6.0999999999999999E-2,-8.7999999999999995E-2,-0.125,-0.17199999999999999,-0.21099999999999999,-0.249]
[null,null,null,null,"Coincident",-1.599,-2.0830000000000002,-2.39,-2.5870000000000002,-2.78,-2.9740000000000002,-3.1640000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.84,22.14,22.94,23.7,24.76,26.51,28.58]
[null,null,null,null,"Coincident",22.54,22.41,22.95,23.95,25.81,27.31,28.29]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.94,22.24,23.05,23.82,24.88,26.64,28.72]
[null,null,null,null,"Coincident",22.69,22.55,23.09,24.1,25.98,27.48,28.47]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.73,21.01,21.8,22.56,23.61,25.36,27.43]
[null,null,null,null,"Coincident",20.23,20.14,20.7,21.7,23.57,25.06,26.05]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.829999999999998,21.11,21.9,22.67,23.73,25.49,27.57]
[null,null,null,null,"Coincident",20.36,20.27,20.83,21.84,23.72,25.22,26.21]
[null,"Revesby 132_11kV","Substation Rating","MVA","Non-Coincident",44.93,44.93,44.93,44.93,44.93,44.93,44.93]
[null,null,null,null,"Coincident",44.93,44.93,44.93,44.93,44.93,44.93,44.93]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.2889999999999999,-1.97,-1.601,-1.597,-1.7649999999999999,-2.1469999999999998,-2.9079999999999999]
[null,null,null,null,"Coincident",-3.55,-4.6609999999999996,-5.3479999999999999,-5.7560000000000002,-6.1379999999999999,-6.5209999999999999,-6.899]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.82,50.4,51.48,53.18,54.81,56.84,59.24]
[null,null,null,null,"Coincident",45.44,46.91,47.91,49.5,51.02,52.91,55.14]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",49.88,51.49,52.59,54.33,56,58.08,60.52]
[null,null,null,null,"Coincident",46.43,47.93,48.95,50.57,52.12,54.05,56.33]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.42,44.97,46.03,47.74,49.37,51.4,53.8]
[null,null,null,null,"Coincident",40.42,41.86,42.85,44.43,45.95,47.84,50.07]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.36,45.94,47.03,48.77,50.44,52.51,54.96]
[null,null,null,null,"Coincident",41.29,42.76,43.77,45.39,46.95,48.88,51.15]
[null,"Riverwood 33_11kV","Substation Rating","MVA","Non-Coincident",42.81,42.81,42.81,42.81,42.81,42.81,42.81]
[null,null,null,null,"Coincident",42.81,42.81,42.81,42.81,42.81,42.81,42.81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.9E-2,-7.8E-2,-0.121,-0.18,-0.25900000000000001,-0.33100000000000002,-0.39600000000000002]
[null,null,null,null,"Coincident",-2.1869999999999998,-2.835,-3.2679999999999998,-3.5760000000000001,-3.9,-4.2240000000000002,-4.5430000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.25,25.86,26.12,26.25,26.29,26.19,26.28]
[null,null,null,null,"Coincident",25.33,25.74,25.87,25.91,25.85,25.94,25.86]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.34,26.98,27.25,27.38,27.43,27.32,27.42]
[null,null,null,null,"Coincident",27.55,28,28.15,28.18,28.12,28.22,28.14]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.05,24.73,25.03,25.19,25.23,25.13,25.22]
[null,null,null,null,"Coincident",22.33,22.72,22.85,22.89,22.83,22.92,22.84]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.09,25.8,26.12,26.28,26.32,26.21,26.31]
[null,null,null,null,"Coincident",24.29,24.72,24.86,24.9,24.83,24.94,24.85]
[null,"Rockdale 132_11kV","Substation Rating","MVA","Non-Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,null,null,"Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.8879999999999999,-1.921,-1.98,-2.0640000000000001,-2.1749999999999998,-2.2770000000000001,-2.2679999999999998]
[null,null,null,null,"Coincident",-2.2269999999999999,-2.8809999999999998,-3.367,-3.774,-4.2480000000000002,-4.7220000000000004,-5.1879999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",56.54,58.62,59.13,59.12,59.08,58.99,58.76]
[null,null,null,null,"Coincident",43.51,45.12,45.51,45.5,45.47,45.4,45.22]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",56.9,58.99,59.51,59.5,59.45,59.37,59.13]
[null,null,null,null,"Coincident",43.79,45.41,45.8,45.79,45.76,45.69,45.51]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",52.13,54.2,54.7,54.69,54.65,54.56,54.32]
[null,null,null,null,"Coincident",40.119999999999997,41.71,42.1,42.09,42.06,41.99,41.81]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.47,54.55,55.05,55.05,55,54.92,54.68]
[null,null,null,null,"Coincident",40.39,41.99,42.37,42.37,42.33,42.27,42.08]
[null,"Rose Bay 132_11kV","Substation Rating","MVA","Non-Coincident",59.25,59.25,59.25,59.25,59.25,59.25,59.25]
[null,null,null,null,"Coincident",59.25,59.25,59.25,59.25,59.25,59.25,59.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.6999999999999998E-2,-7.4999999999999997E-2,-0.124,-0.19800000000000001,-0.29799999999999999,-0.39,-0.47099999999999997]
[null,null,null,null,"Coincident",-2.0910000000000002,-2.7229999999999999,-3.1819999999999999,-3.5529999999999999,-3.98,-4.4059999999999997,-4.8250000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.46,53.66,54.26,54.65,55.05,55.45,55.59]
[null,null,null,null,"Coincident",35.82,36.33,36.35,36.11,36.42,36.479999999999997,36.869999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.46,53.66,54.26,54.65,55.05,55.45,55.6]
[null,null,null,null,"Coincident",36.22,36.74,36.76,36.520000000000003,36.840000000000003,36.89,37.29]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.42,50.27,50.62,50.89,51.29,51.69,51.84]
[null,null,null,null,"Coincident",32.75,33.28,33.32,33.07,33.39,33.450000000000003,33.840000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.43,50.27,50.63,50.9,51.3,51.7,51.84]
[null,null,null,null,"Coincident",33.119999999999997,33.659999999999997,33.69,33.450000000000003,33.770000000000003,33.83,34.22]
[null,"Rothbury 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.184,-0.23799999999999999,-0.27900000000000003,-0.315,-0.35699999999999998,-0.39600000000000002,-0.433]
[null,null,null,null,"Coincident",-0.53700000000000003,-0.69799999999999995,-0.80800000000000005,-0.88900000000000001,-0.97599999999999998,-1.0629999999999999,-1.147]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.74,11.79,11.84,11.91,11.95,11.99,12]
[null,null,null,null,"Coincident",10.039999999999999,10.09,10.130000000000001,10.18,10.220000000000001,10.26,10.27]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.81,14.88,14.94,15.02,15.07,15.13,15.15]
[null,null,null,null,"Coincident",12.67,12.73,12.78,12.85,12.9,12.94,12.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.62,10.68,10.73,10.79,10.84,10.88,10.89]
[null,null,null,null,"Coincident",9.0869999999999997,9.1379999999999999,9.1820000000000004,9.234,9.27,9.3089999999999993,9.3179999999999996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.4,13.48,13.54,13.62,13.67,13.73,13.74]
[null,null,null,null,"Coincident",11.47,11.53,11.59,11.65,11.7,11.75,11.76]
[null,"Rouchel 33_11kV","Substation Rating","MVA","Non-Coincident",5.77,5.77,5.77,5.77,5.77,5.77,5.77]
[null,null,null,null,"Coincident",5.77,5.77,5.77,5.77,5.77,5.77,5.77]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1E-3,-2E-3,-3.0000000000000001E-3,-5.0000000000000001E-3,-7.0000000000000001E-3,-8.9999999999999993E-3,-1.0999999999999999E-2]
[null,null,null,null,"Coincident",-4.2000000000000003E-2,-5.2999999999999999E-2,-6.0999999999999999E-2,-6.8000000000000005E-2,-7.5999999999999998E-2,-8.4000000000000005E-2,-9.1999999999999998E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1779999999999999,1.169,1.1639999999999999,1.167,1.1679999999999999,1.171,1.173]
[null,null,null,null,"Coincident",0.58499999999999996,0.57999999999999996,0.57799999999999996,0.57899999999999996,0.57999999999999996,0.58099999999999996,0.58199999999999996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3089999999999999,1.298,1.294,1.296,1.298,1.3009999999999999,1.3029999999999999]
[null,null,null,null,"Coincident",0.65,0.64500000000000002,0.64200000000000002,0.64400000000000002,0.64500000000000002,0.64600000000000002,0.64700000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1160000000000001,1.107,1.103,1.1060000000000001,1.107,1.1100000000000001,1.1120000000000001]
[null,null,null,null,"Coincident",0.55400000000000005,0.55000000000000004,0.54800000000000004,0.54900000000000004,0.55000000000000004,0.55100000000000005,0.55200000000000005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.24,1.23,1.226,1.228,1.23,1.2330000000000001,1.2350000000000001]
[null,null,null,null,"Coincident",0.61599999999999999,0.61099999999999999,0.60899999999999999,0.61,0.61099999999999999,0.61199999999999999,0.61299999999999999]
[null,"Rutherford 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.23,-0.46,-0.61899999999999999,-0.73899999999999999,-0.871,-0.99399999999999999,-1.113]
[null,null,null,null,"Coincident",-1.5529999999999999,-2.0179999999999998,-2.319,-2.5190000000000001,-2.7210000000000001,-2.923,-3.1219999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.31,36.15,35.89,35.96,35.99,36.01,35.979999999999997]
[null,null,null,null,"Coincident",32.82,32.68,32.44,32.51,32.53,32.549999999999997,32.520000000000003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.409999999999997,36.25,35.979999999999997,36.049999999999997,36.08,36.1,36.06]
[null,null,null,null,"Coincident",32.9,32.76,32.520000000000003,32.590000000000003,32.61,32.630000000000003,32.6]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.85,32.76,32.53,32.6,32.630000000000003,32.65,32.61]
[null,null,null,null,"Coincident",29.69,29.61,29.4,29.47,29.49,29.51,29.48]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.92,32.83,32.590000000000003,32.67,32.700000000000003,32.72,32.68]
[null,null,null,null,"Coincident",29.75,29.67,29.46,29.52,29.55,29.57,29.53]
[null,"Sans Souci 33_11kV","Substation Rating","MVA","Non-Coincident",24.29,24.29,24.29,24.29,24.29,24.29,24.29]
[null,null,null,null,"Coincident",24.29,24.29,24.29,24.29,24.29,24.29,24.29]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.6E-2,-3.5999999999999997E-2,-5.8000000000000003E-2,-0.09,-0.13500000000000001,-0.17599999999999999,-0.21299999999999999]
[null,null,null,null,"Coincident",-1.0149999999999999,-1.323,-1.5369999999999999,-1.6970000000000001,-1.875,-2.0529999999999999,-2.2290000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.46,18.98,19.23,19.32,19.309999999999999,19.260000000000002,19.18]
[null,null,null,null,"Coincident",17.48,17.7,17.8,17.84,17.78,17.73,17.670000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.73,19.25,19.5,19.600000000000001,19.59,19.54,19.45]
[null,null,null,null,"Coincident",17.62,17.850000000000001,17.95,17.989999999999998,17.93,17.88,17.82]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.52,18.14,18.45,18.579999999999998,18.57,18.52,18.440000000000001]
[null,null,null,null,"Coincident",15.38,15.6,15.69,15.73,15.67,15.62,15.56]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.77,18.399999999999999,18.72,18.850000000000001,18.84,18.78,18.7]
[null,null,null,null,"Coincident",15.52,15.73,15.82,15.86,15.81,15.75,15.69]
[null,"Scone 66_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-8.7999999999999995E-2,-0.17899999999999999,-0.24399999999999999,-0.29599999999999999,-0.35499999999999998,-0.41,-0.46300000000000002]
[null,null,null,null,"Coincident",-0.89200000000000002,-1.1579999999999999,-1.33,-1.444,-1.5580000000000001,-1.6719999999999999,-1.7849999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.010000000000002,17.91,17.850000000000001,17.829999999999998,17.8,17.739999999999998,17.66]
[null,null,null,null,"Coincident",15.01,14.93,14.88,14.86,14.83,14.78,14.71]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.02,17.93,17.87,17.850000000000001,17.809999999999999,17.75,17.670000000000002]
[null,null,null,null,"Coincident",15.02,14.94,14.89,14.88,14.84,14.79,14.73]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.36,16.27,16.21,16.190000000000001,16.149999999999999,16.09,16.010000000000002]
[null,null,null,null,"Coincident",13.63,13.56,13.51,13.49,13.46,13.41,13.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.37,16.27,16.22,16.2,16.16,16.100000000000001,16.02]
[null,null,null,null,"Coincident",13.64,13.56,13.52,13.5,13.47,13.42,13.35]
[null,"Sefton 132_11kV","Substation Rating","MVA","Non-Coincident",94.58,94.58,94.58,94.58,94.58,94.58,94.58]
[null,null,null,null,"Coincident",94.58,94.58,94.58,94.58,94.58,94.58,94.58]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.365,-0.73499999999999999,-0.81299999999999994,-0.90500000000000003,-1.022,-1.1299999999999999,-1.226]
[null,null,null,null,"Coincident",-3.383,-4.4260000000000002,-5.0970000000000004,-5.5369999999999999,-5.9790000000000001,-6.4219999999999997,-6.8570000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",59.87,59.74,59.77,60.16,60.56,60.74,60.82]
[null,null,null,null,"Coincident",57.49,57.37,57.4,57.77,58.15,58.33,58.41]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.33,62.2,62.23,62.63,63.05,63.24,63.32]
[null,null,null,null,"Coincident",59.85,59.73,59.76,60.15,60.54,60.73,60.81]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",52.8,52.72,52.78,53.17,53.57,53.75,53.83]
[null,null,null,null,"Coincident",50.7,50.63,50.68,51.06,51.44,51.61,51.69]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.95,54.87,54.93,55.34,55.75,55.94,56.02]
[null,null,null,null,"Coincident",52.77,52.69,52.75,53.14,53.53,53.72,53.8]
[null,"Singleton 66_11kV","Substation Rating","MVA","Non-Coincident",29.84,29.84,29.84,29.84,29.84,29.84,29.84]
[null,null,null,null,"Coincident",29.84,29.84,29.84,29.84,29.84,29.84,29.84]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.64900000000000002,-0.876,-1.05,-0.90600000000000003,-1.0069999999999999,-1.103,-1.1950000000000001]
[null,null,null,null,"Coincident",-0.85899999999999999,-1.115,-1.2869999999999999,-1.41,-1.538,-1.667,-1.7929999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.63,20.37,20.5,20.51,20.49,20.47,20.420000000000002]
[null,null,null,null,"Coincident",19.03,18.79,18.920000000000002,18.93,18.91,18.89,18.84]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.92,22.63,22.78,22.79,22.77,22.75,22.69]
[null,null,null,null,"Coincident",21.15,20.88,21.02,21.03,21.01,20.99,20.93]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.46,18.21,18.36,18.37,18.350000000000001,18.329999999999998,18.27]
[null,null,null,null,"Coincident",17.03,16.809999999999999,16.940000000000001,16.95,16.93,16.91,16.86]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.51,20.239999999999998,20.399999999999999,20.41,20.39,20.36,20.3]
[null,null,null,null,"Coincident",18.93,18.670000000000002,18.82,18.829999999999998,18.809999999999999,18.79,18.73]
[null,"Singleton North 66_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.5999999999999999E-2,-9.4E-2,-0.129,-0.161,-0.19800000000000001,-0.23300000000000001,-0.26500000000000001]
[null,null,null,null,"Coincident",-1.0900000000000001,-1.4370000000000001,-1.6479999999999999,-1.7709999999999999,-1.883,-1.9950000000000001,-2.1059999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.829999999999998,18.73,18.68,18.68,18.63,18.579999999999998,18.5]
[null,null,null,null,"Coincident",15.47,15.4,15.36,15.35,15.31,15.27,15.2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.57,19.47,19.420000000000002,19.41,19.36,19.309999999999999,19.22]
[null,null,null,null,"Coincident",16.079999999999998,16,15.96,15.96,15.91,15.87,15.8]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.010000000000002,16.93,16.88,16.88,16.829999999999998,16.78,16.7]
[null,null,null,null,"Coincident",13.98,13.91,13.88,13.87,13.83,13.79,13.72]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.68,17.600000000000001,17.55,17.54,17.489999999999998,17.440000000000001,17.350000000000001]
[null,null,null,null,"Coincident",14.53,14.46,14.42,14.42,14.38,14.33,14.26]
[null,"Somersby 132_11kV","Substation Rating","MVA","Non-Coincident",56.07,56.07,56.07,56.07,56.07,56.07,56.07]
[null,null,null,null,"Coincident",51.9,51.9,51.9,51.9,51.9,51.9,51.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.861,-2.0470000000000002,-2.165,-2.198,-2.2629999999999999,-2.3260000000000001,-2.3919999999999999]
[null,null,null,null,"Coincident",-0.93799999999999994,-1.2210000000000001,-1.409,-1.542,-1.68,-1.819,-1.9550000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.62,20.9,20.85,20.83,20.96,21.03,21.15]
[null,null,null,null,"Coincident",15.79,16.48,16.45,16.489999999999998,16.510000000000002,16.559999999999999,16.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.09,21.4,21.35,21.32,21.46,21.54,21.66]
[null,null,null,null,"Coincident",16.420000000000002,17.14,17.11,17.16,17.18,17.22,17.2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.07,20.63,20.77,20.85,20.98,21.06,21.17]
[null,null,null,null,"Coincident",14.66,15.36,15.34,15.38,15.4,15.44,15.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.52,21.12,21.27,21.35,21.48,21.56,21.68]
[null,null,null,null,"Coincident",15.25,15.98,15.96,16,16.02,16.07,16.04]
[null,"St Ives 33_11kV","Substation Rating","MVA","Non-Coincident",58.47,58.47,58.47,58.47,58.47,58.47,58.47]
[null,null,null,null,"Coincident",58.47,58.47,58.47,58.47,58.47,58.47,58.47]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-3.7080000000000002,-4.0529999999999999,-4.2830000000000004,-4.4509999999999996,-4.633,-4.8040000000000003,-4.9690000000000003]
[null,null,null,null,"Coincident",-3.145,-4.1580000000000004,-4.7779999999999996,-5.141,-5.4749999999999996,-5.81,-6.14]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.36,52.79,53.05,53.08,53.08,53.02,52.9]
[null,null,null,null,"Coincident",47.57,47.95,48.19,48.21,48.22,48.16,48.05]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.13,54.57,54.84,54.86,54.87,54.8,54.68]
[null,null,null,null,"Coincident",49.17,49.57,49.81,49.84,49.84,49.78,49.67]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.05,45.43,45.66,45.69,45.69,45.63,45.51]
[null,null,null,null,"Coincident",40.93,41.26,41.48,41.5,41.5,41.44,41.34]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.57,46.96,47.2,47.23,47.23,47.16,47.04]
[null,null,null,null,"Coincident",42.3,42.65,42.87,42.9,42.9,42.84,42.73]
[null,"St Peters 132_11kV","Substation Rating","MVA","Non-Coincident",88.63,88.63,88.63,88.63,88.63,88.63,88.63]
[null,null,null,null,"Coincident",88.63,88.63,88.63,88.63,88.63,88.63,88.63]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.04,-7.9000000000000001E-2,-0.13700000000000001,-0.22800000000000001,-0.34899999999999998,-0.45900000000000002,-0.55600000000000005]
[null,null,null,null,"Coincident",-2.95,-3.8079999999999998,-4.4560000000000004,-5.0179999999999998,-5.6749999999999998,-6.3310000000000004,-6.9749999999999996]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.54,59.91,60.59,60.58,61.31,61.95,62.67]
[null,null,null,null,"Coincident",60.46,60.62,60.23,60.11,59.85,59.72,59.4]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.67,60.05,60.73,60.72,61.45,62.1,62.82]
[null,null,null,null,"Coincident",61.33,61.49,61.1,60.98,60.71,60.58,60.26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",56.59,59.83,61.11,61.4,62.14,62.78,63.5]
[null,null,null,null,"Coincident",56.49,56.72,56.37,56.26,55.99,55.87,55.55]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.72,59.97,61.25,61.55,62.28,62.92,63.65]
[null,null,null,null,"Coincident",57.3,57.54,57.19,57.07,56.8,56.67,56.35]
[null,"Stockton 33_11kV","Substation Rating","MVA","Non-Coincident",16.3,16.3,16.3,16.3,16.3,16.3,16.3]
[null,null,null,null,"Coincident",16.3,16.3,16.3,16.3,16.3,16.3,16.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.184,-0.313,-0.23899999999999999,-0.27200000000000002,-0.307,-0.34,-0.372]
[null,null,null,null,"Coincident",-0.59599999999999997,-0.78800000000000003,-0.90700000000000003,-0.97799999999999998,-1.044,-1.1100000000000001,-1.1759999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.01,10.17,10.19,10.17,10.19,10.16,10.1]
[null,null,null,null,"Coincident",9.0670000000000002,9.2129999999999992,9.2260000000000009,9.2129999999999992,9.23,9.1980000000000004,9.1509999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.11,10.27,10.29,10.27,10.29,10.26,10.199999999999999]
[null,null,null,null,"Coincident",9.157,9.3049999999999997,9.3179999999999996,9.3040000000000003,9.3219999999999992,9.2889999999999997,9.2420000000000009]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.2910000000000004,8.4390000000000001,8.4480000000000004,8.4329999999999998,8.4510000000000005,8.4160000000000004,8.3650000000000002]
[null,null,null,null,"Coincident",7.5090000000000003,7.6440000000000001,7.6509999999999998,7.6369999999999996,7.6539999999999999,7.6219999999999999,7.5759999999999996]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.3729999999999993,8.5229999999999997,8.532,8.516,8.5350000000000001,8.5,8.4480000000000004]
[null,null,null,null,"Coincident",7.5839999999999996,7.72,7.7270000000000003,7.7130000000000001,7.7309999999999999,7.6980000000000004,7.6509999999999998]
[null,"Strathfield South 132_11kV","Substation Rating","MVA","Non-Coincident",67.5,67.5,67.5,67.5,67.5,67.5,67.5]
[null,null,null,null,"Coincident",67.260000000000005,67.260000000000005,67.260000000000005,67.260000000000005,67.260000000000005,67.260000000000005,67.260000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5999999999999999E-2,-5.2999999999999999E-2,-8.3000000000000004E-2,-0.125,-0.18099999999999999,-0.23300000000000001,-0.27900000000000003]
[null,null,null,null,"Coincident",-3.5409999999999999,-3.5409999999999999,-3.5409999999999999,-3.5409999999999999,-3.5409999999999999,-3.5409999999999999,-3.5409999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.93,31.46,31.83,32.369999999999997,32.97,33.54,34.159999999999997]
[null,null,null,null,"Coincident",5.8239999999999998,5.9729999999999999,6.0640000000000001,6.1609999999999996,6.25,6.3330000000000002,6.4139999999999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.33,31.86,32.229999999999997,32.770000000000003,33.369999999999997,33.94,34.56]
[null,null,null,null,"Coincident",6.1479999999999997,6.3090000000000002,6.407,6.5140000000000002,6.6130000000000004,6.7039999999999997,6.7939999999999996]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.7,30.43,30.94,31.55,32.15,32.72,33.340000000000003]
[null,null,null,null,"Coincident",5.2439999999999998,5.3860000000000001,5.4720000000000004,5.57,5.6589999999999998,5.742,5.8230000000000004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.09,30.81,31.33,31.93,32.53,33.11,33.72]
[null,null,null,null,"Coincident",5.5380000000000003,5.69,5.7839999999999998,5.891,5.99,6.0819999999999999,6.1710000000000003]
[null,"Summer Hill 33_11kV","Substation Rating","MVA","Non-Coincident",76,76,76,76,76,76,76]
[null,null,null,null,"Coincident",null,76,76,76,76,76,76]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident",null,"Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0999999999999999E-2,55.38,56.29,57.42,58.4,59.32,60.26]
[null,null,null,null,"Coincident",47.8,48.81,49.69,50.68,51.73,52.56,53.47]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2999999999999999E-2,56.72,57.68,58.89,59.95,60.95,61.96]
[null,null,null,null,"Coincident",48.89,49.94,50.87,51.93,53.07,53.97,54.96]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0999999999999999E-2,52.75,53.53,54.59,55.57,56.49,57.43]
[null,null,null,null,"Coincident",43.15,44.1,44.94,45.93,46.98,47.82,48.73]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2999999999999999E-2,54.02,54.84,55.98,57.05,58.04,59.06]
[null,null,null,null,"Coincident",44.13,45.12,46.01,47.08,48.22,49.12,50.11]
[null,"Surry Hills 33_11kV","Substation Rating","MVA","Non-Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,null,null,"Coincident",0.02,0.02,0.02,0.02,0.02,0.02,0.02]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.55500000000000005,-0.92,-1.262,-1.641,-2.149,-2.629,-3.1030000000000002]
[null,null,null,null,"Coincident",-0.874,-1.109,-1.3220000000000001,-1.55,-1.84,-2.129,-2.4129999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.07,49.54,49.32,49.7,50.27,50.76,51.68]
[null,null,null,null,"Coincident",44.55,44.08,43.88,44.22,44.73,45.16,45.98]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.16,51.61,51.37,51.77,52.36,52.87,53.84]
[null,null,null,null,"Coincident",46.41,45.92,45.71,46.06,46.59,47.04,47.9]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.8,48.3,48.09,48.47,49.04,49.53,50.46]
[null,null,null,null,"Coincident",43.42,42.98,42.79,43.13,43.63,44.07,44.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",50.81,50.29,50.07,50.47,51.06,51.57,52.53]
[null,null,null,null,"Coincident",45.21,44.75,44.55,44.91,45.43,45.88,46.74]
[null,"Swansea 33_11kV","Substation Rating","MVA","Non-Coincident",16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002]
[null,null,null,null,"Coincident",16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002,16.420000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.3E-2,-4.5999999999999999E-2,-6.9000000000000006E-2,-9.9000000000000005E-2,-0.13700000000000001,-0.17299999999999999,-0.20499999999999999]
[null,null,null,null,"Coincident",-1.3129999999999999,-1.716,-1.9650000000000001,-2.1150000000000002,-2.2570000000000001,-2.399,-2.5390000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.29,14.64,14.9,15.04,15.04,14.98,14.92]
[null,null,null,null,"Coincident",14.7,14.73,14.72,14.69,14.63,14.59,14.48]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.3,14.65,14.91,15.05,15.05,15,14.93]
[null,null,null,null,"Coincident",14.83,14.86,14.85,14.81,14.76,14.72,14.6]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.38,13.71,13.94,14.08,14.08,14.02,13.96]
[null,null,null,null,"Coincident",12.36,12.38,12.36,12.33,12.28,12.24,12.12]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.38,13.72,13.95,14.09,14.09,14.03,13.97]
[null,null,null,null,"Coincident",12.46,12.49,12.47,12.44,12.39,12.35,12.23]
[null,"Tanilba Bay 33_11kV","Substation Rating","MVA","Non-Coincident",18.73,18.73,18.73,18.73,18.73,18.73,18.73]
[null,null,null,null,"Coincident",18.73,18.73,18.73,18.73,18.73,18.73,18.73]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.23100000000000001,-0.41599999999999998,-0.53400000000000003,-0.61199999999999999,-0.53,-0.59,-0.64800000000000002]
[null,null,null,null,"Coincident",-1.038,-1.3580000000000001,-1.552,-1.6639999999999999,-1.766,-1.867,-1.9670000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.72,11.69,11.74,12,12.19,12.4,12.49]
[null,null,null,null,"Coincident",10.17,10.14,10.18,10.41,10.57,10.75,10.83]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.91,11.88,11.93,12.2,12.39,12.6,12.69]
[null,null,null,null,"Coincident",10.33,10.3,10.35,10.58,10.74,10.92,11.01]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.62,10.58,10.63,10.9,11.08,11.29,11.38]
[null,null,null,null,"Coincident",9.2110000000000003,9.1780000000000008,9.2210000000000001,9.4489999999999998,9.6120000000000001,9.7899999999999991,9.8710000000000004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.8,10.76,10.81,11.08,11.27,11.47,11.57]
[null,null,null,null,"Coincident",9.3610000000000007,9.3279999999999994,9.3729999999999993,9.6039999999999992,9.7690000000000001,9.9499999999999993,10.029999999999999]
[null,"Tarro 33_11kV","Substation Rating","MVA","Non-Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,null,null,"Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.0579999999999998,-2.1840000000000002,-2.327,-2.3380000000000001,-2.41,-2.4769999999999999,-2.633]
[null,null,null,null,"Coincident",-0.97799999999999998,-1.278,-1.468,-1.589,-1.708,-1.827,-1.944]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.62,21.23,21.72,22.79,24.36,26.49,27.05]
[null,null,null,null,"Coincident",18.36,18.91,19.350000000000001,20.3,21.69,23.6,24.09]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.61,22.26,22.77,23.89,25.53,27.77,28.36]
[null,null,null,null,"Coincident",19.25,19.82,20.28,21.28,22.74,24.73,25.26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.8,19.440000000000001,19.940000000000001,21.01,22.58,24.71,25.27]
[null,null,null,null,"Coincident",16.739999999999998,17.309999999999999,17.760000000000002,18.71,20.11,22.01,22.51]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.7,20.38,20.9,22.02,23.67,25.91,26.49]
[null,null,null,null,"Coincident",17.55,18.149999999999999,18.62,19.62,21.08,23.07,23.59]
[null,"Telarah 33_11kV","Substation Rating","MVA","Non-Coincident",15.24,15.24,15.24,15.24,15.24,15.24,15.24]
[null,null,null,null,"Coincident",15.24,15.24,15.24,15.24,15.24,15.24,15.24]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.22,-0.33500000000000002,-0.40899999999999997,-0.46100000000000002,-0.51500000000000001,-0.56599999999999995,-0.61499999999999999]
[null,null,null,null,"Coincident",-1.0389999999999999,-1.3640000000000001,-1.5580000000000001,-1.667,-1.762,-1.8580000000000001,-1.952]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.510000000000002,17.670000000000002,17.760000000000002,18.350000000000001,18.329999999999998,18.3,18.25]
[null,null,null,null,"Coincident",14.07,14.2,14.27,14.75,14.73,14.71,14.67]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.64,17.8,17.899999999999999,18.489999999999998,18.47,18.45,18.39]
[null,null,null,null,"Coincident",14.18,14.31,14.38,14.86,14.85,14.83,14.78]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.73,15.87,15.95,16.54,16.52,16.489999999999998,16.440000000000001]
[null,null,null,null,"Coincident",12.64,12.75,12.82,13.29,13.28,13.25,13.21]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.85,15.99,16.07,16.670000000000002,16.649999999999999,16.62,16.57]
[null,null,null,null,"Coincident",12.74,12.85,12.92,13.4,13.38,13.36,13.32]
[null,"Terrey Hills 33_11kV","Substation Rating","MVA","Non-Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,null,null,"Coincident",23.82,23.82,23.82,23.82,23.82,23.82,23.82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.0029999999999999,-1.1619999999999999,-1.3080000000000001,-1.4370000000000001,-1.5860000000000001,-1.7270000000000001,-1.8640000000000001]
[null,null,null,null,"Coincident",-0.55900000000000005,-0.71599999999999997,-0.83299999999999996,-0.93300000000000005,-1.048,-1.1619999999999999,-1.274]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.36,16.27,16.260000000000002,16.32,16.399999999999999,16.420000000000002,16.46]
[null,null,null,null,"Coincident",14.73,14.65,14.64,14.7,14.77,14.78,14.82]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.41,17.309999999999999,17.29,17.37,17.45,17.47,17.510000000000002]
[null,null,null,null,"Coincident",15.67,15.59,15.57,15.64,15.71,15.73,15.77]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.61,14.54,14.53,14.6,14.68,14.69,14.73]
[null,null,null,null,"Coincident",13.16,13.09,13.08,13.14,13.21,13.23,13.27]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.55,15.47,15.46,15.53,15.61,15.63,15.67]
[null,null,null,null,"Coincident",14,13.92,13.92,13.98,14.06,14.07,14.11]
[null,"Thornton 33_11kV","Substation Rating","MVA","Non-Coincident",61.01,61.01,61.01,61.01,61.01,61.01,61.01]
[null,null,null,null,"Coincident",61.01,61.01,61.01,61.01,61.01,61.01,61.01]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.38100000000000001,-0.62,-1.034,-0.90200000000000002,-1.032,-1.155,-1.667]
[null,null,null,null,"Coincident",-2.3220000000000001,-3.0270000000000001,-3.464,-3.7280000000000002,-3.9769999999999999,-4.226,-4.4710000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.31,41.89,43.4,45.26,48.01,51.5,52.74]
[null,null,null,null,"Coincident",37.72,38.25,39.619999999999997,41.33,43.83,47.02,48.15]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.35,41.94,43.47,45.38,48.18,51.77,53.05]
[null,null,null,null,"Coincident",37.76,38.299999999999997,39.69,41.43,43.99,47.26,48.43]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.39,37.99,39.51,41.37,44.11,47.6,48.84]
[null,null,null,null,"Coincident",34.130000000000003,34.69,36.07,37.770000000000003,40.28,43.46,44.59]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.39,38,39.53,41.42,44.21,47.78,49.05]
[null,null,null,null,"Coincident",34.14,34.700000000000003,36.090000000000003,37.82,40.369999999999997,43.62,44.79]
[null,"Tighes Hill 33_11kV","Substation Rating","MVA","Non-Coincident",38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003]
[null,null,null,null,"Coincident",38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003,38.520000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.7000000000000001E-2,-3.5000000000000003E-2,-5.5E-2,-8.5000000000000006E-2,-0.124,-0.16,-0.192]
[null,null,null,null,"Coincident",-1.1850000000000001,-1.5469999999999999,-1.8,-1.9950000000000001,-2.2080000000000002,-2.42,-2.629]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.96,30.04,30.87,31.13,31.18,31.2,31.34]
[null,null,null,null,"Coincident",21.52,21.55,21.39,21.2,20.98,20.82,20.66]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.8,30.89,31.75,32.01,32.06,32.08,32.229999999999997]
[null,null,null,null,"Coincident",21.97,22,21.84,21.64,21.42,21.26,21.09]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.14,28.19,29,29.24,29.3,29.32,29.46]
[null,null,null,null,"Coincident",19.71,19.739999999999998,19.579999999999998,19.39,19.170000000000002,19.010000000000002,18.850000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.92,28.98,29.81,30.06,30.12,30.14,30.28]
[null,null,null,null,"Coincident",20.13,20.16,20,19.8,19.57,19.41,19.25]
[null,"Tomago 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.63800000000000001,-0.61399999999999999,-0.623,-0.63100000000000001,-0.64200000000000002,-0.65200000000000002,-0.66100000000000003]
[null,null,null,null,"Coincident",-0.2,-0.25600000000000001,-0.30399999999999999,-0.35399999999999998,-0.41599999999999998,-0.47799999999999998,-0.53900000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.92,12.14,12.61,12.69,12.84,12.98,13.16]
[null,null,null,null,"Coincident",5.835,5.95,6.0170000000000003,6.077,6.1529999999999996,6.2190000000000003,6.2949999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.43,12.7,13.2,13.28,13.44,13.58,13.77]
[null,null,null,null,"Coincident",6.1950000000000003,6.3159999999999998,6.3869999999999996,6.4509999999999996,6.532,6.6020000000000003,6.6829999999999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.48,11.75,12.25,12.35,12.49,12.63,12.82]
[null,null,null,null,"Coincident",5.6,5.7190000000000003,5.7880000000000003,5.8479999999999999,5.9249999999999998,5.9909999999999997,6.0670000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.97,12.29,12.82,12.92,13.07,13.22,13.41]
[null,null,null,null,"Coincident",5.9450000000000003,6.0709999999999997,6.1449999999999996,6.2080000000000002,6.2889999999999997,6.359,6.44]
[null,"Tomalpin 33_11kV","Substation Rating","MVA","Non-Coincident",22.16,22.16,22.16,22.16,22.16,22.16,22.16]
[null,null,null,null,"Coincident",20.77,20.77,20.77,20.77,20.77,20.77,20.77]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",-4.0000000000000001E-3,-5.0000000000000001E-3,-6.0000000000000001E-3,-7.0000000000000001E-3,-8.0000000000000002E-3,-8.9999999999999993E-3,-0.01]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8560000000000001,1.8560000000000001,1.8560000000000001,1.8560000000000001,1.857,1.857,1.857]
[null,null,null,null,"Coincident",0.502,0.502,0.502,0.502,0.502,0.501,0.501]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.87,1.87,1.87,1.87,1.871,1.871,1.871]
[null,null,null,null,"Coincident",0.504,0.504,0.504,0.504,0.504,0.503,0.503]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.528,1.528,1.528,1.528,1.5289999999999999,1.5289999999999999,1.5289999999999999]
[null,null,null,null,"Coincident",0.502,0.502,0.502,0.502,0.502,0.501,0.501]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5389999999999999,1.5389999999999999,1.5389999999999999,1.5389999999999999,1.54,1.54,1.54]
[null,null,null,null,"Coincident",0.504,0.504,0.504,0.504,0.504,0.503,0.503]
[null,"Tomaree 33_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1999999999999999E-2,-4.3999999999999997E-2,-6.8000000000000005E-2,-0.10199999999999999,-0.14599999999999999,-0.188,-0.22]
[null,null,null,null,"Coincident",-1.2569999999999999,-1.631,-1.879,-2.0499999999999998,-2.2280000000000002,-2.407,-2.5830000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.93,19.52,19.97,20.18,20.16,20.11,20.059999999999999]
[null,null,null,null,"Coincident",14.79,14.73,14.71,14.67,14.63,14.54,14.44]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.010000000000002,19.59,20.04,20.25,20.239999999999998,20.18,20.13]
[null,null,null,null,"Coincident",14.95,14.89,14.87,14.83,14.79,14.7,14.59]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.13,17.66,18.079999999999998,18.27,18.260000000000002,18.2,18.149999999999999]
[null,null,null,null,"Coincident",12.42,12.37,12.35,12.32,12.28,12.18,12.08]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.190000000000001,17.73,18.149999999999999,18.34,18.329999999999998,18.27,18.22]
[null,null,null,null,"Coincident",12.56,12.5,12.49,12.45,12.41,12.32,12.21]
[null,"Top Ryde 132_11kV","Substation Rating","MVA","Non-Coincident",61.25,61.25,61.25,61.25,61.25,61.25,61.25]
[null,null,null,null,"Coincident",61.25,61.25,61.25,61.25,61.25,61.25,61.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.8320000000000001,-2.4660000000000002,-2.923,-3.2890000000000001,-3.7130000000000001,-4.1139999999999999,-4.5060000000000002]
[null,null,null,null,"Coincident",-2.5289999999999999,-3.2879999999999998,-3.8079999999999998,-4.1959999999999997,-4.6180000000000003,-5.0410000000000004,-5.4550000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",62.62,62.12,61.9,62.1,62.23,62.47,62.45]
[null,null,null,null,"Coincident",59.47,59,58.78,58.98,59.1,59.33,59.31]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",63.2,62.71,62.48,62.68,62.82,63.05,63.04]
[null,null,null,null,"Coincident",60.02,59.55,59.33,59.53,59.66,59.88,59.87]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",55.41,54.99,54.81,55.01,55.14,55.38,55.36]
[null,null,null,null,"Coincident",52.62,52.23,52.05,52.24,52.37,52.59,52.58]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",55.93,55.52,55.32,55.53,55.66,55.9,55.89]
[null,null,null,null,"Coincident",53.12,52.72,52.54,52.74,52.86,53.09,53.08]
[null,"Toronto West 132_11kV","Substation Rating","MVA","Non-Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,null,null,"Coincident",38.11,38.11,38.11,38.11,38.11,38.11,38.11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.46800000000000003,-0.64100000000000001,-0.76,-0.84899999999999998,-0.94899999999999995,-1.042,-1.1319999999999999]
[null,null,null,null,"Coincident",-1.4930000000000001,-1.9450000000000001,-2.23,-2.41,-2.5840000000000001,-2.758,-2.93]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.9,27.13,27.3,27.29,27.24,27.18,27.08]
[null,null,null,null,"Coincident",25.46,25.68,25.84,25.84,25.79,25.73,25.63]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.29,27.52,27.69,27.69,27.64,27.57,27.47]
[null,null,null,null,"Coincident",25.83,26.05,26.22,26.21,26.16,26.1,26]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.54,23.74,23.89,23.89,23.84,23.78,23.67]
[null,null,null,null,"Coincident",22.29,22.48,22.62,22.62,22.57,22.51,22.41]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.89,24.09,24.24,24.24,24.19,24.12,24.02]
[null,null,null,null,"Coincident",22.61,22.8,22.95,22.95,22.9,22.84,22.74]
[null,"Turramurra 33_11kV","Substation Rating","MVA","Non-Coincident",42.3,42.3,42.3,42.3,42.3,42.3,42.3]
[null,null,null,null,"Coincident",42.3,42.3,42.3,42.3,42.3,42.3,42.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.573,-2.9319999999999999,-3.1709999999999998,-3.3410000000000002,-3.5230000000000001,-3.6960000000000002,-3.8639999999999999]
[null,null,null,null,"Coincident",-2.3690000000000002,-3.1339999999999999,-3.6139999999999999,-3.911,-4.1970000000000001,-4.484,-4.7670000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.72,45.36,45.7,45.85,46.06,46.05,46.05]
[null,null,null,null,"Coincident",41.65,42.24,42.57,42.71,42.9,42.89,42.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.13,45.77,46.12,46.27,46.48,46.46,46.47]
[null,null,null,null,"Coincident",42.03,42.63,42.95,43.09,43.29,43.27,43.28]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.380000000000003,40,40.340000000000003,40.49,40.700000000000003,40.68,40.68]
[null,null,null,null,"Coincident",36.68,37.25,37.57,37.71,37.9,37.89,37.89]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.74,40.36,40.700000000000003,40.85,41.06,41.05,41.05]
[null,null,null,null,"Coincident",37.01,37.590000000000003,37.909999999999997,38.049999999999997,38.25,38.229999999999997,38.24]
[null,"Umina 66_11kV","Substation Rating","MVA","Non-Coincident",37.86,37.86,37.86,37.86,37.86,37.86,37.86]
[null,null,null,null,"Coincident",35.700000000000003,35.700000000000003,35.700000000000003,35.700000000000003,35.700000000000003,35.700000000000003,35.700000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-4.8000000000000001E-2,-9.6000000000000002E-2,-0.14499999999999999,-0.20699999999999999,-0.28899999999999998,-0.36499999999999999,-0.433]
[null,null,null,null,"Coincident",-2.62,-3.4350000000000001,-3.944,-4.2539999999999996,-4.5510000000000002,-4.8479999999999999,-5.1420000000000003]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.57,30.29,30.69,30.85,30.89,30.85,30.79]
[null,null,null,null,"Coincident",30.92,30.9,30.86,30.8,30.69,30.53,30.34]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.15,30.88,31.28,31.45,31.49,31.45,31.39]
[null,null,null,null,"Coincident",32.56,32.53,32.49,32.43,32.31,32.15,31.95]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.98,28.77,29.22,29.41,29.44,29.4,29.35]
[null,null,null,null,"Coincident",27.31,27.3,27.26,27.2,27.09,26.94,26.75]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.52,29.33,29.78,29.98,30.01,29.97,29.92]
[null,null,null,null,"Coincident",28.76,28.74,28.7,28.64,28.53,28.36,28.16]
[null,"Vales Point 33_11kV","Substation Rating","MVA","Non-Coincident",15.24,15.24,15.24,15.24,15.24,15.24,15.24]
[null,null,null,null,"Coincident",15.24,15.24,15.24,15.24,15.24,15.24,15.24]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.5620000000000003,7.5620000000000003,7.5620000000000003,7.5629999999999997,7.5629999999999997,7.5629999999999997,7.5629999999999997]
[null,null,null,null,"Coincident",4.8559999999999999,4.8559999999999999,4.8559999999999999,4.8559999999999999,4.8570000000000002,4.8570000000000002,4.8570000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.4019999999999992,8.4019999999999992,8.4030000000000005,8.4030000000000005,8.4030000000000005,8.4030000000000005,8.4030000000000005]
[null,null,null,null,"Coincident",5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5620000000000003,7.5620000000000003,7.5620000000000003,7.5629999999999997,7.5629999999999997,7.5629999999999997,7.5629999999999997]
[null,null,null,null,"Coincident",4.8559999999999999,4.8559999999999999,4.8559999999999999,4.8559999999999999,4.8570000000000002,4.8570000000000002,4.8570000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.4019999999999992,8.4019999999999992,8.4030000000000005,8.4030000000000005,8.4030000000000005,8.4030000000000005,8.4030000000000005]
[null,null,null,null,"Coincident",5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999,5.3959999999999999]
[null,"Wamberal 132_11kV","Substation Rating","MVA","Non-Coincident",36.869999999999997,36.869999999999997,36.869999999999997,36.869999999999997,36.869999999999997,36.869999999999997,36.869999999999997]
[null,null,null,null,"Coincident",34.39,34.39,34.39,34.39,34.39,34.39,34.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.5000000000000001E-2,-0.05,-7.2999999999999995E-2,-0.10100000000000001,-0.13700000000000001,-0.17100000000000001,-0.20200000000000001]
[null,null,null,null,"Coincident",-1.2450000000000001,-1.635,-1.8720000000000001,-2.0070000000000001,-2.1280000000000001,-2.2490000000000001,-2.3690000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.45,16.670000000000002,16.86,17.010000000000002,17.04,17.04,17.04]
[null,null,null,null,"Coincident",14.33,14.72,14.88,14.91,14.91,14.91,14.89]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.47,16.7,16.89,17.04,17.07,17.059999999999999,17.07]
[null,null,null,null,"Coincident",14.46,14.86,15.02,15.05,15.05,15.04,15.03]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.56,15.77,15.95,16.100000000000001,16.13,16.12,16.12]
[null,null,null,null,"Coincident",12.55,12.9,13.05,13.08,13.08,13.07,13.05]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.58,15.8,15.98,16.12,16.149999999999999,16.149999999999999,16.149999999999999]
[null,null,null,null,"Coincident",12.66,13.02,13.17,13.2,13.2,13.19,13.18]
[null,"Waverley 132_11kV","Substation Rating","MVA","Non-Coincident",65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005]
[null,null,null,null,"Coincident",61.79,61.79,61.79,61.79,61.79,61.79,61.79]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1000000000000001E-2,-5.6000000000000001E-2,-0.105,-0.187,-0.29899999999999999,-0.40300000000000002,-0.49399999999999999]
[null,null,null,null,"Coincident",-2.0379999999999998,-2.6139999999999999,-3.081,-3.5190000000000001,-4.056,-4.593,-5.1219999999999999]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.83,48.43,48.09,47.74,47.59,47.41,47.06]
[null,null,null,null,"Coincident",31.86,31.7,31.41,31.23,31.68,31.45,31.12]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.89,48.48,48.15,47.79,47.65,47.46,47.12]
[null,null,null,null,"Coincident",31.93,31.77,31.48,31.31,31.76,31.52,31.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.23,45.74,45.35,44.97,44.82,44.64,44.29]
[null,null,null,null,"Coincident",29.66,29.54,29.26,29.09,29.54,29.3,28.97]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.28,45.79,45.4,45.02,44.87,44.69,44.34]
[null,null,null,null,"Coincident",29.73,29.61,29.33,29.16,29.61,29.37,29.04]
[null,"West Gosford 132_11kV","Substation Rating","MVA","Non-Coincident",65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005]
[null,null,null,null,"Coincident",65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005,65.010000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.4510000000000001,-3.4249999999999998,-4.0170000000000003,-4.5999999999999996,-5.2880000000000003,-3.5470000000000002,-3.8420000000000001]
[null,null,null,null,"Coincident",-2.7770000000000001,-3.5710000000000002,-4.1349999999999998,-4.5839999999999996,-5.085,-5.585,-6.0759999999999996]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.15,58.09,58.18,58.11,60.66,60.9,60.95]
[null,null,null,null,"Coincident",55.71,56.62,56.71,56.64,59.13,59.36,59.42]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.15,58.09,58.18,58.11,60.67,60.91,60.96]
[null,null,null,null,"Coincident",55.71,56.62,56.72,56.64,59.14,59.37,59.42]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.46,52.44,52.56,52.48,55.04,55.28,55.33]
[null,null,null,null,"Coincident",50.16,51.12,51.23,51.16,53.65,53.88,53.94]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.52,52.51,52.63,52.55,55.04,55.28,55.33]
[null,null,null,null,"Coincident",50.22,51.18,51.3,51.22,53.65,53.89,53.94]
[null,"Williamtown 33_11kV","Substation Rating","MVA","Non-Coincident",25.64,25.64,25.64,25.64,25.64,25.64,25.64]
[null,null,null,null,"Coincident",25.64,25.64,25.64,25.64,25.64,25.64,25.64]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-0.38600000000000001,-0.46300000000000002,-0.51500000000000001,-0.55400000000000005,-0.59599999999999997,-0.63500000000000001,-0.67400000000000004]
[null,null,null,null,"Coincident",-0.307,-0.40100000000000002,-0.46300000000000002,-0.50600000000000001,-0.55000000000000004,-0.59399999999999997,-0.63700000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.5460000000000003,6.63,6.7450000000000001,6.76,6.7690000000000001,6.7709999999999999,6.7560000000000002]
[null,null,null,null,"Coincident",6.0949999999999998,6.1740000000000004,6.28,6.2939999999999996,6.3029999999999999,6.3040000000000003,6.29]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.64,6.7249999999999996,6.8410000000000002,6.8570000000000002,6.8659999999999997,6.867,6.8520000000000003]
[null,null,null,null,"Coincident",6.1820000000000004,6.2619999999999996,6.37,6.3840000000000003,6.3929999999999998,6.3940000000000001,6.38]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.8029999999999999,5.8890000000000002,6.0049999999999999,6.02,6.0289999999999999,6.03,6.0149999999999997]
[null,null,null,null,"Coincident",5.4029999999999996,5.4829999999999997,5.5910000000000002,5.6050000000000004,5.6130000000000004,5.6150000000000002,5.601]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8860000000000001,5.9729999999999999,6.09,6.1059999999999999,6.1150000000000002,6.1159999999999997,6.101]
[null,null,null,null,"Coincident",5.48,5.5620000000000003,5.6710000000000003,5.6849999999999996,5.6929999999999996,5.6950000000000003,5.681]
[null,"Woy Woy 66_11kV","Substation Rating","MVA","Non-Coincident",32.659999999999997,32.659999999999997,32.659999999999997,32.659999999999997,32.659999999999997,32.659999999999997,32.659999999999997]
[null,null,null,null,"Coincident",30.75,30.75,30.75,30.75,30.75,30.75,30.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.8000000000000001E-2,-5.7000000000000002E-2,-8.5999999999999993E-2,-0.126,-0.17799999999999999,-0.22600000000000001,-0.26800000000000002]
[null,null,null,null,"Coincident",-1.58,-2.0590000000000002,-2.3690000000000002,-2.5720000000000001,-2.7759999999999998,-2.9809999999999999,-3.1829999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.329999999999998,20.68,20.97,21.18,21.23,21.24,21.27]
[null,null,null,null,"Coincident",22.03,22.15,22.23,22.23,22.19,22.14,22.06]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.94,21.29,21.59,21.8,21.86,21.87,21.9]
[null,null,null,null,"Coincident",23.17,23.3,23.39,23.38,23.34,23.29,23.2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.239999999999998,19.54,19.809999999999999,20,20.059999999999999,20.07,20.100000000000001]
[null,null,null,null,"Coincident",19.510000000000002,19.61,19.68,19.670000000000002,19.63,19.579999999999998,19.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.809999999999999,20.12,20.39,20.6,20.66,20.66,20.7]
[null,null,null,null,"Coincident",20.52,20.62,20.7,20.69,20.65,20.6,20.51]
[null,"Wyong 132_11kV","Substation Rating","MVA","Non-Coincident",54.01,54.01,54.01,54.01,54.01,54.01,54.01]
[null,null,null,null,"Coincident",54.01,54.01,54.01,54.01,54.01,54.01,54.01]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-1.4790000000000001,-1.673,-1.8839999999999999,-2.0449999999999999,-2.222,-2.3879999999999999,-2.5470000000000002]
[null,null,null,null,"Coincident",-2.9470000000000001,-3.8570000000000002,-4.4290000000000003,-4.7859999999999996,-5.13,-5.4749999999999996,-5.8129999999999997]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.81,49.07,50,51.55,52.85,53.05,53.24]
[null,null,null,null,"Coincident",47.83,48.08,49,50.52,51.79,51.98,52.17]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",49.47,49.74,50.68,52.26,53.57,53.77,53.97]
[null,null,null,null,"Coincident",48.48,48.74,49.67,51.21,52.5,52.69,52.88]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.13,43.4,44.34,45.89,47.19,47.38,47.58]
[null,null,null,null,"Coincident",42.26,42.53,43.45,44.97,46.24,46.43,46.62]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.71,43.99,44.94,46.52,47.83,48.03,48.23]
[null,null,null,null,"Coincident",42.84,43.11,44.04,45.58,46.87,47.07,47.26]
[null,"Zetland 132_11kV","Substation Rating","MVA","Non-Coincident",90.31,90.31,90.31,90.31,90.31,90.31,90.31]
[null,null,null,null,"Coincident",83.6,83.6,83.6,83.6,83.6,83.6,83.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",-2.1999999999999999E-2,-4.2999999999999997E-2,-9.2999999999999999E-2,-0.185,-0.311,-0.42499999999999999,-0.54100000000000004]
[null,null,null,null,"Coincident",-2.0299999999999998,-2.5779999999999998,-3.097,-3.6720000000000002,-4.4169999999999998,-5.1630000000000003,-5.8929999999999998]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",64.62,70.959999999999994,74.510000000000005,74.8,75.53,76.150000000000006,76.92]
[null,null,null,null,"Coincident",73.94,75.290000000000006,75.69,75.33,74.97,74.849999999999994,74.53]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",64.680000000000007,70.97,74.56,74.849999999999994,75.53,76.150000000000006,76.92]
[null,null,null,null,"Coincident",73.959999999999994,75.31,75.709999999999994,75.34,74.989999999999995,74.87,74.540000000000006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",62.6,68.95,72.510000000000005,72.81,73.540000000000006,74.150000000000006,74.92]
[null,null,null,null,"Coincident",69.819999999999993,71.25,71.680000000000007,71.319999999999993,70.97,70.849999999999994,70.52]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.64,68.959999999999994,72.540000000000006,72.84,73.58,74.2,74.98]
[null,null,null,null,"Coincident",69.819999999999993,71.25,71.69,71.33,70.97,70.849999999999994,70.53]
[null,"Wyong 132_11kV","Substation Rating","MVA","Non-Coincident",54.01,54.01,54.01,54.01,54.01,54.01,54.01]
[null,null,null,null,"Coincident",54.01,54.01,54.01,54.01,54.01,54.01,54.01]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.23,48.81,49.07,50,51.55,52.85,53.05]
[null,null,null,null,"Coincident",45.17,47.69,47.95,48.86,50.37,51.65,51.83]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.86,49.47,49.74,50.68,52.26,53.57,53.77]
[null,null,null,null,"Coincident",45.79,48.34,48.6,49.53,51.06,52.35,52.54]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.53,43.13,43.4,44.34,45.89,47.19,47.38]
[null,null,null,null,"Coincident",39.61,42.14,42.41,43.33,44.84,46.11,46.3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.09,43.71,43.99,44.94,46.52,47.83,48.03]
[null,null,null,null,"Coincident",40.15,42.72,42.98,43.92,45.45,46.74,46.93]
[null,"Zetland 132_11kV","Substation Rating","MVA","Non-Coincident",83.6,83.6,83.6,83.6,83.6,83.6,83.6]
[null,null,null,null,"Coincident",83.6,83.6,83.6,83.6,83.6,83.6,83.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",70.34,78.290000000000006,79.72,80.14,79.760000000000005,79.38,79.260000000000005]
[null,null,null,null,"Coincident",67.48,75.11,76.48,76.88,76.510000000000005,76.150000000000006,76.03]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",70.38,78.31,79.739999999999995,80.16,79.78,79.400000000000006,79.27]
[null,null,null,null,"Coincident",67.52,75.12,76.489999999999995,76.900000000000006,76.53,76.17,76.05]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",65.84,73.930000000000007,75.44,75.900000000000006,75.52,75.150000000000006,75.02]
[null,null,null,null,"Coincident",63.16,70.92,72.37,72.81,72.45,72.09,71.97]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",65.849999999999994,73.930000000000007,75.44,75.900000000000006,75.52,75.150000000000006,75.02]
[null,null,null,null,"Coincident",63.17,70.92,72.37,72.819999999999993,72.45,72.09,71.97]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Alexandria 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Argenton 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bankstown 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beresfield 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bunnerong North 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Canterbury 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Eraring 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gosford 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gosford 132_66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Homebush 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kooragang 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kuring-gai 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kurnell 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kurri 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Macquarie 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Merewether 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mitchell Line 132_66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morisset 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Munmorah 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Munmorah 330_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Muswellbrook 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ourimbah 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ourimbah 132_66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Peakhurst 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Hacking 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pyrmont 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rozelle 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Singleton 132_66kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Strathfield 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Surry Hills 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sydney East 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tomago 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Waratah (Comsteel) 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Waratah (Domestic) 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Warringah 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Willoughby 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Aberdeen 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Adamstown 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Argenton 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Arncliffe 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Auburn 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Avoca 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Avondale 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Awaba 132_33kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Baerami 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Balgowlah North 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bankstown 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bass Hill 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beacon Hill 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Belmore Park 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Belrose 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Berkeley Vale 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Berowra 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Blackwattle Bay 33_5kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Blakehurst 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Botany 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brandy Hill 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Branxton 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Broadmeadow 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Broadmeadow 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brookvale 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Burwood 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Campbell St 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Camperdown 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Camperdown 33_5kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Campsie 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cardiff 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Careel Bay 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caringbah 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Carrington 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Castle Cove 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cessnock 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cessnock South 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Charlestown 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Charmhaven 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Chatswood 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"City Central 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"City East 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"City North 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"City South 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clovelly 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Concord 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cronulla 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Croudace Bay 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Crows Nest 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Crows Nest 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Croydon 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dalley St 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Darling Harbour 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Darlinghurst 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dee Why West 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Denman 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Double Bay 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Drummoyne 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Dulwich Hill 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Edgeworth 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Empire Bay 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Enfield 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Engadine 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Engadine 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Epping 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Erina 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Five Dock 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Flemington 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Galston 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gateshead 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gore Hill 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,"Green Square 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Greenacre 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Greenacre Park 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gwawley Bay 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gwawley Bay 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Harbord 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Homebush Bay 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hornsby 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hunters Hill 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hurstville North 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jannali 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jesmond 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jewells 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Killarney 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kingsford 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kirrawee 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kogarah 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kotara 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kurnell South 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kurri 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lake Munmorah 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Leichhardt 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Leichhardt 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Leightonfield 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lemington 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lidcombe 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lindfield 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lisarow 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Long Jetty 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,"Macquarie Park 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Maitland 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Manly 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Maroubra 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Marrickville 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Maryland 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mascot 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Matraville 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mayfield West 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Meadowbank 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Medowie 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Menai 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Merriwa 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Metford 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Milperra 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Miranda 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mitchell Line 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mitchells Flat 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mona Vale 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Moonan 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morisset 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mortdale 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mosman 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Hutton 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Thorley 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Muswellbrook 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Narrabeen 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nelson Bay 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"New Lambton 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Newcastle CBD 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Newdell 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Newport 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Noraville 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North Head 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North Sydney 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North Sydney 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nulkaba 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Olympic Park 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Paddington 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Paxton 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Peats Ridge 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pelican 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pennant Hills 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Port Botany 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Potts Hill 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Punchbowl 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pymble 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rathmines 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Raymond Terr NEW 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Revesby 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Riverwood 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"RNS Hospital 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rockdale 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rockdale 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rose Bay 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rothbury 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rouchel 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rutherford 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sans Souci 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Scone 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sefton 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Singleton 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Singleton North 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Somersby 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"St Ives 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"St Peters 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stockton 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Strathfield South 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Summer Hill 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Surry Hills 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Swansea 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tanilba Bay 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tarro 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Telarah 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Terrey Hills 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Thornton 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tighes Hill 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tomago 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tomalpin 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tomaree 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Top Ryde 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Toronto 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Toronto West 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Turramurra 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Umina 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Vales Point 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wamberal 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wamberal 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Waverley 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"West Gosford 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Williamtown 33_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woy Woy 66_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wyong 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Zetland 132_11kV",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.2 Reliability & Cust serv","index":23,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[[5,1,5,7],[16,1,16,3],[28,1,28,3],[70,4,70,8],[40,1,40,3],[52,1,52,3],[55,1,55,8],[67,1,67,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,13.218,13.218,13.218,13.218,13.218]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,67.018000000000001,67.018000000000001,67.018000000000001,67.018000000000001,67.018000000000001]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,133.309,133.309,133.309,133.309,133.309]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,729.02700000000004,729.02700000000004,729.02700000000004,729.02700000000004,729.02700000000004]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E12:E16)","v":942.57200000000012},{"$f":"SUM(F12:F16)","v":942.57200000000012},{"$f":"SUM(G12:G16)","v":942.57200000000012},{"$f":"SUM(H12:H16)","v":942.57200000000012},{"$f":"SUM(I12:I16)","v":942.57200000000012}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,4.2000000000000003E-2,4.2000000000000003E-2,4.2000000000000003E-2,4.2000000000000003E-2,4.2000000000000003E-2]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.59199999999999997,0.59199999999999997,0.59199999999999997,0.59199999999999997,0.59199999999999997]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,0.96799999999999997,0.96799999999999997,0.96799999999999997,0.96799999999999997,0.96799999999999997]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,1.9830000000000001,1.9830000000000001,1.9830000000000001,1.9830000000000001,1.9830000000000001]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E24:E28)","v":3.585},{"$f":"SUM(F24:F28)","v":3.585},{"$f":"SUM(G24:G28)","v":3.585},{"$f":"SUM(H24:H28)","v":3.585},{"$f":"SUM(I24:I28)","v":3.585}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E36:E40)","v":0},{"$f":"SUM(F36:F40)","v":0},{"$f":"SUM(G36:G40)","v":0},{"$f":"SUM(H36:H40)","v":0},{"$f":"SUM(I36:I40)","v":0}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E48:E52)","v":0},{"$f":"SUM(F48:F52)","v":0},{"$f":"SUM(G48:G52)","v":0},{"$f":"SUM(H48:H52)","v":0},{"$f":"SUM(I48:I52)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},31237,31415,31571,31743,31963,32232,32551]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1471587,1479995,1487301,1495419,1505791,1518459,1533484]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},287993,289639,291069,292658,294687,297167,300107]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},2455,2469,2482,2495,2512,2534,2559]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C61:C65)","v":1793272},1803518,1812423,1822315,1834953,1850392,1868701]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Number of calls received",null,null,127459,127459,127459,127459,127459]
[null,"Number of calls answered within 30 seconds",null,null,108340,108340,108340,108340,108340]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E74/E73),\"\")","v":0.84999882315097408},{"$f":"IFERROR((F74/F73),\"\")","v":0.84999882315097408},{"$f":"IFERROR((G74/G73),\"\")","v":0.84999882315097408},{"$f":"IFERROR((H74/H73),\"\")","v":0.84999882315097408},{"$f":"IFERROR((I74/I73),\"\")","v":0.84999882315097408}]

{"sheet":"7.1 Policies and Procedures","index":24,"n_rows":460,"n_cols":5,"rows_kept":460,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[null,"Governance framework"]
[null,"Board Policy - Group Governance Framework","This policy sets out the respective responsibilities of the Ausgrid Asset Partnership (AAP), the Ausgrid Operating Partnership (AOP), Ausgrid Finance Pty Ltd (Ausgrid Finance) and Ausgrid Management Pty Ltd (Ausgrid Management) and the approach to Board decision making. For the purposes of this policy each of AAP, AOP, Ausgrid Finance and Ausgrid Management are referred to as an entity. The Board of each entity has agreed to adopt the governance protocols set out in this document.  The policy is not intended to override any provisions of the Partnership Deeds, Constitutions or constituent documents of each entity.  If there is any inconsistency, the Partnership Deed, constitution or other constituent document prevails.","Opex","No"]
[null,"Board Charters","The company's boards have adopted Charters to guide the boards in the exercise of their responsibilities in the service of their shareholders, customers and other stakeholders. The principles set out in the Charters are in addition to and are not intended to change or interpret any Partnerships or laws for the application of the company's Constitution. The board will review this Charters at least annually and, if appropriate, revise this Charter from time to time. The Charter delineates the functions and responsibilities of the board and management.","Opex","No"]
[null,"Board - Remuneration and Nominations Committee Charter","The company's board has adopted a Charter for a Remuneration and Nominations Committee with the purpose to assist the Board of the Partnership in fulfilling its responsibilities with regard to executive remuneration, director appointments and succession planning.","Opex","No"]
[]
[null,"Board - Audit Committee Charter","The company's board has adopted a Charter for a Audit Committee with the purpose to discharge its responsibilities for oversight and review in relation to: - financial reporting including the integrity of financial reports; - accounting policies; - internal controls; - performance of the internal and external audit functions; and - tax risk management governance.","Opex","No"]
[null,"Board - Safety, Risk and Compliance Committee Charter","The company's board has adopted a Charter for a Safety, Risk and Compliance Committee with the purpose to provide leadership, guidance and discharge its responsibilities for oversight and review in relation to: - Work, Health and Safety (WHS) practices and strategy; - the risk management framework (including insurance programs);  - monitoring processes for compliance with laws, contracts and regulations applicable to the company's operations; and - compliance with the Code of Conduct.","Opex","No"]
[null,"Board Policy - Risk Management","This policy sets out the Ausgrid board's commitment and approach to embed and oversee an effective and integrated risk management framework that is supported by positive risk conduct in all that we do as a company.","Opex","No"]
[null,"Board Policy - Compliance","This policy sets out the Ausgrid's commitment and approach to embed and manage an effective compliance framework with regard to the legal, regulatory and industry requirements that affect the business","Opex","No"]
[null,"Board Policy - Group Delegation of Authority to the Chief Executive Officer","This Delegations Policy sets out the delegations framework and the delegated authority granted to the CEO by the Board of Ausgrid Management Pty Limited (the Board) to support effective decision making. Ausgrid Management Pty Limited (Ausgrid) provides agency services to both the Ausgrid Asset Partnership (AAP) and Ausgrid Operator Partnership (AOP) (collectively The Partnerships). These services are provided in accordance with the terms of the AAP and AOP Partnership Deeds and the Management Agreement. In accordance with the Management Agreement, AAP and AOP have issued directions to Ausgrid in relation to the Agency Services to be performed. Those directions authorise Ausgrid to exercise each and every function and all authority of the Partnerships that is necessary for the day-to-day management of the Partnership Business except for the matters expressly reserved for the decision of the Partnership Boards.","Opex","No"]
[null,"Board Policy - Interim Group Treasury","This policy provides an overview of the manner in which Ausgrid assesses treasury related risks and deploys appropriate measures to manage and mitigate those risks with the objectives of protecting Ausgrid's cash flows, profitability and reputation and maintaining a minimum long term, standalone credit rating.","Opex","No"]
[null,"AAP Board Policy - Tax Governance; Ausgrid Finance Board Policy - Tax Governance; AOP Board Policy - Tax Governance; Ausgrid Management Board Policy - Tax Governance","These policies is to set out the respective Board's commitment and approach to embed and oversee an effective and integrated Tax Governance Framework that supports all tax compliance and related activities and decisions.","Opex","No"]
[null,"Board Policy - Group External Auditor Independence","This document sets out the policy of the Ausgrid Group (the Group) in relation to the independence of the external auditor and the engagement of the external auditor for audit and non-audit services.","Opex","No"]
[null,"Board Policy - Committment to Health, Safety and Environment","Our Commitment: We will conduct our business in a way that: Minimises risks that our assets, operations and activities pose to the health and safety (both physical and mental) of our employees, contractors, visitors and the community; and Drives environmental sustainability and protects the environment. Our Actions We embrace our responsibility to achieve our HSE Commitment by: Visible & Felt Leadership, Collective Accountability, Organisational Learning.","Opex","No"]
[null,"Framework - Risk Management GV000-P0237","The Risk Management Framework (the â\u0080\u009cFrameworkâ\u0080\u009d) has been developed to support management in embedding risk management into all critical processes, decisions and management systems. The Framework supplements the Risk Management Policy and supports its implementation.","Opex, Capex","No"]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Finance Policy FM000-Y0205","The Finance Policy aims to ensure a consistent and uniform application of the Australian Accounting Standards to all financial reporting processes applicable to each entity in the Ausgrid Group.","Opex, Capex","No"]
[null,"Finance Framework FM000-P0206","This finance framework aims to ensure a consistent and uniform application of accounting principles throughout the Ausgrid Groupâ\u0080\u0099s financial reporting processes, while also ensuring compliance with Australian Accounting Standards and ensuring reliability of financial information","Opex, Capex","No"]
[null,"Finance Procedure - Revenue Recognition FM000-P0210","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 4 â\u0080\u0093 Revenue","Revenue, Capex","No"]
[null,"Finance Procedure - Accrued Expenses FM000-P0214","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further detailed explanation of the application and treatment of the accrual principle outlined in the Finance Framework","Opex, Capex","No"]
[null,"Finance Procedure - Capitalisation FM000-P0207","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 1 â\u0080\u0093 Capitalisation","Capex for accounting (not regulatory), Capex","No"]
[null,"Finance Procedure - Impairment of Assets FM000-P0211","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 8 â\u0080\u0093 Impairment of assets.","Opex, Asset value","No"]
[null,"Finance Procedure - Intangible Assets FM000-P0208","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 2 â\u0080\u0093 Intangible assets.","Opex, Capex","No"]
[null,"Finance Procedure - Provisions FM000-P0213","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 10 â\u0080\u0093 Provisions","Asset Value, Capex","No"]
[null,"Finance Procedure - Leases FM000-P0209","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 3 â\u0080\u0093 Leases.","Opex","No"]
[null,"Finance Procedure - Fixed Assets FM000-P0212","This procedure is to be read in conjunction with the Finance Framework. It aims to provide further explanation of the application and treatment of accounting principles outlined in the Finance Framework: Section 9 â\u0080\u0093 Fixed assets.","Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Policy - Asset Management NW000-Y0085","To outline the organisationâ\u0080\u0099s commitment to applying effective asset management practices to support the delivery of the organisationâ\u0080\u0099s corporate strategy and objectives.","Opex; Capex","No"]
[null,"Procedure - Asset Management System Framework Governance NW000-P0203","To outline the decision, endorsement and approval pathways for changes to Ausgridâ\u0080\u0099s Asset Management System (AMS) to ensure the system delivers the objectives outlined in Ausgridâ\u0080\u0099s Asset Management Policy.","Opex; Capex"]
[]
[]
[null,"Division Procedure - Asset Management Strategy NW000-P0217","Outline the process for Asset Strategy management.","Opex; Capex","No"]
[]
[]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"<insert relevant policy, plan, strategy etc>"]
[null,"Distribution and Transmission Annual Planning Report","It has been prepared to comply with National Electricity Rules (NER) clause 5.13.2 \"Distribution Annual Planning Report\" (DAPR) and clause 5.12.2 \"Transmission Annual Planning Report\" (TAPR). Version 183 of the NER has been used for the purpose of this report.","Replacement capex; Maintenance opex; Asset condition assessments; Asset risks","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Policy - Investment Governance Framework GV000-Y0032","To provide a framework which promotes investment decisions which are: streamlined â\u0080\u0093 decision pathways are clear and efficient; consistent â\u0080\u0093 assessment of needs, outcomes and risks are aligned; timely â\u0080\u0093 information is provided within timeframes suitable for appropriate action; relevant â\u0080\u0093 appropriate information is submitted to the necessary forum to enable informed decisions; and value enhancing â\u0080\u0093 selection of investments that deliver value for customers and shareholders.","Capex","No"]
[null,"Procedure - Network Investment Governance GV000-P0033","To provide guidance on the process to obtain endorsement and approval for network investments in order to support investment decisions","Capex","No"]
[null,"Procedure - Network Investment Governance Decision Pathways NW000-P0067","Outlines the decision, endorsement and approval pathways of network investments across the integrated investment governance life cycle and includes references to all the relevant NIGF procedures and forms","Capex","No"]
[null,"Procedure - Capital Budget Request GV000-P0066","To outline the business rules with the electronic entry, endorsement and approval of network and non-network project capital funding requests over key stages of the capital investment.","Opex; Capex","No"]
[null,"Division Workplace Instruction - Development Brief for Network Capital Projects (Subtransmission) NW000-W0060","To outline and describe the tasks in preparing, reviewing and obtaining approval for a Development Brief for Network capital project for subtransmission zone assets. The Development Brief supports the Delivery Plan and Gate 2 investment governance approval process.","Capex","No"]
[null,"Division Workplace Instruction - Program Brief for Network Capital Programs","To outline and describe the tasks in preparing, reviewing and obtaining approval for a Program Brief for Network Capital Programs. The program Brief supports the Delivery Plan and subprogram Gate 2 investment governance approval process.","Capex","No"]
[null,"Procedure - Network Investment Governance Define Network Capital & Maintenance Investment Portfolio","To outline the activities and outputs of the define network investment portfolio process within the identify needs and develop options stage of the integrated investment governance life cycle. The purpose of this process is to identify the steps required to compile the prioritised network capital and maintenance investment portfolios.","Capex","No"]
[null,"Procedure - Network Investment Governance Asset Planning","To outline the activities and outputs of the network asset planning process within the identify needs and develop options stage of the integrated Investment Governance life cycle. The purpose of the asset planning process is to define the steps by which the company plans and invests in its electricity network.","Capex","No"]
[null,"Procedure - Network Investment Governance Preliminary Assessment","To outline the activities and outputs of the preliminary assessment process within the preliminary assessment stage of the integrated network investment governance life cycle. The preliminary assessment process tests the network need for a program/project by developing the preliminary business case/approval documentation for Gate 2 preliminary approval.","Capex","No"]
[null,"Procedure - Network Investment Governance Develop Project","To outline the activities and outputs of the develop project process within the develop program/project stage of the integrated investment governance life cycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Deliverability and Feasibility Assessment","To outline the activities and outputs of the deliverability and feasibility assessment process for network capital projects within the preliminary assessment stage of the integrated Investment Governance life cycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Plan Program","To outline the activities and outputs of the plan program process within the develop project/program stage of the integrated investment governance life cycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Deliver Program/Project/Task","To outline the activities and outputs of the deliver program, project and task process in the execute program, project and task stage of the integrated investment governance life cycle. The company manages program, project and task delivery through to closure, whether delivered by internal resources or the market, so an identified network need is delivered to time, cost and scope.","Capex","No"]
[null,"Procedure - Network Investment Governance Monitor Portfolio Program and Project Performance","To define a performance monitoring framework for network investments","Capex","No"]
[null,"Procedure - Network Investment Governance Initiate Reactive Work Request","To define a repeatable, consistent and scalable process for initiating reactive work requests on company network assets.","Capex","No"]
[null,"Procedure - Network Investment Governance Assess Sub-Program Project Task","To outline the activities and outputs of the assess sub-program project(s)/task process within the develop project/program stage of the integrated Investment Governance life cycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Assess Capital Reactive Work Request","To outline the activities and outputs of the assess reactive work request process within the develop program/project stage of the integrated Investment Governance life cycle.","Capex","No"]
[null,"Procedure - Project Management","To outline the company's project management process and stages (initiate, plan, execute, and close) as part of the overall integrated Network Investment Governance lifecycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Program/Project/Task Close","To outline the activities and outputs of the program, project and task close process within the evaluate stage of the integrated Investment Governance lifecycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Evaluate Program/Project","To outline the activities and outputs of the evaluate program/project process within the evaluate stage of the integrated Investment Governance life cycle.","Capex","No"]
[null,"Procedure - Network Investment Governance Assess Delivery Risks & Constraints","To outline the activities and outputs of the assess delivery risks and constraints process within the identify needs and develop options stage of the integrated Investment Governance lifecycle.","Capex","No"]
[null,"Procedure - Network Resource Planning","To outline the activities and outputs of the workforce planning process within the identify needs and develop options stage of the integrated investment governance life cycle.","Capex","No"]
[null,"Procedure - Investment Evaluation","To outline the process for preparing and reviewing financial evaluations on investment options so that these evaluations are conducted in a streamlined and consistent manner.","Capex","No"]
[null,"Procedure - Network Investment Governance Change Control","To provide a framework for the management, monitoring and implementation of changes to the scope, time, cost, or risk of approved network capital programs/projects in the company's investment portfolios during the approval stages of the investment lifecycle as measured against approved baselines.","Capex","No"]
[null,"Company Procedure - Network Investment Governance Document Repository","To outline/describe the business rules associated with creating and managing the Network Investment Governance Framework (NIGF) documents in HPRM NIG.","Capex","No"]
[]
[]
[]
[]
[]
[]
[null,"Refer to the below Network Standards (NS)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Network Standards (NS)","Full listing of current Network Standard is provided below","Network Standards underlie unit rates, frequency and duration of maintenance tasks, and the construction and operation of the network. Accordingly, they have an indirect impact on our proposal. There have been no changes to technical standards since the proposal that have had a material impact on the current proposal."]
[null,"NS 100 Field Recording of Network Assets","This Network Standard sets out the requirements of recording as-built asset information for Ausgrid's transmission and distribution networks, and third-party fibre assets interacting with company assets. The objective of field recording is to provide an accurate record of the position, type and quantity of Ausgrid's assets, to enable those assets to be quickly identified and located at a later date. In addition, this information is used to maintain Ausgrid's Geographic Information System (GIS).","As above","No"]
[null,"NS 102 Working on or near Poles With Telecommunication Transmitters","This Standard details the procedure to follow so that work may be completed safely and efficiently on Ausgrid poles or street lighting columns where telecommunication transmitter installations are installed. This standard applies to all Ausgrid staff, contractors and ASPs","As above","No"]
[null,"NS 104 Specification for Electrical Network Project Design Plans","Ausgrid's specification for Network Project Design Plans","As above","No"]
[null,"NS 109 Design Standards for Overhead Supply Developments and Distribution Centres","Details design criteria for 415V and 11kV overhead reticulation systems","As above","No"]
[null,"NS 110 Design and Construction Standard for Underground Residential Subdivisions","Provides the design and construction criteria for 415V and 11kV reticulation systems in Underground Residential Distribution (URD) estates situated within the supply area of Ausgrid.","As above","No"]
[null,"NS 112 Design Standards for Industrial and Commercial Developments","Details design criteria for 415V and 11kV reticulation systems and for street lighting in commercial and industrial developments","As above","No"]
[null,"NS 113 Site Selection and Construction Design Requirements for Chamber Substations","Provides Ausgrid's minimum site selection, building design and construction requirements for the establishment of new 11kV Chamber Substations with ratings up to and including 4.5 MVA.","As above","No"]
[null,"NS 114 Electrical Design and Construction Standards for Chamber Type Substations","Details the criteria for electrical design of 11kV chamber type distribution substations","As above","No"]
[null,"NS 116 Design Standards for Distribution Equipment Earthing","Provides the criteria for earthing of distribution substations to be connected to Ausgrid's network.","As above","No"]
[null,"NS 117 Design and Construction Standards for Kiosk Type Substations","Details the criteria for electrical design of kiosk type distribution substations","As above","No"]
[null,"NS 119 Public Lighting Design And Construction","Details the design and construction requirements for all public lighting assets in the Sydney, Central Coast and Hunter regions.","As above","No"]
[null,"NS 122 Pole Mounted Substation Site Selection and Construction","Details the requirements for constructing pole transformers","As above","No"]
[null,"NS 124 Specification for Overhead Connections (100 to 400Amps)","Provides the requirements for the erection and connection of overhead service cables, up to and including nominal 400 Amps in Ausgrid's supply area","As above","No"]
[null,"NS 125 Construction of Low Voltage Overhead Mains","Details the fittings and installation of LV ABC","As above","No"]
[null,"NS 126 Construction of High Voltage Overhead Mains","NS 126 is Ausgrid's specification for the design and construction of 11kV or 12.7kV SWER Overhead lines within the Ausgrid Supply Network area.","As above","No"]
[null,"NS 127 Low Voltage Cable Joints and Terminations","Provides Ausgrid's requirements for making cable joints and terminations on low voltage cables.","As above","No"]
[null,"NS 128 Pole Installation and Removal","Details the requirements for positioning, handling and removal of poles","As above","No"]
[null,"NS 129 11kV Joints and Terminations   Paper Insulated Lead Covered Cables","Details a number of 11kV PILC cable joints and terminations","As above","No"]
[null,"NS 130 Laying of Underground Cables Up to and including 11kV","Details the requirements for trenching, reinstatement, and laying underground conduits and cables, up to and including nominal 11kV in Ausgrid's supply area.","As above","No"]
[null,"NS 135 Construction of 33kV, 66kV and 132kV Overhead Mains","Specifies the requirement for the design and construction of overhead sub-transmission lines for use on the Ausgrid network","As above","No"]
[null,"NS 136 Assessment and Management of Low Voltage Parallels","Defines the management process for low voltage parallels within Ausgrid","As above","No"]
[null,"NS 141 Site Selection and Site Preparation Standards for Kiosk Type Substations","Provides the criteria for siting of kiosk distribution substations in all off-street locations and footpath sites in all areas of Ausgrid.","As above","No"]
[null,"NS 143 Easements, Leases and Rights of Way","Details the basic requirements for easements","As above","No"]
[null,"NS 145 Pole Inspection and Treatment","Describes the inspection, assessment and treatment procedures for timber poles, reinforced poles, concrete and steel poles, composite poles, fibre composite poles, lighting standards, lightning masts and water crossing sign supports. Appendix Describes the various poles owned by Rail Corp, Telstra, RTA, Local Council etc.","As above","No"]
[null,"NS 146 Inspection Procedure for Working on Poles","This Network Standard applies to all staff, contractors, Accredited Service Providers (ASPs), Telecommunication workers and any other personnel who have authority to work on Ausgrid power poles. It also applies when Ausgrid's staff or Ausgrid's contractors work on privately owned power poles, or poles belonging to other Authorities when working on behalf of Ausgrid.","As above","No"]
[null,"NS 148 Overhead Line Support, Street Light Column, Pit and Pillar Labelling","Details the allocation and installation of identification labels for overhead line supports, street lighting poles, pits, distribution pillars, and ancillary assets.","As above","No"]
[null,"NS 149 Drawing Content for Chamber Type Substations, Control Points, Cable Risers and Ductlines","Ausgrid's specification for the minimum content of the design drawing package required by Ausgrid for design of chamber type substations, control points, cable risers and ductlines.","As above","No"]
[null,"NS 156 Working Near or Around Underground Cables","Details the safety requirements that apply to all excavation work carried out in areas where an Ausgrid underground cable installation is located nearby.","As above","No"]
[null,"NS 158 Labelling of Mains and Apparatus","Ausgrid's specification for labelling of mains & apparatus.","As above","No"]
[null,"NS 159 Installation of Cables and Conduits using Trenchless Techniques","This Network Standard is to be used for the installation of underground cables and conduits by trenchless techniques where such techniques are either specified by Ausgrid or have been requested by a third party and reviewed by Ausgrid on a project specific basis. This Standard covers underground cables of all voltages","As above","No"]
[null,"NS 161 Specification for Testing of Underground Cables","Ausgrid's specification for testing pilot, low voltage and high voltage distribution and sub-transmission cable installations.","As above","No"]
[null,"NS 162 Installation of Fibre Optic Communication Cables in Ausgrid Conduit Network and Substations","Details the requirements for installing third party fibre optic or conductive communications cables in Ausgrid's ductlines and extending them through Ausgrid substations","As above","No"]
[null,"NS 165 Safety Requirements for Non Electrical Work in and around Live Substations","Details the specification and requirements for construction work, including excavation, in Ausgrid's major substations and switching stations.","As above","No"]
[null,"NS 166 Routine Overhead Line Inspection","This Network Standard describes the scope for inspection of Ausgrid's overhead pole lines and associated infrastructure","As above","No"]
[null,"NS 167 Positioning of Poles and Lighting Columns","Covers the requirements and responsibilities for selecting distribution and sub-transmission pole positions and street lighting column positions","As above","No"]
[null,"NS 168 Design and Construction of 33kV, 66kV and 132kV Underground Cables","Specifies the requirements for the design and construction of underground sub-transmission lines for use on the Ausgrid network","Unit rates for sub-transmission underground","No"]
[null,"NS 169 Telecommunications Installations on Ausgrid HV Transmission Towers","Specifies the technical requirements for the attachment of telecommunications installations to high voltage steel transmission towers","As above","No"]
[null,"NS 171 Fire Stopping in Substations","Ausgrid's specification and requirements for the installation of firestopping materials in openings in substation walls, floors and ceilings","As above","No"]
[null,"NS 172 Design Requirements for Cable Pits, Vaults and Bays","Network Standard NS 172 describes the design requirements for cable jointing pits and vaults.","As above","No"]
[null,"NS 174 Environmental Procedures","Outlines the environmental procedures to be adopted by all personnel involved in the construction, maintenance and operation of Ausgrid's network.","As above","No"]
[null,"NS 177 11kV Joints (including Transition Joints) & Terminations -Polymeric Insulated Cables","Network Standard NS 177 specifies the requirements for making joints and terminations on 11,000 Volts polymeric insulated cables in Ausgrid's supply area. This Standard also specifies the requirements for transition joints from polymeric insulated cables to paper insulated lead covered (PILC) cables.","As above","No"]
[null,"NS 178 Secondary System Requirements for Major Substations","Network Standard NS 178 covers the planning and design requirements for secondary systems for subtransmission feeders, subtransmission substations and zone substations","As above","No"]
[null,"NS 179 Vegetation Management","Withdrawn and replaced by ISSC3 Guidelines for Managing Vegetation Near Power Lines","As above","No"]
[null,"NS 181 Approval of Materials and Equipment and Network Standard Variations","Details the approval requirements of materials and equipment used in the construction of, and which ultimately forms part of, Ausgrid's electrical network. This NUS also details the approval requirements of Network Standard variations.","As above","No"]
[null,"NS 183 Installation of Private Attachments on Ausgrid Poles","Details the procedures required to ensure that proposals to install third party attachments on Ausgrid's power poles and lighting columns are properly handled and comply with Ausgrid standards.","As above","No"]
[null,"NS184 Fences for Zone and Subtransmission Substations","This Network Standard sets out the minimum requirements for intruder resistant fences and boundary fences for new substations only. Refurbishment works shall conform to this standard where reasonably practicable.","As above","No"]
[null,"NS 185 Major Substations Building Design Standard","NS 185 details the general requirements for various Construction, Architectural, Civil and Structural engineering aspects to be considered and included into the design of Major Substations","As above","No"]
[null,"NS 186 Major Substations Civil Works Design Standard","NS 186 details the general requirements for various Construction, Architectural, Civil and Structural engineering aspects to be considered and included into the design of Major Substations.","As above","No"]
[null,"NS 187 Passive Fire Mitigation Design of Substations","Details Ausgrid's minimum requirements for passive fire protection systems needed to provide protection of Ausgrid's substations.","As above","No"]
[null,"NS 188 Design for Substation Overpressure","Network Standard NS 188 details the design requirements for the management of substation overpressures resulting from  arc faults and deflagrations.","As above","No"]
[null,"NS 189 Oil Containment for Major Substations","NS 189 details the general requirements for oil containment at major substations.","As above","No"]
[null,"NS 190 Oil Containment Operational Requirements for Major Substations","Details the operational requirements for oil containment systems at major substations.","As above","No"]
[null,"NS 191 Batteries & Battery Chargers in Major Substations","Details 110 V battery and battery charger systems within new Major Substations consisting of Sub-transmission and Zone Substations.","As above","No"]
[null,"NS192 Blasting near substations and power lines","This standard sets acceptable limits and controls that need to be put in place to prevent damage to Ausgrid assets resulting from mine and quarry blasting.","As above","No"]
[null,"NS193 Ground movement and vibration limits near buried cables","This standard sets the acceptable ground movement and vibration limits for Ausgrid's buried electrical cables to prevent damage to Ausgrid's assets due to major site works by other organisations","As above","No"]
[null,"NS 194 Embedded Generation","Outlines the requirements an Embedded Generator should fulfil when connecting to the Ausgrid's network.","As above","No"]
[null,"NS 195 High Voltage Customer Connections (HVCs)","Outlines the requirements of a high voltage customer connection to Ausgrid's Distribution System","As above","No"]
[null,"NS 196 Mobile Generators","Details the requirements for the connection and operation of Mobile Generators on Ausgrid's network","As above","No"]
[null,"NS 199 Safe Electrical Work on Specific Undrground Assets","Outlines mandatory safe electrical working requirements applicable to all Accredited Service Providers working on various low voltage assets.","As above","No"]
[null,"NS 200 Major Substations Ventilation Design Standard","NS 200 details the technical aspects to be considered in the design of ventilation systems for Ausgrid major substation buildings. Generally this includes new zone and sub-transmission substations.","As above","No"]
[null,"NS 201 All Dielectric Self Supporting Fibre Optic Cabling for Installation on Poles","Ausgrid's specification for the design and installation of Aerial All Dielectric Self Supporting Fibre Optic Networks - Note: this standard is for Ausgrid fibre installation only - not NBN","As above","No"]
[null,"NS 203 Telecommunications Network: Master Policy Document","Provides the design criteria for Ausgrid personnel associated with the planning, design, construction, maintenance and auditing of communication network assets used to support the electrical network. The document includes communication requirements for protection circuits, which being the most demanding in terms of availability, determine key aspects of the communications network.","As above","No"]
[null,"NS 204 Communication Pits - Specifications and Installation","Provides the specifications and guidelines for the purchase and installation of communication pits (buried and surface) to be used in the Ausgrid communications network for fibre optic cable installations, particularly when installed independently of power cable routes.","As above","No"]
[null,"NS205 Telecommunications Route Markers","This document details the requirements for Ausgrid's buried telecommunications assets installed stand-alone to be made locatable after installation and reinstatement works are complete. This standard defines asset location methods to be applied either at the time of new buried asset installation, or by retrofitting to pre-existing assets. NS205 also defines asset location requirements for Ausgrid telecommunications infrastructure installed through bridge and tunnel voids.","As above","No"]
[null,"NS 208.2.1 Telecommunications Communication Cabinet Architecture Design Work Instruction","Defines the requirements for selection of equipment where standard equipment has not been specified, or a non standard installation is required","As above","No"]
[null,"NS 208.2.2 Telecommunications Substations Communication Cabinet Interconnectivity Design Work Instruction","NS208.2.2 defines the connectivity to be deployed when designing optical fibre systems in substations and depots.","As above","No"]
[null,"NS 208.2.3 Telecommunications Substations Communications Cabinet Allocations Design Work Instruction","NS208.2.3 defines the the quantity and broad function of communications cabinets to be deployed when designing communication systems in substations and depots.","As above","No"]
[]
[null,"NS 210 Documentation and Reference Guide for Major Substations","Provides the general documentation and reference design guidance for the Environmental, Civil, Architectural, Electrical Primary and Electrical Secondary aspects that shall be considered and included into the design and construction of Ausgrid's major substations.","As above","No"]
[null,"NS 211 Working With Asbestos Products   (replaces TS665)","Details the requirements for safely working with, and/or removing from the workplace, materials containing asbestos.","As above","No"]
[null,"NS 212 Integrated Support Requirements for Ausgrid Network Assets","sets out the required support requirements, including documentation, spares  and training required for new network assets.  This information is required to be delivered with any new type of asset being added to the Network","As above","No"]
[null,"NS 214 Guide to HV Live Work Design Principles","applies to the design of overhead mains to facilitate the use of HV Live Line techniques.","As above","No"]
[null,"NS 215 Telecommunications Allocation And Recording Of Fibre Use Design Work Instruction","Specifies the technical requirements for the allocation and recording of usage of optical fibre used throughout the Ausgrid network","As above","No"]
[null,"NS 219 Telecommunications Telephone Allocation And Isolation","Outlines the requirements to be met when installing telephony equipment in a substation where connection external to the substation is via electrically conductive cable.","As above","No"]
[null,"NS 220 Overhead Design Manual","The Overhead Design Manual is to be used to support the overhead line design process. Its purpose is as a standard designer's checking tool and a training aid.","As above","No"]
[null,"NS 221 Telecommunications, Changes To In Service Teleprotection Equipment Configuration Policy","Outlines the requirements to be met when intending to apply hardware and/or software configuration changes to teleprotection equipment carrying live traffic.","As above","No"]
[null,"NS 222 Major Substation Earthing Design","Sets out the objectives and basic configurations required of an earthing layout for major substations. It also specifies procedures and acceptable practice by which these shall be achieved","As above","No"]
[null,"NS 223 Overhead Low Voltage Short Circuiting for De-energised Work","This standard is Ausgrid's specification for the design and use of Low Voltage short circuit sets for personnel protection on Ausgrid's low voltage overhead assets. Note: This standard is not mandatory until the supporting equipment and changes to the Electrical Safety Rules have been made.","As above","No"]
[null,"NS 224 Low Voltage (240/415V) Suburban Commercial & Industrial Underground Distribution Utilising Pillars","Specifies the requirements for the construction of low voltage (240/415 volt) suburban commercial and industrial underground distribution systems utilising pillars in Ausgrid's supply area.","As above","No"]
[null,"NS 230 Testing of Distribution Substations","Applies to the testing of distribution substations throughout all parts of Augrid's supply area. This standard is applicable to pole, kiosk and chamber substations.","As above","No"]
[null,"NS 232 Telecommunications Cables on Ausgrid poles","NS232 is Ausgrid's specification for the design and positioning of NBN cables and fixtures on Ausgrid's overhead assets","As above","No"]
[null,"NS234 Telecommunications Underground Physical Plant Installation","Specifies the requirements for the installation of Ausgrid's telecommunications conduit as well as for the haul of telecommunications cable through underground conduit in Ausgrid's supply area.","As above","No"]
[null,"NS235 Telecommunications Underground to Overhead Transition","Details the minimum requirements for constructing an underground to overhead (UGOH) telecommunications transition on Ausgrid and approved TransGrid assets","As above","No"]
[null,"NS236 Installation of Electronic Perimeter Security at Major Substations","Outlines the minimum requirements for the installation of electronic security equipment for detecting attempted or actual breeches into the live yard perimeters of major substations.","As above","No"]
[null,"NS 238 Supply Quality","Ausgrid's objectives for its electricity network's impact on the characteristics of electricity supplied by retailers to their customers through its electricity network","As above","No"]
[null,"NS243 Telecommunications: Roles, Responsibilities, Training Requirements, Auditing and Quality Assurance Acceptance","Defines the quality assurance processes, documentation and tasks necessary to prove compliance and thus achieve telecommunications asset acceptance by Ausgrid","As above","No"]
[null,"NS245 Telecommunications Approved List of Materials","Lists the approved materials which are specific to the Ausgrid telecommunications network","As above","No"]
[null,"NS250 Requirements for CT, VT, and tripping circuits","Describes requirements for Voltage Transformer (VT), Current Transformer (CT) and Circuit Breaker (CB) trip circuits within zone and subtransmission substations","As above","No"]
[null,"NS251 Secondary Systems - Requirements for Cables Between Panels","This standard describes the following types of electrical cable connections between panels including: - Power supply cables for secondary and auxiliary systems. - Substation control cables.- Secondary CT and VT cables. - Indication and signalling cables.","As above","No"]
[null,"NS252 Secondary Systems - Requirements for wiring within panels","Describes the requirements for secondary wiring within panels in order to facilitate consistency across the network.","As above","No"]
[null,"NS253 Termination of Wiring in Substations Protection and Control Equipment","Standardises the types of cable termination methods, lugs, and crimping tools used across the Ausgrid Network in the wiring of substation control and protection panels and other related substation equipment.","As above","No"]
[null,"NS257 Control and Protection Cabinets and Minor Panel Hardware","Applies to the cabinets used for control and protection equipment within zone and sub-transmission substations. It covers the panel specifications and the minor hardware such as lamps, door locks and similar hardware not directly associated with the design of the control equipment that will be installed in the cabinets.","As above","No"]
[null,"NS259 Requirements for Protection System Segregation","The purpose of this standard is to describe the physical, electrical and logical segregation requirements for protection equipment and functions within zone and subtransmission substations.","As above","No"]
[null,"NS260 Sub-Transmission Feeder Earthing","Provides guidelines on the design and construction of sub-transmission feeder earthing systems.","As above","No"]
[]
[null,"NS262 Private Mains Bushfire Risk Inspection","Prescribes the general procedure and assessment criteria for Private Mains Bush Fire Risk Inspection. It covers the assessment of the bush fire and life threatening safety risks in low voltage private mains.","As above","No"]
[null,"NS263 Setting of 11kV Feeder Protection, Automation and Control Schemes","This standard applies to all new settings issued for the protection, automation and control of 11kV feeders including the setting of protection elements downstream of the zone substation panel.","As above","No"]
[null,"NS264 Major Substation Lightning Protection and Insulation Coordination","This document defines the requirements for: - Design, construction and documentation of major substation lightning protection systems; - Minimum equipment insulation requirements for major substations; and - Minimum overvoltage protective requirements (surge arresters and overhead earth wires) for major substations.","As above","No"]
[null,"NS266 Telecommunications Cables in Ausgrid Premises","Applies to telecommunications \"passive\" cabling in Ausgrid premises. This standard does not include infrastructure requirements outside Ausgrid premises","As above","No"]
[null,"NS268 Specification for Design and Construction of Waterway Crossing","Assists Ausgrid employees and ASPs involved in the design and construction of Ausgrid overhead, under-bored and submarine waterway crossings including 132kV, 66kV, 33kV, 22kV, 11kV, LV and communications cables.","As above","No"]
[null,"NS270 Stray Direct Current Management","Specifies high level requirements that apply to buried assets across the Ausgrid network subject to exposure from stray direct current from external parties, such as railway traction systems and cathodic protection systems.","As above","No"]
[null,"NS272 Underground Cable Rating","This Network Standard covers Ausgrid's approach to underground cable ratings and where it aligns and deviates from IEC60287 - Electric cables - Calculation of the current rating, the considerations for rating of Ausgrid's underground cables and some detail on why this information is required, the information Ausgrid will supply as part of rating Ausgrid assets and a checklist to ensure all aspects of rating an underground are considered.","As above","No"]
[null,"NS273 Secondary Systems Configuration Management","This standard pertains to the configuration management for secondary systems assets installed on the Ausgrid network in line with: - ISO 10007:2017 - Quality Management - Guidelines for Configuration Management; and, - ISO 9001:2016 - Quality Management Systems - Requirements.","As above","No"]
[null,"NS282 Service Testing","This Network Standard sets out the tests to be performed by authorised persons each time a new connection is made, or a service is replaced, on Ausgrid's network. It also establishes the minimum performance that must be achieved in those tests. This applies to both overhead and underground services.","As above","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"TS 7314 Load Survey Recorder","Describes the procedures for the use of a load survey recorder. NOTE: the electronic version of this document is not available. Use the latest release, hard copy version for reference and construction","As above","No"]
[null,"TS 7316 Reading of Electronic Multifunction Registers","Sets out the method of recording readings of electronic multi-function registers associated with Demand, Time-Of-Use Demand and Industrial Development tariffs NOTE: the electronic version of this document is not available. Use the latest release, hard copy version for reference and construction","As above","No"]
[null,"TS 7317 Electronic Meters","Sets out the methods of installing direct-connected electronic meters","As above","No"]
[null,"TS 7318 Sealing and Labelling of Metering and Service Equipment","Details the recommended procedures to be adopted by field staff when sealing and labelling metering and service equipment","As above","No"]
[null,"TS 7319 End Use Monitoring System","Details the procedures to be adopted when an End-Use Monitoring System is to be installed by a Meter Technician","As above","No"]
[null,"TS 7700 Meter Testing General","Provides general information relating to the testing of meter installations.","As above","No"]
[null,"TS 7704 Principles and Application of Q Metering","Provides an introduction to the theory of kVA metering using the measurement of the quantity Q and is for the information of metering personnel.","As above","No"]
[null,"TS 7752 Periodic Maintenance of Metering Equipment","Details the requirements for periodic testing and sample testing of the different types of metering instruments","As above","No"]
[null,"TS 7753 Maintenance of Portable Meter Test Equipment","Sets out the procedures to be adopted for the regular calibration and maintenance of the portable test equipment used in testing of watthour and energy-demand meters in customer installations. NOTE: the electronic version of this document is not available. Use the latest release, hard copy version for reference and construction","As above","No"]
[]
[]
[null,"Policy - Sustainable Procurement PL000-Y0116","To define the considerations and accountabilities for sustainable procurement of externally sourced goods and services in a way that has the most positive environmental, social and economic impacts possible over the entire life cycle.","Sourcing and purchase of goods, stores, materials, equipment, works & services to support Ausgrid's capex and opex programmes","No"]
[null,"Procedure - Purchasing - All Users PL000-P0171","This Procedure supports the Policy â\u0080\u0093 Sustainable Procurement, by describing the requirements, processes, and responsibilities for the purchase of goods and services from external suppliers. In doing so, the principles described in the Policy also apply.","Sourcing and purchase of goods, stores, materials, equipment, works & services to support Ausgrid's capex and opex programmes","No"]
[null,"Procedure - Procurement Source to Contract PL000-P0170","This Procedure describes the requirements, processes and responsibilities for the sourcing of goods and services from suppliers by Procurement as defined by the scope.","Sourcing and purchase of goods, stores, materials, equipment, works & services to support Ausgrid's capex and opex programmes","No"]
[]
[null,"Company Policy - Acceptable Use of Technology","The purpose of this policy is to describe how ICT assets will be allocated to employees to support the performance of their duties, to provide guidelines for the limits of personal use, to define what constitutes inappropriate use of technology and to describe how ICT asset use will be monitored and any inappropriate use identified.","ICT Opex","No"]
[]
[null,"Company Policy - Operation and Control of the Distribution System","Provides clarity on how Ausgrid will meet its Licence Conditions that apply to the operation and control of the distribution system in relation to access outside of Australia and cyber security.","OT Opex","No"]
[null,"Company Procedure - OT Control System Lifecycle and Release Management","To establish management of Control System releases in Control System Master Station environments and to ensure the responsible groups understand their roles.","OT Opex","No"]
[null,"Company Procedure - Network Operations Critical Infrastructure Licence Conditions","This procedure defines the framework in accordance with the requirements of the Company Policy Network Operations Critical Infrastructure Licence Conditions (the 'policy'): - risk management approach to be adopted to support decision making for maintenance activities undertaken in accordance with Licence Condition 9.1; and - approach to manage breaches and non-complying events associated with Licence Condition 9.1. It applies applies only to parties involved in the undertaking of maintenance on the distribution system.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Addition, Removal and Disposal of Assets","Defines the process of adding, removing and disposing of Control System Master Station assets in the most appropriate and safe way, so as to protect the company from security vulnerabilities.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Backup Verification Process","Describes the activities required to backup and restore control system data.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Acceptance Testing","This procedure describes the activities required to certify that the Control System Master Station systems are fit for purpose prior to production deployment. The company Control Rooms use these systems to manage the electricity distribution network. As such the systems are considered mission critical and require a structured certification process prior to being deployed into production.","OT Opex","No"]
[null,"Branch Procedure - Defensive Isolation of Control System Master Station Network Segments","The purpose of this procedure is to: - document the network isolation options for the Control System Master Station available to defend against cyber attack; - confirm the chain of command which: - guarantees the quickest possible decision to limit potential damage; and - gives the order to isolate network segments. - identify the operational employee resources to action the isolation procedures.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Communication Flows","Describes the activities required to manage communication flows to and from the Control Zone and Industrial Demilitarised Zone (Industrial DMZ) of the Control System Master Station.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Network Segment Isolation","Describes the actions required when one of the following scenarios occurs: - isolation of network segments is required to prevent or contain a significant incident, for example Priority 1 (P1), Priority 2 (P2) cyber attack; or - network segments that have been isolated, due to a P1 or P2 incident, are to be re-instated.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Physical and environmental Security","The company maintains policy and procedures for the effective implementation of selected security controls. Policy and procedures reflect applicable laws, directives, regulations, policies, standards, and guidance.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Configuration Management","Defines the configuration management processes that apply to the Control System Master Station environments, to ensure only configurations that have passed acceptance testing before being deployed into Production.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Change Management","To describe the process to effectively manage Change Requests (CRs) within the Control System Master Station environment. The objectives of this procedure are as follows: - improving the handling of CRs; - ensuring a quality review of information included within change(s) is in alignment with standard Information Technology Infrastructure Library (ITIL) practices; - allowing business users to understand change(s) that impact their area, and to communicate the impact to users; and - ensuring senior management has visibility of all change(s) occurring with the Control System Master Station to align with the company's strategy.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Server Management","Describes how servers are added, created, maintained and decommissioned within the Control System Master Station environments.","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Offline Test Environment Management","Describes the management of the Control System Master Station Offline Test Environment","OT Opex","No"]
[null,"Branch Procedure - Control System Master Station Disaster Recovery Process","Describes the activities required to restore the Control System Master Station data from a backup.","OT Opex","No"]
[null,"Branch Procedure - ICT Disaster Recovery","Describes the procedure used by ICT to undertake disaster recovery testing of ICT applications and infrastructure that support mission and business critical processes. This procedure defines: -how the disaster recovery (DR) test calendar is created; -how modifications to the testing calendar are approved; -the process for classifying application criticality and determining the appropriate business requirements (recovery point and time); -the process for undertaking and performing the recovery of an application at its disaster recovery site for either a test or actual disaster; -how a data centre failure is managed; and -managing 3rd party hosted application disaster recovery testing.","ICT Opex","No"]
[null,"Branch Procedure - ICT Change Management","This procedure defines the process by which the ICT Business Unit manages technology changes to the production environment, enabling beneficial changes to be made with the minimum of disruption to ICT services. It applies to all employees and third party service providers that request, approve, or implement change on information technology assets and configuration items that provide production services or are part of the production environment. These include (but are not limited to) operating systems, computing hardware, networks, telecommunications, applications (eg modules, programmes, interfaces) and controlled documentation.","ICT Opex; Technology Plan Capex","No"]
[null,"Company Policy - Application Management Policy","The intention of this policy is to define the roles involved in the management of applications and to describe the key controls for applications in Ausgrid's production environment.","ICT Opex","No"]
[null,"Branch Procedure - ICT Capital Project Approval Process","This Branch procedure defines the approval process for business projects with an Information Communications and Technology (ICT) component (ie Non-Network ICT Capital projects). Its purpose is to protect the company's investment in ICT; direct company resources for maximum business benefit, and maintain budgetary control through the following: -controls to protect company's capital investment in ICT; -project outcomes are closely aligned to company, divisional and ICT Technology Strategic Plan; -business cases have been developed on sound commercial basis where sufficient metrics are in place such that benefits can be measured to review for value for money; -project scope and objectives are clearly defined; -project risks are identified with contingency and mitigation plans; -sufficient information is provided for management to set priorities; and -endorsement/approval is in accordance with applicable sub-delegation of authority.","Technology Plan Capex","No"]
[null,"ICT Application Recovery Procedures (ARPs) (Various)","Recovery Strategies and recovery timelines for each of our identified mission and business critical applications that are tested by ICT. These documents are updated both prior and post to each disaster recovery test / incident that requires disaster recovery to be invoked.","ICT Opex","No"]
[null,null,null,"I"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand Side Engagement","Ausgridâ\u0080\u0099s Demand Side Engagement Document (DSED) meets our obligations under Clause 5.13.1 of the National Electricity Rules setting out our strategy and processes for engaging with non-network providers and considering non-network options (demand management solutions). This document also includes information specified in Chapter 5, schedule 5.9 of the National Electricity Rules.","Demand Management Operating Expenditure Plan","No"]
[]
[]
[]
[null,"Treasury Policy - Insurance Risk; Ausgrid Insurance Program","Ausgrid insurance program and self insurance levels are reviewed at least annually with the Company's insurance brokers and the Board taking into consideration claims experience, market conditions and risk appetite.","Opex","Yes"]
[]
[]
[]
[null,"Network Property Plan","Nominates property acquisitions, including planned network property acquisitions and planned site disposals.","Relevant to system augmentation capex and replacement capex.","No"]
[null,"Corporate Property Plan","Nominates non-system property requirements.","Relevant to non-system property capex.","No"]
[]
[]
[]
[]
[null,"Policy - Organisational Security PF000-Y0089","To set out the organisations commitment to managing security risks to enable the security and safety of our people and the public as well as our assets, information, equipment and workplaces.","Opex; Capex","No"]
[null,"Framework - Organisational Security PF000-P0246","This document outlines the Organisation Security Framework (OSF) and describes how it is embedded into our operational processes and systems. The objectives of the framework are to enable the organisation to effectively manage security risk, compliance with relevant legislative and regulatory requirements and to meet industry standards and community expectations. As a critical infrastructure provider, the organisation is subject to increasing security risks from an expanding range of threat actors including, but not limited to, nation states, organised crime, criminal elements, opportunistic criminals, terrorist groups and trusted insiders.","Opex; Capex","No"]
[null,"Guideline - Physical Security Design PF000-WO173","To provide guidance with regard to the design and installation of physical security controls at Ausgrid.","Opex; Capex","No"]
[null,"Procedure - Personnel Security Senior and External Ausgrid PF000-P0301","This procedure describes the organisations approach to personnel security risk management and details the steps required to implement key personnel security controls.","Opex; Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[null,"Business Continuity Management Policy (GV001-Y005)","To establish and maintain a whole of business approach to BCM that minimises the impacts of disruption-related risk on the Companyâ\u0080\u0099s essential service delivery. This policy covers the Incident Management, ICT Disaster Recovery and Business Continuity. Key policies and plans associated Incident Management and Business Continuity are detailed below. Please refer to the Information Technology Policies or Strategies section for information related to ICT Disaster Recovery.","Opex","No"]
[null,"Emergency Management Plan (EMP001)","Describes the linkage between the NSW State Emergency Management Plan and Ausgrid's Emergency Management Plan","Opex","No"]
[null,"Incident Management System (IMS001)","The Incident Management System (IMS) covers the processes and procedures for the preparation for and response to incidents within Ausgrid. The IMS is applicable to all Ausgrid divisions, applies to all incidents.","Opex","No"]
[null,"Black Start Management Plan","Details the steps to be taken and the cpommunications with TransGrid requierd to recover from a full or partial 'System Black' event.","Opex","No"]
[null,"Emergency Planning HS010-P0100 (Pro16)","Defines the processes to be followed to facilitate the identification of potential emergency situations and develop and implement emergency plans designed to protect the health and safety, so far as is reasonably practicable, of persons (workers, visitors, tenants and others) in the event of an emergency incident on Ausgrid work sites. Ausgrid shall, so far as is reasonably practicable, eliminate or mitigate work hazards and risks to others arising out of our business activity in order to minimise the effects of an emergency incident.","Opex","No"]
[null,"Incident Management HS011-P0100","Describes the overarching process for managing Work Health and Safety (WHS) incidents in terms of immediate response (in conjunction with first aid, emergency planning, and WHS incident investigation procedures), internal and external notifications, worker welfare, reporting/recording and the requirement to commence an investigation. This procedure provides internal and external systems to communicate that a WHS Incident has occurred. The immediate actions taken (or required to be taken) to eliminate or reduce the potential for a re-occurrence of the incident, or to communicate a significant WHS issue that is relevant to the company.","Opex","No"]
[null,"NS 174C Environmental Handbook for Construction and Maintenance - Section 9 Environmental Incidents","Defines the processes to be followed in the event of an environmental incident, including immediate response, notifications and reporting.","Opex","No"]
[null,"Business Continuity Plans","Ausgrid has identified 58 critical processes and developed Business Unit based business continuity plans that document the key requirements and workaround strategies for a loss of key people, systems, facilities or suppliers.","Opex for the planning; Capex for some improvements in workaround strategies","No"]

{"sheet":"7.2 Contingent projects","index":25,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2024-25 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2024-25"}]
[null,"N/A",null,null,null,{"$f":"+E8*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":26,"n_rows":294,"n_cols":5,"rows_kept":294,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"A New Tax System (Goods and Services Tax) Act 1999 (Cth)","GST obligations","OPEX","No"]
[null,"Aboriginal and Torres Strait Islander Heritage Protection Act 1984 (Cth)","Obtain approval to work in protected areas and comply with all permits and approvals.","CAPEX for new installations, repairs or replacement","No"]
[null,"Aboriginal Land Rights Act 1983 (NSW)","Review for strategic property management","CAPEX for new installations","No"]
[null,"Access to Neighbouring Land Act 2000 (NSW)","Development of land for electrical infrastructure, service centres, etc","CAPEX for acquisitions","No"]
[null,"Age Discrimination Act 2004 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Agricultural and Veterinary Chemicals (New South Wales) Act 1994 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Agricultural and Veterinary Chemicals Code Act 1994 (Cth)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Annual Holidays Act 1944 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Anti-Discrimination Act 1977 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Apprenticeship and Traineeship Act 2001 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Australian Business Growth Fund (Coronavirus Economic Response Package) Act 2020","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Australian Human Rights Commission Act 1986 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Australian Jobs Act 2013 (Cth)","Network operations and practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Australian Radiation Protection and Nuclear Safety Act (License Charges) 1998 (Cth)","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Australian Radiation Protection and Nuclear Safety Act 1998 (Cth)","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Australian Securities and Investments Commission Act 2001Â (Cth)","The formation and operation of companies and fund raising","CAPEX and OPEX","No"]
[null,"Bankruptcy Act 1966 (Cth)","Insolvency and Trustee Service Australia","OPEX","No"]
[null,"Biodiversity Conservation Act 2016 (NSW)","Environmental assessment where threatened species may be impacted.","CAPEX for new installations, repairs or replacement","No"]
[null,"Biosecurity (Human Biosecurity Emergency) (Human Coronavirus with Pandemic Potential) (Overseas Travel Ban Emergency Requirements) Determination 2020 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Biosecurity (Listed Human Diseases) Amendment Determination 2020 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Biosecurity Act 2015 (Cth)","Obligations to comply with biosecurity control orders and related requirements","Opex","No"]
[null,"Building and Construction Industry Long Service Payments Act 1986 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Building and Construction Industry Security of Payment Act 1999 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Building Energy Efficiency Disclosure Act 2010 (Cth)","Requirements in relation to energy efficiency certificates for buildings.","OPEX","No"]
[null,"Building Products (Safety) Act 2017 (NSW)","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Civil Aviation Act 1988 (Cth)","Network operations including drones and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Civil Liability Act (NSW) 2002","Provides for claims and other matters","OPEX","No"]
[null,"Clean Energy Legislation (Carbon Tax Repeal) Act 2014 (Cth)","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Coal Mine Subsidence Compensation Act 2017 (NSW)","Regulates development within mine subsidence areas","CAPEX for new installations, repairs or replacement","No"]
[null,"Coastal Management Act 2016 (NSW)","Regulates works in coastal zone and provides for  Coastal Management Plans","Opex","No"]
[null,"Coastal Protection Act 1979 (NSW) and Coastal Protection Regulation 2011","Obtain approval to carry out development within specified parts of coastal zone if required","CAPEX for new installations, repairs or replacement","No"]
[null,"Community Land Development Act 1989 (NSW)","Development of land for electrical infrastructure, field and customer service centres","CAPEX for acquisitions","No"]
[null,"Community Land Management Act 1989 (NSW)","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Competition and Consumer Act 2010 (Cth)","Competition and consumer protection","OPEX","No"]
[null,"Contaminated Land Management Act 1997 (NSW)","Development of land for electrical infrastructure, field and customer service centres","CAPEX for acquisitions","No"]
[null,"Contaminated Land Management Act 1997 (NSW) and Contaminated Land Management Regulations 2013","Remediation of sites","CAPEX for new installations, repairs or replacement","No"]
[null,"Conveyancing Act 1919 (NSW)","Application of general rules affecting property, sales, transactions, mortgages, leases etc","CAPEX for acquisitions","No"]
[null,"Conveyancing Legislation Amendment Act 2018 (NSW)","Review for strategic property management","CAPEX for new installations","No"]
[]
[null,"Conveyancing Legislation Amendment Act 2018 (NSW) No 75","Review for strategic property management","CAPEX for new installations","No"]
[null,"Copyright Act 1968 (Cth)","Comply with obligations imposed by Act in relation to the use of copyright material including obtaining copyright licences.","OPEX","No"]
[null,"Coronavirus Economic Response Package (Payments and Benefits) Act 2020","Workplace and employment obligations, and related process","OPEX","No"]
[]
[null,"Coronavirus Economic Response Package Omnibus (Measures No. 1) Act 2020 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[]
[null,"Coronavirus Economic Response Package Omnibus (Measures No. 2) Act 2020","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Corporations (Fees) Act 2001 (Cth)","Regulates Australian corporations","OPEX","No"]
[null,"Corporations Act 2001 (Cth)","Regulates Australian corporations","OPEX","No"]
[null,"Corporations Amendment (Strengthening Protections for Employee Entitlements) Act 2010","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Court Suppression and Non-publication Orders Act 2010 No 106","Requirement for Australian business","OPEX","No"]
[null,"Crimes Act 1900 (NSW)","Requirement for Australian business","OPEX","No"]
[null,"Criminal Records Act 1991 (NSW)","Powers in relation to security of electricity infrastructure","CAPEX and OPEX","No"]
[null,"Crown Land Management Act 2016 (NSW)","Carrying out of activities on Crown land","CAPEX for acquisitions","No"]
[null,"Crown Lands Act 1989 (NSW)","Creation of line easement/access over crown lands","CAPEX for acquisitions","No"]
[null,"Dangerous Goods (Road and Rail Transport) Act 2008 (NSW)","Handling of hazardous and dangerous materials","OPEX","No"]
[null,"Defamation Act 2005 (NSW)","Requirement for Australian business","OPEX","No"]
[null,"Designs Act 2003 (Cth)","framework to register and protect  designs","OPEX","No"]
[null,"Disability Discrimination Act 1992 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Dividing Fences Act 1991 (NSW)","General requirements in relation to construction, operation, repair, maintenance and safety","CAPEX for acquisitions","No"]
[null,"Duties Act 1997 (NSW)","Payment of stamp and other duties","OPEX","No"]
[null,"Education Services for Overseas Students Act 2000 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Electricity (Consumer Safety) Act 2004 (NSW) and Electricity (Consumer Safety) Regulation 2015 (NSW)","Safety standards and requirements for customer electrical installations","CAPEX for new installations, repairs or replacement","No"]
[null,"Electricity Market Operation Rules (NSW)","Distribution network economic regulation, planning and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Electricity Network Assets (Authorised Transactions) Act 2015","Imposes obligations including certain employment guarantees following the long term lease of Ausgrid network in December 2016.","Opex","No"]
[null,"Electricity Retained Interest Corporations Act 2015 (NSW)","Establishment of the organisation","OPEX","No"]
[null,"Electricity Supply Act 1995 (NSW)","General requirements including operating licence requirements relating to operation, maintenance and safety of distribution networks.","CAPEX for new installations, repairs or replacement","No"]
[null,"Electronic Conveyancing (Adoption of National Law) Act 2012 (NSW)","Application of general rules affecting property, sales, transactions, mortgages, leases etc","CAPEX for acquisitions","No"]
[null,"Electronic Transactions Act 1999 (Cth)","Application of privacy laws and related process","OPEX","No"]
[null,"Electronic Transactions Act 2000 (NSW)","Establishment of the organisation","OPEX","No"]
[null,"Employees Liability Act 1991 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Employment Protection Act 1982 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Encroachment of Buildings Act 1922 (NSW)","Environmental planning, assessment and consultation","CAPEX for acquisitions","No"]
[null,"Energy and Utilities Administration Act 1987 (NSW)","Make annual payments to Climate Change Fund as specified in order by Minister.  (Ausgrid is not a designated energy user)","OPEX","No"]
[null,"Environment Protection and Biodiversity Conservation Act 1999 (Cth)","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Environmental Planning and Assessment Act 1979 (NSW)","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Environmentally Hazardous Chemicals Act 1985 (NSW)","Management of environmentally hazardous chemicals and chemical waste","OPEX","No"]
[null,"Essential Services Act 1988 (NSW)","Comply with orders and requirements following declaration of emergency in relation to essential service.","OPEX","No"]
[null,"Evidence Act 1995 (NSW)","Requirement for Australian business","OPEX","No"]
[null,"Fair Trading Act 1987 (NSW)","Provides for claims and other matters in relation to provision of services to consumers. .","OPEX","No"]
[null,"Fair Work Act 2009 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Fisheries Management Act 1994 (NSW)","Environmental planning, assessment and consultation for dredging and reclamation works in wetlands and other waterways","OPEX","No"]
[null,"Forestry Act 2012 (NSW)","Comply with all requirements relating to activities in State Forests, Timbers Reserves and Flora Reserves.","CAPEX for new installations, repairs or replacement","No"]
[null,"Fringe Benefits Tax Act 1986 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Fringe Benefits Tax Assessment Act 1986 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Fuel Tax Act 2006 (Cth)","Network operations and safety practices","OPEX","No"]
[null,"Gas and Electricity (Consumer Safety) Act 2017 (NSW)","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Government Telecommunications Act 1991 (NSW)","NSW Government Telecommunications Authority","OPEX","No"]
[null,"Greenhouse and Energy Minimum Standards Act 2012Â (Cth)","national framework for product energy efficiency","OPEX","No"]
[null,"Health Records and Information Privacy Act 2002 (NSW)","Application of privacy laws and related process","OPEX","No"]
[null,"Heavy Vehicle National Law 2014 (NSW)","Regulation of Heavy Vehicles","Opex","No"]
[null,"Heritage Act 1977 (NSW)","Heritage consideration in relation to historic, scientific, cultural, social, archaeological, architectural, natural or aesthetic significance.","CAPEX for new installations, repairs or replacement","No"]
[null,"Home Building Act 1989 (NSW)","Licensing to under work, including electrical work, in residential premises  (at customer premises for inspection or in emergency)","CAPEX for new installations, repairs or replacement","No"]
[null,"Hunter Water Act 1991 (NSW)","Obtain approval to connect a sewer or drain to a public sewer or drain.","CAPEX for new installations, repairs or replacement","No"]
[null,"Inclosed Lands Protection Act 1901 (Cth)","Network operations and safety practices","OPEX","No"]
[null,"Income Tax Act 1986 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Income Tax Assessment Act 1936 (Cth) and Income Tax Assessment Act 1997 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Independent Contractors Act 2006 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Independent Pricing and Regulatory Tribunal Act 1992 (NSW)","IPART Requirement","OPEX","No"]
[null,"Industrial Relations (Child Employment) Act 2006 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Industrial Relations Act 1996 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Insurance Act 1973 (Cth)","Regulates Contracts for Insurance","Opex","No"]
[null,"Insurance Contracts Act 1984 (Cth)","Regulates Contracts for Insurance","Opex","No"]
[null,"Jury Act 1977 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Land Acquisition (Just Terms Compensation) Act 1991 (NSW)","Process and compensation for compulsory acquisition of land for electricity system infrastructure","CAPEX for acquisitions","No"]
[null,"Land and Environment Court Act 1979 (NSW)","Property management related","CAPEX for new installations","No"]
[null,"Land Tax Act 1956 (NSW)","Property management related","CAPEX for new installations","No"]
[null,"Land Tax Management Act 1956 (NSW)","Payment of land tax","OPEX","No"]
[null,"Local Government Act 1993 (NSW)","Development of land for construction of zone substations or other electricity system infrastructure","CAPEX for new installations, repairs or replacement","No"]
[null,"Local Government Amendment (Governance and Planning) 2016 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Local Land Services Act 2013 (NSW)","Regulates clearing of native vegetation and other activities in certain rural areas.","CAPEX for new installations, repairs or replacement","No"]
[null,"Long Service Leave Act 1955 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Marine Estate Management Act 2014 (NSW)","Regulates development in Marine Parks and  aquatic reserves","Opex","No"]
[null,"Marine Pollution Act 2012 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Marine Safety Act 1998 (NSW)","Implementation of workplace safety systems, plans, strategies, practices","OPEX","No"]
[null,"Modern Slavery  Act 2019 (Cth)","Network operations and safety practices","OPEX","No"]
[null,"Modern Slavery Act 2018 (NSW)","Network operations and safety practices","OPEX","No"]
[null,"Multicultural NSW Act 2000 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Mutual Recognition (Automatic Licensed Occupations Recognition) Act 2014 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"National Electricity (New South Wales) Act 1997 (NSW), National Electricity Law and National Electricity Rules","Compliance with National Electricity Law as a law in NSW","CAPEX for new installations, repairs or replacement","No"]
[null,"National Energy Retail Law (NSW) and National Energy Retail Rules","Customer connection contracts, customer complaints and dispute resolution, RoLR, customer connection services, obligations in relation to the provision of customer connection services, re-energisation, de-energisation planned and unplanned interruptions, d","Opex","No"]
[null,"National Energy Retail Law 2012 (NSW)","NSW specific distributor liability, regimen and requirements for planned interruptions under the National Energy Retail Law and Rules","CAPEX for new installations, repairs or replacement","No"]
[null,"National Environment Protection Council (New South Wales) Act 1995 (NSW)","National Environment Protection Measures may includes guidelines relevant to network operator activities.","OPEX","No"]
[null,"National Environment Protection Measures (Implementation) Act 1998 (Cth)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"National Greenhouse and Energy Reporting Act 2007 (Cth)","Obligations in relation to reporting on greenhouse gas emissions.","OPEX","No"]
[null,"National Measurement Act 1960 (Cth)","Energy metering and accuracy","OPEX","No"]
[null,"National Parks and Wildlife Act 1974 (NSW)","Environmental planning, assessment and consultation- national parks, historic sites, nature reserves and aboriginal sites.","CAPEX for new installations, repairs or replacement","No"]
[null,"National Vocational Education and Training Regulator Act 2011 (Cth)","Implementation of workplace safety systems, plans, strategies, practices","OPEX","No"]
[null,"Native Title (New South Wales) Act 1994 (NSW)","Process for assessment of Native Title Claims","CAPEX for new installations, repairs or replacement","No"]
[null,"Native Title Act 1993 (Cth)","Management of native title and claims","CAPEX for new installations, repairs or replacement","No"]
[null,"Natural Resources Commission Act 2003 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Ozone Protection Act 1989 (NSW)","Management of equipment with substances that deplete stratospheric ozone","OPEX","No"]
[null,"Ozone Protection and Synthetic Greenhouse Gas Management Act 1989 (Cth)","Management of Equipment with substances that deplete stratospheric ozone","Opex","No"]
[null,"Paid Parental Leave Act 2010 (Cth)","Regulates registered training organisations.","OPEX","No"]
[null,"Paid Parental Leave Amendment (Work Test) Act 2019 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Partnership Act 1892 (NSW) and Partnership Regulation 2017","Establishment of the organisation","OPEX","No"]
[null,"Payment Times Reporting Act 2020","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Payroll Tax Act 2007 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Personal Property Securities Act 2009 (Cth)","Provides scheme for securing interests in personal property","Opex","No"]
[null,"Pesticides Act 1999 (NSW)","Use and management of pesticides for treatment of termites","CAPEX for new installations, repairs or replacement","No"]
[null,"Place Management NSW Act 1998 (NSW)","Regulates certain development in foreshore areas managed by Place Management NSW","CAPEX for new installations, repairs or replacement","No"]
[null,"Plant Diseases Act 1924 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Powers of Attorney Act 2003 and Powers of Attorney Regulation 2016","Establishment of the organisation","OPEX","No"]
[null,"Privacy Act 1988 (Cth)","Application of privacy laws and related process","OPEX","No"]
[null,"Property, Stock and Business Agents Act 2002 (NSW)","Property management related","CAPEX for new installations","No"]
[null,"Protection of the Environment Administration Act 1991 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Protection of the Environment Operations (Noise Control) Regulation 2017 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Protection of the Environment Operations (Underground Petroleum Storage Systems) Regulation 2014","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Protection of the Environment Operations (Waste) Regulation 2014 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Protection of the Environment Operations Act 1997 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Protection of the Environment Operations Amendment (Asbestos Waste) Act 2018 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Public Health (COVID-19 Gatherings) Order (No 2) 2020","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Public Health (COVID-19 Quarantine) Order 2020 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Racial Discrimination Act 1975 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Radiation Control Act 1990 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Radio Communications Act 1992 (Cth)","Governs Licensing of radio spectrum","Opex","No"]
[null,"Rail Safety National Law 2012 (NSW) and Rail Safety (Adoption of National Law) Act 2012","Network operations and safety practices","OPEX","No"]
[null,"Real Property Act 1900 (NSW)","Application of general requirements relating to land transactions","CAPEX for acquisitions","No"]
[null,"Renewable Energy (Electricity) Act 2000 (Cth)","encourage the additional generation of electricity from renewable sources","CAPEX for new installations","No"]
[null,"Residential Tenancies Act 2010 (NSW)","Property management related","CAPEX for new installations","No"]
[null,"Retail Leases Act 1994 (NSW)","Application of general requirements relating to land transactions","OPEX for inspections, maintenance and administration","No"]
[null,"Road Transport Act 2013 (NSW)","Registration of fleet vehicles, driver licensing and other matters.","OPEX","No"]
[null,"Roads Act 1993 (NSW)","Regulates erection of structures on certain public roads","CAPEX for new installations, repairs or replacement","No"]
[null,"Rural Fires Act 1997 (NSW)","Comply with any steps notified to Ausgrid and any other practicable steps notified by the Bush Fire Co-ordinating Committee to prevent bush fires occurring and minimise danger of spread of bushfires from Ausgridâ\u0080\u0099s land.","OPEX","No"]
[null,"Security Industry Act 1997 (NSW)","Security licensing  obligations","OPEX","No"]
[null,"Security of Critical Infrastructure (Consequential and Transitional Provisions) Act 2018 (Cth)","Powers in relation to security of electricity infrastructure","CAPEX and OPEX","No"]
[null,"Security of Critical Infrastructure Act 2018 (Cth)","Powers in relation to security of electricity infrastructure","CAPEX and OPEX","No"]
[null,"Service and Installation Rules of New South Wales","Network operations and safety practices","OPEX","No"]
[null,"Sex Discrimination Act 1984 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Smoke-Free Environment Act 2000 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Soil Conservation Act 1938 (NSW)","Miscellaneous environmental obligations","OPEX","No"]
[null,"State Emergency and Rescue Management Act 1989 (NSW)","Comply with directions to disconnect power supply during emergency.","OPEX","No"]
[null,"State Environmental Planning Policy (Infrastructure) 2007 (SEPP Infrastructure","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"State Environmental Planning Policy (State and Regional Development) 2011","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"State Environmental Planning Policy (Sydney Drinking Water Catchment) 2011","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"State Environmental Planning Policy (Vegetation in Non-Rural Areas) 2017","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"State Records Act 1998 (NSW) and State Records Regulation 2015","Records management","OPEX","No"]
[null,"Statute Law (Miscellaneous Provisions) Act 2019 (NSW) No 1","Requirement for Australian business","OPEX","No"]
[null,"Strata Scheme Management Act 2015 (NSW)","To ensure fair and efficient dealings between parties to retail leases","CAPEX for acquisitions","No"]
[null,"Superannuation Contributions Tax (Assessment and Collection) Act 1997 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Superannuation Contributions Tax Imposition Act 1997 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Superannuation Guarantee (Administration) Act 1992 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Superannuation Guarantee Charge Act 1992 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Superannuation Industry (Supervision) Act 1993 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Surveillance Devices Act 2007 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Sydney Olympic Park Authority Act and Sydney Olympic Park Regulation 2012","Regulates certain activities in Sydney Olympic Park","CAPEX for new installations, repairs or replacement","No"]
[null,"Sydney Water Act 1994 (NSW) and Sydney Water Regulation 2017","Obtain approval of Sydney Water to connect a drain or sewer to a public drain or sewer.","OPEX","No"]
[null,"Taxation Administration Act 1953 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Taxation Administration Act 1996 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Telecommunications (Interception and Access) Act 1979 (Cth)","Licensing as a carrier and nominated carrier Application of privacy laws and related process","OPEX","No"]
[null,"Treasury Laws Amendment (Consumer Data Right) Act (Cth) 2019","Application of privacy laws and related process","OPEX","No"]
[null,"Valuation of Land Act 1916 (NSW)","Property management related","CAPEX for new installations","No"]
[null,"Valuers Act 2003 (NSW)","Property management related","CAPEX for new installations","No"]
[null,"Waste Avoidance and Resource Recovery Act 2001 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Water Act 1912 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Water Act 2014 (NSW) and Water NSW Regulation 2013","Requires approval to work in special and controlled areas","CAPEX for new installations, repairs or replacement","No"]
[null,"Water Management Act 2000 (NSW)","Environmental planning, assessment and consultation - protection of water sources/quality","CAPEX for new installations, repairs or replacement","No"]
[null,"Water NSW Act 2014 (NSW)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Wilderness Act 1987 (NSW)","Environmental Planning, Assessment and Consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Work Health and Safety Act 2011 (NSW)","Workplace and employment obligations, and related process","CAPEX for new installations, repairs or replacement","No"]
[null,"Workers Compensation (Dust Diseases) Act 1942 (NSW)","Workplace and employment obligations, and related process","OPEX for inspections, maintenance and administration","No"]
[null,"Workers Compensation Act 1987 (NSW)","Process for workplace injury claims related to dust diseases","Opex","No"]
[null,"Workplace Gender Equality Act 2012 (Cth)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Workplace Injury Management and Workers Compensation Act 1998 (NSW)","Workplace and employment obligations, and related process","OPEX","No"]
[null,"Workplace Surveillance Act 2005 (NSW)","The compliance requirement is the application of a health and safety management system and the general design requirements relating to electrical plant.","OPEX","No"]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"Aboriginal Heritage Impact Permit (Various)","Miscellaneous environmental obligations","CAPEX for new installations, repairs or replacement","No"]
[null,"Carrier Licence and Nominated Carrier Declaration under Telecommunications Act, 1997 (Cwth)","Operation of telecommunications assets forming part of distribution network","Opex","No"]
[null,"Environment Protection Licences (Various)","Various licences required by Environment Protection legislation","Opex","No"]
[null,"National Electricity Market Registration as Network Operator and Metering Coordinator (Limited).","Operate in National Electricity Market","Opex","No"]
[null,"RULES"]
[null,"National Electricity Rules","Distribution network economic regulation, planning and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"National Energy Retail Rules","Connection services to retail customers and other operations","OPEX","No"]
[null,"NSW â\u0080\u0093 Electricity Market Operation Rules","Rules for B2B Communications in NEM","CAPEX for new installations, repairs or replacement","No"]
[null,"Trade Support Loans Act 2014 (Cth)","Customer electricity equipment and installation - safety and compliance","CAPEX for new installations, repairs or replacement","No"]
[null,"ORDERS"]
[]
[]
[]
[null,"CODES"]
[null,"Code of Practice for the Safe Removal of Asbestos","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"National Electricity Network Safety Code","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"National Guidelines for Aerial Surveillance of Overhead Electricity Networks ENA NENS 08-2004","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"NSW Code of Practice for Authorised Network Operators â\u0080\u0093 NSW Planning and Environment September 2015","Relating to Environmental assessment under Part 5 of the Environmental Planning and Assessment Act 1979","CAPEX for new installations, repairs or replacement","No"]
[null,"NSW Public Lighting Code","Published Minimum Service supply standards","CAPEX for new installations, repairs or replacement","No"]
[null,"SafeWork NSW Code of Practice: Managing Electrical Risks","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"SafeWork NSW, Code of Practice: How to Safely Remove Asbestos","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"SafeWork NSW, Code of Practice: Labelling of workplace hazardous chemicals","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"SafeWork NSW, Code of Practice: Managing risks of hazardous chemicals in the workplace","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"SafeWork NSW, Code of Practice: Preparation of safety data sheets for hazardous chemicals","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"AER Connection Charge Guidelines made under clause 5A.","AER Guidelines for setting out the circumstances in which customers must pay connection charges.","OPEX","No"]
[null,"AER Ring Fencing Guidelines Â made under 6.20 of the National Electricity Rules","AER Guidelines regarding separation of the provision of distribution services and other services.","OPEX","No"]
[null,"All other relevant National Occupational Health and Safety Commission  (NOHSC) guidelines and documents","Safety standards, design and constructions standards","CAPEX for new installations, repairs or replacement","No"]
[null,"All relevant AS/NZS Australian Standards as per National Electricity Network Safety Code S01 (NENS01)","Asset management, and design and construction standards","CAPEX for new installations, repairs or replacement","No"]
[null,"All relevant ESAA guidelines as per NENS01","Asset management, and design and construction standards","CAPEX for new installations, repairs or replacement","No"]
[null,"All relevant HB series of standards","Coordination of power and telecommunications","CAPEX for new installations, repairs or replacement","No"]
[null,"All relevant IEC standards","Asset management, and design and construction standards","CAPEX for new installations, repairs or replacement","No"]
[null,"All relevant IEEE standards","Asset management, and design and construction standards","CAPEX for new installations, repairs or replacement","No"]
[null,"ANSI/IEEE C95.6-2019 Institute of Electrical and Electronics Engineers, Standard for Safety Levels With Respect to Human Exposure to Electromagnetic Fields","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 1319:1994  Australian Standard, Safety signs for the occupational environment","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 1345:1995 Australian Standard, Identification of the contents of pipes, conduits and ducts","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 1940:2017 Australian Standard, The storage and handling of flammable and combustible liquids","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 2067:2016 Australian Standard, Substations and high voltage installations exceeding 1 kV a.c.","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 4332:2004 Australian Standard, The storage and handling of gases in cylinders, Reconfirmed 2016","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 4361.1:2017 Australian Standard, Guide to hazardous paint management - Lead and other hazardous metallic pigments in industrial applications","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 4373:2007 Australian Standard, Pruning of amenity trees (Reconfirmed 2020)","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 4874:2000  Australian Standard, Guide to the investigation of potentially contaminated soil and deposited dust as source of lead available to humans","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 5577:2013 Australian Standard, Electricity network safety management systems","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 5804.1:2010 Australian Standard, High-voltage live working - General","Line design and construction, environmental planning and assessment","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 5804.2:2010 Australian Standard, High-voltage live working - Glove and barrier work","Line design and construction, environmental planning and assessment","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 5804.3:2010 Australian Standard, High-voltage live working - Stick work","Line design and construction, environmental planning and assessment","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 5804.4:2010 Australian Standard, High-voltage live working - Barehand work","Line design and construction, environmental planning and assessment","CAPEX for new installations, repairs or replacement","No"]
[null,"AS 6947:2009 Australian Standard, Crossing of waterways by electricity infrastructure (Reconfirmed 2019)","Line design and construction, environmental planning and assessment","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 1418.10:2011 Australian Standard, Cranes, hoists and winches - Mobile elevating work platforms - Plus Amendment 2017","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 1715:2009 Australian Standard, Selection, use and maintenance of respiratory protective equipment","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 1716:2012 Australian Standard, Respiratory protective devices","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 3017:2022 Australian Standard, Electrical Installations - Verification Guidelines","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 3019:2022 Australian Standard, Electrical installations - Periodic assessment","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 3935.1:2016 Australian Standard, Earth Potential Rise-Protection of telecommunications network users, personnel and plant - Code of Practice","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"AS/NZS 7000:2016 Australian Standard, Overhead Line Design","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Australian and New Zealand Environment and Conservation Council, Australian and New Zealand Guidelines ANZECC & ARMCANZ (2002) for Fresh and Marine Water Quality","Network operations and safety practices","CAPEX for new installations, repairs or replacement","No"]
[null,"Australian Pesticides and Veterinary Medicines Authority (APVMA), Agricultural and Veterinary Chemicals Code, no date","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"CIGRE, Guide for the operation of self-contained fluid filled cable systems, 2016","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"City of Sydney, Construction Hours/Noise within the Central Business District Code of Practice, 1992","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Clean Energy Regulator, NGER Scheme Measurement Technical Guidelines for the estimation of emissions by facilities in Australia, 2017","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Crossings of NSW Navigable Waters: Electricity Industry Code - 2011","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"Current Rating of Bare Overhead Line Conductors, ESAA D(b)5","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"DECC, Storing and handling liquids: environmental protection Participantâ\u0080\u0099s manual, 2007","Environmental planning, assessment and consultation","CAPEX for new installations, repairs or replacement","No"]
[null,"DEFAULT AGREEMENTS "]
[null,"Ausgrid Deemed Customer Connection Contract","Ongoing Connection Services Contract","Opex","No"]
[]
[]
[null,"OTHER"]

{"sheet":"7.4 Shared Assets","index":27,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[40,2,40,8],[32,2,32,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[29,2,29,8],[30,2,30,8],[31,2,31,8],[38,2,38,8],[39,2,39,8],[6,1,7,1],[6,2,7,2],[26,2,26,8],[27,2,27,8],[28,2,28,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service",{"$f":"CONCATENATE(\"Shared asset unregulated revenue  \n($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", FRCP_y5)","v":"Total 2024-25 to 2028-29"}]
[null,"Property Unregulated Revenue (shared assets)","Ausgrid owned system land and buildings leased to external tenants",2168261,1445663,1882107,1809672,1553168,1530339,1466213,{"$f":"SUM(F9:J9)","v":8241499}]
[null,"Pole & Duct Rental (Shared Assets)","Overhead poles, underground ducts, substations, high voltage towers, power poles, on which telecommunications or electric vehicle chargers are installed",21038220,23978340,26831196,29196480,33340670,33500668,34873460,157742474]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]
[null,"N/A","N/A"]

{"sheet":"7.7 TSS-LRMC","index":28,"n_rows":154,"n_cols":22,"rows_kept":154,"cut":false,"hidden":false,"merged":[[68,1,69,1],[88,1,89,1],[5,3,6,4],[10,1,11,1],[22,1,23,1],[34,1,35,1],[48,1,49,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is Ausgrid using the 'Average Incremental Cost' approach?"}]
[null,null,null,null,null,"YES"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C12,4)+1)&\"-\"&MID(C12,3,2)+2),VALUE(LEFT(C12,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure",null,null,15026134,16458829,22775084,12598317,12154884,12154884,12154884,12154884,12154884,12154884]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C13:C19)","v":0},0,15026134,16458829,22775084,12598317,12154884,12154884,12154884,12154884,12154884,12154884,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C24,4)+1)&\"-\"&MID(C24,3,2)+2),VALUE(LEFT(C24,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C25:C31)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C36,4)+1)&\"-\"&MID(C36,3,2)+2),VALUE(LEFT(C36,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex",{"$f":"SUM(C36:C42)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C50,4)+1)&\"-\"&MID(C50,3,2)+2),VALUE(LEFT(C50,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[null,"Incremental opex associated with growth related capex",null,null,292173,320031,442847,244966,236344,236344,236344,236344,236344,236344]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C51:C65)","v":0},0,292173,320031,442847,244966,236344,236344,236344,236344,236344,236344,0,0,0,0,0,0,0,0]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C70,4)+1)&\"-\"&MID(C70,3,2)+2),VALUE(LEFT(C70,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C71:C85)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C90,4)+1)&\"-\"&MID(C90,3,2)+2),VALUE(LEFT(C90,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C91:C105)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C113,4)+1)&\"-\"&MID(C113,3,2)+2),VALUE(LEFT(C113,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[null,"Aggregated demand - all voltage levels",null,4042,4071,4100,4131,4163,4195,4228,4263,4298,4334,4372]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C114:C123)","v":0},-4042,-4071,-4100,-4131,-4163,-4195,-4228,-4263,-4298,-4334,-4372,0,0,0,0,0,0,0,0]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C128,4)+1)&\"-\"&MID(C128,3,2)+2),VALUE(LEFT(C128,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C129:C138)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C143,4)+1)&\"-\"&MID(C143,3,2)+2),VALUE(LEFT(C143,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"-SUM(C144:C153)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"7.8 Export Services","index":29,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.8 EXPORT SERVICES"]
[]
[null,"Expenditure must only be related to DER integration, and must exclude amounts relating to DMIA"]
[]
[null,"Export service related overvoltage complaint management\nexamples include but not limited to: complaint processing, analysis, transformer tapping "]
[]
[null,"7.8.1 - OPEX FOR PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Export service related overvoltage complaint management"]
[null,"Other opex",null,null,2938716.49,3891483.79,3999843.26,3999843.26,4235628.9000000004]
[]
[]
[null,"ICT capex\nexamples include but not limited to: establishing systems for network visibility, hosting capacity assessments, generation of dynamic operating envelopes"]
[null,"Network monitoring capex\nexamples include but not limited to: implementing transformer monitors"]
[]
[null,"7.8.2 - CAPEX FOR THE PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"ICT capex",null,null,4201118.63,4201118.63,135693.89000000001,135693.89000000001,79529.2]
[null,"Network monitoring capex"]
[null,"Other capex",null,null,5990373.6299999999,5514270.1799999997,5312335.07,5114832.13,4901029.46]
[]
[]
[]
[]
[null,"7.8.3 - EXPORT VOLUMES - NET METERED VOLUME OF ENERGY EXPORTED"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"VOLUMES\nMWh"]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,481,562,631,675,711,740]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,1058787,1325052,1446032,1524208,1586567,1638725]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,357965,433779,479659,509306,532954,552734]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,3313,3872,4347,4654,4898,5103]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C45,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},481,562,631,675,711,740,769]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1058787,1325052,1446032,1524208,1586567,1638725,1688477]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},357965,433779,479659,509306,532954,552734,571602]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},3313,3872,4347,4654,4898,5103,5299]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[]
[]
[null,"7.8.4 EXPORT SERVICES - CUSTOMER NUMBERS"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"CUSTOMER NUMBERS\n(0's)"]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},75,87,95,102,108,115,121]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},173021,201245,219813,234856,249754,264245,278594]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},65042,75652,82632,88287,93888,99335,104729]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},732,851,930,993,1056,1118,1178]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C63,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},87,95,102,108,115,121,127]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},201245,219813,234856,249754,264245,278594,293027]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},75652,82632,88287,93888,99335,104729,110155]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},851,930,993,1056,1118,1178,1239]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]

{"sheet":"AER Sheet Heading","index":30,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"}]
[null,{"$f":"dms_Header_Span","v":"2022-23 to 2028-29"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2024)"}]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C15:C35)","v":0},0,0,0,0,0,0]
[null,null,{"$f":"SUM(C15:C36)","v":0},0,0,0,0,0,0]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C46:C66)","v":0},0,0,0,0,0,0]
[null,null,{"$f":"SUM(C46:C67)","v":0},0,0,0,0,0,0]

{"sheet":"AER CF","index":31,"n_rows":77,"n_cols":25,"rows_kept":77,"cut":false,"hidden":true,"merged":[[3,1,3,22],[39,38,39,59],[40,38,40,59],[41,38,41,59],[39,69,39,90],[40,69,40,90],[41,69,41,90]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[null,"CELLS FLAGED \"Y\" and greyed out will be greyed out in the worksheets."]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":true},"=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",null,null,"=INDEX(dms_CF_F10, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6.1","dms_CF_3.6.6.2","dms_CF_3.6.6.3","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.8 (set from dms_MAIFI_flag)","dms_CF_7.12","dms_CF_8.1_A  (and 8.4)","dms_CF_8.1_B  (and 8.4)","dms_CF_8.1_Neg  (and 8.4)","dms_CF_4.4.1","dms_CF_MAIFI_flag (set from dms_MAIFI_flag)","9.5 TUOS (set from Jurisdiction)","dms_CF_F10"]
[null,"Amadeus","NT","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"APA GasNet","Vic","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C7=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ausgrid (Tx Assets)","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C8=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C9=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","Y","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C10=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co.","NSW","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C13=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co. (Vic)","Vic","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C14=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C15=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C16=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C17=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C18=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Energex","Qld","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C19=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C20=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C21=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C22=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution (Tx Assets)","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C23=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C25=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"JGN","Vic","Gas","Distribution","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C26=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Power and Water","NT","Electricity","Distribution",null,"N","N",null,null,"N","Y","N","N","N","Y",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","Y","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C27=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C28=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C29=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Roma to Brisbane Pipeline","Qld","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","N","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C31=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C32=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C33=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C34=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"United Energy","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C35=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE","dms_H2"]
[null,"TOP HEADER","dms_H1"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,5.1109999999999998,"dms_NUM"]
[null,5.45E-2,"dms_NUM%"]
[null,5.5555000000000003,"dms_NUM3d"]
[null,"Text description","dms_Row_Locked"]
[null,"Text description - not locked","dms_Row1"]
[null,"Text description","dms_Row2"]
[null,"Total","dms_T1"]
[null,"Total","dms_T2"]
[null,"EXPENSES","dms_BH"]
[null,2019,"dms_BY1"]
[null,2019,"dms_BY2"]
[null,"VOLUMES","dms_GH"]
[null,2019,"dms_GY1"]
[null,2019,"dms_GY2"]

{"sheet":"AER NRs","index":32,"n_rows":232,"n_cols":16,"rows_kept":232,"cut":false,"hidden":true,"merged":[[4,1,28,1],[176,1,177,1],[179,1,184,1],[65,1,78,1],[135,1,150,1],[84,1,97,1],[152,1,158,1],[118,1,132,1],[208,1,213,1],[199,1,200,1],[32,1,55,1],[100,1,107,1],[110,1,115,1],[191,1,192,1],[195,1,196,1],[160,1,174,1],[33,67,33,88],[34,67,34,88],[35,67,35,88],[36,10,40,10],[44,10,45,10],[33,10,35,10],[33,36,33,57],[34,36,34,57],[35,36,35,57]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Tariff cap"]
[null,null,"Final decision","Weighted average price cap"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Reallocated"]
[null,null,"Recast"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[null,null,null,null,null,null,null,null,null,null,null,null,"GAS ARR & RESET"]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140201_UOM","dms_E050201_UOM","dms_E050202_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number per km","per metre per connection","metres per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","per service per connection","number per connection"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number per connection","number per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","dms_E020202_UOM","Spare"]
[null,null,"number","number","Length of mains replaced"]
[null,null,"number","number","Number of services replaced"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)"]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":{"$error":"#NAME?"}}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]
[]
[]
[]
[null,"PTRM input sheet","DMS_50_01_01a","DMS_50_01_01aa","DMS_50_01_01b","DMS_50_01_01bb","DMS_50_01_01c","DMS_50_01_01d","DMS_50_01_01dd"]

{"sheet":"AER lookups","index":33,"n_rows":101,"n_cols":37,"rows_kept":101,"cut":false,"hidden":true,"merged":[[15,60,15,81],[22,1,22,4],[4,24,4,35],[5,24,5,27],[5,29,7,33],[5,34,7,34],[5,35,7,35],[5,36,7,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Template number",5]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_MAIFI_flag_List","dms_Public_Lighting_List","Name"]
[null,"Ausgrid","Ausgrid",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES",{"$f":"B10","v":"Ausgrid"}]
[null,"Ausgrid (Tx Assets)","Ausgrid (Tx Assets)",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Ausgrid (Tx Assets)"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Australian Distribution Co."]
[null,"Endeavour Energy","Endeavour Energy",11247365823,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"51 Huntingwood Drive",null,"HUNTINGWOOD","NSW",2148,"PO Box 811",null,"SEVEN HILLS","NSW",1730,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Endeavour Energy"]
[null,"Essential Energy","Essential Energy",37428185226,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"8 Buller Street",null,"PORT MACQUARIE","NSW",2444,"PO Box 5730",null,"PORT MACQUARIE","NSW",2444,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Essential Energy"]
[null,"Evoenergy Distribution","Evoenergy Distribution",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"NO","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Evoenergy Distribution"]
[null,"Evoenergy Distribution (Tx Assets)","Evoenergy Distribution (Tx Assets)",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"NO","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Evoenergy Distribution (Tx Assets)"]
[null,"Power and Water","Power and Water Corporation",15947352360,"NT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"x","GPO Box 1921",null,"DARWIN","NT",801,"GPO Box 1921",null,"DARWIN","NT",801,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Power and Water"]
[null,"TasNetworks (D)","TasNetworks (D)",24167357299,"Tas","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,"YES","YES","YES","YES","YES","Critical Infrastructure","Urban","High density commercial","High density rural","Low density rural","NO","YES","TasNetworks (D)"]
[]
[]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"EBSS","Efficiency Benefit Sharing Scheme","EFFICIENCY BENEFIT SHARING SCHEME",5]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"Profitability","Profitability","PROFITABILITY",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88",1988,"PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2014-15"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2019-20"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2024-25"}]
[null,"1988-89",1989,"PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2015-16"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2020-21"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2025-26"}]
[null,"1989-90",1990,"PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2016-17"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2021-22"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2026-27"}]
[null,"1990-91",1991,"PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2017-18"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2022-23"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2027-28"}]
[null,"1991-92",1992,"PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2018-19"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2023-24"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2028-29"}]
[null,"1992-93",1993,"PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2019-20"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2024-25"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2029-30"}]
[null,"1993-94",1994,"PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2020-21"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2025-26"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2030-31"}]
[null,"1994-95",1995,"PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2021-22"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2026-27"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2031-32"}]
[null,"1995-96",1996,"PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2022-23"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2027-28"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2032-33"}]
[null,"1996-97",1997,"PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2023-24"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2028-29"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2033-34"}]
[null,"1997-98",1998,"PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2024-25"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2029-30"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2034-35"}]
[null,"1998-99",1999,"PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2025-26"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2030-31"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2035-36"}]
[null,"1999-00",2000,"PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2026-27"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2031-32"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2036-37"}]
[null,"2000-01",2001,"PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2027-28"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2032-33"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2037-38"}]
[null,"2001-02",2002,"PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2028-29"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2033-34"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2038-39"}]
[null,"2002-03",2003,"PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2029-30"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2034-35"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2039-40"}]
[null,"2003-04",2004,"PRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+16)","v":"2030-31"},"CRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+16)","v":"2035-36"},"FRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+16)","v":"2040-41"}]
[null,"2004-05",2005,"PRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+17)","v":"2031-32"},"CRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+17)","v":"2036-37"},"FRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+17)","v":"2041-42"}]
[null,"2005-06",2006,"PRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+18)","v":"2032-33"},"CRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+18)","v":"2037-38"},"FRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+18)","v":"2042-43"}]
[null,"2006-07",2007,"PRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+19)","v":"2033-34"},"CRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+19)","v":"2038-39"},"FRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+19)","v":"2043-44"}]
[null,"2007-08",2008,"PRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+20)","v":"2034-35"},"CRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+20)","v":"2039-40"},"FRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+20)","v":"2044-45"}]
[null,"2008-09",2009,"PRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+21)","v":"2035-36"},"CRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+21)","v":"2040-41"},"FRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+21)","v":"2045-46"}]
[null,"2009-10",2010,"PRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+22)","v":"2036-37"},"CRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+22)","v":"2041-42"},"FRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+22)","v":"2046-47"}]
[null,"2010-11",2011,"PRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+23)","v":"2037-38"},"CRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+23)","v":"2042-43"},"FRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+23)","v":"2047-48"}]
[null,"2011-12",2012,"PRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+24)","v":"2038-39"},"CRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+24)","v":"2043-44"},"FRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+24)","v":{"$error":"#REF!"}}]
[null,"2012-13",2013]
[null,"2013-14",2014]
[null,"2014-15",2015]
[null,"2015-16",2016]
[null,"2016-17",2017]
[null,"2017-18",2018]
[null,"2018-19",2019]
[null,"2019-20",2020]
[null,"2020-21",2021]
[null,"2021-22",2022,null,"CRY - FRY"]
[null,"2022-23",2023,"dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2022-23"}]
[null,"2023-24",2024,"dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2023-24"}]
[null,"2024-25",2025,"dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2024-25"}]
[null,"2025-26",2026,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2025-26"}]
[null,"2026-27",2027,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2026-27"}]
[null,"2027-28",2028,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2027-28"}]
[null,"2028-29",2029,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2028-29"}]
[null,"2029-30",2030,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2029-30"}]
[null,"2030-31",2031,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2030-31"}]
[null,"2031-32",2032,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2031-32"}]
[null,"2032-33",2033,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2032-33"}]
[null,"2033-34",2034,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2033-34"}]
[null,"2034-35",2035,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2034-35"}]
[null,"2035-36",2036,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2035-36"}]
[null,"2036-37",2037,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2036-37"}]
[null,"2037-38",2038,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2037-38"}]
[null,"2038-39",2039,"dms_y17",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+16),0)","v":"2038-39"}]
[null,"2039-40",2040,"dms_y18",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+17),0)","v":"2039-40"}]
[null,"2040-41",2041,"dms_y19",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+18),0)","v":"2040-41"}]
[null,"2041-42",2042,"dms_y20",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+19),0)","v":"2041-42"}]
[null,"2042-43",2043,"dms_y21",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+20),0)","v":"2042-43"}]
[null,"2043-44",2044,"dms_y22",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+21),0)","v":"2043-44"}]
[null,"2044-45",2045,"dms_y23",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+22),0)","v":"2044-45"}]
[null,"2045-46",2046,"dms_y24",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+23),0)","v":"2045-46"}]
[null,"2046-47",2047,"dms_y25",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+24),0)","v":"2046-47"}]
[null,"2047-48",2048,"dms_y26",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+25),0)","v":"2047-48"}]

{"sheet":"AER ETL","index":34,"n_rows":145,"n_cols":10,"rows_kept":145,"cut":false,"hidden":true,"merged":[[12,4,12,8],[71,1,73,1],[11,0,15,0],[18,0,25,0],[26,0,31,0],[34,0,59,0],[14,2,14,4],[32,37,32,58],[33,37,33,58],[34,37,34,58],[32,68,32,89],[33,68,33,89],[34,68,34,89]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Ausgrid"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"Ausgrid"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Regulatory proposal","dms_Source",{"$f":"IF(dms_Model=\"Reset\", \"Make sure you have set Reg Proposal as source\",\"\")","v":"Make sure you have set Reg Proposal as source"}]
[null,"Data quality","Consolidated","For DB purposes this is always Consoldiated"]
[null,"Data status","Public","For DB purposes this is always Public"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"dd/mm/yy"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality","Consolidated","dms_DataQuality","Always Consolidated"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)","v":"2029"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM",{"$f":"IF(dms_SingleYearModel=\"yes\",\"This is set to an historical template (EB, CA or ARR), apply UOM Named Range to cell !\",\"This is not an historical template, make sure UOM Named Range is not applied\")","v":"This is not an historical template, make sure UOM Named Range is not applied"},null,null,null,null,{"$f":"IFERROR(dms_dollar_nom_UOM, \"NR not applied\")","v":"NR not applied"}]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"NSW"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"2022-23"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"2022"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))","v":"June 2024"},"dms_DollarReal","=IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year","v":"June 2019"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2024-25"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2022-23"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":36},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":38},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":33},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":28},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":42},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2024-25"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2019-20"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2014-15"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2028-29"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2023-24"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2018-19"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2028-29"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2028-29"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2024"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2019"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":"2023"},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2029"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2029"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2024-25 to 2028-29"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_y1&\" to \"&FRCP_final_year,CRY))","v":"2022-23 to 2028-29"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"2022-23"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2028-29"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C50,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"2022-23"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(dms_SingleYearModel=\"yes\",(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(PRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(PRCP_y4,4))))","v":"1-Jul-2017"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060101_StartDateTxt)","v":42917},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"Does the NSP report MAIFI or MAIFIe",{"$f":"INDEX(dms_MAIFI_flag_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_MAIFI_Flag"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes","Must be present for ARRs","=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","0","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2016"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]