{"text_format":"1","workbook":"xlsx","n_sheets":40,"sheets":["CF","AER only","Instructions","Contents","Business & other details","CPI series","2.1 Expenditure summary","2.2 Repex","2.3 Augex (a)","2.3 Augex (b)","2.4 Augex model","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","4.2 Metering","4.3 Fee-based services","4.4 Quoted services","5.4 MD & utilisation-Spatial","6.1 Telephone answering","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.7 TSS-LRMC","7.8 WACC Inputs","Extra info 7.1 7.3","Amendments"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":2,"defined_names":1113,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CF","index":0,"n_rows":125,"n_cols":21,"rows_kept":125,"cut":false,"hidden":true,"merged":[[1,1,1,20]]}
[]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,{"$f":"INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":false},"=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_3.6.6, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":false},"=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_4.1","dms_CF_6.6.1","dms_CF_6.8","dms_CF_7.12","dms_CF_8.1_A","dms_CF_8.1_B","dms_CF_8.1_Neg","dms_CF_4.4.1","Spare2"]
[null,"ActewAGL Distribution","ACT","Electricity","Distribution",null,"Y",null,"Y","Y","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"Energex","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","N","Y","Y","Y","N"]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","N","Y","Y","Y","N"]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"Power and Water","NT","Electricity","Distribution",null,"N",null,"N","Y","N","N","Y","Y","Y","Y","N","Y","Y","N","N"]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","Y","Y","N","N","N"]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"United Energy","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"0"]
[null,null,{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"}]

{"sheet":"AER only","index":1,"n_rows":223,"n_cols":40,"rows_kept":223,"cut":false,"hidden":true,"merged":[[0,1,0,11],[4,27,4,38],[6,27,6,30],[6,33,6,37],[53,25,53,29],[53,30,53,33],[54,1,54,5],[54,14,54,21],[54,25,54,29],[54,30,54,33],[72,14,72,15],[72,25,72,28],[93,1,95,1],[96,1,100,1],[104,1,105,1],[131,11,131,12],[148,1,148,8]]}
[null,"Data in these columns used for data validation and database purposes."]
[null,"Date last modified:","2017-01-16","added (Albury and Victora) for AGN"]
[null,null,"2016-10-17","updated TransGrid's correct legal name, corrected TasNetworks (T) to June financial year"]
[null,null,"2017-02-01","inserted Power and Water, added NRs (dms_FeederCat_1 and dms_FeederCat_2)"]
[null,null,"2017-03-03","inserted AEMO as a business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,"2018-03-28","major changes to accommodate STPIS"]
[null,null,"Template Version",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","MAIFI flag","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_663_List","dms_DeterminationRef_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_ContactName1_List","dms_ContactPh1_List","dms_ContactEmail_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_MAIFI_flag_List","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_Public_Lighting_List","Column1"]
[null,"ActewAGL Distribution","ActewAGL Distribution",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"Robert Walker","02 6248 3847","robert.walker@actewagle.com.au","NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Distribution"]
[null,"ActewAGL Distribution (Tx Assets)","ActewAGL Distribution (Tx Assets)",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"Robert Walker","02 6248 3847","robert.walker@actewagle.com.au","NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Distribution (Tx Assets)"]
[null,"ActewAGL Gas","ActewAGL Gas",76670568688,"ACT","Gas","Distribution","Weighted average price cap","Financial","June",5,5,"x",null,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"Philip Deamer","02 6248 3438","GasAAReview@actewagl.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Gas"]
[null,"AEMO","Australian Energy Market Operator Ltd",94072010327,"Vic","Electricity","Transmission","-","Financial","March",5,5,"x","-","Level 22","530 Collins Street","MELBOURNE","VIC",3000,"GPO Box 2008",null,"MELBOURNE","VIC",3001,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AEMO"]
[null,"AGN (Albury and Victoria)","Australian Gas Networks Limited (reporting data for Albury and Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (Albury)"]
[null,"AGN (Albury)","Australian Gas Networks Limited (reporting data for Albury)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"AGN (SA)","Australian Gas Networks Limited (reporting data for SA)",19078551685,"SA","Gas","Distribution","Weighted average price cap","Financial","June",5,5,5,"distribution determination","Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (SA)"]
[null,"AGN (Victoria)","Australian Gas Networks Limited (reporting data for Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (Victoria)"]
[null,"Amadeus","APT Pipelines (NT) Pty Ltd",39009737393,"NT","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Amadeus"]
[null,"APA GasNet","APA GasNet Australia (Operations) Pty Ltd","065083009","Vic","Gas","Transmission","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","APA GasNet"]
[null,"Ausgrid","Ausgrid",78508211731,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"John Thomson","02 9269 2312","john.thomson@ausgrid.com.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Ausgrid"]
[null,"Ausgrid (Tx Assets)","Ausgrid (Tx Assets)",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"John Thomson","02 9269 2312","john.thomson@ausgrid.com.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Ausgrid (Tx Assets)"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","VIC",8001,"please provide contact details",null,null,"NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","AusNet (D)"]
[null,"AusNet (Gas)","AusNet Gas Services","086015036","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"X",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AusNet (Gas)"]
[null,"AusNet (T)","Ausnet Services (Transmission) Ltd",48116124362,"Vic","Electricity","Transmission","Revenue cap","Financial","March",5,5,2,"transmission determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic",8001,"Clare Thompson","03 9695 6670","clare.e.thompson@ausnetservices.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AusNet (T)"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"-","Electricity","Distribution","Revenue cap","Financial","June",5,5,2,"distribution determination","123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co."]
[null,"Australian Distribution Co. (Gas)","Australian Gas Distribution Co. ",11222333444,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",5,5,null,null,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Australian Distribution Co. (Vic)"]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"distribution determination","123 Straight Street",null,"MELBOURNE","Vic",3000,"PO Box 123",null,"MELBOURNE","VIC",3000,"Bob Smith","02 1234 5678","bob@auselec.net.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co. (Vic)"]
[null,"Australian Transmission Co.","Australian Transmission Co.",11222333444,"-","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Australian Transmission Co."]
[null,"Central Ranges Pipeline (D)","Central Ranges Pipeline Pty Ltd",108218355,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",15,5,5,"distribution determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"Central Ranges Pipeline (T)","Central Ranges Pipeline Pty Ltd",108218355,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",14,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"CitiPower","CitiPower",76064651056,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked Bag 14090",null,"MELBOURNE","VIC",8001,"Hannah Williams","03 9683 4088","hwilliams@powercor.com.au","YES","YES","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","CitiPower"]
[null,"Directlink","Directlink",16779340889,"Qld","Electricity","Transmission","Revenue cap","Financial","June",9,5,5,"transmission determination","Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Directlink"]
[null,"ElectraNet","ElectraNet",41094482416,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","52-55 East Terrace","Rymill Park","ADELAIDE","SA",5000,"PO Box 7096","Hutt Street Post Office","ADELAIDE","SA",5000,"Bill Jackson","08 8404 7969","jackson.bill@electranet.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ElectraNet"]
[null,"Endeavour Energy","Endeavour Energy",11247365823,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","51 Huntingwood Drive",null,"HUNTINGWOOD","NSW",2148,"PO Box 811",null,"SEVEN HILLS","NSW",1730,"Jon Hocking","02 9853 4386 / 0407 348 156","Jon.Hocking@Endeavourenergy.com.au","NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Endeavour Energy"]
[null,"Energex","Energex",40078849055,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","26 Reddacliff Street",null,"NEWSTEAD","Qld",4006,"26 Reddacliff Street",null,"NEWSTEAD","QLD",4006,"Jenny Doyle, General Manager Regulation and Pricing","(07) 3851 6416","jenny.doyle@energyq.com.au","YES","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Energex"]
[null,"Ergon Energy","Ergon Energy",50087646062,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","22 Walker Street",null,"TOWNSVILLE","Qld",4810,"Po Box 264",null,"FORTITUDE VALLEY","QLD",4006,"Jenny Doyle, General Manager Regulation and Pricing","(07) 3851 6416","jenny.doyle@energyq.com.au","NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Ergon Energy"]
[null,"Essential Energy","Essential Energy",37428185226,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","8 Buller Street",null,"PORT MACQUARIE","NSW",2444,"PO Box 5730",null,"PORT MACQUARIE","NSW",2444,"Catherine Waddell","02 6338 3553","catherine.waddell@essentialenergy.com.au","NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Essential Energy"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 16","567 Collins Street","MELBOURNE","VIC",3000,"PO Box 16182",null,"MELBOURNE","VIC",8001,"Matthew Serpell","03 9173 8231","matthew.serpell@jemena.com.au","NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Jemena Electricity"]
[null,"JGN","Jemena Gas Networks (NSW) Ltd","003 004 322","NSW","Gas","Distribution","Weighted average price cap","Financial","June",5,5,null,null,null,null,null,null,null,null,null,null,null,null,"please provide contact details",null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","JGN"]
[null,"Multinet Gas","Multinet Gas (DB No.1) Pty Ltd (ACN 086 026 986), Multinet Gas (DB No.2) Pty Ltd (ACN 086 230 122)","086026986","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"43-45 Centreway",null,"MT WAVERLEY","Vic",3149,null,null,null,null,null,"Andrew Schille","03 8846 9860","andrew.schille@ue.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Multinet Gas"]
[null,"Murraylink","Murraylink",79181207909,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Murraylink"]
[null,"Power and Water","Power and Water Corporation",15947352360,"NT","Electricity","Distribution","Revenue cap","Financial","June",5,5,"x","distribution determination","GPO Box 1921",null,"DARWIN","NT",801,"GPO Box 1921",null,"DARWIN","NT",801,"Lucy Moon","08 8924 5822","Lucy.Moon@powerwater.com.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Power and Water"]
[null,"Powercor Australia","Powercor Australia",89064651109,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked bag 14090",null,"MELBOURNE","VIC",8001,"Hannah Williams","03 9683 4088","hwilliams@powercor.com.au","NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Powercor Australia"]
[null,"Powerlink","Queensland Electricity Transmission Corporation Limited trading as Powerlink Queensland",82078849233,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","33 Harold St",null,"VIRGINIA","Qld",4014,"PO Box 1193",null,"VIRGINIA","QLD",4014,"Jennifer Harris","07 3860 2667","jharris@powerlink.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Powerlink"]
[null,"Roma to Brisbane Pipeline","APT Petroleum Pipelines Limited t/a Roma to Brisbane Pipeline","009 737 393","Qld","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","580 George Street",null,"SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Mark Allen","02 9275 0010","mark.allen@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Roma to Brisbane Pipeline"]
[null,"SA Power Networks","SA Power Networks",13332330749,"SA","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","1 Anzac Highway",null,"KESWICK","SA",5035,"GPO Box 77",null,"ADELAIDE","SA",5000,"Richard Sibly","08 8404 5613","richard.sibly@sapowernetworks.com.au","NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","SA Power Networks"]
[null,"TasNetworks (D)","TasNetworks (D)",24167357299,"Tas","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,"John Sayers","03 6271 6469","john.sayers@tasnetworks.com.au","YES","YES","YES","YES","YES",null,"Critical Infrastructure","High density commercial","Urban","High density rural","Low density rural","YES","TasNetworks (D)"]
[null,"TasNetworks (T)","TasNetworks (T)",24167357299,"Tas","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,"John Sayers","03 6271 6469","john.sayers@tasnetworks.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","TasNetworks (T)"]
[null,"TransGrid","NSW Electricity Networks Operations Pty Ltd trading as TransGrid","70 250 995 390","NSW","Electricity","Transmission","Revenue cap","Financial","June",4,5,5,"transmission determination","180 Thomas Street",null,"SYDNEY","NSW",2000,"PO Box A1000",null,"SYDNEY SOUTH","NSW",1235,"Garrie Chubb","0408 210 221","garrie.chubb@transgrid.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","TransGrid"]
[null,"United Energy","United Energy",70064651029,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 3","6 Nexus Court","MULGRAVE","Vic",3149,"PO Box 449",null,"MOUNT WAVERLEY","VIC",3170,"Mathew Abraham","03 8846 9758","mathew.abraham@ue.com.au","NO","NO","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","United Energy"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For EB & Reset RINs only",null,null,null,null,"For AARs only"]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68",null,null,null,null,null,null,null,null,null,null,null,"Drop down selector box for CA & Reset RINs.","For CA & Reset RINs only",null,null,null,null,null,null,null,null,null,null,"for DNSP only",null,null,null,null,"For DNSPs only"]
[null,"dms_Model_List ","dms_Worksheet_List",null,"dms_RYE_Formula_Result",null,null,null,null,null,null,null,null,"dms_0203_ProjectType","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020603_01_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM","dms_030605_UOM","dms_03060703_UOM"]
[null,"ARR","ANNUAL REPORTING STATEMENT",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"noIN"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","minutes/customer","minutes/customer","Customer / km","%","km","number","number"]
[null,"CA","CATEGORY ANALYSIS",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"noIN"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - dual circuit","Circuit line length in km","0's","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","minutes/customer","minutes/customer","MWh/customer","Number of spans",null,"number","number"]
[null,"CPI","CPI",null,null,null,null,null,null,null,null,null,null,"New line on new route - other","Circuit line length in km","MVA added","MVA added","MVA added","MVA added","0's","km","km","Total length of maintenance spans","0's","$0s","interruptions/customer","interruptions/customer","kVA / customer","Number of spans",null,"number","number"]
[null,"EB","ECONOMIC BENCHMARKING",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"noIN"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Line rebuild over existing route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","interruptions/customer","interruptions/customer",null,"Number of spans",null,"number","number"]
[null,"PTRM","POST TAX REVENUE MODEL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Line rebuild over existing route - dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","(per cent)","0's","0's","Average number of trees per maintenance span",null,null,null,null,null,"Number of spans",null,"number","(per cent)"]
[null,"Reset","REGULATORY REPORTING STATEMENT",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Reconductor - Single circuit","Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,"years","years","Average frequency of cutting cycle",null,null,null,null,null,"Years",null,"number"]
[null,"RFM","ROLL FORWARD MODEL",null,{"$f":"LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)","v":"2020"},"=LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)",null,null,null,null,null,null,null,"Reconductor - Dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,null,null,null,"Years",null,"number"]
[null,"WACC","WEIGHTED AVERAGE COST OF CAPITAL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Other",null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,null,null,null,null,null,null,null,null,"Trees",null,"number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,null,null,null,"Trees",null,"number"]
[null,"dms_DataQuality_List",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,"$0s",null,null,null,null,null,null,null,null,null,null,"Defects",null,"number"]
[null,"Actual",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,null,null,null,"Defects",null,"number"]
[null,"Estimate",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,null,null,null,"Spans",null,"number"]
[null,"Consolidated",null,null,null,null,null,null,null,null,null,null,null,null,null,"$0s",null,null,null,null,null,null,null,null,null,null,null,null,"km",null,"(per cent)"]
[null,"Recast",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Spans",null,"(per cent)",""]
[null,"Public"]
[]
[null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above.",null,null,null,null,null,null,null,null,null,null,null,"For PTRM files - this field set the text for the named range \"DMS_Xfactor\" which in all cases is simply the text \"x factors\" - this saves putting in each old gas PTRM file ",null,null,null,null,null,null,null,null,null,null,"for TNSP only"]
[null,"dms_SourceList","dms_FormControl_Choices",null,null,null,null,null,null,null,null,null,null,null,"DMS_Xfactor",null,null,null,null,null,null,null,null,null,null,"dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,"After appeal","Revenue cap",null,null,null,null,null,null,null,null,null,null,null,"x factors",null,null,null,null,null,null,null,null,null,null,"%",null,"Number of spans","km"]
[null,"Draft decision","Revenue yield",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Years","%"]
[null,"Final decision","Weighted average price cap",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Trees","km"]
[null,"PTRM update 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"Defects","number"]
[null,"PTRM update 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans"]
[null,"PTRM update 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"km"]
[null,"PTRM update 4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"km"]
[null,"PTRM update 5",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans"]
[null,"PTRM update 6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,"PTRM update 7",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,"Regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,"Reporting",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,"Revised regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[]
[]
[]
[null,"Reason for interruption","dms_Reason_Interruption_Detailed","dms_Reason_Interruption","dms_STPIS_Exclusion_List","dms_020301_ProjectType_List","dms_020302_ProjectType_List"]
[null,"Animal","Animal impact","Animal","Weather","New substation establishment","New line on new route - single circuit"]
[null,null,"Animal nesting/burrowing, etc and other","Asset failure","Equipment failure","Capacity upgrade","New line on new route - dual circuit"]
[null,null,"Other","Other","Operational error","Voltage upgrade","New line on new route - other"]
[null,"Asset failure","LV","Overloads","Vegetation","Other","Line rebuild over existing route - single circuit"]
[null,null,"Distribution substation","Planned","Animals",null,"Line rebuild over existing route - dual circuit"]
[null,null,"HV","Network business","Third party impacts",null,"Reconductor - Single circuit"]
[null,null,"Zone substation","Third party","Transmission failure",null,"Reconductor - Dual circuit"]
[null,null,"Subtransmission","Unknown","Load shedding",null,"Reconductor - Other"]
[null,"Other","insert description of 'other'","Vegetation","Inter-distributor connection failure",null,"Line upgrade - raising/retensoring"]
[null,"Overloads","-","Weather","Other",null,"Line upgrade - voltage upgrade"]
[null,"Planned","-","2 - STPIS Exclusion (3.3)(a)",null,null,"Line upgrade - capacity"]
[null,"Network business","Network error","3 - STPIS Exclusion (3.3)(a)",null,null,"String spare circuit"]
[null,null,"Switching and protection error","4 - STPIS Exclusion (3.3)(a)",null,null,"Other"]
[null,"Third party","Fire","5 - STPIS Exclusion (3.3)(a)"]
[null,null,"Other","6 - STPIS Exclusion (3.3)(a)"]
[null,null,"Dig-in","7 - STPIS Exclusion (3.3)(a)"]
[null,null,"Unauthorised access"]
[null,null,"Vehicle impact"]
[null,"Unknown","Unknown"]
[null,"Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,"Grow-in - NSP responsibility"]
[null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,"Grow-in - Other responsible party"]
[null,"Weather"]
[null,"2 - STPIS Exclusion (3.3)(a)"]
[null,"3 - STPIS Exclusion (3.3)(a)"]
[null,"4 - STPIS Exclusion (3.3)(a)"]
[null,"5 - STPIS Exclusion (3.3)(a)"]
[null,"6 - STPIS Exclusion (3.3)(a)"]
[null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[]
[]
[]
[]
[]
[null,"These are indeces and lookup values for various dates. All step from the value placed in FRCP_y1 on the business and other details worksheet",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"},null,null,null,null,null,null,null,null,null,null,null,"These date tables are currently used in the Recast templates to provide column headings and conditional formatting"]
[null,"dms_FRCPlength_Num_List","dms_FinalYear_List","dms_CRCPlength_Num_List","dms_CFinalYear_List","dms_FRCP_years",null,"dms_CRCP_years",null,"dms_CRCP_index",null,"These are static values for cut / paste purposes only",null,null,"CRY from input cell on business sheet","CRY - financial","dms_FinYears","CRY calendar","dms_CalYears"]
[null,1,"dms_FRCP_y1",1,"CRCP_y1",{"$f":"FRCP_y1","v":"2020-21"},"dms_FRCP_y1",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)-1)&\"-\"&TEXT(VALUE(MID(dms_FRCP_y1,3,2)),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)-1))","v":"2019-20"},"dms_CRCP_yZ",1,null,"2005-06","2006",null,{"$f":"'Business & other details'!C48","v":"2018-19"},{"$f":"VALUE(LEFT(CRY,4))&\"-\"&TEXT(MID(CRY,3,2)+1,\"00\")","v":"2018-19"},"dms_CRYf_y1",{"$f":"VALUE(LEFT(CRY,4)+1)","v":2019},"dms_CRYc_y1"]
[null,2,"dms_FRCP_y2",2,"CRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y1,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)+1))","v":"2021-22"},"dms_FRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yZ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yZ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yZ,4)-1))","v":"2018-19"},"dms_CRCP_yY",2,null,"2006-07","2007",null,null,{"$f":"VALUE(LEFT(dms_CRYf_y1,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y1,3,2)+2,\"00\")","v":"2019-20"},"dms_CRYf_y2",{"$f":"VALUE(LEFT(dms_CRYc_y1,4)+1)","v":2020},"dms_CRYc_y2"]
[null,3,"dms_FRCP_y3",3,"CRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y2,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y2,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y2,4)+1))","v":"2022-23"},"dms_FRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yY,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yY,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yY,4)-1))","v":"2017-18"},"dms_CRCP_yX",3,null,"2007-08","2008",null,null,{"$f":"VALUE(LEFT(dms_CRYf_y2,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y2,3,2)+2,\"00\")","v":"2020-21"},"dms_CRYf_y3",{"$f":"VALUE(LEFT(dms_CRYc_y2,4)+1)","v":2021},"dms_CRYc_y3"]
[null,4,"dms_FRCP_y4",4,"CRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y3,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y3,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y3,4)+1))","v":"2023-24"},"dms_FRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yX,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yX,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yX,4)-1))","v":"2016-17"},"dms_CRCP_yW",4,null,"2008-09","2009",null,null,{"$f":"VALUE(LEFT(dms_CRYf_y3,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y3,3,2)+2,\"00\")","v":"2021-22"},"dms_CRYf_y4",{"$f":"VALUE(LEFT(dms_CRYc_y3,4)+1)","v":2022},"dms_CRYc_y4"]
[null,5,"dms_FRCP_y5",5,"CRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y4,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y4,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y4,4)+1))","v":"2024-25"},"dms_FRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yW,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yW,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yW,4)-1))","v":"2015-16"},"dms_CRCP_yV",5,null,"2009-10",2010,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y4,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y4,3,2)+2,\"00\")","v":"2022-23"},"dms_CRYf_y5",{"$f":"VALUE(LEFT(dms_CRYc_y4,4)+1)","v":2023},"dms_CRYc_y5"]
[null,6,"dms_FRCP_y6",6,"CRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y5,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y5,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y5,4)+1))","v":"2025-26"},"dms_FRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yV,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yV,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yV,4)-1))","v":"2014-15"},"dms_CRCP_yU",6,null,"2010-11",2011,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y5,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y5,3,2)+2,\"00\")","v":"2023-24"},"dms_CRYf_y6",{"$f":"VALUE(LEFT(dms_CRYc_y5,4)+1)","v":2024},"dms_CRYc_y6"]
[null,7,"dms_FRCP_y7",7,"CRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y6,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y6,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y6,4)+1))","v":"2026-27"},"dms_FRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yU,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yU,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yU,4)-1))","v":"2013-14"},"dms_CRCP_yT",7,null,"2011-12",2012,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y6,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y6,3,2)+2,\"00\")","v":"2024-25"},"dms_CRYf_y7",{"$f":"VALUE(LEFT(dms_CRYc_y6,4)+1)","v":2025},"dms_CRYc_y7"]
[null,8,"dms_FRCP_y8",8,"CRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y7,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y7,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y7,4)+1))","v":"2027-28"},"dms_FRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yT,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yT,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yT,4)-1))","v":"2012-13"},"dms_CRCP_yS",8,null,"2012-13",2013,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y7,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y7,3,2)+2,\"00\")","v":"2025-26"},"dms_CRYf_y8",{"$f":"VALUE(LEFT(dms_CRYc_y7,4)+1)","v":2026},"dms_CRYc_y8"]
[null,9,"dms_FRCP_y9",9,"CRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y8,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y8,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y8,4)+1))","v":"2028-29"},"dms_FRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yS,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yS,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yS,4)-1))","v":"2011-12"},"dms_CRCP_yR",9,null,"2013-14",2014,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y8,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y8,3,2)+2,\"00\")","v":"2026-27"},"dms_CRYf_y9",{"$f":"VALUE(LEFT(dms_CRYc_y8,4)+1)","v":2027},"dms_CRYc_y9"]
[null,10,"dms_FRCP_y10",10,"CRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y9,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y9,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y9,4)+1))","v":"2029-30"},"dms_FRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yR,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yR,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yR,4)-1))","v":"2010-11"},"dms_CRCP_yQ",10,null,"2014-15",2015,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y9,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y9,3,2)+2,\"00\")","v":"2027-28"},"dms_CRYf_y10",{"$f":"VALUE(LEFT(dms_CRYc_y9,4)+1)","v":2028},"dms_CRYc_y10"]
[null,11,"dms_FRCP_y11",11,"CRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y10,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y10,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y10,4)+1))","v":"2030-31"},"dms_FRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yQ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yQ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yQ,4)-1))","v":"2009-10"},"dms_CRCP_yP",11,null,"2015-16",2016,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y10,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y10,3,2)+2,\"00\")","v":"2028-29"},"dms_CRYf_y11",{"$f":"VALUE(LEFT(dms_CRYc_y10,4)+1)","v":2029},"dms_CRYc_y11"]
[null,12,"dms_FRCP_y12",12,"CRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y11,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y11,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y11,4)+1))","v":"2031-32"},"dms_FRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yP,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yP,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yP,4)-1))","v":"2008-09"},"dms_CRCP_yO",12,null,"2016-17",2017,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y11,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y11,3,2)+2,\"00\")","v":"2029-30"},"dms_CRYf_y12",{"$f":"VALUE(LEFT(dms_CRYc_y11,4)+1)","v":2030},"dms_CRYc_y12"]
[null,13,"dms_FRCP_y13",13,"CRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y12,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y12,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y12,4)+1))","v":"2032-33"},"dms_FRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yO,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yO,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yO,4)-1))","v":"2007-08"},"dms_CRCP_yN",13,null,"2017-18",2018,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y12,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y12,3,2)+2,\"00\")","v":"2030-31"},"dms_CRYf_y13",{"$f":"VALUE(LEFT(dms_CRYc_y12,4)+1)","v":2031},"dms_CRYc_y13"]
[null,14,"dms_FRCP_y14",14,"CRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y13,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y13,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y13,4)+1))","v":"2033-34"},"dms_FRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yN,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yN,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yN,4)-1))","v":"2006-07"},"dms_CRCP_yM",14,null,"2018-19",2019,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y13,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y13,3,2)+2,\"00\")","v":"2031-32"},"dms_CRYf_y14",{"$f":"VALUE(LEFT(dms_CRYc_y13,4)+1)","v":2032},"dms_CRYc_y14"]
[null,15,"dms_FRCP_y15",15,"CRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y14,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y14,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y14,4)+1))","v":"2034-35"},"dms_FRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yM,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yM,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yM,4)-1))","v":"2005-06"},"dms_CRCP_yL",15,null,"2019-20",2020,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y14,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y14,3,2)+2,\"00\")","v":"2032-33"},"dms_CRYf_y15",{"$f":"VALUE(LEFT(dms_CRYc_y14,4)+1)","v":2033},"dms_CRYc_y15"]
[null,null,null,null,null,null,null,null,null,null,null,"2020-21",2021,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y15,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y15,3,2)+2,\"00\")","v":"2033-34"},"dms_CRYf_y16",{"$f":"VALUE(LEFT(dms_CRYc_y15,4)+1)","v":2034},"dms_CRYc_y16"]
[null,"These are drop down lists for businesses to select the correct FRCP_y1 on the business and other details worksheet.\nThis also populates the column headings in the worksheets",null,null,null,null,null,null,null,null,null,"2021-22",2022,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y16,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y16,3,2)+2,\"00\")","v":"2034-35"},"dms_CRYf_y17",{"$f":"VALUE(LEFT(dms_CRYc_y16,4)+1)","v":2035},"dms_CRYc_y17"]
[null,"dms_RCP_fyear_list","dms_CRY_ListF","dms_CRY_ListC","dms_RCP_cyear_list","dms_FRCP_fyear_list","dms_FRCP_ListF","dms_FRCP_ListC","dms_FRCP_cyear_list",null,null,"2022-23",2023,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y17,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y17,3,2)+2,\"00\")","v":"2035-36"},"dms_CRYf_y18",{"$f":"VALUE(LEFT(dms_CRYc_y17,4)+1)","v":2036},"dms_CRYc_y18"]
[null,"dms_fy1","2005-06","2006","dms_cy1","dms_frcp_fy1","2010-11",2011,"dms_crcp_cy1",null,null,"2023-24",2024,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y18,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y18,3,2)+2,\"00\")","v":"2036-37"},"dms_CRYf_y19",{"$f":"VALUE(LEFT(dms_CRYc_y18,4)+1)","v":2037},"dms_CRYc_y19"]
[null,"dms_fy2","2006-07","2007","dms_cy2","dms_frcp_fy2","2011-12",2012,"dms_crcp_cy2",null,null,"2024-25",2025,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y19,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y19,3,2)+2,\"00\")","v":"2037-38"},"dms_CRYf_y20",{"$f":"VALUE(LEFT(dms_CRYc_y19,4)+1)","v":2038},"dms_CRYc_y20"]
[null,"dms_fy3","2007-08","2008","dms_cy3","dms_frcp_fy3","2012-13",2013,"dms_crcp_cy3",null,null,"2025-26",2026]
[null,"dms_fy4","2008-09","2009","dms_cy4","dms_frcp_fy4","2013-14",2014,"dms_crcp_cy4",null,null,"2026-27",2027]
[null,"dms_fy5","2009-10",2010,"dms_cy5","dms_frcp_fy5","2014-15",2015,"dms_crcp_cy5",null,null,"2027-28",2028]
[null,"dms_fy6","2010-11",2011,"dms_cy6","dms_frcp_fy6","2015-16",2016,"dms_crcp_cy6",null,null,"2028-29",2029]
[null,"dms_fy7","2011-12",2012,"dms_cy7","dms_frcp_fy7","2016-17",2017,"dms_crcp_cy7",null,null,"2029-30",2030]
[null,"dms_fy8","2012-13",2013,"dms_cy8","dms_frcp_fy8","2017-18",2018,"dms_crcp_cy8",null,null,"2030-31",2031]
[null,"dms_fy9","2013-14",2014,"dms_cy9","dms_frcp_fy9","2018-19",2019,"dms_crcp_cy9",null,null,"2031-32",2032]
[null,"dms_fy10","2014-15",2015,"dms_cy10","dms_frcp_fy10","2019-20",2020,"dms_crcp_cy10",null,null,"2032-33",2033]
[null,"dms_fy11","2015-16",2016,"dms_cy11","dms_frcp_fy11","2020-21",2021,"dms_crcp_cy11",null,null,"2033-34",2034]
[null,"dms_fy12","2016-17",2017,"dms_cy12","dms_frcp_fy12","2021-22",2022,"dms_crcp_cy12",null,null,"2034-35",2035]
[null,"dms_fy13","2017-18",2018,"dms_cy13","dms_frcp_fy13","2022-23",2023,"dms_crcp_cy13",null,null,"2035-36",2036]
[null,"dms_fy14","2018-19",2019,"dms_cy14","dms_frcp_fy14","2023-24",2024,"dms_crcp_cy14"]
[null,"dms_fy15","2019-20",2020,"dms_cy15","dms_frcp_fy15","2024-25",2025,"dms_crcp_cy15"]
[null,"dms_fy16","2020-21",2021,"dms_cy16"]
[null,"dms_fy17","2021-22",2022,"dms_cy17"]
[null,"dms_fy18","2022-23",2023,"dms_cy18"]
[null,"dms_fy19","2023-24",2024,"dms_cy19"]
[null,"dms_fy20","2024-25",2025,"dms_cy20"]
[]
[]
[]
[]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[null,null,"Table 6.3 sustained interruptions - row descriptions"]
[null,null,"dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[]
[null,null,"Table 6.1 telephone answering - row descriptions and start date"]
[null,null,"dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":"1-Jul-2018"}]
[]
[]
[]
[null,null,null,null,null,null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values"]
[null,null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[null,"dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[]
[]
[]
[null,null,"Table 6.8.1 - row descriptions"]
[null,null,"dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[]
[]
[null,null,"Table 7.9.4 - market impact component - row descriptions"]
[null,"dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[]
[]
[]
[null,null,"Use this to add to existing files"]
[null,null,"ARRs 6.7 STPIS daily performance"]
[null,null,"dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[]
[null,null,"ARR's  6.8 STPIS exclusions"]
[null,null,"dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[null,null,"CA 6.3 sustained interruptions"]
[null,null,"dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]

{"sheet":"Instructions","index":2,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[24,2,24,4],[25,2,25,3],[26,2,26,4],[8,2,8,4],[10,2,10,4],[12,2,12,4],[20,2,20,4],[22,2,22,4],[7,2,7,3],[1,1,1,5],[2,1,2,5],[3,2,3,4],[4,2,4,4],[5,2,5,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Segment,\" Network Service Provider\")","v":"Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,null,{"$f":"CONCATENATE(\"This template is to be used by \",dms_TradingName,\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by Energex to fulfil its reporting obligations to the AER."}]
[null,null,"INSTRUCTIONS"]
[null,null,"Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,null,"Identifying CONFIDENTIAL INFORMATION:\n\nPlease use the macro at the top of each \nworksheet to identify confidential information. \n\nSee Returning completed responses below, for how to deal with confidential and public information."]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selected cells as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return cells to NON-CONFIDENTIAL macro."]
[]
[null,null,"UNITS OF MEASURE\n\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,null,"COLOUR CODING OF INPUT / NON-INPUT CELLS:"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," \nPLEASE DO NOT ENTER TEXT into cells that are to contain numeric data."]
[]
[]
[null,null,"WORKSHEET NAVIGATION\n\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]
[]
[null,null,"RETURNING COMPLETED RESPONSES\n\nPlease return two (2) files to the AER: \n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,null,"SUBMITTING AMENDED DATA TO THE AER\n\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]

{"sheet":"Contents","index":3,"n_rows":34,"n_cols":19,"rows_kept":34,"cut":false,"hidden":false,"merged":[[29,18,29,23]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"CONCATENATE(FRCP_y1,\" to \",FRCP_y5)","v":"2020-21 to 2024-25"}]
[null,"CONTENTS"]
[]
[]
[null,null,null,null,"1. Business and other details",null,null,null,null,null,null,"2. Expenditure",null,null,null,null,null,null,"3. Economic benchmarking"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"4. Alternative control services",null,null,null,null,null,null,"5. Network information",null,null,null,null,null,null,"6. Service & quality"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"7. Other templates"]

{"sheet":"Business & other details","index":4,"n_rows":156,"n_cols":9,"rows_kept":156,"cut":false,"hidden":false,"merged":[[7,1,7,8],[11,1,11,8],[13,2,13,4],[14,2,14,4],[17,2,17,3],[17,4,17,7],[59,2,59,8],[18,4,18,7],[19,2,19,3],[19,4,19,7],[22,2,22,3],[22,4,22,7],[23,4,23,7],[24,2,24,3],[24,4,24,7],[32,1,32,8],[57,2,57,3],[58,4,58,8]]}
[null,{"$f":"IF(dms_DataQuality=\"backcast\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))&\" BACKCAST\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"}]
[null,{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(CRY),CONCATENATE(FRCP_y1,\" to \",dms_MultiYear_FinalYear_Result))","v":"2020-21 to 2024-25"}]
[null,"BUSINESS & OTHER DETAILS"]
[]
[]
[null,"Instructions"]
[null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,"SUBMISSION PARTICULARS INPUT SHEETS"]
[]
[null,"ENTITY DETAILS"]
[]
[null,"Short name","Energex",null,null,"Select business name from drop down list first"]
[null,"ACN / ABN",{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":40078849055}]
[]
[]
[null,"Business address","Address 1",null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"26 Reddacliff Street"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NEWSTEAD"}]
[null,null,null,"State",{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Qld"},"p/code",{"$f":"INDEX(dms_PostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":4006}]
[]
[null,"Postal address","Address 1",null,"GPO Box 1461"]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,"Suburb",null,"BRISBANE"]
[null,null,null,"State",{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"QLD"},"p/code",4001]
[]
[]
[null,"Contact name/s","Karen Stafford",null,null,"General Manager, Legal, Regulation and Pricing"]
[null,"Contact phone/s","07 3851 6793"]
[null,"Contact email address/s","karen.stafford@energyq.com.au"]
[]
[null,"REGULATORY CONTROL PERIODS"]
[]
[null,"Forthcoming regulatory control period","2020-21",{"$f":"dms_FRCP_y2","v":"2021-22"},{"$f":"dms_FRCP_y3","v":"2022-23"},{"$f":"dms_FRCP_y4","v":"2023-24"},{"$f":"dms_FRCP_y5","v":"2024-25"}]
[null,null,{"$f":"dms_FRCP_y6","v":"2025-26"},{"$f":"dms_FRCP_y7","v":"2026-27"},0,{"$f":"dms_FRCP_y9","v":"2028-29"},{"$f":"dms_FRCP_y10","v":"2029-30"}]
[]
[]
[null,"Current regulatory control period",{"$f":"dms_CRCP_FirstYear_Result","v":"2015-16"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+1)&\"-\"&TEXT(MID(CRCP_y1,3,2)+2,\"00\"),VALUE(LEFT(CRCP_y1,4)+1))","v":"2016-17"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+2)&\"-\"&TEXT(VALUE(MID(CRCP_y1,3,2)+3),\"00\"),VALUE(LEFT(CRCP_y1,4)+2))","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+3)&\"-\"&TEXT(MID(CRCP_y1,3,2)+4,\"00\"),VALUE(LEFT(CRCP_y1,4)+3))","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+4)&\"-\"&TEXT(MID(CRCP_y1,3,2)+5,\"00\"),VALUE(LEFT(CRCP_y1,4)+4))","v":"2019-20"}]
[null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+5)&\"-\"&TEXT(MID(CRCP_y1,3,2)+6,\"00\"),VALUE(LEFT(CRCP_y1,4)+5))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+6)&\"-\"&TEXT(MID(CRCP_y1,3,2)+7,\"00\"),VALUE(LEFT(CRCP_y1,4)+6))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+7)&\"-\"&TEXT(MID(CRCP_y1,3,2)+8,\"00\"),VALUE(LEFT(CRCP_y1,4)+7))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+8)&\"-\"&TEXT(MID(CRCP_y1,3,2)+9,\"00\"),VALUE(LEFT(CRCP_y1,4)+8))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+9)&\"-\"&TEXT(MID(CRCP_y1,3,2)+10,\"00\"),VALUE(LEFT(CRCP_y1,4)+9))","v":"2024-25"}]
[null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+10)&\"-\"&TEXT(MID(CRCP_y1,3,2)+11,\"00\"),VALUE(LEFT(CRCP_y1,4)+10))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+11)&\"-\"&TEXT(MID(CRCP_y1,3,2)+12,\"00\"),VALUE(LEFT(CRCP_y1,4)+11))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+12)&\"-\"&TEXT(MID(CRCP_y1,3,2)+13,\"00\"),VALUE(LEFT(CRCP_y1,4)+12))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+13)&\"-\"&TEXT(MID(CRCP_y1,3,2)+14,\"00\"),VALUE(LEFT(CRCP_y1,4)+13))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+14)&\"-\"&TEXT(MID(CRCP_y1,3,2)+15,\"00\"),VALUE(LEFT(CRCP_y1,4)+14))","v":"2029-30"}]
[]
[]
[null,"Previous regulatory control period",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y2,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y2,3,2)),\"00\"),VALUE(LEFT(PRCP_y2,4)-1))","v":"2010-11"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y3,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y3,3,2)),\"00\"),VALUE(LEFT(PRCP_y3,4)-1))","v":"2011-12"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y4,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y4,3,2)),\"00\"),VALUE(LEFT(PRCP_y4,4)-1))","v":"2012-13"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y5,4)-1)&\"-\"&TEXT(VALUE(RIGHT(PRCP_y5,2)-1),\"00\"),VALUE(LEFT(PRCP_y5,4)-1))","v":"2013-14"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)-1)&\"-\"&TEXT(VALUE(RIGHT(CRCP_y1,2)-1),\"00\"),VALUE(LEFT(CRCP_y1,4)-1))","v":"2014-15"}]
[]
[]
[]
[null,"Commencing regulatory year","2018-19","CRY"]
[]
[null,"Last completed regulatory year","2024-25","dms_FinalYear"]
[]
[]
[]
[null,null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Source","Regulatory proposal",null,"Please select the correct submission type from the dropdown list."]
[null,"Data quality (actual, estimate, public, consolidated)","Public",null,"Use Consolidated for Consolidated Confidential version\nUse Public for Consolidated Public version"]
[null,"Amended RIN submission - amendment reason","."]
[null,"Submission Date","2019-01-31","dms_SubmissionDate","Please enter date this file submitted to AER (dd/mm/yyyy)"]
[null,"EBSS - First application of scheme in forthcoming period?","No"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))","v":"2025"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Model or RIN Type","Reset","dms_Model","Drop down selection"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM","If the cover sheet is attached to an ABC RIN apply the NAMED RANGE to the cell"]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"Qld"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FORECAST and MultiYear RINS"]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))","v":{"$error":"#VALUE!"}},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))","v":"June 2020"},"dms_DollarReal","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)","v":"June 2015"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"Single Year Model T/F",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},null,"=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Reference","CRY","dms_SingleYear_FinalYear_Ref","This is the reference for EB, CA & ARR RINs"]
[null,"Single Year Final Year Result",{"$f":"IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")","v":"not a single year RIN"},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Multi Year Final Year Reference",{"$f":"INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))","v":"dms_FRCP_y5"},"dms_MultiYear_FinalYear_Ref","=INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))"]
[null,"Multi Year Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)","v":"2024-25"},"dms_MultiYear_FinalYear_Result","=IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)",null,null,null,"Formula errors OK"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP Final Year Reference",{"$f":"INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))","v":"CRCP_y5"},"dms_CRCP_FinalYear_Ref","=INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))"]
[null,"CRCP First Year Result",{"$f":"INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))","v":"2015-16"},"dms_CRCP_FirstYear_Result","=INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))"]
[null,"CRCP Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)","v":"2019-20"},"dms_CRCP_FinalYear_Result","=IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"Is this a multi year ABC RIN?","No"]
[null,"Multiyear EB, CA or ARR?",{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year RINS",{"$f":"IF(dms_MultiYear_Flag=1,FRY,CRY)","v":"2018-19"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))","v":{"$error":"#VALUE!"}},"dms_0306_Year","=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(SUM(dms_SingleYear_Model)>0,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))","v":"1-Jul-2018"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060701_StartDateTxt)","v":43282},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes",null,"=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","6.8 not present","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"6.8 not present\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2012"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[null,"MISC"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2015-20 Distribution Determination"},"dms_DeterminationRef"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]

{"sheet":"CPI series","index":5,"n_rows":13,"n_cols":12,"rows_kept":13,"cut":false,"hidden":false,"merged":[[9,2,9,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"CPI SERIES"]
[]
[]
[]
[null,"NOMINATED CPI SERIES"]
[]
[null,"Name of CPI series","6401.0 Weighted average of eight capital cities"]
[]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Series data",1.0232558139534831E-2,1.9337016574585641E-2,2.0776874435411097E-2,2.0000000000000018E-2,2.2499999999999964E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2]

{"sheet":"2.1 Expenditure summary","index":6,"n_rows":120,"n_cols":9,"rows_kept":120,"cut":false,"hidden":false,"merged":[[100,1,101,1],[100,2,100,8],[112,1,113,1],[112,2,112,8],[8,1,9,1],[23,1,24,1],[36,1,37,1],[8,2,8,8],[36,2,36,8],[23,2,23,3],[73,1,74,1],[48,1,49,1],[60,1,61,1],[48,2,48,8],[60,2,60,8],[73,2,73,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",135582877.63733715,137439198.15700871,143996960.73142189,124490474.143069,124658642.07152905,126577933.50802249,123716065.41121873]
[null,"Connections",96884813.699527115,95624100.807341591,94806915.803110972,94852139.425295442,94991890.600585237,95112775.904229417,95286074.852574825]
[null,"Augmentation Expenditure",95873057.963252455,71411450.236674145,54776743.423499547,61998716.774702691,61121560.711738288,59838472.957507677,63334823.117498383]
[null,"Non-network",177335563.19265959,161018787.53335029,125202195.33512601,126690304.15547867,138188139.71008226,136460723.02775592,123984937.34092136]
[null,"Public lighting",0,0,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",48751042.183742896,48751042.183742896,47826831.69575794,46094769.9180924,43687319.434322841,40754268.971094191,37366943.162833437]
[null,"Capitalised corporate overheads",9285912.7969034109,9285912.7969034109,9109872.7039538939,8779956.1748747434,8321394.1779662566,7762717.8992560357,7117512.9833968449]
[null,"capcons (included in the above)",54476146.391748235,54288154.387416467,53457892.21438612,53460215.128179178,53463191.459275745,53463147.097288206,53468015.946600333]
[null,"Total",{"$f":"SUM(C11:C18)","v":563713267.47342253},{"$f":"SUM(D11:D18)","v":523530491.71502101},{"$f":"SUM(E11:E18)","v":475719519.69287026},462906360.59151286,470968946.70622396,466506892.26786572,450806356.86844355]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"}]
[null,"Vegetation management",41780559.538444661,41748848.26283104]
[null,"Maintenance",102324236.8279022,102246573.14623186]
[null,"Emergency response",11906862.400911598,11897825.140533568,null," "]
[null,"Non-network",58729049.691796482,58684474.580743007]
[null,"Metering",0,0]
[null,"Network overheads",101310219.15567547,101233325.10931484]
[null,"Corporate overheads",68159689.547360271,68107956.618819997]
[null,"Total",{"$f":"SUM(C26:C32)","v":384210617.16209066},{"$f":"SUM(D26:D32)","v":383919002.85847431}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Metering",2296651.7510614162,1890612.0467826184,1332707.7230553615,1470863.4538312568,1790152.2107842139,1827014.8412850453,1643965.863238313]
[null,"Public lighting",20715839.963431306,29337278.482152235,30729416.604074281,32675232.763070598,34769579.558826603,36705187.200116977,38341348.141044006]
[null,"Fee and quoted",4009102.3676563012,3702520.1809936231,3486494.6474108296,3306546.915094371,3109329.5843878598,2884057.2058559177,2628968.5017463597]
[null,"Network overheads",3421601.3898375896,3268362.6065648366,3380290.7888565199,3259150.7011154052,3019170.8590276958,2806227.6465324746,2458649.569787581]
[null,"Corporate overheads",1488210.2135912867,1346880.2550944814,1463788.3380170751,1400885.6201815768,1311346.2212874149,1220818.6517836507,1098177.4317296047]
[null,"Total",{"$f":"SUM(C39:C44)","v":31931405.685577899},39545653.571587794,40392698.10141407,42112679.453293204,43999578.434313789,45443305.545574069,46171109.507545866]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Metering",17563988.989265002,17563988.989265002,17075280.10439574,16632376.308942825,16229757.590559321,15847620.251564603,15482357.989421759]
[null,"Public lighting",12930101.867667854,12930101.867667854,12852533.032450357,12782409.36687395,12455576.49176129,12124696.855225729,11697988.52115242]
[null,"Fee and quoted",20460536.288196415,18895887.800761212,19375116.57984617,18377012.928379748,17282985.200196266,16033401.047621606,14618536.275780274]
[null,"Network overheads",11130458.374762937,10273283.559922427,10920931.065689825,10541304.905272121,10092448.38548803,9598891.5389414784,9041721.4255120419]
[null,"Corporate overheads",8453419.4306747131,6290716.9040536657,7225505.5924549382,6951816.1007595863,6608289.1071632365,6223208.5297834454,5779461.5414694306]
[null,"Total",{"$f":"SUM(C51:C56)","v":70538504.950566918},65953979.121670164,67449366.374837026,65284919.610228226,62669056.775168136,59827818.223136865,56620065.75333593]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C63:C68)","v":0},{"$f":"SUM(D63:D68)","v":0},0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",{"$f":"SUM(C76:C96)","v":0},{"$f":"SUM(D76:D96)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",0,0,0,0,0,0,0]
[null,"Connections",54476146.391748235,54288154.387416467,53457892.21438612,53460215.128179178,53463191.459275745,53463147.097288206,53468015.946600333]
[null,"Augmentation Expenditure",0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C103:C108)","v":54476146.391748235},{"$f":"SUM(D103:D108)","v":54288154.387416467},53457892.21438612,53460215.128179178,53463191.459275745,53463147.097288206,53468015.946600333]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",29991422.888164163,32914389.97422272,34676126.659115285,32245572.393665742,31072295.663580332,29119444.546730194,25679051.193164717]
[null,"Connections",7775635.1054727519,8609653.6130471323,9012250.9401242435,9222634.0278492291,8961967.5111129079,8287002.4788637692,7550226.232273127]
[null,"Augmentation Expenditure",20269896.987009384,16512911.393376455,13248326.800472315,13406519.67145217,11974450.437595872,11110539.844756266,11255178.720792437]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"capcons (included in the above)",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C115:C118)","v":58036954.980646297},{"$f":"SUM(D115:D118)","v":58036954.980646305},56936704.399711847,54874726.092967145,52008713.612289116,48516986.870350234,44484456.14623028]

{"sheet":"2.2 Repex","index":7,"n_rows":524,"n_cols":11,"rows_kept":524,"cut":false,"hidden":false,"merged":[[9,4,9,10],[182,4,182,10],[355,4,355,10],[11,1,30,1],[31,1,37,1],[38,1,43,1],[184,1,203,1],[204,1,210,1],[211,1,216,1],[106,1,119,1],[77,1,105,1],[61,1,76,1],[44,1,52,1],[53,1,60,1],[357,1,376,1],[377,1,383,1],[384,1,389,1],[129,1,136,1],[120,1,128,1],[302,1,309,1],[293,1,301,1],[279,1,292,1],[250,1,278,1],[234,1,249,1],[226,1,233,1],[217,1,225,1],[399,1,406,1],[390,1,398,1],[475,1,482,1],[466,1,474,1],[452,1,465,1],[423,1,451,1],[407,1,422,1]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.2 REPEX"]
[]
[null,"There is ONE table on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($0's, real June 2020)"}]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,1511379.4279423414,1528364.2785420909,1515342.9070057608,1519529.1428156295,1524071.7064026287,1529058.6872140148,1534291.7035322229]
[null,null,"˂ = 1 kV; Wood",null,7194237.4125217833,6716673.1997955777,7289811.9600474769,6479787.4338094871,6307009.0955802556,6626262.9119486157,6489638.7116006548]
[null,null,"> 1 kV & < = 11 kV; Wood",null,9312109.1689965203,8629138.6486539878,10468020.093959663,10659681.972991675,11094521.666863544,11141059.708953496,11410270.37623436]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",null,1498969.0308063834,1901421.0996310555,4079817.5672676493,3809637.5686222836,4173891.7551572528,4986623.177577069,3735006.1101317648]
[null,null,"> 66 kV & < = 132 kV; Wood",null,706322.810536189,581411.16609214759,714487.02415076829,716461.87398092111,718601.6345707943,720955.07851742662,723422.45908438892]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,6372186.8742046971,6216339.5711659491,6948237.8018142218,6996859.3427095739,7038716.7899807459,7212107.6383483754,7214582.6470281668]
[null,null,"> 1 kV & < = 11 kV",null,3096134.4253815976,3243695.3895367202,3888542.3963203789,3947338.4543034704,4067528.1161213983,4082376.2289339667,4148452.1193239931]
[null,null,"˃ 11 kV & < = 22 kV",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",null,360661.5479206543,485868.75205318636,984841.02987894556,922202.95294055564,1004801.4733471591,1193298.513166236,903763.67793624674]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",4510238.6140554631,5324709.7167443382,4369230.7751518972,3129500.9091620445,3138856.4104649671,3149127.19800267,3159904.7006276911]
[null,null,"> 1 kV & < = 11 kV","per km",3033917.6802690364,4272349.4649724271,4966420.824288602,4980140.892931412,4995028.7986917691,5011373.2480157418,5028524.059951731]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","per km",774013.06950290967,2801100.3410429563,6146705.3651287667,1840285.9666212953,5097740.136395135,5305809.5881206719,4699688.8503092406]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",422869.46386900236,0,2106767.7609969466,1056294.4395936185,1059452.1840048621,1062918.8632234433,1066556.5730135848]
[null,null,"> 1 kV & < = 11 kV","per km",0,0,717904.93187424308,719888.19211190892,722040.26527461153,724402.88439078955,726882.064651608]
[null,null,"> 11 kV & < = 22 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV","per km",6479906.3951467387,4654609.3768690899,8143218.2706147628,733108.78107279958,1629850.4134254172,0,0]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,22705.156163343428,91872.618630204117,1609261.7182044035]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",7376411.3751950366,7082717.0259020831,7310935.8902397435,7352469.3256034208,7419938.93880188,7536533.4886712786,7562759.3932695435]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",623086.26248820778,563583.76748654491,635772.9616938018,639403.72900582443,645262.07599330717,655413.33491295774,657691.4326838468]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,541806.05069968139,548269.54721273016,629843.71109334705,586432.54632257263,581720.79612899362,583632.57594339829,579120.72992215131]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,849559.73564306751,858522.52033161139,908898.19167284854,911347.24832283636,931992.43305844022,917073.18103126751,911186.0333931084]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,8154207.5505228443,8173090.9510111213,8403859.7283263244,8296112.2340303864,8358289.0432585422,8367002.9151739907,8320301.850881218]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,4891379.7956123324,4655793.8543830244,4991354.9074375071,4945931.3647248438,4960704.4806624483,4977006.1794041833,4994018.5587976174]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,457657.09372397099,392285.01151089376,651476.00329053774,522576.37680868054,524137.24989394721,525860.08897073835,461698.12791971787]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,626431.78254289634,626433.8069816482,780231.17761020188,625856.39264578559,627725.73724692466,629789.05892815511,631941.68455442542]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,549877.24923643016,305503.0840403355,547924.11576174293,488346.07522108755,489804.70115927712,491414.68009091826,493094.34058438509]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,5956941.0580221592,10509890.66730061,3337129.1387712806,1339275.3515083801,150813.35974659078,40037.42831848668,189871.73808062213]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,3731311.1594660156,6565389.5011392348,10328286.90974552,5322356.8944795402,2193826.208974062,1171912.4090091852,599276.71544017759]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,1589004.8201130105,257496.32399476203,546629.60668435111,2129872.4009856787,651956.72336919222,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,10342185.555741241,9018318.5115714632,9780163.270694349,11333288.430705015,10019166.456182396,9634510.5245128013,9387976.0825118348]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,5544753.3338747695,2729666.1234763586,4595645.6182352183,1698926.5480508406,71119.710438170034,0,86811.278506257862]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,351390.40917155868,403351.25343510543,399960.28460193152,979054.60663849174,1318115.0355273343,1501950.725594613,413745.1766497863]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,7777443.4658489972,12193623.90434658,5182418.5987206232,1343019.7190450369,655743.33077127393,593546.93212340015,1041187.3476375856]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,16970734.80285513,13231130.16783564,6661290.447019808,6581877.9397104364,6130499.7910963902,5772431.1653071307,4808470.9552273275]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,2869278.0349890953,3358555.5268663629,4108008.6821341403,3804195.9057982746,3487025.5954681858,3437771.0788837844,3067065.4833088368]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,38744.024808121867,168618.17080011038,146499.54567709903,152130.27905961513,136169.87935865507,127049.94628070583,101212.28061592221]
[null,null,"Communications Linear Assets",null,3905498.6939054728,248436.67165845408,1029831.7772888767,835581.04943959683,837939.27304536651,840681.13030721922,843558.2586412027]
[null,null,"AFLC",null,3988.0973322574346,36301.602482415699,77063.053796838925,300267.5290845476,91912.417714099691,0,0]
[null,null,"Other",null,2694366.6123492466,3151277.1252997685,3295182.0192821859,3390160.0665196162,1218300.3127784445,3847194.8466706923,2011032.2787615554]
[null,"OTHER BY: \nenter DNSP defined asset group here","33kV Instrument Transformer",null,176396.37446889759,295350.03607041505,156263.23240489402,302055.62193134479,373467.73776388809,204652.70300516646,406383.71525161742]
[null,null,"110kV Instrument Transformer",null,248778.99860334935,30218.117709454324,0,0,0,0,0]
[null,null,"CAPACITOR BANKS",null,0,0,0,0,0,0,0]
[null,null,"STATIC VAR COMPENSATOR",null,0,0,0,0,0,0,0]
[null,null,"Replace Ageing Cable Terminations",null,626036.37023075379,506010.7250538037,408796.67318282416,136645.69422558174,137044.92821214077,137498.65396888644,137968.73664004647]
[null,null,"Substation Batteries",null,347714.17237641721,399211.26184542588,550685.71934964438,420503.10180821718,451660.81841064763,368929.50454128796,364057.91674844635]
[null,null,"Substation Battery Charger",null,558980.06590754609,984558.98267438042,166729.69055592472,1351.6454871923102,79193.804712846671,362064.52149990434,165969.38754875286]
[null,null,"LV Network Safety",null,0,0,0,6703687.6635314599,13447455.965195887,15177888.623512816,16922037.757195499]
[null,null,"Fire Suppression System / Water Misting",null,513399.89290171716,233677.68941856889,0,0,0,0,0]
[null,null,"Electric Fence",null,0,4221.5728657046438,246426.85100500891,40757.786286313465,259239.27686353782,29440.934531378261,254797.61896568927]
[null,null,"Asbestos",null,0,0,1664512.5725119913,1669110.8994680955,1674100.6309453989,1656355.7396598521,1685326.6799370821]
[null,null,"Substation Miscellaneous Work",null,144677.47295216552,49876.107208366659,0,0,0,0,0]
[null,null,"Reactive Work",null,1847891.4046014284,3502137.5399961835,4115791.6441331962,4127161.7929536197,4139499.7563069155,4153044.7921255832,4167258.0799144506]
[null,null,"Other Non AER asset Categories (ONLY FOR HISTORICAL INFO)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"ASSET REPLACEMENTS (0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,1691.2349171767144,1710.2020377431822,1701.7722063803076,1701.7722063803076,1701.7722063803076,1701.7722063803076,1701.7722063803076]
[null,null,"˂ = 1 kV; Wood",null,2016.8371535677454,1883.0135806821113,2050.5564790192439,1817.6823876198332,1763.9422126815077,1847.1867973898943,1802.9301827348027]
[null,null,"> 1 kV & < = 11 kV; Wood",null,1928.3239242575623,1786.0705200090536,2174.8964916216441,2208.6158170731424,2291.8604017815287,2293.9678596222475,2341.3856610384173]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",null,157.00560913353922,199.15476594791218,428.86767058624474,399.36326081618364,436.24377302875996,519.48835773714654,387.77224269223109]
[null,null,"> 66 kV & < = 132 kV; Wood",null,31.611867610779708,31.611867610779708,38.987970053294973,38.987970053294973,38.987970053294973,38.987970053294973,38.987970053294973]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,4631.1386049792272,4517.3358815804204,5067.3823780079874,5088.4569564151734,5104.2628902205633,5212.7969690175742,5196.9910352121842]
[null,null,"> 1 kV & < = 11 kV",null,2985.2140313779637,3126.4137067061133,3761.8122456827855,3808.1763181785955,3912.4954812941687,3914.6029391348875,3964.1281983917756]
[null,null,"˃ 11 kV & < = 22 kV",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",null,270.80833253234618,365.64393536468532,742.87888885332313,694.40735851679426,754.46990697727574,892.50839554434708,673.33278010960782]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",75.868482265871307,89.566958230542511,73.761024425152655,52.686446017966183,52.686446017966183,52.686446017966183,52.686446017966183]
[null,null,"> 1 kV & < = 11 kV","per km",103.26543419521371,145.41459100958667,169.65035617785111,169.65035617785111,169.65035617785111,169.65035617785111,169.65035617785111]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","per km",0,13.045164034048428,38.819373426037487,32.65505924193544,37.122869864258966,51.105852637427198,30.073423387055097]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",2.1074578407186473,0,10.537289203593236,5.268644601796618,5.268644601796618,5.268644601796618,5.268644601796618]
[null,null,"> 1 kV & < = 11 kV","per km",0,0,1.5805933805389856,1.5805933805389856,1.5805933805389856,1.5805933805389856,1.5805933805389856]
[null,null,"> 11 kV & < = 22 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV","per km",0.63223735221559418,11.380272339880696,10.632124806425576,0,10.537289203593236,0,0]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0.63223735221559418]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",18522.446962076192,17783.782988904306,18423.396443562415,18477.136618500739,18590.939341899546,18821.705975458241,18822.759704378597]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",1564.7874467335955,1415.1579400425717,1601.6679589461719,1606.9366035479686,1616.4201638312024,1636.4410133180297,1636.4410133180297]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,88.513229310183192,89.566958230542511,103.26543419521371,95.889331752698453,94.835602832339134,94.835602832339134,93.781873911979801]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,100.10424743413574,101.15797635449508,107.480349876651,107.480349876651,109.58780771736966,107.480349876651,106.42662095629169]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,460.47953819702445,461.53326711738373,476.28547200241428,468.90936955989901,471.01682740061767,469.96309848025834,465.74818279882106]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,87.459500389823859,83.244584708386569,89.566958230542511,88.513229310183192,88.513229310183192,88.513229310183192,88.513229310183192]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,7.3761024425152657,6.3223735221559423,10.537289203593236,8.4298313628745891,8.4298313628745891,8.4298313628745891,7.3761024425152657]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,4.2149156814372946,4.2149156814372946,5.268644601796618,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,9.4835602832339134,5.268644601796618,9.4835602832339134,8.4298313628745891,8.4298313628745891,8.4298313628745891,8.4298313628745891]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,5.268644601796618,2.1074578407186473,3.1611867610779711,1.0537289203593236,1.0537289203593236,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,6.3223735221559423,2.1074578407186473,4.2149156814372946,5.268644601796618,2.1074578407186473,1.0537289203593236,1.0537289203593236]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,2.1074578407186473,0,0,1.0537289203593236,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,1495.2413379898803,1474.1667595826939,1826.1122189827079,1834.5420503455825,1837.7032371066605,1822.9510322216299,1796.6078092126468]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,86.40577146946454,31.611867610779708,20.020849486827149,25.289494088623769,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,6.3223735221559423,0,5.268644601796618,1.0537289203593236,27.396951929342414,22.128307327545798,7.3761024425152657]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,31.611867610779708,30.558138690420385,27.396951929342414,23.182036247905121,4.2149156814372946,0,6.3223735221559423]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,286.61426633773601,255.00239872695633,348.7842726389361,184.40256106288163,207.58459731078676,221.28307327545795,213.9069708329427]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,12.644747044311885,6.3223735221559423,20.020849486827149,20.020849486827149,21.074578407186472,20.020849486827149,18.967120566467827]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,4.2149156814372946,4.2149156814372946,5.268644601796618,4.2149156814372946,4.2149156814372946]
[null,null,"Communications Linear Assets",null,29137.712105776016,62686.333472176164,27449.63837536038,21074.578407186473,21074.578407186473,21074.578407186473,21074.578407186473]
[null,null,"AFLC",null,0,0,0,1.0537289203593236,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},{"$f":"IF(ISBLANK(C138),\"\",C138)","v":"33kV Instrument Transformer"},null,2.1074578407186473,4.2149156814372946,1.0537289203593236,2.1074578407186473,4.2149156814372946,0,4.2149156814372946]
[null,{"$f":"IF(ISBLANK(B139),\"\",B139)","v":""},{"$f":"IF(ISBLANK(C139),\"\",C139)","v":"110kV Instrument Transformer"},null,2.1074578407186473,4.2149156814372946,0,0,0,0,0]
[null,"","CAPACITOR BANKS",null,0,0,0,0,0,0,0]
[null,"","STATIC VAR COMPENSATOR",null,0,0,0,0,0,0,0]
[null,"","Replace Ageing Cable Terminations",null,62.170006301200097,38.987970053294973,31.611867610779708,10.537289203593236,10.537289203593236,10.537289203593236,10.537289203593236]
[null,"","Substation Batteries",null,77.975940106589945,139.09221748743073,203.36968162934946,105.37289203593237,139.09221748743073,113.80272339880695,97.996789593417105]
[null,"","Substation Battery Charger",null,0,47.417801416169567,11.59101812395256,0,0,10.537289203593236,7.3761024425152657]
[null,"","LV Network Safety",null,0,0,0,21074.578407186473,42149.156814372946,47417.801416169561,52686.446017966184]
[null,"","Fire Suppression System / Water Misting",null,1.0537289203593236,3.1611867610779711,0,0,0,0,0]
[null,"","Electric Fence",null,0,0,1.0537289203593236,0,1.0537289203593236,0,1.0537289203593236]
[null,"","Asbestos",null,0,0,0,0,0,0,0]
[null,"","Substation Miscellaneous Work",null,1.0537289203593236,1.0537289203593236,0,0,0,0,0]
[null,"","Reactive Work"]
[null,"","Other Non AER asset Categories (ONLY FOR HISTORICAL INFO)"]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,null,"ASSET FAILURES (0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473]
[null,null,"> 1 kV & < = 11 kV; Wood",null,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",null,1.0537289203593236,0,0,1.0537289203593236,0,0,1.0537289203593236]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,72.707295504793336,72.707295504793336,72.707295504793336,72.707295504793336,72.707295504793336,72.707295504793336,72.707295504793336]
[null,null,"> 1 kV & < = 11 kV",null,38.987970053294973,38.987970053294973,38.987970053294973,38.987970053294973,38.987970053294973,38.987970053294973,38.987970053294973]
[null,null,"˃ 11 kV & < = 22 kV",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",null,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711]
[null,null,"> 66 kV & < = 132 kV",null,0,0,1.0537289203593236,0,0,1.0537289203593236,0]
[null,null,"> 132 kV",null,0,0,1.0537289203593236,0,0,1.0537289203593236,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",64.277464141918742,64.277464141918742,64.277464141918742,64.277464141918742,64.277464141918742,64.277464141918742,64.277464141918742]
[null,null,"> 1 kV & < = 11 kV","per km",88.513229310183192,88.513229310183192,88.513229310183192,88.513229310183192,88.513229310183192,88.513229310183192,88.513229310183192]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","per km",5.268644601796618,5.268644601796618,5.268644601796618,5.268644601796618,5.268644601796618,5.268644601796618,5.268644601796618]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",61.116277380840771,59.008819540122126,59.008819540122126,59.008819540122126,59.008819540122126,59.008819540122126,59.008819540122126]
[null,null,"> 1 kV & < = 11 kV","per km",40.041698973654299,36.880512212576328,36.880512212576328,36.880512212576328,36.880512212576328,36.880512212576328,36.880512212576328]
[null,null,"> 11 kV & < = 22 kV","per km",1.0537289203593236,0,1.0537289203593236,0,0,1.0537289203593236,0]
[null,null,"> 22 kV & < = 33 kV","per km",0,0,0,1.0537289203593236,0,0,1.0537289203593236]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,1.0537289203593236,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,1.0537289203593236,0,0,0,1.0537289203593236,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",1689.1274593359958,1689.1274593359958,1689.1274593359958,1689.1274593359958,1689.1274593359958,1689.1274593359958,1689.1274593359958]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,17.913391646108501,17.913391646108501,17.913391646108501,17.913391646108501,17.913391646108501,17.913391646108501,17.913391646108501]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,57.9550906197628,57.9550906197628,57.9550906197628,57.9550906197628,57.9550906197628,57.9550906197628,57.9550906197628]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,7.3761024425152657,7.3761024425152657,7.3761024425152657,7.3761024425152657,7.3761024425152657,7.3761024425152657,7.3761024425152657]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0,0,1.0537289203593236,0,0,1.0537289203593236,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946,4.2149156814372946]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0,0,1.0537289203593236,0,0,1.0537289203593236,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,1.0537289203593236,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,1.0537289203593236,0,0,0,0,1.0537289203593236,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,1.0537289203593236,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,1.0537289203593236,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,1.0537289203593236,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,1.0537289203593236,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,248.68002520480039,248.68002520480039,248.68002520480039,248.68002520480039,248.68002520480039,248.68002520480039,248.68002520480039]
[null,null,"˂ = 11 kV  ; Switch",null,73.761024425152655,73.761024425152655,73.761024425152655,73.761024425152655,73.761024425152655,73.761024425152655,73.761024425152655]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,6.3223735221559423,6.3223735221559423,6.3223735221559423,6.3223735221559423,6.3223735221559423,6.3223735221559423,6.3223735221559423]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236,1.0537289203593236]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,711.26702124254348,711.26702124254348,711.26702124254348,711.26702124254348,711.26702124254348,711.26702124254348,711.26702124254348]
[null,null,"Luminaires ;  Minor Road",null,1868.2613757970807,1868.2613757970807,1868.2613757970807,1868.2613757970807,1868.2613757970807,1868.2613757970807,1868.2613757970807]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,7927.2026678631919,7927.2026678631919,7927.2026678631919,7927.2026678631919,7927.2026678631919,7927.2026678631919,7927.2026678631919]
[null,null,"Lamps ; Minor Road",null,16337.013181250953,16337.013181250953,16337.013181250953,16337.013181250953,16337.013181250953,16337.013181250953,16337.013181250953]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,368.80512212576326,368.80512212576326,368.80512212576326,368.80512212576326,368.80512212576326,368.80512212576326,368.80512212576326]
[null,null,"Local Network Wiring Assets",null,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711,3.1611867610779711]
[null,null,"Communications Network Assets",null,87.459500389823859,87.459500389823859,87.459500389823859,87.459500389823859,87.459500389823859,87.459500389823859,87.459500389823859]
[null,null,"Master Station Assets",null,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473,2.1074578407186473]
[null,null,"Communications Site Infrastructure",null,10.537289203593236,10.537289203593236,10.537289203593236,10.537289203593236,10.537289203593236,10.537289203593236,10.537289203593236]
[null,null,"Communications Linear Assets",null,11.59101812395256,11.59101812395256,11.59101812395256,11.59101812395256,11.59101812395256,11.59101812395256,11.59101812395256]
[null,null,"AFLC",null,9.4835602832339134,9.4835602832339134,9.4835602832339134,9.4835602832339134,9.4835602832339134,9.4835602832339134,9.4835602832339134]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},{"$f":"IF(ISBLANK(C138),\"\",C138)","v":"33kV Instrument Transformer"}]
[null,{"$f":"IF(ISBLANK(B139),\"\",B139)","v":""},{"$f":"IF(ISBLANK(C139),\"\",C139)","v":"110kV Instrument Transformer"}]
[null,"","CAPACITOR BANKS"]
[null,"","STATIC VAR COMPENSATOR"]
[null,"","Replace Ageing Cable Terminations"]
[null,"","Substation Batteries"]
[null,"","Substation Battery Charger"]
[null,"","LV Network Safety"]
[null,"","Fire Suppression System / Water Misting"]
[null,"","Electric Fence"]
[null,"","Asbestos"]
[null,"","Substation Miscellaneous Work"]
[null,"","Reactive Work"]
[null,"","Other Non AER asset Categories (ONLY FOR HISTORICAL INFO)"]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]

{"sheet":"2.3 Augex (a)","index":8,"n_rows":126,"n_cols":32,"rows_kept":126,"cut":false,"hidden":false,"merged":[[68,1,68,10],[69,7,69,10],[70,7,70,10],[68,11,68,22],[69,21,69,22],[69,17,69,19],[69,11,69,13],[69,3,70,3],[69,4,70,4],[69,5,70,5],[69,6,70,6],[69,1,70,1],[10,6,11,6],[10,7,10,8],[10,9,10,10],[10,11,10,13],[5,1,5,3],[9,11,9,22],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,21,10,22],[9,30,9,31],[9,23,9,24],[9,26,11,26],[11,27,11,29],[11,30,11,31],[9,27,9,28],[9,29,10,29],[9,25,11,25],[11,23,11,24],[68,30,68,31],[68,29,69,29],[69,14,69,16],[11,14,11,15],[10,14,10,16],[10,17,10,19],[11,17,11,18],[68,25,70,25],[68,26,70,26],[70,27,70,29],[70,30,70,31],[68,23,68,24],[68,27,68,28],[70,23,70,24]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are TWO tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation.  Both ROWS and COLUMNS have been grouped. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"2.3.1 - AUGEX ASSET DATA - SUBTRANSMISSION SUBSTATIONS, SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON-RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"SUBSTATION ID","SUBSTATION TYPE","PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)","SUBSTATION RATING\nNORMAL CYCLIC\n(MVA)",null,"SUBSTATION RATING\nN-1 EMERGENCY\n(MVA)",null,"TRANSFORMERS",null,null,"SWITCHGEAR",null,null,"CAPACITORS",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"PRE","POST","PRE","POST","UNITS ADDED ","MVA ADDED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"UNITS ADDED ",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"MVAR ADDED",null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"}]
[null,"CPR","Subtransmission substation","C0037017","New substation establishment","Demand growth","110/33",0,179.02,0,108,2,160,3175773.4714657264,14,0,2984617.3810632885,20,0,64634.234700346606,11564698.618161175,42343.082999999999,3424378.3021492977,8524068.8992659636,10630943.713247476,{"$f":"SUM(N13,Q13,T13,U13,W13,X13,Y13)","v":40369114.620053269},"2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,15083901.832647556,0,0]
[null,"TRG","Zone substation","C0062273","Capacity upgrade","Demand growth","33/11",18,48,0,21.8,1,25,671285.6847496361,27,0,1387384.267561239,0,0,0,2698555.5540342098,30244,2348933.9919918221,4962746.3066943493,6191689.4844601406,18260595.289491396,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,7848084.3833481045,0,0]
[null,"RCN","Zone substation","C0065191","Capacity upgrade","Demand growth","33/11",28.8,60,19.2,33.75,2,50,1351944.7073350505,3,0,206169.20681069,0,0,0,757694.41353634815,6175.9165999999996,511621.82282575197,279085.32290587685,3359158.333075745,6465673.806489462,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,1648516.3441100125,0,0]
[null,"WSE","Zone substation","C0076665","New substation establishment","Demand growth","33/11",0,16.5,0,0,1,15,569042.68029244023,11,0,561238.54400409828,0,0,0,3288022.194229092,21005,1689467.357580597,317059.29421908362,11124042.186809005,17548872.257134318,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016",0,0,8298867.0953801014,0,0]
[null,"BTY","Zone substation","C0077440","New substation establishment","Demand growth","132/11",0,66,0,37.5,2,60,2312856.7322011306,22,0,0,0,0,0,5600665.5808621608,8207,533924.8946017893,572829.04206797516,6463448.2059105122,15483724.455643568,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015",0,0,5733553.9020389821,0,0]
[null,"SSWMD","Zone substation","C0077634","Capacity upgrade","Demand growth","132/11",0,33,0,0,0,0,0,6,0,3530265.1205999898,0,0,0,3652761.0697897333,16510,1501671.9539951144,2603128.5212069531,13773380.455245029,25061207.120836817,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018, 2019",0,0,8340196.2750732815,0,0]
[null,"BLN","Zone substation","C0107213","Capacity upgrade","Demand growth","33/11",27.5,55,0,31.25,1,25,637140.26436065382,11,0,489017.60208745609,0,0,0,941264.59853247413,3475,278221.02614094067,258805.18694826736,3446892.4691734621,6051341.1472432539,"2013, 2014, 2015,2016",0,0,3005018.6410294129,0,0]
[null,"TWG","Zone substation","C0107382","Other","Fault level issues","33/11",44,44,25.15,25.15,0,0,0,6,0,273629.44825576351,0,0,0,1976120.1729036616,11844,1604831.9170370842,881066.17022857955,1810381.1871904095,6546028.8956154985,"2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,1654411.4019617052,0,0]
[null,"WSS","Zone substation","C0112508","New substation establishment","Demand growth","33/11",0,52.5,0,31.25,2,50,1302296.400833901,17,0,842951.93862745771,5.4,0,124993.43217546011,2859022.1701092618,3387,301031.37186835118,211006.66371159739,9616823.8877387978,15258125.865064826,"2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,5190554.3603345687,0,0]
[null,"WRG","Zone substation","C0117468","Capacity upgrade","Demand growth","33/11",41.25,87.16,31.25,67.5,3,75,2063115.3639699472,29,0,1500773.9416396674,5.4,0,125388.54437474276,5753767.2501487313,14902,1330006.8468845668,1184587.7056402895,2960238.6360267573,14917878.288684702,"2009, 2010, 2011, 2012, 2013, 2014, 2015",0,0,4084121.2573622656,0,0]
[null,"VPK","Zone substation","C0121634","Capacity upgrade","Demand growth","110/11",57.03,126,50,75,2,120,2815113.8100155466,62,0,7591114.7698210254,10.8,0,514522.37429700658,4907876.2979744384,28885,2543021.59080589,880242.61467336863,26089678.970810384,45341570.428397655,"2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018,2019",0,0,22619057.744475711,0,0]
[null,"MLB","Subtransmission substation","C0124994","Other","Reactive power issue","132/11",67.75,67.75,40.5,40.5,0,0,0,10,0,3377950.8155997293,125,0,778978.15471058968,2496939.5879063201,12655,933294.7912386019,110527.87091208038,2478196.2029578164,10175887.423325138,"2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,2301503.2626944445,0,0]
[null,"GBG","Zone substation","C0131194","Capacity upgrade","Demand growth","33/11",52.5,78.75,31.25,62.5,1,25,661289.88997376023,11,0,398672.41929387185,0,0,0,2735505.4599770093,8702,733961.55490688118,175640.70010944654,2540972.9993425789,7246043.0236035474,"2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,2297815.5324288174,0,0]
[null,"AFD","Subtransmission substation","C0230608","Other","Safety","110/33",176,176,100,100,0,0,0,12,0,978024.57600925141,0,0,0,1502626.4829464406,9624,1708700.7230475536,406911.59145145101,3035073.7132995171,7631337.086754214," 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,3515319.0090300012,0,0]
[null,"JDL","Zone substation","C0230644","Other","Safety","33/11",36,36,20.25,20.25,0,0,0,16,0,1073916.5783026146,0,0,0,515734.47685902356,7973,832706.53606841969,609201.80979690014,3468841.7258596346,6500401.1268865932," 2012, 2013, 2014, 2015, 2016, 2017, 2018.2019",0,0,3426848.2658973429,0,0]
[null,"QPT","Zone substation","C0548905","Capacity upgrade","Demand growth","33/11",52.5,52.5,31.25,31.25,0,0,0,1,0,522277.0941147015,0,0,0,1506906.8578614704,2262,3447028.8211570298,126446.03331198037,476646.56904994335,6079305.3754951255,"2019, 2020, 2021, 2022",0,0,3404147.122903402,0,0]
[null,"744","Zone substation","C0562034","Capacity upgrade","Demand growth","132/11",0,66,0,37.5,2,60,2000475.4644555741,23,0,2723927.059946829,0,0,0,5608946.5804281458,22997,15092899.075167749,1543558.6673032027,2322660.3855245532,29292467.23282605,"2022, 2023, 2024, 2025",0,0,9832498.0002596825,0,0]
[null,"539 Petrie","Zone substation","DJ7193621","Capacity upgrade","Demand growth","33/11",0,30,0,33.75,1,25,592306.18211388157,11,0,521531.10452534724,0,0,0,859163.03203786351,9305,1447408.3490442059,870185.38018689724,1511221.9435912452,5801815.9914994417,"2022, 2023, 2024, 2025",0,0,2346019.7849838752,0,0]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",{"$f":"SUM(N45,Q45,T45,U45,W45,X45,Y45)","v":0},"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,null,null,"Non material projects - [forecast]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,null,null,null,0,0]
[]
[]
[null,"2.3.2 - AUGEX ASSET DATA - SUBTRANSMISSION LINES"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"LINE ID",null,"PROJECT ID","PROJECT TYPE","PROJECT TRIGGER","VOLTAGE (KV)","ROUTE LINE LENGTH ADDED",null,null,null,"POLES/TOWERS (INCLUDING STRUCTURES, AND CIVIL WORKS)",null,null,"OVERHEAD LINES",null,null,"UNDERGROUND CABLES",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"KM ADDED",null,null,null,"POLES/TOWERS ADDED","POLES/TOWERS UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"}]
[null,"ABM-ABY",null,"C0583355","New line on new route - single circuit","Demand growth","Other",16,0,0,0,230,0,56502190.50094413,16,0,18834063.500314713,0,0,467927.04348607978,86975939.20797506,15076,331877255.59250206,350945.28261455981,899589.74110198813,{"$f":"SUM(N72,Q72,T72,U72,W72,X72,Y72)","v":495907910.86893862},"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,2402805.36830102,0,0]
[null,"F334, F335","","C0076665","New line on new route - dual circuit","Demand growth","Other",8,0,0,0,0,0,236358.30689994252,15.4,0,378218.80718852615,0.6,0,468766.15288043069,3340231.5196559089,21005,1702053.0014267857,376179.48288678506,11047032.165206404,17548839.436144784,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016",0,0,8298866.3231566017,0,0]
[null,"F845, F846","","C0077634","New line on new route - dual circuit","Demand growth",132,17,0,0,0,0,0,7013454.3970871437,34,0,0,0,0,0,8984466.1116759572,16510,3693567.8309503975,6402751.1069776323,36825646.344545662,62919885.791236795,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018,2019",0,0,20513854.747140981,0,0]
[null,"F7354","","C0100550","New line on new route - single circuit","Demand growth","Other",23,0,0,0,0,0,0,11.1,3.1,318287.68664172344,8.8000000000000007,0,5270797.4195481502,3881350.1973459451,24563,2282951.3144219024,817074.55298431742,27185776.225715395,39756237.396657437,"2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018",0,0,20808619.777157694,0,0]
[null,"DBS-QPT","","C0548905","New line on new route - single circuit","Demand growth","Other",3.6,0,0,0,0,0,0,0,0,56852.111505543959,3.6,0,0,1590118.7513948572,2262,3637374.8891812307,13342.842496199091,502967.14974802663,5800655.7443258576,"2022, 2023, 2024,2025",0,0,3592125.2494115117,0,0]
[null,"Bells Creek","","C0562034","New line on new route - dual circuit","Demand growth",132,12,0,0,0,0,0,1564061.3440985014,24,0,348545.505520078,0,0,0,8417813.301384069,22997,15084112.213684052,1543558.6673032027,2322660.3855245532,29280751.417514455,"2021, 2022,2023,2024,2025",0,0,18136082.102355655,0,0]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",{"$f":"SUM(N104,Q104,T104,U104,W104,X104,Y104)","v":0},"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,"","","","","","","","","","","","","","","","","","","","","","","","",0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"","","","","",""]
[null,null,null,"Non material projects - [forecast]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,203536589.27675852,"2006, 2007,2008, 2009, 2010, 2011, 2012, 2013, 2014, 2015, 2016, 2017, 2018,2019, 2020, 2021, 2022, 2023, 2024, 2025",null,null,null,0,0]

{"sheet":"2.3 Augex (b)","index":9,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[51,1,51,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[45,1,46,2],[5,1,5,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[9,1,10,1],[9,2,10,2],[34,1,34,2],[29,1,30,1],[29,2,30,2],[45,3,45,9],[47,1,47,2],[9,3,9,9],[29,3,29,9],[31,1,31,2],[32,1,32,2],[33,1,33,2],[68,1,69,2],[68,3,68,9],[70,1,70,2],[71,1,71,2],[60,1,61,2],[60,3,60,9],[62,1,62,2],[63,1,63,2],[77,1,77,2],[78,1,78,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,"PROJECT TYPE","Units","VOLUMES (0's)"]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",8.4849999999999994,8.4849999999999994,17.5,20,20,20,20]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",14.595000000000001,14.595000000000001,19.8,16,16,16,16]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",70,70,70,70,70,70,70]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",13,13,13,13,13,13,13]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",88.95,86.95,81,79,79,79,79]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",33,19,17,17,17,17,17]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",135,135,110,110,110,110,110]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",12,12,12,12,12,12,12]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,"PROJECT TYPE",null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,12114008.8747104,4509104.8610358266,5381145.8478006897,6446102.3565579709,6225984.1397153605,6205076.6478441693,6275986.2053269213]
[null,"HV Feeder Augmentations - Underground Cables",null,1753610.0889304397,3537073.5783845508,1707612.1441487779,3446647.909699053,2790516.3938964047,2669655.0194574427,2716360.0765578058]
[null,"HV Feeder Non-Material Projects",null,11937855.725730939,4628418.2025183905,3999484.1074707974,5905637.9998436291,5307444.530267437,5208269.2913887631,5285588.0483090943]
[null,"LV Feeder Augmentations - Overhead Lines",null,17043092.806104783,6007329.2527069105,2453621.5138441534,2455295.2343553109,2462292.3685264308,2470585.5263804533,2478538.6406758022]
[null,"LV Feeder Augmentations - Underground Cables",null,0,0,0,0,0,0,0]
[null,"LV Feeder Non-Material Projects",null,7125032.6636531353,3875409.9591318197,3800634.2442639195,3803230.9990075901,3814082.1048850031,3826918.3622024069,3839230.3702147575]
[null,"Distribution Substation Augmentations - Pole Mounted",null,3663269.7618497107,3419191.8064484568,3448771.0122697325,4321154.9777648607,4333456.3809891678,4348093.200631503,4362068.3159995386]
[null,"Distribution Substation Augmentations - Ground Mounted",null,1032901.4572884691,1132178.8460603557,1034730.6223187832,1035473.8908528502,1038436.3125415692,1041911.8771909187,1045249.2597895964]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,1711698.8613070825,11832057.439194996,4062129.0062369443,4204114.2047923319,2480414.5400022133,4776286.8349533677,11432750.413043646]
[null,"Subtransmission Lines",null,18382755.220841996,16157209.136990529,5933210.0502198022,4660768.7543992987,12440953.543392308,7543527.846416573,9313509.5986691955]
[null,"HV Feeders",null,25805474.68937178,12674596.641938768,11088242.099420264,15798388.266100653,14323945.063879199,14083000.958690375,14277934.330193821]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,4696171.2191381799,4551370.652508812,4483501.6345885145,5356628.8686177116,5371892.6935307374,5390005.0778224217,5407317.5757891349]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,24168125.469757922,9882739.2118387297,6254255.758108072,6258526.233362901,6276374.4734114334,6297503.8885828611,6317769.0108905602]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,21108832.502835497,16313477.154202307,22955404.874925952,25720290.447429799,20227980.397522394,21748148.351042073,16585542.188912025]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,4550974.7063759016,3555946.8478809735,7631534.8580749985,6545277.4302759441,16817934.313293986,14525186.444706764,21181140.738757432]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,91322083.256876558,67855503.38879317,47145208.565424554,55453439.344426744,44303626.398444295,45313286.512800917,42153682.378740951]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,153387.36745325543,2286379.7258463777,2116225.5013262001,242088.05879715353,5566638.8122657966,5395641.4155222736,9742638.3219926525]
[null,"Subtransmission Lines",null,0,0,53742.207788595791,238404.438334935,5549086.466142864,3582594.4281505612,5733809.7190320892]
[null,"HV Feeders",null,2580547.4689371781,1267459.6641938768,2772060.5248550661,3949597.0665251631,3580986.2659697998,3520750.2396725938,3569483.5825484553]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,0,0,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,1817039.8699854685,2107.4578407186477,2689506.6241051359,2115187.8666186919,2121222.7689155256,2026200.3613613348,2135209.1151842331]

{"sheet":"2.4 Augex model","index":10,"n_rows":7857,"n_cols":50,"rows_kept":7857,"cut":false,"hidden":false,"merged":[[1278,4,1278,5],[5,1,5,4],[1276,14,1276,15],[8,11,8,15],[8,16,10,16],[8,1,11,1],[8,2,10,2],[8,3,10,3],[8,4,10,4],[8,5,10,5],[1276,11,1277,11],[1276,12,1277,13],[1275,4,1277,5],[1275,3,1277,3],[1275,11,1275,15],[1275,16,1277,16],[8,17,11,17],[9,6,10,6],[6717,1,6720,1],[6717,2,6719,2],[6717,3,6719,3],[6717,4,6718,5],[6717,6,6717,13],[6717,14,6717,21],[9,7,10,8],[9,9,9,10],[9,11,10,11],[9,12,10,13],[9,14,9,15],[8,6,8,10],[1275,1,1278,1],[1275,2,1277,2],[1275,17,1278,17],[6717,22,6719,22],[6717,23,6720,23],[6718,6,6720,6],[6718,7,6719,8],[6718,9,6718,13],[6718,14,6720,14],[6718,15,6719,16],[6718,17,6718,21],[1275,6,1275,10],[7664,1,7667,1],[7664,2,7667,2],[7664,3,7664,14],[7664,15,7664,26],[7664,27,7666,27],[7664,28,7666,28],[7665,3,7665,13],[7665,14,7666,14],[7665,15,7665,25],[7665,26,7666,26],[7836,1,7840,1],[7836,2,7836,9],[7836,10,7836,17],[7836,18,7836,25],[7836,26,7836,31],[7839,3,7839,9],[7839,11,7839,17],[7839,19,7839,25],[7837,2,7838,9],[7837,10,7838,17],[7837,18,7838,25],[7837,26,7837,31],[7839,26,7839,28],[7839,29,7839,31],[7839,38,7839,40],[7839,41,7839,43],[7839,44,7839,46],[7839,47,7839,49],[7839,32,7839,34],[7839,35,7839,37],[7836,38,7836,43],[7836,44,7836,49],[7837,38,7837,43],[7837,44,7837,49],[7838,26,7838,28],[7838,29,7838,31],[7838,32,7838,34],[7838,35,7838,37],[7838,38,7838,40],[7838,41,7838,43],[7838,44,7838,46],[7838,47,7838,49],[7836,32,7836,37],[7837,32,7837,37],[7727,4,7727,7],[7727,8,7727,11],[7728,1,7730,1],[7728,2,7730,2],[7728,3,7729,3],[7728,5,7730,5],[7728,6,7729,6],[7728,7,7729,7],[7728,9,7730,9],[7728,10,7729,10],[7728,11,7729,11]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.4 AUGEX MODEL"]
[]
[null,"There are SIX tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.4.1 - AUGEX MODEL INPUTS - ASSET STATUS - SUBTRANSMISSION LINES"]
[null,"Line ID","Primary type of area supplied by line","Line voltage","Originating substation","Terminating substation",{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual line maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual line maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network Segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Line rating",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Line rating"]
[null,null,null,null,null,null,null,null,null,"Thermal","N-1 emergency",null,null,null,"Thermal","N-1 emergency"]
[null,null," CBD, urban, long rural, or short rural "," kV "," name "," name "," km "," MVA "," MW "," MVA "," MVA "," km "," MVA "," MW "," MVA "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.2 - AUGEX MODEL INPUTS - ASSET STATUS - HIGH VOLTAGE FEEDERS"]
[null,"High voltage feeder ID","High voltage feeder type","Voltage level","Originating substation",null,{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual high voltage feeder maximum demand (50% PoE) from \", CRCP_y4, \" to \",dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual high voltage feeder maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Rating",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Rating"]
[null,null,null,null,null,null,null,null,null,"Thermal","Operational",null,null,null,"Thermal","Operational"]
[null,null," CBD, urban, short rural, or long rural "," kV "," name ",null," km "," MVA "," MW "," MVA "," MVA "," km "," MVA "," MW "," MVA "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.3 - AUGEX MODEL INPUTS - ASSET STATUS - SUBTRANSMISSION SUBSTATIONS, SUBTRANSMISSION SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"Substation ID","Subtransmission substation, subtransmission switching station, or zone substation","Primary type of area supplied by substation","Substation voltage",null,{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual substation maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual substation maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Number of transformers as at 30 June \",\"Number of transformers as at 31 December \"))","v":"Number of transformers as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Substation rating as at 30 June \",\"Substation rating as at 31 December \"))","v":"Substation rating as at 30 June "},null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Number of transformers as at 30 June \",\"Number of transformers as at 31 December \"))","v":"Number of transformers as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Substation rating as at 30 June \",\"Substation rating as at 31 December \"))","v":"Substation rating as at 30 June "}]
[null,null,null,null,"Primary","Secondary",null,null,null,"tx name plate total\n(ONAN)","tx name plate total\n(in service)","tx normal cyclic total","Substation normal cyclic","N-1 emergency",null,null,null,"tx name plate\n(ONAN)","tx name plate\n(in service)","tx normal cyclic total","Substation normal cyclic","N-1 emergency"]
[null,null," STS, SSW or ZSS ","CBD, Urban, Short rural, Long rural"," kV "," kV ",null," MVA "," MW "," MVA ","MVA "," MVA "," MVA "," MVA ",null," MVA "," MW "," MVA ","MVA "," MVA "," MVA "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.4 - AUGEX MODEL INPUTS - ASSET STATUS - DISTRIBUTION SUBSTATIONS"]
[null,"Distribution substation \ncategory ID","Description of distribution substation category",{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual substation maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual substation maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network segment ID"]
[null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category that were within the following utilisation bands:",null,null,null,null,null,null,null,null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category","Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category that were within the following utilisation bands:",null,null,null,null,null,null,null,null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category"]
[null,null,null,"0-20 %","20-40 %","40-60 %","60-80 %","80-100 %","100-120 %","120-140 %","140-160 %","160-180 %","180-200 %",">200%",null,"0-20 %","20-40 %","40-60 %","60-80 %","80-100 %","100-120 %","120-140 %","140-160 %","160-180 %","180-200 %",">200%"]
[null,null,null," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," MVA "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"ED_AUG245_00001","ED_AUG245_00002","ED_AUG245_00003","ED_AUG245_00004","ED_AUG245_00005","ED_AUG245_00006","ED_AUG245_00007","ED_AUG245_00008"]
[null,"2.4.5 - AUGEX MODEL INPUTS - NETWORK SEGMENT DATA"]
[null,null,null,null,"HISTORICAL",null,null,null,"FORECAST"]
[null,"Network segment ID","Network segment title","AER segment group","Average unit cost of augmentation for the network segment for the period","Capacity factor for the period","Mean value of the utilisation threshold for the period","Standard deviation of the utilisation threshold for the period","Average unit cost of augmentation for the network segment for the period","Capacity factor for the period","Mean value of the utilisation threshold for the period","Standard deviation of the utilisation threshold for the period"]
[null,null,null,null,{"$f":"CONCATENATE(PRCP_y5,\" to \",CRCP_y3)","v":"2014-15 to 2017-18"},null,null,null,{"$f":"CONCATENATE(CRCP_y4,\" to \",FRCP_y5)","v":"2018-19 to 2024-25"}]
[null,null,null," ID ",{"$f":"CONCATENATE(\"$0's, real \", dms_DollarReal, \" \nper MVA\")","v":"$0's, real June 2020 \nper MVA"},null," % "," % ",{"$f":"CONCATENATE(\"$0's, real \", dms_DollarReal, \" \nper MVA\")","v":"$0's, real June 2020 \nper MVA"},null," % "," % "]
[null,1]
[null,2]
[null,3]
[null,4]
[null,5]
[null,6]
[null,7]
[null,8]
[null,9]
[null,10]
[null,11]
[null,12]
[null,13]
[null,14]
[null,15]
[null,16]
[null,17]
[null,18]
[null,19]
[null,20]
[null,21]
[null,22]
[null,23]
[null,24]
[null,25]
[null,26]
[null,27]
[null,28]
[null,29]
[null,30]
[null,31]
[null,32]
[null,33]
[null,34]
[null,35]
[null,36]
[null,37]
[null,38]
[null,39]
[null,40]
[null,41]
[null,42]
[null,43]
[null,44]
[null,45]
[null,46]
[null,47]
[null,48]
[null,49]
[null,50]
[null,51]
[null,52]
[null,53]
[null,54]
[null,55]
[null,56]
[null,57]
[null,58]
[null,59]
[null,60]
[null,61]
[null,62]
[null,63]
[null,64]
[null,65]
[null,66]
[null,67]
[null,68]
[null,69]
[null,70]
[null,71]
[null,72]
[null,73]
[null,74]
[null,75]
[null,76]
[null,77]
[null,78]
[null,79]
[null,80]
[null,81]
[null,82]
[null,83]
[null,84]
[null,85]
[null,86]
[null,87]
[null,88]
[null,89]
[null,90]
[null,91]
[null,92]
[null,93]
[null,94]
[null,95]
[null,96]
[null,97]
[null,98]
[null,99]
[null,100]
[]
[]
[]
[]
[null,"2.4.6 - CAPEX AND NET CAPACITY ADDED BY SEGMENT GROUP"]
[null,"AER DNSP segment group",{"$f":"CONCATENATE(\"CAPEX\n ($0's, real \", dms_DollarReal, \")\")","v":"CAPEX\n ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"CAPEX\n ($0's, real \", dms_DollarReal, \")\")","v":"CAPEX\n ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"CAPEX\n ($0's, real \", dms_DollarReal, \")\")","v":"CAPEX\n ($0's, real June 2020)"},null,null,null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)"]
[null,null,"In total for all purposes",null,null,null,null,null,null,null,"For customer-initiated & capacity-related augmentation",null,null,null,null,null,null,null,"For NSP-initiated & capacity-related augmentation",null,null,null,null,null,null,null,"In total for all purposes",null,null,null,null,null,"For customer-initiated & capacity-related augmentation",null,null,null,null,null,"For NSP-initiated & capacity-related augmentation",null,null,null,null,null,"Residual"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"}]
[null,null,"Historical","Forecast",null,null,null,null,null,null,"Historical","Forecast",null,null,null,null,null,null,"Historical","Forecast",null,null,null,null,null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast"]
[null,null,{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2014-15 to 2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2014-15 to 2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2014-15 to 2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},"type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3"]
[null,"Subtransmission lines",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AA7842-AG7842-AM7842","v":0},{"$f":"AB7842-AH7842-AN7842","v":0},null,{"$f":"AD7842-AJ7842-AP7842","v":0},{"$f":"AE7842-AK7842-AQ7842","v":0}]
[null,"Subtransmission substations and subtransmission switching stations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AA7843-AG7843-AM7843","v":0},{"$f":"AB7843-AH7843-AN7843","v":0},{"$f":"AC7843-AI7843-AO7843","v":0},{"$f":"AD7843-AJ7843-AP7843","v":0},{"$f":"AE7843-AK7843-AQ7843","v":0},{"$f":"AF7843-AL7843-AR7843","v":0}]
[null,"Zone substations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AB7844-AH7844-AN7844","v":0},{"$f":"AC7844-AI7844-AO7844","v":0},0,{"$f":"AE7844-AK7844-AQ7844","v":0},{"$f":"AF7844-AL7844-AR7844","v":0}]
[null,"High voltage feeders - CBD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"High voltage feeders - urban",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"High voltage feeders - short rural",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"High voltage feeders - long rural",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - CBD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - urban ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - short rural ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - long rural ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[]
[null,"Unmodelled augmentation"]
[]
[]
[null,"Unmodelled augmentation - see comments in guidance paper - this should cover capex allocated to the augmentation category that is not considered to be primarily related to peak demand and capacity needs."]

{"sheet":"2.5 Connections","index":11,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[54,1,55,1],[54,2,55,2],[54,3,55,3],[54,4,54,10],[138,1,139,1],[5,1,5,2],[9,4,9,10],[9,2,10,2],[9,1,10,1],[9,3,10,3],[195,4,195,10],[138,2,139,3],[138,4,138,10],[102,1,103,1],[102,2,103,3],[102,4,102,10],[120,4,120,10],[120,2,121,3],[120,1,121,1],[159,4,159,10],[177,4,177,10]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Underground connections","0's",22153.099962537461,22009.709696959544,22149.890177077552,22185.791750832555,22232.716598081595,22232.025045728547,22307.834052673279]
[null,null,"Overhead connections","0's",13704.632638195138,13615.926727195698,13702.646959863445,13724.856848334017,13753.886094545112,13753.458277627182,13800.356210313843]
[null,null,"Distribution substations installed","MVA added",12.514694336913088,12.433690533940547,12.512881069966893,12.533162530463068,12.559671241258449,12.559280570592449,12.602106475386931]
[null,null,"Distribution substations installed","0's",103.76085372960374,103.08924134135833,103.74581971268637,103.91397576982307,104.13376271701897,104.13052361898428,104.48559840735616]
[null,null,"Distribution substations installed ","total spend $0's",2823486.3494441132,2798264.724740536,2776523.4724912657,2742584.3587086932,2887166.4214509837,3001304.0886265459,2971068.8203264028]
[null,null,"Augmentation HV ","net circuit KM added",8.0233316683316662,7.9713990873074616,8.0221691595463227,8.0351718649978654,8.0521669407931959,8.051916476799267,8.0793727157542232]
[null,null,"Augmentation HV","total spend $0's",604213.15039268474,598815.83819276176,594204.61878682883,586929.85552045959,617807.49235787918,642162.84132038918,635622.02722826716]
[null,null,"Augmentation LV","net circuit KM added",73.463758091896224,72.988249571600534,73.453113852356282,73.572170080781021,73.727781513611291,73.725488198686605,73.976884822942026]
[null,null,"Augmentation LV","total spend $0's",10391751.493497584,10298924.107867248,10217806.026279137,10093212.394293431,10627000.174146499,11048933.441440228,10939533.777485808]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",8,8,8,8,8,8,8]
[null,null,"Volume of GSL breaches for residential customers","0's",41,41,41,41,41,41,41]
[null,null,"Volume of customer complaints relating to connection services","0's",535,535,535,535,535,535,535]
[null,null,"GSL payments","$0's",9839.7206583153657,9839.7206583153657,9839.7206583153638,9839.7206583153638,9839.720658315362,9839.7206583153638,9839.7206583153638]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",4943.5157232704405,4776.3747495317784,4776.3747495317784,4776.3747495317784,4776.3747495317784,4776.3747495317784,4776.3747495317784]
[null,null,"Overhead connections","0's",3148.9979035639412,3042.5298340026116,3042.5298340026116,3042.5298340026116,3042.5298340026116,3042.5298340026116,3042.5298340026116]
[null,null,"Distribution substations installed","MVA added",220.37458280922431,212.92368664142219,212.92368664142219,212.92368664142219,212.92368664142219,212.92368664142219,212.92368664142219]
[null,null,"Distribution substations installed","0's",387.2473794549266,374.15449016256235,374.15449016256235,374.15449016256235,374.15449016256235,374.15449016256235,374.15449016256235]
[null,null,"Distribution substations installed ","total spend $0's",22759085.061454728,22158589.340316851,21811057.040482331,21918758.579709679,21621804.252412569,21380017.413934171,21568169.63629771]
[null,null,"Augmentation HV ","net circuit KM added",54.781509433962263,52.92933876389332,52.92933876389332,52.92933876389332,52.92933876389332,52.92933876389332,52.92933876389332]
[null,null,"Augmentation HV","total spend $0's",17363907.101145301,16905762.501381371,16648677.982909475,16728506.743743945,16489827.314707566,16291824.278907824,16421757.68986671]
[null,null,"Augmentation LV","net circuit KM added",49.670621962697233,47.991251129107987,47.991251129107987,47.991251129107987,47.991251129107987,47.991251129107987,47.991251129107987]
[null,null,"Augmentation LV","total spend $0's",2682252.4643917102,2611481.5558279632,2569805.7238302566,2582707.2141969828,2548788.7228870741,2521497.7490097764,2544884.2603274784]
[null,"SUBDIVISION","Underground connections","0's",19512.758014357933,19386.457877647139,19509.930790761096,19541.553395371768,19582.885452319988,19582.276323406109,19649.049949233777]
[null,null,"Overhead connections","0's",211.2656695653711,209.89821126302502,211.23505906501245,211.57743868820864,212.02494306863784,212.01834799746709,212.74130959825203]
[null,null,"Distribution substations installed","MVA added",2.2896771978021979,2.2748568150099131,2.2893454441158143,2.2930561218508068,2.2979061316886251,2.2978346549356408,2.3056700438826918]
[null,null,"Distribution substations installed","0's",4.0999729437229435,4.0734350681995686,4.0993788944222569,4.1060233586860173,4.1147079493046999,4.1145799606285571,4.1286102714152877]
[null,null,"Distribution substations installed ","total spend $0's",1316318.6072942719,1316061.7742061713,1314043.9301047397,1314374.3528926636,1314292.1476793925,1315098.6503974078,1314284.1420359693]
[null,null,"Augmentation HV ","net circuit KM added",6.5094955044955043,6.4673615236645459,6.5085523369904141,6.5191017017907225,6.5328901595114619,6.5326869528748785,6.5549627693855035]
[null,null,"Augmentation HV","total spend $0's",38693157.907950856,38685608.30470223,38624627.132787362,38634821.980049461,38634917.654967219,38661432.487082466,38640338.721910447]
[null,null,"Augmentation LV","net circuit KM added",0.55507326007326008,0.55148044000240315,0.55499283493716711,0.55589239317595307,0.55706815313663627,0.55705082543894313,0.55895031366853132]
[null,null,"Augmentation LV","total spend $0's",250641.563955814,250592.66010645684,250169.87543496425,250243.94617839632,250286.41997158877,250504.95349345697,250415.77709073469]
[null,null,"Cost per lot","$0's",219.90505191866026,218.48167352692886,219.8731896492983,220.22957035691513,220.6953747358971,220.68850996950513,221.44103596524727]
[null,"EMBEDDED GENERATION","Underground connections","0's",114.33,120.67,127,133.33000000000001,139.66999999999999,146,152.33000000000001]
[null,null,"Overhead connections","0's",45.33,51.67,58,64.33,70.67,77,83.33]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Underground connections","0's",21522.97,21383.65,21519.85,21554.73,21600.32,21599.65,21673.3]
[null,null,"Overhead connections","0's",13346.36,13259.97,13344.42,13366.05,13394.32,13393.91,13439.58]
[null,null,"Distribution substations installed","MVA added",9.7899999999999991,9.7200000000000006,9.7899999999999991,9.8000000000000007,9.82,9.82,9.86]
[null,null,"Distribution substations installed","0's",103.6,102.93,103.59,103.76,103.98,103.97,104.33]
[null,null,"Distribution substations installed ","total spend $0's",2298820.0130887488,2284504.4290580521,2295270.4084265763,2300220.3194744997,2311185.4597587045,2317865.8335756483,2332703.0421131882]
[null,null,"Augmentation HV ","net circuit KM added",5.89,5.85,5.88,5.89,5.91,5.91,5.93]
[null,null,"Augmentation HV","total spend $0's",468248.43169162073,465332.47519087937,467525.40488267643,468533.65807352116,470767.15945515543,472127.89062197821,475150.09326590283]
[null,null,"Augmentation LV","net circuit KM added",77.8,77.3,77.790000000000006,77.92,78.08,78.08,78.349999999999994]
[null,null,"Augmentation LV","total spend $0's",9091580.2359015327,9034963.6545346789,9077541.9538428392,9097118.280660823,9140484.2232319005,9166904.3635681588,9225583.8818718884]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",8,8,8,8,8,8,8]
[null,null,"Volume of GSL breaches for residential customers","0's",41,41,41,41,41,41,41]
[null,null,"Volume of customer complaints relating to connection services","0's",535,535,535,535,535,535,535]
[null,null,"GSL payments","$0's",9839.7206583153657,9839.7206583153657,9839.7206583153638,9839.7206583153638,9839.720658315362,9839.7206583153638,9839.7206583153638]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",6120.14,5913.22,5913.22,5913.22,5913.22,5913.22,5913.22]
[null,null,"Overhead connections","0's",3388.5,3273.94,3273.94,3273.94,3273.94,3273.94,3273.94]
[null,null,"Distribution substations installed","MVA added",197.95,191.26,191.26,191.26,191.26,191.26,191.26]
[null,null,"Distribution substations installed","0's",362.98,350.71,350.71,350.71,350.71,350.71,350.71]
[null,null,"Distribution substations installed ","total spend $0's",18040819.754694246,17435161.24182659,17406464.15928093,17415774.07641096,17461861.69933635,17512879.121854499,17565087.992966536]
[null,null,"Augmentation HV ","net circuit KM added",47.95,46.33,46.33,46.33,46.33,46.33,46.33]
[null,null,"Augmentation HV","total spend $0's",8979232.9675670695,8677786.0896528848,8663503.047455892,8668136.7567887902,8691075.376488369,8716467.6440629214,8742452.9165366665]
[null,null,"Augmentation LV","net circuit KM added",50.27,48.58,48.58,48.58,48.58,48.58,48.58]
[null,null,"Augmentation LV","total spend $0's",2552094.6864177454,2466416.8771134377,2462357.3236781224,2463674.3253631401,2470193.9835086879,2477411.0221228036,2484796.605717916]
[null,"SUBDIVISION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",955756.27990617929,949804.43871406361,954280.50663653424,956338.47331366222,960897.33974691154,963674.76252662216,969843.47186613001]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",22114.939552330725,21977.218886363102,22080.787165951875,22128.408430203312,22233.896558967164,22298.164608633997,22440.900902394176]
[null,null,"Cost per lot","$0's",0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,9356958.0013291519,9298688.811680181,9342509.9441557713,9362657.7011144049,9407289.4632728714,9434480.7923614848,9494873.136271622]
[null,null,"Complex connection LV",null,4166927.4974764455,4103590.9507896225,3950915.0585966809,3764323.3677134123,4427529.263866446,4959905.3077233834,4751429.5606092252]
[null,null,"Complex connection HV",null,295565.49452878645,293724.90833074192,295109.11480477662,295745.53969476611,297155.36081604759,298014.27130229573,299921.92815962987]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,851284.7751464491,822705.81546494295,821351.69797960785,821791.00122769014,823965.71902213851,826373.05725168227,828836.61587824055]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,28480346.24774259,27527179.660005145,25890527.637571514,28440754.251262218,27731355.885174319,27045389.213076353,27529580.308087405]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,9765937.4269368164,7566567.1960143475,9043518.2537639122,7909257.2667075535,7665328.6298963539,5496921.4213820938,11351169.360438326]
[null,null,"Complex connection HV (customer connected at HV)",null,615040.23386897612,423215.17657690833,456858.66506535187,2193872.206756976,2559548.0847419673,1391844.4680842406,388965.55945636868]
[null,null,"Complex connection sub-transmission",null,3092635.9432969089,5336165.5494648321,4817284.4928416731,1864297.8116961676,1880221.9711724366,5432811.2820574008,436259.74263155449]
[null,"SUBDIVISION","Complex connection LV",null,3411869.3722957252,4137797.4927629759,2759608.4685486597,749257.15593741892,3988569.6420044047,2196023.7654214962,4570857.6781346276]
[null,null,"Complex connection HV (no upstream asset works)",null,33459678.65943782,33125873.225446209,32953809.367804252,37284299.944537133,33711180.807966486,33702563.374174312,32773622.479901332]
[null,null,"Complex connection HV (with upstream asset works)",null,3388570.0474674092,2988592.0208056723,4475423.1019741474,2165883.1786459773,2499745.7726473119,4328448.9513775194,2860558.483001186]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,9356958.0013291519,9298688.811680181,9342509.9441557713,9362657.7011144049,9407289.4632728714,9434480.7923614848,9494873.136271622]
[null,null,"Complex connection LV",null,2206125.1848239652,2192386.8387726881,2202718.7081915452,2207469.0173996706,2217992.0183568434,2224403.0241020047,2238641.9528197264]
[null,null,"Complex connection HV",null,295565.49452878645,293724.90833074192,295109.11480477662,295745.53969476611,297155.36081604759,298014.27130229573,299921.92815962987]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,851284.7751464491,822705.81546494295,821351.69797960785,821791.00122769014,823965.71902213851,826373.05725168227,828836.61587824055]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,28122336.985345189,27178226.188245684,27133492.687387791,27148005.144717228,27219847.316003833,27299374.142828532,27380758.220006544]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,197613.280922354,190979.094792827,190664.75626898141,190766.73407815842,191271.56293436248,191830.391214528,192402.27023571037]
[null,null,"Complex connection HV (customer connected at HV)",null,361390.75038072013,349258.30159557727,348683.44632629538,348869.94106527313,349793.16079833091,350815.13347144425,351860.97304814227]
[null,null,"Complex connection sub-transmission",null,39521.616884351337,38194.80849388583,38131.942452272444,38152.337474546308,38253.300574752728,38365.063274042121,38479.436052483798]
[null,"SUBDIVISION","Complex connection LV",null,22114.939552330725,21977.218886363102,22080.787165951875,22128.408430203312,22233.896558967164,22298.164608633997,22440.900902394176]
[null,null,"Complex connection HV (no upstream asset works)",null,955756.27990617929,949804.43871406361,954280.50663653424,956338.47331366222,960897.33974691154,963674.76252662216,969843.47186613001]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection LV",null,1960802.3126524799,1911204.1120169347,1748196.3504051354,1556854.3503137417,2209537.2455096031,2735502.2836213782,2512787.6077894988]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,358009.26239740156,348953.47175946063,-1242965.0498162783,1292749.1065449871,511508.56917048572,-253984.92975217826,148822.08808086015]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,9568324.1460144632,7375588.1012215205,8852853.4974949304,7718490.5326293949,7474057.0669619916,5305091.0301675657,11158767.090202617]
[null,null,"Complex connection HV (customer connected at HV)",null,253649.48348825594,73956.874981331042,108175.21873905646,1845002.2656917027,2209754.9239436365,1041029.3346127963,37104.586408226445]
[null,null,"Complex connection sub-transmission",null,3053114.3264125576,5297970.7409709459,4779152.5503894007,1826145.4742216212,1841968.6705976841,5394446.218783359,397780.30657907069]
[null,"SUBDIVISION","Complex connection LV",null,3389754.4327433943,4115820.2738766125,2737527.6813827078,727128.74750721559,3966335.7454454377,2173725.6008128622,4548416.7772322334]
[null,null,"Complex connection HV (no upstream asset works)",null,32503922.379531641,32176068.786732145,31999528.861167718,36327961.471223474,32750283.468219571,32738888.611647692,31803779.008035202]
[null,null,"Complex connection HV (with upstream asset works)",null,3388570.0474674092,2988592.0208056723,4475423.1019741474,2165883.1786459773,2499745.7726473119,4328448.9513775194,2860558.483001186]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,34532,34308,34527,34583,34656,34655,34773]
[null,null,"Complex connection LV",null,60,59,60,60,60,60,60]
[null,null,"Complex connection HV",null,335,333,335,335,336,336,337]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,366,364,366,367,367,367,369]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,2401,2320,2320,2320,2320,2320,2320]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,286,276,276,276,276,276,276]
[null,null,"Complex connection HV (customer connected at HV)",null,9,8,8,8,8,8,8]
[null,null,"Complex connection sub-transmission",null,15,14,14,14,14,14,14]
[null,"SUBDIVISION","Complex connection LV",null,3,3,3,3,3,3,3]
[null,null,"Complex connection HV (no upstream asset works)",null,17247,17136,17245,17273,17309,17309,17368]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,109,115,120,125,131,136,141]
[null,null,"Complex connection HV (small capacity)",null,4,5,6,7,8,9,10]
[null,null,"Complex connection HV (large capacity)",null,1,1,1,1,1,1,1]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,34531.550000000003,34308.04,34526.550000000003,34582.51,34655.65,34654.57,34772.74]
[null,null,"Complex connection LV",null,59.61,59.22,59.6,59.7,59.82,59.82,60.02]
[null,null,"Complex connection HV",null,334.94,332.77,334.89,335.43,336.14,336.13,337.28]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,411.34,397.43,397.43,397.43,397.43,397.43,397.43]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1440.22,1391.53,1391.53,1391.53,1391.53,1391.53,1391.53]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,1380337.7326007325,1402347.4422976919]
[null,null,"Complex connection LV",null,0,0]
[null,null,"Complex connection HV",null,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,112936.15912212786,113299.94820783399]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,16074.993710691824,18761.987421383648]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,648,671.38364779874212]
[null,null,"Complex connection sub-transmission",null,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,355870,355990]
[null,null,"Complex connection HV (small capacity)",null,"",""]
[null,null,"Complex connection HV (large capacity)",null,8,9]

{"sheet":"2.6 Non-network","index":12,"n_rows":123,"n_cols":11,"rows_kept":123,"cut":false,"hidden":false,"merged":[[119,1,119,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[113,1,113,3],[114,1,114,3],[115,1,115,3],[117,1,117,3],[118,1,118,3],[107,1,107,3],[108,1,108,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[93,4,93,10],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[106,1,106,3],[100,1,100,3],[101,1,101,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[5,1,5,2],[19,1,29,1],[32,1,36,1],[39,1,49,1],[64,1,68,1],[69,1,73,1],[74,1,78,1],[79,1,83,1],[84,1,88,1],[55,4,55,10],[8,4,8,10],[62,4,62,10],[55,1,56,3],[12,1,16,1],[59,1,59,3],[58,1,58,3],[57,1,57,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.6 NON NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2020)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,21941975.647332922,21925321.776610591,20494742.779221985,20367344.309702076,20260852.413827442,20173036.612775717,20057076.56938057]
[null,"MOTOR VEHICLES","Car",null,2122662.0150546748,2121050.9231751603,1982657.0179909251,1970332.5173911408,1960030.5142389438,1951535.2324917533,1940317.2827804249]
[null,null,"Light commercial vehicle",null,787035.53355145082,786438.17676643224,735124.81635651423,730555.1675681005,726735.4155350246,723585.55533347116,719426.19083088392]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,4334732.097028262,4331442.0529082548,4048824.9906626022,4023656.8725397778,4002618.9383746609,3985270.5474383412,3962362.1398201399]
[null,null,"Heavy commercial vehicle",null,2832244.7467662776,2830095.0844649081,2645437.6080684955,2628993.1615043739,2615247.3111984655,2603912.1495334748,2588944.1617360488]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,20759046.935865004,20743290.903247643,19389836.819186509,19269306.614849932,19168555.875705823,19085474.371786423,18975765.928836007]
[null,"OTHER","Other expenditure",null,0,0,0,0,0,0,0]
[null,"OTHER - DNSP nominated","Office furniture and equipment",null,0,0,0,0,0,0,0]
[null,null,"Plant and equipment",null,5951352.7161978967,5946835.6635700213,5558817.7230397118,5524263.2581272088,5495379.3123990297,5471560.9099673517,5440108.9053565441]
[null,null,"Non-Network Expenditure Fleet",null,0,0,0,0,0,0,0]
[null,null,"Motor Vehicles Generators",null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,74948827.29980965,49867667.842163734,37003762.064382821,36843387.042695574,42490560.699352413,38467963.302010216,38176224.49935741]
[null,"MOTOR VEHICLES","Car",null,178736.3811035057,185992.22610841217,241815.53843934214,480576.70349371771,480836.71663896157,240572.61152682771,481137.47195942694]
[null,null,"Light commercial vehicle",null,4656794.2455353672,6295217.3548983019,4933809.5313207442,5216085.9210450314,3672866.763010093,4095992.3936088574,5568557.8586446773]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,2833168.9314679159,3511609.5771539328,1239158.0835834052,5545326.6779064517,6660954.8123049652,13727999.640854355,11312318.92604332]
[null,null,"Heavy commercial vehicle",null,11774794.530892376,8007289.9454240547,2422140.4896386028,4735840.0319116181,4070868.3693599436,5945149.6888804818,5464186.7735965746]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,19233957.515145823,30860998.011809111,13582446.679438543,13684237.975219607,22683104.762806963,20082608.0103641,10557041.95770324]
[null,"OTHER","Other expenditure",null,0,0,0,0,0,0,0]
[null,"OTHER - DNSP nominated","Office furniture and equipment",null,0,0,0,0,0,0,0]
[null,null,"Plant and equipment",null,7749086.2320476072,7768977.3464297596,7348915.1516797636,7780000.5560818566,7297437.1430169437,6919185.8938320866,6512010.3244751506]
[null,null,"Non-Network Expenditure Fleet",null,1458069.2415724464,353545.16502372542,704668.10201322113,1127342.9183974299,2218610.8222134169,1699010.1091333739,1461704.5231439113]
[null,null,"Motor Vehicles Generators",null,334638.75074563874,0,4584883.8295281213,61411.662572733672,71733.414567998654,0,2933185.7233397048]
[]
[null,null,"IT & Communications-Capitalised Operational Exp",null,22519773.522341244,22519773.522341244,22092849.092747532,21292750.526388284,20180666.820435833,18825790.510047249,17261068.882950395]
[null,null,"Motor Vehicles-Capitlaised Operational Exp",null,10342022.697361454,10342022.697361454,10145961.127890695,9778522.3734465335,9267806.9829513282,8645591.0650045965,7927005.3933310378]
[null,null,"Buildings & Property-Capitlaised Operational Exp",null,21305693.82501781,21305693.82501781,20901785.625216413,20144821.74777003,19092692.385842472,17810859.786093134,16330494.991339047]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Employee numbers",null,null,2305.1143333333334,2305.1143333333334,2305.1143333333334,2305.1143333333334,2305.1143333333334,2305.1143333333334,2305.1143333333334]
[null,"User numbers",null,null,3977.9199999999996,3977.9199999999996,3977.9199999999996,3977.9199999999996,3977.9199999999996,3977.9199999999996,3977.9199999999996]
[null,"Number of devices",null,null,4372.6666666666661,4372.6666666666661,4372.6666666666661,4372.6666666666661,4372.6666666666661,4372.6666666666661,4372.6666666666661]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"CAR","Average kilometres travelled ","0's",24365.104508670524,24365.104508670524,24365.104508670524,24365.104508670524,24365.104508670524,24365.104508670524,24365.104508670524]
[null,null,"Number purchased","0's",3.348206737911045,4.166657273844856,5.0980765029635027,10.185538267103215,10.160805550800001,5.0542961795999997,10.201927795720625]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",38.75,38.75,38.75,38.75,38.75,38.75,38.75]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.82499999999999996,0.83499999999999996,0.85,0.84899999999999998,0.84699999999999998,0.84199999999999997,0.85]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",24887.544137273591,24887.544137273591,24887.544137273591,24887.544137273591,24887.544137273591,24887.544137273591,24887.544137273591]
[null,null,"Number purchased","0's",78.348037667118575,160.90970622633762,96.863453556306553,111.19212608254344,69.432171263800001,76.656825390600005,111.37104510328349]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",784.83333333333303,784.83333333333303,784.83333333333303,784.83333333333303,784.83333333333303,784.83333333333303,784.83333333333303]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.82499999999999996,0.83499999999999996,0.85,0.84899999999999998,0.84699999999999998,0.84199999999999997,0.85]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",22493.723288909361,22493.723288909361,22493.723288909361,22493.723288909361,22493.723288909361,22493.723288909361,22493.723288909361]
[null,null,"Number purchased","0's",8.0356961709865171,14.224062428847489,8.4967941716058384,15.278307400654825,11.8542731426,37.064838650399999,31.45594403680526]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",235.16666666666666,235.16666666666666,235.16666666666666,235.16666666666666,235.16666666666666,235.16666666666666,235.16666666666666]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.82499999999999996,0.83499999999999996,0.85,0.84899999999999998,0.84699999999999998,0.84199999999999997,0.85]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",24804.442622950828,24804.442622950828,24804.442622950828,24804.442622950828,24804.442622950828,24804.442622950828,24804.442622950828]
[null,null,"Number purchased","0's",52.901666458994519,59.563261420798916,11.045832423087589,28.85902509012578,19.474877305700002,30.325777077599998,29.75562273751849]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",269.41666666666669,269.41666666666669,269.41666666666669,269.41666666666669,269.41666666666669,269.41666666666669,269.41666666666669]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.82499999999999996,0.83499999999999996,0.85,0.84899999999999998,0.84699999999999998,0.84199999999999997,0.85]
[]
[]
[]
[null,"2.6.4 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX BY PURPOSE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"ICT CAPABILITY GROWTH"]
[null,"Distribution operations, asset and works management",null,null,1370634.8373435216,0,1760286.6360780003,1213482.8833454333,1695885.6793611494,1860743.3576550377,1258365.1961351377]
[null,"Customer and market systems",null,null,6048314.1197856124,2710735.7717617908,662903.26494368771,1208730.1092268405,1092817.9893725982,593110.94528013596,778707.2897506475]
[null,"Corporate systems",null,null,0,0,385173.57239919144,65054.174379759927,336978.59684347454,172111.48926055306,530887.49503232539]
[null,"ICT Management systems, productivity and cybersecurity ",null,null,2651131.2792629893,2204356.9608957265,106903.89376266241,359844.73659171705,289851.83022415912,342290.74044749531,390979.58370849321]
[null,"Infrastructure program",null,null,33679.389125416747,0,613446.17428235733,608558.23944706528,604491.72088584385,608024.12317805737,609650.18324534828]
[null,"Minor applications change",null,null,0,0,303737.02503197512,302154.43737644487,303255.5606306612,304475.62495665572,305806.31836179126]
[null,"ICT ASSET EXTENSIONS"]
[null,"Distribution operations, asset and works management",null,null,573984.79392161407,440871.43432830216,572408.49293761281,29460.024504398003,414508.05365310964,25577.784286873266,191296.78885266281]
[null,"Customer and market systems",null,null,1643701.4163250898,330653.60208944959,347503.02395620762,0,0,53188.042292105922,150408.14034064196]
[null,"Corporate systems",null,null,22092.79666292969,440871.43432830216,107022.59397642895,0,0,309233.10957527411,621169.0974668467]
[null,"ICT Management systems, productivity and cybersecurity ",null,null,6601833.3906160081,2247897.4613765422,347437.62844428309,1169495.4202245134,264431.55918293557,1056366.8247031197,507063.55995508831]
[null,"Infrastructure program",null,null,0,2645228.3952240287,0,0,0,0,0]
[null,"Minor applications change",null,null,2303837.822300578,1966287.3536815923,987145.35763828887,982002.0792820428,985580.75678308634,989545.88706647244,993870.55594695464]
[null,"ICT ASSET REMEDIATION"]
[null,"Distribution operations, asset and works management",null,null,55679.03615178667,0,132094.3080384795,6798.4995643168722,95655.712809330245,5902.5656046630611,44145.407903429899]
[null,"Customer and market systems",null,null,0,0,80192.98126586045,0,0,12274.204358694125,34709.575756563499]
[null,"Corporate systems",null,null,1190156.4681529498,0,24697.529774366605,0,0,71361.52757788678,143346.71970876458]
[null,"ICT Management systems, productivity and cybersecurity ",null,null,0,0,80177.946606366546,269883.526142355,61022.626902998898,243777.00845026199,117014.67340878701]
[null,"Infrastructure program",null,null,0,0,0,0,0,0,0]
[null,"Minor applications change",null,null,44185.487952967349,220435.66447770502,227802.74248961158,226615.88063519931,227441.69686348696,228356.71871749181,229354.73877134343]
[null,"ICT ASSET REPLACEMENT"]
[null,"Distribution operations, asset and works management",null,null,8286017.6073781028,17200230.336385831,15138078.816200532,10885088.278206609,14752808.582862889,16715210.631896658,11089844.515282314]
[null,"Customer and market systems",null,null,1332082.268080119,374742.46310041996,5538433.6210873229,10878571.298658758,9835361.5876674931,5272535.7310837181,6823249.316824547]
[null,"Corporate systems",null,null,34413235.555337645,9626813.2547362763,3334842.2381168855,585487.148594914,3032806.8437814494,1168408.7661918164,4013471.6168441842]
[null,"ICT Management systems, productivity and cybersecurity ",null,null,1147500.9945923444,2345435.8788896031,534519.3636758331,1799223.7881643169,2283211.7581216767,1780472.8308740763,2894738.0200125631]
[null,"Infrastructure program",null,null,7129744.8358509382,5570057.0156003134,4200269.7260669842,4742164.1205880083,4698172.1313621774,5132617.1548340814,4919114.0855560964]
[null,"Minor applications change",null,null,101015.1960857864,1543050.8104457476,1518685.1251598755,1510772.3972936871,1516278.0142772344,1522378.2307406201,1529031.6237156559]

{"sheet":"2.10 Overheads","index":13,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,3,8,9],[23,3,23,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE ($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE ($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",101310219.15567547,101233325.10931484,94628073.418473497,94039850.77733092,93548157.709998846,93142695.677186757,92607286.395976841]
[null,"Alternative Control Services","Total  ",11130458.374762937,10273283.559922427,10920931.065689825,10541304.905272121,10092448.38548803,9598891.5389414784,9041721.4255120419]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",48751042.183742888,48751042.183742888,47826831.69575794,46094769.9180924,43687319.434322856,40754268.971094184,37366943.162833437]
[null,"Alternative Control Services","Total  ",3421601.38983759,3268362.6065648366,3380290.7888565203,3259150.7011154052,3019170.8590276954,2806227.6465324746,2458649.569787581]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total  ",1309421.8495934561,1266439.9309368939,1169289.5192459512,1205465.149176196,1145823.1309762369,1147144.8731146122,1143583.1418538312]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",68159689.547360271,68107956.618819997,69900122.636872172,69493772.695231438,69151587.652526602,68863935.881136641,68478174.799640939]
[null,"Alternative Control Services","Total  ",8453419.4306747131,6290716.9040536657,7225505.5924549382,6951816.1007595863,6608289.1071632365,6223208.5297834454,5779461.5414694306]
[null,"CAPEX"]
[null,"Standard Control Services","Total",9285912.7969034091,9285912.7969034091,9109872.7039538957,8779956.1748747453,8321394.1779662604,7762717.8992560375,7117512.9833968477]
[null,"Alternative Control Services","Total",1488210.2135912867,1346880.2550944814,1463788.3380170751,1400885.6201815768,1311346.2212874149,1220818.6517836507,1098177.4317296047]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",565377.11756227468,572412.81717423326,514834.2867547113,580928.71136910701,547231.87116415403,547970.2311490064,546556.05500534817]

{"sheet":"2.11 Labour","index":14,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[8,2,8,8],[9,2,9,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"($0's, real \", dms_DollarReal,\")\")","v":"($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"In-house labour expenditure",258919683.83512744,258723164.84288341,246044531.13942757,244534057.5435873,243269761.07814744,242223500.12556347,240837932.13205656]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",81064047.145466,81002519.861729667,77033021.115811586,76560113.452046856,76164280.324328661,75836710.994988933,75402909.487566993]
[null,"Controllable non-labour expenditure",31655004.129005473,31630978.108971886,30080913.639989272,29896246.150809407,29741675.786590707,29613762.009300791,29444365.229937319]
[null,"Uncontrollable non-labour expenditure",12571882.052491805,12562340.044889404,11946727.183226509,11873385.923075739,11811997.828484161,11761196.47921174,11693920.028336847]
[null,"Total",{"$f":"SUM(C13:C17)","v":384210617.16209072},{"$f":"SUM(D13:D17)","v":383919002.85847437},365105193.07845491,362863803.06951928,360987715.01755095,359435169.60906494,357379126.87789768]
[null,"CAPEX"]
[null,"In-house labour expenditure",234284995.57141668,226738685.0611186,213206400.97087494,202260958.74965823,196112575.06894779,194401797.20590115,191196807.54851314]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",146832100.68206641,122380357.56107469,91166749.832481578,83981674.269389704,103568091.25825831,96904652.0553094,85340155.719458744]
[null,"Controllable non-labour expenditure",128120024.82819128,120123294.7054113,117888476.67512754,123203512.44428588,117825088.919742,121737295.90936705,120801377.65387136]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C20:C24)","v":509237121.08167434},{"$f":"SUM(D20:D24)","v":469242337.32760459},{"$f":"SUM(E20:E24)","v":422261627.47848403},{"$f":"SUM(F20:F24)","v":409446145.46333379},{"$f":"SUM(G20:G24)","v":417505755.24694812},{"$f":"SUM(H20:H24)","v":413043745.17057765},{"$f":"SUM(I20:I24)","v":397338340.92184323}]

{"sheet":"2.14 Forecast price changes","index":15,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[[5,1,5,2],[7,1,7,2],[8,1,8,2],[11,4,11,8],[12,2,12,8],[11,1,13,1],[11,2,11,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet. It has been grouped for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"Energex must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"Labour - internal",0,0,-3.1375543063968969E-3,9.1387375098661225E-4,4.7251369850541056E-3,5.2496028058078778E-3,5.2496028058078778E-3]
[null,"Contractors",0,0,-3.1375543063968969E-3,9.1387375098661225E-4,4.7251369850541056E-3,5.2496028058078778E-3,5.2496028058078778E-3]
[null,"CPI",2.0000000000000018E-2,2.2499999999999964E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2]
[null,"CAPEX"]
[null,"Labour - Internal",0,0,-3.1375543063968969E-3,9.1387375098661225E-4,4.7251369850541056E-3,5.2496028058078778E-3,5.2496028058078778E-3]
[null,"Contractors",0,0,-3.1375543063968969E-3,9.1387375098661225E-4,4.7251369850541056E-3,5.2496028058078778E-3,5.2496028058078778E-3]
[null,"Materials",0,0,0,0,0,0,0]
[null,"Other",0,0,0,0,0,0,0]
[null,"CPI",2.0000000000000018E-2,2.2499999999999964E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2,2.4199999999999999E-2]

{"sheet":"2.16 Opex Summary","index":16,"n_rows":67,"n_cols":12,"rows_kept":67,"cut":false,"hidden":false,"merged":[[29,2,29,11],[57,2,57,11],[43,2,43,11],[56,2,56,11],[5,1,5,6],[15,2,15,11],[14,2,14,11],[28,2,28,11],[42,2,42,11],[7,9,7,11],[9,1,9,7],[9,9,9,10],[8,11,9,11],[8,9,8,10],[8,1,8,7],[10,1,10,7],[10,9,10,10]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nEnergex's total forecast opex must reconcile to Table 2.16.1 (and if Energex owns any dual function assets Table 2.16.3). If Energex did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if Energex owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has Energex used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If Energex does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2018-19"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Base year total opex, excluding category specific",null,null,null,361616964.84756356,361616964.84756356,361616964.84756356,361616964.84756356,361616964.84756356,361616964.84756356,361616964.84756356]
[null,"Increment from base year to final year",null,null,null,null,0]
[null,"Price growth",null,null,null,null,null,-694741.99609549355,-508073.55127088417,589851.64888048091,1918506.3013432771,3337067.3730012109]
[null,"Output growth",null,null,null,null,null,4330486.51617458,8579989.4678786006,12676086.655235916,17515291.565920044,21933324.370524172]
[null,"Productivity growth",null,null,null,null,null,-6383576.5992671214,-13050533.654593101,-20109261.285347659,-27814802.033678439,-35681891.274399951]
[null,"Step changes",null,null,null,null,null,0,0,0,0,0]
[null,"Category specific",null,null,null,0,0,6236060.3100793064,6225455.9599410165,6214073.1512185736,6199208.9279164132,6173661.5612086207]
[null,"Total opex",{"$f":"SUM(C18:C24)","v":0},{"$f":"SUM(D18:D24)","v":0},{"$f":"SUM(E18:E24)","v":0},361616964.84756356,361616964.84756356,365105193.07845485,362863803.06951916,360987715.01755095,359435169.60906488,357379126.87789762]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C32:C38)","v":0},{"$f":"SUM(D32:D38)","v":0},0,0,0,{"$f":"SUM(H32:H38)","v":0},0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Base year total opex, excluding category specific"]
[null,"Increment from base year to final year"]
[null,"Price growth"]
[null,"Output growth"]
[null,"Productivity growth"]
[null,"Step changes"]
[null,"Category specific"]
[null,"Total opex",{"$f":"SUM(C46:C52)","v":0},{"$f":"SUM(D46:D52)","v":0},0,0,0,{"$f":"SUM(H46:H52)","v":0},0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C60:C66)","v":0},{"$f":"SUM(D60:D66)","v":0},0,0,0,{"$f":"SUM(H60:H66)","v":0},0,0,0,0]

{"sheet":"2.17 Step Changes","index":17,"n_rows":93,"n_cols":11,"rows_kept":93,"cut":false,"hidden":false,"merged":[[32,2,32,3],[41,2,41,3],[47,2,47,3],[48,2,48,3],[70,2,70,3],[57,2,57,3],[42,1,42,3],[50,2,50,3],[51,2,51,3],[52,2,52,3],[53,2,53,3],[49,2,49,3],[54,2,54,3],[55,2,55,3],[56,2,56,3],[23,2,23,3],[24,2,24,3],[25,1,25,3],[26,1,26,3],[31,2,31,3],[92,1,92,2],[58,1,58,3],[59,1,59,3],[79,3,79,10],[80,3,80,10],[64,2,64,3],[65,2,65,3],[66,2,66,3],[67,2,67,3],[73,2,73,3],[74,2,74,3],[75,1,75,3],[68,2,68,3],[69,2,69,3],[71,2,71,3],[72,2,72,3],[46,4,46,10],[63,4,63,10],[45,4,45,10],[62,4,62,10],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,2,36,3],[37,2,37,3],[38,2,38,3],[39,2,39,3],[40,2,40,3],[8,1,8,2],[5,1,5,2],[13,4,13,10],[30,4,30,10],[9,1,9,2],[12,4,12,10],[29,4,29,10],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(\"Complete the Tables below in accordance with the regulatory information notice. If \",dms_TradingName,\" does not own any dual function assets,Table 2.17.3 and 2.17.4 may be left blank.\"&\"\n\nThe total step changes in Table 2.17.1 and Table 2.17.3 must reconcile (in each year) to the total step changes for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary', respectively.\")","v":"Complete the Tables below in accordance with the regulatory information notice. If Energex does not own any dual function assets,Table 2.17.3 and 2.17.4 may be left blank.\n\nThe total step changes in Table 2.17.1 and Table 2.17.3 must reconcile (in each year) to the total step changes for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary', respectively."}]
[null," The total category specific forecast in Table 2.17.5 must reconcile (in each year) to the total category specific forecasts for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary'."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"Total",null,null,{"$f":"SUM(E16:E25)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(G$26-'2.16 Opex Summary'!H$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(H$26-'2.16 Opex Summary'!I$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(I$26-'2.16 Opex Summary'!J$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(J$26-'2.16 Opex Summary'!K$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(K$26-'2.16 Opex Summary'!L$23=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"N/A"]
[null,"Total",null,null,{"$f":"SUM(E33:E42)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E49:E58)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(G$26-'2.16 Opex Summary'!H$51=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(H$26-'2.16 Opex Summary'!I$51=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(I$26-'2.16 Opex Summary'!J$51=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(J$26-'2.16 Opex Summary'!K$51=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(K$26-'2.16 Opex Summary'!L$51=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E66:E75)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Category","Description",{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Debt Raising Costs",null,null,null,null,6236060.3100793064,6225455.9599410165,6214073.1512185736,6199208.9279164132,6173661.5612086207]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D90:D92)","v":0},0,0,0,0,0,0,0]

{"sheet":"3.1 Revenue","index":18,"n_rows":53,"n_cols":17,"rows_kept":53,"cut":false,"hidden":false,"merged":[[31,2,31,8],[31,10,31,16],[45,2,45,8],[45,10,45,16],[8,2,8,8],[8,10,8,16],[43,2,43,8],[43,10,43,16],[44,2,44,8],[44,10,44,16],[9,2,9,8],[9,10,9,16],[29,2,29,8],[29,10,29,16],[30,2,30,8],[30,10,30,16],[10,2,10,8],[10,10,10,16]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DREV0101","Revenue from Fixed Customer Charges ",286486703.46633071,283376325.67156279,418774978.85270512,417756354.50262219,416615912.22806013,415564894.1551578,414563251.06279504,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",572830632.07253528,607240887.61350942,505135996.35803211,507554308.42381567,510816877.16311598,513914158.78462636,516782511.95560902,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",28190740.560311113,29008357.131201569,53493866.985318989,53691947.555249527,53364630.055162199,53014329.057125345,52706586.718035512,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",154415.73412168631,186712.71067839881,170437.39082195211,172484.23704002335,174555.6646084596,176651.96872355821,178773.44813705145,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",18569374.144698039,19639163.291463219,14038746.361023618,14167474.43263074,13889878.029789314,13594270.039772257,13331287.902310027,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",78165735.798846424,71058307.657277852,56926027.996034063,56940484.712463029,57039335.906567901,57141761.487919524,57234684.286689907,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",5846499.1485130172,5405067.6337194042,4503903.7849268569,4505047.5791126471,4512868.5405066963,4520972.3021735922,4528324.2176298583,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",8084932.0342696868,7734013.9023294384,12389248.193284741,12404287.853561323,12401934.209254375,12395181.853855362,12392551.145599406,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",404195424.92589635,337971038.52003384,143588821.68837798,141827617.92229047,140190200.51865819,138669658.22646588,137260920.756109,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,75612252.871856794,68602150.991040647,66635351.49384886,65265415.835435085,63985493.914215527,62871226.149439625,61016084.535343021]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,78256460.026710764,79112416.863918543,80898927.943760991,79184937.174163803,77273298.379374713,75067719.468379006,72552251.130647987]
["DREV0112","Revenue from public lighting charges",10327223.84368719,9547481.6511152461,7955670.7998836488,7957691.1916236812,7971506.0946857501,7985820.5345897088,7998806.917494772,null,51059042.933655985,52983457.275109448,54124042.179261863,54335546.480884142,54350183.477830507,54307805.186704002,54202797.015137106]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,23205423.232607346,22701735.99634058,22012923.257176332,22013658.833308719,22017506.95397104,22021783.378870845,22026081.940408699]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":1412851681.7292097},{"$f":"SUM(D13:D25)","v":1371167355.7828913},1216977698.4104092,1216977698.4104095,1216977698.4104092,1216977698.4104095,1216977698.4104095,null,{"$f":"SUM(K13:K25)","v":228133179.06483087},{"$f":"SUM(L13:L25)","v":223399761.1264092},223671244.87404805,220799558.32379174,217626482.72539178,214268534.18339348,209797214.62153682]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DREV0201","Revenue from residential Customers ",735028798.19360924,726001643.29849052,652314280.2187072,652107670.79709506,653037225.87625051,653988491.97661209,654789701.50366008,null,0,0,0,0,0,0,0]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",168857592.41179949,157526087.95112881,127400910.27143136,127670876.21904911,128179888.46022324,128691156.30389483,129168765.24140343,null,0,0,0,0,0,0,0]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",335464245.16661644,317274983.86520118,286267574.98535442,286474931.43948096,286887427.21681404,287342889.45614725,287804120.43615037,null,0,0,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",157327323.10978401,155412091.33856985,138535358.32845148,138261481.1581215,136388782.16712323,134448367.76402119,132687980.09033075,null,0,0,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",16173723.006831985,14952549.329500973,12459574.594805703,12462738.765422948,12484374.620447835,12506792.881024292,12527131.147723828,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",0,0,0,0,0,0,0,null,228133179.0648309,223399761.1264092,223671244.87404805,220799558.32379174,217626482.72539178,214268534.18339348,209797214.62153682]
["DREV02","Total revenue by customer class",{"$f":"SUM(C34:C39)","v":1412851681.8886411},{"$f":"SUM(D34:D39)","v":1371167355.7828913},1216977698.3987501,1216977698.3791697,1216977698.3408589,1216977698.3816998,1216977698.4192686,null,{"$f":"SUM(K34:K39)","v":228133179.0648309},{"$f":"SUM(L34:L39)","v":223399761.1264092},223671244.87404805,220799558.32379174,217626482.72539178,214268534.18339348,209797214.62153682]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DREV0301","EBSS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",0,0,1107220.9751076852,1106086.293334502,1114335.8736133045,1123453.4925085099,1131612.6588006341,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C48:C52)","v":0},{"$f":"SUM(D48:D52)","v":0},1107220.9751076852,1106086.293334502,1114335.8736133045,1123453.4925085099,1131612.6588006341,null,{"$f":"SUM(K48:K52)","v":0},{"$f":"SUM(L48:L52)","v":0},0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":19,"n_rows":88,"n_cols":17,"rows_kept":88,"cut":false,"hidden":false,"merged":[[85,2,85,8],[72,2,72,8],[72,10,72,16],[70,2,70,8],[70,10,70,16],[83,2,83,8],[71,2,71,8],[71,10,71,16],[84,2,84,8],[12,2,12,8],[12,10,12,16],[14,10,14,16],[14,2,14,8],[13,2,13,8],[13,10,13,16]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(\"Forecasts for opex in table 3.2.1 are to be for the opex categories that \",dms_TradingName,\" has reported in its response to its annual reporting RIN.\")","v":"Forecasts for opex in table 3.2.1 are to be for the opex categories that Energex has reported in its response to its annual reporting RIN."}]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPEX0101","Inspection",29481792.166923281,29459415.60597444,27537253.565634064,27366077.767194662,27222992.568664722,27105001.042414285,26949194.20195511,null,0,0,0,0,0,0,0]
["DOPEX0102","Planned maintenance",76538337.845454156,76480245.55676204,71490077.835468039,71045684.529330432,70674217.855806589,70367897.424269572,69963403.812545508,null,0,0,0,0,0,0,0]
["DOPEX0103","Corrective repair",56401459.668841273,56358651.18919602,52681373.221106015,52353897.712246224,52080162.180552572,51854433.219728224,51556359.982574515,null,0,0,0,0,0,0,0]
["DOPEX0104","Vegetation",51351048.017053477,51312072.77941411,47964072.947137393,47665920.90145269,47416696.741040766,47211180.451671846,46939797.881015882,null,0,0,0,0,0,0,0]
["DOPEX0105","Emergency response/storms",17663748.899138659,17650342.185205232,16498696.198699668,16396137.768597325,16310409.567146538,16239716.012286866,16146365.754234143,null,0,0,0,0,0,0,0]
["DOPEX0106","Other network maintenance costs ",0,0,0,0,0,0,0,null,14311137.772590006,13381010.591622422,13684400.818257408,13245269.086284058,12714552.232376004,12138110.239574919,11487308.41767838]
["DOPEX0107","Network operating costs",44898316.216081001,44864238.575765885,41936945.73626969,41676259.239215575,41458352.388334051,41278661.112226568,41041380.259286664,null,0,0,0,0,0,0,0]
["DOPEX0108","Network billing and other energy market services (including meter reading)",3826680.1455960767,3823775.7108512409,3574282.7602618472,3552064.4695424135,3533492.2848786367,3518177.2108053006,3497953.7813897002,null,13104128.646720616,12252448.896941716,12530251.027223568,12128155.903825523,11642199.997376628,11114375.435062299,10518462.591990774]
["DOPEX0109","Customer services (inc call centre)",12680998.624122929,12671373.797484227,11844594.541634077,11770966.722395578,11709421.508474484,11658669.831861056,11591652.660099415,null,760996.11012452119,711536.50894640211,727669.31305937911,704318.44150924904,676097.52240279701,645445.16469338874,610838.71601019742]
["DOPEX0110","DSM initiatives",12688587.804473173,12678957.217677299,11851683.160347512,11778011.277166136,11716429.23036287,11665647.180461163,11598589.90102203,null,0,0,0,0,0,0,0]
["DOPEX0111","Levies",11168032.067883208,11159555.576738076,10431419.132907042,10366575.829101326,10312373.558202252,10267677.050559755,10208655.679647446,null,0,0,0,0,0,0,0]
["DOPEX0112","Debt raising costs",0,0,6236060.3100793064,6225455.9599410165,6214073.1512185736,6199208.9279164132,6173661.5612086207,null,50842.858140651202,47538.416169218755,48616.263821807668,47056.170368124229,45170.704506158967,43122.791968943864,40810.702934923283]
["DOPEX0113","Other operating costs (inc self insurance)",67511615.706523404,67460374.663405716,63058733.668910205,62666750.893335797,62339093.982868783,62068900.144863814,61712111.402918585,null,42311399.56299112,39561444.707990408,40458428.952474847,39160120.008241259,37591036.318506546,35886764.591837302,33962645.324721642]
["DOPEX0114"]
["DOPEX0115"]
["DOPEX0116"]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C17:C65)","v":384210617.16209066},{"$f":"SUM(D17:D65)","v":383919002.85847425},365105193.07845479,362863803.06951922,360987715.01755095,359435169.60906494,357379126.87789762,null,{"$f":"SUM(K17:K65)","v":70538504.950566918},{"$f":"SUM(L17:L65)","v":65953979.121670172},67449366.374837011,65284919.610228211,62669056.775168136,59827818.223136857,56620065.753335923]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPEX0201","Opex for network services",381626096.77566242,381336444.11256045,362649191.67570341,360422879.12145871,358559411.19918084,357017309.50328332,354975097.4267537,null,0,0,0,0,0,0,0]
["DOPEX0202","Opex for metering",396089.94258256181,395789.31191902416,376393.80200165167,374083.11093719857,372149.01652233634,370548.46829634963,368428.85522227426,null,15557164.542304747,14546054.047142208,14875859.528110156,14398493.946238579,13821569.207421837,13194938.182439573,12487473.046643887]
["DOPEX0203","Opex for connection services",2188430.4438456274,2186769.4339948101,2079607.600749725,2066840.8371232613,2056154.8018476395,2047311.6374851353,2035600.5959216075,null,30265076.245765753,28298050.947179142,28939658.098702375,28010985.930123042,26888630.30028598,25669575.523467317,24293265.19276065]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,16368483.102251662,15304642.386961175,15651647.487252673,15149386.908905419,14542375.084037634,13883064.750469012,13138704.742627358]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.2.4 - OPEX FOR HIGH VOLTAGE CUSTOMERS"]
[null,null,"End user costs (not standard control services)"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPEX0401","Opex for high voltage customers",2006078.4138579569,2025751.1964137456,1800604.8780487806,1770756.4544913743,1743856.7635408659,1718267.6666568762,1691100.5048404792]

{"sheet":"3.3 Assets (RAB)","index":20,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[115,2,115,8],[114,2,114,8],[8,2,8,8],[8,10,8,16],[8,18,8,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[114,10,114,16],[114,18,114,24],[115,18,115,24],[115,10,115,16],[21,2,21,8],[21,10,21,16],[21,18,21,24],[22,2,22,8],[98,2,98,8],[98,10,98,16],[98,18,98,24],[22,10,22,16],[22,18,22,24],[97,2,97,8],[97,10,97,16],[97,18,97,24]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",10242895137.045286,10497994842.675222,10780661812.197241,11032324467.916403,11281453672.21847,11524922525.801003,11749445146.787083,null,12574735421.153023,12859289668.621004,13328713506.289703,13611945938.748322,13893046979.136379,14166379942.647493,14416857628.766088,null,513045421.76138216,497342184.81931406,510470676.27704418,495100421.93727165,476546325.1648156,457104266.5357843,436194601.76457578]
["DRAB0102","Inflation addition",179269794.9700065,230801150.99531454,248628286.20908427,248205496.6159524,247751670.30828628,247159041.92086163,246140482.49618009,null,220057869.87017888,283313815.69389307,305197041.48598033,304678057.36328715,304120974.94696176,303393509.72850102,302143204.19114536,null,10260908.435227653,10957363.564997559,11686252.529525226,11046997.908481779,10347534.495076386,9643660.2876048535,8921740.989475552]
["DRAB0103","Straight line depreciation",-344357613.23309714,-355265946.80078262,-361747251.28463876,-351909069.90932441,-365668484.4268955,-380031177.84373093,-394332198.31372941,null,-420686281.30602604,-434012504.12639678,-441930423.6860258,-429911557.89491689,-446720818.68633407,-464267078.303882,-481737994.84299898,null,-45150526.787493743,-46294615.290360503,-45742880.320743427,-46899378.568274453,-48065166.820041947,-49307775.050616272,-49290552.685164571]
["DRAB0105","Actual additions (recognised in RAB)",439662454.12303901,424631015.57317382,373295910.51685631,361915035.01206261,368986528.54049295,364991106.30522645,351062852.18233198,null,504657589.13384241,637621776.34688854,428480104.38080186,415416798.33631003,423533668.08983809,418947604.09025651,402960341.40592384,null,20345399.827401016,49367229.88016735,18875089.057742026,17530633.854826801,18429899.866662841,18909823.337210089,18608947.522581153]
["DRAB0106","Disposals ",-19474930.230013382,-17499250.245686095,-8514289.7221401818,-9082257.4166223444,-7600860.8393509593,-7596349.3962778049,-7600740.2859064722,null,-19474930.230013382,-17499250.245686095,-8514289.7221401818,-9082257.4166223444,-7600860.8393509593,-7596349.3962778049,-7600740.2859064722,null,-1159018.4172030257,-901486.69707428745,-188715.60629628034,-232349.96749018395,-154326.17072858886,-155373.34540717475,-153701.70901405122]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":10497994842.675222},10780661812.197241,11032324467.916403,11281453672.21847,11524922525.801003,11749445146.787083,11944715542.865957,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":12859289668.621004},13328713506.289703,13611945938.748322,13893046979.136379,14166379942.647493,14416857628.766088,14632622439.234253,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":497342184.81931406},510470676.27704418,495100421.93727165,476546325.1648156,457104266.5357843,436194601.76457578,414281035.88245386]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",1731892148.7114263,1869549909.6522684,2008471994.5541549,2130062193.9817731,2248958984.4011321,2368125681.962111,2483283997.166059,null,2435290675.507935,2579985233.412497,2728054406.0804386,2857325038.082581,2984074904.886764,3110397082.0883117,3231480080.4046025,null,0,0,0,0,0,0,0]
["DRAB0202","Inflation addition",30387808.756849505,39122827.347907633,42144683.738434367,42073017.179644428,41996089.624455944,41895633.894565947,41722979.103445739,null,42687589.192419671,54958197.059766807,59203181.133132011,59102506.792150781,58994442.011970699,58853325.784608565,58610787.177945092,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-57742849.233477362,-59571989.1635447,-60658792.45543021,-59009098.642789446,-61316315.813246533,-63724692.479493223,-66122727.653250262,null,-82114060.084453329,-84715215.173165888,-86260719.629467085,-83914748.50662896,-87195760.300777763,-90620627.429840744,-94030788.288829923,null,0,0,0,0,0,0,0]
["DRAB0205","Actual additions (recognised in RAB)",165012801.41746986,159371246.71752346,140104308.14461431,135832871.88250419,138486923.74976972,136987373.78887522,131759862.97888909,null,184121028.79659539,177826190.78134048,156328170.49847731,151562108.5186609,154523495.49035507,152850299.96152288,147017451.47878647,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":1869549909.6522684},2008471994.5541549,2130062193.9817731,2248958984.4011321,2368125681.962111,2483283997.166059,2590644111.5951433,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":2579985233.412497},2728054406.0804386,2857325038.082581,2984074904.886764,3110397082.0883117,3231480080.4046025,3343077530.7725043,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",2021409361.7896574,2029172339.0541344,2044940885.7943163,2061077576.2279489,2077969781.7705233,2093208966.3169968,2106194944.2453108,null,2581231347.4299598,2598485373.8574214,2625713446.7591958,2652554226.4399137,2680170221.1692543,2705792758.0961471,2728471243.7935348,null,0,0,0,0,0,0,0]
["DRAB0302","Inflation addition",35333590.806122929,45490281.439854652,49003961.482798599,48920630.799660869,48831182.864191264,48714377.414924927,48513622.112396479,null,45128249.444669828,58100428.552261658,62588119.32552027,62481688.935366362,62367445.558112904,62218261.019244164,61961855.282857083,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-46987722.740174405,-48476168.859960906,-49360545.236085743,-48018121.775803752,-49895598.937840901,-51855393.727147825,-53806773.220218554,null,-60004945.227669433,-61905742.344099216,-63035121.529029213,-61320800.393442743,-63718403.590711899,-66221129.241837971,-68713108.268946514,null,0,0,0,0,0,0,0]
["DRAB0305","Actual additions (recognised in RAB)",19434482.55484597,18770045.035717163,16500869.684689827,15997798.693790771,16310381.258724838,16133770.854533261,15518097.605129294,null,32148095.566778764,31048997.569040716,27295377.381997675,26463208.362490427,26980275.598093439,26688130.533977877,25669697.323631734,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",-17373.356317641526,-15610.875429034677,-7595.4977700720019,-8102.1750734874904,-6780.6386016901961,-6776.6139963596015,-6780.5310573795532,null,-17373.356317641526,-15610.875429034677,-7595.4977700720019,-8102.1750734874904,-6780.6386016901961,-6776.6139963596015,-6780.5310573795532,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":2029172339.0541344},2044940885.7943163,2061077576.2279489,2077969781.7705233,2093208966.3169968,2106194944.2453108,2116413110.2115602,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":2598485373.8574214},2625713446.7591958,2652554226.4399137,2680170221.1692543,2705792758.0961471,2728471243.7935348,2747382907.6000195,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",1267529271.7113147,1312656449.0117891,1360267254.4854481,1400995976.5153506,1441205994.0790858,1480599073.4737053,1517307383.0019281,null,1817433770.4469337,1883151740.9220288,1952420549.4021711,2011754730.0951266,2070317852.7682965,2127735133.1784639,2181313174.8400526,null,0,0,0,0,0,0,0]
["DRAB0402","Inflation addition",22206360.352349944,28589610.032167368,30797878.238606002,30745506.794437833,30689290.795936272,30615881.220561981,30489711.066640928,null,31837375.356436152,40989073.916019887,44155079.630622774,44079994.416320011,43999397.244296648,43894149.550894223,43713258.739188619,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-47308087.43529585,-48806681.856799528,-49697087.956256062,-48345511.784212418,-50235789.681495659,-52208946.451838538,-54173630.550025389,null,-67448085.8030525,-69584661.822190866,-70854131.594729125,-68927162.432299078,-71622169.41143243,-74435338.456386626,-77236427.843304679,null,0,0,0,0,0,0,0]
["DRAB0405","Actual additions (recognised in RAB)",70228904.383420184,67827877.298291102,59627931.747552671,57810022.553509712,58939578.28017889,58301374.759499371,56076563.389204398,null,101328680.92171122,97864396.38631317,86033232.657061845,83410290.689148799,85040052.577303439,84119230.567081153,80909196.131390378,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":1312656449.0117891},1360267254.4854481,1400995976.5153506,1441205994.0790858,1480599073.4737053,1517307383.0019281,1549700026.907748,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":1883151740.9220288},1952420549.4021711,2011754730.0951266,2070317852.7682965,2127735133.1784639,2181313174.8400526,2228699201.8673272,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",471918598.01345706,485498012.43217403,500383986.43776929,513645786.7350415,526786583.74069506,539670671.33569062,551795424.4072032,null,617775659.43291867,630462760.10296798,645032619.51878071,658069590.23561156,671079769.76706207,683672174.40721142,695316845.22279501,null,0,0,0,0,0,0,0]
["DRAB0502","Inflation addition",8261891.4006113084,10636783.764818918,11458371.445804562,11438886.614551485,11417971.41425628,11390659.33204722,11343717.640876124,null,10810090.025215795,13917465.686844835,14992454.011480274,14966959.512731921,14939593.47908134,14903857.5860346,14842437.763031613,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-13459677.622031016,-13886044.420883352,-14139374.870307384,-13754836.400384935,-14292641.509253081,-14854026.580312379,-15413001.08180525,null,-17618282.872527491,-18176383.228314538,-18507984.596750852,-18004636.171274949,-18708605.672210112,-19443440.581342526,-20175120.132843208,null,0,0,0,0,0,0,0]
["DRAB0505","Actual additions (recognised in RAB)",18777200.640136711,18135234.661659691,15942803.721775033,15456746.791487042,15758757.689992389,15588120.319777761,14993269.384066045,null,19495293.517361071,18828776.957282484,16552501.302101323,16047856.189993553,16361416.833278067,16184253.810891552,15566654.105108548,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":485498012.43217403},500383986.43776929,513645786.7350415,526786583.74069506,539670671.33569062,551795424.4072032,562719410.35034013,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":630462760.10296798},645032619.51878071,658069590.23561156,671079769.76706207,683672174.40721142,695316845.22279501,705550816.95809186,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",697556949.75353789,696640596.86359727,698121989.99811614,699146005.75464094,700543904.72110879,701136678.77124703,700609361.18313873,null,950731093.72351825,945091246.96664107,942869001.95114708,940536332.16000938,938826817.19170392,935949554.96074319,931585897.60886705,null,0,0,0,0,0,0,0]
["DRAB0602","Inflation addition",12190645.682155302,15694864.019274684,16907139.009354867,16878388.610388681,16847527.662960678,16807227.94212098,16737964.198864123,null,16612200.83201292,21387401.448388927,23039369.369031336,23000191.181585055,22958136.948371578,22903220.492466126,22808834.744298227,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-23602219.043572471,-24349874.586447284,-24794102.221433576,-24119794.748947449,-25062862.951523233,-26047279.799163427,-27027469.592298731,null,-32161771.506427001,-33180570.912154984,-33785901.60868372,-32867050.596618347,-34152130.782944262,-35493555.064382888,-36829219.312797464,null,0,0,0,0,0,0,0]
["DRAB0605","Actual additions (recognised in RAB)",10495220.471476587,10136403.701691331,8910978.9686035011,8639305.1050267629,8808109.3387008198,8712734.2689341698,8380251.7100263266,null,9909723.9175369833,9570924.4482720885,8413862.448514659,8157344.4467277629,8316731.6036119452,8226677.2200406799,7912742.8558100844,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":696640596.86359727},698121989.99811614,699146005.75464094,700543904.72110879,701136678.77124703,700609361.18313873,698700107.49973047,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":945091246.96664107},942869001.95114708,940536332.16000938,938826817.19170392,935949554.96074319,931585897.60886705,925478255.89617789,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",3031433724.2553382,3077868331.2943954,3134698676.0275121,3187889643.3018441,3241141152.5795841,3292563306.2753558,3339738626.7837701,null,3102487742.6877446,3149298094.3915,3206762062.8498254,3260545702.2267008,3314414672.0945725,3366390369.484529,3414023393.4610085,null,0,0,0,0,0,0,0]
["DRAB0702","Inflation addition",53016551.479259558,68256234.159595579,73528361.747774467,73403327.59892121,73269114.772900805,73093853.160004854,72792628.359796047,null,54259841.784869812,69856910.021383494,75252674.189789385,75124707.867099807,74987347.61823082,74807975.948038042,74499687.129829958,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-80694835.095055625,-83251032.909710571,-84769825.514918894,-82464401.173454285,-85688705.335268587,-89054378.49669756,-92405599.565059379,null,-82655889.28261593,-85274208.079645485,-86829910.539059117,-84468459.537974879,-87771121.071373671,-91218587.168365464,-94651249.956036925,null,0,0,0,0,0,0,0]
["DRAB0705","Actual additions (recognised in RAB)",77771416.745050803,75112521.811502442,66031910.511751644,64018759.733224712,65269628.587392502,64562882.66260995,62099128.831086606,null,78864925.291699231,76168644.844858676,66960355.196420707,64918898.419698752,66187355.17235183,65470672.014310524,62972276.459846213,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",-3658526.0901974458,-3287378.3282710453,-1599479.4702752787,-1706176.8809520025,-1427884.3292526873,-1427036.8175033438,-1427861.6822949464,null,-3658526.0901974458,-3287378.3282710453,-1599479.4702752787,-1706176.8809520025,-1427884.3292526873,-1427036.8175033438,-1427861.6822949464,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":3077868331.2943954},3134698676.0275121,3187889643.3018441,3241141152.5795841,3292563306.2753558,3339738626.7837701,3380796922.7272987,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":3149298094.3915},3206762062.8498254,3260545702.2267008,3314414672.0945725,3366390369.484529,3414023393.4610085,3455416245.4123526,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",172039547.96674362,176283051.59092861,181349759.58347139,186571865.99980646,191754954.57745206,196950254.29784754,202124396.80244964,null,172039547.96674362,176283121.67164838,181349897.34895006,186572063.26740053,191755209.53308818,196950568.06869805,202124768.75165763,null,0,0,0,0,0,0,0]
["DRAB0802","Inflation addition",3010458.1519515119,3875818.6040759729,4175187.7450916925,4168087.8854783252,4160466.8296963847,4150514.8856987972,4133410.3281586245,null,3010458.1519515114,3875818.604075972,4175187.7450916916,4168087.8854783243,4160466.8296963843,4150514.8856987962,4133410.3281586235,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",1233045.4722334817,1190889.3884668194,1046918.6712433549,1015000.6921672712,1034832.8906991004,1023627.6189033022,984565.44627223606,null,1233115.5529532365,1190957.0732257126,1046978.1733587742,1015058.3802093271,1034891.7059134939,1023685.7972607993,984621.40451276698,null,0,0,0,0,0,0,0]
["DRAB0804","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",{"$f":"SUM(C68+C69+C70+C71)","v":176283051.59092861},{"$f":"SUM(D68+D69+D70+D71)","v":181349759.58347139},{"$f":"SUM(E68+E69+E70+E71)","v":186571865.99980646},191754954.57745206,196950254.29784754,202124396.80244964,207242372.57688048,null,{"$f":"SUM(K68+K69+K70+K71)","v":176283121.67164838},{"$f":"SUM(L68+L69+L70+L71)","v":181349897.34895006},{"$f":"SUM(M68+M69+M70+M71)","v":186572063.26740053},191755209.53308818,196950568.06869805,202124768.75165763,207242800.48432902,null,{"$f":"SUM(S68+S69+S70+S71)","v":0},{"$f":"SUM(T68+T69+T70+T71)","v":0},{"$f":"SUM(U68+U69+U70+U71)","v":0},0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",5061283.7674882328,12987073.51012376,20644121.998091519,27338679.292852424,33831406.108182833,40439785.969260998,46955221.669032134,null,53575859.452595092,58914176.580061913,64073582.814756542,68197635.498182043,72217820.585164011,76197988.727966011,79904506.291944087,null,367444561.88502312,347773914.62452102,333228230.76796162,314164320.30421561,293594869.58211905,271939890.5016098,249032201.50413632]
["DRAB0902","Inflation addition",93444.829938429015,120305.6784215056,129598.11733247107,129377.73719739837,129141.17909708628,128832.2700648154,128301.34341184815,null,940749.02104826958,1211168.6572296422,1304719.6093197861,1302500.948357326,1300119.4169078462,1297009.4977192373,1291664.4323008887,null,7339909.7550363019,7838103.2466956768,8359497.5515807541,7902221.1555805644,7401875.7559744986,6898375.1941722305,6381966.4831758086]
["DRAB0903","Straight line depreciation",-422453.4500198423,-435835.65204630548,-443786.83225727041,-431717.47904942022,-448597.35017707362,-466217.31602755206,-483761.62230738945,null,-4539279.8369203676,-4683072.1525695017,-4768507.9136211826,-4638822.2129635345,-4820197.128131045,-5009524.3917823313,-5198038.6902099578,null,-30413145.714348052,-31183797.417074919,-30812151.785881229,-31591162.624139972,-32376431.1579924,-33213445.205695011,-33201844.315355595]
["DRAB0905","Actual additions (recognised in RAB)",8254798.3627169402,7972578.4615925588,7008746.0096857073,6795066.557182434,6927836.0321581494,6852820.7457338702,6591313.4729363648,null,8936847.9433389138,8631309.7300344966,7587840.9877269017,7356506.3515881766,7500245.8540252009,7419032.4580411538,7135918.2461151658,null,3742648.2010778151,9081373.4638119228,3472176.4480637331,3224856.5187771344,3390281.4477557121,3478566.0098157604,3423218.2488515247]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-340059.50226811244,-281363.14999211224,-83432.677509251895,-105365.77231432551,-70705.126247010878,-71184.995766436434,-70419.229454494853]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":12987073.51012376},20644121.998091519,27338679.292852424,33831406.108182833,40439785.969260998,46955221.669032134,53191074.863072954,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":58914176.580061913},64073582.814756542,68197635.498182043,72217820.585164011,76197988.727966011,79904506.291944087,83134050.28015019,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":347773914.62452102},333228230.76796162,314164320.30421561,293594869.58211905,271939890.5016098,249032201.50413632,225565122.69135359]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",704375598.63694799,711702503.80346715,720563943.00477111,727841534.72196925,735030823.29849982,741677932.15051425,746326438.84117782,null,704491072.06551874,711976595.71635687,720991684.89290619,728404328.39926183,735724627.58359075,742505155.7249676,747285440.1562022,null,137923017.52582407,142159753.68622386,167847438.17930898,171932090.38982564,174506515.46409398,177270326.6224618,179847775.3162882]
["DRAB1002","Inflation addition",12327173.231146233,15870636.605252977,17096488.311235987,17067415.925920125,17036209.355329763,16995458.303013891,16925418.849483158,null,12329445.782346494,15873562.404508807,17099640.099914819,17070562.355017908,17039350.031403057,16998591.466508985,16928539.10099582,null,2767136.4363653362,2954954.7351100608,3151519.710281712,2979127.1034116172,2790497.5381682948,2600678.4808784579,2405993.0681219641]
["DRAB1003","Straight line depreciation",-38512976.586600147,-39732965.281918228,-40457834.772950538,-39357531.964469492,-40896385.728105724,-42502710.240840316,-44102137.247417688,null,-38517174.666287765,-39737296.345607996,-40462244.850524873,-39361822.104316868,-40900843.609615773,-42507343.218614176,-44106944.569597587,null,-12703980.296335943,-13025891.884789653,-12870650.502650199,-13196053.81452143,-13524071.050064661,-13873703.083187554,-13868857.235156048]
["DRAB1005","Actual additions (recognised in RAB)",38817765.520383649,37490640.923796117,32958268.29940382,31953451.643765248,32577793.283792347,32225037.750475649,30995313.225261748,null,38978309.533189878,37645696.163475558,33094578.377456926,32085605.96231319,32712529.778591495,32358315.305325545,31123504.8379592,null,14992538.935305303,36378745.189846873,13909065.931672174,12918335.980554016,13581005.714745758,13934661.64577622,13712946.053859431]
["DRAB1006","Disposals ",-5305056.9984105043,-4766873.0458270796,-2319330.1204911866,-2474047.0286852964,-2070508.0590019366,-2069279.1219857058,-2070475.2197112786,null,-5305056.9984105043,-4766873.0458270796,-2319330.1204911866,-2474047.0286852964,-2070508.0590019366,-2069279.1219857058,-2070475.2197112786,null,-818958.91493491316,-620123.54708217515,-105282.92878702846,-126984.1951758584,-83621.044481578007,-84188.34964073835,-83282.479559556348]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":711702503.80346715},720563943.00477111,727841534.72196925,735030823.29849982,741677932.15051425,746326438.84117782,748074558.44879365,null,{"$f":"SUM(K81+K82+K83+K84+K85)","v":711976595.71635687},720991684.89290619,728404328.39926183,735724627.58359075,742505155.7249676,747285440.1562022,749160064.30584824,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":142159753.68622386},167847438.17930898,171932090.38982564,174506515.46409398,177270326.6224618,179847775.3162882,182014574.72355399]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",139678652.43941537,125636575.46240765,111219200.31366608,97755205.3852541,84230086.942287058,70550175.248357058,55109352.687101386,null,139678652.43941528,125641324.99974817,261446254.6710875,247986292.34279743,234465083.55587852,220789157.90915146,205352278.23378956,null,7677842.3505349858,7408516.5086096106,9395007.3293888029,9004011.2429151237,8444940.1183883306,7894049.4115943359,7314624.9441312524]
["DRAB1102","Inflation addition",2441870.2795755332,3143789.3438857161,3386616.3725871318,3380857.4696879829,3374675.8093978893,3366603.4977944358,3352729.4930435102,null,2441870.2795755309,3143789.3438857128,3386616.372587129,3380857.4696879801,3374675.8093978865,3366603.497794433,3352729.4930435074,null,153862.24382601559,164305.58319182086,175235.26766276115,165649.64948959675,155161.20093359228,144606.61255416428,133781.43817777757]
["DRAB1103","Straight line depreciation",-35626792.026832402,-36755354.069432527,-37425901.424959168,-36408055.940174364,-37831587.119944341,-39317532.752168201,-40797097.781303257,null,-35626792.026832387,-36755354.069432504,-37425901.424959138,-36408055.940174334,-37831587.119944304,-39317532.752168164,-40797097.781303219,null,-2033400.7764361836,-2084925.9881129023,-2060078.0318335281,-2112162.1292250128,-2164664.6115872082,-2220626.761325751,-2219851.1342451107]
["DRAB1105","Actual additions (recognised in RAB)",29636818.555336948,28623577.572964173,25163174.75756371,24396011.359430883,24872687.429111097,24603363.535910487,23664486.139485527,null,29641568.092677541,178845882.39304507,25167207.357685603,24399921.015479039,24876673.476314001,24607306.421804249,23668278.562763199,null,1610212.6906847924,3907111.2257002746,1493846.6776970858,1387441.3552086237,1458612.7038596207,1496595.6813085035,1472783.2195655229]
["DRAB1106","Disposals ",-10493973.785087788,-9429387.9961589351,-4587884.6336036436,-4893931.3319115564,-4095687.8124946449,-4093256.8427923941,-4095622.852842866,null,-10493973.785087788,-9429387.9961589351,-4587884.6336036436,-4893931.3319115564,-4095687.8124946449,-4093256.8427923941,-4095622.852842866,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":125636575.46240765},111219200.31366608,97755205.3852541,84230086.942287058,70550175.248357058,55109352.687101386,37233847.685484305,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":125641324.99974817},261446254.67108753,247986292.34279743,234465083.55587852,220789157.90915146,205352278.23378956,187480565.65545017,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":7408516.5086096106},9395007.3293888029,9004011.2429151237,8444940.1183883306,7894049.4115943359,7314624.9441312524,6701338.467629442]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",1800721029.1818473,1939010952.1032116,2069267094.2679639,2189510589.1914525,2308542333.1816216,2425704839.564085,2536964054.3806009,null,2507637954.460216,2654019819.7464676,2792689722.0815096,2920699971.4846725,3047235993.4875379,3170938581.2464571,3287278805.5885534,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",2025290850.421896,2037056612.4242253,2053009231.0111327,2069523678.9992361,2085589374.0437601,2099701955.2811537,2111304027.2284355,null,2589858360.6436906,2612099410.3083086,2639133836.599555,2666362223.804584,2692981489.6327009,2717132000.9448409,2737927075.6967773,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",1290092860.3615518,1336461851.7486186,1380631615.5003994,1421100985.2972183,1460902533.7763956,1498953228.2378168,1533503704.954838,null,1850292755.6844811,1917786145.1620998,1982087639.7486489,2041036291.4317117,2099026492.9733801,2154524154.0092583,2205006188.3536901,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",478708305.22281551,492940999.43497169,507014886.5864054,520216185.23786831,533228627.53819287,545733047.87144685,557257417.37877166,null,624119209.76794338,637747689.81087434,651551104.87719607,664574680.00133681,677375972.08713675,689494509.81500316,700433831.09044337,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",697098773.30856752,697381293.4308567,698633997.87637854,699844955.23787487,700840291.74617791,700873019.97719288,699654734.3414346,null,947911170.34507966,943980124.45889401,941702667.05557823,939681574.67585659,937388186.07622361,933767726.28480506,928532076.75252247,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",3054651027.7748671,3106283503.6609535,3161294159.6646781,3214515397.9407139,3266852229.4274702,3316150966.529563,3360267774.7555342,null,3125892918.5396223,3178030078.6206627,3233653882.5382633,3287480187.1606369,3340402520.7895508,3390206881.4727688,3434719819.4366808,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",174161299.77883613,178816405.58719999,183960812.79163891,189163410.28862926,194352604.43764979,199537325.55014861,204683384.68966508,null,174161334.81919599,178816509.51029921,183960980.3081753,189163636.40024436,194352888.80089313,199537668.41017783,204683784.61799332,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",9024178.6388059966,16815597.754107639,23991400.645471971,30585042.700517628,37135596.038721919,43697503.819146566,50073148.266052544,null,56245018.016328499,61493879.697409227,66135609.156469293,70207728.041673034,74207904.656565011,78051247.509955049,81519278.286047131,null,357609238.25477207,340501072.69624132,323696275.53608859,303879594.94316733,282767380.0418644,260486046.00287306,237298662.09774494]
["DRAB1209","“Other” assets with long lives",708039051.22020757,716133223.40411913,724202738.86337018,731436179.01023459,738354377.72450709,744002185.49584603,747200498.64498568,null,708233833.89093781,716484140.30463147,724698006.64608407,732064477.99142623,739114891.65427923,744895297.9405849,748222752.23102522,null,140041385.60602397,155003595.93276644,169889764.2845673,173219302.92695981,175888421.04327789,178559050.96937501,180931175.01992109]
["DRAB1210","“Other” assets with short lives",132657613.95091151,118427887.88803686,104487202.8494601,90992646.163770586,77390131.095322058,62829763.967729226,46171600.186292842,null,132659988.71958172,193543789.83541784,254716273.50694245,241225687.94933796,227627120.73251498,213070718.0714705,196416421.94461986,null,7543179.4295722982,8401761.9189992063,9199509.2861519642,8724475.6806517281,8169494.7649913337,7604337.1778627941,7007981.7058803476]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",45,45,45,45,45,45,45,null,44,44,44,44,44,44,44,null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)",60,60,60,60,60,60,60,null,60,60,60,60,60,60,60,null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers",39,39,39,39,39,39,39,null,39,39,39,39,39,39,39,null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",51,51,51,51,51,51,51,null,51,51,51,51,51,51,51,null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",45,45,45,45,45,45,45,null,45,45,45,45,45,45,45,null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers",50,50,50,50,50,50,50,null,50,50,50,50,50,50,50,null,0,0,0,0,0,0,0]
["DRAB1407","Meters",15,15,15,15,15,15,15,null,15,15,15,15,15,15,15,null,15,15,15,15,15,15,15]
["DRAB1408","“Other” assets with long lives",34,34,34,34,34,34,34,null,34,34,34,34,34,34,34,null,22,22,22,22,22,22,22]
["DRAB1409","“Other” assets with short lives",8,8,8,8,8,8,8,null,8,8,8,8,8,8,8,null,8,8,8,8,8,8,8]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",33,33,33,33,33,33,33,null,32,32,32,32,32,32,32,null,0,0,0,0,0,0,0]
["DRAB1502","Underground network assets less than 33kV (cables)",45,45,45,45,45,45,45,null,45,45,45,45,45,45,45,null,0,0,0,0,0,0,0]
["DRAB1503","Distribution substations including transformers",28,28,28,28,28,28,28,null,28,28,28,28,28,28,28,null,0,0,0,0,0,0,0]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",37,37,37,37,37,37,37,null,37,37,37,37,37,37,37,null,0,0,0,0,0,0,0]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",31,31,31,31,31,31,31,null,31,31,31,31,31,31,31,null,0,0,0,0,0,0,0]
["DRAB1506","Zone substations and transformers",37,37,37,37,37,37,37,null,37,37,37,37,37,37,37,null,0,0,0,0,0,0,0]
["DRAB1507","Meters",15,15,15,15,15,15,15,null,11,11,11,11,11,11,11,null,13,13,13,13,13,13,13]
["DRAB1508","“Other” assets with long lives",26,26,26,26,26,26,26,null,26,26,26,26,26,26,26,null,14,14,14,14,14,14,14]
["DRAB1509","“Other” assets with short lives",5,5,5,5,5,5,5,null,5,5,5,5,5,5,5,null,5,5,5,5,5,5,5]

{"sheet":"3.4 Operational data","index":21,"n_rows":88,"n_cols":10,"rows_kept":88,"cut":false,"hidden":false,"merged":[[44,3,44,9],[45,3,45,9],[9,3,9,9],[10,3,10,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPED01","Total energy delivered","GWh",21156.267934157338,21163.377237783119,21222.554544767085,21307.914664665106,21287.745693753368,21435.137250907668,21554.72040534241]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",7622.2064966411453,7582.415472817288,7612.5286863861747,7681.1538519437127,7718.8517738747869,7860.8733017692803,7980.2978177475197]
["DOPED0202","Energy Delivery at On-peak times","GWh",6719.5090594922131,6749.208276700233,6773.3141865430989,6787.9914667129824,6759.1931313917448,6765.887071533386,6771.7625954517616]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",0,0,0,0,0,0,0]
["DOPED0204","Energy Delivery at Off-peak times","GWh",5283.8161889478233,5318.4666418698826,5348.4030720322271,5372.0516559272182,5364.4879453997592,5381.7511904258909,5400.0016789097326]
["DOPED0205","Controlled load energy deliveries","GWh",1347.4951031261567,1327.7518191736822,1301.4182879555865,1278.0027652811953,1254.6733053370801,1233.7722123987251,1208.4695495833951]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",183.24108594999996,185.53502722203518,186.89031184999996,188.71492479999995,190.53953774999991,192.85347478039125,194.18876364999988]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",9564.674450633016,9470.0588295669877,9388.206642877416,9320.1758135635719,9202.9006239259379,9167.3987365287976,9125.3858305526264]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",0,0,0,0,0,0,0]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",11167.389493544362,11168.759509985524,11184.313147083052,11215.768805253148,11186.958310226428,11256.93243803173,11319.216395433403]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",0.5,0.49999999999636202,0.5,0.50000000000363798,0.50000000000363798,0.5,0.49999999999636202]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",103.6715957780473,103.71701261321013,103.20009848415003,102.96338333659251,102.72100887794979,102.75307289835035,102.21993101877797]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",129.01145968612209,128.57059652701341,127.43543307725375,126.6525398714456,125.86837889164802,125.42497811471213,124.29685940363328]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",1143.9148278547641,1244.5966542980773,1374.0181038021826,1500.459681347736,1626.156731062815,1746.1159251701838,1852.4672209265107]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",0,0,0,0,0,0,0]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",7556.2595834118929,7477.7777669881789,7466.0915957331599,7488.0540223301223,7481.041368650117,7574.1629280475299,7642.2693003701852]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",1824.8944607048902,1840.7232922121202,1852.7256817368816,1875.0347094076724,1897.1629434262056,1931.2264209134505,1967.0246174828103]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",5825.4386627718695,5857.1693322110423,5868.3566707828777,5900.6699301127373,5918.7847387417614,5959.4716973154245,5989.5016145169338]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",5766.4341413186858,5802.1718191497439,5848.490284664168,5855.4410780145763,5800.2171051852856,5777.4227298508749,5761.736109322479]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",183.24108594999996,185.53502722203518,186.89031184999996,188.71492479999995,190.53953774999991,192.85347478039125,194.18876364999988]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5552.43110242486,5558.4207545518875,5592.6580273211002,5619.2157204896212,5607.4921499341726,5617.612894937396,5644.9672755151987]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5098.5350352823734,5112.7089636474848,5132.2717465907335,5164.1455306410789,5153.2123329788446,5151.4565973877907,5175.0568133294582]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5243.047957777977,5247.0303182899952,5278.1960394158959,5303.3649369329214,5291.2637961357832,5302.40719037503,5328.4943950176239]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",4808.4600970000029,4819.7317940592766,4836.9749719053507,4866.7591280341148,4855.8614229485393,4855.4099996313453,4878.0261802598834]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5626.9802274703979,5642.0647158622742,5704.7843976020813,5727.4607720375061,5694.5937943458557,5710.3152432441711,5740.9981751441956]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",5191.5201358795166,5214.3061289787292,5263.3470430374146,5290.3576383590698,5257.8932790756226,5262.3553895950317,5289.3983736038208]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",5382.1222891807556,5398.6128132343292,5461.052323102951,5486.0659568309784,5451.9768741130829,5468.757687330246,5500.566899061203]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",4951.5193204879761,4975.324001789093,5024.0371379852295,5053.3019313812256,5020.2584419250488,5026.1679821014404,5054.3972282409668]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5985.289474606514,5991.4915130138397,6027.1864753216505,6052.9555664807558,6042.8907629102468,6052.8932367563248,6081.7116649448872]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5500.3507266938686,5511.647275224328,5536.8564764857292,5570.812518492341,5558.8352086693048,5555.724275931716,5580.5726004242897]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5390.8123447260023,5395.2675687763694,5428.0633385998526,5454.8539282054662,5443.2017216486638,5456.3209321101067,5482.1010896426496]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",4946.5501283298599,4958.3921398317489,4976.4697333594668,5008.5604411925597,4997.4985849105788,4998.2513399082727,5021.4069706459713]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5858.1575393676758,5873.7426195144653,5938.2846689224243,5963.1589593887329,5929.7718839645386,5946.4498624801636,5978.4215974807739]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5405.4586133956909,5429.0880842208862,5479.3389329910278,5508.8078832626343,5475.8519124984741,5480.7834634780884,5508.9604921340942]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",5471.5660107258836,5489.9979338885514,5554.5252352008429,5581.4688474137429,5547.3575315589515,5564.61068742933,5597.0591621702815]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",5033.6439887983825,5058.9801864263336,5110.1189520399903,5140.2607317110605,5108.5705076221739,5115.6186764454678,5144.4532708447741]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.99168890677289201,0.99168890677289201,0.99168890677289201,0.99168890677289201,0.99168890677289201,0.99168890677289201,0.99168890677289201]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.96982731351432772,0.96078192417463026,0.94102623105255168,0.94089147411002505,0.94089146618596065,0.94089203709036251,0.94089214341441541]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.98194781099185324,0.97516312628618507,0.95599209912916838,0.95585967637642555,0.95585966241254761,0.95586035979958417,0.95586049837968901]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.92561283969159147,0.92561281473894652,0.92561277850763901,0.92561283936027328,0.92561278265467728,0.92561282553512259,0.92561281060104017]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0.97535850470071583,0.97908768758877529,0.96364913001695651,0.96364912735059116,0.96364912563560656,0.96364912394593405,0.9636491265940107]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0.93304659125077949,0.96987542354424783,0.97194922249015669,0.97194919428306414,0.97194873371208002,0.97194843801694253,0.97194853847033602]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0.96412864249511121,0.96476434181208082,0.96407276253023666,0.9640727767630719,0.96407277448347783,0.96407276739247216,0.96407276859985802]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW ",0,0,0,0,0,0,0]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW ",3.42,3.42,3.42,3.42,3.42,3.42,3.42]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA",200.881,200.881,200.881,200.881,200.881,200.881,200.881]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA",3379.67,3379.67,3379.67,3379.67,3379.67,3379.67,3379.67]

{"sheet":"3.5 Physical assets","index":22,"n_rows":97,"n_cols":10,"rows_kept":97,"cut":false,"hidden":false,"merged":[[10,3,10,9],[77,3,77,9],[93,3,93,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Circuit length"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",14182,14182,14182,14182,14182,14182,14182]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0104","Overhead 11 kV","km",17534.485000000001,17542.97,17560.47,17580.47,17600.47,17620.47,17640.47]
["DPA0105","Overhead SWER","km",40,40,40,40,40,40,40]
["DPA0106","Overhead 22 kV","km",0,0,0,0,0,0,0]
["DPA0107","Overhead 33 kV","km",2188,2188,2188,2204,2204,2204,2204]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",0,0,0,0,0,0,0]
["DPA0110","Overhead 132 kV","km",332,332,332,366,366,366,390]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0112","Overhead 110kV","km",822,822,822,822,822,822,822]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D15:D28)","v":35098.485000000001},{"$f":"SUM(E15:E28)","v":35106.97},35124.47,35194.47,35214.47,35234.47,35278.47]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",12101,12343.02,12589.8804,12841.678008000001,13098.511568160002,13360.481799523202,13627.691435513667]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",0,0,0,0,0,0,0]
["DPA0204","Underground 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0205","Underground 11 kV","km",6078.5950000000003,6242.7170649999998,6411.2704257549995,6584.3747272503842,6762.1528448861436,6944.730971698069,7132.238707933916]
["DPA0206","Underground SWER","km",0,0,0,0,0,0,0]
["DPA0207","Underground 22 kV","km",0,0,0,0,0,0,0]
["DPA0208","Underground 33 kV","km",846,846,846,846,846,846,846]
["DPA0209","Underground 66 kV","km",0,0,0,0,0,0,0]
["DPA0210","Underground 110 kV","km",152,152,152,152,152,152,152]
["DPA0211","Underground 132 kV","km",13,13,13,13,13,13,13]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D31:D42)","v":19190.595000000001},{"$f":"SUM(E31:E42)","v":19596.737065000001},20012.150825755001,20437.052735250385,20871.664413046146,21316.212771221271,21770.930143447582]
[]
[null,"Circuit Capacity MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001,0.13500000000000001]
["DPA0302","Overhead 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0303","Overhead 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0304","Overhead 11 kV","MVA",0.97,0.97,0.97,0.98,0.98,0.98,0.98]
["DPA0305","Overhead SWER","MVA",0.09,0.09,0.09,0.09,0.09,0.09,0.09]
["DPA0306","Overhead 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0307","Overhead 33 kV","MVA",26.369985329168841,26.367637032646236,26.346635179508798,26.667434913714224,26.965213189974229,27.823185090277871,28.371164830539371]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",0,0,0,0,0,0,0]
["DPA0310","Overhead 110 kV","MVA",150.45107916583504,150.45107916583504,150.45107916583504,150.45107916583504,150.45107916583504,150.45107916583504,150.45107916583504]
["DPA0311","Overhead 132 kV","MVA",163.93517489617091,163.93517489617091,178.02684882174034,178.02684882174034,178.02684882174034,178.02684882174034,176.69666797341318]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.14899999999999999,0.14899999999999999,0.14899999999999999,0.14899999999999999,0.14899999999999999,0.14899999999999999,0.14899999999999999]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0404","Underground 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0405","Underground 11 kV","MVA",2.97,2.97,3,3,3,3,3]
["DPA0406","Underground SWER","MVA",0.09,0.09,0.09,0.09,0.09,0.09,0.09]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0409","Underground 33 kV","MVA",34.509641224234379,34.902992312738327,35.458797127123759,35.876309170570991,35.766459175018205,35.959453118528707,36.039306947161535]
["DPA0410","Underground 66 kV","MVA",0,0,0,0,0,0,0]
["DPA0411","Underground 110 kV","MVA",169.15637487794442,169.15637487794442,169.15637487794442,169.15637487794442,169.15637487794442,169.15637487794442,169.15637487794442]
["DPA0412","Underground 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",15362.45,15823.3235,16298.023205000001,16786.96390115,17290.572818184501,17809.290002730035,18343.568702811936]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",2392.788461538461,2425.076923076922,2457.3653846153829,2489.6538461538439,2521.9423076923049,2554.2307692307659,2586.5192307692269]
["DPA0503","Cold spare capacity included in DPA0501","MVA",123,123,123,123,123,123,123]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",8244.3000030517578,8244.3000030517578,8244.3000030517578,8314.6999969482422,8314.6999969482422,8314.6999969482422,8314.6999969482422]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",8430.7000193595886,8523.20001745224,8515.0000166893005,8532.9000182151794,8532.9000182151794,8532.9000182151794,8532.9000182151794]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",3929.5000095367432,3929.5000095367432,3929.5000095367432,3940.5000095367432,3940.5000095367432,3940.5000095367432,3940.5000095367432]
["DPA0604","Total zone substation transformer  capacity ","MVA",21238.50003194809,21331.000030040741,21322.800029277802,21422.100024700165,21422.100024700165,21422.100024700165,21422.100024700165]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",634,634,634,634,634,634,634]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DPA0701","Public lighting luminaires","0's",331534,333784,339149,344644,350279,356054,361969]
["DPA0702","Public lighting poles","0's",177140,183138.66666666666,188713.55555555553,194494.07407407404,200278.76543209873,205992.13168724277,211751.65706447186]

{"sheet":"3.6 Quality of service","index":23,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[[7,3,7,9],[14,3,14,9],[19,3,19,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DQS0201","Energy Not Supplied (planned)","GWh",2.0699999999999998,2.11,2.14,2.1800000000000002,2.21,2.25,2.2799999999999998]
["DQS0202","Energy Not Supplied (unplanned)","GWh",4.7300000000000004,4.8,4.88,4.96,5.04,5.12,5.2]
["DQS02","Total",null,{"$f":"SUM(D10:D11)","v":6.8000000000000007},{"$f":"SUM(E10:E11)","v":6.91},7.02,7.1400000000000006,7.25,7.37,7.48]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DQS03","System losses","%",4.309950330880008E-2,4.3082683872630145E-2,4.306668523066759E-2,4.3051430986561168E-2,4.3036854937349989E-2,4.3036854937349878E-2,4.3036854937349656E-2]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DQS04","Overall utilisation","%",0.26694900231334701,0.26630174746216484,0.26762579118413027,0.26798084057095983,0.26740467873756452,0.26725502904692938,0.26845034388874028]

{"sheet":"3.7 Operating Environment","index":24,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[8,3,8,9],[15,3,15,9],[33,3,33,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOEF0101","Customer density","Customer / km",0.32829999999999998]
["DOEF0102","Energy density","MWh/customer",14.38]
["DOEF0103","Demand density","kVA / customer",3.73]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOEF0201","Rural proportion","%",0.34510000000000002]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",107221]
["DOEF0203","Rural vegetation maintenance spans","0's",88260]
["DOEF0204","Total vegetation maintenance spans","0's",195481]
["DOEF0205","Total number of spans","0's",417076]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",1.3]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1.6]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",3.12]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",4.43]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",1]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",1]
["DOEF0212","Tropical proportion","Spans",134883]
["DOEF0213","Standard vehicle access","km","        5,186.25",5187.51,5190.09,5201.03,5203.9799999999996,5206.9399999999996,5213.4399999999996]
["DOEF0214","Bushfire risk","Spans",23354]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOEF0301","Route Line length","km",44938,45350,45778,46258,46707,47170,47657]

{"sheet":"4.1 Public lighting","index":25,"n_rows":153,"n_cols":10,"rows_kept":153,"cut":false,"hidden":false,"merged":[[182,1,182,2],[183,1,183,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[156,1,156,2],[151,1,151,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[90,1,90,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[91,1,91,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[210,1,210,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[5,1,5,2],[8,3,8,9],[31,3,31,9],[184,1,184,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[57,1,57,2],[58,1,58,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's",1143,1224,7921.3348969296567,9398.0497631373582,11115.133193488209,12618.726829648869,14544.47657782691]
[null,"Number of poles installed ","0's",412.66666666666669,438.5555555555556,400.40740740740745,417.20987654320993,418.72427983539097,412.11385459533608,416.01600365797896]
[null,"Total expenditure","$0's",13997998.710501075,19317264.658424847,20315868.838521097,21741775.984702699,23007468.84076719,24326831.886644997,25431829.621408779]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's",6158.333333333333,6020.1111111111104,6003.4814814814808,6060.6419753086411,6028.0781893004105,6030.7338820301775,6039.8180155464097]
[null,"Number of poles replaced","0's",294,283.66666666666669,272.22222222222223,283.2962962962963,279.72839506172841,278.41563786008231,280.48010973936903]
[null,"Total expenditure","$0's",6717841.2877098331,10020013.803938214,10413547.76555318,10933456.778367916,11762110.718059419,12378355.31347198,12909518.519635219]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's",75132.333333333328,75285.777777777766,74822.703703703693,75080.271604938258,75062.917695473239,74988.63100137173,75043.940100594409]
[null,"Number of poles maintained","0's",6694,8834.3333333333339,8198.7777777777792,7909.0370370370374,8314.0493827160499,8140.6213991769555,8121.2359396433467]
[null,"Total expenditure","$0's",12930101.867667841,12930101.867667841,12852533.02781431,12782409.362263201,12455576.487268427,12124696.850852223,11697988.516932832]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days",4,4,4,4,4,4,4]
[null,"GSO breaches","0's",0,0,0,0,0,0,0]
[null,"GSL payments ","$0's",0,0,0,0,0,0,0]
[null,"Customer complaints ","0's",6,6,6,6,6,6,6]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"LIGHT INSTALLATION"]
[null,"steel overhead major",null,7017.4833666196446,7026.4986029382744,7020.6055263836706,7021.5291653138629,7022.8777648786008,7021.6708188587118,7022.0259163503924]
[null,"steel underground decorative minor",null,4842.2356320245462,4842.3527130156972,4824.244186384336,4836.2775104748589,4834.2914699582961,4831.604388939164,4834.0577897907724]
[null,"steel underground major",null,11550.625182005455,11587.037370253425,11586.764181274071,11574.808911177648,11582.870154235046,11581.481082228922,11579.720049213871]
[null,"wood pole major",null,1713.7144674777137,1714.1827914423177,1705.3236631118889,1711.0736406773065,1710.1933650771707,1708.8635562887889,1710.0435206810889]
[null,"wood pole minor",null,943.08738372159485,943.43862669504801,940.39452092512079,942.30684378058777,942.04666380025196,941.58267616865351,941.97872791649775]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"High Pressure Sodium - Major",null,352.29670237346727,353.4675122849776,353.97486324663197,353.24635930169222,353.5629116111005,353.59471138647496,353.46799409975591]
[null,"Mercury Vapour Minor",null,236.03527816048853,236.03527816048853,236.0352781604885,236.0352781604885,236.03527816048845,236.0352781604885,236.0352781604885]
[null,"High Pressure Sodium Vapour Minor",null,244.81635249681625,245.98716240832661,247.19699931688729,246.00017140734334,246.39477771085234,246.53064947836103,246.30853286551891]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"Major Road Luminaires",null,29.247218062257225,29.791552111330095,30.153655526234111,29.730808566607141,29.892005401390442,29.92548983141057,29.849434599802716]
[null,"Minor Road Luminaires",null,21.926376966663682,22.565803165587752,23.53452759291849,22.675569241723306,22.925300000076511,23.045132278239436,22.882000506679748]

{"sheet":"4.2 Metering","index":26,"n_rows":92,"n_cols":11,"rows_kept":92,"cut":false,"hidden":false,"merged":[[81,1,83,1],[84,1,86,1],[87,1,89,1],[18,1,21,1],[28,1,30,1],[31,1,33,1],[34,1,36,1],[37,1,39,1],[40,1,42,1],[43,1,45,1],[46,1,48,1],[49,1,51,1],[54,1,56,1],[66,1,68,1],[69,1,71,1],[72,1,74,1],[75,1,77,1],[78,1,80,1],[5,1,5,2],[8,4,8,10],[26,4,26,10],[64,4,64,10],[10,1,13,1],[14,1,17,1],[65,2,65,3],[27,2,27,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.2 METERING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.2.1 - METERING DESCRIPTOR METRIC"]
[null,null,null,null,"VOLUMES (0's)"]
[null,"ASSET CATEGORY","ASSET SUBCATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Meter Type 4","Single phase meter population "]
[null,null,"Multi phase meter population "]
[null,null,"Current transformer connected meter population "]
[null,null,"Direct connect meter population "]
[null,"Meter Type 5","Single phase meter population "]
[null,null,"Multi phase meter population "]
[null,null,"Current transformer connected meter population "]
[null,null,"Direct connect meter population "]
[null,"Meter Type 6","Single phase meter population ",null,1889115.2549999999,1832441.7973499999,1777468.5434295,1724144.4871266149,1672420.1525128165,1622247.5479374321,1573580.1214993091]
[null,null,"Multi phase meter population ",null,141085.04500000001,136852.49365000002,132746.91884050003,128764.51127528503,124901.57593702647,121154.52865891567,117519.89279914821]
[null,null,"Current transformer connected meter population ",null,9174.26,8899.0321999999996,8632.0612339999989,8373.0993969799983,8121.9064150705981,7878.2492226184804,7641.9017459399256]
[null,null,"Direct connect meter population ",null,2021026.04,1960395.2588,1901583.4010359999,1844535.8990049199,1789199.8220347723,1735523.8273737291,1683458.1125525173]
[]
[]
[null,"4.2.2 - COST METRICS"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"}]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Meter purchase ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter testing ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6",590083.61386567703,577996.83737297705,562689.9786535888,553463.45265606069,550857.24237400759,540384.56219426496,523703.36007802247]
[null,"Meter investigation ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Scheduled meter reading ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Special meter reading ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"New meter installation ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter replacement ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter maintenance ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6",1816274.3849297459,1779052.3359917183,1688524.7611683877,1660600.7500813683,1651309.3285430865,1619686.9671234945,1569458.299760669]
[null,"Remote meter reading ",null,"Meter Type 4"]
[null,"Remote meter re-configuration ",null,"Meter Type 4"]
[null,"Other metering ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6",4589033.6011020439,4495891.8990239967,3888807.1535594231,3822477.1509659649,3803268.3183849873,3728480.4247581828,3610881.8975581909]
[null,null,null,"Meter Type 7"]
[null,"IT infrastructure capex ",null,"Meter Type 4"]
[null,"IT infrastructure opex ",null,"Meter Type 4"]
[null,"Communications infrastructure capex ",null,"Meter Type 4"]
[null,"Communications infrastructure opex ",null,"Meter Type 4"]
[]
[null,"VOLUMES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Meter purchase ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter testing ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6",3000,3000,3000,3000,3000,3000,3000]
[null,"Meter investigation ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Scheduled meter reading ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Special meter reading ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"New meter installation ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter replacement ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter maintenance ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6",1827,1773,1719,1668,1618,1569,1522]
[null,"Remote meter reading ",null,"Meter Type 4"]
[null,"Remote meter re-configuration ",null,"Meter Type 4"]

{"sheet":"4.3 Fee-based services","index":27,"n_rows":219,"n_cols":16,"rows_kept":219,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,9,8,15],[8,1,9,1],[5,1,5,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.3 ANCILLARY SERVICES - FEE BASED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.3.1 - COST METRICS FOR FEE-BASED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"COMMON FEE-BASED SERVICES"]
[null,"Energisation"]
[null,"De-energisation"]
[null,"Re-energisation"]
[null,"MISCELLANEOUS FEE-BASED SERVICES"]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). No CT - BH",5480135.6776403412,5034635.9230576744,5050416.5503425691,4730441.5555949202,4369988.3223581715,3952642.5775839128,3474965.4972122889,68271,65513,62065,57927,53100,47583,41377]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). No CT - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). CT - BH",12136.878258988916,11189.273611043152,11164.387131631422,10518.08349730239,9678.1613929087816,8722.1845922947887,7642.4517422521612,108,104,98,92,84,75,65]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). CT - A/T",314.75815942536269,301.34768731700007,319.08906738644237,320.21317099804855,322.7117989426481,162.8662003824557,164.65704270175371,2,2,2,2,2,1,1]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). Non payment - No CT",1025373.1898979016,942020.16920382541,944984.89332188922,885135.70195543626,817623.99550584389,739557.76440146612,650196.54774023965,12774,12258,11613,10839,9935,8903,7742]
[null,"Retailer requested de-energisation of the customer's premises where the de-energisation can be performed at the premises ie by a method other than main switch seal (eg pole, pillar, transformer or meter isolation link). Non payment - CT",3034.2148261262573,2797.3272388998721,2734.1289397440723,2629.5208743255976,2419.5359867854327,2209.6232894988361,1881.218890400532,27,26,24,23,21,19,16]
[null,"Retailer requested de-energisation (MSS). No CT - BH",2661515.2924961224,2445102.5648814752,2452810.6941885725,2297408.5491166576,2122332.9697289756,1919652.0439710636,1687655.626109787,36841,35352,33492,31259,28654,25677,22328]
[null,"Retailer requested de-energisation (MSS). No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation (MSS). No CT - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation (MSS). CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation (MSS). CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation (MSS). CT - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation (MSS). Non payment - No CT",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requested de-energisation (MSS). Non payment - CT",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests a re-energisation of the customer's premises where the customer has not paid their electricity account. No visual required. No CT - BH",551433.076070474,506629.78947240778,508182.65710775333,475959.48842124693,439739.33021110983,397731.38821235113,349654.91582533828,7633,7325,6939,6476,5937,5320,4626]
[null,"Retailer requests a re-energisation of the customer's premises where the customer has not paid their electricity account. No visual required. CT - BH",1765.9513547719009,1606.1450012787679,1611.1850748022662,1527.0869220154489,1357.9087243215463,1279.2573890994145,1108.5754175574564,20,19,18,17,15,14,12]
[null,"Retailer requests a re-energisation of the customer's premises where the customer has not paid their electricity account. No visual required. No CT - AH",1011.7334864294583,968.61756637607164,923.05829210649199,823.42311022389822,829.82535563336592,732.89790172105063,635.11293467700818,10,10,9,8,8,7,6]
[null,"Retailer requests a re-energisation of the customer's premises where the customer has not paid their electricity account. No visual required. CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests a re-energisation of the customer's premises where the customer has not paid their electricity account. No visual required. No CT - A/T",31161.323145885326,28574.112174425107,28717.633943976027,26864.025330723136,24790.975800803881,22510.445326689893,19794.437113752934,308,295,280,261,239,215,187]
[null,"Retailer requests a re-energisation of the customer's premises where the customer has not paid their electricity account. No visual required. CT - A/T",123.65905287793966,118.38659144596429,125.35381986913784,125.7980314635191,126.77838917267943,127.97363067228875,129.367391909508,1,1,1,1,1,1,1]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). No CT - BH",1423192.9493874342,1307485.2497988092,1311578.4911853182,1228484.0786110044,1134863.7377089446,1026475.9271838004,902405.97110935953,19700,18904,17909,16715,15322,13730,11939]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). No CT - AH",6576.2581845495351,6102.2729958910822,6051.210460000204,5661.0004827172252,5290.1322807209444,4816.183767852498,4234.1030277772898,65,63,59,55,51,46,40]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). No CT - A/T",36523.489774029178,33610.905847302507,33743.21397039749,31598.694854481721,29147.550194995529,26384.341566158662,23181.72289529421,361,347,329,307,281,252,219]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). CT - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). Non payment - No CT",1372.6268596354623,1244.9589800856616,1245.0041674069212,1175.9319242470615,1111.016228990356,971.89490003485594,831.43156316809223,19,18,17,16,15,13,11]
[null,"Retailer requests a re-energisation for the customer's premises following a main switch seal (no visual required). Non payment - CT",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises. No CT - BH",6911660.6769637335,6349759.9974222286,6369652.232941268,5966103.7461224645,5511518.1399952918,4985199.116582538,4382603.6083605746,71754,68855,65231,60882,55809,50011,43487]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises. CT - BH",26127.997858694776,23977.022454640257,24045.734015797629,22538.742717060075,20862.380963951469,18814.980110366443,16502.656784093953,217,208,197,184,169,151,131]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises. No CT - AH",209630.67798980913,192689.56129645195,193228.59172394749,181014.85248429628,167209.46024478215,151186.47711060496,132950.87874335973,1554,1492,1413,1319,1209,1083,942]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises. CT - AH ",168.61908865759523,161.43626106267857,170.93537289166511,171.54277017752599,172.88755149322321,174.49705695251134,176.41466076675704,1,1,1,1,1,1,1]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises. No CT - A/T",317953.35468314018,292133.90932094224,293056.52354572504,274472.86781361315,253511.12277298167,229362.32171098707,201684.50303720136,2357,2262,2143,2000,1833,1643,1429]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises. CT - A/T",337.23817731519046,322.87252212535714,341.87074578333022,343.08554035505199,345.75765721939365,174.49705695251134,176.41466076675704,2,2,2,2,2,1,1]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises where the customer has not paid their electricity account. NMI de-energised > 30 days. No CT - BH",3949.2993992165657,3596.5560190377637,3612.9703959844001,3331.8130564905991,3160.2134727790035,2791.0977011982654,2519.4895853578555,41,39,37,34,32,28,25]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises where the customer has not paid their electricity account. NMI de-energised > 30 days. No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises where the customer has not paid their electricity account. NMI de-energised > 30 days. No CT - A/T",134.89906182285355,129.14900885014288,136.74465906758178,137.23421614202084,138.31004119457856,139.60448724234439,141.14180657174705,1,1,1,1,1,1,1]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises where the customer has not paid their electricity account. NMI de-energised > 30 days. CT - BH",240.81671778268293,230.55254097686975,244.1206049302298,244.98730199911896,246.89249533119022,124.60410310714025,125.97447926789276,2,2,2,2,2,1,1]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises where the customer has not paid their electricity account. NMI de-energised > 30 days. CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer or metering coordinator/provider requests a visual examination upon re-energisation (physical) of the customer’s premises where the customer has not paid their electricity account. NMI de-energised > 30 days. CT - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. No dismantling - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. No dismantling - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. No dismantling - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Single Phase. Dismantling - Single ph - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Multi-Phase. Dismantling - Multiph - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Single Phase. Dismantling - Single ph - BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Multi-Phase. Dismantling - Multiph - BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Single Phase. Dismantling - Single ph - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Multi-Phase. Dismantling - Multiph - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Single Phase. Dismantling - Single ph - AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Multi-Phase. Dismantling - Single ph - AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Single Phase. Dismantling - Single ph - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Multi-Phase. Dismantling - Multiph - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Single Phase. Dismantling - Single ph - A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary de-energisation and re-energisation of supply to allow customer or contractor to work close - the service will be physically dismantled or disconnected (e.g. overhead service dropped). This services includes switching if required. Multi-Phase. Dismantling - Multiph - A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested temporary connection (short term) and the recovery of the temporary builders supply. Excludes work on metering equipment. No CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested temporary connection (short term) and the recovery of the temporary builders supply. Excludes work on metering equipment. No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested temporary connection (short term) and the recovery of the temporary builders supply. Excludes work on metering equipment. No CT - A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested temporary connection (short term) and the recovery of the temporary builders supply. Excludes work on metering equipment. CT - BH",86691.952363022196,82997.377263472503,87882.853691791446,88195.090265619132,88881.12386155795,89713.842464086512,90701.658666077259,60,60,60,60,60,60,60]
[null,"Customer requested temporary connection (short term) and the recovery of the temporary builders supply. Excludes work on metering equipment. CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested temporary connection (short term) and the recovery of the temporary builders supply. Excludes work on metering equipment. CT - A/T",24281.54681085534,23246.733231634877,24615.11220966106,24702.550799742763,24894.708331699818,25127.952493580073,25404.618166663742,12,12,12,12,12,12,12]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  CT (complex). BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  CT (complex). BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  No CT (simple). BH",842838.45839543792,782711.31465926254,803932.89576916536,782584.42348348163,764994.8441104251,749010.94832918898,734532.31285057659,3500,3395,3293.2,3194.4,3098.5,3005.6,2915.4]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  No CT (simple). BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  CT (complex). AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  CT (complex). AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  No CT (simple)",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  No CT (simple). AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  CT (complex). A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  CT (complex). A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  No CT (simple). A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Service only.  No CT (simple). A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Meter only. CT. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Meter only. No CT. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex Energy to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Meter only. CT. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Meter only. No CT. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Meter only. CT. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Overhead. Meter only. No CT. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Service only.  CT (complex). BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Service only.  CT (complex). BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Service only.  CT (complex). AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Service only.  CT (complex). AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Service only.  CT (complex). A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  CT (complex). A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  No CT (simple). BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  No CT (simple). BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  No CT (simple)",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  No CT (simple). AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  No CT (simple). A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Service only.  No CT (simple). A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Meter only. No CT. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed. Underground. Meter only. No CT. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Meter only. CT. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Meter only. No CT. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Meter only. CT. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Meter only. CT. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Retailer requests Energex to abolish supply at a connection point and decommission a NMI.  May be used where a property is to be demolished; supply is no longer required; an alternative connection point is to be used; or a redundant supply is to be removed.  Underground. Meter only. No CT. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Single to Multi-ph. BH",340988.35986117541,326456.31875955779,345672.59303375526,346900.68362786947,349599.05811251618,352874.45842820744,356759.87645604741,708,708,708,708,708,708,708]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Single to Multi-ph. BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Multi-ph increase capacity. BH",134372.52521496022,128645.93210754066,136218.44232831692,136702.38011435518,137765.73326253128,139056.46864748473,140587.58604935725,279,279,279,279,279,279,279]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Multi-ph increase capacity. BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Single to Multi-ph. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Single to Multi-ph. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Multi-ph increase capacity. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Multi-ph increase capacity. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Single to Multi-ph. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Single to Multi-ph. A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Multi-ph increase capacity. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Overhead. Multi-ph increase capacity. A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Single to Multi-ph. BH",33713.544401252366,32276.754879304062,34176.666335487156,34298.097586274242,34564.879563298411,34888.721264978318,35272.870991607211,70,70,70,70,70,70,70]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Single to Multi-ph. BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Multi-ph increase capacity. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Multi-ph increase capacity. BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Single to Multi-ph. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Single to Multi-ph. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Multi-ph increase capacity. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Multi-ph increase capacity. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Single to Multi-ph. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Single to Multi-ph. A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Multi-ph increase capacity. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Service upgrade. For example, an upgrade from single phase to multi phase and/or increase capacity. Applies to underground and overhead service upgrades.  Excludes work on metering equipment (if required). Underground. Multi-ph increase capacity. A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Single ph. BH",389632.18062976032,373027.06609525532,394984.64589377295,396387.92268460197,399471.25494058128,403213.90033226198,407653.58287687332,809,809,809,809,809,809,809]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Single ph. BH with traffic control",44790.848056481365,42881.977369180218,45406.141377362721,45567.460038118392,45921.916902766112,46352.161917228514,46862.523084253342,93,93,93,93,93,93,93]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Single ph. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Single ph. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Single ph. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Single ph. A/T with traffic control",1348.9716637446488,1291.4900885014285,1367.5011793620722,1372.3599747919816,1383.0480746446274,1395.993559820929,1411.3676759257633,2,2,2,2,2,2,2]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Multi ph. BH",213743.83890222767,204634.62522789661,216680.0733011784,217449.89558861899,219141.33922263468,221194.46716366126,223629.99637594662,317,317,317,317,317,317,317]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Multi ph. BH with traffic control",45176.135850449762,43250.850831376316,45796.741623742593,45959.443283991335,46316.941406142607,46750.877942970532,47265.641417910592,67,67,67,67,67,67,67]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Multi ph. AH",1888.5679110360629,1808.0861239020001,1914.5162080899026,1921.3146527318381,1936.2533478888358,1954.3944045894684,1975.9181056155162,2,2,2,2,2,2,2]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Multi ph. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Multi ph. A/T",11331.38851173249,10848.481398855667,11487.042659853159,11527.852289647482,11617.537533100069,11726.383531737647,11855.491837095859,12,12,12,12,12,12,12]
[null,"Customer requests their existing overhead service to be replaced or relocated, e.g.as a result of point of attachment relocation. No material change to load. This includes De-energisation, followed by physical dismantling then reattachment of service and re-energisation. Excludes work on metering equipment (if required). Multi ph. A/T with traffic control",1888.5679110360629,1808.0861239020001,1914.5162080899026,1921.3146527318381,1936.2533478888358,1954.3944045894684,1975.9181056155162,2,2,2,2,2,2,2]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Single ph. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Single ph. BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Single ph. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Single ph.  AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Single ph. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Single ph. A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Multi ph. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Multi ph. BH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Multi ph. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Multi ph. AH with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Multi ph. A/T",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Rearrange connection assets at customer's request - simple (upgrade from overhead to underground where main connection point is in existence).\nRecovery of the overhead service and connection of the consumer mains to the pre-existing pillar for a customer requested conversion of existing overhead service to underground service. Multi ph. A/T with traffic control",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Attending loss of Supply - customer fault. BH",85536.070026633068,81890.73920460607,86711.089345109343,87019.158341372065,87696.032905661414,88517.660178458798,89492.303665105486,444,444,444,444,444,444,444]
[null,"Attending loss of Supply - customer fault. AH",90651.108093859919,86787.798174010823,91896.395867511528,92222.889570666957,92940.247927499382,93810.999837097828,94843.934696766868,336,336,336,336,336,336,336]
[null,"Attending loss of Supply - customer fault. A/T",22662.77702346498,21696.945125433162,22974.103515935072,23055.722392666739,23235.057620433086,23452.749959274457,23710.983674191717,84,84,84,84,84,84,84]
[null,"After Hours Removal of Meter - No CT (after hours - incremental costs only - base cost included in MSC). No CT - AH",248355.27615968499,230637.8980804201,236925.97984794236,230586.81193718297,225411.71426251825,220760.12308757304,216489.66211145907,1900,1843,1788,1734,1682,1632,1583]
[null,"After Hours Removal of Meter - No CT (after hours - incremental costs only - base cost included in MSC). CT - AH ",4590.2642263349608,4394.6361010947494,4265.5417476997281,4280.6957441143222,4313.9892768157661,3958.5620336184393,4002.1420199520103,12,12,11,11,11,10,10]
[null,"Customer requested Meter Accuracy Testing of type 5-6 meter (physically test meter). No CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested Meter Accuracy Testing of type 5-6 meter (physically test meter). CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Customer requested Meter Accuracy Testing of type 5-6 meter (physically test meter). No CT - AH",6417.192155770922,6143.6968159163616,6505.3337409515843,5803.0621226098283,5848.2049229728837,5903.001793320007,5967.998963823331,9,9,9,8,8,8,8]
[null,"Customer requested Meter Accuracy Testing of type 5-6 meter (physically test meter). CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Inspection required to check reported or suspected fault and no fault in meter is found. (no physical meter test). No CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Inspection required to check reported or suspected fault and no fault in meter is found. (no physical meter test). No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Inspection required to check reported or suspected fault and no fault in meter is found. (no physical meter test). CT - BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Inspection required to check reported or suspected fault and no fault in meter is found. (no physical meter test). CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to conduct a site review of the state of the customer’s metering installation(s) (no physical meter test), i.e. multiple premises.  Includes provision of meter data above the minimum requirements and meter inspection to check a reported or suspected fault.  Does not include provision of any hardware (business hours) - First Unit. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to conduct a site review of the state of the customer’s metering installation(s) (no physical meter test), i.e. multiple premises.  Includes provision of meter data above the minimum requirements and meter inspection to check a reported or suspected fault.  Does not include provision of any hardware (after hours) - First Unit. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to conduct a site review of the state of the customer’s metering installation(s) (no physical meter test), i.e. multiple premises.  Includes provision of meter data above the minimum requirements and meter inspection to check a reported or suspected fault.  Does not include provision of any hardware (business hours) - Additional Units. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to conduct a site review of the state of the customer’s metering installation(s) (no physical meter test), i.e. multiple premises.  Includes provision of meter data above the minimum requirements and meter inspection to check a reported or suspected fault.  Does not include provision of any hardware (after hours) - Additional Units. AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to make a change from one tariff to another tariff (Controlled Load). No CT - BH",240309.55265732194,223107.52828579064,229257.87069731194,223065.09789250686,218130.75827456731,213640.46528022186,209386.91863158505,1256,1218,1182,1146,1112,1079,1046]
[null,"A request to make a change from one tariff to another tariff (Controlled Load). No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to make a change from one tariff to another tariff (Controlled Load). CT - BH",605.86112295991165,580.039514022905,614.17730904964571,616.36047673027815,621.156535914855,626.98869013019089,633.88678307880059,3,3,3,3,3,3,3]
[null,"A request to make a change from one tariff to another tariff (Controlled Load). CT - AH ",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to make a change from one tariff to another tariff . No CT - BH",735661.0116185518,683243.90431176324,701738.5807907118,683015.19251324725,667731.18619190156,653791.31492785062,640972.17567373021,3845,3730,3618,3509,3404,3302,3202]
[null,"A request to make a change from one tariff to another tariff . No CT - AH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"A request to make a change from one tariff to another tariff . CT - BH",2982.7913113411796,2855.6634291317173,2721.3915796180167,2731.0570934337907,2752.2965475504925,2778.0814043603059,2808.6765999652298,10,10,9,9,9,9,9]
[null,"A request to make a change from one tariff to another tariff . CT - AH ",1655.9963937441682,1585.4154189879609,1678.7476721566147,1684.6996354662019,1697.8046038112,1285.2951719953405,1299.4351519469319,4,4,4,4,4,3,3]
[null,"Change time switch. No CT - BH",6239.8350500414808,5790.0922020572325,5936.3012754344309,5859.72645822091,5708.4643288799753,5563.2439478676752,5423.6380440109133,65,63,61,60,58,56,54]
[null,"Change time switch. CT - BH",275.80669503784486,264.04150810481451,279.58505476691869,280.5784188023066,282.76099239174192,285.41779938899793,288.56554050965303,1,1,1,1,1,1,1]
[null,"Meter alteration – meter is being relocated or meter wiring altered and requires DNSP to visit site to verify the integrity of the metering equipment . No CT - BH",356293.78337359685,330876.19087387616,339774.97694064653,330884.68106643501,323282.51976601337,316566.78976588324,310466.84200107114,1400,1358,1317,1278,1239,1202,1166]
[null,"Meter alteration – meter is being relocated or meter wiring altered and requires DNSP to visit site to verify the integrity of the metering equipment . No CT - AH",1783.9581144644276,1707.919651247018,1808.4685869261145,1814.8797563859694,1463.1939284851792,1476.9135339870072,1493.1671044637151,5,5,5,5,4,4,4]
[null,"Meter alteration – meter is being relocated or meter wiring altered and requires DNSP to visit site to verify the integrity of the metering equipment . CT - BH",43384.046262397875,40496.749984874827,41231.271437531759,40274.341309264739,39475.636193689235,38723.072592108896,38014.680337977043,80,78,75,73,71,69,67]
[null,"Meter alteration – meter is being relocated or meter wiring altered and requires DNSP to visit site to verify the integrity of the metering equipment . CT - AH ",4534.4243168042412,4341.1774596372115,4596.7131109771717,4613.0576346618072,3874.111706346529,3910.4137082585767,3953.465481162897,6,6,6,6,5,5,5]
[null,"Customer requests a check read on the meter due to reported error in the meter reading. This is only used to check the accuracy of the meter reading. BH",110074.14682241331,102221.58188311342,104992.53103586055,102199.48219280252,99906.360157448478,97818.565406118054,95932.723722780647,11000,10670,10350,10039,9738,9446,9163]
[null,"Reading undertaken upon customer move in. Retail requested. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Provision of load profile data where available – Retailer requested. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Reseal and inspection of meter after customer initated work. BH",1083649.4519239871,1006343.1264214567,1033648.9293102117,1006158.965995335,983543.63785511162,963003.38385426172,944431.07418972568,15000,14550,14114,13690,13279,12881,12495]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Customer at fault. BH - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Customer at fault. BH - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Customer at fault. AH - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Customer at fault. AH - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Customer at fault. A/T - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Customer at fault. A/T - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Third party at fault. BH - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Third party at fault. BH - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Third party at fault. AH - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Third party at fault. AH - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Third party at fault. A/T - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  TECHNICAL. Third party at fault. A/T - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  NON TECHNICAL. Customer at fault. BH",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  NON TECHNICAL. Customer at fault. AH",0,0,0,0,0,0,0,5473,5473,5473,5473,5473,5473,5473]
[null," Crews attend site at the customers request and is unable to perform job due to customers fault/fault of a third party.  NON TECHNICAL. Customer at fault. A/T",0,0,0,0,0,0,0,133,133,133,133,133,133,133]
[null,"Travel time to perform the installation of a service requested by a retailer or customer, and the service is unable to be performed due to customer/retailer fault. BH - 1 crew",527183.41070151632,504716.2351924004,534425.45837169432,536324.12449732248,540495.96216317755,545559.86598917271,551566.89517890301,0,0,0,0,0,0,0]
[null,"Travel time to perform the installation of a service requested by a retailer or customer, and the service is unable to be performed due to customer/retailer fault. AH - 1 crew",17941.366723116767,17176.747487956331,18187.822093824689,18252.453574208914,18394.41552782747,18566.763947800788,18771.188410152929,2,2,2,2,2,2,2]
[null,"Travel time to perform the installation of a service requested by a retailer or customer, and the service is unable to be performed due to customer/retailer fault. A/T - 1 crew",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Travel time to perform the installation of a service requested by a retailer or customer, and the service is unable to be performed due to customer/retailer fault. BH - 2 crews",288.98006133921956,276.65951471661015,292.94108667052552,293.99188774765207,296.26401609060713,299.04984745713665,302.33875024294264,0,0,0,0,0,0,0]
[null,"Travel time to perform the installation of a service requested by a retailer or customer, and the service is unable to be performed due to customer/retailer fault. AH - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Travel time to perform the installation of a service requested by a retailer or customer, and the service is unable to be performed due to customer/retailer fault. A/T - 2 crews",0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"4.4 Quoted services","index":28,"n_rows":11,"n_cols":16,"rows_kept":11,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,9,8,15],[8,1,9,1],[5,1,5,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.4 ANCILLARY SERVICES - QUOTED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.4.1 - COST METRICS FOR QUOTED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Service (DNSP to nominate)"]

{"sheet":"5.4 MD & utilisation-Spatial","index":29,"n_rows":11577,"n_cols":12,"rows_kept":11577,"cut":false,"hidden":false,"merged":[[11337,1,11337,2],[11338,1,11338,2],[11339,1,11339,2],[11340,1,11340,2],[11341,1,11341,2],[11342,1,11342,2],[11343,1,11343,2],[11344,1,11344,2],[11345,1,11345,2],[11346,1,11346,2],[11347,1,11347,2],[11348,1,11348,2],[11349,1,11349,2],[11350,1,11350,2],[11351,1,11351,2],[11352,1,11352,2],[11353,1,11353,2],[11354,1,11354,2],[11355,1,11355,2],[11125,1,11125,2],[11126,1,11126,2],[11127,1,11127,2],[11128,1,11128,2],[11129,1,11129,2],[11130,1,11130,2],[11131,1,11131,2],[11132,1,11132,2],[11133,1,11133,2],[11134,1,11134,2],[11271,1,11271,2],[11272,1,11272,2],[11273,1,11273,2],[11274,1,11274,2],[11275,1,11275,2],[11276,1,11276,2],[11277,1,11277,2],[11278,1,11278,2],[11279,1,11279,2],[11280,1,11280,2],[11281,1,11281,2],[11282,1,11282,2],[11283,1,11283,2],[11284,1,11284,2],[11285,1,11285,2],[11286,1,11286,2],[11287,1,11287,2],[11288,1,11288,2],[11289,1,11289,2],[11323,1,11323,2],[11324,1,11324,2],[11325,1,11325,2],[11326,1,11326,2],[11327,1,11327,2],[11328,1,11328,2],[11329,1,11329,2],[11330,1,11330,2],[11331,1,11331,2],[11332,1,11332,2],[11333,1,11333,2],[11334,1,11334,2],[11335,1,11335,2],[11336,1,11336,2],[11205,1,11205,2],[11206,1,11206,2],[11257,1,11257,2],[11258,1,11258,2],[11259,1,11259,2],[11260,1,11260,2],[11261,1,11261,2],[11262,1,11262,2],[11263,1,11263,2],[11264,1,11264,2],[11265,1,11265,2],[11266,1,11266,2],[11267,1,11267,2],[11268,1,11268,2],[11269,1,11269,2],[11270,1,11270,2],[11074,5,11074,6],[11074,7,11074,11],[11077,1,11077,2],[11078,1,11078,2],[11079,1,11079,2],[11080,1,11080,2],[11081,1,11081,2],[11082,1,11082,2],[11083,1,11083,2],[11084,1,11084,2],[11085,1,11085,2],[11086,1,11086,2],[11087,1,11087,2],[11088,1,11088,2],[11089,1,11089,2],[11090,1,11090,2],[11091,1,11091,2],[11092,1,11092,2],[11093,1,11093,2],[11094,1,11094,2],[11095,1,11095,2],[11096,1,11096,2],[11097,1,11097,2],[11098,1,11098,2],[11099,1,11099,2],[11100,1,11100,2],[11101,1,11101,2],[11102,1,11102,2],[11103,1,11103,2],[11104,1,11104,2],[11105,1,11105,2],[11106,1,11106,2],[11107,1,11107,2],[11108,1,11108,2],[11109,1,11109,2],[11110,1,11110,2],[11111,1,11111,2],[11112,1,11112,2],[11113,1,11113,2],[11114,1,11114,2],[11115,1,11115,2],[11116,1,11116,2],[11117,1,11117,2],[11118,1,11118,2],[11119,1,11119,2],[11120,1,11120,2],[11121,1,11121,2],[11122,1,11122,2],[11123,1,11123,2],[11124,1,11124,2],[11489,1,11489,2],[11490,1,11490,2],[11491,1,11491,2],[11492,1,11492,2],[11493,1,11493,2],[11494,1,11494,2],[11495,1,11495,2],[11496,1,11496,2],[11497,1,11497,2],[11455,1,11455,2],[11168,1,11168,2],[11169,1,11169,2],[11170,1,11170,2],[11171,1,11171,2],[11172,1,11172,2],[11173,1,11173,2],[11174,1,11174,2],[11175,1,11175,2],[11176,1,11176,2],[11177,1,11177,2],[11178,1,11178,2],[11179,1,11179,2],[11180,1,11180,2],[11181,1,11181,2],[11182,1,11182,2],[11183,1,11183,2],[11184,1,11184,2],[11185,1,11185,2],[11186,1,11186,2],[11187,1,11187,2],[11188,1,11188,2],[11189,1,11189,2],[11190,1,11190,2],[11191,1,11191,2],[11192,1,11192,2],[11193,1,11193,2],[11194,1,11194,2],[11195,1,11195,2],[11196,1,11196,2],[11197,1,11197,2],[11198,1,11198,2],[11199,1,11199,2],[11200,1,11200,2],[11201,1,11201,2],[11202,1,11202,2],[11203,1,11203,2],[11204,1,11204,2],[11240,1,11240,2],[11241,1,11241,2],[11242,1,11242,2],[11243,1,11243,2],[11244,1,11244,2],[11245,1,11245,2],[11246,1,11246,2],[11247,1,11247,2],[11248,1,11248,2],[11249,1,11249,2],[11250,1,11250,2],[11251,1,11251,2],[11252,1,11252,2],[11253,1,11253,2],[11254,1,11254,2],[11255,1,11255,2],[11256,1,11256,2],[11020,5,11020,6],[11020,7,11020,11],[201,2,202,2],[201,3,202,3],[203,2,204,2],[203,3,204,3],[247,2,248,2],[247,3,248,3],[249,2,250,2],[249,3,250,3],[261,2,262,2],[261,3,262,3],[719,3,720,3],[251,2,252,2],[251,3,252,3],[253,2,254,2],[253,3,254,3],[255,2,256,2],[255,3,256,3],[257,2,258,2],[257,3,258,3],[259,2,260,2],[259,3,260,3],[623,2,624,2],[1113,5,1113,6],[711,2,712,2],[711,3,712,3],[713,2,714,2],[713,3,714,3],[703,2,704,2],[315,2,316,2],[315,3,316,3],[317,2,318,2],[317,3,318,3],[319,2,320,2],[319,3,320,3],[321,2,322,2],[321,3,322,3],[323,2,324,2],[323,3,324,3],[325,2,326,2],[325,3,326,3],[327,2,328,2],[327,3,328,3],[329,2,330,2],[329,3,330,3],[1113,7,1113,11],[697,3,698,3],[699,2,700,2],[699,3,700,3],[701,2,702,2],[701,3,702,3],[691,2,692,2],[311,2,312,2],[311,3,312,3],[313,2,314,2],[331,3,332,3],[211,2,212,2],[211,3,212,3],[213,2,214,2],[205,2,206,2],[205,3,206,3],[207,2,208,2],[691,3,692,3],[9,7,9,11],[41,2,42,2],[41,3,42,3],[43,2,44,2],[43,3,44,3],[45,2,46,2],[45,3,46,3],[107,2,108,2],[107,3,108,3],[35,2,36,2],[35,3,36,3],[157,2,158,2],[157,3,158,3],[159,2,160,2],[159,3,160,3],[161,2,162,2],[161,3,162,3],[163,2,164,2],[163,3,164,3],[37,2,38,2],[37,3,38,3],[39,2,40,2],[39,3,40,3],[29,2,30,2],[29,3,30,3],[31,2,32,2],[537,2,538,2],[537,3,538,3],[495,2,496,2],[495,3,496,3],[497,2,498,2],[497,3,498,3],[499,2,500,2],[499,3,500,3],[137,2,138,2],[137,3,138,3],[139,2,140,2],[139,3,140,3],[141,2,142,2],[287,3,288,3],[289,2,290,2],[289,3,290,3],[291,2,292,2],[295,3,296,3],[297,2,298,2],[297,3,298,3],[11,2,12,2],[11,3,12,3],[13,2,14,2],[13,3,14,3],[15,2,16,2],[15,3,16,3],[71,2,72,2],[71,3,72,3],[73,2,74,2],[73,3,74,3],[169,2,170,2],[169,3,170,3],[109,2,110,2],[109,3,110,3],[111,2,112,2],[111,3,112,3],[101,2,102,2],[101,3,102,3],[95,3,96,3],[97,2,98,2],[97,3,98,3],[99,2,100,2],[99,3,100,3],[89,2,90,2],[89,3,90,3],[91,2,92,2],[91,3,92,3],[93,2,94,2],[93,3,94,3],[83,2,84,2],[83,3,84,3],[85,2,86,2],[85,3,86,3],[87,2,88,2],[87,3,88,3],[77,2,78,2],[77,3,78,3],[153,2,154,2],[131,2,132,2],[131,3,132,3],[133,2,134,2],[133,3,134,3],[79,2,80,2],[135,2,136,2],[135,3,136,3],[143,2,144,2],[143,3,144,3],[145,2,146,2],[145,3,146,3],[147,2,148,2],[147,3,148,3],[149,2,150,2],[149,3,150,3],[153,3,154,3],[167,2,168,2],[167,3,168,3],[23,2,24,2],[23,3,24,3],[25,2,26,2],[17,2,18,2],[17,3,18,3],[19,2,20,2],[19,3,20,3],[21,2,22,2],[21,3,22,3],[151,2,152,2],[151,3,152,3],[31,3,32,3],[33,2,34,2],[33,3,34,3],[797,2,798,2],[299,2,300,2],[299,3,300,3],[301,2,302,2],[301,3,302,3],[303,2,304,2],[303,3,304,3],[305,2,306,2],[305,3,306,3],[307,2,308,2],[307,3,308,3],[79,3,80,3],[81,2,82,2],[81,3,82,3],[539,2,540,2],[539,3,540,3],[507,2,508,2],[507,3,508,3],[509,2,510,2],[509,3,510,3],[511,2,512,2],[511,3,512,3],[501,2,502,2],[501,3,502,3],[503,2,504,2],[503,3,504,3],[505,2,506,2],[505,3,506,3],[533,2,534,2],[533,3,534,3],[535,2,536,2],[535,3,536,3],[199,2,200,2],[199,3,200,3],[281,2,282,2],[281,3,282,3],[283,2,284,2],[283,3,284,3],[285,2,286,2],[285,3,286,3],[287,2,288,2],[309,2,310,2],[309,3,310,3],[103,2,104,2],[103,3,104,3],[105,2,106,2],[105,3,106,3],[95,2,96,2],[649,3,650,3],[651,2,652,2],[651,3,652,3],[811,2,812,2],[811,3,812,3],[813,2,814,2],[703,3,704,3],[787,2,788,2],[787,3,788,3],[789,2,790,2],[789,3,790,3],[791,2,792,2],[667,2,668,2],[667,3,668,3],[669,2,670,2],[669,3,670,3],[629,2,630,2],[795,2,796,2],[795,3,796,3],[655,2,656,2],[655,3,656,3],[657,2,658,2],[657,3,658,3],[661,2,662,2],[661,3,662,3],[663,2,664,2],[769,3,770,3],[771,2,772,2],[771,3,772,3],[773,2,774,2],[773,3,774,3],[763,2,764,2],[663,3,664,3],[665,2,666,2],[665,3,666,3],[573,3,574,3],[575,2,576,2],[575,3,576,3],[341,3,342,3],[343,2,344,2],[343,3,344,3],[345,2,346,2],[345,3,346,3],[347,2,348,2],[347,3,348,3],[349,2,350,2],[349,3,350,3],[351,2,352,2],[541,2,542,2],[579,2,580,2],[579,3,580,3],[581,2,582,2],[275,2,276,2],[275,3,276,3],[277,2,278,2],[25,3,26,3],[27,2,28,2],[27,3,28,3],[207,3,208,3],[209,2,210,2],[209,3,210,3],[245,2,246,2],[245,3,246,3],[263,2,264,2],[263,3,264,3],[265,2,266,2],[265,3,266,3],[267,2,268,2],[267,3,268,3],[269,2,270,2],[269,3,270,3],[271,2,272,2],[271,3,272,3],[273,2,274,2],[273,3,274,3],[389,2,390,2],[389,3,390,3],[277,3,278,3],[279,2,280,2],[279,3,280,3],[313,3,314,3],[491,2,492,2],[491,3,492,3],[493,2,494,2],[291,3,292,3],[293,2,294,2],[293,3,294,3],[295,2,296,2],[331,2,332,2],[213,3,214,3],[215,2,216,2],[215,3,216,3],[217,2,218,2],[217,3,218,3],[155,2,156,2],[155,3,156,3],[141,3,142,3],[165,2,166,2],[165,3,166,3],[831,3,832,3],[833,2,834,2],[833,3,834,3],[815,2,816,2],[815,3,816,3],[805,2,806,2],[805,3,806,3],[807,2,808,2],[807,3,808,3],[809,2,810,2],[809,3,810,3],[877,2,878,2],[877,3,878,3],[783,3,784,3],[785,2,786,2],[785,3,786,3],[581,3,582,3],[583,2,584,2],[583,3,584,3],[585,2,586,2],[585,3,586,3],[587,2,588,2],[587,3,588,3],[589,2,590,2],[589,3,590,3],[591,2,592,2],[591,3,592,3],[593,2,594,2],[593,3,594,3],[595,2,596,2],[595,3,596,3],[597,2,598,2],[859,2,860,2],[859,3,860,3],[861,2,862,2],[861,3,862,3],[779,2,780,2],[779,3,780,3],[769,2,770,2],[853,2,854,2],[853,3,854,3],[855,2,856,2],[855,3,856,3],[857,2,858,2],[857,3,858,3],[847,2,848,2],[847,3,848,3],[849,2,850,2],[849,3,850,3],[851,2,852,2],[851,3,852,3],[841,2,842,2],[841,3,842,3],[843,2,844,2],[843,3,844,3],[845,2,846,2],[863,2,864,2],[863,3,864,3],[839,2,840,2],[839,3,840,3],[865,3,866,3],[659,2,660,2],[659,3,660,3],[649,2,650,2],[871,3,872,3],[873,2,874,2],[873,3,874,3],[875,2,876,2],[837,2,838,2],[837,3,838,3],[337,3,338,3],[339,2,340,2],[339,3,340,3],[405,2,406,2],[405,3,406,3],[407,2,408,2],[407,3,408,3],[341,2,342,2],[799,2,800,2],[799,3,800,3],[801,2,802,2],[801,3,802,3],[803,2,804,2],[803,3,804,3],[763,3,764,3],[765,2,766,2],[765,3,766,3],[767,2,768,2],[767,3,768,3],[673,2,674,2],[673,3,674,3],[675,2,676,2],[675,3,676,3],[677,2,678,2],[677,3,678,3],[747,3,748,3],[749,2,750,2],[749,3,750,3],[721,2,722,2],[721,3,722,3],[693,2,694,2],[693,3,694,3],[695,2,696,2],[469,2,470,2],[469,3,470,3],[471,2,472,2],[471,3,472,3],[473,2,474,2],[473,3,474,3],[475,2,476,2],[475,3,476,3],[477,2,478,2],[477,3,478,3],[479,2,480,2],[479,3,480,3],[481,2,482,2],[481,3,482,3],[483,2,484,2],[483,3,484,3],[485,2,486,2],[485,3,486,3],[487,2,488,2],[487,3,488,3],[489,2,490,2],[489,3,490,3],[829,2,830,2],[829,3,830,3],[831,2,832,2],[1069,2,1070,2],[1069,3,1070,3],[1071,2,1072,2],[1071,3,1072,3],[1073,2,1074,2],[1073,3,1074,3],[1063,2,1064,2],[1063,3,1064,3],[1065,2,1066,2],[1065,3,1066,3],[1067,2,1068,2],[1067,3,1068,3],[1057,2,1058,2],[1057,3,1058,3],[1059,2,1060,2],[1059,3,1060,3],[1061,2,1062,2],[1061,3,1062,3],[1051,2,1052,2],[1051,3,1052,3],[1053,2,1054,2],[1053,3,1054,3],[981,2,982,2],[981,3,982,3],[1055,2,1056,2],[1055,3,1056,3],[1021,2,1022,2],[879,2,880,2],[879,3,880,3],[881,2,882,2],[881,3,882,3],[883,2,884,2],[883,3,884,3],[885,2,886,2],[885,3,886,3],[887,2,888,2],[887,3,888,3],[889,2,890,2],[889,3,890,3],[891,2,892,2],[891,3,892,3],[893,2,894,2],[893,3,894,3],[1021,3,1022,3],[1023,2,1024,2],[1023,3,1024,3],[1025,2,1026,2],[1025,3,1026,3],[1027,2,1028,2],[1027,3,1028,3],[1029,2,1030,2],[1029,3,1030,3],[1031,2,1032,2],[1031,3,1032,3],[1033,2,1034,2],[1033,3,1034,3],[983,2,984,2],[983,3,984,3],[1039,3,1040,3],[1041,2,1042,2],[1041,3,1042,3],[1043,2,1044,2],[1043,3,1044,3],[1045,2,1046,2],[1105,2,1106,2],[1105,3,1106,3],[1107,2,1108,2],[1107,3,1108,3],[1109,2,1110,2],[1109,3,1110,3],[1099,2,1100,2],[1099,3,1100,3],[1101,2,1102,2],[1101,3,1102,3],[1103,2,1104,2],[1103,3,1104,3],[1093,2,1094,2],[1093,3,1094,3],[1095,2,1096,2],[1095,3,1096,3],[1097,2,1098,2],[1097,3,1098,3],[1087,2,1088,2],[1087,3,1088,3],[1089,2,1090,2],[1089,3,1090,3],[1091,2,1092,2],[1091,3,1092,3],[1081,2,1082,2],[1081,3,1082,3],[1083,2,1084,2],[1083,3,1084,3],[1085,2,1086,2],[1085,3,1086,3],[1075,2,1076,2],[1075,3,1076,3],[1077,2,1078,2],[1077,3,1078,3],[1079,2,1080,2],[1079,3,1080,3],[1045,3,1046,3],[1047,2,1048,2],[1047,3,1048,3],[1049,2,1050,2],[1049,3,1050,3],[1035,2,1036,2],[1035,3,1036,3],[1037,2,1038,2],[1037,3,1038,3],[1009,2,1010,2],[1009,3,1010,3],[1011,2,1012,2],[1011,3,1012,3],[1015,2,1016,2],[1015,3,1016,3],[1017,2,1018,2],[1017,3,1018,3],[1019,2,1020,2],[1019,3,1020,3],[1013,2,1014,2],[1013,3,1014,3],[1039,2,1040,2],[967,2,968,2],[967,3,968,3],[927,3,928,3],[929,2,930,2],[929,3,930,3],[919,2,920,2],[641,2,642,2],[641,3,642,3],[333,2,334,2],[333,3,334,3],[335,2,336,2],[335,3,336,3],[337,2,338,2],[351,3,352,3],[353,2,354,2],[353,3,354,3],[355,2,356,2],[355,3,356,3],[357,2,358,2],[357,3,358,3],[359,2,360,2],[359,3,360,3],[361,2,362,2],[361,3,362,3],[363,2,364,2],[363,3,364,3],[365,2,366,2],[365,3,366,3],[367,2,368,2],[367,3,368,3],[369,2,370,2],[369,3,370,3],[371,2,372,2],[371,3,372,3],[373,2,374,2],[373,3,374,3],[375,2,376,2],[375,3,376,3],[377,2,378,2],[597,3,598,3],[567,2,568,2],[567,3,568,3],[219,2,220,2],[219,3,220,3],[221,2,222,2],[221,3,222,3],[223,2,224,2],[223,3,224,3],[225,2,226,2],[225,3,226,3],[227,2,228,2],[227,3,228,3],[229,2,230,2],[229,3,230,3],[231,2,232,2],[231,3,232,3],[233,2,234,2],[233,3,234,3],[235,2,236,2],[235,3,236,3],[237,2,238,2],[237,3,238,3],[239,2,240,2],[239,3,240,3],[241,2,242,2],[241,3,242,3],[243,2,244,2],[243,3,244,3],[577,2,578,2],[577,3,578,3],[377,3,378,3],[379,2,380,2],[379,3,380,3],[381,2,382,2],[381,3,382,3],[383,2,384,2],[383,3,384,3],[385,2,386,2],[385,3,386,3],[387,2,388,2],[387,3,388,3],[527,2,528,2],[527,3,528,3],[447,2,448,2],[447,3,448,3],[449,2,450,2],[449,3,450,3],[451,2,452,2],[451,3,452,3],[453,2,454,2],[453,3,454,3],[455,2,456,2],[455,3,456,3],[457,2,458,2],[457,3,458,3],[459,2,460,2],[459,3,460,3],[461,2,462,2],[461,3,462,3],[529,2,530,2],[529,3,530,3],[569,2,570,2],[569,3,570,3],[571,2,572,2],[571,3,572,3],[573,2,574,2],[613,2,614,2],[613,3,614,3],[615,2,616,2],[615,3,616,3],[617,2,618,2],[995,3,996,3],[985,2,986,2],[985,3,986,3],[987,2,988,2],[987,3,988,3],[989,2,990,2],[989,3,990,3],[909,2,910,2],[971,2,972,2],[971,3,972,3],[949,2,950,2],[949,3,950,3],[951,2,952,2],[951,3,952,3],[953,2,954,2],[953,3,954,3],[955,2,956,2],[955,3,956,3],[957,2,958,2],[957,3,958,3],[959,2,960,2],[959,3,960,3],[961,2,962,2],[969,2,970,2],[969,3,970,3],[895,2,896,2],[895,3,896,3],[897,2,898,2],[897,3,898,3],[899,2,900,2],[899,3,900,3],[931,2,932,2],[931,3,932,3],[933,2,934,2],[933,3,934,3],[935,2,936,2],[935,3,936,3],[925,2,926,2],[925,3,926,3],[757,3,758,3],[759,2,760,2],[759,3,760,3],[919,3,920,3],[961,3,962,3],[963,2,964,2],[963,3,964,3],[965,2,966,2],[965,3,966,3],[937,2,938,2],[937,3,938,3],[939,2,940,2],[939,3,940,3],[943,2,944,2],[943,3,944,3],[945,2,946,2],[945,3,946,3],[947,2,948,2],[947,3,948,3],[941,2,942,2],[941,3,942,3],[909,3,910,3],[911,2,912,2],[679,3,680,3],[681,2,682,2],[681,3,682,3],[683,2,684,2],[683,3,684,3],[737,2,738,2],[737,3,738,3],[739,2,740,2],[739,3,740,3],[741,2,742,2],[741,3,742,3],[743,2,744,2],[743,3,744,3],[745,2,746,2],[745,3,746,3],[747,2,748,2],[715,2,716,2],[715,3,716,3],[717,2,718,2],[717,3,718,3],[775,2,776,2],[775,3,776,3],[845,3,846,3],[793,2,794,2],[793,3,794,3],[761,2,762,2],[761,3,762,3],[751,2,752,2],[751,3,752,3],[753,2,754,2],[753,3,754,3],[755,2,756,2],[755,3,756,3],[723,2,724,2],[723,3,724,3],[725,2,726,2],[725,3,726,3],[709,2,710,2],[709,3,710,3],[719,2,720,2],[777,2,778,2],[777,3,778,3],[757,2,758,2],[797,3,798,3],[927,2,928,2],[865,2,866,2],[813,3,814,3],[875,3,876,3],[869,2,870,2],[869,3,870,3],[823,2,824,2],[823,3,824,3],[825,2,826,2],[825,3,826,3],[827,2,828,2],[827,3,828,3],[835,2,836,2],[835,3,836,3]],"merged_total":11560,"flags":["merged_cut"]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Abermain BS","Substation Rating","MVA","Non-Coincident",263.5,263.5,263.5,263.5,263.5,263.5,263.5]
[null,null,null,null,"Coincident",263.5,263.5,263.5,263.5,263.5,263.5,263.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",112.04302978515625,115.87689208984375,117.79342651367187,120.40871429443359,122.06929779052734,123.51973724365234,125.03247833251953]
[null,null,null,null,"Coincident",109.70864105224609,113.46817016601562,115.41197967529297,118.14990234375,119.90021514892578,121.35795593261719,122.80471801757812]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",113.46833801269531,117.4835205078125,119.49269104003906,122.23638153076172,123.97962188720703,125.50293731689453,127.09233856201172]
[null,null,null,null,"Coincident",110.03823852539062,114.058349609375,116.14976501464844,119.139404296875,121.10664367675781,122.73960876464844,124.3533935546875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",99.580177307128906,103.91829681396484,105.64685821533203,108.46316528320312,110.24629974365234,111.54601287841797,113.01151275634766]
[null,null,null,null,"Coincident",97.579902648925781,101.54315185546875,103.30802917480469,106.25432586669922,108.13430786132812,109.46713256835937,110.94161987304687]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",100.45973205566406,104.97933197021484,106.78289031982422,109.72438049316406,111.58858489990234,112.94821929931641,114.48210144042969]
[null,null,null,null,"Coincident",97.706901550292969,101.86711120605469,103.75088500976562,106.9234619140625,109.74757385253906,111.28658294677734,112.96150970458984]
[null,"Algester BS","Substation Rating","MVA","Non-Coincident",201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219]
[null,null,null,null,"Coincident",201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219,201.69999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",72.261116027832031,71.266754150390625,71.223945617675781,70.859710693359375,70.429336547851562,70.305328369140625,70.004364013671875]
[null,null,null,null,"Coincident",69.184089660644531,68.229103088378906,68.187835693359375,67.838897705078125,67.43212890625,67.31951904296875,67.033050537109375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.914779663085938,72.897659301757812,72.853874206542969,72.481300354003906,72.04107666015625,71.914230346679688,71.60638427734375]
[null,null,null,null,"Coincident",70.427101135253906,69.433212280273438,69.390533447265625,69.025978088378906,68.591911315917969,68.464111328125,68.16192626953125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",65.684707641601562,64.879264831542969,64.661636352539062,64.396568298339844,63.954139709472656,63.652976989746094,63.352958679199219]
[null,null,null,null,"Coincident",62.851737976074219,62.078296661376953,61.869792938232422,61.615959167480469,61.197429656982422,60.914829254150391,60.629276275634766]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.187873840332031,66.363998413085938,66.141387939453125,65.870254516601563,65.417701721191406,65.109642028808594,64.802764892578125]
[null,null,null,null,"Coincident",63.863788604736328,63.059661865234375,62.842151641845703,62.577205657958984,62.132369995117187,61.82855224609375,61.527992248535156]
[null,"Archerfield BS","Substation Rating","MVA","Non-Coincident",175.5,175.5,175.5,175.5,175.5,175.5,175.5]
[null,null,null,null,"Coincident",175.5,175.5,175.5,175.5,175.5,175.5,175.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.215133666992188,68.804389953613281,68.862899780273438,68.594215393066406,67.736221313476563,67.0992431640625,66.689788818359375]
[null,null,null,null,"Coincident",54.470203399658203,54.118343353271484,54.163993835449219,53.951534271240234,53.275951385498047,52.774295806884766,52.449924468994141]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.36187744140625,72.926528930664062,72.988540649414063,72.703758239746094,71.794364929199219,71.119224548339844,70.685234069824219]
[null,null,null,null,"Coincident",55.152183532714844,54.787353515625,54.835136413574219,54.613620758056641,53.908962249755859,53.38604736328125,53.048263549804688]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",67.452613830566406,67.1514892578125,67.022750854492188,66.829017639160156,65.961555480957031,65.173126220703125,64.755233764648438]
[null,null,null,null,"Coincident",52.797859191894531,52.535236358642578,52.434257507324219,52.281688690185547,51.602340698242188,50.984973907470703,50.655975341796875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",71.493766784667969,71.174598693847656,71.03814697265625,70.832809448242188,69.913375854492188,69.077713012695312,68.634780883789063]
[null,null,null,null,"Coincident",53.411415100097656,53.139904022216797,53.0347900390625,52.875930786132812,52.168106079101562,51.525283813476563,51.183094024658203]
[null,"Ashgrove West BS","Substation Rating","MVA","Non-Coincident",168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219]
[null,null,null,null,"Coincident",168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219,168.19999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",80.975349426269531,80.53564453125,80.509986877441406,80.091163635253906,79.21685791015625,78.771514892578125,78.693489074707031]
[null,null,null,null,"Coincident",74.205863952636719,73.766181945800781,73.742622375488281,73.332008361816406,72.463272094726563,72.0125732421875,71.925483703613281]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",82.123428344726563,81.677490234375,81.651466369628906,81.226707458496094,80.340003967285156,79.888343811035156,79.809211730957031]
[null,null,null,null,"Coincident",74.920623779296875,74.469734191894531,74.44677734375,74.03106689453125,73.144500732421875,72.679496765136719,72.586769104003906]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",73.08453369140625,72.778587341308594,72.57440185546875,72.268157958984375,71.455291748046875,70.88836669921875,70.796966552734375]
[null,null,null,null,"Coincident",66.446754455566406,66.140182495117187,65.939064025878906,65.639610290527344,64.831748962402344,64.261146545410156,64.161758422851563]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",74.120735168457031,73.810447692871094,73.603370666503906,73.29278564453125,72.468391418457031,71.8934326171875,71.800735473632812]
[null,null,null,null,"Coincident",67.018333435058594,66.703750610351563,66.499610900878906,66.196922302246094,65.372917175292969,64.786811828613281,64.682212829589844]
[null,"Beaudesert BS","Substation Rating","MVA","Non-Coincident",145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562]
[null,null,null,null,"Coincident",145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562,145.10000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.287933349609375,40.235942840576172,41.06646728515625,42.388015747070312,43.486129760742187,44.783927917480469,45.489849090576172]
[null,null,null,null,"Coincident",40.287933349609375,40.235942840576172,41.06646728515625,42.371753692626953,43.428863525390625,44.685150146484375,45.371658325195313]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.802421569824219,42.747184753417969,43.629547119140625,45.033576965332031,46.200225830078125,47.579025268554688,48.329002380371094]
[null,null,null,null,"Coincident",42.331378936767578,42.274421691894531,43.202369689941406,44.290081024169922,45.585197448730469,46.623081207275391,47.390670776367188]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.168968200683594,37.170448303222656,37.918262481689453,39.375656127929687,40.525405883789063,41.773796081542969,42.489353179931641]
[null,null,null,null,"Coincident",37.168968200683594,37.170448303222656,37.917076110839844,39.323799133300781,40.429695129394531,41.633857727050781,42.328437805175781]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.488792419433594,39.490364074707031,40.28485107421875,41.833206176757813,43.054714202880859,44.381019592285156,45.141239166259766]
[null,null,null,null,"Coincident",39.005306243896484,39.005233764648437,39.845516204833984,41.050716400146484,42.403564453125,43.393383026123047,44.170356750488281]
[null,"Beenleigh BS","Substation Rating","MVA","Non-Coincident",259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562]
[null,null,null,null,"Coincident",259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562,259.60000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",129.66209411621094,129.10580444335937,129.51171875,129.42727661132812,128.37530517578125,128.40682983398437,129.29911804199219]
[null,null,null,null,"Coincident",129.22892761230469,128.66680908203125,129.06536865234375,128.97218322753906,127.91043090820312,127.92852783203125,128.80656433105469]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",129.675537109375,129.11672973632812,129.52445983886719,129.43962097167969,128.38330078125,128.41493225097656,129.31088256835937]
[null,null,null,null,"Coincident",129.50926208496094,128.93193054199219,129.33493041992187,129.23643493652344,128.15138244628906,128.16523742675781,129.05441284179687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",117.62981414794922,117.28078460693359,117.30878448486328,117.3316650390625,116.29899597167969,115.99768829345703,116.73001098632812]
[null,null,null,null,"Coincident",117.22492218017578,116.86431884765625,116.89096069335937,116.91075897216797,115.87542724609375,115.57793426513672,116.31828308105469]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",118.96847534179687,118.60572814941406,118.63482666015625,118.65859985351562,117.58553314208984,117.27249908447266,118.03337097167969]
[null,null,null,null,"Coincident",117.32209777832031,116.95455932617187,116.97994995117187,116.99805450439453,115.94896697998047,115.64599609375,116.39189147949219]
[null,"Beerwah BS","Substation Rating","MVA","Non-Coincident",143.5,143.5,143.5,143.5,143.5,143.5,143.5]
[null,null,null,null,"Coincident",143.5,143.5,143.5,143.5,143.5,143.5,143.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.430313110351562,54.289188385009766,55.071315765380859,55.724971771240234,55.56573486328125,55.602188110351562,55.770401000976562]
[null,null,null,null,"Coincident",52.946102142333984,52.799896240234375,53.612648010253906,54.305423736572266,54.166591644287109,54.215919494628906,54.391490936279297]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.799060821533203,57.649204254150391,58.479736328125,59.173847198486328,59.004756927490234,59.043464660644531,59.222091674804688]
[null,null,null,null,"Coincident",55.059368133544922,54.906147003173828,55.881210327148438,56.732826232910156,56.582611083984375,56.630863189697266,56.814441680908203]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.155635833740234,49.100975036621094,49.768199920654297,50.502758026123047,50.323215484619141,50.216789245605469,50.344711303710938]
[null,null,null,null,"Coincident",47.716567993164063,47.65545654296875,48.359188079833984,49.132823944091797,48.972991943359375,48.881954193115234,49.016994476318359]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.197929382324219,52.139884948730469,52.848407745361328,53.628425598144531,53.437770843505859,53.324760437011719,53.460597991943359]
[null,null,null,null,"Coincident",49.570510864257813,49.507091522216797,50.371791839599609,51.314258575439453,51.14129638671875,51.040508270263672,51.181079864501953]
[null,"Belmont BS","Substation Rating","MVA","Non-Coincident",298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437]
[null,null,null,null,"Coincident",298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437,298.89999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",138.94366455078125,138.13508605957031,138.06619262695312,137.83683776855469,136.81646728515625,136.41438293457031,136.76963806152344]
[null,null,null,null,"Coincident",134.90391540527344,134.11924743652344,134.05162048339844,133.82588195800781,132.82965087890625,132.43208312988281,132.77018737792969]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",140.07685852050781,139.24526977539062,139.17440795898437,138.93855285644531,137.88935852050781,137.47596740722656,137.84121704101562]
[null,null,null,null,"Coincident",134.976318359375,134.18399047851562,134.11557006835937,133.88746643066406,132.8819580078125,132.48030090332031,132.82040405273437]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",125.19239807128906,124.63405609130859,124.22265625,124.13571929931641,123.14659118652344,122.4476318359375,122.70798492431641]
[null,null,null,null,"Coincident",121.57424163818359,121.03235626220703,120.63227081298828,120.54508972167969,119.57956695556641,118.89447784423828,119.14116668701172]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",125.95209503173828,125.37948608398437,124.95762634277344,124.86848449707031,123.85440063476562,123.13796234130859,123.40481567382812]
[null,null,null,null,"Coincident",121.57448577880859,121.03237915039062,122.66836547851562,122.57610321044922,121.56826019287109,120.85064697265625,121.10257720947266]
[null,"Brendale BS","Substation Rating","MVA","Non-Coincident",273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125]
[null,null,null,null,"Coincident",273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125,273.20001220703125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",194.84771728515625,194.65605163574219,195.70698547363281,196.21023559570312,195.06573486328125,194.7779541015625,195.42301940917969]
[null,null,null,null,"Coincident",188.9322509765625,188.73625183105469,189.74151611328125,190.21041870117187,189.08248901367187,188.78070068359375,189.37666320800781]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",198.16390991210937,197.96073913574219,199.07485961914062,199.60847473144531,198.39501953125,198.0899658203125,198.77378845214844]
[null,null,null,null,"Coincident",189.21586608886719,189.01564025878906,190.03916931152344,190.51486206054687,189.36265563964844,189.05232238769531,189.65576171875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",171.72274780273437,171.7965087890625,172.21382141113281,172.8001708984375,171.70159912109375,170.99647521972656,171.49433898925781]
[null,null,null,null,"Coincident",166.78515625,166.84414672851562,167.24897766113281,167.80892944335937,166.7200927734375,166.01040649414062,166.46490478515625]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",173.73355102539062,173.81117248535156,174.25038146972656,174.86761474609375,173.7113037109375,172.9693603515625,173.49319458007812]
[null,null,null,null,"Coincident",166.80915832519531,166.86833190917969,167.27542114257812,167.83843994140625,166.74176025390625,166.02725219726562,166.48323059082031]
[null,"Browns Plains BS","Substation Rating","MVA","Non-Coincident",196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437]
[null,null,null,null,"Coincident",196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437,196.39999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",102.54999542236328,102.16619110107422,102.35832977294922,102.21603393554687,101.28620910644531,100.87656402587891,101.23366546630859]
[null,null,null,null,"Coincident",101.67227935791016,101.29126739501953,101.48117828369141,101.33908081054687,100.41626739501953,100.01093292236328,100.36774444580078]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",109.06581878662109,108.65762329101562,108.86196899414062,108.71063232421875,107.72173309326172,107.28605651855469,107.66584777832031]
[null,null,null,null,"Coincident",102.79395294189453,102.40621948242187,102.59956359863281,102.45520782470703,101.51556396484375,101.10255432128906,101.46563720703125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",95.222793579101563,94.998085021972656,94.914230346679688,94.881393432617188,93.976829528808594,93.353103637695312,93.644699096679688]
[null,null,null,null,"Coincident",94.396339416503906,94.171859741210938,94.087799072265625,94.05255126953125,93.153106689453125,92.536483764648438,92.831779479980469]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",101.27305603027344,101.03407287597656,100.94489288330078,100.90996551513672,99.947929382324219,99.284568786621094,99.594696044921875]
[null,null,null,null,"Coincident",95.384300231933594,95.156051635742188,95.070281982421875,95.034767150878906,94.119041442871094,93.490890502929687,93.791282653808594]
[null,"Burleigh Heads BS","Substation Rating","MVA","Non-Coincident",164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437]
[null,null,null,null,"Coincident",164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437,164.89999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",105.93423461914062,105.93853759765625,105.99656677246094,105.73561096191406,105.02529144287109,104.8397216796875,105.02556610107422]
[null,null,null,null,"Coincident",78.208915710449219,78.208900451660156,78.264595031738281,78.009109497070313,77.309745788574219,77.1119384765625,77.273200988769531]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",105.97337341308594,105.97770690917969,106.03611755371094,105.77346801757812,105.05870056152344,104.87200927734375,105.05897521972656]
[null,null,null,null,"Coincident",81.060745239257813,81.057861328125,81.11663818359375,80.853843688964844,80.123458862304688,79.901008605957031,80.047439575195313]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",101.70339965820312,101.80912780761719,101.65620422363281,101.48381805419922,100.77272033691406,100.40357208251953,100.55226135253906]
[null,null,null,null,"Coincident",74.372238159179688,74.471084594726563,74.321556091308594,74.152214050292969,73.452056884765625,73.076248168945313,73.202201843261719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",101.71944427490234,101.82563018798828,101.67204284667969,101.49891662597656,100.78495788574219,100.4144287109375,100.56366729736328]
[null,null,null,null,"Coincident",77.107322692871094,77.206871032714844,77.053115844726563,76.879356384277344,76.148147583007812,75.741958618164063,75.852584838867188]
[null,"Caboolture BS","Substation Rating","MVA","Non-Coincident",269.5,269.5,269.5,269.5,269.5,269.5,269.5]
[null,null,null,null,"Coincident",269.5,269.5,269.5,269.5,269.5,269.5,269.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",144.91937255859375,144.79922485351562,146.87858581542969,147.67070007324219,146.99700927734375,146.85810852050781,147.17410278320312]
[null,null,null,null,"Coincident",144.31814575195312,144.21224975585937,146.27529907226562,147.0611572265625,146.38246154785156,146.22767639160156,146.52474975585937]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",148.376220703125,148.2496337890625,150.44041442871094,151.27511596679687,150.56520080566406,150.41883850097656,150.75181579589844]
[null,null,null,null,"Coincident",145.0325927734375,144.93836975097656,147.0706787109375,147.88420104980469,147.18666076660156,147.02616882324219,147.33029174804687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",129.13597106933594,129.25289916992187,130.892578125,131.79225158691406,131.11672973632812,130.65092468261719,130.89012145996094]
[null,null,null,null,"Coincident",128.56283569335937,128.71583557128906,130.34709167480469,131.25164794921875,130.574462890625,130.09466552734375,130.31278991699219]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",131.76605224609375,131.88896179199219,133.61277770996094,134.55882263183594,133.84848022460938,133.35870361328125,133.61019897460938]
[null,null,null,null,"Coincident",129.5145263671875,129.68826293945313,131.3896484375,131.75108337402344,131.05796813964844,130.56683349609375,130.78927612304687]
[null,"Cleveland BS","Substation Rating","MVA","Non-Coincident",286.5,286.5,286.5,286.5,286.5,286.5,286.5]
[null,null,null,null,"Coincident",286.5,286.5,286.5,286.5,286.5,286.5,286.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",168.55239868164063,168.04916381835937,168.12324523925781,167.92829895019531,166.74627685546875,166.2728271484375,166.9644775390625]
[null,null,null,null,"Coincident",157.77659606933594,157.25247192382812,157.31544494628906,157.12472534179687,156.02252197265625,155.57064819335938,156.17355346679687]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",171.72517395019531,171.2010498046875,171.27821350097656,171.07516479492187,169.84417724609375,169.35113525390625,170.0714111328125]
[null,null,null,null,"Coincident",159.1280517578125,158.57902526855469,158.64036560058594,158.44157409667969,157.30580139160156,156.83822631835937,157.45533752441406]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",154.14602661132812,153.88067626953125,153.52067565917969,153.49420166015625,152.34022521972656,151.51188659667969,152.07713317871094]
[null,null,null,null,"Coincident",144.57609558105469,144.27850341796875,143.93550109863281,143.90316772460938,142.82452392578125,142.03947448730469,142.52833557128906]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",156.72952270507812,156.45350646972656,156.07904052734375,156.051513671875,154.85125732421875,153.98980712890625,154.57763671875]
[null,null,null,null,"Coincident",146.37269592285156,146.05470275878906,145.6962890625,145.66020202636719,144.54405212402344,143.72994995117187,144.23126220703125]
[null,"Coomera BS","Substation Rating","MVA","Non-Coincident",189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562]
[null,null,null,null,"Coincident",189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562,189.60000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",101.73305511474609,105.21656799316406,106.52074432373047,107.41551971435547,107.50071716308594,108.05426788330078,109.19081115722656]
[null,null,null,null,"Coincident",98.254554748535156,101.83098602294922,103.08667755126953,103.94661712646484,104.02314758300781,104.55310821533203,105.64957427978516]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",106.58820343017578,110.23796844482422,111.60438537597656,112.54186248779297,112.63112640380859,113.21109008789062,114.40187835693359]
[null,null,null,null,"Coincident",100.6221923828125,103.28316497802734,104.55873107910156,105.42601776123047,105.48545074462891,106.01272583007812,107.12413024902344]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",87.666252136230469,91.249618530273438,92.144660949707031,93.031639099121094,93.07891845703125,93.334083557128906,94.301841735839844]
[null,null,null,null,"Coincident",84.692680358886719,88.378890991210938,89.240249633789063,90.094123840332031,90.134803771972656,90.376968383789063,91.311073303222656]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",91.850074768066406,95.604454040527344,96.542205810546875,97.471519470214844,97.52105712890625,97.788398742675781,98.802337646484375]
[null,null,null,null,"Coincident",86.536026000976563,90.351150512695313,91.221023559570313,92.083267211914062,92.104583740234375,92.334571838378906,93.280113220214844]
[null,"Coorparoo BS","Substation Rating","MVA","Non-Coincident",178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562]
[null,null,null,null,"Coincident",178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562,178.60000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",77.984458923339844,77.219642639160156,76.638877868652344,76.2978515625,76.069656372070312,76.416549682617188,77.299285888671875]
[null,null,null,null,"Coincident",71.475410461425781,70.787246704101562,70.274559020996094,69.961616516113281,69.726188659667969,70.014442443847656,70.824638366699219]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",80.0074462890625,79.222785949707031,78.626953125,78.277084350585938,78.04296875,78.398857116699219,79.304496765136719]
[null,null,null,null,"Coincident",73.722991943359375,73.014907836914063,72.488563537597656,72.165718078613281,71.919548034667969,72.213111877441406,73.048286437988281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",68.642616271972656,68.067359924316406,67.374801635742188,67.142433166503906,66.900405883789063,67.022041320800781,67.768714904785156]
[null,null,null,null,"Coincident",62.977062225341797,62.460475921630859,61.842144012451172,61.628643035888672,61.3836669921875,61.469436645507813,62.155506134033203]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",70.423263549804687,69.833084106445313,69.12255859375,68.884162902832031,68.635856628417969,68.760650634765625,69.526695251464844]
[null,null,null,null,"Coincident",64.953201293945313,64.421859741210937,63.786163330078125,63.565914154052734,63.310470581054688,63.395820617675781,64.102874755859375]
[null,"Doboy BS","Substation Rating","MVA","Non-Coincident",262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437]
[null,null,null,null,"Coincident",262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437,262.89999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",136.19528198242187,135.98603820800781,147.55673217773437,145.68302917480469,134.59254455566406,137.7677001953125,141.30485534667969]
[null,null,null,null,"Coincident",125.61990356445312,125.41822052001953,136.09454345703125,135.72526550292969,124.07501983642578,127.44392395019531,131.16236877441406]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",136.26344299316406,136.05178833007812,147.81141662597656,145.89999389648437,134.64323425292969,137.85530090332031,141.44398498535156]
[null,null,null,null,"Coincident",126.34885406494141,126.14014434814453,137.77278137207031,137.38812255859375,124.75440979003906,127.73382568359375,131.55775451660156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",130.00762939453125,129.94949340820313,141.25782775878906,139.46726989746094,128.36488342285156,131.39573669433594,135.00424194335937]
[null,null,null,null,"Coincident",119.48502349853516,119.43096923828125,129.80931091308594,129.56266784667969,117.90071105957031,121.13518524169922,124.92966461181641]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",130.02200317382812,129.96354675292969,141.39620971679687,139.57830810546875,128.37149047851562,131.41888427734375,135.05918884277344]
[null,null,null,null,"Coincident",120.05431365966797,119.99791717529297,131.26789855957031,131.01103210449219,118.42340850830078,121.31996917724609,125.20740509033203]
[null,"Gatton BS","Substation Rating","MVA","Non-Coincident",143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219]
[null,null,null,null,"Coincident",143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219,143.19999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.436983108520508,29.292133331298828,29.338768005371094,29.297857284545898,29.0260009765625,28.813394546508789,28.699611663818359]
[null,null,null,null,"Coincident",29.259468078613281,29.113027572631836,29.160190582275391,29.121711730957031,28.853822708129883,28.643426895141602,28.531087875366211]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.350700378417969,30.201353073120117,30.249435424804688,30.207256317138672,29.926959991455078,29.707756042480469,29.59044075012207]
[null,null,null,null,"Coincident",30.648988723754883,30.493917465209961,30.542942047119141,30.502141952514648,30.220699310302734,29.999168395996094,29.880422592163086]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.397481918334961,26.303396224975586,26.272062301635742,26.2613525390625,26.004623413085938,25.747297286987305,25.636991500854492]
[null,null,null,null,"Coincident",26.229103088378906,26.133428573608398,26.103029251098633,26.094358444213867,25.841367721557617,25.586515426635742,25.477602005004883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.216854095458984,27.119846343994141,27.087541580200195,27.076498031616211,26.811800003051758,26.546487808227539,26.432758331298828]
[null,null,null,null,"Coincident",27.462215423583984,27.360507965087891,27.328334808349609,27.318792343139648,27.053140640258789,26.785272598266602,26.670263290405273]
[null,"Goodna BS","Substation Rating","MVA","Non-Coincident",217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781]
[null,null,null,null,"Coincident",217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781,217.80000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",125.39115142822266,128.19305419921875,130.14317321777344,131.62730407714844,132.23570251464844,134.09919738769531,136.49528503417969]
[null,null,null,null,"Coincident",125.39115142822266,128.19305419921875,130.14317321777344,131.62730407714844,132.23570251464844,134.09919738769531,136.49528503417969]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",125.77005004882812,128.61585998535156,130.597412109375,132.10592651367187,132.72442626953125,134.6192626953125,137.05650329589844]
[null,null,null,null,"Coincident",125.39185333251953,128.19758605957031,130.14987182617188,131.63514709472656,132.24266052246094,134.10824584960937,136.50811767578125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",115.76415252685547,118.55353546142578,119.91954803466797,121.32115936279297,121.73908996582031,123.11157989501953,125.23775482177734]
[null,null,null,null,"Coincident",115.690673828125,118.53656005859375,119.91954803466797,121.32115936279297,121.73908996582031,123.11157989501953,125.23775482177734]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",116.00496673583984,118.83216094970703,120.21737670898437,121.63912963867187,122.06315612792969,123.45592498779297,125.61429595947266]
[null,null,null,null,"Coincident",117.1865234375,120.11000823974609,121.49649810791016,122.90061950683594,123.29692840576172,124.66896057128906,126.81236267089844]
[null,"Griffin BS","Substation Rating","MVA","Non-Coincident",189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562]
[null,null,null,null,"Coincident",189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562,189.10000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",66.743759155273437,67.144790649414062,67.746429443359375,67.912345886230469,67.577079772949219,67.463172912597656,67.631202697753906]
[null,null,null,null,"Coincident",66.743759155273437,67.144790649414062,67.746429443359375,67.912345886230469,67.577079772949219,67.463172912597656,67.631202697753906]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",66.751800537109375,67.154853820800781,67.759925842285156,67.926872253417969,67.589561462402344,67.474990844726563,67.644004821777344]
[null,null,null,null,"Coincident",68.443046569824219,68.860641479492187,69.489341735839844,69.660728454589844,69.308128356933594,69.185470581054687,69.356826782226562]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",58.734828948974609,59.165180206298828,59.532192230224609,59.735141754150391,59.410449981689453,59.156745910644531,59.281024932861328]
[null,null,null,null,"Coincident",58.734828948974609,59.165180206298828,59.532192230224609,59.735141754150391,59.410449981689453,59.156745910644531,59.281024932861328]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",61.583061218261719,62.034282684326172,62.419094085693359,62.631885528564453,62.291446685791016,62.025440216064453,62.155746459960937]
[null,null,null,null,"Coincident",61.457019805908203,61.906501770019531,62.291450500488281,62.501880645751953,62.158840179443359,61.888744354248047,62.014171600341797]
[null,"Gympie BS","Substation Rating","MVA","Non-Coincident",135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219]
[null,null,null,null,"Coincident",135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219,135.19999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.005062103271484,47.96417236328125,48.03448486328125,47.977558135986328,47.689315795898438,47.574039459228516,47.617439270019531]
[null,null,null,null,"Coincident",43.500011444091797,43.459060668945313,43.536430358886719,43.479999542236328,43.17962646484375,43.057609558105469,43.099655151367188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.014690399169922,47.973457336425781,48.044368743896484,47.986953735351563,47.696430206298828,47.580326080322266,47.624031066894531]
[null,null,null,null,"Coincident",44.557498931884766,44.515235900878906,44.594497680664063,44.536262512207031,44.2274169921875,44.101974487304688,44.145015716552734]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.19036865234375,46.194782257080078,46.170986175537109,46.147274017333984,45.856304168701172,45.664093017578125,45.694568634033203]
[null,null,null,null,"Coincident",41.644733428955078,41.651203155517578,41.629859924316406,41.608058929443359,41.304969787597656,41.102615356445313,41.131256103515625]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.190677642822266,46.195098876953125,46.1712646484375,46.147518157958984,45.856311798095703,49.827594757080078,49.860847473144531]
[null,null,null,null,"Coincident",42.647693634033203,42.654136657714844,42.631980895996094,42.609348297119141,42.297748565673828,42.089759826660156,42.119029998779297]
[null,"Hays Inlet BS","Substation Rating","MVA","Non-Coincident",267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438]
[null,null,null,null,"Coincident",267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438,267.89999389648438]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",166.58842468261719,166.80976867675781,167.74002075195312,167.71528625488281,166.51925659179687,166.02133178710937,166.92330932617187]
[null,null,null,null,"Coincident",161.22398376464844,161.4207763671875,162.32070922851562,162.29397583007812,161.12382507324219,160.63203430175781,161.52328491210937]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",167.140380859375,167.36677551269531,168.31846618652344,168.29315185546875,167.06962585449219,166.56039428710937,167.48292541503906]
[null,null,null,null,"Coincident",161.345458984375,161.54132080078125,162.45065307617187,162.42292785644531,161.23905944824219,160.74150085449219,161.64425659179687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",148.7095947265625,149.08888244628906,149.50041198730469,149.62860107421875,148.49305725097656,147.673095703125,148.44920349121094]
[null,null,null,null,"Coincident",143.98350524902344,144.33653259277344,144.73196411132812,144.85447692871094,143.74232482910156,142.93630981445312,143.70472717285156]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",148.91519165039063,149.30039978027344,149.71842956542969,149.84866333007812,148.6953125,147.86288452148437,148.65078735351562]
[null,null,null,null,"Coincident",143.99028015136719,144.34365844726562,144.74015808105469,144.86289978027344,143.74736022949219,142.93940734863281,143.70991516113281]
[null,"Ibis BS","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.963466644287109,10.964662551879883,10.966211318969727,10.968109130859375,10.971034049987793,10.976409912109375,10.982295036315918]
[null,null,null,null,"Coincident",8.1732845306396484,8.1736059188842773,8.1740217208862305,8.1745319366455078,8.1753177642822266,8.176762580871582,8.1783437728881836]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.482917785644531,12.484279632568359,12.486042976379395,12.488204002380371,12.491534233093262,12.497654914855957,12.504356384277344]
[null,null,null,null,"Coincident",9.039921760559082,9.0402603149414062,9.0406990051269531,9.0412368774414062,9.0420656204223633,9.0435886383056641,9.0452556610107422]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.828677177429199,10.830021858215332,10.831254959106445,10.83326244354248,10.836125373840332,10.841163635253906,10.846975326538086]
[null,null,null,null,"Coincident",8.0758113861083984,8.0761728286743164,8.0765037536621094,8.0770435333251953,8.0778131484985352,8.0791664123535156,8.0807285308837891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.329447746276855,12.330979347229004,12.332383155822754,12.33466911315918,12.337928771972656,12.34366512298584,12.350281715393066]
[null,null,null,null,"Coincident",8.9338884353637695,8.9342689514160156,8.9346179962158203,8.9351873397827148,8.9359989166259766,8.9374256134033203,8.9390726089477539]
[null,"Jimboomba BS","Substation Rating","MVA","Non-Coincident",88,88,88,88,88,88,88]
[null,null,null,null,"Coincident",88,88,88,88,88,88,88]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",73.65826416015625,74.645233154296875,76.019233703613281,78.03192138671875,79.450592041015625,80.186386108398437,81.206069946289063]
[null,null,null,null,"Coincident",39.305877685546875,39.841331481933594,40.580589294433594,41.668769836425781,42.439868927001953,42.838283538818359,43.388240814208984]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.601356506347656,77.627761840820312,79.056663513183594,81.149772644042969,82.6251220703125,83.39031982421875,84.45074462890625]
[null,null,null,null,"Coincident",40.516643524169922,41.055454254150391,41.805534362792969,42.937290191650391,43.742145538330078,44.140872955322266,44.695911407470703]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.280597686767578,64.219703674316406,65.22418212890625,67.214515686035156,68.591163635253906,69.044197082519531,69.895767211914062]
[null,null,null,null,"Coincident",33.767917633056641,34.276638031005859,34.817863464355469,35.893833160400391,36.642162322998047,36.888755798339844,37.348163604736328]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",65.809043884277344,66.785667419433594,67.830284118652344,69.900146484375,71.331794738769531,71.802932739257813,72.688529968261719]
[null,null,null,null,"Coincident",34.806995391845703,35.320022583007813,35.867641448974609,36.989532470703125,37.77362060546875,38.017398834228516,38.480678558349609]
[null,"Lockrose BS","Substation Rating","MVA","Non-Coincident",143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437]
[null,null,null,null,"Coincident",143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437,143.89999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",68.892013549804687,68.868965148925781,69.030784606933594,68.9404296875,68.513916015625,68.427467346191406,68.510040283203125]
[null,null,null,null,"Coincident",65.514755249023438,65.484428405761719,65.638809204101563,65.554718017578125,65.158767700195312,65.087699890136719,65.171455383300781]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",69.039840698242187,69.0164794921875,69.180496215820312,69.088912963867188,68.656654357910156,68.569053649902344,68.652725219726563]
[null,null,null,null,"Coincident",65.89825439453125,65.866401672363281,66.022804260253906,65.937171936035156,65.536346435546875,65.46514892578125,65.549552917480469]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.491714477539063,60.553268432617187,60.527477264404297,60.507221221923828,60.101848602294922,59.869525909423828,59.919269561767578]
[null,null,null,null,"Coincident",57.42132568359375,57.472446441650391,57.448284149169922,57.430843353271484,57.054664611816406,56.843959808349609,56.896015167236328]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",60.543422698974609,60.605537414550781,60.579509735107422,60.559070587158203,60.150077819824219,59.915729522705078,59.965904235839844]
[null,null,null,null,"Coincident",57.780666351318359,57.831554412841797,57.806873321533203,57.788841247558594,57.407764434814453,57.194709777832031,57.247016906738281]
[null,"Loganlea BS","Substation Rating","MVA","Non-Coincident",256,256,256,256,256,256,256]
[null,null,null,null,"Coincident",256,256,256,256,256,256,256]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",103.48218536376953,102.79129028320312,102.85282135009766,102.63307189941406,101.71849060058594,101.26615142822266,101.24358367919922]
[null,null,null,null,"Coincident",102.69768524169922,102.01598358154297,102.07919311523437,101.86971282958984,100.97610473632812,100.54597473144531,100.54471588134766]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",104.12282562255859,103.41294860839844,103.47615814208984,103.25040435791016,102.31101989746094,101.84651947021484,101.82334899902344]
[null,null,null,null,"Coincident",102.72281646728516,102.03675842285156,102.10039520263672,101.88973999023437,100.99102783203125,100.55872344970703,100.55758666992187]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",95.433738708496094,94.926063537597656,94.71923828125,94.610374450683594,93.717750549316406,93.053939819335938,92.996551513671875]
[null,null,null,null,"Coincident",94.651634216308594,94.151741027832031,93.948585510253906,93.848625183105469,92.976318359375,92.335220336914063,92.297828674316406]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",95.864730834960938,95.344741821289062,95.1329345703125,95.021453857421875,94.107612609863281,93.428260803222656,93.369544982910156]
[null,null,null,null,"Coincident",96.687980651855469,96.166908264160156,95.95489501953125,95.851753234863281,94.941207885742188,94.272148132324219,94.234580993652344]
[null,"Lytton BS","Substation Rating","MVA","Non-Coincident",238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781]
[null,null,null,null,"Coincident",238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781,238.30000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",128.014404296875,128.0631103515625,129.64897155761719,129.43191528320312,130.6517333984375,134.19142150878906,137.042236328125]
[null,null,null,null,"Coincident",114.05610656738281,114.08060455322266,115.62238311767578,115.42143249511719,116.69052886962891,120.20433044433594,123.01100921630859]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",128.04246520996094,128.09149169921875,129.6890869140625,129.47030639648437,130.70021057128906,134.27510070800781,137.16032409667969]
[null,null,null,null,"Coincident",114.26186370849609,114.28651428222656,115.83196258544922,115.63006591796875,116.89986419677734,120.42027282714844,123.23291015625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",122.09368896484375,122.2398681640625,123.70594787597656,123.58262634277344,124.91374969482422,128.456298828125,131.40327453613281]
[null,null,null,null,"Coincident",108.70169067382812,108.81231689453125,110.25661468505859,110.13860321044922,111.51705932617187,115.05229949951172,117.95735168457031]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",122.09573364257812,122.24220275878906,123.71220397949219,123.58847808837891,124.92459869384766,128.48741149902344,131.45849609375]
[null,null,null,null,"Coincident",108.87220001220703,108.98341369628906,110.43057250976562,110.31207275390625,111.69162750244141,115.23307037353516,118.1441650390625]
[null,"Meeandah BS","Substation Rating","MVA","Non-Coincident",167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781]
[null,null,null,null,"Coincident",167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781,167.80000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.815456390380859,50.809612274169922,55.377735137939453,55.174213409423828,54.524005889892578,54.040920257568359,53.747310638427734]
[null,null,null,null,"Coincident",40.085723876953125,40.081729888916016,43.767719268798828,43.604442596435547,43.082714080810547,42.695117950439453,42.459564208984375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.909328460693359,50.9033203125,55.634876251220703,55.422702789306641,54.745651245117188,54.243427276611328,53.938529968261719]
[null,null,null,null,"Coincident",41.910732269287109,41.906269073486328,45.853984832763672,45.676738739013672,45.110462188720703,44.689823150634766,44.4342041015625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.555049896240234,49.614162445068359,54.275119781494141,54.128376007080078,53.46588134765625,52.860389709472656,52.556713104248047]
[null,null,null,null,"Coincident",39.041801452636719,39.089855194091797,42.851482391357422,42.733871459960937,42.202766418457031,41.717384338378906,41.473972320556641]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.616462707519531,49.676959991455078,54.48681640625,54.334297180175781,53.646530151367188,53.019145965576172,52.704933166503906]
[null,null,null,null,"Coincident",40.773258209228516,40.825294494628906,44.851375579833984,44.723766326904297,44.147617340087891,43.62115478515625,43.357166290283203]
[null,"Molendinar BS","Substation Rating","MVA","Non-Coincident",316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125]
[null,null,null,null,"Coincident",316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125,316.20001220703125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",141.8896484375,143.99394226074219,148.87333679199219,149.37628173828125,148.79994201660156,148.99296569824219,149.81584167480469]
[null,null,null,null,"Coincident",141.8896484375,143.99394226074219,148.87333679199219,149.37628173828125,148.79994201660156,148.99296569824219,149.81584167480469]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",142.57557678222656,144.72236633300781,149.70298767089844,150.21656799316406,149.62803649902344,149.82513427734375,150.66545104980469]
[null,null,null,null,"Coincident",141.911376953125,144.054443359375,149.00762939453125,149.51686096191406,148.93232727050781,149.12718200683594,149.96037292480469]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",128.501220703125,130.92556762695312,135.64718627929687,136.36198425292969,135.88482666015625,135.83062744140625,136.65432739257812]
[null,null,null,null,"Coincident",128.501220703125,130.92556762695312,135.64718627929687,136.36198425292969,135.88482666015625,135.83062744140625,136.65432739257812]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",128.93559265136719,131.40283203125,136.21151733398437,136.93986511230469,136.45364379882812,136.39842224121094,137.23779296875]
[null,null,null,null,"Coincident",130.05874633789063,132.74749755859375,135.66258239746094,136.38090515136719,135.90104675292969,135.84632873535156,136.674072265625]
[null,"Mudgeeraba BS","Substation Rating","MVA","Non-Coincident",98,98,98,98,98,98,98]
[null,null,null,null,"Coincident",98,98,98,98,98,98,98]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.618213653564453,24.64497184753418,24.689352035522461,24.631879806518555,24.424875259399414,24.354497909545898,24.366144180297852]
[null,null,null,null,"Coincident",22.412267684936523,22.436988830566406,22.477989196777344,22.424894332885742,22.233659744262695,22.168645858764648,22.179403305053711]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.973304748535156,26.001537322998047,26.048358917236328,25.987724304199219,25.769325256347656,25.695074081420898,25.707361221313477]
[null,null,null,null,"Coincident",23.207117080688477,23.232690811157227,23.275108337402344,23.220178604125977,23.022342681884766,22.955083847045898,22.966213226318359]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.831775665283203,20.882238388061523,20.862894058227539,20.835039138793945,20.65070915222168,20.539287567138672,20.54248046875]
[null,null,null,null,"Coincident",18.917530059814453,18.964149475097656,18.946277618408203,18.92054557800293,18.750255584716797,18.647321701049805,18.650272369384766]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.978445053100586,22.031686782836914,22.011276245117188,21.981889724731445,21.787412643432617,21.669857025146484,21.673227310180664]
[null,null,null,null,"Coincident",19.591516494750977,19.639745712280273,19.621257781982422,19.594636917114258,19.418468475341797,19.311981201171875,19.315032958984375]
[null,"Myrtletown BS","Substation Rating","MVA","Non-Coincident",239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562]
[null,null,null,null,"Coincident",239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562,239.60000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.392662048339844,42.401908874511719,42.413154602050781,43.060283660888672,42.883060455322266,42.751903533935547,42.672428131103516]
[null,null,null,null,"Coincident",22.800937652587891,22.80693244934082,22.81422233581543,23.233781814575195,23.118881225585937,23.033849716186523,22.982320785522461]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.449150085449219,43.458625793457031,43.47015380859375,44.133407592773438,43.951766967773438,43.817344665527344,43.735885620117188]
[null,null,null,null,"Coincident",23.618505477905273,23.624847412109375,23.632558822631836,24.086870193481445,23.96516227722168,23.875097274780273,23.820518493652344]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.670932769775391,41.699050903320313,41.671737670898438,42.368755340576172,42.185077667236328,42.017566680908203,41.933902740478516]
[null,null,null,null,"Coincident",22.395027160644531,22.413257598876953,22.395549774169922,22.847457885742188,22.728368759155273,22.619766235351563,22.565523147583008]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.709434509277344,42.738250732421875,42.710258483886719,43.424644470214844,43.236392974853516,43.064704895019531,42.978958129882812]
[null,null,null,null,"Coincident",23.18895149230957,23.208234786987305,23.189502716064453,23.678466796875,23.552328109741211,23.437299728393555,23.379850387573242]
[null,"Nambour BS","Substation Rating","MVA","Non-Coincident",143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781]
[null,null,null,null,"Coincident",143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781,143.80000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",10.5,10.5,10.5,10.5,10.5,10.5,10.5]
[null,null,null,null,"Coincident",10.5,10.5,10.5,10.5,10.5,10.5,10.5]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",67.1829833984375,68.219406127929688,68.551315307617188,68.529151916503906,67.880561828613281,67.582748413085938,67.666229248046875]
[null,null,null,null,"Coincident",56.6829833984375,57.717010498046875,58.051315307617187,58.029151916503906,57.380561828613281,57.082748413085938,57.166229248046875]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.23052978515625,68.286651611328125,68.625518798828125,68.602882385253906,67.941024780273437,67.637527465820313,67.722572326660156]
[null,null,null,null,"Coincident",56.684547424316406,57.726737976074219,58.063938140869141,58.041938781738281,57.388824462890625,57.089260101318359,57.173267364501953]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",63.493679046630859,64.702644348144531,64.832077026367188,64.869964599609375,64.221054077148438,63.770847320556641,63.825546264648438]
[null,null,null,null,"Coincident",52.993679046630859,54.185295104980469,54.319892883300781,54.362236022949219,53.716171264648438,53.268291473388672,53.324966430664063]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",63.498012542724609,64.716255187988281,64.846969604492188,64.885246276855469,64.230369567871094,63.776863098144531,63.831924438476562]
[null,null,null,null,"Coincident",53.742294311523438,55.037960052490234,55.183181762695313,55.230506896972656,54.551715850830078,54.081150054931641,54.141178131103516]
[null,"Nudgee BS","Substation Rating","MVA","Non-Coincident",249.5,249.5,249.5,249.5,249.5,249.5,249.5]
[null,null,null,null,"Coincident",249.5,249.5,249.5,249.5,249.5,249.5,249.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",158.6182861328125,161.88467407226562,165.86463928222656,185.06124877929687,183.7149658203125,182.98399353027344,182.6519775390625]
[null,null,null,null,"Coincident",134.40238952636719,137.84770202636719,141.94786071777344,159.81369018554687,158.59939575195312,157.98091125488281,157.72019958496094]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",158.87777709960937,162.19863891601562,166.25038146972656,185.86421203613281,184.48530578613281,183.73680114746094,183.39686584472656]
[null,null,null,null,"Coincident",134.81001281738281,138.48724365234375,142.87820434570312,159.81446838378906,158.59953308105469,157.98092651367187,157.72019958496094]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",150.58638000488281,154.06654357910156,157.73554992675781,174.33731079101562,173.00279235839844,171.9677734375,171.59605407714844]
[null,null,null,null,"Coincident",126.66496276855469,130.31214904785156,134.12884521484375,149.60784912109375,148.40550231933594,147.50297546386719,147.20259094238281]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",150.73057556152344,154.25726318359375,157.98103332519531,174.89375305175781,173.53083801269531,172.47416687011719,172.09475708007812]
[null,null,null,null,"Coincident",126.94438934326172,130.80003356933594,134.87820434570312,150.65229797363281,149.42506408691406,148.50392150878906,148.19754028320312]
[null,"Postmans Ridge BS","Substation Rating","MVA","Non-Coincident",127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781]
[null,null,null,null,"Coincident",127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781,127.30000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.003284454345703,44.918754577636719,44.953853607177734,44.909721374511719,44.702342987060547,44.60614013671875,44.593425750732422]
[null,null,null,null,"Coincident",23.167877197265625,23.091583251953125,23.122777938842773,23.086477279663086,22.910829544067383,22.832530975341797,22.82621955871582]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.593250274658203,47.503852844238281,47.540973663330078,47.494300842285156,47.274990081787109,47.173248291015625,47.159801483154297]
[null,null,null,null,"Coincident",23.6297607421875,23.553190231323242,23.584722518920898,23.547704696655273,23.369396209716797,23.289422988891602,23.28233528137207]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.853542327880859,41.800384521484375,41.78533935546875,41.76007080078125,41.556488037109375,41.420787811279297,41.400440216064453]
[null,null,null,null,"Coincident",21.586734771728516,21.537406921386719,21.52586555480957,21.505685806274414,21.333993911743164,21.222427368164062,21.209537506103516]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.262237548828125,44.206020355224609,44.190109252929688,44.163387298583984,43.948089599609375,43.804576873779297,43.783058166503906]
[null,null,null,null,"Coincident",22.021835327148438,21.972570419311523,21.960714340209961,21.940042495727539,21.765665054321289,21.651884078979492,21.638116836547852]
[null,"Raceview BS","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",110.29792785644531,110.96817016601562,111.17928314208984,113.18044281005859,114.31450653076172,113.7283935546875,113.79065704345703]
[null,null,null,null,"Coincident",108.96968078613281,109.60599517822266,109.80939483642578,111.73828125,112.81600952148437,112.24135589599609,112.30033874511719]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",110.32478332519531,111.00082397460937,111.2138671875,113.23589324951172,114.38375091552734,113.79033660888672,113.85335540771484]
[null,null,null,null,"Coincident",109.02176666259766,109.66374206542969,109.8692626953125,111.85749816894531,112.99635314941406,112.40946197509766,112.46872711181641]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",99.173973083496094,100.07501220703125,99.986244201660156,102.19607543945312,103.46247100830078,102.65158081054687,102.66161346435547]
[null,null,null,null,"Coincident",97.916969299316406,98.780281066894531,98.688262939453125,100.8209228515625,102.02734375,101.23136138916016,101.23906707763672]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",100.82195281982422,101.77084350585937,101.67734527587891,104.00574493408203,105.34087371826172,104.48590850830078,104.49648284912109]
[null,null,null,null,"Coincident",99.917587280273438,98.780410766601563,98.688346862792969,100.83666229248047,102.07411956787109,101.26942443847656,101.27684020996094]
[null,"Richlands BS","Substation Rating","MVA","Non-Coincident",188.10000610351562,188.10000610351562,188.10000610351562,258.5,258.5,258.5,258.5]
[null,null,null,null,"Coincident",188.10000610351562,188.10000610351562,188.10000610351562,258.5,258.5,258.5,258.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",132.32478332519531,132.81553649902344,132.98316955566406,132.61679077148437,131.21144104003906,130.2252197265625,129.98532104492187]
[null,null,null,null,"Coincident",125.82379913330078,126.24436187744141,126.41107940673828,126.07563781738281,124.75754547119141,123.83737945556641,123.64043426513672]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",134.91098022460937,135.42869567871094,135.60556030273437,135.21902465820312,133.73666381835937,132.69667053222656,132.4437255859375]
[null,null,null,null,"Coincident",127.51885223388672,128.01570129394531,128.18821716308594,127.84025573730469,126.47453308105469,125.52112579345703,125.31590270996094]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",125.71237182617187,126.46504211425781,126.27039337158203,126.04143524169922,124.63372802734375,123.36693572998047,123.08180999755859]
[null,null,null,null,"Coincident",119.26954650878906,119.93736267089844,119.75977325439453,119.55461120605469,118.23600769042969,117.05061340332031,116.80960083007812]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",127.94094085693359,128.73374938964844,128.52870178222656,128.28753662109375,126.80506134033203,125.47145843505859,125.17135620117187]
[null,null,null,null,"Coincident",120.77049255371094,121.52381134033203,121.33987426757812,121.12693023681641,119.76126861572266,118.53388214111328,118.283203125]
[null,"Runcorn BS","Substation Rating","MVA","Non-Coincident",187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562]
[null,null,null,null,"Coincident",187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562,187.10000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",67.762771606445312,67.326118469238281,67.3018798828125,67.060798645019531,66.323410034179687,65.898971557617188,66.028427124023437]
[null,null,null,null,"Coincident",64.944053649902344,64.5006103515625,64.475105285644531,64.231216430664062,63.483135223388672,63.05743408203125,63.206703186035156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.879936218261719,67.435081481933594,67.410392761230469,67.164901733398437,66.41448974609375,65.982887268066406,66.114501953125]
[null,null,null,null,"Coincident",64.977310180664063,64.527236938476562,64.501472473144531,64.254249572753906,63.497520446777344,63.067508697509766,63.217159271240234]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",64.030715942382813,63.700008392333984,63.514404296875,63.346004486083984,62.622993469238281,62.071510314941406,62.162487030029297]
[null,null,null,null,"Coincident",61.136028289794922,60.800655364990234,60.611164093017578,60.441307067871094,59.708354949951172,59.153472900390625,59.262420654296875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64.086166381835937,63.750961303710937,63.562908172607422,63.392330169677734,62.660480499267578,62.102825164794922,62.194786071777344]
[null,null,null,null,"Coincident",61.138011932373047,60.801490783691406,60.611598968505859,60.441471099853516,59.827709197998047,59.256317138671875,59.365402221679688]
[null,"Sandgate BS","Substation Rating","MVA","Non-Coincident",191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437]
[null,null,null,null,"Coincident",191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437,191.39999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",86.951446533203125,86.2398681640625,86.050956726074219,85.701812744140625,84.882850646972656,84.575225830078125,85.292381286621094]
[null,null,null,null,"Coincident",81.007667541503906,80.327293395996094,80.159072875976563,79.831169128417969,79.052597045898438,78.744552612304688,79.438613891601562]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",86.980819702148438,86.264503479003906,86.07440185546875,85.723129272460938,84.8995361328125,84.590309143066406,85.311317443847656]
[null,null,null,null,"Coincident",81.261192321777344,80.58221435546875,80.414413452148438,80.087211608886719,79.310287475585938,79.002838134765625,79.695472717285156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",78.401611328125,77.863502502441406,77.480125427246094,77.243453979492187,76.465522766113281,75.987442016601562,76.6104736328125]
[null,null,null,null,"Coincident",73.136138916015625,72.618499755859375,72.267807006835938,72.044586181640625,71.304885864257813,70.83984375,71.444541931152344]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",81.396034240722656,80.837379455566406,80.439353942871094,80.193641662597656,79.386001586914063,78.889663696289062,79.536491394042969]
[null,null,null,null,"Coincident",73.40875244140625,72.892417907714844,72.542716979980469,72.320083618164062,71.58233642578125,71.118492126464844,71.721633911132813]
[null,"Stafford BS","Substation Rating","MVA","Non-Coincident",262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875]
[null,null,null,null,"Coincident",262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875,262.29998779296875]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",183.80244445800781,182.87168884277344,182.93003845214844,164.02899169921875,163.16386413574219,162.63768005371094,162.82479858398437]
[null,null,null,null,"Coincident",167.15399169921875,166.2364501953125,166.29478454589844,148.70291137695312,147.83744812011719,147.31144714355469,147.49696350097656]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",185.03361511230469,184.07110595703125,184.13143920898437,164.64971923828125,163.7613525390625,163.22119140625,163.41326904296875]
[null,null,null,null,"Coincident",167.43678283691406,166.50308227539062,166.56217956542969,148.87791442871094,148.0010986328125,147.46833801269531,147.65487670898437]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",166.98612976074219,166.3409423828125,166.00704956054687,149.3787841796875,148.54925537109375,147.77407836914062,147.895751953125]
[null,null,null,null,"Coincident",151.009033203125,150.37400817871094,150.04414367675781,134.57534790039063,133.74600219726562,132.971923828125,133.09249877929687]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",167.68873596191406,167.02537536621094,166.68214416503906,149.65437316894531,148.80870056152344,148.01878356933594,148.14274597167969]
[null,null,null,null,"Coincident",151.17970275878906,150.84933471679687,151.03305053710937,135.19564819335937,134.3463134765625,133.55299377441406,133.67378234863281]
[null,"Stradbroke Is BS","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",72,72,72,72,72,72,72]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.9072914123535156,5.9288034439086914,5.9659252166748047,6.0013036727905273,5.9989991188049316,6.0227932929992676,6.0697450637817383]
[null,null,null,null,"Coincident",2.9877095222473145,2.9985895156860352,3.0173649787902832,3.0352580547332764,3.0340919494628906,3.0461268424987793,3.0698730945587158]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5651297569274902,6.5890374183654785,6.6302933692932129,6.6696114540100098,6.6670503616333008,6.6934943199157715,6.7456746101379395]
[null,null,null,null,"Coincident",3.1283078193664551,3.1396996974945068,3.1593587398529053,3.1780939102172852,3.1768729686737061,3.1894741058349609,3.2143378257751465]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5007205009460449,5.5282788276672363,5.547480583190918,5.5860023498535156,5.5811724662780762,5.5888524055480957,5.6305761337280273]
[null,null,null,null,"Coincident",2.7820794582366943,2.7960176467895508,2.8057296276092529,2.8252122402191162,2.8227696418762207,2.8266541957855225,2.8477566242218018]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.1132831573486328,6.1439104080200195,6.165250301361084,6.2080621719360352,6.2026944160461426,6.2112293243408203,6.2575993537902832]
[null,null,null,null,"Coincident",2.9130010604858398,2.9275951385498047,2.9377641677856445,2.9581637382507324,2.9556059837341309,2.9596734046936035,2.9817688465118408]
[null,"Sunrise Hills BS","Substation Rating","MVA","Non-Coincident",143,143,143,143,143,143,143]
[null,null,null,null,"Coincident",143,143,143,143,143,143,143]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",82.572746276855469,82.293624877929688,82.413948059082031,82.192832946777344,81.416374206542969,81.275489807128906,81.762733459472656]
[null,null,null,null,"Coincident",77.358665466308594,77.089691162109375,77.197372436523438,76.988029479980469,76.256599426269531,76.129997253417969,76.597900390625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",86.737754821777344,86.444557189941406,86.570945739746094,86.338676452636719,85.523056030273437,85.37506103515625,85.886886596679688]
[null,null,null,null,"Coincident",78.060287475585937,77.783760070800781,77.894317626953125,77.681777954101563,76.937171936035156,76.810539245605469,77.290626525878906]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",74.188545227050781,74.03814697265625,73.94293212890625,73.819557189941406,73.0880126953125,72.772544860839844,73.183738708496094]
[null,null,null,null,"Coincident",69.424034118652344,69.276542663574219,69.182830810546875,69.065361022949219,68.377151489257813,68.086814880371094,68.481880187988281]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",77.930648803710937,77.772666931152344,77.672645568847656,77.543052673339844,76.774604797363281,76.443229675292969,76.875160217285156]
[null,null,null,null,"Coincident",70.873687744140625,70.719680786132813,70.625236511230469,70.506195068359375,69.803977966308594,69.510658264160156,69.918746948242187]
[null,"Tennyson BS","Substation Rating","MVA","Non-Coincident",257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875]
[null,null,null,null,"Coincident",257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875,257.79998779296875]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",190.10482788085937,192.24028015136719,205.793701171875,204.40863037109375,193.48660278320312,196.04350280761719,198.10379028320312]
[null,null,null,null,"Coincident",185.52543640136719,187.74620056152344,201.12028503417969,200.24374389648437,189.05197143554687,191.58384704589844,193.67044067382812]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",190.79733276367187,192.98719787597656,206.91819763183594,205.49217224121094,194.26597595214844,196.89094543457031,199.00752258300781]
[null,null,null,null,"Coincident",186.12591552734375,188.51077270507812,201.14346313476562,200.26359558105469,190.05293273925781,192.27447509765625,194.46798706054687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",172.44779968261719,174.90911865234375,188.05560302734375,186.9339599609375,176.20005798339844,178.44314575195312,180.35821533203125]
[null,null,null,null,"Coincident",168.20137023925781,170.74070739746094,183.71469116210937,183.0999755859375,172.09005737304687,174.31410217285156,176.25946044921875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",172.75360107421875,175.26136779785156,188.69729614257812,187.5484619140625,176.57771301269531,178.86659240722656,180.82235717773437]
[null,null,null,null,"Coincident",168.54649353027344,171.73873901367187,183.76907348632812,183.15057373046875,173.37205505371094,175.21977233886719,177.28811645507812]
[null,"Victoria Park BS","Substation Rating","MVA","Non-Coincident",251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438]
[null,null,null,null,"Coincident",251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438,251.39999389648438]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.822715759277344,73.680671691894531,77.949684143066406,78.860153198242188,79.066978454589844,80.937583923339844,83.118171691894531]
[null,null,null,null,"Coincident",49.947154998779297,53.700412750244141,57.854461669921875,58.673816680908203,58.831672668457031,60.608234405517578,62.677520751953125]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",71.878448486328125,75.849990844726563,80.24468994140625,81.181968688964844,81.394882202148438,83.320556640625,83.1187744140625]
[null,null,null,null,"Coincident",50.469451904296875,54.546161651611328,59.082199096679688,59.930164337158203,60.097705841064453,62.062671661376953,64.336128234863281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",65.625442504882813,69.578353881835938,73.688697814941406,74.599235534667969,74.801689147949219,76.583717346191406,78.754501342773438]
[null,null,null,null,"Coincident",46.066333770751953,49.909030914306641,53.916217803955078,54.734535217285156,54.890605926513672,56.589565277099609,58.651966094970703]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.557594299316406,71.62689208984375,75.858253479003906,76.79559326171875,77.004013061523438,78.838508605957031,81.073204040527344]
[null,null,null,null,"Coincident",46.502529144287109,50.662010192871094,55.042655944824219,55.889629364013672,56.054962158203125,57.938529968261719,60.204322814941406]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Acacia Ridge","Substation Rating","MVA","Non-Coincident",41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906]
[null,null,null,null,"Coincident",41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906,41.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.227575302124023,17.073513031005859,17.071342468261719,16.990886688232422,16.768312454223633,16.59950065612793,16.490589141845703]
[null,null,null,null,"Coincident",15.346343040466309,15.209103584289551,15.207170486450195,15.135499954223633,14.937231063842773,14.786852836608887,14.689833641052246]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.229619979858398,17.074396133422852,17.072212219238281,16.991342544555664,17.49553108215332,17.305103302001953,17.182317733764648]
[null,null,null,null,"Coincident",15.406872749328613,15.265196800231934,15.263202667236328,15.189269065856934,14.984930992126465,14.830144882202148,14.730372428894043]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.611862182617188,16.485752105712891,16.43798828125,16.377006530761719,16.154705047607422,15.950807571411133,15.840963363647461]
[null,null,null,null,"Coincident",14.79786491394043,14.685524940490723,14.642977714538574,14.588654518127441,14.390627861022949,14.208996772766113,14.111146926879883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.319042205810547,17.17686653137207,17.123037338256836,17.054330825805664,16.804023742675781,16.574668884277344,16.451204299926758]
[null,null,null,null,"Coincident",14.840511322021484,14.725020408630371,14.681305885314941,14.625513076782227,14.422328948974609,14.236255645751953,14.136129379272461]
[null,"Albany Creek","Substation Rating","MVA","Non-Coincident",59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547]
[null,null,null,null,"Coincident",59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.329704284667969,30.994739532470703,31.163129806518555,31.185504913330078,30.862390518188477,30.662467956542969,30.582820892333984]
[null,null,null,null,"Coincident",29.322593688964844,29.009088516235352,29.166690826416016,29.187631607055664,28.885217666625977,28.698102951049805,28.623558044433594]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.84490966796875,32.493743896484375,32.670276641845703,32.693737030029297,32.354991912841797,32.145401000976563,32.061904907226563]
[null,null,null,null,"Coincident",29.619499206542969,29.302820205688477,29.462017059326172,29.483169555664063,29.177694320678711,28.988685607910156,28.913385391235352]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.504281997680664,25.266002655029297,25.332889556884766,25.376626968383789,25.101627349853516,24.874675750732422,24.801937103271484]
[null,null,null,null,"Coincident",23.870372772216797,23.647357940673828,23.709959030151367,23.750894546508789,23.493513107299805,23.281101226806641,23.213022232055664]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.737751007080078,26.487947463989258,26.558069229125977,26.603919982910156,26.315622329711914,26.077693939208984,26.001438140869141]
[null,null,null,null,"Coincident",24.112071990966797,23.886798858642578,23.950033187866211,23.991384506225586,23.731395721435547,23.516834259033203,23.448064804077148]
[null,"Alexandra Headland","Substation Rating","MVA","Non-Coincident",130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219]
[null,null,null,null,"Coincident",130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219,130.19999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",82.765472412109375,82.500007629394531,82.645759582519531,85.010948181152344,84.055183410644531,85.909690856933594,86.123908996582031]
[null,null,null,null,"Coincident",82.765472412109375,82.500007629394531,82.645759582519531,85.010948181152344,84.055183410644531,85.909690856933594,86.123908996582031]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",86.806983947753906,86.518112182617188,86.676712036132812,89.250900268554688,88.210563659667969,90.22930908203125,90.462539672851563]
[null,null,null,null,"Coincident",83.740646362304688,83.467086791992188,83.617378234863281,86.122482299804688,85.134735107421875,87.11468505859375,87.334663391113281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",75.640159606933594,75.502021789550781,75.425491333007813,78.018882751464844,77.103958129882813,78.938919067382813,79.100875854492188]
[null,null,null,null,"Coincident",75.640159606933594,75.502021789550781,75.425491333007813,78.018882751464844,77.103958129882813,78.938919067382813,79.100875854492188]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",79.058303833007812,78.908187866210937,78.825027465820313,81.643951416015625,80.6492919921875,82.644363403320313,82.820480346679688]
[null,null,null,null,"Coincident",76.4044189453125,76.26239013671875,76.183479309082031,78.919349670410156,77.974769592285156,79.931411743164063,80.097213745117187]
[null,"Algester","Substation Rating","MVA","Non-Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,null,null,"Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.921905517578125,19.685394287109375,19.677234649658203,19.578752517700195,19.316497802734375,19.116193771362305,18.98486328125]
[null,null,null,null,"Coincident",18.129615783691406,17.91438102722168,17.906955718994141,17.817333221435547,17.578672409057617,17.396389007568359,17.276874542236328]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.131143569946289,19.882230758666992,19.873647689819336,19.770076751708984,19.494483947753906,19.284208297729492,19.146444320678711]
[null,null,null,null,"Coincident",18.754928588867188,18.532270431518555,18.524589538574219,18.431875228881836,18.184982299804687,17.99641227722168,17.872776031494141]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.725034713745117,18.527959823608398,18.468967437744141,18.395055770874023,18.139930725097656,17.905511856079102,17.776676177978516]
[null,null,null,null,"Coincident",17.040422439575195,16.861076354980469,16.807392120361328,16.740129470825195,16.507957458496094,16.294628143310547,16.177383422851563]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.874141693115234,18.66783332824707,18.606119155883789,18.528820037841797,18.262237548828125,18.017618179321289,17.883312225341797]
[null,null,null,null,"Coincident",17.628168106079102,17.442634582519531,17.387100219726563,17.317516326904297,17.077337265014648,16.856649398803711,16.735361099243164]
[null,"Amamoor","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.1265401840209961,4.1345853805541992,4.143702507019043,4.1372909545898437,4.1041431427001953,4.0937066078186035,4.0986475944519043]
[null,null,null,null,"Coincident",3.9784083366394043,3.9861648082733154,3.9949550628662109,3.9887735843658447,3.9568157196044922,3.9467544555664062,3.9515175819396973]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.6067013740539551,4.6156826019287109,4.6258606910705566,4.6187028884887695,4.581697940826416,4.5700473785400391,4.5755634307861328]
[null,null,null,null,"Coincident",4.4204154014587402,4.4290337562561035,4.4388003349304199,4.4319319725036621,4.3964238166809082,4.3852443695068359,4.3905367851257324]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8387024402618408,3.8514304161071777,3.8492295742034912,3.8471469879150391,3.8144891262054443,3.7949728965759277,3.7983088493347168]
[null,null,null,null,"Coincident",3.7009031772613525,3.7131743431091309,3.7110526561737061,3.7090449333190918,3.6775596141815186,3.6587438583374023,3.6619598865509033]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.2853708267211914,4.2995800971984863,4.2971229553222656,4.2947983741760254,4.2583398818969727,4.2365531921386719,4.2402768135070801]
[null,null,null,null,"Coincident",4.1120791435241699,4.1257133483886719,4.1233558654785156,4.1211252212524414,4.0861415863037109,4.0652356147766113,4.0688090324401855]
[null,"Amberley","Substation Rating","MVA","Non-Coincident",26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547]
[null,null,null,null,"Coincident",26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","WINTER","WINTER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0255517959594727,3.8637714385986328,4.8373861312866211,7.0847721099853516,8.6212034225463867,9.5953216552734375,10.381122589111328]
[null,null,null,null,"Coincident",3.736997127532959,3.7403109073638916,4.7922391891479492,6.8634481430053711,8.4345760345458984,9.3876066207885742,10.156396865844727]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.4017224311828613,4.2037687301635742,5.2630581855773926,7.7468142509460449,9.4988889694213867,10.572177886962891,11.437976837158203]
[null,null,null,null,"Coincident",4.0752959251403809,4.0789093971252441,5.2965779304504395,7.7028465270996094,9.5333051681518555,10.644349098205566,11.540189743041992]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.5309958457946777,3.7613861560821533,4.7386131286621094,6.7452902793884277,8.3989009857177734,9.4023332595825195,10.224431991577148]
[null,null,null,null,"Coincident",3.2778911590576172,3.2852706909179687,4.3797574043273926,6.562901496887207,8.2170858383178711,9.198796272277832,10.003098487854004]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8609523773193359,4.0923738479614258,5.1555933952331543,7.3756089210510254,9.2539548873901367,10.359542846679687,11.265334129333496]
[null,null,null,null,"Coincident",3.5746283531188965,3.5826759338378906,4.8506312370300293,7.3876442909240723,9.315129280090332,10.460274696350098,11.397640228271484]
[null,"Ann St","Substation Rating","MVA","Non-Coincident",188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562]
[null,null,null,null,"Coincident",188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562,188.10000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.979965209960938,46.229072570800781,47.517814636230469,49.932037353515625,50.861392974853516,51.920864105224609,53.145473480224609]
[null,null,null,null,"Coincident",40.677589416503906,40.897972106933594,42.038097381591797,44.173912048339844,44.99609375,45.933387756347656,47.016777038574219]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.001621246337891,46.254119873046875,47.563934326171875,50.032295227050781,50.987113952636719,51.921459197998047,53.151378631591797]
[null,null,null,null,"Coincident",40.750370025634766,40.973628997802734,42.141597747802734,44.325183868408203,44.996131896972656,45.934272766113281,47.020000457763672]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.134494781494141,45.440895080566406,46.650901794433594,49.138969421386719,50.025051116943359,50.931072235107422,52.111148834228516]
[null,null,null,null,"Coincident",39.929618835449219,40.20068359375,41.271156311035156,43.472301483154297,44.256198883056641,45.0577392578125,46.101730346679688]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.146385192871094,45.456008911132813,46.682205200195313,49.219463348388672,50.12774658203125,51.058799743652344,52.112213134765625]
[null,null,null,null,"Coincident",39.992958068847656,40.267387390136719,41.364116668701172,43.613307952880859,44.409999847412109,45.057823181152344,46.102996826171875]
[null,"Annerley","Substation Rating","MVA","Non-Coincident",59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453]
[null,null,null,null,"Coincident",59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.866867065429688,16.892812728881836,16.924100875854492,16.873960494995117,16.761892318725586,16.801132202148438,16.869325637817383]
[null,null,null,null,"Coincident",15.110133171081543,15.133376121520996,15.161405563354492,15.116488456726074,15.016093254089355,15.05124568939209,15.112336158752441]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.035411834716797,18.063152313232422,18.096609115600586,18.042993545532227,17.923164367675781,17.965122222900391,18.038040161132812]
[null,null,null,null,"Coincident",15.380373954772949,15.404032707214355,15.432563781738281,15.386842727661133,15.284652709960938,15.320433616638184,15.382616996765137]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.398680686950684,15.443392753601074,15.429132461547852,15.39892578125,15.289301872253418,15.285553932189941,15.342568397521973]
[null,null,null,null,"Coincident",13.794863700866699,13.834919929504395,13.822144508361816,13.795083999633789,13.696877479553223,13.69351863861084,13.744595527648926]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.465507507324219,16.513317108154297,16.498069763183594,16.465768814086914,16.348550796508789,16.34454345703125,16.405508041381836]
[null,null,null,null,"Coincident",14.041581153869629,14.082354545593262,14.069350242614746,14.041805267333984,13.941843032836914,13.938424110412598,13.990414619445801]
[null,"Arana Hills","Substation Rating","MVA","Non-Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,null,null,"Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.375869750976562,34.30047607421875,34.228050231933594,34.133384704589844,33.800071716308594,33.640846252441406,33.822853088378906]
[null,null,null,null,"Coincident",30.637849807739258,30.570650100708008,30.506103515625,30.421726226806641,30.124658584594727,29.982746124267578,30.144960403442383]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.569290161132812,34.492225646972656,34.418193817138672,34.321437835693359,33.980819702148438,33.818130493164063,34.004096984863281]
[null,null,null,null,"Coincident",30.963899612426758,30.895984649658203,30.830751419067383,30.745475769042969,30.445245742797852,30.301824569702148,30.465764999389648]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.972436904907227,30.946638107299805,30.795742034912109,30.741518020629883,30.426692962646484,30.205224990844727,30.358699798583984]
[null,null,null,null,"Coincident",27.604503631591797,27.581510543823242,27.447021484375,27.398693084716797,27.11810302734375,26.920717239379883,27.057502746582031]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.094776153564453,31.068477630615234,30.914669036865234,30.859403610229492,30.538591384887695,30.312973022460937,30.469318389892578]
[null,null,null,null,"Coincident",27.898271560668945,27.875034332275391,27.739114761352539,27.690271377563477,27.406694412231445,27.207208633422852,27.345449447631836]
[null,"Archerfield","Substation Rating","MVA","Non-Coincident",54.299999237060547,54.299999237060547,54.299999237060547,54.299999237060547,54.299999237060547,54.299999237060547,54.299999237060547]
[null,null,null,null,"Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.736377716064453,20.720991134643555,20.735620498657227,20.655036926269531,20.401908874511719,20.214078903198242,20.098104476928711]
[null,null,null,null,"Coincident",12.375995635986328,12.366812705993652,12.375544548034668,12.327449798583984,12.176376342773438,12.064274787902832,11.995059013366699]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.767528533935547,20.751680374145508,20.766748428344727,20.683788299560547,20.423759460449219,20.231374740600586,20.112834930419922]
[null,null,null,null,"Coincident",13.107691764831543,13.097966194152832,13.107213973999023,13.056276321411133,12.896270751953125,12.777542114257813,12.70423412322998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.694757461547852,20.707597732543945,20.66480827331543,20.605245590209961,20.34294319152832,20.103652954101563,19.981765747070313]
[null,null,null,null,"Coincident",12.351156234741211,12.358819961547852,12.333281517028809,12.297733306884766,12.141183853149414,11.998370170593262,11.925624847412109]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.72467041015625,20.737890243530273,20.693843841552734,20.632572174072266,20.363311767578125,20.118501663208008,19.994115829467773]
[null,null,null,null,"Coincident",13.08138370513916,13.08950138092041,13.06245231628418,13.024802207946777,12.858997344970703,12.707740783691406,12.630694389343262]
[null,"Arundel","Substation Rating","MVA","Non-Coincident",53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453]
[null,null,null,null,"Coincident",53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453,53.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.887130737304688,24.670421600341797,24.667852401733398,24.55217170715332,24.231130599975586,23.987770080566406,23.900152206420898]
[null,null,null,null,"Coincident",24.707174301147461,24.492033004760742,24.489482879638672,24.374637603759766,24.055917739868164,23.81431770324707,23.727333068847656]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.265472412109375,25.037405014038086,25.034702301025391,24.912992477416992,24.575359344482422,24.319555282592773,24.227485656738281]
[null,null,null,null,"Coincident",24.717216491699219,24.50079345703125,24.498237609863281,24.382696151733398,24.062168121337891,23.819337844848633,23.731924057006836]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.762004852294922,23.589811325073242,23.522258758544922,23.43580436706543,23.118497848510742,22.827520370483398,22.736194610595703]
[null,null,null,null,"Coincident",23.590185165405273,23.41923713684082,23.3521728515625,23.266342163085937,22.951330184936523,22.662456512451172,22.571792602539063]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.082351684570312,23.901506423950195,23.830577850341797,23.739814758300781,23.406841278076172,23.101696014404297,23.005966186523438]
[null,null,null,null,"Coincident",23.59480094909668,23.423149108886719,23.355802536010742,23.269624710083008,22.953462600708008,22.663740158081055,22.572845458984375]
[null,"Ashgrove","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.066730499267578,26.021457672119141,25.979957580566406,25.732694625854492,25.451536178588867,25.493015289306641,25.510629653930664]
[null,null,null,null,"Coincident",24.510011672973633,24.467443466186523,24.428424835205078,24.195926666259766,23.931560516357422,23.970561981201172,23.987125396728516]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.447992324829102,26.400472640991211,26.356914520263672,26.097452163696289,25.802543640136719,25.846044540405273,25.86451530456543]
[null,null,null,null,"Coincident",24.553688049316406,24.511043548583984,24.471956253051758,24.239044189453125,23.974206924438477,24.013277053833008,24.029870986938477]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.941486358642578,22.932865142822266,22.832859039306641,22.638341903686523,22.380229949951172,22.358865737915039,22.366989135742188]
[null,null,null,null,"Coincident",21.5714111328125,21.563304901123047,21.469270706176758,21.286369323730469,21.043672561645508,21.023584365844727,21.031221389770508]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.176288604736328,23.167289733886719,23.062932968139648,22.860019683837891,22.590908050537109,22.568641662597656,22.577108383178711]
[null,null,null,null,"Coincident",21.609851837158203,21.601730346679688,21.507528305053711,21.324300765991211,21.081172943115234,21.06104850769043,21.068698883056641]
[null,"Astor Terrace","Substation Rating","MVA","Non-Coincident",52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453]
[null,null,null,null,"Coincident",52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.773517608642578,26.939277648925781,27.114326477050781,27.778036117553711,28.194864273071289,28.682346343994141,29.266408920288086]
[null,null,null,null,"Coincident",23.917043685913086,24.065118789672852,24.221490859985352,24.814390182495117,25.186746597290039,25.622219085693359,26.143966674804688]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.112016677856445,27.290485382080078,27.4791259765625,28.195905685424805,28.647245407104492,29.176183700561523,29.267692565917969]
[null,null,null,null,"Coincident",23.970205307006836,24.120859146118164,24.280002593994141,24.883853912353516,25.263431549072266,25.707668304443359,26.24034309387207]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.127721786499023,26.325325012207031,26.422977447509766,27.0970458984375,27.490434646606445,27.893585205078125,28.452262878417969]
[null,null,null,null,"Coincident",23.340147018432617,23.516668319702148,23.603902816772461,24.2060546875,24.557472229003906,24.917610168457031,25.416683197021484]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.418272018432617,26.630275726318359,26.735134124755859,27.460494995117188,27.885015487670898,28.320932388305664,28.9263916015625]
[null,null,null,null,"Coincident",23.383718490600586,23.563095092773438,23.651767730712891,24.264289855957031,24.622104644775391,24.989049911499023,25.497955322265625]
[null,"Bald Hills Bus 1","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.8711209297180176,7.7968859672546387,7.7240982055664062,7.6783227920532227,7.6313176155090332,7.6500277519226074,7.7268209457397461]
[null,null,null,null,"Coincident",6.3781671524047852,6.3180127143859863,6.2590303421020508,6.2219376564025879,6.1838479042053223,6.1990089416503906,6.2612366676330566]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.0976066589355469,8.021235466003418,7.9463539123535156,7.8992609977722168,7.8509030342102051,7.8701515197753906,7.9491548538208008]
[null,null,null,null,"Coincident",6.3892936706542969,6.3290343284606934,6.2699489593505859,6.2327919006347656,6.1946353912353516,6.2098231315612793,6.2721595764160156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.7922477722167969,6.7373614311218262,6.6559734344482422,6.6231961250305176,6.5794854164123535,6.5785999298095703,6.6424612998962402]
[null,null,null,null,"Coincident",5.5039291381835938,5.4594531059265137,5.3935022354125977,5.3669419288635254,5.3315224647521973,5.3308043479919434,5.3825535774230957]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.9876894950866699,6.9312243461608887,6.8474941253662109,6.8137741088867188,6.7688055038452148,6.7678942680358887,6.8335933685302734]
[null,null,null,null,"Coincident",5.5135307312011719,5.4689769744873047,5.4029111862182617,5.3763046264648437,5.3408231735229492,5.3401041030883789,5.3919434547424316]
[null,"Bald Hills Bus 2","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.5739212036132812,9.5253238677978516,9.5397109985351562,9.5208559036254883,9.4343156814575195,9.3885316848754883,9.3808040618896484]
[null,null,null,null,"Coincident",9.3689289093017578,9.3213720321655273,9.3354511260986328,9.3170003890991211,9.2323131561279297,9.1875095367431641,9.1799468994140625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.079401969909668,10.028238296508789,10.04338550567627,10.023534774780273,9.9324254989624023,9.8842239379882812,9.8760881423950195]
[null,null,null,null,"Coincident",9.6330184936523437,9.5841207504272461,9.5985965728759766,9.5796260833740234,9.4925518035888672,9.4464855194091797,9.4387092590332031]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4187459945678711,8.3874320983886719,8.3768272399902344,8.3686971664428711,8.2886438369750977,8.227137565612793,8.2176733016967773]
[null,null,null,null,"Coincident",8.2384872436523437,8.2078437805175781,8.1974668502807617,8.1895103454589844,8.111170768737793,8.0509815216064453,8.0417203903198242]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8632354736328125,8.8302688598632812,8.8191041946411133,8.8105449676513672,8.7262649536132812,8.6615104675292969,8.6515474319458008]
[null,null,null,null,"Coincident",8.4707117080688477,8.4392051696777344,8.4285354614257813,8.4203548431396484,8.3398065567016602,8.2779207229614258,8.2683992385864258]
[null,"Beaudesert","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.719181060791016,19.700538635253906,19.818870544433594,19.867315292358398,19.893972396850586,20.004858016967773,20.090179443359375]
[null,null,null,null,"Coincident",19.719181060791016,19.700538635253906,19.818870544433594,19.867315292358398,19.893972396850586,20.004858016967773,20.090179443359375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.883886337280273,21.863199234008789,21.994522094726562,22.048284530639648,22.07786750793457,22.200925827026367,22.295614242553711]
[null,null,null,null,"Coincident",20.610929489135742,20.59144401550293,20.715127944946289,20.765762329101563,20.79362678527832,20.909526824951172,20.99870491027832]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.63929557800293,17.646644592285156,17.703454971313477,17.764616012573242,17.779903411865234,17.832874298095703,17.903066635131836]
[null,null,null,null,"Coincident",17.63929557800293,17.646644592285156,17.703454971313477,17.764616012573242,17.779903411865234,17.832874298095703,17.903066635131836]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.575679779052734,19.583835601806641,19.646883010864258,19.714756011962891,19.731723785400391,19.790508270263672,19.868406295776367]
[null,null,null,null,"Coincident",18.436986923217773,18.444667816162109,18.504047393798828,18.567974090576172,18.583953857421875,18.639320373535156,18.712686538696289]
[null,"Beenleigh","Substation Rating","MVA","Non-Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,null,null,"Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.352375030517578,31.970279693603516,31.957221984863281,31.797475814819336,31.37175178527832,31.343866348266602,31.654148101806641]
[null,null,null,null,"Coincident",30.823732376098633,30.459690093994141,30.447250366210937,30.295051574707031,29.889442443847656,29.862874984741211,30.158496856689453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.619808197021484,32.218502044677734,32.204795837402344,32.037178039550781,31.590913772583008,31.56170654296875,31.886861801147461]
[null,null,null,null,"Coincident",30.937515258789063,30.566730499267578,30.554061889648437,30.399085998535156,29.986194610595703,29.959156036376953,30.260059356689453]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.75529670715332,28.454423904418945,28.364002227783203,28.250663757324219,27.859027862548828,27.762447357177734,28.028093338012695]
[null,null,null,null,"Coincident",27.396614074707031,27.109958648681641,27.023809432983398,26.915824890136719,26.542694091796875,26.450677871704102,26.703771591186523]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.864128112792969,28.552534103393555,28.458978652954102,28.341770172119141,27.937274932861328,27.837648391723633,28.111793518066406]
[null,null,null,null,"Coincident",27.452817916870117,27.162019729614258,27.074647903442383,26.965147018432617,26.586912155151367,26.493669509887695,26.750167846679688]
[null,"Beenleigh North","Substation Rating","MVA","Non-Coincident",54.5,54.5,54.5,54.5,54.5,54.5,54.5]
[null,null,null,null,"Coincident",54.5,54.5,54.5,54.5,54.5,54.5,54.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.359241485595703,16.215921401977539,16.214149475097656,16.138029098510742,15.926922798156738,16.040105819702148,16.341279983520508]
[null,null,null,null,"Coincident",16.2535400390625,16.111146926879883,16.109386444091797,16.033756256103516,15.824014663696289,15.936466217041016,16.235694885253906]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.398792266845703,16.251911163330078,16.250095367431641,16.172140121459961,15.956157684326172,16.071916580200195,16.380376815795898]
[null,null,null,null,"Coincident",16.472047805786133,16.327739715576172,16.325956344604492,16.249309539794922,16.036746978759766,16.150711059570313,16.453962326049805]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.479741096496582,15.365046501159668,15.320802688598633,15.264243125915527,15.05732536315918,15.125203132629395,15.404153823852539]
[null,null,null,null,"Coincident",15.379722595214844,15.265769004821777,15.221811294555664,15.165616989135742,14.960036277770996,15.027475357055664,15.304623603820801]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.499720573425293,15.382899284362793,15.337862968444824,15.280313491821289,15.069998741149902,15.138951301574707,15.422719955444336]
[null,null,null,null,"Coincident",15.586483001708984,15.470996856689453,15.426448822021484,15.369499206542969,15.161154747009277,15.229499816894531,15.510374069213867]
[null,"Beerwah","Substation Rating","MVA","Non-Coincident",57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453]
[null,null,null,null,"Coincident",57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453,57.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.003473281860352,16.824081420898437,16.819293975830078,16.831329345703125,16.913799285888672,17.012290954589844,17.112646102905273]
[null,null,null,null,"Coincident",17.003473281860352,16.824081420898437,16.819293975830078,16.831329345703125,16.913799285888672,17.012290954589844,17.112646102905273]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.068164825439453,16.883230209350586,16.878297805786133,16.890697479248047,16.975696563720703,17.077259063720703,17.180803298950195]
[null,null,null,null,"Coincident",17.480140686035156,17.295721054077148,17.290798187255859,17.303171157836914,17.387954711914063,17.489206314086914,17.592374801635742]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.815664291381836,14.679341316223145,14.634506225585938,14.65973949432373,14.724488258361816,14.772019386291504,14.854293823242188]
[null,null,null,null,"Coincident",14.815664291381836,14.679341316223145,14.634506225585938,14.65973949432373,14.724488258361816,14.772019386291504,14.854293823242188]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.827760696411133,14.689403533935547,14.643936157226562,14.669523239135742,14.735204696655273,14.783445358276367,14.866996765136719]
[null,null,null,null,"Coincident",15.231000900268555,15.090855598449707,15.044763565063477,15.070704460144043,15.13726806640625,15.186132431030273,15.270712852478027]
[null,"Belmont","Substation Rating","MVA","Non-Coincident",37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906]
[null,null,null,null,"Coincident",37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906,37.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.895389556884766,18.864801406860352,18.827449798583984,18.749155044555664,18.522977828979492,18.385660171508789,18.457937240600586]
[null,null,null,null,"Coincident",18.29290771484375,18.263294219970703,18.227130889892578,18.151332855224609,17.932367324829102,17.799427032470703,17.86939811706543]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.05824089050293,19.026250839233398,18.987194061279297,18.905340194702148,18.669034957885742,18.525678634643555,18.601123809814453]
[null,null,null,null,"Coincident",18.730033874511719,18.699712753295898,18.662685394287109,18.585075378417969,18.360877990722656,18.224761962890625,18.296403884887695]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.825784683227539,16.821449279785156,16.741628646850586,16.688814163208008,16.479562759399414,16.315191268920898,16.373964309692383]
[null,null,null,null,"Coincident",16.289289474487305,16.285091400146484,16.207817077636719,16.156684875488281,15.954108238220215,15.794976234436035,15.851875305175781]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.903818130493164,16.899330139160156,16.816701889038086,16.762050628662109,16.545696258544922,16.375942230224609,16.436618804931641]
[null,null,null,null,"Coincident",16.678537368774414,16.674240112304687,16.595117568969727,16.542764663696289,16.335346221923828,16.172412872314453,16.230670928955078]
[null,"Bethania","Substation Rating","MVA","Non-Coincident",47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547]
[null,null,null,null,"Coincident",47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.400081634521484,21.707281112670898,22.022197723388672,22.27631950378418,22.375154495239258,22.599018096923828,22.967067718505859]
[null,null,null,null,"Coincident",21.193450927734375,21.497684478759766,21.809560775756836,22.061227798461914,22.159109115600586,22.38081169128418,22.745307922363281]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.408388137817383,21.718006134033203,22.035678863525391,22.292221069335938,22.392044067382812,22.618240356445313,22.990394592285156]
[null,null,null,null,"Coincident",21.407186508178711,21.714488983154297,22.029510498046875,22.283716201782227,22.382583618164063,22.606523513793945,22.974695205688477]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.826255798339844,19.122543334960938,19.346216201782227,19.589181900024414,19.666635513305664,19.812152862548828,20.12822151184082]
[null,null,null,null,"Coincident",18.644475936889648,18.937904357910156,19.159414291381836,19.400033950805664,19.476741790771484,19.620851516723633,19.933868408203125]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.551347732543945,19.859045028686523,19.346227645874023,19.589384078979492,19.666946411132813,19.81273078918457,20.12965202331543]
[null,null,null,null,"Coincident",18.83250617980957,19.12889289855957,19.352638244628906,19.595684051513672,19.673164367675781,19.818727493286133,20.134902954101562]
[null,"Birkdale","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.267616271972656,34.184726715087891,34.097885131835938,33.981826782226563,33.608394622802734,33.416664123535156,33.661483764648438]
[null,null,null,null,"Coincident",26.758844375610352,26.694120407104492,26.626306533813477,26.535678863525391,26.244071960449219,26.094358444213867,26.285528182983398]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.390384674072266,34.306179046630859,34.217964172363281,34.100074768066406,33.720817565917969,33.526130676269531,33.774726867675781]
[null,null,null,null,"Coincident",27.012111663818359,26.946775436401367,26.878318786621094,26.786832809448242,26.492465972900391,26.341335296630859,26.53431510925293]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.610069274902344,30.577663421630859,30.415481567382813,30.342508316040039,29.994644165039063,29.746583938598633,29.954700469970703]
[null,null,null,null,"Coincident",23.902748107910156,23.877443313598633,23.750799179077148,23.693815231323242,23.422174453735352,23.228469848632813,23.390981674194336]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.679288864135742,30.646455764770508,30.482143402099609,30.408220291137695,30.055891036987305,29.804714202880859,30.01544189453125]
[null,null,null,null,"Coincident",24.128982543945313,24.103439331054688,23.975595474243164,23.918071746826172,23.64385986328125,23.448322296142578,23.612373352050781]
[null,"Birtinya","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.664011001586914,22.276393890380859,22.926177978515625,25.770938873291016,28.373197555541992,28.787281036376953,29.318181991577148]
[null,null,null,null,"Coincident",21.02470588684082,21.619020462036133,22.249626159667969,25.050296783447266,27.614652633666992,28.015804290771484,28.530603408813477]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.668615341186523,22.281129837036133,22.931051254272461,25.776418685913086,28.379228591918945,28.793399810791016,29.32441520690918]
[null,null,null,null,"Coincident",21.0257568359375,21.620101928710938,22.250738143920898,25.077169418334961,27.692447662353516,28.091583251953125,28.604679107666016]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.27155876159668,19.843332290649414,20.365564346313477,23.285739898681641,25.948301315307617,26.241823196411133,26.699708938598633]
[null,null,null,null,"Coincident",18.702854156494141,19.257755279541016,19.764577865600586,22.640466690063477,25.265289306640625,25.549186706542969,25.993082046508789]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.275655746459961,19.847551345825195,20.369894027709961,23.290689468383789,25.953817367553711,26.247402191162109,26.705385208129883]
[null,null,null,null,"Coincident",18.703788757324219,19.258718490600586,19.765565872192383,22.671346664428711,25.355884552001953,25.637189865112305,26.079057693481445]
[null,"Black Mountain","Substation Rating","MVA","Non-Coincident",17.899999618530273,17.899999618530273,17.899999618530273,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",17.899999618530273,17.899999618530273,17.899999618530273,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0692000389099121,5.0558843612670898,5.0416126251220703,5.0134963989257812,4.9508790969848633,4.9218811988830566,4.9358305931091309]
[null,null,null,null,"Coincident",4.8458871841430664,4.833158016204834,4.8195147514343262,4.7926373481750488,4.7327780723571777,4.7050576210021973,4.7183928489685059]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1050567626953125,5.0912752151489258,5.0765056610107422,5.0474162101745605,4.9826626777648926,4.9526910781860352,4.9671077728271484]
[null,null,null,null,"Coincident",4.8473987579345703,4.8346657752990723,4.8210182189941406,4.7941322326660156,4.7342543601989746,4.7065253257751465,4.7198648452758789]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.6465535163879395,4.6406660079956055,4.6147451400756836,4.593635082244873,4.534080982208252,4.4958944320678711,4.5071601867675781]
[null,null,null,null,"Coincident",4.441859245300293,4.4362311363220215,4.4114522933959961,4.3912720680236816,4.3343415260314941,4.2978367805480957,4.3086066246032715]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.6686406135559082,4.6625776290893555,4.635890007019043,4.6141629219055176,4.5529031753540039,4.5136513710021973,4.5252289772033691]
[null,null,null,null,"Coincident",4.4432449340820313,4.437614917755127,4.4128284454345703,4.3926420211791992,4.335693359375,4.2991776466369629,4.3099508285522461]
[null,"Boonah","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.0986337661743164,7.9887886047363281,7.9946045875549316,8.1123142242431641,8.1760578155517578,8.148371696472168,8.1542758941650391]
[null,null,null,null,"Coincident",7.9241981506347656,7.8167190551757812,7.8224101066589355,7.937584400177002,7.9999547004699707,7.972865104675293,7.978642463684082]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.199885368347168,8.0848779678344727,8.0909652709960937,8.2142143249511719,8.2809906005859375,8.2519845962524414,8.2581701278686523]
[null,null,null,null,"Coincident",8.0312175750732422,7.9222874641418457,7.9280552864074707,8.0447854995727539,8.1079978942871094,8.0805425643920898,8.0863971710205078]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.2538423538208008,7.1652112007141113,7.1505622863769531,7.263157844543457,7.316709041595459,7.2731189727783203,7.276005744934082]
[null,null,null,null,"Coincident",7.0976028442382812,7.0108809471130371,6.9965472221374512,7.106717586517334,7.1591153144836426,7.1164641380310059,7.1192889213562012]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3174667358398438,7.2251973152160645,7.2099533081054687,7.3271684646606445,7.3829536437988281,7.3375434875488281,7.340550422668457]
[null,null,null,null,"Coincident",7.1934590339660645,7.1055660247802734,7.091038703918457,7.2026968002319336,7.2558026313781738,7.2125754356384277,7.2154383659362793]
[null,"Booval","Substation Rating","MVA","Non-Coincident",37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453]
[null,null,null,null,"Coincident",37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453,37.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.117700576782227,30.013284683227539,30.054471969604492,29.983331680297852,29.690290451049805,29.517799377441406,29.563995361328125]
[null,null,null,null,"Coincident",29.764059066772461,29.660869598388672,29.701574325561523,29.631269454956055,29.341667175292969,29.17120361328125,29.21685791015625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.448463439941406,30.340154647827148,30.382875442504883,30.309085845947266,30.005189895629883,29.826351165771484,29.874244689941406]
[null,null,null,null,"Coincident",29.825529098510742,29.720930099487305,29.762189865112305,29.690929412841797,29.39744758605957,29.22474479675293,29.270994186401367]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.684640884399414,26.628381729125977,26.591047286987305,26.554841995239258,26.282669067382813,26.062557220458984,26.094797134399414]
[null,null,null,null,"Coincident",26.371309280395508,26.315711975097656,26.278818130493164,26.243038177490234,25.97406005859375,25.756532669067383,25.788394927978516]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.894111633300781,26.835994720458984,26.797430038452148,26.760034561157227,26.478975296020508,26.251760482788086,26.285036087036133]
[null,null,null,null,"Coincident",26.393423080444336,26.337314605712891,26.300085067749023,26.263982772827148,25.992637634277344,25.773284912109375,25.805410385131836]
[null,"Brendale","Substation Rating","MVA","Non-Coincident",58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547]
[null,null,null,null,"Coincident",58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547,58.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.360378265380859,42.673542022705078,43.150981903076172,43.685676574707031,43.911930084228516,44.33489990234375,44.841529846191406]
[null,null,null,null,"Coincident",39.493076324462891,39.785045623779297,40.230167388916016,40.728672027587891,40.939613342285156,41.333950042724609,41.806285858154297]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.361850738525391,42.675765991210938,43.154636383056641,43.691322326660156,43.918537139892578,44.343498229980469,44.852825164794922]
[null,null,null,null,"Coincident",39.534496307373047,39.828617095947266,40.277095794677734,40.779468536376953,40.992076873779297,41.389583587646484,41.865795135498047]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.91949462890625,37.243144989013672,37.555492401123047,38.059173583984375,38.237899780273438,38.506603240966797,38.933876037597656]
[null,null,null,null,"Coincident",34.432918548583984,34.734771728515625,35.026081085205078,35.495841979980469,35.662528991699219,35.913135528564453,36.311634063720703]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.171466827392578,37.502861022949219,37.822731018066406,38.338657379150391,38.521762847900391,38.797077178955078,39.234935760498047]
[null,null,null,null,"Coincident",34.44561767578125,34.7489013671875,35.041648864746094,35.513851165771484,35.681438446044922,35.933433532714844,36.334220886230469]
[null,"Bribie Island","Substation Rating","MVA","Non-Coincident",41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094]
[null,null,null,null,"Coincident",41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.946512222290039,21.810775756835938,22.332351684570313,22.452651977539063,22.352390289306641,22.346897125244141,22.455022811889648]
[null,null,null,null,"Coincident",18.472139358520508,18.357891082763672,18.796895980834961,18.898151397705078,18.813762664794922,18.809139251708984,18.900146484375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.981271743774414,21.843305587768555,22.373771667480469,22.496242523193359,22.394168853759766,22.388576507568359,22.4986572265625]
[null,null,null,null,"Coincident",18.789815902709961,18.673603057861328,19.120157241821289,19.223154067993164,19.137313842773437,19.132612228393555,19.225183486938477]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.625467300415039,19.530677795410156,19.942325592041016,20.06995964050293,19.970735549926758,19.914314270019531,20.004114151000977]
[null,null,null,null,"Coincident",16.51854133605957,16.438756942749023,16.785236358642578,16.892665863037109,16.809148788452148,16.761659622192383,16.837244033813477]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.631412506103516,19.535917282104492,19.950929641723633,20.07975959777832,19.979598999023437,19.922664642333984,20.013288497924805]
[null,null,null,null,"Coincident",16.802619934082031,16.721464157104492,17.073902130126953,17.18317985534668,17.098226547241211,17.049919128417969,17.126804351806641]
[null,"Brighton","Substation Rating","MVA","Non-Coincident",35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906]
[null,null,null,null,"Coincident",35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906,35.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.545233726501465,10.547792434692383,10.554041862487793,10.525314331054687,10.443120002746582,10.440183639526367,10.48328685760498]
[null,null,null,null,"Coincident",8.3943920135498047,8.396428108215332,8.401402473449707,8.3785343170166016,8.3131046295166016,8.3107681274414062,8.3450803756713867]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.287131309509277,11.28986930847168,11.29655933380127,11.265810012817383,11.177833557128906,11.174691200256348,11.220826148986816]
[null,null,null,null,"Coincident",8.4428234100341797,8.4448709487915039,8.4498739242553711,8.4268741607666016,8.3610668182373047,8.3587169647216797,8.3932275772094727]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3147716522216797,9.3297348022460937,9.3093996047973633,9.2934169769287109,9.2164106369018555,9.1900472640991211,9.2249679565429687]
[null,null,null,null,"Coincident",7.4148988723754883,7.4268097877502441,7.4106216430664063,7.3978991508483887,7.3365993499755859,7.31561279296875,7.3434109687805176]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.9701013565063477,9.9861173629760742,9.964350700378418,9.9472436904907227,9.8648204803466797,9.8366022109985352,9.8739805221557617]
[null,null,null,null,"Coincident",7.457679271697998,7.4696588516235352,7.4533772468566895,7.4405813217163086,7.3789277076721191,7.3578200340270996,7.3857789039611816]
[null,"Broadbeach","Substation Rating","MVA","Non-Coincident",118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219]
[null,null,null,null,"Coincident",118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219,118.19999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.898357391357422,54.823890686035156,54.857303619384766,54.639755249023438,53.965259552001953,53.584335327148438,53.935882568359375]
[null,null,null,null,"Coincident",53.288734436035156,53.216449737548828,53.248882293701172,53.037715911865234,52.38299560546875,52.013240814208984,52.354480743408203]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.943866729736328,54.868198394775391,54.902149200439453,54.68115234375,53.99676513671875,53.610805511474609,53.966987609863281]
[null,null,null,null,"Coincident",53.290885925292969,53.218471527099609,53.250961303710938,53.039440155029297,52.383819580078125,52.013698577880859,52.355274200439453]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",52.716632843017578,52.716899871826172,52.602890014648437,52.447086334228516,51.774761199951172,51.276653289794922,51.596160888671875]
[null,null,null,null,"Coincident",51.170978546142578,51.171237945556641,51.060569763183594,50.909336090087891,50.256721496582031,49.773220062255859,50.083358764648437]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.733165740966797,52.733436584472656,52.618282318115234,52.460979461669922,51.783027648925781,51.281654357910156,51.603164672851563]
[null,null,null,null,"Coincident",51.170989990234375,51.171249389648438,51.060569763183594,50.910739898681641,50.257320404052734,49.773433685302734,50.083797454833984]
[null,"Bromelton","Substation Rating","MVA","Non-Coincident",30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273]
[null,null,null,null,"Coincident",30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273,30.399999618530273]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7113094329833984,8.6530370712280273,9.3474836349487305,10.641410827636719,11.778982162475586,12.972868919372559,13.567126274108887]
[null,null,null,null,"Coincident",8.1506261825561523,8.096104621887207,8.745854377746582,9.9565010070800781,11.020854949951172,12.137900352478027,12.693909645080566]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7662677764892578,8.705510139465332,9.4320907592773437,10.648959159851074,11.813494682312012,13.051295280456543,13.672052383422852]
[null,null,null,null,"Coincident",8.1904067993164062,8.1346826553344727,8.8091697692871094,9.9590663909912109,11.055956840515137,12.137908935546875,12.696250915527344]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.3867855072021484,8.3420419692993164,9.0479612350463867,10.420388221740723,11.620169639587402,12.848467826843262,13.471388816833496]
[null,null,null,null,"Coincident",7.8469891548156738,7.8051257133483887,8.4656095504760742,9.7497034072875977,10.87226390838623,12.021505355834961,12.604333877563477]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.4284505844116211,8.3819828033447266,9.1180620193481445,10.424805641174316,11.649941444396973,12.921704292297363,13.571864128112793]
[null,null,null,null,"Coincident",7.8802218437194824,7.8374848365783691,8.5223302841186523,9.7515029907226562,10.907472610473633,12.021540641784668,12.607205390930176]
[null,"Browns Plains","Substation Rating","MVA","Non-Coincident",80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906]
[null,null,null,null,"Coincident",80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906,80.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.858371734619141,49.634063720703125,49.685890197753906,49.542087554931641,49.020393371582031,48.880012512207031,49.254974365234375]
[null,null,null,null,"Coincident",49.806953430175781,49.582881927490234,49.634654998779297,49.491001129150391,48.9698486328125,48.829612731933594,49.204189300537109]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.081878662109375,49.852005004882813,49.905113220214844,49.757759094238281,49.223346710205078,49.079586029052734,49.463611602783203]
[null,null,null,null,"Coincident",49.816089630126953,49.591518402099609,49.643405914306641,49.499435424804688,48.977176666259766,48.836654663085938,49.212005615234375]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.709049224853516,45.565448760986328,45.486652374267578,45.400714874267578,44.901042938232422,44.656936645507813,44.984767913818359]
[null,null,null,null,"Coincident",45.661911010742188,45.518459320068359,45.439746856689453,45.353897094726562,44.854736328125,44.610885620117187,44.938381195068359]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.837867736816406,45.691333770751953,45.610939025878906,45.523265838623047,45.013687133789063,44.764854431152344,45.099048614501953]
[null,null,null,null,"Coincident",45.663890838623047,45.520278930664063,45.441478729248047,45.355537414550781,44.855892181396484,44.611835479736328,44.939613342285156]
[null,"Bulimba","Substation Rating","MVA","Non-Coincident",58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547]
[null,null,null,null,"Coincident",58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547,58.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.891128540039063,27.921443939208984,27.956134796142578,27.931671142578125,27.911474227905273,32.330455780029297,36.736736297607422]
[null,null,null,null,"Coincident",25.278860092163086,25.306337356567383,25.337779998779297,25.315605163574219,25.297300338745117,29.401697158813477,33.493476867675781]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.165800094604492,28.197305679321289,28.233358383178711,28.20793342590332,28.186943054199219,32.33056640625,36.773021697998047]
[null,null,null,null,"Coincident",25.776390075683594,25.804407119750977,25.836469650268555,25.813858032226563,25.795192718505859,29.407072067260742,33.550300598144531]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.774900436401367,24.835643768310547,24.797611236572266,24.800880432128906,24.771034240722656,29.246988296508789,33.757591247558594]
[null,null,null,null,"Coincident",22.454496383666992,22.509550094604492,22.475078582763672,22.478042602539063,22.450992584228516,26.611764907836914,30.802719116210938]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.935846328735352,24.998622894287109,24.959316253662109,24.96269416809082,24.931850433349609,29.576189041137695,33.762676239013672]
[null,null,null,null,"Coincident",22.896438598632812,22.95257568359375,22.917425155639648,22.920448303222656,22.892866134643555,26.611785888671875,30.837778091430664]
[null,"Bundall","Substation Rating","MVA","Non-Coincident",30.5,30.5,30.5,30.5,30.5,30.5,30.5]
[null,null,null,null,"Coincident",30.5,30.5,30.5,30.5,30.5,30.5,30.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.8224363327026367,13.910162925720215,15.675480842590332,15.608766555786133,15.411508560180664,15.263632774353027,15.17084789276123]
[null,null,null,null,"Coincident",8.2482309341430664,10.544223785400391,11.882375717163086,11.831804275512695,11.682278633117676,11.570184707641602,11.499852180480957]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.349770545959473,14.048733711242676,15.94210147857666,15.870082855224609,15.657332420349121,15.49803638458252,15.398173332214355]
[null,null,null,null,"Coincident",8.6119899749755859,11.178659439086914,12.679586410522461,12.625776290893555,12.466370582580566,12.346908569335938,12.272011756896973]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3920373916625977,12.470488548278809,14.289143562316895,14.243168830871582,14.056912422180176,13.886618614196777,13.798198699951172]
[null,null,null,null,"Coincident",7.0150346755981445,9.4529170989990234,10.831500053405762,10.796649932861328,10.655463218688965,10.526376724243164,10.459352493286133]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.8962650299072266,12.528640747070312,14.452836990356445,14.403738021850586,14.205039024353027,14.023677825927734,13.929631233215332]
[null,null,null,null,"Coincident",7.2780938148498535,9.9951257705688477,11.541807174682617,11.504836082458496,11.35455322265625,11.2171630859375,11.145908355712891]
[null,"Bundamba","Substation Rating","MVA","Non-Coincident",114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891]
[null,null,null,null,"Coincident",114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891,114.40000152587891]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.516891479492188,36.553951263427734,36.654499053955078,36.604335784912109,36.288642883300781,36.220390319824219,36.287380218505859]
[null,null,null,null,"Coincident",35.869441986083984,35.905849456787109,36.004608154296875,35.955337524414062,35.645244598388672,35.578201293945313,35.644004821777344]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.517894744873047,36.555095672607422,36.656074523925781,36.605690002441406,36.288982391357422,36.220596313476563,36.287715911865234]
[null,null,null,null,"Coincident",35.887729644775391,35.924388885498047,36.023841857910156,35.974224090576172,35.662014007568359,35.594524383544922,35.6607666015625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.428020477294922,35.512325286865234,35.511348724365234,35.498493194580078,35.175422668457031,35.018672943115234,35.071956634521484]
[null,null,null,null,"Coincident",34.799873352050781,34.882682800292969,34.881725311279297,34.869098663330078,34.5517578125,34.397785186767578,34.450119018554687]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.460460662841797,35.546512603759766,35.545513153076172,35.532390594482422,35.202880859375,35.043231964111328,35.097484588623047]
[null,null,null,null,"Coincident",34.811431884765625,34.89471435546875,34.893753051757812,34.881053924560547,34.56195068359375,34.407169342041016,34.459774017333984]
[null,"Buranda","Substation Rating","MVA","Non-Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,null,null,"Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.375209808349609,21.267539978027344,21.278907775878906,21.209283828735352,22.634729385375977,24.082448959350586,23.945388793945313]
[null,null,null,null,"Coincident",19.826549530029297,19.726680755615234,19.737224578857422,19.672645568847656,20.994815826416016,22.337646484375,22.210515975952148]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.021905899047852,21.910980224609375,21.922689437866211,21.850959777832031,22.635702133178711,24.089160919189453,23.951356887817383]
[null,null,null,null,"Coincident",20.285741806030273,20.183601379394531,20.194393157958984,20.128314971923828,21.615266799926758,22.346206665039063,22.218204498291016]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.551057815551758,20.476043701171875,20.430259704589844,20.383886337280273,21.89482307434082,23.373815536499023,23.233242034912109]
[null,null,null,null,"Coincident",19.062108993530273,18.992528915405273,18.950061798095703,18.907049179077148,20.308515548706055,21.680353164672852,21.549964904785156]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.172821044921875,21.095537185668945,21.048366546630859,21.000591278076172,21.894838333129883,23.377119064331055,23.236001968383789]
[null,null,null,null,"Coincident",19.509105682373047,19.437936782836914,19.394475936889648,19.35045051574707,20.926666259765625,21.687528610229492,21.556289672851563]
[null,"Burleigh Heads","Substation Rating","MVA","Non-Coincident",120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891]
[null,null,null,null,"Coincident",120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891,120.40000152587891]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.381343841552734,53.630069732666016,53.597564697265625,53.933349609375,54.146110534667969,54.143642425537109,54.251243591308594]
[null,null,null,null,"Coincident",51.864234924316406,51.147731781005859,51.116733551025391,51.436973571777344,51.639888763427734,51.637535095214844,51.740154266357422]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.434989929199219,53.670986175537109,53.637966156005859,53.979217529296875,54.195606231689453,54.193092346191406,54.302574157714844]
[null,null,null,null,"Coincident",51.939857482910156,51.214759826660156,51.183399200439453,51.507423400878906,51.712776184082031,51.710395812988281,51.814258575439453]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.060550689697266,50.423801422119141,50.253627777099609,50.619430541992187,50.794685363769531,50.661319732666016,50.745376586914063]
[null,null,null,null,"Coincident",48.697147369384766,48.089870452880859,47.927574157714844,48.276443481445313,48.443588256835938,48.316394805908203,48.396560668945313]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.0703125,50.429035186767578,50.257881164550781,50.625911712646484,50.802391052246094,50.668083190917969,50.752727508544922]
[null,null,null,null,"Coincident",48.738021850585938,48.125099182128906,47.961353302001953,48.313369750976563,48.482063293457031,48.353687286376953,48.434597015380859]
[null,"Burpengary","Substation Rating","MVA","Non-Coincident",59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094]
[null,null,null,null,"Coincident",59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.067829132080078,26.058317184448242,26.06578254699707,25.972423553466797,25.69792366027832,25.559295654296875,25.555206298828125]
[null,null,null,null,"Coincident",24.781597137451172,24.772554397583008,24.779653549194336,24.690898895263672,24.429943084716797,24.298154830932617,24.294269561767578]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.617315292358398,26.607603073120117,26.615226745605469,26.5198974609375,26.239612579345703,26.098062515258789,26.09388542175293]
[null,null,null,null,"Coincident",25.064292907714844,25.055147171020508,25.062326431274414,24.972560882568359,24.708627700805664,24.575336456298828,24.571405410766602]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.744956970214844,21.766658782958984,21.712574005126953,21.656610488891602,21.417423248291016,21.246925354003906,21.236568450927734]
[null,null,null,null,"Coincident",20.672021865844727,20.692653656005859,20.641237258911133,20.588035583496094,20.360651016235352,20.198564529418945,20.188720703125]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.20332145690918,22.225481033325195,22.170255661010742,22.11311149597168,21.86888313293457,21.694791793823242,21.68421745300293]
[null,null,null,null,"Coincident",20.9078369140625,20.928705215454102,20.876701354980469,20.822893142700195,20.592914581298828,20.428979873657227,20.419023513793945]
[null,"Caboolture","Substation Rating","MVA","Non-Coincident",59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453]
[null,null,null,null,"Coincident",59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.591333389282227,21.364213943481445,21.456619262695313,21.450099945068359,21.262422561645508,21.140680313110352,21.09364128112793]
[null,null,null,null,"Coincident",20.114580154418945,19.902994155883789,19.989078521728516,19.983005523681641,19.808164596557617,19.69474983215332,19.65092658996582]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.643486022949219,21.411952972412109,21.506135940551758,21.499490737915039,21.308231353759766,21.184223175048828,21.136322021484375]
[null,null,null,null,"Coincident",20.345100402832031,20.13109016418457,20.218160629272461,20.212018966674805,20.035173416137695,19.920459747314453,19.876132965087891]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.573469161987305,19.393980026245117,19.423898696899414,19.437568664550781,19.25823974609375,19.098569869995117,19.049833297729492]
[null,null,null,null,"Coincident",18.23472785949707,18.067516326904297,18.095388412475586,18.108123779296875,17.941059112548828,17.79231071472168,17.746906280517578]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.592205047607422,19.410442352294922,19.440731048583984,19.454570770263672,19.273067474365234,19.111570358276367,19.062297821044922]
[null,null,null,null,"Coincident",18.443704605102539,18.274576187133789,18.302768707275391,18.315649032592773,18.146671295166016,17.996217727661133,17.950292587280273]
[null,"Caboolture West","Substation Rating","MVA","Non-Coincident",40,60,60,60,60,60,60]
[null,null,null,null,"Coincident",40,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.085975646972656,27.830638885498047,27.826698303222656,27.834653854370117,27.78547477722168,27.769931793212891,27.769094467163086]
[null,null,null,null,"Coincident",28.085975646972656,27.830638885498047,27.826698303222656,27.834653854370117,27.78547477722168,27.769931793212891,27.769094467163086]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.214200973510742,27.948518753051758,27.944421768188477,27.952693939208984,27.901561737060547,27.885402679443359,27.884532928466797]
[null,null,null,null,"Coincident",28.11436653137207,27.858772277832031,27.854827880859375,27.862791061401367,27.813562393188477,27.798002243041992,27.797164916992188]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.054763793945313,23.868574142456055,23.799074172973633,23.829872131347656,23.776334762573242,23.70172119140625,23.693244934082031]
[null,null,null,null,"Coincident",24.054763793945313,23.868574142456055,23.799074172973633,23.829872131347656,23.776334762573242,23.70172119140625,23.693244934082031]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.066486358642578,23.877742767333984,23.807365417480469,23.838546752929687,23.784347534179688,23.708854675292969,23.700281143188477]
[null,null,null,null,"Coincident",24.079078674316406,23.892702102661133,23.823131561279297,23.853960037231445,23.800369262695313,23.725679397583008,23.717195510864258]
[null,"Cades County","Substation Rating","MVA","Non-Coincident",125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781]
[null,null,null,null,"Coincident",125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781,125.30000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",78.659133911132813,78.176445007324219,78.299346923828125,78.062973022460938,77.540061950683594,77.517623901367188,77.531654357910156]
[null,null,null,null,"Coincident",78.659133911132813,78.176445007324219,78.299346923828125,78.062973022460938,77.540061950683594,77.517623901367188,77.531654357910156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",79.051139831542969,78.553932189941406,78.680511474609375,78.43707275390625,77.898704528808594,77.8756103515625,77.890045166015625]
[null,null,null,null,"Coincident",78.659461975097656,78.176559448242188,78.299507141113281,78.063056945800781,77.540061950683594,77.517623901367188,77.531654357910156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",67.092544555664063,66.771743774414063,66.691436767578125,66.557121276855469,66.079505920410156,65.889938354492187,65.880294799804688]
[null,null,null,null,"Coincident",67.092544555664063,66.771743774414063,66.691436767578125,66.557121276855469,66.079505920410156,65.889938354492187,65.880294799804688]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.198135375976563,66.871536254882813,66.789802551269531,66.653114318847656,66.167266845703125,65.974517822265625,65.964714050292969]
[null,null,null,null,"Coincident",67.156150817871094,66.832977294921875,66.752082824707031,66.616790771484375,66.135749816894531,65.944847106933594,65.935134887695313]
[null,"Calamvale","Substation Rating","MVA","Non-Coincident",59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094]
[null,null,null,null,"Coincident",59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.867454528808594,38.21197509765625,38.177268981933594,37.973045349121094,38.005126953125,38.243801116943359,38.167430877685547]
[null,null,null,null,"Coincident",35.809909820556641,35.20599365234375,35.174018859863281,34.985862731933594,35.015419006347656,35.235317230224609,35.164955139160156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.874687194824219,38.216007232666016,38.181156158447266,37.976131439208984,38.008335113525391,38.247970581054687,38.171279907226563]
[null,null,null,null,"Coincident",35.828731536865234,35.221664428710938,35.189529418945313,35.000446319580078,35.030143737792969,35.251136779785156,35.180419921875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.761814117431641,33.237693786621094,33.115505218505859,32.9715576171875,32.983554840087891,33.105052947998047,33.028125762939453]
[null,null,null,null,"Coincident",31.105911254882812,30.623020172119141,30.510442733764648,30.37782096862793,30.388872146606445,30.500814437866211,30.429939270019531]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.078182220458984,33.537853240966797,33.411918640136719,33.263572692871094,33.275932312011719,33.401145935058594,33.321865081787109]
[null,null,null,null,"Coincident",31.107351303100586,30.623746871948242,30.511035919189453,30.378274917602539,30.389335632324219,30.501396179199219,30.430444717407227]
[null,"Caloundra","Substation Rating","MVA","Non-Coincident",115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109]
[null,null,null,null,"Coincident",115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109,115.09999847412109]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.968875885009766,54.838420867919922,56.044956207275391,57.039802551269531,57.594829559326172,58.451816558837891,59.810890197753906]
[null,null,null,null,"Coincident",48.1661376953125,48.942188262939453,50.018993377685547,50.906879425048828,51.402225494384766,52.167068481445313,53.380016326904297]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.382156372070312,55.280044555664062,56.526760101318359,57.555450439453125,58.129623413085937,59.016532897949219,60.423904418945313]
[null,null,null,null,"Coincident",48.300323486328125,49.085094451904297,50.174243927001953,51.072509765625,51.573722839355469,52.347724914550781,53.575439453125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",49.572067260742188,50.439445495605469,51.406379699707031,52.371620178222656,52.855800628662109,53.503868103027344,54.729972839355469]
[null,null,null,null,"Coincident",44.242073059082031,45.016189575195313,45.879161834716797,46.740623474121094,47.172740936279297,47.751132965087891,48.845401763916016]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.851058959960938,50.743633270263672,51.73944091796875,52.734294891357422,53.233608245849609,53.902217864990234,55.16802978515625]
[null,null,null,null,"Coincident",44.334728240966797,45.116668701171875,45.988590240478516,46.859203338623047,47.295993804931641,47.880718231201172,48.987213134765625]
[null,"Camp Hill","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.577037811279297,34.108043670654297,33.672370910644531,33.525959014892578,33.668251037597656,34.094661712646484,34.553237915039063]
[null,null,null,null,"Coincident",30.105197906494141,29.696859359741211,29.317531585693359,29.190053939819336,29.313943862915039,29.685207366943359,30.08447265625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.642295837402344,34.163742065429688,33.719764709472656,33.570690155029297,33.715568542480469,34.150096893310547,34.617996215820313]
[null,null,null,null,"Coincident",30.428489685058594,30.015766143798828,29.632364273071289,29.503519058227539,29.628738403320313,30.003988265991211,30.407541275024414]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.634309768676758,29.272212982177734,28.818243026733398,28.721858978271484,28.829896926879883,29.119699478149414,29.501697540283203]
[null,null,null,null,"Coincident",25.801712036132812,25.486446380615234,25.091190338134766,25.007268905639648,25.101335525512695,25.353660583496094,25.686254501342773]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.635610580444336,29.272558212280273,29.314783096313477,29.213432312011719,29.327037811279297,29.11982536315918,29.502578735351563]
[null,null,null,null,"Coincident",26.078788757324219,25.760137557983398,25.360637664794922,25.275815963745117,25.370891571044922,25.625926971435547,25.962091445922852]
[null,"Capalaba","Substation Rating","MVA","Non-Coincident",29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547]
[null,null,null,null,"Coincident",29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547,29.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.915922164916992,17.762489318847656,17.772617340087891,17.699886322021484,17.479660034179687,17.311443328857422,17.190561294555664]
[null,null,null,null,"Coincident",16.921211242675781,16.776298522949219,16.785863876342773,16.717170715332031,16.509172439575195,16.35029411315918,16.236124038696289]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.178073883056641,18.014627456665039,18.025413513183594,17.947973251342773,17.713649749755859,17.53483772277832,17.406436920166016]
[null,null,null,null,"Coincident",17.627693176269531,17.476730346679687,17.4866943359375,17.415134429931641,17.198451995849609,17.032939910888672,16.914003372192383]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.209144592285156,17.085029602050781,17.047409057617187,16.994756698608398,16.775238037109375,16.570932388305664,16.449834823608398]
[null,null,null,null,"Coincident",16.25367546081543,16.136451721191406,16.100919723510742,16.051191329956055,15.843859672546387,15.650897979736328,15.53652286529541]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.426170349121094,17.294404983520508,17.254484176635742,17.198623657226563,16.965904235839844,16.749570846557617,16.621465682983398]
[null,null,null,null,"Coincident",16.932287216186523,16.810169219970703,16.773153305053711,16.721349716186523,16.505361557006836,16.304342269897461,16.185192108154297]
[null,"Capalaba South","Substation Rating","MVA","Non-Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,null,null,"Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.175474166870117,15.812251091003418,15.78905200958252,15.834063529968262,15.951244354248047,16.042942047119141,16.07684326171875]
[null,null,null,null,"Coincident",14.962078094482422,14.626102447509766,14.604643821716309,14.646278381347656,14.754669189453125,14.83948802947998,14.870846748352051]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.79582405090332,16.418670654296875,16.394580841064453,16.441318511962891,16.562994003295898,16.658208847045898,16.693408966064453]
[null,null,null,null,"Coincident",15.431833267211914,15.085309028625488,15.063177108764648,15.106118202209473,15.217912673950195,15.305394172668457,15.337737083435059]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.052848815917969,14.734896659851074,14.672513008117676,14.729172706604004,14.831045150756836,14.877817153930664,14.904375076293945]
[null,null,null,null,"Coincident",13.923666000366211,13.629565238952637,13.571861267089844,13.624270439147949,13.718501091003418,13.761764526367188,13.786330223083496]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.630144119262695,15.29999828338623,15.235221862792969,15.294054985046387,15.399833679199219,15.448399543762207,15.475976943969727]
[null,null,null,null,"Coincident",14.360818862915039,14.057483673095703,13.997968673706055,14.052022933959961,14.149211883544922,14.19383430480957,14.219170570373535]
[null,"Carole Park","Substation Rating","MVA","Non-Coincident",42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094]
[null,null,null,null,"Coincident",42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094,42.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.27874755859375,21.173938751220703,21.179536819458008,21.088132858276367,20.940706253051758,20.975482940673828,21.0032958984375]
[null,null,null,null,"Coincident",21.052148818969727,20.948455810546875,20.953994750976562,20.863563537597656,20.717706680297852,20.752113342285156,20.779630661010742]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.933904647827148,21.819431304931641,21.825544357299805,21.725736618041992,21.56480598449707,21.602762222290039,21.633121490478516]
[null,null,null,null,"Coincident",21.075946807861328,20.970890045166016,20.976499557495117,20.884906768798828,20.737228393554687,20.772058486938477,20.799917221069336]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.036653518676758,20.961576461791992,20.909029006958008,20.839775085449219,20.684135437011719,20.665031433105469,20.685659408569336]
[null,null,null,null,"Coincident",20.812631607055664,20.73835563659668,20.686367034912109,20.617851257324219,20.463869094848633,20.444967269897461,20.465375900268555]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.669534683227539,21.587583541870117,21.530235290527344,21.45466423034668,21.284883499145508,21.264047622680664,21.286544799804687]
[null,null,null,null,"Coincident",20.833330154418945,20.75813102722168,20.70550537109375,20.636165618896484,20.480386734008789,20.461271286010742,20.481910705566406]
[null,"Carole Park Central","Substation Rating","MVA","Non-Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,null,null,"Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.473730087280273,25.279499053955078,25.279539108276367,25.163703918457031,24.837396621704102,24.590705871582031,24.432758331298828]
[null,null,null,null,"Coincident",22.192464828491211,22.023252487182617,22.023288726806641,21.922372817993164,21.638097763061523,21.423183441162109,21.285581588745117]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.327774047851563,27.104524612426758,27.104572296142578,26.971458435058594,26.596584320068359,26.313287734985352,26.131952285766602]
[null,null,null,null,"Coincident",22.808803558349609,22.635746002197266,22.6358642578125,22.5322265625,22.240127563476563,22.019319534301758,21.877973556518555]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.194416046142578,25.037134170532227,24.96788215637207,24.878595352172852,24.544254302978516,24.237850189208984,24.074357986450195]
[null,null,null,null,"Coincident",21.949129104614258,21.812107086181641,21.751775741577148,21.673990249633789,21.382715225219727,21.115777969360352,20.973346710205078]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.006750106811523,26.826030731201172,26.746471405029297,26.643905639648437,26.259952545166016,25.908241271972656,25.720636367797852]
[null,null,null,null,"Coincident",22.564943313598633,22.424976348876953,22.363037109375,22.283153533935547,21.983781814575195,21.709430694580078,21.563085556030273]
[null,"Carpendale","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8308553695678711,1.8334580659866333,1.836721658706665,1.8323633670806885,1.8157522678375244,1.8083281517028809,1.807124137878418]
[null,null,null,null,"Coincident",1.5482014417648315,1.5504021644592285,1.5531620979309082,1.5494766235351563,1.5354300737380981,1.5291520357131958,1.5281338691711426]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8911579847335815,1.8938463926315308,1.8972175121307373,1.8927156925201416,1.875557541847229,1.8678888082504272,1.8666452169418335]
[null,null,null,null,"Coincident",1.5578523874282837,1.560066819190979,1.5628440380096436,1.5591355562210083,1.5450013875961304,1.5386842489242554,1.537659764289856]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7251415252685547,1.7299492359161377,1.7282273769378662,1.7258642911911011,1.7093966007232666,1.6980149745941162,1.6963286399841309]
[null,null,null,null,"Coincident",1.4588079452514648,1.4628734588623047,1.4614173173904419,1.4594191312789917,1.4454936981201172,1.4358692169189453,1.4344432353973389]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7819623947143555,1.7869284152984619,1.7851496934890747,1.7827088832855225,1.7656987905502319,1.7539423704147339,1.7522003650665283]
[null,null,null,null,"Coincident",1.4679017066955566,1.4719924926757812,1.4705272912979126,1.4685167074203491,1.4545044898986816,1.4448199272155762,1.443385124206543]
[null,"Charlotte St","Substation Rating","MVA","Non-Coincident",186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437]
[null,null,null,null,"Coincident",186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437,186.89999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378]
[null,null,null,null,"Coincident",0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378,0.85559910535812378]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",95.151168823242188,95.491722106933594,95.828254699707031,104.02960205078125,106.23008728027344,108.69673156738281,109.84464263916016]
[null,null,null,null,"Coincident",87.425041198730469,87.741004943847656,88.053237915039062,95.662399291992188,97.703994750976563,99.992530822753906,101.05755615234375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",95.15118408203125,95.491996765136719,95.829093933105469,104.13102722167969,106.23056793212891,108.70823669433594,109.86604309082031]
[null,null,null,null,"Coincident",87.44293212890625,87.760551452636719,88.074485778808594,95.66241455078125,97.710067749023438,100.01646423339844,101.0872802734375]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",93.692695617675781,94.155860900878906,94.225532531738281,102.84121704101562,105.06093597412109,107.31378936767578,108.39851379394531]
[null,null,null,null,"Coincident",86.071884155273437,86.501602172851562,86.566246032714844,94.559822082519531,96.6192626953125,98.709442138671875,99.715843200683594]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",93.810966491699219,94.285675048828125,94.357124328613281,102.91847991943359,105.18572998046875,107.31735229492187,108.40792846679687]
[null,null,null,null,"Coincident",86.083877563476563,86.5155029296875,86.580421447753906,94.559921264648438,96.623733520507813,98.729560852050781,99.740974426269531]
[null,"Chermside","Substation Rating","MVA","Non-Coincident",65.400001525878906,87.400001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906]
[null,null,null,null,"Coincident",65.400001525878906,87.400001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.161060333251953,40.970184326171875,40.982162475585937,40.80645751953125,40.741592407226562,40.779613494873047,40.545192718505859]
[null,null,null,null,"Coincident",38.856784820556641,38.676593780517578,38.687900543212891,38.52203369140625,38.460800170898437,38.496692657470703,38.275394439697266]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.163600921630859,40.971946716308594,40.983970642089844,40.807662963867188,40.742607116699219,40.780738830566406,40.545726776123047]
[null,null,null,null,"Coincident",38.856830596923828,38.676593780517578,38.687904357910156,38.614242553710937,38.551975250244141,38.588474273681641,38.36346435546875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.938182830810547,38.810455322265625,38.714241027832031,38.587116241455078,38.507259368896484,38.443752288818359,38.210239410400391]
[null,null,null,null,"Coincident",36.758346557617188,36.637771606445313,36.546943664550781,36.426933288574219,36.351547241210937,36.291595458984375,36.071155548095703]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.003585815429688,38.87310791015625,38.774852752685547,38.645076751708984,38.563579559326172,38.498783111572266,38.260639190673828]
[null,null,null,null,"Coincident",36.822578430175781,36.700233459472656,36.608085632324219,36.486347198486328,36.409885406494141,36.349082946777344,36.125564575195313]
[null,"Clayfield","Substation Rating","MVA","Non-Coincident",36,36,36,55,55,55,55]
[null,null,null,null,"Coincident",36,36,36,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.257863998413086,20.149253845214844,20.168846130371094,20.12879753112793,19.894645690917969,19.683200836181641,19.575351715087891]
[null,null,null,null,"Coincident",18.255687713623047,18.157812118530273,18.175468444824219,18.139377593994141,17.928367614746094,17.737821578979492,17.640630722045898]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.550519943237305,20.435850143432617,20.456533432006836,20.414255142211914,20.167173385620117,19.944192886352539,19.830514907836914]
[null,null,null,null,"Coincident",18.600509643554688,18.500785827636719,18.518775939941406,18.482002258300781,18.267007827758789,18.07286262512207,17.973834991455078]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.96641731262207,17.894458770751953,17.862234115600586,17.844732284545898,17.628673553466797,17.396310806274414,17.295326232910156]
[null,null,null,null,"Coincident",16.190715789794922,16.12586784362793,16.096828460693359,16.081056594848633,15.8863525390625,15.67695426940918,15.58595085144043]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.139430999755859,18.064031600952148,18.0302734375,18.011940002441406,17.785728454589844,17.54267692565918,17.437126159667969]
[null,null,null,null,"Coincident",16.49653434753418,16.430459976196289,16.400873184204102,16.384803771972656,16.186422348022461,15.973068237304687,15.880345344543457]
[null,"Cleveland","Substation Rating","MVA","Non-Coincident",65,65,65,65,65,65,65]
[null,null,null,null,"Coincident",65,65,65,65,65,65,65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.622543334960937,26.547458648681641,26.471729278564453,26.345592498779297,26.041257858276367,25.88597297668457,25.981145858764648]
[null,null,null,null,"Coincident",24.416070938110352,24.347206115722656,24.277753829956055,24.162073135375977,23.882963180541992,23.740547180175781,23.827831268310547]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.9041748046875,26.826103210449219,26.747367858886719,26.616247177124023,26.299983978271484,26.138669967651367,26.237533569335938]
[null,null,null,null,"Coincident",24.922243118286133,24.851949691772461,24.781059265136719,24.662979125976562,24.378084182739258,24.232715606689453,24.321807861328125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.494365692138672,24.458581924438477,24.321243286132813,24.229751586914063,23.938344955444336,23.734201431274414,23.813663482666016]
[null,null,null,null,"Coincident",22.464277267456055,22.431459426879883,22.305501937866211,22.221591949462891,21.954338073730469,21.767114639282227,21.839990615844727]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.694883346557617,24.657804489135742,24.515518188476563,24.420751571655273,24.119028091430664,23.907760620117188,23.989986419677734]
[null,null,null,null,"Coincident",22.929986953735352,22.896488189697266,22.767919540405273,22.682270050048828,22.409475326538086,22.21837043762207,22.292757034301758]
[null,"Coolum","Substation Rating","MVA","Non-Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,null,null,"Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.556545257568359,22.494289398193359,22.595285415649414,22.570716857910156,22.400976181030273,22.351203918457031,22.444526672363281]
[null,null,null,null,"Coincident",19.564481735229492,19.51048469543457,19.598079681396484,19.576772689819336,19.429548263549805,19.386379241943359,19.467321395874023]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.56755256652832,22.504806518554688,22.606603622436523,22.581836700439453,22.410776138305664,22.360630035400391,22.454658508300781]
[null,null,null,null,"Coincident",19.744665145874023,19.690170288085938,19.778572082519531,19.757068634033203,19.608488082885742,19.564922332763672,19.646608352661133]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.894723892211914,20.865463256835938,20.90107536315918,20.899394989013672,20.732250213623047,20.632814407348633,20.712175369262695]
[null,null,null,null,"Coincident",18.123096466064453,18.097719192504883,18.128606796264648,18.127147674560547,17.982177734375,17.895929336547852,17.964763641357422]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.896280288696289,20.866926193237305,20.902652740478516,20.900966644287109,20.73332405090332,20.633636474609375,20.71319580078125]
[null,null,null,null,"Coincident",18.290004730224609,18.264392852783203,18.295564651489258,18.294092178344727,18.147787094116211,18.060745239257813,18.130212783813477]
[null,"Coomera","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.916316986083984,37.484413146972656,37.831844329833984,38.045719146728516,37.976070404052734,38.080234527587891,38.449367523193359]
[null,null,null,null,"Coincident",34.533634185791016,37.224456787109375,37.568202972412109,37.7791748046875,37.708461761474609,37.810134887695313,38.174411773681641]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.079109191894531,37.699470520019531,38.054267883300781,38.272705078125,38.201568603515625,38.307960510253906,38.685035705566406]
[null,null,null,null,"Coincident",34.914108276367188,37.225128173828125,37.569206237792969,37.780410766601563,37.709609985351563,37.811393737792969,38.176132202148438]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.576084136962891,33.274948120117187,33.486907958984375,33.706363677978516,33.624336242675781,33.6248779296875,33.933712005615234]
[null,null,null,null,"Coincident",30.204898834228516,33.032695770263672,33.241767883300781,33.458110809326172,33.375049591064453,33.373737335205078,33.677902221679688]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.66132926940918,33.4066162109375,33.622482299804688,33.846019744873047,33.762462615966797,33.763015747070313,34.07763671875]
[null,null,null,null,"Coincident",30.537567138671875,33.409435272216797,33.620784759521484,33.839473724365234,33.755332946777344,33.753856658935547,34.061298370361328]
[null,"Coominya","Substation Rating","MVA","Non-Coincident",12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727]
[null,null,null,null,"Coincident",12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727,12.600000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.3567018508911133,7.3664183616638184,7.3762979507446289,7.3555045127868652,7.2766766548156738,7.2271881103515625,7.2071008682250977]
[null,null,null,null,"Coincident",5.7219085693359375,5.7294659614562988,5.7371501922607422,5.7209773063659668,5.6596665382385254,5.6211752891540527,5.6055517196655273]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.4810099601745605,7.4912505149841309,7.5016636848449707,7.4797482490539551,7.3966879844665527,7.3445601463317871,7.3234052658081055]
[null,null,null,null,"Coincident",5.7613506317138672,5.7691936492919922,5.7771697044372559,5.7603931427001953,5.6968116760253906,5.6569242477416992,5.6407475471496582]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.1244745254516602,7.1435871124267578,7.1333179473876953,7.1203222274780273,7.0405435562133789,6.9744834899902344,6.9526581764221191]
[null,null,null,null,"Coincident",5.5412864685058594,5.5561518669128418,5.5481648445129395,5.5380568504333496,5.4760065078735352,5.424626350402832,5.4076509475708008]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.236412525177002,7.2565317153930664,7.2457213401794434,7.2320418357849121,7.1480879783630371,7.0785999298095703,7.0556488037109375]
[null,null,null,null,"Coincident",5.5737786293029785,5.5891680717468262,5.5809025764465332,5.5704441070556641,5.5062532424926758,5.4531435966491699,5.4356136322021484]
[null,"Cooneana","Substation Rating","MVA","Non-Coincident",26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547]
[null,null,null,null,"Coincident",26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.5202651023864746,8.0689783096313477,8.9136238098144531,9.8258171081542969,10.647254943847656,11.592854499816895,12.57367992401123]
[null,null,null,null,"Coincident",5.9326567649841309,7.4396467208862305,8.2082538604736328,9.037872314453125,9.7841005325317383,10.643608093261719,11.535511016845703]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.151885986328125,8.8506231307983398,9.7770900726318359,10.777647972106934,11.678658485412598,12.715858459472656,13.791696548461914]
[null,null,null,null,"Coincident",5.990013599395752,7.5499916076660156,8.325688362121582,9.1628389358520508,9.9155416488647461,10.782763481140137,11.682868957519531]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.969489574432373,7.4935288429260254,8.2450532913208008,9.0878047943115234,9.8336620330810547,10.670163154602051,11.560723304748535]
[null,null,null,null,"Coincident",5.4315166473388672,6.9212241172790527,7.604820728302002,8.3713407516479492,9.0486898422241211,9.8086271286010742,10.618341445922852]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5477561950683594,8.2194299697875977,9.0437545776367187,9.968144416809082,10.786252975463867,11.70378589630127,12.680615425109863]
[null,null,null,null,"Coincident",5.4840288162231445,7.0291414260864258,7.7188305854797363,8.492243766784668,9.1753034591674805,9.9418249130249023,10.758883476257324]
[null,"Coopers Plains","Substation Rating","MVA","Non-Coincident",52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094]
[null,null,null,null,"Coincident",52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.427614212036133,20.281305313110352,20.295783996582031,20.211776733398437,19.962453842163086,19.78265380859375,19.665775299072266]
[null,null,null,null,"Coincident",16.674789428710937,16.55535888671875,16.567178726196289,16.498603820800781,16.295085906982422,16.148317337036133,16.052909851074219]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.464040756225586,20.313003540039063,20.327938079833984,20.2413330078125,19.984891891479492,19.800519943237305,19.680929183959961]
[null,null,null,null,"Coincident",16.681304931640625,16.560791015625,16.572713851928711,16.50355339050293,16.298479080200195,16.150760650634766,16.054815292358398]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.2420654296875,20.124486923217773,20.083057403564453,20.020090103149414,19.76362419128418,19.535083770751953,19.413305282592773]
[null,null,null,null,"Coincident",16.52332878112793,16.427350997924805,16.393531799316406,16.342132568359375,16.132783889770508,15.94622802734375,15.846822738647461]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.272546768188477,20.151449203491211,20.108827590942383,20.044094085693359,19.781034469604492,19.547451019287109,19.423318862915039]
[null,null,null,null,"Coincident",16.528486251831055,16.431724548339844,16.39764404296875,16.345861434936523,16.135135650634766,15.947608947753906,15.847787857055664]
[null,"Cooran","Substation Rating","MVA","Non-Coincident",35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453]
[null,null,null,null,"Coincident",35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453,35.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6863846778869629,5.6802124977111816,5.6750874519348145,5.6513242721557617,5.5967411994934082,5.5862412452697754,5.6175436973571777]
[null,null,null,null,"Coincident",5.0247879028320312,5.0193343162536621,5.0148053169250488,4.9938077926635742,4.9455747604370117,4.9362964630126953,4.9639573097229004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.8081684112548828,5.8018641471862793,5.7966289520263672,5.7723569869995117,5.7166047096252441,5.7058801651000977,5.7378530502319336]
[null,null,null,null,"Coincident",5.0705471038818359,5.0650439262390137,5.0604739189147949,5.0392851829528809,4.9906125068664551,4.9812498092651367,5.0091629028320313]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.2390923500061035,5.2405409812927246,5.2213068008422852,5.2046842575073242,5.1519370079040527,5.1290035247802734,5.1560549736022949]
[null,null,null,null,"Coincident",4.6295366287231445,4.6308169364929199,4.6138200759887695,4.5991325378417969,4.5525221824645996,4.532257080078125,4.5561614036560059]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.3512964248657227,5.3527765274047852,5.3331303596496582,5.3161516189575195,5.2622742652893066,5.2388501167297363,5.2664809226989746]
[null,null,null,null,"Coincident",4.671696662902832,4.6729884147644043,4.6558370590209961,4.6410155296325684,4.5939807891845703,4.5735311508178711,4.5976529121398926]
[null,"Cooroy","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.2165389060974121,6.2123098373413086,6.2087836265563965,6.1829166412353516,6.1191706657409668,6.0971941947937012,6.1156587600708008]
[null,null,null,null,"Coincident",5.6312093734741211,5.6273784637451172,5.6241841316223145,5.6007528305053711,5.5430092811584473,5.5231022834777832,5.5398283004760742]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3539390563964844,6.349616527557373,6.3460125923156738,6.3195734024047852,6.2544183731079102,6.2319564819335938,6.250828742980957]
[null,null,null,null,"Coincident",5.6738362312316895,5.6699762344360352,5.6667580604553223,5.6431493759155273,5.5849685668945312,5.564910888671875,5.581763744354248]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7380962371826172,5.7420105934143066,5.7228527069091797,5.7047533988952637,5.6432242393493652,5.6084485054016113,5.6235909461975098]
[null,null,null,null,"Coincident",5.1978158950805664,5.2013616561889648,5.1840071678161621,5.1676125526428223,5.1118760108947754,5.0803747177124023,5.0940914154052734]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8649215698242187,5.8689227104187012,5.8493413925170898,5.8308415412902832,5.7679524421691895,5.7324085235595703,5.7478857040405273]
[null,null,null,null,"Coincident",5.2371621131896973,5.2407345771789551,5.2232489585876465,5.2067303657531738,5.1505718231201172,5.1188321113586426,5.1326522827148437]
[null,"Coorparoo","Substation Rating","MVA","Non-Coincident",54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094]
[null,null,null,null,"Coincident",54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094,54.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.2825927734375,19.165353775024414,19.168268203735352,19.083362579345703,18.838848114013672,18.708303451538086,19.071039199829102]
[null,null,null,null,"Coincident",18.191120147705078,18.080516815185547,18.083267211914062,18.003168106079102,17.772493362426758,17.649337768554688,17.991540908813477]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.726114273071289,19.599281311035156,19.602434158325195,19.510612487792969,19.246341705322266,19.105350494384766,19.497287750244141]
[null,null,null,null,"Coincident",18.514247894287109,18.401679992675781,18.40447998046875,18.322957992553711,18.088186264038086,17.96284294128418,18.311124801635742]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.155326843261719,17.074270248413086,17.029556274414062,16.971210479736328,16.745706558227539,16.586759567260742,16.902822494506836]
[null,null,null,null,"Coincident",16.184267044067383,16.107797622680664,16.065614700317383,16.01057243347168,15.797831535339355,15.647882461547852,15.94605541229248]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.434030532836914,17.347131729125977,17.299209594726562,17.236696243286133,16.995265960693359,16.825275421142578,17.163448333740234]
[null,null,null,null,"Coincident",16.464536666870117,16.386743545532227,16.343830108642578,16.287834167480469,16.071409225463867,15.918863296508789,16.222200393676758]
[null,"Cornubia","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.944812774658203,12.861783981323242,12.946528434753418,13.01881217956543,13.028178215026855,13.105197906494141,13.211920738220215]
[null,null,null,null,"Coincident",12.29430103302002,12.215444564819336,12.295930862426758,12.364582061767578,12.373477935791016,12.446627616882324,12.54798698425293]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.119888305664063,13.035736083984375,13.121626853942871,13.194889068603516,13.204381942749023,13.282442092895508,13.390608787536621]
[null,null,null,null,"Coincident",12.374251365661621,12.294881820678711,12.37589168548584,12.444989204406738,12.453943252563477,12.527567863464355,12.629587173461914]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.24933910369873,11.192423820495605,11.234957695007324,11.30907154083252,11.311767578125,11.349282264709473,11.437957763671875]
[null,null,null,null,"Coincident",10.684029579162598,10.629974365234375,10.670371055603027,10.74075984954834,10.743320465087891,10.778949737548828,10.863170623779297]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.401483535766602,11.343798637390137,11.386907577514648,11.462023735046387,11.464756011962891,11.502779006958008,11.592653274536133]
[null,null,null,null,"Coincident",10.753507614135742,10.699101448059082,10.739760398864746,10.810606956481934,10.81318473815918,10.849045753479004,10.93381404876709]
[null,"Crestmead","Substation Rating","MVA","Non-Coincident",51.5,51.5,51.5,51.5,51.5,51.5,51.5]
[null,null,null,null,"Coincident",51.5,51.5,51.5,51.5,51.5,51.5,51.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.353305816650391,26.311548233032227,26.345640182495117,26.363946914672852,26.194826126098633,26.080970764160156,26.107570648193359]
[null,null,null,null,"Coincident",25.227746963500977,25.187774658203125,25.220407485961914,25.237934112548828,25.07603645324707,24.967041015625,24.992502212524414]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.36622428894043,26.323915481567383,26.358457565307617,26.377008438110352,26.205715179443359,26.09050178527832,26.117410659790039]
[null,null,null,null,"Coincident",25.569561004638672,25.529047012329102,25.562122344970703,25.579885482788086,25.415794372558594,25.305322647094727,25.33112907409668]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.835702896118164,24.830158233642578,24.793449401855469,24.835685729980469,24.664506912231445,24.493942260742188,24.510892868041992]
[null,null,null,null,"Coincident",23.77496337890625,23.769657135009766,23.734514236450195,23.774946212768555,23.611078262329102,23.447797775268555,23.464023590087891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.836191177368164,24.830631256103516,24.793828964233398,24.836174011230469,24.664638519287109,24.493942260742188,24.510896682739258]
[null,null,null,null,"Coincident",24.09709358215332,24.091714859008789,24.056097030639648,24.097076416015625,23.930988311767578,23.765495300292969,23.781940460205078]
[null,"Currimundi","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",72,72,72,72,72,72,72]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.526599884033203,18.518947601318359,18.857355117797852,18.890945434570313,18.830600738525391,18.878145217895508,19.01789665222168]
[null,null,null,null,"Coincident",13.763769149780273,14.495662689208984,14.76137638092041,14.787931442260742,14.741114616394043,14.778874397277832,14.888877868652344]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.720026016235352,18.723325729370117,19.065465927124023,19.099428176879883,19.038417816162109,19.08648681640625,19.227781295776367]
[null,null,null,null,"Coincident",13.820627212524414,14.554449081420898,14.821259498596191,14.847928047180176,14.800930976867676,14.83885669708252,14.949320793151855]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.001791000366211,17.047369003295898,17.308765411376953,17.356430053710937,17.291635513305664,17.289239883422852,17.410062789916992]
[null,null,null,null,"Coincident",12.566325187683105,13.337515830993652,13.542888641357422,13.580456733703613,13.53019905090332,13.528889656066895,13.624054908752441]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.178388595581055,17.235504150390625,17.499786376953125,17.547977447509766,17.48246955871582,17.480047225952148,17.602201461791992]
[null,null,null,null,"Coincident",12.618236541748047,13.391461372375488,13.597683906555176,13.635410308837891,13.584959983825684,13.583658218383789,13.67922306060791]
[null,"Currumbin","Substation Rating","MVA","Non-Coincident",37.5,37.5,37.5,37.5,37.5,37.5,37.5]
[null,null,null,null,"Coincident",37.5,37.5,37.5,37.5,37.5,37.5,37.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.956670761108398,21.955154418945313,21.957700729370117,21.873842239379883,21.669647216796875,21.62269401550293,21.695840835571289]
[null,null,null,null,"Coincident",19.983484268188477,19.982105255126953,19.984424591064453,19.908100128173828,19.722257614135742,19.679523468017578,19.746097564697266]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.96124267578125,21.959718704223633,21.962278366088867,21.87799072265625,21.672834396362305,21.625675201416016,21.69914436340332]
[null,null,null,null,"Coincident",20.417705535888672,20.416297912597656,20.418666839599609,20.340682983398437,20.150802612304688,20.107139587402344,20.175161361694336]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.566734313964844,20.593353271484375,20.53868293762207,20.480865478515625,20.279922485351563,20.183769226074219,20.245416641235352]
[null,null,null,null,"Coincident",18.718456268310547,18.742683410644531,18.692926406860352,18.640302658081055,18.457416534423828,18.369905471801758,18.42601203918457]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.56688117980957,20.593528747558594,20.538803100585938,20.480939865112305,20.279922485351563,20.887424468994141,20.951221466064453]
[null,null,null,null,"Coincident",19.125190734863281,19.149944305419922,19.099105834960938,19.045337677001953,18.858478546142578,18.769065856933594,18.826391220092773]
[null,"Darra","Substation Rating","MVA","Non-Coincident",52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453]
[null,null,null,null,"Coincident",52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453,52.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.742170333862305,20.792194366455078,20.798116683959961,20.708887100219727,20.446344375610352,20.249088287353516,20.124916076660156]
[null,null,null,null,"Coincident",17.418886184692383,18.345340728759766,18.350566864013672,18.27183723449707,18.040191650390625,17.866147994995117,17.756589889526367]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.792934417724609,20.890462875366211,20.896690368652344,20.802919387817383,20.527532577514648,20.321147918701172,20.19146728515625]
[null,null,null,null,"Coincident",17.444992065429688,18.407295227050781,18.412666320800781,18.331933975219727,18.094518661499023,17.916290283203125,17.804168701171875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.618242263793945,20.756364822387695,20.704790115356445,20.636772155761719,20.365386962890625,20.116909027099609,19.987041473388672]
[null,null,null,null,"Coincident",17.309541702270508,18.313728332519531,18.268222808837891,18.208209991455078,17.968761444091797,17.74952507019043,17.634939193725586]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.664295196533203,20.852802276611328,20.798616409301758,20.727199554443359,20.442773818969727,20.183111190795898,20.047695159912109]
[null,null,null,null,"Coincident",17.333795547485352,18.375936508178711,18.329269409179688,18.267736434936523,18.022329330444336,17.797855377197266,17.680618286132813]
[null,"Deception Bay","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.305400848388672,31.250253677368164,31.650789260864258,31.622625350952148,31.379491806030273,31.298702239990234,31.533359527587891]
[null,null,null,null,"Coincident",29.863372802734375,29.810766220092773,30.192852020263672,30.165985107421875,29.934051513671875,29.856983184814453,30.080831527709961]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.517604827880859,32.459037780761719,32.884437561035156,32.854526519775391,32.596294403076172,32.510494232177734,32.759716033935547]
[null,null,null,null,"Coincident",30.086933135986328,30.033355712890625,30.422519683837891,30.395153045654297,30.158920288085938,30.080427169799805,30.308418273925781]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.87895393371582,27.86778450012207,28.146772384643555,28.150068283081055,27.920206069946289,27.776472091674805,27.975555419921875]
[null,null,null,null,"Coincident",26.594758987426758,26.584104537963867,26.850240707397461,26.853384017944336,26.634111404418945,26.496997833251953,26.686910629272461]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.879945755004883,28.868093490600586,29.164161682128906,29.167657852172852,28.923721313476563,28.771194458007813,28.982458114624023]
[null,null,null,null,"Coincident",26.759500503540039,26.748659133911133,27.019449234008789,27.022647857666016,26.799539566040039,26.660036087036133,26.853260040283203]
[null,"Doboy","Substation Rating","MVA","Non-Coincident",52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547]
[null,null,null,null,"Coincident",52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.527905464172363,13.523488998413086,13.533369064331055,13.481315612792969,13.316513061523437,13.194234848022461,13.119211196899414]
[null,null,null,null,"Coincident",11.421889305114746,11.418160438537598,11.426502227783203,11.382552146911621,11.243406295776367,11.140164375305176,11.076820373535156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.134316444396973,14.129702568054199,14.14002513885498,14.085638046264648,13.913448333740234,13.785689353942871,13.707302093505859]
[null,null,null,null,"Coincident",11.936419486999512,11.932522773742676,11.941240310668945,11.895310401916504,11.749897003173828,11.642004013061523,11.575806617736816]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.106552124023438,13.120136260986328,13.093345642089844,13.056130409240723,12.890326499938965,12.739007949829102,12.66242504119873]
[null,null,null,null,"Coincident",11.066131591796875,11.077601432800293,11.054981231689453,11.0235595703125,10.883567810058594,10.755806922912598,10.691145896911621]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.694075584411621,13.708268165588379,13.680276870727539,13.641393661499023,13.468156814575195,13.310055732727051,13.230040550231934]
[null,null,null,null,"Coincident",11.56463623046875,11.57662296295166,11.552983283996582,11.520146369934082,11.373847961425781,11.240331649780273,11.172758102416992]
[null,"Duffield Road","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.451438903808594,22.478965759277344,22.516719818115234,22.516403198242188,22.367111206054688,22.331888198852539,22.475456237792969]
[null,null,null,null,"Coincident",21.650400161743164,21.676942825317383,21.713354110717773,21.713050842285156,21.569082260131836,21.535116195678711,21.673563003540039]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.538883209228516,22.567100524902344,22.605804443359375,22.605480194091797,22.452451705932617,22.416353225708008,22.563503265380859]
[null,null,null,null,"Coincident",21.90867805480957,21.935537338256836,21.972383499145508,21.972076416015625,21.826391220092773,21.792018890380859,21.932117462158203]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.495668411254883,21.551362991333008,21.527753829956055,21.549148559570313,21.395978927612305,21.307167053222656,21.437126159667969]
[null,null,null,null,"Coincident",20.728731155395508,20.782438278198242,20.759672164916992,20.780303955078125,20.632596969604492,20.546957015991211,20.672277450561523]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.560375213623047,21.617326736450195,21.593183517456055,21.615060806274414,21.458461761474609,21.367692947387695,21.500524520874023]
[null,null,null,null,"Coincident",20.976015090942383,21.030361175537109,21.00732421875,21.028202056884766,20.878732681274414,20.792072296142578,20.918886184692383]
[null,"Eight Mile Plains Bus 1","Substation Rating","MVA","Non-Coincident",26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453]
[null,null,null,null,"Coincident",26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453,26.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.816537857055664,14.599647521972656,14.589611053466797,14.512543678283691,14.314075469970703,14.241686820983887,14.44816780090332]
[null,null,null,null,"Coincident",14.630904197692871,14.416730880737305,14.406820297241211,14.330718040466309,14.134737014770508,14.063255310058594,14.267148971557617]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.072786331176758,14.852144241333008,14.841934204101563,14.763533592224121,14.561634063720703,14.487993240356445,14.698044776916504]
[null,null,null,null,"Coincident",15.072786331176758,14.852144241333008,14.841934204101563,14.763533592224121,14.561634063720703,14.487993240356445,14.698044776916504]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.561087608337402,13.380793571472168,13.334548950195313,13.277480125427246,13.089607238769531,12.989809036254883,13.173824310302734]
[null,null,null,null,"Coincident",13.391182899475098,13.21314811706543,13.167482376098633,13.111128807067871,12.925609588623047,12.827061653137207,13.008771896362305]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.580196380615234,13.39603328704834,13.348858833312988,13.290678977966309,13.099437713623047,12.998034477233887,13.18510913848877]
[null,null,null,null,"Coincident",13.795622825622559,13.612211227416992,13.565166473388672,13.507110595703125,13.315988540649414,13.21446418762207,13.40166187286377]
[null,"Eight Mile Plains Bus 2","Substation Rating","MVA","Non-Coincident",27.5,27.5,27.5,27.5,27.5,27.5,27.5]
[null,null,null,null,"Coincident",27.5,27.5,27.5,27.5,27.5,27.5,27.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.79998779296875,15.698735237121582,15.801540374755859,15.831454277038574,15.82094669342041,16.06202507019043,16.316707611083984]
[null,null,null,null,"Coincident",15.101874351501465,15.005095481872559,15.103358268737793,15.131950378417969,15.121907234191895,15.352334022521973,15.595763206481934]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.809713363647461,15.707222938537598,15.811285018920898,15.841579437255859,15.830937385559082,16.075302124023437,16.333898544311523]
[null,null,null,null,"Coincident",15.369839668273926,15.271344184875488,15.371350288391113,15.400449752807617,15.390228271484375,15.624743461608887,15.872492790222168]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.458396911621094,13.390381813049316,13.440730094909668,13.47974681854248,13.464324951171875,13.634223937988281,13.845876693725586]
[null,null,null,null,"Coincident",12.863744735717773,12.798735618591309,12.846858978271484,12.884151458740234,12.869411468505859,13.031803131103516,13.234104156494141]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.382402420043945,14.309718132019043,14.363522529602051,14.405218124389648,14.388737678527832,14.570301055908203,14.79648494720459]
[null,null,null,null,"Coincident",13.086010932922363,13.019878387451172,13.068833351135254,13.106769561767578,13.091774940490723,13.256973266601563,13.462769508361816]
[null,"Enoggera","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.005268096923828,19.034818649291992,19.072092056274414,19.041130065917969,18.919858932495117,18.936620712280273,19.019277572631836]
[null,null,null,null,"Coincident",17.683923721313477,17.711420059204102,17.746101379394531,17.717290878295898,17.604452133178711,17.620048522949219,17.69696044921875]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.306524276733398,19.337913513183594,19.377508163452148,19.34461784362793,19.2158203125,19.233619689941406,19.321405410766602]
[null,null,null,null,"Coincident",18.008460998535156,18.036462783813477,18.071781158447266,18.042440414428711,17.927532196044922,17.943414688110352,18.021738052368164]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.187965393066406,17.238162994384766,17.224061965942383,17.213432312011719,17.0955810546875,17.066579818725586,17.135459899902344]
[null,null,null,null,"Coincident",15.992968559265137,16.039674758911133,16.026557922363281,16.016666412353516,15.90700626373291,15.880021095275879,15.944113731384277]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.382658004760742,17.43560791015625,17.420732498168945,17.409521102905273,17.285236358642578,17.254661560058594,17.32728385925293]
[null,null,null,null,"Coincident",16.286474227905273,16.334037780761719,16.3206787109375,16.310606002807617,16.198934555053711,16.171453475952148,16.236722946166992]
[null,"Esk","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5072498321533203,3.4657135009765625,3.4642870426177979,3.4518322944641113,3.4737064838409424,3.5135009288787842,3.514732837677002]
[null,null,null,null,"Coincident",3.5072498321533203,3.4657135009765625,3.4642870426177979,3.4518322944641113,3.4737064838409424,3.5135009288787842,3.514732837677002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6607415676116943,3.6173872947692871,3.615898609161377,3.6028988361358643,3.6257302761077881,3.6672661304473877,3.6685519218444824]
[null,null,null,null,"Coincident",3.6015479564666748,3.5588948726654053,3.5574300289154053,3.5446405410766602,3.5671029090881348,3.6079671382904053,3.6092321872711182]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0146808624267578,2.983039379119873,2.9735503196716309,2.965846061706543,2.983206033706665,3.0095961093902588,3.0096654891967773]
[null,null,null,null,"Coincident",3.0146808624267578,2.983039379119873,2.9735503196716309,2.965846061706543,2.983206033706665,3.0095961093902588,3.0096654891967773]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1466155052185059,3.1135895252227783,3.1036851406097412,3.0956437587738037,3.1137635707855225,3.1413083076477051,3.141380786895752]
[null,null,null,null,"Coincident",3.0957355499267578,3.0632433891296387,3.0534992218017578,3.0455877780914307,3.0634143352508545,3.0905139446258545,3.0905852317810059]
[null,"Eumundi","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.4734504222869873,3.4712169170379639,3.4693894386291504,3.455115795135498,3.4196751117706299,3.4075164794921875,3.417877197265625]
[null,null,null,null,"Coincident",2.9372434616088867,2.9353547096252441,2.9338095188140869,2.9217391014099121,2.8917694091796875,2.8814880847930908,2.8902492523193359]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.889030933380127,3.8865301609039307,3.8844840526580811,3.8685026168823242,3.8288214206695557,3.8152081966400146,3.8268084526062012]
[null,null,null,null,"Coincident",2.9543800354003906,2.9524803161621094,2.9509260654449463,2.9387853145599365,2.9086408615112305,2.8982994556427002,2.907111644744873]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2564287185668945,3.2587716579437256,3.248032808303833,3.2379295825958252,3.2031760215759277,3.1835522651672363,3.1921863555908203]
[null,null,null,null,"Coincident",2.7537238597869873,2.7557051181793213,2.7466237545013428,2.7380802631378174,2.7086915969848633,2.6920974254608154,2.6993982791900635]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.6460435390472412,3.6486668586730957,3.6366429328918457,3.6253311634063721,3.5864195823669434,3.5644478797912598,3.5741147994995117]
[null,null,null,null,"Coincident",2.7697899341583252,2.7717826366424561,2.762648344039917,2.7540550231933594,2.7244949340820313,2.7078039646148682,2.7151472568511963]
[null,"Fisherman Is A","Substation Rating","MVA","Non-Coincident",37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547]
[null,null,null,null,"Coincident",37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547,37.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.34602165222168,11.356537818908691,12.901923179626465,12.477254867553711,15.953643798828125,18.36793327331543,21.627645492553711]
[null,null,null,null,"Coincident",10.027606964111328,10.036900520324707,11.471856117248535,11.428915023803711,13.13276481628418,16.665021896362305,19.296041488647461]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.993625640869141,12.004741668701172,13.638334274291992,13.411725044250488,17.148475646972656,19.743579864501953,23.247425079345703]
[null,null,null,null,"Coincident",10.477787017822266,10.487497329711914,11.911312103271484,11.866726875305176,13.556792259216309,17.081331253051758,19.713747024536133]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.34614372253418,10.369851112365723,11.962313652038574,12.366228103637695,15.835165023803711,18.208267211914062,21.398077011108398]
[null,null,null,null,"Coincident",9.1583976745605469,9.1793842315673828,10.659370422363281,10.630173683166504,12.431612014770508,16.112773895263672,18.870695114135742]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.936676979064941,10.961737632751465,12.64509391784668,13.292383193969727,17.021121978759766,19.571956634521484,23.000663757324219]
[null,null,null,null,"Coincident",9.5532932281494141,9.5751838684082031,11.044014930725098,11.013765335083008,12.803839683532715,16.480842590332031,19.243047714233398]
[null,"Fisherman Is B","Substation Rating","MVA","Non-Coincident",26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547]
[null,null,null,null,"Coincident",26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547,26.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.158564567565918,4.158564567565918,4.158564567565918,4.158564567565918,4.158564567565918,4.158564567565918,4.158564567565918]
[null,null,null,null,"Coincident",2.6900436878204346,2.6900436878204346,2.6900436878204346,2.6900436878204346,2.6900436878204346,2.6900436878204346,2.6900436878204346]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.3167948722839355,4.3167948722839355,4.3167948722839355,4.3167948722839355,4.3167948722839355,4.3167948722839355,4.3167948722839355]
[null,null,null,null,"Coincident",2.8304731845855713,2.8304731845855713,2.8304731845855713,2.8304731845855713,2.8304731845855713,2.8304731845855713,2.8304731845855713]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.057136058807373,4.057136058807373,4.057136058807373,4.057136058807373,4.057136058807373,4.057136058807373,4.057136058807373]
[null,null,null,null,"Coincident",2.6244330406188965,2.6244330406188965,2.6244330406188965,2.6244330406188965,2.6244330406188965,2.6244330406188965,2.6244330406188965]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.2115073204040527,4.2115073204040527,4.2115073204040527,4.2115073204040527,4.2115073204040527,4.2115073204040527,4.2115073204040527]
[null,null,null,null,"Coincident",2.7614374160766602,2.7614374160766602,2.7614374160766602,2.7614374160766602,2.7614374160766602,2.7614374160766602,2.7614374160766602]
[null,"Flinders","Substation Rating","MVA","Non-Coincident",11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273]
[null,null,null,null,"Coincident",11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273,11.899999618530273]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0843973159790039,5.0266561508178711,5.0248270034790039,4.9999375343322754,4.9332246780395508,4.8823323249816895,4.8490562438964844]
[null,null,null,null,"Coincident",4.7225384712219238,4.6689066886901855,4.6672077178955078,4.6440896987915039,4.5821247100830078,4.5348544120788574,4.5039467811584473]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.3978748321533203,5.3365731239318848,5.3346314430236816,5.3082075119018555,5.2373814582824707,5.1833515167236328,5.1480236053466797]
[null,null,null,null,"Coincident",4.9997611045837402,4.9429812431335449,4.9411826133728027,4.9167070388793945,4.851104736328125,4.8010597229003906,4.7683377265930176]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.549067497253418,4.503537654876709,4.4894270896911621,4.4716911315917969,4.4099059104919434,4.3531522750854492,4.3220667839050293]
[null,null,null,null,"Coincident",4.2253084182739258,4.183018684387207,4.1699123382568359,4.1534390449523926,4.0960507392883301,4.0433363914489746,4.0144634246826172]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.8295388221740723,4.7812018394470215,4.7662215232849121,4.7473921775817871,4.6817975044250488,4.6215448379516602,4.5885424613952637]
[null,null,null,null,"Coincident",4.4733424186706543,4.4285702705383301,4.4146947860717773,4.397254467010498,4.3364973068237305,4.2806882858276367,4.2501206398010254]
[null,"Gatton A","Substation Rating","MVA","Non-Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,null,null,"Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.653890609741211,20.535364151000977,20.576391220092773,20.569822311401367,20.400966644287109,20.258033752441406,20.183538436889648]
[null,null,null,null,"Coincident",20.600479125976563,20.482257843017578,20.52318000793457,20.516628265380859,20.348207473754883,20.205644607543945,20.131341934204102]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.855379104614258,20.731420516967773,20.774322509765625,20.767452239990234,20.590921401977539,20.441564559936523,20.363748550415039]
[null,null,null,null,"Coincident",21.224250793457031,21.102449417114258,21.144611358642578,21.137861251831055,20.964340209960937,20.817461013793945,20.740907669067383]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.38658332824707,18.305992126464844,18.291749954223633,18.304340362548828,18.145353317260742,17.971735000610352,17.899784088134766]
[null,null,null,null,"Coincident",18.339035034179688,18.258651733398437,18.24444580078125,18.257003784179687,18.098428726196289,17.925258636474609,17.853494644165039]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.493070602416992,18.409492492675781,18.394723892211914,18.407779693603516,18.242988586425781,18.063169479370117,17.988693237304687]
[null,null,null,null,"Coincident",18.88606071472168,18.803279876708984,18.788650512695312,18.801582336425781,18.638277053833008,18.459941864013672,18.386037826538086]
[null,"Gaven","Substation Rating","MVA","Non-Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,null,null,"Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.663286209106445,30.646244049072266,30.788827896118164,30.807353973388672,30.586151123046875,30.477949142456055,30.485029220581055]
[null,null,null,null,"Coincident",30.369518280029297,30.352640151977539,30.493858337402344,30.512205123901367,30.293123245239258,30.185958862304688,30.192972183227539]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.933732986450195,30.916173934936523,31.063089370727539,31.082178115844727,30.85426139831543,30.742788314819336,30.750082015991211]
[null,null,null,null,"Coincident",30.412025451660156,30.394977569580078,30.537628173828125,30.556161880493164,30.334861755371094,30.226627349853516,30.233709335327148]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.173360824584961,26.194480895996094,26.243444442749023,26.285699844360352,26.084417343139648,25.925079345703125,25.922609329223633]
[null,null,null,null,"Coincident",25.952163696289063,25.973104476928711,26.021652221679688,26.06355094909668,25.863971710205078,25.705978393554688,25.703531265258789]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.31761360168457,26.339273452758789,26.389488220214844,26.432825088500977,26.226409912109375,26.063047409057617,26.060516357421875]
[null,null,null,null,"Coincident",25.961797714233398,25.982856750488281,26.031681060791016,26.073820114135742,25.873115539550781,25.714273452758789,25.711812973022461]
[null,"Geebung","Substation Rating","MVA","Non-Coincident",78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188]
[null,null,null,null,"Coincident",78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188,78.699996948242188]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.702907562255859,36.491043090820313,36.511837005615234,36.362262725830078,35.909809112548828,35.56878662109375,35.342174530029297]
[null,null,null,null,"Coincident",30.292593002319336,30.117731094360352,30.134893417358398,30.011444091796875,29.63801383972168,29.356550216674805,29.169519424438477]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.702919006347656,36.874305725097656,36.896644592285156,36.735992431640625,36.250759124755859,35.885772705078125,35.643600463867188]
[null,null,null,null,"Coincident",30.567045211791992,30.386445999145508,30.404170989990234,30.276687622070312,29.891157150268555,29.600673675537109,29.407697677612305]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.537071228027344,36.375686645507813,36.295581817626953,36.183326721191406,35.715919494628906,35.28546142578125,35.049171447753906]
[null,null,null,null,"Coincident",30.155721664428711,30.022523880004883,29.95640754699707,29.863758087158203,29.477987289428711,29.122709274291992,28.927690505981445]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.923759460449219,36.750408172607422,36.664413452148438,36.543960571289063,36.043163299560547,35.583038330078125,35.330917358398437]
[null,null,null,null,"Coincident",30.425680160522461,30.288129806518555,30.219860076904297,30.124198913574219,29.725992202758789,29.359405517578125,29.158241271972656]
[null,"Gibson Island","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.728382110595703,18.728382110595703,18.728382110595703,18.728382110595703,18.728382110595703,18.728382110595703,18.728382110595703]
[null,null,null,null,"Coincident",16.723184585571289,16.723184585571289,16.723184585571289,16.723184585571289,16.723184585571289,16.723184585571289,16.723184585571289]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.771797180175781,18.771797180175781,18.771797180175781,18.771797180175781,18.771797180175781,18.771797180175781,18.771797180175781]
[null,null,null,null,"Coincident",16.7783203125,16.7783203125,16.7783203125,16.7783203125,16.7783203125,16.7783203125,16.7783203125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.542953491210938,18.542953491210938,18.542953491210938,18.542953491210938,18.542953491210938,18.542953491210938,18.542953491210938]
[null,null,null,null,"Coincident",16.557609558105469,16.557609558105469,16.557609558105469,16.557609558105469,16.557609558105469,16.557609558105469,16.557609558105469]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.582380294799805,18.582380294799805,18.582380294799805,18.582380294799805,18.582380294799805,18.582380294799805,18.582380294799805]
[null,null,null,null,"Coincident",16.607954025268555,16.607954025268555,16.607954025268555,16.607954025268555,16.607954025268555,16.607954025268555,16.607954025268555]
[null,"Glenore Grove","Substation Rating","MVA","Non-Coincident",17.100000381469727,17.100000381469727,17.100000381469727,19.200000762939453,19.200000762939453,19.200000762939453,19.200000762939453]
[null,null,null,null,"Coincident",17.100000381469727,17.100000381469727,17.100000381469727,19.200000762939453,19.200000762939453,19.200000762939453,19.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.195989608764648,10.20920467376709,10.225588798522949,10.198236465454102,10.100725173950195,10.052454948425293,10.038376808166504]
[null,null,null,null,"Coincident",9.6865291595458984,9.6990842819213867,9.7146492004394531,9.6886625289916992,9.5960245132446289,9.5501670837402344,9.5367918014526367]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.343486785888672,10.357283592224121,10.3743896484375,10.345831871032715,10.244043350219727,10.193665504455566,10.178974151611328]
[null,null,null,null,"Coincident",9.7336549758911133,9.7465000152587891,9.7624244689941406,9.7358379364013672,9.6410808563232422,9.5941858291625977,9.5805091857910156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.8298215866088867,8.8533191680908203,8.8429603576660156,8.8281936645507812,8.7395801544189453,8.6753730773925781,8.6603860855102539]
[null,null,null,null,"Coincident",8.3886251449584961,8.41094970703125,8.4011077880859375,8.3870792388916016,8.3028926849365234,8.2418947219848633,8.227656364440918]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.9203290939331055,8.9447460174560547,8.9339818954467773,8.9186382293701172,8.8265819549560547,8.7599039077758789,8.7443428039550781]
[null,null,null,null,"Coincident",8.4092521667480469,8.4319658279418945,8.4219522476196289,8.407679557800293,8.3220481872558594,8.2600278854370117,8.2455539703369141]
[null,"Goodna","Substation Rating","MVA","Non-Coincident",27.5,27.5,27.5,27.5,27.5,27.5,27.5]
[null,null,null,null,"Coincident",27.5,27.5,27.5,27.5,27.5,27.5,27.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.343695640563965,14.427287101745605,14.567612648010254,14.665732383728027,14.666163444519043,14.737850189208984,14.918319702148438]
[null,null,null,null,"Coincident",13.869152069091797,13.949978828430176,14.085661888122559,14.180534362792969,14.180952072143555,14.250267028808594,14.424766540527344]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.490840911865234,14.575289726257324,14.717055320739746,14.816182136535645,14.816616058349609,14.889039039611816,15.071359634399414]
[null,null,null,null,"Coincident",13.945321083068848,14.026591300964355,14.163020133972168,14.258413314819336,14.258833885192871,14.328529357910156,14.503987312316895]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.543928146362305,12.634233474731445,12.721775054931641,12.820371627807617,12.81458568572998,12.843996047973633,12.997016906738281]
[null,null,null,null,"Coincident",12.128926277160645,12.216243743896484,12.30088996887207,12.396223068237305,12.390628814697266,12.419066429138184,12.567025184631348]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.672611236572266,12.763842582702637,12.852282524108887,12.951889991760254,12.946044921875,12.975756645202637,13.13034725189209]
[null,null,null,null,"Coincident",12.195537567138672,12.283334732055664,12.368446350097656,12.464303016662598,12.458678245544434,12.487271308898926,12.636042594909668]
[null,"Goomboorian","Substation Rating","MVA","Non-Coincident",8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633]
[null,null,null,null,"Coincident",8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633,8.8000001907348633]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5922660827636719,2.596827507019043,2.6027843952178955,2.5987992286682129,2.5791637897491455,2.5743203163146973,2.5784645080566406]
[null,null,null,null,"Coincident",2.1245241165161133,2.1282625198364258,2.1331448554992676,2.1298785209655762,2.113785982131958,2.1098167896270752,2.113213062286377]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.7948741912841797,2.7997920513153076,2.8062145709991455,2.8019177913665771,2.780747652053833,2.7755258083343506,2.7799937725067139]
[null,null,null,null,"Coincident",2.137192964553833,2.140953540802002,2.1458652019500732,2.1425793170928955,2.1263906955718994,2.1223978996276855,2.1258144378662109]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4212267398834229,2.4287943840026855,2.4276213645935059,2.4263472557067871,2.4068572521209717,2.3961389064788818,2.3992106914520264]
[null,null,null,null,"Coincident",1.9843465089797974,1.9905484914779663,1.9895871877670288,1.9885430335998535,1.9725695848464966,1.9637855291366577,1.966302752494812]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.610466480255127,2.6186256408691406,2.6173610687255859,2.6159873008728027,2.5949740409851074,2.5834178924560547,2.5867297649383545]
[null,null,null,null,"Coincident",1.996179461479187,2.0024185180664062,2.0014512538909912,2.0004010200500488,1.9843323230743408,1.9754958152770996,1.9780280590057373]
[null,"Grantham","Substation Rating","MVA","Non-Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,null,null,"Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.8815884590148926,6.8879666328430176,6.8936758041381836,6.8678717613220215,6.7846345901489258,6.7231221199035645,6.685882568359375]
[null,null,null,null,"Coincident",5.5974464416503906,5.6026344299316406,5.6072783470153809,5.5862894058227539,5.5185847282409668,5.4685506820678711,5.438260555267334]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2261395454406738,7.2328367233276367,7.2388319969177246,7.211735725402832,7.124330997467041,7.0597386360168457,7.020634651184082]
[null,null,null,null,"Coincident",5.8336606025695801,5.8390674591064453,5.843907356262207,5.8220324516296387,5.7514705657958984,5.6993250846862793,5.6677570343017578]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.8641071319580078,6.8798356056213379,6.8664617538452148,6.8476543426513672,6.7614102363586426,6.6828212738037109,6.6436295509338379]
[null,null,null,null,"Coincident",5.5832271575927734,5.5960206985473633,5.5851426124572754,5.5698447227478027,5.4996943473815918,5.4357705116271973,5.4038920402526855]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.2077827453613281,7.2242989540100098,7.2102556228637695,7.1905064582824707,7.0999441146850586,7.0174202919006348,6.9762663841247559]
[null,null,null,null,"Coincident",5.8307652473449707,5.8441262245178223,5.8327655792236328,5.8167896270751953,5.7435288429260254,5.6767711639404297,5.6434793472290039]
[null,"Grovely","Substation Rating","MVA","Non-Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,null,null,"Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.131149291992187,32.048309326171875,32.086757659912109,31.998115539550781,31.664434432983398,31.452079772949219,31.447900772094727]
[null,null,null,null,"Coincident",31.072793960571289,30.992683410644531,31.029865264892578,30.944141387939453,30.621452331542969,30.416091918945313,30.412050247192383]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.169929504394531,32.085636138916016,32.124755859375,32.034572601318359,31.695337295532227,31.47966194152832,31.475419998168945]
[null,null,null,null,"Coincident",31.085100173950195,31.004570007324219,31.04194450378418,30.955776214599609,30.631473541259766,30.425140380859375,30.421079635620117]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.708417892456055,27.674661636352539,27.631097793579102,27.582536697387695,27.281782150268555,27.028902053833008,27.016458511352539]
[null,null,null,null,"Coincident",26.795740127563477,26.763095855712891,26.720966339111328,26.674003601074219,26.383153915405273,26.138605117797852,26.126571655273438]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.206096649169922,28.170505523681641,28.124574661254883,28.07337760925293,27.756368637084961,27.489917755126953,27.476808547973633]
[null,null,null,null,"Coincident",26.795742034912109,26.763095855712891,27.260318756103516,27.212408065795898,26.915687561035156,26.666202545166016,26.653924942016602]
[null,"Gympie","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.023731231689453,25.91448974609375,25.944416046142578,25.874040603637695,25.608407974243164,25.443447113037109,25.377700805664063]
[null,null,null,null,"Coincident",25.762823104858398,25.65467643737793,25.684303283691406,25.614633560180664,25.351661682128906,25.1883544921875,25.123270034790039]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.161920547485352,26.047822952270508,26.079072952270508,26.005594253540039,25.728500366210938,25.556629180908203,25.488174438476563]
[null,null,null,null,"Coincident",25.796560287475586,25.68720817565918,25.7171630859375,25.646722793579102,25.380905151367187,25.215885162353516,25.150129318237305]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.152690887451172,23.086935043334961,23.049560546875,23.01020622253418,22.763027191162109,22.558042526245117,22.49238395690918]
[null,null,null,null,"Coincident",22.920564651489258,22.855466842651367,22.81846809387207,22.779506683349609,22.534805297851563,22.331876754760742,22.266880035400391]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.188373565673828,23.12095832824707,23.082656860351563,23.042339324951172,22.789396286010742,22.580022811889648,22.513034820556641]
[null,null,null,null,"Coincident",22.928997039794922,22.863494873046875,22.826269149780273,22.787073135375977,22.540969848632813,22.336978912353516,22.271659851074219]
[null,"Gympie North","Substation Rating","MVA","Non-Coincident",55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547]
[null,null,null,null,"Coincident",55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547,55.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.684991836547852,15.655131340026855,15.725754737854004,15.73551082611084,15.625747680664063,15.576322555541992,15.586859703063965]
[null,null,null,null,"Coincident",15.26961612701416,15.240547180175781,15.309300422668457,15.318799018859863,15.211943626403809,15.163825988769531,15.174084663391113]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.242944717407227,16.212020874023438,16.28515625,16.295261383056641,16.18159294128418,16.130409240722656,16.141321182250977]
[null,null,null,null,"Coincident",15.58057689666748,15.550915718078613,15.62106990814209,15.630762100219727,15.521730422973633,15.47263240814209,15.483099937438965]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.587554931640625,14.579634666442871,14.604831695556641,14.628622055053711,14.519597053527832,14.43632698059082,14.441362380981445]
[null,null,null,null,"Coincident",14.201242446899414,14.19353199005127,14.218061447143555,14.241222381591797,14.13508415222168,14.054018020629883,14.058919906616211]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.10646915435791,15.0982666015625,15.124361038208008,15.148996353149414,15.036093711853027,14.949861526489258,14.955076217651367]
[null,null,null,null,"Coincident",14.490446090698242,14.482579231262207,14.507607460021973,14.531240463256836,14.422940254211426,14.34022331237793,14.34522533416748]
[null,"Gympie South","Substation Rating","MVA","Non-Coincident",15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863]
[null,null,null,null,"Coincident",15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.68896484375,7.686312198638916,7.6818523406982422,7.6444964408874512,7.5516295433044434,7.4988455772399902,7.4876222610473633]
[null,null,null,null,"Coincident",7.0948009490966797,7.092353343963623,7.0882377624511719,7.0537686347961426,6.9680776596069336,6.91937255859375,6.9090170860290527]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7031660079956055,8.7001638412475586,8.6951150894165039,8.65283203125,8.5477161407470703,8.4879693984985352,8.4752655029296875]
[null,null,null,null,"Coincident",7.2843785285949707,7.281865119934082,7.2776398658752441,7.2422494888305664,7.154268741607666,7.1042623519897461,7.093630313873291]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6626238822937012,7.6704239845275879,7.6447339057922363,7.6152267456054687,7.519099235534668,7.4472775459289551,7.4336967468261719]
[null,null,null,null,"Coincident",7.07049560546875,7.077692985534668,7.0539884567260742,7.0267610549926758,6.9380617141723633,6.8717904090881348,6.8592591285705566]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.6733512878417969,8.6821794509887695,8.6531009674072266,8.6197013854980469,8.5108938217163086,8.4295997619628906,8.4142265319824219]
[null,null,null,null,"Coincident",7.2594237327575684,7.2668132781982422,7.2424755096435547,7.2145204544067383,7.123450756072998,7.0554089546203613,7.0425424575805664]
[null,"Hamilton","Substation Rating","MVA","Non-Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,null,null,"Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.63286018371582,22.666997909545898,22.794929504394531,22.83952522277832,22.674615859985352,22.553346633911133,22.531078338623047]
[null,null,null,null,"Coincident",21.069545745849609,21.101325988769531,21.220420837402344,21.261936187744141,21.108417510986328,20.995523452758789,20.974794387817383]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.131460189819336,23.168031692504883,23.30511474609375,23.352910995483398,23.176193237304688,23.046283721923828,23.022432327270508]
[null,null,null,null,"Coincident",21.691715240478516,21.724433898925781,21.8470458984375,21.889787673950195,21.731735229492187,21.615507125854492,21.594165802001953]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.258996963500977,20.317216873168945,20.375278472900391,20.43571662902832,20.278409957885742,20.117914199829102,20.091470718383789]
[null,null,null,null,"Coincident",18.859651565551758,18.913850784301758,18.967901229858398,19.024164199829102,18.877723693847656,18.728313446044922,18.703697204589844]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.595794677734375,20.657783508300781,20.719614028930664,20.783987045288086,20.616462707519531,20.445627212524414,20.417488098144531]
[null,null,null,null,"Coincident",19.41656494140625,19.47236442565918,19.528011322021484,19.585935592651367,19.435171127319336,19.281347274780273,19.256004333496094]
[null,"Hamilton Lands","Substation Rating","MVA","Non-Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,null,null,"Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.78544807434082,14.774797439575195,14.784977912902832,14.728102684020996,14.547621726989746,14.413017272949219,14.33098030090332]
[null,null,null,null,"Coincident",10.512664794921875,10.505091667175293,10.512330055236816,10.471891403198242,10.34356689453125,10.247860908508301,10.189531326293945]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.005080223083496,14.993608474731445,15.004573822021484,14.943326950073242,14.749161720275879,14.604544639587402,14.516488075256348]
[null,null,null,null,"Coincident",11.38453483581543,11.376334190368652,11.384172439575195,11.34037971496582,11.201413154602051,11.097769737243652,11.034602165222168]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.755775451660156,14.76524829864502,14.73448657989502,14.692599296569824,14.505577087402344,14.334281921386719,14.248023986816406]
[null,null,null,null,"Coincident",10.49156665802002,10.498302459716797,10.47642993927002,10.446647644042969,10.313672065734863,10.191879272460937,10.130548477172852]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.973122596740723,14.98332405090332,14.950200080871582,14.905108451843262,14.703971862792969,14.52003002166748,14.427509307861328]
[null,null,null,null,"Coincident",11.361687660217285,11.36898136138916,11.345294952392578,11.313042640686035,11.169038772583008,11.037144660949707,10.970727920532227]
[null,"Heathwood","Substation Rating","MVA","Non-Coincident",52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094]
[null,null,null,null,"Coincident",52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094,52.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.186941146850586,27.067081451416016,27.176303863525391,27.160591125488281,26.915939331054687,26.755239486694336,26.70734977722168]
[null,null,null,null,"Coincident",25.936622619628906,25.822275161743164,25.926473617553711,25.911483764648437,25.678083419799805,25.524774551391602,25.479087829589844]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.278776168823242,27.156570434570313,27.267929077148438,27.251907348632813,27.002498626708984,26.838722229003906,26.789922714233398]
[null,null,null,null,"Coincident",26.139217376708984,26.023975372314453,26.128988265991211,26.113882064819336,25.878658294677734,25.724151611328125,25.678108215332031]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.480510711669922,25.402761459350586,25.434602737426758,25.445516586303711,25.204196929931641,24.989072799682617,24.936176300048828]
[null,null,null,null,"Coincident",24.308670043945313,24.2344970703125,24.264873504638672,24.275285720825195,24.045063018798828,23.839832305908203,23.789369583129883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.541027069091797,25.461965560913086,25.494342803955078,25.505439758300781,25.260095596313477,25.041471481323242,24.987728118896484]
[null,null,null,null,"Coincident",24.49854850769043,24.423795700073242,24.454408645629883,24.464902877807617,24.232881546020508,24.02604866027832,23.975191116333008]
[null,"Helidon","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8751416206359863,2.8781917095184326,2.8881106376647949,2.8814105987548828,2.8540654182434082,2.8393826484680176,2.8351590633392334]
[null,null,null,null,"Coincident",2.8751416206359863,2.8781917095184326,2.8881106376647949,2.8814105987548828,2.8540654182434082,2.8393826484680176,2.8351590633392334]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.875476598739624,2.8785467147827148,2.8885347843170166,2.8817875385284424,2.8542771339416504,2.8395249843597412,2.8352837562561035]
[null,null,null,null,"Coincident",2.9323372840881348,2.935448169708252,2.9455642700195313,2.9387309551239014,2.9108419418334961,2.8958671092987061,2.891559362411499]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.478952169418335,2.4849650859832764,2.4866206645965576,2.4833524227142334,2.4586026668548584,2.4396431446075439,2.4352164268493652]
[null,null,null,null,"Coincident",2.478952169418335,2.4849650859832764,2.4866206645965576,2.4833524227142334,2.4586026668548584,2.4396431446075439,2.4352164268493652]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7010054588317871,2.7075569629669189,2.7093608379364014,2.7057998180389404,2.6788330078125,2.6581752300262451,2.6533520221710205]
[null,null,null,null,"Coincident",2.5198068618774414,2.5259189605712891,2.5276017189025879,2.5242795944213867,2.4991219043731689,2.4798500537872314,2.4753503799438477]
[null,"Hemmant","Substation Rating","MVA","Non-Coincident",26.799999237060547,29.600000381469727,29.600000381469727,29.600000381469727,29.600000381469727,29.600000381469727,29.600000381469727]
[null,null,null,null,"Coincident",26.799999237060547,29.600000381469727,29.600000381469727,29.600000381469727,29.600000381469727,29.600000381469727,29.600000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.6676816940307617,8.6291828155517578,8.6318693161010742,8.5950279235839844,8.486302375793457,8.4047679901123047,8.3535709381103516]
[null,null,null,null,"Coincident",7.86895751953125,7.8340067863464355,7.8364453315734863,7.8029990196228027,7.7042922973632812,7.6302714347839355,7.5837917327880859]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.6183872222900391,9.5756664276123047,9.5786476135253906,9.5377645492553711,9.4171142578125,9.3266363143920898,9.2698240280151367]
[null,null,null,null,"Coincident",8.0286464691162109,7.9929866790771484,7.9954743385314941,7.9613494873046875,7.8606395721435547,7.7851166725158691,7.7376937866210938]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6505727767944336,8.6238918304443359,8.6026763916015625,8.5745935440063477,8.4620561599731445,8.359130859375,8.3054914474487305]
[null,null,null,null,"Coincident",7.8534250259399414,7.8292026519775391,7.8099422454833984,7.784447193145752,7.6822800636291504,7.5888400077819824,7.5401430130004883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.5994024276733398,9.5697946548461914,9.5462522506713867,9.5150899887084961,9.3902082443237305,9.2759943008422852,9.2164707183837891]
[null,null,null,null,"Coincident",8.0127992630004883,7.9880847930908203,7.9684333801269531,7.9424209594726562,7.8381805419921875,7.7428445816040039,7.6931591033935547]
[null,"Hendra","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.563240051269531,18.457103729248047,18.460559844970703,18.379447937011719,18.144618988037109,17.967933654785156,17.856100082397461]
[null,null,null,null,"Coincident",17.230312347412109,17.131797790527344,17.135005950927734,17.059719085693359,16.841751098632812,16.677753448486328,16.573949813842773]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.67304801940918,18.562965393066406,18.566549301147461,18.482454299926758,18.239164352416992,18.05628776550293,17.940614700317383]
[null,null,null,null,"Coincident",17.57676887512207,17.476274490356445,17.479547500610352,17.402746200561523,17.180395126342773,17.013099670410156,16.907209396362305]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.75880241394043,16.685699462890625,16.642589569091797,16.586166381835937,16.366376876831055,16.165191650390625,16.059318542480469]
[null,null,null,null,"Coincident",15.555441856384277,15.487587928771973,15.447573661804199,15.39520263671875,15.191194534301758,15.004456520080566,14.906185150146484]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.809196472167969,16.734067916870117,16.689777374267578,16.631830215454102,16.406290054321289,16.200122833251953,16.091739654541016]
[null,null,null,null,"Coincident",15.868222236633301,15.799003601074219,15.758184432983398,15.704760551452637,15.496650695800781,15.306157112121582,15.205909729003906]
[null,"Herring Lagoon","Substation Rating","MVA","Non-Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,null,null,"Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1730000972747803,2.1730000972747803,2.1730000972747803,2.1730000972747803,2.1730000972747803,2.1730000972747803,2.1730000972747803]
[null,null,null,null,"Coincident",1.2513917684555054,1.2513917684555054,1.2513917684555054,1.2513917684555054,1.2513917684555054,1.2513917684555054,1.2513917684555054]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4559345245361328,2.4559345245361328,2.4559345245361328,2.4559345245361328,2.4559345245361328,2.4559345245361328,2.4559345245361328]
[null,null,null,null,"Coincident",1.2791647911071777,1.2791647911071777,1.2791647911071777,1.2791647911071777,1.2791647911071777,1.2791647911071777,1.2791647911071777]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1200001239776611,2.1200001239776611,2.1200001239776611,2.1200001239776611,2.1200001239776611,2.1200001239776611,2.1200001239776611]
[null,null,null,null,"Coincident",1.2208700180053711,1.2208700180053711,1.2208700180053711,1.2208700180053711,1.2208700180053711,1.2208700180053711,1.2208700180053711]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.396033763885498,2.396033763885498,2.396033763885498,2.396033763885498,2.396033763885498,2.396033763885498,2.396033763885498]
[null,null,null,null,"Coincident",1.2479656934738159,1.2479656934738159,1.2479656934738159,1.2479656934738159,1.2479656934738159,1.2479656934738159,1.2479656934738159]
[null,"Holland Park","Substation Rating","MVA","Non-Coincident",42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906]
[null,null,null,null,"Coincident",42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906,42.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.541366577148438,24.362119674682617,24.217979431152344,24.106418609619141,23.970281600952148,24.012870788574219,24.085887908935547]
[null,null,null,null,"Coincident",23.208185195922852,23.038679122924805,22.902366638183594,22.796867370605469,22.668125152587891,22.708396911621094,22.777448654174805]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.55803108215332,26.364053726196289,26.20806884765625,26.08734130859375,25.94001579284668,25.986104965209961,26.06512451171875]
[null,null,null,null,"Coincident",23.596416473388672,23.424074172973633,23.285482406616211,23.178218841552734,23.047321319580078,23.088268280029297,23.158473968505859]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.224004745483398,22.091762542724609,21.900213241577148,21.821300506591797,21.687637329101563,21.670112609863281,21.728889465332031]
[null,null,null,null,"Coincident",21.016712188720703,20.891653060913086,20.710508346557617,20.635883331298828,20.509481430053711,20.492908477783203,20.548490524291992]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.050241470336914,23.907133102416992,23.69984245300293,23.614444732666016,23.469799041748047,23.450834274291992,23.514440536499023]
[null,null,null,null,"Coincident",21.368284225463867,21.241132736206055,21.056957244873047,20.981084823608398,20.852567672729492,20.835718154907227,20.892229080200195]
[null,"Holland Park East","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.6717529296875,19.583667755126953,19.501003265380859,19.410144805908203,19.249992370605469,19.242034912109375,19.347455978393555]
[null,null,null,null,"Coincident",17.988094329833984,17.907548904418945,17.831958770751953,17.748874664306641,17.60243034362793,17.595155715942383,17.691553115844727]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.718257904052734,19.628318786621094,19.543943405151367,19.45123291015625,19.287899017333984,19.279787063598633,19.387287139892578]
[null,null,null,null,"Coincident",18.528223037719727,18.445259094238281,18.367399215698242,18.281820297241211,18.130977630615234,18.123485565185547,18.222776412963867]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.600076675415039,17.545156478881836,17.422693252563477,17.35899543762207,17.207492828369141,17.156002044677734,17.244344711303711]
[null,null,null,null,"Coincident",16.093729019165039,16.043510437011719,15.931527137756348,15.87328052520752,15.734745025634766,15.687660217285156,15.76844310760498]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.611789703369141,17.55622673034668,17.432388305664062,17.368007659912109,17.214973449707031,17.162992477416992,17.252185821533203]
[null,null,null,null,"Coincident",16.576974868774414,16.525247573852539,16.409902572631836,16.349906921386719,16.207212448120117,16.158712387084961,16.241922378540039]
[null,"Hollywell","Substation Rating","MVA","Non-Coincident",59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094]
[null,null,null,null,"Coincident",59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094,59.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.144313812255859,39.15777587890625,39.177318572998047,39.019229888916016,38.636848449707031,38.516822814941406,38.574775695800781]
[null,null,null,null,"Coincident",37.509178161621094,37.522079467773437,37.540805816650391,37.389316558837891,37.022914886474609,36.90789794921875,36.963428497314453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.175846099853516,39.189468383789063,39.209243774414063,39.049289703369141,38.662609100341797,38.541290283203125,38.599864959716797]
[null,null,null,null,"Coincident",37.568981170654297,37.582008361816406,37.600917816162109,37.447959899902344,37.078060150146484,36.961963653564453,37.018013000488281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.944648742675781,35.004329681396484,34.924770355224609,34.818889617919922,34.461105346679688,34.265411376953125,34.30572509765625]
[null,null,null,null,"Coincident",33.484939575195312,33.542129516601563,33.465892791748047,33.364437103271484,33.021598815917969,32.834075927734375,32.872711181640625]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.945503234863281,35.005317687988281,34.925579071044922,34.819488525390625,34.461227416992188,34.265422821044922,34.305751800537109]
[null,null,null,null,"Coincident",33.510643005371094,33.568241119384766,33.491462707519531,33.389293670654297,33.044105529785156,32.855339050292969,32.89422607421875]
[null,"Hope Island","Substation Rating","MVA","Non-Coincident",58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094]
[null,null,null,null,"Coincident",58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094,58.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.892223358154297,40.974071502685547,41.073215484619141,41.011001586914062,40.645206451416016,40.457794189453125,40.462375640869141]
[null,null,null,null,"Coincident",38.622268676757813,38.699569702148438,38.793209075927734,38.734451293945313,38.388961791992188,38.211956024169922,38.216281890869141]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.601432800292969,41.686687469482422,41.789962768554687,41.725154876708984,41.344146728515625,41.148956298828125,41.153732299804688]
[null,null,null,null,"Coincident",38.761421203613281,38.839916229248047,38.935009002685547,38.875339508056641,38.524524688720703,38.344814300537109,38.349208831787109]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.779064178466797,33.892822265625,33.880702972412109,33.863475799560547,33.545299530029297,33.304473876953125,33.297336578369141]
[null,null,null,null,"Coincident",31.903966903686523,32.011405944824219,31.999959945678711,31.983692169189453,31.683177947998047,31.455718994140625,31.448976516723633]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.204666137695313,34.322723388671875,34.310142517089844,34.292263031005859,33.96209716796875,33.712245941162109,33.704841613769531]
[null,null,null,null,"Coincident",31.953102111816406,32.061721801757812,32.050148010253906,32.033702850341797,31.729923248291016,31.500049591064453,31.493236541748047]
[null,"Ibis","Substation Rating","MVA","Non-Coincident",12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727]
[null,null,null,null,"Coincident",12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727,12.100000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.15083856880664825,0.15245690941810608,0.15455551445484161,0.15712589025497437,0.16108901798725128,0.16836792230606079,0.1763397753238678]
[null,null,null,null,"Coincident",3.232254832983017E-2,3.2669335603713989E-2,3.3119037747383118E-2,3.3669833093881607E-2,3.4519072622060776E-2,3.6078836768865585E-2,3.7787090986967087E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.19996924698352814,0.20211470127105713,0.20489688217639923,0.20830446481704712,0.21355845034122467,0.22320820391178131,0.23377662897109985]
[null,null,null,null,"Coincident",3.4070957452058792E-2,3.4436501562595367E-2,3.4910529851913452E-2,3.549112007021904E-2,3.6386296153068542E-2,3.8030434399843216E-2,3.9831090718507767E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.15053583681583405,0.15235835313796997,0.15402770042419434,0.15674713253974915,0.16062344610691071,0.16744814813137054,0.17531903088092804]
[null,null,null,null,"Coincident",3.2257676124572754E-2,3.2648216933012009E-2,3.3005934208631516E-2,3.3588670194149017E-2,3.4419309347867966E-2,3.5881742835044861E-2,3.7568360567092896E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.19956791400909424,0.20198406279087067,0.20419712364673615,0.20780232548713684,0.2129412442445755,0.22198884189128876,0.23242340981960297]
[null,null,null,null,"Coincident",3.4002576023340225E-2,3.4414242953062057E-2,3.4791309386491776E-2,3.5405565053224564E-2,3.628113865852356E-2,3.7822678685188293E-2,3.960052877664566E-2]
[null,"Imbil","Substation Rating","MVA","Non-Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,null,null,"Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3698086738586426,2.3431098461151123,2.3405489921569824,2.3379416465759277,2.3352880477905273,2.3325879573822021,2.3298428058624268]
[null,null,null,null,"Coincident",1.732293963432312,1.7127776145935059,1.7109056711196899,1.7089997529983521,1.7070599794387817,1.7050862312316895,1.7030795812606812]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4003086090087891,2.3707594871520996,2.3679308891296387,2.3650519847869873,2.3621232509613037,2.3591439723968506,2.3561165332794189]
[null,null,null,null,"Coincident",1.8703091144561768,1.8492379188537598,1.8472168445587158,1.8451590538024902,1.8430647850036621,1.8409337997436523,1.8387671709060669]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3120086193084717,2.2859609127044678,2.2834625244140625,2.2809188365936279,2.2783300876617432,2.27569580078125,2.273017406463623]
[null,null,null,null,"Coincident",1.6900429725646973,1.6710026264190674,1.6691763401031494,1.6673169136047363,1.6654244661331177,1.6634988784790039,1.6615411043167114]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3364760875701904,2.3078823089599609,2.3051455020904541,2.3023602962493896,2.2995269298553467,2.2966446876525879,2.2937154769897461]
[null,null,null,null,"Coincident",1.8246918916702271,1.8041346073150635,1.8021628856658936,1.8001552820205688,1.7981120347976685,1.7960330247879028,1.7939193248748779]
[null,"Inala","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.718021392822266,33.683914184570313,33.838943481445312,33.867107391357422,33.642726898193359,33.552410125732422,33.862438201904297]
[null,null,null,null,"Coincident",32.844100952148438,32.810878753662109,32.961887359619141,32.989322662353516,32.770759582519531,32.682777404785156,32.984771728515625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.389049530029297,34.353096008300781,34.516529083251953,34.546222686767578,34.309680938720703,34.2144775390625,34.541301727294922]
[null,null,null,null,"Coincident",32.925125122070313,32.891403198242188,33.044685363769531,33.072536468505859,32.850685119628906,32.761390686035156,33.067916870117188]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.103078842163086,31.113979339599609,31.170581817626953,31.227970123291016,31.006162643432617,30.843135833740234,31.117937088012695]
[null,null,null,null,"Coincident",30.296932220458984,30.307548522949219,30.36268424987793,30.418584823608398,30.202526092529297,30.043725967407227,30.311403274536133]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.635581970214844,31.64704704284668,31.706575393676758,31.766935348510742,31.533664703369141,31.362247467041016,31.651208877563477]
[null,null,null,null,"Coincident",30.343109130859375,30.353857040405273,30.40966796875,30.466259002685547,30.247554779052734,30.086847305297852,30.357757568359375]
[null,"Indooroopilly","Substation Rating","MVA","Non-Coincident",54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094]
[null,null,null,null,"Coincident",54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094,54.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.257772445678711,24.177774429321289,24.19395637512207,24.09889030456543,23.802408218383789,23.579921722412109,23.434329986572266]
[null,null,null,null,"Coincident",23.617713928222656,23.539825439453125,23.555582046508789,23.463024139404297,23.17436408996582,22.957748413085938,22.815998077392578]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.264291763305664,24.1834716796875,24.19981575012207,24.103830337524414,23.804967880249023,23.581193923950195,23.434995651245117]
[null,null,null,null,"Coincident",24.20745849609375,24.127626419067383,24.143775939941406,24.048906326293945,23.75303840637207,23.531013488769531,23.385725021362305]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.600330352783203,22.55650520324707,22.509069442749023,22.44322395324707,22.156454086303711,21.892721176147461,21.750421524047852]
[null,null,null,null,"Coincident",22.004003524780273,21.961336135864258,21.915151596069336,21.851043701171875,21.571840286254883,21.315065383911133,21.176521301269531]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.187713623046875,23.140411376953125,23.089214324951172,23.018157958984375,22.708816528320313,22.424505233764648,22.271177291870117]
[null,null,null,null,"Coincident",22.55345344543457,22.509721755981445,22.462383270263672,22.396673202514648,22.110498428344727,21.847312927246094,21.70530891418457]
[null,"Innisplain","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6249723434448242,4.6317696571350098,4.6390576362609863,4.6263518333435059,4.5653753280639648,4.5602922439575195,4.5634841918945313]
[null,null,null,null,"Coincident",3.930004358291626,3.9357802867889404,3.9419732093811035,3.9311766624450684,3.8930747509002686,3.8736865520477295,3.8674542903900146]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.6462244987487793,4.6532034873962402,4.6606869697570801,4.6476407051086426,4.5657534599304199,4.5606546401977539,4.5638566017150879]
[null,null,null,null,"Coincident",3.9300086498260498,3.9357845783233643,3.9419775009155273,3.9311809539794922,3.8930790424346924,3.8736908435821533,3.8674585819244385]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.3051667213439941,4.3173723220825195,4.3121857643127441,4.3047094345092773,4.2762575149536133,4.2588205337524414,4.2465229034423828]
[null,null,null,null,"Coincident",3.6582539081573486,3.6686253547668457,3.6642179489135742,3.6578652858734131,3.6206710338592529,3.5933444499969482,3.5863883495330811]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.3185086250305176,4.3309917449951172,4.3256869316101074,4.3180408477783203,4.279149055480957,4.2615671157836914,4.249168872833252]
[null,null,null,null,"Coincident",3.6582579612731934,3.6686294078826904,3.6642220020294189,3.6578693389892578,3.6206750869750977,3.5933482646942139,3.5863921642303467]
[null,"Ipswich South","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.246450424194336,22.151355743408203,22.069864273071289,21.978609085083008,21.816856384277344,21.799348831176758,21.842279434204102]
[null,null,null,null,"Coincident",21.06092643737793,20.97089958190918,20.89375114440918,20.80735969543457,20.654226303100586,20.637653350830078,20.678298950195313]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.06092643737793,20.97089958190918,20.89375114440918,20.80735969543457,20.654226303100586,20.637653350830078,20.678298950195313]
[null,null,null,null,"Coincident",21.400432586669922,21.308954238891602,21.230562210083008,21.142778396606445,20.987176895141602,20.9703369140625,21.011636734008789]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.400432586669922,21.308954238891602,21.230562210083008,21.142778396606445,20.987176895141602,20.9703369140625,21.011636734008789]
[null,null,null,null,"Coincident",18.366132736206055,18.312557220458984,18.19464111328125,18.137670516967773,17.99553108215332,17.934696197509766,17.964132308959961]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.405309677124023,19.348339080810547,19.222995758056641,19.16246223449707,19.011495590209961,18.94691276550293,18.978160858154297]
[null,null,null,null,"Coincident",18.662199020385742,18.607759475708008,18.487941741943359,18.4300537109375,18.285623550415039,18.223808288574219,18.253717422485352]
[null,"Jimboomba","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",48,48,48,48,48,48,48]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.038042068481445,31.164417266845703,31.38817024230957,32.407234191894531,33.191062927246094,33.152805328369141,33.231922149658203]
[null,null,null,null,"Coincident",28.78411865234375,28.901317596435547,29.108821868896484,30.062210083007812,30.7972412109375,30.761611938476563,30.834892272949219]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.241621017456055,31.371337890625,31.601047515869141,32.647800445556641,33.453525543212891,33.414188385009766,33.495540618896484]
[null,null,null,null,"Coincident",29.180868148803711,29.2996826171875,29.510046005249023,30.489912033081055,31.248279571533203,31.2119140625,31.286056518554687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.598867416381836,26.743579864501953,26.860967636108398,27.950248718261719,28.792509078979492,28.682167053222656,28.738273620605469]
[null,null,null,null,"Coincident",24.667304992675781,24.801509857177734,24.910371780395508,25.929302215576172,26.718925476074219,26.616395950317383,26.668327331542969]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.696332931518555,26.844100952148438,26.9639892578125,28.077419281005859,28.939434051513672,28.826454162597656,28.883901596069336]
[null,null,null,null,"Coincident",25.007308959960937,25.143363952636719,25.253726959228516,26.300741195678711,27.115175247192383,27.010904312133789,27.063385009765625]
[null,"Jindalee","Substation Rating","MVA","Non-Coincident",35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094]
[null,null,null,null,"Coincident",35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094,35.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.839570999145508,16.72767448425293,16.729301452636719,16.703712463378906,16.580583572387695,16.48365592956543,16.426347732543945]
[null,null,null,null,"Coincident",16.839570999145508,16.72767448425293,16.729301452636719,16.703712463378906,16.580583572387695,16.48365592956543,16.426347732543945]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.881320953369141,16.76666259765625,16.768329620361328,16.742120742797852,16.616060256958008,16.51689338684082,16.458290100097656]
[null,null,null,null,"Coincident",17.207790374755859,17.093446731567383,17.095108032226563,17.068960189819336,16.943140029907227,16.844091415405273,16.785530090332031]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.679875373840332,14.602211952209473,14.563172340393066,14.55555248260498,14.441313743591309,14.319849014282227,14.26539134979248]
[null,null,null,null,"Coincident",14.679875373840332,14.602211952209473,14.563172340393066,14.55555248260498,14.441313743591309,14.319849014282227,14.26539134979248]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.683854103088379,14.605532646179199,14.566183090209961,14.558505058288574,14.443451881408691,14.321259498596191,14.266523361206055]
[null,null,null,null,"Coincident",15.000869750976562,14.921507835388184,14.881614685058594,14.873827934265137,14.757091522216797,14.632970809936523,14.577322006225586]
[null,"Kalbar","Substation Rating","MVA","Non-Coincident",17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547]
[null,null,null,null,"Coincident",17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547,17.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.9633684158325195,6.8875946998596191,6.8854107856750488,6.851630687713623,6.7605400085449219,6.716249942779541,6.8253922462463379]
[null,null,null,null,"Coincident",6.1232132911682129,6.056581974029541,6.0546612739562988,6.0249571800231934,5.9448566436767578,5.9059104919433594,6.0018844604492187]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.0428080558776855,6.9613556861877441,6.959010124206543,6.9227495193481445,6.8251252174377441,6.7777423858642578,6.8946051597595215]
[null,null,null,null,"Coincident",6.2110652923583984,6.1407632827758789,6.1387372016906738,6.1074113845825195,6.0229806900024414,5.9819531440734863,6.0830845832824707]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4832034111022949,6.4213967323303223,6.4015750885009766,6.3765897750854492,6.2887907028198242,6.231471061706543,6.3306617736816406]
[null,null,null,null,"Coincident",5.700981616973877,5.646632194519043,5.6292023658752441,5.607231616973877,5.5300254821777344,5.4796218872070313,5.5668449401855469]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5293865203857422,6.46380615234375,6.4428014755249023,6.4163432121276855,6.3235387802124023,6.263099193572998,6.3677635192871094]
[null,null,null,null,"Coincident",5.7663421630859375,5.7092399597167969,5.6909351348876953,5.6678662300109863,5.5868496894836426,5.5339994430541992,5.6254768371582031]
[null,"Kallangur","Substation Rating","MVA","Non-Coincident",44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094]
[null,null,null,null,"Coincident",44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094,44.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.185874938964844,38.476139068603516,38.663730621337891,38.786663055419922,38.526390075683594,40.486713409423828,42.709957122802734]
[null,null,null,null,"Coincident",36.895553588867188,37.176006317138672,37.357261657714844,37.476039886474609,37.224559783935547,39.118644714355469,41.266761779785156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.506523132324219,38.804531097412109,38.997150421142578,39.123386383056641,38.856128692626953,40.487129211425781,42.717193603515625]
[null,null,null,null,"Coincident",37.27532958984375,37.558670043945313,37.741790771484375,37.861793518066406,37.607723236083984,39.120468139648438,41.275211334228516]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.60441780090332,31.84465217590332,31.999912261962891,32.101657867431641,31.88624382019043,33.847583770751953,36.022117614746094]
[null,null,null,null,"Coincident",30.53648567199707,30.76860237121582,30.918617248535156,31.016923904418945,30.808788299560547,32.703853607177734,34.804908752441406]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.763355255126953,32.008926391601563,32.167659759521484,32.271694183349609,32.051445007324219,34.058231353759766,36.286460876464844]
[null,null,null,null,"Coincident",30.850807189941406,31.08531379699707,31.236871719360352,31.336191177368164,31.125911712646484,33.062240600585937,35.206974029541016]
[null,"Karrabin","Substation Rating","MVA","Non-Coincident",34.5,34.5,34.5,34.5,34.5,34.5,34.5]
[null,null,null,null,"Coincident",34.5,34.5,34.5,34.5,34.5,34.5,34.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.121799468994141,19.174264907836914,19.283729553222656,19.338144302368164,19.295343399047852,19.356897354125977,19.459098815917969]
[null,null,null,null,"Coincident",17.814435958862305,17.863315582275391,17.965291976928711,18.015987396240234,17.976112365722656,18.033456802368164,18.128669738769531]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.156501770019531,19.209959030151367,19.321531295776367,19.377010345458984,19.333370208740234,19.396133422851563,19.500375747680664]
[null,null,null,null,"Coincident",18.219078063964844,18.269067764282227,18.373359680175781,18.425207138061523,18.384426116943359,18.443073272705078,18.540449142456055]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.231712341308594,17.30255126953125,17.353118896484375,17.419624328613281,17.372713088989258,17.383167266845703,17.46922492980957]
[null,null,null,null,"Coincident",16.05357551574707,16.119571685791016,16.166681289672852,16.228641510009766,16.1849365234375,16.194675445556641,16.274850845336914]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.239107131958008,17.310640335083008,17.361721038818359,17.428922653198242,17.38151741027832,17.392080307006836,17.479059219360352]
[null,null,null,null,"Coincident",16.418220520019531,16.485715866088867,16.533895492553711,16.597263336181641,16.55256462097168,16.562524795532227,16.644521713256836]
[null,"Kawana","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.465272903442383,27.233959197998047,27.231884002685547,27.191577911376953,27.142642974853516,27.170370101928711,27.168949127197266]
[null,null,null,null,"Coincident",27.067092895507812,26.839132308959961,26.837087631225586,26.797365188598633,26.749139785766602,26.776466369628906,26.775064468383789]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.419919967651367,29.172143936157227,29.169919967651367,29.126745223999023,29.074329376220703,29.104028701782227,29.102506637573242]
[null,null,null,null,"Coincident",27.849277496337891,27.614728927612305,27.612625122070313,27.571754455566406,27.522136688232422,27.550252914428711,27.548810958862305]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.868057250976563,25.685169219970703,25.612056732177734,25.599924087524414,25.541568756103516,25.501691818237305,25.492006301879883]
[null,null,null,null,"Coincident",25.493032455444336,25.312795639038086,25.240743637084961,25.228786468505859,25.17127799987793,25.131978988647461,25.122434616088867]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.709033966064453,27.513130187988281,27.434812545776367,27.421817779541016,27.359308242797852,27.316593170166016,27.306219100952148]
[null,null,null,null,"Coincident",26.229730606079102,26.044284820556641,25.970149993896484,25.957847595214844,25.898677825927734,25.858242034912109,25.848423004150391]
[null,"Kedron","Substation Rating","MVA","Non-Coincident",56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094]
[null,null,null,null,"Coincident",56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094,56.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.04412841796875,28.798927307128906,28.796674728393555,28.662391662597656,28.288364410400391,28.027669906616211,28.433383941650391]
[null,null,null,null,"Coincident",27.457611083984375,27.225803375244141,27.223674774169922,27.096725463867188,26.743129730224609,26.496675491333008,26.880228042602539]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.165288925170898,28.911201477050781,28.908868789672852,28.769834518432617,28.38300895690918,28.113784790039063,28.532913208007813]
[null,null,null,null,"Coincident",27.463018417358398,27.23036003112793,27.22822380065918,27.100837707519531,26.746131896972656,26.498998641967773,26.883640289306641]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.307254791259766,26.120723724365234,26.046318054199219,25.950986862182617,25.600030899047852,25.298666000366211,25.656473159790039]
[null,null,null,null,"Coincident",24.870237350463867,24.69389533996582,24.623554229736328,24.533430099487305,24.201644897460938,23.916742324829102,24.2550048828125]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.345844268798828,26.155153274536133,26.079147338867188,25.981813430786133,25.62397575378418,25.317333221435547,25.681472778320313]
[null,null,null,null,"Coincident",24.870246887207031,25.192401885986328,25.120641708374023,25.028697967529297,24.690214157104492,24.399560928344727,24.744651794433594]
[null,"Kelvin Grove","Substation Rating","MVA","Non-Coincident",131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562]
[null,null,null,null,"Coincident",131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562,131.60000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.785909652709961,19.723052978515625,19.783937454223633,20.259798049926758,20.555419921875,20.901884078979492,21.318149566650391]
[null,null,null,null,"Coincident",18.994855880737305,18.934513092041016,18.992961883544922,19.449798583984375,19.733600616455078,20.066213607788086,20.465835571289063]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.786981582641602,19.724000930786133,19.785005569458008,20.262029647827148,20.558570861816406,20.906290054321289,21.324306488037109]
[null,null,null,null,"Coincident",19.238033294677734,19.176918029785156,19.236114501953125,19.698799133300781,19.986234664916992,20.32310676574707,20.72784423828125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.785078048706055,17.752748489379883,17.758216857910156,18.203680038452148,18.460422515869141,18.723142623901367,19.089763641357422]
[null,null,null,null,"Coincident",17.074018478393555,17.04298210144043,17.04823112487793,17.475885391235352,17.722362518310547,17.974578857421875,18.326541900634766]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.137086868286133,18.104118347167969,18.109695434570313,18.563976287841797,18.825799942016602,19.093717575073242,19.089879989624023]
[null,null,null,null,"Coincident",17.292604446411133,17.261171340942383,17.266487121582031,17.699615478515625,17.949249267578125,18.204694747924805,18.561162948608398]
[null,"Kenilworth","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",6,6,6,6,6,6,6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6834416389465332,4.6527042388916016,4.6335244178771973,4.6114039421081543,4.6534371376037598,4.6234798431396484,4.6027398109436035]
[null,null,null,null,"Coincident",3.6893751621246338,3.6486306190490723,3.6474153995513916,3.6294624805450439,3.5811500549316406,3.5443224906921387,3.5202827453613281]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.8074607849121094,4.7759099006652832,4.7562222480773926,4.733515739440918,4.7766623497009277,4.7459115982055664,4.7246222496032715]
[null,null,null,null,"Coincident",3.706002950668335,3.6650748252868652,3.6638541221618652,3.645820140838623,3.5972900390625,3.5602965354919434,3.5361485481262207]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4866476058959961,4.4485735893249512,4.423621654510498,4.3924665451049805,4.4243769645690918,4.3828492164611816,4.3475470542907715]
[null,null,null,null,"Coincident",3.5722744464874268,3.537639856338501,3.5266637802124023,3.5128419399261475,3.4644157886505127,3.4199419021606445,3.3956339359283447]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.6054558753967285,4.5663738250732422,4.5407609939575195,4.5087809562683105,4.5415363311767578,4.4989089965820313,4.4626717567443848]
[null,null,null,null,"Coincident",3.5883743762969971,3.5535838603973389,3.5425581932067871,3.5286741256713867,3.4800295829772949,3.4353554248809814,3.4109377861022949]
[null,"Kenmore","Substation Rating","MVA","Non-Coincident",59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453]
[null,null,null,null,"Coincident",59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.251865386962891,36.093105316162109,35.906658172607422,35.693878173828125,35.186058044433594,34.872852325439453,35.164890289306641]
[null,null,null,null,"Coincident",34.157691955566406,34.008102416992188,33.832427978515625,33.631938934326172,33.153453826904297,32.858341217041016,33.133510589599609]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.665496826171875,36.501392364501953,36.308685302734375,36.088787078857422,35.564098358154297,35.240570068359375,35.542228698730469]
[null,null,null,null,"Coincident",34.568733215332031,34.417343139648438,34.239555358886719,34.036651611328125,33.552410125732422,33.253746032714844,33.5322265625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.296640396118164,30.205081939697266,29.965801239013672,29.818248748779297,29.379890441894531,29.043241500854492,29.276866912841797]
[null,null,null,null,"Coincident",28.546482086181641,28.460214614868164,28.234758377075195,28.095729827880859,27.682695388793945,27.365489959716797,27.585622787475586]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.522058486938477,30.42784309387207,30.181661605834961,30.029882431030273,29.579111099243164,29.233074188232422,29.473199844360352]
[null,null,null,null,"Coincident",28.889999389648437,28.802694320678711,28.574525833129883,28.43382453918457,28.015819549560547,27.694795608520508,27.917577743530273]
[null,"Kilcoy","Substation Rating","MVA","Non-Coincident",10.699999809265137,10.699999809265137,10.699999809265137,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863]
[null,null,null,null,"Coincident",10.699999809265137,10.699999809265137,10.699999809265137,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.333026885986328,11.344333648681641,11.360509872436523,11.329178810119629,11.212751388549805,11.142125129699707,11.11219596862793]
[null,null,null,null,"Coincident",9.8596973419189453,9.8695335388183594,9.8836069107055664,9.856348991394043,9.7550573348999023,9.6936111450195313,9.6675748825073242]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.514396667480469,11.526389122009277,11.543547630310059,11.359833717346191,11.240104675292969,11.16755199432373,11.136824607849121]
[null,null,null,null,"Coincident",9.8718137741088867,9.8818035125732422,9.8960990905761719,9.868412971496582,9.7655887603759766,9.7032566070556641,9.6768550872802734]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.847745895385742,10.873372077941895,10.858710289001465,10.839676856994629,10.723122596740723,10.628086090087891,10.596068382263184]
[null,null,null,null,"Coincident",9.4375038146972656,9.4597978591918945,9.4470415115356445,9.4304828643798828,9.3290815353393555,9.2464008331298828,9.2185459136962891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.000359535217285,11.027469635009766,11.011958122253418,10.857538223266602,10.738377571105957,10.641348838806152,10.608687400817871]
[null,null,null,null,"Coincident",9.4438276290893555,9.4663867950439453,9.4534778594970703,9.4367246627807617,9.3341884613037109,9.2506589889526367,9.2225341796875]
[null,"Kingston","Substation Rating","MVA","Non-Coincident",59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906]
[null,null,null,null,"Coincident",59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.764057159423828,35.604999542236328,35.653614044189453,35.705764770507812,35.533790588378906,35.554065704345703,35.783409118652344]
[null,null,null,null,"Coincident",35.306838989257812,35.149814605712891,35.197811126708984,35.249294281005859,35.079513549804688,35.099533081054688,35.325946807861328]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.776313781738281,35.615978240966797,35.66497802734375,35.717544555664062,35.544216156005859,35.564647674560547,35.795825958251953]
[null,null,null,null,"Coincident",35.395763397216797,35.236648559570312,35.285282135009766,35.337451934814453,35.165420532226563,35.185703277587891,35.415126800537109]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.886711120605469,32.785087585449219,32.738899230957031,32.819831848144531,32.646053314208984,32.580398559570313,32.779827117919922]
[null,null,null,null,"Coincident",32.466281890869141,32.365955352783203,32.320358276367187,32.400257110595703,32.22869873046875,32.163887023925781,32.360767364501953]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.325843811035156,33.220165252685547,33.172138214111328,33.256294250488281,33.075599670410156,33.007335662841797,33.214694976806641]
[null,null,null,null,"Coincident",32.520164489746094,32.418712615966797,32.372608184814453,32.453399658203125,32.279933929443359,32.214412689208984,32.413467407226563]
[null,"Kirra","Substation Rating","MVA","Non-Coincident",24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727]
[null,null,null,null,"Coincident",24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727,24.100000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.281040191650391,17.252700805664063,17.262744903564453,17.193807601928711,16.981081008911133,16.822742462158203,16.725135803222656]
[null,null,null,null,"Coincident",16.591753005981445,16.564542770385742,16.574186325073242,16.507999420166016,16.303756713867187,16.151735305786133,16.058021545410156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.448183059692383,17.41834831237793,17.428922653198242,17.356363296508789,17.132631301879883,16.966270446777344,16.863792419433594]
[null,null,null,null,"Coincident",17.219442367553711,17.191202163696289,17.201211929321289,17.13252067565918,16.920551300048828,16.762777328491211,16.665519714355469]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.769378662109375,16.764703750610352,16.727989196777344,16.677980422973633,16.463714599609375,16.268121719360352,16.168434143066406]
[null,null,null,null,"Coincident",16.100500106811523,16.096010208129883,16.060760498046875,16.012746810913086,15.807027816772461,15.619235038757324,15.523525238037109]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.910236358642578,16.905328750610352,16.866786956787109,16.814304351806641,16.589614868164063,16.384759902954102,16.280450820922852]
[null,null,null,null,"Coincident",16.709604263305664,16.704944610595703,16.668361663818359,16.618532180786133,16.405029296875,16.210132598876953,16.110801696777344]
[null,"Labrador","Substation Rating","MVA","Non-Coincident",44.700000762939453,60,60,60,60,60,60]
[null,null,null,null,"Coincident",44.700000762939453,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.963729858398438,24.002546310424805,24.050085067749023,24.013425827026367,23.842084884643555,23.821981430053711,23.903474807739258]
[null,null,null,null,"Coincident",23.158529281616211,23.196041107177734,23.241985321044922,23.20655632019043,23.040969848632812,23.02154541015625,23.100297927856445]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.351938247680664,24.392940521240234,24.443161010742188,24.404434204101563,24.22346305847168,24.202232360839844,24.288295745849609]
[null,null,null,null,"Coincident",23.175741195678711,23.213619232177734,23.260017395019531,23.224237442016602,23.05705451965332,23.037446975708008,23.116947174072266]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.989356994628906,22.055002212524414,22.03746223449707,22.026046752929688,21.858371734619141,21.783596038818359,21.850957870483398]
[null,null,null,null,"Coincident",21.250495910644531,21.313934326171875,21.29698371887207,21.285953521728516,21.123910903930664,21.051645278930664,21.116743087768555]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.270759582519531,22.339805603027344,22.321355819702148,22.309349060058594,22.133024215698242,22.054414749145508,22.125228881835938]
[null,null,null,null,"Coincident",21.253795623779297,21.317535400390625,21.300502777099609,21.289419174194336,21.126649856567383,21.054084777832031,21.119451522827148]
[null,"Laidley","Substation Rating","MVA","Non-Coincident",19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727]
[null,null,null,null,"Coincident",19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727,19.100000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.393303871154785,13.395191192626953,13.405483245849609,13.366745948791504,13.236781120300293,13.176774978637695,13.18439769744873]
[null,null,null,null,"Coincident",12.97331714630127,12.975146293640137,12.985115051269531,12.947591781616211,12.82170295715332,12.763578414916992,12.770961761474609]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.452095985412598,13.454038619995117,13.464634895324707,13.42475700378418,13.291023254394531,13.229308128356934,13.237146377563477]
[null,null,null,null,"Coincident",12.983865737915039,12.985696792602539,12.995673179626465,12.95811939239502,12.832128524780273,12.773956298828125,12.781346321105957]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.423523902893066,11.44071102142334,11.417780876159668,11.396261215209961,11.280031204223633,11.199923515319824,11.202732086181641]
[null,null,null,null,"Coincident",11.065305709838867,11.081954002380371,11.059741973876953,11.038897514343262,10.926311492919922,10.848715782165527,10.851436614990234]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.436378479003906,11.453842163085938,11.430542945861816,11.40868091583252,11.290671348571777,11.209406852722168,11.212255477905273]
[null,null,null,null,"Coincident",11.074302673339844,11.090965270996094,11.068735122680664,11.047873497009277,10.935195922851563,10.857537269592285,10.860260009765625]
[null,"Landsborough","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.051082611083984,12.145412445068359,12.855751037597656,13.515423774719238,13.469411849975586,13.50287914276123,13.615796089172363]
[null,null,null,null,"Coincident",11.920804023742676,12.014115333557129,12.75076961517334,13.437051773071289,13.390715599060059,13.423214912414551,13.534543991088867]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.372880935668945,12.469728469848633,13.19903564453125,13.876323699951172,13.829083442687988,13.863443374633789,13.979376792907715]
[null,null,null,null,"Coincident",12.126014709472656,12.220932960510254,13.021326065063477,13.774673461914063,13.726167678833008,13.758167266845703,13.870711326599121]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.800375938415527,10.89975643157959,11.600546836853027,12.297861099243164,12.248447418212891,12.245038986206055,12.340815544128418]
[null,null,null,null,"Coincident",10.683618545532227,10.781925201416016,11.510831832885742,12.236104011535645,12.18632698059082,12.182138442993164,12.276473045349121]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.088776588439941,11.190810203552246,11.910313606262207,12.626248359680176,12.575515747070313,12.572015762329102,12.67034912109375]
[null,null,null,null,"Coincident",10.867531776428223,10.967531204223633,11.763033866882324,12.56003475189209,12.507874488830566,12.50218677520752,12.597348213195801]
[null,"Lawnton","Substation Rating","MVA","Non-Coincident",45.599998474121094,48.799999237060547,48.799999237060547,48.799999237060547,48.799999237060547,48.799999237060547,48.799999237060547]
[null,null,null,null,"Coincident",45.599998474121094,48.799999237060547,48.799999237060547,48.799999237060547,48.799999237060547,48.799999237060547,48.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.905231475830078,35.948535919189453,36.392116546630859,36.622966766357422,36.460884094238281,36.460674285888672,36.687160491943359]
[null,null,null,null,"Coincident",34.006610870361328,34.047626495361328,34.467754364013672,34.686393737792969,34.532878875732422,34.532680511474609,34.7471923828125]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.938217163085937,35.982120513916016,36.432117462158203,36.666492462158203,36.501922607421875,36.501708984375,36.731689453125]
[null,null,null,null,"Coincident",34.046184539794922,34.087562561035156,34.511474609375,34.732131958007813,34.577194213867188,34.576995849609375,34.793495178222656]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.168071746826172,31.248207092285156,31.546148300170898,31.778253555297852,31.622402191162109,31.540632247924805,31.726163864135742]
[null,null,null,null,"Coincident",29.506912231445313,29.58277702331543,29.864837646484375,30.084573745727539,29.937026977539063,29.859613418579102,30.035255432128906]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.617395401000977,31.701023101806641,31.546175003051758,31.778484344482422,31.622474670410156,31.540657043457031,31.72633171081543]
[null,null,null,null,"Coincident",29.514549255371094,29.590751647949219,29.874128341674805,30.094949722290039,29.94666862487793,29.868879318237305,30.045383453369141]
[null,"Lockrose","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.599841117858887,10.647570610046387,10.695338249206543,10.699870109558105,10.631978988647461,10.629082679748535,10.695998191833496]
[null,null,null,null,"Coincident",9.4406661987304687,9.4831771850585937,9.5257205963134766,9.5297574996948242,9.4692907333374023,9.4667110443115234,9.5263090133666992]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.005892753601074,11.055451393127441,11.105048179626465,11.10975456237793,11.039262771606445,11.0362548828125,11.105733871459961]
[null,null,null,null,"Coincident",9.6133394241333008,9.6566276550292969,9.6999492645263672,9.7040596008300781,9.6424875259399414,9.6398601531982422,9.7005481719970703]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.1966085433959961,9.250615119934082,9.2663717269897461,9.2796421051025391,9.2163295745849609,9.1900472640991211,9.2448740005493164]
[null,null,null,null,"Coincident",8.1908884048461914,8.2389898300170898,8.2530221939086914,8.2648410797119141,8.2084531784057617,8.1850442886352539,8.2338762283325195]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.5489063262939453,9.6049823760986328,9.6213417053222656,9.6351203918457031,9.5693826675415039,9.5420942306518555,9.5990209579467773]
[null,null,null,null,"Coincident",8.3407020568847656,8.389683723449707,8.4039726257324219,8.4160079956054687,8.3585882186889648,8.3347511291503906,8.3844766616821289]
[null,"Logan Village","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.734045028686523,12.563075065612793,13.396675109863281,14.171628952026367,14.832905769348145,15.545919418334961,16.308380126953125]
[null,null,null,null,"Coincident",10.780959129333496,11.542651176452637,12.308542251586914,13.020551681518555,13.628116607666016,14.28321647644043,14.983746528625488]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.018269538879395,12.86738109588623,13.721172332763672,14.514897346496582,15.192192077636719,15.922476768493652,16.703405380249023]
[null,null,null,null,"Coincident",10.81285572052002,11.576801300048828,12.344958305358887,13.059074401855469,13.668437004089355,14.325474739074707,15.028077125549316]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.137269973754883,10.868282318115234,11.557319641113281,12.238195419311523,12.803095817565918,13.383914947509766,14.035740852355957]
[null,null,null,null,"Coincident",9.3138809204101562,9.9855184555053711,10.618587493896484,11.244160652160645,11.763177871704102,12.296820640563965,12.895702362060547]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.382817268371582,11.131536483764648,11.837264060974121,12.534631729125977,13.113215446472168,13.708103179931641,14.375718116760254]
[null,null,null,null,"Coincident",9.3414373397827148,10.015061378479004,10.650003433227539,11.277427673339844,11.797980308532715,12.333202362060547,12.933855056762695]
[null,"Loganholme","Substation Rating","MVA","Non-Coincident",39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547]
[null,null,null,null,"Coincident",39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547,39.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.884355545043945,27.606733322143555,27.600484848022461,27.467624664306641,27.105010986328125,26.829307556152344,26.650415420532227]
[null,null,null,null,"Coincident",27.779788970947266,27.503208160400391,27.496982574462891,27.364620208740234,27.003366470336914,26.728696823120117,26.55047607421875]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.964504241943359,27.678155899047852,27.671716690063477,27.534833908081055,27.161748886108398,26.878595352172852,26.695112228393555]
[null,null,null,null,"Coincident",27.919340133666992,27.636053085327148,27.629678726196289,27.494144439697266,27.124362945556641,26.84333610534668,26.661050796508789]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.811494827270508,25.589351654052734,25.512680053710938,25.415458679199219,25.067882537841797,24.748880386352539,24.575807571411133]
[null,null,null,null,"Coincident",25.714700698852539,25.493391036987305,25.417007446289063,25.320150375366211,24.973876953125,24.656070709228516,24.483648300170898]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.837348937988281,25.610994338989258,25.532949447631836,25.434043884277344,25.081003189086914,24.757770538330078,24.582727432250977]
[null,null,null,null,"Coincident",25.806884765625,25.580898284912109,25.502920150756836,25.404056549072266,25.050746917724609,24.726678848266602,24.550939559936523]
[null,"Loganlea","Substation Rating","MVA","Non-Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,null,null,"Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.530618667602539,16.424980163574219,16.426982879638672,16.353715896606445,16.143669128417969,15.98536491394043,15.884750366210938]
[null,null,null,null,"Coincident",14.96074104309082,14.865134239196777,14.866946220397949,14.800638198852539,14.610539436340332,14.467267990112305,14.376209259033203]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.543769836425781,16.436708450317383,16.438737869262695,16.364524841308594,16.151968002319336,15.991971969604492,15.890376091003418]
[null,null,null,null,"Coincident",15.323129653930664,15.225207328796387,15.227063179016113,15.159149169921875,14.964445114135742,14.817704200744629,14.72443962097168]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.937705993652344,15.85744571685791,15.815441131591797,15.760770797729492,15.550861358642578,15.358639717102051,15.256973266601563]
[null,null,null,null,"Coincident",14.424135208129883,14.351497650146484,14.313482284545898,14.264003753662109,14.074028968811035,13.90006160736084,13.808050155639648]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.943839073181152,15.86281681060791,15.820432662963867,15.765287399291992,15.553762435913086,15.360361099243164,15.25818920135498]
[null,null,null,null,"Coincident",14.773526191711426,14.699129104614258,14.660192489624023,14.609516143798828,14.414939880371094,14.236758232116699,14.142518043518066]
[null,"Lomandra Drive","Substation Rating","MVA","Non-Coincident",null,null,null,55,55,55,55]
[null,null,null,null,"Coincident",null,null,null,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident",null,null,null,"SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident",null,null,null,"SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",null,null,null,0,0,0,0]
[null,null,null,null,"Coincident",null,null,null,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",null,null,null,5.4549756050109863,5.4513859748840332,5.4474773406982422,5.4436964988708496]
[null,null,null,null,"Coincident",null,null,null,4.6242704391479492,4.6212272644042969,4.6179137229919434,4.6147089004516602]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",null,null,null,6.121180534362793,6.1171526908874512,6.1127667427062988,6.1085243225097656]
[null,null,null,null,"Coincident",null,null,null,5.1359066963195801,5.1325268745422363,5.1288466453552246,5.1252870559692383]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",null,null,null,5.1513071060180664,5.1479167938232422,5.1442255973815918,5.140655517578125]
[null,null,null,null,"Coincident",null,null,null,4.3668456077575684,4.3639717102050781,4.3608427047729492,4.357816219329834]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",null,null,null,5.780426025390625,5.7766213417053223,5.7724795341491699,5.7684736251831055]
[null,null,null,null,"Coincident",null,null,null,4.8499999046325684,4.8468079566955566,4.8433327674865723,4.8399715423583984]
[null,"Lota","Substation Rating","MVA","Non-Coincident",40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547]
[null,null,null,null,"Coincident",40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547,40.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.884294509887695,27.869041442871094,27.852268218994141,27.674089431762695,27.406272888183594,27.428550720214844,27.526622772216797]
[null,null,null,null,"Coincident",22.958162307739258,22.945602416992188,22.931793212890625,22.785089492797852,22.564586639404297,22.582929611206055,22.663673400878906]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.187082290649414,28.171192169189453,28.153720855712891,27.968149185180664,27.689313888549805,27.712503433227539,27.814599990844727]
[null,null,null,null,"Coincident",23.236642837524414,23.223930358886719,23.209955215454102,23.061471939086914,22.838293075561523,22.85685920715332,22.938583374023438]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.058408737182617,25.078845977783203,24.994316101074219,24.85944938659668,24.607038497924805,24.563499450683594,24.643253326416016]
[null,null,null,null,"Coincident",20.631509780883789,20.648334503173828,20.578737258911133,20.467697143554687,20.259878158569336,20.224031448364258,20.289693832397461]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.250284194946289,25.271467208862305,25.183853149414063,25.044099807739258,24.782648086547852,24.737564086914063,24.820152282714844]
[null,null,null,null,"Coincident",20.881769180297852,20.898797988891602,20.82835578918457,20.715969085693359,20.50562858581543,20.46934700012207,20.535806655883789]
[null,"Lowood","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1964550018310547,3.1685798168182373,3.168245792388916,3.153383731842041,3.1121461391448975,3.0808858871459961,3.0607430934906006]
[null,null,null,null,"Coincident",3.030517578125,3.00408935546875,3.0037727355957031,2.9896821975708008,2.9505853652954102,2.9209480285644531,2.9018509387969971]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.4387438297271729,3.4087557792663574,3.4083964824676514,3.3924076557159424,3.3480443954467773,3.3144147396087646,3.2927451133728027]
[null,null,null,null,"Coincident",3.205399751663208,3.1774466037750244,3.1771116256713867,3.162208080291748,3.1208548545837402,3.0895073413848877,3.0693082809448242]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8256981372833252,2.8048751354217529,2.7968094348907471,2.7864956855773926,2.7487342357635498,2.7141036987304687,2.6954760551452637]
[null,null,null,null,"Coincident",2.6790077686309814,2.6592657566070557,2.6516187191009521,2.6418404579162598,2.60603928565979,2.5732064247131348,2.5555458068847656]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.0398838520050049,3.0174825191497803,3.008805513381958,2.9977099895477295,2.9570860862731934,2.9198305606842041,2.8997910022735596]
[null,null,null,null,"Coincident",2.8336055278778076,2.8127241134643555,2.804635763168335,2.7942931652069092,2.7564260959625244,2.721698522567749,2.7030186653137207]
[null,"Lytton A","Substation Rating","MVA","Non-Coincident",74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906]
[null,null,null,null,"Coincident",74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906,74.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.937889099121094,26.937889099121094,26.937889099121094,26.937889099121094,26.937889099121094,26.937889099121094,26.937889099121094]
[null,null,null,null,"Coincident",24.733985900878906,24.733985900878906,24.733985900878906,24.733985900878906,24.733985900878906,24.733985900878906,24.733985900878906]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.008033752441406,27.008033752441406,27.008033752441406,27.008033752441406,27.008033752441406,27.008033752441406,27.008033752441406]
[null,null,null,null,"Coincident",25.200674057006836,25.200674057006836,25.200674057006836,25.200674057006836,25.200674057006836,25.200674057006836,25.200674057006836]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.671176910400391,26.671176910400391,26.671176910400391,26.671176910400391,26.671176910400391,26.671176910400391,26.671176910400391]
[null,null,null,null,"Coincident",24.489095687866211,24.489095687866211,24.489095687866211,24.489095687866211,24.489095687866211,24.489095687866211,24.489095687866211]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.72955322265625,26.72955322265625,26.72955322265625,26.72955322265625,26.72955322265625,26.72955322265625,26.72955322265625]
[null,null,null,null,"Coincident",24.930900573730469,24.930900573730469,24.930900573730469,24.930900573730469,24.930900573730469,24.930900573730469,24.930900573730469]
[null,"Lytton B","Substation Rating","MVA","Non-Coincident",52.5,52.5,52.5,52.5,52.5,52.5,52.5]
[null,null,null,null,"Coincident",52.5,52.5,52.5,52.5,52.5,52.5,52.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.496793746948242,17.618688583374023,17.739057540893555,17.778024673461914,17.666650772094727,17.609626770019531,17.614667892456055]
[null,null,null,null,"Coincident",11.549755096435547,11.630218505859375,11.709674835205078,11.735398292541504,11.661879539489746,11.624237060546875,11.627564430236816]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.105253219604492,18.241094589233398,18.37530517578125,18.418767929077148,18.294563293457031,18.230993270874023,18.236612319946289]
[null,null,null,null,"Coincident",11.80096435546875,11.883177757263184,11.964362144470215,11.990645408630371,11.91552734375,11.877066612243652,11.880466461181641]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.354602813720703,17.499332427978516,17.570072174072266,17.626419067382813,17.507574081420898,17.406036376953125,17.405317306518555]
[null,null,null,null,"Coincident",11.455894470214844,11.551430702209473,11.598127365112305,11.635321617126465,11.55687141418457,11.489846229553223,11.489371299743652]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.94688606262207,18.108081817626953,18.186906814575195,18.249711990356445,18.117263793945312,18.004159927368164,18.003358840942383]
[null,null,null,null,"Coincident",11.705061912536621,11.802676200866699,11.850388526916504,11.888391494750977,11.808235168457031,11.739752769470215,11.739267349243164]
[null,"Makerston St","Substation Rating","MVA","Non-Coincident",157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781]
[null,null,null,null,"Coincident",157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781,157.30000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",65.237686157226563,65.444488525390625,65.652008056640625,66.428375244140625,68.318405151367188,70.369659423828125,70.974884033203125]
[null,null,null,null,"Coincident",60.2047119140625,60.395557403564453,60.587070465087891,61.303543090820312,63.047756195068359,64.940765380859375,65.499298095703125]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",65.284217834472656,65.494674682617188,65.70599365234375,66.497673034667969,68.319252014160156,70.382110595703125,70.993232727050781]
[null,null,null,null,"Coincident",60.231128692626953,60.395565032958984,60.587116241455078,61.304039001464844,63.059597015380859,64.978805541992187,65.541450500488281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",64.46112060546875,64.753616333007813,64.778984069824219,65.611091613769531,67.552001953125,69.501914978027344,70.073738098144531]
[null,null,null,null,"Coincident",59.488056182861328,59.757987976074219,59.781398773193359,60.549308776855469,62.340480804443359,64.139961242675781,64.667671203613281]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64.495063781738281,64.792083740234375,64.817855834960937,65.664321899414063,67.646453857421875,69.507843017578125,70.083709716796875]
[null,null,null,null,"Coincident",59.509906768798828,59.781513214111328,59.805072784423828,60.549343109130859,62.349853515625,64.173828125,64.705215454101563]
[null,"Maleny","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.6107091903686523,8.6399374008178711,8.5988836288452148,8.5631113052368164,8.6714601516723633,8.6865177154541016,8.7528038024902344]
[null,null,null,null,"Coincident",6.4199466705322266,6.4126849174499512,6.4064979553222656,6.3788967132568359,6.3160529136657715,6.3025293350219727,6.3359708786010742]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.6207456588745117,8.650242805480957,8.6088113784790039,8.5727148056030273,8.6820592880249023,8.6972589492797852,8.7641754150390625]
[null,null,null,null,"Coincident",6.4681916236877441,6.4608755111694336,6.4546418190002441,6.4268331527709961,6.3635172843933105,6.3498921394348145,6.3835849761962891]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.9354853630065918,7.9470090866088867,7.8974404335021973,7.8466572761535645,7.931370735168457,7.9215669631958008,7.953399658203125]
[null,null,null,null,"Coincident",6.1931815147399902,6.1946101188659668,6.1714878082275391,6.1510930061340332,6.0875654220581055,6.0588583946228027,6.089012622833252]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9401149749755859,7.9517168998718262,7.9018168449401855,7.8507051467895508,7.9359726905822754,7.9261035919189453,7.9581508636474609]
[null,null,null,null,"Coincident",6.2397222518920898,6.2411618232727051,6.2178654670715332,6.1973176002502441,6.1333127021789551,6.1043896675109863,6.1347708702087402]
[null,"Mango Hill Bus 1","Substation Rating","MVA","Non-Coincident",28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727]
[null,null,null,null,"Coincident",28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727,28.600000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.873405456542969,27.21125602722168,27.552450180053711,27.610645294189453,27.464483261108398,27.374774932861328,27.399869918823242]
[null,null,null,null,"Coincident",24.529565811157227,24.837949752807617,25.149385452270508,25.202507019042969,25.069089889526367,24.987205505371094,25.010114669799805]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.875892639160156,27.21478271484375,27.557193756103516,27.61561393737793,27.468896865844727,27.378864288330078,27.404048919677734]
[null,null,null,null,"Coincident",24.578426361083984,24.887424468994141,25.199480056762695,25.252708435058594,25.119026184082031,25.036977767944336,25.059932708740234]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.810897827148438,23.129165649414063,23.354291915893555,23.427211761474609,23.2919921875,23.156013488769531,23.169651031494141]
[null,null,null,null,"Coincident",20.821380615234375,21.111888885498047,21.317380905151367,21.383939743041992,21.260515213012695,21.136394500732422,21.148843765258789]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.329988479614258,23.655500411987305,23.885749816894531,23.960329055786133,23.822032928466797,23.682958602905273,23.696907043457031]
[null,null,null,null,"Coincident",20.862855911254883,21.153942108154297,21.359844207763672,21.426534652709961,21.302864074707031,21.178497314453125,21.190971374511719]
[null,"Mango Hill Bus 2","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.462804794311523,30.587055206298828,30.883575439453125,30.864595413208008,30.585643768310547,30.345756530761719,30.214561462402344]
[null,null,null,null,"Coincident",30.462804794311523,30.587055206298828,30.883575439453125,30.864595413208008,30.585643768310547,30.345756530761719,30.214561462402344]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.472572326660156,30.597427368164063,30.895456314086914,30.876377105712891,30.59600830078125,30.35496711730957,30.223167419433594]
[null,null,null,null,"Coincident",30.465688705444336,30.590261459350586,30.887615203857422,30.868579864501953,30.588846206665039,30.348350524902344,30.216848373413086]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.052753448486328,27.200128555297852,27.387725830078125,27.398481369018555,27.13780403137207,26.855489730834961,26.730630874633789]
[null,null,null,null,"Coincident",27.052753448486328,27.200128555297852,27.387725830078125,27.398481369018555,27.13780403137207,26.855489730834961,26.730630874633789]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.052873611450195,27.200353622436523,27.388128280639648,27.398895263671875,27.137979507446289,26.855520248413086,26.730634689331055]
[null,null,null,null,"Coincident",27.541921615600586,27.691961288452148,27.882951736450195,27.893901824951172,27.628509521484375,27.341091156005859,27.213973999023438]
[null,"Marburg","Substation Rating","MVA","Non-Coincident",7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367]
[null,null,null,null,"Coincident",7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.633965015411377,4.5665683746337891,4.5634708404541016,4.6157889366149902,4.6530356407165527,4.6515622138977051,4.657808780670166]
[null,null,null,null,"Coincident",4.2895922660827637,4.2272043228149414,4.224337100982666,4.2727670669555664,4.3072457313537598,4.3058819770812988,4.3116641044616699]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9169597625732422,4.8454470634460449,4.842160701751709,4.8976736068725586,4.93719482421875,4.935631275177002,4.9422597885131836]
[null,null,null,null,"Coincident",4.3565354347229004,4.2931737899780273,4.2902617454528809,4.3394474983215332,4.3744645118713379,4.3730792999267578,4.3789515495300293]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.0531787872314453,3.9996745586395264,3.9858884811401367,4.0356478691101074,4.0662574768066406,4.0544824600219727,4.0585970878601074]
[null,null,null,null,"Coincident",3.751967191696167,3.7024390697479248,3.6896777153015137,3.7357392311096191,3.7640740871429443,3.753173828125,3.7569830417633057]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.3007049560546875,4.2439332008361816,4.2293047904968262,4.2821030616760254,4.314582347869873,4.3020882606506348,4.3064541816711426]
[null,null,null,null,"Coincident",3.8105201721191406,3.7602190971374512,3.7472586631774902,3.7940390110015869,3.8228161334991455,3.8117456436157227,3.8156144618988037]
[null,"McLachlan St","Substation Rating","MVA","Non-Coincident",125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891]
[null,null,null,null,"Coincident",125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891,125.90000152587891]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197]
[null,null,null,null,"Coincident",0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197,0.91739237308502197]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.4256591796875,52.065948486328125,52.263099670410156,52.615711212158203,52.498989105224609,52.509132385253906,52.736888885498047]
[null,null,null,null,"Coincident",46.77777099609375,47.371612548828125,47.554462432861328,47.881492614746094,47.773239135742188,47.782646179199219,47.993881225585938]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.426353454589844,52.068740844726563,52.266815185546875,52.621391296386719,52.503971099853516,52.514175415039062,52.743335723876953]
[null,null,null,null,"Coincident",46.778106689453125,47.371631622314453,47.554534912109375,47.881748199462891,47.773414611816406,47.782821655273438,47.99420166015625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.697410583496094,49.426200866699219,49.475460052490234,49.857887268066406,49.721893310546875,49.601818084716797,49.799213409423828]
[null,null,null,null,"Coincident",44.247432708740234,44.923355102539062,44.969039916992187,45.323726654052734,45.197597503662109,45.086235046386719,45.269309997558594]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.905521392822266,49.660354614257813,49.711414337158203,50.108009338378906,49.966941833496094,49.842422485351563,50.047142028808594]
[null,null,null,null,"Coincident",44.491920471191406,45.189792633056641,45.236278533935547,45.597518920898437,45.468708038330078,45.354969024658203,45.541316986083984]
[null,"Meeandah","Substation Rating","MVA","Non-Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,null,null,"Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.243659973144531,26.239721298217773,26.259073257446289,26.159002304077148,25.839662551879883,25.602245330810547,25.457880020141602]
[null,null,null,null,"Coincident",21.775711059570313,21.772443771362305,21.78849983215332,21.705467224121094,21.440494537353516,21.243495941162109,21.123708724975586]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.820228576660156,26.815868377685547,26.837287902832031,26.726547241210937,26.373569488525391,26.111560821533203,25.952423095703125]
[null,null,null,null,"Coincident",22.369256973266602,22.365716934204102,22.383121490478516,22.293119430541992,22.006031036376953,21.792713165283203,21.663057327270508]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.259368896484375,25.290012359619141,25.238544464111328,25.167705535888672,24.848520278930664,24.556682586669922,24.410215377807617]
[null,null,null,null,"Coincident",20.958993911743164,20.984420776367188,20.941715240478516,20.882936477661133,20.618091583251953,20.375940322875977,20.25440788269043]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.733827590942383,25.767553329467773,25.710910797119141,25.632980346679688,25.282272338867188,24.962257385253906,24.801887512207031]
[null,null,null,null,"Coincident",21.484838485717773,21.512344360351562,21.466148376464844,21.402572631835938,21.116243362426758,20.854639053344727,20.723413467407227]
[null,"Merrimac","Substation Rating","MVA","Non-Coincident",63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906]
[null,null,null,null,"Coincident",63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906,63.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.076509475708008,29.004222869873047,29.01423454284668,28.906377792358398,28.60137939453125,28.500215530395508,28.564826965332031]
[null,null,null,null,"Coincident",27.925092697143555,27.85566520690918,27.86528205871582,27.761697769165039,27.468774795532227,27.371618270874023,27.43366813659668]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.129417419433594,29.056194305419922,29.066335678100586,28.957090377807617,28.648242950439453,28.545827865600586,28.611236572265625]
[null,null,null,null,"Coincident",27.925094604492188,28.37330436706543,28.383098602294922,28.277589797973633,27.979223251342773,27.88026237487793,27.943464279174805]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.387058258056641,25.358469009399414,25.296943664550781,25.228307723999023,24.950115203857422,24.797719955444336,24.845796585083008]
[null,null,null,null,"Coincident",24.38233757019043,24.354881286621094,24.295791625976563,24.22987174987793,23.962692260742187,23.816328048706055,23.86250114440918]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.40118408203125,25.372377395629883,25.310386657714844,25.241241455078125,24.961071014404297,24.807653427124023,24.856048583984375]
[null,null,null,null,"Coincident",24.833719253540039,24.805755615234375,24.745571136474609,24.678432464599609,24.406305313110352,24.257232666015625,24.30426025390625]
[null,"Miami","Substation Rating","MVA","Non-Coincident",44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453]
[null,null,null,null,"Coincident",44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453,44.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.995759963989258,25.003259658813477,25.016294479370117,24.924045562744141,24.714553833007813,24.706783294677734,24.824642181396484]
[null,null,null,null,"Coincident",20.565322875976562,20.571491241455078,20.582216262817383,20.506317138671875,20.333955764770508,20.327564239501953,20.424531936645508]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.149873733520508,25.157598495483398,25.171024322509766,25.076009750366211,24.86029052734375,24.852291107177734,24.973640441894531]
[null,null,null,null,"Coincident",21.000362396240234,21.006660461425781,21.017612457275391,20.940107345581055,20.764101028442383,20.757574081420898,20.856592178344727]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.73326301574707,23.772750854492188,23.719249725341797,23.655601501464844,23.44549560546875,23.377649307250977,23.481475830078125]
[null,null,null,null,"Coincident",19.52659797668457,19.559087753295898,19.515068054199219,19.462701797485352,19.289833068847656,19.234016418457031,19.319438934326172]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.850984573364258,23.891561508178711,23.836585998535156,23.771190643310547,23.555381774902344,23.485715866088867,23.59233283996582]
[null,null,null,null,"Coincident",19.939662933349609,19.972841262817383,19.927890777587891,19.874416351318359,19.697891235351563,19.640892028808594,19.728122711181641]
[null,"Milton","Substation Rating","MVA","Non-Coincident",125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781]
[null,null,null,null,"Coincident",125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.134899139404297,47.255973815917969,47.455909729003906,48.104194641113281,48.322334289550781,48.655494689941406,49.184421539306641]
[null,null,null,null,"Coincident",44.169773101806641,44.283233642578125,44.470588684082031,45.078094482421875,45.282508850097656,45.594711303710937,46.090366363525391]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.162708282470703,47.285629272460938,47.488731384277344,48.104896545410156,48.32366943359375,48.658172607421875,49.190151214599609]
[null,null,null,null,"Coincident",44.182075500488281,44.296230316162109,44.484771728515625,45.096435546875,45.302356719970703,45.616962432861328,46.116672515869141]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.167213439941406,45.344978332519531,45.410663604736328,46.077407836914063,46.264102935791016,46.462886810302734,46.952590942382813]
[null,null,null,null,"Coincident",42.325870513916016,42.492450714111328,42.554004669189453,43.178806304931641,43.353755950927734,43.540035247802734,43.998935699462891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.17303466796875,45.352142333984375,45.418354034423828,46.091480255126953,46.280281066894531,46.481464385986328,46.977725982666016]
[null,null,null,null,"Coincident",42.329418182373047,42.496585845947266,42.558364868164063,43.185794830322266,43.361579895019531,43.548801422119141,44.010223388671875]
[null,"Moggill","Substation Rating","MVA","Non-Coincident",33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453]
[null,null,null,null,"Coincident",33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453,33.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.799217224121094,21.517427444458008,21.50627326965332,21.396368026733398,21.151573181152344,21.014001846313477,20.911172866821289]
[null,null,null,null,"Coincident",20.251237869262695,19.989458084106445,19.979095458984375,19.876995086669922,19.64958381652832,19.521781921386719,19.426254272460937]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.868997573852539,21.580846786499023,21.56944465637207,21.457122802734375,21.207077026367188,21.066635131835938,20.961698532104492]
[null,null,null,null,"Coincident",20.520404815673828,20.255146026611328,20.244646072387695,20.14118766784668,19.910755157470703,19.781253814697266,19.684455871582031]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.458145141601563,17.255964279174805,17.199237823486328,17.12858772277832,16.924482345581055,16.771022796630859,16.683490753173828]
[null,null,null,null,"Coincident",16.218429565429687,16.030605316162109,15.977907180786133,15.912274360656738,15.722661972045898,15.580099105834961,15.498783111572266]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.461126327514648,17.257867813110352,17.200881958007812,17.129932403564453,16.925127029418945,16.771305084228516,16.683631896972656]
[null,null,null,null,"Coincident",16.433996200561523,16.243675231933594,16.190275192260742,16.123771667480469,15.931638717651367,15.78718090057373,15.70478343963623]
[null,"Molendinar","Substation Rating","MVA","Non-Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,null,null,"Coincident",59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547,59.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.465877532958984,45.225112915039063,45.235439300537109,45.038570404052734,44.465015411376953,44.033950805664063,43.761817932128906]
[null,null,null,null,"Coincident",45.419921875,45.179401397705078,45.189716339111328,44.993045806884766,44.420070648193359,43.98944091796875,43.717582702636719]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.608413696289063,45.360195159912109,45.370838165283203,45.167991638183594,44.577659606933594,44.134620666503906,43.855220794677734]
[null,null,null,null,"Coincident",45.476570129394531,45.232933044433594,45.243381500244141,45.044212341308594,44.464244842529297,44.028644561767578,43.753780364990234]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.866539001464844,42.697677612304687,42.589103698730469,42.446487426757813,41.885791778564453,41.372711181640625,41.103557586669922]
[null,null,null,null,"Coincident",42.823211669921875,42.654518127441406,42.546054840087891,42.403583526611328,41.843456268310547,41.330894470214844,41.06201171875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.937686920166016,42.764919281005859,42.653884887695313,42.508098602294922,41.935615539550781,41.412731170654297,41.138816833496094]
[null,null,null,null,"Coincident",42.851291656494141,42.680965423583984,42.571479797363281,42.427688598632812,41.862678527832031,41.346084594726563,41.07525634765625]
[null,"Mooloolaba","Substation Rating","MVA","Non-Coincident",67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813]
[null,null,null,null,"Coincident",67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813,67.800003051757813]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.800544738769531,40.16998291015625,40.797519683837891,41.270412445068359,41.427726745605469,41.739776611328125,42.207717895507813]
[null,null,null,null,"Coincident",37.363716125488281,37.710540771484375,38.299655914306641,38.743595123291016,38.891277313232422,39.184219360351563,39.623508453369141]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.901424407958984,40.275394439697266,40.910762786865234,41.389667510986328,41.549007415771484,41.865093231201172,42.339164733886719]
[null,null,null,null,"Coincident",37.672538757324219,38.022228240966797,38.6162109375,39.063819885253906,39.212722778320312,39.508087158203125,39.951007843017578]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.941299438476563,34.303058624267578,34.742416381835938,35.180549621582031,35.297672271728516,35.471790313720703,35.857711791992188]
[null,null,null,null,"Coincident",31.863210678100586,32.20281982421875,32.615280151367188,33.026584625244141,33.136539459228516,33.299995422363281,33.662288665771484]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.980087280273437,34.345058441162109,34.788444519042969,35.230724334716797,35.348976135253906,35.524791717529297,35.914546966552734]
[null,null,null,null,"Coincident",32.126567840576172,32.468986511230469,32.884853363037109,33.299556732177734,33.410423278808594,33.575229644775391,33.940517425537109]
[null,"Moorooka","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.7955322265625,16.618490219116211,16.613775253295898,16.532835006713867,16.313602447509766,16.52277946472168,16.897296905517578]
[null,null,null,null,"Coincident",15.666652679443359,15.501509666442871,15.497112274169922,15.421610832214355,15.217113494873047,15.412232398986816,15.761577606201172]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.143276214599609,16.951253890991211,16.946142196655273,16.858417510986328,16.621011734008789,16.847522735595703,17.253734588623047]
[null,null,null,null,"Coincident",16.000263214111328,15.83160400390625,15.827113151550293,15.750003814697266,15.541152000427246,15.740425109863281,16.097209930419922]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.420763969421387,15.279014587402344,15.232361793518066,15.173427581787109,14.965023994445801,15.117802619934082,15.455410957336426]
[null,null,null,null,"Coincident",14.384285926818848,14.25206470489502,14.208547592163086,14.153573989868164,13.95917797088623,14.101688385009766,14.416604995727539]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.657458305358887,15.505011558532715,15.454872131347656,15.391558647155762,15.167893409729004,15.331825256347656,15.694743156433105]
[null,null,null,null,"Coincident",14.690589904785156,14.55555248260498,14.511109352111816,14.454964637756348,14.256429672241211,14.401974678039551,14.723596572875977]
[null,"Morayfield","Substation Rating","MVA","Non-Coincident",47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547]
[null,null,null,null,"Coincident",47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547,47.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.928045272827148,29.572172164916992,30.813796997070312,31.390373229980469,31.282604217529297,31.301830291748047,31.460311889648438]
[null,null,null,null,"Coincident",28.097688674926758,28.739170074462891,29.976882934570313,30.552526473999023,30.447086334228516,30.465192794799805,30.618778228759766]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.055027008056641,29.71345329284668,30.983913421630859,31.574405670166016,31.464012145996094,31.483707427978516,31.646053314208984]
[null,null,null,null,"Coincident",28.099006652832031,28.742403030395508,29.986007690429687,30.565338134765625,30.459291458129883,30.47746467590332,30.631860733032227]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.129812240600586,25.807838439941406,26.980062484741211,27.590045928955078,27.479223251342773,27.422000885009766,27.548374176025391]
[null,null,null,null,"Coincident",24.408477783203125,25.083723068237305,26.255561828613281,26.864503860473633,26.756023406982422,26.699682235717773,26.822046279907227]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.183801651000977,25.873228073120117,27.06695556640625,27.688945770263672,27.575902938842773,27.517539978027344,27.646438598632813]
[null,null,null,null,"Coincident",24.90086555480957,25.595870971679688,26.803691864013672,26.864902496337891,26.756305694580078,26.699909210205078,26.822381973266602]
[null,"Morayfield North","Substation Rating","MVA","Non-Coincident",53.5,53.5,53.5,53.5,53.5,53.5,53.5]
[null,null,null,null,"Coincident",53.5,53.5,53.5,53.5,53.5,53.5,53.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.574522018432617,29.547971725463867,29.713422775268555,29.74226188659668,29.519781112670898,29.388517379760742,29.361001968383789]
[null,null,null,null,"Coincident",29.574522018432617,29.547971725463867,29.713422775268555,29.74226188659668,29.519781112670898,29.388517379760742,29.361001968383789]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.940059661865234,31.911386489868164,32.090072631835938,32.1212158203125,31.880939483642578,31.739179611206055,31.709463119506836]
[null,null,null,null,"Coincident",30.269474029541016,30.242300033569336,30.411638259887695,30.441156387329102,30.213447570800781,30.079099655151367,30.050937652587891]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.14044189453125,27.153045654296875,27.229438781738281,27.283336639404297,27.066232681274414,26.876354217529297,26.842399597167969]
[null,null,null,null,"Coincident",27.14044189453125,27.153045654296875,27.229438781738281,27.283336639404297,27.066232681274414,26.876354217529297,26.842399597167969]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.311288833618164,29.324901580810547,29.407403945922852,29.465612411499023,29.231143951416016,29.026079177856445,28.989408493041992]
[null,null,null,null,"Coincident",27.7781982421875,27.791097640991211,27.869285583496094,27.924449920654297,27.702243804931641,27.507904052734375,27.473152160644531]
[null,"Mt Cotton","Substation Rating","MVA","Non-Coincident",15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137]
[null,null,null,null,"Coincident",15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137,15.699999809265137]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9809360504150391,8.9518499374389648,8.9590072631835938,8.9280500411987305,8.8257341384887695,8.7546091079711914,8.7162408828735352]
[null,null,null,null,"Coincident",8.5582656860351562,8.5305490493774414,8.5373678207397461,8.5078678131103516,8.4103660583496094,8.3425893783569336,8.3060274124145508]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.7821884155273437,9.7505073547363281,9.7583036422729492,9.724583625793457,9.6131391525268555,9.5356683731079102,9.4938774108886719]
[null,null,null,null,"Coincident",8.5849761962890625,8.5571727752685547,8.5640134811401367,8.5344209671020508,8.436614990234375,8.368626594543457,8.3319501876831055]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4439716339111328,8.4281005859375,8.411468505859375,8.3908529281616211,8.2907047271728516,8.2026739120483398,8.1640501022338867]
[null,null,null,null,"Coincident",8.0465726852416992,8.0314474105834961,8.015599250793457,7.9959530830383301,7.9005188941955566,7.8166298866271973,7.7798242568969727]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.1973171234130859,9.1800298690795898,9.1619148254394531,9.1394596099853516,9.0303764343261719,8.9344911575317383,8.8924226760864258]
[null,null,null,null,"Coincident",8.071685791015625,8.056513786315918,8.0406160354614258,8.0209083557128906,7.9251766204833984,7.8410258293151855,7.804105281829834]
[null,"Mt Crosby West","Substation Rating","MVA","Non-Coincident",28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547]
[null,null,null,null,"Coincident",28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547,28.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.09024715423584,14.765140533447266,14.783717155456543,14.745401382446289,14.601287841796875,14.524481773376465,14.514461517333984]
[null,null,null,null,"Coincident",10.425840377807617,10.928296089172363,10.942044258117676,10.913680076599121,10.807007789611816,10.750149726867676,10.742717742919922]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.104609489440918,14.792755126953125,14.811747550964355,14.772577285766602,14.625349998474121,14.546950340270996,14.536725997924805]
[null,null,null,null,"Coincident",10.565434455871582,11.089694023132324,11.103638648986816,11.074837684631348,10.966554641723633,10.908799171447754,10.90118408203125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.697240829467773,13.42288875579834,13.402498245239258,13.381120681762695,13.243738174438477,13.139711380004883,13.12587833404541]
[null,null,null,null,"Coincident",9.3951091766357422,9.9352836608886719,9.9201908111572266,9.9043636322021484,9.8026695251464844,9.7256603240966797,9.7154064178466797]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.697525978088379,13.428049087524414,13.407444953918457,13.385848045349121,13.247165679931641,13.142287254333496,13.128349304199219]
[null,null,null,null,"Coincident",9.5209026336669922,10.08424186706543,10.068916320800781,10.05283260345459,9.9495763778686523,9.8713531494140625,9.8608684539794922]
[null,"Mt Gravatt","Substation Rating","MVA","Non-Coincident",59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547]
[null,null,null,null,"Coincident",59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547,59.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.7972412109375,27.411380767822266,27.394586563110352,27.550933837890625,27.650047302246094,27.662635803222656,27.717449188232422]
[null,null,null,null,"Coincident",26.71759033203125,26.346715927124023,26.330574035644531,26.48084831237793,26.576112747192383,26.588212966918945,26.640897750854492]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.219516754150391,27.814973831176758,27.797369003295898,27.961259841918945,28.06517219543457,28.078371047973633,28.135845184326172]
[null,null,null,null,"Coincident",26.730628967285156,26.357339859008789,26.341096878051758,26.492321014404297,26.588205337524414,26.600383758544922,26.653419494628906]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.942911148071289,24.630205154418945,24.546920776367188,24.711896896362305,24.788873672485352,24.736173629760742,24.777072906494141]
[null,null,null,null,"Coincident",23.974123001098633,23.673563003540039,23.593513488769531,23.752080917358398,23.826068878173828,23.775415420532227,23.814725875854492]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.232172012329102,24.905708312988281,24.818790435791016,24.990976333618164,25.071334838867188,25.016317367553711,25.059015274047852]
[null,null,null,null,"Coincident",23.974912643432617,23.67388916015625,23.59375,23.752510070800781,23.826606750488281,23.775876998901367,23.81524658203125]
[null,"Mt Sylvia","Substation Rating","MVA","Non-Coincident",7.5,7.5,7.5,7.5,7.5,7.5,7.5]
[null,null,null,null,"Coincident",7.5,7.5,7.5,7.5,7.5,7.5,7.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.5867542028427124,1.588637113571167,1.5904909372329712,1.5855072736740112,1.5677592754364014,1.5554672479629517,1.5489640235900879]
[null,null,null,null,"Coincident",1.1524772644042969,1.1538448333740234,1.1551913022994995,1.1515716314315796,1.1386810541152954,1.1297532320022583,1.1250298023223877]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8314179182052612,1.8335912227630615,1.8357309103012085,1.8299788236618042,1.8094942569732666,1.795306921005249,1.7878009080886841]
[null,null,null,null,"Coincident",1.2805192470550537,1.282038688659668,1.2835347652435303,1.279512882232666,1.2651902437210083,1.2552704811096191,1.250022292137146]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4185937643051147,1.4222135543823242,1.4199283123016357,1.4169056415557861,1.4003715515136719,1.3858070373535156,1.3795610666275024]
[null,null,null,null,"Coincident",1.0303404331207275,1.03296959400177,1.0313097238540649,1.0291143655776978,1.0171054601669312,1.0065270662307739,1.0019905567169189]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6373286247253418,1.641506552696228,1.6388689279556274,1.6353802680969238,1.6162967681884766,1.5994864702224731,1.5922774076461792]
[null,null,null,null,"Coincident",1.1448128223419189,1.1477340459823608,1.1458897590637207,1.1434504985809326,1.1301074028015137,1.1183537244796753,1.1133131980895996]
[null,"Mt Tamborine Bus 1","Substation Rating","MVA","Non-Coincident",21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727]
[null,null,null,null,"Coincident",21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727,21.600000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7211418151855469,7.7763533592224121,7.7702970504760742,7.7723140716552734,7.9005374908447266,7.9236721992492676,7.9675893783569336]
[null,null,null,null,"Coincident",7.2995438575744629,7.3185806274414062,7.3407058715820313,7.3415184020996094,7.2967886924743652,7.2898263931274414,7.3133187294006348]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.8595428466796875,7.9157443046569824,7.9095792770385742,7.9116325378417969,8.0421543121337891,8.0657033920288086,8.110407829284668]
[null,null,null,null,"Coincident",7.4721121788024902,7.4915990829467773,7.5142474174499512,7.5150794982910156,7.469292163848877,7.462165355682373,7.4862127304077148]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.3057703971862793,7.3437676429748535,7.3270940780639648,7.3122878074645996,7.4192924499511719,7.4189367294311523,7.4333124160766602]
[null,null,null,null,"Coincident",6.6147828102111816,6.6410751342773437,6.642697811126709,6.6501288414001465,6.6064338684082031,6.583101749420166,6.6021537780761719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.4367260932922363,7.4754042625427246,7.4584317207336426,7.4433598518371582,7.5522828102111816,7.5519204139709473,7.566554069519043]
[null,null,null,null,"Coincident",6.7711629867553711,6.7980766296386719,6.7997379302978516,6.8073444366455078,6.7626166343688965,6.7387328147888184,6.7582354545593262]
[null,"Mt Tamborine Bus 2","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.2857236862182617,8.3450021743774414,8.3385419845581055,8.3407754898071289,8.4784832000732422,8.5034542083740234,8.5507392883300781]
[null,null,null,null,"Coincident",6.7540163993835449,6.7716546058654785,6.7921581268310547,6.7929658889770508,6.7516636848449707,6.7453360557556152,6.7671957015991211]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.4106340408325195,8.4708061218261719,8.4642486572265625,8.4665155410766602,8.6062994003295898,8.6316461563110352,8.6796445846557617]
[null,null,null,null,"Coincident",6.932004451751709,6.9501075744628906,6.9711513519287109,6.9719805717468262,6.9295897483825684,6.923095703125,6.9455313682556152]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8696050643920898,7.9105625152587891,7.8926396369934082,7.8767542839050293,7.9921202659606934,7.9918723106384277,8.007502555847168]
[null,null,null,null,"Coincident",6.4245748519897461,6.4501347541809082,6.4517407417297363,6.4590115547180176,6.416654109954834,6.3941001892089844,6.4127206802368164]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9882421493530273,8.0298166275024414,8.0116243362426758,7.9954991340637207,8.1126041412353516,8.1123523712158203,8.1282186508178711]
[null,null,null,null,"Coincident",6.5938816070556641,6.620114803314209,6.6217632293701172,6.6292257308959961,6.585752010345459,6.5626034736633301,6.5817146301269531]
[null,"Mudgeeraba West Pkg","Substation Rating","MVA","Non-Coincident",45,45,45,45,45,45,45]
[null,null,null,null,"Coincident",45,45,45,45,45,45,45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.540195465087891,24.567317962646484,24.612298965454102,24.554046630859375,24.34423828125,24.272909164428711,24.284711837768555]
[null,null,null,null,"Coincident",22.319492340087891,22.344160079956055,22.38507080078125,22.332090377807617,22.141269683837891,22.076395034790039,22.087129592895508]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.568103790283203,24.595542907714844,24.64105224609375,24.582117080688477,24.369907379150391,24.297782897949219,24.309717178344727]
[null,null,null,null,"Coincident",22.618772506713867,22.643770217895508,22.685230255126953,22.631538391113281,22.438159942626953,22.372415542602539,22.383293151855469]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.706527709960938,20.757675170898438,20.738067626953125,20.709835052490234,20.523006439208984,20.410078048706055,20.413314819335938]
[null,null,null,null,"Coincident",18.832740783691406,18.87925910949707,18.861425399780273,18.835748672485352,18.665826797485352,18.563116073608398,18.566059112548828]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.707029342651367,20.758275985717773,20.738630294799805,20.710344314575195,20.523227691650391,20.410181045532227,20.413419723510742]
[null,null,null,null,"Coincident",19.08526611328125,19.132408142089844,19.114336013793945,19.088314056396484,18.916114807128906,18.812026977539063,18.815010070800781]
[null,"Murarrie","Substation Rating","MVA","Non-Coincident",50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906]
[null,null,null,null,"Coincident",50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906,50.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.21246337890625,23.150497436523438,23.179841995239258,23.099945068359375,22.828413009643555,22.624732971191406,22.484533309936523]
[null,null,null,null,"Coincident",20.752273559570313,20.696876525878906,20.723110198974609,20.651681900024414,20.408927917480469,20.226835250854492,20.101493835449219]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.352218627929687,23.286748886108398,23.3177490234375,23.233362197875977,22.947023391723633,22.732702255249023,22.585416793823242]
[null,null,null,null,"Coincident",20.810413360595703,20.753789901733398,20.780603408813477,20.707601547241211,20.459625244140625,20.273748397827148,20.145868301391602]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.071111679077148,23.040895462036133,23.006181716918945,22.949993133544922,22.669321060180664,22.409091949462891,22.262935638427734]
[null,null,null,null,"Coincident",20.625904083251953,20.59889030456543,20.567855834960937,20.517621994018555,20.266696929931641,20.034048080444336,19.903383255004883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.202924728393555,23.17103385925293,23.134407043457031,23.07514762878418,22.779586791992187,22.506246566772461,22.35302734375]
[null,null,null,null,"Coincident",20.681259155273438,20.653657913208008,20.621950149536133,20.570632934570313,20.314428329467773,20.077079772949219,19.94386100769043]
[null,"Murrumba","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6709823608398437,1.6710641384124756,1.6659070253372192,1.6602790355682373,1.6904183626174927,1.6977365016937256,1.698178768157959]
[null,null,null,null,"Coincident",0.22631505131721497,0.22530533373355865,0.22546464204788208,0.22466948628425598,0.22366434335708618,0.22376307845115662,0.22330497205257416]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8421217203140259,1.8422118425369263,1.83652663230896,1.8303221464157104,1.8635482788085937,1.8716158866882324,1.8721034526824951]
[null,null,null,null,"Coincident",0.22998765110969543,0.22896154224872589,0.22912344336509705,0.22831538319587708,0.22729392349720001,0.22739426791667938,0.22692872583866119]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5912835597991943,1.5882809162139893,1.5810157060623169,1.5720820426940918,1.5976854562759399,1.599840521812439,1.5945204496383667]
[null,null,null,null,"Coincident",0.20165291428565979,0.20102693140506744,0.20061174035072327,0.2001056969165802,0.19911469519138336,0.19868862628936768,0.19821693003177643]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7542603015899658,1.7509500980377197,1.7429407835006714,1.733092188835144,1.7613177299499512,1.7636936902999878,1.7578287124633789]
[null,null,null,null,"Coincident",0.2049252986907959,0.20428915321826935,0.20386722683906555,0.20335297286510468,0.20234589278697968,0.20191290974617004,0.20143355429172516]
[null,"Myrtletown","Substation Rating","MVA","Non-Coincident",49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547]
[null,null,null,null,"Coincident",49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547,49.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.442348480224609,14.451937675476074,14.463593482971191,15.134503364562988,14.950767517089844,14.81479549407959,14.732394218444824]
[null,null,null,null,"Coincident",13.320137977600098,13.328982353210449,13.33973217010498,13.958510398864746,13.78905200958252,13.663644790649414,13.587646484375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.454813003540039,14.464560508728027,14.476408958435059,15.160515785217285,14.972768783569336,14.834015846252441,14.75001049041748]
[null,null,null,null,"Coincident",13.704705238342285,13.713805198669434,13.724864959716797,14.370946884155273,14.196481704711914,14.067368507385254,13.98912525177002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.3724365234375,14.40158748626709,14.373270988464355,15.095911979675293,14.905477523803711,14.731809616088867,14.645073890686035]
[null,null,null,null,"Coincident",13.255658149719238,13.282544136047363,13.256427764892578,13.922918319702148,13.747281074523926,13.58710765838623,13.507111549377441]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.383779525756836,14.413392066955566,14.384627342224121,15.121058464050293,14.926534652709961,14.749414443969727,14.661056518554687]
[null,null,null,null,"Coincident",13.638363838195801,13.66602611541748,13.639155387878418,14.334811210632324,14.15397834777832,13.989066123962402,13.906703948974609]
[null,"Nambour","Substation Rating","MVA","Non-Coincident",55,55,55,55,55,55,55]
[null,null,null,null,"Coincident",55,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.038394927978516,31.913566589355469,32.232818603515625,32.330352783203125,32.051258087158203,31.928459167480469,31.991024017333984]
[null,null,null,null,"Coincident",32.038394927978516,31.913566589355469,32.232818603515625,32.330352783203125,32.051258087158203,31.928459167480469,31.991024017333984]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.077945709228516,31.950901031494141,32.275928497314453,32.375297546386719,32.091037750244141,31.966054916381836,32.029727935791016]
[null,null,null,null,"Coincident",32.136814117431641,32.009963989257813,32.334415435791016,32.433551788330078,32.149887084960938,32.025096893310547,32.088672637939453]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.159624099731445,30.083070755004883,30.299833297729492,30.422147750854492,30.145027160644531,29.952051162719727,30.000917434692383]
[null,null,null,null,"Coincident",30.159624099731445,30.083070755004883,30.299833297729492,30.422147750854492,30.145027160644531,29.952051162719727,30.000917434692383]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.172046661376953,30.094686508178711,30.31379508972168,30.437520980834961,30.157293319702148,29.962347030639648,30.011697769165039]
[null,null,null,null,"Coincident",30.229156494140625,30.151500701904297,30.371400833129883,30.495508193969727,30.214347839355469,30.018608093261719,30.068170547485352]
[null,"Narangba","Substation Rating","MVA","Non-Coincident",47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906]
[null,null,null,null,"Coincident",47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.946537017822266,23.003793716430664,23.171531677246094,23.340261459350586,23.33146858215332,23.375547409057617,23.532926559448242]
[null,null,null,null,"Coincident",22.095054626464844,22.150190353393555,22.311700820922852,22.47416877746582,22.465703964233398,22.508146286010742,22.659685134887695]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.527616500854492,23.586322784423828,23.758308410644531,23.931310653686523,23.922294616699219,23.967489242553711,24.128854751586914]
[null,null,null,null,"Coincident",22.430839538574219,22.486814498901367,22.650777816772461,22.815715789794922,22.807121276855469,22.850210189819336,23.004051208496094]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.873907089233398,20.954524993896484,21.04884147644043,21.223482131958008,21.205287933349609,21.190534591674805,21.326215744018555]
[null,null,null,null,"Coincident",20.099336624145508,20.176961898803711,20.267778396606445,20.435937881469727,20.418418884277344,20.404212951660156,20.534858703613281]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.402500152587891,21.485160827636719,21.581863403320313,21.760927200317383,21.742273330688477,21.727146148681641,21.866262435913086]
[null,null,null,null,"Coincident",20.404792785644531,20.483596801757813,20.575794219970703,20.746509552001953,20.728723526000977,20.714302062988281,20.846933364868164]
[null,"Nerang","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",56.746978759765625,56.666786193847656,56.762763977050781,56.75836181640625,56.480541229248047,56.374099731445313,56.396457672119141]
[null,null,null,null,"Coincident",55.856067657470703,55.777133941650391,55.871604919433594,55.867271423339844,55.59381103515625,55.489036560058594,55.511043548583984]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",56.827358245849609,56.745838165283203,56.843406677246094,56.83892822265625,56.556549072265625,56.448390960693359,56.471107482910156]
[null,null,null,null,"Coincident",55.877140045166016,55.797760009765625,55.892765045166016,55.888404846191406,55.613414764404297,55.508064270019531,55.530193328857422]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.488105773925781,51.485443115234375,51.429763793945312,51.477603912353516,51.201004028320313,50.97265625,50.976173400878906]
[null,null,null,null,"Coincident",50.679756164550781,50.677139282226563,50.622333526611328,50.669425964355469,50.397167205810547,50.172405242919922,50.175868988037109]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.503036499023438,51.500354766845703,51.444240570068359,51.492454528808594,51.213756561279297,50.983791351318359,50.987335205078125]
[null,null,null,null,"Coincident",50.681266784667969,50.678646087646484,50.623748779296875,50.670921325683594,50.398239135742188,50.173183441162109,50.176651000976562]
[null,"Newmarket","Substation Rating","MVA","Non-Coincident",57.5,57.5,57.5,57.5,57.5,57.5,57.5]
[null,null,null,null,"Coincident",57.5,57.5,57.5,57.5,57.5,57.5,57.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.283182144165039,24.039878845214844,24.191156387329102,24.420936584472656,24.206666946411133,23.837289810180664,23.675760269165039]
[null,null,null,null,"Coincident",24.244228363037109,24.001316070556641,24.152349472045898,24.38176155090332,24.16783332824707,23.799051284790039,23.637777328491211]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.828514099121094,24.568527221679688,24.73016357421875,24.975763320922852,24.746738433837891,24.352132797241211,24.179656982421875]
[null,null,null,null,"Coincident",24.793968200683594,24.545547485351563,24.700006484985352,24.934619903564453,24.715841293334961,24.33869743347168,24.173765182495117]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.979406356811523,20.797523498535156,20.870412826538086,21.089887619018555,20.894794464111328,20.522867202758789,20.377119064331055]
[null,null,null,null,"Coincident",20.94575309753418,20.76416015625,20.836933135986328,21.056055068969727,20.861274719238281,20.489944458007813,20.344430923461914]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.309528350830078,21.11662483215332,21.193918228149414,21.426752090454102,21.219778060913086,20.825521469116211,20.671146392822266]
[null,null,null,null,"Coincident",21.420700073242187,21.234989166259766,21.309412002563477,21.533502578735352,21.334306716918945,20.954555511474609,20.805742263793945]
[null,"Newstead","Substation Rating","MVA","Non-Coincident",131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219]
[null,null,null,null,"Coincident",131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219,131.19999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.796077728271484,44.645221710205078,44.941978454589844,45.574409484863281,45.799983978271484,46.136634826660156,46.650436401367188]
[null,null,null,null,"Coincident",37.758800506591797,38.490890502929688,38.746738433837891,39.291988372802734,39.486469268798828,39.776710510253906,40.219684600830078]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.823307037353516,44.685153961181641,44.986854553222656,45.630664825439453,45.860569000244141,46.203937530517578,46.728569030761719]
[null,null,null,null,"Coincident",38.032726287841797,38.791965484619141,39.054191589355469,39.613037109375,39.812210083007813,40.109638214111328,40.563800811767578]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.545322418212891,41.465034484863281,41.624164581298828,42.249847412109375,42.436088562011719,42.635368347167969,43.093700408935547]
[null,null,null,null,"Coincident",34.956161499023438,35.749088287353516,35.886283874511719,36.425716400146484,36.586284637451172,36.758094787597656,37.153244018554688]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.54595947265625,41.469379425048828,41.629470825195312,42.259822845458984,42.447719573974609,42.648902893066406,43.112117767333984]
[null,null,null,null,"Coincident",35.164867401123047,35.984889984130859,36.125267028808594,36.677394866943359,36.841571807861328,37.017288208007813,37.421844482421875]
[null,"Ningi","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.2583684921264648,9.1748666763305664,9.1837635040283203,9.1991729736328125,9.1848077774047852,9.1813392639160156,9.1899271011352539]
[null,null,null,null,"Coincident",8.5253324508666992,8.4483919143676758,8.4565849304199219,8.4708013534545898,8.4576253890991211,8.454472541809082,8.4624118804931641]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.6714019775390625,9.5841751098632812,9.5934686660766602,9.6095657348632812,9.5945606231689453,9.5909366607666016,9.5999069213867187]
[null,null,null,null,"Coincident",8.6981048583984375,8.6196870803833008,8.6280450820922852,8.6425056457519531,8.6289749145507812,8.6256875991821289,8.6337356567382812]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4323616027832031,8.3682422637939453,8.3531427383422852,8.3752985000610352,8.3576278686523437,8.3324527740478516,8.3371744155883789]
[null,null,null,null,"Coincident",7.7640314102172852,7.7049422264099121,7.6910400390625,7.7114672660827637,7.6952519416809082,7.6721158027648926,7.6764955520629883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8085451126098633,8.7415657043457031,8.7257928848266602,8.748936653137207,8.7304773330688477,8.7041797637939453,8.709111213684082]
[null,null,null,null,"Coincident",7.9225406646728516,7.8623318672180176,7.84814453125,7.8689417839050293,7.8523039817810059,7.8286218643188477,7.833035945892334]
[null,"Noosaville","Substation Rating","MVA","Non-Coincident",138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219]
[null,null,null,null,"Coincident",138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219,138.69999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.047004699707031,39.841224670410156,40.319919586181641,40.456615447998047,40.116447448730469,39.960121154785156,39.995128631591797]
[null,null,null,null,"Coincident",31.596792221069336,31.434432983398438,31.81212043762207,31.919971466064453,31.651580810546875,31.528242111206055,31.555862426757813]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.047046661376953,39.932117462158203,40.320182800292969,40.457054138183594,40.116527557373047,39.960132598876953,39.995151519775391]
[null,null,null,null,"Coincident",31.600687026977539,31.43791389465332,31.816595077514648,31.924749374389648,31.655618667602539,31.531959533691406,31.559650421142578]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.980747222900391,35.84466552734375,36.174839019775391,36.334064483642578,36.011238098144531,35.778362274169922,35.797977447509766]
[null,null,null,null,"Coincident",28.388545989990234,28.281177520751953,28.541683197021484,28.66731071472168,28.412603378295898,28.228864669799805,28.244340896606445]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.010471343994141,35.872760772705078,36.206954956054688,36.368202209472656,36.041332244873047,35.805679321289063,35.825523376464844]
[null,null,null,null,"Coincident",28.476627349853516,28.368125915527344,28.631387710571289,28.758352279663086,28.500940322875977,28.315261840820312,28.330900192260742]
[null,"North Maclean","Substation Rating","MVA","Non-Coincident",59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453]
[null,null,null,null,"Coincident",59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.887508392333984,29.909971237182617,30.212625503540039,30.394924163818359,30.34022331237793,30.395969390869141,30.564916610717773]
[null,null,null,null,"Coincident",26.408596038818359,26.428445816040039,26.695869445800781,26.856948852539062,26.808616638183594,26.857872009277344,27.00715446472168]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.002656936645508,30.02556037902832,30.334224700927734,30.520187377929688,30.464384078979492,30.52125358581543,30.693630218505859]
[null,null,null,null,"Coincident",26.778181076049805,26.798309326171875,27.069475173950195,27.232809066772461,27.183801651000977,27.233745574951172,27.385116577148438]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.687189102172852,25.741540908813477,25.929977416992187,26.112728118896484,26.053205490112305,26.033729553222656,26.169858932495117]
[null,null,null,null,"Coincident",22.697193145751953,22.745222091674805,22.911722183227539,23.073202133178711,23.020606994628906,23.003395080566406,23.123680114746094]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.730836868286133,25.78594970703125,25.977060317993164,26.162460327148438,26.102067947387695,26.082309722900391,26.220430374145508]
[null,null,null,null,"Coincident",23.014839172363281,23.063539505004883,23.232370376586914,23.396108627319336,23.342779159545898,23.325325012207031,23.447294235229492]
[null,"North Springwood","Substation Rating","MVA","Non-Coincident",124.5,124.5,124.5,124.5,124.5,124.5,124.5]
[null,null,null,null,"Coincident",124.5,124.5,124.5,124.5,124.5,124.5,124.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.863162994384766,51.124355316162109,51.091197967529297,50.823337554931641,50.130329132080078,49.598152160644531,49.244895935058594]
[null,null,null,null,"Coincident",50.181808471679688,49.466949462890625,49.434867858886719,49.175689697265625,48.505149841308594,47.990226745605469,47.648422241210938]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.120903015136719,52.331111907958984,52.295677185058594,52.009449005126953,51.269195556640625,50.701023101806641,50.324008941650391]
[null,null,null,null,"Coincident",50.261543273925781,49.537120819091797,49.504623413085937,49.242107391357422,48.563236236572266,48.042228698730469,47.696537017822266]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.520034790039063,45.919864654541016,45.762943267822266,45.568901062011719,44.925933837890625,44.334320068359375,44.004138946533203]
[null,null,null,null,"Coincident",45.011898040771484,44.431182861328125,44.279350280761719,44.091598510742188,43.469474792480469,42.897041320800781,42.577564239501953]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.419952392578125,46.781356811523438,46.614456176757813,46.408111572265625,45.724700927734375,45.096317291259766,44.745807647705078]
[null,null,null,null,"Coincident",45.034881591796875,44.449638366699219,44.296695709228516,44.107612609863281,43.481422424316406,42.905735015869141,42.584648132324219]
[null,"Nth Ipswich","Substation Rating","MVA","Non-Coincident",59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094]
[null,null,null,null,"Coincident",59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094,59.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.035480499267578,25.95634651184082,25.98863410949707,25.919975280761719,25.655118942260742,25.490579605102539,25.425239562988281]
[null,null,null,null,"Coincident",25.832324981689453,25.753807067871094,25.785844802856445,25.717721939086914,25.454931259155273,25.291675567626953,25.226844787597656]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.035549163818359,25.956363677978516,25.988668441772461,25.919979095458984,26.121318817138672,25.947776794433594,25.878871917724609]
[null,null,null,null,"Coincident",25.841970443725586,25.763011932373047,25.795228958129883,25.726728439331055,25.462545394897461,25.298477172851563,25.233333587646484]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.138633728027344,23.099754333496094,23.064411163330078,23.026662826538086,22.780414581298828,22.575912475585938,22.510669708251953]
[null,null,null,null,"Coincident",22.958084106445313,22.919509887695313,22.884443283081055,22.846990585327148,22.602663040161133,22.399755477905273,22.335020065307617]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.4718017578125,23.430952072143555,23.393823623657227,23.354167938232422,23.095554351806641,22.880876541137695,22.812404632568359]
[null,null,null,null,"Coincident",22.958194732666016,22.919595718383789,22.88450813293457,22.847038269042969,23.147493362426758,22.939695358276367,22.87339973449707]
[null,"Nth Pine Dam","Substation Rating","MVA","Non-Coincident",6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684]
[null,null,null,null,"Coincident",6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684,6.5999999046325684]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.75779438018798828,0.76193338632583618,0.75967448949813843,0.7569434642791748,0.76476526260375977,0.76077651977539063,0.75831222534179688]
[null,null,null,null,"Coincident",0.3192477822303772,0.31954365968704224,0.31980851292610168,0.31861144304275513,0.31474992632865906,0.31189626455307007,0.31016868352890015]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.88124841451644897,0.88606166839599609,0.88343477249145508,0.88025885820388794,0.88935494422912598,0.88471633195877075,0.88185060024261475]
[null,null,null,null,"Coincident",0.34036144614219666,0.34067687392234802,0.34095925092697144,0.33968302607536316,0.33556610345840454,0.33252373337745667,0.33068189024925232]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.74860930442810059,0.75124102830886841,0.74789571762084961,0.74350821971893311,0.7498137354850769,0.74368953704833984,0.73862302303314209]
[null,null,null,null,"Coincident",0.31860703229904175,0.31933709979057312,0.31871634721755981,0.31784337759017944,0.31384024024009705,0.31019240617752075,0.30837327241897583]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.8705669641494751,0.8736274242401123,0.86973714828491211,0.86463487148284912,0.871967613697052,0.86484569311141968,0.85895383358001709]
[null,null,null,null,"Coincident",0.3396783173084259,0.34045666456222534,0.33979487419128418,0.33886414766311646,0.33459627628326416,0.33070719242095947,0.32876774668693542]
[null,"Nudgee","Substation Rating","MVA","Non-Coincident",41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453]
[null,null,null,null,"Coincident",41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453,41.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.94734001159668,29.7667236328125,29.772525787353516,24.521945953369141,24.208805084228516,23.972114562988281,23.822792053222656]
[null,null,null,null,"Coincident",25.3868408203125,25.233728408813477,25.2386474609375,20.787647247314453,20.522192001342773,20.32154655456543,20.194963455200195]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.52433967590332,31.324056625366211,31.330488204956055,25.524627685546875,25.179634094238281,24.918983459472656,24.754600524902344]
[null,null,null,null,"Coincident",25.501102447509766,25.347299575805664,25.352241516113281,20.789657592773438,20.524175643920898,20.323511123657227,20.196916580200195]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.635374069213867,29.496797561645508,29.420812606811523,23.940338134765625,23.623260498046875,23.331939697265625,23.179014205932617]
[null,null,null,null,"Coincident",25.122381210327148,25.004907608032227,24.940494537353516,20.294609069824219,20.025815963745117,19.778860092163086,19.649221420288086]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.178422927856445,31.02479362487793,30.940563201904297,24.883998870849609,24.535009384155273,24.214546203613281,24.046390533447266]
[null,null,null,null,"Coincident",25.235450744628906,25.117448806762695,25.052745819091797,20.295211791992188,20.026411056518555,19.779447555541992,19.649805068969727]
[null,"Nundah","Substation Rating","MVA","Non-Coincident",44,44,44,44,44,44,44]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.556631088256836,23.133914947509766,22.832279205322266,22.687839508056641,22.688100814819336,23.017452239990234,23.293155670166016]
[null,null,null,null,"Coincident",23.556631088256836,23.133914947509766,22.832279205322266,22.687839508056641,22.688100814819336,23.017452239990234,23.293155670166016]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.179176330566406,23.723628997802734,23.3988037109375,23.24333381652832,23.243614196777344,23.598188400268555,23.895193099975586]
[null,null,null,null,"Coincident",24.030208587646484,23.598995208740234,23.291294097900391,23.143951416015625,23.144218444824219,23.480190277099609,23.761436462402344]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.051471710205078,20.701894760131836,20.375360488891602,20.266870498657227,20.257360458374023,20.498401641845703,20.737138748168945]
[null,null,null,null,"Coincident",21.051471710205078,20.701894760131836,20.375360488891602,20.266870498657227,20.257360458374023,20.498401641845703,20.737138748168945]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.485624313354492,21.111083984375,20.761575698852539,20.645528793334961,20.635358810424805,20.893234252929688,21.148828506469727]
[null,null,null,null,"Coincident",21.474685668945313,21.118082046508789,20.784982681274414,20.674312591552734,20.664609909057617,20.910497665405273,21.154033660888672]
[null,"Oxley","Substation Rating","MVA","Non-Coincident",30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453]
[null,null,null,null,"Coincident",30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453,30.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.817646026611328,19.639413833618164,19.636819839477539,19.544174194335937,19.288055419921875,19.093774795532227,18.995691299438477]
[null,null,null,null,"Coincident",17.806798934936523,17.646652221679687,17.644321441650391,17.561075210571289,17.330944061279297,17.156377792358398,17.068246841430664]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.374521255493164,20.180059432983398,20.177230834960937,20.076192855834961,19.797040939331055,19.58544921875,19.478681564331055]
[null,null,null,null,"Coincident",18.361061096191406,18.195930480957031,18.193527221679688,18.107688903808594,17.870395660400391,17.690395355224609,17.599521636962891]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.441078186035156,18.300142288208008,18.247032165527344,18.17924690246582,17.932392120361328,17.705963134765625,17.609241485595703]
[null,null,null,null,"Coincident",16.569908142089844,16.443273544311523,16.395551681518555,16.334644317626953,16.112836837768555,15.909383773803711,15.822475433349609]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.875701904296875,18.722682952880859,18.665042877197266,18.59149169921875,18.323823928833008,18.078557968139648,17.973865509033203]
[null,null,null,null,"Coincident",17.085670471191406,16.955095291137695,16.905887603759766,16.843084335327148,16.614372253417969,16.404586791992187,16.314973831176758]
[null,"Palm Beach","Substation Rating","MVA","Non-Coincident",44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547]
[null,null,null,null,"Coincident",44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547,44.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.06324577331543,19.089157104492187,19.124668121337891,19.093969345092773,18.968957901000977,18.982244491577148,19.080297470092773]
[null,null,null,null,"Coincident",16.48594856262207,16.508356094360352,16.539064407348633,16.512519836425781,16.404409408569336,16.415899276733398,16.500698089599609]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.102163314819336,19.128597259521484,19.164829254150391,19.133506774902344,19.005996704101563,19.019546508789063,19.119558334350586]
[null,null,null,null,"Coincident",16.863033294677734,16.885953903198242,16.917364120483398,16.89021110534668,16.779628753662109,16.7913818359375,16.878120422363281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.057075500488281,18.106269836425781,18.089694976806641,18.078863143920898,17.951862335205078,17.918085098266602,18.004745483398438]
[null,null,null,null,"Coincident",15.615808486938477,15.658353805541992,15.644018173217773,15.634651184082031,15.524821281433105,15.495611190795898,15.570554733276367]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.077991485595703,18.127956390380859,18.111120223999023,18.100120544433594,17.971172332763672,17.9368896484375,18.024856567382812]
[null,null,null,null,"Coincident",15.972990036010742,16.016508102416992,16.00184440612793,15.992263793945312,15.879921913146973,15.850043296813965,15.926701545715332]
[null,"Palmwoods Central","Substation Rating","MVA","Non-Coincident",30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547]
[null,null,null,null,"Coincident",30.299999237060501,30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547,30.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.601701736450195,20.512557983398437,20.543378829956055,20.505744934082031,20.325965881347656,20.243602752685547,20.259237289428711]
[null,null,null,null,"Coincident",17.211725234985352,18.07880973815918,18.105928421020508,18.0726318359375,17.913959503173828,17.841035842895508,17.854400634765625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.729461669921875,21.692724227905273,21.725315093994141,21.685518264770508,21.495395660400391,21.408292770385742,21.424827575683594]
[null,null,null,null,"Coincident",17.688249588012695,18.601509094238281,18.629396438598633,18.595094680786133,18.431760787963867,18.356618881225586,18.370231628417969]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.311887741088867,19.293148040771484,19.268533706665039,19.252420425415039,19.074108123779297,18.947290420532227,18.955076217651367]
[null,null,null,null,"Coincident",16.079174041748047,17.011629104614258,16.989879608154297,16.97553825378418,16.818078994750977,16.705915451049805,16.712347030639648]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.365440368652344,20.403154373168945,20.377126693725586,20.360084533691406,20.171514511108398,20.037399291992188,20.045633316040039]
[null,null,null,null,"Coincident",16.524341583251953,17.5059814453125,17.483583450317383,17.468782424926758,17.306669235229492,17.191131591796875,17.197607040405273]
[null,"Pandanus Avenue","Substation Rating","MVA","Non-Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,null,null,"Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.3409595489501953,9.3409595489501953,9.3409595489501953,9.3409595489501953,9.3409595489501953,9.3409595489501953,9.3409595489501953]
[null,null,null,null,"Coincident",8.0570650100708008,8.0570650100708008,8.0570650100708008,8.0570650100708008,8.0570650100708008,8.0570650100708008,8.0570650100708008]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9023981094360352,9.9023981094360352,9.9023981094360352,9.9023981094360352,9.9023981094360352,9.9023981094360352,9.9023981094360352]
[null,null,null,null,"Coincident",8.4154500961303711,8.4154500961303711,8.4154500961303711,8.4154500961303711,8.4154500961303711,8.4154500961303711,8.4154500961303711]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.8622903823852539,8.8622903823852539,8.8622903823852539,8.8622903823852539,8.8622903823852539,8.8622903823852539,8.8622903823852539]
[null,null,null,null,"Coincident",7.6441874504089355,7.6441874504089355,7.6441874504089355,7.6441874504089355,7.6441874504089355,7.6441874504089355,7.6441874504089355]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.39495849609375,9.39495849609375,9.39495849609375,9.39495849609375,9.39495849609375,9.39495849609375,9.39495849609375]
[null,null,null,null,"Coincident",7.9842076301574707,7.9842076301574707,7.9842076301574707,7.9842076301574707,7.9842076301574707,7.9842076301574707,7.9842076301574707]
[null,"Parkwood","Substation Rating","MVA","Non-Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,null,null,"Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.799655914306641,16.767715454101563,20.122945785522461,20.97161865234375,21.633508682250977,22.435798645019531,23.283197402954102]
[null,null,null,null,"Coincident",16.466732025146484,16.4354248046875,19.724163055419922,20.556018829345703,21.204792022705078,21.991182327270508,22.821786880493164]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.125177383422852,17.092617034912109,20.512861251831055,21.377979278564453,22.052692413330078,22.870529174804688,23.734348297119141]
[null,null,null,null,"Coincident",16.762126922607422,16.730258941650391,20.102170944213867,20.955659866333008,21.62244987487793,22.430007934570313,23.282657623291016]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.234813690185547,16.226039886474609,19.702066421508789,20.619102478027344,21.321334838867188,22.119234085083008,23.008659362792969]
[null,null,null,null,"Coincident",15.913084030151367,15.904483795166016,19.311624526977539,20.210487365722656,20.8988037109375,21.680891036987305,22.552690505981445]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.54939079284668,16.540447235107422,20.083826065063477,21.018630981445313,21.734472274780273,22.547830581665039,23.454490661621094]
[null,null,null,null,"Coincident",16.19854736328125,16.189792633056641,19.683467864990234,20.605546951293945,21.312911987304687,22.116340637207031,23.011266708374023]
[null,"Peregian","Substation Rating","MVA","Non-Coincident",30,39.599998474121094,39.599998474121094,39.599998474121094,39.599998474121094,39.599998474121094,39.599998474121094]
[null,null,null,null,"Coincident",30,39.599998474121094,39.599998474121094,39.599998474121094,39.599998474121094,39.599998474121094,39.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.567267417907715,13.56965446472168,13.574291229248047,13.531573295593262,13.403117179870605,13.357085227966309,13.389739036560059]
[null,null,null,null,"Coincident",12.740691184997559,12.742932319641113,12.747287750244141,12.707173347473145,12.586543083190918,12.543313980102539,12.573980331420898]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.680813789367676,13.683219909667969,13.687895774841309,13.644820213317871,13.515289306640625,13.4688720703125,13.501799583435059]
[null,null,null,null,"Coincident",12.749765396118164,12.752008438110352,12.756366729736328,12.71622371673584,12.595507621765137,12.552248001098633,12.58293628692627]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.465903282165527,11.483555793762207,11.455653190612793,11.431112289428711,11.317152976989746,11.249185562133789,11.272994041442871]
[null,null,null,null,"Coincident",10.767350196838379,10.783926963806152,10.757724761962891,10.734679222106934,10.627662658691406,10.563836097717285,10.586194038391113]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.561861991882324,11.579662322998047,11.55152702331543,11.526780128479004,11.411867141723633,11.343331336975098,11.367339134216309]
[null,null,null,null,"Coincident",10.775019645690918,10.791607856750488,10.765386581420898,10.742324829101563,10.635231971740723,10.57136058807373,10.593733787536621]
[null,"Pimpama East","Substation Rating","MVA","Non-Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,null,null,"Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.934724807739258,27.802894592285156,28.673444747924805,29.425441741943359,29.946928024291992,30.589225769042969,31.363340377807617]
[null,null,null,null,"Coincident",25.427242279052734,26.247505187988281,27.070018768310547,27.780616760253906,28.273601531982422,28.880666732788086,29.612199783325195]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.320650100708008,28.201259613037109,29.084281921386719,29.847053527832031,30.376012802124023,31.02751350402832,31.812719345092773]
[null,null,null,null,"Coincident",25.50352668762207,26.32585334777832,27.15043830871582,27.862768173217773,28.356838226318359,28.965312957763672,29.698614120483398]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.18162727355957,24.987964630126953,25.692052841186523,26.385612487792969,26.83355712890625,27.331546783447266,28.007221221923828]
[null,null,null,null,"Coincident",22.867048263549805,23.630348205566406,24.296958923339844,24.953620910644531,25.378009796142578,25.849750518798828,26.489557266235352]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.528104782104492,25.34599494934082,26.060173034667969,26.763669967651367,27.218032836914063,27.72315788269043,28.408514022827148]
[null,null,null,null,"Coincident",22.940479278564453,23.705808639526367,24.374139785766602,25.032485961914062,25.457818984985352,25.930644989013672,26.572053909301758]
[null,"Postmans Ridge","Substation Rating","MVA","Non-Coincident",7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367]
[null,null,null,null,"Coincident",7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367,7.1999998092651367]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.3643574714660645,5.2749347686767578,5.2888498306274414,5.2844228744506836,5.2181978225708008,5.2121343612670898,5.2429156303405762]
[null,null,null,null,"Coincident",5.1138324737548828,5.0285859107971191,5.0418510437011719,5.0376310348510742,4.9744987487792969,4.9687185287475586,4.9980621337890625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6272168159484863,5.533411979675293,5.548008918762207,5.5433650016784668,5.4738950729370117,5.4675345420837402,5.499824047088623]
[null,null,null,null,"Coincident",5.1727814674377441,5.0865521430969238,5.0999703407287598,5.0957012176513672,5.0318412780761719,5.0259947776794434,5.0556764602661133]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8750090599060059,4.8002796173095703,4.7996082305908203,4.8004245758056641,4.7379865646362305,4.7202706336975098,4.7465920448303223]
[null,null,null,null,"Coincident",4.6473374366760254,4.5760979652404785,4.5754580497741699,4.5762362480163574,4.5167140960693359,4.4998254776000977,4.5249176025390625]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.113889217376709,5.0354981422424316,5.0347943305969238,5.0356502532958984,4.9701528549194336,4.951568603515625,4.979179859161377]
[null,null,null,null,"Coincident",4.7009086608886719,4.6288480758666992,4.6282010078430176,4.6289877891540527,4.5687799453735352,4.5516963005065918,4.5770778656005859]
[null,"Queensport","Substation Rating","MVA","Non-Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,null,null,"Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.439291000366211,27.307647705078125,27.326990127563477,27.209405899047852,26.864255905151367,26.605186462402344,26.442144393920898]
[null,null,null,null,"Coincident",25.586336135864258,25.463582992553711,25.481618881225586,25.371974945068359,25.050132751464844,24.808557510375977,24.656526565551758]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.728538513183594,27.587762832641602,27.608440399169922,27.48277473449707,27.114397048950195,26.838388442993164,26.664913177490234]
[null,null,null,null,"Coincident",25.653141021728516,25.528049468994141,25.546426773071289,25.434715270996094,25.106952667236328,24.861080169677734,24.706413269042969]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.474586486816406,26.383493423461914,26.329034805297852,26.242166519165039,25.896831512451172,25.58091926574707,25.415828704833984]
[null,null,null,null,"Coincident",24.686777114868164,24.601835250854492,24.551054000854492,24.470052719116211,24.148036956787109,23.853458404541016,23.699516296386719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.699417114257813,26.60255241394043,26.544670104980469,26.452381134033203,26.086019515991211,25.751617431640625,25.577159881591797]
[null,null,null,null,"Coincident",24.7371826171875,24.650785446166992,24.599142074584961,24.516777038574219,24.189495086669922,23.89031982421875,23.734062194824219]
[null,"Raby Bay","Substation Rating","MVA","Non-Coincident",47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906]
[null,null,null,null,"Coincident",47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906,47.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.364038467407227,29.306821823120117,29.240512847900391,29.149440765380859,28.84101676940918,28.690181732177734,28.920331954956055]
[null,null,null,null,"Coincident",27.687957763671875,27.634008407592773,27.571483612060547,27.485607147216797,27.194789886474609,27.052562713623047,27.269577026367188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.708328247070313,29.648704528808594,29.579610824584961,29.484722137451172,29.163459777832031,29.006393432617187,29.246063232421875]
[null,null,null,null,"Coincident",27.69297981262207,27.638803482055664,27.576023101806641,27.48980712890625,27.197929382324219,27.055234909057617,27.272975921630859]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.560901641845703,26.545291900634766,26.41185188293457,26.35612678527832,26.064723968505859,25.861509323120117,26.060432434082031]
[null,null,null,null,"Coincident",25.044824600219727,25.03010368347168,24.904281616210937,24.851736068725586,24.57696533203125,24.385351181030273,24.572919845581055]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.792861938476562,26.776662826538086,26.638198852539063,26.58038330078125,26.278154373168945,26.067483901977539,26.273704528808594]
[null,null,null,null,"Coincident",25.706676483154297,25.691566467285156,25.562419891357422,25.508485794067383,25.22645378112793,25.029775619506836,25.222301483154297]
[null,"Redbank","Substation Rating","MVA","Non-Coincident",43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094]
[null,null,null,null,"Coincident",43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094,43.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.623390197753906,11.540690422058105,11.542549133300781,11.490992546081543,11.343673706054688,11.232681274414063,11.215474128723145]
[null,null,null,null,"Coincident",11.308742523193359,11.228281021118164,11.230090141296387,11.179928779602051,11.036598205566406,10.928609848022461,10.911869049072266]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.666721343994141,11.580185890197754,11.58212947845459,11.528256416320801,11.374651908874512,11.259259223937988,11.241395950317383]
[null,null,null,null,"Coincident",11.549749374389648,11.467573165893555,11.469420433044434,11.418190002441406,11.271804809570313,11.161515235900879,11.144417762756348]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.199356079101562,11.134833335876465,11.105772972106934,11.06731128692627,10.920171737670898,10.785423278808594,10.765375137329102]
[null,null,null,null,"Coincident",10.896186828613281,10.83341121673584,10.805137634277344,10.767716407775879,10.624560356140137,10.493459701538086,10.473954200744629]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.22467041015625,11.157779693603516,11.127685546875,11.087889671325684,10.935994148254395,10.797391891479492,10.776812553405762]
[null,null,null,null,"Coincident",11.128401756286621,11.064288139343262,11.035411834716797,10.997193336486816,10.850986480712891,10.71709156036377,10.697170257568359]
[null,"Redbank Plains","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.216999053955078,29.779718399047852,30.421571731567383,30.951169967651367,31.258594512939453,31.811882019042969,32.524684906005859]
[null,null,null,null,"Coincident",28.289279937744141,28.834133148193359,29.455602645874023,29.968387603759766,30.266048431396484,30.801769256591797,31.491935729980469]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.489810943603516,31.077045440673828,31.746860504150391,32.299530029296875,32.620346069335937,33.197738647460937,33.941593170166016]
[null,null,null,null,"Coincident",28.645605087280273,29.197320938110352,29.826618194580078,30.345861434936523,30.647272109985352,31.189741134643555,31.888601303100586]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.065153121948242,25.582742691040039,26.061729431152344,26.542154312133789,26.792900085449219,27.196792602539062,27.797079086303711]
[null,null,null,null,"Coincident",24.269266128540039,24.770418167114258,25.234197616577148,25.699365615844727,25.942150115966797,26.333217620849609,26.91444206237793]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.157094955444336,26.697231292724609,27.197084426879883,27.69843864440918,27.960107803344727,28.381595611572266,29.008033752441406]
[null,null,null,null,"Coincident",24.574956893920898,25.082420349121094,25.552042007446289,26.023069381713867,26.268911361694336,26.664905548095703,27.253450393676758]
[null,"Redcliffe","Substation Rating","MVA","Non-Coincident",28.299999237060547,28.299999237060547,32.599998474121094,32.599998474121094,32.599998474121094,32.599998474121094,32.599998474121094]
[null,null,null,null,"Coincident",28.299999237060547,28.299999237060547,32.599998474121094,32.599998474121094,32.599998474121094,32.599998474121094,32.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.694252014160156,19.559675216674805,19.56121826171875,19.473115921020508,19.222141265869141,19.032779693603516,19.28254508972168]
[null,null,null,null,"Coincident",18.620212554931641,18.492975234985352,18.494434356689453,18.411136627197266,18.173849105834961,17.994813919067383,18.230958938598633]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.940444946289063,19.798862457275391,19.800485610961914,19.707828521728516,19.44401741027832,19.245111465454102,19.507492065429688]
[null,null,null,null,"Coincident",19.151210784912109,19.020345687866211,19.021846771240234,18.936172485351563,18.692117691040039,18.507978439331055,18.750856399536133]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.755121231079102,18.652359008789063,18.602149963378906,18.537031173706055,18.289327621459961,18.062429428100586,18.29347038269043]
[null,null,null,null,"Coincident",17.732297897338867,17.635139465332031,17.587669372558594,17.526102066040039,17.291906356811523,17.077383041381836,17.29582405090332]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.95368766784668,18.845901489257813,18.793252944946289,18.724983215332031,18.465442657470703,18.227916717529297,18.469781875610352]
[null,null,null,null,"Coincident",18.23797607421875,18.138046264648438,18.089221954345703,18.025899887084961,17.785024642944336,17.564384460449219,17.789054870605469]
[null,"Redland Bay","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.851877212524414,18.999902725219727,19.158971786499023,19.262308120727539,19.237997055053711,19.300790786743164,19.441493988037109]
[null,null,null,null,"Coincident",15.033542633056641,15.151588439941406,15.278438568115234,15.360846519470215,15.341458320617676,15.391533851623535,15.50373649597168]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.868810653686523,19.01881217956543,19.180109024047852,19.284948348999023,19.260280609130859,19.324001312255859,19.466842651367188]
[null,null,null,null,"Coincident",15.131908416748047,15.250726699829102,15.37840747833252,15.46135425567627,15.441839218139648,15.492242813110352,15.605178833007813]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.586952209472656,16.739988327026367,16.833368301391602,16.941221237182617,16.911705017089844,16.923130035400391,17.040916442871094]
[null,null,null,null,"Coincident",13.227368354797363,13.349406242370605,13.423873901367187,13.509881973266602,13.486343383789063,13.495453834533691,13.589384078979492]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.587041854858398,16.740316390991211,16.833913803100586,16.942083358764648,16.912473678588867,16.923934936523438,17.042133331298828]
[null,null,null,null,"Coincident",13.313916206359863,13.436753273010254,13.51170825958252,13.598278999328613,13.574585914611816,13.583756446838379,13.678300857543945]
[null,"Robina","Substation Rating","MVA","Non-Coincident",131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437]
[null,null,null,null,"Coincident",131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437,131.39999389648437]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",52.965007781982422,52.832927703857422,53.003196716308594,52.886466979980469,52.309864044189453,51.924556732177734,51.736099243164062]
[null,null,null,null,"Coincident",52.938621520996094,52.806606292724609,52.976791381835938,52.860118865966797,52.283805847167969,51.898689270019531,51.7103271484375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.032485961914063,52.898216247558594,53.071315765380859,52.952640533447266,52.366786956787109,51.975635528564453,51.784416198730469]
[null,null,null,null,"Coincident",52.956752777099609,52.823993682861328,52.995140075683594,52.877803802490234,52.298385620117187,51.911346435546875,51.722087860107422]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.007381439208984,47.952953338623047,47.974216461181641,47.91680908203125,47.371604919433594,46.901348114013672,46.7158203125]
[null,null,null,null,"Coincident",47.983467102050781,47.929065704345703,47.9503173828125,47.892936706542969,47.348007202148438,46.877983093261719,46.692546844482422]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.015964508056641,47.961181640625,47.982582092285156,47.9248046875,47.376502990722656,46.904159545898438,46.717964172363281]
[null,null,null,null,"Coincident",47.984092712402344,47.929630279541016,47.950904846191406,47.893459320068359,47.348110198974609,47.186893463134766,46.997802734375]
[null,"Rocklea","Substation Rating","MVA","Non-Coincident",31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727]
[null,null,null,null,"Coincident",31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727,31.600000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.938360214233398,22.766578674316406,22.794712066650391,22.713790893554688,22.42167854309082,22.201433181762695,22.061309814453125]
[null,null,null,null,"Coincident",17.233295440673828,17.104238510131836,17.125373840332031,17.064579010009766,16.845119476318359,16.679651260375977,16.574378967285156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.938447952270508,23.394088745117188,23.424533843994141,23.336969375610352,23.020999908447266,22.782901763916016,22.631481170654297]
[null,null,null,null,"Coincident",17.239130020141602,17.109024047851563,17.130325317382813,17.069063186645508,16.84809684753418,16.681686401367188,16.575904846191406]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.600191116333008,22.461523056030273,22.426969528198242,22.369882583618164,22.071577072143555,21.798381805419922,21.653709411621094]
[null,null,null,null,"Coincident",16.979232788085938,16.875053405761719,16.849094390869141,16.806205749511719,16.58209228515625,16.37684440612793,16.268154144287109]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.214067459106445,23.0640869140625,23.026721954345703,22.964994430541992,22.642574310302734,22.347490310668945,22.191305160522461]
[null,null,null,null,"Coincident",16.984193801879883,16.879215240478516,16.853067398071289,16.809877395629883,16.584365844726563,16.378118515014648,16.269012451171875]
[null,"Roderick St","Substation Rating","MVA","Non-Coincident",49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547]
[null,null,null,null,"Coincident",49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.168369293212891,29.109195709228516,29.180870056152344,29.078466415405273,28.698558807373047,28.406312942504883,28.236244201660156]
[null,null,null,null,"Coincident",27.285886764526367,27.230531692504883,27.297580718994141,27.201786041259766,26.846397399902344,26.573013305664063,26.413919448852539]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.710077285766602,30.644046783447266,30.724027633666992,30.609756469726562,30.185937881469727,29.860036849975586,29.670433044433594]
[null,null,null,null,"Coincident",27.382076263427734,27.325531005859375,27.394023895263672,27.296167373657227,26.933271408081055,26.654264450073242,26.491960525512695]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.418216705322266,27.399900436401367,27.391269683837891,27.322654724121094,26.952724456787109,26.609424591064453,26.441450119018555]
[null,null,null,null,"Coincident",25.648687362670898,25.631551742553711,25.623477935791016,25.559291839599609,25.213235855102539,24.892093658447266,24.734958648681641]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.758991241455078,28.738594055175781,28.728982925415039,28.652578353881836,28.24077033996582,27.858795166015625,27.671966552734375]
[null,null,null,null,"Coincident",25.711963653564453,25.694509506225586,25.686286926269531,25.620918273925781,25.268634796142578,24.94194221496582,24.782175064086914]
[null,"Rosewood","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",12,12,12,12,12,12,12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.6700787544250488,6.5798153877258301,6.5936427116394043,6.6020035743713379,6.6477770805358887,6.7170462608337402,6.7260856628417969]
[null,null,null,null,"Coincident",5.724461555480957,5.6469950675964355,5.6588621139526367,5.6660375595092773,5.7053217887878418,5.7647705078125,5.7725286483764648]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.768409252166748,6.6719574928283691,6.6867251396179199,6.6956558227539062,6.7445673942565918,6.8186445236206055,6.8283166885375977]
[null,null,null,null,"Coincident",5.992671012878418,5.9117727279663086,5.9241786003112793,5.9316220283508301,5.9724879264831543,6.0344581604003906,6.0424871444702148]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.07159423828125,5.9983396530151367,5.9942264556884766,6.0076179504394531,6.0453872680664062,6.0916347503662109,6.0974907875061035]
[null,null,null,null,"Coincident",5.2108244895935059,5.1479549407958984,5.1444249153137207,5.1559181213378906,5.1883325576782227,5.2280235290527344,5.2330493927001953]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.131411075592041,6.0538911819458008,6.0495414733886719,6.0637035369873047,6.103665828704834,6.1526374816894531,6.1588411331176758]
[null,null,null,null,"Coincident",5.4568996429443359,5.391268253326416,5.3875532150268555,5.3995180130004883,5.433192253112793,5.4744830131530762,5.4796500205993652]
[null,"Runcorn","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.023494720458984,23.007015228271484,22.988510131835938,22.94764518737793,22.74406623840332,22.663763046264648,22.814298629760742]
[null,null,null,null,"Coincident",20.876996994018555,20.862051010131836,20.845273971557617,20.808221817016602,20.623620986938477,20.550806045532227,20.687307357788086]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.087556838989258,23.070745468139648,23.05186653137207,23.01017951965332,22.802566528320313,22.720699310302734,22.874179840087891]
[null,null,null,null,"Coincident",21.30775260925293,21.292499542236328,21.275375366210938,21.237558364868164,21.049148559570312,20.974832534790039,21.11414909362793]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.24915885925293,21.262897491455078,21.18693733215332,21.170591354370117,20.972690582275391,20.844720840454102,20.976301193237305]
[null,null,null,null,"Coincident",19.268083572387695,19.280542373657227,19.211662292480469,19.196842193603516,19.017391204833984,18.901351928710937,19.020668029785156]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.281351089477539,21.295303344726563,21.218172073364258,21.201576232910156,21.000717163085938,20.870901107788086,21.00438117980957]
[null,null,null,null,"Coincident",19.665643692016602,19.67835807800293,19.608057022094727,19.592931747436523,19.409778594970703,19.291343688964844,19.413122177124023]
[null,"Russell Island","Substation Rating","MVA","Non-Coincident",20.600000381469727,20.600000381469727,20.600000381469727,20.600000381469727,20.600000381469727,20.600000381469727,20.600000381469727]
[null,null,null,null,"Coincident",20.600000381469702,20.600000381469702,20.600000381469702,20.600000381469702,20.600000381469702,20.600000381469702,20.600000381469702]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.2966160774230957,5.2950448989868164,5.2965154647827148,5.2880373001098633,5.2604484558105469,5.2845573425292969,5.3538417816162109]
[null,null,null,null,"Coincident",4.3217506408691406,4.3204689025878906,4.3216686248779297,4.314751148223877,4.2922396659851074,4.3119115829467773,4.3684439659118652]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.3882260322570801,5.3866281509399414,5.3881235122680664,5.3794994354248047,5.351433277130127,5.3759589195251465,5.446441650390625]
[null,null,null,null,"Coincident",4.3718900680541992,4.3705935478210449,4.3718070983886719,4.364809513092041,4.3420367240905762,4.3619370460510254,4.4191250801086426]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.9611983299255371,4.9664883613586426,4.9541044235229492,4.9511594772338867,4.9229602813720703,4.9327630996704102,4.9957985877990723]
[null,null,null,null,"Coincident",4.048067569732666,4.0523843765258789,4.0422797203063965,4.0398769378662109,4.0168676376342773,4.0248656272888184,4.0762991905212402]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0470070838928223,5.0523886680603027,5.0397906303405762,5.0367946624755859,5.0081076622009277,5.0180797576904297,5.0822057723999023]
[null,null,null,null,"Coincident",4.0950322151184082,4.0993990898132324,4.089177131652832,4.0867462158203125,4.0634698867797852,4.0715608596801758,4.1235909461975098]
[null,"Salisbury","Substation Rating","MVA","Non-Coincident",15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863]
[null,null,null,null,"Coincident",15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863,15.800000190734863]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.600189208984375,8.5367832183837891,8.5083808898925781,8.4726295471191406,8.5560140609741211,8.5056524276733398,8.4659566879272461]
[null,null,null,null,"Coincident",7.6635842323303223,7.5727729797363281,7.5762953758239746,7.5433378219604492,7.4482865333557129,7.3757829666137695,7.3244228363037109]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.6634817123413086,8.5971946716308594,8.5675182342529297,8.5301752090454102,8.6172943115234375,8.5646677017211914,8.5232067108154297]
[null,null,null,null,"Coincident",7.6719231605529785,7.5810127258300781,7.5845389366149902,7.5515456199645996,7.4563908576965332,7.3838086128234863,7.332392692565918]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.2008647918701172,8.1246442794799805,8.0855255126953125,8.0331954956054687,8.0973796844482422,8.0258293151855469,7.9597353935241699]
[null,null,null,null,"Coincident",6.4376482963562012,6.3700370788574219,6.3553438186645508,6.3340749740600586,6.2512550354003906,6.1744318008422852,6.1294288635253906]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.2468347549438477,8.16754150390625,8.1268768310546875,8.0725116729736328,8.1391973495483398,8.0648622512817383,7.9962606430053711]
[null,null,null,null,"Coincident",6.4377017021179199,6.3700900077819824,6.3553962707519531,6.3341274261474609,6.2513065338134766,6.1744828224182129,6.1294794082641602]
[null,"Samford","Substation Rating","MVA","Non-Coincident",59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453]
[null,null,null,null,"Coincident",59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453,59.200000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.251632690429688,17.281745910644531,17.315481185913086,17.279163360595703,17.134639739990234,17.084938049316406,17.095691680908203]
[null,null,null,null,"Coincident",15.620708465576172,15.647974014282227,15.678520202636719,15.645636558532715,15.514774322509766,15.469772338867188,15.479507446289063]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.878913879394531,17.910121917724609,17.945083618164063,17.907444000244141,17.757665634155273,17.706157684326172,17.717302322387695]
[null,null,null,null,"Coincident",15.864988327026367,15.892680168151855,15.923704147338867,15.89030647277832,15.757397651672363,15.711691856384277,15.721579551696777]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.850150108337402,14.896353721618652,14.884079933166504,14.867833137512207,14.736391067504883,14.655734062194824,14.660155296325684]
[null,null,null,null,"Coincident",13.446256637573242,13.488090515136719,13.476978302001953,13.462267875671387,13.343250274658203,13.270219802856445,13.274222373962402]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.390110015869141,15.437994956970215,15.425274848937988,15.40843677520752,15.272215843200684,15.188626289367676,15.193207740783691]
[null,null,null,null,"Coincident",13.656532287597656,13.699020385742188,13.687734603881836,13.672794342041016,13.551915168762207,13.477742195129395,13.481807708740234]
[null,"Sandgate","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.861232757568359,34.593418121337891,34.4791259765625,34.36920166015625,34.125331878662109,34.072116851806641,34.129890441894531]
[null,null,null,null,"Coincident",31.828027725219727,31.583518981933594,31.479169845581055,31.378807067871094,31.156154632568359,31.107570648193359,31.160322189331055]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.635288238525391,35.352188110351562,35.231391906738281,35.115219116210937,34.857528686523438,34.801303863525391,34.862342834472656]
[null,null,null,null,"Coincident",32.307819366455078,32.059623718261719,31.953702926635742,31.851827621459961,31.625818252563477,31.576501846313477,31.630048751831055]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.452959060668945,31.253885269165039,31.064321517944336,30.996492385864258,30.761758804321289,30.634544372558594,30.676445007324219]
[null,null,null,null,"Coincident",28.716302871704102,28.534549713134766,28.361480712890625,28.299552917480469,28.085241317749023,27.969095230102539,28.007350921630859]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.037105560302734,31.827281951904297,31.627519607543945,31.556051254272461,31.30876350402832,31.174768447875977,31.218900680541992]
[null,null,null,null,"Coincident",29.149187088012695,28.964693069458008,28.789016723632813,28.726154327392578,28.508611679077148,28.390714645385742,28.429548263549805]
[null,"Scarborough","Substation Rating","MVA","Non-Coincident",45.5,45.5,45.5,45.5,45.5,45.5,45.5]
[null,null,null,null,"Coincident",45.5,45.5,45.5,45.5,45.5,45.5,45.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.69786262512207,19.691568374633789,19.685125350952148,19.637226104736328,19.473554611206055,19.443023681640625,19.573112487792969]
[null,null,null,null,"Coincident",17.655130386352539,17.649490356445313,17.643716812133789,17.600784301757813,17.454084396362305,17.426721572875977,17.543317794799805]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.677890777587891,20.671283721923828,20.664520263671875,20.614236831665039,20.442422866821289,20.410371780395508,20.546932220458984]
[null,null,null,null,"Coincident",17.824058532714844,17.818365097045898,17.812536239624023,17.769191741943359,17.621088027954102,17.593463897705078,17.711175918579102]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.226835250854492,17.244810104370117,17.191408157348633,17.166860580444336,17.015596389770508,16.945085525512695,17.052875518798828]
[null,null,null,null,"Coincident",15.440356254577637,15.45646858215332,15.408602714538574,15.386601448059082,15.251023292541504,15.187825202941895,15.284436225891113]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.083921432495117,18.102790832519531,18.046731948852539,18.020961761474609,17.862173080444336,17.788154602050781,17.90130615234375]
[null,null,null,null,"Coincident",15.588092803955078,15.60435962677002,15.556035995483398,15.53382396697998,15.39694881439209,15.333146095275879,15.430681228637695]
[null,"Scrub Road","Substation Rating","MVA","Non-Coincident",46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453]
[null,null,null,null,"Coincident",46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453,46.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.646270751953125,33.608867645263672,33.5621337890625,33.438976287841797,33.054492950439453,32.824821472167969,32.913295745849609]
[null,null,null,null,"Coincident",31.837913513183594,31.802518844604492,31.758298873901367,31.641759872436523,31.27794075012207,31.060613632202148,31.144336700439453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.663158416748047,33.625358581542969,33.578136444091797,33.453720092773437,33.06561279296875,32.834003448486328,32.923202514648438]
[null,null,null,null,"Coincident",31.896171569824219,31.860349655151367,31.815597534179688,31.697666168212891,31.329580307006836,31.109762191772461,31.194438934326172]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.546470642089844,30.554113388061523,30.427095413208008,30.34599494934082,29.982656478881836,29.697505950927734,29.767805099487305]
[null,null,null,null,"Coincident",28.904712677001953,28.911943435668945,28.791751861572266,28.715011596679688,28.371200561523437,28.101377487182617,28.167898178100586]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.015405654907227,31.023399353027344,30.890548706054688,30.805732727050781,30.42582893371582,30.127771377563477,30.201244354248047]
[null,null,null,null,"Coincident",28.93181037902832,28.939105987548828,28.817838668823242,28.740419387817383,28.393659591674805,28.121627807617188,28.188684463500977]
[null,"Sherwood","Substation Rating","MVA","Non-Coincident",59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453]
[null,null,null,null,"Coincident",59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453,59.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.953386306762695,29.634408950805664,29.345613479614258,29.101709365844727,28.896726608276367,28.953889846801758,29.026840209960938]
[null,null,null,null,"Coincident",28.836353302001953,28.529273986816406,28.251247406005859,28.016439437866211,27.819099426269531,27.87413215637207,27.944362640380859]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.264148712158203,29.933395385742188,29.634040832519531,29.381298065185547,29.168943405151367,29.228157043457031,29.303730010986328]
[null,null,null,null,"Coincident",28.854349136352539,28.545034408569336,28.265092849731445,28.028751373291016,27.830184936523438,27.885553359985352,27.956220626831055]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.419902801513672,25.183490753173828,24.868982315063477,24.687143325805664,24.501468658447266,24.486595153808594,24.540254592895508]
[null,null,null,null,"Coincident",24.47193717956543,24.244342803955078,23.941558837890625,23.766502380371094,23.587753295898437,23.573434829711914,23.625091552734375]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.576240539550781,25.332677841186523,25.008825302124023,24.821672439575195,24.630641937255859,24.61534309387207,24.670541763305664]
[null,null,null,null,"Coincident",24.471942901611328,24.874805450439453,24.56414794921875,24.384538650512695,24.201141357421875,24.186450958251953,24.239450454711914]
[null,"Somerset Dam","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.44008922576904297,0.44053038954734802,0.44115835428237915,0.44223609566688538,0.44406160712242126,0.44664132595062256,0.44938153028488159]
[null,null,null,null,"Coincident",0.31040191650390625,0.31071308255195618,0.3111560046672821,0.31191614270210266,0.31320372223854065,0.31502321362495422,0.31695592403411865]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.48500564694404602,0.48549184203147888,0.48618391156196594,0.48737165331840515,0.48938345909118652,0.49222648143768311,0.49524635076522827]
[null,null,null,null,"Coincident",0.3179624080657959,0.3182811439037323,0.31873485445976257,0.31951352953910828,0.32083246111869812,0.3226962685585022,0.32467606663703918]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.39496895670890808,0.39536488056182861,0.39592850208282471,0.39689570665359497,0.39853408932685852,0.40084928274154663,0.40330854058265686]
[null,null,null,null,"Coincident",0.27857786417007446,0.27885711193084717,0.27925461530685425,0.27993682026863098,0.28109240531921387,0.28272536396980286,0.2844599187374115]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.43528032302856445,0.4357166588306427,0.43633779883384705,0.43740370869636536,0.43920931220054626,0.44176080822944641,0.44447106122970581]
[null,null,null,null,"Coincident",0.28536322712898254,0.28564926981925964,0.28605645895004272,0.2867552638053894,0.28793901205062866,0.28961172699928284,0.29138854146003723]
[null,"Southport","Substation Rating","MVA","Non-Coincident",172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219]
[null,null,null,null,"Coincident",172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219,172.69999694824219]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",77.02032470703125,76.7930908203125,76.828079223632813,76.511428833007813,75.554878234863281,74.840385437011719,74.396041870117187]
[null,null,null,null,"Coincident",73.942924499511719,73.724769592285156,73.75836181640625,73.454360961914063,72.536033630371094,71.850090026855469,71.423500061035156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",77.133392333984375,76.900711059570313,76.936531066894531,76.612457275390625,75.634933471679688,74.906211853027344,74.453666687011719]
[null,null,null,null,"Coincident",73.956993103027344,73.737876892089844,73.771614074707031,73.466323852539062,72.544479370117188,71.856277465820313,71.428451538085938]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",73.583305358886719,73.466232299804687,73.296073913574219,73.067543029785156,72.119361877441406,71.253044128417969,70.806808471679688]
[null,null,null,null,"Coincident",70.643234252929688,70.530838012695312,70.367477416992188,70.148078918457031,69.237785339355469,68.406082153320313,67.977676391601563]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",73.627227783203125,73.508323669433594,73.335563659667969,73.103668212890625,72.143020629882813,71.26751708984375,70.817390441894531]
[null,null,null,null,"Coincident",70.646270751953125,70.533638000488281,70.369949340820313,70.150131225585937,69.238525390625,68.40618896484375,67.977676391601563]
[null,"Spring Creek","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6464581489562988,4.6114277839660645,4.611473560333252,4.5903820991516113,4.5308961868286133,4.485933780670166,4.4571614265441895]
[null,null,null,null,"Coincident",4.2499828338623047,4.2179417610168457,4.2179837226867676,4.1986918449401855,4.1442818641662598,4.1031560897827148,4.076838493347168]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1982283592224121,5.1590375900268555,5.1590890884399414,5.1354928016662598,5.0689435005187988,5.018641471862793,4.986452579498291]
[null,null,null,null,"Coincident",4.5693821907043457,4.5349330902099609,4.534977912902832,4.5142364501953125,4.4557371139526367,4.4115209579467773,4.3832254409790039]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.2751884460449219,4.2487421035766602,4.2370133399963379,4.2218852043151855,4.1651716232299805,4.1131987571716309,4.0854778289794922]
[null,null,null,null,"Coincident",3.910393238067627,3.8862032890319824,3.8754754066467285,3.8616383075714111,3.8097639083862305,3.762225866317749,3.736870288848877]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.782869815826416,4.7532830238342285,4.7401614189147949,4.7232365608215332,4.6597886085510254,4.6016440391540527,4.5706310272216797]
[null,null,null,null,"Coincident",4.2042713165283203,4.1782631874084473,4.1667294502258301,4.1518521308898926,4.0960793495178223,4.0449686050415039,4.017707347869873]
[null,"Springfield","Substation Rating","MVA","Non-Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,null,null,"Coincident",59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906,59.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.762180328369141,34.759323120117188,34.945014953613281,34.970127105712891,34.789146423339844,34.870170593261719,35.111495971679688]
[null,null,null,null,"Coincident",34.762180328369141,34.759323120117188,34.945014953613281,34.970127105712891,34.789146423339844,34.870170593261719,35.111495971679688]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.058319091796875,35.055377960205078,35.246406555175781,35.272239685058594,35.0860595703125,35.169406890869141,35.417686462402344]
[null,null,null,null,"Coincident",34.791500091552734,34.788623809814453,34.975666046142578,35.000965118408203,34.818660736083984,34.900276184082031,35.143379211425781]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.545446395874023,30.584577560424805,30.662778854370117,30.71574592590332,30.542091369628906,30.534235000610352,30.73548698425293]
[null,null,null,null,"Coincident",30.545446395874023,30.584577560424805,30.662778854370117,30.71574592590332,30.542091369628906,30.534235000610352,30.73548698425293]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.727567672729492,30.767684936523437,30.847862243652344,30.902170181274414,30.724128723144531,30.716073989868164,30.92241096496582]
[null,null,null,null,"Coincident",30.551334381103516,30.590610504150391,30.669103622436523,30.722272872924805,30.547967910766602,30.540082931518555,30.742090225219727]
[null,"Springfield Central","Substation Rating","MVA","Non-Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,null,null,"Coincident",54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906,54.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.351137161254883,17.935041427612305,18.79863166809082,19.584978103637695,20.210300445556641,21.363605499267578,22.590362548828125]
[null,null,null,null,"Coincident",16.103399276733398,17.669883728027344,18.519996643066406,19.294004440307617,19.90937614440918,21.048995971679688,22.26092529296875]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.358386993408203,17.9429931640625,18.806964874267578,19.593662261962891,20.219261169433594,21.373077392578125,22.600378036499023]
[null,null,null,null,"Coincident",16.111562728881836,17.681064605712891,18.531463623046875,19.305709838867188,19.921226501464844,21.062759399414062,22.276676177978516]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.979909896850586,15.495807647705078,16.181808471679687,16.861078262329102,17.377004623413086,18.395467758178711,19.514297485351563]
[null,null,null,null,"Coincident",13.769606590270996,15.269546508789063,15.94480037689209,16.613414764404297,17.121086120605469,18.128133773803711,19.234018325805664]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.98610782623291,15.502677917480469,16.188982009887695,16.868555068969727,17.384710311889648,18.403623580932617,19.52294921875]
[null,null,null,null,"Coincident",13.777076721191406,15.280242919921875,15.955698013305664,16.624509811401367,17.132272720336914,18.141313552856445,19.249296188354492]
[null,"St Lucia","Substation Rating","MVA","Non-Coincident",49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547]
[null,null,null,null,"Coincident",49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547,49.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.818059921264648,25.811479568481445,25.829946517944336,25.730287551879883,25.415458679199219,25.182016372680664,25.039493560791016]
[null,null,null,null,"Coincident",24.444339752197266,24.4381103515625,24.455595016479492,24.361238479614258,24.063159942626953,23.842140197753906,23.707199096679688]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.402393341064453,26.395376205444336,26.415069580078125,26.308799743652344,25.97319221496582,25.724451065063477,25.5726318359375]
[null,null,null,null,"Coincident",24.593938827514648,24.587520599365234,24.605537414550781,24.50831413269043,24.201297760009766,23.97376823425293,23.834903717041016]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.325756072998047,25.35382080078125,25.301668167114258,25.229454040527344,24.908769607543945,24.616306304931641,24.468967437744141]
[null,null,null,null,"Coincident",23.978231430053711,24.004802703857422,23.955425262451172,23.887052536010742,23.583431243896484,23.306529998779297,23.167030334472656]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.877599716186523,25.907506942749023,25.851932525634766,25.774990081787109,25.433412551879883,25.122055053710938,24.965255737304688]
[null,null,null,null,"Coincident",24.113855361938477,24.141212463378906,24.090377807617188,24.019994735717773,23.707571029663086,23.422817230224609,23.279426574707031]
[null,"Stafford","Substation Rating","MVA","Non-Coincident",59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906]
[null,null,null,null,"Coincident",59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.961652755737305,28.543050765991211,28.503032684326172,28.731899261474609,28.675586700439453,28.51801872253418,28.474166870117188]
[null,null,null,null,"Coincident",27.360733032226562,26.96527099609375,26.927465438842773,27.143678665161133,27.090480804443359,26.941623687744141,26.900196075439453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.201982498168945,28.770017623901367,28.728733062744141,28.964868545532227,28.906761169433594,28.744194030761719,28.698955535888672]
[null,null,null,null,"Coincident",27.395219802856445,26.995456695556641,26.957252502441406,27.175777435302734,27.122003555297852,26.971559524536133,26.929695129394531]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.456132888793945,25.122402191162109,25.017675399780273,25.24397087097168,25.182384490966797,24.979394912719727,24.932817459106445]
[null,null,null,null,"Coincident",24.048986434936523,23.733707427978516,23.634771347045898,23.84855842590332,23.790374755859375,23.598606109619141,23.554603576660156]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.591899871826172,25.24920654296875,25.141706466674805,25.374017715454102,25.310783386230469,25.102418899536133,25.054616928100586]
[null,null,null,null,"Coincident",24.05537223815918,23.738483428955078,23.639087677001953,23.853897094726563,23.795425415039063,23.602758407592773,23.558561325073242]
[null,"Stapylton","Substation Rating","MVA","Non-Coincident",54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906]
[null,null,null,null,"Coincident",54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906,54.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.117355346679687,10.106694221496582,10.115620613098145,10.078146934509277,9.9565401077270508,9.8658819198608398,9.8087253570556641]
[null,null,null,null,"Coincident",7.8031601905822754,7.7949376106262207,7.8018221855163574,7.7729201316833496,7.6791291236877441,7.6092071533203125,7.56512451171875]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.155693054199219,11.143938064575195,11.153780937194824,11.112461090087891,10.978373527526855,10.878411293029785,10.815388679504395]
[null,null,null,null,"Coincident",7.9203019142150879,7.9119558334350586,7.9189434051513672,7.8896079063415527,7.7944087982177734,7.7234368324279785,7.6786928176879883]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.094229698181152,10.09734058380127,10.07826042175293,10.051044464111328,9.924992561340332,9.8092460632324219,9.7492237091064453]
[null,null,null,null,"Coincident",7.7853240966796875,7.7877235412597656,7.7730073928833008,7.7520170211791992,7.6547970771789551,7.565526008605957,7.519233226776123]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.130193710327148,11.133625030517578,11.11258602142334,11.082576751708984,10.943588256835938,10.815962791442871,10.74977970123291]
[null,null,null,null,"Coincident",7.9021978378295898,7.9046335220336914,7.8896961212158203,7.8683905601501465,7.7697114944458008,7.6791000366210938,7.6321125030517578]
[null,"Stradbroke Is","Substation Rating","MVA","Non-Coincident",7.5,7.5,7.5,7.5,7.5,7.5,7.5]
[null,null,null,null,"Coincident",7.5,7.5,7.5,7.5,7.5,7.5,7.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.8518204689025879,5.8731307983398437,5.9099040031433105,5.9449505805969238,5.9426670074462891,5.9662380218505859,6.0127487182617187]
[null,null,null,null,"Coincident",2.8664822578430176,2.8769209384918213,2.8949344158172607,2.9121015071868896,2.9109828472137451,2.9225292205810547,2.9453120231628418]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.192573070526123,6.2151241302490234,6.2540388107299805,6.2911257743835449,6.2887096405029297,6.3136529922485352,6.3628721237182617]
[null,null,null,null,"Coincident",2.9435930252075195,2.9543123245239258,2.9728105068206787,2.9904394149780273,2.989290714263916,3.0011475086212158,3.024543285369873]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.4490675926208496,5.4763669967651367,5.4953889846801758,5.5335488319396973,5.5287642478942871,5.536372184753418,5.5777044296264648]
[null,null,null,null,"Coincident",2.6691956520080566,2.6825683116912842,2.6918861865997314,2.710578441619873,2.7082350254058838,2.7119617462158203,2.7322080135345459]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.7663674354553223,5.7952570915222168,5.8153862953186035,5.8557682037353516,5.8507051467895508,5.8587560653686523,5.9024953842163086]
[null,null,null,null,"Coincident",2.7409992218017578,2.7547314167022705,2.7643001079559326,2.7834951877593994,2.7810885906219482,2.7849156856536865,2.8057065010070801]
[null,"Strathpine","Substation Rating","MVA","Non-Coincident",52.5,52.5,52.5,52.5,52.5,52.5,52.5]
[null,null,null,null,"Coincident",52.5,52.5,52.5,52.5,52.5,52.5,52.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.966724395751953,26.869110107421875,26.883003234863281,26.772483825683594,26.438936233520508,26.189935684204102,26.029914855957031]
[null,null,null,null,"Coincident",22.188261032104492,22.107942581176758,22.119375228881836,22.028438568115234,21.753995895385742,21.549118041992188,21.417451858520508]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.565803527832031,27.457941055297852,27.473291397094727,27.351222991943359,26.983255386352539,26.708986282348633,26.532928466796875]
[null,null,null,null,"Coincident",22.326236724853516,22.243257522583008,22.255067825317383,22.161136627197266,21.877792358398437,21.666404724121094,21.530618667602539]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.833763122558594,26.773078918457031,26.712713241577148,26.629703521728516,26.285293579101563,25.970561981201172,25.803430557250977]
[null,null,null,null,"Coincident",22.078859329223633,22.028928756713867,21.979259490966797,21.910959243774414,21.627578735351563,21.368616104125977,21.231100082397461]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.41889762878418,27.35188102722168,27.285238265991211,27.193630218505859,26.813976287841797,26.467666625976562,26.284017562866211]
[null,null,null,null,"Coincident",22.213214874267578,22.161642074584961,22.110347747802734,22.039821624755859,21.747343063354492,21.480266571044922,21.338521957397461]
[null,"Sumner","Substation Rating","MVA","Non-Coincident",129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562]
[null,null,null,null,"Coincident",129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562,129.60000610351562]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.814029693603516,40.122703552246094,40.085964202880859,39.92327880859375,39.469696044921875,39.087955474853516,38.807651519775391]
[null,null,null,null,"Coincident",39.087825775146484,38.425739288330078,38.390552520751953,38.234748840332031,37.800350189208984,37.43475341796875,37.166305541992188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.389564514160156,40.673389434814453,40.635334014892578,40.466835021972656,39.997100830078125,39.601837158203125,39.311649322509766]
[null,null,null,null,"Coincident",39.175422668457031,38.505847930908203,38.470268249511719,38.312736511230469,37.873588562011719,37.504074096679688,37.232795715332031]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.690723419189453,35.134010314941406,35.004596710205078,34.897670745849609,34.484596252441406,34.062953948974609,33.807609558105469]
[null,null,null,null,"Coincident",34.181205749511719,33.648040771484375,33.524097442626953,33.421695709228516,33.026092529296875,32.622283935546875,32.377738952636719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.087554931640625,35.512294769287109,35.378597259521484,35.268138885498047,34.841499328613281,34.4061279296875,34.142528533935547]
[null,null,null,null,"Coincident",34.219184875488281,33.681564331054688,33.556617736816406,33.453395843505859,33.054695129394531,32.647857666015625,32.401546478271484]
[null,"Sunnybank","Substation Rating","MVA","Non-Coincident",41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094]
[null,null,null,null,"Coincident",41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094,41.599998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.884086608886719,32.638465881347656,32.639015197753906,32.489959716796875,32.069156646728516,31.751148223876953,31.547723770141602]
[null,null,null,null,"Coincident",30.260000228881836,30.033981323242187,30.034486770629883,29.897323608398437,29.510099411010742,29.21746826171875,29.030277252197266]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.397293090820313,33.132614135742187,33.133205413818359,32.972694396972656,32.520015716552734,32.178390502929688,31.960079193115234]
[null,null,null,null,"Coincident",30.610557556152344,30.375324249267578,30.375850677490234,30.233125686645508,29.830327987670898,29.526056289672852,29.331480026245117]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.741931915283203,31.547798156738281,31.460926055908203,31.348812103271484,30.927913665771484,30.542213439941406,30.336599349975586]
[null,null,null,null,"Coincident",29.208988189697266,29.030345916748047,28.950405120849609,28.847238540649414,28.459926605224609,28.105005264282227,27.915798187255859]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.168498992919922,31.960159301757812,31.866983413696289,31.746780395507812,31.296005249023438,30.883626937866211,30.66407585144043]
[null,null,null,null,"Coincident",29.525798797607422,29.339986801147461,29.256851196289063,29.149574279785156,28.746969223022461,28.378223419189453,28.181724548339844]
[null,"Surfers Paradise","Substation Rating","MVA","Non-Coincident",171,171,171,182,182,182,182]
[null,null,null,null,"Coincident",171,171,171,182,182,182,182]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",73.536323547363281,73.531700134277344,73.616264343261719,73.357658386230469,72.493118286132813,72.319679260253906,72.512184143066406]
[null,null,null,null,"Coincident",72.004966735839844,72.000442504882813,72.083244323730469,71.830024719238281,70.983482360839844,70.81365966796875,71.002151489257813]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",74.8316650390625,74.826713562011719,74.917366027832031,74.640151977539063,73.713935852050781,73.528228759765625,73.734352111816406]
[null,null,null,null,"Coincident",72.031387329101563,72.026824951171875,72.110328674316406,71.854972839355469,71.001884460449219,70.830863952636719,71.02069091796875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",70.718246459960938,70.810211181640625,70.695236206054687,70.517898559570313,69.6533203125,69.307395935058594,69.469108581542969]
[null,null,null,null,"Coincident",69.245574951171875,69.335624694824219,69.223045349121094,69.049400329589844,68.202827453613281,67.864105224609375,68.022453308105469]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",71.815208435058594,71.913497924804688,71.790618896484375,71.601119995117187,70.6778564453125,70.308723449707031,70.48126220703125]
[null,null,null,null,"Coincident",69.255256652832031,69.345794677734375,69.232612609863281,69.058059692382812,68.20770263671875,67.867759704589844,68.026657104492187]
[null,"Tamborine Village","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.5263290405273437,4.5177178382873535,4.5089554786682129,4.4820256233215332,4.4382047653198242,4.4254670143127441,4.4302153587341309]
[null,null,null,null,"Coincident",4.0270099639892578,4.0193490982055664,4.0115537643432617,3.9875948429107666,3.9486081600189209,3.9372756481170654,3.941500186920166]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.6063742637634277,4.5976109504699707,4.5886936187744141,4.5612874031066895,4.5166912078857422,4.5037283897399902,4.5085606575012207]
[null,null,null,null,"Coincident",4.0642995834350586,4.0565676689147949,4.0486998558044434,4.0245194435119629,3.9851715564727783,3.9737341403961182,3.9779977798461914]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8371312618255615,3.8350529670715332,3.8170104026794434,3.7980375289916992,3.7590959072113037,3.7386362552642822,3.7414219379425049]
[null,null,null,null,"Coincident",3.4138412475585937,3.4119923114776611,3.3959400653839111,3.3790600299835205,3.3444144725799561,3.3262114524841309,3.3286898136138916]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.9049882888793945,3.9028732776641846,3.8845117092132568,3.8652031421661377,3.8255729675292969,3.8047513961791992,3.8075864315032959]
[null,null,null,null,"Coincident",3.4454529285430908,3.4435868263244629,3.4273858070373535,3.4103496074676514,3.3753831386566162,3.3570115566253662,3.3595128059387207]
[null,"Tanah Merah","Substation Rating","MVA","Non-Coincident",35.5,35.5,35.5,35.5,35.5,35.5,35.5]
[null,null,null,null,"Coincident",35.5,35.5,35.5,35.5,35.5,35.5,35.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.78453254699707,17.666952133178711,17.685708999633789,17.655824661254883,17.576770782470703,17.619380950927734,17.711696624755859]
[null,null,null,null,"Coincident",17.171483993530273,17.057956695556641,17.076065063476562,17.047210693359375,16.970882415771484,17.01202392578125,17.101158142089844]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.549873352050781,18.42723274230957,18.446796417236328,18.415628433227539,18.333171844482422,18.377614974975586,18.473903656005859]
[null,null,null,null,"Coincident",17.374187469482422,17.259321212768555,17.277643203735352,17.248447418212891,17.171218872070312,17.212844848632812,17.303031921386719]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.91850471496582,15.834819793701172,15.807713508605957,15.796908378601074,15.71861743927002,15.716069221496582,15.793239593505859]
[null,null,null,null,"Coincident",15.369779586791992,15.288979530334473,15.26280689239502,15.252373695373535,15.176782608032227,15.174322128295898,15.248832702636719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.603544235229492,16.516256332397461,16.487983703613281,16.476715087890625,16.395053863525391,16.39239501953125,16.472888946533203]
[null,null,null,null,"Coincident",15.551215171813965,15.469461441040039,15.44297981262207,15.43242359161377,15.355939865112305,15.353450775146484,15.428840637207031]
[null,"Tarampa","Substation Rating","MVA","Non-Coincident",13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137]
[null,null,null,null,"Coincident",13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137,13.199999809265137]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.4873313903808594,8.5032949447631836,8.5213127136230469,8.5055093765258789,8.4366827011108398,8.4145593643188477,8.4214048385620117]
[null,null,null,null,"Coincident",7.3630352020263672,7.3768844604492187,7.392514705657959,7.3788042068481445,7.3190960884094238,7.2999029159545898,7.3058409690856934]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.2872381210327148,9.3047056198120117,9.3244218826293945,9.30712890625,9.2318153381347656,9.2076072692871094,9.2150974273681641]
[null,null,null,null,"Coincident",7.6108946800231934,7.6252102851867676,7.6413669586181641,7.627194881439209,7.5654764175415039,7.5456371307373047,7.5517754554748535]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.476020336151123,7.5002946853637695,7.4953627586364746,7.4890022277832031,7.424830436706543,7.386253833770752,7.3898410797119141]
[null,null,null,null,"Coincident",6.4856905937194824,6.5067481994628906,6.5024700164794922,6.4969520568847656,6.4412808418273926,6.4078145027160645,6.4109268188476562]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.1806135177612305,8.2071752548217773,8.2017784118652344,8.1948184967041016,8.124598503112793,8.0823869705200195,8.0863122940063477]
[null,null,null,null,"Coincident",6.7040166854858398,6.7257828712463379,6.7213606834411621,6.7156572341918945,6.6581120491027832,6.6235189437866211,6.6267361640930176]
[null,"Taringa","Substation Rating","MVA","Non-Coincident",34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906]
[null,null,null,null,"Coincident",34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906,34.900001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.679754257202148,13.69688892364502,13.717823028564453,13.688949584960937,13.599162101745605,13.619147300720215,13.703573226928711]
[null,null,null,null,"Coincident",12.939209938049316,12.955417633056641,12.975218772888184,12.947908401489258,12.862980842590332,12.88188362121582,12.961740493774414]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.523193359375,14.541384696960449,14.56360912322998,14.532955169677734,14.437631607055664,14.458849906921387,14.548480987548828]
[null,null,null,null,"Coincident",13.117584228515625,13.134016036987305,13.15408992767334,13.126402854919434,13.040305137634277,13.059468269348145,13.140425682067871]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.689772605895996,11.720373153686523,11.705764770507813,11.692899703979492,11.610621452331543,11.597681999206543,11.665756225585938]
[null,null,null,null,"Coincident",11.056954383850098,11.085898399353027,11.072080612182617,11.059911727905273,10.982087135314941,10.969849586486816,11.034237861633301]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.410517692565918,12.443004608154297,12.427495002746582,12.413836479187012,12.326486587524414,12.312747955322266,12.38502025604248]
[null,null,null,null,"Coincident",11.209381103515625,11.238723754882813,11.224716186523438,11.212379455566406,11.133481979370117,11.121075630187988,11.186351776123047]
[null,"Tennyson","Substation Rating","MVA","Non-Coincident",54.5,54.5,54.5,54.5,54.5,54.5,54.5]
[null,null,null,null,"Coincident",54.5,54.5,54.5,54.5,54.5,54.5,54.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.588468551635742,11.570588111877441,11.578901290893555,11.534372329711914,11.393190383911133,11.287674903869629,11.221776962280273]
[null,null,null,null,"Coincident",10.892825126647949,10.876017570495605,10.883831977844238,10.841976165771484,10.709268569946289,10.610087394714355,10.548145294189453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.602030754089355,11.58372974395752,11.59223747253418,11.546680450439453,11.402487754821777,11.294977188110352,11.227947235107422]
[null,null,null,null,"Coincident",11.149179458618164,11.132080078125,11.140082359313965,11.097245216369629,10.961418151855469,10.859910011291504,10.79652214050293]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.566009521484375,11.564002990722656,11.540255546569824,11.507465362548828,11.361152648925781,11.226899147033691,11.157713890075684]
[null,null,null,null,"Coincident",10.871713638305664,10.869828224182129,10.847505569458008,10.816683769226074,10.679154396057129,10.552960395812988,10.487927436828613]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.579044342041016,11.576991081237793,11.55269718170166,11.519169807434082,11.369820594787598,11.233154296875,11.162869453430176]
[null,null,null,null,"Coincident",11.129796981811523,11.127975463867188,11.105127334594727,11.073577880859375,10.932787895202637,10.803605079650879,10.737039566040039]
[null,"Tenthill","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5598406791687012,3.5647995471954346,3.5700557231903076,3.5596253871917725,3.5241768360137939,3.5054254531860352,3.4984462261199951]
[null,null,null,null,"Coincident",2.9313580989837646,2.9354414939880371,2.9397692680358887,2.931180477142334,2.9019904136657715,2.8865499496459961,2.8808028697967529]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6276309490203857,3.6329255104064941,3.6385383605957031,3.6274011135101318,3.5895638465881348,3.5695579051971436,3.5621132850646973]
[null,null,null,null,"Coincident",2.931358814239502,2.9354422092437744,2.939769983291626,2.9311811923980713,2.9019911289215088,2.8865506649017334,2.8808035850524902]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2265121936798096,3.2354118824005127,3.2312045097351074,3.2250115871429443,3.1913604736328125,3.1661896705627441,3.158851146697998]
[null,null,null,null,"Coincident",2.6578426361083984,2.6651737689971924,2.6617083549499512,2.656606912612915,2.6288866996765137,2.6081526279449463,2.6021072864532471]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2727842330932617,3.2822282314300537,3.2777633666992187,3.2711918354034424,3.2354998588562012,3.2088198661804199,3.2010443210601807]
[null,null,null,null,"Coincident",2.6578459739685059,2.6651771068572998,2.6617116928100586,2.6566102504730225,2.6288900375366211,2.6081557273864746,2.6021103858947754]
[null,"Tewantin","Substation Rating","MVA","Non-Coincident",58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453]
[null,null,null,null,"Coincident",58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.042469024658203,27.855325698852539,27.884332656860352,27.808521270751953,27.526361465454102,27.550638198852539,27.84760856628418]
[null,null,null,null,"Coincident",27.767257690429688,27.581949234008789,27.610673904418945,27.535604476928711,27.256214141845703,27.280252456665039,27.574310302734375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.445648193359375,28.249790191650391,28.280145645141602,28.200813293457031,27.905618667602539,27.931011199951172,28.241714477539063]
[null,null,null,null,"Coincident",27.769882202148438,27.584085464477539,27.612882614135742,27.537626266479492,27.257606506347656,27.281694412231445,27.576427459716797]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.909894943237305,24.777389526367188,24.734476089477539,24.692089080810547,24.429800033569336,24.38825798034668,24.643070220947266]
[null,null,null,null,"Coincident",24.665424346923828,24.534221649169922,24.491727828979492,24.449756622314453,24.190042495727539,24.148908615112305,24.401218414306641]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.173858642578125,25.035816192626953,24.991115570068359,24.946968078613281,24.673858642578125,24.630615234375,24.895915985107422]
[null,null,null,null,"Coincident",25.194469451904297,25.060453414916992,25.017047882080078,24.974176406860352,24.708890914916992,24.666875839233398,24.924596786499023]
[null,"The Gap","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",36,36,36,36,36,36,36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.512775421142578,18.337190628051758,18.333887100219727,18.246492385864258,18.006477355957031,17.824197769165039,17.911003112792969]
[null,null,null,null,"Coincident",17.360864639282227,17.196205139160156,17.193107604980469,17.111150741577148,16.886070251464844,16.715131759643555,16.796535491943359]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.220174789428711,19.037879943847656,19.034452438354492,18.943716049194336,18.694528579711914,18.505285263061523,18.595407485961914]
[null,null,null,null,"Coincident",17.519250869750977,17.35308837890625,17.349964141845703,17.26725959777832,17.040124893188477,16.867626190185547,16.949773788452148]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.677509307861328,16.541851043701172,16.493051528930664,16.430974960327148,16.207046508789063,16.001588821411133,16.074251174926758]
[null,null,null,null,"Coincident",15.639792442321777,15.512576103210449,15.466813087463379,15.408598899841309,15.198604583740234,15.005929946899414,15.074070930480957]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.314779281616211,17.173938751220703,17.123273849487305,17.058826446533203,16.82634162902832,16.613033294677734,16.688470840454102]
[null,null,null,null,"Coincident",15.782477378845215,15.65410041809082,15.607919692993164,15.549174308776855,15.337264060974121,15.142831802368164,15.211594581604004]
[null,"Tin Can Bay","Substation Rating","MVA","Non-Coincident",15,17.399999618530273,17.399999618530273,17.399999618530273,17.399999618530273,17.399999618530273,17.399999618530273]
[null,null,null,null,"Coincident",15,17.399999618530273,17.399999618530273,17.399999618530273,17.399999618530273,17.399999618530273,17.399999618530273]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.963798999786377,7.9623503684997559,7.9629826545715332,7.9390463829040527,7.8710713386535645,7.8607468605041504,7.903968334197998]
[null,null,null,null,"Coincident",6.5905289649963379,6.5893301963806152,6.5898537635803223,6.5700445175170898,6.5137906074523926,6.505246639251709,6.5410146713256836]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.0342311859130859,8.0327491760253906,8.0333957672119141,8.0088911056518555,7.9393062591552734,7.9287376403808594,7.9729809761047363]
[null,null,null,null,"Coincident",6.6097989082336426,6.608583927154541,6.6091146469116211,6.5890417098999023,6.5320448875427246,6.5233888626098633,6.5596275329589844]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6874146461486816,7.6964950561523438,7.67578125,7.6604208946228027,7.5911808013916016,7.5616626739501953,7.6007499694824219]
[null,null,null,null,"Coincident",6.3618040084838867,6.3693184852600098,6.3521771430969238,6.3394651412963867,6.2821645736694336,6.2577366828918457,6.2900838851928711]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.751338005065918,7.7606301307678223,7.7394332885742187,7.7237153053283691,7.6528677940368652,7.6226673126220703,7.66265869140625]
[null,null,null,null,"Coincident",6.3780980110168457,6.3857078552246094,6.3683490753173828,6.3554768562316895,6.297459602355957,6.2727293968200684,6.3054776191711426]
[null,"Tingalpa","Substation Rating","MVA","Non-Coincident",55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906]
[null,null,null,null,"Coincident",55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906,55.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.745046615600586,24.729080200195313,24.714218139648438,24.613069534301758,24.354694366455078,24.250558853149414,24.312427520751953]
[null,null,null,null,"Coincident",22.724641799926758,22.709980010986328,22.696331024169922,22.603439331054688,22.366161346435547,22.270528793334961,22.32734489440918]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.816041946411133,25.799385070800781,25.783880233764648,25.678354263305664,25.408794403076172,25.300151824951172,25.36469841003418]
[null,null,null,null,"Coincident",23.343351364135742,23.328290939331055,23.31427001953125,23.218849182128906,22.97511100769043,22.876874923706055,22.935237884521484]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.729345321655273,22.745645523071289,22.668994903564453,22.598970413208008,22.350994110107422,22.198003768920898,22.247344970703125]
[null,null,null,null,"Coincident",20.87352180480957,20.888492584228516,20.81810188293457,20.753793716430664,20.52606201171875,20.385564804077148,20.430879592895508]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.713098526000977,23.730104446411133,23.650136947631836,23.577081680297852,23.31837272644043,23.158760070800781,23.210235595703125]
[null,null,null,null,"Coincident",21.441831588745117,21.457210540771484,21.384902954101563,21.318843841552734,21.084911346435547,20.940589904785156,20.987138748168945]
[null,"Toogoolawah","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9926447868347168,4.9336175918579102,4.9315962791442871,4.9069385528564453,4.9318203926086426,5.0035014152526855,5.0212845802307129]
[null,null,null,null,"Coincident",4.9926447868347168,4.9336175918579102,4.9315962791442871,4.9069385528564453,4.9318203926086426,5.0035014152526855,5.0212845802307129]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.0023050308227539,4.9418940544128418,4.9398269653320313,4.9146199226379395,4.940056324005127,5.0134258270263672,5.0316481590270996]
[null,null,null,null,"Coincident",4.994408130645752,4.9348430633544922,4.932805061340332,4.9079513549804687,4.9330310821533203,5.005373477935791,5.023341178894043]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.425565242767334,4.3792047500610352,4.3652830123901367,4.347834587097168,4.3677806854248047,4.4198307991027832,4.434086799621582]
[null,null,null,null,"Coincident",4.425565242767334,4.3792047500610352,4.3652830123901367,4.347834587097168,4.3677806854248047,4.4198307991027832,4.434086799621582]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4261527061462402,4.3795208930969238,4.3655333518981934,4.3480134010314941,4.3680424690246582,4.4203805923461914,4.4347329139709473]
[null,null,null,null,"Coincident",4.4707927703857422,4.4223818778991699,4.4078497886657715,4.3896403312683105,4.4104571342468262,4.4648032188415527,4.4796938896179199]
[null,"Toorbul Point","Substation Rating","MVA","Non-Coincident",17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727]
[null,null,null,null,"Coincident",17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727,17.600000381469727]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.8762407302856445,6.8204474449157715,6.9207534790039062,7.0015325546264648,7.0212907791137695,7.1514506340026855,7.2887258529663086]
[null,null,null,null,"Coincident",5.9691767692565918,5.920743465423584,6.0078177452087402,6.0779409408569336,6.0950927734375,6.2080831527709961,6.3272500038146973]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2047877311706543,7.1463289260864258,7.251427173614502,7.3360657691955566,7.3567681312561035,7.4931468963623047,7.6369814872741699]
[null,null,null,null,"Coincident",6.0066103935241699,5.9578733444213867,6.0454940795898438,6.1160569190979004,6.1333160400390625,6.2470149993896484,6.3669295310974121]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3365521430969238,6.2937064170837402,6.3685731887817383,6.4494004249572754,6.4644918441772461,6.5673418045043945,6.6912126541137695]
[null,null,null,null,"Coincident",5.5006799697875977,5.4634861946105957,5.5284771919250488,5.5986423492431641,5.6117429733276367,5.7010254859924316,5.808556079864502]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.639312744140625,6.5944199562072754,6.6728634834289551,6.7575531005859375,6.7733654975891113,6.8811297416687012,7.0109190940856934]
[null,null,null,null,"Coincident",5.5351758003234863,5.497748851776123,5.5631470680236816,5.6337523460388184,5.6469354629516602,5.7367777824401855,5.8449826240539551]
[null,"Toowong","Substation Rating","MVA","Non-Coincident",43.900001525878906,55,55,55,55,55,55]
[null,null,null,null,"Coincident",43.900001525878906,55,55,55,55,55,55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.457511901855469,32.217617034912109,32.236644744873047,32.136955261230469,31.745223999023438,31.416561126708984,31.226112365722656]
[null,null,null,null,"Coincident",31.566701889038086,31.333389282226563,31.351896286010742,31.25494384765625,30.87396240234375,30.554319381713867,30.369098663330078]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.878467559814453,32.622821807861328,32.643093109130859,32.536907196044922,32.119987487792969,31.770606994628906,31.568330764770508]
[null,null,null,null,"Coincident",31.702287673950195,31.464311599731445,31.483186721801758,31.384307861328125,30.995849609375,30.670042037963867,30.481296539306641]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.264364242553711,29.087673187255859,29.024219512939453,28.963626861572266,28.596820831298828,28.22773551940918,28.047428131103516]
[null,null,null,null,"Coincident",28.461191177368164,28.289348602294922,28.227636337280273,28.168706893920898,27.811967849731445,27.453012466430664,27.277654647827148]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.493085861206055,29.306980133056641,29.240180969238281,29.176410675048828,28.790740966796875,28.403339385986328,28.214334487915039]
[null,null,null,null,"Coincident",28.539260864257813,28.364555358886719,28.301824569702148,28.241926193237305,27.879421234130859,27.514839172363281,27.336795806884766]
[null,"Upper Mt Gravatt","Substation Rating","MVA","Non-Coincident",82,82,82,82,82,82,82]
[null,null,null,null,"Coincident",82,82,82,82,82,82,82]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.894027709960937,31.681848526000977,31.684902191162109,31.542764663696289,31.136804580688477,30.830642700195313,30.635746002197266]
[null,null,null,null,"Coincident",31.412393569946289,31.203418731689453,31.206426620483398,31.066434860229492,30.666604995727539,30.365066528320313,30.173112869262695]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.041191101074219,31.821233749389648,31.824398040771484,31.677139282226563,31.256967544555664,30.940502166748047,30.739238739013672]
[null,null,null,null,"Coincident",31.624002456665039,31.409490585327148,31.412578582763672,31.268899917602539,30.858646392822266,30.549350738525391,30.352506637573242]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.707094192504883,29.54969596862793,29.470670700073242,29.368034362792969,28.976127624511719,28.617183685302734,28.426967620849609]
[null,null,null,null,"Coincident",29.258485794067383,29.103464126586914,29.025630950927734,28.924545288085938,28.538557052612305,28.185033798217773,27.997690200805664]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.782394409179687,29.620586395263672,29.539388656616211,29.43397331237793,29.031900405883789,28.664287567138672,28.469736099243164]
[null,null,null,null,"Coincident",29.415121078491211,29.256336212158203,29.17662239074707,29.07310676574707,28.677949905395508,28.316190719604492,28.124547958374023]
[null,"Varsity Lakes","Substation Rating","MVA","Non-Coincident",64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094]
[null,null,null,null,"Coincident",64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094,64.099998474121094]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.878978729248047,35.771533966064453,35.817916870117187,35.726673126220703,35.366722106933594,35.146568298339844,35.149463653564453]
[null,null,null,null,"Coincident",35.437896728515625,35.331771850585938,35.377582550048828,35.287464141845703,34.931934356689453,34.714488983154297,34.71734619140625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.150444030761719,36.040210723876953,36.087799072265625,35.994190216064453,35.624965667724609,35.399177551269531,35.402145385742188]
[null,null,null,null,"Coincident",35.485034942626953,35.377937316894531,35.424167633056641,35.333229064941406,34.974510192871094,34.755157470703125,34.758041381835938]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.709571838378906,32.656082153320313,32.607833862304688,32.557552337646484,32.214035034179688,31.930906295776367,31.923076629638672]
[null,null,null,null,"Coincident",32.307453155517578,32.254619598388672,32.206966400146484,32.157302856445313,31.818008422851563,31.538362503051758,31.530630111694336]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.902114868164062,32.847358703613281,32.797969818115234,32.746498107910156,32.394924163818359,32.105232238769531,32.097225189208984]
[null,null,null,null,"Coincident",32.329357147216797,32.276165008544922,32.228187561035156,32.178192138671875,31.836675643920898,31.555274963378906,31.547494888305664]
[null,"Victoria Park","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.028247833251953,46.225872039794922,48.533817291259766,49.124710083007813,49.292533874511719,49.601909637451172,50.079269409179687]
[null,null,null,null,"Coincident",38.432479858398438,38.597492218017578,40.524570465087891,41.017951965332031,41.1580810546875,41.416400909423828,41.814987182617188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.028736114501953,46.226810455322266,48.549983978271484,49.147548675537109,49.317462921142578,49.630905151367188,50.115093231201172]
[null,null,null,null,"Coincident",38.470409393310547,38.636562347412109,40.600418090820313,41.098018646240234,41.238822937011719,41.499038696289063,41.900993347167969]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.024272918701172,45.278736114501953,47.561775207519531,48.184425354003906,48.321006774902344,48.494171142578125,48.940273284912109]
[null,null,null,null,"Coincident",37.594184875488281,37.806655883789062,39.712940216064453,40.232837677001953,40.346878051757813,40.491466522216797,40.86395263671875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.093379974365234,45.3533935546875,47.569355010986328,48.197154998779297,48.335033416748047,48.509929656982422,48.960914611816406]
[null,null,null,null,"Coincident",37.627368927001953,37.841266632080078,39.784015655517578,40.308338165283203,40.422760009765625,40.568058013916016,40.943584442138672]
[null,"Victoria Point","Substation Rating","MVA","Non-Coincident",59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906]
[null,null,null,null,"Coincident",59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906,59.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.182321548461914,25.241216659545898,25.393581390380859,25.475543975830078,25.450529098510742,25.531269073486328,25.654571533203125]
[null,null,null,null,"Coincident",23.290306091308594,23.344776153564453,23.485692977905273,23.561498641967773,23.538364410400391,23.613035202026367,23.727071762084961]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.248350143432617,25.308317184448242,25.463478088378906,25.546962738037109,25.521482467651367,25.603731155395508,25.72935676574707]
[null,null,null,null,"Coincident",23.527639389038086,23.582664489746094,23.725017547607422,23.801595687866211,23.778224945068359,23.853656768798828,23.968854904174805]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.329887390136719,23.416332244873047,23.492414474487305,23.591999053955078,23.557504653930664,23.571264266967773,23.677341461181641]
[null,null,null,null,"Coincident",21.577049255371094,21.656999588012695,21.727365493774414,21.819463729858398,21.787559509277344,21.800285339355469,21.898393630981445]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.36570930480957,23.453403472900391,23.530597686767578,23.631658554077148,23.596651077270508,23.610614776611328,23.718284606933594]
[null,null,null,null,"Coincident",21.796924591064453,21.877689361572266,21.948772430419922,22.04180908203125,22.009578704833984,22.022434234619141,22.121543884277344]
[null,"Wacol","Substation Rating","MVA","Non-Coincident",75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906]
[null,null,null,null,"Coincident",75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906,75.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.304265975952148,24.260190963745117,24.274236679077148,24.177427291870117,23.878210067749023,23.655078887939453,23.517337799072266]
[null,null,null,null,"Coincident",20.062005996704102,20.025623321533203,20.03721809387207,19.957305908203125,19.710317611694336,19.526132583618164,19.412433624267578]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.744651794433594,24.69610595703125,24.711574554443359,24.604990005493164,24.276027679443359,24.03118896484375,23.880254745483398]
[null,null,null,null,"Coincident",20.076217651367188,20.039485931396484,20.05120849609375,19.970451354980469,19.720993041992188,19.535116195678711,19.420440673828125]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.1048583984375,24.094198226928711,24.0413818359375,23.969655990600586,23.661651611328125,23.380092620849609,23.236364364624023]
[null,null,null,null,"Coincident",19.897403717041016,19.888605117797852,19.845006942749023,19.785800933837891,19.531558990478516,19.299144744873047,19.180503845214844]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.525142669677734,24.513416290283203,24.455331802368164,24.376487731933594,24.038394927978516,23.730026245117188,23.572877883911133]
[null,null,null,null,"Coincident",19.910772323608398,19.901924133300781,19.857870101928711,19.798057556152344,19.541343688964844,19.306888580322266,19.187292098999023]
[null,"Wacol South","Substation Rating","MVA","Non-Coincident",52.5,52.5,52.5,52.5,52.5,52.5,52.5]
[null,null,null,null,"Coincident",52.5,52.5,52.5,52.5,52.5,52.5,52.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.381553649902344,22.206573486328125,22.206291198730469,22.104120254516602,21.817127227783203,21.600107192993164,21.460847854614258]
[null,null,null,null,"Coincident",20.961454391479492,20.797576904296875,20.797311782836914,20.701623916625977,20.432840347290039,20.229589462280273,20.099166870117188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.914340972900391,22.72618293762207,22.725879669189453,22.616046905517578,22.307680130004883,22.074640274047852,21.925167083740234]
[null,null,null,null,"Coincident",21.388103485107422,21.220890045166016,21.220619201660156,21.122983932495117,20.848730087280273,20.641342163085938,20.508264541625977]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.016141891479492,21.873800277709961,21.812919616699219,21.734445571899414,21.441936492919922,21.17387580871582,21.030477523803711]
[null,null,null,null,"Coincident",20.619226455688477,20.485918045043945,20.428899765014648,20.355403900146484,20.081455230712891,19.830402374267578,19.696102142333984]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.521493911743164,22.368556976318359,22.303159713745117,22.218879699707031,21.904874801635742,21.617321014404297,21.463579177856445]
[null,null,null,null,"Coincident",21.038909912109375,20.902889251708984,20.844709396362305,20.769718170166016,20.490192413330078,20.234029769897461,20.096996307373047]
[null,"Wamuran","Substation Rating","MVA","Non-Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,null,null,"Coincident",9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266,9.6000003814697266]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.3806614875793457,4.3656406402587891,4.3882002830505371,4.3707361221313477,4.3264503479003906,4.3079705238342285,4.3011894226074219]
[null,null,null,null,"Coincident",3.8095262050628662,3.7964637279510498,3.816082239151001,3.8008949756622314,3.7623832225799561,3.7463123798370361,3.7404155731201172]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.4746112823486328,4.4592680931091309,4.4823117256164551,4.464472770690918,4.4192376136779785,4.4003615379333496,4.3934345245361328]
[null,null,null,null,"Coincident",3.8886787891387939,3.8753447532653809,3.8953709602355957,3.8798680305480957,3.8405561447143555,3.8241515159606934,3.8181321620941162]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.9720587730407715,3.9638359546661377,3.9732809066772461,3.9614565372467041,3.9194326400756836,3.8926215171813965,3.8852217197418213]
[null,null,null,null,"Coincident",3.4541957378387451,3.4470450878143311,3.4552586078643799,3.4449758529663086,3.408430814743042,3.385115385055542,3.3786802291870117]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.0572452545166016,4.0488462448120117,4.0584936141967773,4.0464158058166504,4.0034904479980469,3.9761042594909668,3.9685459136962891]
[null,null,null,null,"Coincident",3.5259654521942139,3.5186660289764404,3.527050256729126,3.5165538787841797,3.4792494773864746,3.4554495811462402,3.4488809108734131]
[null,"Wellington Rd","Substation Rating","MVA","Non-Coincident",125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781]
[null,null,null,null,"Coincident",125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781,125.80000305175781]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.135444641113281,57.062301635742188,57.100971221923828,56.885581970214844,57.874107360839844,59.003135681152344,58.667560577392578]
[null,null,null,null,"Coincident",49.639877319335938,49.576328277587891,49.60992431640625,49.422794342041016,50.281635284423828,51.262546539306641,50.970993041992188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.257270812988281,57.182174682617188,57.221874237060547,57.00079345703125,58.016384124755859,59.179172515869141,58.833255767822266]
[null,null,null,null,"Coincident",49.683345794677734,49.619167327880859,49.653095245361328,49.464122772216797,50.356266021728516,51.380680084228516,51.084339141845703]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",53.429882049560547,53.434230804443359,53.322299957275391,53.174701690673828,54.268482208251953,55.372303009033203,55.039402008056641]
[null,null,null,null,"Coincident",46.420444488525391,46.424221038818359,46.326976776123047,46.198741912841797,47.149028778076172,48.108039855957031,47.818813323974609]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",53.470745086669922,53.475166320800781,53.361400604248047,53.211437225341797,54.324295043945313,55.450901031494141,55.110767364501953]
[null,null,null,null,"Coincident",46.437076568603516,46.440876007080078,46.342998504638672,46.213939666748047,47.189456939697266,48.184352874755859,47.891067504882813]
[null,"West End","Substation Rating","MVA","Non-Coincident",126,126,126,126,126,126,126]
[null,null,null,null,"Coincident",126,126,126,126,126,126,126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",71.165435791015625,71.53350830078125,71.687309265136719,71.53082275390625,70.760368347167969,70.193336486816406,69.902938842773438]
[null,null,null,null,"Coincident",64.735664367675781,65.070480346679688,65.21038818359375,65.068038940429688,64.367195129394531,63.851394653320313,63.587238311767578]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",72.387092590332031,72.782005310058594,72.947074890136719,72.779121398925781,71.952682495117188,71.344924926757813,71.033821105957031]
[null,null,null,null,"Coincident",64.835121154785156,65.17803955078125,65.320167541503906,65.175506591796875,64.463699340820313,63.940139770507813,63.672100067138672]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",67.319671630859375,67.796546936035156,67.7537841796875,67.673652648925781,66.912261962890625,66.204566955566406,65.908775329589844]
[null,null,null,null,"Coincident",61.237361907958984,61.671157836914063,61.632255554199219,61.559364318847656,60.866764068603516,60.223011016845703,59.953941345214844]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",68.271415710449219,68.780654907226562,68.734977722167969,68.649391174316406,67.836616516113281,67.081939697265625,66.766738891601563]
[null,null,null,null,"Coincident",61.290374755859375,61.731761932373047,61.692352294921875,61.618522644042969,60.917526245117188,60.266471862792969,59.994487762451172]
[null,"West Maroochydore","Substation Rating","MVA","Non-Coincident",85.5,85.5,85.5,85.5,85.5,85.5,85.5]
[null,null,null,null,"Coincident",85.5,85.5,85.5,85.5,85.5,85.5,85.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.159278869628906,33.191062927246094,33.232948303222656,33.181663513183594,32.901264190673828,32.782371520996094,32.857967376708984]
[null,null,null,null,"Coincident",32.627059936523437,32.658332824707031,32.699542999267578,32.649085998535156,32.373180389404297,32.256195068359375,32.330577850341797]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.403205871582031,33.435848236083984,33.478866577148438,33.426193237304687,33.138248443603516,33.016178131103516,33.093791961669922]
[null,null,null,null,"Coincident",32.648696899414063,32.68017578125,32.721664428710937,32.670867919921875,32.393146514892578,32.275409698486328,32.350269317626953]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.896282196044922,30.968061447143555,30.921232223510742,30.904636383056641,30.628742218017578,30.439321517944336,30.499526977539063]
[null,null,null,null,"Coincident",30.400381088256836,30.471010208129883,30.424932479858398,30.408601760864258,30.137136459350586,29.950754165649414,30.009992599487305]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.081258773803711,31.154836654663086,31.106834411621094,31.089820861816406,30.807058334350586,30.612964630126953,30.674652099609375]
[null,null,null,null,"Coincident",30.409355163574219,30.480312347412109,30.43402099609375,30.417613983154297,30.144933700561523,29.957761764526367,30.017248153686523]
[null,"Whinstanes","Substation Rating","MVA","Non-Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,null,null,"Coincident",52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906,52.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.2614822387695313,9.2700662612915039,13.934109687805176,13.881952285766602,13.713705062866211,13.589370727539063,13.514100074768066]
[null,null,null,null,"Coincident",7.3425998687744141,7.3494052886962891,11.047107696533203,11.005756378173828,10.872368812561035,10.773795127868652,10.714119911193848]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9423704147338867,9.9515857696533203,13.934167861938477,13.881966590881348,14.721912384033203,14.588437080383301,14.507633209228516]
[null,null,null,null,"Coincident",7.8221225738525391,7.8293724060058594,11.799144744873047,11.754979133605957,11.612510681152344,11.507226943969727,11.443489074707031]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.9994363784790039,9.0200586318969727,13.891246795654297,13.853198051452637,13.67872142791748,13.519731521606445,13.440443992614746]
[null,null,null,null,"Coincident",7.1348471641540527,7.1511964797973633,11.013125419616699,10.982959747314453,10.844633102416992,10.718584060668945,10.65572452545166]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.6610593795776367,9.6831979751586914,13.891266822814941,13.853200912475586,14.684356689453125,14.513678550720215,14.428561210632324]
[null,null,null,null,"Coincident",7.600801944732666,7.6182188987731934,11.764486312866211,11.73226261138916,11.584498405456543,11.449850082397461,11.382701873779297]
[null,"Whiteside","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.487354278564453,10.434517860412598,10.443178176879883,10.409244537353516,10.294235229492187,10.217485427856445,10.179704666137695]
[null,null,null,null,"Coincident",10.210209846496582,10.158769607543945,10.167200088500977,10.134162902832031,10.02219295501709,9.9474716186523437,9.9106893539428711]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.283219337463379,11.226372718811035,11.235690116882324,11.19918155670166,11.075444221496582,10.992870330810547,10.952221870422363]
[null,null,null,null,"Coincident",10.786154747009277,10.731812477111816,10.740718841552734,10.705818176269531,10.587532043457031,10.50859546661377,10.469738960266113]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3905782699584961,9.3560066223144531,9.3378286361694336,9.3168668746948242,9.209498405456543,9.1172523498535156,9.0805644989013672]
[null,null,null,null,"Coincident",9.1424179077148438,9.1087589263916016,9.0910625457763672,9.0706539154052734,8.9661226272583008,8.8763132095336914,8.8405961990356445]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.10321044921875,10.066015243530273,10.04645824432373,10.023905754089355,9.9083890914916992,9.80914306640625,9.7696704864501953]
[null,null,null,null,"Coincident",9.6581296920776367,9.6225719451904297,9.6038780212402344,9.5823183059692383,9.4718904495239258,9.3770151138305664,9.3392829895019531]
[null,"Wivenhoe","Substation Rating","MVA","Non-Coincident",11.5,11.5,11.5,11.5,11.5,11.5,11.5]
[null,null,null,null,"Coincident",11.5,11.5,11.5,11.5,11.5,11.5,11.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.3483257293701172,7.3685927391052246,7.4341840744018555,7.4941396713256836,7.4973559379577637,7.508392333984375,7.5466256141662598]
[null,null,null,null,"Coincident",7.1060185432434082,7.1256170272827148,7.1890454292297363,7.2470235824584961,7.2501335144042969,7.2608060836791992,7.2977786064147949]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.8332829475402832,7.8548874855041504,7.9248075485229492,7.9887204170227051,7.9921488761901855,8.0039129257202148,8.0446701049804687]
[null,null,null,null,"Coincident",7.2642698287963867,7.2843050956726074,7.3491458892822266,7.4084153175354004,7.4115943908691406,7.4225049018859863,7.4603009223937988]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3459711074829102,6.3721489906311035,6.4110593795776367,6.4692778587341309,6.4689431190490723,6.4617500305175781,6.4925270080566406]
[null,null,null,null,"Coincident",6.1367154121398926,6.1620302200317383,6.1996574401855469,6.2559561729431152,6.2556324005126953,6.2486767768859863,6.2784390449523926]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.764777660369873,6.7926831245422363,6.8341612815856934,6.8962221145629883,6.8958649635314941,6.8881974220275879,6.9210052490234375]
[null,null,null,null,"Coincident",6.2733802795410156,6.2992591857910156,6.3377242088317871,6.3952765464782715,6.3949456214904785,6.3878350257873535,6.4182600975036621]
[null,"Woodford","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",18,18,18,18,18,18,18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.830211639404297,10.767941474914551,10.776243209838867,10.746360778808594,10.679637908935547,10.654683113098145,10.630767822265625]
[null,null,null,null,"Coincident",10.325251579284668,10.265885353088379,10.273798942565918,10.245309829711914,10.181697845458984,10.157906532287598,10.135107040405273]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.904783248901367,10.840282440185547,10.848880767822266,10.817934036254883,10.748854637145996,10.723024368286133,10.698274612426758]
[null,null,null,null,"Coincident",10.357508659362793,10.297956466674805,10.30589485168457,10.277317047119141,10.213506698608398,10.189640998840332,10.166769981384277]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.7777681350708008,9.7348031997680664,9.7153167724609375,9.6981410980224609,9.6332941055297852,9.5859870910644531,9.5613384246826172]
[null,null,null,null,"Coincident",9.3218774795532227,9.2809162139892578,9.2623386383056641,9.2459630966186523,9.1841402053833008,9.1390390396118164,9.11553955078125]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.8179197311401367,9.7737131118774414,9.7536687850952148,9.7360038757324219,9.6693296432495117,9.6207113265991211,9.5953865051269531]
[null,null,null,null,"Coincident",9.3509998321533203,9.309910774230957,9.2912750244140625,9.2748479843139648,9.2128324508666992,9.1675901412963867,9.144017219543457]
[null,"Woodridge","Substation Rating","MVA","Non-Coincident",85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906]
[null,null,null,null,"Coincident",85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906,85.400001525878906]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.690742492675781,37.354560852050781,37.349899291992187,37.173957824707031,36.687084197998047,36.317829132080078,36.079627990722656]
[null,null,null,null,"Coincident",35.720821380615234,35.402210235595703,35.397792816162109,35.231044769287109,34.769618988037109,34.419662475585938,34.193912506103516]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.698581695556641,37.359661102294922,37.354965209960938,37.177822113037109,36.688453674316406,36.318141937255859,36.079654693603516]
[null,null,null,null,"Coincident",35.731349945068359,35.411506652832031,35.407073974609375,35.239707946777344,34.77667236328125,34.425594329833984,34.199165344238281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.627227783203125,34.365154266357422,34.265670776367188,34.138626098632813,33.675312042236328,33.250358581542969,33.021461486816406]
[null,null,null,null,"Coincident",32.817420959472656,32.569046020507812,32.474761962890625,32.354358673095703,31.915258407592773,31.512516021728516,31.29557991027832]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.956893920898437,34.681221008300781,34.576622009277344,34.443092346191406,33.956508636474609,33.510776519775391,33.270919799804688]
[null,null,null,null,"Coincident",32.819374084472656,32.570564270019531,32.476127624511719,32.355541229248047,31.915882110595703,31.512779235839844,31.295711517333984]
[null,"Wynnum","Substation Rating","MVA","Non-Coincident",58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453]
[null,null,null,null,"Coincident",58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453,58.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.113906860351563,22.055168151855469,22.082212448120117,22.043577194213867,21.872173309326172,21.830667495727539,21.898336410522461]
[null,null,null,null,"Coincident",19.940374374389648,19.887409210205078,19.911796569824219,19.876956939697266,19.72239875793457,19.684970855712891,19.745988845825195]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.377079010009766,22.315452575683594,22.34382438659668,22.303293228149414,22.123519897460938,22.079998016357422,22.150955200195313]
[null,null,null,null,"Coincident",20.447206497192383,20.39289665222168,20.417903900146484,20.382177352905273,20.223691940307617,20.185312271118164,20.247880935668945]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.46281623840332,20.436288833618164,20.404661178588867,20.389488220214844,20.221218109130859,20.130769729614258,20.186557769775391]
[null,null,null,null,"Coincident",18.451570510864258,18.427646636962891,18.399127960205078,18.385446548461914,18.23371696472168,18.152158737182617,18.202463150024414]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.648530960083008,20.620826721191406,20.587799072265625,20.571956634521484,20.396306991577148,20.301931381225586,20.360137939453125]
[null,null,null,null,"Coincident",18.920560836791992,18.896030426025391,18.866786956787109,18.852756500244141,18.697170257568359,18.61353874206543,18.665122985839844]
[null,"Yamanto","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.232028007507324,13.416187286376953,13.597236633300781,15.848036766052246,17.9295654296875,17.932140350341797,17.99683952331543]
[null,null,null,null,"Coincident",11.454898834228516,12.563826560974121,12.733372688293457,14.841175079345703,16.790458679199219,16.792869567871094,16.853458404541016]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.602726936340332,13.822772979736328,14.009308815002441,16.32832145690918,18.472930908203125,18.475584030151367,18.542243957519531]
[null,null,null,null,"Coincident",11.703305244445801,12.842838287353516,13.01606559753418,15.349091529846191,17.542547225952148,17.540895462036133,17.600088119506836]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.611471176147461,11.858658790588379,11.982813835144043,14.337908744812012,16.514993667602539,16.465793609619141,16.510986328125]
[null,null,null,null,"Coincident",9.9372997283935547,11.105251312255859,11.221518516540527,13.42698860168457,15.465758323669434,15.419684410095215,15.462004661560059]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.93305778503418,12.218042373657227,12.34596061706543,14.772427558898926,17.015491485595703,16.964797973632812,17.011360168457031]
[null,null,null,null,"Coincident",10.152796745300293,11.352986335754395,11.471760749816895,13.91713809967041,16.218339920043945,16.165748596191406,16.20591926574707]
[null,"Yandina","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7854008674621582,8.146540641784668,8.1348543167114258,8.0880756378173828,7.985161304473877,7.9310922622680664,7.9275588989257813]
[null,null,null,null,"Coincident",6.7378573417663574,7.060917854309082,7.0508518218994141,7.0103616714477539,6.9211764335632324,6.8742499351501465,6.8710498809814453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.8012876510620117,8.1830739974975586,8.1713352203369141,8.1243476867675781,8.0209712982177734,7.9666595458984375,7.9631104469299316]
[null,null,null,null,"Coincident",6.8202800750732422,7.1528229713439941,7.1426382064819336,7.1016325950622559,7.0112895965576172,6.9637393951416016,6.9604697227478027]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5614547729492188,7.8577213287353516,7.8247838020324707,7.7876944541931152,7.6849255561828613,7.6131234169006348,7.6070785522460938]
[null,null,null,null,"Coincident",6.4633550643920898,6.813023567199707,6.7845306396484375,6.7524299621582031,6.6633400917053223,6.6010174751281738,6.5956330299377441]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.5768842697143555,7.8929595947265625,7.8598747253417969,7.8226189613342285,7.7193889617919922,7.6472644805908203,7.6411929130554199]
[null,null,null,null,"Coincident",6.5424199104309082,6.9021964073181152,6.8733434677124023,6.8408346176147461,6.7505817413330078,6.6874299049377441,6.68194580078125]
[null,"Yatala","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.006626129150391,55.603767395019531,55.602420806884766,55.346179962158203,54.627017974853516,54.082969665527344,53.734092712402344]
[null,null,null,null,"Coincident",48.5667724609375,50.946376800537109,50.945144653320313,50.710365295410156,50.051441192626953,49.552963256835938,49.233306884765625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.934257507324219,57.761741638183594,57.760272979736328,57.481128692626953,56.697887420654297,56.105567932128906,55.725826263427734]
[null,null,null,null,"Coincident",48.593086242675781,51.019241333007813,51.018016815185547,50.780387878417969,50.113666534423828,49.609539031982422,49.286380767822266]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.460094451904297,53.307514190673828,53.158802032470703,52.967414855957031,52.254291534423828,51.600662231445312,51.251277923583984]
[null,null,null,null,"Coincident",46.233539581298828,48.842460632324219,48.706203460693359,48.530845642089844,47.877456665039062,47.278575897216797,46.958454132080078]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.166152954101563,55.261619567871094,55.099815368652344,54.8916015625,54.115993499755859,53.4053955078125,53.025684356689453]
[null,null,null,null,"Coincident",46.244663238525391,48.893169403076172,48.755477905273438,48.578296661376953,47.918304443359375,47.313739776611328,46.990737915039062]
[null,"Zillmere","Substation Rating","MVA","Non-Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,null,null,"Coincident",54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547,54.799999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.487892150878906,36.088970184326172,36.077346801757813,35.900169372558594,35.422698974609375,35.136608123779297,35.709625244140625]
[null,null,null,null,"Coincident",35.029277801513672,34.646305084228516,34.635143280029297,34.465049743652344,34.006668090820313,33.732013702392578,34.282123565673828]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.488590240478516,36.089000701904297,36.077369689941406,36.298286437988281,35.794586181640625,35.493057250976562,36.097206115722656]
[null,null,null,null,"Coincident",35.271026611328125,34.878559112548828,34.867122650146484,34.692844390869141,34.223293304443359,33.9420166015625,34.505443572998047]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.397834777832031,33.077739715576172,32.975471496582031,32.846599578857422,32.394161224365234,32.049625396728516,32.561630249023438]
[null,null,null,null,"Coincident",32.062747955322266,31.755449295043945,31.657268524169922,31.533546447753906,31.09919548034668,30.768430709838867,31.259969711303711]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.665248870849609,33.329727172851562,33.222599029541016,33.087650299072266,32.614299774169922,32.254302978515625,32.789432525634766]
[null,null,null,null,"Coincident",32.233772277832031,31.919551849365234,31.819177627563477,31.692703247070312,31.248802185058594,30.910886764526367,31.413091659545898]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547]
[null,null,null,null,"Coincident",52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547,52.299999237060547]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.523445129394531,18.523445129394531,18.523445129394531,18.523445129394531,18.523445129394531,18.523445129394531,18.523445129394531]
[null,null,null,null,"Coincident",17.647333145141602,17.647333145141602,17.647333145141602,17.647333145141602,17.647333145141602,17.647333145141602,17.647333145141602]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.784235000610352,19.784235000610352,19.784235000610352,19.784235000610352,19.784235000610352,19.784235000610352,19.784235000610352]
[null,null,null,null,"Coincident",18.420343399047852,18.420343399047852,18.420343399047852,18.420343399047852,18.420343399047852,18.420343399047852,18.420343399047852]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.467544555664063,17.467544555664063,17.467544555664063,17.467544555664063,17.467544555664063,17.467544555664063,17.467544555664063]
[null,null,null,null,"Coincident",16.641374588012695,16.641374588012695,16.641374588012695,16.641374588012695,16.641374588012695,16.641374588012695,16.641374588012695]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.656463623046875,18.656463623046875,18.656463623046875,18.656463623046875,18.656463623046875,18.656463623046875,18.656463623046875]
[null,null,null,null,"Coincident",17.370321273803711,17.370321273803711,17.370321273803711,17.370321273803711,17.370321273803711,17.370321273803711,17.370321273803711]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,null,null,"Coincident",8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734,8.3999996185302734]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6883201599121094,5.6883201599121094,5.6883201599121094,5.6883201599121094,5.6883201599121094,5.6883201599121094,5.6883201599121094]
[null,null,null,null,"Coincident",0.88879996538162231,0.88879996538162231,0.88879996538162231,0.88879996538162231,0.88879996538162231,0.88879996538162231,0.88879996538162231]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.4273524284362793,7.4273524284362793,7.4273524284362793,7.4273524284362793,7.4273524284362793,7.4273524284362793,7.4273524284362793]
[null,null,null,null,"Coincident",1.1483837366104126,1.1483837366104126,1.1483837366104126,1.1483837366104126,1.1483837366104126,1.1483837366104126,1.1483837366104126]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.6319999694824219,5.6319999694824219,5.6319999694824219,5.6319999694824219,5.6319999694824219,5.6319999694824219,5.6319999694824219]
[null,null,null,null,"Coincident",0.87999999523162842,0.87999999523162842,0.87999999523162842,0.87999999523162842,0.87999999523162842,0.87999999523162842,0.87999999523162842]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3538141250610352,7.3538141250610352,7.3538141250610352,7.3538141250610352,7.3538141250610352,7.3538141250610352,7.3538141250610352]
[null,null,null,null,"Coincident",1.1370136737823486,1.1370136737823486,1.1370136737823486,1.1370136737823486,1.1370136737823486,1.1370136737823486,1.1370136737823486]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",1.5,1.5,1.5,1.5,1.5,1.5,1.5]
[null,null,null,null,"Coincident",1.5,1.5,1.5,1.5,1.5,1.5,1.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.62418001890182495,0.62418001890182495,0.62418001890182495,0.62418001890182495,0.62418001890182495,0.62418001890182495,0.62418001890182495]
[null,null,null,null,"Coincident",0.59994000196456909,0.59994000196456909,0.59994000196456909,0.59994000196456909,0.59994000196456909,0.59994000196456909,0.59994000196456909]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.70914947986602783,0.70914947986602783,0.70914947986602783,0.70914947986602783,0.70914947986602783,0.70914947986602783,0.70914947986602783]
[null,null,null,null,"Coincident",0.65984779596328735,0.65984779596328735,0.65984779596328735,0.65984779596328735,0.65984779596328735,0.65984779596328735,0.65984779596328735]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.61799997091293335,0.61799997091293335,0.61799997091293335,0.61799997091293335,0.61799997091293335,0.61799997091293335,0.61799997091293335]
[null,null,null,null,"Coincident",0.59399998188018799,0.59399998188018799,0.59399998188018799,0.59399998188018799,0.59399998188018799,0.59399998188018799,0.59399998188018799]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.70212811231613159,0.70212811231613159,0.70212811231613159,0.70212811231613159,0.70212811231613159,0.70212811231613159,0.70212811231613159]
[null,null,null,null,"Coincident",0.65331459045410156,0.65331459045410156,0.65331459045410156,0.65331459045410156,0.65331459045410156,0.65331459045410156,0.65331459045410156]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453]
[null,null,null,null,"Coincident",24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453,24.700000762939453]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.291800498962402,14.57819938659668,14.57819938659668,14.57819938659668,14.57819938659668,14.57819938659668,14.57819938659668]
[null,null,null,null,"Coincident",8.7466001510620117,11.655223846435547,11.655223846435547,11.655223846435547,11.655223846435547,11.655223846435547,11.655223846435547]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.177465438842773,17.012674331665039,17.012674331665039,17.012674331665039,17.012674331665039,17.012674331665039,17.012674331665039]
[null,null,null,null,"Coincident",9.7298183441162109,13.110018730163574,13.110018730163574,13.110018730163574,13.110018730163574,13.110018730163574,13.110018730163574]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.180000305175781,14.466399192810059,14.466399192810059,14.466399192810059,14.466399192810059,14.466399192810059,14.466399192810059]
[null,null,null,null,"Coincident",8.6599998474121094,11.568623542785645,11.568623542785645,11.568623542785645,11.568623542785645,11.568623542785645,11.568623542785645]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.046995162963867,16.882204055786133,16.882204055786133,16.882204055786133,16.882204055786133,16.882204055786133,16.882204055786133]
[null,null,null,null,"Coincident",9.6334829330444336,13.013707160949707,13.013707160949707,13.013707160949707,13.013707160949707,13.013707160949707,13.013707160949707]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1786751747131348,2.1786751747131348,2.1786751747131348,2.1786751747131348,2.1786751747131348,2.1786751747131348,2.1786751747131348]
[null,null,null,null,"Coincident",1.1090546846389771,1.1090546846389771,1.1090546846389771,1.1090546846389771,1.1090546846389771,1.1090546846389771,1.1090546846389771]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.522397518157959,2.522397518157959,2.522397518157959,2.522397518157959,2.522397518157959,2.522397518157959,2.522397518157959]
[null,null,null,null,"Coincident",1.2874324321746826,1.2874324321746826,1.2874324321746826,1.2874324321746826,1.2874324321746826,1.2874324321746826,1.2874324321746826]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1571040153503418,2.1571040153503418,2.1571040153503418,2.1571040153503418,2.1571040153503418,2.1571040153503418,2.1571040153503418]
[null,null,null,null,"Coincident",1.0980739593505859,1.0980739593505859,1.0980739593505859,1.0980739593505859,1.0980739593505859,1.0980739593505859,1.0980739593505859]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4974231719970703,2.4974231719970703,2.4974231719970703,2.4974231719970703,2.4974231719970703,2.4974231719970703,2.4974231719970703]
[null,null,null,null,"Coincident",1.2746856212615967,1.2746856212615967,1.2746856212615967,1.2746856212615967,1.2746856212615967,1.2746856212615967,1.2746856212615967]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",15,15,15,15,15,15,15]
[null,null,null,null,"Coincident",15,15,15,15,15,15,15]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3997678756713867,8.3997678756713867,8.3997678756713867,8.3997678756713867,8.3997678756713867,8.3997678756713867,8.3997678756713867]
[null,null,null,null,"Coincident",4.1907272338867187,4.1907272338867187,4.1907272338867187,4.1907272338867187,4.1907272338867187,4.1907272338867187,4.1907272338867187]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.4815149307250977,9.4815149307250977,9.4815149307250977,9.4815149307250977,9.4815149307250977,9.4815149307250977,9.4815149307250977]
[null,null,null,null,"Coincident",5.0300145149230957,5.0300145149230957,5.0300145149230957,5.0300145149230957,5.0300145149230957,5.0300145149230957,5.0300145149230957]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.3166017532348633,8.3166017532348633,8.3166017532348633,8.3166017532348633,8.3166017532348633,8.3166017532348633,8.3166017532348633]
[null,null,null,null,"Coincident",4.1492347717285156,4.1492347717285156,4.1492347717285156,4.1492347717285156,4.1492347717285156,4.1492347717285156,4.1492347717285156]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.3876380920410156,9.3876380920410156,9.3876380920410156,9.3876380920410156,9.3876380920410156,9.3876380920410156,9.3876380920410156]
[null,null,null,null,"Coincident",4.9802122116088867,4.9802122116088867,4.9802122116088867,4.9802122116088867,4.9802122116088867,4.9802122116088867,4.9802122116088867]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",23.899999618530273,30,30,30,30,30,30]
[null,null,null,null,"Coincident",23.899999618530273,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.382944107055664,13.382944107055664,13.382944107055664,13.382944107055664,13.382944107055664,13.382944107055664,13.382944107055664]
[null,null,null,null,"Coincident",5.8805899620056152,5.8805899620056152,5.8805899620056152,5.8805899620056152,5.8805899620056152,5.8805899620056152,5.8805899620056152]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.633292198181152,13.633292198181152,13.633292198181152,13.633292198181152,13.633292198181152,13.633292198181152,13.633292198181152]
[null,null,null,null,"Coincident",6.0014691352844238,6.0014691352844238,6.0014691352844238,6.0014691352844238,6.0014691352844238,6.0014691352844238,6.0014691352844238]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.250439643859863,13.250439643859863,13.250439643859863,13.250439643859863,13.250439643859863,13.250439643859863,13.250439643859863]
[null,null,null,null,"Coincident",5.8223662376403809,5.8223662376403809,5.8223662376403809,5.8223662376403809,5.8223662376403809,5.8223662376403809,5.8223662376403809]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.488211631774902,13.488211631774902,13.488211631774902,13.488211631774902,13.488211631774902,13.488211631774902,13.488211631774902]
[null,null,null,null,"Coincident",5.9420490264892578,5.9420490264892578,5.9420490264892578,5.9420490264892578,5.9420490264892578,5.9420490264892578,5.9420490264892578]
[null,"Private Sub","Substation Rating","MVA","Non-Coincident",25,25,25,25,25,25,25]
[null,null,null,null,"Coincident",25,25,25,25,25,25,25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER","WINTER"]
[null,null,null,null,"Coincident","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER","SUMMER"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.183681488037109,13.183681488037109,13.183681488037109,13.183681488037109,13.183681488037109,13.183681488037109,13.183681488037109]
[null,null,null,null,"Coincident",12.387777328491211,12.387777328491211,12.387777328491211,12.387777328491211,12.387777328491211,12.387777328491211,12.387777328491211]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.100940704345703,15.100940704345703,15.100940704345703,15.100940704345703,15.100940704345703,15.100940704345703,15.100940704345703]
[null,null,null,null,"Coincident",15.371224403381348,15.371224403381348,15.371224403381348,15.371224403381348,15.371224403381348,15.371224403381348,15.371224403381348]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.053149223327637,13.053149223327637,13.053149223327637,13.053149223327637,13.053149223327637,13.053149223327637,13.053149223327637]
[null,null,null,null,"Coincident",12.26512622833252,12.26512622833252,12.26512622833252,12.26512622833252,12.26512622833252,12.26512622833252,12.26512622833252]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.951425552368164,14.951425552368164,14.951425552368164,14.951425552368164,14.951425552368164,14.951425552368164,14.951425552368164]
[null,null,null,null,"Coincident",32.273643493652344,31.906328201293945,31.776340484619141,31.553886413574219,30.963563919067383,30.594964981079102,31.071853637695313]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Abermain BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Algester BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Archerfield BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ashgrove West BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beaudesert BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beenleigh BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beerwah BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Belmont BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brendale BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Browns Plains BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Burleigh Heads BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caboolture BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cleveland BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coomera BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coorparoo BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Doboy BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gatton BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Goodna BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Griffin BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gympie BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hays Inlet BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ibis BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jimboomba BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lockrose BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Loganlea BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lytton BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Meeandah BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Molendinar BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mudgeeraba BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Myrtletown BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nambour BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nudgee BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Postmans Ridge BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Raceview BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Richlands BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Runcorn BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sandgate BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stafford BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stradbroke Is BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sunrise Hills BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tennyson BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Victoria Park BS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Acacia Ridge","Acacia Ridge","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Albany Creek","Albany Creek","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Alexandra Headland","Alexandra Headland","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Algester","Algester","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Amamoor","Amamoor","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Amberley","Amberley","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ann St","Ann St","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Annerley","Annerley","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Arana Hills","Arana Hills","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Archerfield","Archerfield","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Arundel","Arundel","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ashgrove","Ashgrove","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Astor Terrace","Astor Terrace","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bald Hills Bus 1","Bald Hills Bus 1","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bald Hills Bus 2","Bald Hills Bus 2","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beaudesert","Beaudesert","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beenleigh","Beenleigh","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beenleigh North","Beenleigh North","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Beerwah","Beerwah","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Belmont","Belmont","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bethania","Bethania","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Birkdale","Birkdale","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Birtinya","Birtinya","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Black Mountain","Black Mountain","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Boonah","Boonah","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Booval","Booval","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brendale","Brendale","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bribie Island","Bribie Island","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Brighton","Brighton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Broadbeach","Broadbeach","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bromelton","Bromelton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Browns Plains","Browns Plains","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bulimba","Bulimba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bundall","Bundall","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Bundamba","Bundamba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Buranda","Buranda","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Burleigh Heads","Burleigh Heads","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Burpengary","Burpengary","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caboolture","Caboolture","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caboolture West","Caboolture West","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cades County","Cades County","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Calamvale","Calamvale","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Caloundra","Caloundra","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Camp Hill","Camp Hill","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Capalaba","Capalaba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Capalaba South","Capalaba South","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Carole Park","Carole Park","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Carole Park Central","Carole Park Central","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Carpendale","Carpendale","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Charlotte St","Charlotte St","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Chermside","Chermside","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Clayfield","Clayfield","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cleveland","Cleveland","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coolum","Coolum","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coomera","Coomera","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coominya","Coominya","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cooneana","Cooneana","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coopers Plains","Coopers Plains","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cooran","Cooran","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cooroy","Cooroy","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Coorparoo","Coorparoo","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Cornubia","Cornubia","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Crestmead","Crestmead","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Currimundi","Currimundi","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Currumbin","Currumbin","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Darra","Darra","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Deception Bay","Deception Bay","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Doboy","Doboy","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Duffield Road","Duffield Road","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Eight Mile Plains Bus 1","Eight Mile Plains Bus 1","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Eight Mile Plains Bus 2","Eight Mile Plains Bus 2","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Enoggera","Enoggera","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Esk","Esk","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Eumundi","Eumundi","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Fisherman Is A","Fisherman Is A","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Fisherman Is B","Fisherman Is B","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Flinders","Flinders","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gatton A","Gatton A","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gaven","Gaven","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Geebung","Geebung","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gibson Island","Gibson Island","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Glenore Grove","Glenore Grove","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Goodna","Goodna","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Goomboorian","Goomboorian","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Grantham","Grantham","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Grovely","Grovely","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gympie","Gympie","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gympie North","Gympie North","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Gympie South","Gympie South","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hamilton","Hamilton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hamilton Lands","Hamilton Lands","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Heathwood","Heathwood","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Helidon","Helidon","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hemmant","Hemmant","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hendra","Hendra","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Herring Lagoon","Herring Lagoon","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Holland Park","Holland Park","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Holland Park East","Holland Park East","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hollywell","Hollywell","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Hope Island","Hope Island","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ibis","Ibis","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Imbil","Imbil","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Inala","Inala","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Indooroopilly","Indooroopilly","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Innisplain","Innisplain","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ipswich South","Ipswich South","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jimboomba","Jimboomba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Jindalee","Jindalee","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kalbar","Kalbar","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kallangur","Kallangur","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Karrabin","Karrabin","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kawana","Kawana","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kedron","Kedron","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kelvin Grove","Kelvin Grove","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kenilworth","Kenilworth","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kenmore","Kenmore","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kilcoy","Kilcoy","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kingston","Kingston","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Kirra","Kirra","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Labrador","Labrador","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Laidley","Laidley","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Landsborough","Landsborough","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lawnton","Lawnton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lockrose","Lockrose","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Logan Village","Logan Village","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Loganholme","Loganholme","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Loganlea","Loganlea","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lomandra Drive","Lomandra Drive","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lota","Lota","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lowood","Lowood","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lytton A","Lytton A","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Lytton B","Lytton B","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Makerston St","Makerston St","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Maleny","Maleny","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mango Hill Bus 1","Mango Hill Bus 1","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mango Hill Bus 2","Mango Hill Bus 2","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Marburg","Marburg","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"McLachlan St","McLachlan St","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Meeandah","Meeandah","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Merrimac","Merrimac","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Miami","Miami","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Milton","Milton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Moggill","Moggill","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Molendinar","Molendinar","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mooloolaba","Mooloolaba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Moorooka","Moorooka","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morayfield","Morayfield","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Morayfield North","Morayfield North","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Cotton","Mt Cotton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Crosby West","Mt Crosby West","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Gravatt","Mt Gravatt","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Sylvia","Mt Sylvia","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Tamborine Bus 1","Mt Tamborine Bus 1","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mt Tamborine Bus 2","Mt Tamborine Bus 2","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Mudgeeraba West Pkg","Mudgeeraba West Pkg","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Murarrie","Murarrie","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Murrumba","Murrumba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Myrtletown","Myrtletown","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nambour","Nambour","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Narangba","Narangba","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nerang","Nerang","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Newmarket","Newmarket","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Newstead","Newstead","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Ningi","Ningi","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Noosaville","Noosaville","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North Maclean","North Maclean","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"North Springwood","North Springwood","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nth Ipswich","Nth Ipswich","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nth Pine Dam","Nth Pine Dam","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nudgee","Nudgee","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Nundah","Nundah","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Oxley","Oxley","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Palm Beach","Palm Beach","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Palmwoods Central","Palmwoods Central","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pandanus Avenue","Pandanus Avenue","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Parkwood","Parkwood","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Peregian","Peregian","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Pimpama East","Pimpama East","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Postmans Ridge","Postmans Ridge","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Queensport","Queensport","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Raby Bay","Raby Bay","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Redbank","Redbank","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Redbank Plains","Redbank Plains","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Redcliffe","Redcliffe","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Redland Bay","Redland Bay","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Robina","Robina","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rocklea","Rocklea","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Roderick St","Roderick St","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Rosewood","Rosewood","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Runcorn","Runcorn","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Russell Island","Russell Island","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Salisbury","Salisbury","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Samford","Samford","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sandgate","Sandgate","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Scarborough","Scarborough","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Scrub Road","Scrub Road","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sherwood","Sherwood","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Somerset Dam","Somerset Dam","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Southport","Southport","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Spring Creek","Spring Creek","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Springfield","Springfield","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Springfield Central","Springfield Central","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"St Lucia","St Lucia","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stafford","Stafford","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stapylton","Stapylton","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Stradbroke Is","Stradbroke Is","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Strathpine","Strathpine","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sumner","Sumner","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Sunnybank","Sunnybank","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Surfers Paradise","Surfers Paradise","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tamborine Village","Tamborine Village","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tanah Merah","Tanah Merah","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tarampa","Tarampa","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Taringa","Taringa","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tennyson","Tennyson","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tenthill","Tenthill","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tewantin","Tewantin","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"The Gap","The Gap","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tin Can Bay","Tin Can Bay","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Tingalpa","Tingalpa","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Toogoolawah","Toogoolawah","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Toorbul Point","Toorbul Point","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Toowong","Toowong","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Upper Mt Gravatt","Upper Mt Gravatt","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Varsity Lakes","Varsity Lakes","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Victoria Park","Victoria Park","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Victoria Point","Victoria Point","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wacol","Wacol","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wacol South","Wacol South","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wamuran","Wamuran","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wellington Rd","Wellington Rd","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"West End","West End","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"West Maroochydore","West Maroochydore","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Whinstanes","Whinstanes","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Whiteside","Whiteside","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wivenhoe","Wivenhoe","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woodford","Woodford","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Woodridge","Woodridge","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Wynnum","Wynnum","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yamanto","Yamanto","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yandina","Yandina","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Yatala","Yatala","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"Zillmere","Zillmere","MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.1 Telephone answering","index":30,"n_rows":1834,"n_cols":4,"rows_kept":1834,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"6.1 TELEPHONE ANSWERING"]
[]
[]
[null,"6.1.1 - TELEPHONE ANSWERING DATA"]
["C10 starts at first day of PRCP_y5 and goes for 5 full years","Date","Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) "]
[null,{"$f":"IF(dms_RPT=\"calendar\",DATE(VALUE(PRCP_y3),1,1),(DATE(VALUE(LEFT(PRCP_y3,2)&RIGHT(PRCP_y3,2)),7,1)))","v":"2013-07-01"},377,318]
[null,{"$f":"B9+1","v":"2013-07-02"},310,268]
[null,"2013-07-03",307,277]
[null,"2013-07-04",218,205]
[null,"2013-07-05",311,232]
[null,"2013-07-06",176,144]
[null,"2013-07-07",94,89]
[null,{"$f":"B15+1","v":"2013-07-08"},279,259]
[null,"2013-07-09",223,210]
[null,"2013-07-10",281,249]
[null,"2013-07-11",250,227]
[null,"2013-07-12",220,209]
[null,"2013-07-13",157,149]
[null,"2013-07-14",143,135]
[null,"2013-07-15",324,296]
[null,"2013-07-16",442,338]
[null,"2013-07-17",188,176]
[null,"2013-07-18",236,220]
[null,"2013-07-19",304,274]
[null,"2013-07-20",197,167]
[null,"2013-07-21",101,99]
[null,"2013-07-22",379,310]
[null,"2013-07-23",224,213]
[null,"2013-07-24",304,259]
[null,"2013-07-25",333,309]
[null,"2013-07-26",239,214]
[null,"2013-07-27",254,220]
[null,"2013-07-28",110,98]
[null,"2013-07-29",243,236]
[null,"2013-07-30",205,189]
[null,"2013-07-31",189,164]
[null,"2013-08-01",200,172]
[null,"2013-08-02",184,174]
[null,"2013-08-03",259,230]
[null,"2013-08-04",137,133]
[null,"2013-08-05",302,255]
[null,"2013-08-06",273,254]
[null,"2013-08-07",240,219]
[null,"2013-08-08",339,312]
[null,"2013-08-09",186,177]
[null,"2013-08-10",185,167]
[null,"2013-08-11",139,118]
[null,"2013-08-12",252,230]
[null,"2013-08-13",207,192]
[null,"2013-08-14",180,177]
[null,"2013-08-15",199,185]
[null,"2013-08-16",323,223]
[null,"2013-08-17",153,128]
[null,"2013-08-18",91,84]
[null,"2013-08-19",311,283]
[null,"2013-08-20",295,265]
[null,"2013-08-21",274,201]
[null,"2013-08-22",220,203]
[null,"2013-08-23",228,197]
[null,"2013-08-24",216,180]
[null,"2013-08-25",135,127]
[null,"2013-08-26",213,178]
[null,"2013-08-27",201,189]
[null,"2013-08-28",213,191]
[null,"2013-08-29",201,187]
[null,"2013-08-30",293,241]
[null,"2013-08-31",176,151]
[null,"2013-09-01",98,94]
[null,"2013-09-02",220,201]
[null,"2013-09-03",266,235]
[null,"2013-09-04",216,205]
[null,"2013-09-05",274,243]
[null,"2013-09-06",227,203]
[null,"2013-09-07",148,137]
[null,"2013-09-08",111,102]
[null,"2013-09-09",238,215]
[null,{"$f":"B79+1","v":"2013-09-10"},264,232]
[null,"2013-09-11",284,259]
[null,"2013-09-12",265,237]
[null,"2013-09-13",309,252]
[null,"2013-09-14",235,186]
[null,"2013-09-15",248,212]
[null,"2013-09-16",531,451]
[null,"2013-09-17",560,435]
[null,"2013-09-18",313,269]
[null,"2013-09-19",274,252]
[null,"2013-09-20",192,181]
[null,"2013-09-21",206,190]
[null,"2013-09-22",139,132]
[null,"2013-09-23",262,240]
[null,"2013-09-24",358,315]
[null,"2013-09-25",268,243]
[null,"2013-09-26",237,206]
[null,"2013-09-27",224,191]
[null,"2013-09-28",212,172]
[null,"2013-09-29",114,101]
[null,"2013-09-30",270,243]
[null,"2013-10-01",355,275]
[null,"2013-10-02",309,287]
[null,"2013-10-03",365,309]
[null,"2013-10-04",264,213]
[null,"2013-10-05",214,194]
[null,"2013-10-06",109,106]
[null,"2013-10-07",215,198]
[null,"2013-10-08",286,249]
[null,"2013-10-09",230,202]
[null,"2013-10-10",279,252]
[null,"2013-10-11",304,257]
[null,"2013-10-12",203,175]
[null,"2013-10-13",162,146]
[null,"2013-10-14",368,344]
[null,"2013-10-15",219,210]
[null,"2013-10-16",305,272]
[null,"2013-10-17",263,249]
[null,"2013-10-18",334,300]
[null,"2013-10-19",261,210]
[null,"2013-10-20",159,145]
[null,"2013-10-21",431,393]
[null,"2013-10-22",313,276]
[null,"2013-10-23",208,197]
[null,"2013-10-24",279,235]
[null,"2013-10-25",259,239]
[null,"2013-10-26",198,170]
[null,"2013-10-27",116,109]
[null,"2013-10-28",253,231]
[null,"2013-10-29",405,363]
[null,"2013-10-30",320,283]
[null,"2013-10-31",308,249]
[null,"2013-11-01",237,206]
[null,"2013-11-02",187,163]
[null,"2013-11-03",181,156]
[null,"2013-11-04",234,221]
[null,"2013-11-05",204,195]
[null,"2013-11-06",216,211]
[null,"2013-11-07",230,190]
[null,"2013-11-08",297,246]
[null,"2013-11-09",162,160]
[null,"2013-11-10",0,0]
[null,"2013-11-11",601,461]
[null,"2013-11-12",288,247]
[null,{"$f":"B143+1","v":"2013-11-13"},463,382]
[null,"2013-11-14",748,590]
[null,"2013-11-15",401,353]
[null,"2013-11-16",678,416]
[null,"2013-11-17",263,219]
[null,"2013-11-18",699,518]
[null,"2013-11-19",577,481]
[null,"2013-11-20",461,335]
[null,"2013-11-21",295,262]
[null,"2013-11-22",228,196]
[null,"2013-11-23",669,500]
[null,"2013-11-24",897,637]
[null,"2013-11-25",371,314]
[null,"2013-11-26",329,299]
[null,"2013-11-27",347,298]
[null,"2013-11-28",284,212]
[null,"2013-11-29",287,252]
[null,"2013-11-30",417,326]
[null,"2013-12-01",141,130]
[null,"2013-12-02",313,273]
[null,"2013-12-03",212,198]
[null,"2013-12-04",321,251]
[null,"2013-12-05",374,321]
[null,"2013-12-06",257,237]
[null,"2013-12-07",194,169]
[null,"2013-12-08",122,115]
[null,"2013-12-09",280,226]
[null,"2013-12-10",313,232]
[null,"2013-12-11",362,280]
[null,"2013-12-12",388,343]
[null,"2013-12-13",295,240]
[null,"2013-12-14",231,216]
[null,"2013-12-15",199,181]
[null,"2013-12-16",273,240]
[null,"2013-12-17",292,254]
[null,"2013-12-18",250,217]
[null,"2013-12-19",232,212]
[null,"2013-12-20",380,292]
[null,"2013-12-21",141,130]
[null,"2013-12-22",220,180]
[null,"2013-12-23",232,216]
[null,"2013-12-24",213,190]
[null,"2013-12-25",430,274]
[null,"2013-12-26",124,99]
[null,"2013-12-27",368,332]
[null,"2013-12-28",270,229]
[null,"2013-12-29",0,0]
[null,"2013-12-30",614,521]
[null,"2013-12-31",352,314]
[null,"2014-01-01",181,146]
[null,"2014-01-02",848,592]
[null,"2014-01-03",572,392]
[null,"2014-01-04",1972,956]
[null,"2014-01-05",365,295]
[null,"2014-01-06",0,0]
[null,"2014-01-07",1324,1033]
[null,"2014-01-08",480,413]
[null,"2014-01-09",294,264]
[null,"2014-01-10",301,274]
[null,"2014-01-11",279,219]
[null,"2014-01-12",177,159]
[null,"2014-01-13",427,344]
[null,"2014-01-14",264,242]
[null,"2014-01-15",300,262]
[null,{"$f":"B207+1","v":"2014-01-16"},275,247]
[null,"2014-01-17",254,212]
[null,"2014-01-18",231,204]
[null,"2014-01-19",169,153]
[null,"2014-01-20",272,237]
[null,"2014-01-21",404,311]
[null,"2014-01-22",588,426]
[null,"2014-01-23",665,437]
[null,"2014-01-24",465,405]
[null,"2014-01-25",297,250]
[null,"2014-01-26",257,218]
[null,"2014-01-27",210,188]
[null,"2014-01-28",336,299]
[null,"2014-01-29",326,280]
[null,"2014-01-30",329,288]
[null,"2014-01-31",279,237]
[null,"2014-02-01",210,187]
[null,"2014-02-02",180,128]
[null,"2014-02-03",320,271]
[null,"2014-02-04",267,206]
[null,"2014-02-05",417,346]
[null,"2014-02-06",294,253]
[null,"2014-02-07",273,236]
[null,"2014-02-08",193,164]
[null,"2014-02-09",124,120]
[null,"2014-02-10",243,231]
[null,"2014-02-11",221,211]
[null,"2014-02-12",253,231]
[null,"2014-02-13",362,316]
[null,"2014-02-14",264,246]
[null,"2014-02-15",241,219]
[null,"2014-02-16",412,300]
[null,"2014-02-17",358,296]
[null,"2014-02-18",442,385]
[null,"2014-02-19",458,393]
[null,"2014-02-20",386,319]
[null,"2014-02-21",538,442]
[null,"2014-02-22",298,229]
[null,"2014-02-23",248,207]
[null,"2014-02-24",316,267]
[null,"2014-02-25",255,228]
[null,"2014-02-26",227,213]
[null,"2014-02-27",240,221]
[null,"2014-02-28",361,293]
[null,"2014-03-01",361,265]
[null,"2014-03-02",247,229]
[null,"2014-03-03",328,291]
[null,"2014-03-04",242,200]
[null,"2014-03-05",297,276]
[null,"2014-03-06",254,239]
[null,"2014-03-07",202,183]
[null,"2014-03-08",171,145]
[null,"2014-03-09",164,121]
[null,"2014-03-10",344,275]
[null,"2014-03-11",271,216]
[null,"2014-03-12",246,222]
[null,"2014-03-13",224,179]
[null,"2014-03-14",217,201]
[null,"2014-03-15",125,119]
[null,"2014-03-16",440,332]
[null,"2014-03-17",364,299]
[null,"2014-03-18",385,278]
[null,"2014-03-19",249,212]
[null,"2014-03-20",249,233]
[null,{"$f":"B271+1","v":"2014-03-21"},246,228]
[null,"2014-03-22",145,139]
[null,"2014-03-23",93,92]
[null,"2014-03-24",278,246]
[null,"2014-03-25",319,283]
[null,"2014-03-26",281,249]
[null,"2014-03-27",481,401]
[null,"2014-03-28",626,533]
[null,"2014-03-29",318,247]
[null,"2014-03-30",280,255]
[null,"2014-03-31",361,312]
[null,"2014-04-01",346,298]
[null,"2014-04-02",292,244]
[null,"2014-04-03",285,223]
[null,"2014-04-04",265,206]
[null,"2014-04-05",226,183]
[null,"2014-04-06",497,318]
[null,"2014-04-07",348,282]
[null,"2014-04-08",221,193]
[null,"2014-04-09",233,216]
[null,"2014-04-10",274,244]
[null,"2014-04-11",317,282]
[null,"2014-04-12",212,190]
[null,"2014-04-13",141,134]
[null,"2014-04-14",444,338]
[null,"2014-04-15",231,207]
[null,"2014-04-16",263,230]
[null,"2014-04-17",207,191]
[null,"2014-04-18",240,221]
[null,"2014-04-19",197,176]
[null,"2014-04-20",98,88]
[null,"2014-04-21",137,113]
[null,"2014-04-22",246,243]
[null,"2014-04-23",305,266]
[null,"2014-04-24",204,180]
[null,"2014-04-25",98,93]
[null,"2014-04-26",145,129]
[null,"2014-04-27",172,167]
[null,"2014-04-28",230,212]
[null,"2014-04-29",263,231]
[null,"2014-04-30",278,246]
[null,"2014-05-01",275,230]
[null,"2014-05-02",276,229]
[null,"2014-05-03",245,215]
[null,"2014-05-04",248,207]
[null,"2014-05-05",311,250]
[null,"2014-05-06",259,230]
[null,"2014-05-07",303,218]
[null,"2014-05-08",202,181]
[null,"2014-05-09",210,206]
[null,"2014-05-10",181,166]
[null,"2014-05-11",100,96]
[null,"2014-05-12",349,292]
[null,"2014-05-13",219,212]
[null,"2014-05-14",313,279]
[null,"2014-05-15",337,283]
[null,"2014-05-16",374,296]
[null,"2014-05-17",221,192]
[null,"2014-05-18",132,127]
[null,"2014-05-19",278,252]
[null,"2014-05-20",349,264]
[null,"2014-05-21",319,283]
[null,"2014-05-22",345,273]
[null,"2014-05-23",227,210]
[null,{"$f":"B335+1","v":"2014-05-24"},137,127]
[null,"2014-05-25",115,105]
[null,"2014-05-26",204,180]
[null,"2014-05-27",184,159]
[null,"2014-05-28",215,180]
[null,"2014-05-29",265,206]
[null,"2014-05-30",207,186]
[null,"2014-05-31",200,161]
[null,"2014-06-01",88,84]
[null,"2014-06-02",219,197]
[null,"2014-06-03",257,230]
[null,"2014-06-04",190,182]
[null,"2014-06-05",225,186]
[null,"2014-06-06",253,217]
[null,"2014-06-07",185,177]
[null,"2014-06-08",124,116]
[null,"2014-06-09",145,136]
[null,"2014-06-10",245,225]
[null,"2014-06-11",188,170]
[null,"2014-06-12",195,181]
[null,"2014-06-13",256,224]
[null,"2014-06-14",170,160]
[null,"2014-06-15",162,152]
[null,"2014-06-16",224,206]
[null,"2014-06-17",330,254]
[null,"2014-06-18",235,219]
[null,"2014-06-19",221,205]
[null,"2014-06-20",273,246]
[null,"2014-06-21",197,183]
[null,"2014-06-22",161,147]
[null,"2014-06-23",248,243]
[null,"2014-06-24",312,280]
[null,"2014-06-25",358,295]
[null,"2014-06-26",238,221]
[null,"2014-06-27",246,218]
[null,"2014-06-28",234,216]
[null,"2014-06-29",244,230]
[null,"2014-06-30",297,260]
[null,"2014-07-01",318,283]
[null,"2014-07-02",252,216]
[null,"2014-07-03",248,212]
[null,"2014-07-04",203,188]
[null,"2014-07-05",288,272]
[null,"2014-07-06",126,122]
[null,"2014-07-07",298,256]
[null,"2014-07-08",273,249]
[null,"2014-07-09",316,259]
[null,"2014-07-10",282,208]
[null,"2014-07-11",378,311]
[null,"2014-07-12",182,158]
[null,"2014-07-13",151,127]
[null,"2014-07-14",269,257]
[null,"2014-07-15",228,196]
[null,"2014-07-16",285,242]
[null,"2014-07-17",274,249]
[null,"2014-07-18",1284,817]
[null,"2014-07-19",343,239]
[null,"2014-07-20",164,157]
[null,"2014-07-21",425,344]
[null,"2014-07-22",276,253]
[null,"2014-07-23",239,221]
[null,"2014-07-24",259,248]
[null,"2014-07-25",230,216]
[null,"2014-07-26",160,154]
[null,{"$f":"B399+1","v":"2014-07-27"},135,128]
[null,"2014-07-28",279,270]
[null,"2014-07-29",221,209]
[null,"2014-07-30",237,218]
[null,"2014-07-31",229,216]
[null,"2014-08-01",278,252]
[null,"2014-08-02",158,145]
[null,"2014-08-03",120,103]
[null,"2014-08-04",172,162]
[null,"2014-08-05",257,221]
[null,"2014-08-06",303,235]
[null,"2014-08-07",220,206]
[null,"2014-08-08",190,183]
[null,"2014-08-09",177,145]
[null,"2014-08-10",99,94]
[null,"2014-08-11",231,187]
[null,"2014-08-12",220,199]
[null,"2014-08-13",228,212]
[null,"2014-08-14",247,235]
[null,"2014-08-15",194,183]
[null,"2014-08-16",554,380]
[null,"2014-08-17",318,247]
[null,"2014-08-18",516,433]
[null,"2014-08-19",288,252]
[null,"2014-08-20",211,190]
[null,"2014-08-21",266,246]
[null,"2014-08-22",274,202]
[null,"2014-08-23",387,289]
[null,"2014-08-24",158,154]
[null,"2014-08-25",317,285]
[null,"2014-08-26",217,185]
[null,"2014-08-27",237,211]
[null,"2014-08-28",344,299]
[null,"2014-08-29",244,221]
[null,"2014-08-30",150,138]
[null,"2014-08-31",76,72]
[null,"2014-09-01",434,387]
[null,"2014-09-02",317,289]
[null,"2014-09-03",268,234]
[null,"2014-09-04",346,282]
[null,"2014-09-05",214,189]
[null,"2014-09-06",189,154]
[null,"2014-09-07",106,105]
[null,"2014-09-08",217,198]
[null,"2014-09-09",191,173]
[null,"2014-09-10",227,197]
[null,"2014-09-11",216,182]
[null,"2014-09-12",237,207]
[null,"2014-09-13",257,183]
[null,"2014-09-14",107,104]
[null,"2014-09-15",270,257]
[null,"2014-09-16",202,180]
[null,"2014-09-17",235,193]
[null,"2014-09-18",244,171]
[null,"2014-09-19",206,181]
[null,"2014-09-20",189,171]
[null,"2014-09-21",116,107]
[null,"2014-09-22",243,207]
[null,"2014-09-23",205,187]
[null,"2014-09-24",244,216]
[null,"2014-09-25",613,492]
[null,"2014-09-26",328,268]
[null,"2014-09-27",187,162]
[null,"2014-09-28",102,92]
[null,{"$f":"B463+1","v":"2014-09-29"},399,363]
[null,"2014-09-30",285,249]
[null,"2014-10-01",318,247]
[null,"2014-10-02",230,204]
[null,"2014-10-03",218,185]
[null,"2014-10-04",173,137]
[null,"2014-10-05",102,85]
[null,"2014-10-06",118,98]
[null,"2014-10-07",304,253]
[null,"2014-10-08",244,203]
[null,"2014-10-09",229,191]
[null,"2014-10-10",311,272]
[null,"2014-10-11",144,132]
[null,"2014-10-12",166,151]
[null,"2014-10-13",292,274]
[null,"2014-10-14",287,261]
[null,"2014-10-15",355,257]
[null,"2014-10-16",281,226]
[null,"2014-10-17",244,192]
[null,"2014-10-18",189,173]
[null,"2014-10-19",105,94]
[null,"2014-10-20",360,310]
[null,"2014-10-21",253,222]
[null,"2014-10-22",196,167]
[null,"2014-10-23",269,231]
[null,"2014-10-24",228,205]
[null,"2014-10-25",158,148]
[null,"2014-10-26",221,201]
[null,"2014-10-27",1158,945]
[null,"2014-10-28",579,355]
[null,"2014-10-29",370,326]
[null,"2014-10-30",286,227]
[null,"2014-10-31",296,262]
[null,"2014-11-01",240,201]
[null,"2014-11-02",265,231]
[null,"2014-11-03",264,243]
[null,"2014-11-04",279,229]
[null,"2014-11-05",169,149]
[null,"2014-11-06",498,364]
[null,"2014-11-07",320,287]
[null,"2014-11-08",168,157]
[null,"2014-11-09",96,93]
[null,"2014-11-10",295,281]
[null,"2014-11-11",281,237]
[null,"2014-11-12",243,169]
[null,"2014-11-13",202,171]
[null,"2014-11-14",348,243]
[null,"2014-11-15",253,217]
[null,"2014-11-16",1005,607]
[null,"2014-11-17",419,324]
[null,"2014-11-18",319,265]
[null,"2014-11-19",1463,792]
[null,"2014-11-20",614,455]
[null,"2014-11-21",444,356]
[null,"2014-11-22",390,315]
[null,"2014-11-23",193,184]
[null,"2014-11-24",387,345]
[null,"2014-11-25",376,342]
[null,"2014-11-26",310,285]
[null,"2014-11-27",0,0]
[null,"2014-11-28",4943,4290]
[null,"2014-11-29",884,852]
[null,"2014-11-30",287,198]
[null,"2014-12-01",430,308]
[null,{"$f":"B527+1","v":"2014-12-02"},399,368]
[null,"2014-12-03",376,322]
[null,"2014-12-04",340,260]
[null,"2014-12-05",497,414]
[null,"2014-12-06",389,329]
[null,"2014-12-07",195,187]
[null,"2014-12-08",1484,1373]
[null,"2014-12-09",1208,1026]
[null,"2014-12-10",565,467]
[null,"2014-12-11",1224,1093]
[null,"2014-12-12",679,491]
[null,"2014-12-13",282,246]
[null,"2014-12-14",177,153]
[null,"2014-12-15",454,404]
[null,"2014-12-16",389,337]
[null,"2014-12-17",723,501]
[null,"2014-12-18",0,0]
[null,"2014-12-19",863,639]
[null,"2014-12-20",342,256]
[null,"2014-12-21",187,164]
[null,"2014-12-22",419,364]
[null,"2014-12-23",339,251]
[null,"2014-12-24",273,258]
[null,"2014-12-25",111,108]
[null,"2014-12-26",162,151]
[null,"2014-12-27",374,344]
[null,"2014-12-28",242,193]
[null,"2014-12-29",284,265]
[null,"2014-12-30",403,362]
[null,"2014-12-31",462,388]
[null,"2015-01-01",422,285]
[null,"2015-01-02",259,230]
[null,"2015-01-03",280,251]
[null,"2015-01-04",261,245]
[null,"2015-01-05",329,303]
[null,"2015-01-06",281,253]
[null,"2015-01-07",260,238]
[null,"2015-01-08",285,246]
[null,"2015-01-09",303,275]
[null,"2015-01-10",155,141]
[null,"2015-01-11",172,160]
[null,"2015-01-12",344,329]
[null,"2015-01-13",342,308]
[null,"2015-01-14",310,281]
[null,"2015-01-15",590,423]
[null,"2015-01-16",391,322]
[null,"2015-01-17",473,391]
[null,"2015-01-18",400,337]
[null,"2015-01-19",698,555]
[null,"2015-01-20",395,348]
[null,"2015-01-21",413,321]
[null,"2015-01-22",258,242]
[null,"2015-01-23",720,589]
[null,"2015-01-24",545,279]
[null,"2015-01-25",377,273]
[null,"2015-01-26",405,301]
[null,"2015-01-27",425,370]
[null,"2015-01-28",237,199]
[null,"2015-01-29",378,303]
[null,"2015-01-30",304,262]
[null,"2015-01-31",0,0]
[null,"2015-02-01",338,251]
[null,"2015-02-02",452,389]
[null,"2015-02-03",383,287]
[null,{"$f":"B591+1","v":"2015-02-04"},279,256]
[null,"2015-02-05",311,263]
[null,"2015-02-06",463,330]
[null,"2015-02-07",199,169]
[null,"2015-02-08",194,179]
[null,"2015-02-09",473,348]
[null,"2015-02-10",508,366]
[null,"2015-02-11",362,289]
[null,"2015-02-12",281,223]
[null,"2015-02-13",290,264]
[null,"2015-02-14",178,169]
[null,"2015-02-15",193,169]
[null,"2015-02-16",372,321]
[null,"2015-02-17",370,312]
[null,"2015-02-18",322,277]
[null,"2015-02-19",627,523]
[null,"2015-02-20",961,740]
[null,"2015-02-21",797,417]
[null,"2015-02-22",400,287]
[null,"2015-02-23",412,365]
[null,"2015-02-24",417,367]
[null,"2015-02-25",310,270]
[null,"2015-02-26",411,351]
[null,"2015-02-27",335,278]
[null,"2015-02-28",257,224]
[null,"2015-03-01",182,154]
[null,"2015-03-02",396,320]
[null,"2015-03-03",265,219]
[null,"2015-03-04",278,237]
[null,"2015-03-05",845,592]
[null,"2015-03-06",403,340]
[null,"2015-03-07",234,193]
[null,"2015-03-08",219,211]
[null,"2015-03-09",364,324]
[null,"2015-03-10",328,233]
[null,"2015-03-11",480,373]
[null,"2015-03-12",269,246]
[null,"2015-03-13",269,248]
[null,"2015-03-14",245,223]
[null,"2015-03-15",165,155]
[null,"2015-03-16",274,235]
[null,"2015-03-17",250,225]
[null,"2015-03-18",278,252]
[null,"2015-03-19",289,260]
[null,"2015-03-20",336,295]
[null,"2015-03-21",744,490]
[null,"2015-03-22",395,302]
[null,"2015-03-23",410,366]
[null,"2015-03-24",287,227]
[null,"2015-03-25",309,285]
[null,"2015-03-26",408,335]
[null,"2015-03-27",289,237]
[null,"2015-03-28",221,189]
[null,"2015-03-29",184,154]
[null,"2015-03-30",407,271]
[null,"2015-03-31",285,241]
[null,"2015-04-01",354,322]
[null,"2015-04-02",302,260]
[null,"2015-04-03",173,151]
[null,"2015-04-04",177,157]
[null,"2015-04-05",113,105]
[null,"2015-04-06",148,133]
[null,"2015-04-07",333,283]
[null,"2015-04-08",223,188]
[null,{"$f":"B655+1","v":"2015-04-09"},212,170]
[null,"2015-04-10",260,239]
[null,"2015-04-11",191,175]
[null,"2015-04-12",177,169]
[null,"2015-04-13",123,108]
[null,"2015-04-14",246,204]
[null,"2015-04-15",213,180]
[null,"2015-04-16",269,235]
[null,"2015-04-17",234,215]
[null,"2015-04-18",198,174]
[null,"2015-04-19",141,126]
[null,"2015-04-20",325,286]
[null,"2015-04-21",409,282]
[null,"2015-04-22",217,180]
[null,"2015-04-23",223,196]
[null,"2015-04-24",196,177]
[null,"2015-04-25",133,118]
[null,"2015-04-26",249,180]
[null,"2015-04-27",203,124]
[null,"2015-04-28",186,90]
[null,"2015-04-29",272,172]
[null,"2015-04-30",252,187]
[null,"2015-05-01",0,0]
[null,"2015-05-02",593,239]
[null,"2015-05-03",142,136]
[null,"2015-05-04",352,165]
[null,"2015-05-05",302,204]
[null,"2015-05-06",244,166]
[null,"2015-05-07",259,144]
[null,"2015-05-08",190,121]
[null,"2015-05-09",147,115]
[null,"2015-05-10",94,92]
[null,"2015-05-11",232,165]
[null,"2015-05-12",202,132]
[null,"2015-05-13",171,134]
[null,"2015-05-14",232,118]
[null,"2015-05-15",187,101]
[null,"2015-05-16",134,117]
[null,"2015-05-17",95,85]
[null,"2015-05-18",235,135]
[null,"2015-05-19",193,131]
[null,"2015-05-20",188,111]
[null,"2015-05-21",209,145]
[null,"2015-05-22",325,289]
[null,"2015-05-23",222,195]
[null,"2015-05-24",96,88]
[null,"2015-05-25",258,247]
[null,"2015-05-26",247,215]
[null,"2015-05-27",241,231]
[null,"2015-05-28",237,226]
[null,"2015-05-29",176,166]
[null,"2015-05-30",239,147]
[null,"2015-05-31",100,97]
[null,"2015-06-01",244,227]
[null,"2015-06-02",276,228]
[null,"2015-06-03",281,243]
[null,"2015-06-04",279,226]
[null,"2015-06-05",285,242]
[null,"2015-06-06",193,173]
[null,"2015-06-07",108,97]
[null,"2015-06-08",139,118]
[null,"2015-06-09",266,249]
[null,"2015-06-10",253,229]
[null,"2015-06-11",363,327]
[null,{"$f":"B719+1","v":"2015-06-12"},225,210]
[null,"2015-06-13",180,147]
[null,"2015-06-14",109,103]
[null,"2015-06-15",247,242]
[null,"2015-06-16",245,235]
[null,"2015-06-17",331,315]
[null,"2015-06-18",263,250]
[null,"2015-06-19",210,197]
[null,"2015-06-20",149,134]
[null,"2015-06-21",113,97]
[null,"2015-06-22",232,221]
[null,"2015-06-23",258,220]
[null,"2015-06-24",226,223]
[null,"2015-06-25",232,224]
[null,"2015-06-26",245,238]
[null,"2015-06-27",190,163]
[null,"2015-06-28",125,116]
[null,"2015-06-29",275,267]
[null,"2015-06-30",206,194]
[null,"2015-07-01",229,225]
[null,"2015-07-02",207,195]
[null,"2015-07-03",231,197]
[null,"2015-07-04",138,133]
[null,"2015-07-05",97,92]
[null,"2015-07-06",189,189]
[null,"2015-07-07",188,184]
[null,"2015-07-08",212,205]
[null,"2015-07-09",209,208]
[null,"2015-07-10",192,187]
[null,"2015-07-11",150,144]
[null,"2015-07-12",228,196]
[null,"2015-07-13",350,334]
[null,"2015-07-14",286,271]
[null,"2015-07-15",337,280]
[null,"2015-07-16",308,282]
[null,"2015-07-17",617,592]
[null,"2015-07-18",251,186]
[null,"2015-07-19",156,128]
[null,"2015-07-20",311,300]
[null,"2015-07-21",240,232]
[null,"2015-07-22",231,216]
[null,"2015-07-23",298,292]
[null,"2015-07-24",212,202]
[null,"2015-07-25",163,152]
[null,"2015-07-26",160,140]
[null,"2015-07-27",205,201]
[null,"2015-07-28",297,266]
[null,"2015-07-29",212,207]
[null,"2015-07-30",220,210]
[null,"2015-07-31",182,169]
[null,"2015-08-01",147,137]
[null,"2015-08-02",111,101]
[null,"2015-08-03",204,199]
[null,"2015-08-04",172,166]
[null,"2015-08-05",158,153]
[null,"2015-08-06",163,160]
[null,"2015-08-07",222,211]
[null,"2015-08-08",121,106]
[null,"2015-08-09",99,95]
[null,"2015-08-10",176,175]
[null,"2015-08-11",181,176]
[null,"2015-08-12",297,289]
[null,"2015-08-13",238,225]
[null,"2015-08-14",133,127]
[null,{"$f":"B783+1","v":"2015-08-15"},204,178]
[null,"2015-08-16",92,92]
[null,"2015-08-17",198,186]
[null,"2015-08-18",168,158]
[null,"2015-08-19",184,173]
[null,"2015-08-20",194,179]
[null,"2015-08-21",160,149]
[null,"2015-08-22",135,131]
[null,"2015-08-23",86,82]
[null,"2015-08-24",183,178]
[null,"2015-08-25",212,204]
[null,"2015-08-26",140,138]
[null,"2015-08-27",147,141]
[null,"2015-08-28",206,204]
[null,"2015-08-29",164,137]
[null,"2015-08-30",161,135]
[null,"2015-08-31",250,245]
[null,"2015-09-01",163,159]
[null,"2015-09-02",181,170]
[null,"2015-09-03",336,317]
[null,"2015-09-04",225,211]
[null,"2015-09-05",113,111]
[null,"2015-09-06",86,85]
[null,"2015-09-07",196,195]
[null,"2015-09-08",238,224]
[null,"2015-09-09",205,196]
[null,"2015-09-10",174,170]
[null,"2015-09-11",253,243]
[null,"2015-09-12",356,277]
[null,"2015-09-13",140,129]
[null,"2015-09-14",178,169]
[null,"2015-09-15",163,155]
[null,"2015-09-16",217,206]
[null,"2015-09-17",238,212]
[null,"2015-09-18",233,221]
[null,"2015-09-19",149,140]
[null,"2015-09-20",67,66]
[null,"2015-09-21",236,224]
[null,"2015-09-22",219,210]
[null,"2015-09-23",195,186]
[null,"2015-09-24",127,124]
[null,"2015-09-25",159,152]
[null,"2015-09-26",148,135]
[null,"2015-09-27",223,199]
[null,"2015-09-28",245,240]
[null,"2015-09-29",348,313]
[null,"2015-09-30",229,220]
[null,"2015-10-01",200,188]
[null,"2015-10-02",194,186]
[null,"2015-10-03",132,123]
[null,"2015-10-04",123,123]
[null,"2015-10-05",122,114]
[null,"2015-10-06",226,224]
[null,"2015-10-07",182,169]
[null,"2015-10-08",271,264]
[null,"2015-10-09",195,190]
[null,"2015-10-10",141,125]
[null,"2015-10-11",75,67]
[null,"2015-10-12",201,195]
[null,"2015-10-13",227,221]
[null,"2015-10-14",380,370]
[null,"2015-10-15",161,159]
[null,"2015-10-16",175,159]
[null,"2015-10-17",155,151]
[null,{"$f":"B847+1","v":"2015-10-18"},96,85]
[null,"2015-10-19",193,193]
[null,"2015-10-20",174,155]
[null,"2015-10-21",179,170]
[null,"2015-10-22",490,436]
[null,"2015-10-23",236,228]
[null,"2015-10-24",154,148]
[null,"2015-10-25",68,66]
[null,"2015-10-26",250,244]
[null,"2015-10-27",461,434]
[null,"2015-10-28",371,353]
[null,"2015-10-29",245,233]
[null,"2015-10-30",205,204]
[null,"2015-10-31",166,141]
[null,"2015-11-01",147,140]
[null,"2015-11-02",225,212]
[null,"2015-11-03",250,231]
[null,"2015-11-04",314,301]
[null,"2015-11-05",281,263]
[null,"2015-11-06",357,312]
[null,"2015-11-07",418,323]
[null,"2015-11-08",242,209]
[null,"2015-11-09",310,293]
[null,"2015-11-10",251,245]
[null,"2015-11-11",159,158]
[null,"2015-11-12",179,175]
[null,"2015-11-13",173,166]
[null,"2015-11-14",469,375]
[null,"2015-11-15",200,172]
[null,"2015-11-16",217,212]
[null,"2015-11-17",267,255]
[null,"2015-11-18",209,198]
[null,"2015-11-19",227,222]
[null,"2015-11-20",245,234]
[null,"2015-11-21",278,243]
[null,"2015-11-22",129,114]
[null,"2015-11-23",402,361]
[null,"2015-11-24",272,270]
[null,"2015-11-25",328,298]
[null,"2015-11-26",234,219]
[null,"2015-11-27",247,237]
[null,"2015-11-28",154,144]
[null,"2015-11-29",0,0]
[null,"2015-11-30",688,584]
[null,"2015-12-01",376,346]
[null,"2015-12-02",240,232]
[null,"2015-12-03",323,304]
[null,"2015-12-04",239,223]
[null,"2015-12-05",131,115]
[null,"2015-12-06",107,100]
[null,"2015-12-07",236,220]
[null,"2015-12-08",214,186]
[null,"2015-12-09",281,261]
[null,"2015-12-10",0,0]
[null,"2015-12-11",809,714]
[null,"2015-12-12",243,205]
[null,"2015-12-13",205,185]
[null,"2015-12-14",235,231]
[null,"2015-12-15",231,225]
[null,"2015-12-16",266,244]
[null,"2015-12-17",234,222]
[null,"2015-12-18",199,193]
[null,"2015-12-19",152,135]
[null,"2015-12-20",90,87]
[null,{"$f":"B911+1","v":"2015-12-21"},303,281]
[null,"2015-12-22",179,177]
[null,"2015-12-23",224,217]
[null,"2015-12-24",273,256]
[null,"2015-12-25",89,85]
[null,"2015-12-26",102,101]
[null,"2015-12-27",171,171]
[null,"2015-12-28",140,130]
[null,"2015-12-29",150,148]
[null,"2015-12-30",196,191]
[null,"2015-12-31",128,126]
[null,"2016-01-01",123,115]
[null,"2016-01-02",124,120]
[null,"2016-01-03",128,122]
[null,"2016-01-04",264,262]
[null,"2016-01-05",307,284]
[null,"2016-01-06",278,262]
[null,"2016-01-07",224,204]
[null,"2016-01-08",195,187]
[null,"2016-01-09",124,106]
[null,"2016-01-10",131,125]
[null,"2016-01-11",221,198]
[null,"2016-01-12",307,276]
[null,"2016-01-13",194,186]
[null,"2016-01-14",289,273]
[null,"2016-01-15",270,249]
[null,"2016-01-16",248,194]
[null,"2016-01-17",136,121]
[null,"2016-01-18",218,214]
[null,"2016-01-19",235,230]
[null,"2016-01-20",259,242]
[null,"2016-01-21",189,187]
[null,"2016-01-22",276,264]
[null,"2016-01-23",317,254]
[null,"2016-01-24",174,157]
[null,"2016-01-25",235,227]
[null,"2016-01-26",168,144]
[null,"2016-01-27",203,193]
[null,"2016-01-28",300,278]
[null,"2016-01-29",938,849]
[null,"2016-01-30",614,481]
[null,"2016-01-31",411,333]
[null,"2016-02-01",618,476]
[null,"2016-02-02",571,411]
[null,"2016-02-03",411,369]
[null,"2016-02-04",368,354]
[null,"2016-02-05",285,275]
[null,"2016-02-06",226,204]
[null,"2016-02-07",119,116]
[null,"2016-02-08",285,269]
[null,"2016-02-09",319,293]
[null,"2016-02-10",282,261]
[null,"2016-02-11",185,171]
[null,"2016-02-12",207,190]
[null,"2016-02-13",188,152]
[null,"2016-02-14",126,120]
[null,"2016-02-15",271,251]
[null,"2016-02-16",275,252]
[null,"2016-02-17",264,237]
[null,"2016-02-18",302,273]
[null,"2016-02-19",288,261]
[null,"2016-02-20",270,226]
[null,"2016-02-21",147,140]
[null,"2016-02-22",214,199]
[null,{"$f":"B975+1","v":"2016-02-23"},395,317]
[null,"2016-02-24",277,237]
[null,"2016-02-25",231,209]
[null,"2016-02-26",247,238]
[null,"2016-02-27",179,165]
[null,"2016-02-28",132,124]
[null,"2016-02-29",233,224]
[null,"2016-03-01",312,280]
[null,"2016-03-02",334,301]
[null,"2016-03-03",294,279]
[null,"2016-03-04",256,242]
[null,"2016-03-05",144,134]
[null,"2016-03-06",135,122]
[null,"2016-03-07",238,225]
[null,"2016-03-08",216,204]
[null,"2016-03-09",226,207]
[null,"2016-03-10",246,213]
[null,"2016-03-11",272,241]
[null,"2016-03-12",193,151]
[null,"2016-03-13",206,195]
[null,"2016-03-14",254,246]
[null,"2016-03-15",206,196]
[null,"2016-03-16",201,189]
[null,"2016-03-17",261,250]
[null,"2016-03-18",270,236]
[null,"2016-03-19",326,272]
[null,"2016-03-20",146,141]
[null,"2016-03-21",257,246]
[null,"2016-03-22",205,187]
[null,"2016-03-23",191,176]
[null,"2016-03-24",275,255]
[null,"2016-03-25",143,138]
[null,"2016-03-26",145,133]
[null,"2016-03-27",123,115]
[null,"2016-03-28",126,114]
[null,"2016-03-29",219,198]
[null,"2016-03-30",233,184]
[null,"2016-03-31",152,139]
[null,"2016-04-01",202,174]
[null,"2016-04-02",137,129]
[null,"2016-04-03",101,95]
[null,"2016-04-04",167,156]
[null,"2016-04-05",237,216]
[null,"2016-04-06",183,178]
[null,"2016-04-07",160,159]
[null,"2016-04-08",170,166]
[null,"2016-04-09",114,111]
[null,"2016-04-10",82,79]
[null,"2016-04-11",199,193]
[null,"2016-04-12",214,187]
[null,"2016-04-13",207,183]
[null,"2016-04-14",187,168]
[null,"2016-04-15",174,162]
[null,"2016-04-16",126,112]
[null,"2016-04-17",86,83]
[null,"2016-04-18",175,162]
[null,"2016-04-19",182,173]
[null,"2016-04-20",255,249]
[null,"2016-04-21",121,108]
[null,"2016-04-22",178,163]
[null,"2016-04-23",144,137]
[null,"2016-04-24",128,123]
[null,"2016-04-25",118,112]
[null,"2016-04-26",257,248]
[null,{"$f":"B1039+1","v":"2016-04-27"},214,206]
[null,"2016-04-28",248,228]
[null,"2016-04-29",257,220]
[null,"2016-04-30",252,221]
[null,"2016-05-01",242,211]
[null,"2016-05-02",168,152]
[null,"2016-05-03",278,235]
[null,"2016-05-04",183,168]
[null,"2016-05-05",196,154]
[null,"2016-05-06",172,156]
[null,"2016-05-07",113,110]
[null,"2016-05-08",70,63]
[null,"2016-05-09",227,194]
[null,"2016-05-10",264,245]
[null,"2016-05-11",237,199]
[null,"2016-05-12",193,174]
[null,"2016-05-13",158,139]
[null,"2016-05-14",175,154]
[null,"2016-05-15",147,136]
[null,"2016-05-16",256,214]
[null,"2016-05-17",168,152]
[null,"2016-05-18",168,158]
[null,"2016-05-19",226,221]
[null,"2016-05-20",163,163]
[null,"2016-05-21",113,107]
[null,"2016-05-22",88,88]
[null,"2016-05-23",270,253]
[null,"2016-05-24",194,184]
[null,"2016-05-25",244,234]
[null,"2016-05-26",168,164]
[null,"2016-05-27",243,240]
[null,"2016-05-28",177,158]
[null,"2016-05-29",94,90]
[null,"2016-05-30",216,212]
[null,"2016-05-31",204,204]
[null,"2016-06-01",221,214]
[null,"2016-06-02",220,205]
[null,"2016-06-03",255,228]
[null,"2016-06-04",817,590]
[null,"2016-06-05",721,436]
[null,"2016-06-06",579,539]
[null,"2016-06-07",262,253]
[null,"2016-06-08",356,304]
[null,"2016-06-09",210,206]
[null,"2016-06-10",209,204]
[null,"2016-06-11",148,125]
[null,"2016-06-12",131,123]
[null,"2016-06-13",305,301]
[null,"2016-06-14",218,211]
[null,"2016-06-15",157,151]
[null,"2016-06-16",214,209]
[null,"2016-06-17",195,189]
[null,"2016-06-18",125,105]
[null,"2016-06-19",443,335]
[null,"2016-06-20",492,438]
[null,"2016-06-21",317,305]
[null,"2016-06-22",198,185]
[null,"2016-06-23",263,256]
[null,"2016-06-24",0,0]
[null,"2016-06-25",793,508]
[null,"2016-06-26",205,183]
[null,"2016-06-27",275,259]
[null,"2016-06-28",340,307]
[null,"2016-06-29",227,217]
[null,{"$f":"B1103+1","v":"2016-06-30"},244,235]
[null,"2016-07-01",202,199]
[null,"2016-07-02",119,106]
[null,"2016-07-03",119,113]
[null,"2016-07-04",252,239]
[null,"2016-07-05",261,244]
[null,"2016-07-06",290,262]
[null,"2016-07-07",289,270]
[null,"2016-07-08",215,211]
[null,"2016-07-09",138,125]
[null,"2016-07-10",111,94]
[null,"2016-07-11",214,209]
[null,"2016-07-12",198,191]
[null,"2016-07-13",204,192]
[null,"2016-07-14",177,169]
[null,"2016-07-15",187,178]
[null,"2016-07-16",186,157]
[null,"2016-07-17",115,106]
[null,"2016-07-18",193,186]
[null,"2016-07-19",223,219]
[null,"2016-07-20",177,174]
[null,"2016-07-21",175,165]
[null,"2016-07-22",213,206]
[null,"2016-07-23",188,165]
[null,"2016-07-24",90,78]
[null,"2016-07-25",216,206]
[null,"2016-07-26",214,207]
[null,"2016-07-27",169,153]
[null,"2016-07-28",192,187]
[null,"2016-07-29",195,182]
[null,"2016-07-30",144,136]
[null,"2016-07-31",93,93]
[null,"2016-08-01",196,190]
[null,"2016-08-02",175,164]
[null,"2016-08-03",274,235]
[null,"2016-08-04",322,304]
[null,"2016-08-05",203,194]
[null,"2016-08-06",142,111]
[null,"2016-08-07",108,107]
[null,"2016-08-08",160,156]
[null,"2016-08-09",179,170]
[null,"2016-08-10",166,151]
[null,"2016-08-11",181,158]
[null,"2016-08-12",177,161]
[null,"2016-08-13",112,107]
[null,"2016-08-14",154,132]
[null,"2016-08-15",245,231]
[null,"2016-08-16",190,179]
[null,"2016-08-17",161,154]
[null,"2016-08-18",219,191]
[null,"2016-08-19",178,166]
[null,"2016-08-20",108,96]
[null,"2016-08-21",96,92]
[null,"2016-08-22",220,210]
[null,"2016-08-23",202,186]
[null,"2016-08-24",248,227]
[null,"2016-08-25",269,209]
[null,"2016-08-26",222,192]
[null,"2016-08-27",118,106]
[null,"2016-08-28",104,102]
[null,"2016-08-29",204,194]
[null,"2016-08-30",190,186]
[null,"2016-08-31",207,195]
[null,"2016-09-01",275,261]
[null,{"$f":"B1167+1","v":"2016-09-02"},226,206]
[null,"2016-09-03",178,149]
[null,"2016-09-04",107,106]
[null,"2016-09-05",171,161]
[null,"2016-09-06",148,139]
[null,"2016-09-07",189,156]
[null,"2016-09-08",143,131]
[null,"2016-09-09",159,151]
[null,"2016-09-10",214,176]
[null,"2016-09-11",101,94]
[null,"2016-09-12",142,139]
[null,"2016-09-13",154,141]
[null,"2016-09-14",191,175]
[null,"2016-09-15",166,158]
[null,"2016-09-16",168,154]
[null,"2016-09-17",114,106]
[null,"2016-09-18",76,76]
[null,"2016-09-19",152,146]
[null,"2016-09-20",166,147]
[null,"2016-09-21",183,172]
[null,"2016-09-22",177,168]
[null,"2016-09-23",167,153]
[null,"2016-09-24",128,117]
[null,"2016-09-25",94,90]
[null,"2016-09-26",184,170]
[null,"2016-09-27",205,191]
[null,"2016-09-28",219,216]
[null,"2016-09-29",170,146]
[null,"2016-09-30",213,185]
[null,"2016-10-01",123,116]
[null,"2016-10-02",65,59]
[null,"2016-10-03",310,219]
[null,"2016-10-04",251,235]
[null,"2016-10-05",236,203]
[null,"2016-10-06",247,228]
[null,"2016-10-07",228,196]
[null,"2016-10-08",139,121]
[null,"2016-10-09",113,109]
[null,"2016-10-10",203,189]
[null,"2016-10-11",227,200]
[null,"2016-10-12",174,159]
[null,"2016-10-13",237,208]
[null,"2016-10-14",181,162]
[null,"2016-10-15",106,82]
[null,"2016-10-16",107,97]
[null,"2016-10-17",383,381]
[null,"2016-10-18",202,182]
[null,"2016-10-19",218,208]
[null,"2016-10-20",189,179]
[null,"2016-10-21",208,198]
[null,"2016-10-22",171,145]
[null,"2016-10-23",99,96]
[null,"2016-10-24",156,142]
[null,"2016-10-25",182,169]
[null,"2016-10-26",195,178]
[null,"2016-10-27",203,191]
[null,"2016-10-28",231,201]
[null,"2016-10-29",138,127]
[null,"2016-10-30",133,116]
[null,"2016-10-31",225,217]
[null,"2016-11-01",240,236]
[null,"2016-11-02",254,236]
[null,"2016-11-03",234,214]
[null,"2016-11-04",267,234]
[null,{"$f":"B1231+1","v":"2016-11-05"},244,213]
[null,"2016-11-06",120,109]
[null,"2016-11-07",238,216]
[null,"2016-11-08",371,360]
[null,"2016-11-09",337,312]
[null,"2016-11-10",357,305]
[null,"2016-11-11",284,265]
[null,"2016-11-12",0,0]
[null,"2016-11-13",0,0]
[null,"2016-11-14",527,453]
[null,"2016-11-15",347,321]
[null,"2016-11-16",210,202]
[null,"2016-11-17",259,234]
[null,"2016-11-18",179,157]
[null,"2016-11-19",131,120]
[null,"2016-11-20",90,89]
[null,"2016-11-21",194,169]
[null,"2016-11-22",214,195]
[null,"2016-11-23",204,187]
[null,"2016-11-24",366,311]
[null,"2016-11-25",195,174]
[null,"2016-11-26",206,154]
[null,"2016-11-27",115,109]
[null,"2016-11-28",194,180]
[null,"2016-11-29",223,211]
[null,"2016-11-30",646,588]
[null,"2016-12-01",529,452]
[null,"2016-12-02",382,324]
[null,"2016-12-03",0,0]
[null,"2016-12-04",783,641]
[null,"2016-12-05",367,311]
[null,"2016-12-06",705,600]
[null,"2016-12-07",670,547]
[null,"2016-12-08",454,398]
[null,"2016-12-09",308,283]
[null,"2016-12-10",172,161]
[null,"2016-12-11",145,143]
[null,"2016-12-12",307,297]
[null,"2016-12-13",340,297]
[null,"2016-12-14",306,282]
[null,"2016-12-15",254,241]
[null,"2016-12-16",190,177]
[null,"2016-12-17",197,175]
[null,"2016-12-18",0,0]
[null,"2016-12-19",378,327]
[null,"2016-12-20",328,286]
[null,"2016-12-21",399,363]
[null,"2016-12-22",312,267]
[null,"2016-12-23",189,170]
[null,"2016-12-24",133,127]
[null,"2016-12-25",175,133]
[null,"2016-12-26",177,145]
[null,"2016-12-27",163,134]
[null,"2016-12-28",280,249]
[null,"2016-12-29",172,155]
[null,"2016-12-30",266,250]
[null,"2016-12-31",181,164]
[null,"2017-01-01",182,174]
[null,"2017-01-02",266,218]
[null,"2017-01-03",381,330]
[null,"2017-01-04",284,266]
[null,"2017-01-05",210,194]
[null,"2017-01-06",317,273]
[null,"2017-01-07",195,177]
[null,{"$f":"B1295+1","v":"2017-01-08"},125,122]
[null,"2017-01-09",226,208]
[null,"2017-01-10",203,182]
[null,"2017-01-11",330,267]
[null,"2017-01-12",406,314]
[null,"2017-01-13",385,318]
[null,"2017-01-14",408,336]
[null,"2017-01-15",483,383]
[null,"2017-01-16",331,279]
[null,"2017-01-17",326,283]
[null,"2017-01-18",649,425]
[null,"2017-01-19",280,256]
[null,"2017-01-20",322,298]
[null,"2017-01-21",280,267]
[null,"2017-01-22",167,152]
[null,"2017-01-23",221,205]
[null,"2017-01-24",264,234]
[null,"2017-01-25",239,211]
[null,"2017-01-26",139,97]
[null,"2017-01-27",273,256]
[null,"2017-01-28",176,160]
[null,"2017-01-29",167,122]
[null,"2017-01-30",285,241]
[null,"2017-01-31",352,343]
[null,"2017-02-01",293,270]
[null,"2017-02-02",310,289]
[null,"2017-02-03",244,221]
[null,"2017-02-04",178,146]
[null,"2017-02-05",133,126]
[null,"2017-02-06",279,245]
[null,"2017-02-07",271,249]
[null,"2017-02-08",298,271]
[null,"2017-02-09",322,288]
[null,"2017-02-10",328,264]
[null,"2017-02-11",285,237]
[null,"2017-02-12",1394,492]
[null,"2017-02-13",0,0]
[null,"2017-02-14",406,365]
[null,"2017-02-15",265,243]
[null,"2017-02-16",236,207]
[null,"2017-02-17",266,208]
[null,"2017-02-18",252,211]
[null,"2017-02-19",277,253]
[null,"2017-02-20",267,251]
[null,"2017-02-21",342,307]
[null,"2017-02-22",227,214]
[null,"2017-02-23",244,226]
[null,"2017-02-24",222,198]
[null,"2017-02-25",128,117]
[null,"2017-02-26",112,105]
[null,"2017-02-27",264,246]
[null,"2017-02-28",252,224]
[null,"2017-03-01",332,297]
[null,"2017-03-02",313,250]
[null,"2017-03-03",236,191]
[null,"2017-03-04",195,171]
[null,"2017-03-05",122,116]
[null,"2017-03-06",222,207]
[null,"2017-03-07",197,177]
[null,"2017-03-08",168,157]
[null,"2017-03-09",201,196]
[null,"2017-03-10",163,155]
[null,"2017-03-11",148,142]
[null,"2017-03-12",116,114]
[null,{"$f":"B1359+1","v":"2017-03-13"},253,238]
[null,"2017-03-14",534,508]
[null,"2017-03-15",370,325]
[null,"2017-03-16",367,280]
[null,"2017-03-17",439,385]
[null,"2017-03-18",256,219]
[null,"2017-03-19",251,219]
[null,"2017-03-20",398,357]
[null,"2017-03-21",300,269]
[null,"2017-03-22",444,385]
[null,"2017-03-23",275,255]
[null,"2017-03-24",290,266]
[null,"2017-03-25",204,160]
[null,"2017-03-26",147,137]
[null,"2017-03-27",279,250]
[null,"2017-03-28",195,186]
[null,"2017-03-29",400,314]
[null,"2017-03-30",0,0]
[null,"2017-03-31",0,0]
[null,"2017-04-01",0,0]
[null,"2017-04-02",731,619]
[null,"2017-04-03",645,566]
[null,"2017-04-04",442,357]
[null,"2017-04-05",338,297]
[null,"2017-04-06",268,239]
[null,"2017-04-07",235,201]
[null,"2017-04-08",141,127]
[null,"2017-04-09",149,146]
[null,"2017-04-10",333,311]
[null,"2017-04-11",252,235]
[null,"2017-04-12",233,217]
[null,"2017-04-13",236,225]
[null,"2017-04-14",135,120]
[null,"2017-04-15",94,90]
[null,"2017-04-16",119,118]
[null,"2017-04-17",84,83]
[null,"2017-04-18",278,210]
[null,"2017-04-19",225,211]
[null,"2017-04-20",295,243]
[null,"2017-04-21",193,182]
[null,"2017-04-22",120,113]
[null,"2017-04-23",130,109]
[null,"2017-04-24",154,135]
[null,"2017-04-25",94,92]
[null,"2017-04-26",245,227]
[null,"2017-04-27",205,197]
[null,"2017-04-28",172,157]
[null,"2017-04-29",118,110]
[null,"2017-04-30",97,94]
[null,"2017-05-01",115,113]
[null,"2017-05-02",237,220]
[null,"2017-05-03",217,203]
[null,"2017-05-04",191,176]
[null,"2017-05-05",170,143]
[null,"2017-05-06",140,124]
[null,"2017-05-07",81,79]
[null,"2017-05-08",267,233]
[null,"2017-05-09",274,253]
[null,"2017-05-10",201,195]
[null,"2017-05-11",173,155]
[null,"2017-05-12",142,131]
[null,"2017-05-13",129,114]
[null,"2017-05-14",80,73]
[null,"2017-05-15",281,246]
[null,{"$f":"B1423+1","v":"2017-05-16"},211,198]
[null,"2017-05-17",188,173]
[null,"2017-05-18",192,180]
[null,"2017-05-19",188,160]
[null,"2017-05-20",127,114]
[null,"2017-05-21",136,128]
[null,"2017-05-22",236,223]
[null,"2017-05-23",280,234]
[null,"2017-05-24",197,183]
[null,"2017-05-25",210,197]
[null,"2017-05-26",204,179]
[null,"2017-05-27",121,114]
[null,"2017-05-28",105,96]
[null,"2017-05-29",211,198]
[null,"2017-05-30",199,184]
[null,"2017-05-31",191,187]
[null,"2017-06-01",305,270]
[null,"2017-06-02",194,185]
[null,"2017-06-03",142,130]
[null,"2017-06-04",92,89]
[null,"2017-06-05",251,216]
[null,"2017-06-06",191,178]
[null,"2017-06-07",207,193]
[null,"2017-06-08",199,176]
[null,"2017-06-09",185,170]
[null,"2017-06-10",167,163]
[null,"2017-06-11",156,153]
[null,"2017-06-12",241,204]
[null,"2017-06-13",386,304]
[null,"2017-06-14",310,251]
[null,"2017-06-15",417,266]
[null,"2017-06-16",347,269]
[null,"2017-06-17",221,176]
[null,"2017-06-18",193,125]
[null,"2017-06-19",249,213]
[null,"2017-06-20",216,203]
[null,"2017-06-21",201,165]
[null,"2017-06-22",199,184]
[null,"2017-06-23",182,147]
[null,"2017-06-24",115,106]
[null,"2017-06-25",75,74]
[null,"2017-06-26",225,209]
[null,"2017-06-27",197,188]
[null,"2017-06-28",196,188]
[null,"2017-06-29",239,228]
[null,"2017-06-30",198,184]
[null,"2017-07-01",148,126]
[null,"2017-07-02",123,115]
[null,"2017-07-03",211,204]
[null,"2017-07-04",236,224]
[null,"2017-07-05",170,157]
[null,"2017-07-06",271,233]
[null,"2017-07-07",161,147]
[null,"2017-07-08",151,137]
[null,"2017-07-09",104,98]
[null,"2017-07-10",176,160]
[null,"2017-07-11",179,162]
[null,"2017-07-12",223,183]
[null,"2017-07-13",178,164]
[null,"2017-07-14",235,214]
[null,"2017-07-15",149,134]
[null,"2017-07-16",123,119]
[null,"2017-07-17",192,181]
[null,"2017-07-18",190,164]
[null,{"$f":"B1487+1","v":"2017-07-19"},460,350]
[null,"2017-07-20",264,235]
[null,"2017-07-21",211,187]
[null,"2017-07-22",192,168]
[null,"2017-07-23",121,114]
[null,"2017-07-24",256,222]
[null,"2017-07-25",264,258]
[null,"2017-07-26",229,223]
[null,"2017-07-27",215,214]
[null,"2017-07-28",196,192]
[null,"2017-07-29",139,124]
[null,"2017-07-30",104,98]
[null,"2017-07-31",274,241]
[null,"2017-08-01",150,144]
[null,"2017-08-02",280,266]
[null,"2017-08-03",212,192]
[null,"2017-08-04",190,179]
[null,"2017-08-05",123,101]
[null,"2017-08-06",107,103]
[null,"2017-08-07",226,222]
[null,"2017-08-08",188,181]
[null,"2017-08-09",178,163]
[null,"2017-08-10",241,200]
[null,"2017-08-11",179,161]
[null,"2017-08-12",108,98]
[null,"2017-08-13",114,101]
[null,"2017-08-14",227,200]
[null,"2017-08-15",192,179]
[null,"2017-08-16",218,206]
[null,"2017-08-17",235,195]
[null,"2017-08-18",201,171]
[null,"2017-08-19",210,177]
[null,"2017-08-20",137,131]
[null,"2017-08-21",181,178]
[null,"2017-08-22",229,215]
[null,"2017-08-23",189,180]
[null,"2017-08-24",249,217]
[null,"2017-08-25",185,173]
[null,"2017-08-26",105,97]
[null,"2017-08-27",86,86]
[null,"2017-08-28",211,203]
[null,"2017-08-29",187,166]
[null,"2017-08-30",216,202]
[null,"2017-08-31",209,191]
[null,"2017-09-01",169,156]
[null,"2017-09-02",80,75]
[null,"2017-09-03",113,112]
[null,"2017-09-04",191,186]
[null,"2017-09-05",214,197]
[null,"2017-09-06",177,158]
[null,"2017-09-07",207,194]
[null,"2017-09-08",178,158]
[null,"2017-09-09",119,107]
[null,"2017-09-10",87,86]
[null,"2017-09-11",200,173]
[null,"2017-09-12",204,183]
[null,"2017-09-13",180,154]
[null,"2017-09-14",480,397]
[null,"2017-09-15",145,138]
[null,"2017-09-16",158,143]
[null,"2017-09-17",84,83]
[null,"2017-09-18",215,205]
[null,"2017-09-19",160,155]
[null,"2017-09-20",201,189]
[null,{"$f":"B1551+1","v":"2017-09-21"},210,192]
[null,"2017-09-22",439,365]
[null,"2017-09-23",304,203]
[null,"2017-09-24",145,123]
[null,"2017-09-25",255,237]
[null,"2017-09-26",234,228]
[null,"2017-09-27",240,223]
[null,"2017-09-28",268,243]
[null,"2017-09-29",315,278]
[null,"2017-09-30",151,140]
[null,"2017-10-01",246,225]
[null,"2017-10-02",334,268]
[null,"2017-10-03",329,279]
[null,"2017-10-04",246,222]
[null,"2017-10-05",248,213]
[null,"2017-10-06",359,330]
[null,"2017-10-07",153,138]
[null,"2017-10-08",77,72]
[null,"2017-10-09",212,186]
[null,"2017-10-10",245,204]
[null,"2017-10-11",231,210]
[null,"2017-10-12",244,229]
[null,"2017-10-13",284,252]
[null,"2017-10-14",195,178]
[null,"2017-10-15",278,254]
[null,"2017-10-16",450,396]
[null,"2017-10-17",351,310]
[null,"2017-10-18",346,311]
[null,"2017-10-19",263,225]
[null,"2017-10-20",221,190]
[null,"2017-10-21",172,160]
[null,"2017-10-22",120,118]
[null,"2017-10-23",342,287]
[null,"2017-10-24",786,469]
[null,"2017-10-25",242,209]
[null,"2017-10-26",405,377]
[null,"2017-10-27",332,289]
[null,"2017-10-28",119,98]
[null,"2017-10-29",350,233]
[null,"2017-10-30",502,395]
[null,"2017-10-31",296,253]
[null,"2017-11-01",208,188]
[null,"2017-11-02",204,164]
[null,"2017-11-03",204,166]
[null,"2017-11-04",165,147]
[null,"2017-11-05",109,101]
[null,"2017-11-06",289,254]
[null,"2017-11-07",427,339]
[null,"2017-11-08",275,213]
[null,"2017-11-09",248,210]
[null,"2017-11-10",172,150]
[null,"2017-11-11",129,118]
[null,"2017-11-12",125,119]
[null,"2017-11-13",201,170]
[null,"2017-11-14",212,190]
[null,"2017-11-15",248,236]
[null,"2017-11-16",159,153]
[null,"2017-11-17",213,203]
[null,"2017-11-18",197,172]
[null,"2017-11-19",114,112]
[null,"2017-11-20",220,203]
[null,"2017-11-21",213,199]
[null,"2017-11-22",249,240]
[null,"2017-11-23",211,193]
[null,{"$f":"B1615+1","v":"2017-11-24"},201,168]
[null,"2017-11-25",137,127]
[null,"2017-11-26",106,96]
[null,"2017-11-27",203,178]
[null,"2017-11-28",169,159]
[null,"2017-11-29",248,220]
[null,"2017-11-30",243,223]
[null,"2017-12-01",196,188]
[null,"2017-12-02",156,143]
[null,"2017-12-03",247,201]
[null,"2017-12-04",342,295]
[null,"2017-12-05",279,231]
[null,"2017-12-06",183,155]
[null,"2017-12-07",269,232]
[null,"2017-12-08",308,266]
[null,"2017-12-09",0,0]
[null,"2017-12-10",526,422]
[null,"2017-12-11",280,251]
[null,"2017-12-12",194,183]
[null,"2017-12-13",256,209]
[null,"2017-12-14",283,250]
[null,"2017-12-15",191,180]
[null,"2017-12-16",134,123]
[null,"2017-12-17",129,123]
[null,"2017-12-18",196,187]
[null,"2017-12-19",329,261]
[null,"2017-12-20",282,256]
[null,"2017-12-21",268,231]
[null,"2017-12-22",300,260]
[null,"2017-12-23",207,169]
[null,"2017-12-24",179,131]
[null,"2017-12-25",0,0]
[null,"2017-12-26",505,317]
[null,"2017-12-27",238,217]
[null,"2017-12-28",241,184]
[null,"2017-12-29",195,184]
[null,"2017-12-30",173,158]
[null,"2017-12-31",534,477]
[null,"2018-01-01",375,336]
[null,"2018-01-02",538,420]
[null,"2018-01-03",405,338]
[null,"2018-01-04",342,298]
[null,"2018-01-05",231,214]
[null,"2018-01-06",186,167]
[null,"2018-01-07",164,151]
[null,"2018-01-08",269,222]
[null,"2018-01-09",279,270]
[null,"2018-01-10",349,327]
[null,"2018-01-11",261,255]
[null,"2018-01-12",228,210]
[null,"2018-01-13",437,268]
[null,"2018-01-14",593,374]
[null,"2018-01-15",327,276]
[null,"2018-01-16",246,211]
[null,"2018-01-17",247,212]
[null,"2018-01-18",251,234]
[null,"2018-01-19",234,209]
[null,"2018-01-20",204,173]
[null,"2018-01-21",185,168]
[null,"2018-01-22",236,224]
[null,"2018-01-23",270,258]
[null,"2018-01-24",296,278]
[null,"2018-01-25",315,299]
[null,"2018-01-26",173,154]
[null,{"$f":"B1679+1","v":"2018-01-27"},206,173]
[null,"2018-01-28",164,148]
[null,"2018-01-29",312,293]
[null,"2018-01-30",198,184]
[null,"2018-01-31",283,258]
[null,"2018-02-01",265,232]
[null,"2018-02-02",261,241]
[null,"2018-02-03",252,214]
[null,"2018-02-04",146,130]
[null,"2018-02-05",241,225]
[null,"2018-02-06",294,250]
[null,"2018-02-07",266,241]
[null,"2018-02-08",214,194]
[null,"2018-02-09",219,196]
[null,"2018-02-10",185,170]
[null,"2018-02-11",0,0]
[null,"2018-02-12",0,0]
[null,"2018-02-13",990,854]
[null,"2018-02-14",824,508]
[null,"2018-02-15",765,606]
[null,"2018-02-16",0,0]
[null,"2018-02-17",605,386]
[null,"2018-02-18",258,222]
[null,"2018-02-19",351,313]
[null,"2018-02-20",320,295]
[null,"2018-02-21",382,332]
[null,"2018-02-22",294,272]
[null,"2018-02-23",534,394]
[null,"2018-02-24",412,295]
[null,"2018-02-25",313,249]
[null,"2018-02-26",625,517]
[null,"2018-02-27",462,414]
[null,"2018-02-28",298,277]
[null,"2018-03-01",339,293]
[null,"2018-03-02",278,269]
[null,"2018-03-03",148,144]
[null,"2018-03-04",226,216]
[null,"2018-03-05",302,257]
[null,"2018-03-06",308,277]
[null,"2018-03-07",466,409]
[null,"2018-03-08",285,275]
[null,"2018-03-09",354,320]
[null,"2018-03-10",283,234]
[null,"2018-03-11",157,148]
[null,"2018-03-12",243,222]
[null,"2018-03-13",293,259]
[null,"2018-03-14",370,339]
[null,"2018-03-15",207,205]
[null,"2018-03-16",229,205]
[null,"2018-03-17",157,137]
[null,"2018-03-18",167,156]
[null,"2018-03-19",293,272]
[null,"2018-03-20",280,253]
[null,"2018-03-21",355,321]
[null,"2018-03-22",218,207]
[null,"2018-03-23",202,196]
[null,"2018-03-24",166,143]
[null,"2018-03-25",110,107]
[null,"2018-03-26",266,238]
[null,"2018-03-27",325,278]
[null,"2018-03-28",242,215]
[null,"2018-03-29",201,177]
[null,"2018-03-30",126,118]
[null,"2018-03-31",154,146]
[null,{"$f":"B1743+1","v":"2018-04-01"},108,101]
[null,"2018-04-02",99,96]
[null,"2018-04-03",255,230]
[null,"2018-04-04",241,238]
[null,"2018-04-05",219,196]
[null,"2018-04-06",190,176]
[null,"2018-04-07",157,150]
[null,"2018-04-08",104,99]
[null,"2018-04-09",224,199]
[null,"2018-04-10",211,198]
[null,"2018-04-11",346,326]
[null,"2018-04-12",223,189]
[null,"2018-04-13",252,218]
[null,"2018-04-14",139,129]
[null,"2018-04-15",114,111]
[null,"2018-04-16",217,211]
[null,"2018-04-17",258,240]
[null,"2018-04-18",229,207]
[null,"2018-04-19",183,169]
[null,"2018-04-20",273,255]
[null,"2018-04-21",208,172]
[null,"2018-04-22",110,108]
[null,"2018-04-23",229,204]
[null,"2018-04-24",195,186]
[null,"2018-04-25",78,77]
[null,"2018-04-26",192,171]
[null,"2018-04-27",188,180]
[null,"2018-04-28",96,90]
[null,"2018-04-29",88,80]
[null,"2018-04-30",226,215]
[null,"2018-05-01",225,204]
[null,"2018-05-02",227,215]
[null,"2018-05-03",189,183]
[null,"2018-05-04",207,193]
[null,"2018-05-05",196,164]
[null,"2018-05-06",72,70]
[null,"2018-05-07",115,111]
[null,"2018-05-08",247,224]
[null,"2018-05-09",210,205]
[null,"2018-05-10",183,176]
[null,"2018-05-11",210,202]
[null,"2018-05-12",133,107]
[null,"2018-05-13",116,112]
[null,"2018-05-14",192,177]
[null,"2018-05-15",187,184]
[null,"2018-05-16",195,194]
[null,"2018-05-17",258,235]
[null,"2018-05-18",288,269]
[null,"2018-05-19",170,127]
[null,"2018-05-20",73,73]
[null,"2018-05-21",214,198]
[null,"2018-05-22",200,198]
[null,"2018-05-23",192,186]
[null,"2018-05-24",177,171]
[null,"2018-05-25",175,172]
[null,"2018-05-26",170,141]
[null,"2018-05-27",113,105]
[null,"2018-05-28",211,197]
[null,"2018-05-29",185,149]
[null,"2018-05-30",183,176]
[null,"2018-05-31",211,184]
[null,"2018-06-01",177,169]
[null,"2018-06-02",136,123]
[null,"2018-06-03",89,90]
[null,{"$f":"B1807+1","v":"2018-06-04"},221,208]
[null,"2018-06-05",193,179]
[null,"2018-06-06",195,183]
[null,"2018-06-07",197,189]
[null,"2018-06-08",210,204]
[null,"2018-06-09",115,100]
[null,"2018-06-10",114,105]
[null,"2018-06-11",180,171]
[null,"2018-06-12",209,204]
[null,"2018-06-13",203,200]
[null,"2018-06-14",247,235]
[null,"2018-06-15",197,188]
[null,"2018-06-16",131,115]
[null,"2018-06-17",353,155]
[null,"2018-06-18",241,207]
[null,"2018-06-19",202,193]
[null,"2018-06-20",207,182]
[null,"2018-06-21",249,235]
[null,"2018-06-22",214,208]
[null,"2018-06-23",149,127]
[null,"2018-06-24",110,104]
[null,"2018-06-25",246,228]
[null,"2018-06-26",197,195]
[null,"2018-06-27",222,213]
[null,"2018-06-28",294,267]
[null,"2018-06-29",195,164]
[null,"2018-06-30",148,131]

{"sheet":"6.2 Reliability & Cust serv","index":31,"n_rows":71,"n_cols":9,"rows_kept":71,"cut":false,"hidden":false,"merged":[[28,4,28,8],[40,4,40,8],[66,4,66,8],[24,1,24,3],[36,1,36,3],[48,1,48,3],[5,1,5,7],[63,1,63,8],[51,1,51,8],[54,2,54,8],[12,1,12,7],[13,1,13,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[7,1,7,7],[16,4,16,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"Instructions"]
[null,"This regulatory template requires the input of performance Historicals and proposed targets for the forthcoming regulatory control period under the STPIS."]
[null,{"$f":"CONCATENATE(\"Performance targets for some parameters may cross feeder classifications in tables 6.2.1, 6.2.2 and 6.2.3. However, where a single target for the whole network is prescribed, this should be entered in the \"\"whole network (system)\"\" cell. \",dms_TradingName,\" must define each of the parameters which apply to it. If common definitions exist for the parameter, please attach a reference to the definition.\")","v":"Performance targets for some parameters may cross feeder classifications in tables 6.2.1, 6.2.2 and 6.2.3. However, where a single target for the whole network is prescribed, this should be entered in the \"whole network (system)\" cell. Energex must define each of the parameters which apply to it. If common definitions exist for the parameter, please attach a reference to the definition."}]
[null,{"$f":"CONCATENATE(dms_TradingName,\" should insert \"\"n/a\"\" against parameters which do not apply to it. Do not delete inapplicable fields.\")","v":"Energex should insert \"n/a\" against parameters which do not apply to it. Do not delete inapplicable fields."}]
[null,{"$f":"CONCATENATE(\"If parts of this template are unsuitable to record any of the requested information \",dms_TradingName,\" must provide this information in an alternative format, within it's accompanying regulatory proposal and indicate the section of the regulatory proposal containing the information in the 'addressed at chapter/section of regulatory proposal' column.\")","v":"If parts of this template are unsuitable to record any of the requested information Energex must provide this information in an alternative format, within it's accompanying regulatory proposal and indicate the section of the regulatory proposal containing the information in the 'addressed at chapter/section of regulatory proposal' column."}]
[null,{"$f":"CONCATENATE(dms_TradingName,\" must provide detail of historical unplanned minutes off supply, unplanned interruptions, momentary interruptions, customer numbers \"&\"and customer service in accordance with tables 6.2.1, 6.2.2, 6.2.4 and 6.2.5. \"&\"Table 6.2.3 is not compulsory - those businesses who want to \"&\" include MAIFI in the s-factor calcuation may make such a proposal and submit the relevant MAIFI information \"&\"necessary to establish the MAIFI targets, including the estimated performance for \",CRCP_y4)","v":"Energex must provide detail of historical unplanned minutes off supply, unplanned interruptions, momentary interruptions, customer numbers and customer service in accordance with tables 6.2.1, 6.2.2, 6.2.4 and 6.2.5. Table 6.2.3 is not compulsory - those businesses who want to  include MAIFI in the s-factor calcuation may make such a proposal and submit the relevant MAIFI information necessary to establish the MAIFI targets, including the estimated performance for 2018-19"}]
[null,"Definitions of parameters under the AER's STPIS apply. Where exclusions apply, data provided below must exclude all events outlined under clause 3.3 of the AER's STPIS."]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,2.4,2.4,2.4,2.4,2.4]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,60.118000000000002,60.118000000000002,60.118000000000002,60.118000000000002,60.118000000000002]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,136.29,136.29,136.29,136.29,136.29]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,4.2700000000000002E-2,4.2700000000000002E-2,4.2700000000000002E-2,4.2700000000000002E-2,4.2700000000000002E-2]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.72199999999999998,0.72199999999999998,0.72199999999999998,0.72199999999999998,0.72199999999999998]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1.466,1.466,1.466,1.466,1.466]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E44:E48)","v":0},{"$f":"SUM(F44:F48)","v":0},{"$f":"SUM(G44:G48)","v":0},{"$f":"SUM(H44:H48)","v":0},{"$f":"SUM(I44:I48)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},3912,3955,3999,4042,4086,4129,4172]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1039152,1048062,1056973,1065883,1074794,1083704,1092615]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},433260,448665,464070,479476,494881,510187,525692]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C57:C61)","v":1476324},1500682,1525042,1549401,1573761,1598020,1622479]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Number of calls received",null,null,118746,118746,118746,118746,118746]
[null,"Number of calls answered within 30 seconds",null,null,102122,102122,102122,102122,102122]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E70/E69),\"\")","v":0.860003705387971},0.860003705387971,0.860003705387971,0.860003705387971,0.860003705387971]

{"sheet":"7.1  Policies and Procedures","index":32,"n_rows":219,"n_cols":5,"rows_kept":219,"cut":false,"hidden":false,"merged":[[6,1,6,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"Instructions"]
[null,"List and provide a brief description of key internal plans, policies, procedures or strategies that are used to plan and conduct day to day operations and that have been relied upon in the development of the regulatory proposal. Identify any internal plans, policies, procedures and strategies that have changed in the current regulatory control period or that are expected to change before the next regulatory control period where the change has been identified as a step change."]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"Corporate Strategy","It outlines EQL’s vision of Energising Queensland Communities. It also articulates our strategic objectives and measures","All","No"]
[]
[]
[null,"Governance framework"]
[null,"EQL Statement of Corporate Intent (public version)","It outlines the critical business objectives, key priorities, major initiatives, and financial and non-financial\nperformance measures for Energy Queensland","All","No"]
[null,"EQL qualitative risk appetite statement","This Risk (Threat and Opportunity) Appetite Statement (RAS) considers the most significant risks to which EQL is exposed and provides an outline of the approach to managing these risks.  Risk appetite is the amount and type of risk that an organisation is willing to pursue or retain.\nAll business planning and operational decisions must be consistent with this Risk Appetite Statement.","All","No"]
[null,"EQL Risk evaluation matrix","This matrix is a tool used for ranking risks.","All","No"]
[null,"EQL Risk management standard","The purpose of this Standard is to articulate Energy Queensland’s (EQL) whole-of-business risk management principles and framework.  It forms part of the risk management architecture ","All","No"]
[null,"Risk management and organisational resilience policy","The purpose of this Policy is to define the whole of business portfolio-wide principles-based approach to Risk Management (RM) and Organisational Resilience (OR) through the utilisation of an integrated framework to enable EQL to provide a structured approach to consistently delivering against risk management and organisational resilience objectives and strategies established by the EQL Group.","All","No"]
[null,"Network Risk Framework","The purpose of this Network Risk Framework is to supplement the Enterprise Risk Management Standard by providing additional guidance when undertaking specialised / technical risk assessments.","All","No"]
[null,"EQL Our Customer Strategy","The customer strategy provides the framework and tools to manage the customer experience and enable customer-focused decision making to deliver on our goals.","All","No"]
[null,"EQL Our Community Strategy","The Community Strategy focuses the business where customercommunity- business value intersects.\nDelivering here and profiling our efforts is essential to strengthening the community-orientation seen in the corporate strategy as key to our sustainable competitive advantage.","All","No"]
[null,"Connection policy","It provides an outline of our connection services, when connection charges may be payable by customers and how those charges are calculated.","All","No"]
[null,"Energy Queensland Union Collection Agreement","This Agreement replaces the Ergon Energy Union Collective Agreement 2015; the Energex Union Collective Agreement 2015; and the SPARQ Solut ions Union Collective Agreement 2016.\nThis agreement operates from 25 December 2017 and will nominally expire on 1 March 2021.","All","No"]
[null,"EQL Governance and delegations policy P013","This Policy sets out the overarching decision making governance and delegation of authority framework for Energy Queensland Limited (EQL) and its subsidiaries.","All","No"]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Service classification","It outlines the AER's assessment of our services (service classification).","All","No"]
[null,"Capitalisation Policy","This manual is designed to interpret the Accounting standard guidelines AASB 116 Property Plant and Equipment and AASB 138 Intangible Assets and provide guidance for employees on the application of those standards in practice.","Capex","No"]
[null,"Note: As agreed with the AER on 29 November 2018, additional accounting policies unable to be inserted into this template have been included on the sheet called \"Extra info 7.1 7.3\""]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Policy","The purpose of this policy is to set out Energy Queensland's principles by which it intends to apply asset management to achieve its organisational objectives.","ALL","No"]
[]
[null,"Asset Management Strategies"]
[null,"Corporate Fleet Management Strategy","The Fleet Asset Management Strategy identifies the key strategic initiatives for the Fleet and Equipment Strategy Team in supporting Energy Queensland to achieve its Corporate Strategy to “safely deliver secure, affordable and sustainablity\"","Non-Network Capex / Opex","No"]
[null,"Corporate Tools and Equipment Strategy","The Equipment Asset Management Strategy identifies the key strategic initiatives which support Energy Queensland to support Energy Queensland to achieve its Corporate Strategy to “safely deliver secure, affordable and sustainablity\"","Non-Network Capex / Opex","No"]
[null,"Corporate Property Strategy","This document outlines Energex's baseline and provides direction on the delivery of property services to deliver a safe and efficient, fit–for-purpose and customer centric property portfolio. It is aimed at ensuring to ensure that we have the right depots and facilities in the right locations to enable the efficient operation of the State-wide network. ","Non-Network Capex / Opex","No"]
[null,"Note: As agreed with the AER on 29 November 2018, additional asset management strategies unable to be inserted into this template have been included on the sheet called \"Extra info 7.1 7.3\""]
[null,"Asset Management Plans"]
[null,"Distribution Annual Planning Report (DAPR) Energex","The DAPR covers a five year period and outlines our strategies and plans. In particular, it includes:\n•Planning for subtransmission and distribution network growth\n•Asset repair and replacement planning\n•Planning for future demand on the network\n•Capacity and load forecasts by region\n•Current and future limitations on our subtransmission and distribution networks\n•Possible solutions for network limitations.","Energex Initiated Augex (Capex)","No"]
[null,"Public Lighting Asset Management Plan 2020-2025","This document presents EQL’s Asset Management Plan for public lighting.","ACS"]
[null,"Metering Asset Management Plan 2020-2025","This AMP outlines the treatment of assets for the Asset Class of Metering. This includes meters for revenue purposes to meet compliance and regulatory obligations, as well as non-revenue metering for power quality and statistical purposes. The document provides an overview of the metering equipment, asset condition, maintenance approach and activities, as well as planned replacements. ","ACS","No"]
[null,"Asset Management Plan - Ring Main Units","This document outlines the current practices and strategies for Ring Main Units managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Instrument Transformers","This document outlines the current practices and strategies for the class of instrument transformers, including current transformers, voltage transformers and capacitor voltage transformers managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Overhead conductors","This document outlines the current practices and strategies for overhead conductor and accessories managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Substation DC supply","This document outlines the current practices and strategies for the class of assets used to deliver DC electrical services to devices within substations and on distribution assets including recloser, sectionaliser devices, battery banks and their associated AC chargers managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Underground cables","This document outlines the current practices and strategies for underground cable and accessories managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Switches","This document outlines the current practices and strategies for the class of switches at voltage level of11kV and above (including air break switches, load break switches, isolators, earth switches, disconnect links, sectionaliser and load transfer switches) managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Distribution Transformers","This document outlines the current practices and strategies for the class of assets of covering distribution transformers, regulators and reactors, substation earthing transformers and substation service transformers managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Circuit Breakers","This document outlines the current practices and strategies for >=11kV circuit breakers and reclosers managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Substation Power Transformers","This document outlines the current practices and strategies for the class of assets known as substation power transformers managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - LV services","This document outlines the current practices and strategies for the class of assets known as Services (including cross-linked polyethylene services, polyvinyl chloride flat services, PVC aluminium services, neutral screened services and open wire services) managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Poles","This document outlines the current practices and strategies for poles and lattice towers managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Pole Top Structures","This document outlines the current practices and strategies for pole top structures managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Telecommunications","This document outlines the current practices and strategies for telecommunication equipment and infrastructure managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - AFLC","This document outlines the current practices and strategies for Audio Frequency Load Control (AFLC) units [which are comprised of components such as Local Controllers, Motor Generator or Static Frequency Units (SFU) and Coupling Cells] managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Protection Relays","This document outlines the current practices and strategies for protection relays managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Control Systems","This document outlines the current practices and strategies for the class of assets known as Control Systems (which includes remote terminal units, data concentrators, intelligent electronic devices, human machine interfaces, control boards for field based switch equipment, distribution system SCADA (DSS) radios, readio repeaters and modems for field based switch equipment) managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - Linear communications (pilot & fibre)","This document outlines the current practices and strategies for the class of assets known as “Communications Linear Assets” [which are made up of Fibre optic and Metallic pilot cable connecting substation sites, dedicated communications sites, Control Centre locations, office locations and depot facilities] managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Asset Management Plan - OTE","This document outlines the current practices and strategies for the class of assets known as Operational Technology Equipment (OTE)” [which consists of networking devices that directly support the deployment of critical information technology solutions within a secure network environment including routers, switches, gateways and firewalls, along with software solutions which operate and add additional security layers to this hardware] managed by EQL, recognising and annotating the differences that have arisen due to legacy organisation management. These variations are expected to diminish over time with integration of engineering and asset management practices.","All CAPEX /' All OPEX","No"]
[null,"Strategic Asset Management Plan (SAMP)","The Strategic Asset Management Plan (SAMP) sets out how we will apply the principles stated in our Asset Management Policy to fulfil Energy Queensland’s (EQL’s)Strategic Objectives. It provides direction for asset management activities and form the basis for developing the more specific asset management strategies and plans.\nIt also describes the asset management system, which conceptualises the integration and\ninterrelationship between asset management activities that is necessary to optimise the value\nfrom assets and contribute to the achievement of the asset management objectives.","All CAPEX /' All OPEX","No"]
[null,"Protection Augmentation Strategy","The purpose of this document is to detail the  program to augment obsolete protection schemes that present a safety risk or a significant plant damage risk to the distribution network","Energex Initiated Augex (Capex)","No"]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Asset Exemption Guideline","It explains the circumstances in which the AER may grant an exemption from the\nprohibition on DNSPs owning a restricted asset.","All","No"]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Standard for Transmission and Distribution Planning (RED#01183)","Establishs a set of guidelines for electrical network planning activities within Energex. It is intended to provide an overview of the system planning process and related planning criteria, and reference should be made to other more specific technical documents and standards.","All Capex","No"]
[null,"Joint Planning (RED#00167)","Defines the joint planning process and the role of joint planning","All Capex","No"]
[null,"Produce the Distribution Annual Planning Report (RED#00802)","The purpose of this process is to identify emerging limitations on the existing transmission, sub transmission and primary distribution network.  This process then identifies prudent network planning proposals for publication on the DAPR.","All Capex","No"]
[null,"Prepare the Distribution Annual Planning Report (RED#0951)","This process ensures compliance with the requirements of clause 5.13.2 of the NER and clause 2.3 of the Queensland Electricity Industry Code by preparing a DAPR and publishing it on the Energex website by 30 September each year.","All Capex","No"]
[null,"Conduct Regulatory Investment Test for Distribution RIT-D (RED#00950)","Defines the process for conducting a regulatory investement test for disstribution ","All Capex","No"]
[null,"Substation Design Standards (RED#0364)","Provides a wide range of design standards to be followed as part of the design process for bulk, zone and modular substations.","All Capex","No"]
[null,"Design the Distribution Network (RED#0894)","Defines the distribution network design activities","All Capex","No"]
[null,"Standard Network Building Blocks - Feeder (RED#0694)","This document provides detail of the standard network building block groupings and essential elements to be utilised for the establishment of new sub-transmission and distribution networks within Energex, including overhead and underground electricity networks.","All Capex","No"]
[null,"Standard Network Building Blocks - Substation (RED#0693)","This document provides detail of the standard network building block groupings and essential elements to be utilised for the establishment of new sub-transmission and distribution substations within Energex.","All Capex","No"]
[null,"Vegetation management customer standard (RED#00804)","This standard defines the way Energex interacts with customers in relation to customer-requested and network-generated vegetation management services.\nEnergex is required to maintain its overhead electrical distribution system to deliver the safe and reliable supply of electricity to its customers. This includes the delivery of a planned maintenance program for vegetation that may have grown directly into or within specified limits of the overhead network, in addition to individual ad hoc customer requests for tree trimming. \n","Vegetation management (Opex)","No"]
[null,"Plant Rating Manual ","This manual to provide technical staff with an application guide for the rating of important items of plant in the ENERGEX network. Simplified tables have been presented so that for a particular situation with parameters defined, a rating may be established for a particular item of plant. It also disseminate information in the form of lists referring to ratings of specific items of plant to provide a quick ready reference for operating, design and planning personnel.","All Capex","No"]
[null,"Network planning protocol (RED#01145)","The purpose of this document is to outline the planning protocols for network assets.","All Capex","No"]
[null,"Produce a ten year bulk and zone substation demand forecast (RED#00443)","The purpose of this process is to provide a 10 year forecast of peak demand for all zone and bulk supply substations and all Powerlink Qld connection points in the Energex network. ","All Capex","No"]
[null,"Produce the peak MW demand forecast (RED#00666)","The purpose of this process is to provide a ten year forecast of system 50POE and 10POE peak demand for the Energex network. ","All Capex","No"]
[null,"Customer Outcome Standard (COS) (RED#01179)","The purpose of this document is to establish guidelines for Energex to address network expansion or security limits, network performance or reliability limits, and customer service or safety net targets contained in Energex’s Distribution Authority (DA) license. ","All Capex","No"]
[null,"Reliability Investment Guideline","This guideline provides the investment criteria for assessing the economic worth of a network reliability improvement project. The economic value of reliability has been based on the value of losses incurred by the customer for interruption of electricity supply under the Australian Energy Regulator (AER) Service Target Performance Incentive Scheme (STPIS).\nThis guideline outlines the requirements for economically justifying a reliability improvement project. The economic justification is based on the customer and utility benefits, as measured by the Value of Customer Reliability (VCR), being greater than the cost of the works to improve the reliability. All projects which improve reliability should use the following guidelines to determine the most economical solution.","All Capex","No"]
[null,"Maintenance Acceptability Criteria  (RED#00299)","This document sets out the Maintenance Acceptance Criteria which is used to evaluate the degree of deterioration in condition and performance of network plant and equipment as well as set setting safety criteria to determine if plant is fit to remain in service.\nNote: This document does not identify any safety / environmental hazards or provide warnings / cautions associated with carrying out the inspection or maintenance activities prescribed within it.  ","All Capex and All Opex","No"]
[null,"EQL Standard for High Voltage Live Work Management S016","This describes the process for the management of High Voltage Live Work, in accordance with Section 24 of the Queensland Electricity Safety Regulation 2013.","All Capex and All Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"EQL Sustainable Procurement Policy P011","The Energy Queensland Limited Procurement Policy provides direction in procurement activities that support Energy Queensland’s business in accordance with all applicable legislation. \nAccording to the Policy, procurement activities will be undertaken in accordance with established probity and governance standards. \nIt contains procurement policy principles and behaviours aimed at helping to provide guidance for emergent or extenuating circumstances which arise from time to time that may stretch the boundaries of compliance with this policy such as dealing with natural disasters.\nEnergy Queensland will remain fully compliant with the AER ring fencing guidelines as they apply to procurement activities.\n ","All Capex / All Opex","No"]
[null,"EQL Procurement Business Rules R052","The Business Rules have been developed to provide early process guidance and standards to all EQL business operations about the minimum requirements expected when purchasing on behalf of EQL and its subsidiaries, and in doing so seeks to identify the purchasing needs of both the regulated (and unregulated) businesses.  In respect to the unregulated business, the Strategic Procurement Group has identified that there is a particular need to tailor solutions as opportunities and challenges emerge, while ensuring that we continue to work together within important ring fencing parameters at all times.  \nTHe Procurement Business Rules align and support EQL's Sustainable Procurement Policy.","All Capex / All Opex","No"]
[null,"Information technology policies or strategies"]
[null,"ICT Plan","The purpose of this ICT Plan is to provide an understanding of the required ICT funding allocation from the Australian Energy Regulator (AER) for the next regulatory control period 2020 - 2025, how it will be invested and the benefits that will be derived","Non-Network Capex / Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Demand Management (DM) Strategy","The purpose of this document is to provide information on the Demand Management (DM) activities proposed as part of Energex and Ergon Energy Regulatory Proposal for 2020-2025.","All CAPEX /' All OPEX","No"]
[null,"Demand Management Plan","The purpose of the Demand Management Plan (DM Plan) is to engage and inform our end use customers and industry partners on our planned DM programs for the next five years.","All CAPEX /' All OPEX","No"]
[null,"Note: As agreed with the AER on 29 November 2018, additional asset management strategies unable to be inserted into this template have been included on the sheet called \"Extra info 7.1 7.3\""]
[null,"Self insurance guidelines or policy"]
[null,"Insurance Policy P042","The objective of this risk management plan is to ensure the current EQL Insurance Strategy and Program provides the appropriate balance of risk retention (self-insurance) and risk transfer (commercial insurance), to align to EQL’s risk appetite, ensuring adequate cover for existing and emerging risks that have the potential to impact the ongoing financial stability of EQL.\n\n","All CAPEX / All OPEX","No"]
[]
[null,"Land and easement acquisition polices"]
[null,"CID Approval Process for 110kV and 132kV Line Corridors\n(RED 643)","The control conditions that apply to the acquisition and approval of new line corridors.  Describes the activities required for the acquisition and approval of new line corridors.\n","Non-system opex and capex","No"]
[null,"Infrastructure Acquisitions for Substation Sites\n(RED 00420)","The control conditions that apply to the acquisition and approval of new substation sites. Describes the activities required for the acquisition and approval of new substation sites.","Non-system opex and capex","No"]
[]
[]
[null,"Asset security plans and policies"]
[null,"Summer preparedness plan","The Summer Preparedness Plan is a subset of the EMP which provides details of preparations that Energex is carrying out for summer 2018/19 to provide Queensland with a reliable network so as to minimise interruptions during extreme weather conditions, and where outages do occur, to ensure we keep the community fully informed and respond as quickly as possible to restore supply. ","All Opex / All Capex","No"]
[null,"Bushfire Risk Management Plan","This Bushfire Risk Management Plan is a subset of the Summer Preparedness Plan and targets issues and initiatives relating specifically to bushfires.","All Opex / All Capex","No"]
[null,"Flood Risk Management Plan","This Plan is a subset of the EMP and targets issues and initiatives relating specifically to floods.","All Opex / All Capex","No"]
[null,"Emergency Management Plan (EMP) - Distribution","The EMP provides guidance and direction on the emergency response arrangements. It details the framework and processes to be applied by Energex and Ergon Energy Network when responding to a Level 3 event which disrupts, or has the potential to disrupt the supply and distribution of electricity, or the provision of related services to customers and communities. \nFor EQL, an emergency is defined as a sudden and unexpected event that disrupts the normal operating functions, capabilities, resource and/or people of the organisation and requires an immediate response to prevent escalation of its scale or severity. \nThe EMP covers emergency planning (including Summer Preparedness), Emergency Response and Emergency Event Review ","All Opex / All Capex","No"]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"Manage Level 2 Emergency - Severe Weather (RED 882)","The procedure for extreme weather events that have potential to affect the Energex network (covers Thunderstorms, Winds, Rain and Hot Weather that is likely to result in possible overloads).","Emergency response (Opex)","No"]

{"sheet":"7.2 Contingent projects","index":33,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2020-21 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2020-21"}]
[null,null,null,null,null,{"$f":"+E8*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},{"$f":"+E9*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":34,"n_rows":298,"n_cols":6,"rows_kept":298,"cut":false,"hidden":false,"merged":[[6,1,6,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"Instructions"]
[null,"Outline those obligations and requirements that have been relied upon in the development of the regulatory proposal."]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact","EE Additional Data \n(not required by the AER)"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?","Location (cut and paste location into browser)"]
[null,"LEGISLATION"]
[null,"Electricity - National Scheme (Qld) Act 1997","This legislation provides that the National Electricity Law (NEL) and the National Electricity Rules (NER) apply as a law of Queensland","All","No"]
[null,"National Electricity Law","Electricity distribution entities have a large number of obligations under the NEL. The most significant obligations are to: register with AEMO as a \"Registered Participant\"; comply with the distribution determination that applies to the electricity distribution network services provided; provide the AER with the necessary information or prepare, maintain or keep the information as is requested by the AER in either a \"relevant notice\" or a \"regulatory information instrument\"; provide information to the AER for the purpose of the preparation of a NSP's performance or financial report; comply with the guidelines established by AEMO in relation to the shedding and restoration of loads in order to ensure the safety and security of the National Electricity System; comply with a wide range of obligations relating to the determination and resolution of access disputes, as well as to the restrictions on, variation of and compliance with access determinations; and comply with the general obligation not to prevent or hinder the access of another person to a regulated network service.","All","No"]
[null,"National Electricity Rules and subordinate Regulations","These Rules are made under the NEL and set out the rights and obligations of participants in the NEM, AEMO as market operator, and the market institutions. It includes connections, planning and expansation, economic regulation, metering and transitional requirements. It also includes all procedures established under the Rules","All","No"]
[null,"National Energy Retail Law","The NERL establishes the NECF which is focussed on the sale and supply of energy to residential and small business customers. ","ACS, Connection Policy","No"]
[null,"National Energy Retail Rules","The NERR are made under the NERL and provide the detailed content of the consumer protection measures and model contracts that govern the relationships between customers, retailers and distributors. ","Connection Policy, ACS\n","No"]
[null,"National Energy Retail Law (Qld) Act 2014","This legislation proivdes that the National Energy Retail Law (South Australia) Act applies as an Act in Queensland and provides the Queensland derogations from the national law as a schedule.","Connection Policy, ACS\n","No"]
[null,"National Energy Retail Law (Qld) Regulation 2014","This legislation proivdes the Queensland derogations to the NERR, including protections specific to consumers in regional and remote Queensland.","Connection Policy, ACS\n","No"]
[null,"Electricity Act 1994 (Qld)","The key obligations of an electricity distribution entity under this Act are to:  provide all customers with connection services unless there is a legitimate reason for the refusal of service provision; comply with the provisions of the National Electricity (Queensland) Law and the National Electricity Rules; operate, maintain and protect its supply network to ensure the adequate, economic, reliable and safe connection and supply of electricity; properly take into account the environmental effects of its activities; consider both demand and supply side options to provide for the efficient supply of electricity; pay the amounts required under the authority or regulations for administering the authority and its conditions; and pay any amount that, under the Energy Ombudsman Act 2006, it is required to pay the Energy Ombudsman.","All Capex & All Opex;\nConnection Policy","No"]
[null,"Electricity Regulation 2006 (Qld)","The Regulation sets out a number of provisions which impose specific obligations on electricity distribution entities including: prescribing standards and procedures for the design, building and maintenance of electric lines and works; specifying conditions governing the provision of customer connection services by distribution entities; prescribing standards and procedures for the measurement of energy efficiency and the performance of electrical equipment; specifying caps on fees for certain services; and providing for GOE employee leave, award and allowance entitlements.","All Capex & All Opex","No"]
[null,"Electrical Safety Act 2002 (Qld) ","Electrical distribution entities are required to comply with all relevant provisions under this Act, with the most specific obligation being the responsibility to ensure that all electricity inspection, testing and maintenance works are operated in a way that is electrically safe. ","All Capex & All Opex","No"]
[null,"Electrical Safety Regulation 2013 (Qld) ","This Regulation identifies specific ways for an electricity entity to meet its obligations under the Electrical Safety Act 2002. The provisions of the Regulation include: safety and technical requirements for electrical work and equipment and the works of electrical entities; safety and technical requirements for work in contact with or near exposed parts; requirements for the development of safety management plans; notification and reporting requirements for electrical incidents and dangerous electrical events; all matters concerning electrical licences and electrical licensing provisions; approvals of electrical equipment; and administrative matters.  ","All Capex & All Opex","No"]
[null,"Work Health and Safety Act 2011 (Qld)","This Act details Energex's obligations in relation to having appropriate health and safety standards at its place of business to ensure the safety of its employees and other persons.  Energex must provide and maintain a safe and healthy work environment, provide and maintain safe plant, ensure a safe system of work and provide information, instruction, training and supervision to ensure health and safety.  The Work Health and Safety Act does not apply to circumstances where the Electrical Safety Act applies.","All Capex & All Opex","No"]
[null,"Work Health and Safety Regulation 2011 (Qld)","This instrument provides a framework for health and safety of workers and workplaces.","All","No"]
[null,"Workers Compensation and Rehabilitation Act 2003 (Qld)","Under this Act, Energex, as a registered Queensland business, is legally liable for compensation for injury and damages sustained by a worker. Given the inherently dangerous nature of electricity distribution field operations, Energex is likely to have significantly higher compliance costs under this legislation than a typical Queensland business.","All","No"]
[null,"Workers Compensation and Rehabilitation Regulation 2014 (Qld) ","These Regulations set out the legal requirements for the workers' compensation scheme defined under the Workers' Compensation and Rehabilitation Act 2003.  All organisations operating in Queensland, including an electricity distribution entity is obliged to comply with all provisions under this Regulation. ","Opex","No"]
[null,"Energy and Water Ombudsman Act 2006 (Qld) and subordinate Regulation","Establishes an independent dispute resolution mechanism for small customers who have a complaint about their energy supply.","Opex","No"]
[null,"National Greenhouse and Energy Reporting Act 2007 (Cth)","Establishes the framework for the reporting and dissemination of information related to greenhouse gas emissions, greenhouse gas projects, energy consumption and energy production of corporations.","All","No"]
[null,"Environment Protection and Biodiversity Conservation Act 1999 (Cth) and associated regulation","The objects of this Act include, among other things, protection of the environment; promotion of ecologically sustainable development and biodiversity conservation; and provision for the protection and conservation of heritage.","All","No"]
[null,"Environmental Protection Act 1994 (Qld) and subordinate legislation","This legislation is relevant to Energex in terms of the environmental considerations that must be taken into account in constructing, operating and maintaining distribution network infrastructure.  This entails regular monitoring of environmental exposures and review of incident trends, as well as ensuring compliance with environmental regulations as part of an ongoing internal Environmental Management System.  Distribution entities are also required to comply with the framework established under the Act for the environmental evaluation of individual projects.  If the administering authority believes that an event or activity is causing or likely to cause environmental harm, it can require the responsible entity to either undertake or commission an environmental investigation into the activity and submit an accompanying report.  Electricity distribution entities are also required under the Act to obtain approvals prior to engaging in certain activities.","All","No"]
[null,"Nature Conservation Act 1992 and subordinate legislation (Qld)","The operation of an electricity supply network is classified as a \"service facility\" under the Nature Conservation Act and as such may be granted permission to operate on land situated in a national park.  This legislation provides the framework under which an electricity distribution entity must operate in order to obtain permission to construct distribution network infrastructure on land lying inside national park boundaries. The Act also regulates the taking of protected plants, protected animals and tampering with animal breeding places.","All","No"]
[null,"Native Title Act 1993 (Cth)","This Act provides for the recognition and protection of native title; establishes ways in which future dealings affecting native title may proceed and to set standards for those dealings; establishes a mechanism for determining claims to native title; and provides for, or permits, the validation of past acts, and intermediate period acts, invalidated because of the existence of native title.\n","All","No"]
[null,"Aboriginal Cultural Heritage Act 2003 (Qld) and Torres Strait Islander Cultural Heritage Act 2003 (Qld)","The main purpose of these Acts is to provide effective recognition, protection and conservation of Aboriginal and Torres Strait Islander cultural heritage.\n","All","No"]
[null,"Queensland Heritage Act 1992 (Qld) \nQueensland Heritage Regulation 2015 (Qld)","The obligations of an electricity distribution entity in relation to this legislation relate to the planning of expansions to its distribution network.  Distribution entities must take the provisions of this Act into account when planning an expansion project that has the potential to impact on an area that is registered as a heritage location under this Act.  Distribution entities must also follow the requirements outlined in the Act when applying to enter an area classified as a protected area.","All","No"]
[null,"Vegetation Management Act 1999 (Qld)\nVegetation Management Regulation 2012","Deals with various aspects of clearing, conservation and management of native vegetation.","Opex - Vegetation Management","No"]
[null,"Coastal Protection and Management Act 1995 (Qld) and associated regulation","The main objects of this Act are to: provide for the protection, conservation, rehabilitation and management of the coast, including its resources and biological diversity; and have regard to the goal, core objectives and guiding principles of the National Strategy for Ecologically Sustainable Development in the use of the coastal zone; and provide, in conjunction with other legislation, a coordinated and integrated management and administrative framework for the ecologically sustainable development of the coastal zone; and encourage the enhancement of knowledge of coastal resources and the effect of human activities on the coastal zone. ","All","No"]
[null,"Planning Act 2016 (Qld) and associated regulation","In order to ensure compliance with the provisions of this Act, a distribution entity must consider and attempt to minimise, where practicable, any adverse environmental impacts of its network expansion programs. Under the Act, construction of new electricity infrastructure often requires a full impact assessment involving public consultation and negotiation. To accommodate the longer project delivery times due to such assessments, demand forecasting and project planning must often be initiated earlier than would otherwise be required.  There may also be implications for cost and timing of construction of infrastructure due to design requirements imposed under planning approvals.","All","No"]
[null,"State Development and Public Works Organisation Act 1971 (Qld)","As the provider of facilities that are deemed to be \"public works\", Energex is obligated under this Act to cooperate with the Coordinator-General and provide information upon request to assist in the planning process for the Queensland Government's program of works.  ","All","No"]
[null,"Acquisition of Land Act 1967 (Qld)\nAcquisition of Land Regulation 2014 (Qld)","Electricity distribution entities are required to comply with all obligations under the Act relating to the acquiring of land for the purpose of constructing an easement and the payment of compensation to the holder of the land over which an easement is to be constructed.","All","No"]
[null,"Land Act 1994 (Qld)","There are a large number of specific obligations that a DNSP is required to comply with under this Act relating to the registration and administration of easements. ","All","No"]
[null,"Land Title Act 1994 (Qld)","The obligations upon a DNSP under this legislation relate to the registration and administration of easements and are broadly similar to its obligations under the Land Act 1994. ","All","No"]
[null,"Fire and Emergency Services Act 1990 (Qld)","This Act provide for the prevention of, and responses to, fires and other emergency incidents; provides for rescue services and operations; and establishes a framework for the management of the Queensland Fire and Emergency Service, the State Emergency Service, emergency service units established for an emergency service area, and the conduct of authorised rescue officers.","All","No"]
[null,"Building Fire Safety Regulation 2008 (Qld)","This instrument provdes a framework for safe evacuation of buildings and fire safety installations in buildings.","All","No"]
[null,"Government Owned Corporation Act 1993 (Qld)","This Act makes provision for a structural reform process (corporatisation) for nominated government entities.","All","No"]
[null,"Queensland Competition Authority Act 1997 (Qld)","The key ongoing obligation of Energex under this Act is to report to the QCA in accordance with the Electricity Distribution Network Code.  Part 3 (pricing practices relating to monopoly business activities) and Part 5 (access to services) of the Act are potentially applicable to Energex but do not impose ongoing obligations. ","All","No"]
[null,"Corporations Act 2001 (Cth)","This Act is the principal legislation regulating companies in Australia. It regulates matters such as the formation and operation of companies (in conjunction with a constitution that may be adopted by a company), duties of officers, takeovers and fundraising.","All","No"]
[null,"Financial AccountabilityAct 2009 (Qld)","The Financial Accountability Act 2009 sets out the principles to be observed by all Queensland public sector agencies in relation to their financial management.","All","No"]
[null,"Income Tax Assessment Act 1936 (Cth)\nIncome Tax Assessment Act 1997 (Cth)\nFringe Benefits Tax Assessment Act 1986 (Cth)\nA New Tax System (Goods and Service Tax) Act 1999 (Cth)","These instruments provide a framework for the treatment of income tax, fringe benefits tax, and goods and services tax.","All","No"]
[null,"Tax Administration Act 1953","The TAA and regulations made under it, contain provisions dealing with the administration of tax laws (including GST) by, and the powers of, the ATO.  The TAA has become increasingly important because it contains the PAYG withholding regimes and the generic provisions for tax administration including dealing with penalties for breaches of various tax laws.","All","No"]
[null,"Payroll Tax Act 1971 (Qld), Payroll Tax Act 2007 Act 21 of 2007 (NSW Consolidated Acts), Payroll Tax Act 2007 (Victorian Current Acts), Payroll Tax Act 2009 (South Australia)","Payroll Tax is a state impost controlled by eight separate legislatures. Accordingly, the requirements, liabilities and rates of tax vary from state to state.The legislation in each state broadly provides for payroll tax to be levied on \"wages\", in cash or in kind, provided by employers to employees.","All","No"]
[null,"Competition and Consumer Act 2010 (Cth)","The object of this Act is to enhance the welfare of Australians through the promotion of competition and fair trading and provision for consumer protection.\n","All","No"]
[null,"Fair Trading Act 1989 (Qld)","The principal objective of this Act is to improve consumer wellbeing through consumer empowerment and protection, fostering effective competition and enabling the confident participation of consumers in markets in which both consumers and suppliers trade fairly.","All","No"]
[null,"Privacy Act 1988 (Cth)","Energex is an organisation which is subject to the provisions of the Privacy Act 1988 and the Australian Privacy Principles for the protection of privacy of individuals and the responsible and transparent handling of personal information.  The Act also sets out a procedure for individuals to complain about privacy breaches.\n\n","Non Network Opex and Capex; Overheads","No"]
[null,"Public Records Act 2002 (Qld)","The main purposes of this Act are to ensure—\n(a) the public records of Queensland are made, managed, kept and, if appropriate, preserved in a useable form for the benefit of present and future generations; and\n(b) public access to records under this Act is consistent with the principles of the Right to Information Act 2009 and the Information Privacy Act 2009.","Non Network Opex and Capex; Overheads","No"]
[null,"Right to Information Act 2009 (Qld)","As a public entity, the public has a right of access to information in Energex's possession or control,  unless, on balance, it is contrary to the public interest to give the access.  The RTI Act sets out the procedural steps for releasing information to the public, including when access to information may be refused.","Non Network Opex and Capex; Overheads","No"]
[null,"Information Privacy Act 2009 (Qld)","It contains a set of rules or ‘privacy principles’ that govern how Ergon Energy collect, store, use and disclose personal information. The IP Act also allows an individual to make a complaint about an agency's breach of the privacy principles.\nThe IP Act also allows an individual to make a complaint about an agency's breach of the privacy principles.","Non Network Opex and Capex; Overheads","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"Distribution Authority","The Queensland Regulatory (the Department of Natural Resources, Mines and Energy) has issued Energex a Distribution Authority in accordance with the Electricity Act 1994 (Qld)","All","No"]
[null,"Electrical Worker's Licence","Issued to Qualified Technical Person for Energex in accordance with the Electrical Safety Act 2002 (Qld)","All","No"]
[null,"Electrical Contractor's Licence","Issued to Energex Responsible Person in accordance with the Electrical Safety Act 2002 (Qld)","All","No"]
[]
[null,"RULES"]
[null,"National Electricity Rules","These Rules are made under the NEL and set out the rights and obligations of participants in the NEM, AEMO as market operator, and the market institutions. It includes connections, planning and expansation, economic regulation and transitional requirements. It also includes all procedures established under the Rules","All","No"]
[null,"National Energy Retail Rules","The NERR are made under the NERL and provide the detailed content of the consumer protection measures and model contracts that govern the relationships between customers, retailers and distributors. ","ACS, Connection Policy","No"]
[null,"Market Settlement and Transfer Solution (MSATS) Procedures","Comply with various MSATS Procedures including Consumer Administration and Transfer Solution (CATS) Procedures Principles and Obligations; Wholesale, Interconnector, Generator and Sample (WIGS) NMI; and Meter Data Management (MDM) Procedures","All","No"]
[null,"Note: As agreed with the AER on 29 November 2018, additional Rules unable to be inserted into this template have been included on the sheet called \"Extra info 7.1 7.3\""]
[null,"ORDERS"]
[null,"Regulatory Information Notice","The AER issued a RIN for Energex on xx October 2018 in accordance with section 28F(1)(a) of the NEL.","Reset RIN","No"]
[]
[]
[null,"CODES"]
[null,"Electricity Distribution Network Code","The EDNC has been made under the Electricity Act 1994 and contains a wide range of obligations that impact on Energex's operations.","All","No"]
[null,"Traffic Management for Construction or Maintenance Work Code of Practice 2008","This Code provides advice about how to manage risks associated with working on, or adjacent to, a roadway.","All","No"]
[null,"Electrical Code of Practice 2013 Managing Electrical Risks in the Workplace","This Code gives practical advice on ways to manage electrical risk when working near exposed live parts.  It applies to Energex as an electricity entity and an employer. It also provides benchmarks for ensuring that electrical work (live and de-energised) is performed in ways that are electrically safe.  It also provides guidance on electrical risk.  As such, it applies to Energex's operations.","All","No"]
[null,"Electrical Code of Practice 2010 Works","This Code gives advice on ways for an electricity entity to manage electrical safety risks associated with earthing systems, underground cable systems and supporting structures for overhead lines forming part of the works of an electricity entity.  As such, this Code applies to Energex's operations.","All","No"]
[null,"Code of Practice 2011 How to Manage and Control Asbestos in the workplace","This is a national code of practice that has been developed to assist persons in control of premises to control the risks of asbestos-containing materials in workplaces.  This Code applies to parts of Energex's operations in terms of asset management.","All","No"]
[null,"Code of Practice 2011 How to Safely remove Asbestos","The purpose of this Code is to provide advice for the safe removal of asbestos and asbestos-containing material from buildings and structures, plant and equipment and vehicles.  This Code applies to Energex in terms of asset management.","All","No"]
[null,"Code of Practice 2010 - Working Near Overhead and Underground Electric Lines","A person conducting a business or undertaking at a workplace is required to comply with the requirements of this Code to ensure that no person, plant or thing comes within an unsafe distance (exclusion zone) of an overhead electric line.","All","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"Framework and Approach","The AER issued its Framework and Approach for Energex in accordance with clause 6.8.1 of the NER on 30 July 2018","All","No"]
[null,"Distribution Annual Planning Report","Clause 5.13.2(b) of the NER requires each DNSP to publish a DAPR by the DAPR date each year, setting out the results of the distribution annual planning review for the forward planning period.","All Capex / All Opex","No"]
[null,"Cost Allocation Guideline (Distribution)","These guidelines ouline the required content of Energex's cost allocation method and the basis on which the AER will assess that method for approval.","Overheads","No"]
[null,"Regulatory Investment Test for Distribution (RIT-D)","The RIT-D is required for all investment decisions (subject to a number of exclusions) to identify the credible option that maximises the present value of the net economic benefit to all those who produce, consume and transport electricity in the NEM, in accordance with clause 5.17 of the NER.","All Capex / All Opex","No"]
[null,"Ring-fencing Guideline","These guidelines detail Energex's obligations and related compliance reporting requirements","All","No"]
[null,"Expenditure Forecast Assessment Guideline","The guidelines describe the process, techniques and associated data requirements for the AER's approach to setting efficient expenditure allowances for network businesses, in accordance with clause 6.2.8 of the NER.","All Capex / All Opex","No"]
[null,"Rate of Return Guidelines","The rate of return guideline sets out how the AER will determine the return that electricity and gas network businesses can earn on their investments, in accordance with clause 6.2.8 of the NER.","Rate of return","No"]
[null,"Expenditure Incentives Guideline","The expenditure incentives guideline gives electricity network businesses incentives to spend efficiently and share the benefits of efficiencies with consumers, in accordance with clause 6.2.8 of the NER.","Expenditure incentives","No"]
[null,"Consumer Engagement Guideline","The guideline provides best practice principles and a framework for electricity and gas network service providers to better engage with their consumers.","All","No"]
[null,"Shared Asset Guideline","This guideline outlines how consumers will benefit from the other services electricity network businesses may provide using the assets consumers pay for, in accordance with clause 6.2.8 of the NER.","All","No"]
[null,"Confidentiality Guideline","The confidentiality guideline sets out how energy network businesses must make confidentiality claims over information they submit to us. This guideline balances protecting genuinely confidential information with ensuring that stakeholders can access sufficient information on issues affecting their interests, in accordance with clause 6.2.8 of the NER.","All","No"]
[null,"Post Tax Revenue Model (PTRM)","The PTRM will be used by the AER to determine the maximum allowed revenue (MAR) to be earned by a NSP over a regulatory control period. The AER has issued a PTRM and an associated PTRM Handbook.","Revenue","No"]
[null,"Roll Forward Model (RFM)","The RFM will be used by the AER to determine the closing regulated asset base (RAB) for a regulatory control period. The AER has issued a RFM and associated RFM handbook.","Capex, RAB","No"]
[null,"Service Target Performance Incentive Scheme (STPIS)","The STPIS is designed to ensure DNSPs improve efficiency without a deterioration in service performance for customers, and improving service performance where customers are willing to pay for these improvements, in accordance with clause 6.6.2 of the NER.","STPIS - reliability targets","No"]
[null,"Efficiency Benefit Sharing Scheme (EBSS)","The EBSS should provide for a fair sharing between DNSPs and network users of efficiency gains and efficiency losses in accordance with clause 6.5.8 of the NER.","EBSS","No"]
[null,"Capital Expenditure Sharing Scheme (CESS)","The CESS provides financial rewards for DNSPs whose capex becomes more efficient and imposes financial penalties for those that become less efficient. Consumers benefit from improved efficiency through lower regulated prices, in accordance with clause 6.5.8A of the NER.","CESS","No"]
[null,"Demand Management Incentive Scheme (DMIS) and Demand Management Incentive Allowance (DMIA)","The DMIS provides DNSPs with an incentive to undertake efficient expenditure on non-network options relating to demand management. The separate DMIA provides DNSPs with funding for research and development in demand management projects that have the potential to reduce long term network costs.","DMIS and DMIA","No"]
[null,"Cost Allocation Method","The AER has approved the Cost Allocation Method that Energex submitted to it in accordance with the Cost Allocation Guidelines and clause 6.15 of the NER. This document will be used by Energex for the purposes of attributing costs to, or allocating costs between, its Distribution Services, and other unregulated activities within the Energex Group.","Overheads","No"]
[null,"Connection Charge Guideline","This guideline sets out how DNSPs should charge electricity customers for connection services. ","Connection Policy","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[null,"Standard Coordination Agreement (Annexure A, ENDC)","This is a deemed agreement that applies between Energex and any retailer with whom we have a common customer. The agreement defines the way in which the parties will discharge their respective obligations to customers and establishes common protocols for communicating customer information, in circumstances where a Negotiated Coordination Agreement has not been entered into.","All","No"]
[]
[]
[null,"OTHER"]
[null,"Negotiated Coordination Agreement ","Energex can negotiate with any retailer with whom it has a common customer. The agreement defines the terms and conditions under which the parties will discharge their respective obligations to customers and establish common protocols for communicating customer information.","All","No"]

{"sheet":"7.4 Shared Assets","index":35,"n_rows":26,"n_cols":19,"rows_kept":26,"cut":false,"hidden":false,"merged":[[6,11,6,18],[32,2,32,8],[6,1,7,1],[6,2,7,2],[6,3,6,10],[25,1,26,1],[25,2,26,8],[27,2,27,8],[28,2,28,8],[29,2,29,8],[30,2,30,8],[31,2,31,8],[39,2,39,8],[40,2,40,8],[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service","Shared asset unregulated revenue  ($0's, nominal)",null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Shared asset unregulated revenue  ($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  ($0's, real June 2020)"}]
[null,null,null,{"$f":"PRCP_y1","v":"2010-11"},{"$f":"PRCP_y2","v":"2011-12"},{"$f":"PRCP_y3","v":"2012-13"},{"$f":"PRCP_y4","v":"2013-14"},{"$f":"PRCP_y5","v":"2014-15"},{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CONCATENATE(\"Total \n\",CRCP_y5, \" to \", dms_MultiYear_FinalYear_Result)","v":"Total \n2019-20 to 2024-25"}]
[null,"License fee for use of Energex electricty distribution network assets","Energex owned electricity distribution network assets comprising of aerial transmission towers, distribution wood poles, public lighting columns and underground conduit and pit networks (used to support telephone or fibre optic cable for communication services for example)",7220750.7199999997,7416429.2999999998,7543028.8100000005,6984297.0600000005,6951791.9100000001,6958585.8200000003,7359526.4100000001,7455196.5800000001,7673052.5631158175,7513398.5907680886,7254709.0412028898,7083293.3423187761,6915927.8874426642,6752516.9766087336,6592967.1710688667,{"$f":"SUM(M9:R9)","v":42112813.009410024}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(M10:R10)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]

{"sheet":"7.7 TSS-LRMC","index":36,"n_rows":150,"n_cols":22,"rows_kept":150,"cut":false,"hidden":false,"merged":[[8,1,9,1],[8,2,8,21],[19,1,20,1],[19,2,19,21],[30,1,31,1],[30,2,30,21],[107,2,107,21],[122,2,122,21],[137,2,137,21],[44,1,45,1],[44,2,44,21],[64,1,65,1],[64,2,64,21],[84,1,85,1],[84,2,84,21]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C10,4)+1)&\"-\"&MID(C10,3,2)+2),VALUE(LEFT(C10,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C21,4)+1)&\"-\"&MID(C21,3,2)+2),VALUE(LEFT(C21,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C32,4)+1)&\"-\"&MID(C32,3,2)+2),VALUE(LEFT(C32,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C46,4)+1)&\"-\"&MID(C46,3,2)+2),VALUE(LEFT(C46,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C66,4)+1)&\"-\"&MID(C66,3,2)+2),VALUE(LEFT(C66,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C86,4)+1)&\"-\"&MID(C86,3,2)+2),VALUE(LEFT(C86,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C109,4)+1)&\"-\"&MID(C109,3,2)+2),VALUE(LEFT(C109,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C124,4)+1)&\"-\"&MID(C124,3,2)+2),VALUE(LEFT(C124,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C139,4)+1)&\"-\"&MID(C139,3,2)+2),VALUE(LEFT(C139,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]

{"sheet":"7.8 WACC Inputs","index":37,"n_rows":66,"n_cols":3,"rows_kept":66,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Energex"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.8 WACC AND CAPM PARAMETERS"]
[]
[]
[null,"Business Days means Business Days as defined in the Rate of Return Guideline"]
[]
[null,"7.8 - WACC AND CAPM PARAMETERS"]
[null,"7.8.1 - RATE OF RETURN ON EQUITY"]
[null,"Equity averaging period - nominated (placeholder)"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","N/A"]
[]
[]
[null,"Nominated equity averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","20 days"]
[]
[]
[null,"Nominal risk free rate",2.9999999999999997E-4]
[null,"Equity term - risk free rate","10 years"]
[null,"Forecast Inflation rate","-"]
[null,"Market risk premium",0.06]
[null,"Equity beta",0.6]
[null,"Equity risk premium",{"$f":"C26*C27","v":3.5999999999999997E-2}]
[]
[]
[null,"7.8.2 - RATE OF RETURN ON DEBT - Transition - 'trailing average' approach"]
[null,"Debt averaging period - Year 1 nominated (placeholder)"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","N/A"]
[]
[]
[null,"Year 1 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","40 days"]
[]
[null,"Year 2 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","25 days"]
[]
[null,"Year 3 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","25 days"]
[]
[null,"Year 4 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","25 days"]
[]
[null,"Year 5 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days","25 days"]
[]
[]
[null,"Credit rating","BBB+"]
[]
[null,"Debt term","10 years"]

{"sheet":"Extra info 7.1 7.3","index":38,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["Template 7.1 Policies and procedures"]
["7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
["As agreed with the AER on 29 November 2018, the below information was unable to be inserted into table 7.1.1 because of the protection settings on that template and has been included on this additional sheet"]
[null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
["Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
["Cost allocation method"," The Cost Allocation Methodology governs the manner in which Energex is allowed to allocate costs to the services it provides. Allocation of costs between services is required to accurately represent costs incurred in providing the respective services and prevents cross-subsidisation between distribution services and other services.","Overheads","No"]
["AER Unit Cost Methodology and Estimation Approach ","The purpose of this document is to inform stakeholders of the Unit Cost and Estimation Methodology prior to  Energex submitting its 2020-25 regulatory proposals to the Australian Energy Regulator in January 2019","Unit Costs","No"]
["Asset Management Strategies"]
["Public Lighting Strategy 2020-2025","The EQL Street Light Strategy focuses upon supporting and partnering with customers around street light solutions. Within regulatory, safety and technical boundaries, EQL will approach street lighting in a flexible manner, offering smart technology and tariff solutions to meet customer expectations whilst balancing commercial outcomes. This document focus upon the three main areas of: Streamline Customer Engagement, Standardise Product Offerings and Technology Process Improvement.","ACS","No"]
["Metering Vision and Strategy 2020-2025","This document outlines our vision and strategy to work collaboratively with the market to utilise advanced metering to meet future challenges providing customers with choice and control at the best possible price; enabling better response to network stability, quality of supply challenges, provide critical data and reduce operational costs in terms of service delivery.","ACS","No"]
["Intelligent Grid Technnology Plan","This document details the 2020-2025 activities in supporting the Future Grid Roadmap which details the long term vision EQL is taking to be a world leader in energy supply.The drivers for change are focussed around; changing expectation of customers, industry change and the Energy Queensland Limited (EQL) Business Plan.","Energex Initiated Augex (Capex)","No"]
["Future Grid Roadmap","This Future Grid Roadmap provides a guiding, holistic pathway for transforming Energex's business ","Energex Initiated Augex (Capex)","No"]
["LV Monitoring Strategy","The Low Voltage (LV) Monitoring Strategy has been developed as part of Energy Queensland (EQL) overall Future Grid Roadmap. A key focus of the LV Monitoring Strategy is on identifying the monitoring and visibility requirements across the LV networks that underpin EQL's Future Grid Roadmap.\nThe LV Monitoring Strategy is made up of 4 key concepts: Network monitoring and visibility, customers and network benefits, data sources and deployment strategy.","All CAPEX /' All OPEX","No"]
["Customer Availability and Reliability of Supply Strategy","This strategy outlines the relevant network reliability obligations, economic context, expenditure drivers and future requirements for EQL. It examines the historical and projected reliability performance of Ergon Energy and Energex and the associated programs that underpin the future management of this performance ","All CAPEX /' All OPEX","No"]
["Asset Management Narrative, Risk & Optimisation","The purpose of this document is to provide an overview of the frameworks Energex has put in place to effectively manage investment, risk, optimisation and governance of the Network Program. ","All CAPEX /' All OPEX","No"]
["Customer Quality of Supply Strategy","This strategy outlines the current customer quality of supply obligations, environment, drivers and future requirements for Energy Queensland","All CAPEX /' All OPEX","No"]
["Strategic Proposal - LV Safety & Network Visibility","This document provides the higher level of justification for projects and programs in the strategic program of work.\nGreater level of visibility of the LV network is a critical capability required to detect safety issues in near-real time. Such capability also increases operational efficiencies by reducing the fault investigation time and enabling remote asset inspection instead of regular inspection programs, which are currently difficult to accurately target.","Energex Initiated Augex (Capex)","No"]
["Strategic Proposal - Intelligent Grid Enablement","The Intelligent Grid Enablement proposal seeks to continue to deliver sustainable outcomes for customers and the business with no compromise to existing safety and legislative compliance.  ","All CAPEX /' All OPEX","No"]
["Strategic Proposal - Power Quality Energex","Power Quality (PQ) capital expenditure is primarily intended to allow Energex to identify and deliver works to comply with mandatory quality of supply obligations in accordance with the existing statutory requirements and any future regulatory performance standards and targets. This document is aimed at addressing Energex's current and future network PQ obligations. It has been developed from the Customer Quality of Supply Strategy and the Low Voltage Network Monitoring Strategy. ","All CAPEX /' All OPEX","No"]
["Strategic Proposal - Worst Performing Feeder Program Energex","This document provide a clear view of the profile of Energex's historical and forecast reliability capex (direct cost) relating to the Worst Performing Feeder (WPF) improvement program delivered in the 2015 to 2020 AER regulatory period and into the 2020 to 2025 regulatory period. This program is a continuation of an ongoing program that aims to improve the performance experienced by the customers supplied by consistently poor performing feeders or feeder sections and is required to discharge the improvement obligations in Energex’s Distribution Authority (DA) No.D01/99.","All CAPEX /' All OPEX","No"]
["Strategic Proposal - Distribution Feeder Augmentation Energex","This document provides a high level overview of the projects and programs in the strategic Program of Works for Distribution Feeder Augmentation (DFA). This program is a bottom-up and top-down balance between customer and community expectations, changing economic, technological and regulatory environments, requirements for evolution of our HV and LV networks into smart intelligent grids and optimisation between direct network augmentation and alternative non network solutions to identified constraints.","All CAPEX /' All OPEX","No"]
["Strategic Proposal - Pole Top Structures Energex","The purpose of this document is to outline the forecast volumes of replacement and expenditure associated with pole top structures in accordance with the lifecycle management strategies detailed in Section 9 of the Asset Management Plan.  ","All CAPEX /' All OPEX","No"]
["Demand management policies or strategies"]
["Demand Side Engagement Strategy","This document is required by 5.13.1 of the NER. This document communicates Energex's approach for engagin with stakeholders, customers and non-network providers on teh supply of demand side solutions as an alternative to investing in network infrastructure, either through the formal Regulatory Investment Test for Distribution (RIT-D) or other means depenidng on the requirement.","All CAPEX / All OPEX","No"]
["RED01090 Engaging with non-network providers","This procedure outlines the way in which Energex will meet its obligations to engage with non-network providers and assess non-network options during RIT-D non-network options report consultations.","All CAPEX / All OPEX","No"]
["RED01089 Deliver non-network solution (RIT-D)","This document describes the Energex process for delivering a non-network option, identified as the preferred option (or part option), through application of the RIT-D.","All CAPEX / All OPEX","No"]
["RED01091 Maintain the Energex Demand Side Engagement Facility","This process describes how Energex will maintain a demand side engagement facility to notify those who register of developments in projects subject to the RIT-D as per clauses 5.17.4 (q), 5.17.4 (k2), 5.17.4 (g) and 5.14.1 of the NER.","All CAPEX / All OPEX","No"]
["RED01147 Network Planning and Expansion","The purpose of this Network Planning and Expansion Policy is to set out Energex’s obligations under Chapter 5 of the NER relating to network planning and expansion and how Energex will manage compliance with those obligations.","All CAPEX / All OPEX","No"]
["RED00548 Maintain a non-network toolbox","This document describes the process to develop a non-network options toolbox used to assist in determining if a non-network option could form a potential credible option, or form a significant part of a potential credible option, when undertaking non-network assessments in accordance with the Energex Demand Side Engagement Strategy. Non-network assessments are undertaken for both RIT-D assessments and targeted demand management (DM) campaigns.","All CAPEX / All OPEX","No"]
["RED01092 Screening for non-network options","This procedure describes how Energex will screen for non-network options when undertaking RIT-D assessments in order to determine if either a Notice or Non-network Options Report should be published. ","All CAPEX / All OPEX","No"]
["RED00949 Produce a transmission planning RIT-D project assessment report","The purpose of this document is to:\n• Define Transmission Planning Department involvement in pre-approval project lifecycle;\n• Quantify hand-offs to, from and within Transmission Planning Department; and\n• Provide guidance on the production of Transmission Planning Department key outputs.","All CAPEX / All OPEX","No"]
[]
[]
[]
["Template 7.3"]
["7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
["As agreed with the AER on 29 November 2018, the below information was unable to be inserted into table 7.3.1 because of the protection settings on that template and has been included on this additional sheet."]
[null,"Brief description","Relevance to regulatory proposal","Expenditure impact","EE Additional Data \n(not required by the AER)"]
[null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?","Location (cut and paste location into browser)"]
["RULES"]
["Business to Business (B2B) Procedures","Comply with B2B procudures including Customer and Site Details Notification Process; Service Order Process; and Meter Data Process","All","No"]
["Queensland B2B Process Specification: Network Billing","This document describes the automation of the network billing process, its associated transactions and the associated business rules. ","All","No"]
["Retailer Handbook: Operating Procedures","This document defines the standard protocols for communication and transactions between Energex and retailers operating within its distribution area. In the Standard Coordination Agreement it is known as the Operational Procedures.","Connection Policy, ACS\n","No"]

{"sheet":"Amendments","index":39,"n_rows":3,"n_cols":4,"rows_kept":3,"cut":false,"hidden":false,"merged":[[0,1,0,3]]}
[null,{"$f":"CONCATENATE(dms_TradingName,\" data amendments\")","v":"Energex data amendments"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Energex"},"Table","Comments"]
[null,"Template 7.1 & 7.3","Table 7.1.1 & 7.3.1","As agreed with the AER on 29 November 2018, an additional sheet titled \"Extra info 7.1 7.3\" has been added because the information contained on that sheet was not able to be inserted into table 7.1.1 & 7.3.1 (respectively) because of the protection settings on those templates."]