{"text_format":"1","workbook":"xlsx","n_sheets":34,"sheets":["Instructions","CONTENTS","Business & other details","2.1 Expenditure summary","2.2 Repex","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","5.4 MD & utilisation-Spatial","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.7 TSS-LRMC","7.8 Export Services","AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":1,"defined_names":725,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4],[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[26,2,26,4],[10,2,10,4],[12,1,14,1],[12,2,12,4],[13,2,13,3],[14,2,14,4],[16,2,16,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List)),\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by Power and Water Corporation to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify confidential information\nin the confidential workbook. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selection as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return selection to NON-CONFIDENTIAL macro."]
[]
[null,"RESPONSES","\nPlease return two (2) files to the AER: \n\n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,"AMENDMENTS","\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]
[]
[null,"UNITS OF MEASURE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," PLEASE DO NOT ENTER TEXT into cells that are to contain numbers \n(including 'numbers stored as text')"]
[]
[]
[null,"NAVIGATION","\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]

{"sheet":"CONTENTS","index":1,"n_rows":43,"n_cols":5,"rows_kept":43,"cut":false,"hidden":false,"merged":[[6,3,6,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"TEMPLATE","NOVEMBER 2022"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 Forecast price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[null,null,null,null,"7.8 Export Services"]

{"sheet":"Business & other details","index":2,"n_rows":74,"n_cols":81,"rows_kept":74,"cut":false,"hidden":false,"merged":[[73,25,73,34],[73,37,73,52],[55,25,55,34],[63,25,63,34],[65,25,65,34],[55,37,55,44],[61,25,61,34],[61,37,61,52],[32,37,32,58],[33,37,33,58],[43,37,43,44],[43,46,43,53],[43,55,43,62],[41,37,41,44],[63,37,63,52],[65,37,65,52],[67,37,67,52],[69,37,71,81],[67,25,67,34],[69,25,71,34],[51,46,51,53],[51,37,51,44],[50,73,50,80],[50,64,50,71],[45,25,45,34],[49,25,49,34],[53,25,53,34],[45,46,45,53],[45,37,45,44],[49,37,49,44],[47,73,47,80],[51,73,51,80],[49,73,49,80],[53,37,53,44],[49,46,49,53],[50,46,50,53],[46,46,46,53],[46,37,46,44],[51,64,51,71],[47,46,47,53],[50,55,50,62],[47,37,47,44],[22,60,22,66],[23,60,23,66],[31,60,31,66],[49,64,49,71],[41,55,41,62],[41,64,41,71],[47,64,47,71],[49,55,49,62],[47,55,47,62],[46,64,46,71],[46,55,46,62],[43,64,43,71],[16,37,16,48],[15,21,15,35],[43,73,43,80],[41,73,41,80],[51,55,51,62],[25,21,25,35],[23,21,23,35],[45,73,45,80],[45,64,45,71],[46,73,46,80],[45,55,45,62],[42,73,42,80],[32,21,32,35],[33,21,33,35],[33,60,33,66],[32,60,32,66],[31,21,31,35],[31,68,31,89],[32,68,32,89],[33,68,33,89],[31,37,31,58],[41,46,41,53],[50,37,50,44],[41,25,41,34],[15,37,15,58],[24,37,24,51],[0,7,2,15],[6,21,6,75],[24,21,24,35],[42,37,42,44],[42,46,42,53],[42,55,42,62],[42,64,42,71],[3,21,3,57],[8,16,8,93],[22,68,22,89],[23,68,23,89],[25,68,25,71],[25,80,25,82],[24,68,24,82],[25,37,25,40],[22,37,22,58],[23,37,23,58],[25,49,25,51],[24,60,24,66],[25,60,25,66],[22,21,22,35],[16,21,16,35]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Power and Water"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":15947352360}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 1921"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 1921"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"DARWIN"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"DARWIN"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NT"},null,null,null,null,null,null,null,null,null,"Post code",null,801,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NT"},null,null,null,null,null,null,null,null,null,"Post code",null,801]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2024-25",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2028-29"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2033-34"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2034-35"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2035-36"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2036-37"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2037-38"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2038-39"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2023-24"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2028-29"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2030-31"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2033-34"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2014-15"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2015-16"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2018-19"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2020-21"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2023-24"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2025-26"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2028-29"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2022-23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2028-29"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Regulatory proposal"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Public"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"31/01/23",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"2.1 Expenditure summary","index":3,"n_rows":111,"n_cols":9,"rows_kept":111,"cut":false,"hidden":false,"merged":[[7,1,8,1],[23,1,24,1],[37,1,38,1],[89,1,90,1],[102,1,103,1],[49,1,50,1],[61,1,62,1],[75,1,76,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX (including dual function assets)"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure",{"$f":"SUM('2.2 Repex'!D12:D182)","v":38592859.769823335},{"$f":"SUM('2.2 Repex'!E12:E182)","v":47541407.359175004},{"$f":"SUM('2.2 Repex'!F12:F182)","v":47509401.939582162},{"$f":"SUM('2.2 Repex'!G12:G182)","v":44023794.146622427},{"$f":"SUM('2.2 Repex'!H12:H182)","v":30431118.92790975},{"$f":"SUM('2.2 Repex'!I12:I182)","v":27450230.710457556},{"$f":"SUM('2.2 Repex'!J12:J182)","v":27213012.894361552}]
[null,"Connections",{"$f":"SUM('2.5 Connections'!E123:E136)","v":3839413.9617052604},{"$f":"SUM('2.5 Connections'!F123:F136)","v":3889297.350758425},{"$f":"SUM('2.5 Connections'!G123:G136)","v":1180559.200910527},{"$f":"SUM('2.5 Connections'!H123:H136)","v":1198455.4115700077},{"$f":"SUM('2.5 Connections'!I123:I136)","v":1210568.0653834874},{"$f":"SUM('2.5 Connections'!J123:J136)","v":1220555.3536916368},{"$f":"SUM('2.5 Connections'!K123:K136)","v":1233291.6573989228}]
[null,"Augmentation Expenditure",{"$f":"SUM('2.3 Augex (b)'!D47:D55)","v":6380278.9632214662},{"$f":"SUM('2.3 Augex (b)'!E47:E55)","v":13453934.716456933},{"$f":"SUM('2.3 Augex (b)'!F47:F55)","v":9485176.256310571},{"$f":"SUM('2.3 Augex (b)'!G47:G55)","v":6067060.6457375092},{"$f":"SUM('2.3 Augex (b)'!H47:H55)","v":7288674.2628427297},{"$f":"SUM('2.3 Augex (b)'!I47:I55)","v":5401536.1146545578},{"$f":"SUM('2.3 Augex (b)'!J47:J55)","v":4972602.083693523}]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E32:E50)","v":23981219.873360824},{"$f":"SUM('2.6 Non-network'!F32:F50)","v":28069911.180260375},{"$f":"SUM('2.6 Non-network'!G32:G50)","v":21501051.680954196},{"$f":"SUM('2.6 Non-network'!H32:H50)","v":26154043.730188645},{"$f":"SUM('2.6 Non-network'!I32:I50)","v":24853947.278700236},{"$f":"SUM('2.6 Non-network'!J32:J50)","v":54258332.83919283},{"$f":"SUM('2.6 Non-network'!K32:K50)","v":73252016.973421797}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C23:C25)","v":0},{"$f":"SUM('7.8 Export Services'!D23:D25)","v":0},{"$f":"SUM('7.8 Export Services'!E23:E25)","v":637695.20373502094},{"$f":"SUM('7.8 Export Services'!F23:F25)","v":802492.04958818073},{"$f":"SUM('7.8 Export Services'!G23:G25)","v":5544581.5605401592},{"$f":"SUM('7.8 Export Services'!H23:H25)","v":2937732.3648589291},{"$f":"SUM('7.8 Export Services'!I23:I25)","v":3297810.2387787392}]
[null,"Public lighting"]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",{"$f":"'2.10 Overheads'!D15","v":13841380.007205471},{"$f":"'2.10 Overheads'!E15","v":13841380.007205475},{"$f":"'2.10 Overheads'!F15","v":16888822.31339984},{"$f":"'2.10 Overheads'!G15","v":16344413.225556737},{"$f":"'2.10 Overheads'!H15","v":14693398.930508742},{"$f":"'2.10 Overheads'!I15","v":19543828.309158821},{"$f":"'2.10 Overheads'!J15","v":23881618.209762186}]
[null,"Capitalised corporate overheads",{"$f":"'2.10 Overheads'!D30","v":10700855.966364648},{"$f":"'2.10 Overheads'!E30","v":10700855.96636465},{"$f":"'2.10 Overheads'!F30","v":9867722.6612343919},{"$f":"'2.10 Overheads'!G30","v":9549637.847894324},{"$f":"'2.10 Overheads'!H30","v":8584990.8837101553},{"$f":"'2.10 Overheads'!I30","v":11418977.233276244},{"$f":"'2.10 Overheads'!J30","v":13953440.969560349}]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C10:C18)","v":97336008.541681007},117496786.58022086,107070429.2561267,104139897.05715781,92607279.909595266,122231192.92529057,147803793.02697706]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"}]
[null,"Vegetation management",2857092.1751594623,2867248.4163266551]
[null,"Maintenance",16471471.193448039,16530023.113919346]
[null,"Emergency response",8539015.9743212871,8569370.0197104178,null," "]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E12:E30)","v":4662997.3854155466},{"$f":"SUM('2.6 Non-network'!F12:F30)","v":4679573.1635511015}]
[null,"Export services",{"$f":"SUM('7.8 Export Services'!C13:C14)","v":0},{"$f":"SUM('7.8 Export Services'!D13:D14)","v":0}]
[null,"Metering",48559.996002620421,48732.614525315796]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D12","v":18742015.646296494},{"$f":"'2.10 Overheads'!E12","v":18808638.77890595}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D27","v":20775151.933629278},{"$f":"'2.10 Overheads'!E27","v":20849002.352302324}]
[null,"Total",{"$f":"SUM(C26:C33)","v":72096304.304272726},{"$f":"SUM(D26:D33)","v":72352588.459241107}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Connections",0,0,2750950.4413506691,2827734.211732632,2891126.2084218226,2949443.4406717028,3014398.8545747837]
[null,"Metering",9808567.2002274059,10938830.922405757,5211730.79989985,5297897.2359822607,7401026.1839215569,8882550.9912058506,9803780.6448243186]
[null,"Public lighting",{"$f":"'4.1 Public lighting'!D14+'4.1 Public lighting'!D18","v":0},{"$f":"'4.1 Public lighting'!E14+'4.1 Public lighting'!E18","v":0},{"$f":"'4.1 Public lighting'!F14+'4.1 Public lighting'!F18","v":0},{"$f":"'4.1 Public lighting'!G14+'4.1 Public lighting'!G18","v":0},{"$f":"'4.1 Public lighting'!H14+'4.1 Public lighting'!H18","v":0},{"$f":"'4.1 Public lighting'!I14+'4.1 Public lighting'!I18","v":0},{"$f":"'4.1 Public lighting'!J14+'4.1 Public lighting'!J18","v":0}]
[null,"Fee and quoted",4309387.4035421414,4266608.2137038494,4240314.1674924511,4240314.1674924521,4240314.1674924521,4240314.1674924511,4240314.1674924521]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D16","v":3215525.3334072065},{"$f":"'2.10 Overheads'!E16","v":3373066.5955392458},{"$f":"'2.10 Overheads'!F16","v":4066130.7535547926},{"$f":"'2.10 Overheads'!G16","v":4078534.4002418229},{"$f":"'2.10 Overheads'!H16","v":4600710.9260838609},{"$f":"'2.10 Overheads'!I16","v":4625186.3715513926},{"$f":"'2.10 Overheads'!J16","v":4649012.10392344}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D31","v":3727130.1144513972},{"$f":"'2.10 Overheads'!E31","v":3836621.9955546497},{"$f":"'2.10 Overheads'!F31","v":4388088.2162720785},{"$f":"'2.10 Overheads'!G31","v":4397678.6648317445},{"$f":"'2.10 Overheads'!H31","v":4801423.4138632091},{"$f":"'2.10 Overheads'!I31","v":4820347.7278046655},{"$f":"'2.10 Overheads'!J31","v":4838769.6862257468}]
[null,"Total",{"$f":"SUM(C40:C45)","v":21060610.051628154},22415127.7272035,20657214.378569841,20842158.680280909,23934600.8997829,25517842.698726062,26546275.457040742]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Connections",1184977.6894389081,1173214.4431155489,2018961.1978859187,2018961.1978859182,2018961.1978859187,2018961.1978859184,2018961.1978859184]
[null,"Metering",{"$f":"'3.2 Operating expenditure'!K71","v":6423872.9639646709},{"$f":"'3.2 Operating expenditure'!L71","v":6460324.3388418574},{"$f":"'3.2 Operating expenditure'!M71","v":6687767.8311198801},{"$f":"'3.2 Operating expenditure'!N71","v":6806745.3256401988},{"$f":"'3.2 Operating expenditure'!O71","v":6917744.288565021},{"$f":"'3.2 Operating expenditure'!P71","v":6989966.5113409795},{"$f":"'3.2 Operating expenditure'!Q71","v":7059464.8815970635}]
[null,"Public lighting",{"$f":"'3.2 Operating expenditure'!K73","v":0},{"$f":"'3.2 Operating expenditure'!L73","v":0},{"$f":"'3.2 Operating expenditure'!M73","v":0},{"$f":"'3.2 Operating expenditure'!N73","v":0},{"$f":"'3.2 Operating expenditure'!O73","v":0},{"$f":"'3.2 Operating expenditure'!P73","v":0},{"$f":"'3.2 Operating expenditure'!Q73","v":0}]
[null,"Fee and quoted",1240972.8406633725,1228653.7317591077,1312958.2767939626,1312958.2767939628,1312958.2767939626,1312958.2767939628,1312958.276793963]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D13","v":1618038.150703755},{"$f":"'2.10 Overheads'!E13","v":1614327.5330407987},{"$f":"'2.10 Overheads'!F13","v":1959906.8234940688},{"$f":"'2.10 Overheads'!G13","v":1974570.0516718873},{"$f":"'2.10 Overheads'!H13","v":1988249.9759922801},{"$f":"'2.10 Overheads'!I13","v":1997150.9108820488},{"$f":"'2.10 Overheads'!J13","v":2005716.1480738393}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D28","v":1872277.4240443846},{"$f":"'2.10 Overheads'!E28","v":1863241.5831877538},{"$f":"'2.10 Overheads'!F28","v":2369486.2218547445},{"$f":"'2.10 Overheads'!G28","v":2380823.7697724057},{"$f":"'2.10 Overheads'!H28","v":2391401.0311783934},{"$f":"'2.10 Overheads'!I28","v":2398283.1975472826},{"$f":"'2.10 Overheads'!J28","v":2404905.8038322316}]
[null,"Total",{"$f":"SUM(C52:C57)","v":12340139.06881509},12339761.629945068,14349080.351148576,14494058.621764373,14629314.770415574,14717320.094450193,14802006.308183014]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation expenditure"]
[null,"Non-network"]
[null,"Export services"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C64:C70)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Export services"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total",{"$f":"SUM(C78:C85)","v":0},{"$f":"SUM(D78:D85)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure",0,0,0,0,0,0,0]
[null,"Connections",6547085.8435345665,6552611.0817142036,186888.17166687499,189508.91631946576,191216.11083199081,192590.20850469568,194400.8259038004]
[null,"Augmentation Expenditure",1138516.9402917016,7392396.9523967924,3465381.6185175036,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Export services",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",869793.09869307757,1584901.5950105137,791754.09257092362,41082.523661824802,41452.616321939633,41750.498876749851,42143.011976322618]
[null,"Capitalised corporate overheads",672442.39120718825,1225297.1654734039,462602.40390997392,24003.506117584264,24219.742138142909,24393.787573753587,24623.123304547124]
[null,"Total",{"$f":"SUM(C92:C98)","v":9227838.2737265341},16755206.794594914,4906626.2866652757,254594.94609887482,256888.46929207334,258734.49495519913,261166.96118467016]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Replacement expenditure",12387588.120298695,12075100.845018467,16316901.650310051,15119784.506600145,10451438.123490702,9427664.7672908176,9346193.3191790823]
[null,"Connections",2409173.0544176809,1920442.1607192326,469643.97318019759,476690.43405580724,481436.80207459198,485338.82167687122,490334.89974389569]
[null,"Augmentation Expenditure",2047950.53697457,3417181.5158130717,3257643.3672411921,2083706.125976044,2503264.1172623634,1855134.5616915894,1707818.9965206627]
[null,"Non-network",7697524.2618791712,7129511.4520193506,6493342.2835103758,7938257.5319464561,7937987.8608518122,18185715.729254443,25158093.089914355]
[null,"Export services",0,0,219013.70039242131,275612.47487261554,1904262.9105394308,1008951.6625213383,1132618.8739645381]
[null,"capcons (included in the above)",1542235.4899002658,2810198.7604839173,1254356.4964808975,65086.029779409073,65672.358460082542,66144.286450503438,66766.135280869741]
[null,"Total",{"$f":"SUM(C105:C109)","v":24542235.97357012},24542235.973570123,26756544.974634238,25894051.073451068,23278389.814218901,30962805.542435061,37835059.179322533]

{"sheet":"2.2 Repex","index":4,"n_rows":523,"n_cols":10,"rows_kept":523,"cut":false,"hidden":false,"merged":[[482,1,522,1],[5,1,5,2],[11,1,29,1],[30,1,36,1],[37,1,42,1],[43,1,51,1],[52,1,59,1],[60,1,75,1],[76,1,104,1],[105,1,118,1],[119,1,127,1],[128,1,135,1],[183,1,202,1],[203,1,209,1],[210,1,215,1],[216,1,224,1],[136,1,176,1],[225,1,232,1],[233,1,248,1],[249,1,277,1],[278,1,291,1],[292,1,300,1],[301,1,308,1],[356,1,375,1],[451,1,464,1],[465,1,473,1],[309,1,349,1],[474,1,481,1],[376,1,382,1],[383,1,388,1],[389,1,397,1],[398,1,405,1],[406,1,421,1],[422,1,450,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.2 REPEX"]
[]
[null,"There are THREE sub-tables on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",99979.216892534154,131219.10690496094,165965.25710748334,179919.76975520299,193693.12397294372,207828.60508986702,223229.77305088207]
[null,null,"˃ 11 kV & < = 22 kV; Steel",111149.79472490097,145656.14575120801,183924.57577584049,199045.24286201573,213893.79030549343,229066.76749765969,245552.41839705125]
[null,null,"> 22 kV & < = 66 kV; Steel",1368302.8123607896,574562.55239966011,1213261.6752628989,1989186.6914699513,2160875.3028739868,302168.57108949492,325814.61231656803]
[null,null,"> 66 kV & < = 132 kV; Steel",341940.2279180311,1337701.1053484941,1021096.0306243366,2752824.5289533613,0,0,0]
[null,null,"> 132 kV; Steel",507089.31234399305,632826.30618041474,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",59081.448083810203,77564.355660931265,98132.491405690147,106417.29756038595,114602.14845634057,123009.02343607714,132173.71467243726]
[null,null,"˃ 11 kV & < = 22 kV",593049.32285562484,628065.9574632867,192263.65477795425,207243.44652191753,221765.24931084368,236436.00483510466,252253.34222477479]
[null,null,"> 22 kV & < = 66 kV",1138459.8353468296,625302.25329037185,655461.04820956744,855118.32538840873,926610.03612822946,554206.42948853422,594743.98272945231]
[null,null,"> 66 kV & < = 132 kV",264297.47673065681,263469.1875565318,164275.69108548941,297290.83471534931,298870.26987915568,167510.76653304472,168451.99622255896]
[null,null,"> 132 kV",274832.17143332964,353274.51196585753,224671.50002614877,820152.70313304663,824509.97845994844,229095.94802997287,230383.21996177841]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",10185.358722629686,12583.539518190366,14993.649307974007,15324.660818380915,15563.03365006258,15758.382724193823,15978.6423406987]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",9035.5090031301661,11092.519707285883,13135.24082720906,13343.699938840771,13469.842942350537,13557.097790093621,13664.190317942132]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",108.81282495971837,135.42664465915615,162.41380549857595,166.94150748631046,170.33609722651681,173.09491531724328,175.96232064901835]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",384803.0599318411,141465.33623325799,41403.757802000728,49520.247456755846,51698.066717392772,34479.025501780168,35162.508791845576]
[null,null,"> 66 kV & < = 132 kV",58.764502210246405,218060.52504510226,132653.52846888814,357478.47725983948,97.13483807134233,100.27908061418965,103.68230141632051]
[null,null,"> 132 kV",58.779973461835255,73.870127960746956,89.51550028361433,93.031002682593098,96.070371802797652,98.938593814379729,102.06030143179539]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",1433851.6499493204,1513858.6632563202,1555783.6031432392,1579014.2109767303,1593035.4241275915,1603180.0213265656,1616384.8992718912]
[null,null,"> 11 kV & < = 22 kV",6923642.6698797764,5595664.4572389685,6812592.3438410778,9574919.4517423883,5806342.5470375428,5827931.1592768654,5863173.094625771]
[null,null,"> 22 kV & < = 33 kV",1259021.843103393,6642675.0575595964,49721.273147143293,51986.457425031629,53924.577560409212,55680.969365907833,57491.154932735859]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",278.17778716121779,361.81781175733596,452.4186724775243,483.89691680860108,513.09248618493507,541.45876964209947,571.29699620170436]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",14961.793611007142,18989.169600545123,1855124.7774785778,1876361.310698106,1887197.4680055461,1894268.3579457118,1905783.3501972598]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",15723.29205516774,19600.466849020799,23539.3277533935,24224.972885233481,24753.231048216236,25193.554062378309,25641.889311074945]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",515.90978497287927,672.06288100080712,840.05018227721621,896.69050905320114,947.4950914387349,994.63739582593882,1041.7774279040354]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",78910.555536411717,99249.641526812164,120260.14269010544,124867.95554689945,128728.36230912854,132208.73610173538,135831.8496883511]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",385622.17150755529,487626.00100886315,595901.96093421825,626022.4304590784,655069.30255499866,685234.35424460343,719619.55604294408]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",1654.1403189354669,2008.2917483638466,2352.438116948455,2364.5599963568748,2362.931806246751,2355.0882664142969,2350.2797997573184]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",800971.01864597842,736369.94317641389,737105.2131022315,745934.64839634823,750625.44821004244,753808.30049413664,758745.85984465061]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",10373.18820752745,14252.779281469759,18635.65811134722,20677.525468782504,22600.777524594894,24448.148975554825,26308.78897502254]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",1305922.0216614355,891707.78352936637,1161439.5149578296,1216286.4632907347,1266578.4879774984,1316131.6246611318,1370477.342686618]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",180600.16955388241,238656.62585165759,303867.83095237234,331572.78425519203,359254.09119908599,387922.59073284984,419289.83171087794]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",227662.14928564109,273418.9796858771,317078.88729966857,315808.2366039881,312993.1587531651,309566.36606304045,306644.39687119186]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",296830.15496846114,377745.13027467439,462479.60659835441,484500.82708843873,503201.45033364859,520035.1430540905,537149.2190963272]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",42328.264637465509,53307.114504498655,64696.032114191476,67303.161393181232,69535.578672812961,71602.090165965506,73798.106998366158]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",679915.10478173418,905072.73055870563,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",103043.84168125759,590224.74394029041,828487.02131493308,649075.20490142156,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",1825199.1526378586,1669866.8818045256,2027610.2467985705,2071051.7609182049,2107604.2679974958,2152286.9693806581,2201422.3933658563]
[null,null,"> 11 kV & < = 22 kV  ; Switch",446573.04510737967,755292.59854804282,2104147.5993606867,868410.17521121644,331627.88038224768,341871.06879208359,352664.63561005739]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",177112.23864952094,223510.97877590545,271880.15754785168,283535.52506654087,293719.68684642576,303341.80871395831,313690.04669203673]
[null,null,"> 22 kV & < = 33 kV ; Switch",259213.50904808531,322745.61682851479,396980.77857651561,419277.20633167238,439450.8823060288,459425.59366913885,479172.53831125284]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",1159.8063604314025,1485.2012476378532,1831.3499809588784,1934.2760664908631,2027.7536811693881,2117.823801725121,2213.5129155835848]
[null,null,"> 66 kV & < = 132 kV ; Switch",1757903.3027781365,833924.18551907782,507890.43357946939,364421.19054111512,82312.044583267154,82933.70870296807,83919.600801655644]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",194955.12930162228,159175.85652198794,161688.00805695928,148078.77716517134,137587.79297351959,137716.71563603805,138490.53492050449]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",0,0,0,0,0,0,0]
[null,null,"Local Network Wiring Assets",748774.90227457997,3120394.9195235972,4390185.3838830879,2623418.329942306,167955.48628993711,168112.86412127744,169057.47694930725]
[null,null,"Communications Network Assets",221587.59978596849,180920.58473626169,183775.91678588279,168307.553275535,156383.41455321357,156529.94910938456,157409.47845814933]
[null,null,"Master Station Assets",943145.17305745988,1198340.7279615451,1840516.6040079091,1665530.2612525078,7247.099939053458,7253.8906244732025,7294.6496596179441]
[null,null,"Communications Site Infrastructure",5623079.2963542845,5670077.1014136868,5083408.7737431657,1838761.1350892782,3060336.7551607653,2729917.1092889169,2376715.2765718088]
[null,null,"Communications Linear Assets",1058249.5083403443,1000321.4014144503,1718747.0251599215,1613645.733350947,1277032.9797301404,1398379.7409747723,1165864.079254278]
[null,null,"AFLC",0,0,0,227309.2064218907,0,229267.89294367653,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"OTHER: ","Other",0,0,0,0,0,0,0]
[null,null,"Buildings",287095.29057697108,2035626.7293729985,1536937.5906788572,176074.02170366765,243446.9502617447,15369.472135443402,15455.831978368409]
[null,null,"Instrument Transformers",33248.429267122578,27146.488659023598,27574.92105225171,25253.948260684403,23464.773761464232,23486.760749142002,23618.730991921882]
[null,null,"Metering Units",24902.202335154569,20332.008704677326,20652.893341283321,18914.54553526681,17574.500715870279,17590.968393530889,17689.810647446735]
[null,null,"Pillars",0,0,671464.52445245755,678838.21322779998,682444.71843854454,684687.6518829799,688534.85740495392]
[null,null,"Substation Auxiliary Plant",479854.06941813749,621887.88648627314,1421555.2948217716,709106.79961911659,85091.637773279799,172477.52775236103,117158.55871801652]
[null,null,"Voltage Regulators",0,0,0,0,0,0,0]
[null,null,"Civil and Grounds",1086030.5544981675,3000645.9619853762,3659077.4020222668,1721980.8186428603,272995.35963549564,419968.63867140381,502662.61733883526]
[null,null,"Fire Systems",7219.759960913213,0,271656.01571323408,370791.33607224713,353616.00948132458,0,106492.12826776315]
[null,null,"Capacitor Banks",0,0,0,0,0,0,0]
[null,null,"Cable Tunnels",0,0,149066.50383010393,440517.85843638447,151504.12945182537,152002.06528418857,152856.15281345038]
[null,null,"Power Transformer Refurbishment",0,0,0,0,0,0,0]
[null,null,"Power Transformer Spares",0,0,0,0,0,0,0]
[null,null,"Pole Refurbishment",4493296.779465382,3085198.0695890398,2030906.3857913003,2053208.7875941235,2064116.9952449498,2070900.9543214526,2082537.1822642467]
[null,null,"Tower Refurbishment",0,0,0,0,0,0,0]
[null,null,"EDO Refurbishment",0,0,0,0,0,0,0]
[null,null,"Surge Arrestors",0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",10,11,12,13,14,15,16]
[null,null,"> 1 kV & < = 11 kV; Steel",7,8,8,9,10,10,11]
[null,null,"˃ 11 kV & < = 22 kV; Steel",48,66,59,96,103,11,12]
[null,null,"> 22 kV & < = 66 kV; Steel",0,15,9,24,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",19,19,21,22,24,26,28]
[null,null,"˃ 11 kV & < = 22 kV",91,114,109,156,169,62,65]
[null,null,"> 22 kV & < = 66 kV",37,37,36,36,36,36,36]
[null,null,"> 66 kV & < = 132 kV",68,88,40,40,40,40,40]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",0.112083056028626,0.11345408780548043,0.11476909437452233,0.11602865762930814,0.11721075350726488,0.1182932126963598,0.11927642745029843]
[null,null,"> 1 kV & < = 11 kV",4.3042608920600613E-2,4.329421500081173E-2,4.3524919369762993E-2,4.3735389003803402E-2,4.3915523368724035E-2,4.4055206489092461E-2,4.4155110793767029E-2]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",1.170106947676174E-3,1.1931726434593628E-3,1.2148492399913584E-3,1.2351524541941185E-3,1.2536079331509872E-3,1.2697386267592984E-3,1.2835602698867794E-3]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",7.2323335642052164,10.236726113002691,7.0409987358639716,12.245151138236968,13.249139895039992,0.25292106595038727,0.25649354423315485]
[null,null,"> 22 kV & < = 66 kV",2.7993746519129755E-4,3.0002891283937183,1.8002983171313485,4.8003075036134151,3.1668723009586002E-4,3.2586735534375505E-4,3.3504389209062596E-4]
[null,null,"> 66 kV & < = 132 kV",2.800111658573497E-4,2.8831584585506007E-4,2.966184620016712E-4,3.0491895878846903E-4,3.1321676696636672E-4,3.2151130335712113E-4,3.2980248463378213E-4]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",1.7302459290571572,1.7320285675926543,1.6537176229932138,1.6553151202873315,1.656771409560672,1.658036501696734,1.6591120157123886]
[null,null,"> 1 kV & < = 11 kV",9.1412144320226645,7.418801393078188,7.5194616756693593,8.5201182419292216,7.5207699495332498,7.5214156249066297,7.5220550931150019]
[null,null,"> 11 kV & < = 22 kV",1.512137627639135,6.5126076201850216,1.3066204289472293E-2,1.3513075964012333E-2,1.3942785644025527E-2,1.4349757698642275E-2,1.4733481352179606E-2]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",1.0509345751027219E-4,1.1199454542630536E-4,1.1889065634882728E-4,1.2578152310177353E-4,1.3266563919619862E-4,1.3954143106075954E-4,1.4640849796707119E-4]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",0,0,800,800,800,800,800]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",1,1,1,1,1,1,1]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",10,9,10,10,11,11,12]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",56,50,28,28,28,27,27]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",11,7,7,8,8,9,9]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",1,1,1,0,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",2,2,2,2,2,2,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",2,2,2,3,3,3,3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0,1,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",0,0,0,2,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",1,1,0,1,0,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",9,4,6,7,4,4,4]
[null,null,"> 11 kV & < = 22 kV  ; Switch",0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",1,0,0,1,2,1,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",7,2,0,6,0,1,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,1]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",0,0,24,34,1,1,0]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,1,1]
[null,null,"Communications Network Assets",0,1,39,19,0,0,0]
[null,null,"Master Station Assets",0,0,23,17,17,12,19]
[null,null,"Communications Site Infrastructure",10,17,32,21,22,27,15]
[null,null,"Communications Linear Assets",0,0,0,1,0,1,0]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"Other"]
[null,null,"Buildings",0,0,6,6,7,5,6]
[null,null,"Instrument Transformers",0,0,1,1,1,1,1]
[null,null,"Metering Units",0,0,0,1,1,1,1]
[null,null,"Pillars",42,46,56,56,56,56,56]
[null,null,"Substation Auxiliary Plant",9,9,7,9,6,6,6]
[null,null,"Voltage Regulators",0,0,0,0,0,0,0]
[null,null,"Civil and Grounds",0,0,0,1,0,4,4]
[null,null,"Fire Systems",4,4,32,48,50,0,14]
[null,null,"Capacitor Banks",0,0,0,0,0,0,0]
[null,null,"Cable Tunnels",0,0,52,53,52,52,52]
[null,null,"Power Transformer Refurbishment",0,0,0,0,0,0,0]
[null,null,"Power Transformer Spares",0,0,0,0,0,0,0]
[null,null,"Pole Refurbishment",235,235,180,180,180,180,180]
[null,null,"Tower Refurbishment",0,0,0,0,0,0,0]
[null,null,"EDO Refurbishment",0,0,0,0,0,0,0]
[null,null,"Surge Arrestors",0,0,0,0,0,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C177),\"\",C177)","v":""}]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",1,1,1,1,1,1,1]
[null,null,"> 1 kV & < = 11 kV; Steel",1,1,1,1,1,1,1]
[null,null,"˃ 11 kV & < = 22 kV; Steel",2,2,2,3,3,3,3]
[null,null,"> 22 kV & < = 66 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",9,10,10,11,12,13,14]
[null,null,"> 1 kV & < = 11 kV",2,3,3,3,3,3,3]
[null,null,"˃ 11 kV & < = 22 kV",5,5,5,6,6,6,7]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",8,9,8.8000000000000007,7.1599999999999993,6.992,7.9903999999999993,7.98848]
[null,null,"> 1 kV & < = 11 kV",6.4,5.4799999999999995,4.7759999999999998,4.7311999999999994,4.6774399999999998,5.2129279999999998,4.9755135999999993]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",14.6,15.919999999999998,16.704000000000001,16.844799999999999,16.413759999999996,16.096511999999997,16.395814399999995]
[null,null,"> 22 kV & < = 66 kV",1,1.2,1.24,1.488,1.3856000000000002,1.2627200000000003,1.3152640000000002]
[null,null,"> 66 kV & < = 132 kV",0.2,0.04,4.8000000000000001E-2,5.7600000000000005E-2,6.9120000000000001E-2,8.2944000000000004E-2,5.9532800000000011E-2]
[null,null,"> 132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",14.2,16.240000000000002,17.887999999999998,13.665600000000001,12.59872,14.918464,15.0621568]
[null,null,"> 1 kV & < = 11 kV",29,26,25.2,24.84,24.408000000000001,25.889600000000002,25.267520000000001]
[null,null,"> 11 kV & < = 22 kV",5.2,5.4399999999999995,5.7279999999999998,4.4736000000000002,4.9683200000000003,5.1619840000000012,5.1543808000000002]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",6,6,7,7,7,7,8]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",2,2,2,2,2,2,2]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",8,8,8,8,9,9,9]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",10,11,11,12,12,13,13]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",1,1,1,1,1,2,2]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",2,2,3,3,3,3,3]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",0,0,0,1,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",1,1,1,1,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",1,1,1,1,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",23,24,25,26,26,27,27]
[null,null,"˂ = 11 kV ;  Circuit Breaker",3,3,3,3,4,4,4]
[null,null,"> 11 kV & < = 22 kV  ; Switch",6,6,7,7,7,7,7]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",4,5,5,5,5,6,6]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road"]
[null,null,"Luminaires ;  Minor Road"]
[null,null,"Brackets ; Major Road"]
[null,null,"Brackets ; Minor Road"]
[null,null,"Lamps ; Major Road"]
[null,null,"Lamps ; Minor Road"]
[null,null,"Poles / Columns ; Major Road"]
[null,null,"Poles / Columns ; Minor Road"]
[null,null,"Other"]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",0,0,0,0,0,0,0]
[null,null,"Local Network Wiring Assets",0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",0,0,0,0,0,0,0]
[null,null,"Master Station Assets",0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",0,0,0,0,0,0,0]
[null,null,"AFLC",0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B137),\"\",B137)","v":"OTHER: "},"Other",0,0,0,0,0,0,0]
[null,null,"Buildings",0,0,0,0,0,0,0]
[null,null,"Instrument Transformers",9,10.8,12.959999999999999,15.551999999999998,13.462399999999999,12.35488,13.025855999999999]
[null,null,"Metering Units",5.8,5.36,4.8319999999999999,4.9984000000000002,5.5980800000000004,5.3176959999999998,5.2212351999999997]
[null,null,"Pillars",0,0,0,0,0,0,0]
[null,null,"Substation Auxiliary Plant",0,0,0,0,0,0,0]
[null,null,"Voltage Regulators",0,0,0,0,0,0,0]
[null,null,"Civil and Grounds",0,0,0,0,0,0,0]
[null,null,"Fire Systems",0,0,0,0,0,0,0]
[null,null,"Capacitor Banks",0,0,0,0,0,0,0]
[null,null,"Cable Tunnels",0,0,0,0,0,0,0]
[null,null,"Power Transformer Refurbishment",0,0,0,0,0,0,0]
[null,null,"Power Transformer Spares",0,0,0,0,0,0,0]
[null,null,"Pole Refurbishment",0,0,0,0,0,0,0]
[null,null,"Tower Refurbishment",0,0,0,0,0,0,0]
[null,null,"EDO Refurbishment",5.4,6.4799999999999995,7.7759999999999989,8.7311999999999976,9.0774399999999993,7.4929279999999991,7.9115135999999993]
[null,null,"Surge Arrestors",0,0,0,0,0,0,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C157),\"\",C157)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C177),\"\",C177)","v":""}]

{"sheet":"2.3 Augex (b)","index":5,"n_rows":78,"n_cols":10,"rows_kept":78,"cut":false,"hidden":false,"merged":[[67,1,68,2],[59,1,60,2],[44,1,45,2],[5,1,5,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,null,null,"VOLUMES (0's)"]
[null,"PROJECT TYPE","UNITS",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,22,0,0,0,0,0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",379,728,830,830,830,830,830]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",57.318230017198793,57.318230017198793,58.110230017198795,58.110230017198795,58.110230017198795,58.110230017198795,58.110230017198795]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",46.8,40.799999999999997,44.8,44.8,44.8,44.8,44.8]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",1,1,1,1,1,1,1]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,500,500,500,500,500]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,500,500,500,500,500]
[]
[null,"COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,"PROJECT TYPE",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,628753.14165580284,4293825.2350042313,432702.36087975843,437729.07011672866,440207.20769783808,441564.82383476483,444009.31300018524]
[null,"HV Feeder Augmentations - Underground Cables",null,491766.95664381044,491103.30680457206,884560.19329492655,894836.14114335389,899902.12195589382,902677.45507415698,907674.64946032874]
[null,"HV Feeder Non-Material Projects",null,45656.482751680574,91189.736738073087,92121.655954245231,93191.834489829605,93719.42610543831,94008.460457896217,94528.888378425443]
[null,"LV Feeder Augmentations - Overhead Lines",null,1064002.5306035462,1064346.5879869356,1088930.0576931681,1101580.1730479624,1107816.6042374815,1111233.1536995715,1117384.9059629969]
[null,"LV Feeder Augmentations - Underground Cables",null,0,0,0,0,0,0,0]
[null,"LV Feeder Non-Material Projects",null,0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted",null,62007.051721452372,61923.371902483988,114643.88099155571,115975.70052304771,116632.27958434929,116991.97806743038,117639.64202839376]
[null,"Distribution Substation Augmentations - Ground Mounted",null,0,0,55894.028194113016,56543.349883145573,56863.461591216219,57038.830716727542,57354.595913974008]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,55894.028194113016,56543.349883145573,56863.461591216219,57038.830716727542,57354.595913974008]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,3105690.869679668,5599253.7296643313,5052820.1487478167,1718917.8364476254,705106.92373108119,707281.50088742143,711196.98933327768]
[null,"Subtransmission Lines",null,761298.62343941326,1549200.6366660201,1073165.3413269699,1085632.3177563951,1091778.4625513516,1095145.5497611689,1101208.2415483012]
[null,"HV Feeders",null,1120520.0982996132,4784928.5418088026,1317262.5541746849,1332565.2112600827,1340109.3296537318,1344242.2789089216,1351683.9624605139]
[null,"HV Feeders - Land Purchases and Easements",null,45656.482751680574,91189.736738073087,92121.655954245231,93191.834489829605,93719.42610543831,94008.460457896217,94528.888378425443]
[null,"Distribution Substations",null,62007.051721452372,61923.371902483988,226431.93737978177,229062.4002893389,230359.20276678176,231069.63950088547,232348.83385634181]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,1064002.5306035462,1064346.5879869356,1088930.0576931681,1101580.1730479624,1107816.6042374815,1111233.1536995715,1117384.9059629969]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,221103.30672609282,303092.11169028725,634444.56103390444,506110.87244627508,2719784.3137968644,818555.53143869201,364250.26215366647]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,365662.19030765328,3983658.7799983378,0,0,0,0,0]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,6014616.7729138127,9470275.9364585951,9485176.256310571,6067060.6457375092,7288674.2628427306,5401536.1146545568,4972602.0836935239]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,0,0,0,0,0,0,0]
[null,"Subtransmission Lines",null,0,0,0,0,0,0,0]
[null,"HV Feeders",null,365662.19030765328,3983658.7799983378,0,0,0,0,0]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,0,0,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]

{"sheet":"2.5 Connections","index":6,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,10,3],[54,1,55,1],[54,2,55,2],[54,3,55,3],[138,1,139,1],[138,2,139,3],[102,1,103,1],[102,2,103,2],[102,3,103,3],[120,1,121,1],[120,2,121,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Underground connections","0's",130,131,132,133,134,136,137]
[null,null,"Overhead connections","0's",83.068358188594658,83.995553869858782,84.922749551122877,85.849945232387455,86.777140913651579,86.704336594915674,87.631532276179769]
[null,null,"Distribution substations installed","MVA added",0.87159804445462863,0.87948161760153576,0.88736519074844289,0.89524876389535202,0.90313233704225926,0.91101591018916639,0.91889948333607341]
[null,null,"Distribution substations installed","0's",2.6540239244978703,2.6780294759966838,2.702035027495497,2.7260405789943163,2.7500461304931298,2.774051681991943,2.7980572334907561]
[null,null,"Distribution substations installed ","total spend $0s",646911.81824752677,647279.21387235867,246118.34257615238,250910.82997267912,254487.51122353366,257604.3111681584,261287.52787992108]
[null,null,"Augmentation HV ","net circuit KM added",0.11702586742082796,0.11808436220722877,0.11914285699362957,0.12020135178003062,0.12125984656643143,0.12231834135283223,0.12337683613923302]
[null,null,"Augmentation HV","total spend $0s",813759.49415093532,806367.46890944813,364415.91347656265,367996.06186186225,369742.64891585521,370794.84011562669,372635.46177533525]
[null,null,"Augmentation LV","net circuit KM added",3.4664040601371413,3.4977575609150451,3.529111061692948,3.5604645624708589,3.5918180632487622,3.6231715640266655,3.6545250648045684]
[null,null,"Augmentation LV","total spend $0s",250574.9513369858,248962.83905563381,112812.10832335358,114223.46561118843,115070.08464925773,115702.90095448565,116584.12155675748]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981]
[null,null,"Volume of GSL breaches for residential customers","0's",2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858]
[null,null,"Volume of customer complaints relating to connection services","0's",11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714]
[null,null,"GSL payments","$0's",198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",40,40,41,41,41,41,41]
[null,null,"Overhead connections","0's",22.049973945889185,22.305430616803278,21.580956715034546,21.877087276201109,22.194371819990195,22.533374747224393,22.894675747925334]
[null,null,"Distribution substations installed","MVA added",4.485952119111082,4.5044205619057145,4.5243399398785211,4.5457489338542025,4.5686872717947313,4.5931957575055762,4.6193163001369841]
[null,null,"Distribution substations installed","0's",6.398640461177175,6.4249833471873128,6.4533958077918934,6.4839330162703996,6.5166516395105223,6.5516098789539399,6.5888675126761536]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",1.7286011398507786,1.7357177051681092,1.7433933687852534,1.7516430358362594,1.7604820149553986,1.7699260293387213,1.7799912281119796]
[null,null,"Augmentation HV","total spend $0s",6463491.1606027642,6538461.4717267621,2461361.2534448812,2535299.9991582166,2597304.0412936481,2654785.1322450954,2718277.8654255047]
[null,null,"Augmentation LV","net circuit KM added",1.0312756185389371,1.0355213292065446,1.0401005953900382,1.0450223094249489,1.0502956043732157,1.0559298606224581,1.061934712668029]
[null,null,"Augmentation LV","total spend $0s",314709.64313360647,321017.14121983654,149325.88486703273,155198.00461221856,160476.58774627361,165607.58423323548,171250.39576184683]
[null,"SUBDIVISION","Underground connections","0's",283,283,283,283,283,283,283]
[null,null,"Overhead connections","0's",13,13,13,13,13,13,13]
[null,null,"Distribution substations installed","MVA added",0.6508862190812722,0.6508862190812722,0.6508862190812722,0.6508862190812722,0.6508862190812722,0.6508862190812722,0.6508862190812722]
[null,null,"Distribution substations installed","0's",1.6734982332155477,1.6734982332155477,1.6734982332155477,1.6734982332155477,1.6734982332155477,1.6734982332155477,1.6734982332155477]
[null,null,"Distribution substations installed ","total spend $0s",383944.30031411821,380456.62861302367,140352.05965656566,141730.92699240509,142403.6119145831,142808.85547442542,143517.75712069013]
[null,null,"Augmentation HV ","net circuit KM added",0.30082135633181634,0.30082135633181634,0.30082135633181634,0.30082135633181634,0.30082135633181634,0.30082135633181634,0.30082135633181634]
[null,null,"Augmentation HV","total spend $0s",408250.11707518273,404541.65629291104,149237.12824922227,150703.28558200996,151418.55521359248,151849.45295218175,152603.23202858836]
[null,null,"Augmentation LV","net circuit KM added",3.9067816254416958,3.9067816254416958,3.9067816254416958,3.9067816254416958,3.9067816254416958,3.9067816254416958,3.9067816254416958]
[null,null,"Augmentation LV","total spend $0s",1104858.3203787073,1094822.0127826547,494775.12333430076,499635.96583152504,502007.34368055809,503435.92572482629,505934.97632886277]
[null,null,"Cost per lot","$0's",41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474]
[null,"EMBEDDED GENERATION","Underground connections","0's",1506,1583,1663,1746,1831,1918,2006]
[null,null,"Overhead connections","0's",1268.5576281753874,1332.8927909858803,1400.1994682198401,1469.7992451267346,1541.9335446245177,1615.226134246876,1689.5127317620963]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Underground connections","0's",130,131,132,133,134,136,137]
[null,null,"Overhead connections","0's",83.068358188594658,83.995553869858782,84.922749551122877,85.849945232387455,86.777140913651579,86.704336594915674,87.631532276179769]
[null,null,"Distribution substations installed","MVA added",0.83593459796918868,0.84349559651783057,0.85105659506647235,0.85861759361511603,0.86617859216375803,0.87373959071239982,0.8813005892610416]
[null,null,"Distribution substations installed","0's",2.6540239244978703,2.6780294759966838,2.702035027495497,2.7260405789943163,2.7500461304931298,2.774051681991943,2.7980572334907561]
[null,null,"Distribution substations installed ","total spend $0s",239133.71333417553,241092.07124301797,246118.34257615238,250910.82997267912,254487.51122353366,257604.3111681584,261287.52787992108]
[null,null,"Augmentation HV ","net circuit KM added",0.10043821789271629,0.10134667798224951,0.10225513807178273,0.10316359816131616,0.10407205825084939,0.10498051834038259,0.10588897842991581]
[null,null,"Augmentation HV","total spend $0s",300809.66850229178,300347.66928373132,303679.92789713555,306663.38488488522,308118.87409654597,308995.70009635558,310529.551479446]
[null,null,"Augmentation LV","net circuit KM added",3.4249349363168622,3.4559133503525965,3.4868917643883308,3.5178701784240727,3.548848592459807,3.5798270064955413,3.6108054205312752]
[null,null,"Augmentation LV","total spend $0s",92626.09971181002,92731.181913561624,94010.090269461318,95186.221342657023,95891.737207714774,96419.084128738046,97153.434630631236]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981,3.2737995213295981]
[null,null,"Volume of GSL breaches for residential customers","0's",2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858,2043.7142857142858]
[null,null,"Volume of customer complaints relating to connection services","0's",11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714,11.714285714285714]
[null,null,"GSL payments","$0's",198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713,198191.85714285713]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",40,40,18,19,19,20,20]
[null,null,"Overhead connections","0's",22.049973945889185,22.305430616803278,9.8937038217368922,9.7085583433690772,10.544766019906433,10.40289656620655,11.283535130279233]
[null,null,"Distribution substations installed","MVA added",4.485952119111082,4.5044205619057145,2.0165974586564244,2.0755080130955101,2.135962310817713,2.1980015398108783,2.2616680038148411]
[null,null,"Distribution substations installed","0's",6.4828330988242433,6.5095226017555659,2.9142675634650481,2.9994016179639331,3.0867665990947017,3.1764220293051619,3.2684290434620094]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",1.115468256186005,1.1200605837747986,0.50144325906945997,0.51609184462862534,0.53112429443384024,0.54655085021122185,0.5623820311276384]
[null,null,"Augmentation LV","total spend $0s",116333.762132348,119569.24588723894,124438.23738919394,129331.67051018213,133730.48978856133,138006.3201943629,142708.66313487236]
[null,"SUBDIVISION","Underground connections","0's",283,283,278,278,278,278,278]
[null,null,"Overhead connections","0's",13,13,12,12,12,12,12]
[null,null,"Distribution substations installed","MVA added",0.6508862190812722,0.6508862190812722,0.63769257950530045,0.63769257950530045,0.63769257950530045,0.63769257950530045,0.63769257950530045]
[null,null,"Distribution substations installed","0's",1.6734982332155477,1.6734982332155477,1.6395759717314486,1.6395759717314486,1.6395759717314486,1.6395759717314486,1.6395759717314486]
[null,null,"Distribution substations installed ","total spend $0s",141926.64851343972,141708.67014514911,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",3.9088734982332154,3.9088734982332154,3.8296395759717314,3.8296395759717314,3.8296395759717314,3.8296395759717314,3.8296395759717314]
[null,null,"Augmentation LV","total spend $0s",408415.59144190286,407788.32542005705,412312.60277858394,416363.30485960416,418339.45306713169,419529.93810402189,421612.4802740523]
[null,null,"Cost per lot","$0's",41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474,41903.157244932474]
[null,"EMBEDDED GENERATION","Underground connections","0's",1506,1583,1663,1746,1831,1918,2006]
[null,null,"Overhead connections","0's",1268.5576281753874,1332.8927909858803,1400.1994682198401,1469.7992451267346,1541.9335446245177,1615.226134246876,1689.5127317620963]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,646911.81824752677,647279.21387235867,246118.34257615238,250910.82997267912,254487.51122353366,257604.3111681584,261287.52787992108]
[null,null,"Complex connection LV",null,250574.9513369858,248962.83905563381,112812.10832335358,114223.46561118843,115070.08464925773,115702.90095448565,116584.12155675748]
[null,null,"Complex connection HV",null,813759.49415093532,806367.46890944813,364415.91347656265,367996.06186186225,369742.64891585521,370794.84011562669,372635.46177533525]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,314709.64313360647,321017.14121983654,149325.88486703273,155198.00461221856,160476.58774627361,165607.58423323548,171250.39576184683]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,3895069.6114017367,3736074.7828885969,1332652.5025214679,1299695.6514745415,1259596.4302904543,1216781.3958284887,1176191.6415085017]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,814471.54863794439,804878.66417021456,296092.43014492112,298140.49754520558,298667.93673426996,298604.40694967052,299144.6025553451]
[null,null,"Complex connection HV (customer connected at HV)",null,1753950.0005630832,1997508.0246679503,832616.32077849249,937463.85013846948,1039039.6742689236,1139399.3294669364,1242941.6213616582]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,1104858.3203787073,1094822.0127826547,494775.12333430076,499635.96583152504,502007.34368055809,503435.92572482629,505934.97632886277]
[null,null,"Complex connection HV (no upstream asset works)",null,408250.11707518273,404541.65629291104,149237.12824922227,150703.28558200996,151418.55521359248,151849.45295218175,152603.23202858836]
[null,null,"Complex connection HV (with upstream asset works)",null,383944.30031411821,380456.62861302367,140352.05965656566,141730.92699240509,142403.6119145831,142808.85547442542,143517.75712069013]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,239133.71333417553,241092.07124301797,246118.34257615238,250910.82997267912,254487.51122353366,257604.3111681584,261287.52787992108]
[null,null,"Complex connection LV",null,92626.09971181002,92731.181913561624,94010.090269461318,95186.221342657023,95891.737207714774,96419.084128738046,97153.434630631236]
[null,null,"Complex connection HV",null,300809.66850229178,300347.66928373132,303679.92789713555,306663.38488488522,308118.87409654597,308995.70009635558,310529.551479446]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,116333.762132348,119569.24588723894,124438.23738919394,129331.67051018213,133730.48978856133,138006.3201943629,142708.66313487236]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1439829.0981804342,1391575.673095912,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,301072.88248103164,299793.13422287104,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,648355.1000403025,744011.75979476457,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,408415.59144190286,407788.32542005705,412312.60277858394,416363.30485960416,418339.45306713169,419529.93810402189,421612.4802740523]
[null,null,"Complex connection HV (no upstream asset works)",null,150911.39736752457,150679.61975212122,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,141926.64851343972,141708.67014514911,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,407778.10491335124,406187.14262934076,0,0,0,0,0]
[null,null,"Complex connection LV",null,157948.85162517577,156231.65714207216,18802.018053892261,19037.244268531405,19178.347441542955,19283.81682574761,19430.686926126247]
[null,null,"Complex connection HV",null,512949.82564864354,506019.79962571687,60735.985579427121,61332.67697697704,61623.774819309212,61799.140019271123,62105.910295889225]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,198375.88100125847,201447.8953325976,24887.647477838789,25866.334102036428,26746.097957712274,27601.264038872578,28541.732626974474]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,2455240.5132213025,2344499.1097926847,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,513398.66615691275,505085.52994734352,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,1105594.9005227806,1253496.2648731859,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,696442.72893680434,687033.68736259767,82462.520555716808,83272.660971920865,83667.890613426382,83905.987620804401,84322.496054810472]
[null,null,"Complex connection HV (no upstream asset works)",null,257338.71970765814,253862.03654078979,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,242017.65180067849,238747.95846787459,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,196.64567955596092,198.56104706154454,200.47641456712816,202.39178207271226,204.30714957829588,206.2225170838795,208.13788458946311]
[null,null,"Complex connection LV",null,4.4226786326337448,4.4345068083142296,4.4463349839947144,4.4581631596752018,4.4699913353556866,4.4818195110361749,4.4936476867166597]
[null,null,"Complex connection HV",null,12,12,12,12,12,12,12]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,26.325850089187895,27.099647761399581,27.893703821736892,28.708558343369077,29.544766019906433,30.40289656620655,31.283535130279233]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,30.047525102874356,29.085203945097682,28.122882787321011,27.160561629543942,26.198240471767271,25.235919313990593,24.273598156213922]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,2.654563330894244,2.6473457066328807,2.6399391215631769,2.6323385381341722,2.624538782422237,2.6165345403925455,2.6083203540570183]
[null,null,"Complex connection HV (customer connected at HV)",null,3.022035422932686,3.4732332036731339,3.9244309844134726,4.3756287651539196,4.8268265458942583,5.2780243266347071,5.7292221073751541]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,290,290,290,290,290,290,290]
[null,null,"Complex connection HV (no upstream asset works)",null,3,3,3,3,3,3,3]
[null,null,"Complex connection HV (with upstream asset works)",null,3,3,3,3,3,3,3]
[null,"EMBEDDED GENERATION","Simple connection LV",null,2774.5576281753874,2915.8927909858803,3063.1994682198401,3215.7992451267346,3372.9335446245177,3533.226134246876,3695.5127317620963]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,196.64567955596092,198.56104706154454,200.47641456712816,202.39178207271226,204.30714957829588,206.2225170838795,208.13788458946311]
[null,null,"Complex connection LV",null,4.4226786326337448,4.4345068083142296,4.4463349839947144,4.4581631596752018,4.4699913353556866,4.4818195110361749,4.4936476867166597]
[null,null,"Complex connection HV",null,12,12,12,12,12,12,12]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,26.325850089187895,27.099647761399581,27.893703821736892,28.708558343369077,29.544766019906433,30.40289656620655,31.283535130279233]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,30.047525102874356,29.085203945097682,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,2.654563330894244,2.6473457066328807,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,3.022035422932686,3.4732332036731339,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,290,290,290,290,290,290,290]
[null,null,"Complex connection HV (no upstream asset works)",null,3,3,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,3,3,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,2774.5576281753874,2915.8927909858803,3063.1994682198401,3215.7992451267346,3372.9335446245177,3533.226134246876,3695.5127317620963]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RESIDENTIAL","Simple connection LV",null,59536.463081762311,59999.926163524506,60463.3892452867,60926.852327049011,61390.315408811206,61853.778490573401,62317.241572335595]
[null,null,"Complex connection LV",null,205.74417364819828,207.48834729639611,209.23252094459394,210.97669459279223,212.72086824099006,214.46504188918834,216.20921553738617]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,9892.694618634916,9914.6358811057089,9937.1515761795745,9960.2570177913876,9983.9679344429696,10008.300480568058,10033.271248211999]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1161.6999999999971,1197.3999999999942,1233.0999999999913,1268.8000000000029,1304.5,1340.1999999999971,1375.8999999999942]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,532.36772126325127,533.37832630225955,534.4153894579789,535.47961608361152,536.57173062713389,537.69247715476206,538.84261988891274]
[null,null,"Complex connection HV (customer connected at HV)",null,66.793984817181808,70.587969634364526,74.381954451546335,78.175939268729053,81.969924085910861,85.763908903093579,89.557893720276297]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,19678.531375911356,21780.690949799387,23971.66830948311,26241.373000226853,28578.522266601281,30962.646607617218,33376.428980640434]
[null,null,"Complex connection HV (small capacity)",null,8,8,8,8,8,8,8]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]

{"sheet":"2.6 Non-network","index":7,"n_rows":109,"n_cols":11,"rows_kept":109,"cut":false,"hidden":false,"merged":[[55,1,56,3],[55,4,55,10],[5,1,5,2],[12,1,16,1],[19,1,29,1],[32,1,36,1],[39,1,49,1],[84,1,88,1],[62,4,62,10],[64,1,68,1],[69,1,73,1],[74,1,78,1],[79,1,83,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.6 NON-NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,1837591.4518855391,1844123.6254410108,1833868.2978900454,1848046.2913166545,1853986.1135087528,1856433.9229116766,1862599.6165540309]
[null,"MOTOR VEHICLES","Car",null,271200.27954879851,272164.32805505785,270650.79919322493,272743.25330036174,273619.87984175875,273981.13892014313,274891.10061903053]
[null,null,"Light commercial vehicle",null,775066.66898290801,777821.83525975514,773496.30220609449,779476.35295499617,781981.67490567046,783014.1217415994,785614.71265556186]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,491439.63654393016,493186.58034618228,490443.92803404079,494235.64568126079,495824.17291141581,496478.80730366189,498127.74087893008]
[null,null,"Heavy commercial vehicle",null,391249.35255180072,392640.1451960046,390456.640119071,393475.33654528297,394740.00916037738,395261.18259263376,396573.94645161269]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,838528.65529753128,841509.41290936037,836829.70784645155,843299.4015047634,846009.8576893172,847126.84064271103,849940.36635518377]
[null,"OTHER","Other expenditure",null,0,0,0,0,0,0,0]
[null,"OTHER - DNSP nominated","Non Motor Vehicle fleet costs",null,57921.340605039331,58127.236343730045,57803.985863060792,58250.879749901636,58438.104425968166,58515.259988494035,58709.604188973797]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,17677483.700782172,19558509.036888577,16967968.277827863,19835191.583408829,11293498.636348113,10963570.416846979,11590727.242323047]
[null,"MOTOR VEHICLES","Car",null,205904.28799428756,152371.23163350098,333519.31186681212,287456.43532624049,206395.04333343997,156346.743919614,329487.53559910838]
[null,null,"Light commercial vehicle",null,690542.45136299205,907916.97780466103,893036.80173328752,2031462.9950249842,1442944.0617916172,574544.42518108722,1065511.4278024551]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,1791173.9122296451,731033.27737376187,0,383709.24707888794,1554818.690107133,2110416.1851395285,1021900.7194006069]
[null,null,"Heavy commercial vehicle",null,155298.80558566141,8441.2579329468899,431095.66044411022,709305.52770450013,213046.96347697053,254153.05511366596,0]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,2104425.6424640412,5455089.3184040599,1054023.6480942804,816075.68478807632,8447037.7676402684,38689605.978530198,57651979.844545618]
[null,"OTHER","Other expenditure",null,1356391.0729420208,1256550.0802228728,1821407.9809878385,2090842.2568571263,1696206.1160026954,1509696.0344617569,1592410.203750964]
[null,"OTHER - DNSP nominated"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Employee numbers",null,null,359.72377268581113,363.50967772932512,363.74777875776726,363.74777875776726,363.74777875776726,363.74777875776726,363.74777875776726]
[null,"User numbers",null,null,679.46,679.46,679.46,679.46,679.46,679.46,679.46]
[null,"Number of devices",null,null,1100.8800000000001,1100.8800000000001,1100.8800000000001,1100.8800000000001,1100.8800000000001,1100.8800000000001,1100.8800000000001]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","UNITS",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"CAR","Average kilometres travelled ","0's",12612.452830188678,12612.452830188678,12612.452830188678,12612.452830188678,12612.452830188678,12612.452830188678,12612.452830188678]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395]
[null,null,"Number in fleet","0's",27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395,27.69687165429395]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.83849999999999991,0.83849999999999991,0.83849999999999991,0.83849999999999991,0.83849999999999991,0.83849999999999991,0.83849999999999991]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",14564.560975609756,14564.560975609756,14564.560975609756,14564.560975609756,14564.560975609756,14564.560975609756,14564.560975609756]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094]
[null,null,"Number in fleet","0's",116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094,116.38499539877094]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.49659999999999999,0.49659999999999999,0.49659999999999999,0.49659999999999999,0.49659999999999999,0.49659999999999999,0.49659999999999999]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",15954.315789473685,15954.315789473685,15954.315789473685,15954.315789473685,15954.315789473685,15954.315789473685,15954.315789473685]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018]
[null,null,"Number in fleet","0's",16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018,16.969642434733018]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",8856.375,8856.375,8856.375,8856.375,8856.375,8856.375,8856.375]
[null,null,"Number purchased","0's",1.2843424843401625,1.2843424843401625,1.2843424843401625,1.2843424843401625,1.2843424843401625,1.2843424843401625,1.2843424843401625]
[null,null,"Number leased","0's",25.901033189855646,25.901033189855646,25.901033189855646,25.901033189855646,25.901033189855646,25.901033189855646,25.901033189855646]
[null,null,"Number in fleet","0's",27.185375674195807,27.185375674195807,27.185375674195807,27.185375674195807,27.185375674195807,27.185375674195807,27.185375674195807]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.81926666666666659,0.81926666666666659,0.81926666666666659,0.81926666666666659,0.81926666666666659,0.81926666666666659,0.81926666666666659]
[]
[]
[null,"Table 2.6.4 intentionally omitted"]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"RECURRENT"]
[null,"IT & Communication",null,null,4061005.2796401596,6419429.6177145764,2408559.7913616518,4236879.8681914415,2300989.29858009,3229843.4659512709,5474554.3195811715]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NON-RECURRENT"]
[null,"IT & Communication",null,null,13616478.421142012,13139079.419174001,14559408.48646621,15598311.715217385,8992509.3377680238,7733726.9508957081,6116172.9227418723]

{"sheet":"2.10 Overheads","index":8,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",18742015.646296494,18808638.77890595,26125500.808186166,26270105.406973317,26041401.999035731,27475027.410255156,27429073.673977457]
[null,"Alternative Control Services","Total  ",1618038.150703755,1614327.5330407987,1959906.8234940688,1974570.0516718873,1988249.9759922801,1997150.9108820488,2005716.1480738393]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",13841380.007205471,13841380.007205475,16888822.31339984,16344413.225556737,14693398.930508742,19543828.309158821,23881618.209762186]
[null,"Alternative Control Services","Total  ",3215525.3334072065,3373066.5955392458,4066130.7535547926,4078534.4002418229,4600710.9260838609,4625186.3715513926,4649012.10392344]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total  ",913879.68344899255,912205.1788302291,908858.62033418345,915735.21567650291,918488.98172676656,919587.72266764753,922388.12292311876]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",20775151.933629278,20849002.352302324,22968962.272015493,23441853.724981967,23646518.243321817,23818304.187469143,24039054.119060211]
[null,"Alternative Control Services","Total  ",1872277.4240443846,1863241.5831877538,2369486.2218547445,2380823.7697724057,2391401.0311783934,2398283.1975472826,2404905.8038322316]
[null,"CAPEX"]
[null,"Standard Control Services","Total",10700855.966364648,10700855.96636465,9867722.6612343919,9549637.847894324,8584990.8837101553,11418977.233276244,13953440.969560349]
[null,"Alternative Control Services","Total",3727130.1144513972,3836621.9955546497,4388088.2162720785,4397678.6648317445,4801423.4138632091,4820347.7278046655,4838769.6862257468]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",1427483.715194429,1424868.1322926604,1419640.7945571051,1430382.0639440075,1434683.4575118907,1436399.6952494513,1440773.931632106]

{"sheet":"2.11 Labour","index":9,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"In-house labour expenditure",38368506.548017092,38504896.899408162,43092013.895688683,43545530.618365392,43579751.887868769,44451993.910393029,44591394.424387299]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",16817245.999640476,16877027.062227588,18887599.844335739,19086380.119524714,19101379.595903553,19483690.766802449,19544791.209515385]
[null,"Controllable non-labour expenditure",16715711.032258477,16775131.16367767,18773565.011631269,18971145.140924901,18986054.057211742,19366057.00521446,19426788.550935701]
[null,"Uncontrollable non-labour expenditure",194840.72435667677,195533.33392768109,218827.36537885599,221130.38769335789,221304.16815911824,225733.5370028149,226441.43260694394]
[null,"Total",{"$f":"SUM(C12:C16)","v":72096304.304272726},72352588.459241107,80972006.11703454,81824186.266508371,81888489.709143177,83527475.219412759,83789415.617445335]
[null,"CAPEX"]
[null,"In-house labour expenditure",27641162.231979832,31634126.808121096,27463776.75663586,25179234.159819983,22572404.654766254,20850689.669115324,21153463.361267529]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",33527940.458883859,41152262.696849525,39621125.021969222,36447530.111451305,28973867.523634948,46759347.116297752,58362482.805614054]
[null,"Controllable non-labour expenditure",39833140.038490169,48382156.501102738,40172415.649188526,42702641.702206001,41252223.842026077,54813746.34838216,68482247.685999289]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C19:C23)","v":101002242.72935386},121168546.00607336,107257317.42779361,104329405.97347729,92798496.020427287,122423783.13379523,147998193.8528809]

{"sheet":"2.14 Forecast price changes","index":10,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[[5,1,5,2],[11,4,11,8],[7,1,7,2],[8,1,8,2],[11,2,11,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"Power and Water must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,"DESCRIPTION",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"OPEX"]
[null,"Labour",-3.6689481894301101E-2,-2.3505133390157914E-3,1.6993474921973065E-2,1.4960465614464905E-2,7.190932197755742E-3,4.301082917910275E-3,7.4917581213205953E-3]
[null,"Non Labour",0,0,0,0,0,0,0]
[]
[null,"CAPEX"]
[null,"Labour",-3.6689481894301101E-2,-2.3505133390157914E-3,1.6993474921973065E-2,1.4960465614464905E-2,7.190932197755742E-3,4.301082917910275E-3,7.4917581213205953E-3]
[null,"Non Labour",0,0,0,0,0,0,0]

{"sheet":"2.16 Opex Summary","index":11,"n_rows":63,"n_cols":12,"rows_kept":63,"cut":false,"hidden":false,"merged":[[10,1,10,7],[10,9,10,10],[5,1,5,6],[7,9,7,11],[8,1,8,7],[8,9,8,10],[8,11,9,11],[9,1,9,7],[9,9,9,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nPower and Water's total forecast opex must reconcile to Table 2.16.1 (and if Power and Water owns any dual function assets Table 2.16.3). If Power and Water did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if Power and Water owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has Power and Water used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If Power and Water does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2021-22"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y1","v":"2019-20"},{"$f":"CRCP_y2","v":"2020-21"},{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Base year total opex, excluding category specific",null,null,73316067.873442486,72096304.304272726,72352588.459241107,73349889.592937753,73349889.592937753,73349889.592937753,73349889.592937753,73349889.592937753]
[null,"Increment from base year to final year",null,null,null,null,0,0,0,0,0,0]
[null,"Price growth",null,null,null,null,null,-972144.14848759933,-331123.72347887798,-20280.510716483583,166434.35285186424,492488.1308983998]
[null,"Output growth",null,null,null,null,null,17405.908331709568,290688.0909309464,569795.45777401398,843280.65894152946,1118476.8211717308]
[null,"Productivity growth",null,null,null,null,null,-1080506.6833341841,-1455229.2700223057,-1829102.4059158484,-2203088.4896984505,-2584601.7793202004]
[null,"Step changes",null,null,null,null,null,9657361.4475868754,9969961.5761408582,9818187.5750637781,11370959.104380071,11413162.851757646]
[null,"Category specific",null,null,0,0,0,635584.92210511921,652266.1568958048,669232.47698428109,679056.1715496718,701225.15483194636]
[null,"Total opex",{"$f":"SUM(C17:C23)","v":0},0,73316067.873442486,72096304.304272726,72352588.459241107,81607591.039139673,82476452.423404172,82557722.186127499,84206531.390962437,84490640.772277281]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y1","v":"2019-20"},{"$f":"CRCP_y2","v":"2020-21"},{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C30:C36)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,2017,2018,2019,2020,2021,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Base year total opex, excluding category specific"]
[null,"Increment from base year to final year"]
[null,"Price growth",null,null,null,null,"."]
[null,"Output growth"]
[null,"Productivity growth"]
[null,"Step changes"]
[null,"Category specific"]
[null,"Total opex",{"$f":"SUM(C43:C49)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y1","v":"2019-20"},{"$f":"CRCP_y2","v":"2020-21"},{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C56:C62)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":12,"n_rows":84,"n_cols":11,"rows_kept":84,"cut":false,"hidden":false,"merged":[[5,1,5,2],[36,1,36,3],[20,1,20,3],[21,1,21,3],[83,1,83,2],[67,1,67,3],[51,1,51,3],[52,1,52,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Cyber security",null,null,0,0,743397.84224605653,924773.50493553397,924773.50493553397,924773.50493553397,924773.50493553397]
[null,"Insurance premiums",null,null,0,0,712423.12059054617,838154.05107879743,970171.52809146198,1108789.8789547596,1254339.1473612224]
[null,"Cloud migration",null,null,0,0,780082.02342806803,785575.55880432203,791069.09418057615,796562.62955683016,802056.16493308404]
[null,"Future Network",null,null,0,0,2289334.5463017859,2038258.8892517858,3163077.832835786,3258063.7816825295,3400300.3823273862]
[null,"Regulatory obligations",null,null,0,0,1132676.3334463199,1383751.99049632,1132676.3334463199,1283321.7276763201,1032246.0706263199]
[null,"OT capability uplift",null,null,0,0,3999447.5815740996,3999447.5815740996,2836419.2815740998,3999447.5815740996,3999447.5815740996]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E11:E20)","v":0},0,9657361.4475868754,9969961.5761408582,9818187.5750637781,11370959.104380073,11413162.851757646]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$21,0)-ROUND('2.16 Opex Summary'!H$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$21,0)-ROUND('2.16 Opex Summary'!I$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$21,0)-ROUND('2.16 Opex Summary'!J$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$21,0)-ROUND('2.16 Opex Summary'!K$22,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$21,0)-ROUND('2.16 Opex Summary'!L$22,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E27:E36)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E42:E51)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$21,0)-ROUND('2.16 Opex Summary'!H$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$21,0)-ROUND('2.16 Opex Summary'!I$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$21,0)-ROUND('2.16 Opex Summary'!J$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$21,0)-ROUND('2.16 Opex Summary'!K$48,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$21,0)-ROUND('2.16 Opex Summary'!L$48,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,"STEP CHANGE","DESCRIPTION",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E58:E67)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE \n($0's, real June 2024)"]
[null,"CATEGORY","DESCRIPTION",{"$f":"CRCP_y3","v":"2021-22"},{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Debt raising costs",null,null,null,null,635584.92210511921,652266.1568958048,669232.47698428109,679056.1715496718,701225.15483194636]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D74:D83)","v":0},{"$f":"SUM(E74:E83)","v":0},{"$f":"SUM(F74:F83)","v":0},635584.92210511921,652266.1568958048,669232.47698428109,679056.1715496718,701225.15483194636]

{"sheet":"3.1 Revenue","index":13,"n_rows":50,"n_cols":17,"rows_kept":50,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[28,2,28,8],[28,10,28,16],[41,2,41,8],[41,10,41,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DREV0101","Revenue from Fixed Customer Charges ",42227560.567329787,56267506.990602843,80116672.774423614,90003045.35378249,98487516.087189883,108247891.22617026,109583846.6552404,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",68491698.803007036,52695367.453912139,32707135.860193685,33228247.622908663,33047280.354578935,34199544.119199067,33362478.48255365,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",0,0,28209105.976479385,30805889.004903875,33229528.478021841,34746231.157427713,35912307.908027939,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",0,0,18920600.681816749,19889404.989821084,24389428.338373229,28486083.813872352,29087320.549637541,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",1031727.000796051,1127905.8590958074,1709765.3875743197,1854236.8569410492,2010915.8523301615,2180833.8832309716,2206387.3678384544,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",38582846.398754105,42015715.511569709,9313258.0769442003,9642861.8657477703,9926916.1225220952,10222804.123196743,10486395.820547488,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,8466957.7303129379,8989470.2886024788,13526518.447302124,14194528.57566233,14900230.638421349,15645716.995516481,16433194.811935214]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,2169404.1420696857,2147868.5169473556,3696223.839830779,3696223.8398307799,3696223.8398307799,3696223.8398307799,3696223.8398307804]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,10161351.231397282,10060479.730964484,11261017.252763133,11261017.252763132,11261017.25276313,11261017.252763132,11261017.252763132]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C12:C24)","v":150333832.76988697},152106495.81518051,170976538.75743195,185423685.69410494,201091585.2330161,218083388.32309714,220638736.78384545,null,{"$f":"SUM(K12:K24)","v":20797713.103779905},21197818.536514319,28483759.539896037,29151769.668256238,29857471.731015258,30602958.088110395,31390435.904529124]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DREV0201","Revenue from residential Customers ",91288458.458546475,96726646.990485623,93233506.584427655,100870485.01759309,107785089.68489666,115693237.50540303,116894402.74808134,null,10814640.998597533,11022692.556719314,14811322.388054671,15158682.200433737,15525641.510941846,15913288.32966207,16322770.364366176]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",29129311.808810841,23289788.552589588,52011063.090010807,56739647.822396107,63142757.763167061,69677642.569229528,70648523.518187314,null,2023815.4599837277,2062749.5272223137,2771740.942268488,2836744.6865962897,2905416.2149334387,2977959.1338191638,3054588.2214169153]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",14703763.759326508,16142809.311299318,16755700.798228335,18264233.040869333,19908066.938068599,21699297.138148163,22063873.678384546,null,5309163.5617366098,5411301.0022199266,7271229.172932433,7441756.3368885703,7621905.3589635789,7812210.3690919252,8013234.8042182261]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",14180571.742407091,14819345.101710157,7266502.8971908595,7695082.9563053548,8244754.9945536628,8832377.227085432,8825549.4713538177,null,1661280.7178411693,1693240.3586530418,2275227.1011303449,2328586.4459789721,2384956.5489586708,2444504.5436961651,2507406.7342214468]
["DREV0205","Revenue from unmetered supplies",1031727.000796051,1127905.8590958074,1709765.3875743197,1854236.8569410492,2010915.8523301615,2180833.8832309716,2206387.3678384544,null,110098.83604197224,112216.91230441105,150787.19260109492,154323.50148417783,158059.34375272351,162005.79593195024,166174.54230151232]
["DREV0206","Revenue from Other Customers",0,0,0,0,0,0,0,null,878713.52957889275,895618.17939531174,1203452.7429090061,1231676.4968744917,1261492.7534650003,1292989.9159091213,1326261.2380048481]
["DREV02","Total revenue by customer class",{"$f":"SUM(C32:C37)","v":150333832.76988697},152106495.81518051,170976538.75743198,185423685.69410491,201091585.23301613,218083388.32309714,220638736.78384548,null,{"$f":"SUM(K32:K37)","v":20797713.103779905},21197818.536514319,28483759.539896037,29151769.668256242,29857471.731015258,30602958.088110395,31390435.904529124]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"REVENUE \nForecast ($0's, real \", dms_DollarReal,\")\")","v":"REVENUE \nForecast ($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DREV0301","EBSS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",0,0,-146116.04117223303,-143132.25576068743,-138685.57550559356,-131410.14196234557,-125468.93729596009,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C45:C49)","v":0},0,-146116.04117223303,-143132.25576068743,-138685.57550559356,-131410.14196234557,-125468.93729596009,null,{"$f":"SUM(K45:K49)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":14,"n_rows":75,"n_cols":17,"rows_kept":75,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[66,2,66,8],[66,10,66,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are TWO tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DOPEX0101","Employee benefits expense",12379337.097712364,12423342.514880022,14769624.847237298,15118049.596331002,14886140.350608779,15169884.434898127,14942122.125431122,null,769075.57650576229,768472.527040974,1032105.0666010564,1071209.5231347668,1059531.199709282,1083724.6045953184,1080787.6807513097]
["DOPEX0102","Energy and materials",910308.26982561348,913544.18584023172,908463.88930868485,915487.40079298825,918429.87707476038,919642.47584917909,922696.8446024115,null,2193272.4079555199,2191552.6137088197,2543966.008559728,2564078.0447381027,2578495.2141473894,2591060.5245455387,2606258.2296328438]
["DOPEX0103","External service agreements",2361300.7332134922,2369694.5610092115,8886085.224520836,8838261.5185427796,8834026.85638134,9984071.5838358477,10157947.819239242,null,1249181.0449725825,1248201.5340069409,1571261.1699730556,1576560.9199321854,1652431.133980561,1660036.6915050065,1680048.7919088672]
["DOPEX0104","Other expenses",13492200.192374986,13540161.556807393,14177286.693064138,14407117.109562574,14582746.71267686,14739337.684420137,14930157.501327539,null,3804009.9800515184,3801027.1702307439,4358673.7714159722,4386119.3070463389,4399143.1868280247,4410122.643891599,4426933.646161438]
["DOPEX0105","Repairs and maintenance expense",27866913.546498168,27965973.386787627,27810452.24199751,28025460.271489993,28115537.155194975,28152657.970564246,28246160.175044663,null,0,0,0,0,0,0,0]
["DOPEX0106","Inter-group sales",15086244.46464809,15139872.253916612,15055678.143011192,15172076.526684847,15220841.234190742,15240937.241394892,15291556.30663229,null,2946137.5485901861,2943827.4158462207,3417210.6269012592,3444226.3431199971,3463592.3662309516,3480470.8591347062,3500885.3454737957]
["DOPEX0107"]
["DOPEX0108"]
["DOPEX0109"]
["DOPEX0110"]
["DOPEX0111"]
["DOPEX0112"]
["DOPEX0113"]
["DOPEX0114"]
["DOPEX0115"]
["DOPEX0116"]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C13:C61)","v":72096304.304272711},72352588.459241092,81607591.039139658,82476452.423404187,82557722.186127469,84206531.390962437,84490640.772277281,null,{"$f":"SUM(K13:K61)","v":10961676.55807557},10953081.260833699,12923216.643451072,13042194.137971392,13153193.100896208,13225415.323672168,13294913.693928255]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DOPEX0201","Opex for network services",72096304.304272711,72352588.459241092,81607591.039139658,82476452.423404187,82557722.186127469,84206531.390962437,84490640.772277281,null,3352825.9046719903,3319542.4788762936,4216487.6144452719,4216487.6144452719,4216487.6144452719,4216487.6144452728,4216487.6144452728]
["DOPEX0202","Opex for metering",0,0,0,0,0,0,0,null,6423872.9639646709,6460324.3388418574,6687767.8311198801,6806745.3256401988,6917744.288565021,6989966.5113409795,7059464.8815970635]
["DOPEX0203","Opex for connection services",0,0,0,0,0,0,0,null,1110151.0653903158,1099130.6212463342,1891471.8351161957,1891471.8351161953,1891471.8351161957,1891471.8351161955,1891471.8351161955]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",0,0,0,0,0,0,0,null,74826.624048592232,74083.821869214691,127489.36276972294,127489.36276972291,127489.36276972294,127489.36276972292,127489.36276972292]

{"sheet":"3.3 Assets (RAB)","index":15,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[8,18,8,24],[21,2,21,8],[21,10,21,16],[21,18,21,24],[97,2,97,8],[97,10,97,16],[97,18,97,24],[114,2,114,8],[114,10,114,16],[114,18,114,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",1002438842.807703,{"$f":"C18","v":1121209804.8245811},1220341939.269475,1287649998.9167221,1356293745.8829408,1411507559.0605507,1492385189.8683093,null,1108732594.9576221,{"$f":"K18","v":1232516182.4902391},1334854858.5141246,1404734483.2204292,1476140680.8792543,1534136645.5800788,1617546537.5643475,null,20914717.887212917,{"$f":"S18","v":33311709.321687736},51393319.17625013,54941248.768456362,58167082.227156833,64116699.470029145,71055093.876207665]
["DRAB0102","Inflation addition",85509102.68576175,53313116.564162679,34990804.531979427,35907585.355256945,36836249.781910703,37357587.303914063,38592170.537243158,null,88698607.596609786,55327851.554003119,36297817.332033798,37250471.166708842,38219406.026473299,38780430.459965549,40046485.832946584,null,1673177.4309770337,1495368.0402285806,1415512.6900221081,1476005.4180147052,1525644.8068183698,1651144.7317846613,1801134.2371456726]
["DRAB0103","Straight line depreciation",-58894596.024244539,-63247169.340348519,-68267876.221611008,-69466320.258374944,-72162965.094427288,-77406812.178452313,-81358119.735231757,null,-60416370.199160136,-64868412.268909223,-69954760.816415787,-71208707.414405271,-73964738.477443919,-79268749.907365099,-83276160.398204222,null,-1647426.6875066215,-2587451.1185804131,-3718560.792054106,-4091920.4357357654,-4429443.2114442363,-5060215.4938745787,-5672696.9777404368]
["DRAB0105","Actual additions (recognised in RAB)",92319581.88732487,109227198.99430914,100740883.81583539,102353932.22431892,90687795.378934592,121070054.49532163,147097450.90782094,null,95674662.705652595,112050302.49958976,103702046.25340527,105525341.20962483,93897759.762379572,124050351.94539675,150131281.94202423,null,12371240.691004405,19173692.932914227,5850977.6942382315,5841748.4764215238,8853415.6474981848,10347465.168268438,11266154.547522161]
["DRAB0106","Disposals ",-163126.53196379211,-161011.77322957019,-155752.47895677149,-151450.35498234408,-147266.88880805095,-143198.81302467271,-139242.95003214196,null,-173312.57048500705,-171065.76079824823,-165478.06271883255,-160907.30310310872,-156462.61058451369,-152140.51372842662,-147937.63651729218,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":1121209804.8245811},1220341939.269475,1287649998.9167221,1356293745.8829408,1411507559.0605507,1492385189.8683093,1596577448.6281092,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":1232516182.4902391},1334854858.5141246,1404734483.2204292,1476140680.8792543,1534136645.5800788,1617546537.5643475,1724300207.3045967,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":33311709.321687736},51393319.17625013,54941248.768456362,58167082.227156833,64116699.470029145,71055093.876207665,78449685.683135062]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",73401717.641139552,{"$f":"C31","v":86341271.477295652},95150434.538394362,101611179.61102736,108653364.80032471,115710723.44982173,121874684.80823112,null,95582959.012167186,{"$f":"K31","v":109765290.26486662},119420528.00903444,126501794.32776143,134220345.08786541,141955526.64077154,148711504.70004055,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0202","Inflation addition",6976572.8746273825,4495602.2866694601,2963345.0325815803,3062559.8104645694,3175454.4303241256,3285576.8814185713,3367231.3313745712,null,7646636.7209733753,4927381.7024343181,3247959.0409585736,3356702.8866055384,3480440.4525038255,3601139.5971232187,3690636.5359046087,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0203","Straight line depreciation",-3111326.5314520057,-3304199.5270363949,-3506740.893862152,-3632904.8125448213,-3770036.2198990425,-3907876.271138737,-4030105.0830170806,null,-3410153.3996533086,-3621550.8518154491,-3843545.2724167947,-3981826.5848602368,-4132128.7567026778,-4283207.6340213045,-4417175.8929452561,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0205","Actual additions (recognised in RAB)",9103439.396515144,7646514.5414360771,7031955.9443695303,7639576.9082941292,7678240.0529172458,6811833.8658625158,6896551.0392307946,null,9977777.8040147405,8380922.8299826039,7707339.0489531634,8373318.8729548203,8415695.4132327307,7466075.3799774963,7558929.2009604173,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0206","Disposals ",-29131.903534426383,-28754.239970429244,-27815.010455954303,-27046.71691653191,-26299.613845303171,-25573.117732957598,-24866.661108725595,null,-31929.872635365602,-31515.936433661635,-30486.49876793817,-29644.414596152372,-28825.556127750744,-28029.283810362707,-27254.975670577704,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":86341271.477295652},95150434.538394362,101611179.61102736,108653364.80032471,115710723.44982173,121874684.80823112,128083495.43471067,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":109765290.26486662},119420528.00903444,126501794.32776143,134220345.08786541,141955526.64077154,148711504.70004055,155516639.56828976,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",152048985.47158194,{"$f":"C38","v":178852800.10247764},197100660.63405576,210483858.81052175,225071489.01790443,239690550.49561155,252458972.01422319,null,197996619.33287409,{"$f":"K38","v":227374802.1315046},247375275.5627262,262043860.90674362,278032557.76697826,294055704.70896053,308050467.26754653,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0302","Inflation addition",14451716.686546776,9312476.4479449168,6138461.3369557932,6343981.1368418075,6577838.2312870296,6805952.8790724631,6975097.0990449302,null,15839729.546629928,10206891.786228001,6728028.8922587167,6953287.8090559468,7209605.6714190599,7459629.5547345709,7645019.2047568187,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0303","Straight line depreciation",-6444999.6237274548,-6844529.0114026396,-7264086.0780702932,-7525430.0418805825,-7809492.7591379415,-8095023.4064017022,-8348215.9397475822,null,-7064008.6006535273,-7501910.7256375281,-7961764.0848982688,-8248208.7886788798,-8559554.2650142964,-8872508.6584630962,-9150019.0289202072,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0305","Actual additions (recognised in RAB)",18857443.245529324,15839476.45616708,14566440.698970644,15825105.401718948,15905194.698046139,14110465.828184666,14285954.368189177,null,20668603.421223108,17360776.48543008,15965472.208814131,17345025.165313888,17432806.625531934,15465703.303156512,15658046.612432154,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0306","Disposals ",-60345.677452960961,-59563.361131208265,-57617.781390158161,-56026.28929749802,-54478.692488137174,-52973.782243785055,-51510.383069404561,null,-66141.568569004856,-65284.114798961557,-63151.672157159424,-61407.325456341248,-59711.08995441482,-58061.640841931134,-56457.689723616808,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":178852800.10247764},197100660.63405576,210483858.81052175,225071489.01790443,239690550.49561155,252458972.01422319,265320297.15864033,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":227374802.1315046},247375275.5627262,262043860.90674362,278032557.76697826,294055704.70896053,308050467.26754653,322147056.36609167,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",123230572.60250303,{"$f":"C45","v":135677674.33388674},142006530.49483415,148937216.46083799,156069493.92237207,163360287.82381254,170793309.87327948,null,161395449.52010235,{"$f":"K45","v":175038031.18294692},181974741.34017345,189571083.95158932,197388379.88207152,205379416.93904215,213526342.42418504,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0402","Inflation addition",11780207.757189307,7168945.404702724,4506553.635819112,4575321.7915759571,4647857.9000983937,4722833.1117782826,4799716.1650162423,null,12911635.96160819,7857485.6404952276,4939384.8721935684,5014757.8546727328,5094260.6823492525,5176436.8764630156,5260704.1504777409,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0403","Straight line depreciation",-6288087.0121928249,-6731333.7127300203,-6792683.3874445995,-6983057.2474601883,-7180180.828808452,-7383229.4571909299,-7591940.8182485588,null,-6892025.3419810357,-7377843.6022767872,-7445085.5968667632,-7653743.8843767885,-7869800.1691451082,-8092350.5711597456,-8321107.5821202043,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0405","Actual additions (recognised in RAB)",6971558.4334908938,5907607.0074388282,9232643.7895566076,9555403.7935579792,9838082.5688930023,10107970.722570501,10405146.149736755,null,7641140.6686252514,6475002.1949099274,10119391.612699376,10473151.050608242,10782979.664536685,11078789.183558771,11404506.77796744,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0406","Disposals ",-16577.447103657512,-16362.538464139916,-15828.071927272444,-15390.876139678079,-14965.738742472349,-14552.327690936039,-14150.320067047171,null,-18169.625407889336,-17934.075901832261,-17348.276610348392,-16869.09042197901,-16403.120770209833,-15950.003719138736,-15509.38533613302,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":135677674.33388674},142006530.49483415,148937216.46083799,156069493.92237207,163360287.82381254,170793309.87327948,178392081.04971686,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":175038031.18294692},181974741.34017345,189571083.95158932,197388379.88207152,205379416.93904215,213526342.42418504,221854936.38517389,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",121082277.65642171,{"$f":"C52","v":127912829.0010853},135017824.17409295,135665872.8395378,138638318.50028741,138697748.98800337,137965826.48082656,null,121082277.65642171,{"$f":"K52","v":127912829.0010853},135017824.17409295,135665872.8395378,138638318.50028741,138697748.98800337,137965826.48082656,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0502","Inflation addition",9686582.2125137355,5742027.6628949465,3667315.5171338106,3581664.494480026,3564382.0816652183,3464953.0801492259,3345895.4732324686,null,9686582.2125137355,5742027.6628949465,3667315.5171338106,3581664.494480026,3564382.0816652183,3464953.0801492259,3345895.4732324686,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0503","Straight line depreciation",-4957889.1574414382,-5155321.6631726259,-5384025.1328957332,-5425863.4104563817,-5511081.4702951321,-5546574.746397092,-5570454.1798636587,null,-4957889.1574414382,-5155321.6631726259,-5384025.1328957332,-5425863.4104563817,-5511081.4702951321,-5546574.746397092,-5570454.1798636587,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0505","Actual additions (recognised in RAB)",2110239.4037141493,6526561.6353447773,2372760.5312720402,4824425.7922877744,2013696.153803969,1357056.4269524035,1366129.0871605144,null,2110239.4037141493,6526561.6353447773,2372760.5312720402,4824425.7922877744,2013696.153803969,1357056.4269524035,1366129.0871605144,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0506","Disposals ",-8381.1141228523229,-8272.4620594482731,-8002.2500652659082,-7781.2155617656545,-7566.2774581123158,-7357.267881371773,-7154.0235728240541,null,-8381.1141228523229,-8272.4620594482731,-8002.2500652659082,-7781.2155617656545,-7566.2774581123158,-7357.267881371773,-7154.0235728240541,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":127912829.0010853},135017824.17409295,135665872.8395378,138638318.50028741,138697748.98800337,137965826.48082656,137100242.83778307,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":127912829.0010853},135017824.17409295,135665872.8395378,138638318.50028741,138697748.98800337,137965826.48082656,137100242.83778307,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",60587870.116141267,{"$f":"C59","v":64005782.016233139},67561021.751147121,67885296.196019426,69372666.231556877,69402404.412406847,69036160.675848275,null,60587870.116141267,{"$f":"K59","v":64005782.016233139},67561021.751147121,67885296.196019426,69372666.231556877,69402404.412406847,69036160.675848275,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0602","Inflation addition",4847029.6092913011,2873229.9472425575,1835073.1463567615,1792214.5783127458,1783566.7018176545,1733813.8267790584,1674239.0734474459,null,4847029.6092913011,2873229.9472425575,1835073.1463567615,1792214.5783127458,1783566.7018176545,1733813.8267790584,1674239.0734474459,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0603","Straight line depreciation",-2480858.058960998,-2579650.5102220196,-2694090.5123998248,-2715025.7985192402,-2757667.7180552315,-2775428.0546138482,-2787376.9875322119,null,-2480858.058960998,-2579650.5102220196,-2694090.5123998248,-2715025.7985192402,-2757667.7180552315,-2775428.0546138482,-2787376.9875322119,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0605","Actual additions (recognised in RAB)",1055934.1414851178,3265799.7216514037,1187296.0243888532,2414074.8666581693,1007625.2559953183,679051.96472909523,683591.79639510263,null,1055934.1414851178,3265799.7216514037,1187296.0243888532,2414074.8666581693,1007625.2559953183,679051.96472909523,683591.79639510263,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0606","Disposals ",-4193.7917235487566,-4139.4237579571691,-4004.2134734777183,-3893.610914222435,-3786.0589077751274,-3681.4734528787553,-3579.7728571641915,null,-4193.7917235487566,-4139.4237579571691,-4004.2134734777183,-3893.610914222435,-3786.0589077751274,-3681.4734528787553,-3579.7728571641915,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":64005782.016233139},67561021.751147121,67885296.196019426,69372666.231556877,69402404.412406847,69036160.675848275,68603034.785301462,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":64005782.016233139},67561021.751147121,67885296.196019426,69372666.231556877,69402404.412406847,69036160.675848275,68603034.785301462,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",347994354.97277731,{"$f":"C66","v":375535788.9049964},397925781.04676932,419198661.81374615,428844641.885948,424683103.00531447,416604045.47788435,null,347994354.97277731,{"$f":"K66","v":375535788.9049964},397925781.04676932,419198661.81374615,428844641.885948,424683103.00531447,416604045.47788435,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0702","Inflation addition",27839548.397822198,16857862.539192781,10810192.846142443,11106999.973218864,11065553.537780527,10633589.057081752,10102745.844059451,null,27839548.397822198,16857862.539192781,10810192.846142443,11106999.973218864,11065553.537780527,10633589.057081752,10102745.844059451,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0703","Straight line depreciation",-22348285.535282984,-23427732.582046077,-26611222.548982546,-27851243.101890091,-28595254.996794142,-29096027.890583135,-29391030.705994993,null,-22348285.535282984,-23427732.582046077,-26611222.548982546,-27851243.101890091,-28595254.996794142,-29096027.890583135,-29391030.705994993,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0705","Actual additions (recognised in RAB)",22094667.667706184,29003781.932472613,37116395.621461548,26431534.847025726,13408333.085746367,10422442.150094057,8936948.3772441745,null,22094667.667706184,29003781.932472613,37116395.621461548,26431534.847025726,13408333.085746367,10422442.150094057,8936948.3772441745,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0706","Disposals ",-44496.598026346197,-43919.747846387327,-42485.151644642952,-41311.646152647983,-40170.507366250837,-39060.84402274352,-37981.789356976391,null,-44496.598026346197,-43919.747846387327,-42485.151644642952,-41311.646152647983,-40170.507366250837,-39060.84402274352,-37981.789356976391,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":375535788.9049964},397925781.04676932,419198661.81374615,428844641.885948,424683103.00531447,416604045.47788435,406214727.20383602,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":375535788.9049964},397925781.04676932,419198661.81374615,428844641.885948,424683103.00531447,416604045.47788435,406214727.20383602,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"For easements:"]
["DRAB0801","Opening value",50996073.921066396,{"$f":"C72","v":55075759.83475171},57723748.467529498,59291128.290096283,60858508.112663068,62425887.935229853,63993267.757796638,null,50996073.921066396,{"$f":"K72","v":55075759.83475171},57723748.467529498,59291128.290096283,60858508.112663068,62425887.935229853,63993267.757796638,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0802","Inflation addition",4079685.9136853116,2472359.8015600098,1567379.8225667833,1567379.8225667833,1567379.8225667831,1567379.8225667833,1567379.8225667835,null,4079685.9136853116,2472359.8015600098,1567379.8225667833,1567379.8225667833,1567379.8225667831,1567379.8225667833,1567379.8225667835,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0803","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0804","Disposals ",0,175628.83121777981,0,0,0,0,0,null,0,175628.83121777981,0,0,0,0,0,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["DRAB0805","Closing value",{"$f":"SUM(C68+C69+C70+C71)","v":55075759.83475171},57723748.467529498,59291128.290096283,60858508.112663068,62425887.935229853,63993267.757796638,65560647.580363423,null,{"$f":"SUM(K68+K69+K70+K71)","v":55075759.83475171},57723748.467529498,59291128.290096283,60858508.112663068,62425887.935229853,63993267.757796638,65560647.580363423,null,{"$f":"SUM(S68+S69+S70+S71)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"For meters:"]
["DRAB0901","Opening value",0,{"$f":"C79","v":0},0,0,0,0,0,null,0,{"$f":"K79","v":0},0,0,0,0,0,null,18459324.479427431,{"$f":"S79","v":29400905.842930503},45359729.921540082,48491131.641892187,51338251.399943128,56589382.005999409,62713207.075052783]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,1476745.9583541946,1319811.4370751993,1249331.1260889908,1302721.9918268358,1346533.7032651012,1457299.9038703195,1589680.601659243]
["DRAB0903","Straight line depreciation",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-1454018.3589732125,-2283683.6733874837,-3282000.7722394676,-3611527.8950727554,-3909425.4077047058,-4466144.8574625971,-5006720.853241791]
["DRAB0905","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,10918853.764122089,16922696.31492186,5164071.3665025849,5155925.6612968706,7814022.3104958842,9132670.0226456523,9943505.0259624533]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":29400905.842930503},45359729.921540082,48491131.641892187,51338251.399943128,56589382.005999409,62713207.075052783,69239671.849432692]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",36329288.343468398,{"$f":"C86","v":60682789.049000055},88195864.742336631,104389808.20188439,126269788.78642267,144565343.70579812,206476292.4327594,null,36329288.343468398,{"$f":"K86","v":60682789.049000055},88195864.742336631,104389808.20188439,126269788.78642267,144565343.70579812,206476292.4327594,null,1172830.2420887772,{"$f":"S86","v":1868013.7269282723},2881972.3649286828,3080928.8674730109,3261823.2527909619,3595458.6892775199,3984541.5750706391]
["DRAB1002","Inflation addition",2906343.0674774712,2724060.2533935071,2424677.1889166189,2815285.8350560269,3356116.0041290103,3779920.2863668711,5428990.1693644403,null,2906343.0674774712,2724060.2533935071,2424677.1889166189,2815285.8350560269,3356116.0041290103,3779920.2863668711,5428990.1693644403,null,93826.419367102193,83855.439508719021,79377.407807798852,82769.645809705893,85553.263389522021,92590.896322181841,101001.82631090915]
["DRAB1003","Straight line depreciation",-4965803.8049874427,-5965735.1271392852,-10728265.567784952,-9102722.5127220806,-11253711.861318009,-13167010.301418211,-15958701.519060312,null,-4965803.8049874427,-5965735.1271392852,-10728265.567784952,-9102722.5127220806,-11253711.861318009,-13167010.301418211,-15958701.519060312,null,-92382.400334130478,-145095.95291519075,-208524.95249926735,-229461.76281852403,-248388.9566195299,-283760.64141562115,-318106.63694236323]
["DRAB1005","Actual additions (recognised in RAB)",26412961.44304163,30754750.56708236,24497531.838416077,28167417.26220433,26193150.776564442,71298038.742012605,98043719.17405352,null,26412961.44304163,30754750.56708236,24497531.838416077,28167417.26220433,26193150.776564442,71298038.742012605,98043719.17405352,null,693739.46580652345,1075199.1514068823,328104.04723579629,327586.50232676946,496471.12971656572,580252.63088655856,631769.78224786301]
["DRAB1006","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":60682789.049000055},88195864.742336631,104389808.20188439,126269788.78642267,144565343.70579812,206476292.4327594,293990300.25711703,null,{"$f":"SUM(K81+K82+K83+K84+K85)","v":60682789.049000055},88195864.742336631,104389808.20188439,126269788.78642267,144565343.70579812,206476292.4327594,293990300.25711703,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":1868013.7269282723},2881972.3649286828,3080928.8674730109,3261823.2527909619,3595458.6892775199,3984541.5750706391,4399206.5466870479]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",36767702.08260341,{"$f":"C93","v":37125110.104854703},39660073.420315236,40186976.693050928,42515474.625461392,52971509.244552121,53182630.347460315,null,36767702.08260341,{"$f":"K93","v":37125110.104854703},39660073.420315236,40186976.693050928,42515474.625461392,52971509.244552121,53182630.347460315,null,1282563.1656967106,{"$f":"S93","v":2042789.7518289629},3151616.8897813736,3369188.2590911728,3567007.5744227348,3931858.7747522136,4357345.2260842398]
["DRAB1102","Inflation addition",2941416.166608274,1666552.2205617684,1077806.0055065227,1062177.912740164,1098101.0722419645,1363568.3587010568,1330875.5591368221,null,2941416.166608274,1666552.2205617684,1077806.0055065227,1062177.912740164,1098101.0722419645,1363568.3587010568,1330875.5591368221,null,102605.05325573687,91701.163644662141,86804.156125318492,90513.780378163457,93557.840163746441,101253.93159215996,110451.80917552038]
["DRAB1103","Straight line depreciation",-8297346.3001993988,-9238667.2065994553,-5286762.1001709132,-6230073.3329015775,-5285539.2401193436,-7435642.050708659,-7680294.5017673615,null,-8297346.3001993988,-9238667.2065994553,-5286762.1001709132,-6230073.3329015775,-5285539.2401193436,-7435642.050708659,-7680294.5017673615,null,-101025.9281992785,-158671.49227773878,-228035.06731537048,-250930.77784448621,-271628.8471200018,-310309.9949963601,-347869.48755628074]
["DRAB1105","Actual additions (recognised in RAB)",5713338.1558424197,10107078.301498223,4735859.367400079,7496393.3525718749,14643472.78696811,6283194.7949157953,6479410.9158108933,null,5713338.1558424197,10107078.301498223,4735859.367400079,7496393.3525718749,14643472.78696811,6283194.7949157953,6479410.9158108933,null,758647.46107579395,1175797.4665854874,358802.28049985133,358236.31279788486,542922.20728573413,634542.51473622606,690879.73931184353]
["DRAB1106","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":37125110.104854703},39660073.420315236,40186976.693050928,42515474.625461392,52971509.244552121,53182630.347460315,53312622.320640668,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":37125110.104854703},39660073.420315236,40186976.693050928,42515474.625461392,52971509.244552121,53182630.347460315,53312622.320640668,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":2042789.7518289629},3151616.8897813736,3369188.2590911728,3567007.5744227348,3931858.7747522136,4357345.2260842398,4810807.2870153226]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" VALUE \nForecast\n($0's, real \", dms_DollarReal, \")\")","v":" VALUE \nForecast\n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",79871494.559217602,86869979.312111586,91915642.712577492,95967991.167935908,100195441.58157197,103863639.89999333,107016176.21272898,null,102674124.6385169,109665527.43451619,114785820.42500503,118829026.07781497,123075451.7818162,126719891.99078056,129809811.91863507,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",165450892.7870298,179947999.13157478,190399907.14853302,198794199.42418468,207551209.03078991,215149748.28502566,221680112.47019732,null,212685710.73218936,227168147.0608874,237774647.55624825,246150000.84931824,254946317.07900769,262495642.27455723,268896298.89836603,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",129454123.46819489,132751509.58370842,135525596.59283382,138614162.1289151,141792305.34526056,145028414.39469379,148324692.27152526,null,168216740.35152465,170648900.62106493,172976042.13319257,175668103.54946885,178478009.36084598,181370553.75543973,184347609.32802784,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",124497553.3287535,125723298.92469415,125932505.32678658,124161087.9954038,122112643.9879714,118311444.89809173,114166796.34974909,null,124497553.3287535,125723298.92469415,125932505.32678658,124161087.9954038,122112643.9879714,118311444.89809173,114166796.34974909,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",62296826.066187203,62910171.936447576,63014855.879983962,62128463.541876085,61103450.948252141,59201384.34361878,57127460.456618637,null,62296826.066187203,62910171.936447576,63014855.879983962,62128463.541876085,61103450.948252141,59201384.34361878,57127460.456618637,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",361765071.93888688,369872922.43669009,380894166.04492259,385246596.49129301,376923263.54929662,360169376.28818309,340832442.54338449,null,361765071.93888688,369872922.43669009,380894166.04492259,385246596.49129301,376923263.54929662,360169376.28818309,340832442.54338449,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",53035916.877909049,53927394.349580586,54467698.754686087,54467698.754686087,54467698.754686087,54467698.754686102,54467698.754686102,null,53035916.877909049,53927394.349580586,54467698.754686087,54467698.754686087,54467698.754686087,54467698.754686102,54467698.754686102,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,23930115.161178969,36060506.445160091,44356288.218551934,46042826.965926632,48745418.444715157,52975596.378399655,57711060.698457062]
["DRAB1209","“Other” assets with long lives",48506038.696234226,71715266.642274842,91144099.029800385,107365775.21678735,124097426.96461521,160420758.50141668,229704246.60771173,null,48506038.696234226,71715266.642274842,91144099.029800385,107365775.21678735,124097426.96461521,160420758.50141668,229704246.60771173,null,1520421.9845085246,2291137.6064197589,2818217.7688843291,2925373.5670057628,3097085.2145184958,3365853.4793361528,3666725.5817300072]
["DRAB1210","“Other” assets with short lives",36946406.093729056,36726039.542023212,37179166.83061479,37544689.520447701,42838854.723956332,46808864.226254731,45648545.20516219,null,36946406.093729056,36726039.542023212,37179166.83061479,37544689.520447701,42838854.723956332,46808864.226254731,45648545.20516219,null,1662676.4587628366,2505502.1571605061,3081897.254666293,3199078.8166088099,3386856.2342755841,3680771.1285141762,4009793.575470211]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",0,0,0,0,0,0,0,null,-6415341.617651633,-14039473.671079667,-4830604.7236713273,-243726.99101115938,-239129.56606432417,-234194.83054661637,-229866.14077328573,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,null,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,49.792725031645205,null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)",52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,null,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,52.300284796833004,null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers",44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,null,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,44.555321903731347,null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,null,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,54.343924174110775,null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,null,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,49.613725933874562,null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers",45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,null,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,45.619061322390586,null,0,0,0,0,0,0,0]
["DRAB1407","Meters",16,16,16,16,16,16,16,null,16,16,16,16,16,16,16,null,16,16,16,16,16,16,16]
["DRAB1408","“Other” assets with long lives",29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,null,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,null,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259,29.023808433625259]
["DRAB1409","“Other” assets with short lives",6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,null,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,null,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",27.750630030143952,27.623804221207845,27.13231976033018,27.385546524378451,27.51276509197519,27.366685421704656,27.324493842609325,null,32.187786706611455,31.614396978356876,30.78575773089975,30.812065478781605,30.720979435201876,30.373937510536287,30.157816347208485,null,"","","","","","",""]
["DRAB1502","Underground network assets less than 33kV (cables)",27.750630030143963,27.623804221207852,27.132319760330184,27.385546524378459,27.512765091975201,27.366685421704659,27.324493842609332,null,32.187786706611455,31.614396978356886,30.785757730899761,30.812065478781605,30.72097943520189,30.373937510536287,30.157816347208495,null,"","","","","","",""]
["DRAB1503","Distribution substations including transformers",21.576939706909734,20.19153164359442,20.461860453078469,20.360752578878632,20.255437260361607,20.146322998881804,20.037574251644205,null,25.397183338364538,23.600019881953852,23.74374493602804,23.462602646173092,23.186551623604096,22.915964263697795,22.654665193078753,null,"","","","","","",""]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",25.799856539571334,25.076184369772307,23.450211791935573,23.157109075698266,22.163047287575001,21.264562191489002,20.417366493985071,null,25.799856539571334,25.076184369772307,23.450211791935573,23.157109075698266,22.163047287575001,21.264562191489002,20.417366493985071,null,"","","","","","",""]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",25.79985653957133,25.07618436977231,23.450211791935573,23.157109075698258,22.163047287574994,21.264562191488995,20.417366493985071,null,25.79985653957133,25.07618436977231,23.450211791935573,23.157109075698258,22.163047287574994,21.264562191488995,20.417366493985071,null,"","","","","","",""]
["DRAB1506","Zone substations and transformers",16.803785163390216,16.265676465831323,14.712988315652593,14.005464140339299,13.108555742937213,12.239809807156828,11.419735046511965,null,16.803785163390216,16.265676465831323,14.712988315652593,14.005464140339299,13.108555742937213,12.239809807156828,11.419735046511965,null,"","","","","","",""]
["DRAB1507","Meters","","","","","","","",null,"","","","","","","",null,16,16,13.992071381321827,13.14302096619854,13.140290040193944,12.547176748934112,12.178488650144516]
["DRAB1508","“Other” assets with long lives",12.220134228431021,14.327120240406806,9.2504301028469431,12.996745242284476,11.840111606402687,14.53452442763596,17.135557688906047,null,12.220134228431021,14.327120240406806,9.2504301028469431,12.996745242284476,11.840111606402687,14.53452442763596,17.135557688906047,null,20.220450217487354,19.284596635548311,13.992071381321834,13.14302096619854,13.140290040193946,12.547176748934113,12.178488650144514]
["DRAB1509","“Other” assets with short lives",4.4743353792480045,4.1124461299583963,6.9300161354856167,6.2132396230759506,6.9300161354856167,6.309397958880715,5.9520557683345254,null,4.4743353792480045,4.1124461299583963,6.9300161354856167,6.2132396230759506,6.9300161354856167,6.309397958880715,5.9520557683345254,null,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167,6.9300161354856167]

{"sheet":"3.4 Operational data","index":16,"n_rows":87,"n_cols":10,"rows_kept":87,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DOPED01","TOTAL ENERGY DELIVERED"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",1700.0625107318338,1722.330755343871,1110.24737858667,1110.087506262807,1101.9643956073696,1109.952347511784,1123.4201054116265]
["DOPED0202","Energy Delivery at On-peak times","GWh",0,0,83.981459255047014,85.288736831196303,86.54115514008123,83.751881235770782,79.100673300090065]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",0,0,376.47038316289786,381.46613171072011,386.30568973074276,374.25420138380764,354.02704246627536]
["DOPED0204","Energy Delivery at Off-peak times","GWh",0,0,173.2345877682487,176.26698960821884,179.14332582383085,172.69457908603869,162.31935463307755]
["DOPED0205","Controlled load energy deliveries","GWh",0,0,0,0,0,0,0]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",16,15.994163,16.314046260000001,16.6403271852,16.973133728903999,17.312596403482079,17.658848331551724]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh"]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh"]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh"]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh"]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",30.042874547921368,32.084538096941479,34.240303533619866,36.49115450678481,38.815081765492252,41.366984622070291,44.108540606451342]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",136.38272871297403,154.2181736439185,172.7732639884251,191.97361626847106,211.73696643319897,231.67672488376371,251.67216409959457]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",664.88465993639284,636.76752081055997,602.85941270374326,582.51419263002776,562.61676484669954,539.67765803829047,513.0141323030681]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",102.74439024798203,52.438935115029757,35.576298720509286,19.042398938580561,2.8322951321915495,0,0]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",623.42776199935963,695.60624611539811,677.14542318002555,685.82800247457885,694.03478619471923,675.35971038000662,646.77448405263556]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",309.00569854809919,337.51805330288295,428.35267416858557,465.72477036975528,494.4707201284142,525.61564079910397,559.07855945536573]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",16,15.994163,16.314046260000001,16.6403271852,16.973133728903999,17.312596403482079,17.658848331551724]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",396.54041093929027,412.29648109143727,422.62502040424624,435.1083776270554,443.43053594431569,448.81014847967856,452.80560758089513]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",386.97454855782598,403.41896166179509,414.05331792642608,426.80285210105694,435.25489570086893,440.59096851878337,444.54288790255129]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",344.74768305547269,357.344851972387,366.05254308445723,376.78204163949744,383.87494410100288,388.45808870569709,391.77000343828399]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",336.02611884372124,349.20723707202376,358.16627563409253,369.1140975750215,376.31013910980028,380.84801607448787,384.1157668445021]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",351.55226353427832,367.99948989665114,378.50118146990025,391.46657108308085,402.65508373771189,410.83509608490567,417.63350837051854]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",349.9999892505557,366.44614418435708,376.88611942581161,387.06128919682959,394.89787883648046,403.0768197551028,409.87416061214424]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",252.06452771110733,261.7841796398983,267.50000929651634,276.79619364916681,284.81835722253726,290.68342607547521,295.55788768425964]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",250.9515470496782,260.67043076418344,266.34200981090481,273.63760653672466,279.25644130835434,285.12074194700654,289.99443534150527]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",407.20712593578213,423.53133064309492,434.22665437479799,447.00125810650115,455.50183869855846,461.00753941063886,465.13085109832878]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",397.3844878665459,414.40164134470785,425.40391384726007,438.44546634981219,447.07546627854089,452.53558632729232,456.61331735165356]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",353.97659784135726,367.01548385887992,376.03409904259252,387.00950808630506,394.25376892830218,398.9460706810803,402.36541853263901]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",345.02221155626893,358.6483185117475,367.91860741384852,379.1126195959497,386.45932442463959,391.10433477411078,394.47747961138668]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",365.19487197689489,380.1873021361377,389.42316961618138,403.92840024926227,416.64010299052779,426.25032078485953,434.45110864727849]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",363.58236888550709,378.56981256553934,387.73736844074705,399.31907732990953,408.50397987715962,418.09335110070225,426.2731910922646]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",261.84472320743362,272.59429563161075,279.21641261480204,289.61666297872102,298.73095384420839,305.62148000274425,311.50144490009865]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",260.68855849090858,271.43455560949167,278.00769317201565,286.31177844554514,292.89735357192342,299.7729327392035,305.63787801315368]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.96264887305527858,0.96034357224290035,0.958038271430522,0.95573297061814366,0.95342766980576543,0.95112236899338709,0.94881706818100875]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0,0,0,0,0,0,0]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.97381518943347412,0.97433745187025522,0.97485971430703644,0.97538197674381755,0.97590423918059876,0.97642650161737987,0.97694876405416109]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0,0,0,0,0,0,0]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0.96301715935756871,0.96789295330206571,0.9727687472465627,0.9776445411910597,0.9825203351355567,0.9873961290800537,0.99227192302455069]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.96454988424251831,0.96039442797014274,0.95623897169776717,0.95208351542539149,0.94792805915301592,0.94377260288064035,0.93961714660826479]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0.95589867225558356,0.95459960033015212,0.95330052840472079,0.95200145647928935,0.95070238455385803,0.9494033126284267,0.94810424070299526]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW ",0,0,0,0,0,0,0]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW ",0,0,0,0,0,0,0]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA",0,0,0,0,0,0,0]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA",2854.06,2569.0300000000002,993.49,998.46,1003.45,1008.47,1013.51]

{"sheet":"3.5 Physical assets","index":17,"n_rows":95,"n_cols":10,"rows_kept":95,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",1189.0373781056833,1197.9015559407108,1202.4792206927909,1205.6237695332031,1209.2894274087791,1212.163877788292,1214.8635386117157]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0104","Overhead 11 kV","km",349.77599964562791,352.38355153623615,353.73015114208903,354.6551748077386,355.73349174831378,356.57906125978502,357.37321338704743]
["DPA0105","Overhead SWER","km",9,9,9,9,9,9,9]
["DPA0106","Overhead 22 kV","km",3146.9788933633936,3170.439367413665,3182.5548943272433,3190.877449204108,3200.5792030573862,3208.1868988631809,3215.3319859621997]
["DPA0107","Overhead 33 kV","km",0,0,0,0,0,0,0]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",372,372,372,372,372,372,372]
["DPA0110","Overhead 132 kV","km",354,354,354,354,354,354,354]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0112","Overhead 110kV","km",0,0,0,0,0,0,0]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D13:D26)","v":5420.7922711147048},5455.7244748906123,5473.764266162123,5486.1563935450495,5500.6021222144791,5511.9298379112579,5522.5687379609626]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",709.60303376383138,714.89306719707679,717.62496179975528,719.50159027087204,721.68921027100441,723.40464726841446,725.0157719863663]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",0,0,0,0,0,0,0]
["DPA0204","Underground 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0205","Underground 11 kV","km",712.61834410560402,717.93085643445818,720.67435965442849,722.55896246749046,724.75587830331744,726.47860469306772,728.09657555004776]
["DPA0206","Underground SWER","km",78,78,78,78,78,78,78]
["DPA0207","Underground 22 kV","km",102.52055162027024,103.28483407096577,103.67952705888816,103.95065468502683,104.26671309864369,104.51455243821285,104.74732116516907]
["DPA0208","Underground 33 kV","km",0,0,0,0,0,0,0]
["DPA0209","Underground 66 kV","km",39,39,39,39,39,39,39]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",0,0,0,0,0,0,0]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D29:D40)","v":1641.7419294897056},1653.1087577025007,1658.9788485130721,1663.0112074233894,1667.7118016729655,1671.3978043996949,1674.8596687015831]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
["DPA0302","Overhead 6.6 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0303","Overhead 7.6 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0304","Overhead 11 kV","MVA",6.8,6.8,6.8,6.8,6.8,6.8,6.8]
["DPA0305","Overhead SWER","MVA",0.9,0.9,0.9,0.9,0.9,0.9,0.9]
["DPA0306","Overhead 22 kV","MVA",9.6999999999999993,9.6999999999999993,9.6999999999999993,9.6999999999999993,9.6999999999999993,9.6999999999999993,9.6999999999999993]
["DPA0307","Overhead 33 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0308","Overhead 44 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0309","Overhead 66 kV","MVA",46.72,46.72,46.72,46.72,46.72,46.72,46.72]
["DPA0310","Overhead 110 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0311","Overhead 132 kV","MVA",116.41,116.41,116.41,116.41,116.41,116.41,116.41]
["DPA0312","Overhead 220 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0313","Other ","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
["DPA0402","Underground 5 kV","MVA","                 -  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0403","Underground 6.6 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0404","Underground 7.6 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0405","Underground 11 kV","MVA",5.0999999999999996,5.0999999999999996,5.0999999999999996,5.0999999999999996,5.0999999999999996,5.0999999999999996,5.0999999999999996]
["DPA0406","Underground SWER","MVA",0.7,0.7,0.7,0.7,0.7,0.7,0.7]
["DPA0407","Underground 12.7 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0408","Underground 22 kV","MVA",10.9,10.9,10.9,10.9,10.9,10.9,10.9]
["DPA0409","Underground 33 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0410","Underground 66 kV","MVA",53.8,53.8,53.8,53.8,53.8,53.8,53.8]
["DPA0411","Underground 110 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0412","Underground 132 kV","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
["DPA0413","Other","MVA","-  ","-  ","-  ","-  ","-  ","-  ","-  "]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",1472.5,1489,1505,1522,1538,1554,1571]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",141,143,144,146,148,149,151]
["DPA0503","Cold spare capacity included in DPA0501","MVA",92.1,92.1,92.1,92.1,92.1,92.1,92.1]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",618,618,618,618,618,618,618]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",968.2,968.2,954.2,955.7,951.7,951.7,951.7]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",134,134,134,134,134,134,134]
["DPA0604","Total zone substation transformer  capacity ","MVA",1896.2,1896.2,2007.2,2008.7,2004.7,2004.7,2004.7]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",176,111,236,236,236,236,236]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
["DPA0701","Public lighting luminaires","0's"]
["DPA0702","Public lighting poles","0's"]

{"sheet":"3.6 Quality of service","index":18,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"FORECAST"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DQS0201","Energy Not Supplied (planned)","GWh",0.105,9.6000000000000002E-2,8.6999999999999994E-2,8.5000000000000006E-2,8.6999999999999994E-2,9.1999999999999998E-2,0.09]
["DQS0202","Energy Not Supplied (unplanned)","GWh",0.432,0.45,0.45800000000000002,0.45500000000000002,0.43,0.44500000000000001,0.44700000000000001]
["DQS02","Total",null,{"$f":"SUM(D9:D10)","v":0.53700000000000003},0.54600000000000004,0.54500000000000004,0.54,0.51700000000000002,0.53700000000000003,0.53700000000000003]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"FORECAST"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DQS03","System losses","%",4.7600000000000003E-2,4.5999999999999999E-2,4.4400000000000002E-2,4.2900000000000001E-2,4.2000000000000003E-2,4.2000000000000003E-2,4.2000000000000003E-2]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"FORECAST"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DQS04","Overall utilisation","%",{"$f":"IF('3.5 Physical assets'!D86=0,0,'3.4 Operational data'!D49/'3.5 Physical assets'!D86)","v":0.2040789729763875},{"$f":"IF('3.5 Physical assets'!E86=0,0,'3.4 Operational data'!E49/'3.5 Physical assets'!E86)","v":0.21275127183936035},{"$f":"IF('3.5 Physical assets'!F86=0,0,'3.4 Operational data'!F49/'3.5 Physical assets'!F86)","v":0.20628403643205762},{"$f":"IF('3.5 Physical assets'!G86=0,0,'3.4 Operational data'!G49/'3.5 Physical assets'!G86)","v":0.21247715044608798},{"$f":"IF('3.5 Physical assets'!H86=0,0,'3.4 Operational data'!H49/'3.5 Physical assets'!H86)","v":0.21711722237784653},{"$f":"IF('3.5 Physical assets'!I86=0,0,'3.4 Operational data'!I49/'3.5 Physical assets'!I86)","v":0.2197790036009295},{"$f":"IF('3.5 Physical assets'!J86=0,0,'3.4 Operational data'!J49/'3.5 Physical assets'!J86)","v":0.22175033067419128}]

{"sheet":"3.7 Operating Environment","index":19,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DOEF0101","Customer density","Customer / km",17.718499999999999]
["DOEF0102","Energy density","MWh/customer",20.353400000000001]
["DOEF0103","Demand density","kVA / customer",4.4238]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DOEF0201","Rural proportion","%",0.91]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",2743]
["DOEF0203","Rural vegetation maintenance spans","0's",4921]
["DOEF0204","Total vegetation maintenance spans","0's",6980]
["DOEF0205","Total number of spans","0's",62364]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",1.33]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1.86]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",2.93]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",3.97]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",2.94]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",3.99]
["DOEF0212","Tropical proportion","Spans",5816]
["DOEF0213","Standard vehicle access","km",3075,3075,3074,3074,3074,3074,3074]
["DOEF0214","Bushfire risk","Spans",0]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29"]
["DOEF0301","Route Line length","km",4748,4752,4757,4762,4767,4772,4776]

{"sheet":"4.1 Public lighting","index":20,"n_rows":156,"n_cols":10,"rows_kept":156,"cut":false,"hidden":false,"merged":[[5,1,5,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[54,1,54,2],[55,1,55,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[95,1,95,2],[93,1,93,2],[96,1,96,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[156,1,156,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[212,1,212,2],[213,1,213,2],[214,1,214,2],[215,1,215,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's"]
[null,"Number of poles installed ","0's"]
[null,"Total expenditure","$0's"]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's"]
[null,"Number of poles replaced","0's"]
[null,"Total expenditure","$0's"]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's"]
[null,"Number of poles maintained","0's"]
[null,"Total expenditure","$0's"]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days"]
[null,"GSO breaches","0's"]
[null,"GSL payments ","$0's"]
[null,"Customer complaints ","0's"]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"LIGHT INSTALLATION"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]

{"sheet":"5.4 MD & utilisation-Spatial","index":21,"n_rows":11579,"n_cols":12,"rows_kept":11579,"cut":false,"hidden":false,"merged":[[5,1,5,2],[11,2,12,2],[11,3,12,3],[13,2,14,2],[13,3,14,3],[15,2,16,2],[15,3,16,3],[17,2,18,2],[17,3,18,3],[19,2,20,2],[19,3,20,3],[21,2,22,2],[21,3,22,3],[23,2,24,2],[23,3,24,3],[25,2,26,2],[25,3,26,3],[27,2,28,2],[27,3,28,3],[29,2,30,2],[29,3,30,3],[31,2,32,2],[31,3,32,3],[33,2,34,2],[33,3,34,3],[35,2,36,2],[35,3,36,3],[37,2,38,2],[37,3,38,3],[39,2,40,2],[39,3,40,3],[41,2,42,2],[41,3,42,3],[43,2,44,2],[43,3,44,3],[45,2,46,2],[45,3,46,3],[47,2,48,2],[47,3,48,3],[49,2,50,2],[49,3,50,3],[51,2,52,2],[51,3,52,3],[53,2,54,2],[53,3,54,3],[55,2,56,2],[55,3,56,3],[57,2,58,2],[57,3,58,3],[59,2,60,2],[59,3,60,3],[61,2,62,2],[61,3,62,3],[63,2,64,2],[63,3,64,3],[65,2,66,2],[65,3,66,3],[67,2,68,2],[67,3,68,3],[69,2,70,2],[69,3,70,3],[71,2,72,2],[71,3,72,3],[73,2,74,2],[73,3,74,3],[75,2,76,2],[75,3,76,3],[77,2,78,2],[77,3,78,3],[79,2,80,2],[79,3,80,3],[81,2,82,2],[81,3,82,3],[83,2,84,2],[83,3,84,3],[85,2,86,2],[85,3,86,3],[87,2,88,2],[87,3,88,3],[89,2,90,2],[89,3,90,3],[91,2,92,2],[91,3,92,3],[93,2,94,2],[93,3,94,3],[95,2,96,2],[95,3,96,3],[97,2,98,2],[97,3,98,3],[99,2,100,2],[99,3,100,3],[101,2,102,2],[101,3,102,3],[103,2,104,2],[103,3,104,3],[105,2,106,2],[105,3,106,3],[107,2,108,2],[107,3,108,3],[109,2,110,2],[109,3,110,3],[111,2,112,2],[111,3,112,3],[113,2,114,2],[113,3,114,3],[115,2,116,2],[115,3,116,3],[117,2,118,2],[117,3,118,3],[119,2,120,2],[119,3,120,3],[121,2,122,2],[121,3,122,3],[123,2,124,2],[123,3,124,3],[125,2,126,2],[125,3,126,3],[127,2,128,2],[127,3,128,3],[129,2,130,2],[129,3,130,3],[131,2,132,2],[131,3,132,3],[133,2,134,2],[133,3,134,3],[135,2,136,2],[135,3,136,3],[137,2,138,2],[137,3,138,3],[139,2,140,2],[139,3,140,3],[141,2,142,2],[141,3,142,3],[143,2,144,2],[143,3,144,3],[145,2,146,2],[145,3,146,3],[147,2,148,2],[147,3,148,3],[149,2,150,2],[149,3,150,3],[151,2,152,2],[151,3,152,3],[153,2,154,2],[153,3,154,3],[155,2,156,2],[155,3,156,3],[157,2,158,2],[157,3,158,3],[159,2,160,2],[159,3,160,3],[161,2,162,2],[161,3,162,3],[163,2,164,2],[163,3,164,3],[165,2,166,2],[165,3,166,3],[167,2,168,2],[167,3,168,3],[169,2,170,2],[169,3,170,3],[171,2,172,2],[171,3,172,3],[173,2,174,2],[173,3,174,3],[175,2,176,2],[175,3,176,3],[177,2,178,2],[177,3,178,3],[179,2,180,2],[179,3,180,3],[181,2,182,2],[181,3,182,3],[183,2,184,2],[183,3,184,3],[185,2,186,2],[185,3,186,3],[187,2,188,2],[187,3,188,3],[189,2,190,2],[189,3,190,3],[191,2,192,2],[191,3,192,3],[193,2,194,2],[193,3,194,3],[195,2,196,2],[195,3,196,3],[197,2,198,2],[197,3,198,3],[199,2,200,2],[199,3,200,3],[201,2,202,2],[201,3,202,3],[203,2,204,2],[203,3,204,3],[205,2,206,2],[205,3,206,3],[207,2,208,2],[207,3,208,3],[209,2,210,2],[209,3,210,3],[211,2,212,2],[211,3,212,3],[213,2,214,2],[213,3,214,3],[215,2,216,2],[215,3,216,3],[217,2,218,2],[217,3,218,3],[219,2,220,2],[219,3,220,3],[221,2,222,2],[221,3,222,3],[223,2,224,2],[223,3,224,3],[225,2,226,2],[225,3,226,3],[227,2,228,2],[227,3,228,3],[229,2,230,2],[229,3,230,3],[231,2,232,2],[231,3,232,3],[233,2,234,2],[233,3,234,3],[235,2,236,2],[235,3,236,3],[237,2,238,2],[237,3,238,3],[239,2,240,2],[239,3,240,3],[241,2,242,2],[241,3,242,3],[243,2,244,2],[243,3,244,3],[245,2,246,2],[245,3,246,3],[247,2,248,2],[247,3,248,3],[249,2,250,2],[249,3,250,3],[251,2,252,2],[251,3,252,3],[253,2,254,2],[253,3,254,3],[255,2,256,2],[255,3,256,3],[257,2,258,2],[257,3,258,3],[259,2,260,2],[259,3,260,3],[261,2,262,2],[261,3,262,3],[263,2,264,2],[263,3,264,3],[265,2,266,2],[265,3,266,3],[267,2,268,2],[267,3,268,3],[269,2,270,2],[269,3,270,3],[271,2,272,2],[271,3,272,3],[273,2,274,2],[273,3,274,3],[275,2,276,2],[275,3,276,3],[277,2,278,2],[277,3,278,3],[279,2,280,2],[279,3,280,3],[281,2,282,2],[281,3,282,3],[283,2,284,2],[283,3,284,3],[285,2,286,2],[285,3,286,3],[287,2,288,2],[287,3,288,3],[289,2,290,2],[289,3,290,3],[291,2,292,2],[291,3,292,3],[293,2,294,2],[293,3,294,3],[295,2,296,2],[295,3,296,3],[297,2,298,2],[297,3,298,3],[299,2,300,2],[299,3,300,3],[301,2,302,2],[301,3,302,3],[303,2,304,2],[303,3,304,3],[305,2,306,2],[305,3,306,3],[307,2,308,2],[307,3,308,3],[309,2,310,2],[309,3,310,3],[311,2,312,2],[311,3,312,3],[313,2,314,2],[313,3,314,3],[315,2,316,2],[315,3,316,3],[317,2,318,2],[317,3,318,3],[319,2,320,2],[319,3,320,3],[321,2,322,2],[321,3,322,3],[323,2,324,2],[323,3,324,3],[325,2,326,2],[325,3,326,3],[327,2,328,2],[327,3,328,3],[329,2,330,2],[329,3,330,3],[331,2,332,2],[331,3,332,3],[333,2,334,2],[333,3,334,3],[335,2,336,2],[335,3,336,3],[337,2,338,2],[337,3,338,3],[339,2,340,2],[339,3,340,3],[341,2,342,2],[341,3,342,3],[343,2,344,2],[343,3,344,3],[345,2,346,2],[345,3,346,3],[347,2,348,2],[347,3,348,3],[349,2,350,2],[349,3,350,3],[351,2,352,2],[351,3,352,3],[353,2,354,2],[353,3,354,3],[355,2,356,2],[355,3,356,3],[357,2,358,2],[357,3,358,3],[359,2,360,2],[359,3,360,3],[361,2,362,2],[361,3,362,3],[363,2,364,2],[363,3,364,3],[365,2,366,2],[365,3,366,3],[367,2,368,2],[367,3,368,3],[369,2,370,2],[369,3,370,3],[371,2,372,2],[371,3,372,3],[373,2,374,2],[373,3,374,3],[375,2,376,2],[375,3,376,3],[377,2,378,2],[377,3,378,3],[379,2,380,2],[379,3,380,3],[381,2,382,2],[381,3,382,3],[383,2,384,2],[383,3,384,3],[385,2,386,2],[385,3,386,3],[387,2,388,2],[387,3,388,3],[389,2,390,2],[389,3,390,3],[391,2,392,2],[391,3,392,3],[393,2,394,2],[393,3,394,3],[395,2,396,2],[395,3,396,3],[397,2,398,2],[397,3,398,3],[399,2,400,2],[399,3,400,3],[401,2,402,2],[401,3,402,3],[403,2,404,2],[403,3,404,3],[405,2,406,2],[405,3,406,3],[407,2,408,2],[407,3,408,3],[409,2,410,2],[409,3,410,3],[411,2,412,2],[411,3,412,3],[413,2,414,2],[413,3,414,3],[415,2,416,2],[415,3,416,3],[417,2,418,2],[417,3,418,3],[419,2,420,2],[419,3,420,3],[421,2,422,2],[421,3,422,3],[423,2,424,2],[423,3,424,3],[425,2,426,2],[425,3,426,3],[427,2,428,2],[427,3,428,3],[429,2,430,2],[429,3,430,3],[431,2,432,2],[431,3,432,3],[433,2,434,2],[433,3,434,3],[435,2,436,2],[435,3,436,3],[437,2,438,2],[437,3,438,3],[439,2,440,2],[439,3,440,3],[441,2,442,2],[441,3,442,3],[443,2,444,2],[443,3,444,3],[445,2,446,2],[445,3,446,3],[447,2,448,2],[447,3,448,3],[449,2,450,2],[449,3,450,3],[451,2,452,2],[451,3,452,3],[453,2,454,2],[453,3,454,3],[455,2,456,2],[455,3,456,3],[457,2,458,2],[457,3,458,3],[459,2,460,2],[459,3,460,3],[461,2,462,2],[461,3,462,3],[463,2,464,2],[463,3,464,3],[465,2,466,2],[465,3,466,3],[467,2,468,2],[467,3,468,3],[469,2,470,2],[469,3,470,3],[471,2,472,2],[471,3,472,3],[473,2,474,2],[473,3,474,3],[475,2,476,2],[475,3,476,3],[477,2,478,2],[477,3,478,3],[479,2,480,2],[479,3,480,3],[481,2,482,2],[481,3,482,3],[483,2,484,2],[483,3,484,3],[485,2,486,2],[485,3,486,3],[487,2,488,2],[487,3,488,3],[489,2,490,2],[489,3,490,3],[491,2,492,2],[491,3,492,3],[493,2,494,2],[493,3,494,3],[495,2,496,2],[495,3,496,3],[497,2,498,2],[497,3,498,3],[499,2,500,2],[499,3,500,3],[501,2,502,2],[501,3,502,3],[503,2,504,2],[503,3,504,3],[505,2,506,2],[505,3,506,3],[507,2,508,2],[507,3,508,3],[509,2,510,2],[509,3,510,3],[511,2,512,2],[511,3,512,3],[513,2,514,2],[513,3,514,3],[515,2,516,2],[515,3,516,3],[517,2,518,2],[517,3,518,3],[519,2,520,2],[519,3,520,3],[521,2,522,2],[521,3,522,3],[523,2,524,2],[523,3,524,3],[525,2,526,2],[525,3,526,3],[527,2,528,2],[527,3,528,3],[529,2,530,2],[529,3,530,3],[531,2,532,2],[531,3,532,3],[533,2,534,2],[533,3,534,3],[535,2,536,2],[535,3,536,3],[537,2,538,2],[537,3,538,3],[539,2,540,2],[539,3,540,3],[541,2,542,2],[541,3,542,3],[543,2,544,2],[543,3,544,3],[545,2,546,2],[545,3,546,3],[547,2,548,2],[547,3,548,3],[549,2,550,2],[549,3,550,3],[551,2,552,2],[551,3,552,3],[553,2,554,2],[553,3,554,3],[555,2,556,2],[555,3,556,3],[557,2,558,2],[557,3,558,3],[559,2,560,2],[559,3,560,3],[561,2,562,2],[561,3,562,3],[563,2,564,2],[563,3,564,3],[565,2,566,2],[565,3,566,3],[567,2,568,2],[567,3,568,3],[569,2,570,2],[569,3,570,3],[571,2,572,2],[571,3,572,3],[573,2,574,2],[573,3,574,3],[575,2,576,2],[575,3,576,3],[577,2,578,2],[577,3,578,3],[579,2,580,2],[579,3,580,3],[581,2,582,2],[581,3,582,3],[583,2,584,2],[583,3,584,3],[585,2,586,2],[585,3,586,3],[587,2,588,2],[587,3,588,3],[589,2,590,2],[589,3,590,3],[591,2,592,2],[591,3,592,3],[593,2,594,2],[593,3,594,3],[595,2,596,2],[595,3,596,3],[597,2,598,2],[597,3,598,3],[599,2,600,2],[599,3,600,3],[601,2,602,2],[601,3,602,3],[603,2,604,2],[603,3,604,3],[605,2,606,2],[605,3,606,3],[607,2,608,2],[607,3,608,3],[609,2,610,2],[609,3,610,3],[611,2,612,2],[611,3,612,3],[613,2,614,2],[613,3,614,3],[615,2,616,2],[615,3,616,3],[617,2,618,2],[617,3,618,3],[619,2,620,2],[619,3,620,3],[621,2,622,2],[621,3,622,3],[623,2,624,2],[623,3,624,3],[625,2,626,2],[625,3,626,3],[627,2,628,2],[627,3,628,3],[629,2,630,2],[629,3,630,3],[631,2,632,2],[631,3,632,3],[633,2,634,2],[633,3,634,3],[635,2,636,2],[635,3,636,3],[637,2,638,2],[637,3,638,3],[639,2,640,2],[639,3,640,3],[641,2,642,2],[641,3,642,3],[643,2,644,2],[643,3,644,3],[645,2,646,2],[645,3,646,3],[647,2,648,2],[647,3,648,3],[649,2,650,2],[649,3,650,3],[651,2,652,2],[651,3,652,3],[653,2,654,2],[653,3,654,3],[655,2,656,2],[655,3,656,3],[657,2,658,2],[657,3,658,3],[659,2,660,2],[659,3,660,3],[661,2,662,2],[661,3,662,3],[663,2,664,2],[663,3,664,3],[665,2,666,2],[665,3,666,3],[667,2,668,2],[667,3,668,3],[669,2,670,2],[669,3,670,3],[671,2,672,2],[671,3,672,3],[673,2,674,2],[673,3,674,3],[675,2,676,2],[675,3,676,3],[677,2,678,2],[677,3,678,3],[679,2,680,2],[679,3,680,3],[681,2,682,2],[681,3,682,3],[683,2,684,2],[683,3,684,3],[685,2,686,2],[685,3,686,3],[687,2,688,2],[687,3,688,3],[689,2,690,2],[689,3,690,3],[691,2,692,2],[691,3,692,3],[693,2,694,2],[693,3,694,3],[695,2,696,2],[695,3,696,3],[697,2,698,2],[697,3,698,3],[699,2,700,2],[699,3,700,3],[701,2,702,2],[701,3,702,3],[703,2,704,2],[703,3,704,3],[705,2,706,2],[705,3,706,3],[707,2,708,2],[707,3,708,3],[709,2,710,2],[709,3,710,3],[711,2,712,2],[711,3,712,3],[713,2,714,2],[713,3,714,3],[715,2,716,2],[715,3,716,3],[717,2,718,2],[717,3,718,3],[719,2,720,2],[719,3,720,3],[721,2,722,2],[721,3,722,3],[723,2,724,2],[723,3,724,3],[725,2,726,2],[725,3,726,3],[727,2,728,2],[727,3,728,3],[729,2,730,2],[729,3,730,3],[731,2,732,2],[731,3,732,3],[733,2,734,2],[733,3,734,3],[735,2,736,2],[735,3,736,3],[737,2,738,2],[737,3,738,3],[739,2,740,2],[739,3,740,3],[741,2,742,2],[741,3,742,3],[743,2,744,2],[743,3,744,3],[745,2,746,2],[745,3,746,3],[747,2,748,2],[747,3,748,3],[749,2,750,2],[749,3,750,3],[751,2,752,2],[751,3,752,3],[753,2,754,2],[753,3,754,3],[755,2,756,2],[755,3,756,3],[757,2,758,2],[757,3,758,3],[759,2,760,2],[759,3,760,3],[761,2,762,2],[761,3,762,3],[763,2,764,2],[763,3,764,3],[765,2,766,2],[765,3,766,3],[767,2,768,2],[767,3,768,3],[769,2,770,2],[769,3,770,3],[771,2,772,2],[771,3,772,3],[773,2,774,2],[773,3,774,3],[775,2,776,2],[775,3,776,3],[777,2,778,2],[777,3,778,3],[779,2,780,2],[779,3,780,3],[781,2,782,2],[781,3,782,3],[783,2,784,2],[783,3,784,3],[785,2,786,2],[785,3,786,3],[787,2,788,2],[787,3,788,3],[789,2,790,2],[789,3,790,3],[791,2,792,2],[791,3,792,3],[793,2,794,2],[793,3,794,3],[795,2,796,2],[795,3,796,3],[797,2,798,2],[797,3,798,3],[799,2,800,2],[799,3,800,3],[801,2,802,2],[801,3,802,3],[803,2,804,2],[803,3,804,3],[805,2,806,2],[805,3,806,3],[807,2,808,2],[807,3,808,3],[809,2,810,2],[809,3,810,3],[811,2,812,2],[811,3,812,3],[813,2,814,2],[813,3,814,3],[815,2,816,2],[815,3,816,3],[817,2,818,2],[817,3,818,3],[819,2,820,2],[819,3,820,3],[821,2,822,2],[821,3,822,3],[823,2,824,2],[823,3,824,3],[825,2,826,2],[825,3,826,3],[827,2,828,2],[827,3,828,3],[829,2,830,2],[829,3,830,3],[831,2,832,2],[831,3,832,3],[833,2,834,2],[833,3,834,3],[835,2,836,2],[835,3,836,3],[837,2,838,2],[837,3,838,3],[839,2,840,2],[839,3,840,3],[841,2,842,2],[841,3,842,3],[843,2,844,2],[843,3,844,3],[845,2,846,2],[845,3,846,3],[847,2,848,2],[847,3,848,3],[849,2,850,2],[849,3,850,3],[851,2,852,2],[851,3,852,3],[853,2,854,2],[853,3,854,3],[855,2,856,2],[855,3,856,3],[857,2,858,2],[857,3,858,3],[859,2,860,2],[859,3,860,3],[861,2,862,2],[861,3,862,3],[863,2,864,2],[863,3,864,3],[865,2,866,2],[865,3,866,3],[867,2,868,2],[867,3,868,3],[869,2,870,2],[869,3,870,3],[871,2,872,2],[871,3,872,3],[873,2,874,2],[873,3,874,3],[875,2,876,2],[875,3,876,3],[877,2,878,2],[877,3,878,3],[879,2,880,2],[879,3,880,3],[881,2,882,2],[881,3,882,3],[883,2,884,2],[883,3,884,3],[885,2,886,2],[885,3,886,3],[887,2,888,2],[887,3,888,3],[889,2,890,2],[889,3,890,3],[891,2,892,2],[891,3,892,3],[893,2,894,2],[893,3,894,3],[895,2,896,2],[895,3,896,3],[897,2,898,2],[897,3,898,3],[899,2,900,2],[899,3,900,3],[901,2,902,2],[901,3,902,3],[903,2,904,2],[903,3,904,3],[905,2,906,2],[905,3,906,3],[907,2,908,2],[907,3,908,3],[909,2,910,2],[909,3,910,3],[911,2,912,2],[911,3,912,3],[913,2,914,2],[913,3,914,3],[915,2,916,2],[915,3,916,3],[917,2,918,2],[917,3,918,3],[919,2,920,2],[919,3,920,3],[921,2,922,2],[921,3,922,3],[923,2,924,2],[923,3,924,3],[925,2,926,2],[925,3,926,3],[927,2,928,2],[927,3,928,3],[929,2,930,2],[929,3,930,3],[931,2,932,2],[931,3,932,3],[933,2,934,2],[933,3,934,3],[935,2,936,2],[935,3,936,3],[937,2,938,2],[937,3,938,3],[939,2,940,2],[939,3,940,3],[941,2,942,2],[941,3,942,3],[943,2,944,2],[943,3,944,3],[945,2,946,2],[945,3,946,3],[947,2,948,2],[947,3,948,3],[949,2,950,2],[949,3,950,3],[951,2,952,2],[951,3,952,3],[953,2,954,2],[953,3,954,3],[955,2,956,2],[955,3,956,3],[957,2,958,2],[957,3,958,3],[959,2,960,2],[959,3,960,3],[961,2,962,2],[961,3,962,3],[963,2,964,2],[963,3,964,3],[965,2,966,2],[965,3,966,3],[967,2,968,2],[967,3,968,3],[969,2,970,2],[969,3,970,3],[971,2,972,2],[971,3,972,3],[973,2,974,2],[973,3,974,3],[975,2,976,2],[975,3,976,3],[977,2,978,2],[977,3,978,3],[979,2,980,2],[979,3,980,3],[981,2,982,2],[981,3,982,3],[983,2,984,2],[983,3,984,3],[985,2,986,2],[985,3,986,3],[987,2,988,2],[987,3,988,3],[989,2,990,2],[989,3,990,3],[991,2,992,2],[991,3,992,3],[993,2,994,2],[993,3,994,3],[995,2,996,2],[995,3,996,3],[997,2,998,2],[997,3,998,3],[999,2,1000,2],[999,3,1000,3],[1001,2,1002,2],[1001,3,1002,3],[1003,2,1004,2],[1003,3,1004,3],[1005,2,1006,2],[1005,3,1006,3],[1007,2,1008,2],[1007,3,1008,3],[1009,2,1010,2]],"merged_total":11555,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"DEMAND"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Hudson Creek (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",411.6,411.6,411.6,411.6,411.6,411.6,411.6]
[null,null,null,null,"Coincident",411.6,411.6,411.6,411.6,411.6,411.6,411.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",140.72708,152.41200000000001,164.81989999999999,166.38310000000001,167.08654000000001,0,0]
[null,null,null,null,"Coincident",122.29183251999999,132.44602799999998,143.22849309999998,144.58691390000001,145.19820326000001,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",144.04,156,168.7,170.3,171.02,0,0]
[null,null,null,null,"Coincident",125.17075999999999,135.56399999999999,146.60029999999998,147.9907,148.61638000000002,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",136.29149999999998,147.9178,164.2337,166.8716,171.36580000000001,0,0]
[null,null,null,null,"Coincident",118.30102199999999,128.39265040000001,142.55485159999998,144.84454880000001,148.74551439999999,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",139.5,151.4,168.1,170.8,175.4,0,0]
[null,null,null,null,"Coincident",121.086,131.4152,145.91079999999999,148.2544,152.24719999999999,0,0]
[null,"Pine Creek (132/66kV) - (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.0832,14.0832,14.0832,14.0832,14.0832,0,0]
[null,null,null,null,"Coincident",7.4500128000000005,7.4500128000000005,7.4500128000000005,7.4500128000000005,7.4500128000000005,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.4,14.4,14.4,14.4,14.4,0,0]
[null,null,null,null,"Coincident",7.6176000000000004,7.6176000000000004,7.6176000000000004,7.6176000000000004,7.6176000000000004,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.0832,14.0832,14.0832,14.0832,14.0832,0,0]
[null,null,null,null,"Coincident",7.4218464000000006,7.4218464000000006,7.4218464000000006,7.4218464000000006,7.4218464000000006,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.4,14.4,14.4,14.4,14.4,0,0]
[null,null,null,null,"Coincident",7.5888000000000009,7.5888000000000009,7.5888000000000009,7.5888000000000009,7.5888000000000009,0,0]
[null,"Pine Creek (66/11kV) - (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003]
[null,null,null,null,"Coincident",38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003,38.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.3552,22.3552,22.3552,22.3552,22.3552,0,0]
[null,null,null,null,"Coincident",15.492153599999998,15.492153599999998,15.492153599999998,15.492153599999998,15.492153599999998,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.4,22.4,22.4,22.4,22.4,0,0]
[null,null,null,null,"Coincident",15.523199999999997,15.523199999999997,15.523199999999997,15.523199999999997,15.523199999999997,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.255400000000002,22.255400000000002,22.255400000000002,22.255400000000002,22.255400000000002,0,0]
[null,null,null,null,"Coincident",15.356225999999999,15.356225999999999,15.356225999999999,15.356225999999999,15.356225999999999,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.3,22.3,22.3,22.3,22.3,0,0]
[null,null,null,null,"Coincident",15.386999999999999,15.386999999999999,15.386999999999999,15.386999999999999,15.386999999999999,0,0]
[null,"Lovegrove (66/22 kV) (Alice Springs System)","Substation Rating","MVA","Non-Coincident",95.6,95.6,95.6,95.6,95.6,95.6,95.6]
[null,null,null,null,"Coincident",95.6,95.6,95.6,95.6,95.6,95.6,95.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.321400000000001,21.459199999999999,20.596999999999998,20.501199999999997,20.213799999999999,19.926400000000001,20.022199999999998]
[null,null,null,null,"Coincident",15.3571232,14.763929599999997,14.170735999999998,14.104825599999998,13.9070944,13.709363199999999,13.775273599999997]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.3,22.4,21.5,21.4,21.1,20.8,20.9]
[null,null,null,null,"Coincident",16.0304,15.411199999999997,14.791999999999998,14.723199999999999,14.5168,14.3104,14.379199999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.980199999999996,19.888080000000002,19.830599999999997,19.7348,19.543199999999999,19.16,19.025879999999997]
[null,null,null,null,"Coincident",14.371437,13.623334800000002,13.583961,13.518338000000002,13.387091999999999,13.124600000000001,13.0327278]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.9,20.76,20.7,20.6,20.399999999999999,20,19.86]
[null,null,null,null,"Coincident",15.0015,14.220600000000003,14.179500000000001,14.111000000000002,13.974,13.700000000000001,13.604100000000001]
[null,"Owen Springs (Alice Springs System)","Substation Rating","MVA","Non-Coincident",130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999]
[null,null,null,null,"Coincident",130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999,130.69999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.200000000000003,25.427199999999999,27.468800000000002,27.468800000000002,27.1904,26.912000000000003,27.004800000000003]
[null,null,null,null,"Coincident",13.479199999999999,14.773203199999999,15.959372800000002,15.959372800000002,15.7976224,15.635872000000001,15.689788800000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25,27.4,29.6,29.6,29.3,29,29.1]
[null,null,null,null,"Coincident",14.524999999999999,15.919399999999998,17.197600000000001,17.197600000000001,17.023299999999999,16.849,16.9071]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.993600000000001,24.0352,26.819199999999999,26.726400000000002,26.540800000000004,26.169599999999999,26.076800000000002]
[null,null,null,null,"Coincident",12.756288,13.940415999999999,15.555135999999997,15.501312000000002,15.393664000000001,15.178367999999999,15.124543999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.7,25.9,28.9,28.8,28.6,28.2,28.1]
[null,null,null,null,"Coincident",13.745999999999999,15.021999999999998,16.761999999999997,16.704000000000001,16.588000000000001,16.355999999999998,16.297999999999998]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Archer (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",61.8,61.8,61.8,61.8,61.8,61.8,61.8]
[null,null,null,null,"Coincident",61.8,61.8,61.8,61.8,61.8,61.8,61.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.672469230114821,33.414738460229636,34.15700769034445,34.899276920459272,35.641546150574086,36.383815380688901,37.126084610803723]
[null,null,null,null,"Coincident",28.457720699430006,29.104237198860012,29.750753698290019,30.397270197720022,31.043786697150029,31.690303196580036,32.336819696010039]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.613651471311542,34.377302942623082,35.140954413934622,35.904605885246163,36.668257356557703,37.431908827869243,38.195560299180784]
[null,null,null,null,"Coincident",29.277490431512351,29.942630863024704,30.607771294537056,31.272911726049408,31.93805215756176,32.603192589074112,33.268333020586461]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.889000075170777,32.625400150341555,33.361800225512333,34.098200300683111,34.834600375853896,35.571000451024673,36.307400526195451]
[null,null,null,null,"Coincident",27.775319065473745,28.416723530947493,29.058127996421241,29.699532461894989,30.340936927368741,30.982341392842489,31.623745858316237]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.80761324606047,33.565226492120942,34.322839738181415,35.080452984241887,35.83806623030236,36.595679476362832,37.353292722423305]
[null,null,null,null,"Coincident",28.57543113731867,29.235312274637341,29.895193411956011,30.555074549274682,31.214955686593356,31.874836823912027,32.534717961230697]
[null,"Batchelor (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",25.4,25.4,25.4,25.4,25.4,25.4,25.4]
[null,null,null,null,"Coincident",25.4,25.4,25.4,25.4,25.4,25.4,25.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.282903467552591,2.3273026508427823,2.3717018341329732,2.4161010174231641,2.4605002007133554,2.5048993840035463,2.5492985672937372]
[null,null,null,null,"Coincident",1.8012108358989944,1.8362417915149551,1.8712727471309158,1.9063037027468765,1.9413346583628373,1.976365613978798,2.0113965695947589]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3223839954756778,2.3675510181513553,2.4127180408270328,2.4578850635027103,2.5030520861783878,2.5482191088540653,2.5933861315297428]
[null,null,null,null,"Coincident",1.8323609724303098,1.8679977533214194,1.9036345342125289,1.9392713151036385,1.974908095994748,2.0105448768858576,2.0461816577769674]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2279194953219776,2.2710319605767553,2.3141444258315329,2.357256891086311,2.4003693563410886,2.4434818215958662,2.4865942868506439]
[null,null,null,null,"Coincident",1.7578284818090404,1.7918442168950599,1.8258599519810796,1.8598756870670992,1.8938914221531189,1.9279071572391386,1.9619228923251582]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2664491305411776,2.3103071826823554,2.3541652348235331,2.3980232869647109,2.4418813391058887,2.4857393912470664,2.5295974433882442]
[null,null,null,null,"Coincident",1.7882283639969891,1.8228323671363784,1.8574363702757677,1.892040373415157,1.9266443765545462,1.9612483796939355,1.9958523828333248]
[null,"Berrimah (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",48.8,48.8,48.8,48.8,48.8,48.8,48.8]
[null,null,null,null,"Coincident",48.8,48.8,48.8,48.8,48.8,48.8,48.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.831338307450498,26.786106723862982,27.584511569119051,28.559502614375123,29.383270419631199,30.089086824887271,30.794903230143341]
[null,null,null,null,"Coincident",23.266998825028615,22.393185221149452,23.060651671783525,23.875744185617606,24.564414070811683,25.154476585605757,25.744539100399834]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.574269309497431,27.501136266799776,28.320853767062683,29.321871267325591,30.1676287675885,30.892286267851407,31.616943768114314]
[null,null,null,null,"Coincident",23.888089142739851,22.990949919044613,23.676233749264401,24.513084379484194,25.220137649703986,25.825951319923774,26.431764990143567]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.171583972099107,26.125536911847782,26.923126280440041,27.897301849032303,28.720254177624568,29.425255106216827,30.13025603480909]
[null,null,null,null,"Coincident",22.661101032730656,21.788697784481052,22.453887317886995,23.266349742092942,23.952691984138887,24.540662758584833,25.128633533030779]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.896903462114075,26.822933174381706,27.641813429609901,28.641993684838095,29.486913940066291,30.210734195294485,30.934554450522679]
[null,null,null,null,"Coincident",23.266017487403136,22.370326267434343,23.053272400294656,23.88742273315497,24.592086226015287,25.195752318875599,25.799418411735914]
[null,"Casuarina (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",88.5,88.5,88.5,88.5,88.5,88.5,88.5]
[null,null,null,null,"Coincident",88.5,88.5,88.5,88.5,88.5,88.5,88.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.491137520987301,41.915782720987302,42.060430720987299,42.205078720987302,43.399526682884805,43.399526682884805,43.399526682884805]
[null,null,null,null,"Coincident",38.296319931871281,38.688267451471283,38.821777555471279,38.955287659471281,40.057763128302675,40.057763128302675,40.057763128302675]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.165790163604981,42.597340163604983,42.744340163604981,42.89134016360498,44.105210043582119,44.105210043582119,44.105210043582119]
[null,null,null,null,"Coincident",38.919024321007399,39.317344971007401,39.453025971007399,39.588706971007397,40.709108870226295,40.709108870226295,40.709108870226295]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.487674087192183,40.91231928719219,41.056967287192187,41.201615287192183,42.396063249089686,42.396063249089686,42.396063249089686]
[null,null,null,null,"Coincident",37.370123182478387,37.76207070207839,37.895580806078392,38.029090910078388,39.131566378909781,39.131566378909781,39.131566378909781]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.146010251211571,41.577560251211573,41.724560251211571,41.871560251211569,43.085430131188708,43.085430131188708,43.085430131188708]
[null,null,null,null,"Coincident",37.977767461868282,38.376088111868285,38.511769111868283,38.647450111868281,39.767852011087179,39.767852011087179,39.767852011087179]
[null,"Centre Yard (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.61820758989496483,0.63404352511472961,0.64987946033449429,0.66571539555425907,0.68155133077402386,0.69738726599378864,0.71322320121355332]
[null,null,null,null,"Coincident",0.48343833529786256,0.49582203663971852,0.50820573798157465,0.52058943932343071,0.53297314066528667,0.54535684200714274,0.55774054334899881]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.68613494993891766,0.70371090467783526,0.72128685941675286,0.73886281415567046,0.75643876889458805,0.77401472363350565,0.79159067837242325]
[null,null,null,null,"Coincident",0.53655753085223368,0.55030192745806716,0.56404632406390076,0.57779072066973436,0.59153511727556785,0.60527951388140144,0.61902391048723504]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.60300041345239941,0.61829880156719885,0.6335971896819983,0.64889557779679785,0.66419396591159729,0.67949235402639674,0.69479074214119618]
[null,null,null,null,"Coincident",0.47094332290632396,0.48289136402398242,0.49483940514164071,0.50678744625929917,0.5187354873769574,0.53068352849461586,0.54263156961227421]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.6692568406796886,0.68623618375937723,0.70321552683906585,0.72019486991875448,0.7371742129984431,0.75415355607813173,0.77113289915782035]
[null,null,null,null,"Coincident",0.5226895925708368,0.53595045951607367,0.54921132646131043,0.56247219340654731,0.57573306035178407,0.58899392729702094,0.6022547942422577]
[null,"Cosmo Howley (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",12.2,1,1,1,1,1,1]
[null,null,null,null,"Coincident",12.2,1,1,1,1,1,1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001]
[null,null,null,null,"Coincident",0.293319,0.293319,0.293319,0.293319,0.293319,0.293319,0.293319]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.6,0.6,0.6,0.6,0.6,0.6,0.6]
[null,null,null,null,"Coincident",0.32700000000000001,0.32700000000000001,0.32700000000000001,0.32700000000000001,0.32700000000000001,0.32700000000000001,0.32700000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001,0.53820000000000001]
[null,null,null,null,"Coincident",0.29224260000000002,0.29224260000000002,0.29224260000000002,0.29224260000000002,0.29224260000000002,0.29224260000000002,0.29224260000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.6,0.6,0.6,0.6,0.6,0.6,0.6]
[null,null,null,null,"Coincident",0.32580000000000003,0.32580000000000003,0.32580000000000003,0.32580000000000003,0.32580000000000003,0.32580000000000003,0.32580000000000003]
[null,"Darwin (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,null,null,"Coincident",114.3,114.3,114.3,114.3,114.3,114.3,114.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.644364839152221,31.882292308723184,32.781378778294155,33.541725247865109,33.825050874989898,33.501389002114685,33.177727129239472]
[null,null,null,null,"Coincident",25.583086856188366,27.514418262428105,28.290329885667855,28.946508888907594,29.19101890511628,28.911698708824975,28.632378512533666]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.913587123261575,32.171838858449227,33.079090593636884,33.846342328824534,34.132241044389403,33.805639759954275,33.479038475519147]
[null,null,null,null,"Coincident",25.815425687374738,27.764296934841681,28.547255182308632,29.209393429775574,29.456124021308053,29.174267112840539,28.892410204373025]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.356487257334731,32.33437631967994,33.590898382025145,34.66904044437036,35.133869994999053,34.818287045627741,34.502704096256437]
[null,null,null,null,"Coincident",25.334648503079872,27.904566763883786,28.988945303687704,29.919381903491619,30.320529805684181,30.048181720376746,29.775833635069304]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.623095113354925,32.628028576871785,33.895962040388646,34.983895503905508,35.452946513621647,35.134497523337785,34.816048533053923]
[null,null,null,null,"Coincident",25.5647310828253,28.157988661840349,29.252215240855403,30.191101819870454,30.59589284125548,30.32107136264051,30.046249884025535]
[null,"Frances Bay (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",48.8,48.8,48.8,48.8,48.8,48.8,48.8]
[null,null,null,null,"Coincident",48.8,48.8,48.8,48.8,48.8,48.8,48.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.031530502630012,19.246108403031865,19.460686303433722,19.675264203835575,19.743174604237431,19.811085004639285,19.878995405041138]
[null,null,null,null,"Coincident",15.396508176627679,15.570101698052779,15.74369521947788,15.917288740902983,15.972228254828082,16.027167768753184,16.082107282678283]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.301755073661269,19.519379719099256,19.737004364537242,19.954629009975228,20.023503655413215,20.092378300851202,20.161252946289189]
[null,null,null,null,"Coincident",15.615119854591967,15.791178192751298,15.967236530910629,16.143294869069962,16.199014457229293,16.254734045388624,16.310453633547954]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.564593476556553,18.781924275433546,18.99925507431054,19.216585873187537,19.287249172064531,19.357912470941525,19.428575769818519]
[null,null,null,null,"Coincident",14.981626935581138,15.157012890274872,15.332398844968607,15.507784799662343,15.564810081856075,15.621835364049812,15.678860646243546]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.828188110097923,19.048604741819013,19.269021373540102,19.489438005261192,19.561104636982282,19.632771268703372,19.704437900424463]
[null,null,null,null,"Coincident",15.194347804849025,15.372224026647944,15.550100248446864,15.727976470245784,15.785811442044702,15.843646413843622,15.901481385642542]
[null,"Humpty Doo (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",5,5,5,5,5,5,5]
[null,null,null,null,"Coincident",5,5,5,5,5,5,5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0029856664620667,5.3418544540395905,6.5112028416171137,6.7691512291946374,7.0270996167721602,7.2850480043496839,7.5429963919272076]
[null,null,null,null,"Coincident",3.5626572431512393,4.7542504640952359,5.7949705290392313,6.0245445939832276,6.2541186589272222,6.4836927238712185,6.7132667888152149]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.6117346387811828,6.1542102005064407,7.5013857622316982,7.7985613239569558,8.0957368856822125,8.3929124474074701,8.6900880091327277]
[null,null,null,null,"Coincident",4.1044438285152527,5.4772470784507323,6.6762333283862114,6.9407195783216906,7.2052058282571689,7.4696920781926481,7.7341783281281282]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.9140308161222674,5.2460728301599913,6.4085944441977158,6.65971605823544,6.910837672273165,7.1619592863108883,7.4130809003486124]
[null,null,null,null,"Coincident",3.4756593647165732,4.6585126731820719,5.6908318664475717,5.9138278597130709,6.1368238529785701,6.3598198462440685,6.5828158395095677]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.5092520923067596,6.0438627075575937,7.3831733228084282,7.6724839380592629,7.9617945533100976,8.2511051685609313,8.5404157838117651]
[null,null,null,null,"Coincident",4.0042158579684024,5.3669500843111431,6.5562579106538843,6.8131657369966252,7.070073563339367,7.326981389682107,7.5838892160248479]
[null,"Katherine (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",60.5,60.5,60.5,60.5,60.5,60.5,60.5]
[null,null,null,null,"Coincident",60.5,60.5,60.5,60.5,60.5,60.5,60.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.361164248707311,32.952238576614619,35.575148338668264,38.202909100721918,40.634550862775569,42.892942624829217,43.536407752736523]
[null,null,null,null,"Coincident",28.154212896375366,28.66844756165472,30.950379054641392,33.236530917628073,35.352059250614744,37.316860083601419,37.876674744880773]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.688044695663955,33.2850894713279,35.934493271382088,38.588797071436282,41.045000871490473,43.326204671544666,43.976169447208612]
[null,null,null,null,"Coincident",28.438598885227641,28.958027840055273,31.263009146102416,33.572253452149567,35.709150758196714,37.693798064243857,38.259267419071492]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.615769371336718,32.198246839122213,34.812559741054052,37.431723642985901,39.854768544917739,42.104563446849582,42.739431714635039]
[null,null,null,null,"Coincident",27.474103583691608,27.980276503197206,30.252114414975974,32.528167845754744,34.633793865533512,36.588865635312288,37.140566160017848]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.935120577107796,32.523481655679007,35.164201758640459,37.809821861601918,40.257341964563373,42.529862067524832,43.171143146096]
[null,null,null,null,"Coincident",27.751619781506676,28.262905558785057,30.55769132825856,32.856735197732064,34.983630167205568,36.958450136679076,37.515723393957423]
[null,"Leanyer (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",60.2,60.2,60.2,60.2,60.2,60.2,60.2]
[null,null,null,null,"Coincident",60.2,60.2,60.2,60.2,60.2,60.2,60.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.174480129223486,18.904690187478767,19.53580936573405,20.441147103989334,21.792706282244612,23.199470260499893,24.398955838755178]
[null,null,null,null,"Coincident",14.848550265575588,15.445131883170154,15.960756251804719,16.700417183959281,17.804641032593846,18.953967202828412,19.933946920262979]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.321048517362385,19.057147366410049,19.693356215457712,20.605995064505375,21.968453913553038,23.3865627626007,24.595721611648365]
[null,null,null,null,"Coincident",14.968296638685068,15.56968939835701,16.08947202802895,16.835097967700889,17.94822684737283,19.106821777044772,20.094704556716714]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.740100737416579,18.465165282606165,19.091138947795745,19.99133117298533,21.337744838174913,22.739363303364499,23.933703368554085]
[null,null,null,null,"Coincident",14.475922201731928,15.067574870606629,15.578369381401329,16.312926237156027,17.411599787950731,18.555320455545427,19.529901948740129]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.883166065944131,18.614077905852987,19.245099745761841,20.152551585670697,21.509823425579551,22.922745265488405,24.126717105397262]
[null,null,null,null,"Coincident",14.592663509810411,15.189087571176037,15.704001392541661,16.444482093907286,17.552015915272914,18.704960136638537,19.687401158004164]
[null,"Manton (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",15.9,15.9,15.9,15.9,15.9,15.9,15.9]
[null,null,null,null,"Coincident",15.9,15.9,15.9,15.9,15.9,15.9,15.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1975059082971429,3.6512734485942855,4.1050409888914281,4.5588085291885703,5.0125760694857133,4.9153036097828569,4.8180311500799995]
[null,null,null,null,"Coincident",2.7722376224936229,3.1656540799312456,3.5590705373688678,3.9524869948064905,4.345903452244114,4.2615682296817363,4.1772330071193595]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2494978742857143,3.7106437485714285,4.1717896228571423,4.6329354971428565,5.0940813714285706,4.9952272457142852,4.8963731199999998]
[null,null,null,null,"Coincident",2.8173146570057144,3.2171281300114285,3.6169416030171422,4.0167550760228563,4.4165685490285709,4.3308620220342853,4.2451554950399997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.1253764366628567,3.5815780893257139,4.0377797419885706,4.4939813946514278,4.9501830473142849,4.8553446999771426,4.7605063526399993]
[null,null,null,null,"Coincident",2.7065759941500342,3.1016466253560684,3.4967172565621021,3.8917878877681362,4.2868585189741708,4.204728510180205,4.1225985013862392]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1761955657142855,3.6398151314285712,4.1034346971428564,4.567054262857142,5.0306738285714276,4.9342933942857137,4.8379129599999997]
[null,null,null,null,"Coincident",2.7505853599085714,3.1520799038171425,3.5535744477257136,3.9550689916342847,4.3565635355428567,4.2730980794514277,4.1896326233599996]
[null,"Marrakai (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.90377531531057376,0.89834817782114751,0.89292104033172126,0.8874939028422949,0.88206676535286865,0.87663962786344229,0.87121249037401605]
[null,null,null,null,"Coincident",0.74199953386998108,0.73754385399116207,0.73308817411234306,0.72863249423352405,0.72417681435470505,0.71972113447588615,0.71526545459706714]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.93076757498514295,0.92517834997028581,0.91958912495542866,0.91399989994057151,0.90841067492571437,0.90282144991085722,0.89723222489600007]
[null,null,null,null,"Coincident",0.76416017906280231,0.75957142532560462,0.75498267158840693,0.75039391785120912,0.74580516411401143,0.74121641037681374,0.73662765663961605]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.87922825235863766,0.87353992711727546,0.86785160187591315,0.86216327663455083,0.85647495139318863,0.85078662615182632,0.84509830091046401]
[null,null,null,null,"Coincident",0.72184639518644145,0.71717628016328305,0.71250616514012466,0.70783605011696626,0.70316593509380787,0.69849582007064936,0.69382570504749086]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.90548738656914285,0.89962917313828572,0.89377095970742859,0.88791274627657146,0.88205453284571433,0.87619631941485721,0.87033810598400008]
[null,null,null,null,"Coincident",0.74340514437326621,0.73859555114653253,0.73378595791979884,0.72897636469306515,0.72416677146633146,0.71935717823959777,0.71454758501286397]
[null,"Mary River (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8466270738285711,3.0837389476571428,2.991850821485714,2.8999626953142856,2.8080745691428568,2.7161864429714284,2.6242983167999996]
[null,null,null,null,"Coincident",0.43553394229577141,0.47181205899154283,0.45775317568731422,0.44369429238308566,0.42963540907885711,0.4155765257746285,0.40151764247039995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.0283266742857142,3.2805733485714286,3.1828200228571428,3.0850666971428571,2.9873133714285713,2.8895600457142856,2.7918067199999999]
[null,null,null,null,"Coincident",0.46333398116571428,0.50192772233142857,0.48697146349714282,0.47201520466285712,0.45705894582857143,0.44210268699428568,0.42714642815999998]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.783300251428571,3.0218174628571424,2.9313346742857136,2.8408518857142853,2.7503690971428565,2.6598863085714277,2.5694035199999994]
[null,null,null,null,"Coincident",0.42584493846857135,0.46233807181714276,0.4484942051657142,0.43465033851428564,0.42080647186285708,0.40696260521142846,0.39311873855999985]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9609577142857137,3.2146994285714281,3.1184411428571424,3.0221828571428566,2.9259245714285709,2.8296662857142851,2.7334079999999994]
[null,null,null,null,"Coincident",0.45302653028571421,0.49184901257142849,0.47712149485714278,0.46239397714285707,0.44766645942857136,0.4329389417142856,0.41821142399999989]
[null,"Palmerston (66/11 kV) (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",82.7,82.7,82.7,82.7,82.7,82.7,82.7]
[null,null,null,null,"Coincident",82.7,82.7,82.7,82.7,82.7,82.7,82.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.062953335954795,34.551008937733599,36.039064539512395,37.527120141291199,38.066328018069996,38.605535894848799,39.144743771627603]
[null,null,null,null,"Coincident",30.715483649102008,32.097887303154515,33.480290957207018,34.862694611259521,35.363618728787031,35.864542846314535,36.365466963842039]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.70331634653904,35.220192597078082,36.737068847617124,38.253945098156166,38.803596348695208,39.353247599234251,39.902898849773294]
[null,null,null,null,"Coincident",31.310380885934769,32.719558922685543,34.12873695943631,35.537914996187077,36.04854100793785,36.559167019688623,37.069793031439389]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.280356724407639,33.757110926466481,35.233865128525323,36.710619330584166,37.238525807643015,37.766432284701857,38.294338761760699]
[null,null,null,null,"Coincident",29.956171040250293,31.326598939760899,32.697026839271501,34.067454738782111,34.55735194949272,35.047249160203322,35.537146370913931]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.905562410201469,34.41091837560294,35.91627434100441,37.421630306405881,37.959761271807352,38.497892237208823,39.036023202610295]
[null,null,null,null,"Coincident",30.536361916666966,31.933332252559531,33.330302588452092,34.727272924344661,35.226658460237225,35.726043996129789,36.225429532022353]
[null,"Palmerston (11/22 kV) (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",16,16,16,16,16,16,16]
[null,null,null,null,"Coincident",16,16,16,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.081181551275721,6.3091989105514417,6.5372162698271614,6.7652336291028821,6.6434921383786021,6.521750647654323,6.400009156930043]
[null,null,null,null,"Coincident",5.0473806875588485,5.2366350957576957,5.4258895039565438,5.6151439121553919,5.5140984748542401,5.4130530375530874,5.3120076002519356]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.1675269282715224,6.3987818565430441,6.6300367848145658,6.8612917130860875,6.7378216413576091,6.6143515696291306,6.4908814979006522]
[null,null,null,null,"Coincident",5.1190473504653635,5.3109889409307263,5.502930531396089,5.6948721218614526,5.5923919623268157,5.4899118027921778,5.3874316432575409]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.9450170637640189,6.1789801435280385,6.4129432232920571,6.6469063030560767,6.5311105328200956,6.4153147625841154,6.2995189923481343]
[null,null,null,null,"Coincident",4.9224741287966074,5.1161955588412154,5.3099169888858233,5.5036384189304313,5.4077595211750387,5.311880623419647,5.2160017256642552]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.029429070754583,6.2667141415091665,6.50399921226375,6.7412842830183335,6.6238443537729168,6.5064044245275001,6.3889644952820834]
[null,null,null,null,"Coincident",4.9923672705847943,5.1888393091695892,5.385311347754385,5.5817833863391799,5.4845431249239747,5.3873028635087694,5.290062602093565]
[null,"Pine Creek (66/22 kV) (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.3641272247354217,0.3641272247354217,0.3641272247354217,0.3641272247354217,0.3641272247354217,0.3641272247354217,0.3641272247354217]
[null,null,null,null,"Coincident",0.23012840603278653,0.23012840603278653,0.23012840603278653,0.23012840603278653,0.23012840603278653,0.23012840603278653,0.23012840603278653]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.37042444021914722,0.37042444021914722,0.37042444021914722,0.37042444021914722,0.37042444021914722,0.37042444021914722,0.37042444021914722]
[null,null,null,null,"Coincident",0.23410824621850104,0.23410824621850104,0.23410824621850104,0.23410824621850104,0.23410824621850104,0.23410824621850104,0.23410824621850104]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.35505894230713481,0.35505894230713481,0.35505894230713481,0.35505894230713481,0.35505894230713481,0.35505894230713481,0.35505894230713481]
[null,null,null,null,"Coincident",0.22404219259580205,0.22404219259580205,0.22404219259580205,0.22404219259580205,0.22404219259580205,0.22404219259580205,0.22404219259580205]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.36119933093299572,0.36119933093299572,0.36119933093299572,0.36119933093299572,0.36119933093299572,0.36119933093299572,0.36119933093299572]
[null,null,null,null,"Coincident",0.2279167778187203,0.2279167778187203,0.2279167778187203,0.2279167778187203,0.2279167778187203,0.2279167778187203,0.2279167778187203]
[null,"Strangways (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",60,60,60,60,60,60,60]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.060002189748474,39.519026139496944,39.690550089245413,42.606074038993881,42.77759798874235,42.949121938490819,43.120645888239288]
[null,null,null,null,"Coincident",32.781102047414826,36.95028944042965,37.110664333444461,39.836679226459282,39.9970541194741,40.157429012488919,40.317803905503737]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.775512438518852,40.325536877037699,40.500561315556546,43.475585754075389,43.650610192594236,43.825634631113083,44.000659069631929]
[null,null,null,null,"Coincident",33.450104130015127,37.704376980030254,37.868024830045371,40.64967268006049,40.813320530075615,40.976968380090732,41.140616230105856]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.235584255463891,38.679780030927773,38.836475806391661,41.737171581855542,41.893867357319429,42.050563132783317,42.207258908247198]
[null,null,null,null,"Coincident",32.010271278858738,36.165594328917472,36.312104878976207,39.02425542903493,39.170765979093673,39.317276529152402,39.46378707921113]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.93426964843254,39.469163296865077,39.629056945297613,42.588950593730146,42.748844242162683,42.908737890595219,43.068631539027756]
[null,null,null,null,"Coincident",32.663542121284429,36.903667682568852,37.053168243853271,39.820668805137686,39.970169366422112,40.119669927706532,40.269170488990952]
[null,"Tindal (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",11.4,11.4,11.4,11.4,11.4,11.4,11.4]
[null,null,null,null,"Coincident",11.4,11.4,11.4,11.4,11.4,11.4,11.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6429408337860671,5.7543287482841334,7.3219791627822,8.8896295772802674,10.457279991778336,12.024930406276404,12.136318320774471]
[null,null,null,null,"Coincident",4.0290597553232521,4.1085907262748709,5.2278931222264902,6.3471955181781103,7.4664979141297314,8.5858003100813516,8.665331281032973]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.7639845084638068,5.8777617449276134,7.4790389813914198,9.080316217855227,10.681593454319035,12.282870690782843,12.396647927246651]
[null,null,null,null,"Coincident",4.1154849390431583,4.1967218858783157,5.3400338327134733,6.4833457795486318,7.6266577263837911,8.7699696732189505,8.8512066200541089]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5141536138532086,5.6222930980760184,7.1866950822988276,8.7510970665216377,10.315499050744448,11.879901034967256,11.988040519190065]
[null,null,null,null,"Coincident",3.9205632194496309,3.9974503927320484,5.1097402035144661,6.2220300142968838,7.3343198250793016,8.4466096358617193,8.5234968091441363]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.6324347434659945,5.74289386933199,7.3408529951979853,8.9388121210639806,10.536771246929977,12.134730372795971,12.245189498661967]
[null,null,null,null,"Coincident",4.004661102604322,4.0831975410950445,5.2193464795857674,6.3554954180764902,7.4916443565672131,8.6277932950579359,8.7063297335486585]
[null,"Weddell (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",24.3,24.3,24.3,24.3,24.3,24.3,24.3]
[null,null,null,null,"Coincident",24.3,24.3,24.3,24.3,24.3,24.3,24.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.4196534088160018,8.5598914088160019,8.7001294088160019,8.840367408816002,9.1141654088160031,9.3879634088160024,9.9422374088160019]
[null,null,null,null,"Coincident",6.4073562441089766,6.5140773621089769,6.6207984801089772,6.7275195981089775,6.9358798761089782,7.1442401541089788,7.5660426681089783]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.8256325040000014,8.9726325040000017,9.1196325040000019,9.2666325040000022,9.553632504000003,9.8406325040000038,10.421632504000003]
[null,null,null,null,"Coincident",6.7163063355440009,6.8281733355440011,6.9400403355440012,7.0519073355440014,7.2703143355440023,7.4887213355440032,7.9308623355440027]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.2962263846879996,8.4364643846879996,8.5767023846879997,8.7169403846879998,8.9907383846880009,9.264536384688002,9.8188103846880015]
[null,null,null,null,"Coincident",6.2968358259781922,6.4032764679781922,6.5097171099781921,6.6161577519781929,6.823970433978193,7.0317831159781941,7.4524770819781931]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.6962540720000003,8.8432540720000006,8.9902540720000008,9.1372540720000011,9.4242540720000019,9.7112540720000027,10.292254072000002]
[null,null,null,null,"Coincident",6.6004568406480004,6.7120298406480003,6.8236028406480003,6.9351758406480011,7.1530088406480017,7.3708418406480023,7.8118208406480019]
[null,"Wishart Modular Substation (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",11.8,11.8,11.8,11.8,11.8,11.8,11.8]
[null,null,null,null,"Coincident",11.8,11.8,11.8,11.8,11.8,11.8,11.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.7625878948071487,7.8444160119423589,8.7820909067495077,9.6759948015566568,10.103232496363805,10.176396471170953,10.407136045978103]
[null,null,null,null,"Coincident",2.1409125121452672,4.4634727107952017,4.9970097259404689,5.5056410420857373,5.7487392904310051,5.7903695920962717,5.9216604101615395]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.911214027866059,8.1542785986926809,9.1289926265587393,10.058206654424799,10.502320682290858,10.578374710156917,10.818228738022976]
[null,null,null,null,"Coincident",2.2254807818557873,4.6397845226561349,5.1943968045119222,5.7231195863677105,5.9758204682234979,6.0190952100792847,6.1555721519350728]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.6765130288327681,7.7584614799935983,8.6962567088263665,9.5902809376591343,10.017638966491903,10.090923275324672,10.321783184157439]
[null,null,null,null,"Coincident",2.0882594003770123,4.4068061206363636,4.9394738106133751,5.4472795725903884,5.6900189329674005,5.7316444203844128,5.8627728486014243]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8217391152107778,8.0649287733821193,9.0397678885928965,9.9691070038036749,10.413346119014452,10.48952523422523,10.729504349436008]
[null,null,null,null,"Coincident",2.1707478174397217,4.5808795432810436,5.1345881607207646,5.6624527781604872,5.9147805956002086,5.9580503330399299,6.0943584704796514]
[null,"Woolner (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",86.7,86.7,86.7,86.7,86.7,86.7,86.7]
[null,null,null,null,"Coincident",86.7,86.7,86.7,86.7,86.7,86.7,86.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.856203051875646,34.411697207751281,34.312291363626912,34.212885519502549,33.908317725378183,33.603749931253816,33.299182137129456]
[null,null,null,null,"Coincident",29.836909812405551,29.456412809835093,29.371321407264638,29.286230004694179,29.025519972923725,28.764809941153267,28.504099909382813]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.351118713869823,34.900301427739635,34.799484141609447,34.69866685547926,34.389774569349072,34.080882283218884,33.771989997088696]
[null,null,null,null,"Coincident",30.260557619072568,29.874658022145127,29.788358425217687,29.702058828290244,29.437647031362804,29.173235234435364,28.908823437507923]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.014824531048184,33.572514438096363,33.475304345144551,33.378094252192732,33.075722209240915,32.773350166289099,32.470978123337275]
[null,null,null,null,"Coincident",29.082674974046196,28.704499844572393,28.621385215098588,28.538270585624787,28.279742488900979,28.021214392177178,27.762686295453371]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.497793642036697,34.049203284073393,33.95061292611009,33.852022568146786,33.545357210183482,33.238691852220178,32.932026494256874]
[null,null,null,null,"Coincident",29.495613563941376,29.11206880788275,29.027774051824125,28.943479295765503,28.681280414706876,28.419081533648253,28.156882652589626]
[null,"Lovegrove (22/11 kV) (Alice Springs System)","Substation Rating","MVA","Non-Coincident",26.4,26.4,26.4,26.4,26.4,26.4,26.4]
[null,null,null,null,"Coincident",26.4,26.4,26.4,26.4,26.4,26.4,26.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.20733144200042,19.204222102178125,19.201112762355834,19.198003422533539,19.054349482711245,18.910695542888952,18.767041603066659]
[null,null,null,null,"Coincident",17.075317651938374,17.072553448836356,17.069789245734338,17.067025042632316,16.939316690130298,16.811608337628279,16.68389998512626]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.854865843648664,20.851489796067455,20.848113748486245,20.844737700905036,20.688761653323827,20.532785605742617,20.376809558161408]
[null,null,null,null,"Coincident",18.539975735003662,18.536974428703967,18.533973122404273,18.530971816104579,18.392309109804881,18.253646403505186,18.114983697205492]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.473890779789315,18.467213851332872,18.460536922876432,18.453859994419989,18.306638465963552,18.15941693750711,18.012195409050669]
[null,null,null,null,"Coincident",16.367867230893332,16.361951472280925,16.356035713668518,16.350119955056112,16.219681680843706,16.089243406631301,15.958805132418892]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.058513333104575,20.05126368222896,20.044014031353345,20.036764380477731,19.876914729602117,19.717065078726502,19.557215427850888]
[null,null,null,null,"Coincident",17.771842813130654,17.765419622454857,17.758996431779064,17.752573241103271,17.610946450427477,17.469319659751683,17.327692869075886]
[null,"Lovegrove (22 kV loads) (Alice Springs System)","Substation Rating","MVA","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.99986820900856677,0.99502800917233358,0.99018780933610051,0.98534760949986733,0.98050740966363403,0.97566720982740085,0.97082700999116767]
[null,null,null,null,"Coincident",0.38694899688631529,0.3850758395496931,0.38320268221307091,0.38132952487644861,0.37945636753982637,0.37758321020320418,0.37571005286658188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0109890889874285,1.0060950547748571,1.0012010205622857,0.99630698634971415,0.99141295213714264,0.98651891792457114,0.98162488371199963]
[null,null,null,null,"Coincident",0.3912527774381348,0.38935878619786968,0.38746479495760455,0.38557080371733937,0.38367681247707419,0.38178282123680907,0.37988882999654389]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.97195367951455069,0.96806856466878155,0.9641834498230123,0.96029833497724315,0.9564132201314739,0.95252810528570475,0.9486429904399355]
[null,null,null,null,"Coincident",0.37225825925407297,0.3707702602681433,0.36928226128221375,0.36779426229628415,0.36630626331035449,0.36481826432442493,0.36333026533849527]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.98276408444342844,0.97883575800685696,0.97490743157028548,0.97097910513371399,0.96705077869714251,0.96312245226057103,0.95919412582399954]
[null,null,null,null,"Coincident",0.37639864434183312,0.37489409531662621,0.37338954629141935,0.37188499726621249,0.37038044824100558,0.36887589921579872,0.36737135019059181]
[null,"Sadadeen (Ron Goodin 11kV load) (Alice Springs System)","Substation Rating","MVA","Non-Coincident",62,62,62,62,62,62,62]
[null,null,null,null,"Coincident",62,62,62,62,62,62,62]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.398588972004625,19.147035600015265,18.895482228025905,18.643928856036542,18.392375484047182,18.140822112057823,17.889268740068463]
[null,null,null,null,"Coincident",18.137680688824322,17.902478286014272,17.667275883204223,17.43207348039417,17.196871077584117,16.961668674774067,16.726466271964014]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.734068130218336,19.478164394725599,19.222260659232862,18.966356923740125,18.710453188247389,18.454549452754652,18.198645717261915]
[null,null,null,null,"Coincident",18.451353701754144,18.212083709068438,17.972813716382728,17.733543723697018,17.494273731011308,17.255003738325602,17.015733745639892]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.65780301160251,18.411220433289689,18.164637854976867,17.918055276664042,17.67147269835122,17.424890120038398,17.178307541725573]
[null,null,null,null,"Coincident",17.407730209825147,17.177668664259279,16.947607118693416,16.717545573127552,16.487484027561688,16.257422481995825,16.027360936429961]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.980471018924224,18.729624042003753,18.478777065083282,18.227930088162811,17.97708311124234,17.726236134321869,17.475389157401398]
[null,null,null,null,"Coincident",17.708779460656302,17.474739231189503,17.240699001722703,17.006658772255904,16.772618542789104,16.538578313322304,16.304538083855505]
[null,"Brewer + Sadadeen 22kV (Balance Loads)","Substation Rating","MVA","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.2972508826022384,9.7907545985954094,10.28425831458858,10.826835180581751,11.054882796574921,11.28293041256809,11.510978028561262]
[null,null,null,null,"Coincident",6.8334793987126456,7.1962046299676263,7.558929861222607,7.9577238577275864,8.1253388554825676,8.2929538532375471,8.4605688509925265]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.8801815968142819,10.404627628688003,10.929073660561723,11.505669692435443,11.748015724309163,11.990361756182882,12.232707788056601]
[null,null,null,null,"Coincident",7.2619334736584973,7.6474013070856817,8.0328691405128669,8.45666722394005,8.6347915573672349,8.8129158907944181,8.9910402242216012]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.9609394652568248,9.4546827781620859,9.948426091067347,10.491242553972608,10.719529766877868,10.947816979783129,11.176104192688388]
[null,null,null,null,"Coincident",6.5773295674985093,6.9397371591709707,7.302144750843433,7.7005720346158952,7.8681348488883556,8.0356976631608159,8.2032604774332771]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.5227837037798349,10.0474843551138,10.572185006447766,11.149035657781731,11.391636309115695,11.634236960449659,11.876837611783623]
[null,null,null,null,"Coincident",6.989723238574399,7.3748535166535296,7.7599837947326602,8.1833921728117911,8.3614610508909202,8.5395299289700493,8.7175988070491783]
[null,"Tennant Creek (Tennant Creek System)","Substation Rating","MVA","Non-Coincident",15,15,15,15,15,15,15]
[null,null,null,null,"Coincident",15,15,15,15,15,15,15]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident","-","-","-","-","-","-","-"]
[null,null,null,null,"Coincident","-","-","-","-","-","-","-"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.25515452812538,6.0725552660026372,5.8899560038798935,5.7073567417571507,5.5247574796344079,5.3421582175116651,5.1595589553889223]
[null,null,null,null,"Coincident",5.8485694837972302,5.6778391737124654,5.5071088636277015,5.3363785535429367,5.1656482434581719,4.9949179333734071,4.8241876232886423]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3828107429850816,6.1964849653088132,6.0101591876325449,5.8238334099562765,5.6375076322800082,5.4511818546037398,5.2648560769274715]
[null,null,null,null,"Coincident",5.9679280446910514,5.7937134425637407,5.6194988404364299,5.4452842383091191,5.2710696361818083,5.0968550340544967,4.9226404319271859]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.8951331124618411,5.7048776940348462,5.5146222756078522,5.3243668571808573,5.1341114387538624,4.9438560203268684,4.7536006018998735]
[null,null,null,null,"Coincident",5.4588932621396653,5.282716744676268,5.1065402272128706,4.9303637097494741,4.7541871922860768,4.5780106748226794,4.401834157359283]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0154419514916748,5.821303769423313,5.6271655873549511,5.4330274052865892,5.2388892232182274,5.0447510411498655,4.8506128590815036]
[null,null,null,null,"Coincident",5.5702992470812909,5.3905272904859878,5.2107553338906847,5.0309833772953816,4.8512114207000785,4.6714394641047754,4.4916675075094723]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"ZSSCI",null,"MWh","Non-Coincident",44.9837968,44.782209940000001,48.60427498,55.712702720000003,43.85863715,47.588324319999998,48.109229820000003]
[null,"ZSSHC",null,"MWh","Non-Coincident",142.5894624,144.82335929999999,166.236188,169.3551688,156.8207774,155.96499119999999,158.6400969]
[null,"ZSSOS",null,"MWh","Non-Coincident",18.345431810000001,6.1220114690000003,6.1220114690000003,7.1984066630000001,7.6644571370000003,9.0904637099999999,7.2394700900000002]
[null,"ZSSRG",null,"MWh","Non-Coincident",28.48263094,25.034541149999999,25.034541149999999,20.252879419999999,24.701148159999999,24.701148159999999,23.944851610000001]
[null,"ZSSTC",null,"MWh","Non-Coincident",14.043161469999999,14.50384916,15.126426410000001,14.92259999,14.80880526,14.680968460000001,14.80852986]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"ZSSAR",null,"MWh","Non-Coincident",11.99547332,13.935561310000001,17.226330140000002,19.420369489999999,15.64443357,15.64443357,16.37422561]
[null,"ZSSBA",null,"MWh","Non-Coincident",1.24867145,0.92477363899999998,0.92477363899999998,0.94329903999999998,1.0103794420000001,1.0103794420000001,0.96272104000000003]
[null,"ZSSBE",null,"MWh","Non-Coincident",11.813834,15.074146170000001,15.074146170000001,15.074146170000001,14.259068129999999,14.259068129999999,14.74811495]
[null,"ZSSBR",null,"MWh","Non-Coincident",18.345431810000001,6.1220114690000003,6.1220114690000003,7.1984066630000001,7.6644571370000003,9.0904637099999999,7.2394700900000002]
[null,"ZSSCA",null,"MWh","Non-Coincident",19.219911029999999,19.219911029999999,25.44735872,25.44735872,22.333634870000001,22.333634870000001,22.956379640000002]
[null,"ZSSCP",null,"MWh","Non-Coincident",0.70807383199999996,0.70807383199999996,0.70807383199999996,0.70807383199999996,0.70807383199999996,0.70807383199999996,0.70807383199999996]
[null,"ZSSDA",null,"MWh","Non-Coincident",5.475110817,7.2207177759999999,7.2207177759999999,7.2207177759999999,6.7843160359999999,6.7843160359999999,7.0461570800000004]
[null,"ZSSFB",null,"MWh","Non-Coincident",2.3806024969999999,2.3806024969999999,2.3806024969999999,2.3806024969999999,2.3806024969999999,2.3806024969999999,2.3806024969999999]
[null,"ZSSHD",null,"MWh","Non-Coincident",2.6285543680000001,3.4936577130000002,3.4936577130000002,4.2933144499999996,4.2933144499999996,3.640499739,3.8428888130000001]
[null,"ZSSKA",null,"MWh","Non-Coincident",24.42466752,24.28106124,28.019558929999999,33.622979000000001,22.924957710000001,26.654644879999999,27.100640349999999]
[null,"ZSSLE",null,"MWh","Non-Coincident",2.1673147849999999,2.1673147849999999,2.1673147849999999,2.1673147849999999,2.1673147849999999,2.1673147849999999,2.1673147849999999]
[null,"ZSSLG",null,"MWh","Non-Coincident",27.015610909999999,17.83457495,22.147459470000001,17.130828080000001,21.032118359999998,21.032118359999998,19.83541984]
[null,"ZSSMK",null,"MWh","Non-Coincident",1.1554442140000001,1.1554442140000001,1.1554442140000001,1.1812361709999999,1.1812361709999999,1.165760997,1.1678243530000001]
[null,"ZSSMR",null,"MWh","Non-Coincident",1.3138988949999999,1.3138988949999999,1.3138988949999999,1.626392786,1.626392786,1.438896452,1.4638959629999999]
[null,"ZSSMT",null,"MWh","Non-Coincident",5.7210299779999998,6.5357148550000002,6.5357148550000002,8.0307332500000008,6.7057982340000004,6.7057982340000004,6.9027518859999999]
[null,"ZSSPA",null,"MWh","Non-Coincident",13.01830736,16.622129690000001,16.622129690000001,19.096601410000002,16.339792030000002,16.339792030000002,17.004088970000002]
[null,"ZSSPK",null,"MWh","Non-Coincident",0.88589490900000001,0.33712726599999998,0.42069461200000002,0.41215849199999999,0.51396881999999999,0.51396881999999999,0.43958360200000002]
[null,"ZSSPK",null,"MWh","Non-Coincident",12.703532940000001,12.703532940000001,12.703532940000001,12.703532940000001,12.703532940000001,12.703532940000001,12.703532940000001]
[null,"ZSSSD",null,"MWh","Non-Coincident",28.48263094,25.034541149999999,25.034541149999999,20.252879419999999,24.701148159999999,24.701148159999999,23.944851610000001]
[null,"ZSSSY",null,"MWh","Non-Coincident",18.27573525,18.27573525,18.27573525,20.60489385,18.8580249,18.8580249,18.974482829999999]
[null,"ZSSWN",null,"MWh","Non-Coincident",25.421591159999998,25.421591159999998,33.003318810000003,33.003318810000003,29.212454990000001,29.212454990000001,29.970627749999998]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.2 Reliability & Cust serv","index":22,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[[5,1,5,7],[16,1,16,3],[28,1,28,3],[70,4,70,8],[40,1,40,3],[52,1,52,3],[55,1,55,8],[67,1,67,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,4,4,4,4,4]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,80,80,80,80,80]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,190,190,190,190,190]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,1260,1260,1260,1260,1260]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E12:E16)","v":1534},{"$f":"SUM(F12:F16)","v":1534},{"$f":"SUM(G12:G16)","v":1534},{"$f":"SUM(H12:H16)","v":1534},{"$f":"SUM(I12:I16)","v":1534}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,0.1,0.1,0.1,0.1,0.1]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,1.4,1.4,1.4,1.4,1.4]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,3,3,3,3,3]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,15,15,15,15,15]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E24:E28)","v":19.5},{"$f":"SUM(F24:F28)","v":19.5},{"$f":"SUM(G24:G28)","v":19.5},{"$f":"SUM(H24:H28)","v":19.5},{"$f":"SUM(I24:I28)","v":19.5}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E36:E40)","v":0},{"$f":"SUM(F36:F40)","v":0},{"$f":"SUM(G36:G40)","v":0},{"$f":"SUM(H36:H40)","v":0},{"$f":"SUM(I36:I40)","v":0}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E48:E52)","v":0},{"$f":"SUM(F48:F52)","v":0},{"$f":"SUM(G48:G52)","v":0},{"$f":"SUM(H48:H52)","v":0},{"$f":"SUM(I48:I52)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},6167.6524869203031,6213.7908987745595,6259.5711352659637,6305.4041711040081,6351.2914141651145,6397.2343104450956,6443.2343451043071]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},26253.915046798993,26450.312938506526,26645.186181157045,26840.284175374574,27035.612914082365,27231.178552466899,27426.987412426806]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},49903.357648148762,50276.670131782259,50647.08456737057,51017.926210017722,51389.206451053047,51760.936990235314,52133.129844209179]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},1000.3474295615795,1007.8307373193265,1015.2559516931937,1022.6897297289736,1030.1322997737664,1037.5838963573544,1045.0447603617179]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C61:C65)","v":83325.272611429624},83948.60470638267,84567.097835486784,85186.304286225262,85806.243079074309,86426.933749504664,87048.396362102008]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Number of calls received",null,null,18500,18500,18500,18500,18500]
[null,"Number of calls answered within 30 seconds",null,null,12750,12750,12750,12750,12750]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E74/E73),\"\")","v":0.68918918918918914},{"$f":"IFERROR((F74/F73),\"\")","v":0.68918918918918914},{"$f":"IFERROR((G74/G73),\"\")","v":0.68918918918918914},{"$f":"IFERROR((H74/H73),\"\")","v":0.68918918918918914},{"$f":"IFERROR((I74/I73),\"\")","v":0.68918918918918914}]

{"sheet":"7.1  Policies and Procedures","index":23,"n_rows":221,"n_cols":5,"rows_kept":221,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"Statement of Corporate Intent","Our Statement of Corporate Intent (SCI) sets out the Corporation’s strategies, objectives, initiatives, financial plans and major risks and represents the primary agreement between the Board and the Shareholding Minister.","The SCI covers the the whole corporation not just the Power Networks area. However, the works program outlined in our SCI aligns with the capex and opex forecasts in the Regulatory Proposal. Our SCI is relevant to our entire capex and opex program.","No"]
[]
[]
[null,"Governance framework"]
[null,"Environmental policy statement","Our policy is to minimise our impact on the environment and comply with relevant legislation.","When developing our plans we design plans to minimise the environmental impact and the use of resources. ","No"]
[null,"Health and safety policy statement","This is our policy statement  committing to the protection of our workers and the public","We designed our network with appropropriate standards to ensure people around them are safe. We also plan any work in accordance with best practice to maximise cost efficiency, but also to ensure safety.","No"]
[null,"Risk Management Foundation Document Risk Management Policy","This Risk Management Policy introduces Power and Water's Risk Management Framework. It includes a definition of risk as it applies to Power and Water, a clear risk policy statement and key risk management responsibilities for employees.","This policy underlies our decisions about risk, therefore our capital and operating expenditure plans are implicitly informed by our decisions on risk.","No"]
[null,"Capital Investment and Delivery Policy","To ensure that Power and Water's capital investments achieve value for money, through prudent decision making and efficient and effective delivery.","This policy sets out how our investment decisions are approved and on what basis. At each stage of the investment process we ensure our plans will deliver value for money.","No"]
[null,"Compliance Policy","This policy covers Power and Water's obligations to comply with all applicable legislation, regulations, licences, standards, codes and other legal instruments that relate to its operations.","When we plan our expenditure program we aim to meet appropriate standards and to comply with relevant legislation.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Fixed Asset Plan/Capitalisation Policy","This plan sets out all activities relating to fixed assets.","This is the Corporate statutory capitalisation policy and underpins the regulatory approach to capitalisation.","No"]
[]
[]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Policy","The asset management policy sets our objectives in relation to how we make asset related decisions, including whether to repair or decommission and replace assets though their lives.","This policy underpins our main network expenditure programs.","No"]
[null,"Risk and compliance policy statement ","This statement covers Power and Water’s responsibility to effectively and systematically identify,\nmanage and treat risk and to comply with all relevant legislative, regulatory and commercial obligations,\nand best practice standards. It directly supports all of the Key Result Areas in our Statement of Corporate\nIntent – health and safety; people and culture; financial performance; operational performance; and\ncustomer – and related Risk Appetite and Tolerance Statements.","This statement underpins our main network expenditure programs.","No"]
[null,"Risk Quantification Procedure","The Risk Quantification Procedure defines the economic impact (benefits / costs) to the community that are expected to arise from the occurrence of events (e.g. asset failure) across different value dimensions.","These plans underpin our main network expenditure programs.","No"]
[null,"Power Services Asset Strategies Procedure","The procedure reflects Power and Water's current maintenance strategy, activities and frequency for the majority of network asset classes, and relevant information where changes to strategies have been made over time since the procedure was established.","These plans underpin our main network expenditure programs.","No"]
[null,"Asset Management Strategies"]
[null,"Meter Asset Management Strategy","The purpose of this Meter Asset Management Strategy (MAMS) is 1. to describe the Corporation’s overall approach to maintenance, testing, inspection, and auditing of metering installations, 2. to ensure compliance with the Chapter 7A of the National Electricity Rules (Northern Territory) and 3. to satisfy the requirements of the Northern Territory Electricity System Market Operator (NTESMO).","These plans underpin our meter rollout programs.","No"]
[null,"Fleet Strategy","This Strategy describes our strategic approach, asset management plan and expenditure forecasts in relation to our fleet of vehicles required to deliver our regulated network services for the next regulatory9 period, including passenger and light commercial vehicles, heavy vehicles such as Elevated Work Platforms (EWP), cranes and trucks. This document outlines the key challenges and opportunities that are faced by Power and Water’s fleet for its regulated business. ","These plans underpin our main network expenditure programs.","No"]
[null,"Property Strategy","This Strategy describes our approach, asset management plan and expenditure forecasts for the 2024-29 period in relation to property and buildings expenditure relating to the maintenance, refurbishment and optimisation of offices, operational depots, warehouses, training facilities and other specialist facilities used by our regulated electricity network.  ","These plans underpin our main network expenditure programs.","No"]
[]
[null,"Asset Management Plans"]
[null,"Asset Management Plans","The purpose of this asset management plans is to define our approach to managing each type of assets (eg power transfromers, cables, etc). It frames the rationale and direction that underpins the management of these assets into the future.","These plans underpin our main network expenditure programs.","No"]
[null,"Strategic Asset Management Plan","The strategic asset management plan describes how our asset management systems and strategies are aligned with our asset management policy.","This plan underpins our main network expenditure programs.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Proposed Customer Connection Services Policy","This Connection Policy sets out the circumstances in which Power and Water requires a retail customer or real estate developer to pay a connection charge and how these charges are calculated for the provision of connection services.","This policy is relevant for our capital connections forecast.","Yes"]
[null,"Maximum Demand And Customer Connections","AEMO has prepared this document on behalf of Power and Water to provide information about the methodology, data and assumptions used for forecasting maximum demand and customer connections for the three networks in Darwin-Katherine, Tennant Creek and Alice Springs, as at the date of publication.","This procedure has been used to develop the demand and customer forecast that underpins the augmentation and customer connections capex for the forecast period.","No"]
[null,"Future Network Strategy (Including DER Integration Strategy)","The Future Network Strategy (Including DER Integration Strategy) outlines actions and initiatives that we can commence now to ensure Power and Water is in the best position to meet evolving customer needs.","These plans underpin our main network expenditure programs.","No"]
[null,"Capex Delivery Plan","The Capital Delivery Plan outlines Power and Water’s strategy and approach for capital delivery with a focus on the 2024-29 regulatory period. Power and Water will continue to ensure the right capacity and capability is available to deliver a prudent and efficient capital program","These plans underpin our main network expenditure programs.","No"]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"System  Control Technical Code","The System Control Technical Code sets out the Power System Controller’s competitively neutral operating protocols, arrangements for system security and system dispatch, as well as arrangements for the interruption of supply. The Code places obligations on system participants, including Power Networks to ensure system security. ","The Code underpins a number of obligations that Power Networks must meet, influencing capital and operational expenditure.","No"]
[null,"Network Technical Code and Network Planning Criteria","The Network Technical Code sets out technical requirements designed to ensure that the network and the customer installations and equipment connected to the network may be operated and maintained in a secure and reliable manner. The Network Planning Criteria are designed to ensure that new loads and Generators connected to the network do not compromise the security and reliability of supply to all network users. This document also outlines the legislative requirements that apply to Power and Water Networks and to customers seeking access to its regulated electrical networks.","\nPlease note that the capital and operating expenditure forecasts of Power and Water's regulatory proposal are based on the proposed Network Planning Criteria.","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"Power and Water Corporation's Procurement Framework","The policy establishes the overarching principles for undertaking procurement. The Procurement Sourcing Rules, delegations and guidelines set out the ‘how to’ and mandatory procedures for various procurements.","When we procure external services, materials or other items, we will apply our procurement plan.","No"]
[]
[null,"Information technology policies or strategies"]
[null,"ICT Strategy","This document sets out Power and Water’s Information and Communications Technology strategy for the ten-year period starting 1 July 2017. ","This strategy underpins Power and Water's ICT capital program. ","No"]
[null,"ICT Capital Expenditure Plan","This document describes and justifies Power and Water’s non-network, information, communication and technology (ICT) forecast capital expenditure.","This document describes and justifies Power and Water’s non-network, ICT forecast capital expenditure for Standard Control Services in its first 5-year Regulatory Control Period (RCP1).  It also demonstrates how Power and Water’s ICT forecast capital expenditure meets the objectives, criteria and factors set out in the National Electricity Rules (NER)","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Power Networks Demand Management Procedure","The purpose of this document is to establish the process by which Power Networks will assess the viability of demand management or other non-network solutions for its capital projects and pursue demand management or other non-network alternatives to network investment where they prove to be economically feasible.","This Procedure has been utilised where appropriate during development of Power and Water's capital expenditure forecasts. ","No"]
[]
[]
[null,"Self insurance guidelines or policy"]
[]
[]
[null,"Land and easement acquisition polices"]
[]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"Protective Security Management Policy","This Policy outlines Power and Water's commitment to protecting the security of its people, information and assets by managing security risks proportionately and effectively.","This Procedure has been utilised where appropriate during development of Power and Water's capital expenditure forecasts. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"Power and Water Corporation Emergency Management Plan","Outlines Power and Waters plan for protecting its people, infrastructure and assets by managing its emergency management risks proportionately and effectively.","This plan underpins the framework that outlines how we plan for and respond during emergency events. It influence both our capital and operational expenditure forecasts. ","No"]

{"sheet":"7.2 Contingent projects","index":24,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2024-25 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2024-25"}]
[null,"Renewable Energy Hub",126197065.91371663,"We have identified two triggers for the project:\n\n1. A formal notification from a NTG Minister to Power and Water Corporation, advising that the NTG wishes to provide for a Renewable Energy Hub at a site near Darwin and advising the approximate required capacity and location of that hub; and \n\n2. The completion of a RIT-T by Power and Water that meets the following: \na) Identifies a need to undertake shared transmission works to convey generation from a Renewable Energy Hub near Darwin within the regulatory period. \nb) Identifies a preferred option consistent with the RIT‐T guidelines that maximises the net economic benefit to all those who produce, consume and transport electricity.\nc) Determines that the preferred option has a positive net economic benefit and/or is otherwise consistent with the National Electricity Objective at that time. ",175968438.25887242,{"$f":"+E8*0.05","v":8798421.9129436221}]
[null,"Unlocking existing large scale renewable generation on DKTL",49123439.5208482,"We have identified two triggers for the project:\n\n1. A formal notification from a NTG Minister to Power and Water Corporation, advising that it wishes to accommodate more renewable energy in an area that requires transport of generation on the DKTL and advising the approximate required additional capacity and location of that generation; and\n\n2. the completion of a RIT-T by Power and Water that meets the following: \na) Identifies a need to relieve transmission constraints on the DKTL within the next regulatory period, and \nb) Identifies a preferred option consistent with the RIT‐T guidelines that maximises the net economic benefit to all those who produce, consume and transport electricity in the NEM, and \nc) Determines that the preferred option has a positive net economic benefit and/or is otherwise consistent with the National Electricity Objective at that time. ",{"$f":"+$E$8","v":175968438.25887242},8798421.9129436221]
[null,"Holtze-Kowani land release",64898072.760062784,"We have identified three triggers for the project:\n\n1. An executed Connection Application and an approved HV Master Plan for Stage 3 of the land development in the Greater Holtze Area.\n\n2. A Power and Water planning study demonstrating a likely material constraint in meeting the expected demand arising from Stage 3 of the land development. \n\n3. The completion of a Regulatory Investment Test for Distribution (RIT-D) by Power and Water that meets the following: \na). Identifies a need to undertake augmentation distribution works in the next regulatory period to meet demand for standard control services arising from Stage 3 land release in the Greater Holtze Area, and\nb). Identifies the preferred option consistent with the RIT‐D guidelines that maximises the net economic benefit to all those who produce, consume and transport electricity.",175968438.25887242,8798421.9129436221]
[null,"Commercial development in Middle Arm ",48523592.919780053,"We have identified two triggers for the project:\n\n1. Committed customer connections in the Middle Arm Peninsula in Darwin that, in aggregate, exceeds the existing capacity (15 MVA) of the Weddell zone substation.\n\n2. The completion of a regulatory investment test for distribution by Power and Water that meets the following:\na). Identifies a need to undertake augmentation distribution works to meet demand for standard control services arising from new customer connections in the Middle Arm Peninsula.\nb). Identifies the preferred option consistent with the RIT‐D guidelines that maximise the net economic benefit to all those who produce, consume and transport electricity.",175968438.25887242,8798421.9129436221]
[null,"Wishart ZSS",78310016.423248395,"[c-i-c]",175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]
[null,null,null,null,175968438.25887242,8798421.9129436221]

{"sheet":"7.3 Obligations","index":25,"n_rows":314,"n_cols":5,"rows_kept":314,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"COMMONWEALTH LEGISLATION"]
[null,"A New Tax System (Goods and Services Tax) Act 1999  (Cth)","This Act provides for the  imposition of Goods and Services Tax (GST). ","Business as usual","No"]
[null,"A New Tax System (Goods and Services Tax) Regulations 1999 (Cth)","See Act above. ","Business as usual","No"]
[null,"Age Discrimination Act 2004 (Cth)","This Act makes it unlawful to discriminate on the ground of age. ","Business as usual","No"]
[null,"Competition and Consumer Act 2010 (Cth) (and regulations)","The object of this Act is to enhance the welfare of Australians through the promotion of competition and fair trading and provision for consumer protection.","Business as usual","No"]
[null,"Corporations Act 2001 (Cth) (and regulations)","This Act sets out the laws dealing with business entities in Australia at federal and interstate level. It focuses primarily on companies, although it also covers some laws relating to other entities such as partnerships and managed investment schemes.","Business as usual","No"]
[null,"Disability Discrimination Act 1992","The Disability Discrimination Act 1992 (DDA) makes it unlawful to discriminate against a person, in many areas of public life, including employment, education, getting or using services, renting or buying a house or unit, and accessing public places, because of their disability.","Business as usual","No"]
[null,"Electronic Transactions Act 1999 No. 162 (CTH)","The Electronic Transactions Act 1999 ensures that a transaction under a Commonwealth law will not be invalid simply because it was conducted through electronic communication. If a Commonwealth law requires you to: give information in writing. provide a handwritten signature.","Business as usual","No"]
[null,"Equal Employment Opportunity (Commonwealth Authorities) Act 1987 (Cth)","This Act requires authority (includes PWC) to establish and implement an equal employment opportunity program designed to ensure that appropriate action is taken by the authority to eliminate discrimination by it against; and to promote equal opportunity for; women and persons in designated groups in relation to employment matters. ","Business as usual","No"]
[null,"Environment Protection and Biodiversity Conservation Act 1999 (Cth) (and regulations).","This Act provides a legal framework to protect and manage nationally and internationally important flora, fauna, ecological communities and heritage places.\nUnder the Act, actions that have, or are likely to have, a significant impact on a matter of national environmental significance require approval from the Australian Government Minister for the Environment\nThe following is protected under the Act:\nMatters of national environmental significance, World heritage properties and national heritage places, Wetlands of international importance, Threatened species and ecological communities, Migratory species, Commonwealth marine areas, Great Barrier Reef Marine Park, Nuclear actions, & Water resources","Business as usual","No"]
[null,"Fair Work Act 2009 (Cth) (and related legislation and regulations)","The Fair Work Act (2009) anti-bullying amendments came into effect on 1 January 2014, and have the potential to significantly alter the workplace practices of employers.\n ","Business as usual","No"]
[null,"Fringe Benefits Tax Act 1986 (Cth)\nFringe Benefits Tax Assessment Act 1986 (Cth)\nFringe Benefits Tax Regulations 1992 (Cth)","These instruments provide for a system of tax payable by employers for benefits paid to an employee (or an employee's associate) in place of salary or wages (i.e. Fringe Benefits). ","Opex","No"]
[null,"Fuel Tax Act 2006 (Cth)","This Act provides for a system system of fuel tax credits for business taxpayers registered for GST where a) fuel is acquired, manufactured or imported for use in carrying on the enterprise, or b) where fuel is acquired, manufactured or imported to make taxable supplies ","Business as usual"," "]
[null,"Income Tax Act 1986 (Cth)","This Act provides for a system of taxation of income.","Business as usual","No"]
[null,"Income Tax Assessment Act 1936 (Cth)\nIncome Tax Assessment Act 1997 (Cth)\nIncome Tax Assessment Regulations 1997 (Cth)\nIncome Tax Regulations 1936 (Cth)","This Act provides for the imposition, assessment and collection of income tax.","Business as usual","No"]
[null,"Modern Slavery Act 2018 No. 153 (CTH)","An Act to make provision about slavery, servitude and forced or compulsory labour and about human trafficking, including provision for the protection of victims; to make provision for an Independent Anti-slavery Commissioner; and for connected purposes. The Act established a national Modern Slavery Reporting Requirement (Reporting Requirement). This Reporting Requirement applies to large businesses and other entities in the Australian market with annual consolidated revenue of at least AUD$100 million.","Capex/Opex","No"]
[null,"National Greenhouse and Energy Reporting Act 2007 (Cth)\nNational Greenhouse and Energy Reporting Regulations 2008 (Cth)","Single national framework for reporting and disseminating company information about greenhouse gas emissions, energy production, energy consumption and other information specified under NGER legislation.\n• The objectives of the NGER scheme are to:\no inform government policy\no inform the Australian public\no help meet Australia's international reporting obligations\no assist Commonwealth, state and territory government programmes and activities, and\no avoid duplication of similar reporting requirements in the states and territories.\nRequires an entity to be registered under the Act where its emissions/energy produced or energy consumed meets the relevant thresholds as set out in section 13 of the Act.","Business as usual","No"]
[null,"Native Title Act 1993 (Cth) (and Regulations)","This Act purports to provide for the recognition and protection of native title; and to establish ways in which future dealings affecting native title may proceed and to set standards for those dealings; and to establish a mechanism for determining claims to native title; and to provide for, or permit, the validation of past acts, and intermediate period acts, invalidated because of the existence of native title.","Business as usual","No"]
[null,"Ombudsman Act 1976 (CTH)","The Ombudsman Act provides that the Ombudsman is to investigate the administrative actions of Australian Government departments / agencies and prescribed private sector organisations, and sets out the limits on his jurisdiction.","Business as usual","No"]
[null,"Privacy Act 1988 (Cth) (and Regulations) "," The objects of this Act are:\n- to promote the protection of the privacy of individuals;\n- and to recognise that the protection of the privacy of individuals is balanced with the interests of entities in carrying out their functions or activities; and\n- to provide the basis for nationally consistent regulation of privacy and the handling of personal information; and\n- to promote responsible and transparent handling of personal information by entities; and\n- to facilitate an efficient credit reporting system while ensuring that the privacy of individuals is respected; and\n- to facilitate the free flow of information across national borders while ensuring that the privacy of individuals is respected; and\n- to provide a means for individuals to complain about an alleged interference with their privacy; and\n- to implement Australia’s international obligation in relation to privacy.","Business as usual","No"]
[null,"Privacy Regulation 2013 (Cth)","See Act above. ","Business as usual","No"]
[null,"Racial Discrimination Act 1975 (Cth) (and Regulations)","This Act seeks to eliminate racial and other discrimination by making racial discrimination in certain contexts unlawful.","Business as usual","No"]
[null,"Renewable Energy (Electricity) Act","The Renewable Energy Target legislation provides an incentive for investment in renewable energy power stations and smaller systems while ensuring the energy sources used are ecologically sustainable.","Business as usual","No"]
[null,"Security of Critical Infrastructure Act","The Security of Critical Infrastructure Act 2018 (the Act) seeks to manage the complex and evolving national security risks of sabotage, espionage and coercion posed by foreign involvement in Australia's critical infrastructure.","Capex/Opex","Yes"]
[null,"Sex Discrimination Act 1984 (Cth) (and regulations)","This Act makes it unlawful to discriminate on the grounds of sex, sexual orientation, gender identity, intersex status, marital or relationship status, pregnancy, potential pregnancy, breastfeeding or family responsibilities. It also makes sexual harassment unlawful. ","Business as usual","No"]
[null,"Spam Act","The Spam Act 2003 (Cth) is an Act passed by the Australian Parliament in 2003 to regulate commercial e-mail and other types of commercial electronic messages. The Act restricts spam, especially e-mail spam and some types of phone spam, as well as e-mail address harvesting.","Business as usual","No"]
[null,"Telecommunications (Interception and Access) Act 1979 (Cth)\nTelecommunications (Interception and Access) Regulations 1987 (Cth)","This Act regulates access to telecommunications content and data in Australia. ","Business as usual","No"]
[null,"Telecommunications Act 1997 (Cth)\nTelecommunications Regulations 2001 (Cth)","To operate a network unit (being a line link that connects distinct places in Australia) an owner must have a carrier licence. A constitutional corporation or a public body may apply to the ACMA for a carrier licence. ","Business as usual","No"]
[null,"Trade Marks Act 1995 (Cth)","This Act provides for the regulation of trade marks, collective trade marks, certification trade marks and defensive trade marks and sets out and protects the rights deriving from registration. ","Business as usual","No"]
[null,"Workplace Gender Equality Act 2012 (Cth)","This Act aims to improve and promote equality between all genders in the workplace. ","Business as usual","No"]
[]
[]
[null,"NORTHERN TERRITORY LEGISLATION"]
[null,"Anti-Discrimination Act","The Anti-Discrimination Act aims to promote equality of opportunity and eliminate discrimination against persons for various grounds, including race, sex, sexuality, age, marital status etc. The Act establishes the Anti-Discrimination Commissioner and imposes obligations on various sectors, including employers, educators, accommodation owners etc.","Business as usual","No"]
[null,"Building Act (and Regulations)","The Building Act establishes technical standards for buildings and regulates all aspects of the building industry, including permits, registration of practitioners, and the establishment of a building appeal process.","Capex/Opex","No"]
[null,"Bushfires Management Act (and regulations)","The Bushfires Management Act provides mechanisms for the suppression and prevention of bushfires by, among other things, establishing fire protection zones and fire danger areas,  and establishing councils and committees with powers and functions.","Business as usual","No"]
[null,"Business Tenancies (Fair Dealings) Act 2003 (NT) (and Regulations)"," "," "," "]
[null,"Construction Contracts (Security of Payments) Act","The Construction Contracts (Security for Payments) Act establishes a system to secure payments under construction contracts and provide for the adjudication of disputes about payments.","Business as usual","No"]
[null,"Consumer Affairs and Fair Trading Act","The Consumer Affairs and Fair Trading Act applies the Australian Consumer Law as a law of the Territory, and provides other provisions related to consumer protection.","Business as usual","No"]
[null,"Dangerous Goods Act (NT) (and Regulations)","The Dangerous Goods Act gives provision to the storage, handling and transport of certain dangerous goods. The Act sets out penalties for non compliance. Owners or operators of infrastructure used in connection with dangerous goods also have obligations under this Act. The legislation adopts the Australian Dangerous Goods Code which applies to applies to dangerous goods classified as gases, flammable liquids, corrosive substances, oxidizing substances, substances dangerous if wet etc. ","Business as usual","No"]
[null,"Electrical Workers and Contractors Act (and regulations)","The Electrical Workers and Contractors Act provides for the licensing of electrical workers and contractors. The Act establishes the Electrical Workers and Contractors Licensing Board, and sets out all requirements related to licensing.","Business as usual","No"]
[null,"Electricity Reform Act","The Electricity Reform Act regulates the electricity supply industry in the Northern Territory","Capex/Opex","Yes"]
[null,"Electricity Reform (Administration) Regulations","This Regulation regulates licences, contestable customers and vegetation clearance.","Capex/Opex","No"]
[null,"Electricity Reform (safety and technical) Regulations","This Regulation provides safety and technical requirements which must be complied with.","Capex/Opex","No"]
[null,"Electricity Reform (system control and market operator functions code) Regulations","This Regulation sets out a System Control and Market Operator Functions Code that electricity entities must comply with, to the extent it is applicable to PWC.","Capex/Opex","No"]
[null,"Electronic Transactions (Northern Territory) Act 2000 (NT) (and Regulations)","This Act may be cited as the Electronic Transactions (Northern Territory) Act 2000. This Act comes into operation on the date fixed by the Administrator by notice in the Gazette. (d) enables business and the community to use electronic communications in their dealings with government.","Business as usual","No"]
[null,"Emergency Management Act","The Emergency Management Act makes provisions for emergency managmenet plans at a local, regional and Territory level. The Act confers special powers and duties in the event of an emergency, and establishes the Territory Emergency Management Council. The special powers contained in the Act could mean that PWC would be obliged co comply with various directions made by an authorised officer during a state of emergency or disaster, such as a direction to assist in tasks to save life or property, or a direction to close an area (s 24).","Capex/Opex","No"]
[null,"Environmental Offences and Penalties Act","This Act establishes penalties for offences under the Regulations or other Acts which prescribe offences as being an environmental offence. ","Business as usual","No"]
[null,"Fences Act","The Fences Act requires land owners to equally contribute to fences with adjoining properties, and provides mechanisms for the resolution of disputes.","Business as usual","No"]
[null,"Financial Transaction Reports Act 1992 (NT)","An Act to provide for the giving of further information in relation to suspect transactions reported under the Financial Transaction Reports Act 1988 of the Commonwealth and the giving of information in relation to other suspect transactions, and for related purposes.","Business as usual","No"]
[null,"Financial Management Act (and Regulations)","The Financial Management Act provides terms for the financial manageement of the NT and certain government business activities.  The CEO of PWC is the Accountable Officer, and has obligations under the Act related to trust accounts, the preparation of financial statements, and proper record keeping of financials. ","Business as usual","No"]
[null,"Fire and Emergency Act","The Fire and Emergency Act establishes the fire and rescue service, and provides mechanisms for responding to fires and emergencies to protect life, property and the enivironment. Among the various powers contained in the Act are powers to destroy dangerous structures, to take equipment, cause the electricity supply to a building to be shut off etc.","Business as usual"," "]
[null,"Fire and Emergency Regulations","These Regulations impose a number of obligations on owners/occupiers of land re firebreaks, smoke alarms, stacking requirements, waste, and emergency planning and evacuation.","Business as usual","No"]
[null,"Independent Commissioner Against Corruption Act 2017 (NT)","The purpose of the Act is to address improper conduct in public administration. Importantly, the Act provides built in protections for people who report improper conduct and, who may put themselves at risk of retaliation as a result.","Business as usual","No"]
[null,"Information Act (NT) (and Regulations)","The Information Act provides public access to government held information, and other related matters. The Act requires public sector entities to collect and handle personal information responsibly, promote appropriate records and archives management, and to provide public access to certain information.","Business as usual","No"]
[null,"Land Title Act","This Act consolidates the law regarding the registration of land and interests in land. The Act provides a mechanism for easements to be registered against land titles.","Business as usual","No"]
[null,"Land Title Regulations","These Regulations outline obligations in relation to gaining written consent, requirements for a plan of termination of scheme and requirements for a plan of termination of development.","Business as usual","No"]
[null,"Lands Acquisition Act","This Act provides mechanisms for the acquisition of land. This Act gives the Minister the power generally to acquire land for any purpose.","Business as usual","No"]
[null,"Law of Property Act","This Act consolidates the law regarding conveyancing, property, and contract. The Act deals with, among other things, easements, covenants, freehold estates and contracts for the sale of land.","Business as usual","No"]
[null,"Motor Vehicles Act","This Act governs all aspect of Motor Vehicles in the Territory, including registration, licences, public roads, plates, etc.","Business as usual","No"]
[null,"National Electricity (Northern Territory) (National Uniform Legislation) Act\nNational Electricity Law (NEL)","This Act adopts the National Electricity Law (NEL), subject to amendments made by the National Electricity (Northern Territory) (National Uniform Legislation) (Modification) Regulations. The NEL sets the high level legislative framework within which the market operates and is developed, as well as establishing some high level rights and obligations for both market participants and market institutions. Another key set of obligations under the NEL involve the provision of information to the regulator. ","Capex/Opex","Yes"]
[null,"Northern Territory Aboriginal Sacred Sites Act","This act provides for the protection of an entry onto certain Aboriginal Sacred Sites, and the avoidance of development on sacred sites.","Capex/Opex","No"]
[null,"Northern Territory Environment Protection Authority Act","This Act makes its an offence for a person to provide information or documents to the Territory or EPA that the person knows is misleading and the person does not draw the misleading information to the agency's attention.","Business as usual","No"]
[null,"Occupational Licensing (National Uniform Legislation) Act 2011","This Act provides for the licensing of electricians, plumbers and gas fitters.  It creates an offence for a body corporate to carry out work of that nature without a licence or to hold out an unlicensed person as being licensed to perform that particular work.","Business as usual","No"]
[null,"Payroll Tax Act","This Act regulates the payment of payroll tax.","Business as usual","No"]
[null,"Power and Water Corporation Act","This is the primary statutory instrument which establishes and governs the Power and Water Corporation and the performance of its functions.","Business as usual","No"]
[null,"Price Exploitation Prevention Act","This Act empowers the Territory to gather information and regulate transactions in circumstances where a disaster or lack of competition in the market has resulted or may result in price exploitation.","Business as usual","No"]
[null,"Public Employment (Mobility) Act","This Act regulates the accrual of conditions of employment of public sector employees, including long service leave and sick leave.","Business as usual","No"]
[null,"Public Interest Disclosure Act","This Act protects whistle blowers who make appropriate disclosures of information concerning public offices and public bodies, including statutory corporations and employees of statutory corporations.","Business as usual","No"]
[null,"Public Sector Employment and Management Act (and Regulations)","This Act regulates the employment conditions of public sector employees, including statutory corporation employees.","Business as usual","No"]
[null,"Publications (Legal Deposit) Act 2004","This Act provides for the circumstances in which publications including handbooks, guides, pamplets and newsletters must be provided to the Territory Government.","Business as usual","No"]
[null,"Return to Work Act (and regulations)","This Act regulates workers compensation payments.","Business as usual","No"]
[null,"Special Purposes Leases Act (and Regulations)","This Act provides for the granting of leases to statutory corporations of land belonging to the Territory.","Business as usual","No"]
[null,"Stamp Duty Act","This Act regulates stamp duty in the Territory.","Business as usual","No"]
[null,"Superannuation Act (and Regulations)","This Act provides for superannuation schemes for public sector employees.","Business as usual","No"]
[null,"Superannuation Guarantee (Safety Net) Act","This Act provides for superannuation benefits for certain employees in the public sector.","Business as usual","No"]
[null,"Taxation Administration Act","This Act provides for the administration and enforcement of Territory Taxation Laws.","Business as usual","No"]
[null,"Training and Skills Development Act","This Act regulates the hiring and conditions of trainees and apprentices","Business as usual","No"]
[null,"Utilities Commission Act","This Act creates the Utilities Commission, sets out its functions and regulates the performance of its functions","Business as usual","No"]
[null,"Waste Management and Pollution Control Act (and Regulations)","This Act regulates environmental licences, reporting obligations and incidents which cause pollution","Capex/Opex","No"]
[null,"Weeds Management Act","This Act regulates obligations of owners and occupiers of land with respect to the propagation and management of certain weeds","Capex/Opex","No"]
[null,"Work Health and Safety (National Uniform Legislation) Act","This Act regulates occupational health and safety","Business as usual","No"]
[null,"Work Health and Safety (National Uniform Legislation) Regulations","The Regulations set out occupational health and safety obligations on topics including general risk management, training, hazardous work, confined spaces, high risk works, accrediation of relevant offficers, demolition work, licensing, plant and structures, hazardous chemicals, and administration of WHS matters","Business as usual","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"PWC (Networks) Licence","This licence issued by the Utilities Commisiosn authorises PWC to own and operate an electricity network within the licence area and to connect the electricity network to another electricity network. ","Capex/Opex","No"]
[null,"PWC (System Control) Licence","This licence issued by the Utilities Commission grants PWC a licence to exercise system control over the power system. The licence defines PWC's statutory obligations in order to ensure the safe, secure and reliable operation of the regulated power systems in the NT.","Capex/Opex","No"]
[null,"PWC (Generation) Licecne","This licence issued by the Utilities Commission grants PWC a licence to generate electricity at the electricity generating plants described in schedule 2 for sale as contemplated by paragraph (b) or in any retail licence held by the licensee; and sell and retail electricity to electricity entities holding a retail licence or a generation licence.","Capex/Opex","No"]
[null,"PWC (Retail) Licence","This licence issued by the Utilities Commission grants PWC a licence to trade in electricity; and sell and retail electricity to contestable customers; and sell and retail electricity to non-contestable customers, but only in respect of electrical installations or premisis which are located within the retail area.","Capex/Opex","No"]
[null,"RULES"]
[null,"National Electricity Rules as applied in Northern Territory","The National Electricity Rules set out the detailed obligations of market participants. Key classes of obligations relate to system security, connection and planning, preparing a regulatory proposal and metering.\n","Capex/Opex","No"]
[null,"Chapter 1 Introduction","Applicable from 1 July 2017 wth exceptions: \n1.11 (AEMO Rule Funds) has no effect","N/A","No"]
[null,"Chapter 2 Registered Participants and Registration","Not currently applicable but possible in the future","N/A","No"]
[null,"Chapter 2A Regional Structures","Not currently applicable but possible in the future","N/A","No"]
[null,"Chapter 3 Market Rules","Not currently applicable but possible in the future","N/A","No"]
[null,"Chapter 4 Power System Security","Not currently applicable but possible in the future","N/A","No"]
[null,"Chapter 5 Network Connection, Planning and Expansion","Applicable from 1 July 2019: \nr 5.0, 5.0A, 5.10.2, 5.11, 5.12 (other than clauses 5.12.1(b)(3), 5.12.2(c)(1), (5)(v), (6) and (8)), 5.13, 5.13A, Schedule 5.7, S5.8(except (b)(5)(iii), (h) and (i)), S5.9 except para (h)\n\nApplicable from 1 July 2018: \nPart B and C\n\nNot currently applicable but possible in the future: \nr 5.1 through to 5.9 clauses 5.10.1, 5.10.3, 5.12, 5.12.1(b)(3), 5.12.2(c)(1), (5)(v), (6) and (8), r 5.14 through to 5.22, Schedules S5.1a through to S5.6, S5.8 ((b)(5)(iii), (h) and (i)), S5.9 (h)\n","Capex/Opex","No"]
[null,"Chapter 5A Electricity connection for retail customers","Applicable from 1 July 2017:\nPart A (Preliminary only), Part E (except 5.A.E.2 and 5A.E.4(c) \n\nApplicable from 1 July 2019:\n5A.A.2, Part B, Part C (except cl 5A.C.1(c) and (d)), Part D (except 5A.D.1(a)(7) and (b) and 5A.D.1A), 5A.E.2, 5A.E.4 except (c), Part F (except 5A.F.5(b)(2)), Schedule 5A.1\n\nApplicable once NERL implemented in NT: \nPart C (5A.C.1(c) and (d)), 5A.E.4(c), 5A.F.5(b)(2) \n\nNot currently applicable but possible in the future: \n5.A.A.3, 5A.D.1(a)(7) and (b), 5A.D.1A,  Part G ","Capex/Opex","No"]
[null,"Chapter 6 Economic Regulation of Distribution Services","Applicable from 1 July 2017 with some exceptions.\n\nApplicable from 1 July 2019:\n6.18.9(a)(3), Parts J to N, Schedule 6.2.2B(b) and (c)\n\nExpiring on 1 July 2024:\n6.4.3, 6.6.1(1AB), modifications to 6.6.1(7A), 6.6.1AA, 6.6.1AB, 6.11.1(ba), 6.18.5(ha), modifications to 6.2.5(c)\n\nApplicable once NERL implemented in NT: \n6.6.1(a1)(4), (c)(6)(iii), (l) and (m)\n\nNot currently applicable but possible in the future\nclauses S6.2.1(d) and S6.2.2","Capex/Opex","No"]
[null,"Chapter 6A Economic Regulation of Transmission Services","Not currently applicable but possible in the future","Capex/Opex","No"]
[null,"Chapter 6B Retail Markets","Not currently applicable but possible in the future","Capex/Opex","No"]
[null,"Chapter 7 Metering","Not applicable, Ch 7A applies as a substitute for Ch 7 taking effect at an unspecificed time in the future","Capex/Opex","No"]
[null,"Chapter 7A Metering","Applicable from 1 July 2019","Capex/Opex","No"]
[null,"Chapter 8 Administrative Function","Applicable from 1 July 2017 except the following: \n8.1.3(b)(5) and (7), 8.6.1(d) and (e), 8.6.2(1), 8.6.6, 8.6.7, 8.7.2(a)(2) and (4) and (b)(2), 8.7.6, Part E, Part G\n\nApplicable from 1 July 2019: \nPart B, Part H","Capex/Opex","No"]
[null,"Chapter 8A","Applicable from 1 July 2017: \n8A.14, 8A.15","Capex/Opex","No"]
[null,"Chapter 9 Jurisdictional derogations & transitional arrangements","Not applicable (applies to other jurisdictions)","Capex/Opex","No"]
[null,"Chapter 10 Glossary","Applicable, some definitions to change on 1 July 2017, some definitions to expire on 1 July 2029","Capex/Opex","No"]
[null,"Chapter 11 Savings and Transitional Rules","Not applicable (applies to other jurisdictions)\nNo effect for:\nParts A to ZZI, ZZK, ZZL, ZZN (except for clause 11.86.8), ZZO to ZZT, ZZV and ZZX","Capex/Opex","No"]
[null,"Chapter 11A NT Savings and Transitional Rules","Applicable from 1 July 2019","Capex/Opex","No"]
[null,"ORDERS"]
[null,"Electricity Pricing Order 1 July 2022 - 30 June 2023","Electricity retail prices charged to residential and commercial customers (those consuming less than 750 megawatt hours of electricity per year) are regulated by the NT Government through a pricing order made by the Treasurer under the Electricity Reform Act 2000. The Pricing Order sets the retail prices that customers may be charged for electricity and related services. Compliance with the Electricity Pricing Order is enforced by the Commission.","Capex/Opex","No"]
[null,"System Control Charges – from 1 July 2022","The Power System Controller (a standalone business unit within Power and Water Corporation) is licensed by the Commission to manage the day-to-day operation of the power system. While the Commission is responsible for the regulation of the NT electricity supply industry, the function of monitoring and controlling the power system lays with the Power System Controller, with broad oversight by the Commission. Under the Electricity Reform Act 2000, a system controller is entitled to impose and recover charges relating to the operations of system control. The schedule of charges is approved by the Commission.","Capex/Opex","No"]
[null,"Ancillary services charges","Ancillary services are defined in the System Control Technical Code and include: voltage control, reactive power control, frequency control and black start capability. The Utilities Commission Regulations authorise the Commission to make determinations relating to prices for providing ancillary services in the electricity supply industry. The price for ancillary services provided by Territory Generation in the Darwin‑Katherine system is covered by the System Control Technical Code.","Capex/Opex","No"]
[null,"CODES"]
[null,"AS/NZ 3000:2007 Electrical installations Standard (required to be complied with under the Electricity Reform (Safety and Technical) Regulations 2016 made under the Electricity Reform Act 2000 (NT))","• This standard sets out requirements for the design, construction and verification of electrical installations, including selection of equipment. \n• Intended to protect persons, livestock and property from electric shock, fire, and physical injury hazards.\n• This standard may be applied through legislative requirements, made in each State or Territory of Australia and New Zealand. \n","Business As Usual","No"]
[null,"Commonwealth Model Work Health and Safety Codes of Practice","National Harmonisation of Work Health and Safety Code of Practice","Business As Usual","No"]
[null,"Electricity Industry Performance Code and Gudielines","The Electricity Industry Performance Code sets out: guaranteed service levels performance indicators and payment levels, generation service performance indicators for reporting purposes, network service performance indicators for reporting and network target standards and retail service performance indicators for reporting purposes, which includes retail performance for customers taking, or likely to take less than 160 megawatt hours of electricity during the reporting period, and hardship indicators for residential customers.","Capex/Opex","No"]
[null,"Electricity Reform (System Control and Market Operator Functions Code) Regulations","The Electricity Reform (System Control and Market Operator Functions Code) Regulations requires an electricity entity to comply with the  Code,  as  set  out in the Schedule which covers out-of-balance energy services.","Capex/Opex","No"]
[null,"Electricity Retail Supply Code (NT)","Sets out the rules governing the processes for transferring customers, the obligations of retailers and network providers, retailer of last resort and dispute resolution procedures.","Capex/Opex","No"]
[null,"National Construction Code (including Building Code of Australia)","NCC and Building Code of Australia published by the Australian Building Codes Board as in force from time to time (adopted by States and Territories on 1 May 2016)","Business As Usual","No"]
[null,"Network Technical Code and Network Planning Criteria (NT)","The Network Technical Code and Network Planning Criteria sets out the requirements that apply to all facets of the electricity network. The Network Technical Code is applicable to all connected equipment but particularly generators and large loads. The Network Planning Criteria documents the criteria that are applied to ensure that PWC's networks meet safety standards, provide reliable supply, meet environmental standards, and optimise equipment utilisation. ","Capex/Opex","No"]
[null,"Northern Territory Electricity Ring-fencing Code","A key aspect of PWC's licence conditions is the requirement that certain business units be ring-fenced to ensure against anti-competitive market behaviour. The objective of the Ring-fencing Code is to create an enfironment where the price, quantity and quality of electricity sold to end-use consumers is not biased as a result of PWC's vertical integration.","Business As Usual","No"]
[null,"System Control Technical Code (NT) ","Power and Water Corporation is required to prepare a System Control Technical Code and submit it for approval to the Commission under section 38 of the Electricity Reform Act. The Code sets out Power and Water Corporation's competitively neutral operating protocols, arrangements for system security and system dispatch, as well as arrangements for the interruption of supply. Power and Water Corporation is also required to monitor and enforce the Code on system participants to ensure that the power system is operated in a manner that is safe and secure.","Capex/Opex","No"]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"AER Consumer engagement guideline for network service providers (1 Aug 2013)","Sets out framework for engaging consumers and integrating the long-term interests of consumers into expenditure plans","Opex","No"]
[null,"AER Cost Allocation Guideline (Distribution) (1 Jan 2008)","These Guidelines set out arrangements to manage the attribution of direct costs and the allocation of shared costs by DNSPs between different categories of distribution services. Specifically the guidelines relate to the preparation by a DNSP of its Cost Allocation Method.","Business As Usual","No"]
[null,"AER Distribution Confidentiality Guidelines (19 Nov 2013) ","Clause 16.4A(b) of the NER requires these guidelines specify the manner in which the DNSP may make confidentiality claims in its regulatory proposal, which may include categories of confidential information by reference to which the DNSP must calssify any claims of confidentiality in their regulatory porposals. \n(d) The guidelines are binding on the AER and each DNSP to which they apply.\n","Confidentiality template","No"]
[null,"AER Expenditure forecast assessment guideline - Regulatory information notices for category analysis (7 Mar 2014)","Clause 6.4.5(a) of the NER requires these guidelines specify the approach the AER proposes to use to assess the foreceasts of operating expendutiure and capital expenditure that form part of DNSP's regulatory proposals and the info the AER requires for the purposes of the assessment. ","Capex and Opex","No"]
[null,"AER Expenditure forecast assessment guideline - Regulatory information notices for economic benchmarking (28 Feb 2014)","The Guideline specifies the information required by the AER to assess expenditure and colected by way of RINs.","Capex and Opex","No"]
[null,"AER Expenditure incentives guideline (29 Nov 2013)","Establishes incentives to spend capex efficiently","Capex and Opex","No"]
[null,"AER National Electricity Connection Charge Guideline (1 July 2012)","Clause 5A.E.3 of the NER requires the AER to publish these guidelines to ensure that connection charges are reasonable; to provide a user-pays signal to reflect the efficient cost of proivinging the connection services; and limit cross-subsidisation of connection costs between different classes of retail customer. \nRule 5A.E.3(ga) - Connection charge guidelines in force in the other participating jurisdictions on 1 July 2017 are taken to be those in force in this jurisdiction (NT).","Customer capex","No"]
[null,"AER Rate of Return Guideline (17 Dec 2013)","Establishes the AER's approach to determining the rate of return on regulated assets","Rate of Return","No"]
[null,"AER Ring-fencing Guideline (electricity distribution) ","Applies from 1 July 2019- Rule 6.17.1.1A, with amendments specified in 6.17.1B.  Deal with the accounting and functional separation of the provision of direct control services from the provision of other services.","Cost Allocation","No"]
[null,"AER Shared Asset Guideline (29 November 2013)","Establishes a cost reduction approach in situations where unregulated revenues are earned from regulated assets.","Rate of Return","No"]
[null,"Corporate Governance and Reporting Framework - Government Owned Corporations","The framework provides direction and advice as to the processes, timeframes, content and controls associated with the governance relationships between GOCs, ministers and the Department of Treasury and Finance (DTF).","Business As Usual","No"]
[null,"Utilities Commission Compliance Framework and Reporting Guidelines","The key features of the guidelines are the requirement for annual compliance reporting, additional information on the reporting of material compliance breaches and an annual declaration from the Board of Directors.","Business As Usual","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[null,"Nil"]
[]
[]
[null,"OTHER"]
[null,"AER Regulatory Information Notice for PWC  dated 9 November 2017","Regulatory Information Notice issued to PWC on 9 November 2017 under Division 4 of Part 3 of the National Electricity (Northern Territory) Law","Capex/Opex","No"]
[null,"Approved Target Standards Determination 2014-2019 (NT)","Ceases to apply on 1 July 2019",0,"No"]
[null,"Business-to-Business Process Service Order Procedure (NT)","This document defines the procedure and data requirements which apply to PWC in relation to service orders received from Retailers.","Business as usual ","No"]
[null,"Easement Guidelines (NT)","This procedure provides guidelines covering the management of electricity easements. It is applicable to all electricity easements covering Power and Water underground and overhead power lines.","Business as usual ","No"]
[null,"Northern Territory Emergency Management Plan","PWC is identified as the controlling authority and hazard management authority primarily responsible for controlling a response to a major power outage, and to lead the Public Utilities functional group ","Business as usual ","No"]

{"sheet":"7.4 Shared Assets","index":26,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[6,1,7,1],[6,2,7,2],[26,2,26,8],[27,2,27,8],[28,2,28,8],[29,2,29,8],[30,2,30,8],[31,2,31,8],[38,2,38,8],[39,2,39,8],[40,2,40,8],[32,2,32,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service",{"$f":"CONCATENATE(\"Shared asset unregulated revenue  \n($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  \n($0's, real June 2024)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", FRCP_y5)","v":"Total 2024-25 to 2028-29"}]
[null,"Shared Asset","Fibre optic cable used for PWC's communications network is also used by a third party",1099094.0194298832,1075651.4695242832,1069857.1933278237,1070692.5460646558,1071528.5446656896,1072365.1948757102,1073202.5026282601,{"$f":"SUM(F9:J9)","v":5357645.9815621395}]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]
[null,"Fibre optic cable","Not applicable"]

{"sheet":"7.7 TSS-LRMC","index":27,"n_rows":154,"n_cols":25,"rows_kept":154,"cut":false,"hidden":false,"merged":[[68,1,69,1],[88,1,89,1],[5,3,6,4],[10,1,11,1],[22,1,23,1],[34,1,35,1],[48,1,49,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is Power and Water using the 'Average Incremental Cost' approach?"}]
[null,null,null,null,null,"YES"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C12,4)+1)&\"-\"&MID(C12,3,2)+2),VALUE(LEFT(C12,4)+1))","v":"2023-24"},"2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39","2039-40","2040-41","2041-42","2042-43","2043-44","2044-45"]
[null,"Replacement expenditure",4346469.861139914,6568653.1062947959,3973545.7695348249,4362908.5291616367,2518051.1755079553,1455943.301960991,1427623.8068821228,3521885.0786403199,3521885.0786403199,2516367.799519551,2519836.7901637591,2519836.7901637591,2519836.7901637591,2519836.7901637591,2519836.7901637498,2519836.7901637591,2519836.7901637591,2519836.7901637787,2519836.7901637591,2519836.7901637498,2519836.7901637591,2519836.7901637591,2519836.7901637591]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",1843205.0497427799,3471764.8464598176,1666077.3864603189,1647081.7972659871,2281188.571742571,1748559.5332512863,1628570.6405079814,2040921.1179186772,2040921.1179186772,1458227.0766406513,1460237.3456033061,1460237.3456033061,1460237.3456033061,1460237.3456033061,1460237.3456033003,1460237.3456033061,1460237.3456033061,1460237.3456033175,1460237.3456033061,1460237.3456033003,1460237.3456033061,1460237.3456033061,1460237.3456033061]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Export services",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex",{"$f":"SUM(C13:C19)","v":6189674.9108826937},{"$f":"SUM(D13:D19)","v":10040417.952754613},5639623.1559951436,6009990.3264276236,4799239.7472505262,3204502.8352122772,3056194.4473901042,5562806.196558997,5562806.196558997,3974594.8761602025,3980074.135767065,3980074.135767065,3980074.135767065,3980074.135767065,3980074.1357670501,3980074.135767065,3980074.135767065,3980074.1357670962,3980074.135767065,3980074.1357670501,{"$f":"SUM(W13:W19)","v":3980074.135767065},3980074.135767065,3980074.135767065]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C24,4)+1)&\"-\"&MID(C24,3,2)+2),VALUE(LEFT(C24,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D24,4)+1)&\"-\"&MID(D24,3,2)+2),VALUE(LEFT(D24,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E24,4)+1)&\"-\"&MID(E24,3,2)+2),VALUE(LEFT(E24,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F24,4)+1)&\"-\"&MID(F24,3,2)+2),VALUE(LEFT(F24,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G24,4)+1)&\"-\"&MID(G24,3,2)+2),VALUE(LEFT(G24,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H24,4)+1)&\"-\"&MID(H24,3,2)+2),VALUE(LEFT(H24,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I24,4)+1)&\"-\"&MID(I24,3,2)+2),VALUE(LEFT(I24,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J24,4)+1)&\"-\"&MID(J24,3,2)+2),VALUE(LEFT(J24,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K24,4)+1)&\"-\"&MID(K24,3,2)+2),VALUE(LEFT(K24,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L24,4)+1)&\"-\"&MID(L24,3,2)+2),VALUE(LEFT(L24,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M24,4)+1)&\"-\"&MID(M24,3,2)+2),VALUE(LEFT(M24,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N24,4)+1)&\"-\"&MID(N24,3,2)+2),VALUE(LEFT(N24,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O24,4)+1)&\"-\"&MID(O24,3,2)+2),VALUE(LEFT(O24,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P24,4)+1)&\"-\"&MID(P24,3,2)+2),VALUE(LEFT(P24,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q24,4)+1)&\"-\"&MID(Q24,3,2)+2),VALUE(LEFT(Q24,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R24,4)+1)&\"-\"&MID(R24,3,2)+2),VALUE(LEFT(R24,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S24,4)+1)&\"-\"&MID(S24,3,2)+2),VALUE(LEFT(S24,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T24,4)+1)&\"-\"&MID(T24,3,2)+2),VALUE(LEFT(T24,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U24,4)+1)&\"-\"&MID(U24,3,2)+2),VALUE(LEFT(U24,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"Replacement expenditure",4943500.7609208832,5298592.1724469131,6501072.0451937234,5941074.2158907605,3712159.6275835945,3702881.2764092679,3655343.9205816099,4822089.1455752496,4822089.1455752496,3445356.5580347916,3450106.2252607299,3450106.2252607299,3450106.2252607299,3450106.2252607299,3450106.2252607164,3450106.2252607299,3450106.2252607299,3450106.2252607564,3450106.2252607299,3450106.2252607164,3450106.2252607299,3450106.2252607299,3450106.2252607299]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",3362578.7140164757,8789435.015021665,6364609.8913930831,2978351.5126095684,3072889.9440815421,2131173.2158660535,1914421.4725923655,4087637.1093686786,4087637.1093686786,2920594.5590103115,2924620.8047771929,2924620.8047771929,2924620.8047771929,2924620.8047771929,2924620.8047771817,2924620.8047771929,2924620.8047771929,2924620.8047772152,2924620.8047771929,2924620.8047771817,2924620.8047771929,2924620.8047771929,2924620.8047771929]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Export services",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex",{"$f":"SUM(C25:C31)","v":8306079.4749373589},{"$f":"SUM(D25:D31)","v":14088027.187468577},12865681.936586807,8919425.728500329,6785049.5716651361,5834054.4922753219,5569765.3931739759,8909726.2549439277,8909726.2549439277,6365951.1170451026,6374727.0300379228,6374727.0300379228,6374727.0300379228,6374727.0300379228,6374727.0300378986,6374727.0300379228,6374727.0300379228,6374727.0300379712,6374727.0300379228,6374727.0300378986,{"$f":"SUM(W25:W31)","v":6374727.0300379228},6374727.0300379228,6374727.0300379228]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C36,4)+1)&\"-\"&MID(C36,3,2)+2),VALUE(LEFT(C36,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D36,4)+1)&\"-\"&MID(D36,3,2)+2),VALUE(LEFT(D36,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E36,4)+1)&\"-\"&MID(E36,3,2)+2),VALUE(LEFT(E36,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F36,4)+1)&\"-\"&MID(F36,3,2)+2),VALUE(LEFT(F36,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G36,4)+1)&\"-\"&MID(G36,3,2)+2),VALUE(LEFT(G36,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H36,4)+1)&\"-\"&MID(H36,3,2)+2),VALUE(LEFT(H36,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I36,4)+1)&\"-\"&MID(I36,3,2)+2),VALUE(LEFT(I36,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J36,4)+1)&\"-\"&MID(J36,3,2)+2),VALUE(LEFT(J36,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K36,4)+1)&\"-\"&MID(K36,3,2)+2),VALUE(LEFT(K36,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L36,4)+1)&\"-\"&MID(L36,3,2)+2),VALUE(LEFT(L36,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M36,4)+1)&\"-\"&MID(M36,3,2)+2),VALUE(LEFT(M36,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N36,4)+1)&\"-\"&MID(N36,3,2)+2),VALUE(LEFT(N36,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O36,4)+1)&\"-\"&MID(O36,3,2)+2),VALUE(LEFT(O36,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P36,4)+1)&\"-\"&MID(P36,3,2)+2),VALUE(LEFT(P36,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q36,4)+1)&\"-\"&MID(Q36,3,2)+2),VALUE(LEFT(Q36,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R36,4)+1)&\"-\"&MID(R36,3,2)+2),VALUE(LEFT(R36,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S36,4)+1)&\"-\"&MID(S36,3,2)+2),VALUE(LEFT(S36,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T36,4)+1)&\"-\"&MID(T36,3,2)+2),VALUE(LEFT(T36,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U36,4)+1)&\"-\"&MID(U36,3,2)+2),VALUE(LEFT(U36,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"Replacement expenditure",4217530.2973773703,4772247.2969695404,6153672.8641252043,5104345.2062654532,4420680.8216768689,4448756.1702898862,4441586.7855628058,4794117.0631810194,4794117.0631810194,3425370.6567771873,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274492,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274115,3430092.7720274115]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",1174495.1994622112,1192734.8549754519,1454488.9784571682,1441627.3358619537,1934595.7470186171,1521803.3655372181,1429609.9705931765,1449907.9217008282,1449907.9217008282,1035951.3513271265,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936378,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936265,1037379.4833936265]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex",{"$f":"SUM(C36:C42)","v":5392025.4968395811},5964982.1519449921,7608161.8425823729,6545972.5421274072,6355276.5686954856,5970559.535827104,5871196.7561559826,6244024.9848818481,6244024.9848818481,4461322.0081043141,4467472.2554210378,4467472.2554210378,4467472.2554210378,4467472.2554210378,4467472.2554210378,4467472.2554210378,4467472.2554210378,4467472.2554210871,4467472.2554210378,4467472.2554210378,{"$f":"SUM(W36:W42)","v":4467472.2554210378},4467472.2554210378,4467472.2554210378]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C50,4)+1)&\"-\"&MID(C50,3,2)+2),VALUE(LEFT(C50,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D50,4)+1)&\"-\"&MID(D50,3,2)+2),VALUE(LEFT(D50,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E50,4)+1)&\"-\"&MID(E50,3,2)+2),VALUE(LEFT(E50,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F50,4)+1)&\"-\"&MID(F50,3,2)+2),VALUE(LEFT(F50,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G50,4)+1)&\"-\"&MID(G50,3,2)+2),VALUE(LEFT(G50,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H50,4)+1)&\"-\"&MID(H50,3,2)+2),VALUE(LEFT(H50,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I50,4)+1)&\"-\"&MID(I50,3,2)+2),VALUE(LEFT(I50,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J50,4)+1)&\"-\"&MID(J50,3,2)+2),VALUE(LEFT(J50,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K50,4)+1)&\"-\"&MID(K50,3,2)+2),VALUE(LEFT(K50,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L50,4)+1)&\"-\"&MID(L50,3,2)+2),VALUE(LEFT(L50,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M50,4)+1)&\"-\"&MID(M50,3,2)+2),VALUE(LEFT(M50,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N50,4)+1)&\"-\"&MID(N50,3,2)+2),VALUE(LEFT(N50,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O50,4)+1)&\"-\"&MID(O50,3,2)+2),VALUE(LEFT(O50,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P50,4)+1)&\"-\"&MID(P50,3,2)+2),VALUE(LEFT(P50,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q50,4)+1)&\"-\"&MID(Q50,3,2)+2),VALUE(LEFT(Q50,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R50,4)+1)&\"-\"&MID(R50,3,2)+2),VALUE(LEFT(R50,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S50,4)+1)&\"-\"&MID(S50,3,2)+2),VALUE(LEFT(S50,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T50,4)+1)&\"-\"&MID(T50,3,2)+2),VALUE(LEFT(T50,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U50,4)+1)&\"-\"&MID(U50,3,2)+2),VALUE(LEFT(U50,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"LRMC-Related Operating Expenditure",142362.52295030197,230929.6129133561,129711.3325878883,138229.77750783533,110382.51418676211,73703.565209882363,70292.4722899724,127944.54252085692,127944.54252085692,91415.682151684668,91541.705122642496,91541.705122642496,91541.705122642496,91541.705122642496,91541.705122642161,91541.705122642496,91541.705122642496,91541.705122643209,91541.705122642496,91541.705122642161,91541.705122642496,91541.705122642496,91541.705122642496]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C51:C65)","v":142362.52295030197},{"$f":"SUM(D51:D65)","v":230929.6129133561},129711.3325878883,138229.77750783533,110382.51418676211,73703.565209882363,70292.4722899724,127944.54252085692,127944.54252085692,91415.682151684668,91541.705122642496,91541.705122642496,91541.705122642496,91541.705122642496,91541.705122642161,91541.705122642496,91541.705122642496,91541.705122643209,91541.705122642496,91541.705122642161,91541.705122642496,91541.705122642496,91541.705122642496]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C70,4)+1)&\"-\"&MID(C70,3,2)+2),VALUE(LEFT(C70,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D70,4)+1)&\"-\"&MID(D70,3,2)+2),VALUE(LEFT(D70,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E70,4)+1)&\"-\"&MID(E70,3,2)+2),VALUE(LEFT(E70,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F70,4)+1)&\"-\"&MID(F70,3,2)+2),VALUE(LEFT(F70,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G70,4)+1)&\"-\"&MID(G70,3,2)+2),VALUE(LEFT(G70,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H70,4)+1)&\"-\"&MID(H70,3,2)+2),VALUE(LEFT(H70,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I70,4)+1)&\"-\"&MID(I70,3,2)+2),VALUE(LEFT(I70,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J70,4)+1)&\"-\"&MID(J70,3,2)+2),VALUE(LEFT(J70,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K70,4)+1)&\"-\"&MID(K70,3,2)+2),VALUE(LEFT(K70,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L70,4)+1)&\"-\"&MID(L70,3,2)+2),VALUE(LEFT(L70,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M70,4)+1)&\"-\"&MID(M70,3,2)+2),VALUE(LEFT(M70,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N70,4)+1)&\"-\"&MID(N70,3,2)+2),VALUE(LEFT(N70,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O70,4)+1)&\"-\"&MID(O70,3,2)+2),VALUE(LEFT(O70,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P70,4)+1)&\"-\"&MID(P70,3,2)+2),VALUE(LEFT(P70,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q70,4)+1)&\"-\"&MID(Q70,3,2)+2),VALUE(LEFT(Q70,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R70,4)+1)&\"-\"&MID(R70,3,2)+2),VALUE(LEFT(R70,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S70,4)+1)&\"-\"&MID(S70,3,2)+2),VALUE(LEFT(S70,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T70,4)+1)&\"-\"&MID(T70,3,2)+2),VALUE(LEFT(T70,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U70,4)+1)&\"-\"&MID(U70,3,2)+2),VALUE(LEFT(U70,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"LRMC-Related Operating Expenditure",191039.82792355926,324024.62531177729,295910.68454149656,205146.79175550755,156056.14014829815,134183.2533223324,128104.60404300141,204923.70386371034,204923.70386371034,146416.87569203737,146618.72169087219,146618.72169087219,146618.72169087219,146618.72169087219,146618.72169087167,146618.72169087219,146618.72169087219,146618.72169087335,146618.72169087219,146618.72169087167,146618.72169087219,146618.72169087219,146618.72169087219]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C71:C85)","v":191039.82792355926},{"$f":"SUM(D71:D85)","v":324024.62531177729},{"$f":"SUM(E71:E85)","v":295910.68454149656},{"$f":"SUM(F71:F85)","v":205146.79175550755},{"$f":"SUM(G71:G85)","v":156056.14014829815},{"$f":"SUM(H71:H85)","v":134183.2533223324},{"$f":"SUM(I71:I85)","v":128104.60404300141},{"$f":"SUM(J71:J85)","v":204923.70386371034},{"$f":"SUM(K71:K85)","v":204923.70386371034},{"$f":"SUM(L71:L85)","v":146416.87569203737},{"$f":"SUM(M71:M85)","v":146618.72169087219},{"$f":"SUM(N71:N85)","v":146618.72169087219},{"$f":"SUM(O71:O85)","v":146618.72169087219},{"$f":"SUM(P71:P85)","v":146618.72169087219},{"$f":"SUM(Q71:Q85)","v":146618.72169087167},{"$f":"SUM(R71:R85)","v":146618.72169087219},{"$f":"SUM(S71:S85)","v":146618.72169087219},{"$f":"SUM(T71:T85)","v":146618.72169087335},{"$f":"SUM(U71:U85)","v":146618.72169087219},{"$f":"SUM(V71:V85)","v":146618.72169087167},146618.72169087219,146618.72169087219,146618.72169087219]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C90,4)+1)&\"-\"&MID(C90,3,2)+2),VALUE(LEFT(C90,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D90,4)+1)&\"-\"&MID(D90,3,2)+2),VALUE(LEFT(D90,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E90,4)+1)&\"-\"&MID(E90,3,2)+2),VALUE(LEFT(E90,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F90,4)+1)&\"-\"&MID(F90,3,2)+2),VALUE(LEFT(F90,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G90,4)+1)&\"-\"&MID(G90,3,2)+2),VALUE(LEFT(G90,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H90,4)+1)&\"-\"&MID(H90,3,2)+2),VALUE(LEFT(H90,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I90,4)+1)&\"-\"&MID(I90,3,2)+2),VALUE(LEFT(I90,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J90,4)+1)&\"-\"&MID(J90,3,2)+2),VALUE(LEFT(J90,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K90,4)+1)&\"-\"&MID(K90,3,2)+2),VALUE(LEFT(K90,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L90,4)+1)&\"-\"&MID(L90,3,2)+2),VALUE(LEFT(L90,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M90,4)+1)&\"-\"&MID(M90,3,2)+2),VALUE(LEFT(M90,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N90,4)+1)&\"-\"&MID(N90,3,2)+2),VALUE(LEFT(N90,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O90,4)+1)&\"-\"&MID(O90,3,2)+2),VALUE(LEFT(O90,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P90,4)+1)&\"-\"&MID(P90,3,2)+2),VALUE(LEFT(P90,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q90,4)+1)&\"-\"&MID(Q90,3,2)+2),VALUE(LEFT(Q90,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R90,4)+1)&\"-\"&MID(R90,3,2)+2),VALUE(LEFT(R90,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S90,4)+1)&\"-\"&MID(S90,3,2)+2),VALUE(LEFT(S90,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T90,4)+1)&\"-\"&MID(T90,3,2)+2),VALUE(LEFT(T90,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U90,4)+1)&\"-\"&MID(U90,3,2)+2),VALUE(LEFT(U90,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"LRMC-Related Operating Expenditure",124016.58642731038,137194.58949473483,174987.72237939457,150557.36846893033,146171.36107999619,137322.8693240234,135037.52539158758,143612.57465228249,143612.57465228249,102610.40618639921,102751.86187468388,102751.86187468388,102751.86187468388,102751.86187468388,102751.86187468388,102751.86187468388,102751.86187468388,102751.861874685,102751.86187468388,102751.86187468388,102751.86187468388,102751.86187468388,102751.86187468388]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C91:C105)","v":124016.58642731038},{"$f":"SUM(D91:D105)","v":137194.58949473483},{"$f":"SUM(E91:E105)","v":174987.72237939457},{"$f":"SUM(F91:F105)","v":150557.36846893033},{"$f":"SUM(G91:G105)","v":146171.36107999619},{"$f":"SUM(H91:H105)","v":137322.8693240234},{"$f":"SUM(I91:I105)","v":135037.52539158758},{"$f":"SUM(J91:J105)","v":143612.57465228249},{"$f":"SUM(K91:K105)","v":143612.57465228249},{"$f":"SUM(L91:L105)","v":102610.40618639921},{"$f":"SUM(M91:M105)","v":102751.86187468388},{"$f":"SUM(N91:N105)","v":102751.86187468388},{"$f":"SUM(O91:O105)","v":102751.86187468388},{"$f":"SUM(P91:P105)","v":102751.86187468388},{"$f":"SUM(Q91:Q105)","v":102751.86187468388},{"$f":"SUM(R91:R105)","v":102751.86187468388},{"$f":"SUM(S91:S105)","v":102751.86187468388},{"$f":"SUM(T91:T105)","v":102751.861874685},{"$f":"SUM(U91:U105)","v":102751.86187468388},{"$f":"SUM(V91:V105)","v":102751.86187468388},102751.86187468388,102751.86187468388,102751.86187468388]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C113,4)+1)&\"-\"&MID(C113,3,2)+2),VALUE(LEFT(C113,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D113,4)+1)&\"-\"&MID(D113,3,2)+2),VALUE(LEFT(D113,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E113,4)+1)&\"-\"&MID(E113,3,2)+2),VALUE(LEFT(E113,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F113,4)+1)&\"-\"&MID(F113,3,2)+2),VALUE(LEFT(F113,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G113,4)+1)&\"-\"&MID(G113,3,2)+2),VALUE(LEFT(G113,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H113,4)+1)&\"-\"&MID(H113,3,2)+2),VALUE(LEFT(H113,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I113,4)+1)&\"-\"&MID(I113,3,2)+2),VALUE(LEFT(I113,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J113,4)+1)&\"-\"&MID(J113,3,2)+2),VALUE(LEFT(J113,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K113,4)+1)&\"-\"&MID(K113,3,2)+2),VALUE(LEFT(K113,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L113,4)+1)&\"-\"&MID(L113,3,2)+2),VALUE(LEFT(L113,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M113,4)+1)&\"-\"&MID(M113,3,2)+2),VALUE(LEFT(M113,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N113,4)+1)&\"-\"&MID(N113,3,2)+2),VALUE(LEFT(N113,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O113,4)+1)&\"-\"&MID(O113,3,2)+2),VALUE(LEFT(O113,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P113,4)+1)&\"-\"&MID(P113,3,2)+2),VALUE(LEFT(P113,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q113,4)+1)&\"-\"&MID(Q113,3,2)+2),VALUE(LEFT(Q113,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R113,4)+1)&\"-\"&MID(R113,3,2)+2),VALUE(LEFT(R113,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S113,4)+1)&\"-\"&MID(S113,3,2)+2),VALUE(LEFT(S113,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T113,4)+1)&\"-\"&MID(T113,3,2)+2),VALUE(LEFT(T113,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U113,4)+1)&\"-\"&MID(U113,3,2)+2),VALUE(LEFT(U113,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"System Peak Demand (MW)",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"SUM(C114:C123)","v":0},{"$f":"SUM(D114:D123)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(W114:W123)","v":0},0,0]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C128,4)+1)&\"-\"&MID(C128,3,2)+2),VALUE(LEFT(C128,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D128,4)+1)&\"-\"&MID(D128,3,2)+2),VALUE(LEFT(D128,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E128,4)+1)&\"-\"&MID(E128,3,2)+2),VALUE(LEFT(E128,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F128,4)+1)&\"-\"&MID(F128,3,2)+2),VALUE(LEFT(F128,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G128,4)+1)&\"-\"&MID(G128,3,2)+2),VALUE(LEFT(G128,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H128,4)+1)&\"-\"&MID(H128,3,2)+2),VALUE(LEFT(H128,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I128,4)+1)&\"-\"&MID(I128,3,2)+2),VALUE(LEFT(I128,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J128,4)+1)&\"-\"&MID(J128,3,2)+2),VALUE(LEFT(J128,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K128,4)+1)&\"-\"&MID(K128,3,2)+2),VALUE(LEFT(K128,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L128,4)+1)&\"-\"&MID(L128,3,2)+2),VALUE(LEFT(L128,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M128,4)+1)&\"-\"&MID(M128,3,2)+2),VALUE(LEFT(M128,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N128,4)+1)&\"-\"&MID(N128,3,2)+2),VALUE(LEFT(N128,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O128,4)+1)&\"-\"&MID(O128,3,2)+2),VALUE(LEFT(O128,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P128,4)+1)&\"-\"&MID(P128,3,2)+2),VALUE(LEFT(P128,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q128,4)+1)&\"-\"&MID(Q128,3,2)+2),VALUE(LEFT(Q128,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R128,4)+1)&\"-\"&MID(R128,3,2)+2),VALUE(LEFT(R128,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S128,4)+1)&\"-\"&MID(S128,3,2)+2),VALUE(LEFT(S128,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T128,4)+1)&\"-\"&MID(T128,3,2)+2),VALUE(LEFT(T128,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U128,4)+1)&\"-\"&MID(U128,3,2)+2),VALUE(LEFT(U128,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"System Peak Demand (MW)",103.45708574202202,108.29728244815,111.38778852143535,115.20332767172945,118.49595591823483,120.90322313439914,122.90390410192101,125.0465432383868,127.25797454534145,129.42172739511696,131.58846313093707,133.75519886675718,135.92193460257729,138.08867033839741,140.25540607421749,142.4221418100376,144.58887754585771,146.75561328167782,148.92234901749794,151.08908475331802,153.25582048913813,155.42255622495824,157.58929196077835]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"SUM(C129:C138)","v":103.45708574202202},{"$f":"SUM(D129:D138)","v":108.29728244815},111.38778852143535,115.20332767172945,118.49595591823483,120.90322313439914,122.90390410192101,125.0465432383868,127.25797454534145,129.42172739511696,131.58846313093707,133.75519886675718,135.92193460257729,138.08867033839741,140.25540607421749,142.4221418100376,144.58887754585771,146.75561328167782,148.92234901749794,151.08908475331802,{"$f":"SUM(W129:W138)","v":153.25582048913813},155.42255622495824,157.58929196077835]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2024"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C143,4)+1)&\"-\"&MID(C143,3,2)+2),VALUE(LEFT(C143,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D143,4)+1)&\"-\"&MID(D143,3,2)+2),VALUE(LEFT(D143,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E143,4)+1)&\"-\"&MID(E143,3,2)+2),VALUE(LEFT(E143,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F143,4)+1)&\"-\"&MID(F143,3,2)+2),VALUE(LEFT(F143,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G143,4)+1)&\"-\"&MID(G143,3,2)+2),VALUE(LEFT(G143,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H143,4)+1)&\"-\"&MID(H143,3,2)+2),VALUE(LEFT(H143,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I143,4)+1)&\"-\"&MID(I143,3,2)+2),VALUE(LEFT(I143,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J143,4)+1)&\"-\"&MID(J143,3,2)+2),VALUE(LEFT(J143,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K143,4)+1)&\"-\"&MID(K143,3,2)+2),VALUE(LEFT(K143,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L143,4)+1)&\"-\"&MID(L143,3,2)+2),VALUE(LEFT(L143,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M143,4)+1)&\"-\"&MID(M143,3,2)+2),VALUE(LEFT(M143,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N143,4)+1)&\"-\"&MID(N143,3,2)+2),VALUE(LEFT(N143,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O143,4)+1)&\"-\"&MID(O143,3,2)+2),VALUE(LEFT(O143,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P143,4)+1)&\"-\"&MID(P143,3,2)+2),VALUE(LEFT(P143,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q143,4)+1)&\"-\"&MID(Q143,3,2)+2),VALUE(LEFT(Q143,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R143,4)+1)&\"-\"&MID(R143,3,2)+2),VALUE(LEFT(R143,4)+1))","v":"2038-39"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S143,4)+1)&\"-\"&MID(S143,3,2)+2),VALUE(LEFT(S143,4)+1))","v":"2039-40"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T143,4)+1)&\"-\"&MID(T143,3,2)+2),VALUE(LEFT(T143,4)+1))","v":"2040-41"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U143,4)+1)&\"-\"&MID(U143,3,2)+2),VALUE(LEFT(U143,4)+1))","v":"2041-42"},{"$f":"W$12","v":"2042-43"},{"$f":"X$12","v":"2043-44"},"2044-45"]
[null,"System Peak Demand (MW)",248.09517779225632,259.70220744850116,267.11339294846493,276.26324341135143,284.15912781947708,289.93187295050654,294.72960426859754,299.86775825479873,305.17087924780992,310.35966495652542,315.55560377262123,320.75154258871703,325.94748140481283,331.14342022090864,336.33935903700444,341.53529785310025,346.73123666919605,351.92717548529191,357.12311430138772,362.31905311748352,367.51499193357932,372.71093074967513,377.90686956577093]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand",{"$f":"SUM(C144:C153)","v":248.09517779225632},{"$f":"SUM(D144:D153)","v":259.70220744850116},267.11339294846493,276.26324341135143,284.15912781947708,289.93187295050654,294.72960426859754,299.86775825479873,305.17087924780992,310.35966495652542,315.55560377262123,320.75154258871703,325.94748140481283,331.14342022090864,336.33935903700444,341.53529785310025,346.73123666919605,351.92717548529191,357.12311430138772,362.31905311748352,{"$f":"SUM(W144:W153)","v":367.51499193357932},372.71093074967513,377.90686956577093]

{"sheet":"7.8 Export Services","index":28,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"REGULATORY PERIOD FROM \", FRCP_y1,\" TO \",dms_MultiYear_FinalYear_Result)","v":"REGULATORY PERIOD FROM 2024-25 TO 2028-29"}]
[null,"7.8 EXPORT SERVICES"]
[]
[null,"Expenditure must only be related to DER integration, and must exclude amounts relating to DMIA"]
[]
[null,"Export service related overvoltage complaint management\nexamples include but not limited to: complaint processing, analysis, transformer tapping "]
[]
[null,"7.8.1 - OPEX FOR PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"Export service related overvoltage complaint management",0,0,0,0,0,0,0]
[null,"Other opex",0,0,0,0,0,0,0]
[]
[]
[null,"ICT capex\nexamples include but not limited to: establishing systems for network visibility, hosting capacity assessments, generation of dynamic operating envelopes"]
[null,"Network monitoring capex\nexamples include but not limited to: implementing transformer monitors"]
[]
[null,"7.8.2 - CAPEX FOR THE PROVISION OF EXPORT SERVICES"]
[null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2024)"}]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"ICT capex",0,0,637695.20373502094,802492.04958818073,5544581.5605401592,2937732.3648589291,3297810.2387787392]
[null,"Network monitoring capex",0,0,0,0,0,0,0]
[null,"Other capex",0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,"7.8.3 - EXPORT VOLUMES - NET METERED VOLUME OF ENERGY EXPORTED"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"VOLUMES\nMWh"]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,{"$f":"C41","v":0.15279100000000001},{"$f":"D41","v":0.171791},0.19079099999999999,0.20979100000000001,0.22879099999999999,0.24779100000000001]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,{"$f":"C42","v":15.16703787691222},{"$f":"D42","v":15.783640596221254},16.317766166719345,16.78889830934488,17.210340371976184,17.591581091193483]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,{"$f":"C43","v":62},69,76,83,90,97]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,{"$f":"C44","v":1.002484586756238},1.0440167878193769,1.0799936168086315,1.1117274289733885,1.140114291265014,1.1657933317689737]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C45,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0.15279100000000001,0.171791,0.19079099999999999,0.20979100000000001,0.22879099999999999,0.24779100000000001,0.266791]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},15.16703787691222,15.783640596221254,16.317766166719345,16.78889830934488,17.210340371976184,17.591581091193483,17.939626599152]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},62,69,76,83,90,97,104]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},1.002484586756238,1.0440167878193769,1.0799936168086315,1.1117274289733885,1.140114291265014,1.1657933317689737,1.1892364590257818]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[]
[]
[null,"7.8.4 EXPORT SERVICES - CUSTOMER NUMBERS"]
[null,"A. BY FEEDER CLASSIFICATION"]
[null,null,"CUSTOMER NUMBERS\n(0's)"]
[null,null,{"$f":"CRCP_y4","v":"2022-23"},{"$f":"CRCP_y5","v":"2023-24"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"FRCP_y2","v":"2025-26"},{"$f":"FRCP_y3","v":"2026-27"},{"$f":"FRCP_y4","v":"2027-28"},{"$f":"FRCP_y5","v":"2028-29"}]
[null,"i. Beginning of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},19,{"$f":"C59","v":21},{"$f":"D59","v":22},23,24,25,25]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},2807,{"$f":"C60","v":792},{"$f":"D60","v":981},1215,1504,1862,2306]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},13017,{"$f":"C61","v":10019},12070,14121,16172,18223,20274]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},171,{"$f":"C62","v":133},160,188,215,242,269]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},null,{"$f":"IF(dms_TradingName=\"TasNetworks (D)\",C63,\"\")","v":""},"","","","",""]
[null,"ii. End of period"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},21,22,23,24,25,25,26]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},792,981,1215,1504,1862,2306,2855]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},10019,12070,14121,16172,18223,20274,22325]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},133,160,188,215,242,269,296]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]

{"sheet":"AER Sheet Heading","index":29,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"dms_Header_Span","v":"2022-23 to 2028-29"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2024)"}]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C15:C35)","v":0},{"$f":"SUM(D15:D35)","v":0},0,0,0,0,0]
[null,null,{"$f":"SUM(C15:C36)","v":0},{"$f":"SUM(D15:D36)","v":0},0,0,0,0,0]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"dms_y1","v":"2022-23"},{"$f":"dms_y2","v":"2023-24"},{"$f":"dms_y3","v":"2024-25"},{"$f":"dms_y4","v":"2025-26"},{"$f":"dms_y5","v":"2026-27"},{"$f":"dms_y6","v":"2027-28"},{"$f":"dms_y7","v":"2028-29"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"SUM(C46:C66)","v":0},{"$f":"SUM(D46:D66)","v":0},{"$f":"SUM(E46:E66)","v":0},{"$f":"SUM(F46:F66)","v":0},{"$f":"SUM(G46:G66)","v":0},{"$f":"SUM(H46:H66)","v":0},{"$f":"SUM(I46:I66)","v":0}]
[null,null,{"$f":"SUM(C46:C67)","v":0},{"$f":"SUM(D46:D67)","v":0},{"$f":"SUM(E46:E67)","v":0},{"$f":"SUM(F46:F67)","v":0},{"$f":"SUM(G46:G67)","v":0},{"$f":"SUM(H46:H67)","v":0},{"$f":"SUM(I46:I67)","v":0}]

{"sheet":"AER CF","index":30,"n_rows":77,"n_cols":25,"rows_kept":77,"cut":false,"hidden":true,"merged":[[3,1,3,22],[39,38,39,59],[40,38,40,59],[41,38,41,59],[39,69,39,90],[40,69,40,90],[41,69,41,90]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[null,"CELLS FLAGED \"Y\" and greyed out will be greyed out in the worksheets."]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":true},"=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",null,null,"=INDEX(dms_CF_F10, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6.1","dms_CF_3.6.6.2","dms_CF_3.6.6.3","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.8 (set from dms_MAIFI_flag)","dms_CF_7.12","dms_CF_8.1_A  (and 8.4)","dms_CF_8.1_B  (and 8.4)","dms_CF_8.1_Neg  (and 8.4)","dms_CF_4.4.1","dms_CF_MAIFI_flag (set from dms_MAIFI_flag)","9.5 TUOS (set from Jurisdiction)","dms_CF_F10"]
[null,"Amadeus","NT","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"APA GasNet","Vic","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C7=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ausgrid (Tx Assets)","NSW","Electricity","Distribution",null,"Y","N","N","N","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C8=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C9=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","Y","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C10=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co.","NSW","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C13=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Australian Distribution Co. (Vic)","Vic","Electricity","Distribution","N","N","N","N",null,"N","N","N","N","N","N","Y","N","N","N","N","N","N",{"$f":"IF('AER CF'!$C14=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C15=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C16=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-","Y","N","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C17=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C18=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Energex","Qld","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N",{"$f":"IF('AER CF'!$C19=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C20=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y","N","Y","Y","N","N","N","Y","N","N","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C21=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C22=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Evoenergy Distribution (Tx Assets)","ACT","Electricity","Distribution",null,"Y","N","Y","Y","Y","Y","N","Y","N","Y","Y","Y","N","Y","Y","N","N",{"$f":"IF('AER CF'!$C23=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N","Y","N","N","N","Y","N","N",{"$f":"IF('AER CF'!$C25=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"JGN","Vic","Gas","Distribution","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C26=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Power and Water","NT","Electricity","Distribution",null,"N","N",null,null,"N","Y","N","N","N","Y",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","Y","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C27=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C28=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C29=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"Roma to Brisbane Pipeline","Qld","Gas","Transmission","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","N","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C31=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"Y","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C32=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C33=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,null,null,"N","N","N","N","N","-",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","Y","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C34=\"Vic\",\"Y\",\"N\")","v":"N"}]
[null,"United Energy","Vic","Electricity","Distribution",null,"N","N",null,null,"N","N","N","N","N","N",{"$f":"IFERROR(IF(_xlfn.SINGLE(dms_MAIFI_Flag)=\"Yes\",\"N\",\"Y\"),\"Y\")","v":"Y"},"N","N","N","Y","N",{"$f":"IFERROR(LEFT(_xlfn.SINGLE(dms_MAIFI_Flag)),\"N\")","v":"N"},{"$f":"IF('AER CF'!$C35=\"Vic\",\"Y\",\"N\")","v":"Y"}]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE","dms_H2"]
[null,"TOP HEADER","dms_H1"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,5.1109999999999998,"dms_NUM"]
[null,5.45E-2,"dms_NUM%"]
[null,5.5555000000000003,"dms_NUM3d"]
[null,"Text description","dms_Row_Locked"]
[null,"Text description - not locked","dms_Row1"]
[null,"Text description","dms_Row2"]
[null,"Total","dms_T1"]
[null,"Total","dms_T2"]
[null,"EXPENSES","dms_BH"]
[null,2019,"dms_BY1"]
[null,2019,"dms_BY2"]
[null,"VOLUMES","dms_GH"]
[null,2019,"dms_GY1"]
[null,2019,"dms_GY2"]

{"sheet":"AER NRs","index":31,"n_rows":232,"n_cols":16,"rows_kept":232,"cut":false,"hidden":true,"merged":[[33,67,33,88],[34,67,34,88],[35,67,35,88],[36,10,40,10],[44,10,45,10],[33,10,35,10],[33,36,33,57],[34,36,34,57],[35,36,35,57],[208,1,213,1],[199,1,200,1],[32,1,55,1],[100,1,107,1],[110,1,115,1],[191,1,192,1],[195,1,196,1],[160,1,174,1],[4,1,28,1],[176,1,177,1],[179,1,184,1],[65,1,78,1],[135,1,150,1],[84,1,97,1],[152,1,158,1],[118,1,132,1]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Tariff cap"]
[null,null,"Final decision","Weighted average price cap"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Reallocated"]
[null,null,"Recast"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[null,null,null,null,null,null,null,null,null,null,null,null,"GAS ARR & RESET"]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140201_UOM","dms_E050201_UOM","dms_E050202_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number per km","per metre per connection","metres per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","per service per connection","number per connection"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number per connection","number per connection"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","dms_E020202_UOM","Spare"]
[null,null,"number","number","Length of mains replaced"]
[null,null,"number","number","Number of services replaced"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)",""]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":{"$error":"#NAME?"}}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]
[]
[]
[]
[null,"PTRM input sheet","DMS_50_01_01a","DMS_50_01_01aa","DMS_50_01_01b","DMS_50_01_01bb","DMS_50_01_01c","DMS_50_01_01d","DMS_50_01_01dd"]

{"sheet":"AER lookups","index":32,"n_rows":101,"n_cols":37,"rows_kept":101,"cut":false,"hidden":true,"merged":[[15,60,15,81],[22,1,22,4],[4,24,4,35],[5,24,5,27],[5,29,7,33],[5,34,7,34],[5,35,7,35],[5,36,7,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Template number",5]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_MAIFI_flag_List","dms_Public_Lighting_List","Name"]
[null,"Ausgrid","Ausgrid",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES",{"$f":"B10","v":"Ausgrid"}]
[null,"Ausgrid (Tx Assets)","Ausgrid (Tx Assets)",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Ausgrid (Tx Assets)"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Australian Distribution Co."]
[null,"Endeavour Energy","Endeavour Energy",11247365823,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"51 Huntingwood Drive",null,"HUNTINGWOOD","NSW",2148,"PO Box 811",null,"SEVEN HILLS","NSW",1730,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Endeavour Energy"]
[null,"Essential Energy","Essential Energy",37428185226,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"8 Buller Street",null,"PORT MACQUARIE","NSW",2444,"PO Box 5730",null,"PORT MACQUARIE","NSW",2444,"NO","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","YES","Essential Energy"]
[null,"Evoenergy Distribution","Evoenergy Distribution",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"NO","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Evoenergy Distribution"]
[null,"Evoenergy Distribution (Tx Assets)","Evoenergy Distribution (Tx Assets)",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"NO","YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Evoenergy Distribution (Tx Assets)"]
[null,"Power and Water","Power and Water Corporation",15947352360,"NT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"x","GPO Box 1921",null,"DARWIN","NT",801,"GPO Box 1921",null,"DARWIN","NT",801,"YES","YES","YES","YES","NO","CBD","Urban","Short rural","Long rural",null,"NO","NO","Power and Water"]
[null,"TasNetworks (D)","TasNetworks (D)",24167357299,"Tas","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,5,"1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,"YES","YES","YES","YES","YES","Critical Infrastructure","Urban","High density commercial","High density rural","Low density rural","NO","YES","TasNetworks (D)"]
[]
[]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"EBSS","Efficiency Benefit Sharing Scheme","EFFICIENCY BENEFIT SHARING SCHEME",5]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"Profitability","Profitability","PROFITABILITY",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88",1988,"PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2014-15"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2019-20"},{"$f":"FRCP_y1","v":"2024-25"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2024-25"}]
[null,"1988-89",1989,"PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2015-16"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2020-21"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2025-26"}]
[null,"1989-90",1990,"PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2016-17"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2021-22"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2026-27"}]
[null,"1990-91",1991,"PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2017-18"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2022-23"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2027-28"}]
[null,"1991-92",1992,"PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2018-19"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2023-24"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2028-29"}]
[null,"1992-93",1993,"PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2019-20"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2024-25"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2029-30"}]
[null,"1993-94",1994,"PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2020-21"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2025-26"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2030-31"}]
[null,"1994-95",1995,"PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2021-22"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2026-27"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2031-32"}]
[null,"1995-96",1996,"PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2022-23"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2027-28"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2032-33"}]
[null,"1996-97",1997,"PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2023-24"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2028-29"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2033-34"}]
[null,"1997-98",1998,"PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2024-25"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2029-30"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2034-35"}]
[null,"1998-99",1999,"PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2025-26"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2030-31"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2035-36"}]
[null,"1999-00",2000,"PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2026-27"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2031-32"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2036-37"}]
[null,"2000-01",2001,"PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2027-28"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2032-33"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2037-38"}]
[null,"2001-02",2002,"PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2028-29"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2033-34"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2038-39"}]
[null,"2002-03",2003,"PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2029-30"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2034-35"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2039-40"}]
[null,"2003-04",2004,"PRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+16)","v":"2030-31"},"CRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+16)","v":"2035-36"},"FRCP_y17",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+16)","v":"2040-41"}]
[null,"2004-05",2005,"PRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+17)","v":"2031-32"},"CRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+17)","v":"2036-37"},"FRCP_y18",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+17)","v":"2041-42"}]
[null,"2005-06",2006,"PRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+18)","v":"2032-33"},"CRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+18)","v":"2037-38"},"FRCP_y19",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+18)","v":"2042-43"}]
[null,"2006-07",2007,"PRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+19)","v":"2033-34"},"CRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+19)","v":"2038-39"},"FRCP_y20",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+19)","v":"2043-44"}]
[null,"2007-08",2008,"PRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+20)","v":"2034-35"},"CRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+20)","v":"2039-40"},"FRCP_y21",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+20)","v":"2044-45"}]
[null,"2008-09",2009,"PRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+21)","v":"2035-36"},"CRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+21)","v":"2040-41"},"FRCP_y22",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+21)","v":"2045-46"}]
[null,"2009-10",2010,"PRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+22)","v":"2036-37"},"CRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+22)","v":"2041-42"},"FRCP_y23",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+22)","v":"2046-47"}]
[null,"2010-11",2011,"PRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+23)","v":"2037-38"},"CRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+23)","v":"2042-43"},"FRCP_y24",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+23)","v":"2047-48"}]
[null,"2011-12",2012,"PRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+24)","v":"2038-39"},"CRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+24)","v":"2043-44"},"FRCP_y25",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+24)","v":{"$error":"#REF!"}}]
[null,"2012-13",2013]
[null,"2013-14",2014]
[null,"2014-15",2015]
[null,"2015-16",2016]
[null,"2016-17",2017]
[null,"2017-18",2018]
[null,"2018-19",2019]
[null,"2019-20",2020]
[null,"2020-21",2021]
[null,"2021-22",2022,null,"CRY - FRY"]
[null,"2022-23",2023,"dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2022-23"}]
[null,"2023-24",2024,"dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2023-24"}]
[null,"2024-25",2025,"dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2024-25"}]
[null,"2025-26",2026,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2025-26"}]
[null,"2026-27",2027,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2026-27"}]
[null,"2027-28",2028,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2027-28"}]
[null,"2028-29",2029,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2028-29"}]
[null,"2029-30",2030,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2029-30"}]
[null,"2030-31",2031,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2030-31"}]
[null,"2031-32",2032,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2031-32"}]
[null,"2032-33",2033,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2032-33"}]
[null,"2033-34",2034,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2033-34"}]
[null,"2034-35",2035,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2034-35"}]
[null,"2035-36",2036,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2035-36"}]
[null,"2036-37",2037,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2036-37"}]
[null,"2037-38",2038,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2037-38"}]
[null,"2038-39",2039,"dms_y17",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+16),0)","v":"2038-39"}]
[null,"2039-40",2040,"dms_y18",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+17),0)","v":"2039-40"}]
[null,"2040-41",2041,"dms_y19",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+18),0)","v":"2040-41"}]
[null,"2041-42",2042,"dms_y20",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+19),0)","v":"2041-42"}]
[null,"2042-43",2043,"dms_y21",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+20),0)","v":"2042-43"}]
[null,"2043-44",2044,"dms_y22",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+21),0)","v":"2043-44"}]
[null,"2044-45",2045,"dms_y23",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+22),0)","v":"2044-45"}]
[null,"2045-46",2046,"dms_y24",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+23),0)","v":"2045-46"}]
[null,"2046-47",2047,"dms_y25",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+24),0)","v":"2046-47"}]
[null,"2047-48",2048,"dms_y26",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+25),0)","v":"2047-48"}]

{"sheet":"AER ETL","index":33,"n_rows":145,"n_cols":10,"rows_kept":145,"cut":false,"hidden":true,"merged":[[32,37,32,58],[33,37,33,58],[34,37,34,58],[32,68,32,89],[33,68,33,89],[34,68,34,89],[12,4,12,8],[71,1,73,1],[11,0,15,0],[18,0,25,0],[26,0,31,0],[34,0,59,0],[14,2,14,4]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"Power and Water"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Regulatory proposal","dms_Source",{"$f":"IF(dms_Model=\"Reset\", \"Make sure you have set Reg Proposal as source\",\"\")","v":"Make sure you have set Reg Proposal as source"}]
[null,"Data quality","Consolidated","For DB purposes this is always Consoldiated"]
[null,"Data status","Public","For DB purposes this is always Public"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"31/01/23"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality","Consolidated","dms_DataQuality","Always Consolidated"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)","v":"2029"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),dms_RYE_result)"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM",{"$f":"IF(dms_SingleYearModel=\"yes\",\"This is set to an historical template (EB, CA or ARR), apply UOM Named Range to cell !\",\"This is not an historical template, make sure UOM Named Range is not applied\")","v":"This is not an historical template, make sure UOM Named Range is not applied"},null,null,null,null,{"$f":"IFERROR(dms_dollar_nom_UOM, \"NR not applied\")","v":"NR not applied"}]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"NT"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"2022-23"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"2022"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))","v":"June 2024"},"dms_DollarReal","=IF(dms_Model=\"RFM\",dms_DollarReal_Prev, IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRY_start_year,2)&RIGHT(dms_CRY_start_year,2))),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year","v":"June 2019"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2024-25"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2022-23"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":36},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":38},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":33},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":28},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":42},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2024-25"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2019-20"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2014-15"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2028-29"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2023-24"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2018-19"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2028-29"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2028-29"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2024"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2019"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":"2023"},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2029"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2029"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2024-25 to 2028-29"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_y1&\" to \"&FRCP_final_year,CRY))","v":"2022-23 to 2028-29"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"2022-23"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2028-29"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C50,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"2022-23"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"x"},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(dms_SingleYearModel=\"yes\",(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(PRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(PRCP_y4,4))))","v":"1-Jul-2017"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060101_StartDateTxt)","v":42917},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"Does the NSP report MAIFI or MAIFIe",{"$f":"INDEX(dms_MAIFI_flag_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_MAIFI_Flag"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes","Must be present for ARRs","=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","0","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2016"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]